{"text_format":"1","workbook":"xlsx","n_sheets":49,"sheets":["Start","Vodič kroz program","Unos podataka","Analiza i dimenzioniranje","Sile i krakovi","Dodatni proračuni","Rasprostiranje vertikalnog opt","MT","Poprečni presjek zida","Tlocrt temelja i pogled na zid","Dijagram momenata","Sidra","Iskaz armature","Dopušteno","P III-III","P Mmin","P Mmax","P VI-VI","P VII-VII","P VIII-VIII","P IX-IX","P X-X","P XI-XI","P XII-XII","P XIII-XIII","P XIV-XIV","P XV-XV","P XVI-XVI","P XVII-XVII","P XVIII-XVIII","P XIX-XIX","P XX-XX","Slijeganje","T1","T2","Dopušteno Vs+","Dopušteno Vs-","ProjektniPristupi","Troškovnik","C III-V","C VI-VII","C VIII-IX","C X-XI","C XII-XIII","C XIV-XV","C XVI-XVII","C XVIII-XIX","HT III-XX","Kontrafore"],"not_rendered":{"charts":213,"images":2,"macros":1,"external_links":0,"defined_names":25,"comments":38,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Start","index":0,"n_rows":5,"n_cols":2,"rows_kept":5,"cut":false,"hidden":false,"merged":[[76,0,76,9],[11,0,12,4]]}
[]
[]
[]
[]
[null,"Lozinka: ABC"]

{"sheet":"Vodič kroz program","index":1,"n_rows":39,"n_cols":5,"rows_kept":39,"cut":false,"hidden":false,"merged":[[23,1,23,9],[11,1,11,9],[6,1,6,9],[5,1,5,9],[15,1,15,9],[17,1,17,9],[19,1,19,9],[21,1,21,9],[8,1,8,9],[10,1,10,9],[13,1,13,9],[0,0,0,9],[1,1,1,9],[2,1,2,9],[3,1,3,9],[4,1,4,9],[30,1,30,9],[32,1,32,9],[33,1,33,9],[38,1,38,9],[25,1,25,9],[27,1,27,9],[29,1,29,9],[28,1,28,9],[37,1,37,9],[35,1,35,9],[36,1,36,9],[31,1,31,9],[34,1,34,9]]}
["VODIČ KROZ PROGRAM   "]
["1.","Općenito "]
[null,"   Ova verzija programa predstavlja nadogradnju prethodnih verzija te sadrži dodatno prilagođavanje prikaza i ispisa EC7 te poboljšanja preciznosti pojedinih proračuna. \n   U odnosu na starije verzije programa, razlike u Faktorima sigurnosti su minimalne.\n   Program je izrađen u Excelu uz podršku VBA (Visaual basic) modula. \n   Ulazni podaci upisuju se u 7 Formi: 1. Karakteristike tla,  2. Djelovanja, 3. Dimenzije zida,   4. Sidra i konzola, 5. Kontrafore,  6. Gradivo i  7. Profil terena, koje se pojavljuju nakon upisa lozinke. \n     Nove podatke treba potvrditi na svakoj formi sa tipkom Potvrda unosa novih podataka.\n     Ovaj Vodič kroz program i dodatni tekstovi u komentarima pojedinih ćelija na stranici (sheet): Analiza i dimenzioniranje pripremljeni su tako da bi trebali dati dovoljno objašnjenja za korištenje programa. \n    Ukoliko korisnik ima dodatnih pitanja, ista se mogu poslati autoru na priloženu e-mail adresu ili na broj:             +385 98 213 632.                                                                                                                                                                                 "]
["2.","Analiza stabilnosti   "]
["2.1.","      Potpornog, obložnog, potporno-obložnog i gravitacijskog zida, sa ili bez rasteretne konzole, sa ili bez sidara (do 4 reda sidara), sa ili bez kontrafora, zida iza kojeg mogu biti tri sloja tla (tlo u zoni temeljenja je četvrti sloj) i raznovrsna opterećenja (prometno, opterećenje temeljem, linijsko i točkasto). Umjesto Opterećenja temeljem može se upisati bilo koje drugo opterećenje (npr. specijalno vozilo). \n      Osim navedenih opterećenja moguće je u analizi, osim NPV (nivo podzemne vode) iza zida,  imati i vodu ispred zida (rijeka, jezero).                                                                                                                                                                                                                                                                 Ovi podaci ulaze u kontrole graničnih stanja nosivosti i dimenzioniranje zida. \n     Na gravitacijskom zidu, konzole, sidra i kontrafore se ne izvode ali je ovim programom moguće napraviti i takve analize.\n     Nakon izbora: Projektnog pristupa, popunjavanja svih čelija s plavom bojom (ostale vrijednosti su računske) u Formama od 1 do 7 i napravljene Potvrde unosa novih podataka, dobivaju se konačni Stupnjevi iskorištenosti (Faktori sigurnosti) za prevrtanje, klizanje i nosivost tla ispod zida.  \n    Program je u potpunosti usklađen s EC2, EC7 i EC8. \n    Ukoliko ne koristite EC, u čelije N27 do N45, P31 do P34 i R31 do R34, stranici (sheet) Analiza i dimenzioniranje, mogu se upisati vrijednosti parcijalnih koeficijenata koje su u skladu s  propisima pojedine države (prema uputama u komentaru čelije N24). U navedenim čelijama izvorno su upisane vrijednosti parcijalnih faktora propisanih u Hrvatskoj gdje je predviđen Projektni pristup 3.\n                                                                                                                                                      "]
["2.2.","    Obložni zid: Ako se npr. ispred sloja 2 i 3 izvodi obložni zid, tada su kutevi trenja za te slojeve - fiktivni (j*), odnosno oni kutevi koji u vrijednosti  Q=45+j/2 daju pokos prirodnog terena Q, odnosno klizne plohe (plohe aktivnog klina).   Na primjer: Prirodni pokos (ujedno klizna ploha) ima kut Q=80o. Računski - fiktivni kut unutrašnjeg trenja: j* = (80-45)*2=70o,  i kohezija C=0. \n     Ukoliko je zid po čitavoj visini obložni, tada se takvi fiktivni kutevi unutrašnjeg trenja upisuju za sva tri sloja."]
["2.3.","     Masivni -gravitacijski zid: Ukoliko se projektira Masivni zid, u Formi 3, ispod podataka o masivnom zidu, izaberi DA, a ako je predviđen armirano betonski zid izaberi  NE. \n     Oblikovanje zida predviđeno je prema Švicarskim propisima. U tako oblikovanom zidu, u bilo kojem presjeku, nema vlačnih naprezanja, pa prema tome nije potrebna nikakva armatura. Ipak, predlažem iz konstruktivnih razloga ugraditi samo sidrenu armaturu (ankere) iz temelja s pripadajućom razdjelnom armaturom. \n- Projektant određuje i upisuje samo visinu zida i širinu zida u kruni, a sve ostale dimenzije određuju se automatski.\n- Nakon Potvrde unosa novih podataka, proračun je završen.\n   Ukoliko kontrola iskorištenosti (faktori sigurnosti) za klizanje, prevrtanje i nosivost tla (vidi u Formi 3, Dimenzije zida) ne  zadovoljava (Iskorištenost>100% ili Fs<1) ili je preniska (Iskorištenost<50%, Fs previsoki), nije nužno ali je moguće navedeni  postupak ponoviti s promjenom dimenzija zida ili smanjenom širinom zida u kruni."]
["3.","Konzola"]
[null,"     Ukoliko zid ima rasteretnu konzolu u Formi 4. Sidra i konzola, izaberi DA, a ako nema konzole, izaberi NE. \n     Konzola se može koristiti za povećanje stabilnosti na prevrtanje ali u tom slučaju treba povećati  širinu konzole, koja u tom slučaju treba biti veća odširine temelja iza zida. \n      Izvedbom konzole smanjuje se moment savijanja u presjeku zid-temelj, što utječe na uštedu betona i armature.\n      Napomena: Analiza i dimenzioniranje u ovom programu predviđeni su za konzolu na visinama većim od 1/2 ukupne visine zida (H). Na manjim visinama korist od konzole je zanemariva i nije ekonomski opravdana.    \n      U originalnom programu to je  6,0 m/2=3,0 m tj. +E48/2<E79 (u Analizi i dimenzioniranje).\n     Budući da su rezne sile izračunate za unaprijed određene presjeke, preporučam visine podgleda konzole postaviti u jedan takav presjek, označen u sheet Analiza i dimenzioniranje (čelije K72 do K81) \n     \n     \n\n\n    \n "]
["4.","Sidra"]
[null,"     Proračun nosivosti sidara i određivanje slobodne i sidrišne dionice            "]
[null,"     Ukoliko je zid projektiran sa sidrima, u Formi 4. Sidra i konzola, izaberi DA, a ako sidara nema, izaberi NE. Zadane sile u sidrima su sile po m' zida. Orijentacijska nosivost sidara računa se automatski nakon upisa podataka o sidrima.  Nakon Potvrde unosa novih podataka obavezno treba provjeriti da li je minimalna duljina slobodne dionice veća od zadane (u Formi 4.). Ukoliko je predviđena slobodna dionica pojedinog sidra manja od minimalne potrebno je slobodnu dionicu produljiti na vrijednost iznad minimalne. U programu su predviđena 1 do 4  reda sidara. Ukoliko projektant stavlja samo jedan red tada se drugi i svi ostali redovi ne zadaju (početne programske upisane vrijednosti se brišu s DELETE). \n      Ukoliko je razmak sidara I. i II. III. i IV. reda različit,  treba taj razmak ujednačiti iz estetskih razloga. Razmak sidara mijenja se produljivanjem ili skraćivanjem sidrišne dionice. Nakon svake promjene sidrišne dionice napravite Potvrdu unosa novih podataka kako bi ustanovili da li ste postigli željeni razmak sidara. Za postizanje tog cilja, postupak će vjerojatno trebati ponoviti. \n Važno: I. red sidara je uvijek najviši red, II. red je ispod I. reda itd.\n                                                                                                                                                             "]
["5.","Kontrafore"]
[null,"     Ukoliko je predviđena izvedba kontrafora, u Formi 5. Kontrafore, izaberi DA, a ako kontrafora nema izaberi NE.    \n     Izvedbom kontrafora može se uštedjeti na betonu zida, smanjenjem visine presjeka zida u kruni i na kontaktu sa temeljem, ali pri izradi kontrafora treba voditi računa i o troškovima betona, oplate i rada za izradu kontrafora. Smatram da, sa toga stanovišta, pri odluci o korištenju kontrafora treba izvršiti detaljniju analizu isplativosti korištenja kontrafora.\n     S produženjem temelja na mjestu kontrafora efikasno se može povećati stabilnost zida a da pri tome nije potrebno povećavati širinu temelja \"B\" po čitavoj duljini zida. To naročito vrijedi za temelje u stjenovitom tlu jer se u tom slučaju bitno smanjuju troškovi iskopa u stijeni (iskop samo za temelje kontrafore). Čak niti sa ovakvom izvedbom (što se tiče duljine temelja kontrafore) ne treba pretjerivati jer se u tom slučaju znatno povećava potresna sila (ukoliko se zid računa sa potresom).      Zadovoljavajući rezultat dobiva se produljenjem temelja kontrafore već za cca 1 m (kao u originalu ovog programa)."]
["6.","Gradivo"]
[null,"    Klasu betona i armaturu, posebno za temelje, a posebno za zid, konzolu i kontrafore, izabire projektant u Formi    6. Gradivo.\n    Ovim programom armiranje temelja i zida moguće je sa rebrastom armaturom ili armaturnim mrežama.  Izbor profila rebraste armature moguć je putem padajućeg menija.\n    Ukoliko se predvidi ugradnja armature mreže u zidu a pri tome najjača armaturna mreža nema dovoljno površine, slijedi upozorenje o potrebi ugradnje rebraste armature. I tada je moguće odabrati armaturnu mrežu, ali izvan ovog programa, jer će u tom slučaju biti potrebno preklopiti 2 ili više mreža što programom nije predviđeno.  Isto vrijedi i za armaturu temelja. \n    Ukoliko se za zid odabere armaturna mreža, broj sidrenih šipki (ankera) iz temelja odgovara broju nosivih šipki po m'  armaturne mreže (radi nastavka sidrenih šopki na nosivu armaturne mreže).\n    Bitno je u oba slučaja zadovoljiti proračunom predviđenu površinu armature.\n    "]
["7.","Dimenzioniranje",null,null,"(za gravitacioni zid nije potrebno)"]
[null,"     Dimenzioniranje armirano betonskog zida provodi se, prema Metodi graničnog stanja (EC2), u pet programiranih presjeka kroz zid i temelj (presjeci od I-I do V-V) i presjek kroz konzolu. Presjek IV-IV je na visini zida gdje je računski moment savijanja minimalan (Mmin), osim presjeka III-III koji je uvijek minimalan kada nema konzole. \n     Presjek V-V je na mjestu maksimalnog računskog momenta savijanja (Mmax), osim 0. \n    Projektant može izvršiti i provjeru armature u bilo kojem presjeku, koristeći pri tome vrijednosti momenata savijanja i uzdužnih sila iz čelija T43 do AI51 u stranici (sheet)  Analiza i dimenzioniranje.  "]
["8.","Dijagram momenata, poprečnih i uzdužnih sila"]
[null,"     Prikazan je na stranici (sheet) Analiza i dimenzioniranje (izvan zone ispisa). Uz presjeke kroz zid I-I do V-V, za koje je izvršeno i dimenzioniranje, izračunati su momenti savijanja u približno petnaestinama visine zida. Na ovaj način, dobivena je realna raspodjela momenata savijanja duž zida.   "]
["9.","Iskaz armature i sidara",null,null,"(za gravitacioni zid potrebna je samo Poz. 5)"]
[null,"     Nacrt armature prikazan je na stranici (sheet) Analiza stabilnosti, a iskaz armature i sidara na stranici (sheet) Iskaz armature, koji daje uvid u oblike i količinu armature i sidara."]
["10.","Dokaznica mjera",null,null,"(za gravitacijski zid, stavke 3. i 4.2 u Troškovniku nisu potrebne)"]
[null,"     Količine betona, armature, drenaže i ostalih materijala na stranicu (sheet) Troškovnik ulaze automatski. \n     Za proračun količina, potrebno je u Formi 6. Profil terena popuniti ćelije s plavom bojom. Ukoliko se ove vrijednosti u postojećim ćelijama ne izmijene, na stranici (sheet) Troškovnik, sve količine potrebne za izradu količina, rezultat su prethodnog proračuna. "]
["11.","Troškovnik",null,null,"(za gravitacijski zid, stavke 3. i 4.2 u Troškovniku nisu potrebne)"]
[null,"     Stranica (sheet) Troškovnik daje, nakon upisivanja jediničnih cijena, iznos troškova gradnje projektiranog potpornog zida. Ovdje je, za razliku od ostalih stranica (sheetova), moguća izmjena teksta (ćelije s plavom i crnom bojom). Stranica (sheet) je zaštićena samo u dijelu gdje podaci dolaze s drugih stranica (npr: jedinice, količina iskopa, betona, armature, sidara i sl).\n     Promjena valute izvodi se preko padajućeg menija u čeliji Q53.                                                                                                                                                  "]
["12.","Proračun i ispis dokumenta"]
[null,"     Nakon ispunjavanja svih 7 Formi i Potvrde unosa novih podataka, proračun je završen. Postupak se može, prije izlaza iz programa, ponavljati neograničeno puta.      \n  Svaki proračun može se spremiti kao \"Save as ....\", kao XLSM dokument, kao PDF dokument ili ispisati kompletni dokument s tipkom Ispis dokumenta koja se nalazi na kraju upisa svih podataka u Formi 7. Profil terena. \nIspis obuhvaća: Analizu i dimenzioniranje s nacrtom armature (10 stranica), Presjek zida (1), Tlocrt i pogled na zid (1), Iskaz armature (2) i Troškovnik (2).  Moguć je ispis i pojedine stranice (sheet). Ispisati se može i sve što se selektira, što je povoljno kada potporni zid nema konzole, sidara ili kontrafora.                                   "]
["13."," Napomene:"]
[null,"NIKADA NE SPREMAJTE RADNU KNJIGU (FILE) NA KOJOJ RADITE NA STICK S ORIGINALNIM PROGRAMOM.   \nUKOLIKO TO NAPRAVITE, PROGRAM ĆE SE BLOKIRATI BEZ MOGUĆNOSTI OPORAVKA.  SVOJU RADNU KNJIGU (UPISANE PODATKE)  SPREMAJTE NA DRUGI MEDIJ (RAČUNALO, DRUGI STICK) KAO PDF ILI SAVE AS….."]
["13.1.","    Nakon Potvrde unosa novih podataka, ukoliko se pojavi natpis o grešci, vjerojatno je došlo do greške pri upisu podataka. Za nastavak rada bez izlaska iz programa treba ići na stranicu (sheet) Start, kliknuti na Start i nakon toga pojavit će se jedna od Formi, pa je moguć normalni nastavak rada na programu."]
["13.2.","     Programom PotporniZID moguće je izraditi analizu stabilnosti i dimenzioniranje SVIH vrsta zidova bez obzira na oblik, dimenzije zida i vrstu opterećenja.                                                                                                                                                                            "]
["13.3.","     Nacrt armature prikazan je na stranici (sheet) Analiza i dimenzioniranje, a iskaz armature i sidara na stranici (sheet) Iskaz armature, koji daje uvid u oblike, dimenzije i količinu armature i sidara."]
["13.4.","     Program se otvara isključivo lozinkom po izboru autora ili zainteresirane strane. "]
["13.5.","     Ukoliko zid ima preveliku konzolu i ili prevelike sile prednaprezanja u sidrima, vlačna zona moguća je i na licu zida. Zbog toga, uz svaki dimenzionirani presjek postoji napomena o položaju glavne armature. Ista je u nacrtu armature prikazana na pravom mjestu tj. u vlačnoj zoni."]
["13.6.","     Program je testiran za \"sve\" moguće vrijednosti djelovanja, oblike i dimenzije temelja i zida.  Međutim, ukoliko korisnik tijekom rada naiđe na problem koji nije uočen tijekom testiranja, obavijestite me o tome na priloženi e-mail i problem će biti riješen u kratkom roku. Ukoliko je to greška u programu, svi korisnici programa dobit će, u zamjenu za stari, novi DVD s odgovarajućim ispravcima. \n\n                                                              \n                                                    \n\n\n                                                                \n\n\n"]
["13.7.","     Svi dijagrami i crteži mogu se promjenama vrijednosti na osima x i y, prilagoditi veličini zida pri čemu, radi realne slike, treba zadržati postojeći omjer na osima (Nacrt armature u programu je 12:7). \n     Kada na zidu nema npr. kontrafora, konzole ili sidara, crtež se može i pomaknuti na dio bez teksta, jednostavnim dodirom miša sa okvirom crteža i pomicanjem crteža na prazan prostor.\n\n\n                                                                                       \n\n\n\n\n\n\n                                                              \n                                                    \n\n\n                                                                \n\n\n"]
["13.8.","    Vertikalna komponenta potresa\nUkoliko se u analizu uključuje i vertikalna komponenta potresa, na stranici (sheet) Analiza i dimenzioniranje u ćeliju B149 upišite odgovarajuću vrijednost  (+ za djelovanje prema dole, - za djelovanje prema gore  ili 0 ukoliko analiza ne ukljućuje vertikalnu komponentu potresa) prema komentaru u ćeliji."]
[null,"Autor: Nikola Sapunar, dipl. ing. građ."]

{"sheet":"Unos podataka","index":2,"n_rows":144,"n_cols":29,"rows_kept":144,"cut":false,"hidden":true,"merged":[[0,0,0,5],[111,17,111,19],[0,24,0,26],[48,16,48,17],[49,16,49,17],[50,16,50,17],[51,16,51,17],[52,16,52,17],[58,16,58,17],[60,16,60,17],[77,16,77,17],[66,15,66,19],[83,18,83,19],[46,22,46,23],[46,16,46,17],[45,16,45,17],[1,24,1,26],[38,8,38,9],[39,8,39,9],[38,10,38,11],[39,10,39,11],[36,13,36,15],[5,13,5,14],[14,13,14,21],[21,13,21,21],[7,13,7,17],[9,7,9,8],[13,0,13,7],[2,0,2,4],[1,13,1,14],[18,9,18,11],[2,13,2,14],[3,13,3,14],[85,3,85,5],[90,3,90,5],[4,13,4,14],[35,13,35,15],[64,12,71,12],[72,12,84,12],[9,17,11,17],[106,5,106,6],[10,13,10,16],[15,9,15,11],[112,4,112,8],[109,10,109,11],[109,12,109,13],[109,14,109,16],[108,10,108,16],[89,15,89,17],[106,11,106,13],[47,16,47,17],[131,15,131,16],[117,7,117,8],[113,3,113,4],[113,5,113,6],[113,7,113,8]]}
[{"$error":"#REF!"},null,null,null,null,null,null,null,null,null,null,null,null,"Projektni pristup",{"$f":"+IF(L11=N9,N9,IF(L11=O9,O9,IF(L11=P9,2,IF(L11=Q9,Q9,R9))))","v":3},"Stupanj iskorišt.  U%","Fs","Napomena",null,null,null,null,null,null,"Ukoliko kontrafore ima u čeliju AB81 automatski dolazi upis",null,null,"DA"]
["NAZIV I STACIONAŽA ZIDA",null,null,null,null,null,null,null,null,null,null,null,null,"prevrtanje",null,{"$f":"+'Analiza i dimenzioniranje'!B179","v":{"$error":"#VALUE!"}},{"$f":"+IF(P2=\"\",\"\",1/P2)","v":{"$error":"#VALUE!"}},{"$f":"IF(P2=\"\",\"\",+IF(P2<100%,\"Zadovoljava\",\"NE zadovoljava\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+IF(AB1=\"\",\"\",\"Kontrafore\")","v":"Kontrafore"}]
["KARAKTERISTIKE TLA",null,null,null,null,"1. sloj","2. sloj","3. sloj ","tlo ispod temelja",null,null,{"$f":"+IF(L2='P X-X'!M1,\"\",\"Password?\")","v":"Password?"},null,"klizanje",null,{"$f":"+'Analiza i dimenzioniranje'!G179","v":{"$error":"#VALUE!"}},{"$f":"+IF(P3=\"\",\"\",1/P3)","v":{"$error":"#VALUE!"}},{"$f":"IF(P3=\"\",\"\",+IF(P3<100%,\"Zadovoljava\",\"NE zadovoljava\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+IF(AB1=\"\",\"\",\"duljina temelja kontrafore\")","v":"duljina temelja kontrafore"},null,{"$f":"+IF(AB1=\"\",\"\",\"lk =\")","v":"lk ="},1,{"$f":"+AB3+0.000001","v":1.0000009999999999}]
["kut unutrašnjag trenja ....................",null,null,"j","°",22,18,20,18,null,null,"ADD-Ins",null,"projektna otpornost tla",null,{"$f":"+'Analiza i dimenzioniranje'!F249","v":{"$error":"#VALUE!"}},{"$f":"+IF(P4=\"\",\"\",1/P4)","v":{"$error":"#VALUE!"}},{"$f":"IF(P4=\"\",\"\",+IF(P4<100%,\"Zadovoljava\",\"NE zadovoljava\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+IF(AB1=\"\",\"\",\"širina temelja kontrafore\")","v":"širina temelja kontrafore"},null,{"$f":"+IF(AB1=\"\",\"\",\"b =\")","v":"b ="},1,{"$f":"+AB4","v":1}]
["kohezija ...........................................",null,null,{"$f":"+'Analiza i dimenzioniranje'!C15","v":"c (kPa)"},"(kPa)",10,22,12,25,null,null,"Unos podataka",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(AB1=\"\",\"\",\"broj kontrafora sa 2 na kraju zida\")","v":"broj kontrafora sa 2 na kraju zida"},null,{"$f":"+IF(AB1=\"\",\"\",\"n =\")","v":"n ="},3,{"$f":"+AB5","v":3}]
["zapreminska težina .........................",null,null,"g","(kN/m3)",20,20,20,20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(AB1=\"\",\"\",\"širina  kontrafore\")","v":"širina  kontrafore"},null,{"$f":"+IF(AB1=\"\",\"\",\"bk=\")","v":"bk="},0.25,{"$f":"+AB6","v":0.25}]
["debljina sloja ...................................",null,null,{"$f":"+'Analiza i dimenzioniranje'!C17","v":"h (m)"},"(m)",2,2.8,{"$f":"+F41","v":1.2},null,{"$f":"+IF(O48=\"\",G7,O38-F7-H7)","v":2.8},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(AB1=\"\",\"\",\"duljina kontrafore na temelju do zida\")","v":"duljina kontrafore na temelju do zida"},null,{"$f":"+IF(AB1=\"\",\"\",\"dk=\")","v":"dk="},{"$f":"IF(AB1=\"\",\"\",+Kontrafore!E7)","v":1.9000001}]
["nagib slojeva tla ..............................",null,null,"e","°",6,4,2,{"$f":"+IF(F10>F4,F4,F10)","v":10},null,null,null,null,"FAKTORI ZA PROJEKTNE PRISTUPE  EC7",null,null,null,null,"EC8",null,null,null,null,null,{"$f":"+IF(AB1=\"\",\"\",\"visina kontrafore s temeljem\")","v":"visina kontrafore s temeljem"},null,{"$f":"+IF(AB1=\"\",\"\",\"hk=\")","v":"hk="},{"$f":"IF(AB1=\"\",\"\",+Kontrafore!E10)","v":5.5}]
["nadvišenje tla iznad zida .................",null,null,"hn","(m)",0,{"$f":"+'Analiza i dimenzioniranje'!E20","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E20","v":{"$error":"#VALUE!"}},{"$f":"+IF('Analiza i dimenzioniranje'!G55=\"\",\"\",\"Nosivost tla na kosini Ne zadovoljava\")","v":""},null,null,null,null,"1K1","1K2",2,3,"EQU","Potres","Propisi",null,null,null,null,{"$f":"+IF(AB1=\"\",\"\",\"udaljenost kontr. od ruba temelja\")","v":"udaljenost kontr. od ruba temelja"},null,{"$f":"+IF(AB1=\"\",\"\",\"l =\")","v":"l ="},{"$f":"IF(AB1=\"\",\"\",0.5)","v":0.5}]
["nagib kosine iza zida ......................  ",null,null,"b1","°",10,{"$f":"+F9+0.000001","v":9.9999999999999995E-7},"nagib padine ispred zida   b2⁰ =",null,0,null,null,null,"A1+M1+R1","A2+M2+R1","A1+M1+R2","A2+M2+R3 ","Kruta podlloga i zid ne utjeće bitno na prevrtanje, klizanje i nosivost",null,"Ovu kolonu    NE dirati","Faktori bez potresa","Naziv faktora",null,null,{"$f":"+IF(AB1=\"\",\"\",\"osni razmak kontrafora\")","v":"osni razmak kontrafora"},null,{"$f":"+IF(AB1=\"\",\"\",\"lk=\")","v":"lk="},{"$f":"IF(AB1=\"\",\"\",+Kontrafore!E8)","v":4}]
["Poissonov koeficijent .......................",null,"............................",{"$f":"+'Analiza i dimenzioniranje'!C21","v":"n"},null,0.3,{"$f":"+F10+0.000001","v":10.000000999999999},null,"j Zasipa=",30,{"$f":"+'Analiza i dimenzioniranje'!M23","v":"EC7"},3,null,"Parcijani faktori svojstava tla",null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(AB1=\"\",\"\",\"širina temelja zida\")","v":"širina temelja zida"},null,{"$f":"+IF(AB1=\"\",\"\",\"B =\")","v":"B ="},{"$f":"IF(AB1=\"\",\"\",+Kontrafore!E9)","v":2.9000021999999994}]
["prosječni modul stišljivosti tla ispod temelja  Ms (kN/m2)",null,null,null,null,8000,null,null,null,"Parcijalni faktori svojstava tla:",null,null,null,"M1","M2","M1","M2",null,null,null,null,null,null,null,{"$f":"+IF(AB1=\"\",\"\",\"visina zida s temeljem\")","v":"visina zida s temeljem"},null,{"$f":"+IF(AB1=\"\",\"\",\"H=\")","v":"H="},{"$f":"IF(AB1=\"\",\"\",+Kontrafore!E12)","v":6}]
[" Ukoliko se pritisci računaju sa Ka u čeliju F13 automatski se upisuje Ka ",null,null,null,null,"Ka","  a ako ne, Ko",null,null,"kut unutrašnjeg trenja","gj =",{"$f":"IF(L11=T9,T13,IF(L11=S9,S13,IF(L11=R9,R13,IF($L$11=$N$9,N13,IF($L$11=$O$9,O13,IF($L$11=$P$9,P13,Q13))))))","v":1.25},null,1,1.25,1,1.25,1.25,1,{"$f":"+U13","v":1.25},{"$f":"+'Analiza i dimenzioniranje'!N27","v":1.25},"gj"]
["DJELOVANJA ",null,null,null,null,null,null,null,0,"kohezija","gc =",{"$f":"IF(L11=T9,T14,IF(S9=L11,S14,IF(L11=R9,R14,IF($L$11=$N$9,N14,IF($L$11=$O$9,O14,IF($L$11=$P$9,P14,Q14))))))","v":1.25},null,1,1.25,1,1.25,1.25,1,{"$f":"+U14","v":1.25},{"$f":"+'Analiza i dimenzioniranje'!N28","v":1.25},"gc"]
["PROMETNO OPTEREĆENJE .............................",null,null,null,"Pp=",10,"kN/m2 ",{"$f":"+F15+0","v":10},null,"Parcijalni faktori djelovanja:",null,null,null,"Parcijalni faktori djelovanja"]
["širina opterećenja ................................................................."," ",null,null,"B =",3,"m",null,null,"  trajna",null,null,null,"A1","A2","A1","A2"]
["udaljenost opterećenja od vrha zida ................"," ",null,null,"x =",4.5,"m",null,null,"nepovoljna","       gG=",{"$f":"IF(L11=T9,T17,IF(S9=L11,S17,IF(L11=R9,R17,IF($L$11=$N$9,N17,IF($L$11=$O$9,O17,IF($L$11=$P$9,P17,Q17))))))","v":1},null,1.35,1,1.35,1,1.1000000000000001,1,{"$f":"+U17","v":1.1000000000000001},{"$f":"+'Analiza i dimenzioniranje'!N31","v":1.1000000000000001},"gG,dst"]
["hor. udaljenost vrha pokosa od zida ................."," ",null,null,"b =",1.5,"m",{"$f":"+F18+0.000001","v":1.5000009999999999},null,"povoljna","       gG=",{"$f":"IF(L11=T9,T18,IF(S9=L11,S18,IF(L11=R9,R18,IF($L$11=$N$9,N18,IF($L$11=$O$9,O18,IF($L$11=$P$9,P18,Q18))))))","v":1},null,1,1,1,1,0.9,1,{"$f":"+U18","v":0.9},{"$f":"+'Analiza i dimenzioniranje'!N32","v":0.9},"gG,stb"]
["OPTEREĆENJE TEMELJEM ....................",null,null,".....................................",{"$f":"+IF(A19=\"OPTEREĆENJE TEMELJEM ....................\",\"Qt=\",\" Qv=\")","v":"Qt="},120,"kN/m2 ",null,null," promjenjiva",null,null,null,"A1","A2","A1","A2"]
[{"$f":"+IF(A19=\"OPTEREĆENJE TEMELJEM ....................\",\"širina temelja .................................................................\",\"širina vozila .........................................................\")","v":"širina temelja ................................................................."}," ",null,null,{"$f":"+IF(A19=\"OPTEREĆENJE TEMELJEM ....................\",\"B =\",\" Bv=\")","v":"B ="},1,"m",null,null,"nepovoljno","       gQ=",{"$f":"IF(L11=T9,T20,IF(S9=L11,S20,IF(L11=R9,R20,IF($L$11=$N$9,N20,IF($L$11=$O$9,O20,IF($L$11=$P$9,P20,Q20))))))","v":1.3},null,1.5,1.3,1.5,1.3,1.5,1,{"$f":"+U20","v":1.5},{"$f":"+'Analiza i dimenzioniranje'!N33","v":1.5},"gQ,dst"]
[{"$f":"+IF(A19=\"OPTEREĆENJE TEMELJEM ....................\",\"duljina temelja ............................................................................\",\"duljina vozila ..................................................\")","v":"duljina temelja ............................................................................"}," ",null,null,{"$f":"+IF(A19=\"OPTEREĆENJE TEMELJEM ....................\",\"L =\",\" Lv=\")","v":"L ="},10,"m",null,null,"povoljno","       gQ=",{"$f":"IF(L11=T10,T21,IF(S10=L12,S21,IF(L12=R10,R21,IF($L$11=$N$9,N21,IF($L$11=$O$9,O21,IF($L$11=$P$9,P21,Q21))))))","v":0},null,0,0,0,0,0,0,{"$f":"+U21","v":0},{"$f":"+'Analiza i dimenzioniranje'!N34","v":0},"gQ,stb"]
[{"$f":"+IF(A19=\"OPTEREĆENJE TEMELJEM ....................\",\"dubina temeljenja (ispod vrha zida) .................................................\",\"visina vozila iznad zida  ..................................\")","v":"dubina temeljenja (ispod vrha zida) ................................................."}," ",null,null,{"$f":"+IF(A19=\"OPTEREĆENJE TEMELJEM ....................\",\"Df=\",\"vv=\")","v":"Df="},-1,"m",{"$f":"+IF(E22=\"vv=\",'Analiza i dimenzioniranje'!E20,F22)","v":-1},null,null,null,null,null,"Parcijalni faktori otpora"]
[{"$f":"+IF(A19=\"OPTEREĆENJE TEMELJEM ....................\",\"hor. udaljenost temelja od vrha zida .......................\",\"hor. udaljenost vozila od vrha zida ........................................................\")","v":"hor. udaljenost temelja od vrha zida ......................."}," ",null,null,"x =",3,"m",null,null,"Dimenzioniranje  (EC2)",null,null,null,null,"R1","R2","R3","R4"]
[{"$f":"+IF(A19=\"OPTEREĆENJE TEMELJEM ....................\",\"visina temelja .......................................................\",\"\")","v":"visina temelja ......................................................."}," ",null,null,{"$f":"+IF(A19=\"OPTEREĆENJE TEMELJEM ....................\",\"h =\",\"\")","v":"h ="},1,{"$f":"+IF(A19=\"Opterećenje temeljem ....................\",\"m\",\"\")","v":"m"},{"$f":"+IF(E24=\"\",\"\",F24)","v":1},null,"Parcijalni faktori za gradivo:",null,null,null,"prevrtanje",1,1,1,1,1,{"$f":"+U24","v":1},{"$f":"+'Analiza i dimenzioniranje'!N36","v":1}," gR"]
["LINIJSKO IZA ZIDA ........................................."," ",null,null,"PL=",20,"kN/m'",{"$f":"+F25+0.000001","v":20.000001000000001},null,"čelik","gs =",{"$f":"IF(L11=T9,T27,IF(L11=S9,S27,O27))","v":1.1499999999999999},null,"klizanje",1,1.1000000000000001,1,1,1.1000000000000001,1,{"$f":"+'Analiza i dimenzioniranje'!N37","v":1},"gR;h"]
["udaljenost opterećenja od vrha zida ................"," ",null,null,"x =",2.5,"m",null,null,"beton","gc =",{"$f":"IF(L11=T9,T28,IF(L11=S9,S28,O28))","v":1.5},null,"nosivost",1,1.4,1,1,1.4,1,{"$f":"+'Analiza i dimenzioniranje'!N38","v":1}," gR;v"]
["TOČKASTO OPTEREĆENJE .............................."," ",null,null,"PT=",20,"kN",{"$f":"+F27+0.000001","v":20.000001000000001},null,null,null,null,null,"čelik",1.1499999999999999,{"$f":"+O27","v":1.1499999999999999},{"$f":"+P27","v":1.1499999999999999},1.1499999999999999,1.1499999999999999,1.1499999999999999,{"$f":"+'Analiza i dimenzioniranje'!N41","v":1.1499999999999999},"gs"]
["udaljenost centra opterećenja od vrha zida ............."," ",null,null,"x =",1.5,"m",{"$f":"+F28-0.5","v":1},null,"Parcijalni faktori djelovanja:",null,null,null,"beton",1.5,{"$f":"+O28","v":1.5},1.5,1.5,{"$f":"+R28","v":1.5},1.5,{"$f":"+'Analiza i dimenzioniranje'!N42","v":1.5},"gc"]
["SILA U SIDRIMA (ukupna).................................",null,null,null,"PS=",{"$f":"IF(G63=\"\",0,'Analiza i dimenzioniranje'!E38)","v":-100.00000009999999},"kN/m'",null,null,"trajna","gG=",{"$f":"IF(L11=T9,T29,IF(L11=S9,S29,O29))","v":1.35},null,"stalno djelovanje",1.35,{"$f":"+O29","v":1.35},1.35,1.35,{"$f":"+R29","v":1.35},1.35,{"$f":"+'Analiza i dimenzioniranje'!N44","v":1.35},"gG"]
["otklon sidara od horizontale ............................."," ",null,null,"a =",15,"°    ",null,null,"promjenjiva","gQ=",{"$f":"IF(L11=T9,T30,IF(L11=S9,S30,O30))","v":1.5},null,"promjenjivo djelovanje",1.5,{"$f":"+O30","v":1.5},1.5,1.5,{"$f":"+R30","v":1.5},1.5,{"$f":"+'Analiza i dimenzioniranje'!N45","v":1.5},"gQ"]
["visina rezultante (iznad točke A) ......................."," ",null,null,"hs=",{"$f":"+'Analiza i dimenzioniranje'!E40","v":3.9999999960000001},"m",null,null,"Voda ispred zida",null,null,null,null,null,null,0,0]
["NPV IZA ZIDA .................................................."," ",null,null,"hw=",0.6,"m",null,null,0.8]
["POTRES (y)  Fwy=SG*kh ....................................."," ",null,null,"Fwy=",{"$f":"+'Analiza i dimenzioniranje'!E43","v":{"$error":"#VALUE!"}},"kN/m'"]
[" kh= amax*S/r","r=",{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},null,"amax =",0.1,"S=",1]
[" Ukoliko se zid računa s potresom, u čeliju F34 se autom upisuje vrijednost amax>0 a ako NE, u čeliju F34, upisuje 0."]
["DIMENZIJE ZIDA",null,null,null,null,{"$f":"-G38","v":-4},null,null,null,null,null,null,null,"Masivni zid"]
["visina zida i temelja ..........................................."," ",null,null,"H =",{"$f":"+'Analiza i dimenzioniranje'!E48","v":6},"m",null,null,null,null,null,null,"prema Švicarskim propisima"]
["dužina zida ........................................................"," ",null,null,"L =",12,{"$f":"+IF(G39=0,0.000001,G39)","v":4},null,null,null,null,null,null,"H =",6,"m"]
["otklon zida uz tlo od vertikale............................"," ",null,null," b =",4,{"$f":"IF(O48=\"DA\",0,+F39)","v":4},null,"Crtež kontrafore",null,"Crtež kontrafore kada zid ide od 0 a ne od 2",null,null,"b =",0,"°    "]
["visina temelja prema padini ..............................",null,null,null,"hA=",0.7,{"$f":"+IF(O48=\"DA\",O40,F40)","v":0.7},null,"Temelj kontrafore",null,"Temelj kontrafore",null,null,"hA=",{"$f":"ROUND((O41-(O43+O44-G49)/5),2)","v":1.06},"m"]
["visina temelja prema zasipu .............................",null,null,null,"hB=",1.2,{"$f":"+IF(O48=\"DA\",O41,F41)","v":1.2},null,{"$f":"IF(AB1=\"\",0,'C III-V'!B3+G49)","v":2},{"$f":"IF(AB1=\"\",0,IF(Kontrafore!E1=\"\",'C III-V'!C2,(('Analiza i dimenzioniranje'!E52-'Analiza i dimenzioniranje'!E51)-('Analiza i dimenzioniranje'!E61*'Analiza i dimenzioniranje'!E52-'Analiza i dimenzioniranje'!E61*'Analiza i dimenzioniranje'!E51)/('Analiza i dimenzioniranje'!E61+'Unos podataka'!AC3))))","v":0.12820515121628623},{"$f":"IF('Analiza i dimenzioniranje'!A83=\"\",0,+I41-2)","v":0},{"$f":"+J41","v":0.12820515121628623},null,"hB=",{"$f":"+(0.28*O38)","v":1.6800000000000002},"m"]
["nagib dna temelja  ..................................................                  "," ",null,"1: n2 .....","n2=",{"$f":"+'Analiza i dimenzioniranje'!E53","v":7.8000043999999988},null,null,{"$f":"IF(I41=0,0,'C III-V'!B3)","v":2},{"$f":"IF(AB1=\"\",0,'C III-V'!C3)","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!A83=\"\",0,+I42-2)","v":0},{"$f":"+J42","v":1.2},null,"d =",1.4,"m"]
["širina zida u kruni .............................................."," ",null,null,"d =",0.6,{"$f":"+IF(O48=\"DA\",O42,F43)","v":0.6},null,{"$f":"2+F50-MT!G13","v":1.75},{"$f":"IF(AB1=\"\",0,J42)","v":1.2},{"$f":"+I43-2","v":-0.25},{"$f":"+J43","v":1.2},null,"d1=",{"$f":"ROUND(O42+0.144*O38,2)","v":2.2599999999999998},"m"]
["širina zida na temelju ........................................"," ",null,null,"d1=",0.8,{"$f":"+IF(O48=\"DA\",O43,F44)","v":0.8},null,{"$f":"+I45-'Analiza i dimenzioniranje'!$E$60","v":1},{"$f":"+J43","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!A83=\"\",0,+I44-2)","v":-1},{"$f":"+J44","v":1.2},null,"b1=",{"$f":"0.14*O38","v":0.84000000000000008},"m"]
["nagib lica zida ................................................."," ",null," n1: 1 .....","n1=",{"$f":"+'Analiza i dimenzioniranje'!E56","v":{"$error":"#VALUE!"}},null,null,{"$f":"2-Kontrafore!$E$3+'Analiza i dimenzioniranje'!$E$60","v":1},{"$f":"+L45","v":0},{"$f":"+I45-2","v":-1},0,null,"b2=",0,"m"]
["nagib zida  uz tlo .........................................................."," ",null," n3: 1 .....","n3=",{"$f":"+IF(G46>100,\">100\",G46)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F57","v":{"$error":"#VALUE!"}},null,{"$f":"IF(AB1=\"\",0,I43+G49)","v":1.75},{"$f":"+Kontrafore!B17","v":9.6153895463470418E-2},{"$f":"IF('Analiza i dimenzioniranje'!A83=\"\",0,+I46-2)","v":-0.25},{"$f":"+J46","v":9.6153895463470418E-2},null," n =",{"$f":"+O41/5","v":0.33600000000000002},"m","Sidra",null,"1. ","2.","3.","4."]
["širina temelja ispred zida .................................."," ",null,null,"b1=",0.7,{"$f":"IF(O48=\"DA\",O44,+F47+0.000001)","v":0.70000099999999998},null,{"$f":"+I41","v":2},{"$f":"+J41","v":0.12820515121628623},{"$f":"+K41","v":0},{"$f":"+J47","v":0.12820515121628623},null,null,"DA ili NE","kut otklona temelja od vertikale","visina sidra od dna temelja",null,{"$f":"IF(G63=\"DA\",F67,0)","v":5},{"$f":"IF(G63=\"DA\",G67,0)","v":3},{"$f":"IF(G63=\"DA\",H67,0)","v":0},{"$f":"IF(G63=\"DA\",I67,0)","v":0}]
["širina temelja iza zida ......................................."," ",null,null,"b2=",1.4,{"$f":"IF(O48=\"DA\",O45,+F48+0.0000001)","v":1.4000001},null,"Rebro kontrafore",null,null,null,null,null,null,{"$f":"IF(O48=\"\",0,ATAN(+O46/O41)*180/PI())","v":0},"slobodna dionica",null,{"$f":"IF(G63=\"DA\",F68,0)","v":5.9},{"$f":"IF(G63=\"DA\",G68,0)","v":4.9000000000000004},{"$f":"IF(G63=\"DA\",H68,0)","v":0},{"$f":"IF(G63=\"DA\",I68,0)","v":0}]
["nagib temeljne plohe uz tlo ........................",null,null,"hB: n .....","n =",0,{"$f":"+IF(O48=\"DA\",O46,F49)","v":0},null,{"$f":"IF(AB1=\"\",0,+'C III-V'!B4-Kontrafore!E11)","v":1.5000010000000001},{"$f":"IF(AB1=\"\",0,J42)","v":1.2},{"$f":"+I49-2","v":-0.49999899999999986},{"$f":"+J49","v":1.2},null,null,null,null,"sidrišna dionica dionica",null,{"$f":"IF(G63=\"DA\",F69,0)","v":6.7},{"$f":"IF(G63=\"DA\",G69,0)","v":4.8},{"$f":"IF(G63=\"DA\",H69,0)","v":0},{"$f":"IF(G63=\"DA\",I69,0)","v":0}]
["ukupna širina temelja ........................................"," ",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m",null,{"$f":"+I49","v":1.5000010000000001},{"$f":"IF(J49=0,0,J49+0.5)","v":1.7},-0.49999899999999986,1.7,null,null,{"$f":"+'Analiza i dimenzioniranje'!L462","v":2.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!M462","v":1.2},"sila prednaprezanja",null,{"$f":"IF(G63=\"DA\",F70,0)","v":50},{"$f":"IF(G63=\"DA\",G70,0)","v":50},{"$f":"IF(G63=\"DA\",H70,0)","v":0},{"$f":"IF(G63=\"DA\",I70,0)","v":0}]
["zapreminska težina zida i temelja......................"," ",null,null,"gb=",25,"kN/m3 ",null,{"$f":"IF(AB1=\"\",0,IF(G39=0,I52-0.5,IF(AB1=\"\",0,IF(G39=0,I53-0.5,(2+'Analiza i dimenzioniranje'!E59-('Analiza i dimenzioniranje'!E48-'Analiza i dimenzioniranje'!E52-0.5)/'Analiza i dimenzioniranje'!F57))-0.5)))","v":{"$error":"#VALUE!"}},{"$f":"IF(AB1=\"\",0,IF(I51=0,0,IF(F9>=0,F37-0.5,IF(AB1=\"\",0, 'Analiza i dimenzioniranje'!$E$48-0.5+F9))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,{"$f":"+'Analiza i dimenzioniranje'!L461","v":5},{"$f":"+'Analiza i dimenzioniranje'!M461","v":1.2},"nosivost sidra",null,{"$f":"+'Analiza i dimenzioniranje'!P26","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Q26","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!R26","v":""},{"$f":"+'Analiza i dimenzioniranje'!S26","v":""}]
["zapreminska težina zasipa (drenaže i klina)......."," ",null,null,"gz=",20,"kN/m3 ",null,{"$f":"IF(G39=0,I53,+I53-(J52-J54)/G46)","v":{"$error":"#VALUE!"}},{"$f":"+J51","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,null,"razmak sidara",null,{"$f":"+'Analiza i dimenzioniranje'!P27","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Q27","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!R27","v":""},{"$f":"+'Analiza i dimenzioniranje'!S27","v":""},{"$f":"+'Analiza i dimenzioniranje'!T26","v":""}]
["debljina zasipa (drenaže) iza zida ....................."," ",null,null,"d =",0.5,"m",null,{"$f":"+IF(AB1=\"\",0,+'C III-V'!$AE$108)","v":3.4000000999999997},{"$f":"IF(AB1=\"\",0,+'C III-V'!$AF$108)","v":1.2},1.4000000999999997,1.2,null,null,null,null,"Minimalna duljina slobodne dionice",null,{"$f":"+'Analiza i dimenzioniranje'!P28","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Q28","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!R28","v":""},{"$f":"+'Analiza i dimenzioniranje'!S28","v":""},{"$f":"+'Analiza i dimenzioniranje'!T27","v":""}]
["visina nasipa na temelju ispred zida ................."," ",null,null,"hn=",0.3,{"$f":"+F54+0.000001","v":0.30000099999999996},null,{"$f":"+I49","v":1.5000010000000001},{"$f":"+J49","v":1.2},-0.49999899999999986,1.2]
["zapreminska težina nasipa ..............................."," ",null,null,"gn=",20,"kN/m3 ",null,null,null,null,{"$f":"+T59","v":""},null,null,null,"tg",{"$f":"+I8","v":10},{"$f":"+TAN(Q55*PI()/180)","v":0.17632698070846498},{"$f":"IF(T55=T56,S56,'C III-V'!U7)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!V7","v":6},{"$f":"+'Analiza i dimenzioniranje'!F95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!G94","v":6}]
[null,null,"Ukoliko zid ima konzolu u čeliju G57 automatski se upisuje  DA a ako konzole nema, čelija se briše sa DELETE",null,null,null,null,null,null,null,null,{"$f":"+T60","v":""},null,null,null,null,"rač. nadviš h=",{"$f":"IF(F8<=F4,0,IF(H15>0,(T57-T56)-H18*R55,X60-R55*(-X59+S56)-T55))","v":0},{"$f":"2+G48-(T56-F41)/G46","v":{"$error":"#VALUE!"}},{"$f":"IF(H15=0,+'C III-V'!V8,'C III-V'!V8)","v":6},{"$f":"+'Analiza i dimenzioniranje'!F98","v":-8},{"$f":"+T56+(U55-U56)*TAN(F10*PI()/180)","v":{"$error":"#VALUE!"}}]
["KONZOLA",null,null,null,null,null,"DA",null,null,null,null,null,null,null,null,"tg",{"$f":"+F10","v":10},{"$f":"+TAN(Q57*PI()/180)","v":0.17632698070846498},null,{"$f":"IF(F12<F4,T56+H18*+R57,IF(H15=0,T56+H18*TAN(F10*PI()/180),T56+H18*TAN(F10*PI()/180)))","v":6.2644906473896782}]
["duljina konzole (zida) .............................................................."," ",null,{"$f":"+IF(G57=0,\"\",\"............................\")","v":"............................"},"lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},{"$f":"+'Analiza i dimenzioniranje'!F78","v":"m"},"F37/2=",{"$f":"+'Analiza i dimenzioniranje'!E48/2","v":3},null,null,null,null,null,null,"tg",{"$f":"+Q57-Q55","v":0},{"$f":"+TAN(Q58*PI()/180)*(S55-'C III-V'!AE104)","v":{"$error":"#VALUE!"}},-8,{"$f":"IF(H15>0,T57,V56)","v":6.2644906473896782}]
["visina podgleda konzole (od dna temelja) ............"," ",null,null,"vk=",3.14,{"$f":"+'Analiza i dimenzioniranje'!F81","v":"m"},{"$f":"+F59","v":3.14},null,null,null,null,null,null,null,null,"Nadvišenje terena kada ima prometa",null,{"$f":"IF('Unos podataka'!F9>0,+S55,\"\")","v":""},{"$f":"+IF(F9>0,'Analiza i dimenzioniranje'!G94,\"\")","v":""}]
["širina konzole .................................................",null,null,{"$f":"+IF(G57=\"\",\"\",\"................\")","v":"................"},"bk=",1,{"$f":"+'Analiza i dimenzioniranje'!F79","v":"m"},null,null,"MASA ZIDA I TEMELJA ZA UZGON",null,null,null,null,null,null,{"$f":"IF(H15>0,(T57-T55)+'Unos podataka'!R58,'Unos podataka'!R58)","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(F9<=0,\"\",S55)","v":""},{"$f":"+IF(F9<=0,\"\",T55)","v":""}]
["visina presjeka konzole ..................................",null,null,{"$f":"+IF(G57=\"\",\"\",\"................\")","v":"................"},"hk=",0.3,{"$f":"+'Analiza i dimenzioniranje'!F80","v":"m"},null,null,null,null,null,null,null,null,null,"Linija terena s prometom"]
[null,null," Ukoliko zid ima sidra u čeliju G63automatski se upisuje  DA a ako sidara nemabrisati sa DELETE.",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!E24=0,'Analiza i dimenzioniranje'!L457,S55-2)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E24=0,'Analiza i dimenzioniranje'!M457,T55)","v":6}]
["SIDRA       ",null,null,null,null,null,"DA",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!E24=0,'Analiza i dimenzioniranje'!L457,S56-2)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E24=0,'Analiza i dimenzioniranje'!M457,T56)","v":6}]
[{"$f":"+IF(G63=\"\",\"\",\"promjer injektirane bušotine .............................\")","v":"promjer injektirane bušotine ............................."}," ",null,null,"d≈",0.1,"m",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!E24=0,'Analiza i dimenzioniranje'!L457,+B105-2)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E24=0,'Analiza i dimenzioniranje'!M457,+T57)","v":6.2644906473896782}]
[{"$f":"+IF(G63=\"\",\"\",\"faktor sigurnosti ( za dop. opt. sidra) ................ \")","v":"faktor sigurnosti ( za dop. opt. sidra) ................ "}," ",null,null,"gs=",2,null,null,null,null,null,null,"Padajući menu za klase betona",20,null,null,{"$f":"IF('Analiza i dimenzioniranje'!E24=0,'Analiza i dimenzioniranje'!L456,Q64-8)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E24=0,'Analiza i dimenzioniranje'!M456,T58)","v":6.2644906473896782}]
[{"$f":"+IF(G63=\"\",\"\",\"  Nosivost i razmak sidara\")","v":"  Nosivost i razmak sidara"},null,null,null," ","I. red","II. red","III. red","IV. red",null,null,null,null,25,null,null,{"$f":"IF('Analiza i dimenzioniranje'!E24=0,'Analiza i dimenzioniranje'!L456,Q65-3)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Analiza i dimenzioniranje'!E24=0,'Analiza i dimenzioniranje'!M456,R65+3)","v":9.2644906473896782}]
[{"$f":"+IF(G63=\"\",\"\",\"visina sidra od dna temelja (m) ..........................\")","v":"visina sidra od dna temelja (m) .........................."}," ",null,null,"hs=",5,3,null,null,null,null,null,null,30,null,"Koordinate točaka pravaca",null,null,null,null,null,"Linija terena"]
[{"$f":"+IF(G63=\"\",\"\",\"duljina slobodne dionice  (m) .............................\")","v":"duljina slobodne dionice  (m) ............................."}," ",null,null,"lsl=",5.9,4.9000000000000004,null,null,null,null,null,null,37,null,"x=",{"$f":"+Q65","v":{"$error":"#VALUE!"}},{"$f":"+Q66","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!L455","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!M455","v":{"$error":"#VALUE!"}},null,{"$f":"IF(H15>0,S56-H18,X59)","v":{"$error":"#VALUE!"}},{"$f":"+T57","v":6.2644906473896782}]
[{"$f":"+IF(G63=\"\",\"\",\"duljina sidrišne dionice  (m) ................................\")","v":"duljina sidrišne dionice  (m) ................................"}," ",null,null,"lsidr=",6.7,4.8,null,null,null,null,null,null,45,null,"Y=",{"$f":"+R65","v":6.2644906473896782},{"$f":"+R66","v":9.2644906473896782},{"$f":"+'Analiza i dimenzioniranje'!L456","v":-21.16},{"$f":"+'Analiza i dimenzioniranje'!M456","v":{"$error":"#VALUE!"}},null,{"$f":"+S56","v":{"$error":"#VALUE!"}},{"$f":"IF(F8<=F4,T56,IF(H15>0,#REF!,+#REF!+R56))","v":6}]
[{"$f":"IF(G63=\"\",\"\",IF(T49>0,\"sile u sidrima (kN) ..............................................\",\"sila u sidru (kN) ......................................................\"))","v":"sile u sidrima (kN) .............................................."}," ",null,null,"Ps=",50,50,null,null,null,null,null,null,50,null,"Jednadžbe pravaca",null,null,null,"x","y",{"$f":"+S55","v":{"$error":"#VALUE!"}},{"$f":"'C III-V'!C9","v":"A"}]
[{"$f":"+IF(G63=\"\",\"\",\"Dop. opterećenje sidra .................................... \")","v":"Dop. opterećenje sidra .................................... "}," ",null,null,"Pdop=",{"$f":"+'Analiza i dimenzioniranje'!D74","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E74","v":{"$error":"#VALUE!"}},{"$f":"+IF(H70=\"\",\"\",'Analiza i dimenzioniranje'!F74)","v":""},{"$f":"+'Analiza i dimenzioniranje'!G74","v":""},null,null,null,null,55,null,"Y=",{"$f":"(R69-Q69)/(R68-Q68)","v":{"$error":"#VALUE!"}},"*x             +",{"$f":"-Q71*Q68+Q69","v":{"$error":"#VALUE!"}},{"$f":"+Q65","v":{"$error":"#VALUE!"}},{"$f":"Q71*T71+S71","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(G63=\"\",\"\",\"Razmak sidara .................................................\")","v":"Razmak sidara ................................................."}," ",null,null,"b<",{"$f":"IF(G63=\"\",\"\",'Analiza i dimenzioniranje'!P27)","v":{"$error":"#VALUE!"}},{"$f":"IF(G63=\"\",\"\",'Analiza i dimenzioniranje'!Q27)","v":{"$error":"#VALUE!"}},{"$f":"IF(G63=\"\",\"\",'Analiza i dimenzioniranje'!R27)","v":""},{"$f":"IF(G63=\"\",\"\",'Analiza i dimenzioniranje'!S27)","v":""},{"$f":"IF(G63=\"\",\"\",'Analiza i dimenzioniranje'!T27)","v":""},null,null,null,60,null,"Y=",{"$f":"+(T69-T68)/(S69-S68)","v":{"$error":"#VALUE!"}},"*x             +",{"$f":"-Q72*S69+T69","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!L455","v":{"$error":"#VALUE!"}},{"$f":"Q72*T72+S72","v":{"$error":"#VALUE!"}}]
["Minimalna duljina slobodne dionice ......................"," ",null,null,"lsl>=",{"$f":"+'Analiza i dimenzioniranje'!P28","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Q28","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!R28","v":""},{"$f":"+'Analiza i dimenzioniranje'!S28","v":""},{"$f":"+'Analiza i dimenzioniranje'!T28","v":""},null,null,"Padajući menu za profil armatuire",8,null,"sjecište"]
["Padajući menu",null,null,null,null,null,null,null,null,null,null,null,null,10,null,"X=",{"$f":"IF('Analiza i dimenzioniranje'!E24=0,'Unos podataka'!S69,-(S72-S71)/(1+Q72))","v":{"$error":"#VALUE!"}},"Y=",{"$f":"IF('Analiza i dimenzioniranje'!E24=0,'Unos podataka'!T69,+Q71*Q74+S71)","v":{"$error":"#VALUE!"}}]
["OPTERECENJE TEMELJEM ............................",null,null,null,null,null,null,null,null,null,null,null,null,12,null,"X=",{"$f":"+Q65","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+R65","v":6.2644906473896782}]
["OPTERECENJE VOZILOM ..............................",null,null,null,"Rezultat",null,null,null,null,null,null,null,null,14,null,"X=",{"$f":"IF('Analiza i dimenzioniranje'!E24=0,'Unos podataka'!Q75,+Q64)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"IF('Analiza i dimenzioniranje'!E24=0,'Unos podataka'!S75,+R64)","v":6.2644906473896782}]
[null,null,null,null,"Projektni pristup",null,"Stupanj iskorištenost","Fs","Napomena",null,null,null,null,16,null,"X=",{"$f":"+S55-2","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+T56","v":6}]
[null,null,null,null,"prevrtanje",null,{"$f":"+'Analiza i dimenzioniranje'!B179","v":{"$error":"#VALUE!"}},{"$f":"100/G78/100","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C179","v":"(Zadovoljava)       "},null,null,null,null,18,null,null,"Koordinate točaka pravaca"]
[null,null,null,null,"klizanje",null,{"$f":"+'Analiza i dimenzioniranje'!G179","v":{"$error":"#VALUE!"}},{"$f":"100/G79/100","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!H179","v":{"$error":"#VALUE!"}},null,null,null,null,20,null,"x=",{"$f":"+'Analiza i dimenzioniranje'!Y538","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y539","v":-1}]
[null,null,null,null,"projektna otpornost tla",null,{"$f":"+'Analiza i dimenzioniranje'!F249","v":{"$error":"#VALUE!"}},{"$f":"100/G80/100","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!G249","v":{"$error":"#VALUE!"}},null,null,null,null,22,null,"Y=",{"$f":"+'Analiza i dimenzioniranje'!Z538","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z539","v":1.2}]
["GRADIVO",null,null,null,null,null,null,null,null,null,null,null,null,25,null,"Jednadžbe pravaca",null,null,null,"x","y"]
["Beton","Temelj",null,{"$f":"+IF(G57=\"\",\"Zid\",\"Zid i konzola\")","v":"Zid i konzola"},null,null,null,null,null,null,null,null,null,28,null,"Y=",{"$f":"(R80-Q80)/(R79-Q79)","v":{"$error":"#VALUE!"}},"*x             +",{"$f":"-Q82*Q79+Q80","v":{"$error":"#VALUE!"}},{"$f":"-(S82-U82)/Q82","v":{"$error":"#VALUE!"}},{"$f":"+R65","v":6.2644906473896782}]
["    Razred    C ",{"$f":"IF(B84=20,16,IF(B84=25,20,IF(B84=30,25,IF(B84=37,30,IF(B84=45,35,IF(B84=50,40,IF(B84=55,45,IF(B84=60,50,\"\"))))))))","v":25},"C ",{"$f":"IF(D84=20,16,IF(D84=25,20,IF(D84=30,25,IF(D84=37,30,IF(D84=45,35,IF(D84=50,40,IF(D84=55,45,IF(D84=60,50,\"\"))))))))","v":30},null,null,null,null,null,null,null,null,null,32]
[null,30,null,37,null,null,null,null,"MASA ZIDA I TEMELJA ZA UZGON",null,null,null,null,36,null,"Jednadžba pravca"," točke  6 i 7",null,"jednadžba pravca privremenog iskopa"]
["  Armatura",null,null,null,null,null,null,null,null,null,null,null,null,40,null,"x=",{"$f":"+K117","v":-2},{"$f":"+K118","v":5},0,{"$f":"+K112","v":{"$error":"#VALUE!"}}]
["  Temelj",null,null,"Zarebrastu armaturu u čeliju G86 dolazi  iz VBA   RA a za mreže MA",null,null,"RA",null,null,null,null,null,null,null,null,"Y=",{"$f":"+L117","v":7},{"$f":"+L118","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+L112","v":{"$error":"#VALUE!"}}]
[null,{"$f":"IF(+G86=\"RA\",\"šipka\",\"mreža\")","v":"šipka"},"B500B",{"$f":"+'Analiza i dimenzioniranje'!J48","v":""},null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"(R86-Q86)/(R85-Q85)","v":-0.82857142857142851},"*x              +",{"$f":"-Q87*Q85+Q86","v":5.3428571428571434}," "]
[null,"Glavna","kom/m' zida",null,"Razdjelna","razmak",null,null,null,null,null,null,null,null,null,"Y=",{"$f":"-(T86-S86)/(S85-T85)","v":{"$error":"#VALUE!"}},"*x              +",{"$f":"-(S85*Q88-S86)","v":{"$error":"#VALUE!"}}," "]
["f",14,{"$f":"+'Analiza i dimenzioniranje'!P52","v":0},"f",8,40,"cm",null,null,null,null,null,null,null,null,"X=",{"$f":"+(S88-S87)/(Q87-Q88)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+Q88*Q89+S88","v":{"$error":"#VALUE!"}}]
["f",14,{"$f":"+'Analiza i dimenzioniranje'!P55","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,"koord. pravac 2-sjecište s prometom"]
["  Zid",null,null,"Za rebrastu armaturu u čeliju G91 dolazi  iz VBA   RA a za mreže MA",null,null,"RA",null,null,null,null,null,null,null,null,"x=",{"$f":"+Q74","v":{"$error":"#VALUE!"}},{"$f":"+Troškovnik!AC73","v":-21.16}]
[null,{"$f":"IF(+G91=\"RA\",\"šipka\",\"mreža\")","v":"šipka"},"B500B",{"$f":"+'Analiza i dimenzioniranje'!J52","v":""},null,null,null,null,null,null,null,null,null,null,null,"y=",{"$f":"+S74","v":{"$error":"#VALUE!"}},{"$f":"+Troškovnik!AC74","v":{"$error":"#VALUE!"}}]
[null,"Glavna","kom/m' zida",null,"Razdjelna","razmak"]
["f",12,{"$f":"+'Analiza i dimenzioniranje'!P58","v":{"$error":"#VALUE!"}},"f",{"$f":"+E89","v":8},40,"cm"]
[{"$f":"+IF(G57=\"\",\"\",\"  Konzola\")","v":"  Konzola"},"šipka","B500B"]
[null,{"$f":"+IF(G57=\"\",\"\",\"Glavna\")","v":"Glavna"},{"$f":"+IF(G57=\"\",\"\",\"kom/m' zida\")","v":"kom/m' zida"},null,{"$f":"+IF(G57=\"\",\"\",\"Razdjelna\")","v":"Razdjelna"},{"$f":"+IF(G57=\"\",\"\",\"razmak\")","v":"razmak"}]
[{"$f":"+IF(G57=\"\",\"\",\"f\")","v":"f"},12,{"$f":"+'Analiza i dimenzioniranje'!P67","v":{"$error":"#VALUE!"}},{"$f":"+IF(G57=\"\",\"\",\"f\")","v":"f"},{"$f":"+E94","v":8},40,"cm"]
[]
["Zaštitni sloj        d=",null,5,"cm"]
[]
["Pukotine -ograničenje",null,0.3,"mm"]
["Koordinate površine i slojeva tla "]
["Teren",{"$f":"B104-(C103-C104)/G46","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$E$48","v":6},"Koordinate  klizne plohe",null,null,null,"Površina i volumen tla iznad zida"]
[null,{"$f":"+V69","v":{"$error":"#VALUE!"}},{"$f":"+T55","v":6},"j1=",{"$f":"+'Unos podataka'!F4","v":22}]
[null,{"$f":"S56-H18","v":{"$error":"#VALUE!"}},{"$f":"+W68","v":6.2644906473896782},"j2=",{"$f":"+'Unos podataka'!G4","v":18},"x","y"]
[null,-8,{"$f":"IF(F9<0,C105,IF('Analiza i dimenzioniranje'!$E$24=0,'Unos podataka'!G106,IF(C104<C103,C105-'Analiza i dimenzioniranje'!$E$20,IF('Analiza i dimenzioniranje'!$E$24=0,'Unos podataka'!C104-('Unos podataka'!B106-'Unos podataka'!B103)*TAN('Analiza i dimenzioniranje'!$H$20*PI()/180),'Unos podataka'!C105))))","v":6.2644906473896782},"j3=",{"$f":"+'Unos podataka'!H4","v":20},{"$f":"+B106","v":-8},{"$f":"+C105+TAN('Analiza i dimenzioniranje'!$H$20*PI()/180)*(B105-B106)","v":{"$error":"#VALUE!"}}]
["sloj 1. ",{"$f":"+'C III-V'!B29","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E48-'Analiza i dimenzioniranje'!D17","v":4},null,null,null,null,null,null,"m=",1.5,"Nagib iskopa iza zida m:1   "]
[null,-8,{"$f":"'Unos podataka'!C107+('Unos podataka'!B107-'Unos podataka'!B108)*TAN('Analiza i dimenzioniranje'!D18*PI()/180)","v":{"$error":"#VALUE!"}}]
["Sloj 2.",2,{"$f":"+'Analiza i dimenzioniranje'!$F$17","v":1.2},null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!K454","v":"Oznaka točke"},"Koordinate točaka"]
[null,-8,{"$f":"+C109+(B109-B110)*TAN('Analiza i dimenzioniranje'!$E$18*PI()/180)","v":1.8992681194351042},null,null,null,null,null,null,null,"TEREN i iskop",null,"Zid",null,"Koordinate zida -  zida ide od 0 a ne od 2 (crtež za troškovnik)"]
["Sloj 3.",2,0,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!L454","v":"x"},{"$f":"+'Analiza i dimenzioniranje'!M454","v":"y"},"x","y","točke \nna zidu","x","y"]
[null,{"$f":"+B110","v":-8},{"$f":"+C111+(B111-B112)*TAN('Analiza i dimenzioniranje'!$F$18*PI()/180)","v":0.34920769491747727},null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!K455","v":1},{"$f":"+'Analiza i dimenzioniranje'!L455","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!M455","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!B2","v":2},{"$f":"+'C III-V'!C2","v":0.12820515121628623},2,{"$f":"+'C III-V'!$B$2-2","v":0},{"$f":"+'C III-V'!C2","v":0.12820515121628623},"Jednadžba  projektiranog pokosa iza zida"]
["horizontala na vrhu zida",null,null,null,"Jednadžbe pravaca terena i klizne plohe iza zia",null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!K456","v":2},{"$f":"+'Analiza i dimenzioniranje'!L456","v":-21.16},{"$f":"+'Analiza i dimenzioniranje'!M456","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!B3","v":2},{"$f":"+'C III-V'!C3","v":1.2},3,{"$f":"+'C III-V'!B3-2","v":0},{"$f":"+'C III-V'!C3","v":1.2},"x=",{"$f":"+P119","v":{"$error":"#VALUE!"}},{"$f":"+K113","v":-21.16}]
[-5,{"$f":"+C104","v":6},"Točke","Horizontala",null,"Teren",null,"Klizna",null,{"$f":"+'Analiza i dimenzioniranje'!K457","v":3},-15,9.5,{"$f":"+'C III-V'!B4","v":3.4000010999999999},{"$f":"+'C III-V'!C4","v":1.2},4,{"$f":"+'C III-V'!B4-2","v":1.4000010999999999},{"$f":"+'C III-V'!C4","v":1.2},"y=",{"$f":"+Q119","v":"A"},{"$f":"S114-TAN(V114*PI()/180)*(T113-S113)","v":{"$error":"#VALUE!"}},"b =",{"$f":"+'Analiza i dimenzioniranje'!H20","v":10.000000999999999},"o"]
[{"$f":"+B103","v":{"$error":"#VALUE!"}},{"$f":"+C103","v":6},null,"T1  ","T2","T3","T4","T5","T6",{"$f":"+'Analiza i dimenzioniranje'!K458","v":4},-10,9,{"$f":"+'C III-V'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C5","v":3.14},5,{"$f":"+'C III-V'!B5-2","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C5","v":3.14},"Y=",{"$f":"(T114-S114)/(T113-S113)","v":{"$error":"#VALUE!"}},"*x       +",{"$f":"-S115*S113+S114","v":{"$error":"#VALUE!"}}]
[null,null,"x=",{"$f":"+A114","v":-5},{"$f":"+A115","v":{"$error":"#VALUE!"}},{"$f":"+B105","v":{"$error":"#VALUE!"}},{"$f":"+B106","v":-8},{"$f":"+H121","v":-1.0572404418349119},{"$f":"+H122","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!K459","v":5},-4,8,{"$f":"+'C III-V'!B6","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C6","v":3.14},6,{"$f":"+'C III-V'!B6-2","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C6","v":3.14}]
[null,null,"Y=",{"$f":"+B114","v":6},{"$f":"+B115","v":6},{"$f":"+C105","v":6.2644906473896782},{"$f":"+C106","v":6.2644906473896782},4.2,{"$f":"+I122","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!K460","v":6},-2,7,{"$f":"+'C III-V'!B7","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C7","v":3.44},7,{"$f":"+'C III-V'!B7-2","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C7","v":3.44}]
[null,null,"Y=",{"$f":"-(I117-H117)/(H116-I116)","v":{"$error":"#VALUE!"}},"* x        +",{"$f":"-(H116*D118-H117)","v":{"$error":"#VALUE!"}},"Klizna","Klizna ploha",null,{"$f":"+'Analiza i dimenzioniranje'!K461","v":7},5,1.2,{"$f":"+'C III-V'!B8","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C8","v":3.44},8,{"$f":"+'C III-V'!B8-2","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C8","v":3.44}]
[null,null,"Y=",{"$f":"-(G117-F117)/(F116-G116)","v":{"$error":"#VALUE!"}},"* x        +",{"$f":"-(F116*D119-F117)","v":{"$error":"#VALUE!"}},"Teren",{"$f":"+'Analiza i dimenzioniranje'!$A94","v":1.75},{"$f":"+'Analiza i dimenzioniranje'!$B94","v":0},{"$f":"+'Analiza i dimenzioniranje'!K462","v":8},{"$f":"+'Analiza i dimenzioniranje'!L462+G49","v":2.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!M462","v":1.2},{"$f":"+'C III-V'!B9","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C9","v":"A"},9,{"$f":"+'C III-V'!B9-2","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C9","v":"A"}]
[null,null,"X=",{"$f":"+(F119-F118)/(D118-D119)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+D119*D120+F119","v":{"$error":"#VALUE!"}},"Klizna teren",{"$f":"+'Analiza i dimenzioniranje'!$A95","v":0.97707863658009864},{"$f":"+'Analiza i dimenzioniranje'!$B95","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!K463","v":9},{"$f":"+'Analiza i dimenzioniranje'!L463+G49","v":2.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!M463","v":0.5},{"$f":"+'C III-V'!B10","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C10","v":"A"},10,{"$f":"+'C III-V'!B10-2","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C10","v":"A"}]
[null,null,"Y=",{"$f":"(E117-D117)/(E116-D116)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-D121*D116+D117","v":{"$error":"#VALUE!"}},"Horizontala",{"$f":"+'Analiza i dimenzioniranje'!$A96","v":-1.0572404418349119},{"$f":"+'Analiza i dimenzioniranje'!$B96","v":4},{"$f":"+'Analiza i dimenzioniranje'!K464","v":10},{"$f":"+G49","v":0},{"$f":"+'Analiza i dimenzioniranje'!M464","v":0},{"$f":"+'C III-V'!B11","v":4.2000010999999997},{"$f":"+'C III-V'!C11","v":1.2},11,{"$f":"+'C III-V'!B11-2","v":2.2000010999999997},{"$f":"+'C III-V'!C12","v":1.2}]
[null,null,"X=",{"$f":"+(F121-F118)/(D118-D121)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+D121*D122+F121","v":{"$error":"#VALUE!"}}," Klizna Horiz",{"$f":"+'Analiza i dimenzioniranje'!$A97","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$B97","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!K465","v":11},{"$f":"+'Analiza i dimenzioniranje'!L465","v":-1},{"$f":"+'Analiza i dimenzioniranje'!M465","v":1.2},{"$f":"+'C III-V'!B12","v":4.2000010999999997},{"$f":"+'C III-V'!C12","v":1.2},12,{"$f":"+'C III-V'!B12-2","v":2.2000010999999997},{"$f":"+'C III-V'!C12","v":1.2}]
[null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!K468","v":1},{"$f":"+'Analiza i dimenzioniranje'!L468","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!M468","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!B13","v":4.2000010999999997},{"$f":"+'C III-V'!C13","v":1.2},13,{"$f":"+'C III-V'!B13-2","v":2.2000010999999997},{"$f":"+'C III-V'!C13","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!$L$469","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$U$515","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!B14","v":4.9000021999999994},{"$f":"+'C III-V'!C14","v":1.2},14,{"$f":"+'C III-V'!B14-2","v":2.9000021999999994},{"$f":"+'C III-V'!C14","v":1.2}]
["Količine betona temelja, betona zida i drenažnog materijala automatski se računaju i prenose u Troškovnik.",null,null,null,null,null,null,null,null,null,1.5,null,{"$f":"+'C III-V'!B15","v":4.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5},15,{"$f":"+'C III-V'!B15-2","v":2.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5}]
["Za količine iskopa i zasipa potrebno je upisati koordinate terena prije iskopa, u tablicu (čelije K114 do L118) i nagib iskopa (čelija K107).",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B16","v":2},{"$f":"+'C III-V'!C16","v":0.12820515121628623},1,{"$f":"+'C III-V'!B16-2","v":0},{"$f":"+'C III-V'!C16","v":0.12820515121628623}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Voda ispred zida"]
[{"$f":"'Analiza i dimenzioniranje'!L460","v":-2},{"$f":"'Analiza i dimenzioniranje'!M460","v":7},{"$f":"+'Analiza i dimenzioniranje'!$L$460","v":-2},{"$f":"+'Analiza i dimenzioniranje'!$M$460","v":7},{"$f":"+'Analiza i dimenzioniranje'!L455","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!M455","v":{"$error":"#VALUE!"}},null,{"$f":"+('Analiza i dimenzioniranje'!$L$455+'Analiza i dimenzioniranje'!$L$465)/2","v":{"$error":"#VALUE!"}},{"$f":"+('Analiza i dimenzioniranje'!$M$455+'Analiza i dimenzioniranje'!$M$465)/2","v":{"$error":"#VALUE!"}}]
[{"$f":"'Analiza i dimenzioniranje'!L461","v":5},{"$f":"'Analiza i dimenzioniranje'!M461","v":1.2},{"$f":"+C128","v":-2},{"$f":"+D128+2","v":9},{"$f":"+E128","v":{"$error":"#VALUE!"}},{"$f":"+F128+2","v":{"$error":"#VALUE!"}},null,{"$f":"+H128-3.5","v":{"$error":"#VALUE!"}},{"$f":"+I128","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!E42","v":0.8},null,null,"nagib zida prema tlu   1:",{"$f":"+'Analiza i dimenzioniranje'!$E$57","v":{"$error":"#VALUE!"}},"visina vode iznad temelja",null,{"$f":"+'Analiza i dimenzioniranje'!$E$42-'Analiza i dimenzioniranje'!$E$52","v":-0.39999999999999991}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nagib lica zida  1:",{"$f":"+'Analiza i dimenzioniranje'!$E$56","v":{"$error":"#VALUE!"}},"volumen temelja i zida do vode"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temelj kontrafore",null,"                 Temelj",null,"presjek kroz zid s vodom"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+I41","v":2},{"$f":"+J41","v":0.12820515121628623},{"$f":"+P137","v":1.75},{"$f":"+Q137","v":9.6153895463470418E-2},{"$f":"+'Analiza i dimenzioniranje'!$A$92+1.5","v":6.4000021999999994},{"$f":"'Analiza i dimenzioniranje'!E42","v":0.8}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+I42","v":2},1.2,{"$f":"+P136","v":1.75},{"$f":"IF('Analiza i dimenzioniranje'!E42=0,0,IF(+Q136>'Analiza i dimenzioniranje'!E42,'Analiza i dimenzioniranje'!E42,Q136))","v":0.8},{"$f":"+P135-0.5","v":1.25},{"$f":"+U133","v":0.8}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.75,1.2,{"$f":"+M114","v":3.4000010999999999},{"$f":"+S134","v":0.8}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+P135","v":1.75},1.2,{"$f":"+M115","v":{"$error":"#VALUE!"}},{"$f":"IF(S134=0,0,S135+(U133-S135))","v":0.8}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+P136","v":1.75},{"$f":"+Q138","v":9.6153895463470418E-2},{"$f":"+'Analiza i dimenzioniranje'!A92","v":4.9000021999999994},{"$f":"IF(S134=0,0,+U133)","v":0.8}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+I46","v":1.75},9.6153895463470418E-2,{"$f":"+M123","v":4.2000010999999997},{"$f":"IF(S134=0,0,IF(+N123>'Analiza i dimenzioniranje'!E42,'Analiza i dimenzioniranje'!E42,N123))","v":0.8}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+I47","v":2},{"$f":"+J47","v":0.12820515121628623},4.9000021999999994,{"$f":"+S138","v":0.8}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.9000021999999994,0.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+R133","v":1.75},{"$f":"+S133","v":9.6153895463470418E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  A=",{"$f":"IF(-0.5*(+(R133*S134-R134*S133)+(R134*S135-R135*S134)+(R135*S136-R136*S135)+(R136*S137-R137*S136)+(R137*S138-R138*S137)+(R138*S139-R139*S138)+(R139*S140-R140*S139)+(R140*S141-R141*S140))<0,0,-0.5*(+(R133*S134-R134*S133)+(R134*S135-R135*S134)+(R135*S136-R136*S135)+(R136*S137-R137*S136)+(R137*S138-R138*S137)+(R138*S139-R139*S138)+(R139*S140-R140*S139)+(R140*S141-R141*S140)))","v":{"$error":"#VALUE!"}},"m3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"xt=",{"$f":"IF(R142=0,0,-((R133*S134-R134*S133)*(R133+R134)+(R134*S135-R135*S134)*(R134+R135)+(R135*S136-R136*S135)*(R135+R136)+(R136*S137-R137*S136)*(R136+R137)+(R137*S138-R138*S137)*(R137+R138)+(R138*S139-R139*S138)*(R138+R139)+(R139*S140-R140*S139)*(R139+R140)+(R140*S141-R141*S140)*(R140+R141))/6/R142)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yt=",{"$f":"IF(R142=0,0,-((R133*S134-R134*S133)*(S133+S134)+(R134*S135-R135*S134)*(S134+S135)+(R135*S136-R136*S135)*(S135+S136)+(R136*S137-R137*S136)*(S136+S137)+(R137*S138-R138*S137)*(S137+S138)+(R138*S139-R139*S138)*(S138+S139)+(R139*S140-R140*S139)*(S139+S140)+(R140*S141-R141*S140)*(S140+S141))/6/R142)","v":{"$error":"#VALUE!"}},"m"]

{"sheet":"Analiza i dimenzioniranje","index":3,"n_rows":762,"n_cols":80,"rows_kept":762,"cut":false,"hidden":false,"merged":[[81,32,81,33],[82,32,82,35],[101,25,101,26],[71,49,71,51],[54,7,54,9],[34,7,34,9],[28,7,28,9],[39,7,39,9],[69,11,69,13],[70,11,70,13],[72,49,73,51],[38,11,38,12],[28,11,28,12],[62,0,62,2],[57,0,57,2],[68,0,68,2],[64,0,64,2],[69,10,70,10],[70,0,70,1],[71,0,71,1],[71,34,71,35],[61,0,61,2],[2,48,2,49],[3,48,3,49],[4,48,4,49],[9,8,10,9],[23,12,24,12],[23,11,24,11],[39,11,39,12],[51,7,52,7],[9,0,9,7],[34,11,34,12],[25,11,25,12],[41,0,41,2],[0,0,5,9],[10,0,10,7],[42,11,42,12],[25,6,25,9],[12,6,12,7],[0,45,0,46],[0,42,0,43],[0,36,0,37],[0,39,0,40],[0,31,0,32],[23,13,24,13],[8,60,8,61],[58,32,59,32],[53,50,54,50],[60,32,61,32],[23,0,23,2],[47,0,47,2],[33,0,33,2],[40,0,40,2],[43,0,43,2],[45,0,45,2],[38,0,38,2],[35,0,35,2],[34,0,34,2],[25,0,25,2],[47,7,48,7],[29,12,29,13],[29,14,29,15],[29,16,29,17],[44,0,44,2],[57,7,58,7],[42,7,42,9],[45,7,45,9],[52,0,52,1],[58,0,58,2],[485,48,487,49],[403,33,403,34],[403,24,404,24],[83,0,83,1],[91,4,91,5],[83,24,83,25],[171,0,171,1],[170,0,170,1],[84,0,84,1],[116,3,117,3],[116,0,117,1],[118,0,118,1],[133,0,133,1],[131,0,132,1],[116,8,117,8],[116,6,117,6],[116,7,117,7],[131,6,132,6],[131,7,132,7],[131,8,132,8],[248,6,248,7],[159,3,159,5],[160,3,160,5],[279,0,280,0],[303,0,304,0],[116,2,117,2],[82,0,82,1],[72,0,72,1],[78,0,78,2],[79,0,79,2],[80,0,80,2],[131,2,132,2],[77,0,77,2],[73,0,73,1],[74,0,74,1],[75,0,75,1],[114,0,115,3],[164,0,165,5],[577,14,577,15],[577,16,577,17],[375,24,375,26],[87,4,87,5],[89,4,89,5],[498,26,498,27],[105,13,106,13],[161,3,161,5],[162,3,162,5],[131,3,132,3],[158,3,158,5],[178,7,178,8],[178,2,178,3]]}
["   Autor i vlasnik programa: Nikola Sapunar, d.i.g. Zagreb, Gundulićeva 36,         mob. +385 98 213 632              e-mail: niksapunar@gmail.com",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  ","krak                  y  ","M destab. i stab.","za Mzida                                              krakovi                                                                               x                  y",null,"Moment zida III-III","za M u                                 presjeku II-II                                                                 krakovi                                                   x               y",null,"Moment                 II-II","za M u      temelju ispod zida                                                                                                                                                  krakovi                                                              x                  y",null,"Moment  ","za M u     presjeku I-I                                                                                                                                               krakovi                                                                     x                  y",null,"Moment      I-I"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+E61","v":4.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5},null,null,null,{"$f":"2+E61-G57-E55/2","v":3.8000010999999998},{"$f":"+E52","v":1.2},null,{"$f":"2+'Unos podataka'!$G$49+F46+Kontrafore!E3","v":4.4000010999999999},{"$f":"'C III-V'!AC46+(E52-'C III-V'!AC46)/2","v":0.75384613757397367},null,{"$f":"2+F46+E55/2","v":3.8000010999999998},{"$f":"+'C III-V'!AC43","v":0.35897429750167836},null,{"$f":"2+F46+E55","v":4.2000010999999997},{"$f":"'C III-V'!AC49+(E52-'C III-V'!AC49)/2","v":0.8051281599277047}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-C110","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+C110*AI3","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null," Eh1 ....................................................."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-C111","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," Eh2 ............................................."," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-C112","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+F122","v":{"$error":"#VALUE!"}},null,{"$f":"+AG5-$AG$2","v":{"$error":"#VALUE!"}},{"$f":"AC5*AI5","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-AO2+'C III-V'!F93","v":{"$error":"#VALUE!"}},{"$f":"+AO5*AC5","v":{"$error":"#VALUE!"}},null,null,null,null,null,null," Eh3 ....................................................."," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-B124","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," EPrometno ...................................."," "]
[null,null,null,null,null,null,"                 Program je autorski zaštićen.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-B125","v":{"$error":"#VALUE!"}},null,null,{"$f":"+F125","v":0},null,{"$f":"+AG7-$AG$2","v":-0.5},{"$f":"AD7*AI7","v":{"$error":"#VALUE!"}},null,{"$f":"+AG7-$AL$2","v":-1.2},{"$f":"AL7*AD7","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-B126","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+Y8","v":{"$error":"#VALUE!"}},null,null,{"$f":"+F126","v":{"$error":"#VALUE!"}},null,{"$f":"+AG8-$AG$2","v":{"$error":"#VALUE!"}},{"$f":"+Y8*AI8","v":{"$error":"#VALUE!"}},null,{"$f":"+AG8-$AL$2","v":{"$error":"#VALUE!"}},{"$f":"AL8*AD8","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null," EPLinijsko ................................"," "]
[{"$f":"IF(A68=\"\",\"\",'Unos podataka'!G57)","v":"DA"},{"$f":"+'Unos podataka'!G63","v":"DA"},{"$f":"+'Unos podataka'!F13","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-B127","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+Y9","v":{"$error":"#VALUE!"}},null,null,{"$f":"+F127","v":0},null,{"$f":"+IF(D83=\"\",-0.2)","v":false},{"$f":"+Y9*AI9","v":{"$error":"#VALUE!"}},null,{"$f":"+AG9-$AL$2","v":-1.2},{"$f":"AL9*AD9","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+E40-AU2","v":3.1948718360722954},{"$f":"+AB10*AU9","v":0}," EQTemelj ...................................................."," "]
[{"$f":"IF('Unos podataka'!F44='Unos podataka'!O43,\"ANALIZA STABILNOSTI GRAVITACIONOG  ZIDA\",+IF(F14>60,\"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNO OBLOŽNOG ZIDA\",\" ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA \"))","v":" ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA "},null,null,null,null,null,null,null,null,null,null,"Marka betona (staro)",20,25,30,40,45,50,55,null,null,null,null,null,{"$f":"-B128","v":-96.592582725499412},null,null,{"$f":"IF(E40<=E52,Y10,0)","v":0},null,{"$f":"IF(E40<=E52,0,Y10)","v":-96.592582725499412},null,null,{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+AG10-$AG$2","v":{"$error":"#REF!"}},{"$f":"-Y10*AI10","v":{"$error":"#REF!"}},null,{"$f":"+AG10-$AL$2","v":{"$error":"#REF!"}},{"$f":"IF(E40<E52,0,AL10*AD10)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null," HSidro ..............................."," "]
[{"$f":"+'Unos podataka'!A2","v":"NAZIV I STACIONAŽA ZIDA"},null,null,null,null,null,null,null,null,null,null,null,"EC2",null,null,null,null,null,null,null,{"$f":"+O78","v":0},null,null,null,{"$f":"-E43","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+Y11-AD11","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!M16","v":0},null,null,{"$f":"+F130","v":{"$error":"#VALUE!"}},null,{"$f":"+AG11-$AG$2","v":{"$error":"#VALUE!"}},{"$f":"+Y11*AI11","v":{"$error":"#VALUE!"}},null,{"$f":"F130-E52","v":{"$error":"#VALUE!"}},{"$f":"AL11*AD11","v":{"$error":"#VALUE!"}},null,{"$f":"-AO2+'C III-V'!U115","v":4.6153862426026704E-2},{"$f":"+AC11*AO11","v":{"$error":"#VALUE!"}},null,null,null,null,null,null," HPotres ........................................."," "]
[null,null,{"$f":"IF('C III-V'!B6<'C III-V'!D110,+'C III-V'!B71*0.5/SQRT(F112)+F15,F15)","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF('C III-V'!B6<'C III-V'!D110,+'C III-V'!B71*0.5/SQRT(F111)+E15,E15)","v":{"$error":"#VALUE!"}},null,null,null,null,null," Razred (klasa) betona C","16/20","20/25","25/30","30/37","35/45","40/50","45/55",null,"*x             +",null,"Sidro 1",null,null,null,null,{"$f":"SUM(AB3:AB6)","v":0},{"$f":"SUM(AC3:AC11)","v":{"$error":"#VALUE!"}},{"$f":"SUM(AD3:AD11)","v":{"$error":"#VALUE!"}},{"$f":"SUM(AE3:AE11)","v":0},null,null,"x",null,null,null,null,null,null,null,{"$f":"SUM(AP3:AP11)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AS3:AS11)","v":0},null,null,{"$f":"SUM(AV3:AV11)","v":0}]
["    KARAKTERISTIKE TLA",null,null,"1. sloj","   2. sloj","     3. sloj","          4. sloj \n      temeljno tlo       zasip\n        ",null,null,null,null," fcm (N/mm2)",24,28,33,38,43,48,53,null,"Y=",null,null,null,77.500002499999979,null,21.677419429760654,null,null,null,null,{"$f":"+J137","v":0},null,{"$f":"+$AF$2-AF13","v":4.9000021999999994},null,{"$f":"+Y13*AH13","v":379.75018275000537},null,null,null,{"$f":"AN2-'C III-V'!V59-Kontrafore!E3","v":1.2588240992358712},null,{"$f":"+AN13*Y16","v":79.015457827235778},{"$f":"+AQ2-'C III-V'!X59","v":8.1300761203646488E-3},null,{"$f":"+'C III-V'!X61*AQ13","v":0.13675205960988993},{"$f":"AT2-'C III-V'!Z59","v":-0.34297241985289872},null,{"$f":"+'C III-V'!Z61*AT13","v":-4.470740731161519}," Gtem .......U61+Q61+S61............................."," "]
["kut unutrašnjeg trenja ..............................",null,"j (°)",{"$f":"+'Unos podataka'!F4","v":22},{"$f":"+'Unos podataka'!G4","v":18},{"$f":"+'Unos podataka'!H4","v":20},{"$f":"+'Unos podataka'!I4","v":18},{"$f":"+'Unos podataka'!$J$11","v":30},null,null,null," ecu  (%0)",3.5,3.5,3.5,3.5,3.8,4.0999999999999996,4.2,null,{"$f":"+U11","v":0},null,null,null,{"$f":"+B136","v":{"$error":"#VALUE!"}},{"$f":"+Y14","v":{"$error":"#VALUE!"}},"Duljine:","Koord.",null,null,null,0,null,4.9000021999999994,null,{"$f":"+Y14*AH14","v":{"$error":"#VALUE!"}},{"$f":"+$AK$2-AF14","v":3.8000010999999998},null,{"$f":"+Z14*AK14","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null," Gzid+konz ...................................."," "]
["kohezija .................................................",null,"c (kPa)",{"$f":"+'Unos podataka'!F5","v":10},{"$f":"+'Unos podataka'!G5","v":22},{"$f":"+'Unos podataka'!H5","v":12},{"$f":"+'Unos podataka'!I5","v":25},0,null,null,null," fck valjak (N/mm2)",16,20,25,30,35,40,45,null,"*x             +",null,"sidro 2",null,null,{"$f":"+B138","v":{"$error":"#VALUE!"}},"Sidro 1",{"$f":"+P100","v":{"$error":"#VALUE!"}},{"$f":"+Q100","v":5},null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$f":"+B138*AH15","v":{"$error":"#VALUE!"}},{"$f":"+$AK$2-AF15","v":{"$error":"#VALUE!"}},null,{"$f":"+Z15*AK15","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null," Gnasip na konzoli............................."," "]
["jedinična težina .................................",null,"g (kN/m3)",{"$f":"+'Unos podataka'!F6","v":20},{"$f":"+'Unos podataka'!G6","v":20},{"$f":"+'Unos podataka'!H6","v":20},{"$f":"+'Unos podataka'!I6","v":20},{"$f":"+'Unos podataka'!F52","v":20},null,null,null," fck kocka (N/mm2)",20,25,30,37,45,50,55,null,"Y=",null,null,41.225808863683653,{"$f":"+'C III-V'!V61","v":62.769260514792791},null,"sidro.kl.ploha",null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"+AN2-AF16-Kontrafore!E3","v":{"$error":"#VALUE!"}},null,{"$f":"+B139*AN16","v":{"$error":"#VALUE!"}},null,null,null,null,null,null," Gnasipa na temelju iza............."," "]
["debljina slojeva tla .......................................",null,"h (m)",{"$f":"+'Unos podataka'!F7","v":2},{"$f":"IF('Unos podataka'!$O$48=\"\",'Unos podataka'!$J$7,'Unos podataka'!$O$38-F17-D17)","v":2.8},{"$f":"+E52","v":1.2},{"$f":"+IF(E41<=-2,\"\",\"γ'=\")","v":"γ'="},{"$f":"+IF(H18=G16,\"\",G16-10)","v":10},{"$f":"+IF(G17=\"\",\"\",\"(kN/m³)\")","v":"(kN/m³)"},null,null," Ecm (N/mm2)",29000,30000,31000,33000,34000,35000,36000,null,{"$f":"+U14","v":0},null,null,{"$f":"+Y23","v":{"$error":"#VALUE!"}},null,null,"Sidro 2",{"$f":"+P105","v":{"$error":"#VALUE!"}},{"$f":"+Q105","v":3},null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$f":"+Y23*AH17","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,{"$f":"AT2-(2+E61-G57/2)","v":-0.35000054999999985},null,{"$f":"+AT17*X17","v":{"$error":"#VALUE!"}}," Gnasipa na temelju ispred ........................"," "]
["nagib slojeva tla .......................................",null,"e (°)",{"$f":"+'Unos podataka'!F8","v":6},{"$f":"+'Unos podataka'!G8","v":4},{"$f":"+'Unos podataka'!H8","v":2},null,{"$f":"+IF(E41<=-2,G16,(G16-10))","v":10},null,null,null,"Visina temelja",null,null,null,"PODACI ZA CRTANJE  I  PRORAČUN SIDARA",null,null,null,null,{"$f":"+AG17","v":0},null,"sidro 3",null,{"$f":"+Y24","v":{"$error":"#VALUE!"}},null,"sidro.kl.ploha",null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AN$2-AH18","v":{"$error":"#VALUE!"}},null,{"$f":"+Y24*AN18","v":{"$error":"#VALUE!"}},null,null,null,null,null,null," PPrometno ......................."," "]
["trenje zid-tlo .........................................",null,"d (°)",{"$f":"+IF(D14<=23,0,IF(D14<=28,0.5*D14,2*D14/3))","v":0},{"$f":"+IF(E14<=23,0,IF(E14<=28,0.5*E14,2*E14/3))","v":0},{"$f":"+IF(F14<=23,0,IF(F14<=28,0.5*F14,2*F14/3))","v":0},null,"nagib terena iznad zida",null,{"$f":"+IF(E24>0,+TAN((H20+L119)*PI()/180)*E27+'Unos podataka'!$G$10,(TAN((H20+L119)*PI()/180)-TAN(F103*PI()/180))*C103+'Unos podataka'!$G$10)","v":0.4303745669501296},null,null,null,{"$f":"A177","v":"MEd,dst ="},null,{"$f":"+'Unos podataka'!F64","v":0.1},"I. red sidara je najviši red!!",null,null,null,"Y=",null,null,null,{"$f":"+Y25","v":{"$error":"#VALUE!"}},null,"Sidro3",{"$f":"+P110","v":-20},{"$f":"+Q110","v":0},null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AN$2-AH19","v":{"$error":"#VALUE!"}},null,{"$f":"+Y25*AN19","v":{"$error":"#VALUE!"}},null,null,null,null,null,null," PTočkasto ......................"," "]
[{"$f":"+IF(E24>0,\"računsko nadvišenje tla iznad zida .................\",\"nadvišenje tla iznad vrha zida .................\")","v":"računsko nadvišenje tla iznad zida ................."},null,"hn (m)",{"$f":"+IF(E24>0.000001,E20,'Unos podataka'!F9)","v":{"$error":"#VALUE!"}},{"$f":"+IF(E43=0,J20,IF(E24=0,IF((H20-F103+L119)<0,J20,J19),J20))","v":{"$error":"#VALUE!"}},{"$f":"+E20","v":{"$error":"#VALUE!"}},"b1=",{"$f":"+'Unos podataka'!G11","v":10.000000999999999},"°",{"$f":"+IF(H20>F103,IF(E24>0,+TAN(H20*PI()/180)*E27+'Unos podataka'!$G$10,(TAN(H20*PI()/180)-TAN(F103*PI()/180))*C103+'Unos podataka'!$G$10),IF(E24>0,+TAN(H20*PI()/180)*E27+'Unos podataka'!$G$10,'Unos podataka'!$G$10))","v":0.26449167438360077},null,null,null,"MOMENTI SAVIJANJA U PRESJECIMA ",null,{"$f":"+'Unos podataka'!F65","v":2},{"$f":"+P22","v":5},{"$f":"+P23","v":5.9},null,null,{"$f":"+U17","v":0},null,null,null,{"$f":"+Y26","v":{"$error":"#VALUE!"}},null,"sidro.kl.ploha",null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AN$2-AH20","v":{"$error":"#VALUE!"}},null,{"$f":"+Y26*AN20","v":{"$error":"#VALUE!"}},null,null,null,null,null,null," PLinijsko ........................."," "]
["Poissonov koeficijent ..................................",null,"n",{"$f":"+'Unos podataka'!F11","v":0.3},null,{"$f":"+'Unos podataka'!I8","v":10},null,"nagib terena ispod zida",null,null,null,null,null,"Temelj",null,"I. red","II.  red","III.  red","IV.  red",null,{"$f":"AI19","v":0},null,"sidro 4",null,{"$f":"+Y27","v":{"$error":"#VALUE!"}},null,"Sidro 4",{"$f":"+P115","v":-20},{"$f":"+Q115","v":0},null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AN$2-AH21","v":{"$error":"#VALUE!"}},null,{"$f":"+Y27*AN21","v":{"$error":"#VALUE!"}},null,null,null,null,null,null," QTemelj .............................."," "]
["prosj.modul stišlj.tla ispod temelja …........",null,"Ms (kN/m2)",{"$f":"+'Unos podataka'!F12","v":8000},null,{"$f":"+IF(F21>E18,F21,E18)","v":10},"b2=",{"$f":"+'Unos podataka'!J10","v":0},"°",{"$f":"+IF(E19>F18,E19,F18)","v":2},null,null,null,"    M I-I",null,{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!S47,0)","v":5},{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!T47,0)","v":3},{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!U47,0)","v":0},{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!V47,0)","v":0},null,"Y=",null,null,null,null,{"$f":"+Y28","v":25.881904536133977},"sidro.kl.ploha",null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AK$2-AF22","v":{"$error":"#VALUE!"}},null,{"$f":"IF(E40<E52,0,Z22*AK22)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null," VSidro .............................."," "]
["    DJELOVANJA",null,{"$f":"+E34+0.00000000001","v":20.000001000010002},null,null,null,null,null,null,null,null,"Ulazni podaci:",{"$f":"+IF(M24=\"Propisi\",\"\",\"EC7\")","v":"EC7"},"Država",null,{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!S48,0)","v":5.9},{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!T48,0)","v":4.9000000000000004},{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!U48,0)","v":0},{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!V48,0)","v":0},null,{"$f":"+U12","v":"*x             +"},null,null,null,{"$f":"+B140","v":{"$error":"#VALUE!"}},{"$f":"+Y29","v":{"$error":"#VALUE!"}},"Sidro 5",{"$f":"+P120","v":-20},{"$f":"+Q120","v":0},null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AK$2-AF23","v":{"$error":"#VALUE!"}},null,{"$f":"+Z23*AK23","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null," Ev1 ...................................."," "]
["PROMETNO OPTEREĆENJE ........................................",null,null,"Pp=",{"$f":"+'Unos podataka'!H15","v":10},"kN/m2 ",null,{"$f":"+IF('Unos podataka'!L11=\"Propisi\",\"Propisi:\",\"\")","v":""},{"$f":"IF(H24=\"Regulations:\",N24,+M23)","v":"EC7"},null,null,{"$f":"+IF(M24=\"Propisi\",\"\",\"Projektni pristup\")","v":"Projektni pristup"},{"$f":"+'Unos podataka'!L11","v":3},"HRVATSKA",null,{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!S49,0)","v":6.7},{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!T49,0)","v":4.8},{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!U49,0)","v":0},{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!V49,0)","v":0},{"$f":"+SUM(P24:S24)","v":11.5},"*x             +",null,"sidro 5",null,{"$error":"#VALUE!"},null,"sidro.kl.ploha",null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,{"$f":"+$AK$2-AF24","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null," Ev2  .........................."," "]
["širina opterećenja ...............................................",null,"........................","B =",{"$f":"IF(E24=0,0,'Unos podataka'!F16)","v":3},"m",null,null,{"$f":"+IF(H24=\"Propisi:\",\"\",\" Projektni pristup:    \")","v":" Projektni pristup:    "},{"$f":"IF(M24=\"Propisi\",\"\",+'Unos podataka'!L11)","v":3},{"$f":"+E26-E27","v":2.9999989999999999},null,null,null,null,{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!S50,0)","v":50},{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!T50,0)","v":50},{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!U50,0)","v":0},{"$f":"IF('Unos podataka'!$G$63=\"DA\",'Unos podataka'!V50,0)","v":0},null,"Y=",null,null,null,{"$error":"#VALUE!"},null,null,null,null,null,null,{"$f":"+J128","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"+$AN$2-'C III-V'!E93","v":2.4000010999999999},null,{"$f":"+B148*(G58+Kontrafore!E3)","v":{"$error":"#VALUE!"}},{"$f":"+$AN$2-AN25","v":2},null,null,null,null,null," Ev3 (na temelj) ........................................"," "]
["udaljenost opterećenja od zida ....................................",null,null,"x =",{"$f":"IF(E24=0,0,'Unos podataka'!F17)","v":4.5},"m","      Parcijalni koeficijenti svojstava tla:  M",null,null,null,null,"   Parcijalni koeficijenti za svojstva tla:    M",null,null,null,{"$f":"IF(P25=0,\"\",D74)","v":{"$error":"#VALUE!"}},{"$f":"IF(Q25=0,\"\",E74)","v":{"$error":"#VALUE!"}},{"$f":"IF(R25=0,\"\",F74)","v":""},{"$f":"IF(S25=0,\"\",G74)","v":""},{"$f":"IF(T25=0,\"\",$P$19*PI()*T24*('C III-V'!$AK$21*$D$16)/$P$20)","v":""},{"$f":"+SUM(S29:T29)","v":0},null,null,null,{"$error":"#VALUE!"},null,{"$f":"SUM(AA25:AA25)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AP13:AP24)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AS13:AS25)","v":0.13675205960988993},null,null,{"$f":"SUM(AV13:AV25)","v":{"$error":"#VALUE!"}}]
["udaljenost vrha pokosa od zida .............................",null,".........................","b =",{"$f":"IF(E24=0,0,'Unos podataka'!H18)","v":1.5000009999999999},"m","za kut unutrašnjeg trenja",null,"gj=",{"$f":"+M27","v":1.25},{"$f":"+E27+0.000001","v":1.5000019999999998},"za kut unutr. trenja    gj=",{"$f":"IF(M24=\"Propisi\",N27,ProjektniPristupi!B23)","v":1.25},1.25,null,{"$f":"IF(P25=0,\"\",ABS((P26/P25)))","v":{"$error":"#VALUE!"}},{"$f":"IF(Q25=0,\"\",ABS((Q26/Q25)))","v":{"$error":"#VALUE!"}},{"$f":"IF(R25=0,\"\",ABS((R26/R25)))","v":""},{"$f":"IF(S25=0,\"\",ABS((S26/S25)))","v":""},{"$f":"IF(T25=0,\"\",ABS((T26/T25)))","v":""},{"$f":"+IF(P22=T22,T25,IF(P22=S22,S25,IF(P22=R22,R25,IF(P22=Q22,Q25,IF(P22=P22,P25,\"\")))))","v":50},null,null,"V-V",{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,"II-II","sredina","I-I"]
[{"$f":"+'Unos podataka'!A19","v":"OPTEREĆENJE TEMELJEM ...................."},null,"......................",{"$f":"+'Unos podataka'!E19","v":"Qt="},{"$f":"+'Unos podataka'!F19","v":120},"kN/m2 ","za koheziju",null,"gc=",{"$f":"+M28","v":1.25},{"$f":"+IF(E35=0,0.0000000001,E35)","v":2.5},"za koheziju            gc =",{"$f":"IF(M24=\"Propisi\",N28,ProjektniPristupi!B24)","v":1.25},1.25,null,{"$f":"+IF(P25=\"\",\"\",'C III-V'!BE14)","v":{"$error":"#VALUE!"}},{"$f":"+IF(Q25=\"\",\"\",'C III-V'!BE20)","v":{"$error":"#VALUE!"}},{"$f":"+IF(R25=\"\",\"\",'C III-V'!BE26)","v":""},{"$f":"IF(S25=0,\"\",'C III-V'!BE32)","v":""},{"$f":"IF(T25=0,\"\",+'C III-V'!BE38)","v":""},{"$f":"SUM(P25:S25)+0.0000001","v":100.00000009999999},null,null,"VI-VI",25.881904536133977,null,{"$f":"+'C III-V'!X76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+'C III-V'!V76","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X76","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z76","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"$AN$2-'C III-V'!V77-Kontrafore!E3","v":{"$error":"#VALUE!"}},null,{"$f":"+AH28*AN28","v":{"$error":"#VALUE!"}},{"$f":"$AQ$2-'C III-V'!X77","v":{"$error":"#VALUE!"}},null,{"$f":"+AQ28*AI28","v":{"$error":"#VALUE!"}},{"$f":"+AT2-'C III-V'!Z77","v":{"$error":"#VALUE!"}},null,{"$f":"+AJ28*AT28","v":{"$error":"#VALUE!"}},"Kont naponi U76, S76, Q76....................."]
[{"$f":"+'Unos podataka'!A20","v":"širina temelja ................................................................."},null,".................",{"$f":"+'Unos podataka'!E20","v":"B ="},{"$f":"IF(E28=0,0,'Unos podataka'!F20)","v":1},"m",null,"Parcijalni.koeficijenti djelovanja:   A",null,null,{"$f":"+K27+K25","v":4.5000009999999993},"     Parcijalni koeficijenti djelovanja:         A",null,{"$f":"+'Sile i krakovi'!Q259","v":{"$error":"#VALUE!"}},null,{"$f":"IF(P25=0,\"\",4.5*$P$19*PI()*P24*('C III-V'!$AC$21*(($D$16*$D$17+$E$16*$E$17+$F$16*$F$17)/($D$17+$E$17+$F$17))*(($E$103*$D$17+$E$104*$E$17+$E$105*$F$17)/($D$17+$E$17+$F$17)))/$P$20)","v":{"$error":"#VALUE!"}},{"$f":"IF(Q25=0,\"\",4.5*$P$19*PI()*Q24*('C III-V'!$AE$21*(($D$16*$D$17+$E$16*$E$17+$F$16*$F$17)/($D$17+$E$17+$F$17))*(($E$103*$D$17+$E$104*$E$17+$E$105*$F$17)/($D$17+$E$17+$F$17)))/$P$20)","v":{"$error":"#VALUE!"}},{"$f":"IF(R25=0,\"\",4.5*$P$19*PI()*R24*('C III-V'!$AG$21*(($D$16*$D$17+$E$16*$E$17+$F$16*$F$17)/($D$17+$E$17+$F$17))*(($E$103*$D$17+$E$104*$E$17+$E$105*$F$17)/($D$17+$E$17+$F$17)))/$P$20)","v":""},{"$f":"IF(S25=0,\"\",4.5*$P$19*PI()*S24*('C III-V'!$AI$21*(($D$16*$D$17+$E$16*$E$17+$F$16*$F$17)/($D$17+$E$17+$F$17))*(($E$103*$D$17+$E$104*$E$17+$E$105*$F$17)/($D$17+$E$17+$F$17)))/$P$20)","v":""},null,0,null,null,"VII-VII",{"$error":"#VALUE!"},null,null,{"$f":"+AJ29","v":{"$error":"#VALUE!"}},{"$f":"+AH29","v":{"$error":"#VALUE!"}},null,{"$f":"+AI29","v":{"$error":"#VALUE!"}},null,null,{"$f":"+X35*(F46+Kontrafore!E3)/(E61+Kontrafore!E3)","v":{"$error":"#VALUE!"}},{"$f":"+X35*E55/E61","v":{"$error":"#VALUE!"}},{"$f":"+X35*(G57-'Unos podataka'!G49)/(E61+Kontrafore!E3)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AO2-'C III-V'!AC44","v":{"$error":"#VALUE!"}},{"$f":"-AC29*AO29","v":{"$error":"#VALUE!"}},null,{"$f":"+AR2-'C III-V'!AC43","v":0},{"$f":"AI29*AR29","v":{"$error":"#VALUE!"}},null,{"$f":"+AU2-'C III-V'!AC52","v":{"$error":"#VALUE!"}},{"$f":"-AJ29*AU29","v":{"$error":"#VALUE!"}},"Trenje ..................................."]
[{"$f":"+'Unos podataka'!A21","v":"duljina temelja ............................................................................"},null,"...................",{"$f":"+'Unos podataka'!E21","v":"L ="},{"$f":"IF(E28=0,0,'Unos podataka'!F21)","v":10},"m","Djelovanja","EQU","STR","GEO",null,null,"EQU",null,"STR",null,"GEO",null,null,null,{"$f":"P22*P25","v":250},null,null,"VIII-VIII",{"$f":"+AH28","v":{"$error":"#VALUE!"}},null,{"$f":"+AA26+AA28","v":{"$error":"#VALUE!"}},{"$f":"AB12+AB29","v":{"$error":"#VALUE!"}},{"$f":"AC12+AC29","v":{"$error":"#VALUE!"}},{"$f":"AD12+AD28+AD29","v":{"$error":"#VALUE!"}},{"$f":"+AE12+AE29","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(AH29:AJ29)","v":{"$error":"#VALUE!"}}]
[{"$f":"+'Unos podataka'!A22","v":"dubina temeljenja (ispod vrha zida) ................................................."},null,".....................",{"$f":"+'Unos podataka'!E22","v":"Df="},{"$f":"IF(E28=0,0,'Unos podataka'!H22)","v":-1},"m","      Trajna nepovoljna ",{"$f":"M31","v":1.1000000000000001},{"$f":"+O31","v":1.35},{"$f":"+Q31","v":1},{"$f":"-E31","v":1},"        Trajna nepovoljna ",{"$f":"IF(M24=\"Propisi\",N31,ProjektniPristupi!B13)","v":1.1000000000000001},1.1000000000000001,{"$f":"IF(M24=\"Propisi\",P31,ProjektniPristupi!B28)","v":1.35},1.35,{"$f":"IF(M24=\"Propisi\",R31,ProjektniPristupi!B34)","v":1},1,null,null,{"$f":"P22*P25+Q22*Q25","v":400},null,null,"IX-IX",null,{"$f":"+AB30+AC30+AD30+AE30","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AP12+AP25+AP26+AP28+AP29","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AS12+AS26+AS28+AS29","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AV12+AV26+AV28+AV29","v":{"$error":"#VALUE!"}}]
[{"$f":"+'Unos podataka'!A23","v":"hor. udaljenost temelja od vrha zida ......................."},null,"....................",{"$f":"+'Unos podataka'!E23","v":"x ="},{"$f":"IF(E28=0,0,'Unos podataka'!F23)","v":3},"m","Trajna povoljna           ",{"$f":"M32","v":0.9},{"$f":"+O32","v":1},{"$f":"+Q32","v":1},null,"        Trajna povoljna           ",{"$f":"IF(M24=\"Propisi\",N32,ProjektniPristupi!B14)","v":0.9},0.9,{"$f":"IF(M24=\"Propisi\",P32,ProjektniPristupi!B29)","v":1},1,{"$f":"IF(M24=\"Propisi\",R32,ProjektniPristupi!B35)","v":1},1,null,null,{"$f":"P22*P25+Q22*Q25+R22*R25","v":400},null,null,"X-X",null,null,null,null,null,null,null,null,null,null,"y","x"]
[{"$f":"+'Unos podataka'!A24","v":"visina temelja ......................................................."},null,{"$f":"+IF(D31=\"vv=\",\"\",\"........................\")","v":"........................"},{"$f":"+'Unos podataka'!E24","v":"h ="},{"$f":"IF(E28=0,0,'Unos podataka'!H24)","v":1},{"$f":"+IF(E33=\"h\",\"m\",\"\")","v":""},"Promjenjiva nepovoljna     ",{"$f":"M33","v":1.5},{"$f":"+O33","v":1.5},{"$f":"+Q33","v":1.3},null,"           Promjenjiva nepovoljna     ",{"$f":"IF(M24=\"Propisi\",N33,ProjektniPristupi!B15)","v":1.5},1.5,{"$f":"IF(M24=\"Propisi\",P33,ProjektniPristupi!B30)","v":1.5},1.5,{"$f":"IF(M24=\"Propisi\",R33,ProjektniPristupi!B36)","v":1.3},1.3,null,null,{"$f":"P22*P25+Q22*Q25+R22*R25+S22*S25","v":400},null,null,"XI-XI",null,null,null,null,null,null,null,null,null,null,{"$f":"+AN2","v":4.4000010999999999},{"$f":"+AO2","v":0.75384613757397367}]
["LINIJSKO OPTEREĆENJE .........................................",null,null,"PL=",{"$f":"+'Unos podataka'!H25","v":20.000001000000001},"kN/m'","Promjenjiva povoljna        ",{"$f":"M34","v":0},{"$f":"+O34","v":0},{"$f":"+Q34","v":0},null,"           Promjenjiva povoljna        ",{"$f":"IF(M24=\"Propisi\",N34,ProjektniPristupi!B16)","v":0},0,{"$f":"IF(M24=\"Propisi\",P34,ProjektniPristupi!B31)","v":0},0,{"$f":"IF(M24=\"Propisi\",R34,ProjektniPristupi!B37)","v":0},0,null,null,{"$f":"P22*P25+Q22*Q25+R22*R25+S22*S25+T22*T25","v":400}]
["udaljenost centra opterećenja od vrha zida .....................",null,null,"x =",{"$f":"IF('Unos podataka'!$H$25=0.000001,0,'Unos podataka'!F26)","v":2.5},"m",null,"   Parcijalni koeficijenti otpora:    R",null,null,null,"     Parcijalni koeficijenti za otpornost:      R",null,null,null,null,null,null,null,null,null,null,null,{"$f":"B167","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"omega"]
["TOČKASTO OPTEREĆENJE .......................................",null,null,"PT=",{"$f":"+'Unos podataka'!H27","v":20.000001000000001},"kN",null,"Prevrtanje"," gR =",{"$f":"+M36","v":1},null,"Prevrtanje              gR =",{"$f":"IF(M24=\"Propisi\",N36,ProjektniPristupi!B40)","v":1},1,null,null,null,null,"IV-IV","V-V","III-III","VI-VI","VII-VII","VIII-VIII","IX-IX","X-X","XI-XI","XII-XII","XIII-XIII","XIV-XIV","XV-XV","XVI-XVI","XVII-XVII","XVIII-XVIII","XIX-XIX","XX-XX","Vrh",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," a°","   b°","   b-a","   eta°"]
["udaljenost  centra opterećenja od vrha zida ..................",null,null,"x =",{"$f":"IF('Unos podataka'!H27=0.000001,0,'Unos podataka'!$F$28)","v":1.5},"m",null,"Klizanje","gRh=",{"$f":"+M37","v":1},{"$f":"+IF(H77=0,-2,0)","v":0},"Klizanje                   gRh=",{"$f":"IF(M24=\"Propisi\",N37,ProjektniPristupi!B41)","v":1},1,null,null,null,null,{"$f":"IF($J$53<AN44,0,10*($J$53-AN44)*($J$53-AN44)/2)","v":{"$error":"#VALUE!"}},{"$f":"IF($J$53<AO44,0,10*($J$53-AO44)*($J$53-AO44)/2)","v":{"$error":"#VALUE!"}},null,{"$f":"IF($J$53<V44,0,10*($J$53-V44)*($J$53-V44)/2)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF($J$53<U44,0,10*($J$53-U44)*($J$53-U44)/2)","v":0},{"$f":"IF($J$53<AJ52,0,10*($J$53-AJ52)*($J$53-AJ52)/2)","v":1.7999999999999998},"Pritisak vode",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG35=0,0,ATAN(BH35/BG35)*180/PI())","v":0},{"$f":"IF(BG35=0,0,ATAN(BJ35/BG35)*180/PI())","v":0},{"$f":"BR37-BQ37","v":0},{"$f":"BQ37+BS37/2","v":0}]
[{"$f":"+'Unos podataka'!A29:D29","v":"SILA U SIDRIMA (ukupna)................................."},null,"........................","PS=",{"$f":"-K39","v":-100.00000009999999},"kN/m'",null,"Nosivost ","gRv=",{"$f":"+M38","v":1},{"$f":"+IF(H77=0,-2,1)","v":1},"Nosivost                gRv=",{"$f":"IF(M24=\"Propisi\",N38,ProjektniPristupi!B42)","v":1},1,null,null,null,null,{"$f":"IF(($J$53-AN44)/3<0,0,($J$53-AN44)/3)","v":{"$error":"#VALUE!"}},{"$f":"IF(($J$53-AO44)/3<0,0,($J$53-AO44)/3)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(($J$53-V44)/3<0,0,($J$53-V44)/3)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(($J$53-U44)/3<0,0,($J$53-U44)/3)","v":0},{"$f":"IF(($J$53-AJ52)/3<0,0,($J$53-AJ52)/3)","v":0.19999999999999998},"težište od presjeka",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BE36=0,0,ATAN(BF36/BE36)*180/PI())","v":0},{"$f":"IF(BE36=0,0,ATAN(BH36/BE36)*180/PI())","v":0},{"$f":"BP38-BO38","v":0},{"$f":"BO38+BQ38/2","v":0}]
["otklon rezultante od horizontale .................................",null,null,"a =",{"$f":"+'Unos podataka'!F30","v":15},"° ",null,null,"EC2",null,{"$f":"+U28","v":100.00000009999999},"Dimenzioniranje                      EC2   ",null,null,null,null,null,"UTROŠAK GRADIVA",{"$f":"+IF($E$44=0,S37*S38*$J$44,S37*S38)","v":{"$error":"#VALUE!"}},{"$f":"+IF($E$44=0,T37*T38*$J$44,T37*T38)","v":{"$error":"#VALUE!"}},null,{"$f":"+IF($E$44=0,V37*V38*$J$44,V37*V38)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0.35999999999999993,"Dodatni M od vode"]
["visina rezultante  .......................................................",null,null,"hs=",{"$f":"IF(U34=0,0,U34/U28)","v":3.9999999960000001},"m",null,"Parcijalni koeficijenti za gradivo:",null,null,null,"     Parcijalni koeficijenti za gradivo:",null,null,null,"KONTAKTNI NAPONI",null,"beton            m3",{"$f":"IF(AN44>=$P$22,0,IF(AN44>=$Q$22,$P$25,IF(AN44>=$R$22,SUM($P$31:$Q$31),IF(AN44>=$S$22,SUM($P$31:$R$31),IF(AN44>=$T$22,SUM($P$30:$S$30),SUM($P$30:$T$30))))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AO44>=$P$22,0,IF(AO44>=$Q$22,$P$25,IF(AO44>=$R$22,SUM($P$31:$Q$31),IF(AO44>=$S$22,SUM($P$31:$R$31),IF(AO44>=$T$22,SUM($P$30:$S$30),SUM($P$30:$T$30))))))","v":{"$error":"#VALUE!"}},{"$f":"IF(E52>=$P$22,0,IF(E52>=$Q$22,$P$25,IF(E52>=$R$22,SUM($P$31:$Q$31),IF(E52>=$S$22,SUM($P$31:$R$31),IF(E52>=$T$22,SUM($P$30:$S$30),SUM($P$30:$T$30))))))","v":2.35},{"$f":"IF(V44>=$P$22,0,IF(V44>=$Q$22,$P$25,IF(V44>=$R$22,SUM($P$31:$Q$31),IF(V44>=$S$22,SUM($P$31:$R$31),IF(V44>=$T$22,SUM($P$30:$S$30),SUM($P$30:$T$30))))))","v":2.35},2.35,2.35,2.35,2.35,50,50,50,50,50,50,0,0,0,{"$f":"IF(U44>=$P$22,0,IF(U44>=$Q$22,$P$25,IF(U44>=$R$22,SUM($P$31:$Q$31),IF(U44>=$S$22,SUM($P$31:$R$31),IF(U44>=$T$22,SUM($P$30:$S$30),SUM($P$30:$T$30))))))","v":2.35},{"$f":"IF(AJ52>=$P$22,0,IF(AJ52>=$Q$22,$P$25,IF(AJ52>=$R$22,SUM($P$31:$Q$31),IF(AJ52>=$S$22,SUM($P$31:$R$31),IF(AJ52>=$T$22,SUM($P$30:$S$30),SUM($P$30:$T$30))))))","v":2.35},"sila"]
["NPV IZA ZIDA .................................................................",null,null,"hw=",{"$f":"+'Unos podataka'!F32","v":0.6},"m",null,"Čelik"," gs= ",{"$f":"+M41","v":1.1499999999999999},null,"Čelik                         gs= ",{"$f":"+'Unos podataka'!$L$25","v":1.1499999999999999},1.1499999999999999,"Fskl","sA (kN/m2)","sB (kN/m2)","čelik RA          kg",{"$f":"+IF(AN44<$T$22,$U$34,IF(AN44<$S$22,$U$33,IF(AN44<$R$22,$U$32,IF(AN44<$Q$22,$U$31,IF(AN44<$P$22,$U$30,$U$29)))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(AO44<$T$22,$U$34,IF(AO44<$S$22,$U$33,IF(AO44<$R$22,$U$32,IF(AO44<$Q$22,$U$31,IF(AO44<$P$22,$U$30,$U$29)))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(P44<$T$22,$U$34,IF(P44<$S$22,$U$33,IF(P44<$R$22,$U$32,IF(P44<$Q$22,$U$31,IF(P44<$P$22,$U$30,$U$29)))))","v":400},{"$f":"+IF(V44<$T$22,$U$34,IF(V44<$S$22,$U$33,IF(V44<$R$22,$U$32,IF(V44<$Q$22,$U$31,IF(V44<$P$22,$U$30,$U$29)))))","v":400},400,400,400,400,250,250,250,250,250,250,0,0,0,{"$f":"+IF(U44<$T$22,$U$34,IF(U44<$S$22,$U$33,IF(U44<$R$22,$U$32,IF(U44<$Q$22,$U$31,IF(U44<$P$22,$U$30,$U$29)))))","v":400},{"$f":"+IF(AJ52<$T$22,$U$34,IF(AJ52<$S$22,$U$33,IF(AJ52<$R$22,$U$32,IF(AJ52<$Q$22,$U$31,IF(AJ52<$P$22,$U$30,$U$29)))))","v":400},"M sidra"]
["NIVO VODE ISPRED ZIDA ...................................................",null,null,"h =",{"$f":"IF('Unos podataka'!J32=\"\",0,'Unos podataka'!J32)","v":0.8},"m",null,"Beton","gc=",{"$f":"+M42","v":1.5},null,"Beton                     gc=",{"$f":"+'Unos podataka'!L26","v":1.5},1.5,{"$f":"J177","v":{"$error":"#VALUE!"}},{"$f":"F190","v":{"$error":"#VALUE!"}},{"$f":"F193","v":{"$error":"#VALUE!"}},"mreža MA       kg",{"$f":"+IF(S40=0,0,S41/S40)","v":{"$error":"#VALUE!"}},{"$f":"IF(T40=0,0,T41/T40)","v":{"$error":"#VALUE!"}},{"$f":"+IF(U40=0,0,U41/U40)","v":170.21276595744681},{"$f":"IF(V40=0,0,V41/V40)","v":170.21276595744681},170.21276595744681,170.21276595744681,170.21276595744681,170.21276595744681,5,5,5,5,5,5,0,0,0,170.21276595744681,170.21276595744681,"krak"]
["POTRES (y)    Fy=SG*kh         kh=",null,"amax*S/r .....","Fy=",{"$f":"'C III-V'!$AM$132","v":{"$error":"#VALUE!"}},"kN/m'",null," Parcijalni koeficijenti djelovanja:",null,null,null,null,null,null,null,null,"Momenti na koti + (m)",null,{"$f":"+E79","v":3.14},"oznaka presjeka","MIII","Mz VI-VI","Mz VII-VII","Mz VIII-VIII","M IX-IX","M X-X","M XI-XI","M XII-XII","M XIII-XIII","M XIV-XIV","M XV-XV","M XVI-XVI","M XVII-XVII","M XVIII-XVIII","M XIX-XIX","Vrh",null,"VEd max","VEd min","M IV-IV          M min","M V-V             \n M max"]
["projektno seizmičko ubrzanje .........................................",null,null,"amax=",{"$f":"+'Unos podataka'!F34","v":0.1},{"$f":"+E42","v":0.8},null,"Trajno","gG=",{"$f":"+'Unos podataka'!L29","v":1.35},null,"Trajno                  gG=",{"$f":"+'Unos podataka'!L29","v":1.35},1.35,"Temelj",null,{"$f":"+AN44","v":{"$error":"#VALUE!"}},{"$f":"+AO44","v":{"$error":"#VALUE!"}},"Mkonzole (kNm/m')","presjek na visini (m)",{"$f":"+U52","v":1.2},{"$f":"+U53","v":1.52},{"$f":"+U54","v":1.84},{"$f":"+U55","v":2.16},{"$f":"+U56","v":2.48},{"$f":"+U57","v":2.8},{"$f":"+U58","v":3.14},{"$f":"+U59","v":3.44},{"$f":"+U60","v":3.76},{"$f":"+U61","v":4.08},{"$f":"+U62","v":4.4000000000000004},{"$f":"+U63","v":4.72},{"$f":"+U64","v":5.04},{"$f":"+U65","v":5.36},{"$f":"+U66","v":5.6800000000000006},{"$f":"+'Unos podataka'!F37","v":6},null,{"$f":"+U44","v":1.2},{"$f":"+IF(AM51=U51,U44,IF(AM51=V51,V44,IF(AM51=W51,W44,IF(AM51=X51,X44,IF(AM51=Y51,Y44,IF(AM51=Z51,Z44,IF(AM51=AA51,AA44,IF(AM51=AB51,AB44,IF(AM51=AC51,AC44,IF(AM51=AD51,AD44,IF(AM51=AE51,AE44,IF(AM51=AF51,AF44,IF(AM51=AG51,AG44,IF(AM51=AH51,AH44,IF(AM51=AI51,AI44)))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+'Dijagram momenata'!$Q$21","v":{"$error":"#VALUE!"}},{"$f":"+'Dijagram momenata'!$Q$22","v":{"$error":"#VALUE!"}}]
["parametar dozvoljenog pomaka zida ..........................",null,null,"r=",{"$f":"IF('Unos podataka'!$O$48=\"\",1,1.5)","v":1},{"$f":"+IF(G78=0,E52,H77)","v":3.14},null,"Promjenjivo","          gQ=",{"$f":"+'Unos podataka'!L30","v":1.5},null,"Promjenjiva            gQ=",{"$f":"+'Unos podataka'!L30","v":1.5},1.5,"M II-II",null,"Mz min","Mz max",{"$f":"+'C III-V'!D63","v":{"$error":"#VALUE!"}},"Mg",{"$f":"-'Sile i krakovi'!T$173","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!U$173","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!V$173","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!W$173","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!X$173","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!Y$173","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!Z$173","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AA$173","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AB$173","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AC$173","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AD$173","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AE$173","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AF$173","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AG$173","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AH$173","v":{"$error":"#VALUE!"}},0,null,{"$error":"#VALUE!"},null,{"$f":"+Q46","v":{"$error":"#VALUE!"}},{"$f":"+IF($V$44=$AO$44,V45,IF($W$44=$AO$44,W45,IF($X$44=$AO$44,X45,IF($Y$44=$AO$44,Y45,IF($Z$44=$AO$44,Z45,IF($AA$44=$AO$44,AA45,IF($AB$44=$AO$44,AB45,IF($AC$44=$AO$44,AC45,IF($AD$44=$AO$44,AD45,IF($AE$44=$AO$44,AE45,IF($AF$44=$AO$44,AF45,IF($AG$44=$AO$44,AG45,IF($AH$44=$AO$44,AH45,AI45)))))))))))))","v":{"$error":"#VALUE!"}}]
["parametar tipa tla ..............................................................",null,null,"S=",{"$f":"+'Unos podataka'!H34","v":1},{"$f":"+G58+0.000001","v":1.4000010999999999},null,"   Gradivo temelja i zida:",null,null,null,null,null,null,"stalno opterećenje",null,{"$f":"+IF(Q44=V44,V45,IF(Q44=W44,W45,IF(Q44=X44,X45,IF(Q44=Y44,Y45,IF(Q44=Z44,Z45,IF(Q44=AA44,AA45,IF(Q44=AB44,AB45,IF(Q44=AC44,AC45,IF(Q44=AD44,AD45,IF(Q44=AE44,AE45,IF(Q44=AF44,AF45,IF(Q44=AG44,AG45,IF(Q44=AH44,AH45,IF(Q44=AI44,AI45,IF(Q44=U44,U45,\"\")))))))))))))))","v":{"$error":"#VALUE!"}},null,null,"Mp",{"$f":"'Sile i krakovi'!T129","v":{"$error":"#VALUE!"}},{"$f":"'Sile i krakovi'!U129","v":{"$error":"#VALUE!"}},{"$f":"'Sile i krakovi'!V129","v":{"$error":"#VALUE!"}},{"$f":"'Sile i krakovi'!W129","v":{"$error":"#VALUE!"}},{"$f":"'Sile i krakovi'!X129","v":{"$error":"#VALUE!"}},{"$f":"'Sile i krakovi'!Y129","v":{"$error":"#VALUE!"}},{"$f":"'Sile i krakovi'!Z129","v":{"$error":"#VALUE!"}},{"$f":"'Sile i krakovi'!AA129","v":{"$error":"#VALUE!"}},{"$f":"'Sile i krakovi'!AB129","v":{"$error":"#VALUE!"}},{"$f":"'Sile i krakovi'!AC129","v":{"$error":"#VALUE!"}},{"$f":"'Sile i krakovi'!AD129","v":{"$error":"#VALUE!"}},{"$f":"'Sile i krakovi'!AE129","v":{"$error":"#VALUE!"}},{"$f":"'Sile i krakovi'!AF129","v":{"$error":"#VALUE!"}},{"$f":"'Sile i krakovi'!AG129","v":{"$error":"#VALUE!"}},{"$f":"'Sile i krakovi'!AH129","v":{"$error":"#VALUE!"}},0,null,{"$error":"#VALUE!"},null,{"$f":"+Q47","v":{"$error":"#VALUE!"}},{"$f":"+IF($V$44=$AO$44,V46,IF($W$44=$AO$44,W46,IF($X$44=$AO$44,X46,IF($Y$44=$AO$44,Y46,IF($Z$44=$AO$44,Z46,IF($AA$44=$AO$44,AA46,IF($AB$44=$AO$44,AB46,IF($AC$44=$AO$44,AC46,IF($AD$44=$AO$44,AD46,IF($AE$44=$AO$44,AE46,IF($AF$44=$AO$44,AF46,IF($AG$44=$AO$44,AG46,IF($AH$44=$AO$44,AH46,AI46)))))))))))))","v":{"$error":"#VALUE!"}}]
["    DIMENZIJE ZIDA",null,{"$f":"+'Unos podataka'!F36","v":-4},{"$f":"+ATAN('Unos podataka'!F49)*180/PI()*(-1)","v":0},{"$f":"IF('Unos podataka'!L2=\"\",\"A\",IF('Unos podataka'!L2='P X-X'!M1,E48,\"A\"))","v":"A"},null,null,null,"Temelj:",{"$f":"+IF(E78=\"\",\"\",1)","v":1},{"$f":"+IF(E78=\"\",\"\",0)","v":0},null,null,null,"dinamičko opterećenje",null,{"$f":"+IF(Q44=V44,V46,IF(Q44=W44,W46,IF(Q44=X44,X46,IF(Q44=Y44,Y46,IF(Q44=Z44,Z46,IF(Q44=AA44,AA46,IF(Q44=AB44,AB46,IF(Q44=AC44,AC46,IF(Q44=AD44,AD46,IF(Q44=AE44,AE46,IF(Q44=AF44,AF46,IF(Q44=AG44,AG46,IF(Q44=AH44,AH46,IF(Q44=AI44,AI46,IF(Q44=U44,U46,\"\")))))))))))))))","v":{"$error":"#VALUE!"}},null,"(Kozasipa/Ki)≈","MEd (kNm/m')",{"$f":"IF($E$44=0,+U45*$J$44+U46*$J$45,U45+U46)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,null,{"$error":"#VALUE!"},null,{"$f":"IF($E$44>0,+AN45*$J$44+AN46*$J$45,AN45+AN46)","v":{"$error":"#VALUE!"}},{"$f":"+IF($V$44=$AO$44,V47,IF($W$44=$AO$44,W47,IF($X$44=$AO$44,X47,IF($Y$44=$AO$44,Y47,IF($Z$44=$AO$44,Z47,IF($AA$44=$AO$44,AA47,IF($AB$44=$AO$44,AB47,IF($AC$44=$AO$44,AC47,IF($AD$44=$AO$44,AD47,IF($AE$44=$AO$44,AE47,IF($AF$44=$AO$44,AF47,IF($AG$44=$AO$44,AG47,IF($AH$44=$AO$44,AH47,AI47)))))))))))))","v":{"$error":"#VALUE!"}}]
["visina zida i temelja ....................................................",null,null,"H =",{"$f":"+D17+E17+F17","v":6},"m",null,"C",{"$f":"+'Unos podataka'!B83","v":25},{"$f":"+IF(H50=\"šipka\",\"\",IF(I271>7.85,\"KORISTI  ŠIPKE\",\"\"))","v":""},{"$f":"+IF(E78=\"\",\"\",4)","v":4},null,null,"GORNJE VRIJEDNOSTI MOMENATA SU BEZ PARCIJALNIH FAKTORA ZA DIMENZIONIRANJE",null,null,null,null,1,"NG (kN/m')",{"$f":"-('Sile i krakovi'!T151)","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!U151","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!V151","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!W151","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!X151","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!Y151","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!Z151","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AA151","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AB151","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AC151","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AD151","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AE151","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AF151","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AG151","v":{"$error":"#VALUE!"}},{"$f":"-'Sile i krakovi'!AH151","v":{"$error":"#VALUE!"}},0,null,{"$error":"#VALUE!"},{"$f":"+AF48","v":{"$error":"#VALUE!"}},{"$f":"IF($V$44=$AN$44,V48,IF($W$44=$AN$44,W48,IF($X$44=$AN$44,X48,IF($Y$44=$AN$44,Y48,IF($Z$44=$AN$44,Z48,IF($AA$44=$AN$44,AA48,IF($AB$44=$AN$44,AB48,IF($AC$44=$AN$44,AC48,IF($AD$44=$AN$44,AD48,IF($AE$44=$AN$44,AE48,IF($AF$44=$AN$44,AF48,IF($AG$44=$AN$44,AG48,IF($AH$44=$AN$44,AH48,AH48)))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"IF($V$44=$AO$44,V48,IF($W$44=$AO$44,W48,IF($X$44=$AO$44,X48,IF($Y$44=$AO$44,Y48,IF($Z$44=$AO$44,Z48,IF($AA$44=$AO$44,AA48,IF($AB$44=$AO$44,AB48,IF($AC$44=$AO$44,AC48,IF($AD$44=$AO$44,AD48,IF($AE$44=$AO$44,AE48,IF($AF$44=$AO$44,AF48,IF($AG$44=$AO$44,AG48,IF($AH$44=$AO$44,AH48,AI48)))))))))))))","v":{"$error":"#VALUE!"}}]
["dužina zida ......................................................................",null,".......................","L =",{"$f":"+'Unos podataka'!F38","v":12},"m",null,null,{"$f":"+'Unos podataka'!B84","v":30},null,null,{"$f":"+IF(I57=\"\",\"\",0.05)","v":0.05},0,"PODACI O ARMATURI",null,null,{"$f":"+IF(J48=\"MA\",\"\",\"zaštitni sloj\")","v":"zaštitni sloj"},null,"Ko=1-sinj zasipa ","visina presjeka (cm)",{"$f":"('C III-V'!$P12-'C III-V'!$P11)*100","v":{"$error":"#VALUE!"}},{"$f":"('C III-V'!$S7-'C III-V'!$S6)*100","v":{"$error":"#VALUE!"}},{"$f":"('C III-V'!$S9-'C III-V'!$S8)*100","v":{"$error":"#VALUE!"}},{"$f":"('C III-V'!$S11-'C III-V'!$S10)*100","v":{"$error":"#VALUE!"}},{"$f":"('C III-V'!$S13-'C III-V'!$S12)*100","v":{"$error":"#VALUE!"}},{"$f":"('C III-V'!$S15-'C III-V'!$S14)*100","v":{"$error":"#VALUE!"}},{"$f":"('C III-V'!$S17-'C III-V'!$S16)*100","v":{"$error":"#VALUE!"}},{"$f":"('C III-V'!$S19-'C III-V'!$S18)*100","v":{"$error":"#VALUE!"}},{"$f":"('C III-V'!$S21-'C III-V'!$S20)*100","v":{"$error":"#VALUE!"}},{"$f":"('C III-V'!$S23-'C III-V'!$S22)*100","v":{"$error":"#VALUE!"}},{"$f":"('C III-V'!$P2-'C III-V'!$P1)*100","v":{"$error":"#VALUE!"}},{"$f":"('C III-V'!$P4-'C III-V'!$P3)*100","v":{"$error":"#VALUE!"}},{"$f":"('C III-V'!$P6-'C III-V'!$P5)*100","v":{"$error":"#VALUE!"}},{"$f":"('C III-V'!$P8-'C III-V'!$P7)*100","v":{"$error":"#VALUE!"}},{"$f":"('C III-V'!$P10-'C III-V'!$P9)*100","v":{"$error":"#VALUE!"}},0,null,{"$error":"#VALUE!"},{"$f":"+IF(AM44=U44,U49,IF(AM44=V44,V49,IF(AM44=W44,W49,IF(AM44=X44,X49,IF(AM44=Y44,Y49,IF(AM44=Z44,Z49,IF(AM44=AA44,AA49,IF(AM44=AB44,AB49,IF(AM44=AC44,AC49,IF(AM44=AD44,AD44,IF(AM44=AE44,AE49,IF(AM44=AF44,AF49,IF(AM44=AG44,AG49,IF(AM44=AH44,AH49,IF(AM44=AI44,AI49)))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"('C III-V'!S3-'C III-V'!S2)*100","v":{"$error":"#VALUE!"}},{"$f":"+IF($V$44=$AO$44,V49,IF($W$44=$AO$44,W49,IF($X$44=$AO$44,X49,IF($Y$44=$AO$44,Y49,IF($Z$44=$AO$44,Z49,IF($AA$44=$AO$44,AA49,IF($AB$44=$AO$44,AB49,IF($AC$44=$AO$44,AC49,IF($AD$44=$AO$44,AD49,IF($AE$44=$AO$44,AE49,IF($AF$44=$AO$44,AF49,IF($AG$44=$AO$44,AG49,IF($AH$44=$AO$44,AH49,AI49)))))))))))))","v":{"$error":"#VALUE!"}}]
["otklon zida (od vertikale) uz tlo .......................................",null,".........................","b =",{"$f":"+'Unos podataka'!$G$39","v":4},"°",null,{"$f":"+'Unos podataka'!B87","v":"šipka"},"B500B",null,null,{"$f":"+IF(I57=\"\",\"\",0.05)","v":0.05},{"$f":"+IF(I57=\"\",\"\",1)","v":1},{"$f":"+IF(H50=\"MA\",\"\",\"Armatura\")","v":"Armatura"},{"$f":"+IF(H50=\"MA\",\"\",\"f\")","v":"f"},{"$f":"+IF(H50=\"MA\",\"\",\"kom/m'\")","v":"kom/m'"},"(m)","(m)",{"$f":"+M105","v":0.58068606531123268},"MEds",{"$f":"(U47+U48*(U49/2-'Unos podataka'!$C$99)/100)","v":{"$error":"#VALUE!"}},{"$f":"IF(V45>0,V47+V48*(V49/2-'Unos podataka'!$C$99)/100,(V47+V48*(V49/2-'Unos podataka'!$C$99)/100))","v":{"$error":"#VALUE!"}},{"$f":"IF(W45>0,W47+W48*(W49/2-'Unos podataka'!$C$99)/100,(W47+W48*(W49/2-'Unos podataka'!$C$99)/100))","v":{"$error":"#VALUE!"}},{"$f":"IF(X45>0,X47+X48*(X49/2-'Unos podataka'!$C$99)/100,(X47+X48*(X49/2-'Unos podataka'!$C$99)/100))","v":{"$error":"#VALUE!"}},{"$f":"IF(Y45>0,Y47+Y48*(Y49/2-'Unos podataka'!$C$99)/100,(Y47+Y48*(Y49/2-'Unos podataka'!$C$99)/100))","v":{"$error":"#VALUE!"}},{"$f":"IF(Z45>0,Z47+Z48*(Z49/2-'Unos podataka'!$C$99)/100,(Z47+Z48*(Z49/2-'Unos podataka'!$C$99)/100))","v":{"$error":"#VALUE!"}},{"$f":"IF(AA45>0,AA47+AA48*(AA49/2-'Unos podataka'!$C$99)/100,(AA47+AA48*(AA49/2-'Unos podataka'!$C$99)/100))","v":{"$error":"#VALUE!"}},{"$f":"IF(AB45>0,AB47+AB48*(AB49/2-'Unos podataka'!$C$99)/100,(AB47+AB48*(AB49/2-'Unos podataka'!$C$99)/100))","v":{"$error":"#VALUE!"}},{"$f":"IF(AC45>0,AC47+AC48*(AC49/2-'Unos podataka'!$C$99)/100,(AC47+AC48*(AC49/2-'Unos podataka'!$C$99)/100))","v":{"$error":"#VALUE!"}},{"$f":"IF(AD45>0,AD47+AD48*(AD49/2-'Unos podataka'!$C$99)/100,(AD47+AD48*(AD49/2-'Unos podataka'!$C$99)/100))","v":{"$error":"#VALUE!"}},{"$f":"IF(AE45>0,AE47+AE48*(AE49/2-'Unos podataka'!$C$99)/100,(AE47+AE48*(AE49/2-'Unos podataka'!$C$99)/100))","v":{"$error":"#VALUE!"}},{"$f":"IF(AF45>0,AF47+AF48*(AF49/2-'Unos podataka'!$C$99)/100,(AF47+AF48*(AF49/2-'Unos podataka'!$C$99)/100))","v":{"$error":"#VALUE!"}},{"$f":"IF(AG45>0,AG47+AG48*(AG49/2-'Unos podataka'!$C$99)/100,(AG47+AG48*(AG49/2-'Unos podataka'!$C$99)/100))","v":{"$error":"#VALUE!"}},{"$f":"IF(AH45>0,AH47+AH48*(AH49/2-'Unos podataka'!$C$99)/100,(AH47+AH48*(AH49/2-'Unos podataka'!$C$99)/100))","v":{"$error":"#VALUE!"}},{"$f":"IF(AI45>0,AI47+AI48*(AI49/2-'Unos podataka'!$C$99)/100,(AI47+AI48*(AI49/2-'Unos podataka'!$C$99)/100))","v":{"$error":"#VALUE!"}},0,null,{"$error":"#VALUE!"},null,{"$f":"+IF($V$44=$AN$44,V50,IF($W$44=$AN$44,W50,IF($X$44=$AN$44,X50,IF($Y$44=$AN$44,Y50,IF($Z$44=$AN$44,Z50,IF($AA$44=$AN$44,AA50,IF($AB$44=$AN$44,AB50,IF($AC$44=$AN$44,AC50,IF($AD$44=$AN$44,AD50,IF($AE$44=$AN$44,AE50,IF($AF$44=$AN$44,AF50,IF($AG$44=$AN$44,AG50,IF($AH$44=$AN$44,AH50,AH50)))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF($V$44=$AO$44,V50,IF($W$44=$AO$44,W50,IF($X$44=$AO$44,X50,IF($Y$44=$AO$44,Y50,IF($Z$44=$AO$44,Z50,IF($AA$44=$AO$44,AA50,IF($AB$44=$AO$44,AB50,IF($AC$44=$AO$44,AC50,IF($AD$44=$AO$44,AD50,IF($AE$44=$AO$44,AE50,IF($AF$44=$AO$44,AF50,IF($AG$44=$AO$44,AG50,IF($AH$44=$AO$44,AH50,AI50)))))))))))))","v":{"$error":"#VALUE!"}}]
["visina temelja prema padini ...............................",null,".......................","hA=",{"$f":"+'Unos podataka'!G40","v":0.7},"m",null,{"$f":"-'Unos podataka'!F36","v":4},"Zid:",null,null,null,null,{"$f":"+IF(H50=\"šipka\",\"Armatura temelja  Presjek I-I\",\"Armatura temelja Presjek I-I mreža\")","v":"Armatura temelja  Presjek I-I"},null,null,null,"Glavna armatura na dnu temelja ",null,"VG (kN/m')",{"$f":"+'Sile i krakovi'!T112","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!U112","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!V112","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!W112","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!X112","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!Y112","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!Z112","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!AA112","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!AB112","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!AC112","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!AD112","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!AE112","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!AF112","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!AG112","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!AH112","v":{"$error":"#VALUE!"}},0,null,{"$error":"#VALUE!"},{"$f":"MIN(U51:AI51)","v":{"$error":"#VALUE!"}},{"$f":"IF($V$44=$AN$44,V51,IF($W$44=$AN$44,W51,IF($X$44=$AN$44,X51,IF($Y$44=$AN$44,Y51,IF($Z$44=$AN$44,Z51,IF($AA$44=$AN$44,AA51,IF($AB$44=$AN$44,AB51,IF($AC$44=$AN$44,AC51,IF($AD$44=$AN$44,AD51,IF($AE$44=$AN$44,AE51,IF($AF$44=$AN$44,AF51,IF($AG$44=$AN$44,AG51,IF($AH$44=$AN$44,AH51,AH51)))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"IF($V$44=$AO$44,V51,IF($W$44=$AO$44,W51,IF($X$44=$AO$44,X51,IF($Y$44=$AO$44,Y51,IF($Z$44=$AO$44,Z51,IF($AA$44=$AO$44,AA51,IF($AB$44=$AO$44,AB51,IF($AC$44=$AO$44,AC51,IF($AD$44=$AO$44,AD51,IF($AE$44=$AO$44,AE51,IF($AF$44=$AO$44,AF51,IF($AG$44=$AO$44,AG51,IF($AH$44=$AO$44,AH51,AI51)))))))))))))","v":{"$error":"#VALUE!"}}]
["visina temelja prema zasipu .................................",null,".........................","h =",{"$f":"+'Unos podataka'!G41","v":1.2},"m",null,"C",{"$f":"IF(I53=20,16,IF(I53=25,20,IF(I53=30,25,IF(I53=37,30,IF(I53=45,35,IF(I53=50,40,IF(I53=55,45,IF(I53=60,50,\"\"))))))))","v":30},{"$f":"IF(H54=\"šipka\",\"\",IF(F320>7.85,\"KORISTI  ŠIPKE\",\"\"))","v":""},null,null,null,null,{"$f":"IF(H50=\"MA\",\"\",'Unos podataka'!B89)","v":14},null,{"$f":"IF(H50=\"MA\",\"\",Q58)","v":0.05},null,null,{"$f":"+U52","v":1.2},{"$f":"+E52","v":1.2},"III-III",null,null,null,null,null,null,null,"DIMENZIONIRANJE PRESJEKA NA POPREČNU SILA U PRESJEKU III-III",null,null,null,null,null,null,null,"          DIMENZIONIRANJE PRESJEKA NA POPREČNU SILU NA KONZOLI ",null,null,null,null,null,null,{"$f":"+C335","v":{"$error":"#VALUE!"}},"m"]
["nagib dna temelja  ....................................",null," .............. 1:n2 ...","n2=",{"$f":"IF(E52=E51,\"0,00\",(E61+D83)/(E52-E51))","v":7.8000043999999988},null,null,null,{"$f":"+'Unos podataka'!D84","v":37},{"$f":"IF(E41<=0,0,E41)","v":0.6},null,null,null,{"$f":"+IF(H50=\"mreža\",\"\",\"Razdjelna\")","v":"Razdjelna"},null,{"$f":"+B270","v":{"$error":"#VALUE!"}},null,{"$f":"+'Unos podataka'!F89/100","v":0.4},null,{"$f":"+T52+X53","v":1.52},{"$f":"+U52+X$53","v":1.52},"VI-VI",{"$f":"IF('Unos podataka'!F9>0,+'Unos podataka'!$T$55-U52-'Unos podataka'!F9,+'Unos podataka'!$T$55-U52)","v":4.8},{"$f":"+W53/15","v":0.32},null,null,null,null,"          Poprečna sila",null,null,"               Uzdužna sila:",null,null,null,null,null,"        Poprečna sila",null,null,"Uzdužna sila "]
["širina zida u kruni ................................................",null,"........................","d=",{"$f":"+'Unos podataka'!G43","v":0.6},"m",null,{"$f":"+'Unos podataka'!B92","v":"šipka"},"B500B",null,null,null,null,{"$f":"+IF(H50=\"šipka\",\"Armatura temelja Presjek II-II\",\"Armatura temelja Presjek II-II mreža\")","v":"Armatura temelja Presjek II-II"},null,null,null,"Glavna armatura na vrhu temelja ",null,{"$f":"+T53+$X$53","v":1.84},1.84,"VII-VII",{"$f":"+IF(Y54=0,U52+2*X53,Y54)","v":1.8399999999999999},{"$f":"+$E$79","v":3.14},{"$f":"+IF(X54>$U$52+2*$X$53-$X$53/2,IF(X54<$U$52+2*$X$53+$X$53/2,X54,$U$52+2*$X$53))","v":1.8399999999999999},{"$f":"+IF(AB54=0,X52+2*Y51,AB54)","v":1.8399999999999999},{"$f":"+$E$79+$E$81","v":3.44},{"$f":"+IF(AA54>$U$52+2*$X$53-$X$53/2,IF(AA54<$U$52+2*$X$53+$X$53/2,AA54,$U$52+2*$X$53))","v":1.8399999999999999},"VG =",{"$f":"+U51","v":{"$error":"#VALUE!"}},"kN","NG =",{"$f":"+AG56/1.35","v":{"$error":"#VALUE!"}},"kN",null,null,null,"VG =",{"$f":"+B138+E80*E81*E62","v":{"$error":"#VALUE!"}},"kN","NG =",{"$f":"+AP56/1.35","v":{"$error":"#VALUE!"}},"kN"]
["širina zida na temelju .......…..........................................",null,"............................","d1=",{"$f":"+'Unos podataka'!G44","v":0.8},"m",null,"Ograničenje pukotina",null,null,null,null,null,{"$f":"+IF(H50=\"MA\",\"\",\"Glavna\")","v":"Glavna"},{"$f":"+'Unos podataka'!B90","v":14},{"$f":"IF(H50=\"MA\",\"\",B297)","v":{"$error":"#VALUE!"}},{"$f":"+Q52","v":0.05},{"$f":"+IF(H50=\"MA\",\"\",1/P55)","v":{"$error":"#VALUE!"}},null,2.16,2.16,"VIII-VIII",{"$f":"+IF(Y55=0,$U$52+3*$X$53,Y55)","v":2.16},3.14,{"$f":"+IF(X55>$U$52+3*$X$53-$X$53/2,IF(X55<$U$52+3*$X$53+$X$53/2,X55,$U$52+3*$X$53))","v":2.16},null,3.44,{"$f":"+IF(AA55>$U$52+3*$X$53-$X$53/2,IF(AA55<$U$52+3*$X$53+$X$53/2,AA55,$U$52+3*$X$53))","v":2.16},"VQ =",0,"kN","NQ =",{"$f":"+AP55","v":0},"kN","za presjek temelj kontrafora",null,null,"VQ =",0,"kN","NQ =",0,"kN"]
["nagib lica zida ..............................................",null," …........ n1:1 …","n1=",{"$f":"+IF(F56>100,\">100\",F56)","v":{"$error":"#VALUE!"}},{"$f":"IF('C III-V'!B10-'C III-V'!B11=0,\">100\",IF('C III-V'!C10-'C III-V'!C11/(0+'C III-V'!B11-'C III-V'!B10)>100,\">100\",('C III-V'!C10-'C III-V'!C11)/('C III-V'!B11-'C III-V'!B10)))","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Unos podataka'!C101","v":0.3},"mm",null,null,null,{"$f":"+IF(H50=\"mreža\",\"\",\"Razdjelna\")","v":"Razdjelna"},null,{"$f":"+B297","v":{"$error":"#VALUE!"}},null,{"$f":"+R53","v":0.4},null,2.48,2.48,"IX-IX",{"$f":"+IF(Y56=0,$U$52+4*$X$53,Y56)","v":2.48},3.14,{"$f":"+IF(X56>$U$52+4*$X$53-$X$53/2,IF(X56<$U$52+4*$X$53+$X$53/2,X56,$U$52+4*$X$53))","v":2.48},null,3.44,{"$f":"+IF(AA56>$U$52+4*$X$53-$X$53/2,IF(AA56<$U$52+4*$X$53+$X$53/2,AA56,$U$52+4*$X$53))","v":2.48}," VEd=",{"$f":"+U51*N44+U52*N45","v":{"$error":"#VALUE!"}},"kN","NEd=",{"$f":"+U48","v":{"$error":"#VALUE!"}},"kN"," VEd=",{"$f":"+AD56*H84","v":{"$error":"#VALUE!"}},"kN"," VEd=",{"$f":"+AM54*N44+AM55*N45","v":{"$error":"#VALUE!"}},"kN","NEd=",{"$f":"+AR56-AR57","v":{"$error":"#VALUE!"}},"kN",{"$f":"+IF($Y$44=$E$79,Y51,IF(Z44=E79,Z51,IF(AA44=E79,AA51,IF(AB44=739,AB51,IF(AC44=E79,AC51,AD51)))))","v":{"$error":"#VALUE!"}}]
["nagib zida uz tlo .....................................",null,"........ n3:1 ...","n3=",{"$f":"+IF(F57>100,\">100\",'Unos podataka'!G46)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!F15","v":{"$error":"#VALUE!"}},{"$f":"+E58+0.0000001","v":0.70000109999999993},null,{"$f":"+IF(G78=0,\"\",\"Konzola:\")","v":"Konzola:"},null,null,null,null,"Armatura zida Presjek III-III",null,null,null,{"$f":"+F415","v":"Armatura u Presjeku III-III  pokrivena sa Poz. 5,  Poz. 15 i Poz. 19"},null,2.8,{"$f":"IF(U56=$Y$66,$AB$66,W57)","v":2.8},"X-X",{"$f":"+IF(Y57=0,$U$52+5*$X$53,Y57)","v":2.8},3.14,{"$f":"+IF(X57>$U$52+5*$X$53-$X$53/2,IF(X57<$U$52+5*$X$53+$X$53/2,X57,$U$52+5*$X$53))","v":2.8},null,3.44,{"$f":"+IF(AA57>$U$52+5*$X$53-$X$53/2,IF(AA57<$U$52+5*$X$53+$X$53/2,AA57,$U$52+5*$X$53))","v":2.8},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF($X$44=$E$79+$E$81,X51,IF(Y44=E79+E81,Y51,IF(Z44=E79+E81,AZ51,IF(AA44=E79+E81,AA51,IF(AB44=E79+E81,AB51,IF(AC44=E79+E81,AC51,AD51))))))","v":{"$error":"#VALUE!"}}]
["širina temelja ispred zida .............................................",null,".................","b1=",{"$f":"+'Unos podataka'!G47","v":0.70000099999999998},"m",{"$f":"+E59+0.0000000000000001","v":1.4000001},{"$f":"+IF(G78=0,\"\",\"C\")","v":"C"},{"$f":"IF(I59=20,16,IF(I59=25,20,IF(I59=30,25,IF(I59=37,30,IF(I59=45,35,IF(I59=50,40,IF(I59=55,45,IF(I59=60,50,\"\"))))))))","v":30},null,null,null,null,{"$f":"+IF(H54=\"MA\",\"\",\"Glavna\")","v":"Glavna"},{"$f":"+IF(H54=\"MA\",\"mreža R\",'Unos podataka'!B94)","v":12},{"$f":"IF(H54=\"MA\",\"\",B321)","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!C99/100","v":0.05},{"$f":"+IF(P58=0,\"\",IF(H54=\"MA\",\"\",1/P58))","v":{"$error":"#VALUE!"}},null,3.1199999999999997,3.14,"XI-XI",{"$f":"+IF(Y58=0,$U$52+6*$X$53,Y58)","v":3.14},3.14,{"$f":"+IF(X58>$U$52+6*$X$53-$X$53/2,IF(X58<$U$52+6*$X$53+$X$53/2,X58,$U$52+6*$X$53))","v":3.14},null,3.44,{"$f":"+IF(AA58>$U$52+6*$X$53-$X$53/2,IF(AA58<$U$52+6*$X$53+$X$53/2,AA58,$U$52+6*$X$53))","v":3.12},"Dimenzije presjeka: na visini: ",null,{"$f":"+U44","v":1.2},"m","Gradivo:",null,null,null,null,"        Dimenzije presjeka:",null,null,null,"Gradivo:"]
["širina temelja iza zida .................................................",null,".................","b2=",{"$f":"+'Unos podataka'!G48","v":1.4000001},"m",null,null,{"$f":"+IF(G78=0,\"\",I53)","v":37},null,null,null,null,{"$f":"+IF(H54=\"mreža\",\"\",\"Razdjelna\")","v":"Razdjelna"},{"$f":"+'Unos podataka'!E94","v":8},null,null,{"$f":"+'Unos podataka'!F94/100","v":0.4},null,3.4399999999999995,3.44,"XII-XII",{"$f":"+IF(Y59=0,$U$52+7*$X$53,Y59)","v":3.4400000000000004},3.14,{"$f":"+IF(X59>$U$52+7*$X$53-$X$53/2,IF(X59<$U$52+7*$X$53+$X$53/2,X59,$U$52+7*$X$53))","v":false},null,3.44,{"$f":"+IF(AA59>$U$52+7*$X$53-$X$53/2,IF(AA59<$U$52+7*$X$53+$X$53/2,AA59,$U$52+7*$X$53))","v":3.44},null,"širina presjeka      b =",100,"cm","Beton   C",{"$f":"+I52","v":30},null,null,null,null,"širina   b =",{"$f":"+AE59","v":100},"cm","Beton:  C",{"$f":"+I52","v":30}]
["otklon temeljne plohe uz tlo ...................",null,"............... n:hB ...","n=",{"$f":"+'Unos podataka'!G49","v":0},"m",null,{"$f":"+IF(G78=0,\"\",\"šipka\")","v":"šipka"},{"$f":"+IF(G78=0,\"\",I54)","v":"B500B"},null,null,null,null,{"$f":"IF(I56=\"mreža\",\"\",\"Armatura zida Presjek IV-IV\")","v":"Armatura zida Presjek IV-IV"},null,null,null,{"$f":"+F335","v":{"$error":"#VALUE!"}},null,3.7599999999999993,3.76,"XIII-XIII",{"$f":"+IF(Y60=0,$U$52+8*$X$53,Y60)","v":3.76},3.14,{"$f":"+IF(X60>$U$52+8*$X$53-$X$53/2,IF(X60<$U$52+8*$X$53+$X$53/2,X60,$U$52+8*$X$53))","v":false},null,3.44,{"$f":"+IF(AA60>$U$52+8*$X$53-$X$53/2,IF(AA60<$U$52+8*$X$53+$X$53/2,AA60,$U$52+8*$X$53))","v":false},null,"visina presjeka      h =",{"$f":"+AL49","v":{"$error":"#VALUE!"}},"cm",null,{"$f":"+I53","v":37},null,null,null,null,"visina   h =",{"$f":"+E81*100","v":30},"cm",null,{"$f":"+I53","v":37}]
[{"$f":"+IF(H83>0,\"širina temelja bez kontrafore ........................................\",\"širina temelja.............................................\")","v":"širina temelja bez kontrafore ........................................"},null,".........................","B =",{"$f":"+G57+F46+E55-'Unos podataka'!G49","v":2.9000021999999994},"m",null,null,null,null,null,null,null,{"$f":"+IF(I56=\"MA\",\"\",\"Glavna\")","v":"Glavna"},{"$f":"IF(H54=\"MA\",\"     mreža R\",O58)","v":12},{"$f":"+IF(H54=\"šipka\",B350,G430)","v":{"$error":"#VALUE!"}},{"$f":"IF(H54=\"šipka\",+Q58,\"\")","v":0.05},{"$f":"+IF(P61=0,\"\",IF(H60=\"MA\",\"\",1/P61))","v":{"$error":"#VALUE!"}},null,4.0799999999999992,4.08,"XIV-XIV",{"$f":"+IF(Y61=0,$U$52+9*$X$53,Y61)","v":4.08},3.14,{"$f":"+IF(X61>$U$52+9*$X$53-$X$53/2,IF(X61<$U$52+9*$X$53+$X$53/2,X61,$U$52+9*$X$53))","v":false},null,3.44,{"$f":"+IF(AA61>$U$52+9*$X$53-$X$53/2,IF(AA61<$U$52+9*$X$53+$X$53/2,AA61,$U$52+9*$X$53))","v":false},null,"zaštitni sloj      a =",{"$f":"+Q58*100","v":5},"cm","Čelik:  RA","B 500",null,null,null,null,"zaštitni sloj   a =",{"$f":"+AE61","v":5},"cm","Čelik:  RA","B 500"]
["jedinična težina zida i temelja ..................................",null,".................","gb=",{"$f":"+'Unos podataka'!F51","v":25},"kN/m3 ",null,null,null,null,null,null,null,{"$f":"+IF(I56=\"mreža\",\"\",\"Razdjelna\")","v":"Razdjelna"},{"$f":"+IF(H54=\"MA\",\"\",'Unos podataka'!E94)","v":8},null,null,{"$f":"IF(H54=\"MA\",\"\",R59)","v":0.4},null,4.3999999999999995,4.4000000000000004,"XV-XV",{"$f":"+IF(Y62=0,$U$52+10*$X$53,Y62)","v":4.4000000000000004},3.14,{"$f":"+IF(X62>$U$52+10*$X$53-$X$53/2,IF(X62<$U$52+10*$X$53+$X$53/2,X62,$U$52+10*$X$53))","v":false},null,3.44,{"$f":"+IF(AA62>$U$52+10*$X$53-$X$53/2,IF(AA62<$U$52+10*$X$53+$X$53/2,AA62,$U$52+10*$X$53))","v":false},null,"statička visina   d =",{"$f":"+AE60-AE61","v":{"$error":"#VALUE!"}},"cm",null,560,null,null,null,null,"statička visina   d =",{"$f":"+AN60-AN61","v":25},"cm",null,560]
["jedinična težina zasipa iza zida..........................................",null,".................","gz=",{"$f":"+'Unos podataka'!F52","v":20},"kN/m3 ",null,null,null,null,null,null,null,{"$f":"IF(H60=\"mreža\",\"\",\"Armatura zida Presjek V-V\")","v":"Armatura zida Presjek V-V"},null,null,null,{"$f":"+F363","v":{"$error":"#VALUE!"}},null,4.72,4.72,"XVI-XVI",{"$f":"+IF(Y63=0,$U$52+11*$X$53,Y63)","v":4.72},3.14,{"$f":"+IF(X63>$U$52+11*$X$53-$X$53/2,IF(X63<$U$52+11*$X$53+$X$53/2,X63,$U$52+11*$X$53))","v":false},null,3.44,{"$f":"+IF(AA63>$U$52+11*$X$53-$X$53/2,IF(AA63<$U$52+11*$X$53+$X$53/2,AA63,$U$52+11*$X$53))","v":false},null,null,"za gradivo:",null,null,null,null,null,null,null,null,"za gradivo:"]
["debljina zasipa (drenaže) iza zida .....................................",null,"......................","d =",{"$f":"+'Unos podataka'!F53","v":0.5},"m",null,null,null,null,null,null,null,{"$f":"+IF(H60=\"MA\",\"\",\"Glavna\")","v":"Glavna"},{"$f":"IF(H54=\"MA\",\"    mreža R\",O61)","v":12},{"$f":"+IF(H54=\"šipka\",B377,G430)","v":{"$error":"#VALUE!"}},{"$f":"IF(H54=\"šipka\",+Q58,\"\")","v":0.05},{"$f":"+IF(P64=0,\"\",IF(H60=\"MA\",\"\",1/P64))","v":{"$error":"#VALUE!"}},null,5.04,5.04,"XVII-XVII",{"$f":"+IF(Y64=0,$U$52+12*$X$53,Y64)","v":5.04},3.14,{"$f":"+IF(X64>$U$52+12*$X$53-$X$53/2,IF(X64<$U$52+12*$X$53+$X$53/2,X64,$U$52+12*$X$53))","v":false},null,3.44,{"$f":"+IF(AA64>$U$52+12*$X$53-$X$53/2,IF(AA64<$U$52+12*$X$53+$X$53/2,AA64,$U$52+12*$X$53))","v":false},"gc =",{"$f":"+M42","v":1.5},null,"gs =",{"$f":"+M41","v":1.1499999999999999},null,null,null,null,"gc =",{"$f":"+M42","v":1.5},null,"gs =",{"$f":"+M41","v":1.1499999999999999}]
["visina nasipa na temelju ispred zida ...............................",null,".................","hn=",{"$f":"+'Unos podataka'!G54","v":0.30000099999999996},"m",null,null,null,null,null,null,null,{"$f":"+IF(H60=\"mreža\",\"\",\"Razdjelna\")","v":"Razdjelna"},{"$f":"+IF(H54=\"MA\",\"\",O62)","v":8},null,null,{"$f":"IF(H54=\"MA\",\"\",R59)","v":0.4},null,5.36,5.36,"XVIII-XVIII",{"$f":"+IF(Y65=0,U52+13*X53,Y65)","v":5.36},3.14,{"$f":"+IF(X65>$U$52+13*$X$53-$X$53/2,IF(X65<$U$52+13*$X$53+$X$53/2,X65,$U$52+13*$X$53))","v":false},null,3.44,{"$f":"+IF(AA65>$U$52+13*$X$53-$X$53/2,IF(AA65<$U$52+13*$X$53+$X$53/2,AA65,$U$52+13*$X$53))","v":false},"fck=",{"$f":"IF(I53=25,I52,IF(I53=30,I52,IF(I53=37,I52,IF(I53=45,I52,IF(I53=50,I52,IF(I53=55,I52,IF(I53=60,I52)))))))","v":30},"Mpa","fyk=",500,"Mpa",null,null,null,"fck=",{"$f":"+AD65","v":30},"MPa","fyk=",{"$f":"+AG65","v":500},"MPa"]
["jedinična težina nasipa ispred zida ...........................................",null,"......................","gn=",{"$f":"+'Unos podataka'!F55","v":20},"kN/m3 ",null,null,null,null,null,null,null,{"$f":"+IF(G78>0,\"Armatura konzole\",\"\")","v":"Armatura konzole"},null,{"$f":"+IF(E426>0.252,\"DVOSTRUKO ARMIRANJE\",\"\")","v":""},null,null,null,5.6800000000000006,{"$f":"+T66","v":5.6800000000000006},"XIX",{"$f":"+IF(Y66=0,U53+14*X53,Y66)","v":3.14},3.14,{"$f":"+MAX(Y54:Y65)","v":3.14},null,null,{"$f":"+MAX(AB54:AB65)","v":3.44},"fcd=",{"$f":"IF(I53=25,I52/10/'Unos podataka'!L26,IF(I53=30,I52/10/'Unos podataka'!L26,IF(I53=37,I52/10/'Unos podataka'!L26,IF(I53=45,I52/10/'Unos podataka'!L26,IF(I53=50,I52/10/'Unos podataka'!L26,IF(I53=55,I52/10/'Unos podataka'!L26,IF(I53=60,I52/10/'Unos podataka'!L26,)))))))","v":2},"kN/cm2","fyd=",{"$f":"+AG65/10/'Unos podataka'!$L$25","v":43.478260869565219},"kN/cm2",null,null,null,"fcd=",{"$f":"+AD66","v":2},"kN/cm2","fyd=",{"$f":"+AG66","v":43.478260869565219},"kN/cm2"]
[{"$f":"+IF(B9=\"\",\"\",\"    SIDRA\")","v":"    SIDRA"},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(G78=0,\"\",\"Glavna\")","v":"Glavna"},{"$f":"IF('Unos podataka'!G57=\"\",\"\",'Unos podataka'!B97)","v":12},{"$f":"IF(G78=0,\"\",B405)","v":{"$error":"#VALUE!"}},{"$f":"IF(G78=0,\"\",Q58)","v":0.05},{"$f":"+IF(P67=0,\"\",IF(H60=\"MA\",\"\",1/P67))","v":{"$error":"#VALUE!"}},null,6.0000000000000009,{"$f":"+U66+$X$53","v":6.0000000000000009},"XX"]
[{"$f":"IF(A67=\"\",\"\",\"promjer injektirane bušotine………………………………………………………….\")","v":"promjer injektirane bušotine…………………………………………………………."},null,null,{"$f":"+IF('Unos podataka'!G63=\"\",\"\",'Unos podataka'!E64)","v":"d≈"},{"$f":"+IF('Unos podataka'!G63=\"\",\"\",'Unos podataka'!F64)","v":0.1},{"$f":"IF('Unos podataka'!G63=\"\",\"\",'Unos podataka'!G64)","v":"m"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(G78=0,\"\",'Unos podataka'!F97/100)","v":0.4},null,null,{"$f":"+U67","v":6.0000000000000009},"Vrh",null,null,null,null,null,null,"      - nosivost presjeka na poprečnu silu bez poprečne armature",null,null,null,null,null,null,null,null,"      - nosivost presjeka na poprečnu silu bez poprečne armature"]
[{"$f":"+IF(A67=\"\",\"\",\"faktor sigurnosti (koeficijent redukcije sile u sidrima)….\")","v":"faktor sigurnosti (koeficijent redukcije sile u sidrima)…."},null,null,{"$f":"+IF('Unos podataka'!G63=\"\",\"\",\"g=\")","v":"g="},{"$f":"+IF('Unos podataka'!G63=\"\",\"\",'Unos podataka'!F65)","v":2},null,null,{"$f":"+IF($B$9=\"\",\"\",IF(H70=0,\"\",T21))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"-U69*('Sile i krakovi'!U208-'Sile i krakovi'!U210)","v":{"$error":"#VALUE!"}},"     v11=",{"$f":"+'Sile i krakovi'!Z190","v":{"$error":"#VALUE!"}},{"$f":"+U69*W69","v":{"$error":"#VALUE!"}},0,null,null,null,null,null,"VRd,c =","[CRd,c*k*(100*r1*fck)1/3+k1*scp]*b*d",null,null,null,null,null,null,null,"VRd,c =","[CRd,c*k*(100*r1*fck)1/3+k1*scp]*b*d"]
[null,null,null,{"$f":"+IF($B$9=\"\",\"\",IF(D71=0,\"\",P21))","v":"I. red"},{"$f":"+IF($B$9=\"\",\"\",IF(E71=0,\"\",Q21))","v":"II.  red"},{"$f":"+IF($B$9=\"\",\"\",IF(F71=0,\"\",R21))","v":""},{"$f":"+IF($B$9=\"\",\"\",IF(G71=0,\"\",S21))","v":""},null,null,null,{"$f":"+IF(A77=\"\",\"\",\"Preporučene visine       \n podgleda konzole\")","v":"Preporučene visine       \n podgleda konzole"},"        KONTROLA RAVNOTEŽE ELEMENTA",null,null,null,null,null,null,{"$f":"+U70*('Sile i krakovi'!V208-'Sile i krakovi'!V210)","v":{"$error":"#VALUE!"}},"¸¸",{"$f":"-'Sile i krakovi'!AB190","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"CRd,c =",{"$f":"0.18/AD64","v":0.12},"k = ",{"$f":"IF(1+SQRT(20/AE62)>2,2,1+SQRT(20/AE62))","v":{"$error":"#VALUE!"}},{"$f":"+IF(AF70>2,\"\",\"≤ 2,00\")","v":{"$error":"#VALUE!"}},"k1 =",0.15,null,null,"CRd,c =",{"$f":"0.18/AM64","v":0.12},"k = ",{"$f":"IF(AN60=0,0,IF(1+SQRT(20/AN62)>2,2,1+SQRT(20/AN62)))","v":1.8944271909999157},{"$f":"+IF(AO70>2,\"\",\"≤ 2,00\")","v":"≤ 2,00"},"k1 =",0.15]
[{"$f":"+IF(B9=\"\",\"\",\"visina sidra od dna temelja ……........ (m)\")","v":"visina sidra od dna temelja ……........ (m)"},null,{"$f":"+IF(B9=\"\",\"\",\"hs=\")","v":"hs="},{"$f":"IF($B$9=\"\",\"\",IF(P22=0,\"\",P22))","v":5},3,"",{"$f":"IF($B$9=\"\",\"\",IF(S22=0,\"\",S22))","v":""},null,null,null,null," Između presjeka I-I,II-II, III-III i dna temelja",null,null,null,null,null,null,{"$f":"+U69+U71+U73+U75","v":{"$error":"#VALUE!"}},"     v22=",{"$f":"+'Sile i krakovi'!Z191","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"    - površina armature u presjeku   SAs1 =",{"$f":"IF(+'Iskaz armature'!U18*'Iskaz armature'!Z18>F321,+'Iskaz armature'!U18*'Iskaz armature'!Z18,F321)","v":{"$error":"#VALUE!"}},"cm2",null,null," ",null,null,null,"    - površina armature u presjeku   SAs1 =",{"$f":"IF(H54=\"mreža\",F348,F349)","v":{"$error":"#VALUE!"}},"cm2"]
[{"$f":"+IF(B9=\"\",\"\",\"dužina slobodne dionice ……….......... (m)\")","v":"dužina slobodne dionice ……….......... (m)"},null,{"$f":"+IF(B9=\"\",\"\",\"lsl=\")","v":"lsl="},5.9,4.9000000000000004,"",{"$f":"IF($B$9=\"\",\"\",IF(S23=0,\"\",S23))","v":""},null,null,null,{"$f":"IF(A$77=\"\",\"\",+U57)","v":2.8}," SV=",{"$f":"+'Sile i krakovi'!F258","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,{"$f":"+U70+U72+U74+U76","v":{"$error":"#VALUE!"}},"     h22=",{"$f":"-'Sile i krakovi'!AB191","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"ρ1=",{"$f":"IF(AG71/AE59/AE62>0.02,0.02,AG71/AE59/AE62)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AD72<0.02,\"<   0,02\",\">    0,02\")","v":{"$error":"#VALUE!"}},null,"scp=Ned/Ac=",{"$f":"-IF(AG56/AE59/AE60>0.2*AD66,0.2,AG56/AE59/AE60)","v":{"$error":"#VALUE!"}}," <  =    0,02  *    fcd  =",null,{"$f":"0.02*AD66","v":0.04},"ρ1=",{"$f":"IF(AP71/AN59/AN62>0.02,0.02,AP71/AN59/AN62)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AM72<0.02,\"<   0,02\",\">    0,02\")","v":{"$error":"#VALUE!"}},"scp =",{"$f":"IF(AN60=0,0,IF(AP56/AN59/AN60>0.2*AM66,0.2,AP56/AN59/AN60))","v":{"$error":"#VALUE!"}}," <  =   0,02  *  fcd  =",null,{"$f":"0.02*AM66","v":0.04}]
[{"$f":"+IF(B9=\"\",\"\",\"dužina sidrišne dionice .................... (m)\")","v":"dužina sidrišne dionice .................... (m)"},null,{"$f":"+IF(B9=\"\",\"\",\"lsidr=\")","v":"lsidr="},{"$f":"IF($B$9=\"\",\"\",IF(P24=0,\"\",P24))","v":6.7},{"$f":"IF($B$9=\"\",\"\",IF(Q24=0,\"\",Q24))","v":4.8},{"$f":"IF($B$9=\"\",\"\",IF(R24=0,\"\",R24))","v":""},{"$f":"IF($B$9=\"\",\"\",IF(S24=0,\"\",S24))","v":""},{"$f":"+SUM(D73:G73)","v":11.5},null,{"$f":"+MAX(D74:G74)","v":{"$error":"#VALUE!"}},3.14," SH=",{"$f":"+'Sile i krakovi'!F233","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,{"$f":"+U73*('Sile i krakovi'!U209-'Sile i krakovi'!U208)","v":{"$error":"#VALUE!"}},"     v33=",{"$f":"+'Sile i krakovi'!Z192","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"VRd,c =",{"$f":"(AD70*AF70*(100*AD72*AD65)^(1/3)+AI70*AH72)*AE59*AE62/10","v":{"$error":"#VALUE!"}},"kN",null,"k1 =",0.15,"VRd,c =",{"$f":"+AD73*H84","v":{"$error":"#VALUE!"}},null,"VRd,c =",{"$f":"IF(AN60=0,0,(0.18/AM64*AO70*(100*AM72*AM65)^(1/3)+AR70*AP72)*AN59*AN62/10)","v":{"$error":"#VALUE!"}},"kN"]
[{"$f":"+IF(B9=\"\",\"\",IF(E70=\"\",\"računska sila u sidru\",\"računske sile u sidrima ……............. (kN)\"))","v":"računske sile u sidrima ……............. (kN)"},null,{"$f":"+IF(B9=\"\",\"\",\"Rd=\")","v":"Rd="},{"$f":"IF($B$9=\"\",\"\",P29)","v":{"$error":"#VALUE!"}},{"$f":"IF($B$9=\"\",\"\",Q29)","v":{"$error":"#VALUE!"}},{"$f":"IF($B$9=\"\",\"\",R29)","v":""},{"$f":"IF($B$9=\"\",\"\",S29)","v":""},null,null,{"$f":"+IF(J73<160,\"R32L\",IF(J73<230,\"R32N\",\"R32S\"))","v":{"$error":"#VALUE!"}},3.44," SM=",{"$f":"+'Sile i krakovi'!AC253","v":{"$error":"#VALUE!"}},"kNm",null,null,null,null,{"$f":"U74*('Sile i krakovi'!V209-'Sile i krakovi'!V208)","v":{"$error":"#VALUE!"}},"     h33=",{"$f":"-'Sile i krakovi'!AB192","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"VRd,c,min=","(nmin+k1*scp)*b*d",null,null,null,null,null,null,null,"VRd,c,min =","(nmin+k1*scp)*b*d"]
[{"$f":"+IF(B9=\"\",\"\",IF(Q27>0,\"računske sile po m' zida …...…... (kN/m') \",\"računska sila po m' zida …..... (kN/m')\"))","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(B9=\"\",\"\",\"Psi=\")","v":"Psi="},{"$f":"IF($B$9=\"\",\"\",IF(P25=0,\"\",P25))","v":50},{"$f":"IF($B$9=\"\",\"\",IF(Q25=0,\"\",Q25))","v":50},{"$f":"IF($B$9=\"\",\"\",IF(R25=0,\"\",R25))","v":""},{"$f":"IF($B$9=\"\",\"\",IF(S25=0,\"\",S25))","v":""},null,null,null,3.76,null,null,null,null,null,null,{"$f":"+'Sile i krakovi'!D257+'Sile i krakovi'!D220+'Sile i krakovi'!D232+'Sile i krakovi'!D261","v":0},{"$f":"U75*('Sile i krakovi'!Q209-'Sile i krakovi'!U208)","v":{"$error":"#VALUE!"}},"     vtem=",{"$f":"+'Sile i krakovi'!Z193","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"n1=",{"$f":"0.6*(1-AH59/250)","v":0.52800000000000002},"nmin=",{"$f":"0.035*POWER(AF70,1.5)*SQRT(AD65)","v":{"$error":"#VALUE!"}},"acw =",{"$f":"1+AG56/AE62/AE59/AD66","v":{"$error":"#VALUE!"}},"z =",{"$f":"0.9*AE62","v":{"$error":"#VALUE!"}},"cm","n1=",{"$f":"0.6*(1-AQ59/250)","v":0.52800000000000002},"nmin=",{"$f":"IF(AN60=0,0,0.035*POWER(AO70,1.5)*SQRT(AM65))","v":0.49985673669876474},"acw =",{"$f":"1+AP56/AN62/AN59/AM66","v":{"$error":"#VALUE!"}},"z =",{"$f":"0.9*AN62","v":22.5},"cm"]
[{"$f":"+IF(A67=\"\",\"\",\"razmak između sidara …................ (m')\")","v":"razmak između sidara …................ (m')"},null,{"$f":"+IF(B9=\"\",\"\",\"b<=\")","v":"b<="},{"$f":"IF(D75=\"\",\"\",ABS(ROUNDDOWN(P27,1)))","v":{"$error":"#VALUE!"}},{"$f":"IF(E75=\"\",\"\",ABS(ROUNDDOWN(Q27,1)))","v":{"$error":"#VALUE!"}},{"$f":"IF(F75=\"\",\"\",ABS(ROUNDDOWN(R27,1)))","v":""},{"$f":"IF(G75=\"\",\"\",ABS(ROUNDDOWN(S27,1)))","v":""},{"$f":"+E65+0.0001","v":0.30010099999999995},null,null,4.08,null,null,null,null,null,null,{"$f":"+U74*('Sile i krakovi'!V209-'Sile i krakovi'!V208)","v":{"$error":"#VALUE!"}},{"$f":"-U76*('Sile i krakovi'!V208-'Sile i krakovi'!R209)","v":{"$error":"#VALUE!"}},"     htem=",{"$f":"-'Sile i krakovi'!AB193","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"VRd,c,min =",{"$f":"+(AF75*0.1+0.15*AH72)*AE59*AE62","v":{"$error":"#VALUE!"}},"kN",null,null,"VRd,c,min =",{"$f":"+AD76*H84","v":{"$error":"#VALUE!"}},"za temelj-kontrafora",null,"VRd,c,min =",{"$f":"+(AO75*0.1+0.15*AP72)*AN59*AN62","v":{"$error":"#VALUE!"}},"kN"]
[{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"    KONZOLA\")","v":"    KONZOLA"},{"$f":"+G78+0.0000001","v":1.0000001000000001},{"$f":"+IF(G78=0,0.000001,H79)","v":0.3},null,null,null,null,{"$f":"+IF('Unos podataka'!G57=\"\",0,E79)","v":3.14},null,null,4.4000000000000004,"  za n =",{"$f":"+M79/(1+M79)","v":0.40913898899476464},null,null,null,null,{"$f":"U70*('Sile i krakovi'!V210-'Sile i krakovi'!V208)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S69:S76)","v":{"$error":"#VALUE!"}},"MI-I",{"$f":"+'Sile i krakovi'!Q259","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"       - maksimalna vrijednost poprečne sile:",null,null,null,null,"za presjek temelj kontrafora",null,null,null,"       - maksimalna vrijednost poprečne sile:"]
[{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"duljina konzole (zida) ..........................................\")","v":"duljina konzole (zida) .........................................."},null,null,{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"lk=\")","v":"lk="},{"$f":"IF('Unos podataka'!G57=\"\",\"\",E49)","v":12},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"m\")","v":"m"},{"$f":"+IF(H77=0,0,H78)","v":1},{"$f":"+IF('Unos podataka'!G57=\"\",0,E80)","v":1},null,null,4.72,"Ko=n/(1-n) =",{"$f":"+M77/(1-M77)","v":0.69244539980509801},null,null,null,null,{"$f":"-U76*('Sile i krakovi'!V208-'Sile i krakovi'!R209)","v":{"$error":"#VALUE!"}},{"$f":"+R75+S77","v":{"$error":"#VALUE!"}},"MII-II",{"$f":"'Sile i krakovi'!R259","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"VRd,max =","acw*b*z*n1*fcd*1/(ctgΘ+tgΘ)",null,null,null,"VRd,max =",{"$f":"(+AH75*AE59*10*AJ75*10*AD75*AD66*10*1/(AJ79+AH79))/1000*H84","v":{"$error":"#VALUE!"}},"kN",null,"VRd,max =","acw*b*z*n1*fcd*1/(ctgΘ+tgΘ)",null,null,null,"VRd,max =",{"$f":"(+AQ75*AN59*10*AS75*10*AM75*AM66*10*1/(AS79+AQ79))/1000","v":{"$error":"#VALUE!"}},"kN"]
[{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"visina podgleda konzole (od dna temelja) .............\")","v":"visina podgleda konzole (od dna temelja) ............."},null,null,{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"hk=\")","v":"hk="},{"$f":"IF(E78=0,\"\",'Unos podataka'!H59)","v":3.14},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"m\")","v":"m"},null,{"$f":"+IF('Unos podataka'!G57=\"\",0,E81)","v":0.3},null,null,5.04,"Ko=1-sinjd1 =",{"$f":"+M110","v":0.69244539980509812},null,null,null,null,null,null,"M III-III",{"$f":"+'Sile i krakovi'!S259","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"kut nagiba tlačnih dijagonala  Θ =",40,"°       tgΘ =",{"$f":"+TAN(AF79*PI()/180)","v":0.83909963117727993},"ctg Θ =",{"$f":"1/AH79","v":1.19175359259421},null,null,null,"kut nagiba tlačnih dijagonala  Θ =",39.799999999999997,"°     tgΘ =",{"$f":"+TAN(AO79*PI()/180)","v":0.83316858923505821},"ctg Θ =",{"$f":"1/AQ79","v":1.2002372784097775}]
[{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"širina konzole .....................................................\")","v":"širina konzole ....................................................."},null,null,{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"bk=\")","v":"bk="},{"$f":"IF(E78=0,\"\",'Unos podataka'!F60)","v":1},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"m\")","v":"m"},null,null,null,null,5.36,null,null,null,"X","y",null,null,null,"M sredina",{"$f":"+'Sile i krakovi'!T259","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"a =",90,"°",null,null,null,null,null,null,"a =",90,"°"]
[{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"visina presjeka konzole ........................................\")","v":"visina presjeka konzole ........................................"},null,null,{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"dk=\")","v":"dk="},{"$f":"IF(E78=0,\"\",'Unos podataka'!F61)","v":0.3},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"m\")","v":"m"},null,null,null,null,5.6800000000000006,"jednadžba pravca klizne plohe",null,null,{"$f":"+(P81-N84)/L84","v":{"$error":"#VALUE!"}},{"$f":"'C III-V'!AF104","v":{"$error":"#VALUE!"}},null,null,null,null,"SM=",null,null,null,null,null,null,null,"      - Provjera:",null,null,null,null,null,null,null,null,"      - Provjera:"]
[{"$f":"+IF(Kontrafore!E3=\"\",\"\",\"   KONTRAFORE\")","v":"   KONTRAFORE"},{"$f":"+IF(A82=\"\",\"CRTEŽ, SHEMA ZIDA ...., TREBA PREMJESTITI NA OVAJ PRAZNI PROSTOR\",\"\")","v":""},null,null,null,null,null,null,{"$f":"IF(Kontrafore!E3=0,\"\",Kontrafore!E10)","v":5.5},null,null,2,0,null,{"$f":"+(P81-N84)/L84-0.2*E48","v":{"$error":"#VALUE!"}},{"$f":"+P81","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,"VRd,c =",{"$f":"+AD73","v":{"$error":"#VALUE!"}},{"$f":"+IF(AD82>AD56,\"kN   >   VEd=\",\"kN   <   VEd=\")","v":{"$error":"#VALUE!"}},{"$f":"+AD56","v":{"$error":"#VALUE!"}},{"$f":"+IF(AG83=\"Postojeća armatura zadovoljava\",\"\",\"kN      <      VRd,max =\")","v":{"$error":"#VALUE!"}},null,{"$f":"+AI78","v":{"$error":"#VALUE!"}},"kN",null,"VRd,c =",{"$f":"+AM73","v":{"$error":"#VALUE!"}},{"$f":"+IF(AM73>AM56,\"kN    >    VEd=\",\"kN     <     VEd=\")","v":{"$error":"#VALUE!"}},{"$f":"+AM56","v":{"$error":"#VALUE!"}},{"$f":"+IF(AP83=\"Postojeća armatura zadovoljava\",\"\",\"kN             <            VRd,max =\")","v":{"$error":"#VALUE!"}},null,{"$f":"+AR78","v":{"$error":"#VALUE!"}},"kN"]
[{"$f":"+IF(Kontrafore!E3=\"\",\"\",\"duljina temelja kontrafore ..................\")","v":"duljina temelja kontrafore .................."},null,{"$f":"+IF(Kontrafore!E3=\"\",\"\",\"l =\")","v":"l ="},{"$f":"+IF(Kontrafore!E3=0,\"\",'Unos podataka'!AB3)","v":1},{"$f":"+IF(Kontrafore!E3=0,\"\",\"m\")","v":"m"},null,{"$f":"+IF(Kontrafore!E3=0,\"\",\"duljina kontrafore dk=\")","v":"duljina kontrafore dk="},{"$f":"+IF(Kontrafore!E3=0,\"\",Kontrafore!E7)","v":1.9000001},{"$f":"+IF(Kontrafore!E3=0,\"\",\"m\")","v":"m"},null,null,{"$f":"+'C III-V'!AE104","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AF104","v":{"$error":"#VALUE!"}},null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(AD73<AD56,\"Potrebne su spone\", \"Postojeća armatura zadovoljava \")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"+IF(AM73<AM56,\"Potrebne su spone\", \"Postojeća armatura zadovoljava \")","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(Kontrafore!E3=\"\",\"\",\"širina temelja kontrafore.....................\")","v":"širina temelja kontrafore....................."},null,{"$f":"+IF(Kontrafore!E3=\"\",\"\",\"b₁=\")","v":"b₁="},{"$f":"+IF(Kontrafore!E3=0,\"\",'Unos podataka'!AB4)","v":1},null,null,{"$f":"+IF(Kontrafore!E3=0,\"\",\"m         osni razmak kontrafora lk=\")","v":"m         osni razmak kontrafora lk="},{"$f":"IF(Kontrafore!E3=0,\"\",Kontrafore!E8)","v":4},{"$f":"+IF(Kontrafore!E3=0,\"\",\"m\")","v":"m"},null,null,{"$f":"++(M83-M82)/(L83-L82)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-L84*L82+M82","v":{"$error":"#VALUE!"}},{"$f":"+(P84-N84)/L84-0.2*E48","v":{"$error":"#VALUE!"}},{"$f":"-P85-P86","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(AH84=\"\",\"\",\"Proračun poprečne armature\")","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+IF(AD73>AD56,\"\",\"m =\")","v":{"$error":"#VALUE!"}},1,null,null,{"$f":"+IF(AM73>AM56,\"\",\"      - proračun poprečne armature:\")","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+IF(AM73>AM56,\"\",\"m =\")","v":{"$error":"#VALUE!"}},1]
[{"$f":"+IF(Kontrafore!E3=\"\",\"\",\"broj kontrafora ..............................................\")","v":"broj kontrafora .............................................."},null,{"$f":"+IF(Kontrafore!E3=\"\",\"\",\"n =\")","v":"n ="},{"$f":"IF(D83=0,\"\",'Unos podataka'!AB5)","v":3},null,null,{"$f":"+IF(Kontrafore!E3=0,\"\",\"visina kontrafore hk=\")","v":"visina kontrafore hk="},{"$f":"IF(Kontrafore!E3=0,\"\",I82-E52)","v":4.3},{"$f":"+IF(Kontrafore!E3=0,\"\",\"m\")","v":"m"},null,null,"Razmak do sidrene linije d=",{"$f":"0.2*E48","v":1.2000000000000002},"m",{"$f":"+(P85-N84)/L84","v":{"$error":"#VALUE!"}},0,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(AH84=\"\",\"\",\"spone   f=\")","v":{"$error":"#VALUE!"}},{"$f":"IF(AH84=\"\",\"\",+'Unos podataka'!E94)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AH84=\"\",\"\",\"Asw=\")","v":{"$error":"#VALUE!"}},{"$f":"IF(AD73>AD56,\"\",+AI84*AD85^2*PI()/4/100)","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(AD73>AD56,\"\",\"     razmak spona:\")","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+IF(AM73>AM56,\"\",\"spone  ф =\")","v":{"$error":"#VALUE!"}},{"$f":"IF(AL85=\"\",\"\",+'Unos podataka'!E97)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AM73>AM56,\"\",\"A¹sw =\")","v":{"$error":"#VALUE!"}},{"$f":"IF(AM73>AM56,\"\",+AR84*AM85^2*PI()/4/100)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AM73>AM56,\"\",\"cm²\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(AM73>AM56,\"\",\"     razmak spona:\")","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(Kontrafore!E3=\"\",\"\",\"širina kontrafore ...................................\")","v":"širina kontrafore ..................................."},null,{"$f":"+IF(Kontrafore!E3=\"\",\"\",\"b =\")","v":"b ="},{"$f":"+IF(Kontrafore!E3=0,\"\",Kontrafore!E6)","v":0.25},{"$f":"+IF(Kontrafore!E3=0,\"\",\"m\")","v":"m"},null,null,null,null,null,null,"a=",{"$f":"+ATAN(L84)*180/PI()","v":{"$error":"#VALUE!"}},null,"Y*=",{"$f":"+COS(M86*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(AD73>AD56,\"\",\"      - maksimalni razmak spona:\")","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+IF(AC73>AC56,\"\",\"S₁ =\")","v":""},{"$f":"+IF(AD73>AD56,\"\",\"S₁ =\")","v":{"$error":"#VALUE!"}},{"$f":"IF(AD73>AD56,\"\",+AF85*AJ75*AG66*AJ79/AD56)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AD73>AD56,\"\",\"cm\")","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(AM73>AM56,\"\",\"      - maksimalni razmak spona:\")","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+IF(AM73>AM56,\"\",\"S₁ =\")","v":{"$error":"#VALUE!"}},{"$f":"IF(AN60=0,0,IF(AM73>AM56,\"\",+AO85*AS75*AP66*AS79/AM56))","v":{"$error":"#VALUE!"}},{"$f":"+IF(AM73>AM56,\"\",\"cm\")","v":{"$error":"#VALUE!"}}]
[null,null,"Temelj ili vozilo",null,null,null,"Voda iza zida",null,"Zid i temelj",null,0.2,{"$f":"IF(E24>0.1,+ROUNDUP(E48,),ROUNDUP(E48+2,)-1)","v":6},null,{"$f":"+'C III-V'!B25-2.3","v":{"$error":"#VALUE!"}},{"$f":"+'Dijagram momenata'!$Q$22","v":{"$error":"#VALUE!"}},{"$f":"IF(E24=0,Q87,'C III-V'!W14)","v":{"$error":"#VALUE!"}},{"$f":"'C III-V'!B9","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(AD73>AD56,\"\",\"ρw,min =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(AD73>AD56,\"\",IF((0.08*SQRT(AD65)/AG65>0.15*2.2/AG66*10),0.08*SQRT(AD65)/AG65,0.15*2.2/(AG66*10)))","v":{"$error":"#VALUE!"}},null,null,{"$f":"+IF(AC73>AC56,\"\",\"S₁,max =\")","v":""},{"$f":"+IF(AD73>AD56,\"\",\"S₁,max =\")","v":{"$error":"#VALUE!"}},{"$f":"IF(AD73>AD56,\"\",+AF85/(AD87*AE59*SIN(AF80*PI()/180)))","v":{"$error":"#VALUE!"}},{"$f":"+AJ86","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(AM73>AM56,\"\",\"ρw,min =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(AM73>AM56,\"\",IF((0.08*SQRT(AM65)/AP65>0.15*2.2/AP66*10),0.08*SQRT(AM65)/AP65,0.15*2.2/(AP66*10)))","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+IF(AM73>AM56,\"\",\"S₁,max =\")","v":{"$error":"#VALUE!"}},{"$f":"IF(AM73>AM56,\"\",+AO85/(AM87*AN59*SIN(AO80*PI()/180)))","v":{"$error":"#VALUE!"}},{"$f":"+AS86","v":{"$error":"#VALUE!"}}]
[null,"Točkasto",{"$f":"IF(A28=\"OPTEREĆENJE TEMELJEM ....................\",'C III-V'!W38,C91)","v":{"$error":"#VALUE!"}},{"$f":"IF(E28=0,-5,+D89+0.5)","v":{"$error":"#VALUE!"}},"(m)  na os   i y",null,{"$f":"IF(H88<0,7,IF(H88>=E52,2+E59-(E41-E51)/F57,2+E60*(E52-E41)/E52))","v":2},{"$f":"E41","v":0.6},{"$f":"+'C III-V'!B2","v":2},{"$f":"+'C III-V'!C2","v":0.12820515121628623},{"$f":"+ROUNDUP('C III-V'!$AH$45,)","v":8},0.2,null,{"$f":"+N90","v":5.4000021999999994},{"$f":"+O87","v":{"$error":"#VALUE!"}},{"$f":"IF(E24=0,Q88,'C III-V'!X14)","v":6.2644906473896782},{"$f":"+'C III-V'!C9","v":"A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(AM73>AM56,\"\",\"Smax =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(AM73>AM56,\"\",IF(AR87<30,AR87,30))","v":{"$error":"#VALUE!"}},{"$f":"+IF(AM73>AM56,\"\",\"cm\")","v":{"$error":"#VALUE!"}}]
[{"$f":"+'C III-V'!W23","v":{"$error":"#VALUE!"}},{"$f":"+E48+'HT III-XX'!E53","v":{"$error":"#VALUE!"}},{"$f":"+C88","v":{"$error":"#VALUE!"}},{"$f":"IF(E28=0,-5,IF(A28=\"OPTEREĆENJE TEMELJEM ....................\",'C III-V'!X34,D90))","v":{"$error":"#VALUE!"}},0,{"$f":"+E48+1","v":7},{"$f":"+G90+0.05","v":-1.8499999999999999},{"$f":"+H88","v":0.6},{"$f":"+'C III-V'!B3","v":2},{"$f":"+'C III-V'!C3","v":1.2},{"$f":"-IF(F190/100>F193/100,F190/100,F193/100)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+N87","v":{"$error":"#VALUE!"}},{"$f":"+'Dijagram momenata'!$Q$21","v":{"$error":"#VALUE!"}},{"$f":"+N93-0.1","v":3.3000010999999998},{"$f":"+E52+0.01","v":1.21},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(AC73>AC56,\"\",\"Smax =\")","v":""},{"$f":"+IF(AD73>AD56,\"\",\"Smax =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(AD73>AD56,\"\",IF(AI87<30,AI87,30))","v":{"$error":"#VALUE!"}},{"$f":"+IF(AD73>AD56,\"\",\"cm\")","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"+'C III-V'!W37","v":{"$error":"#VALUE!"}},{"$f":"IF(E28=0,-5,IF(A28=\"OPTEREĆENJE TEMELJEM ....................\",'C III-V'!X34,D91))","v":{"$error":"#VALUE!"}},"(m)  na os   i   x",null,{"$f":"+G91+0.05","v":-1.9},{"$f":"+H92-0.25","v":0.35},{"$f":"+'C III-V'!B4","v":3.4000010999999999},{"$f":"+'C III-V'!C4","v":1.2},0.2,{"$f":"+ROUNDUP(K89-1,)","v":{"$error":"#VALUE!"}},null,{"$f":"+N96","v":5.4000021999999994},{"$f":"+Q44","v":{"$error":"#VALUE!"}},{"$f":"+N92+0.1","v":4.3000010999999994},{"$f":"+Q89","v":1.21},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(AD73>AD56,\"\",\"Asw =\")","v":{"$error":"#VALUE!"}},{"$f":"IF(AD73>AD56,\"\",AF85*100/AI86)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AD73>AD56,\"\",\"cm²\")","v":{"$error":"#VALUE!"}},{"$f":"IF(AD73>AD56,\"\",ROUND(AD90/AF85,0)+1)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AD73<AD56,\"kom/m'\",\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+IF(AM73>AM56,\"\",\"Asw =\")","v":{"$error":"#VALUE!"}},{"$f":"IF(AM73>AM56,\"\",AO85*100/AR86)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AM73>AM56,\"\",\"cm²\")","v":{"$error":"#VALUE!"}},{"$f":"IF(AM73>AM56,\"\",ROUND(AM90/AO85,0)+1)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AM73<AM56,\"kom/m'\",\"\")","v":{"$error":"#VALUE!"}}]
["Voda izvan",null,{"$f":"+'C III-V'!W37","v":{"$error":"#VALUE!"}},{"$f":"IF(E28=0,-5,IF(A28=\"OPTEREĆENJE TEMELJEM ....................\",'C III-V'!X35,E48+E31))","v":{"$error":"#VALUE!"}},{"$f":"2+E61+2","v":6.9000021999999994},0.2,{"$f":"-2+0.05","v":-1.95},{"$f":"+H92+0.25","v":0.85},null,null,null,null,null,{"$f":"+'C III-V'!B11","v":4.2000010999999997},{"$f":"+O93","v":1.3}]
[{"$f":"IF(E42<=E52,2+E61+E60,2+E59+E55-(B92-E52)/F56)","v":4.9000021999999994},{"$f":"IF(E42=0,-5,+E42)","v":0.8},{"$f":"+'C III-V'!W34","v":{"$error":"#VALUE!"}},{"$f":"+D91","v":{"$error":"#VALUE!"}}," *100kN/m2",null,{"$f":"-2+0.05","v":-1.95},{"$f":"+H93","v":0.6},null,null,null,{"$f":"+'C III-V'!AE101","v":0},{"$f":"+'C III-V'!AF101","v":0},{"$f":"+N91","v":4.2000010999999997},0]
[{"$f":"+A92+2","v":6.9000021999999994},{"$f":"+B92","v":0.8},{"$f":"+C92","v":{"$error":"#VALUE!"}},{"$f":"+D90","v":{"$error":"#VALUE!"}},0.2,{"$f":"-+IF(MAX(F190:F195)/100<2,2)","v":{"$error":"#VALUE!"}},-8,{"$f":"+H88","v":0.6},null,null,null,{"$f":"+'C III-V'!AE104","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AF104","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!B4","v":3.4000010999999999},{"$f":"+E52+0.1","v":1.3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD85","v":{"$error":"#VALUE!"}},{"$f":"+IF(AC86=\"\",\"\",\"na razmaku\")","v":{"$error":"#VALUE!"}},{"$f":"IF(AE93=\"\",\"\",+MIN(AI86:AI89))","v":{"$error":"#VALUE!"}},{"$f":"+IF(AE93=\"\",\"\",\"cm\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+AM85","v":{"$error":"#VALUE!"}},{"$f":"+IF(AL86=\"\",\"\",\"na razmaku\")","v":{"$error":"#VALUE!"}},{"$f":"IF(AN93=\"\",\"\",+MIN(AR86:AR88))","v":{"$error":"#VALUE!"}},{"$f":"+IF(AN93=\"\",\"\",\"cm\")","v":{"$error":"#VALUE!"}}]
[{"$f":"+'C III-V'!Y101","v":1.75},0,{"$f":"IF(A28=\"OPTEREĆENJE TEMELJEM ....................\",+C93-0.3,C93)","v":{"$error":"#VALUE!"}},{"$f":"+D93","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Unos podataka'!T55-'Unos podataka'!$F$9","v":6},{"$f":"+'C III-V'!U7","v":{"$error":"#VALUE!"}},null,null,null," ",-2.8,{"$f":"+N93+E60","v":3.4000010999999999},{"$f":"+O92","v":0},null,null,null,null,null,null,null,null,null,null,"Dimenzioniranje  presjeka radi redukcije Poz.7  "]
[{"$f":"+'C III-V'!Y102","v":0.97707863658009864},{"$f":"+'C III-V'!$Z$102","v":1.2},{"$f":"+C94","v":{"$error":"#VALUE!"}},{"$f":"+D88","v":{"$error":"#VALUE!"}},null,{"$f":"+'Unos podataka'!S55","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!T56","v":6},{"$f":"+'C III-V'!U8","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+(M93-M92)/(L92-L93)","v":{"$error":"#VALUE!"}},{"$f":"+ATAN(L95)*180/PI()","v":{"$error":"#VALUE!"}},{"$f":"2-0.3","v":1.7},{"$f":"+E52+0.03","v":1.23},null,null,null,"kom","3 Karakteristične točke sidra",null,"Poz 6a"]
[{"$f":"+'C III-V'!Y103","v":-1.0572404418349119},{"$f":"+'C III-V'!$Z$103","v":4},{"$f":"IF(A28=\"OPTEREĆENJE TEMELJEM ....................\",C95,+C88)","v":{"$error":"#VALUE!"}},{"$f":"+D88","v":{"$error":"#VALUE!"}},"1.sloj dno",{"$f":"+'Unos podataka'!S56","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!T57","v":6.2644906473896782},{"$f":"+'C III-V'!U9","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+SQRT((M93*M93+(-L93+L92)*(-L93+L92)))","v":{"$error":"#VALUE!"}},{"$f":"0.2*L96","v":{"$error":"#VALUE!"}},{"$f":"2+E61+0.5","v":5.4000021999999994},{"$f":"+O95","v":1.23},null,"Koordinate armature Poz. 6a",null,{"$f":"IF(R100=0,-3,S97+0.15)","v":{"$error":"#VALUE!"}},{"$f":"+IF($P$22>0,1,0)","v":1},null,null,{"$f":"+IF(U28=0,-20,R98)","v":{"$error":"#VALUE!"}},null,null,null,"presjek na visini (m)",{"$f":"+AB97","v":3.44}]
[{"$f":"+'C III-V'!Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!$Z$104","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!B29","v":{"$error":"#VALUE!"}},{"$f":"+E48-D17","v":4},{"$f":"+'Unos podataka'!B105","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!T58","v":6.2644906473896782},-8,null,null,null,{"$f":"IF(A67=\"\",0,+'C III-V'!U104-0.2*E48)","v":{"$error":"#VALUE!"}},{"$f":"+IF(P25+Q25+R25+S25+T25=0,\"\",P82)","v":{"$error":"#VALUE!"}},null,"x","x","y",null,{"$f":"IF(R100=0,-3,P22+0.06)","v":{"$error":"#VALUE!"}},{"$f":"+IF($P$22>0,1,0)","v":1},{"$f":"+U98+1.5","v":{"$error":"#VALUE!"}},{"$f":"+V98+(U97-U98)*TAN($E$39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"IF(U28=0,-20,R100+1.2)","v":{"$error":"#VALUE!"}},null,null,null,"hk=",{"$f":"IF(E79>0,+E79+E81,AB44)","v":3.44},"      MEd=",{"$f":"+IF(AB97>=AI44,AI45,IF($AB$97>=$AH$44,AH45,IF($AB$97>=$AG$44,AG45,IF($AB$97>=$AF$44,AF45,IF($AB$97>=$AE$44,AE45,IF($AB$97>=$AD$44,AD45,IF($AB$97>=$AC$44,AC45,IF($AB$97>=$AB$44,AB45,AA45))))))))*1.35","v":{"$error":"#VALUE!"}},"kNm/m'   ","      NEd=",{"$f":"+IF(AB97>AI44,AI48,IF($AB$97>=$AH$44,AH48,IF($AB$97>=$AG$44,AG48,IF($AB$97>=$AF$44,AF48,IF($AB$97>=$AE$44,AE48,IF($AB$97>=$AD$44,AD48,IF($AB$97>=$AC$44,AD48,IF($AB$97>=$AB$44,AB48,AA45))))))))","v":{"$error":"#VALUE!"}},"kN/m'"]
[{"$f":"+'Unos podataka'!$B$103","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!$C$103","v":6},null,-8,{"$f":"E97+(D97-D98)*TAN(D18*PI()/180)","v":{"$error":"#VALUE!"}},-8,null,null,{"$f":"+'C III-V'!V10","v":6.2644906473896782},{"$f":"+'C III-V'!C13","v":1.2},null,{"$f":"IF(A67=\"\",0,+'C III-V'!U101-0.2*E48)","v":0.54999999999999982},0,{"$f":"+IF(P25+Q25+R25+S25+T25=0,\"\",P83)","v":0},"sidro I",{"$f":"IF(P25=0,-20,P100+0.5)","v":{"$error":"#VALUE!"}},{"$f":"+Q100","v":5},{"$f":"IF(E56=\">100\",R100,R99-(S96-S97)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"+P22","v":5},null,{"$f":"+P100","v":{"$error":"#VALUE!"}},{"$f":"+Q100","v":5},null,{"$f":"IF(U28=0,0,S96)","v":{"$error":"#VALUE!"}},null,null,"MEd (kNm/m')",null,"     MEds=",{"$f":"+'Dijagram momenata'!P27","v":{"$error":"#VALUE!"}},{"$f":"+IF(AG98<AD99,\"kNm/m' >\",\"kNm/m'     <\")","v":{"$error":"#VALUE!"}},"      MRd,lim=",{"$f":"+E367","v":{"$error":"#VALUE!"}},"kN/m'"]
[{"$f":"+A94-0.2*$E$48","v":0.54999999999999982},{"$f":"+B94","v":0},null,-8,{"$f":"E98+(D98-D99)*TAN(D18*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+'C III-V'!B14","v":4.9000021999999994},{"$f":"+'C III-V'!C14","v":1.2},null,"Poz. 1",{"$f":"+SQRT(E61^2+(E52-E51)^2)","v":2.94278996192471},null,null,{"$f":"IF(P25=0,-20,P98-1)","v":{"$error":"#VALUE!"}},{"$f":"+Q98","v":5},{"$f":"IF(E56=\">100\",R100,R100-(S97-P22)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"IF(R100=0,-3,P22-0.09)","v":{"$error":"#VALUE!"}},{"$f":"+IF($P$22>0,1,0)","v":1},{"$f":"+P102","v":{"$error":"#VALUE!"}},{"$f":"+V98-(U98-U99)*TAN($E$39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"IF(U28=0,-20,R99)","v":{"$error":"#VALUE!"}},{"$f":"IF(U28=0,0,(X98+X107)/2)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+ABS(AD98)","v":{"$error":"#VALUE!"}},null,"fyd =",{"$f":"+G369","v":43.478260869565219},"kN/cm2"]
[{"$f":"+A97-0.2*$E$48","v":{"$error":"#VALUE!"}},{"$f":"+B97","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+'C III-V'!B15","v":4.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5},null,"Poz. 2",{"$f":"+E61","v":2.9000021999999994},null,null,{"$f":"IF(P22=0,-20,R100+0.07)","v":{"$error":"#VALUE!"}},{"$f":"IF(P25=0,0,P22)","v":5},{"$f":"IF(Q100=0,0,'C III-V'!Z35-0.035)","v":{"$error":"#VALUE!"}},{"$f":"IF(R100=0,-3,S99-0.15)","v":{"$error":"#VALUE!"}},{"$f":"+IF($P$22>0,1,0)","v":1},null,null,{"$f":"+W97","v":{"$error":"#VALUE!"}},null,null,null,null,null,"   b=",100,"cm ","fcd =",{"$f":"+G370","v":1.7},"kN/cm2"]
[{"$f":"IF(A83=\"\",-15,+A94)","v":1.75},{"$f":"+B94","v":0},null,{"$f":"+'Unos podataka'!I121","v":4},{"$f":"+'Unos podataka'!C114","v":"Točke"},null,null,null,{"$f":"+'C III-V'!B16","v":2},{"$f":"+'C III-V'!C16","v":0.12820515121628623},null,null,null,null,null,{"$f":"+P100-P23*COS(E39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+Q100-P23*SIN(E39*PI()/180)","v":3.4729676338951276},{"$f":"IF(E56=\">100\",R100,R100+(P22-S99)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"IF(R105=0,-3,S102+0.15)","v":{"$error":"#VALUE!"}},{"$f":"+IF($Q$22>0,1,0)","v":1},null,null,null,{"$f":"IF(U28=0,0,S97)","v":{"$error":"#VALUE!"}},null,null,null,null,"  h=",{"$f":"+IF($AB$97>=$AH$44,AH49,IF($AB$97>=$AG$44,AG49,IF($AB$97>=$AF$44,AF49,IF($AB$97>=$AE$44,AE49,IF($AB$97>=$AD$44,AD49,IF($AB$97>=$AC$44,AC49,IF($AB$97>=$AB$44,AB49,AA49)))))))","v":{"$error":"#VALUE!"}},"cm ","  mSd=",{"$f":"+G315","v":{"$error":"#VALUE!"}}]
[{"$f":"+A101","v":1.75},{"$f":"+B95","v":1.2},null,{"$f":"+'Unos podataka'!I122","v":{"$error":"#VALUE!"}},"tgj","j","kh=",{"$f":"+E44*E46/E45","v":0.1},"tgQ=",{"$f":"IF(E41<=E52,H102/(1+H103),G16*H102/(G16-10)/(1+H103))","v":9.5238095238095233E-2},null,null,null,null,null,{"$f":"+P101-$D$73*COS($E$39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+Q101-$D$73*SIN($E$39*PI()/180)","v":1.7388800317082387},{"$f":"IF(E56=\">100\",R100,R101+(S99-S100)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"IF(R105=0,-3,Q22+0.06)","v":{"$error":"#VALUE!"}},{"$f":"+IF($Q$22>0,1,0)","v":1},{"$f":"+U103+1.5","v":{"$error":"#VALUE!"}},{"$f":"+V103+(U102-U103)*TAN($E$39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"IF(U28=0,-20,R101)","v":{"$error":"#VALUE!"}},{"$f":"+X99","v":{"$error":"#VALUE!"}},null,null,null,null,"d1=",{"$f":"+B315","v":5},"cm ","ζ =",{"$f":"+G316","v":{"$error":"#VALUE!"}}]
["Dužina od vrha zida do sjecišta j i b    X =",null,{"$f":"+A98-A97","v":{"$error":"#VALUE!"}},1,{"$f":"+TAN(D14*PI()/180)/J27","v":0.32322098066812543},{"$f":"+ATAN(E103)*180/PI()","v":17.911920978999142},"kv=",{"$f":"+H102/2","v":0.05},"Q=",{"$f":"+ATAN(J102)*180/PI()","v":5.4403320310055063},null,"Prosječna vrijenost koeficijenta tlaka ili tlaka mirovanja za slojeve tla   ",null,null,"sidro II",{"$f":"IF(Q25=0,-20,P105+0.5)","v":{"$error":"#VALUE!"}},{"$f":"+Q105","v":3},{"$f":"IF(E56=\">100\",R105,R104-(S101-S102)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"+Q22","v":3},null,{"$f":"+P105","v":{"$error":"#VALUE!"}},{"$f":"+Q105","v":3},{"$f":"+W97","v":{"$error":"#VALUE!"}},null,null,null,null,null,"d=",{"$f":"AD101-AD102","v":{"$error":"#VALUE!"}},"cm "]
[null,null,null,2,{"$f":"+TAN(E14*PI()/180)/J27","v":0.25993575698632504},{"$f":"+ATAN(E104)*180/PI()","v":14.57076836070997},{"$f":"+IF(F103<=23,0,IF(F103<=28,0.5*F103,2*F103/3))","v":0},"Ka1","Ka2","Ka3",null,"Ki=",{"$f":"+IF('Unos podataka'!F13=\"Ko\",M112,IF(E44>0,M109,M115))","v":0.7086817997211472},null,"S h=",{"$f":"IF(Q25=0,-20,P103-1)","v":{"$error":"#VALUE!"}},{"$f":"+Q103","v":3},{"$f":"IF(E56=\">100\",R105,R105-(S102-Q22)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"IF(R105=0,-3,Q22-0.09)","v":{"$error":"#VALUE!"}},{"$f":"+IF($Q$22>0,1,0)","v":1},{"$f":"+P107","v":{"$error":"#VALUE!"}},{"$f":"+V103-(U103-U104)*TAN($E$39*PI()/180)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(U28=0,0,S99)","v":{"$error":"#VALUE!"}},null,null,"Popr. sila Ved=",{"$f":"+IF($AB$97>=$AH$44,AH51,IF($AB$97>=$AG$44,AG51,IF($AB$97>=$AF$44,AF51,IF($AB$97>=$AE$44,AE51,IF($AB$97>=$AD$44,AD51,IF($AB$97>=$AC$44,AC51,IF($AB$97>=$AB$44,AB51,AA51)))))))","v":{"$error":"#VALUE!"}},"kN",null,null,"     As1,min≥",{"$f":"0.0015*AD100*AD103","v":{"$error":"#VALUE!"}},"cm2"]
[null,null,null,null,{"$f":"+TAN(F14*PI()/180)/J27","v":0.29117618741296186},{"$f":"+ATAN(E105)*180/PI()","v":16.234302131351505},{"$f":"+IF(F104<=23,0,IF(F104<=28,0.5*F104,2*F104/3))","v":0},{"$f":"IF(E44=0,SIN((90-C47+F103)*PI()/180)^2,SIN((90-C47+F103-J103)*PI()/180)^2)","v":0.91960514591160514},{"$f":"IF(E44=0,SIN((90-C47+F104)*PI()/180)^2,SIN((90-C47+F104-J103)*PI()/180)^2)","v":0.94839439752214283},{"$f":"IF(E44=0,SIN((90-D47+F105)*PI()/180)^2,SIN((90-D47+F105-J103)*PI()/180)^2)","v":0.96492697466368027},null,"Ko  zasipa =",{"$f":"1-SIN((F107*PI()/180))","v":0.58068606531123268},null,null,{"$f":"IF(Q25=0,-20,R105+0.07)","v":{"$error":"#VALUE!"}},{"$f":"IF(Q25=0,0,Q22)","v":3},{"$f":"IF(Q105=0,0,'C III-V'!Z33-0.035)","v":{"$error":"#VALUE!"}},{"$f":"IF(R100=0,-3,S104-0.15)","v":{"$error":"#VALUE!"}},{"$f":"+IF($Q$22>0,1,0)","v":1},null,null,{"$f":"IF(U28=0,-20,R102)","v":{"$error":"#VALUE!"}},{"$f":"+X102","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"     As1,max=",{"$f":"0.31*AD100*AD103*AG100/AG99","v":{"$error":"#VALUE!"}},"cm2"]
[null,null,null,null,{"$f":"+TAN(G14*PI()/180)/J27","v":0.25993575698632504},{"$f":"+ATAN(E106)*180/PI()","v":14.57076836070997},{"$f":"+IF(F105<=23,0,IF(F105<=28,0.5*F105,2*F105/3))","v":0},{"$f":"IF(E44=0,SIN((90-C47)*PI()/180)^2*SIN((90-C47-G104)*PI()/180),COS(J103*PI()/180)*SIN((90-C47)*PI()/180)^2*SIN((90-C47-J103)*PI()/180))","v":0.99033842321851395},{"$f":"IF(E44=0,SIN((90-C47)*PI()/180)^2*SIN((90-C47-G105)*PI()/180),COS(J103*PI()/180)*SIN((90-C47)*PI()/180)^2*SIN((90-C47-J103)*PI()/180))","v":0.99033842321851395},{"$f":"IF(E44=0,SIN((90-D47)*PI()/180)^2*SIN((90-D47-G106)*PI()/180),COS(J103*PI()/180)*SIN((90-D47)*PI()/180)^2*SIN((90-D47-J103)*PI()/180))","v":0.99101123595505614},null,null,null,null,null,{"$f":"+P105-Q23*COS(E39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+Q105-Q23*SIN(E39*PI()/180)","v":1.7317866789976484},{"$f":"IF(E56=\">100\",R105,R105+(Q22-S104)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"IF(R110=0,-3,S107+0.15)","v":-3},{"$f":"+IF($R$22>0,1,0)","v":0},null,null,{"$f":"+W103","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+A375","v":"odabrano:"},{"$f":"+B375","v":"f"},{"$f":"+C375","v":12},null," potrebno As1=",{"$f":"ABS(IF(AD98<AG98,ABS(AD98)*100/(AG99*AG102*AD103)+AG97/AG99,AG98*100/(BF89*AD103*AG99)+((AD98-AG98)*100)/((AD103-AD102)*AG99)+AG97/AG99))","v":{"$error":"#VALUE!"}},"cm2"]
[null,null,null,null,{"$f":"+TAN(H14*PI()/180)/J27","v":0.4618802153517006},{"$f":"+ATAN(E107)*180/PI()","v":24.79128089714489},null,{"$f":"IF(E24>0,IF(E44=0,SIN((F103+G104)*PI()/180)*SIN((F103-0)*PI()/180),SIN((F103*PI()/180)*SIN((F103-J103-0)*PI()/180))),IF(E44=0,SIN((F103+G104)*PI()/180)*SIN((F103-H20)*PI()/180),SIN((F103*PI()/180)*SIN((F103-J103-H20)*PI()/180))))","v":6.7461157272396766E-2},{"$f":"IF(F104-J103-D18<0,0,IF(E44=0,SIN((F104+G105)*PI()/180)*SIN((F104-D18)*PI()/180),SIN((F1120*PI()/180)*SIN((F104-J103-D18)*PI()/180))))","v":0},{"$f":"IF(IF(E44=0,SIN((F105+G106)*PI()/180)*SIN((F105-E18)*PI()/180),SIN((F105*PI()/180)*SIN((F105-J103-E18)*PI()/180)))<0,0.000015,IF(E44=0,SIN((F105+G106)*PI()/180)*SIN((F105-E18)*PI()/180),SIN((F105*PI()/180)*SIN((F105-J103-E18)*PI()/180))))","v":3.3512933905284654E-2},null,"K1=",{"$f":"+K132","v":0.59693740409312213},null,null,{"$f":"+P106-$E$73*COS($E$39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+Q106-$E$73*SIN($E$39*PI()/180)","v":0.48945526250554883},{"$f":"IF(E56=\">100\",R105,R106+(S104-S105)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"IF(R110=0,-3,R22+0.06)","v":-3},{"$f":"+IF($R$22>0,1,0)","v":0},{"$f":"+U108+1.5","v":-18.5},{"$f":"+V108+(U107-U108)*TAN($E$39*PI()/180)","v":0.40192378864668404},null,{"$f":"IF(U28=0,0,S100)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+A376","v":"potrebno:"},{"$f":"IF(H54=\"šipka\",TRUNC(AG107/(PI()*AD106*AD106/400))+1)","v":{"$error":"#VALUE!"}},{"$f":"+C376","v":"kom/m'"},null," mjerodavno: As1=",{"$f":"+MAX(AG106,AG104)","v":{"$error":"#VALUE!"}},"cm2"]
[{"$f":"IF('Unos podataka'!F13=\"Ko\",\"          TLAK MIROVANJA\",IF(E44>0,\"         AKTIVNI SEIZMIČKI TLAK\",\"         AKTIVNI TLAK \"))","v":"         AKTIVNI SEIZMIČKI TLAK"},null,null,null,null,null,null,{"$f":"IF(E24>0,IF(E44=0,SIN((90-C47-G104)*PI()/180)*SIN((90-C47+0)*PI()/180),SIN((90-C47-J103)*PI()/180)*SIN((90-E50-0)*PI()/180)),IF(E44=0,SIN((90-E50-2*G104)*PI()/180)*SIN((90-E50+H20)*PI()/180),SIN((90-E50-J103)*PI()/180)*SIN((90-C47-H20)*PI()/180)))","v":0.9972488635503951},{"$f":"IF(E44=0,SIN((90-C47-G105)*PI()/180)*SIN((90-C47+D18)*PI()/180),SIN((90-C47-J103)*PI()/180)*SIN((90-C47-D18)*PI()/180))","v":0.99907506312792527},{"$f":"IF(E44=0,SIN((90-D47-G106)*PI()/180)*SIN((90-D47+E18)*PI()/180),SIN((90-D47-J103)*PI()/180)*SIN((90-D47-E18)*PI()/180))","v":0.99307049565614069},null,"K2=",{"$f":"+L132","v":0.78849922516973658},null,null,{"$f":"IF(R25=0,-20,P110+0.5)","v":-20},{"$f":"+Q110","v":0},{"$f":"IF(E56=\">100\",R110,R109-(S106-S107)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"+R22","v":0},null,{"$f":"+P110","v":-20},{"$f":"+Q110","v":0},null,{"$f":"+X105","v":{"$error":"#VALUE!"}},null,null,null,"odabrano:",{"$f":"IF(B322=\"\",F322,IF(+AC107<=5,5,AD110))","v":{"$error":"#VALUE!"}},{"$f":"IF(AC107=0,G322,+C377)","v":{"$error":"#VALUE!"}},null,{"$f":"+E377","v":"A₁="},{"$f":"IF(H54=\"šipka\",+AD106*AD106*PI()*(AC108)/400)","v":{"$error":"#VALUE!"}},{"$f":"IF(AC107>0,\"cm²\",\"\")","v":{"$error":"#VALUE!"}}]
[null,"Ea (kN/m')","Eh (kN/m')","Ev (kN/m')",{"$f":"IF('Unos podataka'!$F$13=\"Ko\",\"        Ko=1-sinϕd\",IF(F112=N111,\"\",IF(F112=J112,\"      Coulumb-Poncelot\",\"      Mononobe-Okabe\")))","v":"      Mononobe-Okabe"},null,null,{"$f":"IF(H107<=0,0,SQRT(H107/H108))","v":0.2600908766690041},{"$f":"SQRT(I107/I108)","v":0},{"$f":"SQRT(J107/J108)","v":0.18370297324861343},null,"prosječni računski K1=",{"$f":"+(M107*K111+M108*K112)/(K111+K112)","v":0.7086817997211472},null,null,{"$f":"IF(R25=0,-20,P108-1)","v":-20},{"$f":"+Q108","v":0},{"$f":"IF(E56=\">100\",R110,R110-(S107-R22)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"IF(R110=0,-3,R22-0.09)","v":-3},{"$f":"+IF($R$22>0,1,0)","v":0},{"$f":"+P112","v":-20},{"$f":"+V108-(U108-U109)*TAN($E$39*PI()/180)","v":0},null,null,null,null,null,null,"Potrebno iznad presjeka",{"$f":"+AC108","v":{"$error":"#VALUE!"}},{"$f":"+AD108","v":{"$error":"#VALUE!"}}]
["sloj 1. .......................",{"$f":"+'C III-V'!B85","v":{"$error":"#VALUE!"}},{"$f":"+B110*COS((G104-$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"ABS(B110*SIN((G104-$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$F$13=\"Ko\",\"Ko₁=\",IF(E44>0,\"K₁=\",\"Ka₁=\"))","v":"K₁="},{"$f":"IF('Unos podataka'!$F$13=\"Ko\",+M110,IF(E44>0,K132,H112))","v":0.59693740409312213},null,{"$f":"(1+H109)^2","v":1.5878290174644589},{"$f":"(1+I109)^2","v":1},{"$f":"(1+J109)^2","v":1.4011527288776078},"visine slojeva","Ko1=",{"$f":"1-SIN((F103*PI()/180))","v":0.69244539980509812},"Ko3=",null,{"$f":"IF(R25=0,-20,R110+0.07)","v":-20},{"$f":"IF(R25=0,0,R22)","v":0},{"$f":"IF(Q110=0,0,'C III-V'!Z31-0.035)","v":0},{"$f":"+S109-0.15","v":-3.15},{"$f":"+IF($R$22>0,1,0)","v":0},null,null,null,null,null,null,null,null,"Poz 7 +Poz 7' (ukupna u presjeku III-III)",{"$f":"+B322","v":{"$error":"#VALUE!"}},{"$f":"+AE109","v":{"$error":"#VALUE!"}}]
["sloj 2. .......................",{"$f":"IF('C III-V'!D85<0,0,'C III-V'!D85)","v":{"$error":"#VALUE!"}},{"$f":"+$B$111*COS((G105-$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"ABS(B111*SIN((G105-$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$F$13=\"Ko\",\"Ko₂=\",IF(E44>0,\"K₂=\",\"Ka₂=\"))","v":"K₂="},{"$f":"IF('Unos podataka'!$F$13=\"Ko\",+M111,IF(E44>0,L132,I112))","v":0.78849922516973658},null,"Ka1","Ka2","Ka3",{"$f":"+D17","v":2},"Ko2=",{"$f":"1-SIN(F104*PI()/180)","v":0.74842438848759574},{"$f":"1-SIN((F105*PI()/180))","v":0.72043403044116916},null,{"$f":"+P110-R23*COS(E39*PI()/180)","v":-20},{"$f":"+Q110-R23*SIN(E39*PI()/180)","v":0},{"$f":"IF(E56=\">100\",R110,R110+(R22-S109)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"IF(R115=0,-3,S112+0.15)","v":-3},{"$f":"+IF($S$22>0,1,0)","v":0},null,null,null,null,null,null,null,null," Poz 7 (duga armatura)",{"$f":"+IF(AD109=AD110,AD110,AD109)","v":{"$error":"#VALUE!"}},{"$f":"+AE110","v":{"$error":"#VALUE!"}},null,0]
["sloj 3. .......................",{"$f":"+'C III-V'!F85","v":{"$error":"#VALUE!"}},{"$f":"+B112*COS((G106)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"B112*SIN((G106)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$F$13=\"Ko\",\"Ko₃=\",IF(E44>0,\"K₃=\",\"Ka₃=\"))","v":"K₃="},{"$f":"IF('Unos podataka'!$F$13=\"Ko\",+N111,IF(E44>0,M132,J112))","v":0.71000444573298527},null,{"$f":"(H105/H106)/H110","v":0.58480897527521336},{"$f":"(I105/I106)/I110","v":0.95764677537194132},{"$f":"(J105/J106)/J110","v":0.69491292897772694},{"$f":"+E17","v":2.8},"prosječni računski Ko=",{"$f":"(M110*K111+M111*K112)/(K111+K112)","v":0.72509980986988842},null,null,{"$f":"+P111-F$73*COS($E$39*PI()/180)","v":-20},{"$f":"+Q111-F$73*SIN($E$39*PI()/180)","v":0},{"$f":"IF(E56=\">100\",R110,R111+(S109-S110)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"IF(R115=0,-3,S22+0.06)","v":-3},{"$f":"+IF($S$22>0,1,0)","v":0},{"$f":"+U113+1.5","v":-18.5},{"$f":"+V113+(U112-U113)*TAN($E$39*PI()/180)","v":0.40192378864668404},null,null,null,null,null,null," Poz 7' (kratka armatura)",{"$f":"+AD110-AD111","v":{"$error":"#VALUE!"}},{"$f":"+AE111","v":{"$error":"#VALUE!"}}]
["SEa=",{"$f":"SUM(B110:B112)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C110:C112)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D110:D112)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"Ka1=",{"$f":"+H112","v":0.58480897527521336},null,null,{"$f":"IF(S25=0,-20,P115+0.5)","v":-20},{"$f":"+Q115","v":0},{"$f":"IF(E56=\">100\",R115,R114-(S111-S112)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"+S22","v":0},null,{"$f":"+P115","v":-20},{"$f":"+Q115","v":0},null,null,null,null,null,null,{"$f":"ROUND(6/'Iskaz armature'!T4,1)","v":2.1}]
[null,{"$f":"+COS(($G$105-$H$51)*PI()/180)","v":0.9975640502598242},{"$f":"ABS(SIN(($G$105-$H$51)*PI()/180))","v":6.9756473744125302E-2},null,null,null,null,null,null,null,null,"Ka2=",{"$f":"+I112","v":0.95764677537194132},null,null,{"$f":"IF(S25=0,-20,P113-1)","v":-20},{"$f":"+Q113","v":0},{"$f":"IF(E56=\">100\",R115,R115-(S112-S22)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"IF(R115=0,-3,S22-0.09)","v":-3},{"$f":"+IF($S$22>0,1,0)","v":0},{"$f":"P117","v":-20},{"$f":"+V113-(U113-U114)*TAN($E$39*PI()/180)","v":0},null,null,null,null,null,null,{"$f":"(TRUNC(AC113))","v":2},"kom po m'"]
["SILE KOJE ULAZE U KONTROLE GRANIČNIH STANJA NOSIVOSTI ZIDA",null,null,null,null,null,null,"PARCIJALNI KOEFICIJENTI DJELOVANJA",null,null,null,"prosječni računski Ka=",{"$f":"+(M113*K111+M114*K112)/(K111+K112)","v":0.80229769199830459},null,null,{"$f":"IF(S25=0,-20,R115+0.07)","v":-20},{"$f":"IF(S25=0,0,S22)","v":0},{"$f":"IF(Q115=0,0,+'C III-V'!Z29-0.035)","v":0},{"$f":"+S114-0.15","v":-3.15},{"$f":"+IF($S$22>0,1,0)","v":0},null,null,null,null,null,null,null,null,{"$f":"+'Iskaz armature'!U1/'Iskaz armature'!U4/2","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+P115-S23*COS(E39*PI()/180)","v":-20},{"$f":"+Q115-S23*SIN(E39*PI()/180)","v":0},{"$f":"IF(E56=\">100\",R115,R115+(S22-S114)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"IF(R120=0,-3,S117+0.15)","v":-3},{"$f":"+IF($T$22>0,1,0)","v":0}]
["Horizontalne sile",null,"Krakovi do točke prevrtanja\"A\"","Momenti od horiz. sila na točku \"A\"",null,null,"PREVRTANJE","KLIZANJE","SLOM TEMELJNOG TLA",null,null,null,{"$f":"1-SIN((F105*PI()/180))","v":0.72043403044116916},null,null,{"$f":"+P116-G$73*COS($E$39*PI()/180)","v":-20},{"$f":"Q116-G73*SIN(E39*PI()/180)","v":0},{"$f":"IF(E56=\">100\",R115,R116+(S114-S115)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"IF(R120=0,-3,T22+0.06)","v":-3},{"$f":"+IF($T$22>0,1,0)","v":0},{"$f":"+U118+1.5","v":-18.5},{"$f":"+V118+(U117-U118)*TAN($E$39*PI()/180)","v":0.40192378864668404}]
[null,null,null,null,null,null,null,"KLIZANJE",null,"kh=amax*S/r=",{"$f":"+E44*E46/E45","v":0.1},{"$f":"-0.5*K118","v":-0.05},null,null,"sidro IV",{"$f":"IF(T25=0,-20,P120+0.5)","v":-20},{"$f":"+Q120","v":0},{"$f":"IF(E56=\">100\",R120,R119-(S116-S117)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"+T22","v":0},null,{"$f":"+P120","v":-20},{"$f":"+Q120","v":0}]
["(kN/m')",null,"(m)","(kNm/m')",null,null,"EQU problem","GEO problem","GEO problem","tgq=kh/(1±kv)=",{"$f":"K118/(1+L118)","v":0.10526315789473685},{"$f":"+ATAN(K119)*180/PI()","v":6.0090059574945256},null,null,null,{"$f":"IF(T25=0,-20,P118-1)","v":-20},{"$f":"+Q118","v":0},{"$f":"IF(E56=\">100\",R120,R120-(S117-T22)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"IF(R120=0,-3,T22-0.09)","v":-3},{"$f":"+IF($T$22>0,1,0)","v":0},{"$f":"+P122","v":-20},{"$f":"+V118-(U118-U119)*TAN($E$39*PI()/180)","v":0}]
["Eh1 ............................",{"$f":"+C110","v":{"$error":"#VALUE!"}},{"$f":"IF(B120<=0,0,+'C III-V'!B87-'C III-V'!C15)","v":{"$error":"#VALUE!"}},{"$f":"+B120*C120","v":{"$error":"#VALUE!"}},null,null,{"$f":"+H$31","v":1.1000000000000001},{"$f":"+J$31","v":1},{"$f":"+J$31","v":1},null,{"$f":"+'Sile i krakovi'!T76","v":0},"nagib gornje plohe  b   ","y=",{"$f":"90-C47","v":94},{"$f":"90-D47","v":90},{"$f":"IF(T25=0,-20,R120+0.07)","v":-20},{"$f":"IF(T25=0,0,T22)","v":0},{"$f":"IF(Q120=0,0,'C III-V'!Z27-0.035)","v":0},{"$f":"+S119-0.15","v":-3.15},{"$f":"+IF($T$22>0,1,0)","v":0}]
["Eh2 ............................",{"$f":"+C111","v":{"$error":"#VALUE!"}},{"$f":"IF(B121<=0,0,'C III-V'!D87-'C III-V'!C15)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,{"$f":"+H$31","v":1.1000000000000001},{"$f":"+J$31","v":1},{"$f":"+J$31","v":1},null,"j"," b","(y+j-q)",null,null,{"$f":"+P120-T23*COS(E39*PI()/180)","v":-20},{"$f":"+Q120-T23*SIN(E39*PI()/180)","v":0},{"$f":"IF(E56=\">100\",R120,R120+(T22-S119)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T96:T120)","v":8},{"$f":"SUM(T96:T120)","v":8}]
["Eh3 ............................",{"$f":"+C112","v":{"$error":"#VALUE!"}},{"$f":"IF(B122=0,0,F122-'C III-V'!C15)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,{"$f":"+'C III-V'!F87","v":{"$error":"#VALUE!"}},{"$f":"+H$31","v":1.1000000000000001},{"$f":"+J$31","v":1},{"$f":"+J$31","v":1},"sloj 1",{"$f":"+F103","v":17.911920978999142},{"$f":"IF(E24>0,0,H20)","v":0},{"$f":"$N$120+K122-$L$119","v":105.90291502150463},null,null,{"$f":"+P121-H$72*COS($E$39*PI()/180)","v":-20},{"$f":"+Q121-H$72*SIN($E$39*PI()/180)","v":0},{"$f":"IF(E56=\">100\",R120,R121+(S119-S120)/$F$56)","v":{"$error":"#VALUE!"}},{"$f":"+(Q124*COS($E$39*PI()/180))","v":48.296291314453413},"VI=",{"$f":"+Q124*SIN($E$39*PI()/180)","v":12.940952255126037}]
["Ehw ...........................",{"$f":"IF(J53=0,0,10*(E41*E41)/2)","v":1.7999999999999998},{"$f":"IF(B123=0,0,(J53/3-'C III-V'!C15))","v":-0.30000000000000004},{"$f":"IF(C123<0,0,+B123*C123)","v":0},null,null,{"$f":"+H$31","v":1.1000000000000001},{"$f":"+I$31","v":1.35},{"$f":"+I$31","v":1.35},"sloj 2",{"$f":"+F104","v":14.57076836070997},{"$f":"+D18","v":6},{"$f":"$N$120+K123-$L$119","v":102.56176240321544},null,null,null,"Ukupno komada:",{"$f":"SUM(T96:T120)","v":8},{"$f":"+(Q125*COS($E$39*PI()/180))","v":48.296291314453413},"VII=",{"$f":"+Q125*SIN($E$39*PI()/180)","v":12.940952255126037}]
["EPrometno ....................",{"$f":"'HT III-XX'!G40","v":{"$error":"#VALUE!"}},{"$f":"IF(B124<0.001,0,+'HT III-XX'!G41-(E52-E51))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,{"$f":"+H$33","v":1.5},{"$f":"+J$33","v":1.3},{"$f":"+J$33","v":1.3},"sloj 3",{"$f":"+F105","v":16.234302131351505},{"$f":"+E18","v":4},{"$f":"$O$120+K124-$L$119","v":100.22529617385699},null,null,"SI=",{"$f":"+D75","v":50},"HI=",{"$f":"+(Q126*COS($E$39*PI()/180))","v":0},"VIII=",{"$f":"+Q126*SIN($E$39*PI()/180)","v":0}]
["EPTočkasto ....................",{"$f":"'HT III-XX'!G80","v":{"$error":"#VALUE!"}},{"$f":"IF(B125<0.001,0,+'HT III-XX'!G81-(E52-E51))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,{"$f":"+H$31","v":1.1000000000000001},{"$f":"+J$31","v":1},{"$f":"+J$31","v":1},null,{"$f":"+SIN(M122*PI()/180)*SIN(M122*PI()/180)","v":0.9249195345095288},{"$f":"+SIN(M123*PI()/180)*SIN(M123*PI()/180)","v":0.95269727631316292},{"$f":"+SIN(M124*PI()/180)*SIN(M124*PI()/180)","v":0.96848691697817646},null,null,"SII=",{"$f":"+E75","v":50},"HII=",{"$f":"+(Q129*COS($E$39*PI()/180))","v":0},"VIV=",{"$f":"+Q129*SIN($E$39*PI()/180)","v":0}]
["EPLinijsko .....................",{"$f":"'HT III-XX'!G120","v":{"$error":"#VALUE!"}},{"$f":"IF(B126<0.001,0,+'HT III-XX'!G121-(E52-E51))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,{"$f":"+C126+($E$52-$E$51)","v":{"$error":"#VALUE!"}},{"$f":"+H$31","v":1.1000000000000001},{"$f":"+J$31","v":1},{"$f":"+J$31","v":1},null,{"$f":"+COS($L$119*PI()/180)*SIN($N$120*PI()/180)*SIN($N$120*PI()/180)*SIN(($N$120-$L$119)*PI()/180)","v":0.98905790448605813},{"$f":"+COS($L$119*PI()/180)*SIN($N$120*PI()/180)*SIN($N$120*PI()/180)*SIN(($N$120-$L$119)*PI()/180)","v":0.98905790448605813},{"$f":"+COS($L$119*PI()/180)*SIN($O$120*PI()/180)*SIN($O$120*PI()/180)*SIN(($O$120-$L$119)*PI()/180)","v":0.98904109589041089},null,null,"SIII=",{"$f":"+F75","v":""},"HIII=",{"$f":"+(Q130*COS($E$39*PI()/180))","v":0},"VV=",{"$f":"+Q130*SIN($E$39*PI()/180)","v":0}]
["EQTemelj ili vozilo.....................",{"$f":"+'Sile i krakovi'!T109","v":{"$error":"#VALUE!"}},{"$f":"IF(B127=0,0,+'Sile i krakovi'!T126-(E52-E51))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,{"$f":"IF(D31=\"VV=\",H33,H31)","v":1.1000000000000001},{"$f":"IF(D31=\"VV=\",J33,J31)","v":1},{"$f":"IF(D31=\"VV=\",J33,J31)","v":1}]
["Hsidro .........................",{"$f":"K39*COS(E39*PI()/180)","v":96.592582725499412},{"$f":"IF(B128<=0.00001,0,'Sile i krakovi'!E131)","v":3.4999999960000001},{"$f":"+B128*C128","v":338.07403915287762},null,null,{"$f":"+H32","v":0.9},{"$f":"+$J$32","v":1},{"$f":"+J32","v":1},{"$f":"2+$E$61-C148","v":{"$error":"#VALUE!"}}]
["Hvoda ispred zida...............",{"$f":"'Sile i krakovi'!$P$109","v":3.2},{"$f":"IF(B129=0,0,'Sile i krakovi'!E111)","v":-0.23333333333333328},{"$f":"+B129*C129","v":-0.74666666666666659},null,null,{"$f":"+H34","v":0},{"$f":"+$I$34","v":0},{"$f":"+I34","v":0},null,{"$f":"IF(K122-L122-L119<=0,0,1+SQRT((SIN(K122*PI()/180)*SIN((K122-L122-$L$119)*PI()/180)/SIN(($N$120-$L$119)*PI()/180)*SIN(($N$120+L122)*PI()/180))))","v":1.2516321801807924},{"$f":"IF(K123-L123-L119<=0,0,SQRT((SIN(K123*PI()/180)*SIN((K123-L123-$L$119)*PI()/180)/SIN(($N$120-$L$119)*PI()/180)*SIN(($N$120+L123)*PI()/180))))","v":0.10526385393210554},{"$f":"IF(K124-L124-L119<=0,0,SQRT((SIN(K124*PI()/180)*SIN((K124-L124-$L$119)*PI()/180)/SIN(($O$120-$L$119)*PI()/180)*SIN(($O$120+L124)*PI()/180))))","v":0.17438143293962521},{"$f":"+E52+H76","v":1.5001009999999999},{"$f":"2+E61+0.2","v":5.1000021999999996},"SIV=",{"$f":"+G75","v":""},"HIV=",{"$f":"+S122+S123+S124+S125+S126","v":96.592582628906825},"SV=",{"$f":"+U122+U123+U124+U125+U126","v":25.881904510252074}]
["HPotres ........................",{"$f":"+E43","v":{"$error":"#VALUE!"}},{"$f":"IF(B130=0,0,'C III-V'!Y113-'C III-V'!C15)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,{"$f":"+IF($D$83=\"\",'C III-V'!$AC$135,'C III-V'!$AK$113)","v":{"$error":"#VALUE!"}},1,1,1,null,{"$f":"+K129*K129","v":1.5665831144641236},{"$f":"+(1+L129)*(1+L129)","v":1.2216081868088509},{"$f":"+(1+M129)*(1+M129)","v":1.3791717500333274},{"$f":"+N129-TAN(H22*PI()/180)*2","v":1.5001009999999999},{"$f":"+O129+2","v":7.1000021999999996},"SV=",{"$f":"+H74","v":0},"HV=",{"$f":"+S122*('C III-V'!B15-P100)","v":{"$error":"#VALUE!"}},"MMVI=",{"$f":"+U122*(Q100-(E52-E51))","v":58.234285148067165}]
[null,null,null,null,null,null,null,null,null,null,"K1","K2","K3",null,null,"Rsidra=",{"$f":"+Q124+Q125+Q126+Q129+Q130","v":100},"SH=",{"$f":"+S123*('C III-V'!B15-P105)","v":{"$error":"#VALUE!"}},"MVII=",{"$f":"+U123*(Q105-(E52-E51))","v":32.352380637815095}]
["Vertikalne sile",null,"Krakovi do točke prevrtanja\"A\"","Momenti od vert. sila na točku A",null,null,"PREVRTANJE","KLIZANJE","SLOM TEMELJNOG TLA",null,{"$f":"IF(L122<=K122-L119,K125/K126/K130,K125/K126)","v":0.59693740409312213},{"$f":"+IF(L123<=K123-L119,L125/L126/L130,L125/L126)","v":0.78849922516973658},{"$f":"IF(L124<=K124-L119,M125/M126/M130,M125/M126)","v":0.71000444573298527},null,null,null,null,"MHI=",{"$f":"+S124*('C III-V'!B15-P110)","v":0},"MVIII=",{"$f":"+U124*(Q110-(E52-E51))","v":0}]
[null,null,null,null,null,null,null,"KLIZANJE",null,null,null,null,null,null,null,null,null,"MHII=",{"$f":"+S125*('C III-V'!B15-P115)","v":0},"MVIV=",{"$f":"+U125*(Q115-(E52-E51))","v":0}]
["(kN/m')",null,"(m)","(kNm/m')",null,null,"EQU problem","GEO problem","GEO problem",null,null,null,null,null,null,null,null,"MHIII=",{"$f":"+S126*('C III-V'!B15-P120)","v":0},"MVV=",{"$f":"+U126*(Q120-(E52-E51))","v":0}]
["Gtem ..........................",{"$f":"+Kontrafore!AO36","v":{"$error":"#VALUE!"}},{"$f":"2+E59+E55+E58-Kontrafore!AO33","v":{"$error":"#VALUE!"}},{"$f":"B135*C135","v":{"$error":"#VALUE!"}},null,null,{"$f":"+H$32","v":0.9},{"$f":"+$I$32","v":1},{"$f":"+Dopušteno!X10","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"MHIV=",{"$f":"+S130+S131+S132+S133+S134","v":{"$error":"#VALUE!"}},"SVV=",{"$f":"+U130+U131+U132+U133+U134","v":90.586665785882261}]
["Gzid+konz .....................",{"$f":"+'C III-V'!D61","v":{"$error":"#VALUE!"}},{"$f":"2+E60+E61-'C III-V'!D59","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,0.9,1,{"$f":"+Dopušteno!X11","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"MHV=",{"$f":"IF(S129=0,0,+S135/S129)","v":{"$error":"#VALUE!"}},"krak x=",{"$f":"IF(U129=0,0,U135/U129)","v":3.5}]
["Grebra kontrafora ............",{"$f":"IF(A82=\"\",0,Kontrafore!AC17)","v":{"$error":"#VALUE!"}},{"$f":"IF(B137=0,0,'C III-V'!$U$2-Kontrafore!AC13)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,0.9,1,{"$f":"+Dopušteno!X12","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"SMH="]
["Gnasip na konzoli ............",{"$f":"'C III-V'!J61","v":{"$error":"#VALUE!"}},{"$f":"IF(B138=0,0,2+E61-'C III-V'!J59)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,0.9,1,{"$f":"+Dopušteno!X13","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"krak y="]
["Gnasipa iza zida .............",{"$f":"+Kontrafore!N32","v":{"$error":"#VALUE!"}},{"$f":"IF(B139=0,0,+'C III-V'!$U$2-Kontrafore!N33)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,0.9,1,{"$f":"+Dopušteno!X14","v":{"$error":"#VALUE!"}},{"$f":"2+$E$61-C138","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Gnasipa ispred zida .............",{"$f":"+Kontrafore!W11","v":{"$error":"#VALUE!"}},{"$f":"IF(B140=0,0,+Kontrafore!W12)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,0.9,1,{"$f":"+Dopušteno!X15","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["PPrometno ....................",{"$f":"+'Rasprostiranje vertikalnog opt'!R28","v":{"$error":"#VALUE!"}},{"$f":"IF(B141=0,0,+'Rasprostiranje vertikalnog opt'!S29)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,{"$f":"+H34","v":0},{"$f":"+$J$34","v":0},{"$f":"+Dopušteno!X16","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["PTočkasto .....................",{"$f":"IF('Unos podataka'!$O$48=\"\",+'Rasprostiranje vertikalnog opt'!R46,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B142<=0.00001,0,+'Rasprostiranje vertikalnog opt'!S47)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,{"$f":"+H32","v":0.9},{"$f":"+$J$32","v":1},{"$f":"+Dopušteno!X17","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["PLinijsko ......................",{"$f":"IF('Unos podataka'!$O$48=\"\",IF(E35<0,E34,+'Rasprostiranje vertikalnog opt'!R37),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B143<=0.00001,0,IF(E35<0,'Unos podataka'!B103+E35,+'Rasprostiranje vertikalnog opt'!S38))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,{"$f":"+H32","v":0.9},{"$f":"+$J$32","v":1},{"$f":"+Dopušteno!X18","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["QTemelj ili vozilo.....................",{"$f":"IF(E28=0,0,+'Rasprostiranje vertikalnog opt'!R19)","v":{"$error":"#VALUE!"}},{"$f":"IF(B144=0,0,+'Rasprostiranje vertikalnog opt'!S20)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,{"$f":"IF(D31=\"VV=\",H34,H32)","v":0.9},{"$f":"IF(D31=\"VV=\",$J$34,$J$32)","v":1},{"$f":"+Dopušteno!X19","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["VSidro .........................",{"$f":"+K39*SIN(E39*PI()/180)","v":25.881904536133977},{"$f":"IF(B145=0,0,IF(D71=\"\",0,+'Sile i krakovi'!J132))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,{"$f":"+H32","v":0.9},{"$f":"+$J$32","v":1},{"$f":"+Dopušteno!X20","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["Ev1 ...........................",{"$f":"D110","v":{"$error":"#VALUE!"}},{"$f":"IF(B146<0.0001,0,2+'Unos podataka'!G49+E61-'C III-V'!A93)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,{"$f":"+H32","v":0.9},{"$f":"+$J$32","v":1},{"$f":"+Dopušteno!X21","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["Ev2  ..........................",{"$f":"D111","v":{"$error":"#VALUE!"}},{"$f":"IF(B147<0.0001,0,2+'Unos podataka'!G49+E61-'C III-V'!C93)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,{"$f":"+H32","v":0.9},{"$f":"+$J$32","v":1},{"$f":"+Dopušteno!X22","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["Ev3  ..........................",{"$f":"D112","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!AB1=\"\",E61,IF(B148<=0.0001,0,2+E61+'Unos podataka'!AB3-'C III-V'!E93))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,{"$f":"+H32","v":0.9},{"$f":"+$J$32","v":1},{"$f":"+IF('Dopušteno Vs+'!$H$84>'Dopušteno Vs-'!$H$84,$J$32,$J$31)","v":1},{"$error":"#VALUE!"}]
["Vpotres........................",0,{"$f":"IF(B149>=0,0,+'C III-V'!Y139)","v":0},{"$f":"IF(B149<0,-B149*C149*I149,0)","v":0},null,null,1,1,1]
["Uzgon ….......................",{"$f":"-'Unos podataka'!$R$142*10","v":{"$error":"#VALUE!"}},{"$f":"IF(B150=0,0,+'Unos podataka'!R139-'Unos podataka'!R143)","v":{"$error":"#VALUE!"}},{"$f":"+B150*C150","v":{"$error":"#VALUE!"}},null,null,{"$f":"+H33","v":1.5},{"$f":"+I33","v":1.5},0]
[]
["SUMA FAKTORIZIRANIH SILA I MOMENATA ZA KONTROLE GRANIČNIH STANJA NOSIVOSTI ZIDA"]
[]
["SUMA FAKTORIZIRANIH MOMENATA ZA KONTROLU SLOMA PREVRTANJEM"]
["MEd,dst =",{"$f":"+D120*G120+D121*G121+D122*G122+D123*G123+D124*G124+D125*G125+D126*G126+D127*G127+D130*G130-D149*G149-D150*G150","v":{"$error":"#VALUE!"}},"kNm/m'"]
["MEd,stb=",{"$f":"-(+D135*G135+D136*G136+D137*G137+D138*G138+D139*G139+D140*G140+D141*G141+D142*G142+D143*G143+D144*G144+D145*G145+D146*G146+D147*G147+D148*G148+D128*G128+D129*G129)","v":{"$error":"#VALUE!"}},"kNm/m'"]
[]
["SUMA FAKTORIZIRANIH SILA ZA KONTROLU SLOMA KLIZANJEM TEMELJA"]
["Σ(Hi  x γi ) =",{"$f":"+B120*H120+B121*H121+B122*H122+B123*H123+B124*H124+B125*H125+B126*H126+B127*H127+B130*H130-B128*H128-B129*H129","v":{"$error":"#VALUE!"}},"kN/m'","Rezultanta sila ..................................",null,null,"      R  =",{"$f":"SQRT(B159^2+B160^2)","v":{"$error":"#VALUE!"}},"kN/m'"]
["Σ(Vi  x γi ) =",{"$f":"+B135*H135+B136*H136+B137*H137+B138*H138+B139*H139+B140*H140+B141*H141+B142*H142+B143*H143+B144*H144+B145*H145+B146*H146+B147*H147+B148*H148+B149*H149+B150*H150","v":{"$error":"#VALUE!"}},"kN/m'","sila okomita na temelj .......................",null,null,{"$f":"+IF(H162=0,\"Rv=\",\"RN=\")","v":"RN="},{"$f":"H159*COS((H163-H162)*PI()/180)","v":{"$error":"#VALUE!"}},"kN/m'"]
[null,null,null,"sila uzduž temelja .............................",null,null,{"$f":"IF(H162=0,\"     RH=\",\"     RT=\")","v":"     RT="},{"$f":"+H159*SIN((H163-H162)*PI()/180)","v":{"$error":"#VALUE!"}},"kN/m'"]
[null,null,null,"nagib temelja ....................................",null,null,"b =",{"$f":"IF('Unos podataka'!AB1=\"\",ATAN('C III-V'!C15/(E61))*180/PI(),ATAN('C III-V'!C15/(E61+'Unos podataka'!AB3))*180/PI())","v":7.3057554566405489},"°"]
[null,null,null,"otklon rezultante od vertikale.......",null,null,"a =",{"$f":"ATAN(B159/B160)*180/PI()","v":{"$error":"#VALUE!"}},"°"]
[]
["SUMA FAKTORIZIRANIH SILA I MOMENATA ZA KONTROLU SLOMA GUBITKOM NOSIVOSTI TLA ISPOD TEMELJA"]
[]
["Σ(Hi  x γi ) =",{"$f":"+B120*I120+B121*I121+B122*I122+B123*I123+B124*I124+B125*I125+B126*I126+B127*I127+B130*I130-B128*I128-B129*I129","v":{"$error":"#VALUE!"}},"kN/m'","MEd,H,A =",{"$f":"+D120*I120+D121*I121+D122*I122+D123*I123+D124*I124+D125*I125+D126*I126+D127*I127-D128*I128-D129*I129+D130*I130","v":{"$error":"#VALUE!"}},null,"      yA = ",{"$f":"E167/B167","v":{"$error":"#VALUE!"}}]
["Σ(Vi  x γi ) =",{"$f":"+Dopušteno!V26","v":{"$error":"#VALUE!"}},"kN/m'","MEd,V,A=",{"$f":"+Dopušteno!V27","v":{"$error":"#VALUE!"}},null,"      xA = ",{"$f":"E168/B168","v":{"$error":"#VALUE!"}}]
["Rezultanta sila      R =",{"$f":"+SQRT(B167^2+B168^2)","v":{"$error":"#VALUE!"}},"kN/m'"]
["Otklon rezultante od vertikale ...............",null,"a =",{"$f":"ATAN(B167/B168)*180/PI()","v":{"$error":"#VALUE!"}},"°"]
["Moment oko osi temelja ........................",null,"     Ms =",{"$f":"+Dopušteno!V28","v":{"$error":"#VALUE!"}},"kNm/m'"]
[null,null,null,null,null,null,null,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"crtanje zida"]
[null,null,null,"KONTROLE GRANIČNIH STANJA NOSIVOSTI ZIDA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B2","v":2},{"$f":"+'C III-V'!C2","v":0.12820515121628623}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B3","v":2},{"$f":"+'C III-V'!C3","v":1.2}]
[null,"KONTROLA SLOMA PREVRTANJEM",null,null,"KONTROLA SLOMA KLIZANJEM TEMELJA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B4","v":3.4000010999999999},{"$f":"+'C III-V'!C4","v":1.2}]
["MEd,stb/gR=",{"$f":"+(D135*G135+D136*G136+D137*G137+D138*G138+D139*G139+D140*G140+D141*G141+D142*G142+D143*G143+D144*G144+D145*G145+D146*G146+D147*G147+D148*G148+D128*G128+D129*G129)/M36","v":{"$error":"#VALUE!"}},"kNm/m'",null,"Rd=RN","* tgd4/gRh=     ",{"$f":"+H160*I176/M37","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"(TAN(F106*PI()/180))","v":0.25993575698632504},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B10","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C10","v":"A"}]
["MEd,dst =",{"$f":"+D120*G120+D121*G121+D122*G122+D123*G123+D124*G124+D125*G125+D126*G126+D127*G127+D130*G130+D149*G149","v":{"$error":"#VALUE!"}},"kNm/m'",null,{"$f":"+H160*I176/M37","v":{"$error":"#VALUE!"}},"Hd=RT=",{"$f":"+H161","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(E177/I178<0,\">10\",E177/I178)","v":{"$error":"#VALUE!"}},{"$f":"+E177/I178","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B11","v":4.2000010999999997},{"$f":"+'C III-V'!C11","v":1.2}]
["MEd,dst",{"$f":"+IF(B176>B177,\"≤\",\">\")","v":{"$error":"#VALUE!"}},"MEd,stb",null,null,"Hd",{"$f":"+IF(G176>G177,\"≤\",\">\")","v":{"$error":"#VALUE!"}},"Rd",{"$f":"H161","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C5","v":3.14}]
["Iskorištenost:",{"$f":"+B177/B176","v":{"$error":"#VALUE!"}},{"$f":"+IF(A177<A176,\"(Zadovoljava)       \",\"(NE Zadovoljava)\")","v":"(Zadovoljava)       "},null,null,"Iskorištenost:",{"$f":"+G177/G176","v":{"$error":"#VALUE!"}},{"$f":"+IF(E177>I178,\"(Zadovoljava)\",\"(Ne zadovoljava)\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B6","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C6","v":3.14}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B14","v":4.9000021999999994},{"$f":"+'C III-V'!C14","v":1.2}]
[null,null,null,"KONTROLA SLOMA GUBITKOM NOSIVOSTI TLA ISPOD TEMELJA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B15","v":4.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5}]
[null,null,"             Kontaktna naprezanje: temelj-tlo",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B16","v":2},{"$f":"+'C III-V'!C16","v":0.12820515121628623}]
[null,{"$f":"+IF(A82=\"\",\"         Temelj\", \"          Temelj s kontraforama\" )","v":"          Temelj s kontraforama"},null,null,null,"Rotacija temelja i otklon vrha zida",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B25","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C25","v":{"$error":"#VALUE!"}}]
[]
[null,"   B =",{"$f":"+MT!G13","v":3.1500021999999994},"m",null,"a ≈",{"$f":"IF(Slijeganje!M76<=0,0,Slijeganje!M76)","v":{"$error":"#VALUE!"}},"°",{"$f":"IF(E51=E52,\"\",+E61/COS(H162*PI()/180))","v":2.9237380594839224},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ARM I-I"]
[null,"       W =",{"$f":"+MT!G14","v":1.653752310000806},"m3",null,"D ≈",{"$f":"IF(G185>0,+Slijeganje!AB31,0)","v":{"$error":"#VALUE!"}},"cm",{"$f":"IF(E51=E52,\"\",+(I185^2)/6)","v":1.4247073734124687},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AS188","v":1.95},{"$f":"+AT194","v":7.8205151216286226E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(AS186+AS188)/2","v":1.95},{"$f":"+(AT186+AT188)/2","v":0.66410257560814312}]
[null,null,"visine temelja u presjeku",null,null,"naprezanja temelj-tlo",null,null,null,"Mt",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AS174-A260","v":1.95},{"$f":"+AT174+Q52","v":1.25}]
[null,null,null,null,null,null,null,{"$f":"+H190","v":4.9000010999999999},0,{"$f":"((F192-F191)*E55*E5*E55/3)/(E55*F191+E55*(F192-F191)*0.5*2/3)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AS192","v":2.0499999999999998},{"$f":"+AT192","v":0.17820515121628622}]
[null," hA=",{"$f":"E51","v":0.7},"m","sA  =",{"$f":"$B$168/$C$185+$D$171/$C$186","v":{"$error":"#VALUE!"}},"kN/m2",{"$f":"+Kontrafore!P29","v":4.9000010999999999},{"$f":"-F190/100","v":{"$error":"#VALUE!"}},{"$f":"+E62*C192*(F46+0.000001)*(F46+0.000001)/2","v":21.861604843542246}]
[null,"   dl-l=",{"$f":"+E52-(F46+Kontrafore!E3+E55)*(E52-E51)/(E61+Kontrafore!E3)","v":0.78974368014459062},"m"," s l-l=",{"$f":"+Kontrafore!C50","v":{"$error":"#VALUE!"}},"kN/m2",{"$f":"+Kontrafore!P28","v":4.2000000999999996},{"$error":"#VALUE!"},{"$f":"+E62*(C193-C192)*(F46+0.000001)*(F46+0.000001)/3","v":2.9486333315725139},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ARM II-II"]
[null," dll-ll=",{"$f":"E52-(F46+Kontrafore!E3)*(E52-E51)/(E61+Kontrafore!E3)","v":0.89230772485205256},"m"," sll-ll=",{"$f":"+Kontrafore!C49","v":{"$error":"#VALUE!"}},"kN/m2",{"$f":"+Kontrafore!P27","v":3.4000000999999997},{"$error":"#VALUE!"},{"$f":"SUM(J190:J191)","v":24.810238175114758},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AS173+A287","v":2.0499999999999998},{"$f":"+AT173+A287","v":0.17820515121628622}]
[null," hB=",{"$f":"E52-D83*SIN(H162*PI()/180)","v":1.0728357545883234},"m","sB  =",{"$f":"IF('Unos podataka'!O48=\"\",+Kontrafore!C48,$B$168/$C$185-$D$171/$C$186)","v":{"$error":"#VALUE!"}},"kN/m2",{"$f":"+Kontrafore!P26","v":2},{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(AS192+AS194)/2","v":2.0499999999999998},{"$f":"+(AT192+AT194)/2","v":0.12820515121628623}]
[null,{"$f":"+IF(D83=\"\",\"\",\"hҝ =\")","v":"hҝ ="},{"$f":"IF(D83=\"\",\"\",+E52-'Unos podataka'!J46)","v":1.1038461045365295},{"$f":"+IF(D83=\"\",\"\",\"m\")","v":"m"},{"$f":"+IF(A83=\"\",\"\",\"sk  =\")","v":"sk  ="},{"$f":"IF(A83=\"\",\"\",$B$168/$C$185-$D$171/$C$186)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Unos podataka'!AB1=\"\",\"\",\"kN/m²\")","v":"kN/m²"},{"$f":"2+E61-C185+E60","v":1.75},{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AS192","v":2.0499999999999998},{"$f":"+AT182-A287","v":7.8205151216286226E-2}]
[null,{"$f":"+IF(D83=\"\",\"\",\"h₀ =\")","v":"h₀ ="},{"$f":"+IF(D83=\"\",\"\",E52)","v":1.2},{"$f":"+IF(D83=\"\",\"\",\"m\")","v":"m"},{"$f":"+IF(A84=\"\",\"\",\"so  =\")","v":"so  ="},{"$f":"IF(A83=\"\",\"\",+Kontrafore!C46)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Unos podataka'!AB1=\"\",\"\",\"kN/m²\")","v":"kN/m²"},{"$f":"2-Kontrafore!E3-E60","v":1},{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AS175-A287","v":3.3500011000000001},{"$f":"+AT194","v":7.8205151216286226E-2}]
["     PRORAČUN PROJEKTNE OTPORNOSTI  TLA    ",null,null,null,null,null,null,{"$f":"+H195","v":1},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ankeri"]
[" ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B548+2","v":{"$error":"#VALUE!"}},{"$f":"+C548","v":{"$error":"#VALUE!"}}]
[" Proračun projektne otpornosti tla provodi se prema EC7, prema izrazu:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B550+2","v":{"$error":"#VALUE!"}},{"$f":"+C550","v":1.6923077248520526}]
[null,"  qa=R/A'= c' *Nc*bc*sc*ic+q' *Nq*bq*sq*iq+0,5*g' *B' *Ng*bg*sg*ig",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B547+2","v":{"$error":"#VALUE!"}},{"$f":"+C547","v":{"$error":"#VALUE!"}}]
[]
["gdje je:",null," "]
[" g ..............................."," prostorna efektivna težina"]
[" B' ............................"," širina temelja (efektivna)"]
[" Nc, Nq, Ng .................."," faktori nosivosti",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESJEK I-I"]
[" ic, iq, ig  ....................."," faktori nagiba opterećenja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W2","v":{"$error":"#VALUE!"}},null,{"$f":"+BQ601","v":0}]
[" sc,sq, sg ....................."," faktori oblika temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W3","v":{"$error":"#VALUE!"}},null,0,{"$f":"+BR577","v":{"$error":"#VALUE!"}},{"$f":"+BS575","v":0}]
[" bc, bq, bg  .................."," faktori nagiba dna temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESJEK II-II",null,0,{"$error":"#VALUE!"},{"$f":"+BS576","v":0}]
[" cR,jR  .........................","faktorizirani parametri čvrstoće tla",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$error":"#VALUE!"},{"$f":"+BS577","v":0}]
[" q .............................."," opterećenje tla u razini temeljenja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W5","v":4.8500021999999996},{"$f":"+'C III-V'!X2","v":-0.5},0,{"$error":"#VALUE!"},{"$f":"+BS578","v":0}]
[" A' .............................."," reducirana površina temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W6","v":4.8500021999999996},{"$f":"+'C III-V'!X3","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},"kN/m2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,69.600052799999986,"m3"]
[null,"Parametri čvrstoće tla:",null,null,"           Dimenzije temelja:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESJEK III-III",null,0,16.820025520009676,"m3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W8","v":4.4000021999999994},{"$f":"+'C III-V'!X5","v":-0.5}]
["      j =",{"$f":"+G14","v":18},"°",null,"    B =",{"$f":"+G240","v":3.1500021999999994},"m      (širina temelja)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W9","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X6","v":{"$error":"#VALUE!"}}]
["       c =",{"$f":"+G15","v":25},"kPa",null,"     L =",{"$f":"+E49","v":12},"m      (duljina temelja)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ARM III-III ZID",null,{"$f":"+(AT188-AT189)/(AS188-AS189)","v":-10.717948487837152},{"$f":"+TAN(AP251)*180/PI()","v":0}]
["ϒ =",{"$f":"+G16","v":20},"kN/m³",null,"     Df=",{"$f":"+E52+H76","v":1.5001009999999999},"m      (dubina temeljenja)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AT179+O303","v":{"$error":"#VALUE!"}}]
[{"$f":"IF(H17=G16,\"\",+G17)","v":"γ'="},{"$f":"IF(H17=G16,\"\",H17)","v":10},{"$f":"IF(B217=\"\",\"\",+C216)","v":"kN/m³"},null,"a =",{"$f":"+H162","v":7.3057554566405489},"°       (kut nagiba temelja) ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(AQ216+AQ218)/2","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X8","v":{"$error":"#VALUE!"}}]
[null," ",null," "," "," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AS180+O303","v":4.9000021999999994},{"$f":"+'C III-V'!X9","v":{"$error":"#VALUE!"}}]
["            Parcijalni faktori svojstava tla:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mreža R131"]
[null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AS176-O303","v":{"$error":"#VALUE!"}},{"$f":"+AU179","v":3.14}]
["gj=",{"$f":"+M27","v":1.25},"gc=",{"$f":"+M28","v":1.25},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AS177-O303","v":4.2000010999999997},{"$f":"+(AR220+AR222)/2","v":3.14}]
["            Faktorizirani parametri čvrstoće tla:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AT178-O303","v":3.14}]
[null," ",null,null," "," "," "," "]
[null,"   tgjR=  tgj/gj=",{"$f":"TAN(G14*PI()/180)/B221","v":0.25993575698632504},"o --> j' =",{"$f":"+ATAN(C224)*180/PI()","v":14.57076836070997},"° --> Nq= ",{"$f":"+Dopušteno!H54","v":3.7840646174850825},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AT176","v":"A"}]
[null,"cR= c/gc=",{"$f":"+G15/D221","v":20},"kPa"," ","    Nc=",{"$f":"+Dopušteno!H55","v":10.710596970300873},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AT177-O303","v":1.2}]
[null,null,null,null,null,"Ng=",{"$f":"+Dopušteno!H56","v":1.4473558577295844}]
["            Faktori :"]
[]
[null,"sq=1+(B'/L')*sinj'=",{"$f":"+Dopušteno!D59","v":{"$error":"#VALUE!"}},"    iq=",{"$f":"+Dopušteno!F59","v":{"$error":"#VALUE!"}},"    bq=",{"$f":"+Dopušteno!H59","v":0.93480999420900812}]
[null,"sg= 1-0.30*B'/L' =",{"$f":"+Dopušteno!D60","v":{"$error":"#VALUE!"}},"    ig=",{"$f":"+Dopušteno!F60","v":{"$error":"#VALUE!"}},"    bg=",{"$f":"+Dopušteno!H60","v":0.93480999420900812}]
[null,"sc=(sq*Nq-1)/(Nq-1)=",{"$f":"+Dopušteno!D61","v":{"$error":"#VALUE!"}},"    ic=",{"$f":"+Dopušteno!F61","v":{"$error":"#VALUE!"}},"    bc=",{"$f":"+Dopušteno!H61","v":0.91139460798908856}]
[null,"q'=g*Df =",{"$f":"IF(E42>=0,IF(E42-(E52-E51)>(E51+E65),E51*(F16-10)+E65*(E66-10),IF(E42-(E52-E51)>E51,(E65+E51-(E42-(E52-E51)))*E66+(E42-(E52-E51)-E51)*(E66-10)+E51*(F16-10),E65*E66+(E51-(E42-(E52-E51)))*F16+(E42-(E52-E51))*(F16-10))),F16*E51+E66*E65)","v":17.000019999999999},"kPa"]
[]
["            Projektna otpornost tla:"]
[]
[null,"   qa =",{"$f":"+Dopušteno!D68","v":{"$error":"#VALUE!"}},"kPa"]
[]
[null,"Opterećenje temeljnog tla:",null,null,null,"          Dimenzije temelja:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,15,20,25,30,35,40]
["       Vd =",{"$f":"+Dopušteno!C76","v":{"$error":"#VALUE!"}},"kN     Vertikalna sila",null,null,"    B =",{"$f":"+Dopušteno!G43","v":3.1500021999999994},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TERZAGHI",null,null,0.17453333333333335,0.26180000000000003,0.34906666666666669,0.4363333333333333,0.52360000000000007,0.61086666666666667,0.69813333333333338,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["      Hx=",{"$f":"+Dopušteno!C77","v":0},"kN     komponenta u smjeru x",null,null,"       L =",{"$f":"+Dopušteno!G44","v":12},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   fi=",0,5,14.7,18.600000000000001,25,35,52,82,141,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["      Hy=",{"$f":"+Dopušteno!C78","v":{"$error":"#VALUE!"}},"kN     komponenta u smjeru y",null,null,"      Df=",{"$f":"+Dopušteno!G45","v":1.5000009999999999},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"firad=",0,8.7266666666666673E-2,1.4918841531648999,1.8152354940517035,2.2122076426731692,2.7098430302810956,3.3504355509523527,4.2031178827643583,5.3871829422020223]
["      Mx=",{"$f":"+Dopušteno!C79","v":{"$error":"#VALUE!"}},"kNm  moment oko osi x",null,null,"     ex=",{"$f":"+Dopušteno!P19","v":{"$error":"#VALUE!"}},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kpgam=",10.8,12.2]
["      My=",{"$f":"+Dopušteno!C80","v":0},"kNm  moment oko osi y",null,null,"     ey=",{"$f":"-Dopušteno!P20","v":{"$error":"#VALUE!"}},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"    a=",1,1.2242229849419868]
[]
["            Reducirana površina temelja:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["B'=B-2*ey =",{"$f":"+Dopušteno!D84","v":{"$error":"#VALUE!"}},"m","      USPOREDBA OPTEREĆENJA I OTPORNOSTI TEMELJNOG TLA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"AS251+BF299/AS252-BF298/AS254","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["        L'= L-2*ex =",{"$f":"+Dopušteno!D85","v":{"$error":"#VALUE!"}},"m  ","    Vd =",{"$f":"+Dopušteno!I86","v":{"$error":"#VALUE!"}},{"$f":"+IF(E248>H248,\"kN     >  \",\"kN     ≤  \")","v":{"$error":"#VALUE!"}},"Rd = R / gRv=",{"$f":"+Dopušteno!G86","v":{"$error":"#VALUE!"}},"kN",{"$f":"+I249/I250/M38","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AS251+BF299/AS252+BF298/AS254","v":{"$error":"#VALUE!"}}]
["        A' = L' *B' =",{"$f":"+Dopušteno!D86","v":{"$error":"#VALUE!"}},"m2    ",null,"Iskorištenost:  ",{"$f":"+E248/H248","v":{"$error":"#VALUE!"}},{"$f":"+IF(F249<=100%,\"(Zadovoljava)\",\"(Ne zadovoljava)\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF('Unos podataka'!L11=2,C236*B249/M38,IF('Unos podataka'!L11='Unos podataka'!S9,C236*B249/M38,C236*B249/M38))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      p1=",{"$f":"AS251-BF299/AS252-BF298/AS254","v":{"$error":"#VALUE!"}}]
["           Otpornost temeljnog tla",null,null,null,null,null,null,null,{"$f":"+B240","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      p2=",{"$f":"AS251-BF299/AS252+BF298/AS254","v":{"$error":"#VALUE!"}}]
["R = A' * qa =",{"$f":"+C236*B249","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      p3=",{"$f":"BD297/(BB298*BB297)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      p4=",{"$f":"BB298*BB298*BB297/6","v":75.600052799999986}]
["    DIMENZIONIRANJE   -  EC2",null,null,null,{"$f":"+S48","v":1},{"$f":"+IF('Unos podataka'!O48=\"\",\"\",\"DIMENZIONIRANJE ZA MASIVNI ZID SE NE PRINTA\")","v":""},null,{"$f":"+B241","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     V/F=",{"$f":"BB298*BB297*BB297/6","v":19.845027720009671},null,null,null,null,null,null,null,null,null,45,50]
["                    PRESJEK I-I:","  KROZ TEMELJ",null,null,null,{"$f":"+IF('Unos podataka'!O48=\"\",\"Glavna armatura na dnu temelja - ispred zida. Poz.1\",\"Armatura nije potrebna\")","v":"Glavna armatura na dnu temelja - ispred zida. Poz.1"}]
["MG  =",{"$f":"(N29-B257)","v":{"$error":"#VALUE!"}},"kNm/m'   ","NG =",{"$f":"-U69-E257","v":{"$error":"#VALUE!"}},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      W1=",null,null,null,null,null,null,null,null,null,null,0.78539999999999988,0.87266666666666659]
["MQ  =",{"$f":"0","v":0},"kNm/m'   ","NQ =",{"$f":"+B124","v":{"$error":"#VALUE!"}},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      W2=",null,null,null,null,null,null,null,null,null,null,298,800]
["MEd=",{"$f":"IF(E44=0,B256*$J$44+B257*$J$45,B256*1+B257*1)","v":{"$error":"#VALUE!"}},"kNm/m'   "," NEd=",{"$f":"IF(E44=0,E256*$J$44+E257*$J$45,E256*1+E257*1)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"+IF($I$53<=45,0.296,0.252)","v":0.29599999999999999},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      Naponi u krajnjim",null,null,null,null,null,null,null,null,null,null,7.1228449099070072,9.8530310416333471]
["     MEds=",{"$f":"IF(B258>0,B258-E258*(B264-B262/2)/100,B258-E258*(B264-B262/2)/100)","v":{"$error":"#VALUE!"}},{"$f":"+IF(E259<B260,\"kNm/m' >\",\"kNm/m'   <\")","v":{"$error":"#VALUE!"}},"      MRd,lim=",{"$f":"G258*G262*B261*B264*B264/100","v":2294.6788536361296},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      to~kama temelja"]
[{"$f":"+Q52","v":0.05},{"$f":"+ABS(B259)","v":{"$error":"#VALUE!"}}," ",null,null,null,null,null,221,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(AV242*AV242)/(2*(COS(0.785+AV240/2))^2)","v":2.6908744422194575},4.4411099217096952,7.4292672658983747,12.702327289822522,22.419953865567066,41.365578867864834,81.106783844524017,{"$f":"(BC258*BC258)/(2*(COS(0.785+BC256/2))^2)","v":172.88810760506249},{"$f":"(BD258*BD258)/(2*(COS(0.785+BD256/2))^2)","v":414.05608235723651}]
["   b =",100,"cm ",null,{"$f":"+B260*100/(B261*B264*B264*G262)","v":{"$error":"#VALUE!"}},"fyd =",{"$f":"500/'Unos podataka'!L25/10","v":43.478260869565219},"kN/cm2","es1,lim(%o)=",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BC533*AP283<1,\"temelj klizi\",BC533*AP283)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"(AV260-1)/(TAN(AV240))","v":9.5894025972747148},12.842365613816176,17.664221773540596,25.095655006623552,37.100343484654204,57.647845734836132,95.467230921551575,{"$f":"(BC260-1)/(TAN(BC256))","v":171.88747622594806},{"$f":"(BD260-1)/(TAN(BD256))","v":346.59376996935327}]
["  hI =",{"$f":"+C191*100","v":78.97436801445906},"cm ",null,null,"fcd =",{"$f":"0.85*I48/10/+'Unos podataka'!L26","v":1.4166666666666667},"kN/cm2","  mlim=",{"$f":"+IF($I$49<=60,4.28,IF($I$49=67,5.76,IF($I$49=75,5.39,IF($I$49=85,5.01,IF($I$49=95,4.83,4.83)))))","v":4.28},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   Nq=",{"$f":"(AT244*AT244)/(2*(COS(0.785+AT242/2))^2)","v":0.99920430692091899},{"$f":"(AU244*AU244)/(2*(COS(0.785+AU242/2))^2)","v":1.6403903265132889},{"$f":"(TAN(AV240)/2)*(AV241/(COS(AV240)^2)-1)","v":1.2481372923965159},2.5368723260664181,4.9703674143416272,9.7016824981702374,19.726218273075155,42.434131933505725,100.38899317189207,{"$f":"(TAN(BC256)/2)*(BC257/(COS(BC256)^2)-1)","v":297.50218740368746},{"$f":"(TAN(BD256)/2)*(BD257/(COS(BD256)^2)-1)","v":1153.1638594437377}]
["       a =",{"$f":"+Q52*100","v":5},"cm ",null,null,"  mSd=",{"$f":"+E261","v":{"$error":"#VALUE!"}},null,"ζlim=",{"$f":"+IF($I$49<=60,0.296,IF($I$49=67,0.224,IF($I$49=75,0.211,0.195)))","v":0.29599999999999999},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   Nc=",5.7,{"$f":"(AU262-1)/(TAN(AU242))","v":7.319677722428426},10,5,0,5,0,0,0,0,0]
["d =",{"$f":"+B262-A260*100","v":73.97436801445906},"cm ",null,{"$f":"IF(E261<0.096,-17900.704*E261*E261*E261*E261*E261+5359.131*E261*E261*E261*E261-610.514*E261*E261*E261+31.533*E261*E261-1.242*E261+0.998,-1.60447*E261*E261-0.23713*E261+0.97269)","v":{"$error":"#VALUE!"}},"ζ =",{"$f":"150376*G263^6-62291*G263^5+10258*G263^4-854.43*G263^3+36.991*G263^2-1.213*G263+0.9978","v":{"$error":"#VALUE!"}},null,503,{"$f":"+IF($I$49<=60,0.45,0.35)","v":0.45},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ngama=",{"$f":"(TAN(AT242)/2)*(AT243/(COS(AT242)^2)-1)","v":0},{"$f":"(TAN(AU242)/2)*(AU243/(COS(AU242)^2)-1)","v":0.49402263136734342},19,20,19,20,19,20,20,20,20]
[null,null,null,null,"     As1,min≥",{"$f":"0.0015*B261*B264","v":11.096155202168859},"cm2",null,785,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"    c=",10,10,2.2000000000000002,1,2.2000000000000002,1,2.2000000000000002,1,1,1,1]
[null,null,null,null,"     As1,max=",{"$f":"0.31*B261*B264*G262/G261","v":74.720276225271519},"cm2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"TAN(AC566*PI()/180)","v":0}," gama=",20,20]
[null,null,null,null,"As1=",{"$f":"B260*100/(G261*G264*B264)+E258/G261","v":{"$error":"#VALUE!"}},"cm2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(BA293-BA292)*AR266+AR269","v":3.0001009999999999},"    B=",1,1,1,1,1,1,1,1,1,1,1]
[{"$f":"IF(H50=\"mreža\",\"\",\"odabrano:\")","v":"odabrano:"},{"$f":"IF(H50=\"šipka\",\"   f\",\"\")","v":"   f"},{"$f":"IF(H50=\"mreža\",\"\",O52)","v":14},null," mjerodavno: As1=",{"$f":"IF('Unos podataka'!$O$48=\"\",MAX(F265,F267,G278),MIN(F265,F267,G278))","v":{"$error":"#VALUE!"}},"cm2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+AF564","v":3.0001009999999999},null,null,null,1,1,1,1,1,1,1,1,1]
[{"$f":"IF(H50=\"mreža\",\"\",\"potrebno:\")","v":"potrebno:"},{"$f":"IF($M$569=1,IF($H$50=\"mreža\",\"\",TRUNC(F268/(PI()*C268*C268/400))+1))","v":{"$error":"#VALUE!"}},{"$f":"IF(H50=\"mreža\",\"\",\"kom/m'\")","v":"kom/m'"},null,{"$f":"+IF(H50=\"mreža\",\"\",\"A₁=\")","v":"A₁="},{"$f":"IF(H50=\"mreža\",\"\",B270*C268*C268*PI()/400)","v":{"$error":"#VALUE!"}},{"$f":"+IF(E269=\"\",\"\",\"cm2\")","v":"cm2"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AR268","v":3.0001009999999999},"    D=",1,1,1,1,1,1,1,1,1,1,1]
[{"$f":"IF(H50=\"mreža\",\"\",\"odabrano:\")","v":"odabrano:"},{"$f":"IF(B269=0,0,+IF($H$50=\"mreža\",\"\",IF(B269<=5,5,IF(B269<10,10,B269))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H50=\"mreža\",\"\",\"kom/m'\")","v":"kom/m'"},null,{"$f":"IF(H50=\"mreža\",\"odabrano:\",\"\")","v":""},{"$f":"IF(H50=\"mreža\",\"mreža R\",\"\")","v":""},{"$f":"+IF(H50=\"šipka\",\"\",IF(F268<5.03,503,IF(F268<5.24,524,IF(F268<6.36,636,IF(F268<7.85,785,\"785+ R?\")))))","v":""},{"$f":"+IF(H50=\"šipka\",\"\",IF(P279<0,\"\",IF(P279<3.35,335,IF(P279<5.03,503,IF(P279<7.85,785,\"7,85  +\")))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," ",null,{"$f":"+AR269-AR266*2","v":3.0001009999999999},"   sc=",1,1]
[null,null,null,null,null,null,null,null,{"$f":"+MAX(F295,F295)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sgama=",1,1,{"$f":"AV263*AV261*AV268+AV264*AV267*AV260+0.5*AV264*AV265*AV262*AV269","v":173.10670978600402},178.40274976393897,245.03675701180913,476.54164581127054,838.257085353045,1251.6528966923538,2626.0256086094009,6432.7840261381243,19812.760241582106," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      ex=",null,null,null,null,null,{"$f":"AU274","v":3},{"$f":"AV272","v":3},3,3,3,3,3,3,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      ey=",null,null," qult=",{"$f":"AT265*AT263*AT270+AT266*AT269*AT262+0.5*AT266*AT267*AT264*AT271","v":76.984086138418377},{"$f":"AU265*AU263*AU270+AU266*AU269*AU262+0.5*AU266*AU267*AU264*AU271","v":110.94481006822348},null,null,null,null,null,null,"   qa=",{"$f":"AT273/AT274","v":25.661362046139459},{"$f":"AU273/AU274","v":36.981603356074494},{"$f":"AV271/AV272","v":57.702236595334675},{"$f":"AW271/AW272","v":59.467583254646321}]
[null,"Ograničenje pukotina:     wk=",{"$f":"+I56","v":0.3},"mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      L'=","     +My",null,"   Fs=",3,{"$f":"AT274","v":3}]
["kc=",0.4,"Fs= MEds/z+NEd",null,null,"Fs  =",{"$f":"ABS((((B256/$J$44)+(B257*0.5/$J$45)-(E256/$J$44+E257*0.5/$J$45))/(0.9*B264/100))+(E256/$J$44+E257/$J$45))","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      B'=",{"$f":"BD296/BD297+BD299","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"(3.1416*AC562)/180","v":0.31415999999999999},{"$f":"RADIANS(AC566)","v":0},"HANSEN VESI]"]
["k =",0.8,"Fcr = kc*k*fct,eff*Ac",null,null,"Fcr =",{"$f":"+B275*B276*B277*B278","v":591.79494411567259},"kN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     FMr=",{"$f":"-BD295/BD297+BE531","v":{"$error":"#VALUE!"}}]
["fct,eff =",0.25,"Fcr,eff = b*2,5*(h-d)*fct,eff",null,null,"Fcr,eff =",{"$f":"+B261*2.5*(B262-B264)*B277","v":312.5},"kN",null,null,null,null,null,"za Presjeke I-I i II-II",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      Al=",{"$f":"IF(BD297=0,BB298,+BB298-ABS(2*AQ275))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"     j =",{"$f":"+G14","v":18},"°          Hx =",{"$f":"+BD293","v":0},"kN           j'=",{"$f":"ATAN(TAN(BA277*3.14159/180)/B221)*180/3.14159","v":14.5707680719339},"°        ex="]
["Ac =",{"$f":"B261*B264","v":7397.436801445906},"cm2",null,null,"As =",{"$f":"IF(G275-0.4*G277<0,0,SQRT(C268*G277*(G275-0.4*G277)/(3.6*20000*C274*B277)))","v":{"$error":"#VALUE!"}},"cm2",null,null,null,null,null,"     As,min=",{"$f":"+MAX(F265,F294)","v":{"$error":"#VALUE!"}},{"$f":"+MAX(O279:O280)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      Ig=",{"$f":"IF(BD297=0,BB297,+BB297-ABS(2*AQ276))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"          ","       c =",{"$f":"+G15","v":25},"kPa      Hy =",{"$f":"+BD294","v":{"$error":"#VALUE!"}},"kN           c' =",{"$f":"BA278/D221","v":20},"kPa    ey="]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"     As,1 mjer =",{"$f":"+IF(F267>O278,F267,O278)","v":{"$error":"#VALUE!"}},{"$f":"+O279-7.85","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     Igm=",{"$f":"BF294*3.14159/180","v":0.2543076625950379},{"$f":"IF(AC570=1,\"kPa\",\"\")","v":""},null,null,null,null,null,null,"q=g*Df","g =",{"$f":"+H18","v":10},"kN/m3    Mx =",{"$f":"-BD295","v":{"$error":"#VALUE!"}},"kNm",null,"           L'="]
["                As=  ","f*Fcr,eff *(Fs-0,4*Fcr,eff )      ",null,null,null,null,null,null,null,null,null,null,null,"     As,2 mjer =",{"$f":"+IF(F295>O278,F295,O278)","v":{"$error":"#VALUE!"}},{"$f":"+O280-7.85","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      Ic=",null,null,null,null,null,null,null,null,"    ","   (y)    B =",{"$f":"+E61","v":2.9000021999999994},"m         My =",{"$f":"+BD296","v":0},"kNm         H=",{"$f":"SQRT(BC277*BC277+BC278*BC278)","v":{"$error":"#VALUE!"}},"kN      B'="]
[null,"     (3,6*E*wk*fct,eff)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"3.14159*BG534","v":0.81661083746289675},null,null,null,null,null,null,null,null,"    ","      (x)    L =",{"$f":"+E49","v":12},"m           V =",{"$f":"+BD297","v":{"$error":"#VALUE!"}},"kN            V=",{"$f":"BC281","v":{"$error":"#VALUE!"}},"kPa  FMr="]
["                    PRESJEK II-II:","  KROZ TEMELJ",null,null,null,{"$f":"+IF('Unos podataka'!O48=\"\",\"Glavna armatura na vrhu temelja - prema tlu.  Poz.2\",\"Armatura nije potrebna\")","v":"Glavna armatura na vrhu temelja - prema tlu.  Poz.2"},null,null,null,null,null,null,null,-0.7,-1.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      A'=",null,null,null,null,null,null,null,null," ","      Df =",{"$f":"+(E51+H76)","v":1.0001009999999999},"m"," ","     Mx=",{"$f":"BC279-BC281*BC284","v":{"$error":"#VALUE!"}},"kNm    Al="]
["MG  =",{"$f":"IF('Unos podataka'!O48=\"\",('Sile i krakovi'!R259-B284),0)","v":{"$error":"#VALUE!"}},"kNm/m'   ","NG =",{"$f":"+IF('Unos podataka'!$O$48=\"\",+U71,0)","v":{"$error":"#VALUE!"}},"kN/m'",null,null,null,null,null,null,null,-0.55000000000000004,-3.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(TAN(BF294*3.14159/180)*BD297<=BF296,\"\",TAN(BF294*3.14159/180)*BD297/BF296)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null," ","a =",{"$f":"+ATAN((E52-E51)/E61)*180/PI()","v":9.7823997540577476},"°           ex° =",0,"     My=",{"$f":"BC280+BC281*BC283","v":{"$error":"#VALUE!"}},"kNm     iq="]
["MQ  =",{"$f":"+B141*(C141-G57-E55*0.5)","v":{"$error":"#VALUE!"}},"kNm/m'   ","NQ =",0,"kN/m'",null,null,null,null,null,null,null,-0.4,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," ","g' =",{"$f":"+H17","v":10},"kN/m3  ey°=",0,"    pa =",{"$f":"C236","v":{"$error":"#VALUE!"}},"kPa      ig="]
["MEd=",{"$f":"IF($E$44=0,B283*$J$44+B284*$J$45,B283*1+B284*1)","v":{"$error":"#VALUE!"}},"kNm/m'   "," NEd=",{"$f":"IF(E44=0,E283*$J$44+E284*$J$45,E283*1+E284*1)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"+IF($I$53<=45,0.296,0.252)","v":0.29599999999999999},null,null,null,null,null,null,7.1,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AQ277*AQ278","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"pa=0.5*g....","     Fj =",{"$f":"+J27","v":1.25},null,null,"    R =",{"$f":"BE284*BT575*BT576","v":{"$error":"#VALUE!"}},"kN        ic="]
["     MEds=",{"$f":"IF(B285>0,B285-E285*(B291-B289/2)/100,B285-E285*(B291-B289/2)/100)","v":{"$error":"#VALUE!"}},{"$f":"+IF(E286<B287,\"kNm/m'   >\",\"kNm/m'   <\")","v":{"$error":"#VALUE!"}},"      MRd,lim=",{"$f":"G285*G289*B288*B291*B291/100","v":2975.0957920285496},"kNm/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      Fc =",{"$f":"+J28","v":1.25},{"$f":"IF(B221*BT571>10,\"Fkl >\",\"Fkl =\")","v":{"$error":"#VALUE!"}},{"$f":"IF(B221*BT571>10,10,BV570)","v":{"$error":"#VALUE!"}}]
[{"$f":"+B290/100","v":0.05},{"$f":"+ABS(B286)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+IF(F292/2>F294,F295/2,MAX(F294,F295,G303))","v":{"$error":"#VALUE!"}},null,null,221,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BE277*3.14159/180","v":0.2543076625950379},{"$f":"45*PI()/180","v":0.78539816339744828},{"$f":"AY287/2","v":0.12715383129751895},{"$f":"AZ287+BA287","v":0.91255199469496717},{"$f":"TAN(BB287)","v":1.293166607643838},{"$f":"BC287*BC287","v":1.672279875125072},{"$f":"TAN(AY287)","v":0.25993552228740757},{"$f":"3.14159*BE287","v":0.81661083746289675}]
["   b =",100,"cm ",null,{"$f":"+B287*100/(B288*B291*B291*G289)","v":{"$error":"#VALUE!"}},"fyd =",{"$f":"+G261","v":43.478260869565219},"kN/cm2","es1,lim(%o)=",{"$f":"+IF(J295-I287>0,J295-I287,\"\")","v":""}]
["  hII =",{"$f":"+C192*100","v":89.23077248520525},"cm ",null,null,"fcd =",{"$f":"+G262","v":1.4166666666666667},"kN/cm2","  mlim=",{"$f":"+IF($I$49<=60,4.28,IF($I$49=67,5.76,IF($I$49=75,5.39,IF($I$49=85,5.01,IF($I$49=95,4.83,4.83)))))","v":4.28},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["       a =",{"$f":"+Q58*100","v":5},"cm ",null,null,"  mSd=",{"$f":"+E288","v":{"$error":"#VALUE!"}},null,"ζlim=",{"$f":"+IF($I$49<=60,0.296,IF($I$49=67,0.224,IF($I$49=75,0.211,0.195)))","v":0.29599999999999999},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(AU290-1)/BE287","v":10.710596970300873},"      Nq=",{"$f":"EXP(BF287)*BD287","v":3.7840646174850825},{"$f":"IF(BR578<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}}]
["d =",{"$f":"+B289-A287*100","v":84.23077248520525},"cm ",null,{"$f":"IF(E288<0.096,-17900.704*E288*E288*E288*E288*E288+5359.131*E288*E288*E288*E288-610.514*E288*E288*E288+31.533*E288*E288-1.242*E288+0.998,-1.60447*E288*E288-0.23713*E288+0.97269)","v":{"$error":"#VALUE!"}},"ζ =",{"$f":"150376*G290^6-62291*G290^5+10258*G290^4-854.43*G290^3+36.991*G290^2-1.213*G290+0.9978","v":{"$error":"#VALUE!"}},null,503,{"$f":"+IF($I$49<=60,0.45,0.35)","v":0.45}]
[null,null,null,null,"     As1,min≥",{"$f":"0.0015*B288*B291","v":12.634615872780786},"cm2",null,785,{"$f":"+IF(J295-I291>0,J295-I291,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BR577<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,0]
[null,null,null,null,"     As1,max=",{"$f":"0.31*B288*B291*G289/G288","v":85.08009944109773},"cm2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+AF562","v":5.1500021999999994},null,"kPa    Hx=",0,"KN      Cm=",{"$f":"BB294/BC532","v":20},"kPa"]
[null,null,null,null,"As1=",{"$f":"B287*100/(G288*G291*B291)-E285/G288","v":{"$error":"#VALUE!"}},"cm2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BR579<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"+BA293","v":5.1500021999999994},{"$f":"G15","v":25},"°     Hy=",{"$f":"H161*BB298","v":{"$error":"#VALUE!"}},"      jm=",{"$f":"ATAN(TAN(BB295*3.14159/180)/BC533)*180/3.14159","v":14.5707680719339},"°"]
[{"$f":"IF(H50=\"mreža\",\"\",\"odabrano:\")","v":"odabrano:"},{"$f":"IF(H50=\"šipka\",\"   f\",\"\")","v":"   f"},{"$f":"IF(H50=\"mreža\",\"\",O55)","v":14},null," mjerodavno: As1=",{"$f":"IF('Unos podataka'!$O$48=\"\",MAX(F292,F294,G303),MIN(F292,F294,G303))","v":{"$error":"#VALUE!"}},"cm2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+BA294+2","v":7.1500021999999994},{"$f":"G14","v":18},"kN/m2  Mx=",{"$f":"-D171*BB298","v":{"$error":"#VALUE!"}},"KNm"," "]
[{"$f":"IF(H50=\"mreža\",\"\",\"potrebno:\")","v":"potrebno:"},{"$f":"IF($M$569=1,IF($H$50=\"mreža\",\"\",TRUNC(F295/(PI()*C295*C295/400))+1),TRUNC(F294/(PI()*C295*C295/400)))","v":{"$error":"#VALUE!"}},{"$f":"IF(H50=\"mreža\",\"\",\"kom/m'\")","v":"kom/m'"},null,{"$f":"+IF(H50=\"mreža\",\"\",\"A₁=\")","v":"A₁="},{"$f":"IF(H50=\"mreža\",\"\",B297*C295*C295*PI()/400)","v":{"$error":"#VALUE!"}},{"$f":"+G269","v":"cm2"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"G16","v":20},"m     My=",0,"KNm   H=",{"$f":"SQRT(BD293*BD293+BD294*BD294)","v":{"$error":"#VALUE!"}},"kN"]
[{"$f":"IF(H50=\"mreža\",\"\",\"odabrano:\")","v":"odabrano:"},{"$f":"IF(B296=0,0,+IF($H$50=\"mreža\",\"\",IF(B296<=5,5,IF(B296<10,10,B296))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H50=\"mreža\",\"\",\"kom/m'\")","v":"kom/m'"},null,{"$f":"IF(H50=\"mreža\",\"odabrano:\",\"\")","v":""},{"$f":"IF(H50=\"mreža\",\"mreža R\",\"\")","v":""},{"$f":"+IF(H50=\"šipka\",\"\",IF(F295<5.03,503,IF(F295<5.24,524,IF(F295<6.36,636,IF(F295<7.85,785,\"785+ R?\")))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"C185","v":3.1500021999999994},"m      V=",{"$f":"+B168*E49","v":{"$error":"#VALUE!"}},"KN       V=",{"$f":"BD297+0.0001","v":{"$error":"#VALUE!"}},"kPa"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"E49","v":12},"m"," ","      Mx=",{"$f":"BD295-BD297*BE531","v":{"$error":"#VALUE!"}},"kNm"]
[null,"Ograničenje pukotina:     wk=",{"$f":"+I56","v":0.3},"mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"E51+H76","v":1.0001009999999999},"     ex°=",0,"      My=",{"$f":"BD296+BD297*BD299","v":{"$error":"#VALUE!"}},"kNm"]
["kc=",0.4,"Fs= MEds/z+NEd",null,null,"Fs  =",{"$f":"ABS((((B283/$J$44)+(B284*0.5/$J$45)-(E283/$J$44+E284*0.5/$J$45))/(0.9*B291/100))+(E283/$J$44+E284/$J$45))","v":{"$error":"#VALUE!"}},"kN"]
["k =",0.8,"Fcr = kc*k*fct,eff*Ac",null,null,"Fcr =",{"$f":"+B300*B301*B302*B303","v":673.84617988164212},"kN"]
["fct,eff =",0.25,"Fcr,eff = b*2,5*(h-d)*fct,eff",null,null,"Fcr,eff =",{"$f":"+B288*2.5*(B289-B291)*B302","v":312.5},"kN"]
["Ac =",{"$f":"B288*B291","v":8423.0772485205252},"cm2",null,null,"As =",{"$f":"IF(G300-0.4*G302<0,0,SQRT(C295*G302*(G300-0.4*G302)/(3.6*20000*C299*B302)))","v":{"$error":"#VALUE!"}},"cm2"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+MAX(F292,F425)","v":12.634615872780786},{"$f":"+MAX(O307:O308)","v":{"$error":"#VALUE!"}}]
[" PRESJEK III-III:",{"$f":"\"SPOJ ZID - TEMELJ      +\"","v":"SPOJ ZID - TEMELJ      +"},null,{"$f":"+E52","v":1.2},"m",{"$f":"IF('Unos podataka'!O48=\"\",IF(B311<0,\"Glavna armatura - armatura konzole ili ankeri iz temelja. Poz.10 i Poz.5\",\"Glavna armatuira uz tlo. Poz.7\"),\"Pokriva produžen anker s vanjske strane zida\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"+IF(F294>O306,F294,O306)","v":{"$error":"#VALUE!"}},{"$f":"+O307-7.85","v":{"$error":"#VALUE!"}}]
["MG  =",{"$f":"+U45","v":{"$error":"#VALUE!"}},"kNm/m'   ","NG =",{"$f":"+U48","v":{"$error":"#VALUE!"}},"kN/m'"]
["MQ  =",{"$f":"+U46","v":{"$error":"#VALUE!"}},"kNm/m'   ","NQ =",{"$f":"0","v":0},"kN/m'",null,{"$f":"+H417","v":0},{"$f":"+I417","v":0}]
["MEd=",{"$f":"IF($E$44=0,B308*$J$44+B309*$J$45,B308*1+B309*1)","v":{"$error":"#VALUE!"}},"kNm/m'   "," NEd=",{"$f":"IF($E$44=0,E308*$J$44+E309*$J$45,E308*1+E309*1)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"+IF($I$53<=45,0.296,0.252)","v":0.29599999999999999},{"$f":"+H418","v":0.29599999999999999},0,0]
["     MEds=",{"$f":"IF(B310>0,B310+E310*(B316-B314/2)/100,B310+E310*(B316-B314/2)/100)","v":{"$error":"#VALUE!"}},{"$f":"+IF(E311<B312,\"kNm/m'   >\",\"kNm/m'   <\")","v":{"$error":"#VALUE!"}},"      MRd,lim=",{"$f":"0.296*G314*B313*B316*B316/100","v":2830.5},"kN/m'",null,{"$f":"+H419","v":0},0,0]
[{"$f":"+B315/100","v":0.05},{"$f":"+ABS(B311)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+D420","v":0},{"$f":"+E420","v":0},{"$f":"+F420","v":0},{"$f":"+G420","v":0},0,0]
["   b =",100,"cm",null,{"$f":"+ABS(B312*100/(B313*B316*B316*G314))","v":{"$error":"#VALUE!"}},"fyd =",{"$f":"500/10/'Unos podataka'!L25","v":43.478260869565219},"kN/cm2",{"$f":"+H420","v":0},0]
["  hIII =",{"$f":"+E55*100","v":80},"cm",{"$f":"+D422","v":0},0,"fcd =",{"$f":"0.85*I52/10/+'Unos podataka'!L26","v":1.7},"kN/cm2",{"$f":"+I422","v":0}]
["       a =",{"$f":"+Q58*100","v":5},"cm",0,0,"  mSd=",{"$f":"+E313","v":{"$error":"#VALUE!"}},{"$f":"+H423","v":0},0,0.29599999999999999]
["d =",{"$f":"+B314-B315","v":75},"cm",0,0,"ζ =",{"$f":"150376*G315^6-62291*G315^5+10258*G315^4-854.43*G315^3+36.991*G315^2-1.213*G315+0.9978","v":{"$error":"#VALUE!"}},0,0,0.45]
[{"$f":"+A425","v":0},0,0,0,"     As1,min≥",{"$f":"0.0015*B313*B316","v":11.25},"cm2",0,0,0.81299999999999994]
[0,{"$error":"#VALUE!"},0,0,"     As1,max=",{"$f":"0.31*B313*B316*G314/G313","v":90.907499999999999},"cm2",0,0,0]
[{"$f":"+B427","v":{"$error":"#VALUE!"}},{"$f":"+B427","v":{"$error":"#VALUE!"}},{"$f":"+C427","v":0},{"$f":"+D427","v":0},"As1=",{"$f":"IF(B311<E311,ABS(ABS(B311)*100/(G313*G316*B316)+E310/G313),E311*100/(G310*B316*G313)+((B311+E311)*100)/((B316-B315)*G313)+E310/G313)","v":{"$error":"#VALUE!"}},"cm2",0,0,0]
[{"$f":"IF(H54=\"mreža\",\"\",\"odabrano:\")","v":"odabrano:"},{"$f":"IF(H54=\"mreža\",\"\",\"f\")","v":"f"},{"$f":"+IF(H54=\"mreža\",\"\",+E729)","v":12},null," mjerodavno: As1=",{"$f":"IF('Unos podataka'!$O$48=\"\",MAX(F317,F319,G330),MIN(F317,F319,G330))","v":{"$error":"#VALUE!"}},"cm2",0,null,0]
[{"$f":"IF(H54=\"mreža\",\"\",\"potrebno:\")","v":"potrebno:"},{"$f":"IF(F320=0,0,IF($H$54=\"mreža\",\"\",TRUNC(F320/(PI()*C320*C320/400))+1))","v":{"$error":"#VALUE!"}},{"$f":"IF(H54=\"mreža\",\"\",\"kom/m'\")","v":"kom/m'"},null,{"$f":"+IF(H54=\"mreža\",\"\",\"A₁=\")","v":"A₁="},{"$f":"IF(H54=\"mreža\",\"\",+C320*C320*PI()*B322/400)","v":{"$error":"#VALUE!"}},{"$f":"+IF(H54=\"mreža\",\"\",\"cm²\")","v":"cm²"},null,{"$f":"+I429","v":0},0]
[{"$f":"IF(H54=\"mreža\",\"\",\"odabrano:\")","v":"odabrano:"},{"$f":"IF(B321=\"\",0,+IF($H$54=\"mreža\",\"\",IF(B321<=5,5,IF(B321<10,10,B321))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H54=\"mreža\",\"\",\"kom/m'\")","v":"kom/m'"},null,{"$f":"IF(H54=\"mreža\",\"odabrano:\",\"\")","v":""},{"$f":"IF(H54=\"šipka\",\"\",\" mreža R\")","v":""},{"$f":"+IF(H54=\"šipka\",\"\",IF(F320<5.03,503,IF(F320<5.24,524,IF(F320<6.36,636,IF(F320<7.85,785,\"785+ R?\")))))","v":""},{"$f":"+H430","v":0},0,0]
[{"$f":"+A431","v":0},0,0,0,0,0,0,{"$f":"+H431","v":0},0,0]
[{"$f":"+A432","v":0},null,null,null,null,null,null,null,0,0]
[{"$f":"+A433","v":0},null,null,null,null,null,null,null,null,{"$f":"+J433","v":0}]
[null,"Ograničenje pukotina:     wk=",{"$f":"+I56","v":0.3},{"$f":"+D434","v":"mm"},0,0,0,0]
["kc =",0.4,"Fs= MEds/z+NEd",null,{"$f":"+E435","v":0},"Fs  =",{"$f":"ABS((((B308/$J$44)+(B309*0.5/$J$45)-(E308/$J$44+E309*0.5/$J$45))/(0.9*B316/100))+(E308/$J$44+E309/$J$45))","v":{"$error":"#VALUE!"}},"kN",0]
["k =",0.8,"Fcr = kc*k*fct,eff*Act",null,{"$f":"+E436","v":0},"Fcr =",{"$f":"+B327*B328*B329*B330","v":600.00000000000011},"kN",{"$f":"+I436","v":0},0]
["fct,eff =",0.25,"Fcr,eff = b*2,5*(h-d)*fct,eff",null,null,"Fcr,eff =",{"$f":"+B313*2.5*(B314-B316)*B329","v":312.5},"kN",0,0]
["Ac =",{"$f":"B313*B316","v":7500},"cm2",{"$f":"+D438","v":0},{"$f":"+E438","v":0},"As =",{"$f":"IF(G327-0.4*G329<0,0,SQRT(C320*G329*(G327-0.4*G329)/(3.6*20000*C326*B329)))","v":{"$error":"#VALUE!"}},"cm2",0,0]
[null,null,null,{"$f":"+D440","v":0},0,0,0,0,0,0]
[null,"Dimenzioniranje na poprečnu silu:","VED=",{"$f":"+AD56","v":{"$error":"#VALUE!"}},{"$f":"+IF(D332>G332,\"kN       > \",\"kN       < \")","v":{"$error":"#VALUE!"}},"VRd,c=",{"$f":"+AD73","v":{"$error":"#VALUE!"}},{"$f":"IF(G332>D332,\"kN    (Zadovoljava)\",\"kN  (NE Zadovoljava)\")","v":{"$error":"#VALUE!"}},0,0]
[{"$f":"+IF(D332<G332,\"\",    \"           spone\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(D332<G332,\"\",\"Asw\")","v":{"$error":"#VALUE!"}},{"$f":"(+AE90)","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(D332<G332,\"\",\"odabrano:\")","v":{"$error":"#VALUE!"}},null,null,null,0]
[{"$f":"+IF(D332<G332,\"\",\"f\")","v":{"$error":"#VALUE!"}},{"$f":"IF(D332<G332,\"\",AD93)","v":{"$error":"#VALUE!"}},{"$f":"IF(AD86>AD70,\"\",AD90)","v":{"$error":"#VALUE!"}},{"$f":"IF(AD86>AD70,\"\",AH85)","v":{"$error":"#VALUE!"}},{"$f":"IF(AD86>AD70,\"\",AC87)","v":{"$error":"#VALUE!"}},{"$f":"IF(AD86>AD70,\"\",AF93)","v":{"$error":"#VALUE!"}},{"$f":"+IF(B334>0,\"cm\",\"\")","v":{"$error":"#VALUE!"}}]
[null,"        PRESJEK NA VISINI:+",{"$f":"+Q44","v":{"$error":"#VALUE!"}},"m   (Mmin)",null,{"$f":"IF('Unos podataka'!O48=\"\",IF(B338<0,\"Glavna armatura - armatura konzole. Poz. 10\",IF(C335<C550,\"Glavna armatura - ankeri iz temelja. Poz.5\",\"Glavna armatura - uz tlo. Poz. 7\")),\"Armatura nije potrebna\")","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+J441","v":0}]
["MG  =",{"$f":"AN45","v":{"$error":"#VALUE!"}},"kNm/m'   ","NG =",{"$f":"AN48","v":{"$error":"#VALUE!"}},"kN/m'"]
["MQ  =",{"$f":"+AN46","v":{"$error":"#VALUE!"}},"kNm/m'   ","NQ =",{"$f":"0","v":0},"kN/m'"]
["MEd=",{"$f":"IF($E$44=0,B336*$J$44+B337*$J$45,B336*1+B337*1)","v":{"$error":"#VALUE!"}},"kNm/m'   "," NEd=",{"$f":"IF($E$44=0,E336*$J$44+E337*$J$45,E336*1+E337*1)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"+IF($I$53<=45,0.296,0.252)","v":0.29599999999999999}]
["     MEds=",{"$f":"IF(B338>0,B338+E338*(B344-B342/2)/100,B338+E338*(B344-B342/2)/100)","v":{"$error":"#VALUE!"}},{"$f":"+IF(E339<B340,\"kNm/m'   >\",\"kNm/m'   <\")","v":{"$error":"#VALUE!"}},"      MRd,lim=",{"$f":"0.296*G342*B341*B344*B344/100","v":{"$error":"#VALUE!"}},"kN/m'"]
[null,{"$f":"+ABS(B339)","v":{"$error":"#VALUE!"}}]
["   b =",100,"cm ",{"$f":"IF(E341<0.096,-17900.704*E341*E341*E341*E341*E341+5359.131*E341*E341*E341*E341-610.514*E341*E341*E341+31.533*E341*E341-1.242*E341+0.998,-1.60447*E341*E341-0.23713*E341+0.97269)","v":{"$error":"#VALUE!"}},{"$f":"+ABS(B340*100/(B341*B344*B344*G342))","v":{"$error":"#VALUE!"}},"fyd =",{"$f":"+G313","v":43.478260869565219},"kN/cm2","es1,lim(%o)="]
["  hIV =",{"$f":"+('C III-V'!U35-'C III-V'!U34)*100","v":{"$error":"#VALUE!"}},"cm ",null,null,"fcd =",{"$f":"+G314","v":1.7},"kN/cm2","  mlim=",{"$f":"+IF($I$49<=60,4.28,IF($I$49=67,5.76,IF($I$49=75,5.39,IF($I$49=85,5.01,IF($I$49=95,4.83,4.83)))))","v":4.28}]
["       a =",{"$f":"+Q58*100","v":5},"cm ",null,null,"  mSd=",{"$f":"+E341","v":{"$error":"#VALUE!"}},null,"ζlim=",{"$f":"+IF($I$49<=60,0.296,IF($I$49=67,0.224,IF($I$49=75,0.211,0.195)))","v":0.29599999999999999}]
["d =",{"$f":"+B342-B343","v":{"$error":"#VALUE!"}},"cm ",null,null,"ζ =",{"$f":"150376*G343^6-62291*G343^5+10258*G343^4-854.43*G343^3+36.991*G343^2-1.213*G343+0.9978","v":{"$error":"#VALUE!"}},null,null,{"$f":"+IF($I$49<=60,0.45,0.35)","v":0.45}]
[null,null,null,null,"     As1,min≥",{"$f":"0.0015*B341*B344","v":{"$error":"#VALUE!"}},"cm2",null,null,{"$f":"+IF($I$53<=60,0.813,IF($I$53=67,0.863,IF($I$53=75,0.868,IF($I$53=85,0.873,IF($I$53=95,0.8758,0.8765)))))","v":0.81299999999999994}]
[null,{"$f":"+IF(F345>F347,F345,F347)","v":{"$error":"#VALUE!"}},null,null,"     As1,max=",{"$f":"0.31*B341*B344*G342/G341","v":{"$error":"#VALUE!"}},"cm2"]
[null,null,null,null,"As1=",{"$f":"ABS(IF(B339<E339,ABS(ABS(B339)*100/(G341*G344*B344)-E338/G341),E339*100/(J346*B344*G341)+((B339-E339)*100)/((B344-B343)*G341)+E338/G341))","v":{"$error":"#VALUE!"}},"cm2"]
[{"$f":"IF(H54=\"šipka\",\"odabrano:\",\"\")","v":"odabrano:"},{"$f":"+IF(H54=\"šipka\",\"f\",\"\")","v":"f"},{"$f":"+IF(H54=\"mreža\",\"\",+E729)","v":12},null," mjerodavno: As1=",{"$f":"IF('Unos podataka'!$O$51=\"\",MAX(F345,F347,G358),MAX(F345,F347,G358))","v":{"$error":"#VALUE!"}},"cm2"]
[{"$f":"IF(H54=\"šipka\",\"potrebno:\",\"\")","v":"potrebno:"},{"$f":"IF($M$569=1,IF($H$54=\"mreža\",\"\",TRUNC(F348/(PI()*C348*C348/400))+1))","v":{"$error":"#VALUE!"}},{"$f":"IF(H54=\"mreža\",\"\",\"kom/m'\")","v":"kom/m'"},null,{"$f":"+IF(H54=\"mreža\",\"\",\"A₁=\")","v":"A₁="},{"$f":"IF(H54=\"mreža\",\"\",+C348*C348*PI()*B350/400)","v":{"$error":"#VALUE!"}},{"$f":"+G321","v":"cm²"}]
[{"$f":"IF(H54=\"šipka\",\"odabrano:\",\"\")","v":"odabrano:"},{"$f":"+IF(B349=\"\",0,+IF($H$54=\"mreža\",\"\",IF(B349<=5,5,IF(B349<10,10,B349))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H54=\"mreža\",\"\",\"kom/m'\")","v":"kom/m'"},null,{"$f":"IF(H54=\"mreža\",\"odabrano:\",\"\")","v":""},{"$f":"IF(H54=\"šipka\",\"\",\" mreža R\")","v":""},{"$f":"+IF(H54=\"šipka\",\"\",IF(F348<5.03,503,IF(F348<5.24,524,IF(F348<6.36,636,IF(F348<7.85,785,\"785+ R?\")))))","v":""}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"IF(G351>0,\"kom/m'\",\"\")","v":""}]
[]
[null,"Ograničenje pukotina:     wk=",{"$f":"+I56","v":0.3},"mm"]
["kc=",0.4,"Fs= MEds/z+NEd",null,null,"Fs  =",{"$f":"ABS((((B336/$J$44)+(B337*0.5/$J$45)-(E336/$J$44+E337*0.5/$J$45))/(0.9*B344/100))+(E336/$J$44+E337/$J$45))","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["k =",0.8,"Fcr = kc*k*fct,eff*Ac",null,null,"Fcr =",{"$f":"+B355*B356*B357*B358","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(T356=\"\",\"\",1)","v":""}]
["fct,eff =",0.25,"Fcr,eff = b*2,5*(h-d)*fct,eff",null,null,"Fcr,eff =",{"$f":"+B341*2.5*(B342-B344)*B357","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,null,null,null,"Razdjelna lijevo",null,null,null,null,{"$f":"+IF(T357=\"\",\"\",1)","v":""}]
["Ac =",{"$f":"B341*B344","v":{"$error":"#VALUE!"}},"cm2",null,null,"As =",{"$f":"IF(G355-0.4*G357<0,0,SQRT(C348*G357*(G355-0.4*G357)/(3.6*20000*C354*B357)))","v":{"$error":"#VALUE!"}},"cm2",null,null,null,null,null,null,null,null,null,null,"Razdjelna na vrhu zida"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Razdjelna vrha"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Razdjelna na spoju zida i konzole",null,null,{"$f":"+AE377","v":{"$error":"#VALUE!"}},-0.40499999999999997,{"$f":"+IF(S360>0,1,0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(B563=\"   785  +\",785,785)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Razdjelna  između akera ",null,null,{"$error":"#VALUE!"},-7.4999999999999997E-2,{"$f":"+IF(S361>0,1,0)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+N376+Q58+0.03","v":3.4800010999999995},{"$f":"+E544-0.03","v":1.1099999999999999},{"$f":"+IF(P362=0,0,1)","v":1},{"$error":"#VALUE!"},-7.4999999999999997E-2,{"$f":"+IF(S362>0,1,0)","v":{"$error":"#VALUE!"}}]
[null,"        PRESJEK NA VISINI:+",{"$f":"+R44","v":{"$error":"#VALUE!"}},"m   (Mmax)",null,{"$f":"IF('Unos podataka'!O48=\"\",IF(B367>0,\"Postojeća armatura uz tlo\",IF(B367>=0,IF(A82=\"\",\"Ankeri iz temelja Poz. 5\",\"Postojeća armatura konzole Poz. 10\"))),\"Armatura nije potrebna\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,{"$f":"IF(E59=0,S374,B548+0.02)","v":{"$error":"#VALUE!"}},{"$f":"IF(E59=0,T374,C548+0.01)","v":{"$error":"#VALUE!"}},1,{"$error":"#VALUE!"},-0.40499999999999997,{"$f":"+IF(S363>0,1,0)","v":{"$error":"#VALUE!"}}]
["MG  =",{"$f":"AO45","v":{"$error":"#VALUE!"}},"kNm/m'   ","NG =",{"$f":"AO48","v":{"$error":"#VALUE!"}},"kN/m'",null,null,null,null,null,null,null,null,null,{"$f":"+N385-0.06","v":4.1400011000000001},{"$f":"+Q362","v":1.1099999999999999},{"$f":"+IF(P364=0,0,1)","v":1},null,"kom",{"$f":"SUM(U360:U363)","v":{"$error":"#VALUE!"}}]
["MQ  =",{"$f":"+AO46","v":{"$error":"#VALUE!"}},"kNm/m'   ","NQ =",{"$f":"0*E263","v":0},"kN/m'",null,null,null,null,null,null,null,null,null,{"$f":"+B552","v":{"$error":"#VALUE!"}},{"$f":"+C552-0.005","v":{"$error":"#VALUE!"}},{"$f":"+IF(P365=-2,0,1)","v":{"$error":"#VALUE!"}},"Ukupno:","kom",{"$f":"U379+U391+U364","v":{"$error":"#VALUE!"}}]
["MEd=",{"$f":"IF($E$44=0,B364*$J$44+B365*$J$45,B364*1+B365*1)","v":{"$error":"#VALUE!"}},"kNm/m'   "," NEd=",{"$f":"IF($E$44=0,E364*$J$44+E365*$J$45,E364*1+E365*1)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"+IF($I$53<=45,0.296,0.252)","v":0.29599999999999999},null,null,null,null,null,null,null,null,null,"kom",{"$f":"SUM(R362:R365)","v":{"$error":"#VALUE!"}},"vertikalna armatura temelja - desno",null,null,{"$f":"IF(K39=0,0,V367-(W366-W367)/F56)","v":{"$error":"#VALUE!"}},{"$f":"IF(K39=0,0,W367+0.15)","v":4.2249999960000002}]
["     MEds=",{"$f":"IF($E$44>0,B365*$J$44+B366*$J$45,B365*1+B366*1)","v":{"$error":"#VALUE!"}},{"$f":"+IF(E367<B368,\"kNm/m'   >\",\"kNm/m'   <\")","v":{"$error":"#VALUE!"}},"      MRd,lim=",{"$f":"0.296*G370*B369*B372*B372/100","v":{"$error":"#VALUE!"}},"kN/m'",null,null,null,null,null,null,null,null,null,"Ukupno:","kom",{"$f":"R381+R393+R366","v":{"$error":"#VALUE!"}},{"$f":"+$F$550-0.015","v":4.8350021999999999},{"$f":"IF(M569=\"\",-1,G550-0.015)","v":1.105},{"$f":"+IF(S367<=-2,0,1)","v":1},{"$f":"IF(K39=0,0,V368-(W367-W368)/F56)","v":{"$error":"#VALUE!"}},{"$f":"IF(K39=0,0,+W368+0.075)","v":4.0749999959999998},null,"Armatura uz sidra"]
[null,{"$f":"+ABS(B367)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+IF($I$53<=60,0.813,IF($I$53=67,0.863,IF($I$53=75,0.868,IF($I$53=85,0.873,IF($I$53=95,0.8758,0.8765)))))","v":0.81299999999999994},null,null,null,null,null,null,"Betonski presjek",null,"vertikalna armatura temelja - lijevo",null,null,{"$f":"(IF(E52-(E52-E51)<1.01,-2,+$F$550-0.02))","v":-2},{"$f":"IF(M569=\"\",-1,IF(S368=0,0,T369+(T367-T369)/2))","v":0.97750000000000004},{"$f":"+IF(S368<=-2,0,1)","v":0},{"$f":"IF(K39=0,0,'C III-V'!AB10-0.07)","v":{"$error":"#VALUE!"}},{"$f":"IF(K39=0,0,E40)","v":3.9999999960000001},{"$f":"+IF(W366=0,0,1)","v":1},{"$f":"+R118","v":{"$error":"#VALUE!"}},{"$f":"+S116","v":-3}]
["   b =",100,"cm ",{"$f":"IF(E369<0.096,-17900.704*E369*E369*E369*E369*E369+5359.131*E369*E369*E369*E369-610.514*E369*E369*E369+31.533*E369*E369-1.242*E369+0.998,-1.60447*E369*E369-0.23713*E369+0.97269)","v":{"$error":"#VALUE!"}},{"$f":"+ABS(B368*100/(B369*B372*B372*G370))","v":{"$error":"#VALUE!"}},"fyd =",{"$f":"+G341","v":43.478260869565219},"kN/cm2",null,null,null,null,null,{"$f":"+AS173-2","v":0},{"$f":"+AT173","v":0.12820515121628623},{"$f":"2.08+E60*0.07/E52-0.01","v":2.0700000000000003},{"$f":"IF(M569=\"\",-1,+Q376-0.01)","v":1.0999999999999999},{"$f":"+IF(P369=-2,0,1)","v":1},{"$f":"IF(T369=0,-2,+$F$550-0.015)","v":4.8350021999999999},{"$f":"+IF(M569=\"\",-1,(E52-E51)+E51/2)","v":0.85},{"$f":"+IF(S369<=-2,0,1)","v":1},{"$f":"IF(K39=0,0,V368+(W368-W369)/F56)","v":{"$error":"#VALUE!"}},{"$f":"IF(K39=0,0,+W368-0.075)","v":3.9249999959999999},{"$f":"+IF(W367=0,0,1)","v":1},{"$f":"+R119","v":{"$error":"#VALUE!"}},{"$f":"+S117","v":-3}]
["  hV =",{"$f":"+('C III-V'!U30-'C III-V'!U29)*100","v":{"$error":"#VALUE!"}},"cm ",null,null,"fcd =",{"$f":"+G342","v":1.7},"kN/cm2",null,null,null,null,null,{"$f":"+AS174-2","v":0},{"$f":"+AT174","v":1.2},{"$f":"IF(E52<1.01,-2,(P371+P369)/2)","v":2.0700000000000003},{"$f":"IF(M569=\"\",-1,IF(Q369-Q371<'Unos podataka'!F94/100,\"\",+IF(P370=0,0,(Q369+Q371)/2)))","v":0.84999999999999987},{"$f":"+IF(P370=-2,0,1)","v":1},{"$f":"IF(E52-(E52-E51)<1.01,-2,+$F$550-0.02)","v":-2},{"$f":"IF(M569=\"\",-1,IF(S370=0,0,T399+(T369-T399)/2))","v":0.71155172675386247},{"$f":"+IF(S370<=-2,0,1)","v":0},{"$f":"IF(K39=0,0,V369+(W369-W370)/F56)","v":{"$error":"#VALUE!"}},{"$f":"IF(K39=0,0,W369-0.15)","v":3.774999996}]
["       a =",{"$f":"+Q58*100","v":5},"cm ",null,null,"  mSd=",{"$f":"+E369","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+AS175-2","v":1.4000010999999999},{"$f":"+AT175","v":1.2},{"$f":"IF(Q371=0,-2,(P369+P373)/2)","v":2.0700000000000003},{"$f":"IF(M569=\"\",-1,IF(Q369-Q373<'Unos podataka'!F94/100,\"\",E52/2))","v":0.6},{"$f":"+IF(P371=-2,0,1)","v":1},{"$f":"+S367","v":4.8350021999999999},{"$f":"+IF(M569=\"\",-1,T399)","v":0.57310345350772507},{"$f":"+IF(S371<=-2,0,1)","v":1},"Poz. 6a",{"$f":"+Y368","v":{"$error":"#VALUE!"}},{"$f":"+IF(W369=0,0,1)","v":1},{"$f":"+R121","v":{"$error":"#VALUE!"}},{"$f":"+S119","v":-3}]
["d =",{"$f":"+B370-B371","v":{"$error":"#VALUE!"}},"cm ",null,null,"ζ =",{"$f":"150376*G371^6-62291*G371^5+10258*G371^4-854.43*G371^3+36.991*G371^2-1.213*G371+0.9978","v":{"$error":"#VALUE!"}},null,null,null,null,"                          Koordinatte temelja kontrafore",null,{"$f":"+AS176-2","v":{"$error":"#VALUE!"}},{"$f":"+AT176","v":"A"},{"$f":"IF(E52<1.01,-2,(P373+P371)/2)","v":2.0700000000000003},{"$f":"IF(M571=\"\",-1,IF(Q371-Q373<'Unos podataka'!F96/100,\"\",+IF(P372=0,0,(Q371+Q373)/2)))","v":0.41341291716581502},{"$f":"+IF(P372=-2,0,1)","v":1},"Ukupno:","kom",{"$f":"SUM(U367:U371)","v":3},null,{"$f":"+Y374","v":{"$error":"#VALUE!"}},{"$f":"+IF(W370=0,0,1)","v":1},{"$f":"+R122","v":{"$error":"#VALUE!"}},{"$f":"+S120","v":-3.15}]
[null,null,null,null,"     As1,min≥",{"$f":"0.0015*B369*B372","v":{"$error":"#VALUE!"}},"cm2",null,null,null,null,null,null,{"$f":"+AS177-2","v":2.2000010999999997},{"$f":"+AT177","v":1.2},{"$f":"2.08+E60-0.01","v":2.0700000000000003},{"$f":"IF(M569=\"\",-1,E551+0.02)","v":0.22682583433163006},{"$f":"+IF(P373=-2,0,1)","v":1},"Razdjelna dole lijevo R1dl do R10dl",null,null,null,{"$f":"+Y369","v":{"$error":"#VALUE!"}},{"$f":"+Z368","v":-3},{"$f":"+Y372","v":{"$error":"#VALUE!"}},{"$f":"+Z372","v":-3.15}]
[null,null,null,null,"     As1,max=",{"$f":"0.31*B369*B372*G370/G369","v":{"$error":"#VALUE!"}},"cm2",null,null,null,null,{"$f":"IF(Kontrafore!E3=\"\",-10,N374)","v":2},{"$f":"IF('Unos podataka'!$AB$1=\"\",0,+O374)","v":0.12820515121628623},{"$f":"+'C III-V'!B2","v":2},{"$f":"+'C III-V'!C2","v":0.12820515121628623},"Ukupno:","kom",{"$f":"SUM(R369:R373)","v":5},{"$f":"+P373","v":2.0700000000000003},{"$f":"+Q373","v":0.22682583433163006},null,"Razdjelna uz glavnu armaturu",null,{"$f":"+T22+0.5","v":0.5},{"$f":"+Y373+1","v":{"$error":"#VALUE!"}},{"$f":"+T22+0.5","v":0.5}]
[{"$f":"IF(H54=\"šipka\",\"odabrano:\",\"\")","v":"odabrano:"},{"$f":"IF(H54=\"šipka\",\"f\",\"\")","v":"f"},{"$f":"IF(H54=\"mreža\",\"\",E729)","v":12},null,"As1=",{"$f":"ABS(IF(B367<E367,ABS(B367)*100/(G369*G372*B372)+E366/G369,E367*100/(J374*B372*G369)+((B367-E367)*100)/((B372-B371)*G369)+E366/G369))","v":{"$error":"#VALUE!"}},"cm2",null,null,null,null,{"$f":"IF(Kontrafore!E3=\"\",-10,N375)","v":2},{"$f":"IF('Unos podataka'!$AB$1=\"\",0,O375)","v":1.2},{"$f":"+'C III-V'!B3","v":2},{"$f":"+'C III-V'!C3","v":1.2},"Razdjelna gore lijevo  Rh13 do RH20",null,null,{"$f":"S374+0.4","v":2.4700000000000002},{"$f":"IF(M569=\"\",-1,T374+$R$56*TAN($F$217*PI()/180))","v":0.27810785668536103},{"$f":"+IF(S375<0,0,1)","v":1},{"$f":"IF(E56=\">100\",V376,B563-0.015)","v":{"$error":"#VALUE!"}},{"$f":"+W378","v":-0.40499999999999997},{"$f":"+Z369","v":-3},{"$f":"+Y371","v":{"$error":"#VALUE!"}},{"$f":"+Z371","v":-3}]
[{"$f":"IF(H54=\"šipka\",\"potrebno:\",\"\")","v":"potrebno:"},{"$f":"IF($M$569=1,IF($H$54=\"mreža\",\"\",TRUNC(F376/(PI()*C375*C375/400))+1))","v":{"$error":"#VALUE!"}},{"$f":"IF(H54=\"mreža\",\"\",\"kom/m'\")","v":"kom/m'"},null," mjerodavno: As1=",{"$f":"IF('Unos podataka'!$O$51=\"\",MAX(F373,F375,G386),MAX(F373,F375,G386))","v":{"$error":"#VALUE!"}},"cm2",null,null,null,null,{"$f":"IF(Kontrafore!E3=\"\",-10,L375-Kontrafore!E3)","v":1},{"$f":"IF('Unos podataka'!$AB$1=\"\",0,O376)","v":1.2},{"$f":"+'C III-V'!B4","v":3.4000010999999999},{"$f":"+'C III-V'!C4","v":1.2},{"$f":"+P369","v":2.0700000000000003},{"$f":"+E544-0.03","v":1.1099999999999999},0,{"$f":"IF(S375+$R$56>$P$363-0.1,-2,S375+$R$56)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",-1,T375+$R$56*TAN($F$217*PI()/180)-0.01)","v":0.319389879039092},{"$f":"+IF(S376<0,0,1)","v":{"$error":"#VALUE!"}},{"$f":"+A562","v":{"$error":"#VALUE!"}},{"$f":"+C561-0.005","v":-5.5E-2},null,"Razdjelna konzola Rk",null,null,null,null,null,null,"POZ. 6"]
[{"$f":"IF(H54=\"šipka\",\"odabrano:\",\"\")","v":"odabrano:"},{"$f":"+IF(B376=\"\",0,+IF($H$54=\"mreža\",\"\",IF(B376<=5,5,IF(B376<10,10,B376))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H54=\"mreža\",\"\",\"kom/m'\")","v":"kom/m'"},null,{"$f":"IF(H54=\"šipka\",\"A₁=\",\"\")","v":"A₁="},{"$f":"IF(H54=\"mreža\",\"\",+C375*C375*PI()*(B377+B378)/400)","v":{"$error":"#VALUE!"}},{"$f":"+IF(H54=\"mreža\",\"\",\"cm²\")","v":"cm²"},null,null,null,null,{"$f":"+L376+E60","v":1},{"$f":"+IF('Unos podataka'!$AB$1=\"\",0,0)","v":0},{"$f":"+'C III-V'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C5","v":3.14},{"$f":"P373+R56","v":2.4700000000000002},{"$f":"IF(M569=\"\",-1,IF(P377=0,0,$E$544-0.03))","v":1.1099999999999999},{"$f":"+IF(P377=-2,0,1)","v":1},{"$f":"IF($S$375+2*$R$53+0.1>$P$363,-2,$S$375+2*$R$53)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",-1,T376+$R$56*TAN($F$217*PI()/180))","v":0.37067190139282297},{"$f":"+IF(S377<0,0,1)","v":{"$error":"#VALUE!"}},{"$f":"+B561+0.02","v":{"$error":"#VALUE!"}},{"$f":"+W376","v":-5.5E-2},{"$f":"+IF(V375=0,0,1)","v":{"$error":"#VALUE!"}},{"$f":"IF($F$556-0.01<=D555,-2,$F$556-0.01)","v":{"$error":"#VALUE!"}},{"$f":"IF($G$78=0,0,G555-0.02)","v":3.37},{"$f":"+IF(Y377<=-2,0,1)","v":{"$error":"#VALUE!"}},{"$f":"+V378","v":{"$error":"#VALUE!"}},{"$f":"+W378","v":-0.40499999999999997},{"$f":"+X380","v":{"$error":"#VALUE!"}},{"$f":"+AB377","v":{"$error":"#VALUE!"}},{"$f":"+IF(W375<$E$79,W375,IF(W375>$E$79+$E$81,W375,-5))","v":-0.40499999999999997},{"$f":"+IF(AE377<=0,0,1)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,{"$f":"IF(H54=\"mreža\",\"odabrano:\",\"\")","v":""},{"$f":"IF(H54=\"šipka\",\"\",\" mreža R\")","v":""},{"$f":"+IF(H54=\"šipka\",\"\",IF(F376<5.03,503,IF(F376<5.24,524,IF(F376<6.36,636,IF(F376<7.85,785,\"785+ R?\")))))","v":""},null,null,null,null,{"$f":"+L374","v":2},{"$f":"+IF('Unos podataka'!$AB$1=\"\",0,M374)","v":0.12820515121628623},{"$f":"+'C III-V'!B6","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C6","v":3.14},{"$f":"IF($P$377+$R$53+0.1>$P$362,-2,$P$377+$R$53)","v":2.87},{"$f":"IF(M569=\"\",-1,IF(P378=0,0,$E$544-0.03))","v":1.1099999999999999},1,{"$f":"IF($S$375+3*$R$53+0.1>$P$363,-2,$S$375+3*$R$53)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",-1,T377+$R$56*TAN($F$217*PI()/180))","v":0.42195392374655394},{"$f":"+IF(S378<0,0,1)","v":{"$error":"#VALUE!"}},{"$f":"IF(H51=0.000001,V377,V377+(W377-W378)/F57)","v":{"$error":"#VALUE!"}},{"$f":"+W377-0.35","v":-0.40499999999999997},{"$f":"+IF(V376=0,0,1)","v":{"$error":"#VALUE!"}},{"$f":"IF(Y377=-2,-2,U406)","v":{"$error":"#VALUE!"}},{"$f":"IF(Y378=0,0,Z377)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+V377","v":{"$error":"#VALUE!"}},{"$f":"+W377","v":-5.5E-2},{"$f":"+X379","v":{"$error":"#VALUE!"}},{"$f":"+AB378","v":{"$error":"#VALUE!"}},{"$f":"+IF(W376<$E$79,W376,IF(W376>$E$79+$E$81,W376,-5))-0.02","v":-7.4999999999999997E-2},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B7","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C7","v":3.44},{"$f":"IF($P$377+2*$R$53+0.1>$P$362,-2,$P$377+2*$R$53)","v":3.2700000000000005},{"$f":"IF(P379=0,0,$E$544-0.03)","v":1.1099999999999999},1,{"$f":"IF($S$375+4*$R$53+0.1>$P$363,-2,$S$375+4*$R$53)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",-1,T378+$R$56*TAN($F$217*PI()/180))","v":0.47323594610028491},{"$f":"+IF(S379<0,0,1)","v":{"$error":"#VALUE!"}},{"$f":"IF(W379<0,-2,IF($H$54=\"šipka\",V378+0.004+$R$59*TAN($H$51*PI()/180),-2))","v":-2},{"$f":"IF(W378-$R$59<$E$52,-5,W378-$R$59)","v":-5},{"$f":"+IF(V377=0,0,1)","v":{"$error":"#VALUE!"}},{"$f":"IF(Y378=0,-2,IF(Y378-$R$68-0.2<=$D$555,-2,Y378-$R$68))","v":{"$error":"#VALUE!"}},{"$f":"IF(Y379=0,-5,Z378)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+V376","v":{"$error":"#VALUE!"}},{"$f":"+W377","v":-5.5E-2},{"$f":"+X378","v":{"$error":"#VALUE!"}},{"$f":"+AB379","v":{"$error":"#VALUE!"}},{"$f":"+IF(W377<$E$79,W377,IF(W377>$E$79+$E$81,W377,-5))-0.02","v":-7.4999999999999997E-2},{"$error":"#VALUE!"}]
[null,null,null,null,null,{"$f":"IF(B367<E367,\"\",(B367-E367)*100/((B372-B371)*G369))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+'C III-V'!B8","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C8","v":3.44},{"$f":"IF($P$377+3*$R$53+0.1>$P$362,-2,$P$377+3*$R$53)","v":-2},{"$f":"IF(M569=\"\",-1,IF(P380=0,0,$E$544-0.03))","v":1.1099999999999999},0,{"$f":"IF($S$375+5*$R$53+0.1>$P$363,-2,$S$375+5*$R$53)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",-1,T379+$R$56*TAN($F$217*PI()/180))","v":0.52451796845401588},{"$f":"+IF(S380<=0,0,1)","v":{"$error":"#VALUE!"}},{"$f":"IF(W380<0,-2,IF($H$54=\"šipka\",V379+$R$59*TAN($H$51*PI()/180),-2))","v":-2},-5,{"$f":"+IF(V378=0,0,1)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(Y380=0,0,Z379)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+V375","v":{"$error":"#VALUE!"}},-0.40499999999999997,{"$f":"+X377","v":{"$error":"#VALUE!"}},{"$f":"+AB380","v":{"$error":"#VALUE!"}},{"$f":"+IF(W378<$E$79,W378,IF(W378>$E$79+$E$81,W378,-5))","v":-0.40499999999999997},{"$error":"#VALUE!"}]
[null,null,null,null,null,{"$f":"IF(B367<E367,\"\",IF(H54=\"šipka\",B381*B381*PI()*D381/400,\"Odabrano:\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+'C III-V'!B9","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C9","v":"A"},{"$f":"IF($P$377+4*$R$53+0.1>$P$362,-2,$P$377+4*$R$53)","v":-2},{"$f":"IF(M569=\"\",-1,IF(P381=0,0,$E$544-0.03))","v":1.1099999999999999},0,{"$f":"IF($S$375+6*$R$53+0.1>$P$363,-2,$S$375+6*$R$53)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",-1,T380+$R$56*TAN($F$217*PI()/180))","v":0.57579999080774691},{"$f":"+IF(S381<=0,0,1)","v":{"$error":"#VALUE!"}},-2,-5,{"$f":"+IF(V379=-2,0,1)","v":0},{"$error":"#VALUE!"},{"$f":"IF(Y381=0,0,Z380)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+V376","v":{"$error":"#VALUE!"}},-5,{"$f":"+X381","v":0},{"$f":"+IF($H$54=\"šipka\",V379,V379-1)","v":-2},-5,0]
[null,"Ograničenje pukotina:     wk=",{"$f":"+I56","v":0.3},"mm",null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B10","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C10","v":"A"},{"$f":"IF($P$377+5*$R$53+0.1>$P$362,-2,$P$377+5*$R$53)","v":-2},{"$f":"IF(M569=\"\",-1,IF(P382=0,0,$E$544-0.03))","v":1.1099999999999999},0,{"$f":"IF($S$375+7*$R$53+0.1>$P$363,-2,$S$375+7*$R$53)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",-1,T381+$R$56*TAN($F$217*PI()/180))","v":0.62708201316147794},{"$f":"+IF(S382<=0,0,1)","v":{"$error":"#VALUE!"}},-2,-5,0,{"$error":"#VALUE!"},{"$f":"IF(Y382=0,0,Z381)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+V377","v":{"$error":"#VALUE!"}},-5,0,-2,-5,0]
["kc=",0.4,"Fs= MEds/z+NEd",null,null,"Fs  =",{"$f":"ABS((((B364/$J$44)+(B365*0.5/$J$45)-(E364/$J$44+E365*0.5/$J$45))/(0.9*B372/100))+(E364/$J$44+E365/$J$45))","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,null,{"$f":"+'C III-V'!B11","v":4.2000010999999997},{"$f":"+'C III-V'!C11","v":1.2},{"$f":"IF($P$377+6*$R$53+0.1>$P$362,-2,$P$377+6*$R$53)","v":-2},{"$f":"IF(M569=\"\",-1,IF(P383=0,0,$E$544-0.03))","v":1.1099999999999999},0,{"$f":"IF($S$375+8*$R$53+0.1>$P$363,-2,$S$375+8*$R$53)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",-1,T374+$R$56*TAN($F$217*PI()/180)-0.01)","v":0.26810785668536102},0,-2,-5,0,{"$error":"#VALUE!"},{"$f":"IF(Y383=0,0,Z382)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+V378","v":{"$error":"#VALUE!"}},-5,0,-2,-5,0]
["k =",0.8,"Fcr = kc*k*fct,eff*Ac",null,null,"Fcr =",{"$f":"+B383*B384*B385*B386","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,null,{"$f":"+'C III-V'!B12","v":4.2000010999999997},{"$f":"+'C III-V'!C12","v":1.2},{"$f":"IF($P$377+7*$R$53+0.1>$P$362,-2,$P$377+7*$R$53)","v":-2},{"$f":"IF(M569=\"\",-1,IF(P384=0,0,$E$544-0.03))","v":1.1099999999999999},0,"Ukupno:","kom",{"$f":"SUM(U374:U383)","v":{"$error":"#VALUE!"}},-2,-5,0,{"$error":"#VALUE!"},{"$f":"IF(Y384=0,0,Z383)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AC384=0,0,IF($H$54=\"šipka\",AB383+$R$59*1/$F$56,0))","v":{"$error":"#VALUE!"}},-5,0,-2,-5,0]
["fct,eff =",0.25,"Fcr,eff = b*2,5*(h-d)*fct,eff",null,null,"Fcr,eff =",{"$f":"+B369*2.5*(B370-B372)*B385","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,null,{"$f":"+'C III-V'!B13","v":4.2000010999999997},{"$f":"+'C III-V'!C13","v":1.2},{"$f":"IF(P384+8*$R$53<$P$362,-2,P383-8*$R$53)","v":-2},{"$f":"IF(M569=\"\",-1,IF(P385=0,0,$E$544-0.03))","v":1.1099999999999999},0,null,null,null,-2,{"$f":"IF(IF(W384-$R$59<$E$52,-5,W384-$R$59)>E79,IF(W384-$R$59<$E$52,-5,W384-$R$59),IF(IF(W384-$R$59<$E$52,-5,W384-$R$59)<E79+E81,IF(W384-$R$59<$E$52,-5,W384-$R$59),-5))","v":-5},0,{"$f":"IF(G78=0,-2,F555+0.04)","v":{"$error":"#VALUE!"}},{"$f":"IF(Y385=0,0,+Z377)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},-5,0,-2,-5,0]
["Ac =",{"$f":"B369*B372","v":{"$error":"#VALUE!"}},"cm2",null,null,"As =",{"$f":"IF(G383-0.4*G385<0,0,SQRT(C375*G385*(G383-0.4*G385)/(3.6*20000*C382*B385)))","v":{"$error":"#VALUE!"}},"cm2",null,null,null,null,null,{"$f":"+'C III-V'!B14","v":4.9000021999999994},{"$f":"+'C III-V'!C14","v":1.2},"Ukupno:","kom",{"$f":"SUM(R376:R385)","v":3},"Razdjelna dole desno R1dd do R10dd",null,null,-2,{"$f":"IF(W385-$R$59<$E$52,-5,W385-$R$59)","v":-5},0,null,"kom",{"$f":"SUM(AA377:AA385)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},-5,0,-2,-5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B15","v":4.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5},"Razdjelna gore desno          Rh1 do Rh 12",null,null,null,null,null,-2,-5,0,{"$f":"+Y377","v":{"$error":"#VALUE!"}},{"$f":"+Z377","v":3.37},null,{"$error":"#VALUE!"},-5,0,-2,-5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+N374","v":2},{"$f":"+O374","v":0.12820515121628623},null,null,null,{"$f":"IF($H$50=\"mreža\",0,IF(P365=-2,-2,IF(P365+$R$53>$S$398-0.15,-2,P365+$R$53)))","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!F41='Unos podataka'!G40,Q365,IF(S388=0,0,Q365+$R$56*TAN($F$217*PI()/180)))","v":{"$error":"#VALUE!"}},{"$f":"+IF(S388=-2,0,1)","v":{"$error":"#VALUE!"}},-2,-5,0,{"$f":"+K482","v":{"$error":"#VALUE!"}},{"$f":"+L482","v":3.2},0,{"$error":"#VALUE!"},-5,0,-2,-5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(M569=\"\",\"\",S369)","v":4.8350021999999999},{"$f":"IF(M569=\"\",\"\",+T369)","v":0.85},null,null,null,{"$f":"IF($H$50=\"mreža\",0,IF(S388=-2,-2,IF(S388+$R$53>$S$398-0.15,-2,S388+$R$53)))","v":{"$error":"#VALUE!"}},{"$f":"IF(S389=0,0,T388+$R$56*TAN($F$217*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"+IF(S389=-2,0,1)","v":{"$error":"#VALUE!"}},-2,-5,0,{"$f":"Y388","v":{"$error":"#VALUE!"}},{"$f":"+Z388","v":3.2},0,{"$error":"#VALUE!"},-5,0,-2,-5,0]
[{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"PRESJEK:\")","v":"PRESJEK:"},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"KONZOLA- ZID\")","v":"KONZOLA- ZID"},null,null,null,{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"Glavna armatura - u gornjoj zoni konzole.  Poz. 10\")","v":"Glavna armatura - u gornjoj zoni konzole.  Poz. 10"},null,null,null,null,null,null,null,{"$f":"+IF(M569=\"\",\"\",N389+0.5)","v":5.3350021999999999},{"$f":"+O389","v":0.85},{"$f":"+IF(P391-$R$53<$P$364,-2,P391-$R$53)","v":-2},{"$f":"IF(P390=0,0,IF($H$50=\"mreža\",0,Q364))","v":1.1099999999999999},{"$f":"+IF(P390<=-2,0,1)","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+IF(S390<=0,0,1)","v":{"$error":"#VALUE!"}},-2,-5,0,{"$f":"IF(Z390=0,-2,Y389+$R$68*TAN('C III-V'!$AC$35*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"IF(Z389-$R$68<$G$557,0,(Z389-$R$68))","v":2.8000000000000003},{"$f":"IF(Z390<$E$52,0,IF(Y390=0,0,1))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},-5,0,-2,-5,0]
[{"$f":"+IF(A390=\"\",\"\",\"MG  =\")","v":"MG  ="},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",-S45)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"kNm/m'\")","v":"kNm/m'"},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"NG =\")","v":"NG ="},{"$f":"IF(D391=\"\",\"\",+AP54)","v":{"$error":"#VALUE!"}},{"$f":"+IF(E391=\"\",\"\",\"kN/m'\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"IF('Unos podataka'!O48=\"\",2+E61-B315/100,-5)","v":4.8500021999999996},{"$f":"+(E52-E51+0.2)","v":0.7},-2,{"$f":"IF(P391=0,0,IF($H$50=\"mreža\",0,Q390))","v":1.1099999999999999},0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},-2,-5,0,{"$f":"IF(Z391=0,-2,Y390+$R$68*TAN('C III-V'!$AC$35*PI()/180))","v":{"$error":"#VALUE!"}},2.4000000000000004,{"$f":"IF(Z391<$E$52,0,IF(Y391=0,0,1))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},-5,0,-2,-5,0]
[{"$f":"+IF(A391=\"\",\"\",\"MQ  =\")","v":"MQ  ="},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",0)","v":0},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"kNm/m'\")","v":"kNm/m'"},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"NQ =\")","v":"NQ ="},{"$f":"+IF(D392=\"\",\"\",0)","v":0},{"$f":"+F391","v":{"$error":"#VALUE!"}},null,{"$f":"+I53","v":37},null,null,null,null,null,{"$f":"IF('Unos podataka'!O48=\"\",+N391+0.6,-5)","v":5.4500021999999992},{"$f":"+O391","v":0.7},-2,1.1099999999999999,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},-2,-5,0,{"$f":"IF(Z392=0,-2,Y391+$R$68*TAN('C III-V'!$AC$35*PI()/180))","v":{"$error":"#VALUE!"}},2.0000000000000004,{"$f":"IF(Z392<$E$52,0,IF(Y392=0,0,1))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},-5,0,-2,-5,0]
[{"$f":"+IF(A391=\"\",\"\",\"MEd =\")","v":"MEd ="},{"$f":"IF(A391=\"\",\"\",IF($E$44=0,B391*$J$44+B392*$J$45,B391*1+B392*1))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"kNm/m'\")","v":"kNm/m'"},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\" NEd=\")","v":" NEd="},{"$f":"IF(A391=\"\",\"\",IF(E44=0,+E391*J44,+E391))","v":{"$error":"#VALUE!"}},{"$f":"+F392","v":{"$error":"#VALUE!"}},{"$f":"+IF($I$53<=45,0.296,0.252)","v":0.29599999999999999},null,null,560,null,null,null,{"$f":"IF(M569=\"\",-1,2+(Q369-O393)*'Unos podataka'!G49/(Q369-Q373)+0.05)","v":2.0499999999999998},{"$f":"IF(M569=\"\",-1,O394)","v":0.48},-2,1.1099999999999999,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},-2,-5,0,{"$f":"IF(Z393=0,-2,Y392+$R$68*TAN('C III-V'!$AC$35*PI()/180))","v":{"$error":"#VALUE!"}},1.6000000000000005,0,{"$error":"#VALUE!"},-5,0,-2,-5,0]
[{"$f":"+IF(A391=\"\",\"\",\"MEds=\")","v":"MEds="},{"$f":"IF(B393=\"\",\"\",IF(B393>0,B393-E393*(B399-B397/2)/100,B393+E393*(B399-B397/2)/100))","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!G57=\"\",\"\",+IF(B394<E394,\"kNm/m'    <\",\"kNm/m'\"))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\" MRd,lim=\")","v":" MRd,lim="},{"$f":"IF(D394=\"\",\"\",0.296*G397*B396*B399*B399/100)","v":314.5},{"$f":"+F393","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"1.5","v":1.5},{"$f":"IF(M569=\"\",-1,0.4*E52)","v":0.48},-2,1.1099999999999999,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},-2,-5,0,{"$f":"IF(Z394=0,-2,Y393+$R$68*TAN('C III-V'!$AC$35*PI()/180))","v":{"$error":"#VALUE!"}},1.2000000000000006,{"$f":"IF(Z394<$E$52,0,IF(Y394=0,0,0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},-5,0,-2,-5,0]
[{"$f":"IF('Unos podataka'!G57=\"\",\"\",+IF(G78=0,0.000001,100))","v":100},{"$f":"IF('Unos podataka'!G57=\"\",\"\",ABS(IF(B393>0,B393-E393*((B397/2/100-B398/100)),B393+E393*((B397/2/100-B398/100)))))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,221,null,null,null,null,{"$f":"IF(M569=\"\",\"\",2+E59+E55/2)","v":3.8000000999999997},{"$f":"IF(M569=\"\",-2,+I560)","v":1.1399999999999999},-2,1.1099999999999999,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},-2,-5,0,{"$f":"IF(Z395=0,-2,Y394+$R$68*TAN('C III-V'!$AC$35*PI()/180))","v":-2},0,{"$f":"IF(Z395<$E$52,0,IF(Y395=0,0,1))","v":0},{"$error":"#VALUE!"},-5,0,-2,-5,0]
[{"$f":"+IF(A391=\"\",\"\",\"b =\")","v":"b ="},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",100)","v":100},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"cm\")","v":"cm"},{"$f":"IF(A390=\"\",\"\",IF(E396<0.096,-17900.704*E396*E396*E396*E396*E396+5359.131*E396*E396*E396*E396-610.514*E396*E396*E396+31.533*E396*E396-1.242*E396+0.998,-1.60447*E396*E396-0.23713*E396+0.97269))","v":{"$error":"#VALUE!"}},{"$f":"IF(B397=\"\",\"\",+ABS(B395*100/(B396*B399*B399*G397)))","v":{"$error":"#VALUE!"}},{"$f":"+IF(G396=\"\",\"\",\"fyd =\")","v":"fyd ="},{"$f":"IF('Unos podataka'!G57=\"\",\"\",G369)","v":43.478260869565219},{"$f":"+IF(G396=0,\"\",\"kN/cm²\")","v":"kN/cm²"},"es1,lim(%o)=",{"$f":"+IF(J405-I395>0,J405-I395,\"\")","v":""},null,null,null,{"$f":"+N395-0.8","v":3.0000000999999994},{"$f":"IF(M569=\"\",-2,+O395+0.5)","v":1.64},-2,1.1099999999999999,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},-2,-5,0,{"$f":"IF(Z396=0,-2,Y395+$R$68*TAN('C III-V'!$AC$35*PI()/180))","v":-2},0,0,{"$error":"#VALUE!"},-5,0,-2,-5,0]
[{"$f":"+IF(A391=\"\",\"\",\"h =\")","v":"h ="},{"$f":"IF('Unos podataka'!G57=\"\",\"\",C77*100)","v":30},{"$f":"+IF($A$9=\"\",\"\",\"cm\")","v":"cm"},null,null,{"$f":"+IF(G397=\"\",\"\",\"fcd =\")","v":"fcd ="},{"$f":"IF('Unos podataka'!G57=\"\",\"\",G370)","v":1.7},{"$f":"+IF(G397=0,\"\",\"kN/cm²\")","v":"kN/cm²"},null,{"$f":"+IF($I$49<=60,4.28,IF($I$49=67,5.76,IF($I$49=75,5.39,IF($I$49=85,5.01,IF($I$49=95,4.83,4.83)))))","v":4.28},null,null,null,{"$f":"IF(M569=\"\",\"\",(B547+B548)/2+0.04)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",-2,(C547+C548)/2)","v":{"$error":"#VALUE!"}},-2,1.1099999999999999,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},-2,-5,0,{"$f":"IF(Z397=0,-2,Y396+$R$68*TAN('C III-V'!$AC$35*PI()/180))","v":-2},0,0,{"$error":"#VALUE!"},-5,0,-2,-5,0]
[{"$f":"+IF(A391=\"\",\"\",\"a =\")","v":"a ="},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",+Q58*100)","v":5},{"$f":"+IF($A$9=\"\",\"\",\"cm\")","v":"cm"},null,null,{"$f":"+IF(G398=\"\",\"\",\"µSd=\")","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!G57=\"\",\"\",+E396)","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(G396=\"\",\"\",\"ζlim=\")","v":"ζlim="},null,null,null,null,{"$f":"+N397","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",-2,+O397+0.2)","v":{"$error":"#VALUE!"}},4.4350021999999996,1.1099999999999999,1,{"$f":"S399-R56","v":4.4400021999999995},{"$f":"T399-$R$56*TAN($F$217*PI()/180+0.01)","v":0.51775032994672077},1,-2,-5,0,{"$f":"IF(Z398=0,-2,Y397+$R$68*TAN('C III-V'!$AC$35*PI()/180))","v":-2},0,0,{"$error":"#VALUE!"},-5,0,-2,-5,0]
[{"$f":"+IF(A391=\"\",\"\",\"d =\")","v":"d ="},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",+A401)","v":25},{"$f":"+IF($A$9=\"\",\"\",\"cm\")","v":"cm"},null,null,{"$f":"+IF(G399=\"\",\"\",\"ζ =\")","v":{"$error":"#VALUE!"}},{"$f":"IF(B396=\"\",\"\",150376*G398^6-62291*G398^5+10258*G398^4-854.43*G398^3+36.991*G398^2-1.213*G398+0.9978)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+IF($I$49<=60,0.45,0.35)","v":0.45},null,null,null,{"$f":"P371","v":2.0700000000000003},{"$f":"+Q371","v":0.6},{"$f":"S367","v":4.8350021999999999},1.1099999999999999,null,{"$f":"+F551-0.01","v":4.8400021999999998},{"$f":"+G551+0.01","v":0.57310345350772507},null,-2,-5,0,{"$f":"IF(Z399=0,-2,Y398+$R$68*TAN('C III-V'!$AC$35*PI()/180))","v":-2},0,0,{"$error":"#VALUE!"},-5,0,-2,-5,0]
[{"$f":"IF('Unos podataka'!G57=\"\",\"\",IF(G78=0,0.000001,B423))","v":5},null,null,null,{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"As₁,min≥\")","v":"As₁,min≥"},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",0.0015*B396*B399)","v":3.75},{"$f":"+IF($G$396=0,\"\",\"cm²\")","v":"cm²"},null,{"$f":"+IF(G396=\"\",\"\",785)","v":785},null,null,null,null,{"$f":"+N399-0.5","v":1.5700000000000003},{"$f":"+O399","v":0.6},null,null,null,null,"kom",{"$f":"SUM(U387:U399)","v":{"$error":"#VALUE!"}},-2,-5,0,{"$f":"IF(Z400=0,-2,Y399+$R$68*TAN('C III-V'!$AC$35*PI()/180))","v":-2},0,0,{"$error":"#VALUE!"},-5,0,-2,-5,0]
[{"$f":"IF('Unos podataka'!G57=\"\",\"\",IF((B397-A400)<0,0.000001,B397-A400))","v":25},null,null,null,{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"As₁,max=\")","v":"As₁,max="},{"$f":"IF('Unos podataka'!G57=\"\",\"\",0.31*A395*A401*G397/G396)","v":30.302499999999998},{"$f":"+IF($G$396=0,\"\",\"cm²\")","v":"cm²"},null,null,null,null,null,null,{"$f":"+B546","v":4.1600000999999995},{"$f":"+C546","v":1.2},null,null,null,"Ukupno:","kom",{"$f":"U372+U384+U400","v":{"$error":"#VALUE!"}},-2,-5,0,{"$f":"IF(Z401=0,-2,Y400+$R$68*TAN('C III-V'!$AC$35*PI()/180))","v":-2},0,0,{"$error":"#VALUE!"},-5,0,-2,-5,0]
[null,null,null,null,{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"As₁=\")","v":"As₁="},{"$f":"IF('Unos podataka'!G57=\"\",\"\",+B395*100/(G396*G399*A401))","v":{"$error":"#VALUE!"}},{"$f":"+IF($G$396=0,\"\",\"cm²\")","v":"cm²"},null,null,null,null,null,null,{"$f":"+N401+0.8","v":4.9600000999999994},{"$f":"+O401+0.8","v":2},null,"kom",{"$f":"SUM(R389:R401)","v":1},"Ukupno:","kom",null,-2,-5,0,{"$f":"IF(Z402=0,-2,Y401+$R$68*TAN('C III-V'!$AC$35*PI()/180))","v":-2},0,0,{"$error":"#VALUE!"},-5,0,-2,-5,0]
[{"$f":"IF('Unos podataka'!G57=\"\",\"\",IF(H60=\"mreža\",\"\",\"odabrano:\"))","v":"odabrano:"},{"$f":"IF('Unos podataka'!G57=\"\",\"\",IF(H60=\"šipka\",\"   f\",\"\"))","v":"   f"},{"$f":"IF('Unos podataka'!G57=\"\",\"\",IF(H60=\"mreža\",\"\",O67))","v":12},null,{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"mjerodavno: As₁=\")","v":"mjerodavno: As₁="},{"$f":"IF(B391=\"\",\"\",IF('Unos podataka'!$O$48=\"\",MAX(F400,F402,G411),MAX(F400,F402,G411)))","v":{"$error":"#VALUE!"}},{"$f":"+IF($G$396=0,\"\",\"cm²\")","v":"cm²"},null,null,null,null,null,null,{"$f":"IF('Unos podataka'!$O$48=\"\",+IF(M569=\"\",\"\",P362),-5)","v":3.4800010999999995},{"$f":"IF(N403=\"\",-2,+Q362)","v":1.1099999999999999},"Ukupno:","kom",{"$f":"R374+R386+R402","v":9},{"$f":"+N591","v":3.4500010999999997},{"$f":"+O591","v":1.2},"y",-2,-5,0,{"$f":"IF(Z403=0,-2,Y402+$R$68*TAN('C III-V'!$AC$35*PI()/180))","v":-2},0,0,{"$error":"#VALUE!"},-5,0,-2,-5,0]
[{"$f":"IF('Unos podataka'!G57=\"\",\"\",IF(H60=\"mreža\",\"\",\"potrebno:\"))","v":"potrebno:"},{"$f":"IF(A77=\"\",\"\",IF($M$569=1,IF($H$60=\"mreža\",\"\",TRUNC(F403/(PI()*C403*C403/400))+1),TRUNC(F402/(PI()*C403*C403/400))+1))","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!G57=\"\",\"\",IF(H60=\"mreža\",\"\",\"kom/m'\"))","v":"kom/m'"},null,{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"A₁=\")","v":"A₁="},{"$f":"IF('Unos podataka'!G57=\"\",\"\",IF(H60=\"mreža\",\"\",B405*C403*C403*PI()/400))","v":{"$error":"#VALUE!"}},{"$f":"+IF($G$396=0,\"\",\"cm²\")","v":"cm²"},null,null,null,null,null,null,{"$f":"IF(M569=\"\",-5,+N407)","v":1.5},{"$f":"IF(M569=\"\",-2,+E52/2+0.2)","v":0.8},null,null,{"$f":"+R403+R366+U364","v":{"$error":"#VALUE!"}},{"$f":"+N592","v":{"$error":"#VALUE!"}},{"$f":"+O592","v":-0.05},{"$f":"+Z377","v":3.37},-2,-5,0,"razdjelna konzola uz lice zida","kom",{"$f":"SUM(AA388:AA399)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},-5,0,-2,-5,0,"Ukupnpo armature"]
[{"$f":"IF('Unos podataka'!G57=\"\",\"\",IF(H60=\"mreža\",\"\",\"odabrano:\"))","v":"odabrano:"},{"$f":"IF(B404=\"\",\"\",+IF(B404<=5,5,IF(B404<=10,10,B404)))","v":{"$error":"#VALUE!"}},{"$f":"+C404","v":"kom/m'"},null,{"$f":"IF(H60=\"mreža\",\"odabrano:\",\"\")","v":""},{"$f":"IF('Unos podataka'!G57=\"\",\"\",IF(H60=\"mreža\",\"mreža Q\",\"\"))","v":""},{"$f":"IF('Unos podataka'!G57=\"\",\"\",+IF(I180=\"šipka\",\"\",IF(O431<5.03,503,IF(O431<=7.85,785,\"785   + Q \"))))","v":""},{"$f":"IF('Unos podataka'!G57=\"\",\"\",IF(I180=\"šipka\",\"\",IF(P431<0,\"\",IF(P431<3.35,335,IF(P431<5.03,503,IF(P431<7.85,785,\"7,85  +\"))))))","v":""},null,null,null,null,null,{"$f":"+IF(M569=\"\",-5,P373)","v":2.0700000000000003},{"$f":"+IF(M569=\"\",-2,Q373)","v":0.22682583433163006},null,null,null,null,null,"x",-2,-5,0,null,null,{"$f":"+AA404+AA386","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},-5,0,-2,-5,0,{"$f":"+AG416","v":{"$error":"#VALUE!"}},"AG398"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M569=1,+Q371,-1)","v":0.6},null,null,null,{"$f":"-(T404-T403)/(S404-S403)","v":{"$error":"#VALUE!"}},{"$f":"S406*S404+T404","v":{"$error":"#VALUE!"}},{"$f":"IF(S403=S404,S403+0.03,(T406-U404)/S406+0.03)","v":{"$error":"#VALUE!"}},-2,-5,0,"Poz. 10",null,null,{"$error":"#VALUE!"},-5,0,-2,-5,{"$f":"+IF(AF406=-5,0,1)","v":0},{"$f":"+R374","v":5},"R356"]
[null,{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"Ograničenje pukotina:     wk=\")","v":"Ograničenje pukotina:     wk="},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",+I56)","v":0.3},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"mm\")","v":"mm"},null,null,null,null,null,null,null,null,null,{"$f":"1.5","v":1.5},{"$f":"IF(M569=1,+O404,-1)","v":0.8},null,null,null,{"$f":"+R403+U402+X417","v":9},null,null,-2,-5,0,{"$f":"+(Y391+Y392)/2","v":{"$error":"#VALUE!"}},{"$f":"+(Z391+Z392)/2","v":2.2000000000000002},null,{"$error":"#VALUE!"},-5,0,-2,-5,{"$f":"+IF(AF407=-5,0,1)","v":0},{"$f":"+R386","v":3},"R368"]
[{"$f":"+IF(G396=\"\",\"\",\"kc=\")","v":"kc="},{"$f":"+IF(G396=\"\",\"\",0.4)","v":0.4},{"$f":"+IF(G396=\"\",\"\",\"Fs= MEds/z+Ned\")","v":"Fs= MEds/z+Ned"},null,null,{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"Fs  =\")","v":"Fs  ="},{"$f":"IF(F408=\"\",\"\",ABS(IF('Unos podataka'!G57=\"\",\"\",(((B391/$J$44)+(B392*0.2/$J$45)-(E391/$J$44+E392*0.2/$J$45))/(0.9*B399/100))+(E391/$J$44+E392/$J$45))))","v":{"$error":"#VALUE!"}},{"$f":"+IF($A$9=\"\",\"\",\"kN\")","v":"kN"},null,null,null,null,null,null,null,null,null,null,null,null,null,-2,-5,0,{"$f":"+Y407+1","v":{"$error":"#VALUE!"}},{"$f":"+Z407","v":2.2000000000000002},null,{"$error":"#VALUE!"},-5,0,-2,-5,{"$f":"+IF(AF408=-5,0,1)","v":0},{"$f":"+R402","v":1},"R384"]
[{"$f":"+IF(G396=\"\",\"\",\"k =\")","v":"k ="},{"$f":"+IF(G396=\"\",\"\",0.8)","v":0.8},{"$f":"+IF(G396=\"\",\"\",\"Fcr = kc*k*fct,eff*Ac\")","v":"Fcr = kc*k*fct,eff*Ac"},null,null,{"$f":"+IF(G409=\"\",\"\",\"Fcr =\")","v":"Fcr ="},{"$f":"IF('Unos podataka'!G57=\"\",\"\",B408*B409*B410*B411)","v":200.00000000000003},{"$f":"+IF($A$9=\"\",\"\",\"kN\")","v":"kN"},null,null,null,null,null,"Poz. 1",null,null,null,null,null,null,null,null,null,0,null,null,null,{"$error":"#VALUE!"},-5,0,{"$f":"2+E59+B290/100+0.03","v":3.4800000999999994},{"$f":"+E52","v":1.2},{"$f":"+IF(AF409=-5,0,1)","v":1},{"$f":"+U372","v":3},"U356"]
[{"$f":"+IF(G396=\"\",\"\",\"fct,eff =\")","v":"fct,eff ="},{"$f":"+IF(G396=\"\",\"\",0.25)","v":0.25},{"$f":"+IF(G396=\"\",\"\",\"Fcr,eff = b*2,5*(h-d)*fct,eff\")","v":"Fcr,eff = b*2,5*(h-d)*fct,eff"},null,null,{"$f":"+IF(F409=\"\",\"\",\"Fcr,eff =\")","v":"Fcr,eff ="},{"$f":"IF('Unos podataka'!G57=\"\",\"\",A395*2.5*(B397-A401)*B410)","v":312.5},{"$f":"+IF($A$9=\"\",\"\",\"kN\")","v":"kN"},null,null,null,null,null,{"$f":"IF(M569=\"\",\"\",(+S377+P363)/2)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",\"\",+(T377+Q363)/2)","v":{"$error":"#VALUE!"}},null,null,null,"temelj gore lijevo","temelj dole lijevo","temelj desno","temelj gore desno","temelj dole desno",0,null,null,null,{"$error":"#VALUE!"},-5,0,null,null,null,{"$f":"+U400","v":{"$error":"#VALUE!"}},"U384"]
[{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"Ac =\")","v":"Ac ="},{"$f":"IF('Unos podataka'!G57=\"\",\"\",+A395*A401)","v":2500},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"cm²\")","v":"cm²"},null,null,{"$f":"+IF(F410=\"\",\"\",\"As =\")","v":"As ="},{"$f":"IF('Unos podataka'!G57=\"\",\"\",IF(G408-0.4*G410<0,0,SQRT(C403*G410*(G408-0.4*G410)/(3.6*20000*C407*B410))))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"cm²\")","v":"cm²"},null,null,null,null,null,{"$f":"IF(M569=\"\",\"\",+N410-0.3)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",\"\",+O410+0.25)","v":{"$error":"#VALUE!"}},null,"Specifikacija poz 6",null,"R368","U368","U356","R384","U384",null,null,null,null,null,0,0,null,null,null,{"$f":"+U586","v":{"$error":"#VALUE!"}},"U570"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," ankeri","temelj vertik. lijevo",{"$f":"+R386","v":3},{"$f":"+U384","v":{"$error":"#VALUE!"}},{"$f":"+U372","v":3},{"$f":"+R402","v":1},{"$f":"+U400","v":{"$error":"#VALUE!"}},"na zidu prema tlu","konzola gore","konzola dole","konzola uz lice zida","Ukupno:","temelj dole desno","na zidu prema tlu",null,null,null,{"$f":"+U384","v":{"$error":"#VALUE!"}},"U368"]
[null,{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"Dimenzioniranje na poprečnu silu:\")","v":"Dimenzioniranje na poprečnu silu:"},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"VEd=\")","v":"VEd="},{"$f":"IF('Unos podataka'!G57=\"\",\"\",+AM56)","v":{"$error":"#VALUE!"}},{"$f":"IF(E79=\"\",\"\",IF(D413>G413,\"kN/m'  >  \",\"kN/m'    < \"))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Unos podataka'!G57=\"\",\"\",\"VRd,c=\")","v":"VRd,c="},{"$f":"IF('Unos podataka'!G57=\"\",\"\",+AM82)","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!G57=\"\",\"\",IF(G413>D413,\"kN/m'    (Zadovoljava)\",\"kN/m'    (NE Zadovoljava)\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"U570","R356",null,null,null,null,null,"AG398","AA368","L473","AA386",null,"U384","AG398",null,null,null,{"$f":"SUM(AH405:AH412)","v":{"$error":"#VALUE!"}},"kom"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U586","v":{"$error":"#VALUE!"}},{"$f":"+R374","v":5},"POZ. 6 na zidu tlo","POZ. 6 na licu zida","Poz. 3","Poz.4",null,{"$f":"+AG416","v":{"$error":"#VALUE!"}},{"$f":"+AA386","v":{"$error":"#VALUE!"}},{"$f":"+L491","v":{"$error":"#VALUE!"}},{"$f":"+AA404","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q414:AA414)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[{"$f":"+IF(A82=\"\",\"\",\"PRESJEK III-III:\")","v":"PRESJEK III-III:"},{"$f":"+IF(A83=\"\",\"\",\"SPOJ KONTRAFORA - TEMELJ\")","v":"SPOJ KONTRAFORA - TEMELJ"},null,null,null,{"$f":"IF(A82=\"\",\"\",IF('Unos podataka'!O48=\"\",\"Armatura u Presjeku III-III  pokrivena sa Poz. 5,  Poz. 15 i Poz. 19\",\"Armatura nije potrebna\"))","v":"Armatura u Presjeku III-III  pokrivena sa Poz. 5,  Poz. 15 i Poz. 19"},null,null,null,null,null,null,null,null,null,null,"Pozicije armature kada je masivni zid",null,{"$f":"IF('Unos podataka'!O48=\"\",+P480,-5)","v":-3.1},{"$f":"IF('Unos podataka'!O48=\"\",H548,-5)","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!O48=\"\",+N393,-5)","v":2.0499999999999998},{"$f":"IF('Unos podataka'!O48=\"\",+N392,-5)","v":5.4500021999999992},null,null,null,null,null,null,0,0]
[{"$f":"+IF(A82=\"\",\"\",\"MG =\")","v":"MG ="},{"$f":"IF(A82=\"\",\"\",B308*$H$84)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Unos podataka'!AB1=\"\",\"\",\"kNm/kontr.   Ng\")","v":"kNm/kontr.   Ng"},{"$f":"+IF(A82=\"\",\"\",\"NG =\")","v":"NG ="},{"$f":"IF(A82=\"\",\"\",E308*$H$84)","v":{"$error":"#VALUE!"}},{"$f":"IF(A83=\"\",\"\",+IF('Unos podataka'!AB1=\"\",\"kN\",\"kN/kontrafori\"))","v":"kN/kontrafori"},null,null,null,null,null,null,null,null,null,null,"Poz 6 Uz temelj lijevo","Poz 6 Uz temelj desno",{"$f":"+IF(S415=\"\",\"\",Q480)","v":-4.8},{"$f":"IF(T415=\"\",\"\",+I549)","v":{"$error":"#VALUE!"}},{"$f":"+IF(U415=\"\",\"\",O393)","v":0.48},{"$f":"+IF(V415=\"\",\"\",O391)","v":0.7},null,null,null,null,null,null,null,null,null,"Poz. 6",{"$f":"SUM(AG377:AG415)","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(A416=\"\",\"\",\"MQ =\")","v":"MQ ="},{"$f":"IF(A82=\"\",\"\",B309*H84)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Unos podataka'!AB1=\"\",\"\",\"kNm/kontr.\")","v":"kNm/kontr."},{"$f":"+IF(D416=\"\",\"\",\"NQ =\")","v":"NQ ="},{"$f":"IF(A82=\"\",\"\",+IF('Unos podataka'!$AB$1=\"\",E309,E309*H84))","v":0},{"$f":"+F416","v":"kN/kontrafori"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Unos podataka'!$O$48=\"\",+N404,-5)","v":1.5},{"$f":"IF('Unos podataka'!$O$48=\"\",2+E61+1,-5)","v":5.9000021999999994},"Površina presjeka žica (cm2/m')",null,"Duljina mreže    (mm)","Masa     (kg/m2)","Masa kg/kom   (toler. 1%)",null,null,null,null,null,null,null,null,null,{"$f":"SUM(AG377:AG413)","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(A417=\"\",\"\",\"MEd=\")","v":"MEd="},{"$f":"IF(A82=\"\",\"\",IF($E$44=0,B416*$J$44+B417*$J$45,B416*1+B417*1))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Unos podataka'!AB1=\"\",\"\",\"kNm/kontr.\")","v":"kNm/kontr."},{"$f":"+IF(D417=\"\",\"\",\"NEd=\")","v":"NEd="},{"$f":"IF(A82=\"\",\"\",+IF(H84=\"\",E310,+E310*H84))","v":{"$error":"#VALUE!"}},{"$f":"+F417","v":"kN/kontrafori"},null,{"$f":"+IF($I$53<=45,0.296,0.252)","v":0.29599999999999999},null,null,null,null,null,"      UZDUŽNO NOSIVE MREŽE   (R mreže)     š=2150 mm",null,null,{"$f":"+O404","v":0.8},{"$f":"+F559","v":0.96}]
[{"$f":"+IF(A418=\"\",\"\",\"MEds=\")","v":"MEds="},{"$f":"IF(A82=\"\",\"\",IF(B418=\"\",\"\",B311*H84))","v":{"$error":"#VALUE!"}},{"$f":"IF(A82=\"\",\"\",+IF(B419<E419,\"kNm/kontr.<\",\"kNm/kontr.\"))","v":{"$error":"#VALUE!"}},{"$f":"+IF(D418=\"\",\"\",\"MRd,lim=\")","v":"MRd,lim="},{"$f":"IF(E418=\"\",\"\",+IF('Unos podataka'!$AB$1=\"\",E311,H418*G422*B421*B424*B424/100))","v":{"$error":"#VALUE!"}},{"$f":"+F418","v":"kN/kontrafori"},null,null,null,null,null,null,null,"Oznaka mreže","Promjer žica (mm)",null,"Razmak žica (mm)",null,"uzdužnih","poprečnih"]
[null,{"$f":"+ABS(B419)","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(A419=\"\",\"\",\"b =\")","v":"b ="},{"$f":"IF(A82=\"\",\"\",+IF('Unos podataka'!AB1=\"\",+B313,'Unos podataka'!AB6*100))","v":25},{"$f":"+IF(A83=\"\",\"\",\"cm \")","v":"cm "},null,{"$f":"+ABS(B420*100/(B421*B424*B424*G422))","v":{"$error":"#VALUE!"}},{"$f":"+IF(A82=\"\",\"\",\"fyd =\")","v":"fyd ="},{"$f":"IF(A82=\"\",\"\",50/'Unos podataka'!L25)","v":43.478260869565219},{"$f":"+IF(A83=\"\",\"\",\"kN/cm²\")","v":"kN/cm²"},null,null,null,null,null,null,"uzdužne","poprečne","uzdužno","poprečno",1.31,0.5,5000,1.52,16.34]
[{"$f":"+IF(A421=\"\",\"\",\"hııı=\")","v":"hııı="},{"$f":"IF(B421=\"\",\"\",+IF('Unos podataka'!AB1=\"\",B314,('Unos podataka'!I53-'Unos podataka'!I50)*100))","v":189.99990999999997},{"$f":"+C421","v":"cm "},null,null,{"$f":"+IF(F421=\"\",\"\",\"fcd =\")","v":"fcd ="},{"$f":"IF(G421=\"\",\"\",+G397)","v":1.7},{"$f":"+H421","v":"kN/cm²"},null,null,null,null,null,null,"D","d","a","t",1.39,0.55000000000000004,5000,1.53,16.829999999999998]
[{"$f":"+IF(A422=\"\",\"\",\"a =\")","v":"a ="},{"$f":"+IF(B422=\"\",\"\",Q58*100)","v":5},{"$f":"+C422","v":"cm "},null,null,{"$f":"+IF(F422=\"\",\"\",\"µSd=\")","v":"µSd="},{"$f":"IF(G422=\"\",\"\",IF(E421=\"\",0,E421))","v":{"$error":"#VALUE!"}},null,null,{"$f":"+IF($I$49<=60,0.296,IF($I$49=67,0.224,IF($I$49=75,0.211,0.195)))","v":0.29599999999999999},null,null,null,"R-131",5,4,150,250,1.66,0.55000000000000004,5000,1.74,19.14]
[{"$f":"+IF(A423=\"\",\"\",\"d =\")","v":"d ="},{"$f":"IF(B423=\"\",\"\",+IF('Unos podataka'!AB1=\"\",B316,B422-B423))","v":184.99990999999997},{"$f":"+C423","v":"cm "},null,null,{"$f":"+IF(F423=\"\",\"\",\"ζ =\")","v":"ζ ="},{"$f":"IF(G423=\"\",\"\",150376*G423^6-62291*G423^5+10258*G423^4-854.43*G423^3+36.991*G423^2-1.213*G423+0.9978)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+IF($I$49<=60,0.45,0.35)","v":0.45},null,null,null,"R-139",4.2,4.2,100,250,1.96,0.55000000000000004,5000,1.98,21.89]
[null,null,null,null,{"$f":"+IF(A82=\"\",\"\",\" As1,min≥\")","v":" As1,min≥"},{"$f":"IF(A82=\"\",\"\",+IF('Unos podataka'!$AB$1=\"\",+F317,0.0015*B421*B424))","v":6.9374966249999988},{"$f":"+IF(A82=\"\",\"\",\"cm²\")","v":"cm²"},null,null,{"$f":"+IF($I$53<=60,0.813,IF($I$53=67,0.863,IF($I$53=75,0.868,IF($I$53=85,0.873,IF($I$53=95,0.8758,0.8765)))))","v":0.81299999999999994},null,null,null,"R-166",4.5999999999999996,4.2,100,250,2.21,0.66,6000,2.27,30.57]
[null,{"$f":"+IF(F425>F427,F425,F427)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+IF(E425=\"\",\"\",\"As1,max=\")","v":"As1,max="},{"$f":"IF(F425=\"\",\"\",IF('Unos podataka'!$AB$1=\"\",+F318,0.31*B421*B424*G422/G421))","v":56.059597727749988},{"$f":"+G425","v":"cm²"},null,null,null,null,null,null,"R-196",5,4.2,100,250,2.38,0.55000000000000004,6000,2.31,30.61]
[null,{"$f":"+IF(B429<B322,5,IF(B429-B322<5,5,B429-B322))","v":{"$error":"#VALUE!"}},null,null,{"$f":"+IF(E426=\"\",\"\",\"As1=\")","v":"As1="},{"$f":"IF(F426=\"\",\"\",+IF('Unos podataka'!$AB$1=\"\",+F319,IF(B419<E419,ABS(ABS(B419)*100/(G421*G424*B424)-E418/G421),E419*100/(H418*B424*G421)+((B419+E419)*100)/((B424-B423)*G421)-E418/G421)))","v":{"$error":"#VALUE!"}},{"$f":"+G426","v":"cm²"},null,null,null,null,null,null,"R-221",6.5,4.2,150,250,2.83,0.55000000000000004,6000,2.66,35.229999999999997]
[{"$f":"+IF(A82=\"\",\"\",\"odabrano:\")","v":"odabrano:"},{"$f":"+IF(A82=\"\",\"\",\"f\")","v":"f"},{"$f":"IF(A82=\"\",\"\",+E729)","v":12},null,{"$f":"+IF(E427=\"\",\"\",\"mjerodavno: As1=\")","v":"mjerodavno: As1="},{"$f":"IF(F427=\"\",\"\",+MAX(F425,F427,G438))","v":{"$error":"#VALUE!"}},{"$f":"+G427","v":"cm²"},null,null,null,null,null,null,"R-238",5.5,4.2,100,250,3.35,0.78,6000,3.41,43.99]
[{"$f":"+IF(A428=\"\",\"\",\"potrebno:\")","v":"potrebno:"},{"$f":"IF(B428=\"\",\"\",IF(B419=0,0,IF(M569=1,+TRUNC(F428/(PI()*C428*C428/400)+1),+TRUNC(F427/(PI()*C428*C428/400)))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(A83=\"\",\"\",\"kom/rebru\")","v":"kom/rebru"},null,{"$f":"IF(E428=\"\",\"\",\"A₁=\")","v":"A₁="},{"$f":"IF(F428=\"\",\"\",+C428*C428*PI()*B430/400)","v":{"$error":"#VALUE!"}},{"$f":"+G428","v":"cm²"},null,null,null,null,null,null,"R-283",6,4.2,100,250,3.78,0.78,6000,3.77,48.63]
[{"$f":"+IF(A429=\"\",\"\",\"odabrano:\")","v":"odabrano:"},{"$f":"+B429","v":{"$error":"#VALUE!"}},{"$f":"+C429","v":"kom/rebru"},null,null,null,null,null,null,null,null,null,null,"R-335",8,5,150,250,3.85,0.78,6000,3.64,48.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"R-378",8.5,5,150,250,4.24,1.1299999999999999,6000,4.22,57.02]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"R-385",7,5,100,250,5.03,1.1299999999999999,6000,4.84,64.209999999999994]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"R-424",9,6,150,250,5.24,1.1299999999999999,6000,5.24,67.599999999999994]
[null,{"$f":"+IF(A82=\"\",\"\",\"Ograničenje pukotina:     wk=\")","v":"Ograničenje pukotina:     wk="},{"$f":"IF(A82=\"\",\"\",+I56)","v":0.3},{"$f":"+IF(A83=\"\",\"\",\"mm\")","v":"mm"},null,null,null,null,null,null,null,null,null,"R-503",8,6,100,250,6.36,1.1299999999999999,6000,5.88,78.069999999999993]
[{"$f":"+IF(A82=\"\",\"\",\"kc=\")","v":"kc="},{"$f":"+IF(A82=\"\",\"\",0.4)","v":0.4},{"$f":"+IF(C434=\"\",\"\",\"Fs= MEds/z+Ned\")","v":"Fs= MEds/z+Ned"},null,null,{"$f":"+IF(A82=\"\",\"\",\"Fs  =\")","v":"Fs  ="},{"$f":"IF(F435=\"\",\"\",ABS((((B416/$J$44)+(B417*0.5/$J$45)-(E416/$J$44+E417*0.5/$J$45))/(0.9*B424/100))+(E416/$J$44+E417/$J$45)))","v":{"$error":"#VALUE!"}},{"$f":"+IF(A83=\"\",\"\",\"kN\")","v":"kN"},null,null,null,null,null,"R-524",10,6,150,250,7.85,1.1299999999999999,6000,7.06,93.76]
[{"$f":"+IF(A435=\"\",\"\",\"k =\")","v":"k ="},{"$f":"+IF(B435=\"\",\"\",0.8)","v":0.8},{"$f":"+IF(C435=\"\",\"\",\"Fcr = kc*k*fct,eff*Ac\")","v":"Fcr = kc*k*fct,eff*Ac"},null,null,{"$f":"+IF(F435=\"\",\"\",\"Fcr =\")","v":"Fcr ="},{"$f":"IF(G435=\"\",\"\",+B435*B436*B437*B438)","v":{"$error":"#VALUE!"}},{"$f":"+H435","v":"kN"},null,null,null,null,null,"R-636",9,6,100,250]
[{"$f":"+IF(A436=\"\",\"\",\"fct,eff =\")","v":"fct,eff ="},{"$f":"IF(B436=\"\",\"\",0.25)","v":0.25},{"$f":"+IF(C436=\"\",\"\",\"Fcr,eff = b*2,5*(h-d)*fct,eff\")","v":"Fcr,eff = b*2,5*(h-d)*fct,eff"},null,null,{"$f":"+IF(F436=\"\",\"\",\"Fcr,eff =\")","v":"Fcr,eff ="},{"$f":"IF(G436=\"\",\"\",+B421*2.5*(B422-B424)*B437)","v":{"$error":"#VALUE!"}},{"$f":"+H436","v":"kN"},null,null,null,null,null,"R-785",10,6,100,250]
[{"$f":"+IF(A437=\"\",\"\",\"Ac =\")","v":"Ac ="},{"$f":"IF(B437=\"\",\"\",B421*B424)","v":4624.9977499999995},{"$f":"+IF(C437=\"\",\"\",\"cm²\")","v":"cm²"},null,null,{"$f":"+IF(F437=\"\",\"\",\"As =\")","v":"As ="},{"$f":"IF(G436=\"\",\"\",+IF(G435-0.4*G437<0,0,SQRT(C428*G437*(G435-0.4*G437)/(3.6*20000*C434*B437))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(A83=\"\",\"\",\"cm²\")","v":"cm²"},null,null,null,null,null,null,null,null,null,null,"Površina presjeka žica (cm2/m')",null,"Duljina mreže    (mm)","Masa     (kg/m2)","Masa kg/kom    (toler. 1%)"]
[null,{"$f":"+IF(A82=\"\",\"\",\"Dimenzioniranje na poprečnu silu:\")","v":"Dimenzioniranje na poprečnu silu:"},{"$f":"+IF(A82=\"\",\"\",\"VEd=\")","v":"VEd="},{"$f":"IF(C439=\"\",\"\",+IF(H84=\"\",D332,+AJ56))","v":{"$error":"#VALUE!"}},{"$f":"IF(C439=\"\",\"\",+IF(D439>G439,\"kN       > \",\"kN       < \"))","v":{"$error":"#VALUE!"}},{"$f":"+IF(F438=\"\",\"\",\"VRd,c=\")","v":"VRd,c="},{"$f":"IF(F439=\"\",\"\",IF(H84=\"\",G332,+AJ73))","v":{"$error":"#VALUE!"}},{"$f":"IF(A82=\"\",\"\",+IF(G439>D439,\"kN      (Zadovoljava)\",\"kN       (NE Zadovoljava)\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,"      MREŽE NOSIVE U DVA SMJERA   (Q mreže)   š=2150 mm"]
[{"$f":"+IF(A77=\"    KONZOLA\",\"\",IF(A82=\"\",\"     UKOLIKO NEMA KONZOLE I KONTRAFORA, NACRT ARMATURE MOŽE SE STAVITI NA  STRANICU 8\",\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"Oznaka mreže","Promjer žica  (mm)",null,"Razmak žica (mm)",null,"uzdužnih","poprečnih"]
[]
[null,null,null,null,null,null,null,null,3.5,null,null,null,null,null,"uzdužne","poprečne","uzdužno","poprečno",1.88,1.88,6000,3.05,33.44]
[null,null,null,null,null,null,null,null,5,11.8,null,null,null,null,"D","d","a","t",2.21,2.21,6000,3.6,39.47]
[null,null,null,null,null,null,null,null,0.2,11.5,null,null,null,"Q-188",6,6,150,{"$f":"+Q444","v":150},2.57,2.57,6000,4.16,45.61]
[null,null,null,null,null,null,null,null,{"$f":"7","v":7},12,null,null,null,"Q-221",6.5,6.5,150,150,2.83,2.83,6000,4.4400000000000004,49.68]
[null,null,null,null,null,null,null,null,null,0.1,null,null,null,"Q-257",7,7,150,150,3.35,3.35,6000,5.44,59.65,null,null,null,"Vrh zida","T2","T3","T4",null,"Vrh zida","T2","vrh temelja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Q-283",6,6,100,100,5.03,5.03,6000,7.9,88.49,null,null,"x=",{"$f":"+'Unos podataka'!$S$55-2","v":{"$error":"#VALUE!"}},-21.16,{"$f":"+L457","v":-15},{"$f":"+L458","v":-10},"x=",{"$f":"+AA447","v":{"$error":"#VALUE!"}},{"$f":"+AB447","v":-21.16},{"$f":"0-D83","v":-1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Q-335",8,8,150,150,6.86,6.86,6000,9.98,131.69999999999999,null,null,"Y=",{"$f":"+'C III-V'!C10+'Unos podataka'!F9","v":0},{"$f":"AA448-(AB447-AA447)*TAN(H20*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+M457","v":9.5},{"$f":"+M458","v":9},"Y=",{"$f":"+AA448","v":0},{"$f":"+AB448","v":{"$error":"#VALUE!"}},1.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Q-503",8,8,100,100,7.85,7.85,6000,12.34,138.18,null,null,"Y=",{"$f":"(AB448-AA448)/(AB447-AA447)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AA449*AA447+AA448","v":{"$error":"#VALUE!"}},"Jednadžba pravca proj. kosine od vrha","Y=",{"$f":"(AG448-AF448)/(AG447-AF447)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AF449*AF447+AF448","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Q-636",9,9,100,100,null,null,null,null,null,null,null,"Y=",{"$f":"-(AD448-AC448)/(AC447-AD447)","v":-0.1},"*x    +",{"$f":"-(AC447*AA450-AC448)","v":8},"Jednadžba pravca terena od 3-4","Y=",{"$f":"-(AI448-AH448)/(AH447-AI447)","v":-1.2},"*x    +",{"$f":"-(AH447*AF450-AH448)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Q-785",10,10,100,{"$f":"+Q451","v":100},null,null,null,null,null,null,null,"X=",{"$f":"+(AC450-AC449)/(AA449-AA450)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AA450*AA451+AC450","v":{"$error":"#VALUE!"}},"sjecište","X=",{"$f":"+(AH450-AH449)/(AF449-AF450)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AF450*AF451+AH450","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pravac 1-2","T2","T1","sredina","privremani iskop",null,"T1","T11","Sredina"]
[null,null,null,null,null,null,null,null,null,null,"OBLIK TERENA PRIJE ISKOPA \nZADAJE SE ZA TOČKE 3 do 7. \n(ČELIJE  L439 DO M459)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+AB447","v":-21.16},{"$f":"+AG536","v":{"$error":"#VALUE!"}},{"$f":"+(AA453+AB453)/2","v":{"$error":"#VALUE!"}},{"$f":"+AF451","v":{"$error":"#VALUE!"}},{"$f":"+AH447","v":-1},{"$f":"+AB453","v":{"$error":"#VALUE!"}},{"$f":"+L467","v":-1},{"$f":"+(AF453+AG453)/2","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Oznaka točke","x","y",null,null,null,null,"  T A B L I C A   R E B R A S T E   A R M A T U R E",null,null,null,null,null,null,null,"Y=",{"$f":"+AB448","v":{"$error":"#VALUE!"}},{"$f":"+AH536","v":{"$error":"#VALUE!"}},{"$f":"+(AA454+AB454)/2","v":{"$error":"#VALUE!"}},{"$f":"+AH451","v":{"$error":"#VALUE!"}},{"$f":"+AH448","v":1.2},{"$f":"+AB454","v":{"$error":"#VALUE!"}},{"$f":"+M467","v":1.2},{"$f":"+(AF454+AG454)/2","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,1,{"$f":"+AG536","v":{"$error":"#VALUE!"}},{"$f":"+AH536","v":{"$error":"#VALUE!"}},null,null,null,null,"Površina presjeka za komada",5,6,7,8,9,null,null,null,null,null,null,null,null,"Opseg     (cm)","Profil (mm)"]
[null,null,null,null,null,null,null,null,null,null,2,{"$f":"IF(H20=0,-15,AA453)","v":-21.16},{"$f":"AA454","v":{"$error":"#VALUE!"}},"PROFIL","Kom",null,null,null,{"$f":"+$O458*S$455","v":1.413},1.6956000000000002,1.9782000000000002,2.2608000000000001,2.5434000000000001,null,null,null,null,null,null,"   (kg/m)"]
[null,null,null,null,null,null,null,null,null,null,3,{"$f":"+'Unos podataka'!K114","v":-15},{"$f":"+'Unos podataka'!L114","v":9.5},"F",1,2,3,4,2.5120000000000005,3.0144000000000002,3.5168000000000004,4.0192000000000005,4.5216000000000003,10,11,12,13,14,15,"RA 400-1","RA 400-2"]
[null,null,null,null,null,null,null,null,null,null,4,{"$f":"+'Unos podataka'!K115","v":-10},{"$f":"+'Unos podataka'!L115","v":9},6,{"$f":"+N458*N458*3.14/4/100","v":0.28260000000000002},{"$f":"+$O458*$P$457","v":0.56520000000000004},{"$f":"+$O458*Q$457","v":0.84780000000000011},1.1304000000000001,3.9250000000000003,4.71,5.4950000000000001,6.28,7.0650000000000004,{"$f":"+$O458*X$457","v":2.8260000000000001},3.1086,3.3912000000000004,3.6738000000000004,3.9564000000000004,4.2389999999999999,0.23,0.22800000000000001,{"$f":"+AG458*3.14/10","v":1.8839999999999999},{"$f":"+N458","v":6}]
[null,null,null,null,null,null,null,null,null,null,5,{"$f":"+'Unos podataka'!K116","v":-4},{"$f":"+'Unos podataka'!L116","v":8},8,0.50240000000000007,1.0048000000000001,1.5072000000000001,2.0096000000000003,5.6520000000000001,6.7824000000000009,7.9128000000000007,9.0432000000000006,10.1736,5.0240000000000009,5.5264000000000006,6.0288000000000004,6.531200000000001,7.0336000000000007,7.5360000000000014,0.40899999999999997,0.40500000000000003,2.512,8]
[null,null,null,null,null,null,null,null,null,null,6,{"$f":"+'Unos podataka'!K117","v":-2},{"$f":"'Unos podataka'!L117","v":7},10,0.78500000000000003,1.57,2.355,3.14,7.6930000000000014,9.2316000000000003,10.770200000000001,12.308800000000002,13.847400000000002,7.8500000000000005,8.6349999999999998,9.42,10.205,10.99,11.775,0.64900000000000002,0.63300000000000001,3.14,10]
[null,null,null,null,null,null,null,null,null,null,7,{"$f":"+'Unos podataka'!K118","v":5},{"$f":"+'Unos podataka'!L118","v":1.2},12,1.1304000000000001,2.2608000000000001,3.3912000000000004,4.5216000000000003,10.048000000000002,12.057600000000001,14.067200000000001,16.076800000000002,18.086400000000001,11.304,12.4344,13.564800000000002,14.695200000000002,15.825600000000001,16.956,0.92,0.91100000000000003,3.7679999999999998,12]
[null,null,null,null,null,null,null,null,null,null,8,{"$f":"+E61+'Unos podataka'!$G$49","v":2.9000021999999994},{"$f":"+M463+E51","v":1.2},14,1.5386000000000002,3.0772000000000004,4.6158000000000001,6.1544000000000008,12.717000000000001,15.260400000000001,17.803800000000003,20.347200000000001,22.890599999999999,15.386000000000003,16.924600000000002,18.463200000000001,20.001800000000003,21.540400000000002,23.079000000000004,1.252,1.242,4.3959999999999999,14]
[null,null,null,null,null,null,null,null,null,null,9,{"$f":"+E61+'Unos podataka'!$G$49","v":2.9000021999999994},{"$f":"+E52-E51","v":0.5},16,2.0096000000000003,4.0192000000000005,6.0288000000000004,8.0384000000000011,15.700000000000001,18.84,21.98,25.12,28.26,20.096000000000004,22.105600000000003,24.115200000000002,26.124800000000004,28.134400000000003,30.144000000000005,null,1.621,5.024,16]
[null,null,null,null,null,null,null,null,null,null,10,{"$f":"+'Unos podataka'!$G$49-Kontrafore!E3","v":-1},0,18,2.5434000000000001,5.0868000000000002,7.6302000000000003,10.1736,18.997,22.796399999999998,26.595800000000001,30.395199999999999,34.194600000000001,25.434000000000001,27.977400000000003,30.520800000000001,33.0642,35.607600000000005,38.151000000000003,null,2.2879999999999998,5.6520000000000001,18]
[null,null,null,null,null,null,null,null,null,null,11,{"$f":"-Kontrafore!E3","v":-1},{"$f":"IF('Unos podataka'!O48=\"DA\",M472,+'Unos podataka'!F41)","v":1.2},20,3.14,6.28,9.42,12.56,24.53125,29.4375,34.34375,39.25,44.15625,31.400000000000002,34.54,37.68,40.82,43.96,47.1,null,2.5154700000000001,6.28,20]
[null,null,null,null,null,null,null,null,null,null,12,0,{"$f":"+M465","v":1.2},22,3.7993999999999999,7.5987999999999998,11.398199999999999,15.1976,30.772000000000006,36.926400000000001,43.080800000000004,49.235200000000006,55.389600000000009,37.994,41.793399999999998,45.592799999999997,49.392199999999995,53.191600000000001,56.991,null,3.0579999999999998,6.9079999999999995,22]
[null,null,null,null,null,null,null,null,null,null,11,{"$f":"IF(A82=\"\",0,-'Unos podataka'!AB3)","v":-1},{"$f":"+M465","v":1.2},25,4.90625,9.8125,14.71875,19.625,40.192000000000007,48.230400000000003,56.268800000000006,64.307200000000009,72.345600000000005,49.0625,53.96875,58.875,63.78125,68.6875,73.59375,null,3.9510000000000001,7.85,25]
[null,null,null,null,{"$f":"2+E61+1","v":5.9000021999999994},0.02,null,null,null,null,1,{"$f":"+L455","v":{"$error":"#VALUE!"}},{"$f":"+M455","v":{"$error":"#VALUE!"}},28,6.1544000000000008,12.308800000000002,18.463200000000001,24.617600000000003,50.868000000000002,61.041600000000003,71.21520000000001,81.388800000000003,91.562399999999997,61.544000000000011,67.698400000000007,73.852800000000002,80.007200000000012,86.161600000000007,92.316000000000017,null,4.9560000000000004,8.7919999999999998,28]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(L465+L468)/2","v":{"$error":"#VALUE!"}},{"$f":"+(M468-M465)/2+M465","v":{"$error":"#VALUE!"}},32,8.0384000000000011,16.076800000000002,24.115200000000002,32.153600000000004,62.800000000000004,75.36,87.92,100.48,113.04,80.384000000000015,88.42240000000001,96.460800000000006,104.49920000000002,112.53760000000001,120.57600000000002,null,6.4740000000000002,10.048,32]
[null,null,null,null,null,null,null,null,null,null,null,"6'",{"$f":"+'Unos podataka'!$Q$89","v":{"$error":"#VALUE!"}},36,10.1736,20.347200000000001,30.520800000000001,40.694400000000002,20,16.670000000000002,14.3,12.5,11.11,101.736,111.90960000000001,122.08320000000001,132.2568,142.43040000000002,152.60400000000001,null,8.1999999999999993,11.304,36]
[null,null,null,null,null,null,null,null,{"$f":"IF(A82=\"\",\"\",+I442)","v":3.5},null,{"$f":"IF(K472=-5,-5,K472-0.9)","v":{"$error":"#VALUE!"}},{"$f":"S593","v":1.4923077248520527},{"$f":"+'Poprečni presjek zida'!BF2","v":0.12820515121628623},40,12.56,25.12,37.68,50.24,{"$f":"+S102","v":{"$error":"#VALUE!"}},{"$f":"+R106","v":{"$error":"#VALUE!"}},{"$f":"+S104","v":{"$error":"#VALUE!"}},{"$f":"+R107","v":{"$error":"#VALUE!"}},{"$f":"+S105","v":{"$error":"#VALUE!"}},125.60000000000001,138.16,150.72,163.28,175.84,188.4,null,10.117000000000001,12.56,40]
[null,null,null,null,null,null,null,null,{"$f":"IF(A82=\"\",\"\",+I443)","v":5},{"$f":"IF(I471=\"\",-1,J443)","v":11.8},{"$f":"+IF('Iskaz armature'!A31=\"\",-5,IF(E50=0,N592,2+E59+Q58-(L472-E52)/F57))","v":{"$error":"#VALUE!"}},{"$f":"+L471","v":1.4923077248520527},{"$f":"+'Poprečni presjek zida'!BF3","v":1.2},null,100,50,33.340000000000003,25,{"$f":"+Q474","v":{"$error":"#VALUE!"}},{"$f":"+R474","v":{"$error":"#VALUE!"}},{"$f":"+S472","v":{"$error":"#VALUE!"}},{"$f":"+T472","v":{"$error":"#VALUE!"}},{"$f":"+U472","v":{"$error":"#VALUE!"}},10,9.1,8.33,7.7,7.14,6.67,"Odgovarajući razmak u cm za  1 m širine ploče"]
[null,null,null,null,null,null,null,null,{"$f":"IF(I471=\"\",\"\",I444)","v":0.2},{"$f":"IF(A82=\"\",-1,J444)","v":11.5},"Oznaka pozijie 12",null,null,{"$f":"+'C III-V'!X41-0.06","v":{"$error":"#VALUE!"}},{"$f":"+O474","v":{"$error":"#VALUE!"}},{"$f":"+R103","v":{"$error":"#VALUE!"}},{"$f":"+S101","v":{"$error":"#VALUE!"}},{"$f":"+R104","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,{"$f":"IF(I471=\"\",\"\",I445)","v":7},{"$f":"IF(I473=\"\",-1,+J445)","v":12},{"$f":"+K476+0.25","v":{"$error":"#VALUE!"}},null,null,{"$f":"+N473+1","v":{"$error":"#VALUE!"}},{"$f":"+B550+1","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!G67=0,6,1+(P473+V471)/2)","v":{"$error":"#VALUE!"}},{"$f":"(Q473+W471)/2-0.05","v":{"$error":"#VALUE!"}},{"$f":"+P474","v":{"$error":"#VALUE!"}},-5]
[null,{"$f":"+IF(A83=\"\",\"KADA NEMA KONTRAFORA, OVA STRANICA SE NE PRINTA\",\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(I474=\"\",-1,+J446)","v":0.1},"Vilica konzole",{"$f":"IF(E78=\"\",-5,+L474-0.4)","v":-0.4}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(A77=\"\",-5,N378+0.05)","v":{"$error":"#VALUE!"}},{"$f":"+E79+0.05","v":3.19},null,null,null,null,null,-5]
[null,null,null,null,null,null,null,null,null,null,{"$f":"K476","v":{"$error":"#VALUE!"}},{"$f":"+G555","v":3.39}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+F556","v":{"$error":"#VALUE!"}},{"$f":"+G556","v":3.39},null,{"$f":"+Y381","v":{"$error":"#VALUE!"}},{"$f":"+Z381","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+K482+0.01","v":{"$error":"#VALUE!"}},{"$f":"+L476","v":3.19},null,{"$f":"+N478-0.3","v":{"$error":"#VALUE!"}},{"$f":"+O478-0.6","v":{"$error":"#VALUE!"}},{"$f":"+AE383","v":-2},{"$f":"+W381","v":-5}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+K476","v":{"$error":"#VALUE!"}},{"$f":"+L476","v":3.19},null,{"$f":"+AE384","v":-2},{"$f":"+W382","v":-5},{"$f":"+N481","v":-3.1},{"$f":"+O481","v":-4.8}]
[null,null,null,null,null,null,null,null,null,null,"Vertikalna armatura konzole",null,null,{"$f":"+N480-1.1","v":-3.1},{"$f":"+O480+0.2","v":-4.8}]
[null,null,null,null,null,null,null,null,null,{"$f":"+IF(K482>-2,1,0)","v":{"$error":"#VALUE!"}},{"$f":"+Y377+(E81-2*0.06)/F56","v":{"$error":"#VALUE!"}},{"$f":"+L490","v":3.2}]
[null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$f":"+Y378+(E81-2*0.06)/F56","v":{"$error":"#VALUE!"}},{"$f":"+L482","v":3.2},null,"ZID",null,"  Beton zida "]
[null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$f":"+Y379","v":{"$error":"#VALUE!"}},3.2,null,{"$f":"+N374-2","v":0},{"$f":"+O374","v":0.12820515121628623},{"$f":"+N376","v":3.4000010999999999},{"$f":"+O376","v":1.2}]
[null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.2,null,0,1.2,{"$error":"#VALUE!"},3.14]
[null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.2,null,1.4000010999999999,1.2,{"$error":"#VALUE!"},3.14]
[null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.2,{"$f":"SUM(M488:M496)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.44]
[null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.2,{"$f":"+IF(K482=-2,0,1)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.44,null,null,"za  x=",{"$f":"IF(E58=0,-2,B552+1-0.2)","v":{"$error":"#VALUE!"}},{"$f":"IF(E58=0,-2,U488+0.8)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.2,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.44,{"$error":"#VALUE!"},"A",null,{"$f":"+U593","v":0.18682583433163008},"Y=",{"$f":"+(U490*U488-U490*R491)+S489","v":{"$error":"#VALUE!"}},{"$f":"++E52+0.1","v":1.3}]
[null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+E79+0.06","v":3.2},{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.44,{"$error":"#VALUE!"},"A","Poz. 2 desno",{"$f":"+U594","v":0.54310345350772504},null,{"$f":"+(S490-S489)/(R492-R491)","v":0.12678908905341604}]
[null,null,null,null,null,null,null,null,null,null,"Ukupno kom",{"$f":"SUM(J482:J490)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Unos podataka'!S55-2","v":{"$error":"#VALUE!"}},"A",4.2000010999999997,1.2,{"$f":"+T593","v":2.0499999999999998}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(K493=\"\",\"\",+S369)","v":4.8350021999999999},{"$f":"+IF(K492=\"\",\"\",T399)","v":0.57310345350772507},{"$error":"#VALUE!"},{"$f":"+N382-2","v":{"$error":"#VALUE!"}},"A",{"$f":"+P484","v":3.4000010999999999},{"$f":"+Q484","v":1.2},{"$f":"+T594","v":4.8600021999999994},{"$f":"+O374","v":0.12820515121628623},"za  x=",{"$f":"IF(F57=0,-2,B558+0.1)","v":{"$error":"#VALUE!"}},{"$f":"IF(F57=0,-2,1.5)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M569=\"\",\"\",+N390)","v":5.3350021999999999},{"$f":"+IF(K493=\"\",\"\",O390)","v":0.85},{"$error":"#VALUE!"},2.2000010999999997,1.2,"  Beton temelja",null,"Poz. 2  lijevo",{"$f":"+O375","v":1.2},"Y=",{"$f":"+(U490*U492-U490*R491)+S489","v":{"$error":"#VALUE!"}},{"$f":"+E52-0.3","v":0.89999999999999991}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(K493=\"\",\"\",+S369)","v":4.8350021999999999},{"$f":"+IF(K494=\"\",\"\",T399)","v":0.57310345350772507},{"$error":"#VALUE!"},2.2000010999999997,1.2,{"$f":"+N384-2","v":2.2000010999999997},{"$f":"+O384","v":1.2},{"$f":"+N374","v":2},{"$f":"+O386","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},2.2000010999999997,1.2,{"$f":"+N385-2","v":2.2000010999999997},{"$f":"+O385","v":1.2},{"$f":"+N375","v":2},{"$f":"+O387","v":0.5}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},2.9000021999999994,1.2,{"$f":"+N386-2","v":2.9000021999999994},{"$f":"+O386","v":1.2},{"$f":"+N386","v":4.9000021999999994},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,2.9000021999999994,0.5,{"$f":"+N387-2","v":2.9000021999999994},{"$f":"+O387","v":0.5},{"$f":"+N387","v":4.9000021999999994}]
[null,null,null,null,null,null,null,null,null,null,null,null,"aalokinranupass",0,0.12820515121628623,{"$f":"+N388-2","v":0},{"$f":"+O388","v":0.12820515121628623},{"$f":"+R494","v":2},null,"Nagib iskopa iza zida m:1          m=",{"$f":"+'Unos podataka'!K107","v":1.5},null,"Zasip"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Poz. 13",null,null,null,null,null,null,"Uređeni pokos iza zida 1:n         n=",{"$f":"IF(F21=0,1000,1/TAN(F21*PI()/180))","v":5.6712818196177093},null,"Koordinate točaka"]
[null,null,null,null,null,null,null,null,null,null,null,"y","y","d","  y  koordinate  x",null,null,null,null,null,null,null,"x"]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U44","v":1.2},{"$f":"+IF($AD$73>$AD$56,-10,L501)","v":{"$error":"#VALUE!"}},{"$f":"+U$49-2*$Q$52*100","v":{"$error":"#VALUE!"}},{"$f":"+IF(AD86>AD70,-10,+M501)","v":{"$error":"#VALUE!"}},{"$f":"+(M512-M511)*(O501-M513)/(M514-M513)+M511","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+W506","v":-1}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M501+#REF!/100","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+V$49-2*$Q$52*100","v":{"$error":"#VALUE!"}},{"$f":"+O501","v":{"$error":"#VALUE!"}},{"$f":"+P501+N501/100","v":{"$error":"#VALUE!"}},null,null,null,null,"sredina 5-6",null,{"$f":"+AG536","v":{"$error":"#VALUE!"}},"y"]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+L502+#REF!/100","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+W$49-2*$Q$52*100","v":{"$error":"#VALUE!"}},{"$f":"+M502","v":{"$error":"#VALUE!"}},{"$f":"+(M512-M511)*(O503-M513)/(M514-M513)+M511","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+(L455+L456)/2","v":{"$error":"#VALUE!"}},{"$f":"+(M455+M456)/2","v":{"$error":"#VALUE!"}},{"$f":"+N491","v":{"$error":"#VALUE!"}},{"$f":"+X508","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L503+#REF!/100<$M$501+2.2,L503+#REF!/100,L503)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+X$49-2*$Q$52*100","v":{"$error":"#VALUE!"}},{"$f":"+O503","v":{"$error":"#VALUE!"}},{"$f":"+P503+N502/100","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+U503-1","v":{"$error":"#VALUE!"}},{"$f":"+V503-2","v":{"$error":"#VALUE!"}},{"$f":"+N490","v":{"$error":"#VALUE!"}},{"$f":"+AH536","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L504+#REF!/100<$M$501+2.2,L504+#REF!/100,L504)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+Y$49-2*$Q$52*100","v":{"$error":"#VALUE!"}},{"$f":"+M503","v":{"$error":"#VALUE!"}},{"$f":"+(M512-M511)*(O505-M513)/(M514-M513)+M511","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,0,{"$f":"+O492","v":"A"}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L505+#REF!/100<$M$501+2.2,L505+#REF!/100,L505)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(M506=0,0,Z$49-2*$Q$52*100)","v":{"$error":"#VALUE!"}},{"$f":"+O505","v":{"$error":"#VALUE!"}},{"$f":"+P505+N503/100","v":{"$error":"#VALUE!"}},null,null,null,null,"sredina 5-6",null,{"$f":"0-Kontrafore!E3","v":-1},{"$f":"+O493","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L506+#REF!/100<$M$501+2.2,L506+#REF!/100,L506)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(M507=0,0,AA$49-2*$Q$52*100)","v":{"$error":"#VALUE!"}},{"$f":"+M504","v":{"$error":"#VALUE!"}},{"$f":"+(M512-M511)*(O507-M513)/(M514-M513)+M511","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+(L459+L460)/2","v":-3},{"$f":"+(M459+M460)/2","v":7.5},"Drenažni sloj iza zida",{"$f":"+X506","v":1.2},"Dodatni iskop za prometnicu"]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L507+#REF!/100<$M$501+2.2,L507+#REF!/100,L507)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(M508=0,0,AB$49-2*$Q$52*100)","v":{"$error":"#VALUE!"}},{"$f":"+O507","v":{"$error":"#VALUE!"}},{"$f":"+P507+N504/100","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+U507+1","v":-2},{"$f":"+V507+2","v":9.5},"x",0,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L508+#REF!/100<$M$501+2.2,L508+#REF!/100,L508)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(M509=0,0,AC$49-2*$Q$52*100)","v":{"$error":"#VALUE!"}},{"$f":"+M505","v":{"$error":"#VALUE!"}},{"$f":"+(M512-M511)*(O509-M513)/(M514-M513)+M511","v":{"$error":"#VALUE!"}},null,null,null,null,"Temelj kontrafore",null,{"$f":"+N486","v":1.4000010999999999},null,{"$f":"+L455","v":{"$error":"#VALUE!"}},{"$f":"+M455","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,"Jednadžba armture naprema tlu",null,null,{"$f":"+O509","v":{"$error":"#VALUE!"}},{"$f":"+P509+N505/100","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+A612-2","v":0},{"$f":"+B612","v":0.12820515121628623},{"$f":"+W509-E64","v":0.90000109999999989},"y",{"$f":"+'Unos podataka'!$T$82","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!$U$82","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,"b4",{"$f":"+'C III-V'!$B$4+Q52","v":3.4500010999999997},null,{"$f":"+M506","v":{"$error":"#VALUE!"}},{"$f":"+(M512-M511)*(O511-M513)/(M514-M513)+M511","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+A613-2","v":0},{"$f":"+B613","v":1.2},{"$f":"+N491-E64","v":{"$error":"#VALUE!"}},{"$f":"+O486","v":1.2},{"$f":"+'Unos podataka'!Q75","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!S75","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,"b9",{"$f":"+'C III-V'!$B$9+Q52","v":{"$error":"#VALUE!"}},null,{"$f":"+O511","v":{"$error":"#VALUE!"}},{"$f":"+P511+N506/100","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+N491","v":{"$error":"#VALUE!"}},{"$f":"+X511","v":1.2},{"$f":"+'Unos podataka'!$Q$74","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!$S$74","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,"c4",{"$f":"+'C III-V'!$C$4","v":1.2},null,{"$f":"+M507","v":{"$error":"#VALUE!"}},{"$f":"+(M512-M511)*(O513-M513)/(M514-M513)+M511","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+W509","v":1.4000010999999999},{"$f":"+O491+'Unos podataka'!$F9","v":0},{"$f":"+Y509","v":{"$error":"#VALUE!"}},{"$f":"+Z509","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,"c9",{"$f":"+'C III-V'!$C$9","v":"A"},null,{"$f":"+O513","v":{"$error":"#VALUE!"}},{"$f":"+P513+N507/100","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+X513","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M508","v":{"$error":"#VALUE!"}},{"$f":"+(M512-M511)*(O515-M513)/(M514-M513)+M511","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+(M465+M468)/2","v":{"$error":"#VALUE!"}},null,null,{"$f":"+X511","v":1.2},null,{"$f":"IF(E24=0,0,ABS(0.5*((Y509*Z510-Y510*Z509)+(Y510*Z511-Y511*Z510)+(Y511*Z512-Y512*Z511)+(Y512*Z513-Y513*Z512)+(Y513*Z514-Y514*Z513))))","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+O515","v":{"$error":"#VALUE!"}},{"$f":"+P515+N508/100","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+'Unos podataka'!$S$89","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oznaka   Poz 13."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Iskaz armature'!A51=\"\",-10,+O509)","v":{"$error":"#VALUE!"}},{"$f":"IF(O518=-10,\"\",+(P509+P510)/2)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Iskaz armature'!A51=\"\",-10,+O518+0.3)","v":{"$error":"#VALUE!"}},{"$f":"IF(O519=-10,\"\",P518+0.8)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+L467","v":-1},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+M464","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"L=",{"$f":"+E49","v":12},"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11]
[null,null,null,null,null,null,null,null,null,null,null,null,"Količine iskopa za zid ",null,"Količine zasipa za zid "]
[null,null,null,null,null,null,null,null,null,null,null,null,"Iskop",null,null,"Zasip"]
[null,null,null,null,null,null,null,null,null,null,null,"F=",{"$f":"IF(ABS(0.5*((L468*M465-L465*M468)+(L465*M464-L464*M465)+(L464*M463-L463*M464)+(L463*M462-L462*M463)+(L462*M461-L461*M462)+(L461*M460-L460*M461)+(L460*M459-L459*M460)+(L459*M458-L458*M459)+(L458*M457-L457*M458)+(L457*M456-L456*M457)+(L456*M455-L455*M456))+Z515),ABS(0.5*((M470*M465-L465*U516)+(L465*M464-L464*M465)+(L464*M463-L463*M464)+(L463*M462-L462*M463)+(L462*M461-L461*M462)+(L461*U516-M470*M461))))","v":{"$error":"#VALUE!"}},"m2","F=",{"$f":"ABS(0.5*((W501*X504-W502*X503)+(W502*X505-W503*X504)+(W503*X506-W504*X505)+(W504*X507-W505*X506)+(W505*X508-W506*X507)))-S528","v":{"$error":"#VALUE!"}},"m2"]
[null,null,null,null,null,null,null,null,null,null,null,"V=",{"$f":"(M525*T521)","v":{"$error":"#VALUE!"}},"m3","V=",{"$f":"(P525*T521)","v":{"$error":"#VALUE!"}},"m3",null,"m"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Količine betona temelja, betona zida i drenaže za zid duljine L=",{"$f":"+T521","v":12},{"$f":"-0.5*((W509*X512-W510*X511)+(W510*X513-W511*X512)+(W511*X514-W512*X513)+(W512*X515-W513*X514))","v":{"$error":"#VALUE!"}},"m2"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Beton temelja",null,"Beton zida. konzole i kontrafora",null,null,"Drenažni sloj iza zida",{"$f":"(S528*T521)","v":{"$error":"#VALUE!"}},"m3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"m2","F=",{"$f":"+Kontrafore!B68","v":{"$error":"#VALUE!"}},"m2","F="]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"m3","V=",{"$f":"+P530*E49","v":{"$error":"#VALUE!"}},"m3","V=",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AC570=1,          \"   za  Fs =\",\"\")","v":""},null,{"$f":"J28","v":1.25}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ukupno kom","Ukupno kg",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" IF(AC570=1,\"      qdop =\",\"\")","v":""},null,{"$f":"J27","v":1.25},"KN/m3",null,"    Vdop="]
[null,null,null,null,null,null,null,null,null,null,null,"ISKAZ ARMATURE",null,null,null,null,null,null,null,"šipka","MA",null,null,null,"Sjecišta 1 i 2",null,"Pokos od vrha zida 1:n ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BT562+BC536","v":0.91255083129751902},{"$f":"TAN(BD534)","v":1.2931634987249276},{"$f":"BE534*BE534","v":1.672271834434496},{"$f":"TAN(BS561)","v":0.25993552228740757}]
[null," glavna armatura uz tlo",null,"Poz. 7.  i 9.                               x           y",null,"Poz.  5. i 7.                                x           y",null,"Poz.  7.                                x           y",null,null,null,"Poz.","Vrsta armature",null,"f","kom mreža/m'     ","kom/m'\nili kom","m'/kom",{"$f":"IF(M537=\"šipka\",Q537*E49+1,P537*E49+1)-'Iskaz armature'!V63","v":{"$error":"#VALUE!"}},{"$f":"IF(H50=\"mreža\",\"\",IF(O537=10,S535*R537*$AD$460,IF(O537=12,$AD$461*S535*R537,IF(O537=14,$AD$462*S535*R537,IF(O537=16,S535*R537*$AE$463,IF(O537=18,S535*R537*$AE$464,IF(O537=20,S535*R537*$AE$465,IF(O537=22,S535*R537*$AE$466,S535*R537*$AE$467))))))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H50=\"šipka\",\"\",IF(N537=503,S535*$W$447,IF(N537=785,S535*$W$449,\"izračunaj\")))","v":""},null,null,null,{"$f":"+AG536","v":{"$error":"#VALUE!"}},{"$f":"+AH536","v":{"$error":"#VALUE!"}},{"$f":"+N491","v":{"$error":"#VALUE!"}},{"$f":"+O491","v":"A"},null,null,null,null,"x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"H17","v":10},{"$f":"(BF535-1)/BG534","v":10.710526973644175},"      Nq=",{"$f":"EXP(AP281)*BF534","v":3.7840464228675654}]
[null,{"$f":"+N376+Q58","v":3.4500010999999997},{"$f":"+O376","v":1.2},{"$f":"IF(B536=B537,B537,(E536-C536+A537*B536)/A537)","v":{"$error":"#VALUE!"}},{"$f":"+E47-0.3","v":-0.3},{"$f":"+F537-1.2","v":{"$error":"#VALUE!"}},{"$f":"+G537","v":1.7},{"$f":"IF(B536=B537,2+E59+Q58,(I537-C536+A537*B536)/A537)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M538=\"šipka\",Q538*E49+1,P538*E49+1)-'Iskaz armature'!V65","v":{"$error":"#VALUE!"}},{"$f":"IF(H50=\"mreža\",\"\",IF(O538=10,S536*R538*$AD$460,IF(O538=12,$AD$461*S536*R538,IF(O538=14,$AD$462*S536*R538,IF(O538=16,S536*R538*$AE$463,IF(O538=18,S536*R538*$AE$464,IF(O538=20,S536*R538*$AE$465,IF(O538=22,S536*R538*$AE$466,S536*R538*$AE$467))))))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H50=\"šipka\",\"\",IF(N538=503,S536*$W$447,IF(N538=785,S536*$W$449,\"izračunaj\")))","v":""},null,null,null,{"$f":"+AG542","v":{"$error":"#VALUE!"}},{"$f":"+AH542","v":{"$error":"#VALUE!"}},{"$f":"AA535-U499*5","v":{"$error":"#VALUE!"}},{"$f":"+AB535+5","v":5},"y=",{"$f":"+(AB536-AB535)/(AA536-AA535)","v":{"$error":"#VALUE!"}},"*X",{"$f":"-(AB536-AB535)*AA535/(AA536-AA535)+AB535+'Unos podataka'!F9","v":{"$error":"#VALUE!"}},{"$f":"(AF539-AF536)/(AD536-AD539)","v":{"$error":"#VALUE!"}},{"$f":"+AD539*AG536+AF539","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BS561/2","v":0.12715383129751895},null," Fs kliz=",{"$f":"IF(BF296=0,\"\",AR261)","v":{"$error":"#VALUE!"}},null," "]
[{"$f":"+(C537-C536)/(B537-B536)","v":{"$error":"#VALUE!"}},{"$f":"+N381+Q58","v":{"$error":"#VALUE!"}},{"$f":"+O381-Q58","v":-0.05},{"$f":"+D536-1","v":{"$error":"#VALUE!"}},{"$f":"+E536","v":-0.3},{"$f":"IF('Unos podataka'!$G$38=0.000001,B537,2+E59+Q58-(G536-E52)/F57)","v":{"$error":"#VALUE!"}},{"$f":"IF(H57=\"RA\",+E52+0.5,2)","v":1.7},{"$f":"+H536-1","v":{"$error":"#VALUE!"}},{"$f":"+E47-1","v":-1},null,null,1,{"$f":"IF(H50=\"mreža\",\"mreža R\",\"šipka\")","v":"šipka"},{"$f":"+G297","v":""},{"$f":"IF(N537=503,\"8/8\",IF(N537=785,\"10/10\",C295))","v":14},{"$f":"IF(M537=\"šipka\",\"\",IF(($G$57)>#REF!,1,0.5))","v":""},{"$f":"IF(M537=\"šipka\",B297,\"\")","v":{"$error":"#VALUE!"}},{"$f":"E61-2*B263/100","v":2.8000021999999993},{"$f":"+Q539*E49+1","v":{"$error":"#VALUE!"}},{"$f":"+IF(O539=8,$AD$459*S537*R539,IF(O539=10,S537*R539*$AD$460,IF(O539=12,$AD$461*S537*R539,IF(O539=14,$AD$462*S537*R539,IF(O539=16,S537*R539*$AE$463,IF(O539=18,S537*R539*$AE$464,IF(O539=20,S537*R539*$AE$465,IF(O539=22,S537*R539*$AE$466,S537*R539*$AE$467))))))))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,"Linija iskopa m:1"]
[null,null,null,null,null,null,null,null,{"$f":"+I537","v":-1},null,null,2,{"$f":"IF(H50=\"mreža\",\"mreža R\",\"šipka\")","v":"šipka"},{"$f":"+G270","v":""},{"$f":"IF(N538=503,\"8/8\",IF(N538=785,\"10/10\",B722))","v":14},{"$f":"IF(M538=\"šipka\",\"\",IF($E$61>#REF!,1,0.5))","v":""},{"$f":"IF(M538=\"šipka\",B270,\"\")","v":{"$error":"#VALUE!"}},{"$f":"+R537+0.01","v":2.8100021999999991},{"$f":"+Q540*E49+1","v":{"$error":"#VALUE!"}},{"$f":"+IF(O540=8,$AD$459*S538*R540,IF(O540=10,S538*R540*$AD$460,IF(O540=12,$AD$461*S538*R540,IF(O540=14,$AD$462*S538*R540,IF(O540=16,S538*R540*$AE$463,IF(O540=18,S538*R540*$AE$464,IF(O540=20,S538*R540*$AE$465,IF(O540=22,S538*R540*$AE$466,S538*R540*$AE$467))))))))","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+Y535","v":{"$error":"#VALUE!"}},{"$f":"+Z535","v":{"$error":"#VALUE!"}},{"$f":"+N485","v":0},{"$f":"+O485","v":1.2},null,null,null,null,"x","y"]
[null,"armatura na licu zida",null,"Poz. 8                                 x           zay",null,"Poz.  5. i 8.                                x           y",null,"Arm. temelja dole Poz 2",null,null,null,3,"šipka",null,{"$f":"+H720","v":10},null,{"$f":"IF(H50=\"mreža\",10,G721)","v":{"$error":"#VALUE!"}},{"$f":"+H722","v":1.9631741656683699},{"$f":"+Q541*E49+1","v":{"$error":"#VALUE!"}},{"$f":"+IF(O541=8,$AD$459*S539*R541,IF(O541=10,S539*R541*$AD$460,IF(O541=12,$AD$461*S539*R541,IF(O541=14,$AD$462*S539*R541,IF(O541=16,S539*R541*$AE$463,IF(O541=18,S539*R541*$AE$464,IF(O541=20,S539*R541*$AE$465,IF(O541=22,S539*R541*$AE$466,S539*R541*$AE$467))))))))","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"IF('Unos podataka'!AB1=\"\",0,+N485-'Unos podataka'!AB3)","v":-1},{"$f":"+O485","v":1.2},-3,{"$f":"+AB538-U498*AA539","v":5.7},"y=",{"$f":"+(AB539-AB538)/(AA539-AA538)","v":-1.5},"*X",{"$f":"-(AB539-AB538)*AA538/(AA539-AA538)+AB538","v":1.2},{"$f":"(AF542-AF539)/(AD539-AD542)","v":-4.8571428571428577},{"$f":"+AD542*AG539+AF542","v":8.4857142857142858}]
[null,{"$f":"+N382-Q58+0.005","v":{"$error":"#VALUE!"}},{"$f":"+O382-Q58","v":-0.05},{"$f":"IF(B540=B541,B541,(E540-C540+A541*B540)/A541)","v":{"$error":"#VALUE!"}},{"$f":"+E47-1","v":-1},{"$f":"IF(B540=B541,B540,(G540-C540+A541*B540)/A541)","v":{"$error":"#VALUE!"}},{"$f":"+C550-0.2","v":1.4923077248520527},{"$f":"+N375+'Unos podataka'!G49+Q58","v":2.0499999999999998},null,null,null,4,"šipka",null,{"$f":"+B731","v":10},null,{"$f":"IF(H50=\"mreža\",10,A732)","v":{"$error":"#VALUE!"}},{"$f":"+B733","v":1.5868965464922749},{"$f":"+Q542","v":{"$error":"#VALUE!"}},{"$f":"+IF(O542=8,$AD$459*S540*R542,IF(O542=10,S540*R542*$AD$460,IF(O542=12,$AD$461*S540*R542,IF(O542=14,$AD$462*S540*R542,IF(O542=16,S540*R542*$AE$463,IF(O542=18,S540*R542*$AE$464,IF(O542=20,S540*R542*$AE$465,IF(O542=22,S540*R542*$AE$466,S540*R542*$AE$467))))))))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,"Teren zadnji"]
[{"$f":"+(C541-C540)/(B541-B540)","v":{"$error":"#VALUE!"}},{"$f":"+N383-Q58","v":4.1500010999999999},{"$f":"+O383","v":1.2},{"$f":"+D540+1","v":{"$error":"#VALUE!"}},{"$f":"+E540","v":-1},{"$f":"+F540+1","v":{"$error":"#VALUE!"}},{"$f":"+G540","v":1.4923077248520527},{"$f":"N387-Q58+0.01","v":4.8600021999999994},{"$f":"+(H540*(I545-I546)/(H544-H545)-H545*(I545-I546)/(H544-H545)+I546)+Q58+M374","v":0.18682583433163008},null,null,5,"šipka",null,{"$f":"+E729","v":12},null,{"$f":"+D730","v":{"$error":"#VALUE!"}},{"$f":"+E731","v":{"$error":"#VALUE!"}},{"$f":"+Q543","v":8},{"$f":"+IF(K39=0,\"\",IF(O543=10,S541*R543*$AD$460,IF(O543=12,$AD$461*S541*R543,IF(O543=14,$AD$462*S541*R543,IF(O543=16,S541*R543*$AE$463,IF(O543=18,S541*R543*$AE$464,IF(O543=20,S541*R543*$AE$465,IF(O543=22,S541*R543*$AE$466,S541*R543*$AE$467))))))))","v":119.1904},null,{"$f":"+(2.15-0.2)*(6-0.3)","v":11.115},null,null,{"$f":"+N491","v":{"$error":"#VALUE!"}},{"$f":"+O491+'Unos podataka'!$F$9","v":0},{"$f":"+L457","v":-15},{"$f":"+M457","v":9.5},null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,{"$f":"+(H541*(I545-I546)/(H544-H545)-H545*(I545-I546)/(H544-H545)+I546)+Q58","v":0.54310345350772504},null,null,6,"šipka",null,{"$f":"+'Unos podataka'!E94","v":8},null,{"$f":"+R403+U401+AG417+M487","v":{"$error":"#VALUE!"}},{"$f":"+H731","v":11.9},{"$f":"IF(M544=\"šipka\",Q544*E49+1,P544*E49)","v":{"$error":"#VALUE!"}},{"$f":"+IF(H54=\"mreža\",\"\",IF(O544=10,S542*R544*$AD$460,IF(O544=12,$AD$461*S542*R544,IF(O544=14,$AD$462*S542*R544,IF(O544=16,S542*R544*$AE$463,IF(O544=18,S542*R544*$AE$464,IF(O544=20,S542*R544*$AE$465,IF(O544=22,S542*R544*$AE$466,S542*R544*$AE$467))))))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H54=\"šipka\",\"\",IF(N544=503,S542*$W$432,IF(N544=636,S542*$W$434,IF(N544=785,S542*$W$435,\"?\"))))","v":""},{"$f":"+V544/V541","v":{"$error":"#VALUE!"}},null,null,{"$f":"+Y535","v":{"$error":"#VALUE!"}},{"$f":"+Z535","v":{"$error":"#VALUE!"}},{"$f":"+L458","v":-10},{"$f":"+M458","v":9},"y=",{"$f":"+(AB542-AB541)/(AA542-AA541)","v":-0.1},"*X",{"$f":"-(AB542-AB541)*AA541/(AA542-AA541)+AB541","v":8},{"$f":"(AF545-AF542)/(AD542-AD545)","v":{"$error":"#VALUE!"}},{"$f":"+AD545*AG542+AF545","v":{"$error":"#VALUE!"}}]
[null,null,null,"Vezna armatura Poz.  3",null,"Vezna ar. Poz.  4",null,"Beton dno",null,null,null,{"$f":"+IF(K39=0,\"\",\"6a\")","v":"6a"},{"$f":"+IF(K39=0,\"\",\"šipka\")","v":"šipka"},null,{"$f":"+IF(K39=0,\"\",14)","v":14},null,{"$f":"+IF(K39=0,\"\",+R123)","v":8},{"$f":"+IF(K39=0,\"\",+H740)","v":11.9},{"$f":"+P545*E49","v":{"$error":"#VALUE!"}},null,{"$f":"IF(N545=283,S543*W445,IF(N545=335,S543*W446,IF(N545=503,S543*W447,IF(N545=636,S543*W448,S543*W449))))","v":{"$error":"#VALUE!"}},{"$f":"+(2.15-0.2)*(5.1-0.2)","v":9.5549999999999979},null,null,null,null,"Pokos od vrha zida 1:n "," "]
[null,"Ankeri Poz 5.",null,{"$f":"+D545+0.5","v":2.5499999999999998},{"$f":"+E545","v":1.1399999999999999},{"$f":"+F545-0.5","v":4.3500021999999996},{"$f":"+G545","v":1.1399999999999999},{"$f":"+'C III-V'!AB64","v":2},null,null,null,7,{"$f":"IF(H54=\"mreža\",\"mreža R\",\"šipka\")","v":"šipka"},{"$f":"IF(H54=\"mreža\",G322,\"\")","v":""},{"$f":"IF(N544=503,\"8/6\",IF(N544=636,\"9/6\",IF(N544=785,\"10/10\",C320)))","v":12},{"$f":"+V542","v":{"$error":"#VALUE!"}},{"$f":"+IF(H54=\"mreža\",\"\",AD111-AD112)","v":{"$error":"#VALUE!"}},{"$f":"+R545","v":{"$error":"#VALUE!"}},{"$f":"+Q546*E49+1","v":{"$error":"#VALUE!"}},{"$f":"+IF(O546=8,$AD$459*S544*R546,IF(O546=10,S544*R546*$AD$460,IF(O546=12,$AD$461*S544*R546,IF(O546=14,$AD$462*S544*R546,IF(O546=16,S544*R546*$AE$463,IF(O546=18,S544*R546*$AE$464,IF(O546=20,S544*R546*$AE$465,IF(O546=22,S544*R546*$AE$466,S544*R546*$AE$467))))))))","v":{"$error":"#VALUE!"}},null,{"$f":"+R545*1","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+N491","v":{"$error":"#VALUE!"}},{"$f":"+O491","v":"A"}]
[null,{"$f":"IF('Unos podataka'!F45=\">100\",B546,(B546-(C550-C546)/E56))","v":{"$error":"#VALUE!"}},{"$f":"+C550","v":1.6923077248520526},{"$f":"IF(M569=\"\",\"\",+H559)","v":2.0499999999999998},{"$f":"+I560","v":1.1399999999999999},{"$f":"+H560","v":4.8500021999999996},{"$f":"+I561","v":1.1399999999999999},{"$f":"+N387","v":4.9000021999999994},{"$f":"+'C III-V'!AC64","v":0},null,null,8,"mreža Q",{"$f":"IF('Unos podataka'!AB1=\"\",283,335)","v":335},{"$f":"IF(N545=283,\"6/6\",IF(N545=353,\"8/8\",IF(N545=503,\"8/8\",IF(N545=636,\"9/9\",IF(N545=785,\"10/10\",\"\")))))","v":""},{"$f":"+V544/V543","v":{"$error":"#VALUE!"}},null,{"$f":"+E740","v":{"$error":"#VALUE!"}},{"$f":"IF(G78=0,\"\",Q547*E49+1)","v":{"$error":"#VALUE!"}},{"$f":"IF(G78=0,\"\",IF(O547=8,$AD$459*S545*R547,IF(O547=10,S545*R547*$AD$460,IF(O547=12,$AD$461*S545*R547,IF(O547=14,$AD$462*S545*R547,IF(O547=16,S545*R547*$AE$463,IF(O547=18,S545*R547*$AE$464,IF(O547=20,S545*R547*$AE$465,S545*R547*$AE$466))))))))","v":{"$error":"#VALUE!"}},null,{"$f":"SUM(T548:U548)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AA536","v":{"$error":"#VALUE!"}},{"$f":"+AB536","v":5},"y=",{"$f":"+(AB545-AB544)/(AA545-AA544)","v":{"$error":"#VALUE!"}},"*X",{"$f":"-(AB545-AB544)*AA544/(AA545-AA544)+AB544","v":{"$error":"#VALUE!"}}]
[null,{"$f":"2+E59+E55-Q58+0.01","v":4.1600000999999995},{"$f":"+E52","v":1.2},{"$f":"+'C III-V'!$B$2+Q55","v":2.0499999999999998},{"$f":"+U593-0.01","v":0.17682583433163007},{"$f":"+T594","v":4.8600021999999994},{"$f":"+U594+0.01","v":0.55310345350772505},"Poz 6. razdj.arm na licu zida",{"$f":"+O387","v":0.5},null,null,9,"šipka",null,{"$f":"+B749","v":10},null,{"$f":"+Q541","v":{"$error":"#VALUE!"}},{"$f":"+B751","v":{"$error":"#VALUE!"}},{"$f":"+Q548","v":{"$error":"#VALUE!"}},{"$f":"IF(G78=0,\"\",IF(O548=8,$AD$459*S546*R548,IF(O548=10,S546*R548*$AD$460,IF(O548=12,$AD$461*S546*R548,IF(O548=14,$AD$462*S546*R548,IF(O548=16,S546*R548*$AE$463,IF(O548=18,S546*R548*$AE$464,IF(O548=20,S546*R548*$AE$465,S546*R548*$AE$466))))))))","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+IF(E58=0,2+E55+G58-Q58-0.01,'C III-V'!AJ37-Q58+0.01)","v":{"$error":"#VALUE!"}},{"$f":"+C548+(B547-B548)*TAN(F217*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"IF(F46>0,+D546+0.5,D546+0.5)","v":2.5499999999999998},{"$f":"IF(F46>0,E546+0.6*TAN(F217*PI()/180),E546+0.7*TAN(F217*PI()/180))","v":0.25374886786222656},{"$f":"+F546-0.5","v":4.3600021999999994},{"$f":"+G546-0.8*TAN(F217*PI()/180)","v":0.45053940880026311},{"$f":"+V375","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+IF(G78=0,\"\",10)","v":10},{"$f":"IF(G78=0,\"\",H60)","v":"šipka"},{"$f":"+IF(M547=\"mreža\",I403,\"\")","v":""},{"$f":"+C403","v":12},null,{"$f":"IF(G78=0,\"\",B405)","v":{"$error":"#VALUE!"}},{"$f":"+E749","v":{"$error":"#VALUE!"}},{"$f":"+'Iskaz armature'!V48","v":25},{"$f":"+'Iskaz armature'!W48","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2*(AU290-1)*TAN(BE277*PI()/180)","v":1.4473558577295844}]
[{"$f":"+B549+(C549-C548)*F57/100","v":{"$error":"#VALUE!"}},{"$f":"'C III-V'!S75","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$O$48=\"\",'C III-V'!S76,'C III-V'!S76+0.07)","v":{"$error":"#VALUE!"}},"Crtanje Poz 3",null,"Crtanje Poz 4",null,{"$f":"+H547+1","v":{"$error":"#VALUE!"}},{"$f":"+W375","v":-0.40499999999999997},null,null,{"$f":"+IF(G78=0,\"\",11)","v":11},{"$f":"IF(G78=0,\"\",H60)","v":"šipka"},null,{"$f":"+I748","v":8},null,{"$f":"+H748","v":{"$error":"#VALUE!"}},{"$f":"+H749","v":11.9},"S(kg)",{"$f":"SUM(T536:T547)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U536:U546)","v":{"$error":"#VALUE!"}},null,null,null,null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BR580<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}}]
[null,{"$f":"2+E59+Q58+0.005","v":3.4550000999999995},{"$f":"+C546","v":1.2},{"$f":"+IF(M571=\"\",\"\",D544)","v":2.5499999999999998},{"$f":"+IF(D549=\"\",-2,E544-0.02)","v":1.1199999999999999},{"$f":"+IF(M572=\"\",\"\",F544)","v":4.3500021999999996},{"$f":"IF(F549=\"\",-2,+G544-0.02)","v":1.1199999999999999},{"$f":"+V377","v":{"$error":"#VALUE!"}},{"$f":"+(I550+I548)/2","v":-0.22999999999999998},"Jednadžb pravca ankera desno",null,12,"šipka",null,{"$f":"+'Iskaz armature'!E48","v":8},null,{"$f":"+'Iskaz armature'!U48","v":2},{"$f":"+'Iskaz armature'!T48","v":{"$error":"#VALUE!"}},{"$f":"+Q551*E59","v":12.6000009},{"$f":"+IF(O551=8,$AD$459*S549*R551,IF(O551=10,S549*R551*$AD$460,IF(O551=12,$AD$461*S549*R551,IF(O551=14,$AD$462*S549*R551,IF(O551=16,S549*R551*$AE$463,IF(O551=18,S549*R551*$AE$464,IF(O551=20,S549*R551*$AE$465,IF(O551=22,S549*R551*$AE$466,S549*R551*$AE$467))))))))","v":{"$error":"#VALUE!"}}]
[{"$f":"+C192+75*E729/1000-2*Q58","v":1.6923077248520526},{"$f":"IF('C III-V'!B4='C III-V'!B9,B549,+B549-(C550-C549)/'C III-V'!F15)","v":{"$error":"#VALUE!"}},{"$f":"IF(D17+E17+C192<A550,D17+E17+C192-2*Q58,IF(A550>D17+E17+C192-2*Q58,D17+E17+C192-2*Q58,A550))","v":1.6923077248520526},{"$f":"IF(M571=\"\",\"\",+D545)","v":2.0499999999999998},{"$f":"+IF(D550=\"\",-2,E549)","v":1.1199999999999999},{"$f":"+IF(M572=\"\",\"\",F545)","v":4.8500021999999996},{"$f":"IF(F550=\"\",-2,G549)","v":1.1199999999999999},"Poz 10",{"$f":"+W377","v":-5.5E-2},{"$f":"+B545","v":{"$error":"#VALUE!"}},{"$f":"+C545","v":1.6923077248520526},{"$f":"+T593","v":2.0499999999999998},{"$f":"+U593","v":0.18682583433163008}]
[null,"Armatura uz a5",null,{"$f":"IF(M571=\"\",\"\",IF(E60=0,+D550,+D550+(0.9*E60)))","v":2.0499999999999998},{"$f":"IF(D551=\"\",-2,E546+0.03)","v":0.20682583433163007},{"$f":"IF(M572=\"\",\"\",F546-0.01)","v":4.8500021999999996},{"$f":"IF(F551=\"\",-2,G546+0.01)","v":0.56310345350772506},{"$f":"IF(A77=\"\",\"\",+IF(G78=0,-5,F555+0.1))","v":{"$error":"#VALUE!"}},null,{"$f":"+B546","v":4.1600000999999995},{"$f":"+C546","v":1.2},{"$f":"+T594","v":4.8600021999999994},{"$f":"+U594","v":0.54310345350772504},null,{"$f":"+'Iskaz armature'!E95","v":12},null,{"$f":"+'Iskaz armature'!V95","v":9},{"$f":"+'Iskaz armature'!T95","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      "]
[null,{"$f":"+B547-0.02","v":{"$error":"#VALUE!"}},{"$f":"+C547+0.012","v":{"$error":"#VALUE!"}},{"$f":"+IF(M571=\"\",\"\",D547)","v":2.5499999999999998},{"$f":"IF(D552=\"\",-2,E551+(D552-D551)*TAN(F217*PI()/180))","v":0.2709283622737938},{"$f":"IF(M572=\"\",\"\",+F547-0.01)","v":4.3500021999999996},{"$f":"IF(F552=\"\",-2,G551-(F551-F552)*TAN(F217*PI()/180)+0.001)","v":0.5000009255655613},{"$f":"IF(H551=\"\",\"\",IF(H551=\"\",-5,+H551))","v":{"$error":"#VALUE!"}},{"$f":"IF(A77=\"\",-5,+Z385+0.01)","v":{"$error":"#VALUE!"}},{"$f":"(K551-J551)/(K550-J550)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-J552*J550+J551","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"          "]
[null,null,null,null,null,null,null,null,{"$f":"IF(A77=\"\",-5,+I552+0.4)","v":{"$error":"#VALUE!"}},{"$f":"-(M551-L551)/(L550-M550)","v":2.3169593192291225},"*x    +",{"$f":"-(L550*J553-L551)","v":0.11023559558029916}]
[null,"Arnatura vrha zida",null,"Armatura  konzole",null,"Crtanje",null,"Poz 11",null,{"$f":"+(L553-L552)/(J552-J553)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+J553*J554+L553","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D O P U Š T E N O  O P T E R E Ć E N J E  T L A - NA KOSINI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"    "]
[null,{"$f":"+'C III-V'!B32+Q58","v":{"$error":"#VALUE!"}},{"$f":"+C556-0.4","v":-0.45},{"$f":"IF(G78=0,0,N379+Q58)","v":{"$error":"#VALUE!"}},{"$f":"IF(G78=0,0,O379-Q58)","v":3.39},{"$f":"IF(G78=0,0,+'C III-V'!B7+Q58)","v":{"$error":"#VALUE!"}},{"$f":"IF(G78=0,0,E555)","v":3.39},{"$f":"+Y379","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"    "]
[null,{"$f":"+N592","v":{"$error":"#VALUE!"}},{"$f":"+O592","v":-0.05},{"$f":"IF(G78=0,0,'C III-V'!AB37-0.02)","v":{"$error":"#VALUE!"}},{"$f":"+E555","v":3.39},{"$f":"IF(G78=0,0,D556-0.04)","v":{"$error":"#VALUE!"}},{"$f":"IF(G78=0,0,E556)","v":3.39},{"$f":"+H557-1.5","v":{"$error":"#VALUE!"}},{"$f":"+Z379","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," prema: DIN 4017 teil1, teil2,",null,null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,{"$f":"+N595","v":{"$error":"#VALUE!"}},{"$f":"+C556","v":-0.05},{"$f":"IF(G78=0,0,N385-Q58)","v":4.1500010999999999},{"$f":"+IF(G78=0,0,O385)","v":1.2},{"$f":"+D557-0.02","v":4.1300011000000003},{"$f":"IF(G78=0,0,E557)","v":1.2},{"$f":"IF(G78=0,-2,+Y391)","v":{"$error":"#VALUE!"}},{"$f":"+I558","v":2.0000000000000004}]
[null,{"$f":"B557+0.5*F56/100","v":{"$error":"#VALUE!"}},{"$f":"+C556-0.4","v":-0.45},null,"oznaka Poz. 6 temelj desno",null,null,"Crtanje Poz.2",{"$f":"IF(H78=0,-2,+(Z392))","v":2.0000000000000004},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     qdop=cm*Nc*sc*kc*wc+g*Df*Nd*sd*kd*wd+g'*B'*Nb*sb*kb*wb",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"Crtanje",null,null,{"$f":"IF('Unos podataka'!$O$48=\"\",2+E61+1,\"\")","v":5.9000021999999994},{"$f":"IF('Unos podataka'!$O$48=\"\",+(E52-E52/5),-5)","v":0.96},null,{"$f":"+H540-'Unos podataka'!G49+E60*0.065/E52","v":2.0499999999999998},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," ",null,null,null," "]
[null,{"$f":"+B555+0.01","v":{"$error":"#VALUE!"}},{"$f":"+C555","v":-0.45},null,{"$f":"IF('Unos podataka'!$O$48=\"\",+P398,\"\")","v":4.4350021999999996},{"$f":"+IF(F559=\"\",\"\",Q398)","v":1.1099999999999999},null,{"$f":"+H541-0.01","v":4.8500021999999996},{"$f":"IF(M569=\"\",-1,O375-Q58-0.01)","v":1.1399999999999999},null,{"$f":"+IF(B574>0,1,0)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"            Karakteristike tla:",null,null,null,"           Dimenzije temelja:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," ",null,null,null," "]
[null,{"$f":"+B556+0.01","v":{"$error":"#VALUE!"}},{"$f":"+C556","v":-0.05},null,{"$f":"+E559","v":5.9000021999999994},{"$f":"+F559","v":0.96},null,null,{"$f":"+I560","v":1.1399999999999999},null,1,"ozn. Mreže centar",null,"koordinate",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"                     "," ",null,{"$f":"BF294*3.14159/180","v":0.2543076625950379}]
[{"$f":"+B562","v":{"$error":"#VALUE!"}},{"$f":"+B557-0.01","v":{"$error":"#VALUE!"}},{"$f":"+C557","v":-0.05},null,{"$f":"IF('Unos podataka'!$O$48=\"\",+S369,\"\")","v":4.8350021999999999},{"$f":"IF(F561=\"\",\"\",+T369)","v":0.85},"Oznaka pozicije 1.",null,null,null,1,{"$f":"+I575","v":1.5500010000000002},{"$f":"+I576","v":{"$error":"#VALUE!"}},{"$f":"+(L563+M563)/2-1","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,"kut unutrašnjeg trenja  j =",{"$f":"+G14","v":18},"°  ","B =",{"$f":"+C185","v":3.1500021999999994},"m      okomito na padinu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.78539700000000001]
[null,{"$f":"IF(E56=\">100\",B562,B562+(C562-C563)/E56)","v":{"$error":"#VALUE!"}},{"$f":"+C558","v":-0.45},null,{"$f":"+E561","v":5.9000021999999994},{"$f":"+F561","v":0.96},{"$f":"+B547","v":{"$error":"#VALUE!"}},{"$f":"+C547","v":{"$error":"#VALUE!"}},null,null,1,{"$f":"+J576","v":1.22},{"$f":"+J577","v":{"$error":"#VALUE!"}},{"$f":"IF(D83=\"\",\"\",+L564*N562+N564)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,"kohezija     c =",{"$f":"+G15","v":25},"kPa","L =",{"$f":"+E49","v":12},"m      paralelno s padinom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"1.8*BD535*BG534*BG534","v":1.302610609800845}]
[null,null,null,null,{"$f":"+IF('Unos podataka'!$O$48=\"\",S371,\"\")","v":4.8350021999999999},{"$f":"+IF(F563=\"\",\"\",T371)","v":0.57310345350772507},{"$f":"+B548","v":{"$error":"#VALUE!"}},{"$f":"+C548","v":{"$error":"#VALUE!"}},"Ozn. Poz 1",null,1,{"$f":"(M563-L563)/(M562-L562)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"IF(D83=\"\",\"\",-L564*L562+L563)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,"zapreminska težina       g =",null,{"$f":"+G16","v":20},"kN/m3","Df =",{"$f":"+E51+H76","v":1.0001009999999999},"m      dubina temeljenja"]
[null,null,null,null,{"$f":"+E559","v":5.9000021999999994},{"$f":"IF(F564=\"\",\"\",+Q371)","v":0.6},{"$f":"+(G563-G564)*0.666666666666667+G564","v":{"$error":"#VALUE!"}},{"$f":"+(H563-H564)*2/3+H564","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$O$48=\"\",-5,+G565-0.07)","v":-5},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"g' =",{"$f":"+H17","v":10},"kN/m3"]
[null,null,null,null,{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",+N407)","v":""},{"$f":"+IF(F565=\"\",\"\",O407)","v":0.8},{"$f":"+G565-2","v":{"$error":"#VALUE!"}},{"$f":"+E51+0.7","v":1.4},"ozn. Poz 1 i 5",{"$f":"+H566","v":1.4},1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"b =",{"$f":"+H22","v":0},"°  ",null,null,null,null,"°    (DIN)"]
["          Armatura Poz. 2'",null,"Vezna armatura Poz.  3'",null,"Crtež armature Poz. 3'",null,"Vezna armatura Poz.  4'",null,{"$f":"+IF('Unos podataka'!$O$48=\"\",G566+0.05,-5)","v":{"$error":"#VALUE!"}},null,1]
[{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,2-Kontrafore!E3+'Unos podataka'!C99/100)","v":1.05},{"$f":"+I560","v":1.1399999999999999},{"$f":"+A568+D83","v":2.0499999999999998},{"$f":"+B568","v":1.1399999999999999},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,C568+0.025)","v":2.0749999999999997},{"$f":"+D568-0.01","v":1.1299999999999999},{"$f":"+F544","v":4.3500021999999996},{"$f":"+G544","v":1.1399999999999999},"Crtež  Poz.  4'",{"$f":"+H566","v":1.4},1,null,"pozicije armature",null,null,null,null,null,null,null,null,null,null,null,null,null,"            Mobilizirani parametri           ",null,null,null,null,null," Parametri nosivosti za jm=",{"$f":"+AC572","v":14.5707680719339}]
[{"$f":"+IF('Unos podataka'!AB1=\"\",-15,+H560)","v":4.8500021999999996},{"$f":"+I561","v":1.1399999999999999},{"$f":"+A568","v":1.05},{"$f":"+D568","v":1.1399999999999999},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,C569+0.015)","v":1.0649999999999999},{"$f":"+F568","v":1.1299999999999999},{"$f":"+F545","v":4.8500021999999996},{"$f":"+G545","v":1.1399999999999999},{"$f":"+G568","v":4.3500021999999996},null,{"$f":"SUM(K560:K568)","v":9},null,{"$f":"+'Iskaz armature'!A4","v":1}]
["Armatura Poz. 1'",null,{"$f":"+A571","v":1.05},{"$f":"+B571","v":0.05},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,C570)","v":1.05},{"$f":"+D570+0.008","v":5.8000000000000003E-2},{"$f":"+F546","v":4.8600021999999994},{"$f":"+(E52-E51)+'Unos podataka'!C99/100","v":0.55000000000000004},{"$f":"+G569","v":4.8500021999999996},{"$f":"+H568-0.015","v":1.125},"Poz. 12",null,{"$f":"+'Iskaz armature'!A7","v":2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fj =",{"$f":"+J27","v":1.25},null,"Nc =",{"$f":"(AF571-1)/TAN(AI573)","v":10.710774242262502},"    wc =",{"$f":"IF(BD275=0,1,(AF571*AF574*AH571-1)/((AF571-1)*AF574))","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BT575*BT576","v":{"$error":"#VALUE!"}},"A'",{"$f":"IF(BT571<1,\"temelj klizi\",B221*BT571)","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Unos podataka'!AB1=\"\",-15,2-Kontrafore!E3+'Unos podataka'!C99/100+E60)","v":1.05},{"$f":"+'Unos podataka'!C99/100","v":0.05},{"$f":"+C568","v":2.0499999999999998},{"$f":"IF(E52=E51,D570,+D570+(C571-A571)/D572)","v":0.17820505588432745},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,C571)","v":2.0499999999999998},{"$f":"IF(E52=E51,F570,F570+D83/D572)","v":0.18620505588432745},{"$f":"+F547","v":4.3600021999999994},{"$f":"+H570-0.5/D572","v":0.48589747205783629},{"$f":"+G570","v":4.8600021999999994},{"$f":"+J570","v":1.125},{"$f":"+IF(A77=\"\",-5,K484)","v":{"$error":"#VALUE!"}},{"$f":"+L484","v":3.2},{"$f":"+'Iskaz armature'!A10","v":3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fc =",{"$f":"+J28","v":1.25},null,"Nd =",{"$f":"EXP(3.1416*TAN(AI573))*(TAN(0.7854+0.5*AI573))^2","v":3.7841201699990723},"    wd =",{"$f":"(1-0.89*TAN(BD275))^2","v":1},{"$f":"+IF(AF562>AF563,AF563,AF562)","v":3.1500021999999994},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BE280=0,100,TAN(BE277*3.14159/180)*BC281/BE280)","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Unos podataka'!AB1=\"\",-15,T594)","v":4.8600021999999994},{"$f":"+U594","v":0.54310345350772504},"nagib dna temelja 1:",{"$f":"+E53","v":7.8000043999999988},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,B552)","v":{"$error":"#VALUE!"}},{"$f":"+C552","v":{"$error":"#VALUE!"}},"Visina područja \"U\" vilica   h=",null,{"$f":"+G571","v":4.3600021999999994},{"$f":"+H570-0.02","v":0.53},{"$f":"IF(A77=\"\",-5,K485)","v":{"$error":"#VALUE!"}},{"$f":"+L485","v":3.2},{"$f":"+'Iskaz armature'!A14","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"jm =",{"$f":"+AE628","v":14.5707680719339},"°  ","Nb =",{"$f":"(AF571-1)*TAN(AI573)","v":0.72369419293803572},"    wb =",{"$f":"(1-0.79*TAN(BD275))^2","v":1},{"$f":"+IF(AF562>AF563,AF562,AF563)","v":12}]
["crtež razdjelne  armature \nPoz. 6' vertikalna lijevo",null,"duljina zone","Razmak","Armatura zida kontrafore  Poz. 14",null,"Crtež Q mreže\nPoz. 14","             oznaka mreže Poz. 14",{"$f":"+H576-H574","v":{"$error":"#VALUE!"}},{"$f":"+H571+0.02","v":0.50589747205783631},{"$f":"+(K571+K572)/2","v":{"$error":"#VALUE!"}},{"$f":"+L572","v":3.2},5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"cm =",{"$f":"AC563/AC571","v":20},"kPa","    kc =",{"$f":"AF574-(1-AF574)/(AF571-1)","v":{"$error":"#VALUE!"}},"    sc =",{"$f":"IF(AI573=0,1+0.2*(AI571/AI572),(AH574*AF571-1)/(AF571-1))","v":1.089758607811288},{"$f":"ATAN(TAN(BC275)/AC570)","v":0.25430849107571019},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BC280/BC281+BC283","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Unos podataka'!AB1=\"\",-15,+A575+0.4)","v":1.8800000000000003},{"$f":"IF(A574=\"\",\"\",B575)","v":1.0999999999999999},{"$f":"+F581-E581","v":2.6000000999999999},{"$f":"+'Unos podataka'!$F$94/100","v":0.4},{"$f":"+E575","v":1.5000010000000001},{"$f":"+F575-0.5","v":1.2},{"$f":"IF('Unos podataka'!AB1=\"\",-15,G575)","v":1.5500010000000002},{"$f":"+F574+0.02","v":1.22},null,"m",{"$f":"+K573-0.5","v":{"$error":"#VALUE!"}},{"$f":"+L573-0.5","v":2.7},{"$f":"+'Iskaz armature'!A28","v":7},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"    kd =",{"$f":"(1-0.7*AB580/(AB578+AB590*AC573/TAN(AI573)))^3","v":{"$error":"#VALUE!"}},"    sd =",{"$f":"IF(AF563/AF562>10,1,1+(AI571/AI572)*SIN(AI573))","v":1.066038798772742},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-BC279/BC281+BC284","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Unos podataka'!AB1=\"\",-15,+A576+0.4)","v":1.4800000000000004},{"$f":"+B576","v":1.0999999999999999},{"$f":"+C574/D574-1","v":5.5000002499999994},"kom",{"$f":"+'Unos podataka'!$I50","v":1.5000010000000001},{"$f":"+'Unos podataka'!$J50","v":1.7},{"$f":"IF('Unos podataka'!AB1=\"\",-15,E575+0.05)","v":1.5500010000000002},{"$f":"+F575-0.05","v":1.65},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,+G574)","v":1.5500010000000002},null,null,null,{"$f":"+'Iskaz armature'!A34","v":8},null,null,null,null,null,null,"Poz. 5",null,null,null,null,null,null,null,null,null,null,"    kb =",{"$f":"(1-AB580/(AB578+AB590*AC573/TAN(AI573)))^3","v":{"$error":"#VALUE!"}},"sb =",{"$f":"IF(AF563/AF562>10,1,1-0.3*(AI571/AI572))","v":0.92124994500000001},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BC281=0,BA281,+BA281-ABS(2*BT573))","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Unos podataka'!AB1=\"\",-15,P369-Kontrafore!E3+0.01)","v":1.0800000000000003},{"$f":"+Q369","v":1.0999999999999999},"oznaka Poz. 15",null,{"$f":"+'Unos podataka'!$I51","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!$J51","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!AB1=\"\",-15,E576+0.05)","v":{"$error":"#VALUE!"}},{"$f":"+F576-0.05","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,G577)","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$AB$1=\"\",\"\",+H574)","v":1.22},null,{"$f":"+(I575+I576)/2","v":{"$error":"#VALUE!"}},{"$f":"+'Iskaz armature'!A37","v":9},null,null,null,null,null,{"$f":"+N403","v":3.4800010999999995},{"$f":"+O403","v":1.1099999999999999},{"$f":"+IF(S576>0,1,\"\")","v":1},"Oznaka Poz. 1(5)",null,null,null,null,"            Opterećenje na vrhu temelja:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BC281=0,E61,+E61-ABS(2*BT574))","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Unos podataka'!AB1=\"\",-15,+P370-Kontrafore!E3+0.01)","v":1.0800000000000003},{"$f":"+(B576+B578)/2","v":0.84249999999999992},{"$f":"IF('Unos podataka'!AB1=\"\",-15,A585)","v":1.5500010000000002},{"$f":"IF('Unos podataka'!$AB$1=\"\",\"\",+F574-0.3)","v":0.89999999999999991},{"$f":"+E576+0.5","v":{"$error":"#VALUE!"}},{"$f":"+F576","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!AB1=\"\",-15,G582)","v":{"$error":"#VALUE!"}},{"$f":"+H576","v":{"$error":"#VALUE!"}},"oznaka mreže Poz 17",{"$f":"IF('Unos podataka'!$AB$1=\"\",\"\",+H577)","v":{"$error":"#VALUE!"}},null,null,"OZNAKE kada nema masvbog zida",null,null,null,null,null,{"$f":"+B545-0.02","v":{"$error":"#VALUE!"}},{"$f":"+C545-0.1","v":1.5923077248520525},{"$error":"#VALUE!"},{"$f":"+(S577+S578)/2","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",+(T577+T578)/2,-1)","v":-1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(BR581+BE283/BR582+BE282/BR583)","v":{"$error":"#VALUE!"}},null,{"$f":"BE277*3.14159/180","v":0.2543076625950379}]
[{"$f":"IF('Unos podataka'!AB1=\"\",-15,P371-Kontrafore!E3+0.01)","v":1.0800000000000003},{"$f":"+(B576+B580)/2","v":0.58499999999999996},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,0.5)","v":0.5},{"$f":"+IF('Unos podataka'!$AB$1=\"\",\"\",1.5)","v":1.5},{"$f":"+'Unos podataka'!$I53","v":3.4000000999999997},{"$f":"+'Unos podataka'!$J53","v":1.2},{"$f":"IF('Unos podataka'!AB1=\"\",-15,N596)","v":4.1500010999999999},{"$f":"+F579+0.02","v":1.22},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,(I575+I576)/2)","v":{"$error":"#VALUE!"}},null,null,null,"Poz 7. 9.",null,"Poz. 2",null,"Veznna armatura temelja masivnog zida",null,{"$f":"+B546-0.02","v":4.1400001},{"$f":"+C546","v":1.2},1,{"$f":"+V577+1.2","v":{"$error":"#VALUE!"}},{"$f":"+W577","v":-1},null,null,null,"V=",{"$f":"+AB648","v":{"$error":"#VALUE!"}},"kN","vertikalno",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BR581+BE283/BR582-BE282/BR583","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Unos podataka'!AB1=\"\",-15,P372-Kontrafore!E3+0.01)","v":1.0800000000000003},{"$f":"+(B578+B580)/2","v":0.32750000000000001},{"$f":"IF('Unos podataka'!AB1=\"\",-15,A587)","v":1.9500010000000003},{"$f":"IF('Unos podataka'!$AB$1=\"\",\"\",B588-0.2)","v":1.671794931295167},{"$f":"+E575","v":1.5000010000000001},{"$f":"+F574","v":1.2},{"$f":"+G575","v":1.5500010000000002},{"$f":"+H578","v":1.22},null,{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,+(J576+J577)/2)","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(M569=\"\",\"\",+P592-0.1)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",-1,+Q592)","v":-0.3},{"$f":"+N396","v":3.0000000999999994},{"$f":"+IF(M569=\"\",-1,O396+0.1)","v":1.74},{"$f":"+P362","v":3.4800010999999995},{"$f":"IF(M569=\"\",+Q362,-1)","v":-1},{"$f":"+(S578+S580)/2","v":{"$error":"#VALUE!"}},{"$f":"+(T578-0.05+T580)/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+V578+0.1","v":{"$error":"#VALUE!"}},{"$f":"+W577","v":-1},null,null,null,"Hx=",{"$f":"+AB649","v":0},"kN        ","horizontalno u smjeru x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BR581-BE283/BR582+BE282/BR583","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Unos podataka'!AB1=\"\",-15,+P373-Kontrafore!E3+0.01)","v":1.0800000000000003},{"$f":"+'Unos podataka'!$C$99/100+0.02","v":7.0000000000000007E-2},{"$f":"IF('Unos podataka'!AB1=\"\",-15,C578)","v":0.5},{"$f":"+D578","v":1.5},"Prostor za  ankere",null,"Nagib lica zida",null,null,null,null,null,"Poz. 8",null,"Poz. 1",null,null,null,{"$f":"+B547-0.02","v":{"$error":"#VALUE!"}},{"$f":"+C547+0.01","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"poz.2 (6.)",null,null,null,null,"Hy=",{"$f":"+AB650","v":{"$error":"#VALUE!"}},"kN        ","horizontalno u smjeru y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BR581-BE283/BR582-BE282/BR583","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Unos podataka'!AB1=\"\",-15,A580+0.4)","v":1.4800000000000004},{"$f":"IF(E52=E51,B580,B580+0.2/D572+0.007)","v":0.10264101117686551},{"$f":"IF('Unos podataka'!AB1=\"\",-15,A589)","v":2.3500010000000002},{"$f":"IF('Unos podataka'!$AB$1=\"\",\"\",B594-0.7)","v":1.32564099835636},{"$f":"+G575","v":1.5500010000000002},{"$f":"+G578","v":4.1500010999999999},"n=",{"$f":"+F56","v":{"$error":"#VALUE!"}},"Nagib kontrafore prema tlu",null,null,null,{"$f":"IF(M569=\"\",\"\",+P596+0.1)","v":{"$error":"#VALUE!"}},{"$f":"+IF(M569=\"\",-1,Q596)","v":-1},{"$f":"IF(M569=\"\",\"\",N398)","v":{"$error":"#VALUE!"}},{"$f":"+IF(M569=\"\",-1,O398+0.1)","v":{"$error":"#VALUE!"}},{"$f":"+P371","v":2.0700000000000003},{"$f":"IF(M569=\"\",+Q371,-1)","v":-1},{"$f":"+(S580+S582)/2","v":{"$error":"#VALUE!"}},{"$f":"+(T580+T582)/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+S585","v":{"$error":"#VALUE!"}},{"$f":"+IF(M569=\"\",T585,-1)","v":-1},null,null,null,"Mx=",{"$f":"+AB651","v":{"$error":"#VALUE!"}},"kNm     ","moment oko osi x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BC281/(BA281*E61)","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Unos podataka'!AB1=\"\",-15,A581+0.4)","v":1.8800000000000003},{"$f":"IF(E52=E51,B580,B581+0.3/D572+0.01)","v":0.15110252794216378},{"$f":"IF('Unos podataka'!AB1=\"\",-15,+C578)","v":0.5},{"$f":"+D580","v":1.5},{"$f":"+F575","v":1.7},{"$f":"+H575","v":1.65},{"$f":"+G578-(H576-H574)/H581","v":{"$error":"#VALUE!"}},{"$f":"+H576","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!I49","v":1.5000010000000001},null,null,null,"poz. 5",null,"Poz 7",null,null,null,{"$f":"+B548+0.03","v":{"$error":"#VALUE!"}},{"$f":"+C548+0.01","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"2+E61+0.5","v":5.4000021999999994},{"$f":"+IF(M569=\"\",W583,-1)","v":-1},null,null,null,"My=",{"$f":"+AB652","v":0},"kNm     ","moment oko osi y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BA281*BA281*E61/6","v":69.600052799999986}]
["nagib vertikale temelja  1:",{"$f":"+E60","v":0},"koordinate \"U\" vilica Poz.19",null,{"$f":"+H577-H574","v":{"$error":"#VALUE!"}},{"$f":"0.3/H581","v":{"$error":"#VALUE!"}},{"$f":"+(+D585-$H$574)/$H$581","v":{"$error":"#VALUE!"}},null,{"$f":"+'Unos podataka'!I51-0.000001","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!J49+0.5","v":1.7},null,null,{"$f":"IF(M569=\"\",\"\",+R596+0.1)","v":{"$error":"#VALUE!"}},{"$f":"+IF(M569=\"\",-1,S594)","v":1.4923077248520527},{"$f":"IF(M569=\"\",\"\",+T590-0.1)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",-1,+U590)","v":-1},{"$f":"P373","v":2.0700000000000003},{"$f":"IF(M569=\"\",+Q373+0.1,Q373)","v":0.22682583433163006},{"$f":"+(S582+S584)/2","v":{"$error":"#VALUE!"}},{"$f":"+(T582+T584-0.05)/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+S579","v":{"$error":"#VALUE!"}},{"$f":"+IF(M569=\"\",T579,-1)","v":-1},null,null,null,"ey=",{"$f":"(AB581)/AB578","v":{"$error":"#VALUE!"}},"m","excentricitet",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BA281*E61*E61/6","v":16.820025520009676}]
["Ankeri za rebro kontrafore Poz. 15",null,"\"U\" vilice izvana Poz 19",null,null,"\"U\" vilice Poz. 16",null,"Oznaka Poz 19","n=",{"$f":"+'Unos podataka'!J51","v":{"$error":"#VALUE!"}},null,null,"Poz. 4",null,null,null,null,null,{"$f":"+B549+0.02","v":3.4750000999999995},{"$f":"+C549","v":1.2},1,{"$f":"+S581","v":{"$error":"#VALUE!"}},{"$f":"+IF(M569=\"\",T581,-1)","v":-1},null,null,null,"ex=",{"$f":"(AB579*AG565+AB582)/AB578","v":{"$error":"#VALUE!"}},"m"]
[{"$f":"IF('Unos podataka'!$AB$1=\"\",\"\",+E581)","v":1.5500010000000002},{"$f":"IF($E$52=$E$51,0.05,IF(A585=\"\",\"\",(A585-(2-'Unos podataka'!$AB$3))/$D$572+0.05))","v":0.12051290894143601},{"$f":"G577","v":{"$error":"#VALUE!"}},{"$f":"+H577-0.05","v":{"$error":"#VALUE!"}},1,{"$f":"+G576","v":{"$error":"#VALUE!"}},{"$f":"+D585","v":{"$error":"#VALUE!"}},{"$f":"+(C589+C590)/2","v":{"$error":"#VALUE!"}},null,{"$f":"+(J584-J583)/(I583-I582)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+IF(M569=\"\",\"\",N392+0.1)","v":5.5500021999999989},{"$f":"IF(M569=\"\",-1,O392)","v":0.7},null,null,null,null,{"$f":"+B550+0.04","v":{"$error":"#VALUE!"}},{"$f":"+C550-0.1","v":1.5923077248520525},{"$error":"#VALUE!"},{"$f":"+V583","v":{"$error":"#VALUE!"}},{"$f":"+W583","v":-1}]
[{"$f":"+A585","v":1.5500010000000002},{"$f":"IF('Unos podataka'!$AB$1=\"\",\"\",+B585+$E$52+0.5)","v":1.820512908941436},{"$f":"+C585-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D585","v":{"$error":"#VALUE!"}},null,{"$f":"+F585+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"2-E59+E55+1","v":2.3999999000000001},{"$f":"+D589","v":{"$error":"#VALUE!"}},"Poz 16",null,null,"Poz. 6",null,null,null,null,null,"vezna arm uz ankere     ",null,{"$f":"SUM(U576:U584)","v":{"$error":"#VALUE!"}},"oznaka  poz.2 (6)",null,null,null,null,"            Reducirane dimenzije temelja:",null,null,null,null,null,"smjer y - okomit na padinu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(BC277=0,100000,(BC278/BC277))","v":100000}]
[{"$f":"IF('Unos podataka'!$AB$1=\"\",\"\",A586+$D$574)","v":1.9500010000000003},{"$f":"IF($E$52=$E$51,0.05,$B585+(A587-$A585)/$D$572)","v":0.17179493129516701},{"$f":"+C585+$F$583","v":{"$error":"#VALUE!"}},{"$f":"+D585-0.3","v":{"$error":"#VALUE!"}},2,{"$f":"+F585-0.3/$J$585","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+(C597+C598)/2-0.1","v":{"$error":"#VALUE!"}},{"$f":"+D597-0.5","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$AB$1=\"\",\"\",(F589+F590)/2)","v":{"$error":"#VALUE!"}}," S Poz 15"," S Poz 19",{"$f":"IF(M569=\"\",\"-1\",K493+0.1)","v":5.4350021999999996},{"$f":"+IF(M569=\"\",-1,O407)","v":0.8},null,null,null,null,null,null,{"$f":"+V582+0.1","v":5.5000021999999991},{"$f":"IF(M569=\"\",+W583,-1)","v":-1},null,null,null,null,null,null,null,null,null,null,"smjer x - paralelan s padinom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,{"$f":"ATAN(BT586)*180/PI()","v":89.999427042204886}]
[{"$f":"+A587","v":1.9500010000000003},{"$f":"IF(A588=\"\",\"\",IF('Unos podataka'!$AB$1=\"\",\"\",+B587+$E$52+0.5))","v":1.8717949312951669},{"$f":"+C587-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D587","v":{"$error":"#VALUE!"}},null,{"$f":"+F587+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+H586+2","v":4.3999999000000001},{"$f":"+D597","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$AB$1=\"\",\"\",J587-1.5)","v":{"$error":"#VALUE!"}},{"$f":"+IF(A585>0,1,0)","v":1},{"$f":"+IF(G585>0,1,\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"Poz. 7",null,null,null,null,null,null,"        B' = B-2ey =",{"$f":"AF562-2*AB583","v":{"$error":"#VALUE!"}},"m",null,{"$f":"IF(AC594*AB590<AB578,\"NOSIVOST TLA NA KOSINI NE ZADOVOLJAVA\",\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(2+(BT576/BT575))/(1+(BT576/BT575))","v":{"$error":"#VALUE!"}},null,{"$f":"+COS(BT587*PI()/180)*COS(BT587*PI()/180)","v":9.9999999990320259E-11}]
[{"$f":"IF(A587+$D$574+0.1>(2+$E$59+$E$55),\"\",(IF('Unos podataka'!$AB$1=\"\",\"\",+A587+$D$574)))","v":2.3500010000000002},{"$f":"IF($E$52=$E$51,0.05,$B587+(A589-$A587)/$D$572)","v":0.22307695364889799},{"$f":"+C587+$F$583","v":{"$error":"#VALUE!"}},{"$f":"IF(D587-0.3<$F$574,\"\",D587-0.3)","v":{"$error":"#VALUE!"}},3,{"$f":"+F587-0.3/$J$585","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+(C603+C604)/2-0.2","v":{"$error":"#VALUE!"}},{"$f":"+I587","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$AB$1=\"\",\"\",(F597+F598)/2)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"IF(M569=\"\",\"\",+S590)","v":1.7},{"$f":"IF(M569=\"\",\"\",IF(N591=N592,2+E59+Q58,(U589-O591+M592*N591)/M592))","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",\"\",+E47-1)","v":-1},null,null,null,null,null,"        L' = L-2.ex =",{"$f":"AF563-2*AB584","v":{"$error":"#VALUE!"}},"m",null,{"$f":"IF(AB580=0,\"\",AB578*TAN(BC275)/AB580)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(2+(BT575/BT576))/(1+(BT575/BT576))","v":{"$error":"#VALUE!"}},null,{"$f":"+SIN(BT587*PI()/180)*SIN(BT587*PI()/180)","v":0.99999999989999999}]
[{"$f":"+A589","v":2.3500010000000002},{"$f":"IF(A590=\"\",\"\",IF('Unos podataka'!$AB$1=\"\",\"\",+B589+$E$52+0.5))","v":1.9230769536488979},{"$f":"+C589-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D589","v":{"$error":"#VALUE!"}},null,{"$f":"+F589+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+H588","v":4.3999999000000001},{"$f":"+D603","v":{"$error":"#VALUE!"}},{"$f":"+J588","v":{"$error":"#VALUE!"}},{"$f":"+IF(A587>0,1,0)","v":1},{"$f":"+IF(G587>0,1,\"\")","v":{"$error":"#VALUE!"}},null," Poz 7",null,"POZ 7 i 9",null,"Poz.  5. i 7.                                x           y",{"$f":"IF(M569=\"\",\"\",IF(H57=\"ribbed\",+E52+0.5,2))","v":1.7},{"$f":"IF(M569=\"\",\"\",+T589-1)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",\"\",+U589)","v":-1},null,null,null,null,null,"       A' = L' . B' =",{"$f":"AB588*AB589","v":{"$error":"#VALUE!"}},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+BR589*BT588+BR588*BT589","v":{"$error":"#VALUE!"}}]
[{"$f":"IF(A589=\"\",\"\",IF(A589+$D$574+1>(2+$E$59+$E$55),\"\",(IF('Unos podataka'!$AB$1=\"\",\"\",+A589+$D$574))))","v":2.7500010000000001},{"$f":"IF(A591=\"\",\"\",IF($E$52=$E$51,0.05,$B589+(A591-$A589)/$D$572))","v":0.27435897600262898},{"$f":"+C589+$F$583","v":{"$error":"#VALUE!"}},{"$f":"IF(D589-0.3<$F$574,\"\",D589-0.3)","v":{"$error":"#VALUE!"}},4,{"$f":"+F589-0.3/$J$585","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Zid i temelj",{"$f":"+I589","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$AB$1=\"\",\"\",(F603+F604)/2)-0.2","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"IF(M574=\"\",\"\",+N376+Q58)","v":3.4500010999999997},{"$f":"+IF(N591=\"\",\"\",O376)","v":1.2},{"$f":"IF(M569=\"\",\"\",IF(N591=N592,N592,(Q591-O591+M592*N591)/M592))","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",\"\",E47-0.3)","v":-0.3},{"$f":"IF(M569=\"\",\"\",+R592-1.2)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4," ",{"$f":"+((1-BE280/(BE281+BT575*BT576*BE278*1/TAN(BE277*PI()/180))))","v":{"$error":"#VALUE!"}}]
[{"$f":"+A591","v":2.7500010000000001},{"$f":"IF(A592=\"\",\"\",IF('Unos podataka'!$AB$1=\"\",\"\",+B591+$E$52+0.5))","v":1.974358976002629},{"$f":"+C591-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D591","v":{"$error":"#VALUE!"}},null,{"$f":"+F591+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(A83=\"\",\"\",+N374)","v":2},null,{"$f":"+J590","v":{"$error":"#VALUE!"}},{"$f":"+IF(A589>0,1,0)","v":1},{"$f":"+IF(G589>0,1,\"\")","v":{"$error":"#VALUE!"}},{"$f":"+(O592-O591)/(N592-N591)","v":{"$error":"#VALUE!"}},{"$f":"+IF(M574=\"\",\"\",N381+Q58)","v":{"$error":"#VALUE!"}},{"$f":"IF(M574=\"\",\"\",O381-Q58)","v":-0.05},{"$f":"IF(M569=\"\",\"\",+P591-1)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",\"\",Q591)","v":-0.3},{"$f":"IF(M569=\"\",\"\",IF('Unos podataka'!$G$38=0.000001,N592,2+E59+Q58-(S589-E52)/F57))","v":{"$error":"#VALUE!"}},null,"Poz 1",null,null,null,null,null,null,null,{"$f":"IF(AC570=1,\"     GRANIČNO OPTEREĆENJE\",\"     DOPUŠTENO OPTEREĆENJE\")","v":"     DOPUŠTENO OPTEREĆENJE"},null,null,"                      DOPUŠTENA VERTIKALNA SILA"]
[{"$f":"IF(A591=\"\",\"\",IF(A591+$D$574+0.1>(2+$E$59+$E$55),\"\",(IF('Unos podataka'!$AB$1=\"\",\"\",+A591+$D$574))))","v":3.1500010000000001},{"$f":"IF(A593=\"\",\"\",IF($E$52=$E$51,0.05,$B591+(A593-$A591)/$D$572))","v":0.32564099835635996},{"$f":"+C591+$F$583","v":{"$error":"#VALUE!"}},{"$f":"IF(D591-0.3<$F$574,\"\",D591-0.3)","v":{"$error":"#VALUE!"}},5,{"$f":"+F591-0.3/$J$585","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(A83=\"\",\"\",+N375)","v":2},{"$f":"IF(A83=\"\",\"\",+O374)","v":0.12820515121628623},null,null,null,null,null,null,null,null,null,{"$f":"IF(M569=\"\",\"\",+C550-0.2)","v":1.4923077248520527},{"$f":"IF(M569=\"\",\"\",N375+'Unos podataka'!G49+Q58)","v":2.0499999999999998},{"$f":"IF(M569=\"\",\"\",(T593*(I545-I546)/(H544-H545)-H545*(I545-I546)/(H544-H545)+I546)+Q58+M374)","v":0.18682583433163008}]
[{"$f":"+A593","v":3.1500010000000001},{"$f":"IF(A594=\"\",\"\",IF('Unos podataka'!$AB$1=\"\",\"\",+B593+$E$52+0.5))","v":2.0256409983563599},{"$f":"+C593-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D593","v":{"$error":"#VALUE!"}},null,{"$f":"+F593+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(A83=\"\",\"\",+N376)","v":3.4000010999999999},{"$f":"IF(A83=\"\",\"\",+O375)","v":1.2},null,{"$f":"+IF(A591>0,1,0)","v":1},{"$f":"+IF(G591>0,1,\"\")","v":{"$error":"#VALUE!"}},null,"Poz. 8",null,"Poz. 8                                 x           zay",null,"Poz.  5. i 8.                                x           y",{"$f":"+S593","v":1.4923077248520527},{"$f":"IF(M569=\"\",\"\",N387-Q58+0.01)","v":4.8600021999999994},{"$f":"IF(M569=\"\",\"\",(T594*(I545-I546)/(H544-H545)-H545*(I545-I546)/(H544-H545)+I546)+Q58)","v":0.54310345350772504},null,null,null,null,null,null,{"$f":"IF(AC570=1,\"qult =\",\"qdop =\")","v":"qdop ="},{"$f":"AC573*AF570*AF573*AH573*AH570+AC564*AF564*AF571*AF574*AH574*AH571+AC565*AB588*AF572*AF575*AH575*AH572","v":{"$error":"#VALUE!"}},"kPa","Vdop=",{"$f":"+IF(AC570=1,+AC594/BB533*AB590,+AC594*AB590)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AF594>AB578,\"kN   >  V =\",\" kN   <  V =\")","v":{"$error":"#VALUE!"}},{"$f":"+AB578","v":{"$error":"#VALUE!"}},"kN"]
[{"$f":"IF(A593=\"\",\"\",IF(A593+$D$574+0.1>(2+$E$59+$E$55),\"\",(IF('Unos podataka'!$AB$1=\"\",\"\",+A593+$D$574))))","v":3.550001},{"$f":"IF(A595=\"\",\"\",IF($E$52=$E$51,0.05,$B593+(A595-$A593)/$D$572))","v":0.37692302071009093},{"$f":"+C593+$F$583","v":{"$error":"#VALUE!"}},{"$f":"IF(D593-0.3<$F$574,\"\",D593-0.3)","v":{"$error":"#VALUE!"}},6,{"$f":"+F593-0.3/$J$585","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(A83=\"\",\"\",N377)","v":{"$error":"#VALUE!"}},{"$f":"IF(A83=\"\",\"\",+O376)","v":1.2},null,null,null,null,{"$f":"+IF(M575=\"\",\"\",N382-Q58+0.005)","v":{"$error":"#VALUE!"}},{"$f":"IF(N595=\"\",\"\",O382-Q58)","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",\"\",IF(N595=N596,N596,(Q595-O595+M596*N595)/M596))","v":{"$error":"#VALUE!"}},{"$f":"IF(M569=\"\",\"\",+E47-1)","v":-1},{"$f":"IF(M569=\"\",\"\",IF(N595=N596,N595,(S593-O595+M596*N595)/M596))","v":{"$error":"#VALUE!"}}]
[{"$f":"+A595","v":3.550001},{"$f":"IF(A596=\"\",\"\",IF('Unos podataka'!$AB$1=\"\",\"\",+B595+$E$52+0.5))","v":2.0769230207100908},{"$f":"+C595-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D595","v":{"$error":"#VALUE!"}},null,{"$f":"+F595+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(A83=\"\",\"\",+N378)","v":{"$error":"#VALUE!"}},{"$f":"IF(A83=\"\",\"\",+O377)","v":3.14},null,{"$f":"+IF(A593>0,1,0)","v":1},{"$f":"+IF(G593>0,1,\"\")","v":{"$error":"#VALUE!"}},{"$f":"+(O596-O595)/(N596-N595)","v":{"$error":"#VALUE!"}},{"$f":"IF(M575=\"\",\"\",+N383-Q58)","v":4.1500010999999999},{"$f":"IF(N596=\"\",\"\",O383)","v":1.2},{"$f":"IF(M569=\"\",\"\",+P595+1)","v":{"$error":"#VALUE!"}},{"$f":"+Q595","v":-1},{"$f":"IF(M569=\"\",\"\",+R595+1)","v":{"$error":"#VALUE!"}}]
[{"$f":"IF(A595=\"\",\"\",IF(A595+$D$574+0.1>(2+$E$59+$E$55),\"\",(IF('Unos podataka'!$AB$1=\"\",\"\",+A595+$D$574))))","v":3.9500009999999999},{"$f":"IF(A597=\"\",\"\",IF($E$52=$E$51,0.05,$B595+(A597-$A595)/$D$572))","v":0.4282050430638219},{"$f":"IF(D597=\"\",\"\",+C595+$F$583)","v":{"$error":"#VALUE!"}},{"$f":"IF(D595-0.3<$F$574,\"\",D595-0.3)","v":{"$error":"#VALUE!"}},7,{"$f":"+F595-0.3/$J$585","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(A83=\"\",\"\",+N379)","v":{"$error":"#VALUE!"}},{"$f":"IF(A82=\"\",\"\",+O378)","v":3.14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D O P U Š T E N O   O P T E R E Ć E N J E   T L A"]
[{"$f":"+A597","v":3.9500009999999999},{"$f":"IF(A598=\"\",\"\",IF('Unos podataka'!$AB$1=\"\",\"\",+B597+$E$52+0.5))","v":2.1282050430638217},{"$f":"+C597-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D597","v":{"$error":"#VALUE!"}},null,{"$f":"+F597+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(A83=\"\",\"\",+N380)","v":{"$error":"#VALUE!"}},{"$f":"IF(A83=\"\",\"\",+O379)","v":3.44},null,{"$f":"+IF(A595>0,1,0)","v":1},{"$f":"+IF(G595>0,1,\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   Proračun dopuštenog opterećenja provodi se prema \"Pravilniku o tehničkim normativima za"]
[{"$f":"IF(A597=\"\",\"\",IF(A597+$D$574+0.1>(2+$E$59+$E$55),\"\",(IF('Unos podataka'!$AB$1=\"\",\"\",+A597+$D$574))))","v":""},{"$f":"IF(A599=\"\",\"\",IF($E$52=$E$51,0.05,$B597+(A599-$A597)/$D$572))","v":""},{"$f":"IF(D599=\"\",\"\",+C597+$F$583)","v":{"$error":"#VALUE!"}},{"$f":"IF(D597-0.3<$F$574,\"\",D597-0.3)","v":{"$error":"#VALUE!"}},8,{"$f":"+F597-0.3/$J$585","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(A83=\"\",\"\",+N381)","v":{"$error":"#VALUE!"}},{"$f":"IF(A83=\"\",\"\",+O380)","v":3.44},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   temeljenje građevinskih objekata\", Sl. list br. 15/90, prema izrazu:"]
[{"$f":"+A599","v":""},{"$f":"IF(A600=\"\",\"\",IF('Unos podataka'!$AB$1=\"\",\"\",+B599+$E$52+0.5))","v":""},{"$f":"+C599-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D599","v":{"$error":"#VALUE!"}},null,{"$f":"+F599+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(A83=\"\",\"\",+N382)","v":{"$error":"#VALUE!"}},{"$f":"IF(A83=\"\",\"\",+O381)","v":"A"},null,{"$f":"+IF(A597>0,1,0)","v":1},{"$f":"+IF(G597>0,1,\"\")","v":{"$error":"#VALUE!"}}]
[{"$f":"IF(A599=\"\",\"\",IF(A599+$D$574+0.1>(2+$E$59+$E$55),\"\",(IF('Unos podataka'!$AB$1=\"\",\"\",+A599+$D$574))))","v":""},{"$f":"IF(A601=\"\",\"\",IF($E$52=$E$51,0.05,$B599+(A601-$A599)/$D$572))","v":""},{"$f":"IF(D601=\"\",\"\",+C599+$F$583)","v":{"$error":"#VALUE!"}},{"$f":"IF(D599-0.3<$F$574,\"\",D599-0.3)","v":{"$error":"#VALUE!"}},9,{"$f":"+F599-0.3/$J$585","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(A83=\"\",\"\",+N383)","v":4.2000010999999997},{"$f":"+IF(A83=\"\",\"\",+O382)","v":"A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"pa = Vdop/A' = 0,5*g'*B'*Ng*sg*ig+(cm+q*tgjm)*Nc*sc*dc*ic+q   "]
[{"$f":"+A601","v":""},{"$f":"IF(A602=\"\",\"\",IF('Unos podataka'!$AB$1=\"\",\"\",+B601+$E$52+0.5))","v":""},{"$f":"+C601-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D601","v":{"$error":"#VALUE!"}},null,{"$f":"+F601+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(A83=\"\",\"\",+N384)","v":4.2000010999999997},{"$f":"IF(A83=\"\",\"\",+O383)","v":1.2},null,{"$f":"+IF(A599>0,1,0)","v":0},{"$f":"+IF(G599>0,1,\"\")","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,IF(D603=\"\",\"\",+C601+$F$583))","v":{"$error":"#VALUE!"}},{"$f":"IF(D601-0.3<$F$574,\"\",D601-0.3)","v":{"$error":"#VALUE!"}},10,{"$f":"+F601-0.3/$J$585","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(A83=\"\",\"\",+N385)","v":4.2000010999999997},{"$f":"IF(A83=\"\",\"\",+O384)","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"gdje je:"," "]
[null,null,{"$f":"+C603-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D603","v":{"$error":"#VALUE!"}},null,{"$f":"+F603+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(A83=\"\",\"\",+N386)","v":4.9000021999999994},{"$f":"IF(A83=\"\",\"\",+O385)","v":1.2},null,{"$f":"+IF(A601>0,1,0)","v":0},{"$f":"+IF(G601>0,1,\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"    "]
[{"$f":"+IF(A82=\"\",-2,(A595+A597)/2)","v":3.7500010000000001},{"$f":"IF(A82=\"\",-5,(B595+B597)/2)","v":0.40256403188695644},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,IF(D605=\"\",\"\",+C603+$F$583))","v":{"$error":"#VALUE!"}},{"$f":"IF(D603-0.3<$F$574,\"\",D603-0.3)","v":{"$error":"#VALUE!"}},11,{"$f":"+F603-0.3/$J$585","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(A83=\"\",\"\",+N387)","v":4.9000021999999994},{"$f":"IF(A83=\"\",\"\",+O386)","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"g.........................................",null,"    prostorna efektivna težina"]
[{"$f":"+A605","v":3.7500010000000001},{"$f":"IF(A82=\"\",-5,+B605+0.2)","v":0.60256403188695651},{"$f":"+C605-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D605","v":{"$error":"#VALUE!"}},null,{"$f":"+F605+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(A83=\"\",\"\",+N388)","v":2},{"$f":"IF(A83=\"\",\"\",+O387)","v":0.5},null,{"$f":"+IF(A603>0,1,0)","v":0},{"$f":"+IF(G603>0,1,\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,"B...................................",null,"    širina temelja (efektivna)"]
[{"$f":"IF(A82=\"\",-5,+A609)","v":2.300001},{"$f":"IF(A82=\"\",A607,+E52-0.05)","v":1.1499999999999999},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,IF(D607=\"\",\"\",+C605+$F$583))","v":{"$error":"#VALUE!"}},{"$f":"IF(D605-0.3<$F$574,\"\",D605-0.3)","v":{"$error":"#VALUE!"}},12,{"$f":"+F605-0.3/$J$585","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Poz. 14",{"$f":"+I593","v":0.12820515121628623},null,{"$f":"SUM(K588:K606)","v":7},null,null,null,null,null,null,null,null,null,null,null,null,null,"Nc, Ng..........................",null,"    faktori nosivosti"]
[{"$f":"+A607","v":2.300001},{"$f":"IF(A82=\"\",A608,+B607-0.2)","v":0.95},{"$f":"+C607-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D607","v":{"$error":"#VALUE!"}},null,{"$f":"+F607+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF('Unos podataka'!AB1=\"\",-15,P595)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+IF(G605>0,1,\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,"ic, ig................................",null,"    faktori nagiba opterećenja"]
[{"$f":"+(A589+A591)/2-0.25","v":2.300001},{"$f":"+(B589+B591)/2-0.015","v":0.23371796482576346},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,IF(D609=\"\",\"\",+C607+$F$583))","v":{"$error":"#VALUE!"}},{"$f":"IF(D607-0.3<$F$574,\"\",D607-0.3)","v":{"$error":"#VALUE!"}},13,{"$f":"IF(C609=\"\",\"\",+F607-0.3/$J$585)","v":{"$error":"#VALUE!"}},{"$f":"IF(D609=\"\",\"\",+D609)","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!AB1=\"\",-15,P596)","v":{"$error":"#VALUE!"}},{"$f":"+Q595","v":-1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sc, sg ............................",null,"    faktori oblika temelja"]
[{"$f":"+A609","v":2.300001},{"$f":"+(B590+B592)/2-1.6","v":0.34871796482576345},{"$f":"+C609-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D609","v":{"$error":"#VALUE!"}},null,{"$f":"+F609+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Poz 1'",{"$f":"+Q596","v":-1},null,null,{"$f":"+IF(G607>0,1,\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,"cm, jm ............................",null,"    mobilizirani parametri čvrstoće tla"]
["Temelj kontrafore",null,{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,IF(D611=\"\",\"\",+C609+$F$583))","v":{"$error":"#VALUE!"}},{"$f":"IF(D609-0.3<$F$574,\"\",D609-0.3)","v":{"$error":"#VALUE!"}},14,{"$f":"IF(C611=\"\",\"\",+F609-0.3/$J$585)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(B429<B322,J613,+(A572-A571)/2+A571)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dc ...................................",null,"    faktor dubine temeljenja"]
[{"$f":"+Kontrafore!I55","v":2},{"$f":"+Kontrafore!J55","v":0.12820515121628623},{"$f":"+C611-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D611","v":{"$error":"#VALUE!"}},null,{"$f":"+F611+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(B429>B322,+H611,0.1+H611)","v":{"$error":"#VALUE!"}},{"$f":"IF(B322<B429,+(B572-B571)/2+B571,K613)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+IF(G609>0,1,\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,"q ..................................",null,"    opterećenje tla u razini temeljenja"]
[{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,+Kontrafore!I56)","v":2},{"$f":"+Kontrafore!J56","v":1.2},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,IF(D613=\"\",\"\",+C611+$F$583))","v":{"$error":"#VALUE!"}},{"$f":"IF(D611-0.3<$F$574,\"\",D611-0.3)","v":{"$error":"#VALUE!"}},15,{"$f":"IF(C613=\"\",\"\",+F611-0.3/$J$585)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Poz. 8' Q mreža na licu",{"$f":"+I612+0.5","v":{"$error":"#VALUE!"}},{"$f":"+A589+0.05","v":2.4000010000000001},{"$f":"+B589","v":0.22307695364889799},null,null,null,null,null,null,null,null,null,null,null,null,null,"A' ...............................",null,"    reducirana površina temelja"]
[{"$f":"+Kontrafore!I57","v":1.75},{"$f":"+Kontrafore!J57","v":1.2},{"$f":"+C613-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D613","v":{"$error":"#VALUE!"}},null,{"$f":"+F613+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF('Unos podataka'!AB1=\"\",-15,R595)","v":{"$error":"#VALUE!"}},null,{"$f":"+J613+0.1","v":2.5000010000000001},{"$f":"+K613+0.5","v":0.72307695364889801},{"$f":"+IF(G611>0,1,\"\")","v":{"$error":"#VALUE!"}}]
[{"$f":"+Kontrafore!I58","v":1.75},{"$f":"+Kontrafore!J58","v":9.6153895463470418E-2},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,IF(D615=\"\",\"\",+C613+$F$583))","v":{"$error":"#VALUE!"}},{"$f":"IF(D613-0.3<$F$574,\"\",D613-0.3)","v":{"$error":"#VALUE!"}},16,{"$f":"IF(C615=\"\",\"\",+F613-0.3/$J$585)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+H614+0.5","v":{"$error":"#VALUE!"}},{"$f":"+S593","v":1.4923077248520527},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"          Karakteristike tla:",null,null,"           Dimenzije temelja:"]
[{"$f":"+A612","v":2},{"$f":"+Kontrafore!J59","v":0.12820515121628623},{"$f":"+C615-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D615","v":{"$error":"#VALUE!"}},null,{"$f":"+F615+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Poz. 2'",{"$f":"+S594","v":1.4923077248520527},null,null,{"$f":"+IF(G613>0,1,\"\")","v":{"$error":"#VALUE!"}}]
["Oznaka Poz. 3'",null,{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,IF(D617=\"\",\"\",+C615+$F$583))","v":{"$error":"#VALUE!"}},{"$f":"IF(D615-0.3<$F$574,\"\",D615-0.3)","v":{"$error":"#VALUE!"}},17,{"$f":"IF(C617=\"\",\"\",+F615-0.3/$J$585)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+A605","v":3.7500010000000001},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     j =",{"$f":"BB295","v":18},"°","     B =",{"$f":"BB297","v":3.1500021999999994},"m (širina temelja)"]
[{"$f":"+E570-B618*E60","v":1.05},{"$f":"+(D569+D570)/5","v":0.23799999999999999},{"$f":"+C617-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D617","v":{"$error":"#VALUE!"}},null,{"$f":"+F617+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+H617","v":3.7500010000000001},{"$f":"+O395","v":1.1399999999999999},null,null,{"$f":"+IF(G615>0,1,\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"       c =",{"$f":"BB294","v":25},"kPa","     L =",{"$f":"BB298","v":12},"m (dužina temelja)"]
[{"$f":"IF('Unos podataka'!AB1=\"\",-15,+A618-0.65)","v":0.4},{"$f":"+B618","v":0.23799999999999999},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,IF(D619=\"\",\"\",+C617+$F$583))","v":{"$error":"#VALUE!"}},{"$f":"IF(D617-0.3<$F$574,\"\",D617-0.3)","v":{"$error":"#VALUE!"}},18,{"$f":"IF(C619=\"\",\"\",+F617-0.3/$J$585)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Nama armature",{"$f":"+I618-0.2","v":0.94},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"    g =",{"$f":"BB296","v":20},"kN/m3","     Df =",{"$f":"BB299","v":1.0001009999999999},"m (dubina temeljenja)"]
["Oznaka Poz. 6' ",null,{"$f":"+C619-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D619","v":{"$error":"#VALUE!"}},null,{"$f":"+F619+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},3,null,null,null,{"$f":"+IF(G617>0,1,\"\")","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Unos podataka'!AB1=\"\",-15,A581)","v":1.4800000000000004},{"$f":"+B581","v":0.10264101117686551},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,IF(D621=\"\",\"\",+C619+$F$583))","v":{"$error":"#VALUE!"}},{"$f":"IF(D619-0.3<$F$574,\"\",D619-0.3)","v":{"$error":"#VALUE!"}},19,{"$f":"IF(C621=\"\",\"\",+F619-0.3/$J$585)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,10]
[{"$f":"+IF('Unos podataka'!AB1=\"\",-15,0.5)","v":0.5},0.6,{"$f":"+C621-0.8","v":{"$error":"#VALUE!"}},{"$f":"+D621","v":{"$error":"#VALUE!"}},null,{"$f":"+F621+0.8","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,null,{"$f":"+IF(G619>0,1,\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"          Faktori sigurnosti:"]
[{"$f":"IF('Unos podataka'!AB1=\"\",-15,A578)","v":1.0800000000000003},{"$f":"+B578","v":0.58499999999999996},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,IF(D623=\"\",\"\",+C621+$F$583))","v":{"$error":"#VALUE!"}},{"$f":"IF(D621-0.3<$F$574,\"\",D621-0.3)","v":{"$error":"#VALUE!"}},20,{"$f":"IF(C623=\"\",\"\",+F621-0.3/$J$585)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[{"$f":"+A622","v":0.5},{"$f":"+B622","v":0.6},{"$f":"IF(D624=\"\",\"\",+C622+$F$583)","v":{"$error":"#VALUE!"}},{"$f":"+D623","v":{"$error":"#VALUE!"}},null,{"$f":"IF(C624=\"\",\"\",+F622-0.3/$J$585)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,null,{"$f":"+IF(G621>0,1,\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"    Fc =",{"$f":"BC532","v":1.25},"   Fj =",{"$f":"BC533","v":1.25}]
[{"$f":"IF('Unos podataka'!AB1=\"\",-15,A574)","v":1.8800000000000003},{"$f":"+B574","v":1.0999999999999999},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," ",null," "," "," "]
[{"$f":"+A624","v":0.5},{"$f":"+B624","v":0.6},null,null,null,null,null,null,null,null,null,{"$f":"+IF(G623>0,1,\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"          Mobilizirani parametri čvrstoće tla:"]
[{"$f":"+A576","v":1.0800000000000003},{"$f":"+B576","v":1.0999999999999999},"Oznaka Poz. 17 i Poz. 18",null,null,null,null,null,null,null,null,{"$f":"SUM(L588:L626)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null," ",null,null," "," "," "," "]
[{"$f":"+A622","v":0.5},{"$f":"+B622","v":0.6},{"$f":"+(G576+G577)/2","v":{"$error":"#VALUE!"}},{"$f":"+H576","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   tgjm = tgj/Fj =",{"$f":"TAN(BB295*PI()/180)/BC533","v":0.25993575698632504}," ---->jm = ",{"$f":"BF294","v":14.5707680719339},"° --> Ng =",{"$f":"BT563","v":1.302610609800845}]
["Oznaka poz. 17",null,{"$f":"+C628+1","v":{"$error":"#VALUE!"}},{"$f":"+D628+0.3","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," ","           cm = c/Fc =",{"$f":"BF293","v":20},null,null,"     Nc =",{"$f":"BD535","v":10.710526973644175}]
[{"$f":"IF('Unos podataka'!$AB$1=\"\",-5,+(A639-(E52+0.5)/E56))","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,+(B634+B635)/3-0.1)","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Unos podataka'!$AB$1=\"\",\"\",+H615)","v":{"$error":"#VALUE!"}},{"$f":"+B630+0.3","v":{"$error":"#VALUE!"}},null,null,null,"oznaka Poz. 17",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Poz. 17"]
[{"$f":"IF(D83=\"\",-10,+B647)","v":4.8500021999999996},{"$f":"IF(D83=\"\",-10,+D637)","v":0.54180921946894223},{"$f":"+A572","v":4.8600021999999994},{"$f":"+G577","v":{"$error":"#VALUE!"}},{"$f":"+G578","v":4.1500010999999999},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"          Faktori oblika temelja:"]
[{"$f":"+B648","v":{"$error":"#VALUE!"}},{"$f":"+D638","v":{"$error":"#VALUE!"}},{"$f":"+B572","v":0.54310345350772504},{"$f":"+H577","v":{"$error":"#VALUE!"}},{"$f":"+H578","v":1.22},{"$f":"+A639","v":{"$error":"#VALUE!"}},{"$f":"+B639+0.25","v":{"$error":"#VALUE!"}}]
[{"$f":"+B649","v":{"$error":"#VALUE!"}},{"$f":"+D639","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-B645*B643+B644","v":-8.5894574072191185E-2},"Poz 1.",{"$f":"+F634+0.3","v":{"$error":"#VALUE!"}},{"$f":"+G634","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"          sg = 1- 0.40",{"$f":"IF(AH649>AH648,\"* B' / L' =\",\"*  L' / B' =\")","v":{"$error":"#VALUE!"}},{"$f":"IF(AH649>AH648,1-0.4*AQ278/AQ277,1-0.4*AQ277/AQ278)","v":{"$error":"#VALUE!"}},"    ig ="]
[{"$f":"+G576","v":{"$error":"#VALUE!"}},{"$f":"+B635","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-(D633*B646-D634)","v":{"$error":"#VALUE!"}},"Poz 15.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"           sc =1+ 0.20",{"$f":"IF(AH649>AH648,\"* B' / L' =\",\"*  L' / B' =  \")","v":{"$error":"#VALUE!"}},{"$f":"IF(AH649>AH648,1+0.2*AQ278/AQ277,1+0.2*AQ277/AQ278)","v":{"$error":"#VALUE!"}},"       ic ="]
["Crtež  Poz. 17",null,"Y=",{"$f":"+B645*B647+D635","v":0.54180921946894223},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"         dc =1+ 0.35    ","* Df / B'  =  ",{"$f":"IF((1+0.35*BB299/AQ278)>1.35,1.35,1+0.35*BB299/AQ278)","v":{"$error":"#VALUE!"}}]
[{"$f":"IF(D83=\"\",-10,+A633)","v":4.8500021999999996},{"$f":"IF(D83=\"\",-10,+B633+0.0195)","v":0.56130921946894219},"Y=",{"$f":"+B646*B648+D636","v":{"$error":"#VALUE!"}},"sjecište",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"       q =g*Df =",{"$f":"BB296*BB299","v":20.002019999999998},"kPa"]
[{"$f":"IF(D83=\"\",-10,+A634-0.025)","v":{"$error":"#VALUE!"}},{"$f":"IF(D83=\"\",-10,+B634+0.0195)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+B646*B649+D636","v":{"$error":"#VALUE!"}}]
[{"$f":"IF(D83=\"\",-10,+A635-0.025)","v":{"$error":"#VALUE!"}},{"$f":"IF(D83=\"\",-10,+B635-0.01)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"       Dopušteno opterećenje tla za glavno + dopunsko opterećenje iznosi :"]
[{"$f":"IF(D83=\"\",-10,+A636+0.025)","v":{"$error":"#VALUE!"}},{"$f":"+IF(D83=\"\",-10,+B640)","v":{"$error":"#VALUE!"}}]
["Jednadžbe pravaca armature Poz. 1 i poz.15.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"    pa =",null,"kPa"]
["X=",{"$f":"+A571","v":1.05}]
["Y=",{"$f":"+B571","v":0.05},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"         DOPUŠTENO OPTEREĆENJE"]
["Y=",{"$f":"(C634-B644)/(C633-B643)","v":0.1294234038782773}]
["Y=",{"$f":"-(E634-D634)/(D633-E633)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"        Ukupno opterećenje temelja:",null,null,null,null,"             Reducirane dimenzije temelja:",null,null,"m"]
["X=",{"$f":"+H604-0.05","v":4.8500021999999996},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m"]
["X=",{"$f":"+(D636-D635)/(B645-B646)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      V =",{"$f":"BD297","v":{"$error":"#VALUE!"}},"kN    Vertikalna sila",null,null,null,"        B' = B-2ey =",{"$f":"AQ278","v":{"$error":"#VALUE!"}},"m2"]
["X=",{"$f":"+G577","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      Hx =",{"$f":"BD293","v":0},"kN    komponenta u smjeru x",null,null,null,"        L' = L-2.ex =",{"$f":"AQ277","v":{"$error":"#VALUE!"}}]
["oznaka Poz.18 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      Hy =",{"$f":" BD294","v":{"$error":"#VALUE!"}},"kN    komponenta u smjeru y",null,null,null,"       A' = L' . B' =",{"$f":"AQ285","v":{"$error":"#VALUE!"}}]
[{"$f":"+F607","v":{"$error":"#VALUE!"}},{"$f":"+G607","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      Mx =",{"$f":"-BD295","v":{"$error":"#VALUE!"}},"kNm  moment oko osi x"]
[{"$f":"+A651-0.5","v":{"$error":"#VALUE!"}},{"$f":"+B663+0.5","v":2.15},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      My =",{"$f":"BD296","v":0},"kNm  moment oko osi y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  ",null," "]
["Poz. 18"]
[{"$f":"+A661","v":2.0800010000000002},{"$f":"IF(E52=E51,0.05,(D83+0.05)/E53)","v":0.13461530867854385}]
[{"$f":"+A585","v":1.5500010000000002},{"$f":"IF(E52=E51,0.06,0.05+0.5/D572)","v":0.11410252794216373}]
[{"$f":"+G575","v":1.5500010000000002},1.65]
[{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["crtež Poz.18"]
[{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,A662+0.5)","v":2.0800010000000002},{"$f":"IF(E52=E51,0.065,+B662+0.5/D572+0.01)","v":0.20320505588432747}]
[{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,A656+0.03)","v":1.5800010000000002},{"$f":"IF(E52=E51,B661,+B656+0.015)","v":0.12910252794216373}]
[{"$f":"+A662","v":1.5800010000000002},{"$f":"+B657","v":1.65}]
[{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,+A658+0.03)","v":{"$error":"#VALUE!"}},{"$f":"+B658-0.03","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Unos podataka'!$AB$1=\"\",-15,+A659-0.03)","v":{"$error":"#VALUE!"}},{"$f":"+B664","v":{"$error":"#VALUE!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"x=",{"$f":"+N595","v":{"$error":"#VALUE!"}},{"$f":"+N596","v":4.1500010999999999}]
[null,null,null,null,"Y=",{"$f":"+O595","v":{"$error":"#VALUE!"}},{"$f":"+O596","v":1.2}]
[null,null,null,null,"Y=",{"$f":"(G680-F680)/(G679-F679)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-F681*F679+F680","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,"X=",{"$f":"+G679","v":4.1500010999999999}]
[null,null,null,null,"Y=",{"$f":"+F681*F683+H681","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,"Po8. 8 na vrhu zida"]
[null,null,null,null,"X=",{"$f":"+(F687-H681)/F681","v":{"$error":"#VALUE!"}},{"$f":"+F686+1","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"Y=",{"$f":"+IF('Unos podataka'!$O$48=\"\",F680-1.5,-5)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Unos podataka'!$O$48=\"\",F687,-5)","v":{"$error":"#VALUE!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["         ISKAZ  ARMATURE ",null,null,"Poz. 2","(glavna armatura)",null,"Poz. 3","(vezna armatura)"]
[null,null,{"$f":"+G270","v":""},{"$f":"+IF(H50=\"šipka\",\"f\",\"\")","v":"f"},{"$f":"C295","v":14},{"$f":"+G297","v":""},"f",10]
["Poz. 1","(glavna armatura)",null,{"$f":"+IF(H50=\"šipka\",B297,\"\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(H50=\"šipka\",\"kom/m' zida\",\"\")","v":"kom/m' zida"},null,{"$f":"IF(D721>A723,D721,IF(D721=\"\",D730,A723))","v":{"$error":"#VALUE!"}},"kom/m' zida"]
[{"$f":"+IF(H50=\"šipka\",\"f\",\"\")","v":"f"},{"$f":"IF(H50=\"mreža\",F270,C268)","v":14},"m","L=",{"$f":"+SQRT(POWER((T594-T593),2)+POWER((U593-U592),2))","v":2.8162060038957639},"m","L=",{"$f":"2*H723+H724","v":1.9631741656683699}]
[{"$f":"+IF(H50=\"šipka\",B270,\"\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(H50=\"šipka\",\"kom/m' zida\",\"\")","v":"kom/m' zida"},null,null,null,null,"l1=",{"$f":"+D544-D545","v":0.5},"m"]
["L=",{"$f":"+H560-H559","v":2.8000021999999998},null,null,null,null,"l2=",{"$f":"+E545-E546","v":0.96317416566836989},"m"]
[null,null,null,null,null,{"$f":"+ATAN('Unos podataka'!G49/E52)*180/PI()","v":0},"a3  =",{"$f":"90-F725","v":90},"m        "]
[null,null,null,null,null,null,"b3  =",{"$f":"90-F217+F725","v":82.694244543359446},"°"]
[null,null,null,null,null,null,null,null,"°"]
[null,null,null,"Poz. 5","(ankeri)",null,"Poz. 6","(razdjelna armatura)"]
[null,null,null,"f",{"$f":"+IF(O58>12,O58,12)","v":12},null,"f",{"$f":"+'Unos podataka'!E94","v":8}]
["Poz. 4","(vezna armatura)",null,{"$f":"+IF(H54=\"šipka\",MAX(B405,B350),10)","v":{"$error":"#VALUE!"}},"kom/m' zida",null,{"$f":"+'Iskaz armature'!U22","v":{"$error":"#VALUE!"}},"kom"]
["f",10,"m       ","L=",{"$f":"+E732+E733+E734","v":{"$error":"#VALUE!"}},"m","L=",{"$f":"+E49-2*Q58","v":11.9}]
[{"$f":"+G721","v":{"$error":"#VALUE!"}},"kom/m' zida ","m","l1=",{"$f":"+'Iskaz armature'!AX15","v":{"$error":"#VALUE!"}},"m",null,null,"m"]
["L=",{"$f":"2*B734+B735","v":1.5868965464922749},"m","l2=",{"$f":"+SQRT(POWER((B547-B548),2)+POWER((C547-C548),2))","v":{"$error":"#VALUE!"}},"m"]
["l1=",{"$f":"+F545-F544","v":0.5},"°","l3=",{"$f":"+'Iskaz armature'!AX16","v":{"$error":"#VALUE!"}},"m"]
["l2=",{"$f":"+G545-G546","v":0.58689654649227485},"°","a5  =",{"$f":"(ATAN(F56)*180/PI()+F217)","v":{"$error":"#VALUE!"}},"°"]
["a4  =",{"$f":"90+F217","v":97.305755456640554},null,"b5  =",{"$f":"(90+H51-F217)","v":86.694244543359446},"°"]
["b4  =",90]
[null,null,null,"Poz. 8",{"$f":"+\"(Q mreža na licu zida)\"","v":"(Q mreža na licu zida)"},null,{"$f":"+IF('Unos podataka'!G63=\"\",\"\",\"Poz. 6a\")","v":"Poz. 6a"},{"$f":"+IF('Unos podataka'!G63=\"\",\"\",\"(armatura uz sidra)\")","v":"(armatura uz sidra)"}]
[null,null,{"$f":"+IF(H54=\"mreža\",G430,\"\")","v":""},null,"mreža Q",{"$f":"IF(G430>283,G430,283)","v":283},{"$f":"+IF('Unos podataka'!G63=\"\",\"\",\"f\")","v":"f"},{"$f":"+IF('Unos podataka'!G63=\"\",\"\",14)","v":14}]
[{"$f":"+IF(A746=\"\",\"Poz. 7\",\"Poz. 7 i 7'\")","v":{"$error":"#VALUE!"}},"(glavna armatura)",{"$f":"+IF(H54=\"mreža\",\"m\",\"\")","v":""},"L=",{"$f":"+SQRT(POWER((N596-N595),2)+POWER((O596-O595),2))","v":{"$error":"#VALUE!"}},"m",{"$f":"+IF('Unos podataka'!G63=\"\",\"\",\"L=\")","v":"L="},{"$f":"IF('Unos podataka'!G63=\"\",\"\",H731)","v":11.9}]
[{"$f":"+IF(H54=\"mreža\",\"\",\"f\")","v":"f"},{"$f":"IF(H54=\"šipka\",C320,F430)","v":12},{"$f":"+IF(H54=\"šipka\",\"m\",\"\")","v":"m"},null,null,null,null,{"$f":"+IF('Unos podataka'!G63=\"\",\"\",\"(4 kom/redu sidara)\")","v":"(4 kom/redu sidara)"},{"$f":"+IF('Unos podataka'!G63=\"\",\"\",\"m\")","v":"m"}]
[{"$f":"IF(H54=\"mreža\",\"L=\",B430)","v":{"$error":"#VALUE!"}},{"$f":"+IF(H54=\"šipka\",\"kom/m' zida\",+E740)","v":"kom/m' zida"}]
[{"$f":"+IF(H54=\"šipka\",\"L=\",\"\")","v":"L="},{"$f":"IF(H54=\"šipka\",IF(B368<0,SQRT(POWER((N592-N591),2)+POWER((O592-O591),2)),E740),\"\")","v":{"$error":"#VALUE!"}},{"$f":"IF('Iskaz armature'!T31=\"\",\"\",IF(#REF!=\"šipka\",\"m\",\"\"))","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Iskaz armature'!T31=\"\",\"\",+'Iskaz armature'!U28)","v":{"$error":"#VALUE!"}},{"$f":"IF('Iskaz armature'!T31=0,\"\",+IF(H54=\"šipka\",\"kom/m' zida\",+E742))","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Iskaz armature'!U31>0,\"L'=\",\"\")","v":{"$error":"#VALUE!"}},{"$f":"IF('Iskaz armature'!U31>0,'Iskaz armature'!T31,\"\")","v":{"$error":"#VALUE!"}}]
[{"$f":"+'Iskaz armature'!U31","v":{"$error":"#VALUE!"}},{"$f":"IF('Iskaz armature'!T31=\"\",\"\",IF(H54=\"šipka\",\"kom/m' zida\",+E744))","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(G78=0,\"\",\"Poz. 10\")","v":"Poz. 10"},{"$f":"+IF(G78=0,\"\",\"(armatura konzole)\")","v":"(armatura konzole)"},null,{"$f":"+IF(G78>0,\"Poz. 11\",\"\")","v":"Poz. 11"},{"$f":"+IF(G78=0,\"\",\"(razdjelna armatura konzole)\")","v":"(razdjelna armatura konzole)"}]
[null,null,null,{"$f":"+IF(G78>0,\"f\",\"\")","v":"f"},{"$f":"+C403","v":12},null,null,{"$f":"+IF(G78>0,\"f\",\"\")","v":"f"}]
["Poz. 9","(armatura vrha zida)",null,{"$f":"+IF(G78=0,\"\",B405)","v":{"$error":"#VALUE!"}},{"$f":"+IF(G78=0,\"\",\"kom/m'  konzole-zida\")","v":"kom/m'  konzole-zida"},null,null,{"$f":"+IF(G78=0,\"\",AA405)","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!G57=\"\",\"\",'Unos podataka'!E97)","v":8}]
["f",10,"m",{"$f":"+IF(E78=\"\",\"\",\"L=l₁+l₂=\")","v":"L=l₁+l₂="},{"$f":"IF(G78=0,\"\",E750+E751)","v":{"$error":"#VALUE!"}},{"$f":"+IF(G78=0,\"\",\"m\")","v":"m"},{"$f":"+IF(G78=0,\"\",\"L=\")","v":"L="},{"$f":"IF(G78=0,\"\",E49-2*Q58)","v":11.9},{"$f":"+IF(G78=0,\"\",\"kom\")","v":"kom"}]
[{"$f":"IF(H54=\"šipka\",B350,D730)","v":{"$error":"#VALUE!"}},"kom/m' zida","m",{"$f":"+IF(G78=0,\"\",\"l₁ =\")","v":"l₁ ="},{"$f":"IF(G78=0,\"\",D556-D555)","v":{"$error":"#VALUE!"}},{"$f":"+IF(G78=0,\"\",\"m\")","v":"m"},null,null,{"$f":"+IF(G78=0,\"\",\"m\")","v":"m"}]
["L=2*l₁+l₂=",{"$f":"2*B752+B753","v":{"$error":"#VALUE!"}},"m",{"$f":"+IF(G78=0,\"\",\"l₂ =\")","v":"l₂ ="},{"$f":"IF(G78=0,\"\",SQRT(POWER((D557-D556),2)+POWER((E557-E556),2)))","v":{"$error":"#VALUE!"}},{"$f":"+IF(G78=0,\"\",\"m\")","v":"m"}]
["l₁=",{"$f":"+C557-C558","v":0.4},"°",{"$f":"+IF(G78=0,\"\",\"a10 =\")","v":"a10 ="},{"$f":"IF(G78=0,\"\",B754)","v":{"$error":"#VALUE!"}},{"$f":"+IF(G78=0,\"\",\"°\")","v":"°"}]
["l₂ =",{"$f":"+B557-B556","v":{"$error":"#VALUE!"}},"°"]
["a9 =",{"$f":"IF(F56=\">100\",90,90+ATAN(1/F56)*180/PI())","v":{"$error":"#VALUE!"}}]
["b9 =",{"$f":"90-H51","v":86},null,null,null,{"$f":"+IF(AD86>AD70,\"\",\"Poz. 13\")","v":"Poz. 13"},{"$f":"+IF(AD86>AD70,\"\",\"(spone)\")","v":"(spone)"}]
[null,null,null,null,null,{"$f":"IF(AD86>AD70,\"\",AC87)","v":{"$error":"#VALUE!"}},{"$f":"+AD87","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E78=\"\",\"\",\"Poz. 12\")","v":"Poz. 12"},{"$f":"+IF(E78=\"\",\"\",\" (vilice)\")","v":" (vilice)"},{"$f":"+IF(E78=\"\",\"\",\"m\")","v":"m"},null,null,{"$f":"+IF(AD86>AD70,\"\",\"L=2*l1+l2=\")","v":"L=2*l1+l2="},{"$f":"IF(AD86>AD70,\"\",(G759+2*G758))","v":{"$error":"#VALUE!"}},{"$f":"+IF(AD86>AD70,\"\",\"m       do\")","v":"m       do"}]
[{"$f":"IF(E81=\"\",\"\",+'Iskaz armature'!U48)","v":2},{"$f":"+IF(E78=\"\",\"\",\"kom/m' zida\")","v":"kom/m' zida"},{"$f":"+IF(E78=\"\",\"\",\"m\")","v":"m"},null,null,{"$f":"+IF(AD86>AD70,\"\",\"l1=\")","v":"l1="},{"$f":"+IF(AD86>AD70,\"\",0.15)","v":0.15},{"$f":"+IF(AD86>AF53,\"\",\"m\")","v":"m"},{"$f":"IF(AD86>AD70,\"\",G758*2+I760)","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E78=\"\",\"\",\"L=3*l₁+l₂+l₃=\")","v":"L=3*l₁+l₂+l₃="},{"$f":"+'Iskaz armature'!T48","v":{"$error":"#VALUE!"}},{"$f":"+IF(E78=\"\",\"\",\"m\")","v":"m"},null,null,{"$f":"+IF(AD86>AD70,\"\",\"l2=\")","v":"l2="},{"$f":"IF(AD86>AD70,\"\",N508/100)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AD86>AD70,\"\",\"m       do\")","v":"m       do"}]
[{"$f":"+IF(E78=\"\",\"\",\"l₁=\")","v":"l₁="},{"$f":"'Iskaz armature'!J49","v":0.19999999999999998},{"$f":"+IF(E78=\"\",\"\",\"m\")","v":"m"},null,null,null,null,null,{"$f":"IF(AD86>AD70,\"\",N501/100)","v":{"$error":"#VALUE!"}},{"$f":"+IF(F755=\"\",\"\",\"m\")","v":"m"}]
[{"$f":"+IF(E78=\"\",\"\",\"l₂=\")","v":"l₂="},{"$f":"'Iskaz armature'!M48","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+IF(F755=\"\",\"\",\"m\")","v":"m"}]
[{"$f":"+IF(E78=\"\",\"\",\"l₃=\")","v":"l₃="},{"$f":"'Iskaz armature'!M50","v":{"$error":"#VALUE!"}}]

{"sheet":"Sile i krakovi","index":4,"n_rows":347,"n_cols":49,"rows_kept":347,"cut":false,"hidden":true,"merged":[[220,2,224,2],[337,8,337,11],[337,12,337,13],[327,8,327,9],[325,4,325,11],[326,8,326,11],[326,12,326,13],[327,12,327,13],[330,12,330,13],[327,4,327,5],[336,4,336,5],[337,4,337,7],[259,12,259,13],[327,10,327,11],[213,14,213,15],[102,0,102,5],[158,3,158,4],[103,3,103,4],[127,0,127,5],[128,3,128,4],[157,0,157,5],[158,1,158,2],[102,10,102,11],[111,10,111,11],[102,8,102,9],[111,8,111,9],[320,0,320,1],[324,0,324,1],[216,0,216,1],[273,0,273,1],[271,0,271,1],[235,3,235,5],[233,3,233,5],[234,3,234,4],[333,12,333,13],[236,2,238,2],[215,2,217,2],[218,2,219,2],[252,2,254,2],[255,2,256,2],[230,2,231,2],[227,2,229,2],[225,2,226,2],[327,6,327,7],[326,4,326,7],[234,6,234,7],[234,8,234,9],[259,8,259,9],[297,0,297,1],[307,0,307,1],[317,0,317,1],[311,0,311,1],[200,0,200,1],[190,3,190,4],[190,5,190,6],[195,14,195,15],[121,0,121,5],[213,8,213,9],[190,11,190,12],[213,12,213,13],[213,3,213,4],[212,3,212,19],[138,10,138,14],[314,0,314,1],[190,9,190,10],[213,6,213,7],[239,2,241,2],[234,14,234,15],[259,10,259,11],[234,12,234,13],[259,14,259,15],[234,10,234,11],[214,3,214,5],[213,10,213,11],[0,1,0,2],[14,3,14,4],[22,1,22,2],[0,4,0,5],[22,3,22,5],[67,3,67,5],[99,2,99,3],[31,3,31,5],[39,3,39,5],[39,1,39,2],[48,3,48,5],[57,3,57,5],[99,0,99,1],[95,0,95,3],[88,0,88,3],[81,0,81,3],[92,0,92,1],[85,0,85,1],[94,4,94,5],[95,4,95,5],[278,25,280,25],[278,26,280,26],[278,27,280,27],[152,17,154,18],[205,20,205,21],[194,20,194,21],[195,24,195,25],[188,20,188,21],[194,24,194,29],[195,26,195,27],[195,28,195,29],[181,22,181,23],[194,18,194,19],[188,18,188,19],[210,22,211,22],[210,20,211,20],[210,21,211,21],[182,18,182,21],[189,20,189,21],[205,18,205,19],[181,18,181,21],[85,31,85,32],[85,25,85,26],[85,27,85,28],[85,29,85,30],[88,25,88,29],[94,17,96,18],[130,17,132,18],[198,22,199,22],[205,14,205,15],[191,14,192,15],[111,12,111,15],[189,22,190,22],[86,20,87,23],[88,30,88,32],[138,15,138,16],[101,12,101,15],[92,17,92,34],[102,12,102,13],[102,14,102,15],[93,17,93,18],[89,6,89,15],[102,6,102,7],[109,48,110,48],[109,39,110,39],[109,41,110,41],[112,17,114,18],[109,46,110,46],[97,43,97,48],[97,36,97,41],[103,43,103,44],[103,36,103,37],[99,43,99,44],[99,36,99,37],[100,43,100,44],[100,36,100,37],[101,43,101,44],[101,36,101,37],[102,43,102,44],[102,36,102,37]]}
[{"$f":"+'C III-V'!A1","v":"Točke"},{"$f":"+'C III-V'!B1","v":"ZID I TEMELJ"},null,{"$f":"+A1","v":"Točke"},"TEMELJ"]
[null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",+B7,2-'Analiza i dimenzioniranje'!D83)","v":1},0,{"$f":"+A7","v":1},2,0.12820515121628623]
[null,{"$f":"+B2","v":1},{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,+F3)","v":1.2},2,2,1.2]
[null,{"$f":"+B7","v":2},{"$f":"IF('Analiza i dimenzioniranje'!$D$83=0,'Sile i krakovi'!B7,'Unos podataka'!J43)","v":1.2},3,3.4000010999999999,1.2]
[null,{"$f":"+B4","v":2},{"$f":"+C7","v":0.12820515121628623},{"$f":"+A10","v":4},{"$f":"+E4","v":3.4000010999999999},{"$f":"+F4-'Analiza i dimenzioniranje'!$C$192","v":0.30769227514794739}]
[null,{"$f":"+B2","v":1},0,5,{"$f":"+E5","v":3.4000010999999999},{"$f":"+F7","v":1.2}]
[{"$f":"+'C III-V'!A2","v":1},{"$f":"+'C III-V'!B2","v":2},{"$f":"+'C III-V'!C2","v":0.12820515121628623},6,{"$f":"+B16","v":4.2000010999999997},1.2]
[{"$f":"+'C III-V'!A3","v":2},{"$f":"+'C III-V'!B3","v":2},{"$f":"+'C III-V'!C3","v":1.2},7,4.2000010999999997,1.2]
[{"$f":"+'C III-V'!A4","v":3},{"$f":"+'C III-V'!B4","v":3.4000010999999999},{"$f":"+'C III-V'!C4","v":1.2},8,4.2000010999999997,1.2]
[{"$f":"+'C III-V'!A5","v":4},{"$f":"+'C III-V'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C5","v":3.14},9,4.9000021999999994,1.2]
[{"$f":"+'C III-V'!A6","v":5},{"$f":"+'C III-V'!B6","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C6","v":3.14},10,4.9000021999999994,0.5]
[{"$f":"+'C III-V'!A7","v":6},{"$f":"+'C III-V'!B7","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C7","v":3.44},11,2,0.12820515121628623]
[{"$f":"+'C III-V'!A8","v":7},{"$f":"+'C III-V'!B8","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C8","v":3.44}]
[{"$f":"+'C III-V'!A9","v":8},{"$f":"+'C III-V'!B9","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C9","v":"A"}]
[{"$f":"+'C III-V'!A10","v":9},{"$f":"+'C III-V'!B10","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C10","v":"A"},"Temelj kontrafore"]
[{"$f":"+'C III-V'!A11","v":10},{"$f":"+'C III-V'!B11","v":4.2000010999999997},{"$f":"+'C III-V'!C11","v":1.2},{"$f":"'Unos podataka'!I49","v":1.5000010000000001},{"$f":"'Unos podataka'!J49","v":1.2}]
[{"$f":"+'C III-V'!A12","v":11},{"$f":"+'C III-V'!B12","v":4.2000010999999997},{"$f":"+'C III-V'!C12","v":1.2},{"$f":"'Unos podataka'!I50","v":1.5000010000000001},{"$f":"'Unos podataka'!J50","v":1.7}]
[{"$f":"+'C III-V'!A13","v":12},{"$f":"+'C III-V'!B13","v":4.2000010999999997},{"$f":"+'C III-V'!C13","v":1.2},{"$f":"'Unos podataka'!I51","v":{"$error":"#VALUE!"}},{"$f":"'Unos podataka'!J51","v":{"$error":"#VALUE!"}}]
[{"$f":"+'C III-V'!A14","v":13},{"$f":"+'C III-V'!B14","v":4.9000021999999994},{"$f":"+'C III-V'!C14","v":1.2},{"$f":"'Unos podataka'!I52","v":{"$error":"#VALUE!"}},{"$f":"'Unos podataka'!J52","v":{"$error":"#VALUE!"}}]
[{"$f":"+'C III-V'!A15","v":14},{"$f":"+'C III-V'!B15","v":4.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5},{"$f":"'Unos podataka'!I53","v":3.4000000999999997},{"$f":"'Unos podataka'!J53","v":1.2}]
[{"$f":"+'C III-V'!A16","v":15},{"$f":"+'C III-V'!B16","v":2},{"$f":"+'C III-V'!C16","v":0.12820515121628623},{"$f":"'Unos podataka'!I54","v":1.5000010000000001},{"$f":"'Unos podataka'!J54","v":1.2}]
[]
[null,"Naprezanja",null,"Beton do profila II-II"]
[1,{"$f":"+B37","v":1},{"$f":"+C37","v":{"$error":"#VALUE!"}},"oznaka","x","y"]
[2,{"$f":"+B26","v":4.9000010999999999},0,1,{"$f":"+Y197","v":1.75},9.6153895463470418E-2]
[3,{"$f":"+'Analiza i dimenzioniranje'!H190","v":4.9000010999999999},{"$f":"-'Analiza i dimenzioniranje'!F190/100","v":{"$error":"#VALUE!"}},2,1.75,{"$error":"#VALUE!"}]
[4,{"$f":"+'Analiza i dimenzioniranje'!H191","v":4.2000000999999996},{"$f":"-'Analiza i dimenzioniranje'!F191/100","v":{"$error":"#VALUE!"}},3,3.4000000999999997,{"$error":"#VALUE!"}]
[5,{"$f":"+B27","v":4.2000000999999996},0,4,3.4000000999999997,{"$error":"#VALUE!"}]
[6,{"$f":"+B28","v":4.2000000999999996},{"$f":"-'Analiza i dimenzioniranje'!F191/100","v":{"$error":"#VALUE!"}},5,1.75,9.6153895463470418E-2]
[7,{"$f":"+'Analiza i dimenzioniranje'!H192","v":3.4000000999999997},{"$f":"'Analiza i dimenzioniranje'!I192","v":{"$error":"#VALUE!"}},6,{"$f":"+Y188","v":"sredina dole"},{"$f":"+Z188","v":0}]
[8,{"$f":"+B30","v":3.4000000999999997},0]
[9,{"$f":"+B31","v":3.4000000999999997},{"$f":"'Analiza i dimenzioniranje'!I192","v":{"$error":"#VALUE!"}},"Naprezanja do profila II-II"]
[10,{"$f":"+'Analiza i dimenzioniranje'!H193","v":2},{"$f":"'Analiza i dimenzioniranje'!I193","v":{"$error":"#VALUE!"}},"oznaka","x","y"]
[11,{"$f":"+B33","v":2},0,1,{"$f":"+B31","v":3.4000000999999997},{"$f":"+C31","v":0}]
[12,{"$f":"+B33","v":2},{"$f":"'Analiza i dimenzioniranje'!I193","v":{"$error":"#VALUE!"}},2,{"$f":"+B30","v":3.4000000999999997},{"$f":"+C30","v":{"$error":"#VALUE!"}}]
[13,{"$f":"+'Analiza i dimenzioniranje'!H194","v":1.75},{"$f":"'Analiza i dimenzioniranje'!I194","v":{"$error":"#VALUE!"}},3,{"$f":"+B33","v":2},{"$f":"+C33","v":{"$error":"#VALUE!"}}]
[14,{"$f":"+'Analiza i dimenzioniranje'!H195","v":1},{"$f":"'Analiza i dimenzioniranje'!I195","v":{"$error":"#VALUE!"}},4,{"$f":"IF('Analiza i dimenzioniranje'!$D$83=\"\",'Sile i krakovi'!E36,B36)","v":1.75},{"$f":"+C36","v":{"$error":"#VALUE!"}}]
[null,null,null,5,{"$f":"+IF('Analiza i dimenzioniranje'!$D$83=\"\",'Sile i krakovi'!B34,B37)","v":1},{"$f":"+C37","v":{"$error":"#VALUE!"}}]
[null,null,null,6,{"$f":"+E34","v":3.4000000999999997},{"$f":"+F34","v":0}]
[{"$f":"+D1","v":"Točke"},"TEMELJ",null,"Beton ispod zida"]
[1,{"$f":"+E2","v":2},{"$f":"+F2","v":0.12820515121628623},"oznaka","x","y"]
[2,2,1.2,1,{"$f":"+B44","v":3.4000010999999999},0.30769227514794739]
[3,3.4000010999999999,1.2,2,3.4000010999999999,1.2]
[4,3.4000010999999999,0.30769227514794739,3,4.2000010999999997,1.2]
[5,3.4000010999999999,1.2,4,{"$f":"+E44","v":4.2000010999999997},{"$f":"+F44-'Analiza i dimenzioniranje'!$C$191","v":0.41025631985540933}]
[6,4.2000010999999997,1.2,5,{"$f":"+E42","v":3.4000010999999999},{"$f":"+F42","v":0.30769227514794739}]
[7,4.2000010999999997,1.2,6,{"$f":"+E42","v":3.4000010999999999},{"$f":"+F42","v":0.30769227514794739}]
[8,4.2000010999999997,1.2]
[9,4.9000021999999994,1.2,"Naponi ispod zida"]
[10,4.9000021999999994,0.5,"oznaka","x","y"]
[11,2,0.12820515121628623,1,{"$f":"+E42","v":3.4000010999999999},0]
[null,null,null,2,{"$f":"+E44","v":4.2000010999999997},0]
[{"$f":"+A40","v":"Točke"},"TEMELJ",null,3,{"$f":"+E52","v":4.2000010999999997},{"$f":"+'Analiza i dimenzioniranje'!$I$192","v":{"$error":"#VALUE!"}}]
[1,{"$f":"+B41","v":2},0.12820515121628623,4,{"$f":"+E51","v":3.4000010999999999},{"$f":"+'Analiza i dimenzioniranje'!$I$191","v":{"$error":"#VALUE!"}}]
[2,2,1.2,5,{"$f":"+E54","v":3.4000010999999999},{"$f":"+L28","v":0}]
[3,3.4000010999999999,1.2]
[4,3.4000010999999999,0.30769227514794739]
[5,{"$f":"+E5","v":3.4000010999999999},{"$f":"+C45","v":1.2},"Beton do I-I"]
[6,{"$f":"+B46","v":4.2000010999999997},1.2,"oznaka","x","y"]
[7,4.2000010999999997,1.2,1,{"$f":"+E45","v":4.2000010999999997},{"$f":"+F45","v":0.41025631985540933}]
[8,4.2000010999999997,1.2,2,{"$f":"+E44","v":4.2000010999999997},{"$f":"+F44","v":1.2}]
[9,4.9000021999999994,1.2,3,{"$f":"+B62","v":4.9000021999999994},{"$f":"+C59","v":1.2}]
[10,4.9000021999999994,0.5,4,{"$f":"+B63","v":4.9000021999999994},{"$f":"+C63","v":0.5}]
[11,2,0.12820515121628623,5,{"$f":"+E60","v":4.2000010999999997},{"$f":"+F60","v":0.41025631985540933}]
[]
[]
[]
[null,null,null,"Naponi ispod I-I"]
[null,null,null,"oznaka","x","y"]
[null,null,null,1,{"$f":"+E73","v":4.2000010999999997},0]
[null,null,null,2,{"$f":"+B62","v":4.9000021999999994},0]
[null,null,null,3,{"$f":"+E71","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!$I$190","v":{"$error":"#VALUE!"}}]
[null,null,null,4,{"$f":"+E53","v":4.2000010999999997},{"$f":"+F54","v":{"$error":"#VALUE!"}}]
[null,null,null,5,{"$f":"+E73","v":4.2000010999999997},{"$f":"+L44","v":0}]
[]
[]
[]
[]
[]
[]
[]
["Jednadžba leđa zida sa horizontalnim silama"]
["x=",{"$f":"+B9","v":3.4000010999999999},{"$f":"+B14","v":{"$error":"#VALUE!"}}]
["Y=",{"$f":"+C9","v":1.2},{"$f":"+C14","v":"A"}]
["Y=",{"$f":"(C84-B84)/(C83-B83)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-B85*B83+B84","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"x",{"$f":"2+'Poprečni presjek zida'!O26","v":2},{"$f":"2+'Poprečni presjek zida'!O21+'Poprečni presjek zida'!O24","v":3.5000009999999997},"x",{"$f":"2+'Poprečni presjek zida'!O21","v":2.8},{"$f":"+P85","v":2.8}]
["Vrijednosti X za poznati Y",null,"naprimjer za  +c 115",null,null,null,null,null,null,null,null,"Y",0,{"$f":"+'Poprečni presjek zida'!O18-'Poprečni presjek zida'!O16","v":0.5},"Y",{"$f":"+'Poprečni presjek zida'!O18","v":1.2},{"$f":"+Q85*M87+O87","v":0.26666648888900746}]
["X=",{"$f":"+D87/$B$85-$D$85/$B$85","v":{"$error":"#VALUE!"}},"y=",2.2599999999999998,null,null,null,null,null,null,null,"Y=",{"$f":"(N86-M86)/(N85-M85)","v":0.33333311111125935},"*x    +",{"$f":"-M87*M85+M86","v":-0.6666662222225187}]
[null,null,null,null,null,null,null,null,null,null,null,"x=",4.09,"y=",{"$f":"+M87*M88+O87","v":0.69666620222253195}]
["Jednadžba osi zida sa horizontalnim silama"]
["x=",{"$f":"+(B83+B97)/2","v":3.8000010999999998},{"$f":"+(C83+C97)/2","v":{"$error":"#VALUE!"}},null,null,null,"Dijagrami pritiska vode ispred i iza zida s težištima"]
["Y=",{"$f":"+C16","v":1.2},{"$f":"+C84","v":"A"}]
["Y=",{"$f":"(C91-B91)/(C90-B90)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-B92*B90+B91","v":{"$error":"#VALUE!"}}]
["Vrijednosti X za poznati Y",null,"naprimjer za  +c 115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ove tablice odnose se isključivo na presjeke iznad temelja (III-III do XX-XX) "]
["X=",{"$f":"+D94/$B$92-$D$92/$B$92","v":{"$error":"#VALUE!"}},"y=",2.2599999999999998,null,null,null,null,null,null,null,null,null,null,null,null,null,"Visinski položaj vanjskog opterećenja temeljem",null,{"$f":"+'Analiza i dimenzioniranje'!E48+'Analiza i dimenzioniranje'!E31","v":5},{"$f":"+T94","v":5},{"$f":"+U94","v":5},{"$f":"+V94","v":5},5,5,5,5,5,5,5,5,5,5,5,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Horizontalne komponente sila sidara i tlakova",null,"PIII","PVI","PVII","PVIII","PIX","PX","P XI","P XII","P XIII","P XIV","P XV","PXVI","PXVII","PXVIII","PXIX","PXX"]
["Jednadžba lica zida sa horizontalnim silama",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+T97/$B$92-$D$92/$B$92","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["x=",{"$f":"+B18","v":4.2000010999999997},{"$f":"+B15","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72},{"$f":"+'Analiza i dimenzioniranje'!AG44","v":5.04},{"$f":"+'Analiza i dimenzioniranje'!AH44","v":5.36},{"$f":"+'Analiza i dimenzioniranje'!AI44","v":5.6800000000000006},{"$f":"+'Analiza i dimenzioniranje'!AJ44","v":6}]
["Y=",{"$f":"+C18","v":1.2},{"$f":"+C15","v":"A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sh1=",{"$f":"IF(F107=\"\",0,-IF($F$107=\"\",\"\",$F$107))","v":-48.296291314453413},{"$f":"IF($C107>T$97,$S98,0)","v":-48.296291314453413},-48.296291314453413,-48.296291314453413,-48.296291314453413,-48.296291314453413,-48.296291314453413,-48.296291314453413,-48.296291314453413,-48.296291314453413,-48.296291314453413,-48.296291314453413,-48.296291314453413,0,0,0,0,null,"VODA IZA ZIDA ",null,null,null,null,null,null,"VODA ISPRED ZIDA "]
["Y=",{"$f":"(C98-B98)/(C97-B97)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-B99*B97+B98","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,"Sh2=",{"$f":"IF(F108=\"\",0,-IF($F$108=\"\",\"\",$F$108))","v":-48.296291314453413},{"$f":"IF($C108>T$97,$S99,0)","v":-48.296291314453413},-48.296291314453413,-48.296291314453413,-48.296291314453413,-48.296291314453413,-48.296291314453413,0,0,0,0,0,0,0,0,0,0]
["Vrijednosti X za poznati Y",null,"naprimjer za  +c 115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sh3=",null,null,{"$f":"IF($C109>U$97,$S100,0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,"visina vode  h=",null,{"$f":"+'Analiza i dimenzioniranje'!E41","v":0.6},"m",null,null,null,"visina vode  h=",null,{"$f":"IF('Analiza i dimenzioniranje'!E42=\"\",0,'Analiza i dimenzioniranje'!E42)","v":0.8},"m"]
["X=",{"$f":"+D101/B99-D99/B99","v":{"$error":"#REF!"}},"za        y=",{"$f":"+C115","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,"Sh4=",null,null,{"$f":"IF($C110>U$97,$S101,0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,null," Visina temelja",null,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m",null,null,null," Visina temelja",null,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[null,null,null,null,null,null,null,null,"Voda iza zida",null,null,null,"Ukupno vode za okretanje oko \"A\"",null,null,null,null,"Voda ispred =",{"$f":"-N109","v":0},{"$f":"-AV114","v":0},{"$f":"-$AV115","v":0},{"$f":"-$AV116","v":0},{"$f":"-$AV117","v":0},{"$f":"-$AV118","v":0},{"$f":"-$AV119","v":0},{"$f":"-$AV120","v":0},{"$f":"-$AV121","v":0},{"$f":"-$AV122","v":0},{"$f":"-$AV123","v":0},{"$f":"-$AV124","v":0},{"$f":"-$AV125","v":0},{"$f":"-$AV126","v":0},{"$f":"-$AV127","v":0},{"$f":"-$AV128","v":0},{"$f":"-$AV129","v":0},null,"Visina segmenta",null,{"$f":"+AT102","v":-7.9999999999999988E-2},"m",null,null,null,"Visina segmenta",null,{"$f":"+(AT100-AT101)/5","v":-7.9999999999999988E-2},"m"]
["horizontalne S I L E   i  vert.  KRAKOVI SILA za prevrtanje oko točke A",null,null,null,null,null,"Pritisak vode iza zida \niznad  III-III",null,"Pritisak vode iza zida od 0,00",null,"Pritisak vode ispred zida  \nod 0 do III-III",null,"Pritisak vode ispred zida\niznad III-III",null,"Pritisak vode ispred od 0 do Vrha vode",null,null,"Eh1=",{"$f":"+'Analiza i dimenzioniranje'!C110","v":{"$error":"#VALUE!"}},{"$f":"+T176","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[null,"Koordinate na licu zida",null,"X      Točka A      Y",null,"Sile",0,{"$f":"+J115","v":0.6},{"$f":"+I113","v":0},{"$f":"+J113","v":0},0,0,{"$f":"+K106","v":0},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+K104","v":0},0,null,"Eh2=",{"$f":"+'Analiza i dimenzioniranje'!C111","v":{"$error":"#VALUE!"}},{"$f":"+S104","v":{"$error":"#VALUE!"}},{"$f":"+U179","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,null,"Dijagram pritiska vode",null,null,null,null,null,null,"Dijagram pritiska vode"]
[null,"X","Y",{"$f":"+B20","v":4.9000021999999994},{"$f":"+C20","v":0.5},"kN/m' zida",0,{"$f":"+'Analiza i dimenzioniranje'!E41","v":0.6},{"$f":"+I114","v":0},{"$f":"+H105","v":0.6},0,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},0,{"$f":"+'Analiza i dimenzioniranje'!F44","v":0.8},{"$f":"+K105","v":0},{"$f":"+'Analiza i dimenzioniranje'!E42","v":0.8},null,"Eh3=",{"$f":"+'Analiza i dimenzioniranje'!C112","v":{"$error":"#VALUE!"}},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,null,null,null,null,null,0,0]
["SS=",{"$f":"IF(C106=0,0,+C106/$B$99-$D$99/$B$99)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E40","v":3.9999999960000001},{"$f":"IF(B106=\"\",\"\",$D$105-B106)","v":{"$error":"#VALUE!"}},{"$f":"IF(C106=\"\",\"\",C106-$E$105)","v":3.4999999960000001},{"$f":"+'Analiza i dimenzioniranje'!B128","v":96.592582725499412},{"$f":"+(H105-H104)*10","v":0},{"$f":"+H104","v":0.6},{"$f":"+G106","v":0},{"$f":"+J115","v":0.6},{"$f":"IF('Analiza i dimenzioniranje'!E42=0,0,IF('Analiza i dimenzioniranje'!E42>'Analiza i dimenzioniranje'!E52,'Sile i krakovi'!O106,+M107))","v":0},{"$f":"IF('Analiza i dimenzioniranje'!E42<'Analiza i dimenzioniranje'!E52,'Analiza i dimenzioniranje'!E42,+N104)","v":0.8},0,{"$f":"+N104","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!F44=\"\",0,+M107)","v":0},{"$f":"+L106","v":0.8},null,"Eprometno=",{"$f":"+T106","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!G40","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!I40","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!K40","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!M40","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!O40","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!Q40","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!S40","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!U40","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!W40","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!Y40","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!AA40","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!AC40","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!AE40","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!AG40","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!AI40","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!AK40","v":{"$error":"#VALUE!"}},null,0,{"$f":"+AM100","v":0.6},null,null,null,null,null,0,{"$f":"+AT100","v":0.8}]
["Sh1 (za MIII-III)",{"$f":"IF(C107=\"\",\"\",+C107/$B$99-$D$99/$B$99)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!D71","v":5},{"$error":"#VALUE!"},4.5,{"$f":"IF('Analiza i dimenzioniranje'!D$71=\"\",\"\",'Analiza i dimenzioniranje'!D$75*COS('Analiza i dimenzioniranje'!$E$39*PI()/180))","v":48.296291314453413},0,{"$f":"+H104","v":0.6},{"$f":"+I116","v":6},{"$f":"+J116","v":0},{"$f":"IF('Analiza i dimenzioniranje'!E42=0,0,+('Analiza i dimenzioniranje'!E42-'Sile i krakovi'!L104)*10)","v":8},0,{"$f":"IF('Analiza i dimenzioniranje'!F44=\"\",0,-IF('Analiza i dimenzioniranje'!F44<'Analiza i dimenzioniranje'!E52,0,+(N104-N105)*10))","v":0},{"$f":"+N104","v":1.2},{"$f":"+P105*10","v":8},0,null,"Etočkasto  =",{"$f":"+T107","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!G80","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!I80","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!K80","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!M80","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!O80","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!Q80","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!S80","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!U80","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!W80","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!Y80","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!AA80","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!AC80","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!AE80","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!AG80","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!AI80","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!AK80","v":{"$error":"#VALUE!"}},null,{"$f":"+AL106*10","v":6},0,null,null,null,null,null,{"$f":"+AS106*10","v":8},0]
["Sh2 (za MIII-III)",{"$f":"IF(C108=\"\",\"\",C108/$B$99-$D$99/$B$99)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E71","v":3},{"$error":"#VALUE!"},2.5,{"$f":"IF('Analiza i dimenzioniranje'!$E$71=\"\",\"\",'Analiza i dimenzioniranje'!E$75*COS('Analiza i dimenzioniranje'!$E$39*PI()/180))","v":48.296291314453413},{"$f":"+G107","v":0},{"$f":"+H104","v":0.6},{"$f":"+I117","v":0},{"$f":"+J117","v":0},{"$f":"+K104","v":0},{"$f":"+L107","v":0},{"$f":"+M107","v":0},{"$f":"+N104","v":1.2},{"$f":"+K108","v":0},0,null,"Elinijsko    = ",{"$f":"+T108","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!G120","v":{"$error":"#VALUE!"}},{"$f":"++'HT III-XX'!I120","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!K120","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!M120","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!O120","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!Q120","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!S120","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!U120","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!W120","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!Y120","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AA120","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AC120","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AE120","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AG120","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AI120","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AK120","v":{"$error":"#VALUE!"}},null,0,0,null,null,null,null,null,0,0]
["Sh3 (za MIII-III)",{"$f":"++IF(C109=\"\",\"\",C109/$B$99-$D$99/$B$99)","v":""},{"$f":"+'Analiza i dimenzioniranje'!F71","v":""},"","",{"$f":"IF('Analiza i dimenzioniranje'!$F$71=\"\",\"\",'Analiza i dimenzioniranje'!F$75*COS('Analiza i dimenzioniranje'!$E$39*PI()/180))","v":""},"A=",{"$f":"-IF('Analiza i dimenzioniranje'!E41=0,0,0.5*(+(G104*H105-G105*H104)+(G105*H106-G106*H105)+(G106*H107-G107*H106) +(G107*H108-G108*H107)))","v":0},"A=",{"$f":"-IF('Analiza i dimenzioniranje'!H46=0,0,0.5*(+(I104*J105-I105*J104)+(I105*J106-I106*J105)+(I106*J107-I107*J106) +(I107*J108-I108*J107)))","v":1.7999999999999998},"A=",{"$f":"IF('Analiza i dimenzioniranje'!$E$42=\"\",0,IF(-0.5*((K104*L105-K105*L104)+(K105*L106-K106*L105)+(K106*L107-K107*L106)+(K107*L108-K108*L107))<0,0,-0.5*((K105*L106-K106*L105)+(K106*L107-K107*L106)+(K107*L108-K108*L107))))","v":3.2},"A=",{"$f":"0.5*(+(M104*N105-M105*N104)+(M105*N106-M106*N105)+(M106*N107-M107*N106)+(M107*N108-M108*N107))","v":0},"A=",{"$f":"IF('Analiza i dimenzioniranje'!$E$42<=0,0,IF(-0.5*((O104*P105-O105*P104)+(O105*P106-O106*P105)+(O106*P107-O107*P106)+(O107*P108-O108*P107))<0,0,-0.5*((O105*P106-O106*P105)+(O106*P107-O107*P106)+(O107*P108-O108*P107))))","v":3.2},null,"Etemelja   =",{"$f":"+'HT III-XX'!G160","v":{"$error":"#VALUE!"}},{"$f":"+IF(T$94>'HT III-XX'!D$176,'HT III-XX'!G$160,IF(T$94>'HT III-XX'!D$216,'HT III-XX'!G$200,IF(T$94>'HT III-XX'!D$257,'HT III-XX'!G$240,IF(T$94>'HT III-XX'!D$296,'HT III-XX'!G$280,IF(T$94>'HT III-XX'!D$336,'HT III-XX'!G$320,IF(T$94>'HT III-XX'!D$376,'HT III-XX'!G$360,IF(T$94>'HT III-XX'!D$416,'HT III-XX'!G$400,IF(TT94>'HT III-XX'!D$456,'HT III-XX'!G$440,IF(T$94>'HT III-XX'!D$496,'HT III-XX'!G$480,IF(T$94>'HT III-XX'!D$536,'HT III-XX'!G$520,IF(T$94>'HT III-XX'!D$576,'HT III-XX'!G$560,IF(T$94>'HT III-XX'!D$616,'HT III-XX'!G$600,IF(T$94>'HT III-XX'!D$656,'HT III-XX'!G$640,IF(T$94>'HT III-XX'!D$687,'HT III-XX'!$G682,'HT III-XX'!$G$689))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Sile i krakovi'!U94>'HT III-XX'!D176,'HT III-XX'!I160,IF(U94>'HT III-XX'!D216,'HT III-XX'!I200,IF(U94>'HT III-XX'!D257,'HT III-XX'!I240,IF(U94>'HT III-XX'!D296,'HT III-XX'!I280,IF(U94>'HT III-XX'!D336,'HT III-XX'!I320,IF(U94>'HT III-XX'!D376,'HT III-XX'!I360,IF(U94>'HT III-XX'!D416,'HT III-XX'!I400,IF(U94>'HT III-XX'!D456,'HT III-XX'!I440,IF(U94>'HT III-XX'!D496,'HT III-XX'!I480,IF(U94>'HT III-XX'!D536,'HT III-XX'!I520,IF(U94>'HT III-XX'!D576,'HT III-XX'!I560,IF(U94>'HT III-XX'!D616,'HT III-XX'!I600,IF(U94>'HT III-XX'!D656,'HT III-XX'!I640,IF(U94>'HT III-XX'!D687,'HT III-XX'!G680,+'HT III-XX'!G687))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Sile i krakovi'!U94>'HT III-XX'!D176,'HT III-XX'!K160,IF(U94>'HT III-XX'!D216,'HT III-XX'!K200,IF(U94>'HT III-XX'!D257,'HT III-XX'!K240,IF(U94>'HT III-XX'!D296,'HT III-XX'!K280,IF(U94>'HT III-XX'!D336,'HT III-XX'!K320,IF(U94>'HT III-XX'!D376,'HT III-XX'!K360,IF(U94>'HT III-XX'!D416,'HT III-XX'!K400,IF(U94>'HT III-XX'!D456,'HT III-XX'!K440,IF(U94>'HT III-XX'!D496,'HT III-XX'!K480,IF(U94>'HT III-XX'!D536,'HT III-XX'!K520,IF(U94>'HT III-XX'!D576,'HT III-XX'!K560,IF(U94>'HT III-XX'!D616,'HT III-XX'!K600,IF(U94>'HT III-XX'!D656,'HT III-XX'!K640,IF(U94>'HT III-XX'!$D687,'HT III-XX'!G680,+'HT III-XX'!$G687))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Sile i krakovi'!W94>'HT III-XX'!$D176,'HT III-XX'!M160,IF(W94>'HT III-XX'!$D216,'HT III-XX'!M200,IF(W94>'HT III-XX'!$D257,'HT III-XX'!M240,IF(W94>'HT III-XX'!$D296,'HT III-XX'!M280,IF(W94>'HT III-XX'!$D336,'HT III-XX'!M320,IF(W94>'HT III-XX'!$D376,'HT III-XX'!M360,IF(W94>'HT III-XX'!$D416,'HT III-XX'!M400,IF(W94>'HT III-XX'!$D456,'HT III-XX'!M440,IF(W94>'HT III-XX'!$D496,'HT III-XX'!M480,IF(W94>'HT III-XX'!$D536,'HT III-XX'!M520,IF(W94>'HT III-XX'!DD576,'HT III-XX'!M560,IF(W94>'HT III-XX'!$D616,'HT III-XX'!M600,IF(W94>'HT III-XX'!$D656,'HT III-XX'!M640,IF(W94>'HT III-XX'!$D687,'HT III-XX'!$G680,+'HT III-XX'!$G687))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Sile i krakovi'!V94>'HT III-XX'!D176,'HT III-XX'!O160,IF(V94>'HT III-XX'!D216,'HT III-XX'!O200,IF(V94>'HT III-XX'!D257,'HT III-XX'!O240,IF(V94>'HT III-XX'!D296,'HT III-XX'!O280,IF(V94>'HT III-XX'!D336,'HT III-XX'!O320,IF(V94>'HT III-XX'!D376,'HT III-XX'!O360,IF(V94>'HT III-XX'!D416,'HT III-XX'!O400,IF(V94>'HT III-XX'!D456,'HT III-XX'!O440,IF(V94>'HT III-XX'!D496,'HT III-XX'!O480,IF(V94>'HT III-XX'!D536,'HT III-XX'!O520,IF(V94>'HT III-XX'!D576,'HT III-XX'!O560,IF(V94>'HT III-XX'!D616,'HT III-XX'!O600,IF(V94>'HT III-XX'!D656,'HT III-XX'!O640,IF(V94>'HT III-XX'!D687,'HT III-XX'!$G680,+'HT III-XX'!$G687))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Sile i krakovi'!X94>'HT III-XX'!$D176,'HT III-XX'!Q160,IF(X94>'HT III-XX'!$D216,'HT III-XX'!Q200,IF(X94>'HT III-XX'!$D257,'HT III-XX'!Q240,IF(X94>'HT III-XX'!$D296,'HT III-XX'!Q280,IF(X94>'HT III-XX'!$D336,'HT III-XX'!Q320,IF(X94>'HT III-XX'!$D376,'HT III-XX'!Q360,IF(X94>'HT III-XX'!$D416,'HT III-XX'!Q400,IF(X94>'HT III-XX'!$D456,'HT III-XX'!Q440,IF(X94>'HT III-XX'!$D496,'HT III-XX'!Q480,IF(X94>'HT III-XX'!$D536,'HT III-XX'!Q520,IF(X94>'HT III-XX'!$D576,'HT III-XX'!Q560,IF(X94>'HT III-XX'!$D616,'HT III-XX'!Q600,IF(X94>'HT III-XX'!$D656,'HT III-XX'!Q640,IF(X94>'HT III-XX'!$D687,'HT III-XX'!$G680,+'HT III-XX'!$G687))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Sile i krakovi'!W94>'HT III-XX'!$D176,'HT III-XX'!S160,IF(W94>'HT III-XX'!$D216,'HT III-XX'!S200,IF(W94>'HT III-XX'!$D257,'HT III-XX'!S240,IF(W94>'HT III-XX'!$D296,'HT III-XX'!S280,IF(W94>'HT III-XX'!$D336,'HT III-XX'!S320,IF(W94>'HT III-XX'!$D376,'HT III-XX'!S360,IF(W94>'HT III-XX'!$D416,'HT III-XX'!S400,IF(W94>'HT III-XX'!$D456,'HT III-XX'!S440,IF(W94>'HT III-XX'!$D496,'HT III-XX'!S480,IF(W94>'HT III-XX'!$D536,'HT III-XX'!S520,IF(W94>'HT III-XX'!$D576,'HT III-XX'!S560,IF(W94>'HT III-XX'!$D616,'HT III-XX'!S600,IF(W94>'HT III-XX'!$D656,'HT III-XX'!S640,IF(W94>'HT III-XX'!$D687,'HT III-XX'!$G680,+'HT III-XX'!$G687))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Sile i krakovi'!X94>'HT III-XX'!$D176,'HT III-XX'!U160,IF(X94>'HT III-XX'!$D216,'HT III-XX'!U200,IF(X94>'HT III-XX'!$D257,'HT III-XX'!U240,IF(X94>'HT III-XX'!$D296,'HT III-XX'!U280,IF(X94>'HT III-XX'!$D336,'HT III-XX'!U320,IF(X94>'HT III-XX'!$D376,'HT III-XX'!U360,IF(X94>'HT III-XX'!$D416,'HT III-XX'!U400,IF(X94>'HT III-XX'!$D456,'HT III-XX'!U440,IF(X94>'HT III-XX'!$D496,'HT III-XX'!U480,IF(X94>'HT III-XX'!$D536,'HT III-XX'!U520,IF(X94>'HT III-XX'!$D576,'HT III-XX'!U560,IF(X94>'HT III-XX'!$D616,'HT III-XX'!U600,IF(X94>'HT III-XX'!$D656,'HT III-XX'!U640,IF(X94>'HT III-XX'!$D687,'HT III-XX'!$G680,+'HT III-XX'!$G687))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Sile i krakovi'!Y94>'HT III-XX'!$D176,'HT III-XX'!W160,IF(Y94>'HT III-XX'!$D216,'HT III-XX'!W200,IF(Y94>'HT III-XX'!$D257,'HT III-XX'!W240,IF(Y94>'HT III-XX'!$D296,'HT III-XX'!W280,IF(Y94>'HT III-XX'!$D336,'HT III-XX'!W320,IF(Y94>'HT III-XX'!$D376,'HT III-XX'!W360,IF(Y94>'HT III-XX'!$D416,'HT III-XX'!W400,IF(Y94>'HT III-XX'!$D456,'HT III-XX'!W440,IF(Y94>'HT III-XX'!$D496,'HT III-XX'!W480,IF(Y94>'HT III-XX'!$D536,'HT III-XX'!W520,IF(Y94>'HT III-XX'!$D576,'HT III-XX'!W560,IF(Y94>'HT III-XX'!$D616,'HT III-XX'!W600,IF(Y94>'HT III-XX'!$D656,'HT III-XX'!W640,IF(Y94>'HT III-XX'!$D687,'HT III-XX'!$G680,+'HT III-XX'!$G687))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Sile i krakovi'!Z94>'HT III-XX'!$D176,'HT III-XX'!Y160,IF(Z94>'HT III-XX'!$D216,'HT III-XX'!Y200,IF(Z94>'HT III-XX'!$D257,'HT III-XX'!Y240,IF(Z94>'HT III-XX'!$D296,'HT III-XX'!Y280,IF(Z94>'HT III-XX'!$D336,'HT III-XX'!Y320,IF(Z94>'HT III-XX'!$D376,'HT III-XX'!Y360,IF(Z94>'HT III-XX'!$D416,'HT III-XX'!Y400,IF(Z94>'HT III-XX'!$D456,'HT III-XX'!Y440,IF(Z94>'HT III-XX'!$D496,'HT III-XX'!Y480,IF(Z94>'HT III-XX'!$D536,'HT III-XX'!Y520,IF(Z94>'HT III-XX'!$D576,'HT III-XX'!Y560,IF(Z94>'HT III-XX'!$D616,'HT III-XX'!Y600,IF(Z94>'HT III-XX'!$D656,'HT III-XX'!Y640,IF(Z94>'HT III-XX'!$D687,'HT III-XX'!$G680,+'HT III-XX'!$G687))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Sile i krakovi'!Z94>'HT III-XX'!$D176,'HT III-XX'!AA160,IF(Z94>'HT III-XX'!$D216,'HT III-XX'!AA200,IF(Z94>'HT III-XX'!$D257,'HT III-XX'!AA240,IF(Z94>'HT III-XX'!$D296,'HT III-XX'!AA280,IF(Z94>'HT III-XX'!$D336,'HT III-XX'!AA320,IF(Z94>'HT III-XX'!$D376,'HT III-XX'!AA360,IF(Z94>'HT III-XX'!$D416,'HT III-XX'!AA400,IF(Z94>'HT III-XX'!$D456,'HT III-XX'!AA440,IF(Z94>'HT III-XX'!$D496,'HT III-XX'!AA480,IF(Z94>'HT III-XX'!$D536,'HT III-XX'!AA520,IF(Z94>'HT III-XX'!$D576,'HT III-XX'!AA560,IF(Z94>'HT III-XX'!$D616,'HT III-XX'!AA600,IF(Z94>'HT III-XX'!$D656,'HT III-XX'!Y640,IF(Z94>'HT III-XX'!$D687,'HT III-XX'!$G680,+'HT III-XX'!$G687))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Sile i krakovi'!AC94>'HT III-XX'!$D176,'HT III-XX'!AC160,IF(AC94>'HT III-XX'!$D216,'HT III-XX'!AC200,IF(AC94>'HT III-XX'!$D257,'HT III-XX'!AC240,IF(AC94>'HT III-XX'!$D296,'HT III-XX'!AC280,IF(AC94>'HT III-XX'!$D336,'HT III-XX'!AC320,IF(AC94>'HT III-XX'!$D376,'HT III-XX'!AC360,IF(AC94>'HT III-XX'!$D416,'HT III-XX'!AC400,IF(AC94>'HT III-XX'!$D456,'HT III-XX'!AC440,IF(AC94>'HT III-XX'!$D496,'HT III-XX'!AC480,IF(AC94>'HT III-XX'!$D536,'HT III-XX'!AC520,IF(AC94>'HT III-XX'!$D576,'HT III-XX'!AC560,IF(AC94>'HT III-XX'!$D616,'HT III-XX'!AC600,IF(AC94>'HT III-XX'!$D656,'HT III-XX'!AC640,IF(AC94>'HT III-XX'!$D680,'HT III-XX'!$G687,+'HT III-XX'!$G687))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Sile i krakovi'!AD94>'HT III-XX'!$D176,'HT III-XX'!AE160,IF(AD94>'HT III-XX'!$D216,'HT III-XX'!AE200,IF(AD94>'HT III-XX'!$D257,'HT III-XX'!AE240,IF(AD94>'HT III-XX'!$D296,'HT III-XX'!AE280,IF(AD94>'HT III-XX'!$D336,'HT III-XX'!AE320,IF(AE94>'HT III-XX'!$D376,'HT III-XX'!AE360,IF(AD94>'HT III-XX'!$D416,'HT III-XX'!AE400,IF(AD94>'HT III-XX'!$D456,'HT III-XX'!AE440,IF(AD94>'HT III-XX'!$D496,'HT III-XX'!AE480,IF(AD94>'HT III-XX'!$D536,'HT III-XX'!AE520,IF(AD94>'HT III-XX'!$D576,'HT III-XX'!AE560,IF(AD94>'HT III-XX'!$D616,'HT III-XX'!AE600,IF(AD94>'HT III-XX'!$D656,'HT III-XX'!AE640,IF(AD94>'HT III-XX'!$D687,'HT III-XX'!$G680,+'HT III-XX'!$G687))))))))))))))","v":0},{"$f":"+IF('Sile i krakovi'!AE94>'HT III-XX'!$D176,'HT III-XX'!AI160,IF(AE94>'HT III-XX'!$D216,'HT III-XX'!AI200,IF(AE94>'HT III-XX'!$D257,'HT III-XX'!AI240,IF(AE94>'HT III-XX'!$D296,'HT III-XX'!AI280,IF(AE94>'HT III-XX'!$D336,'HT III-XX'!AI320,IF(AF94>'HT III-XX'!$D376,'HT III-XX'!AI360,IF(AE94>'HT III-XX'!$D416,'HT III-XX'!AI400,IF(AE94>'HT III-XX'!$D456,'HT III-XX'!AI440,IF(AE94>'HT III-XX'!$D496,'HT III-XX'!AI480,IF(AE94>'HT III-XX'!$D536,'HT III-XX'!AI520,IF(AE94>'HT III-XX'!$D576,'HT III-XX'!AI560,IF(AE94>'HT III-XX'!$D616,'HT III-XX'!AI600,IF(AE94>'HT III-XX'!$D656,'HT III-XX'!AH640,IF(AE94>'HT III-XX'!$D687,'HT III-XX'!$G680,+'HT III-XX'!$G687))))))))))))))","v":0},{"$f":"+IF('Sile i krakovi'!AE94>'HT III-XX'!$D176,'HT III-XX'!AK160,IF(AE94>'HT III-XX'!$D216,'HT III-XX'!AK200,IF(AE94>'HT III-XX'!$D257,'HT III-XX'!AK240,IF(AE94>'HT III-XX'!$D296,'HT III-XX'!AK280,IF(AE94>'HT III-XX'!$D336,'HT III-XX'!AK320,IF(AF94>'HT III-XX'!$D376,'HT III-XX'!AK360,IF(AE94>'HT III-XX'!$D416,'HT III-XX'!AK400,IF(AE94>'HT III-XX'!$D456,'HT III-XX'!AK440,IF(AE94>'HT III-XX'!$D496,'HT III-XX'!AK480,IF(AE94>'HT III-XX'!$D536,'HT III-XX'!AK520,IF(AE94>'HT III-XX'!$D576,'HT III-XX'!AK560,IF(AE94>'HT III-XX'!$D616,'HT III-XX'!AK600,IF(AE94>'HT III-XX'!$D656,'HT III-XX'!AK640,IF(AE94>'HT III-XX'!$D687,'HT III-XX'!$G680,+'HT III-XX'!$G687))))))))))))))","v":0},0]
["Sh4 (za MIII-III)",{"$f":"+IF(C110=\"\",\"\",C110/$B$99-$D$99/$B$99)","v":""},{"$f":"+'Analiza i dimenzioniranje'!G71","v":""},"","",{"$f":"IF('Analiza i dimenzioniranje'!$G$71=\"\",\"\",'Analiza i dimenzioniranje'!G$75*COS('Analiza i dimenzioniranje'!$E$39*PI()/180))","v":""},"x=",{"$f":"IF(H109=0,0,-((G104*H105-G105*H104)*(G104+G105)+(G105*H106-G106*H105)*(G105+G106)+(G106*H107-G107*H106)*(G106+G107)+(G107*H108-G108*H107)*(G107+G108))/6/H109)","v":0},"x=",{"$f":"IF(J109=0,0,-((I104*J105-I105*J104)*(I104+I105)+(I105*J106-I106*J105)*(I105+I106)+(I106*J107-I107*J106)*(I106+I107)+(I107*J108-I108*J107)*(I107+I108))/6/J109)","v":2},"x=",{"$f":"IF(L109=0,0,-((K104*L105-K105*L104)*(K104+K105)+(K105*L106-K106*L105)*(K105+K106)+(K106*L107-K107*L106)*(K106+K107)+(K107*L108-K108*L107)*(K107+K108))/6/L109)","v":2.6666666666666665},"x=",{"$f":"IF(N109=0,0,IF('Analiza i dimenzioniranje'!E42<='Analiza i dimenzioniranje'!E52,0,((M104*N105-M105*N104)*(M104+M105)+(M105*N106-M106*N105)*(M105+M106)+(M106*N107-M107*N106)*(M106+M107)+(M107*N108-M108*N107)*(M107+M107))/6/N109))","v":0},"x=",{"$f":"IF(P109=0,0,-((O104*P105-O105*P104)*(O104+O105)+(O105*P106-O106*P105)*(O105+O106)+(O106*P107-O107*P106)*(O106+O107)+(O107*P108-O108*P107)*(O107+O108))/6/P109)","v":2.6666666666666665},null,"E voda iza    =",{"$f":"+H109","v":0},{"$f":"$AO114","v":0},{"$f":"$AO115","v":0},{"$f":"$AO116","v":0},{"$f":"$AO117","v":0},{"$f":"$AO118","v":0},{"$f":"$AO119","v":0},{"$f":"$AO120","v":0},{"$f":"$AO121","v":0},{"$f":"$AO122","v":0},{"$f":"$AO123","v":0},{"$f":"$AO124","v":0},{"$f":"$AO125","v":0},{"$f":"$AO126","v":0},{"$f":"$AO127","v":0},{"$f":"$AO128","v":0},{"$f":"$AO129","v":0},null,null,null,null,"visina vode od presjeka do vrha vode",null,"koord. težišta",null,null,null,null,"visina vode od presjeka do vrha vode",null,"koord. težišta"]
["Voda izvan zida",{"$f":"+D105","v":4.9000021999999994},{"$f":"+P111","v":0.26666666666666672},0,-0.23333333333333328,{"$f":"+P109","v":3.2},"Y=",{"$f":"IF(H109=0,0,-((G104*H105-G105*H104)*(H104+H105)+(G105*H106-G106*H105)*(H105+H106)+(G106*H107-G107*H106)*(H106+H107)+(G107*H108-G108*H107)*(H107+H108))/6/H109)","v":0},"Y=",{"$f":"IF(J109=0,0,-((I104*J105-I105*J104)*(J104+J105)+(I105*J106-I106*J105)*(J105+J106)+(I106*J107-I107*J106)*(J106+J107)+(I107*J108-I108*J107)*(J107+J108))/6/J109)","v":0.19999999999999998},"Y=",{"$f":"IF(L109=0,0,-((K104*L105-K105*L104)*(L104+L105)+(K105*L106-K106*L105)*(L105+L106)+(K106*L107-K107*L106)*(L106+L107)+(K107*L108-K108*L107)*(L107+L108))/6/L109)","v":0.26666666666666672},"Y=",{"$f":"IF('Analiza i dimenzioniranje'!E43>0,0,IF('Analiza i dimenzioniranje'!E42<='Analiza i dimenzioniranje'!E52,0,((M104*N105-M105*N104)*(N104+N105)+(M105*N106-M106*N105)*(N105+N106)+(M106*N107-M107*N106)*(N106+N107)+(M107*N108-M108*N107)*(N107+N108))/6/N109))","v":{"$error":"#VALUE!"}},"Y=",{"$f":"IF(P109=0,0,-((O104*P105-O105*P104)*(P104+P105)+(O105*P106-O106*P105)*(P105+P106)+(O106*P107-O107*P106)*(P106+P107)+(O107*P108-O108*P107)*(P107+P108))/6/P109)","v":0.26666666666666672},null,"Hpotres    =",{"$f":"+F226","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AE114","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!$AC$114","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!$AE$114","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!$AC$114","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!$AE$114","v":{"$error":"#VALUE!"}},{"$f":"'C X-XI'!AC114","v":{"$error":"#VALUE!"}},{"$f":"'C X-XI'!AE114","v":{"$error":"#VALUE!"}},{"$f":"'C XII-XIII'!AC114","v":{"$error":"#VALUE!"}},{"$f":"'C XII-XIII'!AE114","v":{"$error":"#VALUE!"}},{"$f":"'C XIV-XV'!AC114","v":{"$error":"#VALUE!"}},{"$f":"'C XIV-XV'!AE114","v":{"$error":"#VALUE!"}},{"$f":"'C XVI-XVII'!AC114","v":{"$error":"#VALUE!"}},{"$f":"'C XVI-XVII'!AE114","v":{"$error":"#VALUE!"}},{"$f":"'C XVIII-XIX'!AC114","v":{"$error":"#VALUE!"}},{"$f":"'C XVIII-XIX'!AE114","v":{"$error":"#VALUE!"}},0,null,"oznaka ","Presjeci za krakove y",null,null,"Tlak vode",null,null,"oznaka ","Presjeci za krakove y",null,null,"Tlak vode"]
["Eh1 (za MIII-III)",{"$f":"+$C112/$B$85-$D$85/$B$85","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!$B$87","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Pritisak vode iza zida\nod 0 do III-III",null,"Pritisak vode\nod 0 do I-I",null,"Voda ispred zida razdjeljena\nod 0 do A                        od A do III-III",null,null,null,null,"SH=",{"$f":"SUM(S98:S111)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,null,"presjeka","intezitet","y",null,null,"y",null,"presjeka","intezitet","y",null,null,"y"]
["Eh2 (za MIII-III)",{"$f":"+$C113/$B$85-$D$85/$B$85","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!$D$87","v":{"$error":"#VALUE!"}},null,null,null,null,null,0,0,null,null,0,0,0,{"$f":"+P114","v":0.41025631985540933},null,"Vertikalni krakovi od vrha temalja do težišta horizontalnih sila\n                                     \n                                   SILA",null,"PIII","PVI","PVII","PVIII","PIX","PX","P XI","P XII","P XIII","P XIV","PXV","PXVI","PXVII","PXVIII","PXIX","PXX",null,"presjek na  koti 0",{"$f":"IF(+AN113*10<=0,0,AN113*10)","v":6},0,{"$f":"+$AL$106-AM113","v":0.6},{"$f":"+AL113*AN113/2-AO114","v":1.7999999999999998},{"$f":"IF(AL113=0,0,+AN113/3)","v":0.19999999999999998},null,"presjek na  koti 0",{"$f":"IF(+AU113*10<=0,0,AU113*10)","v":8},0,{"$f":"+$AS$106-AT113","v":0.8},{"$f":"+AS113*AU113/2-AV114","v":3.2},{"$f":"IF(AS113=0,0,+AU113/3)","v":0.26666666666666666}]
["Eh3 (za MIII-III)",{"$f":"2","v":2},{"$f":"+'C III-V'!$F$87","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!C112","v":{"$error":"#VALUE!"}},null,null,0,{"$f":"IF('Analiza i dimenzioniranje'!E41>'Analiza i dimenzioniranje'!E52,'Analiza i dimenzioniranje'!E52,+'Analiza i dimenzioniranje'!E41)","v":0.6},null,null,0,{"$f":"+'Analiza i dimenzioniranje'!E52-'Analiza i dimenzioniranje'!C191","v":0.41025631985540933},{"$f":"IF('Analiza i dimenzioniranje'!E42=0,0,+M115)","v":3.8974368014459069},{"$f":"+N115","v":0.41025631985540933},null,null,null,{"$f":"+T97","v":1.2},1.52,1.84,2.16,2.48,2.8,3.14,3.44,3.76,4.08,4.4000000000000004,4.72,5.04,5.36,5.6800000000000006,6,null,"III-III",{"$f":"IF(AN114*10<0,0,AN114*10)","v":0},{"$f":"+T97","v":1.2},{"$f":"IF(+$AL$106-AM114<0,0,+$AL$106-AM114)","v":0},{"$f":"+AN114*10*AN114/2","v":0},0,null,"III-III",{"$f":"IF(AU114*10<0,0,AU114*10)","v":0},{"$f":"+AM114","v":1.2},{"$f":"IF(+$AS$106-AT114<0,0,+$AS$106-AT114)","v":0},{"$f":"+AU114*10*AU114/2","v":0},0]
["Eprometno (III-III)",{"$f":"IF('Analiza i dimenzioniranje'!E24=0,0,+C115/$B$85-$D$85/$B$85)","v":{"$error":"#REF!"}},{"$f":"IF(A115=0,0,#REF!)","v":{"$error":"#REF!"}},null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!$E41<'Analiza i dimenzioniranje'!$E52,0,+('Analiza i dimenzioniranje'!$E41-'Analiza i dimenzioniranje'!$E52)*10)","v":0},{"$f":"+J114","v":0.6},null,null,{"$f":"+O107-N115*10","v":3.8974368014459069},{"$f":"+N114","v":0.41025631985540933},{"$f":"+O106","v":0},{"$f":"+P106","v":0.8},null,null,null,{"$f":"+T96","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,"VI",0,{"$f":"+U97","v":1.52},0,0,0,null,"VI",0,1.52,0,0,0]
["EPTočkasto (III-III)",{"$f":"IF('Analiza i dimenzioniranje'!E36=0,0,+C116/$B$85-$D$85/$B$85)","v":{"$error":"#REF!"}},{"$f":"IF(A116=0,0,#REF!)","v":{"$error":"#REF!"}},null,null,null,null,null,{"$f":"'Analiza i dimenzioniranje'!E41*10","v":6},0,null,null,{"$f":"+O107","v":8},{"$f":"+P107","v":0},0,{"$f":"+P115","v":0.8},null,"Sh1=",{"$f":"+C107","v":5},{"$f":"IF(IF($S116=\"\",0,+$S116-T$114)<0,0,IF($S$116=\"\",0,+$S116-T$114))","v":3.8},{"$f":"IF(IF($S$116=\"\",0,+$S116-U$114)<0,0,IF($S$116=\"\",0,+$S116-U$114))","v":3.48},3.16,2.84,2.52,2.2000000000000002,1.8599999999999999,1.56,1.2400000000000002,0.91999999999999993,0.59999999999999964,0.28000000000000025,0,0,0,0,null,"VII",0,{"$f":"+V97","v":1.84},0,0,0,null,"VII",0,1.84,0,0,0]
["EPLinijsko  (III-III)",{"$f":"IF('Analiza i dimenzioniranje'!E34=0,0,+C117/$B$85-$D$85/$B$85)","v":{"$error":"#REF!"}},{"$f":"IF(A117=0,0,#REF!-('Analiza i dimenzioniranje'!E52-'Analiza i dimenzioniranje'!E51))","v":{"$error":"#REF!"}},null,null,null,null,null,{"$f":"+I113","v":0},0,null,null,{"$f":"+M113","v":0},{"$f":"+N113","v":0},0,{"$f":"+P113","v":0.41025631985540933},null,"Sh2=",{"$f":"+C108","v":3},{"$f":"IF(IF($S117=\"\",0,+$S117-T$114)<0,0,IF($S$117=\"\",0,+$S117-T$114))","v":1.8},1.48,1.1599999999999999,0.83999999999999986,0.52,0.20000000000000018,0,0,0,0,0,0,0,0,0,0,null,"VIII",0,{"$f":"+W97","v":2.16},0,0,0,null,"VIII",0,2.16,0,0,0]
["EQTemelj(EIII-III)",{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,+C118/$B$85-$D$85/$B$85)","v":{"$error":"#REF!"}},{"$f":"IF(A118=0,0,#REF!-('Analiza i dimenzioniranje'!E52-'Analiza i dimenzioniranje'!E51))","v":{"$error":"#REF!"}},null,null,null,null,null,"A=",{"$f":"IF('Analiza i dimenzioniranje'!E41<=0,0,IF(-0.5*((I113*J114-I114*J113)+(I114*J115-I115*J114)+(I115*J116-I116*J115)+(I116*J117-I117*J116))<0,0,-0.5*((I114*J115-I115*J114)+(I115*J116-I116*J115)+(I116*J117-I117*J116))))","v":1.7999999999999998},null,null,"A=",{"$f":"IF('Analiza i dimenzioniranje'!$E$42=\"\",0,IF(-0.5*((M113*N114-M114*N113)+(M114*N115-M115*N114)+(M115*N116-M116*N115)+(M116*N117-M117*N116))<0,0,-0.5*((M114*N115-M115*N114)+(M115*N116-M116*N115)+(M116*N117-M117*N116))))","v":2.4404993189367552},"A=",{"$f":"(0.5*((O113*P114-O114*P113)+(O114*P115-O115*P114)+(O115*P116-O116*P115)+(O116*P117-O117*P116)))","v":0.75950068106324509},null,"Sh3=",{"$f":"+C109","v":""},{"$f":"IF(IF($S118=\"\",0,+$S118-T$114)<0,0,IF($S118=\"\",0,+$S118-T$114))","v":0},{"$f":"IF(IF($S118=\"\",0,+$S118-U$114)<0,0,IF($S118=\"\",0,+$S118-U$114))","v":0},{"$f":"IF(IF($S118=\"\",0,+$S118-V$114)<0,0,IF($S$118=\"\",0,+$S118-V$114))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,null,"IX",0,{"$f":"+X97","v":2.48},0,0,0,null,"IX",0,2.48,0,0,0]
["Evoda (I-I)",{"$f":"2","v":2},{"$f":"+'Analiza i dimenzioniranje'!$E$41/3","v":0.19999999999999998},null,null,{"$f":"+J118","v":1.7999999999999998},null,null,"x=",{"$f":"IF(J118=0,0,-((I113*J114-I114*J113)*(I113+I114)+(I114*J115-I115*J114)*(I114+I115)+(I115*J116-I116*J115)*(I115+I116)+(I116*J117-I117*J116)*(I116+I117))/6/J118)","v":2},null,null,"x=",{"$f":"IF(N118=0,0,-((M113*N114-M114*N113)*(M113+M114)+(M114*N115-M115*N114)*(M114+M115)+(M115*N116-M116*N115)*(M115+M116)+(M116*N117-M117*N116)*(M116+M117))/6/N118)","v":3.0922489125113861},"x=",{"$f":"IF(P118=0,0,((O113*P114-O114*P113)*(O113+O114)+(O114*P115-O115*P114)*(O114+O115)+(O115*P116-O116*P115)*(O115+O116)+(O116*P117-O117*P116)*(O116+O117))/6/P118)","v":1.2991456004819688},null,"Sh4=",{"$f":"+C110","v":""},{"$f":"IF(IF($S119=\"\",0,+$S119-T$114)<0,0,IF($S119=\"\",0,+$S119-T$114))","v":0},{"$f":"IF(IF($S119=\"\",0,+$S119-U$114)<0,0,IF($S119=\"\",0,+$S119-U$114))","v":0},{"$f":"IF(IF($S119=\"\",0,+$S119-V$114)<0,0,IF($S119=\"\",0,+$S119-V$114))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,null,"X",0,{"$f":"+Y97","v":2.8},0,0,0,null,"X",0,2.8,0,0,0]
["Hpotres  (III-III)",{"$f":"+'C III-V'!Y112","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Y113","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Y=",{"$f":"IF(J118=0,0,-((I113*J114-I114*J113)*(J113+J114)+(I114*J115-I115*J114)*(J114+J115)+(I115*J116-I116*J115)*(J115+J116)+(I116*J117-I117*J116)*(J116+J117))/6/J118)","v":0.19999999999999998},null,null,"Y=",{"$f":"IF(N118=0,0,-((M113*N114-M114*N113)*(N113+N114)+(M114*N115-M115*N114)*(N114+N115)+(M115*N116-M116*N115)*(N115+N116)+(M116*N117-M117*N116)*(N116+N117))/6/N118)","v":0.18155021749772274},"Y=",{"$f":"IF(P118=0,0,((O113*P114-O114*P113)*(P113+P114)+(O114*P115-O115*P114)*(P114+P115)+(O115*P116-O116*P115)*(P115+P116)+(O116*P117-O117*P116)*(P116+P117))/6/P118)","v":0.54017087990360635},null,"Voda ispred =",{"$f":"IF('Analiza i dimenzioniranje'!F44=\"\",0,+'Analiza i dimenzioniranje'!F44)","v":0.8},{"$f":"IF('Analiza i dimenzioniranje'!E42<'Analiza i dimenzioniranje'!E52,0,+$N$111-T114)","v":0},{"$f":"+IF($S$120>U$114,($S$120-U$114)/3,0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,"XI",0,{"$f":"+Z97","v":3.14},0,0,0,null,"XI",0,3.14,0,0,0]
[null,"hb=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},null,"x","y","x","y","x","y","x","y","x","y",null,"Eh1=",{"$f":"+'C III-V'!C76","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-T$114<0,0,'C III-V'!B87-T114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-U$114<0,0,'C VI-VII'!I87-U114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-V$114<0,0,'C VI-VII'!N87-V114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-W$114<0,0,'C VIII-IX'!I87-W114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-X$114<0,0,'C VIII-IX'!N87-X114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-Y$114<0,0,'C X-XI'!$I$87-Y114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-Z$114<0,0,'C X-XI'!$N$87-Z114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-AA$114<0,0,'C XII-XIII'!$I$87-AA114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-AB$114<0,0,'C XII-XIII'!N87-AB114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-AC$114<0,0,'C XIV-XV'!$I$87-AC114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-AD$114<0,0,'C XIV-XV'!N87-AD114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-AE$114<0,0,'C XVI-XVII'!$I$87-AE114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-AF$114<0,0,'C XVI-XVII'!N87-AF114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-AG$114<0,0,'C XVIII-XIX'!$I$87-AG114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-AH$114<0,0,'C XVIII-XIX'!$N$87-AH114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S121-AI114<0,0,AH121-'Analiza i dimenzioniranje'!$X$53)","v":{"$error":"#VALUE!"}},null,"XX",0,{"$f":"+AA97","v":3.44},0,0,0,null,"XX",0,3.44,0,0,0]
["koordinate sila i kraka vode  -  samo voda iznad nivoa temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eh2=",{"$f":"+'C III-V'!E76","v":{"$error":"#VALUE!"}},{"$f":"+IF($S122-T$114<0,0,'C III-V'!D87-T114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S122-U$114<0,0,'C VI-VII'!K87-U114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S122-V$114<0,0,'C VI-VII'!P87-V114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S122-W$114<0,0,'C VIII-IX'!K87-W114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S122-X$114<0,0,'C VIII-IX'!P87-X114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S122-Y$114<0,0,'C X-XI'!$K$87-Y114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S122-Z$114<0,0,'C X-XI'!$P$87-Z114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S122-AA$114<0,0,'C XII-XIII'!$K$87-AA114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S122-AB$114<=0,0,'C XII-XIII'!$P$87-AB114)","v":{"$error":"#VALUE!"}},{"$f":"+IF($S122-AC$114<=0,0,'C XIV-XV'!$K$87-AC114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S122-AD$114<0,0,'C XIV-XV'!$P$87-AD114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S122-AE$114<0,0,'C XVI-XVII'!$K$87-AE114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S122-AF$114<0,0,'C XVI-XVII'!P87-AF114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S122-AG$114<0,0,'C XVIII-XIX'!$K$87-AG114)","v":{"$error":"#VALUE!"}},{"$f":"IF($S122-AH$114<0,0,'C XVIII-XIX'!$P$87-AH114)","v":{"$error":"#VALUE!"}},0,null,"XIII",0,{"$f":"+AB97","v":3.76},0,0,0,null,"XIII",0,3.76,0,0,0]
["Evoda",{"$f":"+B119+'Analiza i dimenzioniranje'!E59","v":3.4000000999999997},{"$f":"+('Analiza i dimenzioniranje'!E41-'Analiza i dimenzioniranje'!E52)/3+'Analiza i dimenzioniranje'!E52","v":1},{"$f":"IF(B123=\"\",\"\",$D$105-B123)","v":1.5000020999999997},{"$f":"C123/3+('Analiza i dimenzioniranje'!E52-'Analiza i dimenzioniranje'!E51)","v":0.83333333333333326},{"$f":"+AO114","v":0},null,null,null,null,null,null,null,null,null,null,null,"Eprometno=",{"$f":"+S106","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!G41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!I41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!K41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!M41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!O41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!Q41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!S41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!U41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!W41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!Y41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AA41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AC41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AE41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AG41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AI41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AK41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},null,"XIV",0,{"$f":"+AC97","v":4.08},0,0,0,null,"XIV",0,4.08,0,0,0]
["Ewater izvan",{"$f":"IF('Analiza i dimenzioniranje'!F44=\"\",0,IF('Analiza i dimenzioniranje'!F44=0,0,2+'Analiza i dimenzioniranje'!E59+'Analiza i dimenzioniranje'!E55))","v":4.2000000999999996},{"$f":"IF('Analiza i dimenzioniranje'!F44=\"\",0,('Analiza i dimenzioniranje'!F44-'Analiza i dimenzioniranje'!E52)/3+'Analiza i dimenzioniranje'!E52)","v":1.0666666666666667},{"$f":"IF(B124=\"\",\"\",$D$105-B124)","v":0.70000209999999985},{"$f":"+C123/3+('Analiza i dimenzioniranje'!E52-'Analiza i dimenzioniranje'!E51)","v":0.83333333333333326},{"$f":"+AV114","v":0},null,null,null,"x","y",null,null,null,null,null,null,"Etočkasto  =",{"$f":"+S107","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!G81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!I81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!K81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!M81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!O81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!Q81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!S81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!U81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!W81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!Y81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AA81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AC81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AE81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AG81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AI81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AK81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},null,"XV",0,{"$f":"+AD97","v":4.4000000000000004},0,0,0,null,"XV",0,4.4000000000000004,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Elinijsko    = ",{"$f":"+S108","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!G121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!I121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!K121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!M121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!O121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!Q121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!S121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!U121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!W121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!Y121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AA121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AC121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AE121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AG121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AI121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},{"$f":"+'HT III-XX'!AK121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},null,"XVI",0,{"$f":"+AE97","v":4.72},0,0,0,null,"XVI",0,4.72,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Etemelja   =",null,{"$f":"+IF(T$94>'HT III-XX'!$D$176,'HT III-XX'!$G$161,IF(T$94>'HT III-XX'!$D$216,'HT III-XX'!$G$201,IF(T$94>'HT III-XX'!$D$257,'HT III-XX'!$G$241,IF(T$94>'HT III-XX'!$D$296,'HT III-XX'!$G$281,IF(T$94>'HT III-XX'!$D$336,'HT III-XX'!$G$321,IF(T$94>'HT III-XX'!$D$376,'HT III-XX'!$G$361,IF(T$94>'HT III-XX'!$D$416,'HT III-XX'!$G$401,IF(T$94>'HT III-XX'!$D$456,'HT III-XX'!$G$441,IF(T$94>'HT III-XX'!$D$496,'HT III-XX'!$G$481,IF(T$94>'HT III-XX'!$D$536,'HT III-XX'!$G$521,IF(T$94>'HT III-XX'!$D$576,'HT III-XX'!$G$561,IF(T$94>'HT III-XX'!$D$616,'HT III-XX'!$G$601,IF(T$94>'HT III-XX'!$D$656,'HT III-XX'!$G$641,IF(T$94>'HT III-XX'!$D$687,'HT III-XX'!$G$699,'HT III-XX'!$G$689))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(U$94>'HT III-XX'!$D$176,'HT III-XX'!I$161,IF(U$94>'HT III-XX'!D$216,'HT III-XX'!I$201,IF(U$94>'HT III-XX'!D$257,'HT III-XX'!I$241,IF(U$94>'HT III-XX'!$D$296,'HT III-XX'!I$281,IF(U$94>'HT III-XX'!$D$336,'HT III-XX'!I$312,IF(U$94>'HT III-XX'!$D$376,'HT III-XX'!I$361,IF(U$94>'HT III-XX'!$D$416,'HT III-XX'!I$401,IF(U94>'HT III-XX'!$D$456,'HT III-XX'!I$441,IF(U$94>'HT III-XX'!$D$496,'HT III-XX'!I$481,IF(U$94>'HT III-XX'!$D$536,'HT III-XX'!I$521,IF(U$94>'HT III-XX'!$D$576,'HT III-XX'!I$561,IF(U$94>'HT III-XX'!$D$616,'HT III-XX'!I$601,IF(U$94>'HT III-XX'!$D$656,'HT III-XX'!I$641,IF(U$94>'HT III-XX'!$D$687,'HT III-XX'!$G692,'HT III-XX'!$G$688))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(V$94>'HT III-XX'!$D$176,'HT III-XX'!K$161,IF(V$94>'HT III-XX'!D$216,'HT III-XX'!K$201,IF(V$94>'HT III-XX'!D$257,'HT III-XX'!K$241,IF(V$94>'HT III-XX'!$D$296,'HT III-XX'!K$281,IF(V$94>'HT III-XX'!$D$336,'HT III-XX'!K$321,IF(V$94>'HT III-XX'!$D$376,'HT III-XX'!K$361,IF(V$94>'HT III-XX'!$D$416,'HT III-XX'!K$401,IF(V94>'HT III-XX'!$D$456,'HT III-XX'!K$441,IF(V$94>'HT III-XX'!$D$496,'HT III-XX'!K$481,IF(V$94>'HT III-XX'!$D$536,'HT III-XX'!K$521,IF(V$94>'HT III-XX'!$D$576,'HT III-XX'!K$561,IF(V$94>'HT III-XX'!$D$616,'HT III-XX'!K$601,IF(V$94>'HT III-XX'!$D$656,'HT III-XX'!K641,IF(V$94>'HT III-XX'!$D$687,'HT III-XX'!$G692,'HT III-XX'!$G$688))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(W$94>'HT III-XX'!$D$176,'HT III-XX'!M161,IF(W$94>'HT III-XX'!D$216,'HT III-XX'!M$201,IF(W$94>'HT III-XX'!D$257,'HT III-XX'!M$241,IF(W$94>'HT III-XX'!$D$296,'HT III-XX'!M$281,IF(W$94>'HT III-XX'!$D$336,'HT III-XX'!M$312,IF(W$94>'HT III-XX'!$D$376,'HT III-XX'!M$361,IF(W$94>'HT III-XX'!$D$416,'HT III-XX'!M$401,IF(W94>'HT III-XX'!$D$456,'HT III-XX'!M$441,IF(W$94>'HT III-XX'!$D$496,'HT III-XX'!M$481,IF(W$94>'HT III-XX'!$D$536,'HT III-XX'!M$521,IF(W$94>'HT III-XX'!$D$576,'HT III-XX'!M$561,IF(W$94>'HT III-XX'!$D$616,'HT III-XX'!M$601,IF(W$94>'HT III-XX'!$D$656,'HT III-XX'!M$641,IF(W$94>'HT III-XX'!$D$687,'HT III-XX'!$G692,'HT III-XX'!$G$688))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(X$94>'HT III-XX'!$D$176,'HT III-XX'!O161,IF(X$94>'HT III-XX'!D$216,'HT III-XX'!O$201,IF(X$94>'HT III-XX'!D$257,'HT III-XX'!O$241,IF(X$94>'HT III-XX'!$D$296,'HT III-XX'!O$281,IF(X$94>'HT III-XX'!$D$336,'HT III-XX'!O$321,IF(X$94>'HT III-XX'!$D$376,'HT III-XX'!O$361,IF(X$94>'HT III-XX'!$D$416,'HT III-XX'!O$401,IF(X94>'HT III-XX'!$D$456,'HT III-XX'!O$441,IF(X$94>'HT III-XX'!$D$496,'HT III-XX'!O$481,IF(X$94>'HT III-XX'!$D$536,'HT III-XX'!O$521,IF(X$94>'HT III-XX'!$D$576,'HT III-XX'!O$561,IF(X$94>'HT III-XX'!$D$616,'HT III-XX'!O$601,IF(X$94>'HT III-XX'!$D$656,'HT III-XX'!O$641,IF(X$94>'HT III-XX'!$D$687,'HT III-XX'!$G692,'HT III-XX'!$G$688))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(Y$94>'HT III-XX'!$D$176,'HT III-XX'!Q161,IF(Y$94>'HT III-XX'!D$216,'HT III-XX'!Q$201,IF(Y$94>'HT III-XX'!D$257,'HT III-XX'!Q$241,IF(Y$94>'HT III-XX'!$D$296,'HT III-XX'!Q$281,IF(Y$94>'HT III-XX'!$D$336,'HT III-XX'!Q$312,IF(Y$94>'HT III-XX'!$D$376,'HT III-XX'!Q$361,IF(Y$94>'HT III-XX'!$D$416,'HT III-XX'!Q$401,IF(Y94>'HT III-XX'!$D$456,'HT III-XX'!Q$441,IF(Y$94>'HT III-XX'!$D$496,'HT III-XX'!Q$481,IF(Y$94>'HT III-XX'!$D$536,'HT III-XX'!Q$521,IF(Y$94>'HT III-XX'!$D$576,'HT III-XX'!Q$561,IF(Y$94>'HT III-XX'!$D$616,'HT III-XX'!Q$601,IF(Y$94>'HT III-XX'!$D$656,'HT III-XX'!Q$641,IF(Y$94>'HT III-XX'!$D$687,'HT III-XX'!$G692,'HT III-XX'!$G$688))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(Y$94>'HT III-XX'!$D$176,'HT III-XX'!S161,IF(Y$94>'HT III-XX'!D$216,'HT III-XX'!S$201,IF(Y$94>'HT III-XX'!D$257,'HT III-XX'!S$241,IF(Y$94>'HT III-XX'!$D$296,'HT III-XX'!S$281,IF(Y$94>'HT III-XX'!$D$336,'HT III-XX'!S$312,IF(Y$94>'HT III-XX'!$D$376,'HT III-XX'!S$361,IF(Y$94>'HT III-XX'!$D$416,'HT III-XX'!S$401,IF(Y94>'HT III-XX'!$D$456,'HT III-XX'!S$441,IF(Y$94>'HT III-XX'!$D$496,'HT III-XX'!S$481,IF(Y$94>'HT III-XX'!$D$536,'HT III-XX'!S$521,IF(Y$94>'HT III-XX'!$D$576,'HT III-XX'!S$561,IF(Y$94>'HT III-XX'!$D$616,'HT III-XX'!S$601,IF(Y$94>'HT III-XX'!$D$656,'HT III-XX'!S$641,IF(Y$94>'HT III-XX'!$D$687,'HT III-XX'!$G692,'HT III-XX'!$G$688))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(Z$94>'HT III-XX'!$D$176,'HT III-XX'!U161,IF(Z$94>'HT III-XX'!D$216,'HT III-XX'!U$201,IF(Z$94>'HT III-XX'!D$257,'HT III-XX'!U$241,IF(Z$94>'HT III-XX'!$D$296,'HT III-XX'!U$281,IF(Z$94>'HT III-XX'!$D$336,'HT III-XX'!U$321,IF(Z$94>'HT III-XX'!$D$376,'HT III-XX'!U$361,IF(Z$94>'HT III-XX'!$D$416,'HT III-XX'!U$401,IF(Z94>'HT III-XX'!$D$456,'HT III-XX'!U$441,IF(Z$94>'HT III-XX'!$D$496,'HT III-XX'!U$481,IF(Z$94>'HT III-XX'!$D$536,'HT III-XX'!U$521,IF(Z$94>'HT III-XX'!$D$576,'HT III-XX'!U$561,IF(Z$94>'HT III-XX'!$D$616,'HT III-XX'!U$601,IF(Z$94>'HT III-XX'!$D$656,'HT III-XX'!U$641,IF(Z$94>'HT III-XX'!$D$687,'HT III-XX'!$G692,'HT III-XX'!$G$688))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(AA$94>'HT III-XX'!$D$176,'HT III-XX'!W161,IF(AA$94>'HT III-XX'!D$216,'HT III-XX'!W$201,IF(AA$94>'HT III-XX'!D$257,'HT III-XX'!W$241,IF(AA$94>'HT III-XX'!$D$296,'HT III-XX'!W$281,IF(AA$94>'HT III-XX'!$D$336,'HT III-XX'!W$321,IF(AA$94>'HT III-XX'!$D$376,'HT III-XX'!W$361,IF(AA$94>'HT III-XX'!$D$416,'HT III-XX'!W$401,IF(AA94>'HT III-XX'!$D$456,'HT III-XX'!W$441,IF(AA$94>'HT III-XX'!$D$496,'HT III-XX'!W$481,IF(AA$94>'HT III-XX'!$D$536,'HT III-XX'!W$521,IF(AA$94>'HT III-XX'!$D$576,'HT III-XX'!W$561,IF(AA$94>'HT III-XX'!$D$616,'HT III-XX'!W$601,IF(AA$94>'HT III-XX'!$D$656,'HT III-XX'!W$641,IF(AA$94>'HT III-XX'!$D$687,'HT III-XX'!$G692,'HT III-XX'!$G$688))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(AB$94>'HT III-XX'!$D$176,'HT III-XX'!Y161,IF(AB$94>'HT III-XX'!D$216,'HT III-XX'!Y$201,IF(AB$94>'HT III-XX'!D$257,'HT III-XX'!Y$241,IF(AB$94>'HT III-XX'!$D$296,'HT III-XX'!Y$281,IF(AB$94>'HT III-XX'!$D$336,'HT III-XX'!Y$321,IF(AB$94>'HT III-XX'!$D$376,'HT III-XX'!Y$361,IF(AB$94>'HT III-XX'!$D$416,'HT III-XX'!Y$401,IF(AB94>'HT III-XX'!$D$456,'HT III-XX'!Y$441,IF(AB$94>'HT III-XX'!$D$496,'HT III-XX'!Y$481,IF(AB$94>'HT III-XX'!$D$536,'HT III-XX'!Y$521,IF(AB$94>'HT III-XX'!$D$576,'HT III-XX'!Y$561,IF(AB$94>'HT III-XX'!$D$616,'HT III-XX'!Y$601,IF(AB$94>'HT III-XX'!$D$656,'HT III-XX'!Y$641,IF(AB$94>'HT III-XX'!$D$687,'HT III-XX'!$G692,'HT III-XX'!$G$688))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(AD$94>'HT III-XX'!$D$176,'HT III-XX'!AA161,IF(AD$94>'HT III-XX'!D$216,'HT III-XX'!AA$201,IF(AD$94>'HT III-XX'!D$257,'HT III-XX'!AA$241,IF(AD$94>'HT III-XX'!$D$296,'HT III-XX'!AA$281,IF(AD$94>'HT III-XX'!$D$336,'HT III-XX'!AA$321,IF(AD$94>'HT III-XX'!$D$376,'HT III-XX'!AA$361,IF(AD$94>'HT III-XX'!$D$416,'HT III-XX'!AA$401,IF(AD94>'HT III-XX'!$D$456,'HT III-XX'!AA$441,IF(AD$94>'HT III-XX'!$D$496,'HT III-XX'!AA$481,IF(AD$94>'HT III-XX'!$D$536,'HT III-XX'!AA$521,IF(AD$94>'HT III-XX'!$D$576,'HT III-XX'!AA$561,IF(AD$94>'HT III-XX'!$D$616,'HT III-XX'!AA$601,IF(AD$94>'HT III-XX'!$D$656,'HT III-XX'!AA$641,IF(AD$94>'HT III-XX'!$D$687,'HT III-XX'!$G692,'HT III-XX'!$G$688))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(AC$94>'HT III-XX'!$D$176,'HT III-XX'!AC161,IF(AC$94>'HT III-XX'!D$216,'HT III-XX'!AC$201,IF(AC$94>'HT III-XX'!D$257,'HT III-XX'!AC$241,IF(AC$94>'HT III-XX'!$D$296,'HT III-XX'!AC$281,IF(AC$94>'HT III-XX'!$D$336,'HT III-XX'!AC$321,IF(AC$94>'HT III-XX'!$D$376,'HT III-XX'!AC$361,IF(AC$94>'HT III-XX'!$D$416,'HT III-XX'!AC$401,IF(AC94>'HT III-XX'!$D$456,'HT III-XX'!AC$441,IF(AC$94>'HT III-XX'!$D$496,'HT III-XX'!AC$481,IF(AC$94>'HT III-XX'!$D$536,'HT III-XX'!AC$521,IF(AC$94>'HT III-XX'!$D$576,'HT III-XX'!AC$561,IF(AC$94>'HT III-XX'!$D$616,'HT III-XX'!AC$601,IF(AC$94>'HT III-XX'!$D$656,'HT III-XX'!AC$641,IF(AC$94>'HT III-XX'!$D$687,'HT III-XX'!$G692,'HT III-XX'!$G$688))))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(AD$94>'HT III-XX'!$D$176,'HT III-XX'!AG161,IF(AD$94>'HT III-XX'!D$216,'HT III-XX'!AG$201,IF(AD$94>'HT III-XX'!D$257,'HT III-XX'!AG$241,IF(AD$94>'HT III-XX'!$D$296,'HT III-XX'!AG$281,IF(AD$94>'HT III-XX'!$D$336,'HT III-XX'!AG$321,IF(AD$94>'HT III-XX'!$D$376,'HT III-XX'!AG$361,IF(AD$94>'HT III-XX'!$D$416,'HT III-XX'!AG$401,IF(AD94>'HT III-XX'!$D$456,'HT III-XX'!AG$441,IF(AD$94>'HT III-XX'!$D$496,'HT III-XX'!AG$481,IF(AD$94>'HT III-XX'!$D$536,'HT III-XX'!AG$521,IF(AD$94>'HT III-XX'!$D$576,'HT III-XX'!AG$561,IF(AD$94>'HT III-XX'!$D$616,'HT III-XX'!AG$601,IF(AD$94>'HT III-XX'!$D$656,'HT III-XX'!AG$641,IF(AD$94>'HT III-XX'!$D$687,'HT III-XX'!$G692,'HT III-XX'!$G$688))))))))))))))","v":0},{"$f":"+IF(AE$94>'HT III-XX'!$D$176,'HT III-XX'!AI161,IF(AE$94>'HT III-XX'!D$216,'HT III-XX'!AI$201,IF(AE$94>'HT III-XX'!D$257,'HT III-XX'!AI$241,IF(AE$94>'HT III-XX'!$D$296,'HT III-XX'!AI$281,IF(AE$94>'HT III-XX'!$D$336,'HT III-XX'!AI$321,IF(AE$94>'HT III-XX'!$D$376,'HT III-XX'!AI$361,IF(AE$94>'HT III-XX'!$D$416,'HT III-XX'!AI$401,IF(AE94>'HT III-XX'!$D$456,'HT III-XX'!AI$441,IF(AE$94>'HT III-XX'!$D$496,'HT III-XX'!AI$481,IF(AE$94>'HT III-XX'!$D$536,'HT III-XX'!AI$521,IF(AE$94>'HT III-XX'!$D$576,'HT III-XX'!AI$561,IF(AE$94>'HT III-XX'!$D$616,'HT III-XX'!AI$601,IF(AE$94>'HT III-XX'!$D$656,'HT III-XX'!AI$641,IF(AE$94>'HT III-XX'!$D$687,'HT III-XX'!$G692,'HT III-XX'!$G$688))))))))))))))","v":0},{"$f":"+IF(AF$94>'HT III-XX'!$D$176,'HT III-XX'!AK161,IF(AF$94>'HT III-XX'!D$216,'HT III-XX'!AK$201,IF(AF$94>'HT III-XX'!D$257,'HT III-XX'!AK$241,IF(AF$94>'HT III-XX'!$D$296,'HT III-XX'!AK$281,IF(AF$94>'HT III-XX'!$D$336,'HT III-XX'!AK$321,IF(AF$94>'HT III-XX'!$D$376,'HT III-XX'!AK$361,IF(AF$94>'HT III-XX'!$D$416,'HT III-XX'!AK$401,IF(AF94>'HT III-XX'!$D$456,'HT III-XX'!AK$441,IF(AF$94>'HT III-XX'!$D$496,'HT III-XX'!AK$481,IF(AF$94>'HT III-XX'!$D$536,'HT III-XX'!AK$521,IF(AF$94>'HT III-XX'!$D$576,'HT III-XX'!AK$561,IF(AF$94>'HT III-XX'!$D$616,'HT III-XX'!AK$601,IF(AF$94>'HT III-XX'!$D$656,'HT III-XX'!AK$641,IF(AF$94>'HT III-XX'!$D$687,'HT III-XX'!$G692,'HT III-XX'!$G$688))))))))))))))","v":0},0,{"$f":"+(AI126-AF126)/3","v":0},"XVII",0,{"$f":"+AF97","v":5.04},0,0,0,null,"XVII",0,5.04,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E voda    =",{"$f":"+'Analiza i dimenzioniranje'!E41","v":0.6},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!T114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!T114)/3,0)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!U114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!U114)/3,0)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!V114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!V114)/3,0)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!W114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!W114)/3,0)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!X114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!X114)/3,0)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!Y114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!Y114)/3,0)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!Z114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!Z114)/3,0)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!AA114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!AA114)/3,0)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!AB114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!AB114)/3,0)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!AC114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!AC114)/3,0)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!AD114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!AD114)/3,0)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!AE114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!AE114)/3,0)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!AF114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!AF114)/3,0)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!AG114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!AG114)/3,0)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!AH114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!AH114)/3,0)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$E$41>'Sile i krakovi'!AI114,('Analiza i dimenzioniranje'!$E$41-'Sile i krakovi'!AI114)/3,0)","v":0},null,"XVIII",0,{"$f":"+AG97","v":5.36},0,0,0,null,"XVIII",0,5.36,0,0,0]
[" vertikalne S I L E   i  HORIZ.  KRAKOVI SILA za prevrtanje oko točke A",null,null,null,null,null,null,null,"EQTemelj",null,null,null,null,null,null,null,null,"Hpotres    =",{"$f":"+'C III-V'!AE113","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AE113-T114","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!AC113-'Sile i krakovi'!U114","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!AE113-'Sile i krakovi'!V114","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!AC113-'Sile i krakovi'!W114","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!AE113-'Sile i krakovi'!X114","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!AC113-'Sile i krakovi'!Y114","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!AE113-'Sile i krakovi'!Z114","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!AC113-AA114","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!AE113-AB114","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!AC113-AC114","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!AE113-AD114","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!AC113-AE114","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!AE113-AF114","v":{"$error":"#VALUE!"}},{"$f":"+'C XVIII-XIX'!AC113-AG114","v":{"$error":"#VALUE!"}},{"$f":"+'C XVIII-XIX'!AE113-AH114","v":{"$error":"#VALUE!"}},0,null,"XIX",0,{"$f":"+AH97","v":5.6800000000000006},0,0,0,null,"XIX",0,5.6800000000000006,0,0,0]
["Koord. na licu zida i temelja za opterećenja",null,null,"X      Točka A      Y",null,"Sile",null,null,null,null,null,null,null,null,null,null,null,"Eprometno=","Mprometno",{"$f":"+T123*T106","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,"XX",0,{"$f":"+AI97","v":6},0,0,0,null,"XX",0,6,0,0,0]
["koordinate","X","Y",{"$f":"+D105","v":4.9000021999999994},0.5,"kN",null,null,null,null,null,null,null,null,null,null,null,null,"SMH=",{"$f":"+T98*T116+T117*T99+T100*T118+T101*T119+T102*T120+T103*T121+T122*T104+T106*T123+T124*T107+T108*T125+T126*T109+T110*T127+T128*T111-T129","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["SS=",{"$f":"+B106","v":{"$error":"#VALUE!"}},3.9999999960000001,{"$error":"#VALUE!"},3.4999999960000001,{"$f":"SUM(F132:F135)","v":25.881904510252074},null,null,"y","x",null,null,null,null,null,null,null,"Vertikalne komponente sila sidara i tlakova, uzgona ",null,"PIII","PVI","PVII","PVIII","PIX","PX","P XI","P XII","P XIII","P XIV","PXV","PXVI","PXVII","PXVIII","PXIX","PXX"]
["Sv1=",{"$error":"#VALUE!"},5,{"$error":"#VALUE!"},4.5,{"$f":"+S134","v":12.940952255126037},null,null,{"$f":"IF(F131=0,0,+(I133*F132+I134*F133+I135*F134+I136*F135)/F131)","v":3.5},{"$f":"IF(F131=0,0,+(F132*J133+F133*J134+F134*J135+F135*J136)/F131)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,{"$f":"+T96","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Sv2=",{"$error":"#VALUE!"},3,{"$error":"#VALUE!"},2.5,{"$f":"+S135","v":12.940952255126037},null,null,{"$f":"+IF(E132=\"\",0,E132)","v":4.5},{"$f":"+IF(D132=\"\",0,D132)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,{"$f":"+T97","v":1.2},1.52,1.84,2.16,2.48,2.8,3.14,3.44,3.76,4.08,4.4000000000000004,4.72,5.04,5.36,5.6800000000000006,6]
["Sv3=","","","","",{"$f":"+S136","v":0},null,null,{"$f":"+IF(E133=\"\",0,E133)","v":2.5},{"$f":"+IF(D133=\"\",0,D133)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"Sv1=",{"$f":"IF(F107=\"\",0,'Analiza i dimenzioniranje'!D75*SIN('Analiza i dimenzioniranje'!$E$39*PI()/180))","v":12.940952255126037},{"$f":"IF($C132>T$133,$S134,0)","v":12.940952255126037},{"$f":"IF($C$132>U$133,$S134,0)","v":12.940952255126037},12.940952255126037,12.940952255126037,12.940952255126037,12.940952255126037,12.940952255126037,12.940952255126037,12.940952255126037,12.940952255126037,12.940952255126037,12.940952255126037,0,0,0,0]
["Sv4=","","","","",{"$f":"+S137","v":0},null,null,{"$f":"+IF(E134=\"\",0,E134)","v":0},{"$f":"+IF(D134=\"\",0,D134)","v":0},null,null,null,null,null,null,null,"Sv2=",{"$f":"IF(F108=\"\",0,'Analiza i dimenzioniranje'!E75*SIN('Analiza i dimenzioniranje'!$E$39*PI()/180))","v":12.940952255126037},{"$f":"IF($C$133>T$133,$S135,0)","v":12.940952255126037},12.940952255126037,12.940952255126037,12.940952255126037,12.940952255126037,12.940952255126037,0,0,0,0,0,0,0,0,0,0]
["Voda izvan zida",{"$f":"+P110","v":2.6666666666666665},{"$f":"+P111","v":0.26666666666666672},{"$f":"+D130-B136","v":2.2333355333333329},{"$f":"+C136-E130","v":-0.23333333333333328},{"$f":"+P109","v":3.2},null,null,{"$f":"+IF(E135=\"\",0,E135)","v":0},{"$f":"+IF(D135=\"\",0,D135)","v":0},null,null,null,null,null,null,null,"Sv3=",{"$f":"IF(F109=\"\",0,'Analiza i dimenzioniranje'!F75*SIN('Analiza i dimenzioniranje'!$E$39*PI()/180))","v":0},{"$f":"IF($C$134>T$133,$S136,0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Ev1=",{"$f":"+B112","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,{"$f":"+S139","v":{"$error":"#VALUE!"}},null,null,{"$f":"+IF(E136=\"\",0,E136)","v":-0.23333333333333328},{"$f":"+IF(D136=\"\",0,D136)","v":2.2333355333333329},null,null,null,null,null,null,null,"Sv4=",{"$f":"IF(F110=\"\",0,'Analiza i dimenzioniranje'!G75*SIN('Analiza i dimenzioniranje'!$E$39*PI()/180))","v":0},{"$f":"IF($C$135>T$133,$S137,0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Ev2=",{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,{"$f":"+S140","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,"Voda ispred =",{"$f":"+'Analiza i dimenzioniranje'!B131","v":0},0,{"$f":"IF($C$136>U$133,$S138,0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Ev3=",2,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!D112","v":{"$error":"#VALUE!"}},null,null,null,null,"koordinate leđa zida s položajem horizontalnih sila",null,null,null,null,"Sjecište presjeka u zidu\n i leđa zida",null,"Ev1=",{"$f":"'Analiza i dimenzioniranje'!D110","v":{"$error":"#VALUE!"}},{"$f":"-T177","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
["Eprometno",{"$f":"+'Rasprostiranje vertikalnog opt'!S30","v":{"$error":"#VALUE!"}},{"$f":"+C8","v":1.2},{"$f":"+D130-B140","v":{"$error":"#VALUE!"}},null,{"$f":"+'Analiza i dimenzioniranje'!B141","v":{"$error":"#VALUE!"}},null,null,null,null,"visina presjeka","X","E1","X","E2","x","y","Ev2=",{"$f":"'Analiza i dimenzioniranje'!D111","v":{"$error":"#VALUE!"}},{"$f":"-T180","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0]
["EPTočkasto",{"$f":"+'Rasprostiranje vertikalnog opt'!$S$48","v":{"$error":"#VALUE!"}},{"$f":"+C140","v":1.2},{"$f":"+D130-B141","v":{"$error":"#VALUE!"}},null,{"$f":"+'Analiza i dimenzioniranje'!B142","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+C8","v":1.2},{"$f":"+M141/$B$85-$D$85/$B$85","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!B87","v":{"$error":"#VALUE!"}},{"$f":"+O141/$B$85-$D$85/$B$85","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!D87","v":{"$error":"#VALUE!"}},{"$f":"+Q141/$B$85-$D$85/$B$85","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U52","v":1.2},"Ev3=",{"$f":"'Analiza i dimenzioniranje'!B148","v":{"$error":"#VALUE!"}},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EPLinijsko ",{"$f":"+'Rasprostiranje vertikalnog opt'!$S$39","v":{"$error":"#VALUE!"}},{"$f":"+C141","v":1.2},{"$f":"+D130-B142","v":{"$error":"#VALUE!"}},null,{"$f":"+'Analiza i dimenzioniranje'!B143","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+K141+'Analiza i dimenzioniranje'!X$53","v":1.52},{"$error":"#VALUE!"},{"$f":"+'C VI-VII'!I$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'C VI-VII'!K87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!U53","v":1.52},"Eprometno=",{"$f":"+'Analiza i dimenzioniranje'!B141","v":{"$error":"#VALUE!"}},{"$f":"IF($C$140>T$133,$S142,0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EQTemelj",{"$f":"+'Rasprostiranje vertikalnog opt'!$S$21","v":{"$error":"#VALUE!"}},{"$f":"+C142","v":1.2},{"$f":"+D130-B143","v":{"$error":"#VALUE!"}},null,{"$f":"+'Analiza i dimenzioniranje'!B144","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+K142+'Analiza i dimenzioniranje'!X$53","v":1.84},{"$error":"#VALUE!"},{"$f":"+'C VI-VII'!N87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'C VI-VII'!P87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!U54","v":1.84},"Etočkasto  =",{"$f":"+F141","v":{"$error":"#VALUE!"}},{"$f":"IF($C$141>T$133,$S143,0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Vsidro",{"$f":"+B131","v":{"$error":"#VALUE!"}},{"$f":"+C131","v":3.9999999960000001},{"$f":"+D131","v":{"$error":"#VALUE!"}},{"$f":"+E131","v":3.4999999960000001},{"$f":"+'Analiza i dimenzioniranje'!B145","v":25.881904536133977},null,null,null,null,{"$f":"+K143+'Analiza i dimenzioniranje'!X$53","v":2.16},{"$error":"#VALUE!"},{"$f":"+'C VIII-IX'!I$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'C VIII-IX'!K$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!U55","v":2.16},"Elinijsko    = ",{"$f":"+F142","v":{"$error":"#VALUE!"}},{"$f":"IF($C$142>T$133,$S144,0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Vvoda",{"$f":"+J145","v":0},{"$f":"+J146","v":0},{"$f":"+B145","v":0},{"$f":"+C145-('Analiza i dimenzioniranje'!E52-'Analiza i dimenzioniranje'!E51)","v":-0.5},null,null,null,null,null,{"$f":"+K144+'Analiza i dimenzioniranje'!X$53","v":2.48},{"$error":"#VALUE!"},{"$f":"+'C VIII-IX'!N$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'C VIII-IX'!P$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!U56","v":2.48},"Etemelja   =",{"$f":"+F143","v":{"$error":"#VALUE!"}},{"$f":"IF($C$143>T$133,$S145,0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Gtemelja",{"$f":"+$D$130-D146","v":{"$error":"#VALUE!"}},0.5,{"$f":"+'Analiza i dimenzioniranje'!C135","v":{"$error":"#VALUE!"}},null,{"$f":"+'Analiza i dimenzioniranje'!B135","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+K145+'Analiza i dimenzioniranje'!X$53","v":2.8},{"$error":"#VALUE!"},{"$f":"+'C X-XI'!I$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'C X-XI'!K$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!U57","v":2.8},"Gtemelja",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Gzid+konzola",{"$f":"+$D$130-D147","v":{"$error":"#VALUE!"}},0.5,{"$f":"+'Analiza i dimenzioniranje'!C136","v":{"$error":"#VALUE!"}},null,{"$f":"+S147","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+K146+'Analiza i dimenzioniranje'!X$53","v":3.1199999999999997},{"$error":"#VALUE!"},{"$f":"+'C X-XI'!N$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'C X-XI'!P$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!U58","v":3.14},"Gzid+konzola",{"$f":"+'Analiza i dimenzioniranje'!B136","v":{"$error":"#VALUE!"}},{"$f":"-'C III-V'!$H$61","v":{"$error":"#VALUE!"}},{"$f":"-'C VI-VII'!L61","v":{"$error":"#VALUE!"}},{"$f":"-'C VI-VII'!P61","v":{"$error":"#VALUE!"}},{"$f":"-'C VIII-IX'!L61","v":{"$error":"#VALUE!"}},{"$f":"-'C VIII-IX'!P61","v":{"$error":"#VALUE!"}},{"$f":"-'C X-XI'!$L61","v":{"$error":"#VALUE!"}},{"$f":"-'C X-XI'!$P61","v":{"$error":"#VALUE!"}},{"$f":"-'C XII-XIII'!$L61","v":{"$error":"#VALUE!"}},{"$f":"-'C XII-XIII'!$P61","v":{"$error":"#VALUE!"}},{"$f":"-'C XIV-XV'!$L61","v":{"$error":"#VALUE!"}},{"$f":"-'C XIV-XV'!$P61","v":{"$error":"#VALUE!"}},{"$f":"-'C XVI-XVII'!$L61","v":{"$error":"#VALUE!"}},{"$f":"-'C XVI-XVII'!$P61","v":{"$error":"#VALUE!"}},{"$f":"-'C XVIII-XIX'!$L61","v":{"$error":"#VALUE!"}},{"$f":"-'C XVIII-XIX'!$P61","v":{"$error":"#VALUE!"}},0]
["Gnasip na konzoli ",{"$f":"+$D$130-D148","v":{"$error":"#VALUE!"}},0.5,{"$f":"+'Analiza i dimenzioniranje'!C138","v":{"$error":"#VALUE!"}},null,{"$f":"+S148","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+K147+'Analiza i dimenzioniranje'!X$53","v":3.4399999999999995},{"$error":"#VALUE!"},{"$f":"+'C XII-XIII'!I$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'C XII-XIII'!K$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!U59","v":3.44},"Gnasip na konzoli ",{"$f":"+'Analiza i dimenzioniranje'!B138","v":{"$error":"#VALUE!"}},{"$f":"-S148","v":{"$error":"#VALUE!"}},{"$f":"-'C VI-VII'!N61","v":{"$error":"#VALUE!"}},{"$f":"-'C VI-VII'!R61","v":{"$error":"#VALUE!"}},{"$f":"-'C VIII-IX'!R61","v":{"$error":"#VALUE!"}},{"$f":"-'C VIII-IX'!R61","v":{"$error":"#VALUE!"}},{"$f":"-'C VI-VII'!N61","v":{"$error":"#VALUE!"}},{"$f":"-'C X-XI'!R61","v":{"$error":"#VALUE!"}},{"$f":"-'C XII-XIII'!N61","v":{"$error":"#VALUE!"}},{"$f":"-'C XII-XIII'!R61","v":{"$error":"#VALUE!"}},{"$f":"-'C XIV-XV'!N61","v":{"$error":"#VALUE!"}},{"$f":"-'C XIV-XV'!R61","v":{"$error":"#VALUE!"}},{"$f":"-'C XVI-XVII'!N61","v":{"$error":"#VALUE!"}},{"$f":"-'C XVI-XVII'!R61","v":{"$error":"#VALUE!"}},{"$f":"-'C XVIII-XIX'!N61","v":{"$error":"#VALUE!"}},{"$f":"-'C XVIII-XIX'!R61","v":{"$error":"#VALUE!"}},{"$f":"-'P XX-XX'!$B130","v":0}]
["Gnasipa iza zida",{"$f":"+$D$130-D149","v":{"$error":"#VALUE!"}},0.5,{"$f":"+'Analiza i dimenzioniranje'!C139","v":{"$error":"#VALUE!"}},null,{"$f":"+'Analiza i dimenzioniranje'!B139","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+K148+'Analiza i dimenzioniranje'!X$53","v":3.7599999999999993},{"$error":"#VALUE!"},{"$f":"+'C XII-XIII'!N$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'C XII-XIII'!P$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!U60","v":3.76},"Gnasipa iza zida ",{"$f":"+'Analiza i dimenzioniranje'!B139","v":{"$error":"#VALUE!"}},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Gnasipa ispred zida",{"$f":"+$D$130-D150","v":{"$error":"#VALUE!"}},0.5,{"$f":"+'Analiza i dimenzioniranje'!C140","v":{"$error":"#VALUE!"}},null,{"$f":"+S150","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+K149+'Analiza i dimenzioniranje'!X$53","v":4.0799999999999992},{"$error":"#VALUE!"},{"$f":"+'C XII-XIII'!I$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'C XIV-XV'!K$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!U61","v":4.08},"Gnasipa ispred zida",{"$f":"+'Analiza i dimenzioniranje'!B140","v":{"$error":"#VALUE!"}},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,{"$f":"+'C III-V'!B68","v":"E1"},null,{"$f":"+'C III-V'!D68","v":"E2"},null,{"$f":"+'C III-V'!F68","v":"E3"},null,null,null,null,{"$f":"+K150+'Analiza i dimenzioniranje'!X$53","v":4.3999999999999995},{"$error":"#VALUE!"},{"$f":"+'C XIV-XV'!N$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'C XIV-XV'!P$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!U62","v":4.4000000000000004},"SV=",{"$f":"SUM(S134:S150)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T134:T150)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U134:U148)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0]
[{"$f":"+'C III-V'!M79","v":0},{"$f":"+'C III-V'!K79","v":0},{"$f":"+'C III-V'!L79","v":0},null,{"$f":"+'C III-V'!N79","v":0},{"$f":"+'C III-V'!O79","v":0},null,null,null,null,{"$f":"+K151+'Analiza i dimenzioniranje'!X$53","v":4.72},{"$error":"#VALUE!"},{"$f":"+'C XVI-XVII'!I$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'C XVI-XVII'!K$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!U63","v":4.72}]
[{"$f":"+A161","v":1},{"$f":"+'C III-V'!B70","v":0},{"$f":"+'C III-V'!C70","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!D71","v":0},{"$f":"+'C III-V'!E71","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!F69","v":0},null,null,{"$f":"+'C III-V'!P79","v":0},null,{"$f":"+K152+'Analiza i dimenzioniranje'!X$53","v":5.04},{"$error":"#VALUE!"},{"$f":"+'C XVI-XVII'!N$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'C XVI-XVII'!P$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!U64","v":5.04},"Horizontalni krakovi od osi zida do točke djelovanja na zidu za izračun momenta u tom presjeku",null,"PIII","PVI","PVII","PVIII","PIX","PX","P XI","P XII","P XIII","P XIV","PXV","PXVI","PXVII","PXVIII","PXIX","PXX"]
[{"$f":"+A162","v":2},{"$f":"+'C III-V'!B71","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C71","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!D72","v":0},{"$f":"+'C III-V'!E72","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!F72","v":0},null,null,{"$f":"+'C III-V'!G69","v":1.2},null,{"$f":"+K153+'Analiza i dimenzioniranje'!X$53","v":5.36},{"$error":"#VALUE!"},{"$f":"+'C XVIII-XIX'!I$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'C XVIII-XIX'!K$87","v":0},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!U65","v":5.36},null,null,{"$f":"+T132","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[{"$f":"+A163","v":3},{"$f":"+'C III-V'!B72","v":0},{"$f":"+'C III-V'!C72","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!D69","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!E69","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!F70","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!G72","v":0},null,{"$f":"+K154+'Analiza i dimenzioniranje'!X$53","v":5.6800000000000006},{"$error":"#VALUE!"},{"$f":"+'C XVIII-XIX'!N$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'C XVIII-XIX'!P$87","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!U66","v":5.6800000000000006},null,null,{"$f":"+T133","v":1.2},1.52,1.84,2.16,2.48,2.8,3.14,3.44,3.76,4.08,4.4000000000000004,4.72,5.04,5.36,5.6800000000000006,6]
[4,{"$f":"+'C III-V'!B69","v":0},{"$f":"+'C III-V'!C69","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!D70","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!E70","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!F71","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!G70","v":{"$error":"#VALUE!"}},null,{"$f":"+K155+'Analiza i dimenzioniranje'!X$53","v":6.0000000000000009},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!U67","v":6.0000000000000009},"Sv1=",{"$f":"+B132","v":{"$error":"#VALUE!"}},{"$f":"-IF($S156=\"\",0,T$154-$S156)","v":{"$error":"#VALUE!"}},{"$f":"-IF($S$156=\"\",0,U154-$S$156)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,null,"x=",{"$f":"+B163","v":12.361875887090893},{"$f":"+B162","v":{"$error":"#VALUE!"}},22.79]
[null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!G71","v":0},null,null,null,null,null,null,null,null,"Sv2=",{"$f":"+B133","v":{"$error":"#VALUE!"}},{"$f":"-IF($S157=\"\",0,T$154-$S157)","v":{"$error":"#VALUE!"}},{"$f":"-IF($S157=\"\",0,U$154-$S157)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,null,"Y=",{"$f":"+C163","v":{"$error":"#VALUE!"}},{"$f":"+AC133","v":4.08}]
["Linije AKTIVNIH TLAKOVA ZA PRESJEK III-III umanjeni za  koheziju",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sv3=",{"$f":"+B134","v":""},{"$f":"-IF($S158=\"\",0,T$154-$S158)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,"  Jednadžba pravca E1",null,"Y=",{"$f":"(AP157-AO157)/(AP156-AO156)","v":{"$error":"#VALUE!"}},"*x        +",{"$f":"-AO158*AO156+AO157","v":{"$error":"#VALUE!"}}]
[{"$f":"+'C III-V'!A78","v":"Oznaka"},{"$f":"+B151","v":"E1"},{"$f":"+'C III-V'!C60","v":"m"},{"$f":"+D151","v":"E2"},{"$f":"+'C III-V'!E60","v":"m"},{"$f":"+F151","v":"E3"},null,null,null,null,null,null,null,null,null,null,null,"Sv4=",{"$f":"+B135","v":""},{"$f":"-IF($S159=\"\",0,T$154-$S159)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,"X=",{"$f":"-AP157/$AO$158+$AQ$158/$AO$158","v":{"$error":"#VALUE!"}},"za Y=",4.2]
[{"$f":"+A152","v":0},{"$f":"+'C III-V'!B79","v":"x"},{"$f":"+'C III-V'!C79","v":"y"},{"$f":"+'C III-V'!D79","v":"x"},{"$f":"+'C III-V'!E79","v":"y"},{"$f":"+'C III-V'!F79","v":"x"},null,null,null,null,null,null,null,null,null,null,null,"Water",{"$f":"+B136","v":2.6666666666666665},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"+'C III-V'!A80","v":1},{"$f":"+'C III-V'!B80","v":12.361875887090893},{"$f":"+'C III-V'!C80","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!D80","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!E80","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!F80","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!G79","v":"y"},null,null,null,null,null,null,null,null,"Ev1=",{"$f":"+S121","v":{"$error":"#VALUE!"}},{"$f":"+IF(T139<0,T$154-$L141,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(U139<0,U$154-$L142,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(V139<0,V$154-$L143,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(W139<0,W$154-$L144,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(X139<0,X$154-$L145,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(Y139<0,Y$154-$L146,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(Z139<0,Z$154-$L147,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AA139<0,AA$154-$L148,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AB139<0,AB$154-$L149,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AC139<0,AC$154-$L150,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AD139<0,AD$154-$L151,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AE139<0,AE$154-$L152,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AF139<0,AF$154-$L152,0)","v":{"$error":"#VALUE!"}},{"$f":"+AF161","v":{"$error":"#VALUE!"}},{"$f":"+IF(AH139<0,AH$154-$L155,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AI139<0,AI$154-$L156,0)","v":0},null,null,null,null,"x=",{"$f":"+D163","v":{"$error":"#VALUE!"}},{"$f":"+D164","v":{"$error":"#VALUE!"}},{"$f":"+AO161","v":{"$error":"#VALUE!"}}]
[{"$f":"+'C III-V'!A81","v":2},{"$f":"+'C III-V'!B81","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C81","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!D81","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!E81","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!F81","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!G80","v":0},null,null,null,null,null,null,null,null,"Ev2=",{"$f":"+S122","v":{"$error":"#VALUE!"}},{"$f":"+IF(T140<0,T$154-$N141,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(U140<0,U$154-$N142,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(V140<0,V$154-$N143,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(W140<0,W$154-$N144,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(X140<0,X$154-$N145,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(Y140<0,Y$154-$N146,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(Z140<0,Z$154-$N147,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AA140<0,AA$154-$N148,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AB140<0,AB$154-$N149,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AC140<0,AC$154-$N150,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AD140<0,AD$154-$N151,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AE140<0,AE$154-$N152,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AF140<0,AF$154-$N153,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AG140<0,AG$154-$N154,0)","v":0},{"$f":"+IF(AH140<0,AH$154-$N155,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(AI140<0,AI$154-$N156,0)","v":0},null,null,null,null,"Y=",{"$f":"+E162","v":{"$error":"#VALUE!"}},{"$f":"+E164","v":{"$error":"#VALUE!"}}]
[{"$f":"+'C III-V'!A82","v":3},{"$f":"+'C III-V'!B82","v":12.361875887090893},{"$f":"+'C III-V'!C82","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!D82","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!E82","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!F82","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!G81","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"Eprometno=",{"$f":"+'Rasprostiranje vertikalnog opt'!V34","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,"  Jednadžba pravca E2",null,"Y=",{"$f":"(AP162-AO162)/(AP161-AO161)","v":{"$error":"#VALUE!"}},"*x        +",{"$f":"-AO163*AO161+AO162","v":{"$error":"#VALUE!"}}]
[{"$f":"+'C III-V'!A83","v":4},{"$f":"+'C III-V'!B83","v":12.361875887090893},{"$f":"+'C III-V'!C83","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!D83","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!E83","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!F83","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!G82","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"Etočkasto  =",{"$f":"+'Rasprostiranje vertikalnog opt'!AF48","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,"X=",{"$f":"-4.2/$AO$163+$AQ$163/$AO$163","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!G83","v":0},null,null,null,null,null,null,null,null,"Elinijsko    = ",{"$f":"+'Rasprostiranje vertikalnog opt'!AF38","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Etemelja   =",{"$f":"+'Rasprostiranje vertikalnog opt'!AF20","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,"x=",{"$f":"+F164","v":{"$error":"#VALUE!"}},{"$f":"+F163","v":{"$error":"#VALUE!"}},{"$f":"+AO166","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gzid+konz",{"$f":"+'C III-V'!H59","v":{"$error":"#VALUE!"}},{"$f":"+T154-'C III-V'!$H$59","v":{"$error":"#VALUE!"}},{"$f":"U154-'C VI-VII'!$L$59","v":{"$error":"#VALUE!"}},{"$f":"V154-'C VI-VII'!$P59","v":{"$error":"#VALUE!"}},{"$f":"W154-'C VIII-IX'!$L$59","v":{"$error":"#VALUE!"}},{"$f":"X154-'C VIII-IX'!$P59","v":{"$error":"#VALUE!"}},{"$f":"Y154-'C X-XI'!$L$59","v":{"$error":"#VALUE!"}},{"$f":"Z154-'C X-XI'!$P$59","v":{"$error":"#VALUE!"}},{"$f":"AA154-'C XII-XIII'!$L$59","v":{"$error":"#VALUE!"}},{"$f":"AB154-'C XII-XIII'!$P$59","v":{"$error":"#VALUE!"}},{"$f":"IF(AC154-'C XIV-XV'!$L$59<0,0,AC154-'C XIV-XV'!$L$59)","v":{"$error":"#VALUE!"}},{"$f":"IF(AD154-'C XIV-XV'!$P$59<0,0,AD154-'C XIV-XV'!$P$59)","v":{"$error":"#VALUE!"}},{"$f":"IF(AE154-'C XVI-XVII'!$L$59<0,0,AE154-'C XVI-XVII'!$L$59)","v":{"$error":"#VALUE!"}},{"$f":"IF(AF154-'C XVI-XVII'!$P$59<0,0,AF154-'C XVI-XVII'!$P$59)","v":{"$error":"#VALUE!"}},{"$f":"IF(AG154-'C XVIII-XIX'!$L$59<0,0,AG154-'C XVIII-XIX'!$L$59)","v":{"$error":"#VALUE!"}},{"$f":"IF(AH154-'C XVIII-XIX'!$L$59<0,0,AH154-'C XVIII-XIX'!$L$59)","v":{"$error":"#VALUE!"}},0,null,null,null,null,"Y=",{"$f":"+I165","v":0},{"$f":"+I164","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gnasip na konzoli ",{"$f":"+'C III-V'!$J$59","v":{"$error":"#VALUE!"}},{"$f":"+T154-'C III-V'!$J$59","v":{"$error":"#VALUE!"}},{"$f":"U154-'C VI-VII'!$N59","v":{"$error":"#VALUE!"}},{"$f":"V154-'C VI-VII'!R59","v":{"$error":"#VALUE!"}},{"$f":"W154-'C VIII-IX'!$N59","v":{"$error":"#VALUE!"}},{"$f":"X154-'C VIII-IX'!R59","v":{"$error":"#VALUE!"}},{"$f":"Y154-'C X-XI'!$N$59","v":{"$error":"#VALUE!"}},{"$f":"Z154-'C X-XI'!$R$59","v":{"$error":"#VALUE!"}},{"$f":"AA154-'C XII-XIII'!$N$59","v":{"$error":"#VALUE!"}},{"$f":"AB154-'C XII-XIII'!$R$59","v":{"$error":"#VALUE!"}},{"$f":"AC154-'C XIV-XV'!$N$59","v":{"$error":"#VALUE!"}},{"$f":"AD154-'C XII-XIII'!$R$59","v":{"$error":"#VALUE!"}},{"$f":"AE154-'C XVI-XVII'!$N$59","v":{"$error":"#VALUE!"}},{"$f":"AF154-'C XVI-XVII'!$R$59","v":{"$error":"#VALUE!"}},{"$f":"AG154-'C XVIII-XIX'!$N$59","v":{"$error":"#VALUE!"}},{"$f":"AH154-'C XVIII-XIX'!$R$59","v":{"$error":"#VALUE!"}},{"$f":"-'P XX-XX'!$B145","v":0},null,null,"  Jednadžba pravca E3",null,"Y=",{"$f":"(AP167-AO167)/(AP166-AO166)","v":{"$error":"#VALUE!"}},"*x        +",{"$f":"-AO168*AO166+AO167","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SMV=",{"$f":"+T134*T156+T135*T157+T136*T158+T137*T159+T138*T160+T139*T161+T140*T162+T142*T163+T143*T164+T144*T165+T145*T166+T147*T167+T148*T168","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,null,"X=",{"$f":"-S257/AO168+AQ168/AO168","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+T167-U167","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"oznaka profila","PIII","PVI","PVII","PVIII","PIX","PX","P XI","P XII","P XIII","P XIV","PXV","PXVI","PXVII","PXVIII","PXIX","PXX"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"h=",{"$f":"+T155","v":1.2},1.52,1.84,2.16,2.48,2.8,3.14,3.44,3.76,4.08,4.4000000000000004,4.72,5.04,5.36,5.6800000000000006,6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SM=",{"$f":"-T169-T130","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E1=",{"$f":"+'C III-V'!B85","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!I85","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!N85","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!I85","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!N85","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!I85","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!N85","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!I85","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!N85","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!I85","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!N85","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!I85","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!N85","v":{"$error":"#VALUE!"}},{"$f":"+'C XVIII-XIX'!I85","v":{"$error":"#VALUE!"}},{"$f":"+'C XVIII-XIX'!N85","v":{"$error":"#VALUE!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EH1=",{"$f":"+'Analiza i dimenzioniranje'!C110","v":{"$error":"#VALUE!"}},{"$f":"+U175*COS(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+V175*COS(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+W175*COS(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+X175*COS(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+Y175*COS(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+Z175*COS(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AA175*COS(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AB175*COS(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AC175*COS(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AD175*COS(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AE175*COS(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AF175*COS(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AG175*COS(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AH175*COS(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AI175*COS(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EV1=",{"$f":"+'Analiza i dimenzioniranje'!D110","v":{"$error":"#VALUE!"}},{"$f":"ABS(U175*SIN(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"ABS(V175*SIN(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"ABS(W175*SIN(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"ABS(X175*SIN(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"ABS(Y175*SIN(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"ABS(Z175*SIN(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"ABS(AA175*SIN(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"ABS(AB175*SIN(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"ABS(AC175*SIN(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"ABS(AD175*SIN(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"ABS(AE175*SIN(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"ABS(AF175*SIN(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"ABS(AG175*SIN(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"ABS(AH175*SIN(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"ABS(AI175*SIN(('Analiza i dimenzioniranje'!$D$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E2=",{"$f":"+'C III-V'!D85","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!K85","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!P85","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!K85","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!P85","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!K85","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!P85","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!K85","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!P85","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!K85","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!P85","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!K85","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!P85","v":{"$error":"#VALUE!"}},{"$f":"+'C XVIII-XIX'!K85","v":0},{"$f":"+'C XVIII-XIX'!P85","v":{"$error":"#VALUE!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EH2=",{"$f":"+'Analiza i dimenzioniranje'!C111","v":{"$error":"#VALUE!"}},{"$f":"+U178*COS(('Analiza i dimenzioniranje'!$E$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+V178*COS(('Analiza i dimenzioniranje'!$E$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+W178*COS(('Analiza i dimenzioniranje'!$E$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+X178*COS(('Analiza i dimenzioniranje'!$E$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+Y178*COS(('Analiza i dimenzioniranje'!$E$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+Z178*COS(('Analiza i dimenzioniranje'!$E$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AA178*COS(('Analiza i dimenzioniranje'!$E$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AB178*COS(('Analiza i dimenzioniranje'!$E$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AC178*COS(('Analiza i dimenzioniranje'!$E$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AD178*COS(('Analiza i dimenzioniranje'!$E$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AE178*COS(('Analiza i dimenzioniranje'!$E$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AF178*COS(('Analiza i dimenzioniranje'!$E$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AG178*COS(('Analiza i dimenzioniranje'!$E$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":0},{"$f":"+AH178*COS(('Analiza i dimenzioniranje'!$E$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AI178*COS(('Analiza i dimenzioniranje'!$E$19-'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EV2=",{"$f":"+'Analiza i dimenzioniranje'!D111","v":{"$error":"#VALUE!"}},{"$f":"+SQRT(U178*U178-U179*U179)","v":{"$error":"#VALUE!"}},{"$f":"+SQRT(V178*V178-V179*V179)","v":{"$error":"#VALUE!"}},{"$f":"+SQRT(W178*W178-W179*W179)","v":{"$error":"#VALUE!"}},{"$f":"+SQRT(X178*X178-X179*X179)","v":{"$error":"#VALUE!"}},{"$f":"+SQRT(Y178*Y178-Y179*Y179)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Točke u kojima djeluje trenje",null,null,null,"Položaj sile trenja na dnu"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba dna temelja gdje djeluje naprezanje",null,null,null,"x","Y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+Q196","v":1.75},{"$f":"+O204","v":4.9000010999999999},null,{"$f":"+T184","v":1.75},0,"lijevi tub temelja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+B218","v":9.6153895463470418E-2},{"$f":"+('Analiza i dimenzioniranje'!E52-'Analiza i dimenzioniranje'!E51)","v":0.5},null,{"$f":"+T184+(S192-T184)/2","v":2.5750000499999999},{"$f":"+$T$186*W185+$V$186","v":0.20192308279325966},"lijevo"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"(U185-T185)/(U184-T184)","v":0.12820506778125557},"*x    +",{"$f":"-T186*T184+T185","v":-0.12820497315372681},{"$f":"+Q199+'Analiza i dimenzioniranje'!E55/2","v":3.8000000999999997},{"$f":"IF('Unos podataka'!O48=\"DA\",B319,$T$186*W186+$V$186)","v":0.35897429723555108},"sredina"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Naponi ispod kontrafore",null,null,null,null,null,null,null,{"$f":"S198+(U184-S198)/2","v":4.5500005999999997},{"$f":"+$T$186*W187+$V$186","v":0.45512816217402663},"desno"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+O202","v":1.75},{"$f":"+P202","v":{"$error":"#VALUE!"}},null,null,"Trenje:",null,null,null,{"$f":"+J200","v":4.2000000999999996},{"$f":"+$T$186*W188+$V$186","v":0.41025632434805326},"sredina dole"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2-'Analiza i dimenzioniranje'!D83","v":1},{"$f":"-'Analiza i dimenzioniranje'!F195/100","v":{"$error":"#VALUE!"}},null,null,"vertikale u naponima",null,"Hor sila trenja"]
[null,null,null,"Jednadžba dna temelja s KF",null,null,null,null,null,null,null,null,null,null,{"$f":"+O189","v":1},0,null,null,"x","y","trenje po presjecima",null,"Horizontalne sile",null,"V11=",{"$f":"+S150+AD204+V202","v":{"$error":"#VALUE!"}},"h11",{"$f":"+U193+AV113","v":{"$error":"#VALUE!"}}]
[null,null,"Točke","pravca 1",null,null,null,null,null,"Položaji djelovanja",null,"Koord trenja u dnu",null,null,null,null,"x","y",{"$f":"+O200","v":3.4000000999999997},{"$f":"+I164","v":{"$error":"#VALUE!"}},{"$f":"'Analiza i dimenzioniranje'!B167*(O200-O202)/(O198-O202)","v":{"$error":"#VALUE!"}},"II-II",null,null,"V22=",{"$f":"(+S141+S142+S143+S144+S145+S149+R202+Z204+'Analiza i dimenzioniranje'!B137+'Analiza i dimenzioniranje'!B151)","v":{"$error":"#VALUE!"}},"h22",{"$f":"(+U191-F114-'C III-V'!AH135-'Sile i krakovi'!F119)","v":{"$error":"#VALUE!"}}]
[null,null,null,"T1  ","T2",null,null,null,null,"X","Y","X","Y",null,"Vertikale u betonskim presjecima",null,{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+K196+'Analiza i dimenzioniranje'!E51/2","v":0.85},{"$f":"+S191","v":3.4000000999999997},{"$f":"+P200","v":{"$error":"#VALUE!"}},{"$f":"'Analiza i dimenzioniranje'!B167*(O199-O200)/(O198-O202)","v":{"$error":"#VALUE!"}},"sredina ","kN",null,"V33=",{"$f":"+S147+S148+S134+S135+S136+S137-S138+S139+S140","v":{"$error":"#VALUE!"}},"h33",{"$f":"-T112","v":{"$error":"#VALUE!"}}]
[null,null,"x=",{"$f":"+'Unos podataka'!I41","v":2},{"$f":"+J195","v":4.9000010999999999},null,null,null,null,2,{"$f":"+B202","v":0.12820515121628623},{"$f":"IF('Unos podataka'!O48=\"DA\",0,+W185)","v":2.5750000499999999},{"$f":"+R208","v":{"$error":"#VALUE!"}},"lijevo",null,null,{"$f":"IF('Unos podataka'!O48=\"DA\",'Sile i krakovi'!A326,S191)","v":3.4000000999999997},{"$f":"+(AB198-AB197)/2+AB197","v":{"$error":"#VALUE!"}},{"$f":"+O199","v":4.2000000999999996},{"$f":"+T191","v":{"$error":"#VALUE!"}},{"$f":"'Analiza i dimenzioniranje'!B167*(O198-O199)/(O198-O202)","v":{"$error":"#VALUE!"}},"I-I",{"$f":"SUM(U191:U193)","v":{"$error":"#VALUE!"}},null,"Vtemelja=",{"$f":"+AB204+T202","v":{"$error":"#VALUE!"}},"Htemelja=",{"$f":"+U192","v":{"$error":"#VALUE!"}}]
[null,null,"Y=",{"$f":"+'Unos podataka'!J41","v":0.12820515121628623},{"$f":"+K196","v":0.5},null,null,null,null,{"$f":"+J193","v":2},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+W186","v":3.8000000999999997},{"$f":"+X186","v":0.35897429723555108},"sredina","Točka na II-II za MII-II",null,{"$f":"+S198","v":4.2000000999999996},{"$f":"IF('Unos podataka'!O48=\"DA\",'Sile i krakovi'!B313,(AD197-AD198)/2+AD198)","v":{"$error":"#VALUE!"}},{"$f":"+S193","v":4.2000000999999996},{"$f":"+P199","v":{"$error":"#VALUE!"}},{"$f":"SUM(U191:U193)","v":{"$error":"#VALUE!"}},"III-III",{"$f":"'Analiza i dimenzioniranje'!B167","v":{"$error":"#VALUE!"}},null,"SV=",{"$f":"SUM(Z190:Z193)","v":{"$error":"#VALUE!"}},"SH=",0]
[null,null,"Y=",{"$f":"(E194-D194)/(E193-D193)","v":0.12820507164073619},"*x    +",{"$f":"-D195*D193+D194","v":-0.12820499206518615}," ",null,null,{"$f":"+O197","v":4.9000010999999999},{"$f":"+K194","v":1.2},{"$f":"+W187","v":4.5500005999999997},{"$f":"+X187","v":0.45512816217402663},"desno","Točka na I-I za MI-I",null,"vert. Napr. Lijevo",null,"vert. napr između II-II i I-I",null,"Vert. Napr. Desno",null,null,null,"TEMELJ"]
[null,null,"Y=",{"$f":"+D195*A204+F195","v":0.30769239253889569},null,null,null,null,null,{"$f":"+J195","v":4.9000010999999999},{"$f":"+K195-'Analiza i dimenzioniranje'!E51","v":0.5},"Naprezanje ",null,null,"Raspodjela naprezanja",null,{"$f":"+Q197","v":1.75},0,{"$f":"+Q199","v":3.4000000999999997},{"$f":"+R200","v":0},{"$f":"+O199","v":4.2000000999999996},{"$f":"+T199","v":0},null,null,"x     lijevo      y",null,"x   centar   y","desno","x   desno   y","lijevo"]
[null,null,null,null,null,null,null,null,null,{"$f":"+J193","v":2},{"$f":"+K193","v":0.12820515121628623},"X","Y",null,{"$f":"+O198","v":4.9000010999999999},0,{"$f":"+O202","v":1.75},{"$f":"IF(Q196=2,0,P202*100)","v":{"$error":"#VALUE!"}},{"$f":"+S196","v":3.4000000999999997},{"$f":"+R199","v":{"$error":"#VALUE!"}},{"$f":"+O199","v":4.2000000999999996},{"$f":"+P199*100","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF('Unos podataka'!$O$48=\"DA\",2+'Analiza i dimenzioniranje'!E60,+Kontrafore!$AF$23)","v":1.75},{"$f":"+B228","v":9.6153895463470418E-2},{"$f":"+S196","v":3.4000000999999997},{"$f":"+AB198-'Analiza i dimenzioniranje'!C192","v":{"$error":"#VALUE!"}},{"$f":"+AA199","v":4.2000000999999996},{"$f":"+AB199","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!E59","v":3.4000000999999997},{"$f":"+Z200","v":{"$error":"#VALUE!"}},{"$f":"+IF('Unos podataka'!O48=\"DA\",0,R203)","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!O48=\"DA\",0,+R204)","v":{"$error":"#VALUE!"}},"lijevo",{"$f":"+'Analiza i dimenzioniranje'!H190","v":4.9000010999999999},{"$f":"-'Analiza i dimenzioniranje'!F190/100","v":{"$error":"#VALUE!"}},{"$f":"+O201","v":2},{"$f":"+P201*100","v":{"$error":"#VALUE!"}},{"$f":"+O199","v":4.2000000999999996},{"$f":"+P199*100","v":{"$error":"#VALUE!"}},{"$f":"+O198","v":4.9000010999999999},{"$f":"+P198*100","v":{"$error":"#VALUE!"}},null,null,{"$f":"+Kontrafore!$AF$23","v":1.75},{"$f":"+T209","v":{"$error":"#VALUE!"}},{"$f":"AA197-'Analiza i dimenzioniranje'!E60","v":3.4000000999999997},{"$f":"+Z199","v":{"$error":"#VALUE!"}},{"$f":"+AC197","v":4.2000000999999996},{"$f":"+AB200","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,{"$f":"+J198","v":3.4000000999999997},{"$f":"+K194","v":1.2},{"$f":"+T203","v":{"$error":"#VALUE!"}},{"$f":"+T204","v":{"$error":"#VALUE!"}},"sredina",{"$f":"+'Analiza i dimenzioniranje'!H191","v":4.2000000999999996},{"$f":"-'Analiza i dimenzioniranje'!F191/100","v":{"$error":"#VALUE!"}},{"$f":"+O200","v":3.4000000999999997},{"$f":"+P200*100","v":{"$error":"#VALUE!"}},{"$f":"+S198","v":4.2000000999999996},0,{"$f":"+U198","v":4.9000010999999999},0,"Vertikalne sile",null,{"$f":"2+'Analiza i dimenzioniranje'!E59","v":3.4000000999999997},{"$f":"+T209","v":{"$error":"#VALUE!"}},{"$f":"+S193","v":4.2000000999999996},{"$f":"+T193","v":{"$error":"#VALUE!"}},{"$f":"+U198","v":4.9000010999999999},{"$f":"+'Sile i krakovi'!AD197-'Analiza i dimenzioniranje'!C190","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,{"$f":"+J199+'Analiza i dimenzioniranje'!E55","v":4.2000000999999996},{"$f":"+AB200","v":{"$error":"#VALUE!"}},{"$f":"+V203","v":{"$error":"#VALUE!"}},{"$f":"+V204","v":{"$error":"#VALUE!"}},"desno",{"$f":"+'Analiza i dimenzioniranje'!H192","v":3.4000000999999997},{"$f":"-'Analiza i dimenzioniranje'!F192/100","v":{"$error":"#VALUE!"}},{"$f":"+Q199","v":3.4000000999999997},0,{"$f":"+S196","v":3.4000000999999997},{"$f":"+T196","v":0},{"$f":"+U196","v":4.2000000999999996},{"$f":"+V196","v":0},null,null,{"$f":"Y199+'Analiza i dimenzioniranje'!E60","v":3.4000000999999997},{"$f":"+AB201","v":{"$error":"#VALUE!"}},{"$f":"+AA199","v":4.2000000999999996},{"$f":"IF('Unos podataka'!$O$48=\"DA\",'Sile i krakovi'!B310,+AB199-'Analiza i dimenzioniranje'!C191)","v":{"$error":"#VALUE!"}},{"$f":"+AC199","v":4.9000010999999999},{"$f":"+AB199","v":{"$error":"#VALUE!"}}]
["Zid i temelj",null,null,null,null,null,null,null,null,{"$f":"+J200","v":4.2000000999999996},{"$f":"+K199","v":1.2},null,null,null,{"$f":"+'Analiza i dimenzioniranje'!H193","v":2},{"$f":"-'Analiza i dimenzioniranje'!F193/100","v":{"$error":"#VALUE!"}},{"$f":"+Q196","v":1.75},{"$f":"+R196","v":0},{"$f":"+S200","v":3.4000000999999997},{"$f":"+T200","v":0},{"$f":"+U200","v":4.2000000999999996},{"$f":"+V200","v":0},"kN",null,{"$f":"+Y197","v":1.75},{"$f":"IF('Analiza i dimenzioniranje'!D83>0,+Z197,0)","v":9.6153895463470418E-2},{"$f":"+AA197","v":3.4000000999999997},{"$f":"+AB197","v":{"$error":"#VALUE!"}},{"$f":"+AA199","v":4.2000000999999996},{"$f":"+AB199","v":{"$error":"#VALUE!"}},"Temelj"]
[{"$f":"+B7","v":2},0.12820515121628623,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!H194","v":1.75},{"$f":"+'Analiza i dimenzioniranje'!$I$194","v":{"$error":"#VALUE!"}},"A=",{"$f":"-0.5*((Q196*R197-Q197*R196)+(Q197*R198-Q198*R197)+(Q198*R199-Q199*R198)+(Q199*R200-Q200*R199)+(Q200*R201-Q201*R200))","v":{"$error":"#VALUE!"}},"A=",{"$f":"-0.5*((S196*T197-S197*T196)+(S197*T198-S198*T197)+(S198*T199-S199*T198)+(S199*T200-S200*T199)+(S200*T201-S201*T200))","v":{"$error":"#VALUE!"}},"A=",{"$f":"-0.5*((U196*V197-U197*V196)+(U197*V198-U198*V197)+(U198*V199-U199*V198)+(U199*V200-U200*V199)+(U200*V201-U201*V200))","v":{"$error":"#VALUE!"}},{"$f":"SUM(R202:V202)","v":{"$error":"#VALUE!"}},null,"A=",{"$f":"-0.5*(+(Y197*Z198-Y198*Z197)+(Y198*Z199-Y199*Z198)+(Y199*Z200-Y200*Z199)+(Y200*Z201-Y201*Z200))","v":{"$error":"#VALUE!"}},"A=",{"$f":"-0.5*(+(AA197*AB198-AA198*AB197)+(AA198*AB199-AA199*AB198)+(AA199*AB200-AA200*AB199)+(AA200*AB201-AA201*AB200))","v":{"$error":"#VALUE!"}},"A=",{"$f":"0.5*(+(AC197*AD198-AC198*AD197)+(AC198*AD199-AC199*AD198)+(AC199*AD200-AC200*AD199)+(AC200*AD201-AC201*AD200))","v":{"$error":"#VALUE!"}},"kN"]
[2,1.2,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!E59+'Analiza i dimenzioniranje'!E51","v":4.1000000999999999},null,null,null,null,{"$f":"+O202","v":1.75},0,"x=",{"$f":"-((Q196*R197-Q197*R196)*(Q196+Q197)+(Q197*R198-Q198*R197)*(Q197+Q198)+(Q198*R199-Q199*R198)*(Q198+Q199)+(Q199*R200-Q200*R199)*(Q199+Q200)+(Q200*R201-Q201*R200)*(Q200+Q201))/6/R202","v":{"$error":"#VALUE!"}},"x=",{"$f":"-((S196*T197-S197*T196)*(S196+S197)+(S197*T198-S198*T197)*(S197+S198)+(S198*T199-S199*T198)*(S198+S199)+(S199*T200-S200*T199)*(S199+S200)+(S200*T201-S201*T200)*(S200+S201))/6/T202","v":{"$error":"#VALUE!"}},"x=",{"$f":"-((U196*V197-U197*V196)*(U196+U197)+(U197*V198-U198*V197)*(U197+U198)+(U198*V199-U199*V198)*(U198+U199)+(U199*V200-U200*V199)*(U199+U200)+(U200*V201-U201*V200)*(U200+U201))/6/V202","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!B168","v":{"$error":"#VALUE!"}},null,"x=",{"$f":"-IF(Z202=0,0,((Y197*Z198-Y198*Z197)*(Y197+Y198)+(Y198*Z199-Y199*Z198)*(Y198+Y199)+(Y199*Z200-Y200*Z199)*(Y199+Y200)+(Y200*Z201-Y201*Z200)*(Y200+Y201))/6/Z202)","v":{"$error":"#VALUE!"}},"x=",{"$f":"-IF(AB202=0,0,((AA197*AB198-AA198*AB197)*(AA197+AA198)+(AA198*AB199-AA199*AB198)*(AA198+AA199)+(AA199*AB200-AA200*AB199)*(AA199+AA200)+(AA200*AB201-AA201*AB200)*(AA200+AA201))/6/AB202)","v":{"$error":"#VALUE!"}},"x=",{"$f":"IF(AD202=0,0,((AC197*AD198-AC198*AD197)*(AC197+AC198)+(AC198*AD199-AC199*AD198)*(AC198+AC199)+(AC199*AD200-AC200*AD199)*(AC199+AC200)+(AC200*AD201-AC201*AD200)*(AC200+AC201))/6/AD202)","v":{"$error":"#VALUE!"}}]
[3.4000010999999999,1.2,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+O197","v":4.9000010999999999},0,"Y=",{"$f":"-IF(R202=0,0,((Q197*R198-Q198*R197)*(R197+R198)+(Q198*R199-Q199*R198)*(R198+R199)+(Q199*R200-Q200*R199)*(R199+R200)+(Q200*R201-Q201*R200)*(R200+R201))/6/R202)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"-IF(T202=0,0,((S197*T198-S198*T197)*(T197+T198)+(S198*T199-S199*T198)*(T198+T199)+(S199*T200-S200*T199)*(T199+T200)+(S200*T201-S201*T200)*(T200+T201))/6/T202)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"-IF(V202=0,0,((U197*V198-U198*V197)*(V197+V198)+(U198*V199-U199*V198)*(V198+V199)+(U199*V200-U200*V199)*(V199+V200)+(U200*V201-U201*V200)*(V200+V201))/6/V202)","v":{"$error":"#VALUE!"}},{"$f":"+W202+W203","v":{"$error":"#VALUE!"}},null,"G=",{"$f":"+Z202*'Analiza i dimenzioniranje'!$E$62","v":{"$error":"#VALUE!"}},"G=",{"$f":"+AB202*'Analiza i dimenzioniranje'!$E$62","v":{"$error":"#VALUE!"}},"G=",{"$f":"+AD202*'Analiza i dimenzioniranje'!$E$62","v":{"$error":"#VALUE!"}},{"$f":"+Z204+AB204+AD204","v":{"$error":"#VALUE!"}}]
[{"$error":"#VALUE!"},3.14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"-IF(Z202=0,0,((Y197*Z198-Y198*Z197)*(Z197+Z198)+(Y198*Z199-Y199*Z198)*(Z198+Z199)+(Y199*Z200-Y200*Z199)*(Z199+Z200)+(Y200*Z201-Y201*Z200)*(Z200+Z201))/6/Z202)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"-IF(AB202=0,0,((AA197*AB198-AA198*AB197)*(AB197+AB198)+(AA198*AB199-AA199*AB198)*(AB198+AB199)+(AA199*AB200-AA200*AB199)*(AB199+AB200)+(AA200*AB201-AA201*AB200)*(AB200+AB201))/6/AB202)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"IF(AD202=0,0,((AC197*AD198-AC198*AD197)*(AD197+AD198)+(AC198*AD199-AC199*AD198)*(AD198+AD199)+(AC199*AD200-AC200*AD199)*(AD199+AD200)+(AC200*AD201-AC201*AD200)*(AD200+AD201))/6/AD202)","v":{"$error":"#VALUE!"}},{"$f":"+Z204+AB204+AD204","v":{"$error":"#VALUE!"}}]
[{"$error":"#VALUE!"},3.14,null,null,null,null,null,null,null,null,null,null,null,null,"Težište naprezanja",null,"Težište sila trenja",null,"Gornja linija za SM",null,"položaj djelovanja u presjecoma "]
[{"$error":"#VALUE!"},3.44,null,null,null,null,null,null,null,null,null,null,null,null,"x","y","x","y","x","y","x","y","presjek"]
[{"$error":"#VALUE!"},3.44,null,null,null,null,null,null,null,null,null,null,null,"lijevo",{"$f":"+R203","v":{"$error":"#VALUE!"}},null,{"$f":"(+S197-A218)/2+A218","v":2.5750000499999999},{"$f":"IF('Analiza i dimenzioniranje'!E59=0,0,+(Z200-C7)*(Q208-Q198)/(Q199-Q198)+C7)","v":{"$error":"#VALUE!"}},{"$f":"+Y199","v":3.4000000999999997},{"$f":"+Z199","v":{"$error":"#VALUE!"}},{"$f":"+AA197","v":3.4000000999999997},{"$f":"+(AB198-AB197)/2+AB197","v":{"$error":"#VALUE!"}},"II-II"]
[{"$error":"#VALUE!"},"A",null,null,null,null,null,null,null,null,null,null,null,"sredina",{"$f":"+T203","v":{"$error":"#VALUE!"}},null,{"$f":"+(U210-U208)/2+U208","v":3.8000000999999997},{"$f":"+(Z200+AB200)/2","v":{"$error":"#VALUE!"}},{"$f":"+AA199","v":4.2000000999999996},{"$f":"+AB199","v":{"$error":"#VALUE!"}},{"$f":"+(AA198+AA199)/2","v":3.8000000999999997},{"$f":"+AB198","v":{"$error":"#VALUE!"}},"između I-I i II-II na vrhu temelja"]
[{"$error":"#VALUE!"},"A",null,null,null,null,null,null,null,null,null,null,null,"desno",{"$f":"+V203","v":{"$error":"#VALUE!"}},null,{"$f":"+(AC200-AA200)/2+AA200","v":4.5500005999999997},{"$f":"+(AB200+AD199)/2","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AC197","v":4.2000000999999996},{"$f":"+(AB199-AB200)/2+AB200","v":{"$error":"#VALUE!"}},"I-I"]
[4.2000010999999997,1.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U209","v":3.8000000999999997},{"$f":"+R209","v":{"$error":"#VALUE!"}},"između I-I i II-II na dnu temelja"]
[4.2000010999999997,1.2]
[4.2000010999999997,1.2,null,"SVE SILE I MOMENTI"]
[4.9000021999999994,1.2,null,"HORIZONTALNE SILE",null,"Sila","Koord. djelovanja na zid",null,"Presjek II-II Lijevo",null,"Presjek I-I Desno ",null,"Presjek sredina dolje",null,"Presjek III-III",null,"MI-I","MII-II","MIII-III","Msred dole"]
[4.9000021999999994,0.5,null,"Koordinate djelovanja na zid   ",null,null,"x","y","koordinata y ","krak","koordinata y","krak","koordinata y","krak","koordinata y","krak"]
[2,0.12820515121628623,{"$f":"+F216+F217+F218","v":{"$error":"#VALUE!"}},"Eh1",null,{"$f":"+'Analiza i dimenzioniranje'!B120*'Analiza i dimenzioniranje'!I120","v":{"$error":"#VALUE!"}},{"$f":"+B112","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!B87","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+$B$203","v":1.2},{"$f":"+H216-O216","v":{"$error":"#VALUE!"}},null,null,{"$f":"+F216*P216","v":{"$error":"#VALUE!"}}]
["Reducirani temelj kontrafore",null,null,"Eh2",null,{"$f":"+'Analiza i dimenzioniranje'!B121*'Analiza i dimenzioniranje'!I121","v":{"$error":"#VALUE!"}},{"$f":"+B113","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!D87","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+$B$203","v":1.2},{"$f":"+H217-O217","v":{"$error":"#VALUE!"}},null,null,{"$f":"+F217*P217","v":{"$error":"#VALUE!"}}]
[{"$f":"+A224","v":1.75},{"$f":"+B224","v":9.6153895463470418E-2},null,"Eh3",null,{"$f":"+'Analiza i dimenzioniranje'!B122*'Analiza i dimenzioniranje'!I122","v":{"$error":"#VALUE!"}},{"$f":"+B114+'Analiza i dimenzioniranje'!E60","v":2},{"$f":"+'C III-V'!F87","v":{"$error":"#VALUE!"}},{"$f":"+V208","v":{"$error":"#VALUE!"}},{"$f":"H218-I218","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+J218*F218","v":{"$error":"#VALUE!"}}]
[{"$f":"+A222","v":2},{"$f":"+(2-B2)*C7","v":0.12820515121628623},{"$f":"+F219+F220","v":2.4299999999999997},"Ew-iza zida","iznad III-III",{"$f":"+H109*'Analiza i dimenzioniranje'!I123","v":0},{"$f":"+J119","v":2},{"$f":"+J120","v":0.19999999999999998},null,null,null,null,null,null,{"$f":"+B203","v":1.2},{"$f":"+H219-O219","v":-1},null,null,{"$f":"+F219*P219","v":0}]
[{"$f":"+A219","v":2},{"$f":"+C3","v":1.2},null,"Ew-iza zida","ispod III-III",{"$f":"+J118*'Analiza i dimenzioniranje'!I123","v":2.4299999999999997},{"$f":"+G218","v":2},{"$f":"+J111","v":0.19999999999999998},{"$f":"+V208","v":{"$error":"#VALUE!"}},{"$f":"+H220-I220","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+J220*F220","v":{"$error":"#VALUE!"}}]
[{"$f":"+B4","v":2},{"$f":"+C4","v":1.2},{"$f":"+F221+F222+F223+F224","v":{"$error":"#VALUE!"}},"E Prometno",null,{"$f":"+'Analiza i dimenzioniranje'!B124*'Analiza i dimenzioniranje'!I124","v":{"$error":"#VALUE!"}},null,{"$f":"+'HT III-XX'!G41","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+$B$203","v":1.2},{"$f":"+IF('Analiza i dimenzioniranje'!E44>0,0,H221-O221)","v":0},null,null,{"$f":"+F221*P221","v":{"$error":"#VALUE!"}}]
[{"$f":"+B5","v":2},{"$f":"+C5","v":0.12820515121628623},null,"E točkasto",null,{"$f":"IF('Analiza i dimenzioniranje'!E36=0,0.00001,+'Analiza i dimenzioniranje'!B125)*'Analiza i dimenzioniranje'!I125","v":{"$error":"#VALUE!"}},null,{"$f":"+'HT III-XX'!G81","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,1.2,{"$f":"+H222-O222","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[{"$f":"+A219","v":2},{"$f":"+B219","v":0.12820515121628623},null,"E Linijsko",null,{"$f":"+'Analiza i dimenzioniranje'!B126*'Analiza i dimenzioniranje'!I126","v":{"$error":"#VALUE!"}},null,{"$f":"+'HT III-XX'!G121","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,1.2,{"$f":"+H223-O223","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[{"$f":"+A223+'Analiza i dimenzioniranje'!$E$61-MT!$G$13","v":1.75},{"$f":"+Kontrafore!$B$17","v":9.6153895463470418E-2},null,"E Temelja",null,{"$f":"+'Analiza i dimenzioniranje'!B127*'Analiza i dimenzioniranje'!I127","v":{"$error":"#VALUE!"}},null,{"$f":"+T126","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,1.2,{"$f":"+H224-O224","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[{"$f":"+A224","v":1.75},{"$f":"+B220","v":1.2},null,"H Sidro",null,{"$f":"-'Analiza i dimenzioniranje'!B128*'Analiza i dimenzioniranje'!I128","v":-96.592582725499412},{"$f":"+B131","v":{"$error":"#VALUE!"}},{"$f":"+C131","v":3.9999999960000001},null,null,null,null,null,null,1.2,{"$f":"+H225-O225","v":2.7999999960000004},null,null,-270.45923124502804]
[{"$f":"+A220","v":2},{"$f":"+B220","v":1.2},{"$f":"+F226+F227","v":{"$error":"#VALUE!"}},"Potres            iznad III-III",null,{"$f":"+'C III-V'!AE114*'Analiza i dimenzioniranje'!I130","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AE112","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AE113","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,1.2,{"$f":"+H226-O226","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[{"$f":"+A226","v":2},{"$f":"+(A219-B2)*C7","v":0.12820515121628623},null,"Potres            ispod III-III",null,{"$f":"+'C III-V'!AH135*'Analiza i dimenzioniranje'!I130","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AM119","v":1.75},{"$f":"+'C III-V'!AJ135","v":0.83205129848782378},{"$f":"+V208","v":{"$error":"#VALUE!"}},{"$f":"+H227-I227","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+J227*F227","v":{"$error":"#VALUE!"}}]
[{"$f":"+A224","v":1.75},{"$f":"+B224","v":9.6153895463470418E-2},{"$f":"+F228+F229+F230","v":{"$error":"#VALUE!"}},"Trenje lijevo",null,{"$f":"-U191","v":{"$error":"#VALUE!"}},{"$f":"+Q208","v":2.5750000499999999},{"$error":"#VALUE!"},{"$f":"+V208","v":{"$error":"#VALUE!"}},{"$f":"+H228-I228","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+J228*F228","v":{"$error":"#VALUE!"}}]
[1,0,null,"Trenje sred",null,{"$f":"-U192","v":{"$error":"#VALUE!"}},3.8000000999999997,{"$error":"#VALUE!"},null,null,null,null,{"$f":"+B273","v":{"$error":"#VALUE!"}},{"$f":"+H229-M229","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+N229*F229","v":{"$error":"#VALUE!"}}]
[null,null,null,"Trenje desno",null,{"$f":"-U193","v":{"$error":"#VALUE!"}},4.5500005999999997,{"$error":"#VALUE!"},null,null,{"$f":"+V210","v":{"$error":"#VALUE!"}},{"$f":"+H230-K230","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+L230*F230","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"+F231+F232","v":0},"Voda ispred iznad III-III",null,{"$f":"-N109*'Analiza i dimenzioniranje'!I129","v":0},{"$f":"+N110","v":0},{"$f":"+N111","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+$B$203","v":1.2},{"$f":"+H231-O231","v":{"$error":"#VALUE!"}},null,null,{"$f":"+F231*P231","v":{"$error":"#VALUE!"}},null,{"$f":"+D231","v":"Voda ispred iznad III-III"}]
[null,null,null,"Voda ispred     do III-III",null,{"$f":"-L109*'Analiza i dimenzioniranje'!I129","v":0},{"$f":"+L110","v":2.6666666666666665},{"$f":"+L111","v":0.26666666666666672},null,null,{"$f":"+K230","v":{"$error":"#VALUE!"}},{"$f":"+H232-K232","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+L232*F232","v":{"$error":"#VALUE!"}},null,null,null,"Voda ispred     do III-III"]
[null,null,null,null,"SH=",{"$f":"SUM(F216:F232)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(Q214:Q232)","v":{"$error":"#VALUE!"}},{"$f":"SUM(R214:R232)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S214:S232)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T214:T232)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SMH=","MI-I","MII-II","MIII-III","Msred dole"]
[null,null,null,"VERTIKALNE SILE",null,"Sila /m'","koordinate",null,"Presjek II-II Lijevo",null,"Presjek I-I Desno ",null,"Presjek sredina dolje",null,"Presjek III-III sred. gore ",null,"MI-I","MII-II","MIII-III","Msred dole"]
[null,null,null,"Horiz. koordinat. presjeka",null,null,"x","y","koordinata  X ","krak","koordinata x","krak od A","koordinata x","krak","koordinata x","krak"]
[null,null,{"$f":"+F237+F238+F239","v":{"$error":"#VALUE!"}},"Ev1",null,{"$f":"+'Analiza i dimenzioniranje'!B146*'Analiza i dimenzioniranje'!I146","v":{"$error":"#VALUE!"}},{"$f":"+G216","v":{"$error":"#VALUE!"}},{"$f":"+H216","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!$E$59+'Analiza i dimenzioniranje'!$E$55/2","v":3.8000000999999997},{"$f":"+G237-O237","v":{"$error":"#VALUE!"}},null,null,{"$f":"+P237*F237","v":{"$error":"#VALUE!"}},null,"Ev1"]
[null,null,null,"Ev2",null,{"$f":"+'Analiza i dimenzioniranje'!B147*'Analiza i dimenzioniranje'!I147","v":{"$error":"#VALUE!"}},{"$f":"+G217","v":{"$error":"#VALUE!"}},{"$f":"+H217","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!$E$59+'Analiza i dimenzioniranje'!$E$55/2","v":3.8000000999999997},{"$f":"+G238-O238","v":{"$error":"#VALUE!"}},null,null,{"$f":"+P238*F238","v":{"$error":"#VALUE!"}},null,"Ev2"]
[null,null,null,"Ev3",null,{"$f":"+'Analiza i dimenzioniranje'!B148*'Analiza i dimenzioniranje'!I148","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$O$48=\"\",+G218+'Analiza i dimenzioniranje'!E60,A326)","v":2},null,{"$f":"2+'Analiza i dimenzioniranje'!$E$59+'Analiza i dimenzioniranje'!$E$60/2","v":3.4000000999999997},{"$f":"+G239-I239","v":-1.4000000999999997},null,null,null,null,null,null,null,{"$f":"+J239*F239","v":{"$error":"#VALUE!"}},null,null,"Ev3",null,null,"Analiza ravnoteže čvora između presjeka I-I, II-II, III-III i dna temelja u sredini"]
[null,null,{"$f":"+F240+F241+F242","v":{"$error":"#VALUE!"}},{"$f":"+U240","v":"G tem lijevo"},null,{"$f":"Z204*'Analiza i dimenzioniranje'!$I$135","v":{"$error":"#VALUE!"}},{"$f":"IF(O48=\"\",+Z203,0)","v":{"$error":"#VALUE!"}},null,{"$f":"2+'Analiza i dimenzioniranje'!$E$59+'Analiza i dimenzioniranje'!$E$60/2","v":3.4000000999999997},{"$f":"+G240-I240","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+J240*F240","v":{"$error":"#VALUE!"}},null,null,"G tem lijevo",null,null,null,null,null,"Sile","Krakovi","Momenti"]
[null,null,null,{"$f":"+U241","v":"G tem sred"},null,{"$f":"+AB204*'Analiza i dimenzioniranje'!$I$135","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!O48=\"\",+AB203,J335)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"IF('Unos podataka'!$O$48=\"\",2+'Analiza i dimenzioniranje'!E59+'Analiza i dimenzioniranje'!E55-'Analiza i dimenzioniranje'!E55/2,+A319)","v":3.8000000999999997},{"$f":"+G241-M241","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+N241*F241","v":{"$error":"#VALUE!"}},"G tem sred",null,null,"Q259","MI-I =",{"$f":"+Q259","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Sile i krakovi'!Q259","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+U242","v":"G tem desno"},null,{"$f":"AD204*'Analiza i dimenzioniranje'!$I$135","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!O48=\"\",+AD203,'Sile i krakovi'!L335)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+A212","v":4.2000010999999997},{"$f":"+G242-K242","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+L242*F242","v":{"$error":"#VALUE!"}},null,null,null,"G tem desno",null,null,"R259","MII-II =",{"$f":"+R259","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Sile i krakovi'!R259","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+U243","v":"G zid+konz"},null,{"$f":"+'C III-V'!D61*'Analiza i dimenzioniranje'!$I$136","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!D59","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!$E$59+'Analiza i dimenzioniranje'!$E$55/2","v":3.8000000999999997},{"$f":"+G243-O243","v":{"$error":"#VALUE!"}},null,null,{"$f":"+P243*F243","v":{"$error":"#VALUE!"}},null,"G zid+konz",null,null,"S259","MIII-III =",{"$f":"+S259","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Sile i krakovi'!S259","v":{"$error":"#VALUE!"}}]
[null,null,null,"G kontrafora",null,{"$f":"+Kontrafore!AC16*'Analiza i dimenzioniranje'!$I$137","v":{"$error":"#VALUE!"}},{"$f":"+Kontrafore!AC13","v":{"$error":"#VALUE!"}},null,{"$f":"2+'Analiza i dimenzioniranje'!$E$59+'Analiza i dimenzioniranje'!$E$60/2","v":3.4000000999999997},{"$f":"+G244-I244","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+J244*F244","v":{"$error":"#VALUE!"}},{"$f":"+P244*F244","v":{"$error":"#VALUE!"}},null,{"$f":"+D244","v":"G kontrafora"},null,null,"T259","Msr dole =",{"$f":"+T259","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Sile i krakovi'!T259","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+U245","v":"Gnasip-konz"},null,{"$f":"+'C III-V'!J61*'Analiza i dimenzioniranje'!$I$138","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!J59","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!$E$59+'Analiza i dimenzioniranje'!$E$55/2","v":3.8000000999999997},{"$f":"+G245-O245","v":{"$error":"#VALUE!"}},null,null,{"$f":"+P245*F245","v":{"$error":"#VALUE!"}},null,"Gnasip-konz",null,null,"U69","     v11=",{"$f":"+'Analiza i dimenzioniranje'!U69","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U69","v":{"$error":"#VALUE!"}},{"$f":"+('Sile i krakovi'!U210-'Sile i krakovi'!U208)","v":0.79999999999999982},{"$f":"+AA245*AB245","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+U246","v":"Gnasip iza zida"},null,{"$f":"+Kontrafore!L32*'Analiza i dimenzioniranje'!$I$139","v":{"$error":"#VALUE!"}},{"$f":"+Kontrafore!L33","v":{"$error":"#VALUE!"}},null,{"$f":"2+'Analiza i dimenzioniranje'!$E$59+'Analiza i dimenzioniranje'!$E$60/2","v":3.4000000999999997},{"$f":"+G246-I246","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+J246*F246","v":{"$error":"#VALUE!"}},null,null,"Gnasip iza zida",null,null,"U70","     h11=",{"$f":"+'Analiza i dimenzioniranje'!U70","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U70","v":{"$error":"#VALUE!"}},{"$f":"+('Sile i krakovi'!V210-'Sile i krakovi'!V208)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,"Gnasip ispred",null,{"$f":"+Kontrafore!W11*'Analiza i dimenzioniranje'!$I$140","v":{"$error":"#VALUE!"}},{"$f":"+Kontrafore!W9","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+K242","v":4.2000010999999997},{"$f":"+G247-K247","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+L247*F247","v":{"$error":"#VALUE!"}},null,null,null,"Gnasip ispred",null,null,"U71","     v22=",{"$f":"+'Analiza i dimenzioniranje'!U71","v":{"$error":"#VALUE!"}},{"$f":"+Z247","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,null,null,"V Promet",null,{"$f":"+'Analiza i dimenzioniranje'!B141*'Analiza i dimenzioniranje'!$I$141","v":{"$error":"#VALUE!"}},{"$f":"+'Rasprostiranje vertikalnog opt'!S30","v":{"$error":"#VALUE!"}},{"$f":"+H221","v":{"$error":"#VALUE!"}},{"$f":"2+'Analiza i dimenzioniranje'!$E$59+'Analiza i dimenzioniranje'!$E$60/2","v":3.4000000999999997},{"$f":"+G248-I248","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+J248*F248","v":{"$error":"#VALUE!"}},null,null,"V Promet",null,null,"U72","     h22=",{"$f":"+'Analiza i dimenzioniranje'!U72","v":{"$error":"#VALUE!"}},{"$f":"+Z248","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"}]
[null,null,null,"V Točkasto",null,{"$f":"+'Rasprostiranje vertikalnog opt'!R46*'Analiza i dimenzioniranje'!$I$142","v":{"$error":"#VALUE!"}},{"$f":"+'Rasprostiranje vertikalnog opt'!S48","v":{"$error":"#VALUE!"}},{"$f":"+H222","v":{"$error":"#VALUE!"}},{"$f":"2+'Analiza i dimenzioniranje'!$E$59+'Analiza i dimenzioniranje'!$E$60/2","v":3.4000000999999997},{"$f":"+G249-I249","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+J249*F249","v":{"$error":"#VALUE!"}},null,null,"V Točkasto",null,null,"U73","     v33=",{"$f":"+'Analiza i dimenzioniranje'!U73","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U73","v":{"$error":"#VALUE!"}},{"$f":"+('Sile i krakovi'!U209-'Sile i krakovi'!U208)","v":0.39999999999999991},{"$error":"#VALUE!"}]
[null,null,null,"V Linijsko",null,{"$f":"+'Rasprostiranje vertikalnog opt'!R37*'Analiza i dimenzioniranje'!$I$143","v":{"$error":"#VALUE!"}},{"$f":"+'Rasprostiranje vertikalnog opt'!S39","v":{"$error":"#VALUE!"}},{"$f":"+H223","v":{"$error":"#VALUE!"}},{"$f":"2+'Analiza i dimenzioniranje'!$E$59+'Analiza i dimenzioniranje'!$E$60/2","v":3.4000000999999997},{"$f":"+G250-I250","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+J250*F250","v":{"$error":"#VALUE!"}},null,null,"V Linijsko",null,null,"U74","     h33=",{"$f":"+'Analiza i dimenzioniranje'!U74","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U74","v":{"$error":"#VALUE!"}},{"$f":"+('Sile i krakovi'!V209-'Sile i krakovi'!V208)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,"V temelj",null,{"$f":"+'Rasprostiranje vertikalnog opt'!R19*'Analiza i dimenzioniranje'!$I$144","v":{"$error":"#VALUE!"}},{"$f":"+'Rasprostiranje vertikalnog opt'!S21","v":{"$error":"#VALUE!"}},{"$f":"+H224","v":{"$error":"#VALUE!"}},{"$f":"+I249","v":3.4000000999999997},{"$f":"+G251-I251","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+J251*F251","v":{"$error":"#VALUE!"}},null,null,"V temelj",null,null,"U75","     vtem=",{"$f":"+'Analiza i dimenzioniranje'!U75","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U75","v":{"$error":"#VALUE!"}},{"$f":"+('Sile i krakovi'!U209-'Sile i krakovi'!U208)","v":0.39999999999999991},{"$error":"#VALUE!"}]
[null,null,null,"V Sidra",null,{"$f":"+F131*'Analiza i dimenzioniranje'!$I$145","v":{"$error":"#VALUE!"}},{"$f":"+G225","v":{"$error":"#VALUE!"}},{"$f":"+H225","v":3.9999999960000001},null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!$E$59+'Analiza i dimenzioniranje'!$E$55/2","v":3.8000000999999997},{"$f":"+G252-O252","v":{"$error":"#VALUE!"}},null,null,{"$f":"+P252*F252","v":{"$error":"#VALUE!"}},null,"V Sidra",null,null,"U76","     htem=",{"$f":"+'Analiza i dimenzioniranje'!U76","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U76","v":{"$error":"#VALUE!"}},{"$f":"('Sile i krakovi'!V211-'Sile i krakovi'!V208)","v":{"$error":"#VALUE!"}},{"$f":"AA252*AB252","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"+F253+F254+F255","v":{"$error":"#VALUE!"}},"Naprezanja lijevo",null,{"$f":"R202","v":{"$error":"#VALUE!"}},{"$f":"IF(F253=0,0,R203)","v":{"$error":"#VALUE!"}},{"$f":"+R204","v":{"$error":"#VALUE!"}},{"$f":"2+'Analiza i dimenzioniranje'!$E$59+'Analiza i dimenzioniranje'!$E$60/2","v":3.4000000999999997},{"$f":"+G253-I253","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+J253*F253","v":{"$error":"#VALUE!"}},null,null,"Napr lijevo",null,null,null,null,null,null,"SM=",{"$f":"SUM(AC241:AC252)-AC254","v":{"$error":"#VALUE!"}},"kNm/m'"]
[null,null,null,"Naprezanja sred",null,{"$f":"+T202","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!O48=\"\",+T203,'Sile i krakovi'!F335)","v":{"$error":"#VALUE!"}},{"$f":"+T204","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"IF('Unos podataka'!$O$48=\"\",M241,+A319)","v":3.8000000999999997},{"$f":"+G254-M254","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+N254*F254","v":{"$error":"#VALUE!"}},"Napr sred",null,null,null,null,null,null,null,{"$f":"SUM(AC241:AC252)","v":{"$error":"#VALUE!"}}]
[null,null,null,"Naprezanja desno",null,{"$f":"+V202","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!O48=\"\",+V203,'Sile i krakovi'!H335)","v":{"$error":"#VALUE!"}},{"$f":"+V204","v":{"$error":"#VALUE!"}},null,null,{"$f":"+A212","v":4.2000010999999997},{"$f":"+G255-K255","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+L255*F255","v":{"$error":"#VALUE!"}},null,null,null,"Napr desno"]
[null,null,{"$f":"+F256+F257","v":{"$error":"#VALUE!"}},"Potres  v+",null,{"$f":"+'Analiza i dimenzioniranje'!B149*'Analiza i dimenzioniranje'!I149","v":0}]
[null,null,null,"Uzgon",null,{"$f":"+'Analiza i dimenzioniranje'!B150*'Analiza i dimenzioniranje'!I150","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"SV=",{"$f":"SUM(F237:F257)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"SMV=",{"$f":"SUM(Q240:Q257)","v":{"$error":"#VALUE!"}},{"$f":"SUM(R235:R257)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S237:S257)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T240:T256)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AC241:AC252)","v":{"$error":"#VALUE!"}},"kNm/m'",{"$f":"+Q258+Q233","v":{"$error":"#VALUE!"}},{"$f":"+R258+R233","v":{"$error":"#VALUE!"}},{"$f":"+S258+S233","v":{"$error":"#VALUE!"}},{"$f":"+T258+T233","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,"Presjek II-II Lijevo",null,"Presjek I-I Desno ",null,"Presjek sredina dolje",null,"Presjek III-III sred. gore ",null,"MI-I","MII-II","MIII-III","Msred dole"]
["Težište beton između I-I i II-II"]
[{"$f":"+A204","v":3.4000010999999999},1.2]
[{"$f":"+A211","v":4.2000010999999997},1.2]
[{"$f":"+A263","v":4.2000010999999997},{"$f":"+AD198","v":{"$error":"#VALUE!"}}]
[{"$f":"2+'Analiza i dimenzioniranje'!E59","v":3.4000000999999997},{"$f":"+Z200","v":{"$error":"#VALUE!"}}]
[{"$f":"+A262","v":3.4000010999999999},{"$f":"+B262","v":1.2}]
[{"$f":"+A265","v":3.4000000999999997},1.2]
["  A=",{"$f":"-0.5*((A262*B263-A263*B262)+(A263*B264-A264*B263)+(A264*B265-A265*B264)+(A265*B266-A266*B265))","v":{"$error":"#VALUE!"}}]
["xt=",{"$f":"-((A262*B263-A263*B262)*(A262+A263)+(A263*B264-A264*B263)*(A263+A264)+(A264*B265-A265*B264)*(A264+A265)+(A265*B266-A266*B265)*(A265+A266)+(A266*B267-A267*B266)*(A266+A267)+(A267*Y271-X272*B267)*(A267+X272)+(X272*Y272-X273*Y271)*(X272+X273)+(X273*Y273-X274*Y272)*(X273+X274))/6/B268","v":{"$error":"#VALUE!"}}]
["yt=",{"$f":"-((A262*B263-A263*B262)*(B262+B263)+(A263*B264-A264*B263)*(B263+B264)+(A264*B265-A265*B264)*(B264+B265)+(A265*B266-A266*B265)*(B265+B266)+(A266*B267-A267*B266)*(B266+B267)+(A267*Y271-X272*B267)*(B267+Y271)+(X272*Y272-X273*Y271)*(Y271+Y272)+(X273*Y273-X274*Y272)*(Y272+Y273))/6/B268","v":{"$error":"#VALUE!"}}]
[]
["Koord. Temelja dole sredina"]
[{"$f":"+(+A265+A264)/2","v":3.8000005999999997},{"$f":"+(B264+B265)/2","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"SM="]
["sredina dna kada nema KF"]
[{"$f":"+(S198-'Analiza i dimenzioniranje'!H195)/2+'Analiza i dimenzioniranje'!H195","v":2.6000000499999998},{"$f":"+AD198/2","v":{"$error":"#VALUE!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"y=",{"$f":"B262-0.723","v":0.47699999999999998},{"$f":"1.2-0.287","v":0.91300000000000003},{"$f":"1.2-1.2","v":0},{"$f":"1.2-0.764","v":0.43599999999999994}]
["Temelj masivnog zida",null,null,null,null,null,null,null,null,null,"x=",{"$f":"4.2-3.4","v":0.80000000000000027},{"$f":"4.2-3.8","v":0.40000000000000036},{"$f":"4.2-3.8","v":0.40000000000000036},{"$f":"4.2-4.2","v":0}]
[{"$f":"2+'Unos podataka'!O46","v":2.3359999999999999},0,null,null,null,null,null,null,null,null,null,"II    ","DOLE   ","   III","I"]
[2,{"$f":"+'Unos podataka'!O41","v":1.6800000000000002}]
[2,{"$f":"+'Unos podataka'!O38","v":6}]
[{"$f":"2+'Unos podataka'!O42","v":3.4},{"$f":"+B301","v":6}]
[{"$f":"2+'Unos podataka'!O43","v":4.26},{"$f":"+B300","v":1.6800000000000002}]
[{"$f":"+A303+'Unos podataka'!O44","v":5.0999999999999996},{"$f":"+B303","v":1.6800000000000002}]
[{"$f":"+A304","v":5.0999999999999996},{"$f":"+B304-'Unos podataka'!O40","v":0.62000000000000011}]
[{"$f":"+A299","v":2.3359999999999999},{"$f":"+B299","v":0}]
[]
["Presjek I-I"]
[{"$f":"+A303","v":4.26},{"$f":"+B303","v":1.6800000000000002}]
[{"$f":"+A309","v":4.26},{"$f":"+(B305-B306)*(A303-A306)/(A305-A306)","v":0.43157742402315497}]
[]
["Težište vertikale   I-I"]
[{"$f":"+A303","v":4.26},{"$f":"+B310+(B303-B310)/2","v":1.0557887120115776}]
[]
["Težište na dnu desno do  I-I"]
[{"$f":"+A309+(A305-A303)/2","v":4.68},{"$f":"+(B305+B310)/2","v":0.52578871201157751}]
[]
["Težište  I-I do II-II na dnu"]
[{"$f":"2+'Analiza i dimenzioniranje'!E60+(A310-A323)/2","v":2.9619999999999997},{"$f":"+(B310+B306)/2","v":0.21578871201157748}]
[]
["Presjek II-II"]
[{"$f":"+A300","v":2},{"$f":"+B300","v":1.6800000000000002}]
[{"$f":"+A299","v":2.3359999999999999},{"$f":"+B299","v":0}]
[]
["Težište \"vertikale\"   II-II"]
[{"$f":"+(A322+A323)/2","v":2.1680000000000001},{"$f":"+(B322+B323)/2","v":0.84000000000000008},null,null,"Kontrola samo gravitacionog zida",null,null,null,null,null,null,null,"Kontrola momenata destabilnosti i stabilnoati oko točke \"A\"",null,null,null,null,null,null,null,null,null,4.7119999999999997]
[null,null,null,null,"SILA NAPREZANJA NA DNO TEMELJA ",null,null,null,"MASA GRAVITACIONOG ZIDA",null,null,null,"Vrh temelja ispod zida",null,"Momenti destabilnosti",null,null,null,"Momenti stabilnosti"]
[null,null,null,null,"Temelj sredina",null,"temelj desno",null,"mase temelja  lijevo do I-I",null,"mase temelja  desno od I-I",null,"x","y","naziv sile","sila","Krak","Moment","naziv sile","sila","Krak","Moment"]
[null,null,null,null,{"$f":"+A323","v":2.3359999999999999},{"$f":"+B323","v":0},{"$f":"+'Analiza i dimenzioniranje'!H191","v":4.2000000999999996},0,{"$f":"+A299","v":2.3359999999999999},{"$f":"+B299","v":0},{"$f":"+A310","v":4.26},{"$f":"+B310","v":0.43157742402315497},{"$f":"+S208","v":3.4000000999999997},{"$f":"+T208","v":{"$error":"#VALUE!"}},"EH1",{"$f":"+'Analiza i dimenzioniranje'!B120","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C120","v":{"$error":"#VALUE!"}},{"$f":"+P329*Q329","v":{"$error":"#VALUE!"}},"Gtem ..........................",{"$f":"+'Analiza i dimenzioniranje'!B135","v":{"$error":"#VALUE!"}},{"$f":"+K331-J345","v":1.5826390360750926},{"$f":"+U329*T329","v":{"$error":"#VALUE!"}}]
[null,null,null,null,{"$f":"+E329","v":2.3359999999999999},{"$f":"-'Analiza i dimenzioniranje'!F192/100","v":{"$error":"#VALUE!"}},{"$f":"+G329","v":4.2000000999999996},{"$f":"-'Analiza i dimenzioniranje'!F191/100","v":{"$error":"#VALUE!"}},{"$f":"+A300","v":2},{"$f":"+B300","v":1.6800000000000002},{"$f":"+K329","v":4.26},{"$f":"+B300","v":1.6800000000000002},{"$f":"+S209","v":4.2000000999999996},{"$f":"+T209","v":{"$error":"#VALUE!"}},"EH2",{"$f":"+'Analiza i dimenzioniranje'!B121","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C121","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Gzid+konz ...................",{"$f":"+'Analiza i dimenzioniranje'!B136","v":{"$error":"#VALUE!"}},{"$f":"+K331-N345","v":2.1681602914389795},{"$f":"+U330*T330","v":{"$error":"#VALUE!"}}]
[null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!H191","v":4.2000000999999996},{"$f":"+H330","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!H190","v":4.9000010999999999},{"$f":"-'Analiza i dimenzioniranje'!F190/100","v":{"$error":"#VALUE!"}},{"$f":"+A303","v":4.26},{"$f":"+B303","v":1.6800000000000002},{"$f":"+A304","v":5.0999999999999996},{"$f":"B304","v":1.6800000000000002},"Težiše  spojnice na vrhu temelja",null,"EH3",{"$f":"+'Analiza i dimenzioniranje'!B122","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C122","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Grebra kontrafora ............",{"$f":"+'Analiza i dimenzioniranje'!B137","v":{"$error":"#VALUE!"}}]
[null,null,null,null,{"$f":"+E331","v":4.2000000999999996},0,{"$f":"+G331","v":4.9000010999999999},{"$f":"+H329","v":0},{"$f":"+I331","v":4.26},{"$f":"+B310","v":0.43157742402315497},{"$f":"+K331","v":5.0999999999999996},{"$f":"+B305","v":0.62000000000000011},{"$f":"2+(M330-M329)/2","v":2.4},{"$f":"+N330","v":{"$error":"#VALUE!"}},"Hvode iza",{"$f":"+J109","v":1.7999999999999998},{"$f":"+'Analiza i dimenzioniranje'!C123","v":-0.30000000000000004},-0.54,"Gnasip na konzoli ............",{"$f":"+'Analiza i dimenzioniranje'!B138","v":{"$error":"#VALUE!"}}]
[null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!H193","v":2},0,{"$f":"+G329","v":4.2000000999999996},{"$f":"+H329","v":0},{"$f":"+I329","v":2.3359999999999999},{"$f":"+J329","v":0},{"$f":"+A303","v":4.26},{"$f":"+L329","v":0.43157742402315497},null,null,{"$f":"+'Analiza i dimenzioniranje'!A124","v":"EPrometno ...................."},{"$f":"+'Analiza i dimenzioniranje'!B124","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C124","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Gnasipa iza zida .............",{"$f":"+'Analiza i dimenzioniranje'!B139","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+F334*100+H334*100","v":{"$error":"#VALUE!"}},"A=",{"$f":"(0.5*((E329*F330-E330*F329)+(E330*F331-E331*F330)+(E331*F332-E332*F331)+(E332*F333-E333*F332)))","v":{"$error":"#VALUE!"}},"A=",{"$f":"(0.5*((G329*H330-G330*H329)+(G330*H331-G331*H330)+(G331*H332-G332*H331)+(G332*H333-G333*H332)))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-(0.5*((I329*J330-I330*J329)+(I330*J331-I331*J330)+(I331*J332-I332*J331)+(I332*J333-I333*J332)))","v":3.0993825180897252},"F=",{"$f":"-(0.5*((K329*L330-K330*L329)+(K330*L331-K331*L330)+(K331*L332-K332*L331)+(K332*L333-K333*L332)))","v":0.96953748191027378},"Točka \"A\"",null,{"$f":"+'Analiza i dimenzioniranje'!A125","v":"EPTočkasto ...................."},{"$f":"+'Analiza i dimenzioniranje'!B125","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C125","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Gnasipa ispred zida .........",{"$f":"+'Analiza i dimenzioniranje'!B140","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"x=",{"$f":"((E329*F330-E330*F329)*(E329+E330)+(E330*F331-E331*F330)*(E330+E331)+(E331*F332-E332*F331)*(E331+E332)+(E332*F333-E333*F332)*(E332+E333))/6/F334","v":{"$error":"#VALUE!"}},"x=",{"$f":"((G329*H330-G330*H329)*(G329+G330)+(G330*H331-G331*H330)*(G330+G331)+(G331*H332-G332*H331)*(G331+G332)+(G332*H333-G333*H332)*(G332+G333))/6/H334","v":{"$error":"#VALUE!"}},"x=",{"$f":"-((I329*J330-I330*J329)*(I329+I330)+(I330*J331-I331*J330)*(I330+I331)+(I331*J332-I332*J331)*(I331+I332)+(I332*J333-I333*J332)*(I332+I333))/6/J334","v":3.1572431438672135},"x=",{"$f":"-((K329*L330-K330*L329)*(K329+K330)+(K330*L331-K331*L330)*(K330+K331)+(K331*L332-K332*L331)*(K331+K332)+(K332*L333-K333*L332)*(K332+K333))/6/L334","v":4.6685726465720467},"x","y",{"$f":"+'Analiza i dimenzioniranje'!A126","v":"EPLinijsko ....................."},{"$f":"+'Analiza i dimenzioniranje'!B126","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C126","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"PPrometno ...................",{"$f":"+'Analiza i dimenzioniranje'!B141","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"Y=",{"$f":"-((E329*F330-E330*F329)*(F329+F330)+(E330*F331-E331*F330)*(F330+F331)+(E331*F332-E332*F331)*(F331+F332)+(E332*F333-E333*F332)*(F332+F333))/6/F334","v":{"$error":"#VALUE!"}},"Y=",{"$f":"-((G329*H330-G330*H329)*(H329+H330)+(G330*H331-G331*H330)*(H330+H331)+(G331*H332-G332*H331)*(H331+H332)+(G332*H333-G333*H332)*(H332+H333))/6/H334","v":{"$error":"#VALUE!"}},"Y=",{"$f":"-((I329*J330-I330*J329)*(J329+J330)+(I330*J331-I331*J330)*(J330+J331)+(I331*J332-I332*J331)*(J331+J332)+(I332*J333-I333*J332)*(J332+J333))/6/J334","v":0.95874920459308866},"Y=",{"$f":"-((K329*L330-K330*L329)*(L329+L330)+(K330*L331-K331*L330)*(L330+L331)+(K331*L332-K332*L331)*(L331+L332)+(K332*L333-K333*L332)*(L332+L333))/6/L334","v":1.1016127063810903},{"$f":"+K332","v":5.0999999999999996},{"$f":"+L332","v":0.62000000000000011},{"$f":"+'Analiza i dimenzioniranje'!A127","v":"EQTemelj ili vozilo....................."},{"$f":"+'Analiza i dimenzioniranje'!B127","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C127","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"PTočkasto ....................",{"$f":"+'Analiza i dimenzioniranje'!B142","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,"S=",{"$f":"+J337+L337","v":101.72299999999997},"GT lijevo=",{"$f":"+J334*'Analiza i dimenzioniranje'!$E$62","v":77.484562952243124},"GT desno=",{"$f":"+L334*'Analiza i dimenzioniranje'!$E$62","v":24.238437047756843},null,null,{"$f":"+'Analiza i dimenzioniranje'!A130","v":"HPotres ........................"},{"$f":"+'Analiza i dimenzioniranje'!B130","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C130","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"PLinijsko ......................",{"$f":"+'Analiza i dimenzioniranje'!B143","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"koordinate sile trenja",null,null,null,"koordinate težišta mase",null,null,null,"Masa zida",null,{"$f":"+'Analiza i dimenzioniranje'!A149","v":"Vpotres........................"},{"$f":"+'Analiza i dimenzioniranje'!B149","v":0},{"$f":"+'Analiza i dimenzioniranje'!C149","v":0},0,"QTemelj ......................",{"$f":"+'Analiza i dimenzioniranje'!B144","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"x= ",{"$f":"+(E331-E330)/2+E330","v":3.2680000499999995},null,{"$f":"+(G331-G330)/2+G330","v":4.5500005999999997},null,{"$f":"+(I331-I330)/2+I330","v":3.13},null,{"$f":"+(K331-K330)/2+K330","v":4.68},{"$f":"+I330","v":2},{"$f":"+J330","v":1.6800000000000002},null,null,"SMH=",{"$f":"SUM(R329:R338)","v":{"$error":"#VALUE!"}},"VSidro ........................",{"$f":"+'Analiza i dimenzioniranje'!B145","v":25.881904536133977}]
[null,null,null,null,"y= ",{"$f":"+(F331+F330)/2","v":{"$error":"#VALUE!"}},null,{"$f":"+(H331+H330)/2","v":{"$error":"#VALUE!"}},null,{"$f":"+(J331+J330)/2","v":1.6800000000000002},null,{"$f":"+(L331+L330)/2-0.24","v":1.4400000000000002},{"$f":"+A301","v":2},6,null,null,null,null,"Ev1 ...........................",{"$f":"+'Analiza i dimenzioniranje'!B146","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,3.4,6,null,null,null,null,"Ev2  ..........................",{"$f":"+'Analiza i dimenzioniranje'!B147","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,4.26,1.6800000000000002,null,null,null,null,"Ev3  ..........................",{"$f":"+'Analiza i dimenzioniranje'!B148","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M339","v":2},{"$f":"+N339","v":1.6800000000000002},null,null,null,null,"VPotres ........................",{"$f":"+'Analiza i dimenzioniranje'!B151","v":0}]
[null,null,null,null,null,null,null,null,"F=",{"$f":"+J337+L337","v":101.72299999999997},null,null,"F=",{"$f":"-(0.5*((M339*N340-M340*N339)+(M340*N341-M341*N340)+(M341*N342-M342*N341)+(M342*N343-M343*N342)))","v":7.905599999999998},null,null,null,null,"HSidro (hor. sila)........................",{"$f":"+'Analiza i dimenzioniranje'!B128","v":96.592582725499412}]
[null,null,null,null,null,null,null,null,"x=",{"$f":"+(J335*J337+L335*L337)/(J337+L337)","v":3.517360963924907},null,null,"x=",{"$f":"-((M339*N340-M340*N339)*(M339+M340)+(M340*N341-M341*N340)*(M340+M341)+(M341*N342-M342*N341)*(M341+M342)+(M342*N343-M343*N342)*(M342+M343))/6/N344","v":2.9318397085610202},null,null,null,null,"Hvoda ispred zida (hor sila)...............",{"$f":"+'Analiza i dimenzioniranje'!B129","v":3.2}]
[null,null,null,null,null,null,null,null,"Y=",{"$f":"+(J336*J337+L336*L337)/(J337+L337)","v":0.99279055212030054},null,null,"Y=",{"$f":"-((M339*N340-M340*N339)*(N339+N340)+(M340*N341-M341*N340)*(N340+N341)+(M341*N342-M342*N341)*(N341+N342)+(M342*N343-M343*N342)*(N342+N343))/6/N344","v":3.6708196721311479},null,null,null,null,"+"]
[null,null,null,null,null,null,null,null,null,null,null,null,"GT lijevo=",{"$f":"+N344*'Analiza i dimenzioniranje'!$E$62","v":197.63999999999996}]

{"sheet":"Dodatni proračuni","index":5,"n_rows":31,"n_cols":37,"rows_kept":31,"cut":false,"hidden":true,"merged":[[26,27,26,28],[0,29,0,36],[23,27,23,28],[5,18,5,26],[8,18,8,26],[0,27,0,28],[16,27,16,28],[20,27,20,28],[17,27,17,28],[0,18,0,20],[0,21,0,23],[0,24,0,26],[21,30,21,31],[26,30,26,31]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"visine presjeka",null,null,"Kontaktni naponi",null,null,"dimenzije temelja",null,null,"koordinate zida s temeljem",null,"Komponente horiz sila sila"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," hA=",{"$f":"+'Analiza i dimenzioniranje'!C190","v":0.7},"C174","sA=",{"$f":"+'Analiza i dimenzioniranje'!F190","v":{"$error":"#VALUE!"}},"F174","b2=",{"$f":"+'Analiza i dimenzioniranje'!E59","v":1.4000001},"E58",{"$f":"+'C III-V'!B2","v":2},{"$f":"+'C III-V'!C2","v":0.12820515121628623},null,"sila","krak do A","koordin.  Y",null,"sila","krak do A","koordin.  X"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   dl-l=",{"$f":"+'Analiza i dimenzioniranje'!C191","v":0.78974368014459062},"C175"," s l-l=",{"$f":"+'Analiza i dimenzioniranje'!F191","v":{"$error":"#VALUE!"}},"F175","d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"E54",{"$f":"+'C III-V'!B3","v":2},{"$f":"+'C III-V'!C3","v":1.2},null,null,null,null,"Gtem ..........................",{"$f":"+'Analiza i dimenzioniranje'!B135","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C135","v":{"$error":"#VALUE!"}},{"$f":"2+$Z$5-AJ3","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," dll-ll=",{"$f":"+'Analiza i dimenzioniranje'!C192","v":0.89230772485205256},"C176"," sll-ll=",{"$f":"+'Analiza i dimenzioniranje'!F192","v":{"$error":"#VALUE!"}},"F176","B-b2-d1=",{"$f":"+'Analiza i dimenzioniranje'!E61-Z2-Z3","v":0.70000209999999941},"E50-E58-E54",{"$f":"+'C III-V'!B4","v":3.4000010999999999},{"$f":"+'C III-V'!C4","v":1.2},null,null,null,null,"Gzid+konz ...................",{"$f":"+'Analiza i dimenzioniranje'!B136","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C136","v":{"$error":"#VALUE!"}},{"$f":"2+$Z$5-AJ4","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," hB=",{"$f":"+'Analiza i dimenzioniranje'!C193","v":1.0728357545883234},"C177","sB=",{"$f":"+'Analiza i dimenzioniranje'!F193","v":{"$error":"#VALUE!"}},"F177","B=",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},{"$f":"+T5-T2","v":0.37283575458832341},{"$f":"+'C III-V'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C5","v":3.14},null,null,null,null,"Gnasip na konzoli ............",{"$f":"+'Analiza i dimenzioniranje'!B138","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C138","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Težišta - udaljenost od lijevog ruba elementa i od točke B",null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B6","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C6","v":3.14},"HPotres ........................",{"$f":"+'Analiza i dimenzioniranje'!B130","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C130","v":{"$error":"#VALUE!"}},{"$f":"+$AA$5+AF6","v":{"$error":"#VALUE!"}},"Gnasipa iza zida .............",{"$f":"+'Analiza i dimenzioniranje'!B139","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C139","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x1=",{"$f":"(T4*Z2*Z2*0.5+Z2*(T5-T4)*0.5*Z2/3)/((T5+T4)*Z2*0.5)","v":0.67856486707928043},{"$f":"2+T7","v":2.6785648670792805},"x2=",{"$f":"(T3*Z3*Z3*0.5+Z3*(T4-T3)*0.5*Z3/3)/((T4+T3)*Z3*0.5)","v":0.39186992387963182},{"$f":"2+Z2+W7","v":3.7918700238796315},"x3=",{"$f":"(T2*Z4*Z4*0.5+Z4*(T3-T2)*0.5*Z4/3)/((T3+T2)*Z4*0.5)","v":0.34297290981272888},{"$f":"2+Z2+Z3+Z7","v":4.5429730098127283},{"$f":"+'C III-V'!B7","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C7","v":3.44},"Ehw ...........................",{"$f":"+'Analiza i dimenzioniranje'!B123","v":1.7999999999999998},{"$f":"+'Analiza i dimenzioniranje'!C123","v":-0.30000000000000004},{"$f":"+$AA$5+AF7","v":7.2835754588323365E-2},"Gnasipa ispred zida .........",{"$f":"+'Analiza i dimenzioniranje'!B140","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C140","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y1=",{"$f":"+T5/2","v":0.53641787729416168},null,"y2=",{"$f":"+T4*0.5+(T5-T4)","v":0.62668189216229708},null,"y2=",{"$f":"+T4*0.5+(T4-T3)","v":0.54871790713348823},null,{"$f":"+'C III-V'!B8","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C8","v":3.44},"EPrometno ....................",{"$f":"+'Analiza i dimenzioniranje'!B124","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C124","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"PPrometno ...................",{"$f":"+'Analiza i dimenzioniranje'!B141","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C141","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X  koordinata za trenje na bazi temelja",null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B9","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C9","v":"A"},"EPTočkasto ....................",{"$f":"+'Analiza i dimenzioniranje'!B125","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C125","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"PTočkasto ....................",{"$f":"+'Analiza i dimenzioniranje'!B142","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C142","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x1=",{"$f":"2+Z2/2","v":2.7000000499999999},null,"x2=",{"$f":"2+Z2+Z3/2","v":3.8000000999999997},null,"x3=",{"$f":"(W2*Z4*Z4*0.5+Z4*(W3-W2)*0.5*Z4/3)/((W3+W2)*Z4*0.5)","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!B10","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C10","v":"A"},"EPLinijsko .....................",{"$f":"+'Analiza i dimenzioniranje'!B126","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C126","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"PLinijsko ......................",{"$f":"+'Analiza i dimenzioniranje'!B143","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C143","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y1=",{"$f":"IF(T2=T5,0,+Z2*0.5/'Analiza i dimenzioniranje'!$E$53)","v":8.9743545529282015E-2},null,"y2=",{"$f":"IF(T2=T5,0,(Z2+Z3*0.5)/'Analiza i dimenzioniranje'!$E$53)","v":0.23076911341229506},null,"y3=",{"$f":"IF(T2=T5,0,(Z2+Z3+Z4*0.5)/'Analiza i dimenzioniranje'!$E$53)","v":0.32692303994084931},null,{"$f":"+'C III-V'!B11","v":4.2000010999999997},{"$f":"+'C III-V'!C11","v":1.2},"EQTemelj ......................",{"$f":"+'Analiza i dimenzioniranje'!B127","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C127","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"QTemelj ......................",{"$f":"+'Analiza i dimenzioniranje'!B144","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C144","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B12","v":4.2000010999999997},{"$f":"+'C III-V'!C12","v":1.2},"HSidro ........................",{"$f":"+'Analiza i dimenzioniranje'!B128","v":96.592582725499412},{"$f":"+'Analiza i dimenzioniranje'!C128","v":3.4999999960000001},3.8728357505883233,"VSidro ........................",{"$f":"+'Analiza i dimenzioniranje'!B145","v":25.881904536133977},{"$f":"+'Analiza i dimenzioniranje'!C145","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B13","v":4.2000010999999997},{"$f":"+'C III-V'!C13","v":1.2},"Eh1 ............................",{"$f":"+'Analiza i dimenzioniranje'!B120","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C120","v":{"$error":"#VALUE!"}},{"$f":"+$AA$5+AF13","v":{"$error":"#VALUE!"}},"Ev1 ...........................",{"$f":"+'Analiza i dimenzioniranje'!B146","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C146","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"krak E3",{"$f":"+T4*0.5-'C III-V'!F87","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+'C III-V'!B14","v":4.9000021999999994},{"$f":"+'C III-V'!C14","v":1.2},"Eh2 ............................",{"$f":"+'Analiza i dimenzioniranje'!B121","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C121","v":{"$error":"#VALUE!"}},{"$f":"+$AA$5+AF14","v":{"$error":"#VALUE!"}},"Ev2  ..........................",{"$f":"+'Analiza i dimenzioniranje'!B147","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C147","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"krak  Vt",{"$f":"1-T7","v":0.32143513292071957},null,null,null,null,null,null,null,{"$f":"+'C III-V'!B15","v":4.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5},"Eh3 ............................",{"$f":"+'Analiza i dimenzioniranje'!B122","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C122","v":{"$error":"#VALUE!"}},{"$f":"+$AA$5+AF15","v":{"$error":"#VALUE!"}},"Ev3  ..........................",{"$f":"+'Analiza i dimenzioniranje'!B148","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C148","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B16","v":2},{"$f":"+'C III-V'!C16","v":0.12820515121628623},"SRh=",{"$f":"SUM(AE6:AE15)","v":{"$error":"#VALUE!"}},"kn",null,"SRv=",{"$f":"SUM(AI3:AI15)","v":{"$error":"#VALUE!"}},"kn"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"linije presjeka"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"krakEt",{"$f":"+T4/2-T11","v":0.35641031689674429},null,null,null,null,null,null,null,"Presjek I-I"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AB22+Z3","v":4.2000000999999996},{"$f":"+AC22","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AB19","v":4.2000000999999996},{"$f":"+AC23","v":1.3728357545883234}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek II-II"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+Z2","v":3.4000000999999997},0,null,"Ver Komponente  betona"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AB22","v":3.4000000999999997},{"$f":"+T5+0.3","v":1.3728357545883234},null,"B     II-II",{"$f":"+(T4+T5)*Z2*'Analiza i dimenzioniranje'!E62/2","v":34.390013346635925}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek III-III",null,null,"II-II     I-I",{"$f":"+(T3+T4)*Z3*'Analiza i dimenzioniranje'!E62/2","v":16.820514049966434}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+Z2-0.25","v":3.1500000999999997},{"$f":"+T5","v":1.0728357545883234},null,"I-I      A",{"$f":"+(T2+T3)*Z4*'Analiza i dimenzioniranje'!E62/2","v":13.035296307036761}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+Z2+Z3+0.25","v":4.4500000999999996},{"$f":"+AC25","v":1.0728357545883234},"kn","S=",{"$f":"SUM(AF23:AF25)","v":64.245823703639118}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hor Komponente trenja",null,"kn","Ver Komponente  napona"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B     II-II",{"$f":"+Z2*AE16/Z5","v":{"$error":"#VALUE!"}},"kn","B     II-II",{"$f":"+(W4+W5)*Z2/2","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"II-II     I-I",{"$f":"+Z3*AE16/Z5","v":{"$error":"#VALUE!"}},"kn","II-II     I-I",{"$f":"+(W3+W4)*Z3/2","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"I-I      A",{"$f":"+Z4*AE16/Z5","v":{"$error":"#VALUE!"}},"kn","I-I      A",{"$f":"+(W2+W3)*Z4/2","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S=",{"$f":"SUM(AC28:AC30)","v":{"$error":"#VALUE!"}},null,"S=",{"$f":"SUM(AF28:AF30)","v":{"$error":"#VALUE!"}}]

{"sheet":"Rasprostiranje vertikalnog opt","index":6,"n_rows":67,"n_cols":24,"rows_kept":67,"cut":false,"hidden":true,"merged":[[46,12,46,13],[39,8,39,11],[43,8,43,11],[15,17,15,18],[24,17,24,18],[33,17,33,18],[42,17,42,18],[22,15,22,16],[31,15,31,16],[40,15,40,16],[37,12,37,13],[12,20,12,23],[32,20,32,23],[6,12,6,18],[13,15,13,16],[19,12,19,13],[29,12,29,13],[28,12,28,13],[30,0,30,2],[35,0,35,2],[42,0,42,2],[21,0,21,2],[13,20,13,21],[36,1,36,3]]}
[null,null,null,"Rasprostiranje vertikalnog opterećenja"]
[]
[null,null,null,"koordinate zida i opterećenja"]
[]
["Točke",{"$f":"+'C III-V'!B1","v":"ZID I TEMELJ"}]
[1,{"$f":"+'C III-V'!B2","v":2},{"$f":"+'C III-V'!C2","v":0.12820515121628623}]
[2,{"$f":"+'C III-V'!B3","v":2},{"$f":"+'C III-V'!C3","v":1.2},null,null,null,null,null,null,null,null,null,"vertikalno opter od rasprostiranje na vrhu temelja za stabilnost oko točke A",null,null,null,null,null,null,"Za II-II"]
[3,{"$f":"+'C III-V'!B4","v":3.4000010999999999},{"$f":"+'C III-V'!C4","v":1.2}]
[4,{"$f":"+'C III-V'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C5","v":3.14},null,null,null,null,null,null,null,null,null,null,"zid",null,null,"temelj"]
[5,{"$f":"+'C III-V'!B6","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C6","v":3.14},null,null,null,null,null,null,null,null,null,"zid",{"$f":"+B13","v":{"$error":"#VALUE!"}},{"$f":"+C13","v":"A"}]
[6,{"$f":"+'C III-V'!B7","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C7","v":3.44},null,null,null,null,null,null,null,null,null,"linija temelja",{"$f":"+B8","v":3.4000010999999999},{"$f":"+O14","v":1.2}]
[7,{"$f":"+'C III-V'!B8","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C8","v":3.44},null,null,null,null,null,null,null,null,null,null,-10,{"$f":"+O11","v":1.2}]
[8,{"$f":"+'C III-V'!B9","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C9","v":"A"},null,null,null,null,null,null,null,null,null,null,"Temelj  -","Vozilo",null,null,"tg","j",null,"Os zida"]
[9,{"$f":"+'C III-V'!B10","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C10","v":"A"},null,null,null,null,null,null,null,null,null,"lijevi vrh temelja",{"$f":"2+'Analiza i dimenzioniranje'!E61-MT!G13","v":1.75},{"$f":"+C7","v":1.2},"duljina opt na temelju",null,{"$f":"+TAN(S14*PI()/180)","v":0.57735026918962573},30,null,"Visina presjeka",null,"x","y"]
[10,{"$f":"+'C III-V'!B11","v":4.2000010999999997},{"$f":"+'C III-V'!C11","v":1.2},null,null,null,null,null,null,null,null,null,"položaj na temelju",{"$f":"+B26","v":{"$error":"#VALUE!"}},{"$f":"C26","v":{"$error":"#VALUE!"}},{"$f":"+B27","v":{"$error":"#VALUE!"}},{"$f":"+O15","v":{"$error":"#VALUE!"}},"h=",{"$f":"+O15-O14","v":{"$error":"#VALUE!"}},null,"III",{"$f":"+'Sile i krakovi'!T$97","v":1.2},{"$f":"+'Sile i krakovi'!T$96","v":{"$error":"#VALUE!"}},{"$f":"+IF($AB$14=V15,W15,0)","v":0}]
[11,{"$f":"+'C III-V'!B12","v":4.2000010999999997},{"$f":"+'C III-V'!C12","v":1.2},null,null,null,null,null,null,null,null,null,"x lijevo=",{"$f":"+N15-S15*$R$14","v":{"$error":"#VALUE!"}},{"$f":"+O14","v":1.2},{"$f":"P15+S15*$R$14","v":{"$error":"#VALUE!"}},{"$f":"+O16","v":1.2}," = x  desno",null,null,"VI",{"$f":"+'Sile i krakovi'!U$97","v":1.52},{"$f":"+'Sile i krakovi'!U$96","v":{"$error":"#VALUE!"}},{"$f":"+IF($AB$14=V16,W16,0)","v":0}]
[12,{"$f":"+'C III-V'!B13","v":4.2000010999999997},{"$f":"+'C III-V'!C13","v":1.2},null,null,null,null,null,null,null,null,null,"opter. Temelja zida od temelja",null,null,null,"Q/m' zida=",{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,+'Analiza i dimenzioniranje'!E28*'Analiza i dimenzioniranje'!E29)","v":120},"kN/m'",null,"VII",{"$f":"+'Sile i krakovi'!V$97","v":1.84},{"$f":"+'Sile i krakovi'!V$96","v":{"$error":"#VALUE!"}},0]
[13,{"$f":"+'C III-V'!B14","v":4.9000021999999994},{"$f":"+'C III-V'!C14","v":1.2},null,null,null,null,null,null,null,null,null,null,"duljina rasprostiranja=",{"$f":"+P16-N16","v":{"$error":"#VALUE!"}},null,"specifično opterećenje =",{"$f":"+R17/O18","v":{"$error":"#VALUE!"}},"kN/m'",null,"VIII",{"$f":"+'Sile i krakovi'!W$97","v":2.16},{"$f":"+'Sile i krakovi'!W$96","v":{"$error":"#VALUE!"}},0]
[14,{"$f":"+'C III-V'!B15","v":4.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5},null,null,null,null,null,null,null,null,null,null,"dio iznad temelja=",{"$f":"+P16-N14","v":{"$error":"#VALUE!"}},null,"opt na nivo temelja =",{"$f":"IF(O20<=0.0001,0,+R18*O19)","v":{"$error":"#VALUE!"}},"kN",null,"IX",{"$f":"+'Sile i krakovi'!X$97","v":2.48},{"$f":"+'Sile i krakovi'!X$96","v":{"$error":"#VALUE!"}},0]
[15,{"$f":"+'C III-V'!B16","v":2},{"$f":"+'C III-V'!C16","v":0.12820515121628623},null,null,null,null,null,null,null,null,null,"Optreć. dio temelja =",null,{"$f":"IF(O19<=0,0,IF(O19>'Analiza i dimenzioniranje'!$E$59+Kontrafore!$E$4,'Analiza i dimenzioniranje'!$E$59+Kontrafore!$E$4,O19))","v":{"$error":"#VALUE!"}},"m",null,"krak od \"A\"=",{"$f":"IF(O20=0,0,$B$18-S21)","v":{"$error":"#VALUE!"}},{"$f":"+$N$11-S21","v":{"$error":"#VALUE!"}},"X",{"$f":"+'Sile i krakovi'!Y97","v":2.8},{"$f":"+'Sile i krakovi'!Y$96","v":{"$error":"#VALUE!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koord težišta opterećenja",{"$f":"+N14+O20/3","v":{"$error":"#VALUE!"}},null,"XI",{"$f":"+'Sile i krakovi'!Z$97","v":3.14},{"$f":"+'Sile i krakovi'!Z96","v":{"$error":"#VALUE!"}},0]
["Opter. Temeljem",null,null,null,null,null,null,null,null,null,null,null,null,"Promet",null,null,null,null,null,null,"XIII",{"$f":"+'Sile i krakovi'!AA$97","v":3.44},{"$f":"+'Sile i krakovi'!AA$96","v":{"$error":"#VALUE!"}},0]
[null,{"$f":"+'Analiza i dimenzioniranje'!C88","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!D88","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"lijevi vrh temelja",{"$f":"+N14","v":1.75},{"$f":"+C7","v":1.2},"duljina opt na temelju",null,{"$f":"+R14","v":0.57735026918962573},{"$f":"+S14","v":30},null,"XIII",{"$f":"+'Sile i krakovi'!AB$97","v":3.76},{"$f":"+'Sile i krakovi'!AB$96","v":{"$error":"#VALUE!"}},0]
[null,{"$f":"+'Analiza i dimenzioniranje'!C89","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!D89","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"položaj na temelju",{"$f":"+B35","v":{"$error":"#VALUE!"}},{"$f":"+C35","v":6.2644906473896782},{"$f":"+B32","v":{"$error":"#VALUE!"}},{"$f":"+O24","v":6.2644906473896782},"h=",{"$f":"+O24-O23","v":5.064490647389678},null,"XIV",{"$f":"+'Sile i krakovi'!AC$97","v":4.08},{"$f":"+'Sile i krakovi'!AC$96","v":{"$error":"#VALUE!"}},0]
[null,{"$f":"+'Analiza i dimenzioniranje'!C90","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!D90","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"x lijevo=",{"$f":"+N24-S24*$R$23","v":{"$error":"#VALUE!"}},{"$f":"+O23","v":1.2},{"$f":"P24+S24*$R$14","v":{"$error":"#VALUE!"}},{"$f":"+O25","v":1.2}," = x  desno",null,null,"XV",{"$f":"+'Sile i krakovi'!AD$97","v":4.4000000000000004},{"$f":"+'Sile i krakovi'!AD$96","v":{"$error":"#VALUE!"}},0]
[null,{"$f":"+'Analiza i dimenzioniranje'!C91","v":{"$error":"#VALUE!"}},{"$f":"+C27","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"opter. Temelja zida od prometa",null,null,null,"Q/m' zida=",{"$f":"IF('Analiza i dimenzioniranje'!E24=0,0,+'Analiza i dimenzioniranje'!E24*'Analiza i dimenzioniranje'!E25)","v":30},"kN/m'",null,"XVI",{"$f":"+'Sile i krakovi'!AE$97","v":4.72},{"$f":"+'Sile i krakovi'!AE$96","v":{"$error":"#VALUE!"}},0]
[null,{"$f":"+'Analiza i dimenzioniranje'!C92","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!D92","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Oznaka linije djelovanja na dijagramu",null,null,null,null,"duljina rasprostiranja=",{"$f":"+P25-N25","v":{"$error":"#VALUE!"}},null,"specifično opterećenje =",{"$f":"+R26/O27","v":{"$error":"#VALUE!"}},"kN/m'",null,"XVII",{"$f":"+'Sile i krakovi'!AF$97","v":5.04},{"$f":"+'Sile i krakovi'!AF$96","v":{"$error":"#VALUE!"}},0]
[null,{"$f":"+'Analiza i dimenzioniranje'!C93","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!D93","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Temelj","x=",{"$f":"+(N14+O20/2)","v":{"$error":"#VALUE!"}},{"$f":"+K28","v":{"$error":"#VALUE!"}},null,"dio iznad temelja=",{"$f":"+P25-N23","v":{"$error":"#VALUE!"}},null,"opt na nivo temelja =",{"$f":"IF(O29<=0.001,0,+R27*O28)","v":{"$error":"#VALUE!"}},"kN",null,"XVIII",{"$f":"+'Sile i krakovi'!AG$97","v":5.36},{"$f":"+'Sile i krakovi'!AG$96","v":{"$error":"#VALUE!"}},0]
[null,{"$f":"+'Analiza i dimenzioniranje'!C94","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!D94","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,"y=",{"$f":"+O11","v":1.2},2.2000000000000002,"Optreć. dio temelja =",null,{"$f":"IF(O28<=0,0,IF(O28>'Analiza i dimenzioniranje'!$E$59+Kontrafore!$E$4,'Analiza i dimenzioniranje'!$E$59+Kontrafore!$E$4,O28))","v":{"$error":"#VALUE!"}},"m",null,"krak od \"A\"=",{"$f":"IF(O29=0,0,$B$18-S30)","v":{"$error":"#VALUE!"}},{"$f":"+$N$11-S30","v":{"$error":"#VALUE!"}},"XIX",{"$f":"+'Sile i krakovi'!AH$97","v":5.6800000000000006},{"$f":"+'Sile i krakovi'!AH$96","v":{"$error":"#VALUE!"}},0]
[null,{"$f":"+'Analiza i dimenzioniranje'!C95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!D95","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Promet","x=",{"$f":"+S30","v":{"$error":"#VALUE!"}},{"$f":"+K30","v":{"$error":"#VALUE!"}},null,null,null,null,null,"koord",{"$f":"+N23+O29/3","v":{"$error":"#VALUE!"}},null,"XX",{"$f":"+'Sile i krakovi'!AI$97","v":6},{"$f":"+'Sile i krakovi'!AI$96","v":{"$error":"#VALUE!"}},{"$f":"+IF($AB$14=V30,W30,0)","v":0}]
["opt prometom",null,null,null,null,null,null,null,null,"y=",{"$f":"+K29","v":1.2},{"$f":"+L29","v":2.2000000000000002},null,"linijsko",null,null,null,null,null,null,null,null,null,{"$f":"SUM(X15:X30)","v":0}]
[null,{"$f":"+'C III-V'!W14","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X14","v":6.2644906473896782},null,null,null,null,null,"Linijsko","x=",{"$f":"+S39","v":{"$error":"#VALUE!"}},{"$f":"+K32","v":{"$error":"#VALUE!"}},"lijevi vrh temelja",{"$f":"+N14","v":1.75},{"$f":"+C7","v":1.2},"duljina opt na temelju",null,{"$f":"+R23","v":0.57735026918962573},{"$f":"+S23","v":30}]
[null,{"$f":"+'C III-V'!W15","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X15+0.8","v":7.2644906473896782},null,null,null,null,null,null,"y=",{"$f":"+K31","v":1.2},{"$f":"+L31","v":2.2000000000000002},"položaj na temelju",{"$f":"+D40-0.5","v":{"$error":"#VALUE!"}},{"$f":"+C40","v":{"$error":"#VALUE!"}},{"$f":"+N33+1","v":{"$error":"#VALUE!"}},{"$f":"+O33","v":{"$error":"#VALUE!"}},"h=",{"$f":"+O33-O32","v":{"$error":"#VALUE!"}},null,"Krak sile na konzoli"]
[null,{"$f":"+'C III-V'!W16","v":{"$error":"#VALUE!"}},{"$f":"+C33","v":7.2644906473896782},null,null,null,null,null,"Točkasto","x=",{"$f":"+S48","v":{"$error":"#VALUE!"}},{"$f":"+S48","v":{"$error":"#VALUE!"}},"x lijevo=",{"$f":"+N33-S33*$R$32","v":{"$error":"#VALUE!"}},{"$f":"+O32","v":1.2},{"$f":"P33+S33*$R$14","v":{"$error":"#VALUE!"}},{"$f":"+O34","v":1.2}," = x  desno",null,null,"promet",{"$f":"IF(+$X$31-2*AB28/3<$X$31,X$31-2*AB28/3,0)","v":0}]
[null,{"$f":"+'C III-V'!W17","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X17","v":6.2644906473896782},null,null,null,null,null,null,"y=",{"$f":"+K33","v":1.2},{"$f":"+L33","v":2.2000000000000002},"opter. Temelja zida od linijskog",null,null,null,"Q/m' zida=",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'",null,"točkasto",{"$f":"IF(+$X$31-2*AB47/3<$X$31,X31-2*AB47/3,0)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"duljina rasprostiranja=",{"$f":"+P34-N34","v":{"$error":"#VALUE!"}},null,"specifično opterećenje =",{"$f":"+R35/O36","v":{"$error":"#VALUE!"}},"kN/m'",null,"linijsko",{"$f":"IF(+$X$31-2*AB37/3<$X$31,X$31-2*AB37/3,0)","v":0}]
[null,"linijsko opterećenje Temelj",null,null,null,null,null,null,null,null,null,null,null,"dio iznad temelja=",{"$f":"+P34-N32","v":{"$error":"#VALUE!"}},null,"opt na nivo temelja =",{"$f":"IF(O38<=0.0001,0,+R36*O37)","v":{"$error":"#VALUE!"}},"kN",null,"temelj",{"$f":"IF(+$X$31-2*AB38/3<$X$31,X$31-2*AB19/3,0)","v":0}]
[null,{"$f":"+B39","v":{"$error":"#VALUE!"}},{"$f":"+C39+0.35","v":{"$error":"#VALUE!"}},null,null,null,null,null,"za konzolu",-8,5,null,"Optreć. dio temelja =",null,{"$f":"+O37","v":{"$error":"#VALUE!"}},"m",null,"krak od \"A\"=",{"$f":"IF(O38=0,0,$B$18-S39)","v":{"$error":"#VALUE!"}},{"$f":"+$N$11-S39","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+D40-0.5","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X27","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+C12","v":3.44},{"$f":"+C12","v":3.44},null,null,null,null,null,null,"koord",{"$f":"+N32+O38/3","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+D40+0.5","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X27","v":{"$error":"#VALUE!"}},{"$f":"+N10-'Analiza i dimenzioniranje'!E35","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$36=0.000001,\"\",+C40)","v":{"$error":"#VALUE!"}},null,null,null,"Jednadžba osi zida sa horizontalnim silama",null,null,null,null,"točkasto"," - površina 1*1 m"]
[null,{"$f":"+B40","v":{"$error":"#VALUE!"}},{"$f":"+C38","v":{"$error":"#VALUE!"}},{"$f":"+D40","v":{"$error":"#VALUE!"}},{"$f":"IF(E40=\"\",\"\",+E40+0.5)","v":{"$error":"#VALUE!"}},null,null,null,"x=",{"$f":"+N42","v":{"$error":"#VALUE!"}},{"$f":"+N43","v":{"$error":"#VALUE!"}},null,"lijevi vrh temelja",{"$f":"+D46-0.5","v":{"$error":"#VALUE!"}},{"$f":"+C7","v":1.2},"duljina opt na temelju",null,{"$f":"+R32","v":0.57735026918962573},{"$f":"+S32","v":30}]
[null,{"$f":"+B38","v":{"$error":"#VALUE!"}},{"$f":"+C38","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Y=",{"$f":"+O42","v":{"$error":"#VALUE!"}},{"$f":"+O43","v":1.2},null,"položaj na temelju",{"$f":"D47-0.5","v":{"$error":"#VALUE!"}},{"$f":"+C46","v":{"$error":"#VALUE!"}},{"$f":"+D47+0.5","v":{"$error":"#VALUE!"}},{"$f":"+O42","v":{"$error":"#VALUE!"}},"h=",{"$f":"+O42-O41","v":{"$error":"#VALUE!"}}]
["točkasto",null,null,null,null,null,null,null,"Y=",{"$f":"(K42-J42)/(K41-J41)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-J43*J41+J42","v":{"$error":"#VALUE!"}},"x lijevo=",{"$f":"+N42-S42*$R$23","v":{"$error":"#VALUE!"}},{"$f":"+O41","v":1.2},{"$f":"P42+S42*$R$14","v":{"$error":"#VALUE!"}},{"$f":"+O43","v":1.2}," = x  desno"]
[null,{"$f":"+B45","v":{"$error":"#VALUE!"}},{"$f":"+C45+0.2","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Vrijednosti X za poznati Y",null,null,null,"opter. Temelja zida od točkastog",null,null,null,"Q/m' zida=",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN"]
[null,{"$f":"+D46+0.5","v":{"$error":"#VALUE!"}},{"$f":"+C46","v":{"$error":"#VALUE!"}},null,null,null,null,null,"X=",{"$f":"+L45/$J$43-$L$43/$L$43","v":{"$error":"#VALUE!"}},null,{"$f":"+J39","v":3.44},null,"duljina rasprostiranja=",{"$f":"+P43-N43","v":{"$error":"#VALUE!"}},null,"specifično opterećenje =",{"$f":"+R44/O45","v":{"$error":"#VALUE!"}},"kN/m'"]
[null,{"$f":"+D46-0.5","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X23","v":{"$error":"#VALUE!"}},{"$f":"+N10-'Analiza i dimenzioniranje'!E37","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$36=0.000001,-5,+C46)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"dio iznad temelja=",{"$f":"+P43-N41","v":{"$error":"#VALUE!"}},null,"opt na nivo temelja =",{"$f":"IF(O47<=0.0001,0,+R45*O46)","v":{"$error":"#VALUE!"}},"kN"]
[null,{"$f":"+D46-0.5","v":{"$error":"#VALUE!"}},{"$f":"+C44","v":{"$error":"#VALUE!"}},{"$f":"+D46","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$36=0.000001,-5,+E46+0.6)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"Optreć. dio temelja =",null,{"$f":"+O46","v":{"$error":"#VALUE!"}},"m",null,"krak od \"A\"=",{"$f":"IF(O47=0,0,$B$18-S48)","v":{"$error":"#VALUE!"}},{"$f":"+$N$11-S48","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+B44","v":{"$error":"#VALUE!"}},{"$f":"+C44","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koord",{"$f":"+N41+O47/3","v":{"$error":"#VALUE!"}}]
[]
["teren"]
[null,{"$f":"+'Analiza i dimenzioniranje'!F95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!G94","v":6},null,null,null,null,"Jednadžbe pravaca rasprostiranja",null,null,"Temelj","X=",{"$f":"+Kontrafore!H20","v":1.75},{"$f":"+Kontrafore!J20","v":3.4000010999999999}]
[null,{"$f":"+'Analiza i dimenzioniranje'!F96","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!G95","v":6},null,null,null,"prema tlu","x=",{"$f":"+N15","v":{"$error":"#VALUE!"}},{"$f":"+N16","v":{"$error":"#VALUE!"}},null,"y=",{"$f":"+I54*$M$51+K54","v":{"$error":"#VALUE!"}},{"$f":"+I54*$N$51+K54","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+'Analiza i dimenzioniranje'!F97","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!G96","v":6.2644906473896782},null,null,null,null,"Y=",{"$f":"+O15","v":{"$error":"#VALUE!"}},{"$f":"+O16","v":1.2}]
[null,{"$f":"+'Analiza i dimenzioniranje'!F98","v":-8},{"$f":"+'Analiza i dimenzioniranje'!G97","v":6.2644906473896782},null,null,null,null,"Y=",{"$f":"(J53-I53)/(J52-I52)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-I54*I52+I53","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,"prema zidu","x=",{"$f":"+P15","v":{"$error":"#VALUE!"}},{"$f":"+P16","v":{"$error":"#VALUE!"}},null,"y=",{"$f":"+I58*$M$51+K58","v":{"$error":"#VALUE!"}},{"$f":"+I58*$N$51+K58","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,"Y=",{"$f":"+Q15","v":{"$error":"#VALUE!"}},{"$f":"+O25","v":1.2}]
[null,null,null,null,null,null,null,"Y=",{"$f":"(J57-I57)/(J56-I56)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-I58*I56+I57","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,null,"Jednadžbe pravaca rasprostiranja",null,null,"Promet"]
[null,null,null,null,null,null,"prema tlu","x=",{"$f":"+P24","v":{"$error":"#VALUE!"}},{"$f":"+P25","v":{"$error":"#VALUE!"}},null,"y=",{"$f":"+I63*$M$51+K63","v":{"$error":"#VALUE!"}},{"$f":"+I63*$N$51+K63","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,"Y=",{"$f":"+I53","v":{"$error":"#VALUE!"}},{"$f":"+Q25","v":1.2}]
[null,null,null,null,null,null,null,"Y=",{"$f":"(J62-I62)/(J61-I61)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-I63*I61+I62","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,"prema zidu","x=",{"$f":"+P24","v":{"$error":"#VALUE!"}},{"$f":"++'Analiza i dimenzioniranje'!E48+'Analiza i dimenzioniranje'!E20","v":{"$error":"#VALUE!"}},null,"y=",{"$f":"+I67*$M$51+K67","v":{"$error":"#VALUE!"}},{"$f":"+I67*$N$51+K67","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,"Y=",{"$f":"+P25","v":{"$error":"#VALUE!"}},{"$f":"+O25","v":1.2}]
[null,null,null,null,null,null,null,"Y=",{"$f":"(J66-I66)/(J65-I65)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-I67*I65+I66","v":{"$error":"#VALUE!"}}]

{"sheet":"MT","index":7,"n_rows":193,"n_cols":20,"rows_kept":193,"cut":false,"hidden":true,"merged":[[3,2,3,3],[15,5,15,7]]}
[null,"IZRAČUN MOMENATA TROMOSTI ZA n KONTRAFORA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH1","v":"x"},{"$f":"+'Poprečni presjek zida'!CI1","v":"y"}]
[null,null,null,null,"n= 0 - 10",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH2","v":4},{"$f":"+'Poprečni presjek zida'!CI2","v":4.9000021999999994}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH3","v":0},{"$f":"+'Poprečni presjek zida'!CI3","v":4.9000021999999994}]
[null,"Oznaka","Koordinate točaka",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH4","v":0},{"$f":"+'Poprečni presjek zida'!CI4","v":2}]
[null,"točke","x","y",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH5","v":1.5},{"$f":"+'Poprečni presjek zida'!CI5","v":2}]
[null,1,{"$f":"2+G11","v":4.9000021999999994},{"$f":"+G10","v":4},null,"duljina zida             L=",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH6","v":1.5},{"$f":"+'Poprečni presjek zida'!CI6","v":1}]
[null,2,{"$f":"+C6","v":4.9000021999999994},0,null,"duljina kontrafore   l=",{"$f":"+Kontrafore!$E$3","v":1},null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH7","v":2.5},{"$f":"+'Poprečni presjek zida'!CI7","v":1}]
[null,3,2,0,null,"širina kontrafore    b=",{"$f":"+Kontrafore!$E$4","v":1},null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH8","v":2.5},{"$f":"+'Poprečni presjek zida'!CI8","v":2}]
[null,4,{"$f":"+C8","v":2},{"$f":"0+(D6-G8)/2","v":1.5},null,"broj kontrafora      n=",{"$f":"+Kontrafore!E5","v":3},null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH9","v":4},{"$f":"+'Poprečni presjek zida'!CI9","v":2}]
[null,null,{"$f":"+C9-G7","v":1},{"$f":"+D9","v":1.5},null,"dulj tem. za 1 rebro b=",{"$f":"IF(G9=0,0,+G6/G9)","v":4},null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH10","v":4},{"$f":"+'Poprečni presjek zida'!CI10","v":4.9000021999999994}]
[null,null,{"$f":"+C10","v":1},{"$f":"+D10++G7","v":2.5},null,"širina temelja        B=",{"$f":"+'Analiza i dimenzioniranje'!$E$61","v":2.9000021999999994},null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH11","v":8},{"$f":"+'Poprečni presjek zida'!CI11","v":4.9000021999999994}]
[null,5,{"$f":"+C9","v":2},{"$f":"+D11","v":2.5},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH12","v":4},{"$f":"+'Poprečni presjek zida'!CI12","v":4.9000021999999994}]
[null,6,{"$f":"+C9","v":2},{"$f":"+D10","v":1.5},null,"B=",{"$f":"+IF($G$9=F18,H18,IF($G$9=F19,H19,IF($G$9=F20,H20,IF($G$9=F21,H21,IF($G$9=F22,H22,IF($G$9=F23,H23,IF($G$9=F24,H24,IF($G$9=F25,H25,IF($G$9=F26,H26,IF($G$9=F27,H27, H28))))))))))","v":3.1500021999999994},"m",null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH13","v":4},{"$f":"+'Poprečni presjek zida'!CI13","v":2}]
[null,7,{"$f":"+C12","v":2},{"$f":"+D12","v":2.5},null,"W=",{"$f":"+IF(G9=F18,G18,IF(G9=F20,G20,IF(G9=F21,G21,IF(G9=F22,G22,IF(G9=F23,G23,IF(G9=F24,G24,IF(G9=F25,G25,IF(G9=F26,G26,IF(G9=F27,G27,G28)))))))))","v":1.653752310000806},"m3",null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH14","v":5.5},{"$f":"+'Poprečni presjek zida'!CI14","v":2}]
[null,8,{"$f":"+C14","v":2},{"$f":"+D6","v":4},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH15","v":5.5},{"$f":"+'Poprečni presjek zida'!CI15","v":1}]
[null,9,{"$f":"+C6","v":4.9000021999999994},{"$f":"+D6","v":4},null,"Izračun W  i B  po broju n KF",null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH16","v":6.5},{"$f":"+'Poprečni presjek zida'!CI16","v":1}]
[null,"  A=",{"$f":"-0.5*(+(C6*D7-C7*D6)+(C7*D8-C8*D7)+(C8*D9-C9*D8)+(C9*D10-C10*D9)+(C10*D11-C11*D10)+(C11*D12-C12*D11)+(C12*D13-C13*D12)+(C13*D14-C14*D13)+(C14*D15-C15*D14)+(C15*D16-C16*D15))","v":12.600008799999998},"m2",null,"n     KF","W a' m'","B",null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH17","v":6.5},{"$f":"+'Poprečni presjek zida'!CI17","v":2}]
[null,"xt=",{"$f":"IF(C17=0,0,-((C6*D7-C7*D6)*(C6+C7)+(C7*D8-C8*D7)*(C7+C8)+(C8*D9-C9*D8)*(C8+C9)+(C9*D10-C10*D9)*(C9+C10)+(C10*D11-C11*D10)*(C10+C11)+(C11*D12-C12*D11)*(C11+C12)+(C12*D13-C13*D12)*(C12+C13)+(C13*D14-C14*D13)*(C13+C14)+(C14*D15-C15*D14)*(C14+C15)+(C15*D16-C16*D15)*(C15+C16))/6/C17)","v":3.2952392160241724},"m",null,0,{"$f":"+I39","v":1.4016687933341394},{"$f":"+I38","v":2.9000021999999994},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH18","v":8},{"$f":"+'Poprečni presjek zida'!CI18","v":2}]
[null,"yt=",{"$f":"IF(C17=0,0,((D6*C7-D7*C6)*(D6+D7)+(D7*C8-D8*C7)*(D7+D8)+(D8*C9-D9*C8)*(D8+D9)+(D9*C10-D10*C9)*(D9+D10)+(D10*C11-D11*C10)*(D10+D11)+(D11*C12-D12*C11)*(D11+D12)+(D12*C13-D13*C12)*(D12+D13)+(D13*C14-D14*C13)*(D13+D14)+(D14*C15-D15*C14)*(D14+D15)+(D15*C16-D16*C15)*(D15+D16))/6/C17)","v":2},"m",null,1,{"$f":"+I54","v":1.4833818174082136},{"$f":"+I53","v":2.9833355333333329},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH19","v":8},{"$f":"+'Poprečni presjek zida'!CI19","v":4.9000021999999994}]
[null,null,null,null,null,2,{"$f":"+I69","v":1.5674096562971023},{"$f":"+I68","v":3.0666688666666659},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH20","v":12},{"$f":"+'Poprečni presjek zida'!CI20","v":0}]
[null,"  A=",{"$f":"IF(Kontrafore!E1=\"\",0,+G8*G7)","v":1},"m2",null,3,{"$f":"+I84","v":1.653752310000806},{"$f":"+I83","v":3.1500021999999994},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH21","v":8},{"$f":"+'Poprečni presjek zida'!CI21","v":4.9000021999999994}]
[null,"xt=",{"$f":"2-G7/2","v":1.5},"m",null,4,{"$f":"+I99","v":1.7424097785193247},{"$f":"+I98","v":3.2333355333333329},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH22","v":8},{"$f":"+'Poprečni presjek zida'!CI22","v":2}]
[null,"yt=",{"$f":"+C27","v":2},"m",null,5,{"$f":"+I114","v":1.8333820618526577},{"$f":"+I113","v":3.3166688666666659},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH23","v":9.5},{"$f":"+'Poprečni presjek zida'!CI23","v":2}]
[null,null,null,null,null,6,{"$f":"+I129","v":1.9266691600008059},{"$f":"+I128","v":3.4000021999999994},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH24","v":9.5},{"$f":"+'Poprečni presjek zida'!CI24","v":1}]
[null,"  A=",{"$f":"+G11*G10","v":11.600008799999998},"m2",null,7,{"$f":"+I144","v":2.0222710729637692},{"$f":"+I143","v":3.4833355333333329},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH25","v":10.5},{"$f":"+'Poprečni presjek zida'!CI25","v":1}]
[null,"xt=",{"$f":"2+G11/2","v":3.4500010999999997},"m",null,8,{"$f":"+I159","v":2.1201878007415464},{"$f":"+I158","v":3.5666688666666659},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH26","v":10.5},{"$f":"+'Poprečni presjek zida'!CI26","v":2}]
[null,"yt=",{"$f":"+G10/2","v":2},"m",null,9,{"$f":"+I174","v":2.220419343334139},{"$f":"+I173","v":3.6500021999999994},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH27","v":12},{"$f":"+'Poprečni presjek zida'!CI27","v":2}]
[null,null,null,null,null,10,{"$f":"+I189","v":2.322965700741547},{"$f":"+I188","v":3.7333355333333329},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH28","v":12},{"$f":"+'Poprečni presjek zida'!CI28","v":4.9000021999999994}]
[null,null,null,null,"Broj rebara",null,0,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH29","v":16},{"$f":"+'Poprečni presjek zida'!CI29","v":0}]
[null,null,null,null,1,{"$f":"2+J35","v":4.9000021999999994},10,null,"duljina zida             L=",{"$f":"+'Analiza i dimenzioniranje'!$E$49","v":12},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH30","v":12},{"$f":"+'Poprečni presjek zida'!CI30","v":4.9000021999999994}]
[null,null,null,null,2,{"$f":"+F30","v":4.9000021999999994},0,null,"duljina kontrafore   l=",{"$f":"+Kontrafore!$E$3","v":1},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH31","v":12},{"$f":"+'Poprečni presjek zida'!CI31","v":2}]
[null,null,null,null,3,2,0,null,"širina kontrafore    b=",{"$f":"+Kontrafore!$E$4","v":1},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH32","v":13.5},{"$f":"+'Poprečni presjek zida'!CI32","v":2}]
[null,null,null,null,4,{"$f":"+F32","v":2},{"$f":"0+(G30-J32)/2","v":4.5},null,"broj kontrafora      n=",{"$f":"+G29","v":0},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH33","v":13.5},{"$f":"+'Poprečni presjek zida'!CI33","v":1}]
[null,null,null,null,null,2,{"$f":"+G33","v":4.5},null,"temelja za 1 rebro  b=",0,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH34","v":14.5},{"$f":"+'Poprečni presjek zida'!CI34","v":1}]
[null,null,null,null,null,2,{"$f":"+G34++J31","v":5.5},null,"širina zida              B=",{"$f":"+'Analiza i dimenzioniranje'!$E$61","v":2.9000021999999994},null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH35","v":14.5},{"$f":"+'Poprečni presjek zida'!CI35","v":2}]
[null,null,null,null,5,{"$f":"+F33","v":2},{"$f":"+G35","v":5.5},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH36","v":16},{"$f":"+'Poprečni presjek zida'!CI36","v":2}]
[null,null,null,null,6,{"$f":"+F33","v":2},{"$f":"+G34","v":4.5},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH37","v":16},{"$f":"+'Poprečni presjek zida'!CI37","v":4.9000021999999994}]
[null,null,null,null,7,{"$f":"+F36","v":2},{"$f":"+G36","v":5.5},"B=",{"$f":"+$G$11+G29/$G$6","v":2.9000021999999994},null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH38","v":20},{"$f":"+'Poprečni presjek zida'!CI38","v":0}]
[null,null,null,null,8,{"$f":"+F38","v":2},{"$f":"+G30","v":10},"W=",{"$f":"+I38*I38/6","v":1.4016687933341394},null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH39","v":16},{"$f":"+'Poprečni presjek zida'!CI39","v":0}]
[null,null,null,null,9,{"$f":"+F30","v":4.9000021999999994},{"$f":"+G30","v":10},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH40","v":16},{"$f":"+'Poprečni presjek zida'!CI40","v":0}]
[null,null,null,null,"  A=",{"$f":"-0.5*(+(F30*G31-F31*G30)+(F31*G32-F32*G31)+(F32*G33-F33*G32)+(F33*G34-F34*G33)+(F34*G35-F35*G34)+(F35*G36-F36*G35)+(F36*G37-F37*G36)+(F37*G38-F38*G37)+(F38*G39-F39*G38)+(F39*G40-F40*G39))","v":29.000021999999994},"m2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH41","v":17.5},{"$f":"+'Poprečni presjek zida'!CI41","v":0}]
[null,null,null,null,"xt=",{"$f":"IF(F41=0,0,-((F30*G31-F31*G30)*(F30+F31)+(F31*G32-F32*G31)*(F31+F32)+(F32*G33-F33*G32)*(F32+F33)+(F33*G34-F34*G33)*(F33+F34)+(F34*G35-F35*G34)*(F34+F35)+(F35*G36-F36*G35)*(F35+F36)+(F36*G37-F37*G36)*(F36+F37)+(F37*G38-F38*G37)*(F37+F38)+(F38*G39-F39*G38)*(F38+F39)+(F39*G40-F40*G39)*(F39+F40))/6/F41)","v":3.4500010999999988},"m",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH42","v":17.5},{"$f":"+'Poprečni presjek zida'!CI42","v":0}]
[null,null,null,null,"yt=",{"$f":"IF(F41=0,0,((G30*F31-G31*F30)*(G30+G31)+(G31*F32-G32*F31)*(G31+G32)+(G32*F33-G33*F32)*(G32+G33)+(G33*F34-G34*F33)*(G33+G34)+(G34*F35-G35*F34)*(G34+G35)+(G35*F36-G36*F35)*(G35+G36)+(G36*F37-G37*F36)*(G36+G37)+(G37*F38-G38*F37)*(G37+G38)+(G38*F39-G39*F38)*(G38+G39)+(G39*F40-G40*F39)*(G39+G40))/6/F41)","v":5},"m",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH43","v":18.5},{"$f":"+'Poprečni presjek zida'!CI43","v":0}]
[null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Poprečni presjek zida'!CH44","v":18.5},{"$f":"+'Poprečni presjek zida'!CI44","v":0}]
[null,null,null,null,1,{"$f":"2+J50","v":4.9000021999999994},{"$f":"+G6/G44","v":12},null,"duljina zida             L=",{"$f":"+'Analiza i dimenzioniranje'!$E$49","v":12}]
[null,null,null,null,2,{"$f":"+F45","v":4.9000021999999994},0,null,"duljina kontrafore   l=",{"$f":"+Kontrafore!$E$3","v":1}]
[null,null,null,null,3,2,0,null,"širina kontrafore    b=",{"$f":"+Kontrafore!$E$4","v":1}]
[null,null,null,null,4,{"$f":"+F47","v":2},{"$f":"0+(G45-J47)/2","v":5.5},null,"broj kontrafora      n=",{"$f":"+G44","v":1}]
[null,null,null,null,null,{"$f":"+F48-J46","v":1},{"$f":"+G48","v":5.5},null,"temelja za 1 rebro  b=",10]
[null,null,null,null,null,{"$f":"+F49","v":1},{"$f":"+G49++J46","v":6.5},null,"širina zida              B=",{"$f":"+'Analiza i dimenzioniranje'!$E$61","v":2.9000021999999994}]
[null,null,null,null,5,{"$f":"+F48","v":2},{"$f":"+G50","v":6.5},null,"razmak težišta      lT=",{"$f":"+C3-(2-$G$7/2)","v":-1.5}]
[null,null,null,null,6,{"$f":"+F48","v":2},{"$f":"+G49","v":5.5}]
[null,null,null,null,7,{"$f":"+F51","v":2},{"$f":"+G51","v":6.5},"B=",{"$f":"+$G$11+G44/$G$6","v":2.9833355333333329}]
[null,null,null,null,8,{"$f":"+F53","v":2},{"$f":"+G45","v":12},"W=",{"$f":"+I53*I53/6","v":1.4833818174082136}]
[null,null,null,null,9,{"$f":"+F45","v":4.9000021999999994},{"$f":"+G45","v":12}]
[null,null,null,null,"  A=",{"$f":"-0.5*(+(F45*G46-F46*G45)+(F46*G47-F47*G46)+(F47*G48-F48*G47)+(F48*G49-F49*G48)+(F49*G50-F50*G49)+(F50*G51-F51*G50)+(F51*G52-F52*G51)+(F52*G53-F53*G52)+(F53*G54-F54*G53)+(F54*G55-F55*G54))","v":35.800026399999993},"m2"]
[null,null,null,null,"xt=",{"$f":"-((F45*G46-F46*G45)*(F45+F46)+(F46*G47-F47*G46)*(F46+F47)+(F47*G48-F48*G47)*(F47+F48)+(F48*G49-F49*G48)*(F48+F49)+(F49*G50-F50*G49)*(F49+F50)+(F50*G51-F51*G50)*(F50+F51)+(F51*G52-F52*G51)*(F51+F52)+(F52*G53-F53*G52)*(F52+F53)+(F53*G54-F54*G53)*(F53+F54)+(F54*G55-F55*G54)*(F54+F55))/6/F56","v":3.3955318356980047},"m"]
[null,null,null,null,"yt=",{"$f":"((G45*F46-G46*F45)*(G45+G46)+(G46*F47-G47*F46)*(G46+G47)+(G47*F48-G48*F47)*(G47+G48)+(G48*F49-G49*F48)*(G48+G49)+(G49*F50-G50*F49)*(G49+G50)+(G50*F51-G51*F50)*(G50+G51)+(G51*F52-G52*F51)*(G51+G52)+(G52*F53-G53*F52)*(G52+G53)+(G53*F54-G54*F53)*(G53+G54)+(G54*F55-G55*F54)*(G54+G55))/6/F56","v":6},"m"]
[null,null,null,null,"Broj rebara",null,{"$f":"+F20","v":2}]
[null,null,null,null,1,{"$f":"2+J65","v":4.9000021999999994},{"$f":"+J64","v":6},null,"duljina zida             L=",{"$f":"+'Analiza i dimenzioniranje'!$E$49","v":12}]
[null,null,null,null,2,{"$f":"+F60","v":4.9000021999999994},0,null,"duljina kontrafore   l=",{"$f":"+Kontrafore!$E$3","v":1}]
[null,null,null,null,3,2,0,null,"širina kontrafore    b=",{"$f":"+Kontrafore!$E$4","v":1}]
[null,null,null,null,4,{"$f":"+F62","v":2},{"$f":"0+(G60-J62)/2","v":2.5},null,"broj kontrafora      n=",{"$f":"+G59","v":2}]
[null,null,null,null,null,{"$f":"+F63-J61","v":1},{"$f":"+G63","v":2.5},null,"temelja za 1 rebro  b=",{"$f":"+J60/J63","v":6}]
[null,null,null,null,null,{"$f":"+F64","v":1},{"$f":"+G64++J61","v":3.5},null,"širina zida              B=",{"$f":"+'Analiza i dimenzioniranje'!$E$61","v":2.9000021999999994}]
[null,null,null,null,5,{"$f":"+F63","v":2},{"$f":"+G65","v":3.5},null,"razmak težišta      lT=",{"$f":"+C18-(2-$G$7/2)","v":1.7952392160241724}]
[null,null,null,null,6,{"$f":"+F63","v":2},{"$f":"+G64","v":2.5}]
[null,null,null,null,7,{"$f":"+F66","v":2},{"$f":"+G66","v":3.5},"B=",{"$f":"+$G$11+G59/$G$6","v":3.0666688666666659}]
[null,null,null,null,8,{"$f":"+F68","v":2},{"$f":"+G60","v":6},"W=",{"$f":"+I68*I68/6","v":1.5674096562971023}]
[null,null,null,null,9,{"$f":"+F60","v":4.9000021999999994},{"$f":"+G60","v":6}]
[null,null,null,null,"  A=",{"$f":"-0.5*(+(F60*G61-F61*G60)+(F61*G62-F62*G61)+(F62*G63-F63*G62)+(F63*G64-F64*G63)+(F64*G65-F65*G64)+(F65*G66-F66*G65)+(F66*G67-F67*G66)+(F67*G68-F68*G67)+(F68*G69-F69*G68)+(F69*G70-F70*G69))","v":18.400013199999997},"m2"]
[null,null,null,null,"xt=",{"$f":"-((F60*G61-F61*G60)*(F60+F61)+(F61*G62-F62*G61)*(F61+F62)+(F62*G63-F63*G62)*(F62+F63)+(F63*G64-F64*G63)*(F63+F64)+(F64*G65-F65*G64)*(F64+F65)+(F65*G66-F66*G65)*(F65+F66)+(F66*G67-F67*G66)*(F66+F67)+(F67*G68-F68*G67)*(F67+F68)+(F68*G69-F69*G68)*(F68+F69)+(F69*G70-F70*G69)*(F69+F70))/6/F71","v":3.3440228553756972},"m"]
[null,null,null,null,"yt=",{"$f":"((G60*F61-G61*F60)*(G60+G61)+(G61*F62-G62*F61)*(G61+G62)+(G62*F63-G63*F62)*(G62+G63)+(G63*F64-G64*F63)*(G63+G64)+(G64*F65-G65*F64)*(G64+G65)+(G65*F66-G66*F65)*(G65+G66)+(G66*F67-G67*F66)*(G66+G67)+(G67*F68-G68*F67)*(G67+G68)+(G68*F69-G69*F68)*(G68+G69)+(G69*F70-G70*F69)*(G69+G70))/6/F71","v":3},"m"]
[null,null,null,null,"Broj rebara",null,3]
[null,null,null,null,1,{"$f":"2+J80","v":4.9000021999999994},{"$f":"+J79","v":4},null,"duljina zida             L=",{"$f":"+'Analiza i dimenzioniranje'!$E$49","v":12}]
[null,null,null,null,2,{"$f":"+F75","v":4.9000021999999994},0,null,"duljina kontrafore   l=",{"$f":"+Kontrafore!$E$3","v":1}]
[null,null,null,null,3,2,0,null,"širina kontrafore    b=",{"$f":"+Kontrafore!$E$4","v":1}]
[null,null,null,null,4,{"$f":"+F77","v":2},{"$f":"0+(G75-J77)/2","v":1.5},null,"broj kontrafora      n=",{"$f":"+G74","v":3}]
[null,null,null,null,null,{"$f":"+F78-J76","v":1},{"$f":"+G78","v":1.5},null,"temelja za 1 rebro  b=",{"$f":"+J75/J78","v":4}]
[null,null,null,null,null,{"$f":"+F79","v":1},{"$f":"+G79++J76","v":2.5},null,"širina zida              B=",{"$f":"+'Analiza i dimenzioniranje'!$E$61","v":2.9000021999999994}]
[null,null,null,null,5,{"$f":"+F78","v":2},{"$f":"+G80","v":2.5},null,"razmak težišta      lT=",{"$f":"+F63-(2-$G$7/2)","v":0.5}]
[null,null,null,null,6,{"$f":"+F78","v":2},{"$f":"+G79","v":1.5}]
[null,null,null,null,7,{"$f":"+F81","v":2},{"$f":"+G81","v":2.5},"B=",{"$f":"+$G$11+G74/$G$6","v":3.1500021999999994}]
[null,null,null,null,8,{"$f":"+F83","v":2},{"$f":"+G75","v":4},"W=",{"$f":"+I83*I83/6","v":1.653752310000806}]
[null,null,null,null,9,{"$f":"+F75","v":4.9000021999999994},{"$f":"+G75","v":4}]
[null,null,null,null,"  A=",{"$f":"-0.5*(+(F75*G76-F76*G75)+(F76*G77-F77*G76)+(F77*G78-F78*G77)+(F78*G79-F79*G78)+(F79*G80-F80*G79)+(F80*G81-F81*G80)+(F81*G82-F82*G81)+(F82*G83-F83*G82)+(F83*G84-F84*G83)+(F84*G85-F85*G84))","v":12.600008799999998},"m2"]
[null,null,null,null,"xt=",{"$f":"-((F75*G76-F76*G75)*(F75+F76)+(F76*G77-F77*G76)*(F76+F77)+(F77*G78-F78*G77)*(F77+F78)+(F78*G79-F79*G78)*(F78+F79)+(F79*G80-F80*G79)*(F79+F80)+(F80*G81-F81*G80)*(F80+F81)+(F81*G82-F82*G81)*(F81+F82)+(F82*G83-F83*G82)*(F82+F83)+(F83*G84-F84*G83)*(F83+F84)+(F84*G85-F85*G84)*(F84+F85))/6/F86","v":3.2952392160241724},"m"]
[null,null,null,null,"yt=",{"$f":"((G75*F76-G76*F75)*(G75+G76)+(G76*F77-G77*F76)*(G76+G77)+(G77*F78-G78*F77)*(G77+G78)+(G78*F79-G79*F78)*(G78+G79)+(G79*F80-G80*F79)*(G79+G80)+(G80*F81-G81*F80)*(G80+G81)+(G81*F82-G82*F81)*(G81+G82)+(G82*F83-G83*F82)*(G82+G83)+(G83*F84-G84*F83)*(G83+G84)+(G84*F85-G85*F84)*(G84+G85))/6/F86","v":2},"m"]
[null,null,null,null,"Broj rebara",null,{"$f":"+F22","v":4}]
[null,null,null,null,1,{"$f":"2+J95","v":4.9000021999999994},{"$f":"+J94","v":3},null,"duljina zida             L=",{"$f":"+'Analiza i dimenzioniranje'!$E$49","v":12}]
[null,null,null,null,2,{"$f":"+F90","v":4.9000021999999994},0,null,"duljina kontrafore   l=",{"$f":"+Kontrafore!$E$3","v":1}]
[null,null,null,null,3,2,0,null,"širina kontrafore    b=",{"$f":"+Kontrafore!$E$4","v":1}]
[null,null,null,null,4,{"$f":"+F92","v":2},{"$f":"0+(G90-J92)/2","v":1},null,"broj kontrafora      n=",{"$f":"+G89","v":4}]
[null,null,null,null,null,{"$f":"+F93-J91","v":1},{"$f":"+G93","v":1},null,"temelja za 1 rebro  b=",{"$f":"+J90/J93","v":3}]
[null,null,null,null,null,{"$f":"+F94","v":1},{"$f":"+G94++J91","v":2},null,"širina zida              B=",{"$f":"+'Analiza i dimenzioniranje'!$E$61","v":2.9000021999999994}]
[null,null,null,null,5,{"$f":"+F93","v":2},{"$f":"+G95","v":2},null,"razmak težišta      lT=",{"$f":"+$C$18-(2-$G$7/2)","v":1.7952392160241724}]
[null,null,null,null,6,{"$f":"+F93","v":2},{"$f":"+G94","v":1}]
[null,null,null,null,7,{"$f":"+F96","v":2},{"$f":"+G96","v":2},"B=",{"$f":"+$G$11+G89/$G$6","v":3.2333355333333329}]
[null,null,null,null,8,{"$f":"+F98","v":2},{"$f":"+G90","v":3},"W=",{"$f":"+I98*I98/6","v":1.7424097785193247}]
[null,null,null,null,9,{"$f":"+F90","v":4.9000021999999994},{"$f":"+G90","v":3}]
[null,null,null,null,"  A=",{"$f":"-0.5*(+(F90*G91-F91*G90)+(F91*G92-F92*G91)+(F92*G93-F93*G92)+(F93*G94-F94*G93)+(F94*G95-F95*G94)+(F95*G96-F96*G95)+(F96*G97-F97*G96)+(F97*G98-F98*G97)+(F98*G99-F99*G98)+(F99*G100-F100*G99))","v":9.7000065999999983},"m2"]
[null,null,null,null,"xt=",{"$f":"-((F90*G91-F91*G90)*(F90+F91)+(F91*G92-F92*G91)*(F91+F92)+(F92*G93-F93*G92)*(F92+F93)+(F93*G94-F94*G93)*(F93+F94)+(F94*G95-F95*G94)*(F94+F95)+(F95*G96-F96*G95)*(F95+F96)+(F96*G97-F97*G96)*(F96+F97)+(F97*G98-F98*G97)*(F97+F98)+(F98*G99-F99*G98)*(F98+F99)+(F99*G100-F100*G99)*(F99+F100))/6/F101","v":3.2489701955468009},"m"]
[null,null,null,null,"yt=",{"$f":"((G90*F91-G91*F90)*(G90+G91)+(G91*F92-G92*F91)*(G91+G92)+(G92*F93-G93*F92)*(G92+G93)+(G93*F94-G94*F93)*(G93+G94)+(G94*F95-G95*F94)*(G94+G95)+(G95*F96-G96*F95)*(G95+G96)+(G96*F97-G97*F96)*(G96+G97)+(G97*F98-G98*F97)*(G97+G98)+(G98*F99-G99*F98)*(G98+G99)+(G99*F100-G100*F99)*(G99+G100))/6/F101","v":1.5},"m"]
[null,null,null,null,"Broj rebara",null,{"$f":"+F23","v":5}]
[null,null,null,null,1,{"$f":"2+J110","v":4.9000021999999994},{"$f":"+J109","v":2.4},null,"duljina zida             L=",{"$f":"+'Analiza i dimenzioniranje'!$E$49","v":12}]
[null,null,null,null,2,{"$f":"+F105","v":4.9000021999999994},0,null,"duljina kontrafore   l=",{"$f":"+Kontrafore!$E$3","v":1}]
[null,null,null,null,3,2,0,null,"širina kontrafore    b=",{"$f":"+Kontrafore!$E$4","v":1}]
[null,null,null,null,4,{"$f":"+F107","v":2},{"$f":"0+(G105-J107)/2","v":0.7},null,"broj kontrafora      n=",{"$f":"+G104","v":5}]
[null,null,null,null,null,{"$f":"+F108-J106","v":1},{"$f":"+G108","v":0.7},null,"temelja za 1 rebro  b=",{"$f":"+J105/J108","v":2.4}]
[null,null,null,null,null,{"$f":"+F109","v":1},{"$f":"+G109++J106","v":1.7},null,"širina zida              B=",{"$f":"+'Analiza i dimenzioniranje'!$E$61","v":2.9000021999999994}]
[null,null,null,null,5,{"$f":"+F108","v":2},{"$f":"+G110","v":1.7},null,"razmak težišta      lT=",{"$f":"+$C$18-(2-$G$7/2)","v":1.7952392160241724}]
[null,null,null,null,6,{"$f":"+F108","v":2},{"$f":"+G109","v":0.7}]
[null,null,null,null,7,{"$f":"+F111","v":2},{"$f":"+G111","v":1.7},"B=",{"$f":"+$G$11+G104/$G$6","v":3.3166688666666659}]
[null,null,null,null,8,{"$f":"+F113","v":2},{"$f":"+G105","v":2.4},"W=",{"$f":"+I113*I113/6","v":1.8333820618526577}]
[null,null,null,null,9,{"$f":"+F105","v":4.9000021999999994},{"$f":"+G105","v":2.4}]
[null,null,null,null,"  A=",{"$f":"-0.5*(+(F105*G106-F106*G105)+(F106*G107-F107*G106)+(F107*G108-F108*G107)+(F108*G109-F109*G108)+(F109*G110-F110*G109)+(F110*G111-F111*G110)+(F111*G112-F112*G111)+(F112*G113-F113*G112)+(F113*G114-F114*G113)+(F114*G115-F115*G114))","v":7.9600052799999972},"m2"]
[null,null,null,null,"xt=",{"$f":"-((F105*G106-F106*G105)*(F105+F106)+(F106*G107-F107*G106)*(F106+F107)+(F107*G108-F108*G107)*(F107+F108)+(F108*G109-F109*G108)*(F108+F109)+(F109*G110-F110*G109)*(F109+F110)+(F110*G111-F111*G110)*(F110+F111)+(F111*G112-F112*G111)*(F111+F112)+(F112*G113-F113*G112)*(F112+F113)+(F113*G114-F114*G113)*(F113+F114)+(F114*G115-F115*G114)*(F114+F115))/6/F116","v":3.2050262499330668},"m"]
[null,null,null,null,"yt=",{"$f":"((G105*F106-G106*F105)*(G105+G106)+(G106*F107-G107*F106)*(G106+G107)+(G107*F108-G108*F107)*(G107+G108)+(G108*F109-G109*F108)*(G108+G109)+(G109*F110-G110*F109)*(G109+G110)+(G110*F111-G111*F110)*(G110+G111)+(G111*F112-G112*F111)*(G111+G112)+(G112*F113-G113*F112)*(G112+G113)+(G113*F114-G114*F113)*(G113+G114)+(G114*F115-G115*F114)*(G114+G115))/6/F116","v":1.2},"m"]
[null,null,null,null,"Broj rebara",null,{"$f":"+F24","v":6}]
[null,null,null,null,1,{"$f":"2+J125","v":4.9000021999999994},{"$f":"+J124","v":2},null,"duljina zida             L=",{"$f":"+'Analiza i dimenzioniranje'!$E$49","v":12}]
[null,null,null,null,2,{"$f":"+F120","v":4.9000021999999994},0,null,"duljina kontrafore   l=",{"$f":"+Kontrafore!$E$3","v":1}]
[null,null,null,null,3,2,0,null,"širina kontrafore    b=",{"$f":"+Kontrafore!$E$4","v":1}]
[null,null,null,null,4,{"$f":"+F122","v":2},{"$f":"0+(G120-J122)/2","v":0.5},null,"broj kontrafora      n=",{"$f":"+G119","v":6}]
[null,null,null,null,null,{"$f":"+F123-J121","v":1},{"$f":"+G123","v":0.5},null,"temelja za 1 rebro  b=",{"$f":"+J120/J123","v":2}]
[null,null,null,null,null,{"$f":"+F124","v":1},{"$f":"+G124++J121","v":1.5},null,"širina zida              B=",{"$f":"+'Analiza i dimenzioniranje'!$E$61","v":2.9000021999999994}]
[null,null,null,null,5,{"$f":"+F123","v":2},{"$f":"+G125","v":1.5},null,"razmak težišta      lT=",{"$f":"+$C$18-(2-$G$7/2)","v":1.7952392160241724}]
[null,null,null,null,6,{"$f":"+F123","v":2},{"$f":"+G124","v":0.5},null,null,null,null,null,null,null,null,null,null,null,{"$f":"3.6*3.6/6","v":2.16}]
[null,null,null,null,7,{"$f":"+F126","v":2},{"$f":"+G126","v":1.5},"B=",{"$f":"+$G$11+G119/$G$6","v":3.4000021999999994}]
[null,null,null,null,8,{"$f":"+F128","v":2},{"$f":"+G120","v":2},"W=",{"$f":"+I128*I128/6","v":1.9266691600008059}]
[null,null,null,null,9,{"$f":"+F120","v":4.9000021999999994},{"$f":"+G120","v":2}]
[null,null,null,null,"  A=",{"$f":"-0.5*(+(F120*G121-F121*G120)+(F121*G122-F122*G121)+(F122*G123-F123*G122)+(F123*G124-F124*G123)+(F124*G125-F125*G124)+(F125*G126-F126*G125)+(F126*G127-F127*G126)+(F127*G128-F128*G127)+(F128*G129-F129*G128)+(F129*G130-F130*G129))","v":6.8000043999999988},"m2"]
[null,null,null,null,"xt=",{"$f":"-((F120*G121-F121*G120)*(F120+F121)+(F121*G122-F122*G121)*(F121+F122)+(F122*G123-F123*G122)*(F122+F123)+(F123*G124-F124*G123)*(F123+F124)+(F124*G125-F125*G124)*(F124+F125)+(F125*G126-F126*G125)*(F125+F126)+(F126*G127-F127*G126)*(F126+F127)+(F127*G128-F128*G127)*(F127+F128)+(F128*G129-F129*G128)*(F128+F129)+(F129*G130-F130*G129)*(F129+F130))/6/F131","v":3.1632364179065586},"m"]
[null,null,null,null,"yt=",{"$f":"((G120*F121-G121*F120)*(G120+G121)+(G121*F122-G122*F121)*(G121+G122)+(G122*F123-G123*F122)*(G122+G123)+(G123*F124-G124*F123)*(G123+G124)+(G124*F125-G125*F124)*(G124+G125)+(G125*F126-G126*F125)*(G125+G126)+(G126*F127-G127*F126)*(G126+G127)+(G127*F128-G128*F127)*(G127+G128)+(G128*F129-G129*F128)*(G128+G129)+(G129*F130-G130*F129)*(G129+G130))/6/F131","v":1},"m"]
[null,null,null,null,"Broj rebara",null,{"$f":"+F25","v":7}]
[null,null,null,null,1,{"$f":"2+J140","v":4.9000021999999994},{"$f":"+J139","v":1.7142857142857142},null,"duljina zida             L=",{"$f":"+'Analiza i dimenzioniranje'!$E$49","v":12}]
[null,null,null,null,2,{"$f":"+F135","v":4.9000021999999994},0,null,"duljina kontrafore   l=",{"$f":"+Kontrafore!$E$3","v":1}]
[null,null,null,null,3,2,0,null,"širina kontrafore    b=",{"$f":"+Kontrafore!$E$4","v":1}]
[null,null,null,null,4,{"$f":"+F137","v":2},{"$f":"0+(G135-J137)/2","v":0.3571428571428571},null,"broj kontrafora      n=",{"$f":"+G134","v":7}]
[null,null,null,null,null,{"$f":"+F138-J136","v":1},{"$f":"+G138","v":0.3571428571428571},null,"temelja za 1 rebro  b=",{"$f":"+J135/J138","v":1.7142857142857142}]
[null,null,null,null,null,{"$f":"+F139","v":1},{"$f":"+G139++J136","v":1.3571428571428572},null,"širina zida              B=",{"$f":"+'Analiza i dimenzioniranje'!$E$61","v":2.9000021999999994}]
[null,null,null,null,5,{"$f":"+F138","v":2},{"$f":"+G140","v":1.3571428571428572},null,"razmak težišta      lT=",{"$f":"+$C$18-(2-$G$7/2)","v":1.7952392160241724}]
[null,null,null,null,6,{"$f":"+F138","v":2},{"$f":"+G139","v":0.3571428571428571}]
[null,null,null,null,7,{"$f":"+F141","v":2},{"$f":"+G141","v":1.3571428571428572},"B=",{"$f":"+$G$11+G134/$G$6","v":3.4833355333333329}]
[null,null,null,null,8,{"$f":"+F143","v":2},{"$f":"+G135","v":1.7142857142857142},"W=",{"$f":"+I143*I143/6","v":2.0222710729637692}]
[null,null,null,null,9,{"$f":"+F135","v":4.9000021999999994},{"$f":"+G135","v":1.7142857142857142}]
[null,null,null,null,"  A=",{"$f":"-0.5*(+(F135*G136-F136*G135)+(F136*G137-F137*G136)+(F137*G138-F138*G137)+(F138*G139-F139*G138)+(F139*G140-F140*G139)+(F140*G141-F141*G140)+(F141*G142-F142*G141)+(F142*G143-F143*G142)+(F143*G144-F144*G143)+(F144*G145-F145*G144))","v":5.9714323428571427},"m2"]
[null,null,null,null,"xt=",{"$f":"-((F135*G136-F136*G135)*(F135+F136)+(F136*G137-F137*G136)*(F136+F137)+(F137*G138-F138*G137)*(F137+F138)+(F138*G139-F139*G138)*(F138+F139)+(F139*G140-F140*G139)*(F139+F140)+(F140*G141-F141*G140)*(F140+F141)+(F141*G142-F142*G141)*(F141+F142)+(F142*G143-F143*G142)*(F142+F143)+(F143*G144-F144*G143)*(F143+F144)+(F144*G145-F145*G144)*(F144+F145))/6/F146","v":3.1234460981112924},"m"]
[null,null,null,null,"yt=",{"$f":"((G135*F136-G136*F135)*(G135+G136)+(G136*F137-G137*F136)*(G136+G137)+(G137*F138-G138*F137)*(G137+G138)+(G138*F139-G139*F138)*(G138+G139)+(G139*F140-G140*F139)*(G139+G140)+(G140*F141-G141*F140)*(G140+G141)+(G141*F142-G142*F141)*(G141+G142)+(G142*F143-G143*F142)*(G142+G143)+(G143*F144-G144*F143)*(G143+G144)+(G144*F145-G145*F144)*(G144+G145))/6/F146","v":0.85714285714285698},"m"]
[null,null,null,null,"Broj rebara",null,{"$f":"+F26","v":8}]
[null,null,null,null,1,{"$f":"2+J155","v":4.9000021999999994},{"$f":"+J154","v":1.5},null,"duljina zida             L=",{"$f":"+'Analiza i dimenzioniranje'!$E$49","v":12}]
[null,null,null,null,2,{"$f":"+F150","v":4.9000021999999994},0,null,"duljina kontrafore   l=",{"$f":"+Kontrafore!$E$3","v":1}]
[null,null,null,null,3,2,0,null,"širina kontrafore    b=",{"$f":"+Kontrafore!$E$4","v":1}]
[null,null,null,null,4,{"$f":"+F152","v":2},{"$f":"0+(G150-J152)/2","v":0.25},null,"broj kontrafora      n=",{"$f":"+G149","v":8}]
[null,null,null,null,null,{"$f":"+F153-J151","v":1},{"$f":"+G153","v":0.25},null,"temelja za 1 rebro  b=",{"$f":"+J150/J153","v":1.5}]
[null,null,null,null,null,{"$f":"+F154","v":1},{"$f":"+G154++J151","v":1.25},null,"širina zida              B=",{"$f":"+'Analiza i dimenzioniranje'!$E$61","v":2.9000021999999994}]
[null,null,null,null,5,{"$f":"+F153","v":2},{"$f":"+G155","v":1.25},null,"razmak težišta      lT=",{"$f":"+$C$18-(2-$G$7/2)","v":1.7952392160241724}]
[null,null,null,null,6,{"$f":"+F153","v":2},{"$f":"+G154","v":0.25}]
[null,null,null,null,7,{"$f":"+F156","v":2},{"$f":"+G156","v":1.25},"B=",{"$f":"+$G$11+G149/$G$6","v":3.5666688666666659}]
[null,null,null,null,8,{"$f":"+F158","v":2},{"$f":"+G150","v":1.5},"W=",{"$f":"+I158*I158/6","v":2.1201878007415464}]
[null,null,null,null,9,{"$f":"+F150","v":4.9000021999999994},{"$f":"+G150","v":1.5}]
[null,null,null,null,"  A=",{"$f":"-0.5*(+(F150*G151-F151*G150)+(F151*G152-F152*G151)+(F152*G153-F153*G152)+(F153*G154-F154*G153)+(F154*G155-F155*G154)+(F155*G156-F156*G155)+(F156*G157-F157*G156)+(F157*G158-F158*G157)+(F158*G159-F159*G158)+(F159*G160-F160*G159))","v":5.3500032999999991},"m2"]
[null,null,null,null,"xt=",{"$f":"-((F150*G151-F151*G150)*(F150+F151)+(F151*G152-F152*G151)*(F151+F152)+(F152*G153-F153*G152)*(F152+F153)+(F153*G154-F154*G153)*(F153+F154)+(F154*G155-F155*G154)*(F154+F155)+(F155*G156-F156*G155)*(F155+F156)+(F156*G157-F157*G156)*(F156+F157)+(F157*G158-F158*G157)*(F157+F158)+(F158*G159-F159*G158)*(F158+F159)+(F159*G160-F160*G159)*(F159+F160))/6/F161","v":3.0855151379072288},"m",null,null,null,null,null,null,null,null,null,null,null,{"$f":"3.8*3.5/6","v":2.2166666666666663}]
[null,null,null,null,"yt=",{"$f":"((G150*F151-G151*F150)*(G150+G151)+(G151*F152-G152*F151)*(G151+G152)+(G152*F153-G153*F152)*(G152+G153)+(G153*F154-G154*F153)*(G153+G154)+(G154*F155-G155*F154)*(G154+G155)+(G155*F156-G156*F155)*(G155+G156)+(G156*F157-G157*F156)*(G156+G157)+(G157*F158-G158*F157)*(G157+G158)+(G158*F159-G159*F158)*(G158+G159)+(G159*F160-G160*F159)*(G159+G160))/6/F161","v":0.74999999999999989},"m"]
[null,null,null,null,"Broj rebara",null,9]
[null,null,null,null,1,{"$f":"2+J170","v":4.9000021999999994},{"$f":"+J169","v":1.3333333333333333},null,"duljina zida             L=",{"$f":"+'Analiza i dimenzioniranje'!$E$49","v":12}]
[null,null,null,null,2,{"$f":"+F165","v":4.9000021999999994},0,null,"duljina kontrafore   l=",{"$f":"+Kontrafore!$E$3","v":1}]
[null,null,null,null,3,2,0,null,"širina kontrafore    b=",{"$f":"+Kontrafore!$E$4","v":1}]
[null,null,null,null,4,{"$f":"+F167","v":2},{"$f":"0+(G165-J167)/2","v":0.16666666666666663},null,"broj kontrafora      n=",{"$f":"+G164","v":9}]
[null,null,null,null,null,{"$f":"+F168-J166","v":1},{"$f":"+G168","v":0.16666666666666663},null,"temelja za 1 rebro  b=",{"$f":"+J165/J168","v":1.3333333333333333}]
[null,null,null,null,null,{"$f":"+F169","v":1},{"$f":"+G169++J166","v":1.1666666666666665},null,"širina zida              B=",{"$f":"+'Analiza i dimenzioniranje'!$E$61","v":2.9000021999999994}]
[null,null,null,null,5,{"$f":"+F168","v":2},{"$f":"+G170","v":1.1666666666666665},null,"razmak težišta      lT=",{"$f":"+$C$18-(2-$G$7/2)","v":1.7952392160241724}]
[null,null,null,null,6,{"$f":"+F168","v":2},{"$f":"+G169","v":0.16666666666666663}]
[null,null,null,null,7,{"$f":"+F171","v":2},{"$f":"+G171","v":1.1666666666666665},"B=",{"$f":"+$G$11+G164/$G$6","v":3.6500021999999994}]
[null,null,null,null,8,{"$f":"+F173","v":2},{"$f":"+G165","v":1.3333333333333333},"W=",{"$f":"+I173*I173/6","v":2.220419343334139}]
[null,null,null,null,9,{"$f":"+F165","v":4.9000021999999994},{"$f":"+G165","v":1.3333333333333333}]
[null,null,null,null,"  A=",{"$f":"-0.5*(+(F165*G166-F166*G165)+(F166*G167-F167*G166)+(F167*G168-F168*G167)+(F168*G169-F169*G168)+(F169*G170-F170*G169)+(F170*G171-F171*G170)+(F171*G172-F172*G171)+(F172*G173-F173*G172)+(F173*G174-F174*G173)+(F174*G175-F175*G174))","v":4.8666695999999989},"m2"]
[null,null,null,null,"xt=",{"$f":"-((F165*G166-F166*G165)*(F165+F166)+(F166*G167-F167*G166)*(F166+F167)+(F167*G168-F168*G167)*(F167+F168)+(F168*G169-F169*G168)*(F168+F169)+(F169*G170-F170*G169)*(F169+F170)+(F170*G171-F171*G170)*(F170+F171)+(F171*G172-F172*G171)*(F171+F172)+(F172*G173-F173*G172)*(F172+F173)+(F173*G174-F174*G173)*(F173+F174)+(F174*G175-F175*G174)*(F174+F175))/6/F176","v":3.0493161839744691},"m"]
[null,null,null,null,"yt=",{"$f":"((G165*F166-G166*F165)*(G165+G166)+(G166*F167-G167*F166)*(G166+G167)+(G167*F168-G168*F167)*(G167+G168)+(G168*F169-G169*F168)*(G168+G169)+(G169*F170-G170*F169)*(G169+G170)+(G170*F171-G171*F170)*(G170+G171)+(G171*F172-G172*F171)*(G171+G172)+(G172*F173-G173*F172)*(G172+G173)+(G173*F174-G174*F173)*(G173+G174)+(G174*F175-G175*F174)*(G174+G175))/6/F176","v":0.66666666666666663},"m"]
[null,null,null,null,"Broj rebara",null,10]
[null,null,null,null,1,{"$f":"2+J185","v":4.9000021999999994},{"$f":"+J184","v":1.2},null,"duljina zida             L=",{"$f":"+'Analiza i dimenzioniranje'!$E$49","v":12}]
[null,null,null,null,2,{"$f":"+F180","v":4.9000021999999994},0,null,"duljina kontrafore   l=",{"$f":"+Kontrafore!$E$3","v":1}]
[null,null,null,null,3,2,0,null,"širina kontrafore    b=",{"$f":"+Kontrafore!$E$4","v":1}]
[null,null,null,null,4,{"$f":"+F182","v":2},{"$f":"0+(G180-J182)/2","v":9.9999999999999978E-2},null,"broj kontrafora      n=",{"$f":"+G179","v":10}]
[null,null,null,null,null,{"$f":"+F183-J181","v":1},{"$f":"+G183","v":9.9999999999999978E-2},null,"temelja za 1 rebro  b=",{"$f":"+J180/J183","v":1.2}]
[null,null,null,null,null,{"$f":"+F184","v":1},{"$f":"+G184++J181","v":1.1000000000000001},null,"širina zida              B=",{"$f":"+'Analiza i dimenzioniranje'!$E$61","v":2.9000021999999994}]
[null,null,null,null,5,{"$f":"+F183","v":2},{"$f":"+G185","v":1.1000000000000001},null,"razmak težišta      lT=",{"$f":"+$C$18-(2-$G$7/2)","v":1.7952392160241724}]
[null,null,null,null,6,{"$f":"+F183","v":2},{"$f":"+G184","v":9.9999999999999978E-2}]
[null,null,null,null,7,{"$f":"+F186","v":2},{"$f":"+G186","v":1.1000000000000001},"B=",{"$f":"+$G$11+G179/$G$6","v":3.7333355333333329}]
[null,null,null,null,8,{"$f":"+F188","v":2},{"$f":"+G180","v":1.2},"W=",{"$f":"+I188*I188/6","v":2.322965700741547}]
[null,null,null,null,9,{"$f":"+F180","v":4.9000021999999994},{"$f":"+G180","v":1.2}]
[null,null,null,null,"  A=",{"$f":"-0.5*(+(F180*G181-F181*G180)+(F181*G182-F182*G181)+(F182*G183-F183*G182)+(F183*G184-F184*G183)+(F184*G185-F185*G184)+(F185*G186-F186*G185)+(F186*G187-F187*G186)+(F187*G188-F188*G187)+(F188*G189-F189*G188)+(F189*G190-F190*G189))","v":4.4800026399999995},"m2","B'=",{"$f":"+F191/J184","v":3.7333355333333329}]
[null,null,null,null,"xt=",{"$f":"-((F180*G181-F181*G180)*(F180+F181)+(F181*G182-F182*G181)*(F181+F182)+(F182*G183-F183*G182)*(F182+F183)+(F183*G184-F184*G183)*(F183+F184)+(F184*G185-F185*G184)*(F184+F185)+(F185*G186-F186*G185)*(F185+F186)+(F186*G187-F187*G186)*(F186+F187)+(F187*G188-F188*G187)*(F187+F188)+(F188*G189-F189*G188)*(F188+F189)+(F189*G190-F190*G189)*(F189+F190))/6/F191","v":3.0147332538185512},"m"]
[null,null,null,null,"yt=",{"$f":"((G180*F181-G181*F180)*(G180+G181)+(G181*F182-G182*F181)*(G181+G182)+(G182*F183-G183*F182)*(G182+G183)+(G183*F184-G184*F183)*(G183+G184)+(G184*F185-G185*F184)*(G184+G185)+(G185*F186-G186*F185)*(G185+G186)+(G186*F187-G187*F186)*(G186+G187)+(G187*F188-G188*F187)*(G187+G188)+(G188*F189-G189*F188)*(G188+G189)+(G189*F190-G190*F189)*(G189+G190))/6/F191","v":0.6}]

{"sheet":"Poprečni presjek zida","index":8,"n_rows":217,"n_cols":91,"rows_kept":217,"cut":false,"hidden":false,"merged":[[0,24,1,24],[2,24,22,24],[18,11,18,12],[0,26,0,27],[0,28,0,29],[37,25,43,25],[45,47,45,48],[42,49,42,50],[45,41,45,42],[45,43,45,44],[45,45,45,46],[21,50,21,51],[22,50,22,51],[27,12,27,13],[22,47,22,48],[29,47,29,48],[32,11,32,13],[33,11,33,13],[34,11,34,13],[42,41,42,42],[42,43,42,44],[42,45,42,46],[42,47,42,48],[38,50,38,51],[173,2,180,2],[173,6,180,6],[181,2,188,2],[181,6,188,6],[189,2,196,2],[189,6,196,6],[197,2,204,2],[197,6,204,6],[126,2,132,2],[126,6,132,6],[133,2,140,2],[133,6,140,6],[141,2,148,2],[141,6,148,6],[149,2,156,2],[149,6,156,6],[157,2,164,2],[157,6,164,6],[165,2,172,2],[165,6,172,6],[91,73,91,74],[102,21,102,22],[103,21,103,22],[106,21,106,23],[91,4,91,5],[93,4,93,5],[83,6,83,7],[83,8,83,9],[83,12,83,13],[83,14,83,15],[94,5,94,6],[94,7,94,8],[94,9,94,10],[94,11,94,12],[85,4,85,5],[86,4,86,5],[87,4,87,5],[88,4,88,5],[89,4,89,5],[90,4,90,5],[97,16,97,20],[101,21,101,22],[73,72,81,72],[82,72,90,72],[51,25,57,25],[72,29,72,30],[98,21,98,22],[99,21,99,22],[100,21,100,22],[55,68,63,68],[58,25,64,25],[65,25,71,25],[97,21,97,23],[29,59,29,60],[31,56,31,57],[31,59,31,60],[33,59,33,60],[35,59,35,60],[23,25,29,25],[29,45,29,46],[36,45,36,46],[33,42,33,43],[29,50,29,51],[31,50,31,51],[29,42,29,43],[27,45,27,46],[25,42,25,43],[33,53,33,54],[35,53,35,54],[33,45,33,46],[30,25,36,25],[29,53,29,54],[31,53,31,54],[31,47,31,48],[33,47,33,48],[35,47,35,48],[29,56,29,57],[10,68,18,68],[19,68,27,68],[9,25,15,25],[16,25,22,25],[7,45,7,46],[0,59,0,60],[0,47,0,48],[0,50,0,51],[0,53,0,54],[22,59,22,60],[16,59,16,60],[0,45,0,46],[9,45,9,46],[14,45,14,46],[17,45,17,46],[20,45,20,46],[2,25,8,25],[3,42,3,43],[20,42,20,43],[0,41,15,41],[12,50,12,51],[21,56,21,57],[22,53,22,54],[22,56,22,57],[0,56,0,57],[0,42,0,43],[16,42,16,43],[11,42,11,43],[9,42,9,43],[6,42,6,43],[8,50,8,51],[12,56,12,57],[16,53,16,54],[16,47,16,48],[42,55,42,56],[45,55,45,56],[48,49,48,50],[48,43,48,44],[42,53,42,54],[45,53,45,54],[48,53,48,54],[42,51,42,52],[45,49,45,50],[45,51,45,52],[48,51,48,52],[48,45,48,46],[48,47,48,48],[108,17,108,18],[108,19,108,20],[108,1,108,2],[108,3,108,4],[108,7,108,8],[108,9,108,10],[108,11,108,12],[108,13,108,14],[48,55,48,56],[44,25,50,25],[47,41,47,42],[50,41,50,42],[50,43,50,44],[107,21,107,22],[50,51,50,52]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kontrafore","Koordinate",null,"Rebra",null,null,null,null,null,null,null,null,null,null,null,null,null,"H kotna c. gore",null,null,"Kote temelja u B",null,"Kontrafora",null,null,"Kontrafora",null,null,"ZID i TEMELJ",null,null,"Masa temelja",null,null,"Masa masivnog zida",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"br.","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ8-0.8","v":3.0000021999999991},{"$f":"+BC10","v":"A"},null,{"$f":"+AT6-0.1","v":-0.55000000000000004},0,"visina kontrafore",null,null,0.5,null,null,{"$f":"+'C III-V'!B2-2","v":0},{"$f":"+'C III-V'!C2","v":0.12820515121628623},null,{"$f":"+BB2","v":0},{"$f":"+BC2","v":0.12820515121628623},null,{"$f":"+BB3","v":0},{"$f":"+BC3","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"+Kontrafore!X75","v":4},{"$f":"+Kontrafore!W$75","v":4.9000021999999994}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NAPOMENA:  Za prijenos tlocrta u ACAD koristiti koordinate  iz tablice            ",1,{"$f":"+Kontrafore!AB73","v":0},{"$f":"+Kontrafore!AA73","v":3.4000000999999997},{"$f":"+AA4","v":1.875},{"$f":"IF(AA3=\"\",\"\",+$O$18)","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ8+0.1","v":3.9000021999999994},{"$f":"+AR2","v":"A"},null,{"$f":"+AT6+0.1","v":-0.35},0,{"$f":"IF(Kontrafore!E1=\"\",-5,+BB50)","v":3.1000010999999996},{"$f":"IF(Kontrafore!E1=\"\",-5,+BC26+0.6)","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(Kontrafore!E1=\"\",-5,-0.5+('Poprečni presjek zida'!BB21+0.5)/2)","v":-0.375},{"$f":"IF(Kontrafore!E1=\"\",-5,+AG66+0.5+0.1)","v":0.6},null,{"$f":"+'C III-V'!B3-2","v":0},{"$f":"+'C III-V'!C3","v":1.2},null,{"$f":"+BB3","v":0},{"$f":"+BC3","v":1.2},null,{"$f":"+BB9","v":{"$error":"#VALUE!"}},"A",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!X74","v":0},{"$f":"+Kontrafore!W$74","v":4.9000021999999994}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB74","v":1.875},{"$f":"+Kontrafore!AA74","v":3.4000000999999997},{"$f":"+AC3","v":1.875},{"$f":"IF(AA3=\"\",\"\",+AD3+0.5)","v":1.7},null,null,null,null,null,null,null,null,null,null,null,null,"H kotna c. Dole",null,null,{"$f":"+AT2","v":-0.55000000000000004},{"$f":"+BC12","v":1.2},{"$f":"+AV3","v":3.1000010999999996},{"$f":"+O18-0.1","v":1.0999999999999999},null,{"$f":"+AY3","v":-0.375},{"$f":"IF(Kontrafore!E1=\"\",-5,AG66-0.1)","v":-0.1},null,{"$f":"+'C III-V'!B4-2","v":1.4000010999999999},{"$f":"+'C III-V'!C4","v":1.2},null,{"$f":"+BB14","v":2.9000021999999994},1.2,null,{"$error":"#VALUE!"},"A",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!X81","v":0},{"$f":"+Kontrafore!W$81","v":2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB75","v":1.875},{"$f":"+Kontrafore!AA75","v":1.5},{"$f":"+AC4+'Analiza i dimenzioniranje'!$D$86","v":2.125},{"$f":"+AD4","v":1.7},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ2","v":3.0000021999999991},0,null,{"$f":"+AT3","v":-0.35},{"$f":"+AU4","v":1.2},{"$f":"+AV4-0.1","v":3.0000010999999995},{"$f":"IF(Kontrafore!E1=\"\",-5,BC26)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(Kontrafore!E1=\"\",-5,AY4-0.1)","v":-0.47499999999999998},{"$f":"IF(Kontrafore!E1=\"\",-5,+AG66+0.5)","v":0.5},null,{"$f":"+'C III-V'!B5-2","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C5","v":3.14},null,2.9000021999999994,0.5,null,2.2000010999999997,1.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!X80","v":1.5},{"$f":"+Kontrafore!W$80","v":2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB76","v":2.125},{"$f":"+Kontrafore!AA76","v":1.5},{"$f":"+AC4","v":1.875},{"$f":"+AD5","v":1.7},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ3","v":3.9000021999999994},0,null,{"$f":"+IF(Kontrafore!E1=\"\",-0.2,-0.2+'Poprečni presjek zida'!BB20)","v":-0.45},{"$f":"+AU2-0.1","v":-0.1},{"$f":"+AV4+0.1","v":3.2000010999999997},{"$f":"IF(Kontrafore!E1=\"\",-5,+AW5)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(Kontrafore!E1=\"\",-5,+AV19-0.05)","v":-0.65},{"$f":"+AZ5","v":0.5},null,{"$f":"+'C III-V'!B6-2","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C6","v":3.14},null,0,0.12820515121628623,null,{"$f":"+BH2","v":0},{"$f":"+BI2","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!X79","v":1.5},{"$f":"+Kontrafore!W$79","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB77","v":2.125},{"$f":"+Kontrafore!AA77","v":3.4000000999999997},{"$f":"+AC6","v":1.875},{"$f":"+IF(AA3=\"\",\"\",O13-0.5)","v":5.5},null,null,null,null,null,null,null,null,null,null,null,null,"Oznaka visine zida i temelja",null,null,{"$f":"+AT6","v":-0.45},{"$f":"+BC11+0.1","v":1.3},{"$f":"IF(Kontrafore!E1=\"\",\"\",AV3-0.05)","v":3.0500010999999998},{"$f":"IF(Kontrafore!E1=\"\",-5,(AW5+AG66)/2)","v":{"$error":"#VALUE!"}},null,0.5,null,null,{"$f":"+'C III-V'!B7-2","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C7","v":3.44},null,"  A=",{"$f":"-0.5*((BE2*BF3-BE3*BF2)+(BE3*BF4-BE4*BF3)+(BE4*BF5-BE5*BF4)+(BE5*BF6-BE6*BF5))","v":2.5691044797107176},null,"  A=",{"$f":"-0.5*((BH2*BI3-BH3*BI2)+(BH3*BI4-BH4*BI3)+(BH4*BI5-BH5*BI4)+(BH5*BI6-BH6*BI5))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!X78","v":2.5},{"$f":"+Kontrafore!W$78","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB78","v":2.125},{"$f":"+Kontrafore!AA78","v":3.4000000999999997},{"$f":"+AA6","v":2.125},{"$f":"+AD7","v":5.5},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Analiza i dimenzioniranje'!E61+0.9","v":3.8000021999999993},{"$f":"+AR2+0.1","v":{"$error":"#VALUE!"}},null,"h",null,"kontr gore",null,null,{"$f":"+AY3","v":-0.375},{"$f":"+IF(Kontrafore!E1=\"\",-5,BC13+(AZ6-AG66)/2)","v":1.45},null,{"$f":"+'C III-V'!B8-2","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C8","v":3.44},null,"xt=",{"$f":"IF(BF7=0,0,-((BE2*BF3-BE3*BF2)*(BE2+BE3)+(BE3*BF4-BE4*BF3)*(BE3+BE4)+(BE4*BF5-BE5*BF4)*(BE4+BE5)+(BE5*BF6-BE6*BF5)*(BE5+BE6))/6/BF7)","v":1.348577969648914},null,"xt=",{"$f":"IF(BI7=0,0,-((BH2*BI3-BH3*BI2)*(BH2+BH3)+(BH3*BI4-BH4*BI3)*(BH3+BH4)+(BH4*BI5-BH5*BI4)*(BH4+BH5)+(BH5*BI6-BH6*BI5)*(BH5+BH6))/6/BI7)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!X77","v":2.5},{"$f":"+Kontrafore!W$77","v":2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB79","v":4},{"$f":"+Kontrafore!AA79","v":3.4000000999999997},{"$f":"+AA7","v":2.125},{"$f":"+AD3","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ8","v":3.8000021999999993},-0.1,null,{"$f":"IF('Unos podataka'!$G$57=\"DA\",AT6-0.05,-0.35)","v":-0.5},{"$f":"+AG66/2","v":0},{"$f":"IF(Kontrafore!E1=\"\",\"\",BB26-0.1)","v":{"$error":"#VALUE!"}},{"$f":"IF(Kontrafore!E1=\"\",-5,BC26-0.2)","v":{"$error":"#VALUE!"}},null,"kot cr gore",null,null,{"$f":"+'C III-V'!B9-2","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C9","v":"A"},null,"yt=",{"$f":"IF(BF7=0,0,-((BE2*BF3-BE3*BF2)*(BF2+BF3)+(BE3*BF4-BE4*BF3)*(BF3+BF4)+(BE4*BF5-BE5*BF4)*(BF4+BF5)+(BE5*BF6-BE6*BF5)*(BF5+BF6))/6/BF7)","v":0.75054981042380386},null,"yt=",{"$f":"IF(BI7=0,0,-((BH2*BI3-BH3*BI2)*(BI2+BI3)+(BH3*BI4-BH4*BI3)*(BI3+BI4)+(BH4*BI5-BH5*BI4)*(BI4+BI5)+(BH5*BI6-BH6*BI5)*(BI5+BI6))/6/BI7)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!X82","v":4},{"$f":"IF(CH9=0,0,+Kontrafore!W$82)","v":2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"+Kontrafore!AB82","v":4},{"$f":"+Kontrafore!AA82","v":3.4000000999999997},{"$f":"+AA11","v":5.875},{"$f":"IF(AA10=\"\",\"\",+$O$18)","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,"Oznaka H",null,null,"Kote temelja u A",null,{"$f":"IF(Kontrafore!E1=\"\",\"\",+BB27+0.1)","v":{"$error":"#VALUE!"}},{"$f":"+AW9","v":{"$error":"#VALUE!"}},null,{"$f":"IF(Kontrafore!E1=\"\",-5,AV3)","v":3.1000010999999996},{"$f":"+IF(Kontrafore!E1=\"\",-5,AR3+0.1)","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!B10-2","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C10","v":"A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH2","v":4},{"$f":"+Kontrafore!W$75","v":4.9000021999999994}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB83","v":5.875},{"$f":"+Kontrafore!AA83","v":3.4000000999999997},{"$f":"+AC10","v":5.875},{"$f":"IF(AA10=\"\",\"\",+AD10+0.5)","v":1.7},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ9-0.05","v":3.7500021999999995},{"$f":"+AR8/2","v":{"$error":"#VALUE!"}},null,{"$f":"+AT13","v":3.1000021999999996},{"$f":"+(AG66-AG65)","v":0},"kotne crte",null,null,{"$f":"+AY10","v":3.1000010999999996},{"$f":"+O18","v":1.2},null,{"$f":"+'C III-V'!B11-2","v":2.2000010999999997},{"$f":"+'C III-V'!C11","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"+CH2+Kontrafore!$E$8","v":8},{"$f":"+$CI$2","v":4.9000021999999994}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dimenzije i oznake zida      ",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB84","v":5.875},{"$f":"+Kontrafore!AA84","v":1.5},{"$f":"+AC11+'Analiza i dimenzioniranje'!$D$86","v":6.125},{"$f":"+AD11","v":1.7},null,null,null,null,null,null,null,null,null,null,null,null,"Kotne c širine temelja",null,null,{"$f":"+AT14","v":3.3000021999999998},{"$f":"+AU11","v":0},{"$f":"IF(Kontrafore!E1=\"\",\"\",+BB26)","v":{"$error":"#VALUE!"}},{"$f":"IF(Kontrafore!E1=\"\",-5,AW9-0.1)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(Kontrafore!E1=\"\",-5,+AY11-0.05)","v":3.0500010999999998},{"$f":"IF(Kontrafore!$E$1=\"\",-5,+BC26+0.5/2)","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!B12-2","v":2.2000010999999997},{"$f":"+'C III-V'!C12","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH3+Kontrafore!$E$8","v":4},{"$f":"+CI$3","v":4.9000021999999994}]
[null,null,null,null,null,null,null,null,null,null,null,null,"H ","=",{"$f":"+'Analiza i dimenzioniranje'!E48","v":6},{"$f":"+'Analiza i dimenzioniranje'!F48","v":"m"},null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB85","v":6.125},{"$f":"+Kontrafore!AA85","v":1.5},{"$f":"+AC11","v":5.875},{"$f":"+AD12","v":1.7},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Kontrafore!E1=\"\",'Analiza i dimenzioniranje'!E60,-Kontrafore!E3)","v":-1},-0.4,null,{"$f":"+'Analiza i dimenzioniranje'!E61+0.2","v":3.1000021999999996},{"$f":"+AG66","v":0},{"$f":"+AV12","v":{"$error":"#VALUE!"}},{"$f":"IF(Kontrafore!E1=\"\",-5,AW9+0.1)","v":{"$error":"#VALUE!"}},null,"Kontr na temelju",null,null,{"$f":"+'C III-V'!B13-2","v":2.2000010999999997},{"$f":"+'C III-V'!C13","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH4+Kontrafore!$E$8","v":4},{"$f":"+CI$4","v":2}]
[null,null,null,null,null,null,null,null,null,null,null,null,"L ","=",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},{"$f":"+'Analiza i dimenzioniranje'!F49","v":"m"},null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB86","v":6.125},{"$f":"+Kontrafore!AA86","v":3.4000000999999997},{"$f":"+AC13","v":5.875},{"$f":"+IF(AA10=\"\",\"\",O13-0.5)","v":5.5},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ13","v":-1},-0.2,null,{"$f":"+AT13+0.2","v":3.3000021999999998},{"$f":"+AU13","v":0},{"$f":"IF(Kontrafore!E1=\"\",\"\",+BB27)","v":{"$error":"#VALUE!"}},{"$f":"+AW12","v":{"$error":"#VALUE!"}},null,{"$f":"+BB24-0.1","v":-0.59999899999999984},{"$f":"+IF(Kontrafore!$E$1=\"\",-5,BC20-0.3)","v":0.89999999999999991},null,{"$f":"+'C III-V'!B14-2","v":2.9000021999999994},{"$f":"+'C III-V'!C14","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH5+Kontrafore!$E$8","v":5.5},{"$f":"+CI$5","v":2}]
[null,null,null,null,null,null,null,null,null,null,null,null,"b ","=",{"$f":"+'Analiza i dimenzioniranje'!E50","v":4},{"$f":"+'Analiza i dimenzioniranje'!F50","v":"°"},null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB87","v":6.125},{"$f":"+Kontrafore!AA87","v":3.4000000999999997},{"$f":"+AA13","v":6.125},{"$f":"+AD14","v":5.5},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!E61+'Analiza i dimenzioniranje'!E60","v":2.9000021999999994},-0.4,null,"kota hA",null,{"$f":"+AV14","v":{"$error":"#VALUE!"}},{"$f":"+AW13","v":{"$error":"#VALUE!"}},null,{"$f":"+BB4+0.1","v":1.5000011},{"$f":"+AZ14","v":0.89999999999999991},null,{"$f":"+'C III-V'!B15-2","v":2.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH6+Kontrafore!$E$8","v":5.5},{"$f":"+CI$6","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,"h","A","=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},{"$f":"+'Analiza i dimenzioniranje'!F51","v":"m"},null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB88","v":8},{"$f":"+Kontrafore!AA88","v":3.4000000999999997},{"$f":"+AA14","v":6.125},{"$f":"+AD10","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ15","v":2.9000021999999994},-0.2,null,{"$f":"+AT19","v":3.2000021999999997},{"$f":"+AG66+0.1","v":0.1},0.5,null,null,{"$f":"+AY14+0.1","v":-0.49999899999999986},{"$f":"IF(Kontrafore!$E$1=\"\",-5,+AZ14-0.1)","v":0.79999999999999993},null,{"$f":"+'C III-V'!B16-2","v":0},{"$f":"+'C III-V'!C16","v":0.12820515121628623},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH7+Kontrafore!$E$8","v":6.5},{"$f":"+CI$7","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,"h","B","=",{"$f":"+'Analiza i dimenzioniranje'!C193","v":1.0728357545883234},{"$f":"+'Analiza i dimenzioniranje'!F52","v":"m"},null,null,null,null,null,null,null,null,null,3,{"$f":"+Kontrafore!AB91","v":8},{"$f":"+Kontrafore!AA91","v":3.4000000999999997},{"$f":"+AA18","v":9.875},{"$f":"IF(AA17=\"\",\"\",+$O$18)","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,"Oznaka B",null,null,{"$f":"+AT16","v":3.2000021999999997},{"$f":"+(AG66-AG65)-0.1","v":-0.1},{"$f":"IF(Kontrafore!E1=\"\",\"\",(AV13+AV14)/2)","v":{"$error":"#VALUE!"}},{"$f":"IF(Kontrafore!E1=\"\",-5,AW10-0.05)","v":{"$error":"#VALUE!"}},null,{"$f":"+AY16","v":-0.49999899999999986},{"$f":"IF(Kontrafore!$E$1=\"\",-5,+AZ14+0.1)","v":0.99999999999999989},null,"Kontrafora",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH8+Kontrafore!$E$8","v":6.5},{"$f":"+CI$8","v":2}]
[null,null,null,null,null,null,null,null,null,null,null,"h",{"$f":"+IF('Analiza i dimenzioniranje'!D83=\"\",\"B\",\"0\")","v":"0"},"=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!F52","v":"m"},null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB92","v":9.875},{"$f":"+Kontrafore!AA92","v":3.4000000999999997},{"$f":"+AC17","v":9.875},{"$f":"IF(AA17=\"\",\"\",+AD17+0.5)","v":1.7},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!D83=\"\",-0.1+'Analiza i dimenzioniranje'!E60,-'Analiza i dimenzioniranje'!D83-0.1)","v":-1.1000000000000001},-0.3,null,"hA",null,"kontr dole",null,null,{"$f":"+BB4","v":1.4000010999999999},{"$f":"+AZ16","v":0.79999999999999993},null,{"$f":"+'Unos podataka'!I41-2","v":0},{"$f":"+'Unos podataka'!J41","v":0.12820515121628623},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH9+Kontrafore!$E$8","v":8},{"$f":"+CI$9","v":2}]
[null,null,null,null,null,null,null,null,null,null,null,"n2",null,"=",{"$f":"+'Analiza i dimenzioniranje'!E53","v":7.8000043999999988},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB93","v":9.875},{"$f":"+Kontrafore!AA93","v":1.5},{"$f":"+AC22","v":10.125},{"$f":"+AD18","v":1.7},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Analiza i dimenzioniranje'!E61+0.1+'Analiza i dimenzioniranje'!E60","v":3.0000021999999995},{"$f":"+AR18","v":-0.3},null,{"$f":"+(AT11+AT12)/2","v":3.2000021999999997},{"$f":"+(AU12+AU13)/2","v":0},{"$f":"IF(Kontrafore!$E$1=\"\",-5,-AV16-0.1)","v":-0.6},{"$f":"IF(Kontrafore!E1=\"\",-5,+AR27)","v":1.5},null,{"$f":"+AY18","v":1.4000010999999999},{"$f":"+AZ17","v":0.99999999999999989},null,{"$f":"+'Unos podataka'!I42-2","v":0},{"$f":"+'Unos podataka'!J42","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH10+Kontrafore!$E$8","v":8},{"$f":"+CI$10","v":4.9000021999999994}]
[null,null,null,null,null,null,null,null,null,null,null,null,"d ","=",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},{"$f":"+'Analiza i dimenzioniranje'!F54","v":"m"},null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB94","v":10.125},{"$f":"+Kontrafore!AA94","v":1.5},{"$f":"+AC18","v":9.875},{"$f":"+AD19","v":1.7},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Kontrafore!E1=\"\",(+'Analiza i dimenzioniranje'!E61)/2+'Analiza i dimenzioniranje'!E60,('Analiza i dimenzioniranje'!E61+BB21)/2)","v":1.3250010999999997},{"$f":"+AR19","v":-0.3},null,null,null,{"$f":"+IF(Kontrafore!E1=\"\",-5,0)","v":0},{"$f":"+AW19","v":1.5},null,{"$f":"+(A147+A148)/2","v":0},{"$f":"+AZ14","v":0.89999999999999991},null,{"$f":"+'Unos podataka'!I43-2","v":-0.25},{"$f":"+'Unos podataka'!J43","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"+CH11+Kontrafore!$E$8","v":12},{"$f":"IF(CH20>'Analiza i dimenzioniranje'!$E$30,0,$CI$2)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,"d1","=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},{"$f":"+'Analiza i dimenzioniranje'!F55","v":"m"},null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB95","v":10.125},{"$f":"+Kontrafore!AA95","v":3.4000000999999997},{"$f":"+AC20","v":9.875},{"$f":"+IF(AA17=\"\",\"\",O13-0.5)","v":5.5},null,null,null,null,null,null,null,null,null,null,null,null,"Temelj prema tlu",null,null,"kote d",null,0.5,null,null,null,null,null,{"$f":"+'Unos podataka'!I46-2","v":-0.25},{"$f":"+'Unos podataka'!J46","v":9.6153895463470418E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH12+Kontrafore!$E$8","v":8},{"$f":"IF(CH20=0,0,CI3)","v":4.9000021999999994}]
[null,null,null,null,null,null,null,null,null,null,null,null,"n1","=",{"$f":"+'Analiza i dimenzioniranje'!E56","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB96","v":10.125},{"$f":"+Kontrafore!AA96","v":3.4000000999999997},{"$f":"+AA20","v":10.125},{"$f":"+AD21","v":5.5},null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+BC3+0.2","v":1.4},null,{"$f":"+BB9","v":{"$error":"#VALUE!"}},{"$f":"+BC9+0.2","v":{"$error":"#VALUE!"}},{"$f":"IF(Kontrafore!E1=\"\",-5,-AV21/2)","v":-0.25},{"$f":"IF(Kontrafore!E1=\"\",-5,AW19+0.05)","v":1.55},null,"Konzola",null,null,{"$f":"+BB18","v":0},{"$f":"+'Unos podataka'!J47","v":0.12820515121628623},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH13+Kontrafore!$E$8","v":8},2]
[null,null,null,null,null,null,null,null,null,null,null,null,"n3","=",{"$f":"IF(+'Analiza i dimenzioniranje'!F57>100,\"100\",+'Analiza i dimenzioniranje'!F57)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB97","v":12},{"$f":"+Kontrafore!AA97","v":3.4000000999999997},{"$f":"+AA21","v":10.125},{"$f":"+AD17","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ22","v":0},{"$f":"+AR22+0.2","v":1.5999999999999999},null,{"$f":"+AT22","v":{"$error":"#VALUE!"}},{"$f":"+AU22+0.2","v":{"$error":"#VALUE!"}},0.5,null,null,"Konzola L",null,null,"Rebra",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH14+Kontrafore!$E$8","v":9.5},2]
[null,null,null,null,null,null,null,null,null,null,null,null,"b1","=",{"$f":"+'Analiza i dimenzioniranje'!E58","v":0.70000099999999998},{"$f":"+'Analiza i dimenzioniranje'!F58","v":"m"},null,null,null,null,null,null,null,null,null,4,{"$f":"+Kontrafore!AB100","v":""},{"$f":"+Kontrafore!AA100","v":""},{"$f":"+AA25","v":""},{"$f":"IF(AA24=\"\",\"\",+$O$18)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+BB4","v":1.4000010999999999},{"$f":"+AR22","v":1.4},null,{"$f":"+BB10","v":{"$error":"#VALUE!"}},{"$f":"+AU22","v":{"$error":"#VALUE!"}},{"$f":"+IF(Kontrafore!E1=\"\",-5,0)","v":0},{"$f":"+IF(Kontrafore!E1=\"\",-5,-0.2)","v":-0.2},null,{"$f":"IF('Unos podataka'!$G$57=\"DA\",BB7,-5)","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$G$57=\"DA\",BC5-0.3,-5)","v":2.8400000000000003},null,{"$f":"+'Unos podataka'!I49-2","v":-0.49999899999999986},{"$f":"+'Unos podataka'!J49","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH15+Kontrafore!$E$8","v":9.5},1]
[null,null,null,null,null,null,null,null,null,null,null,null,"b2","=",{"$f":"+'Analiza i dimenzioniranje'!E59","v":1.4000001},{"$f":"+'Analiza i dimenzioniranje'!F59","v":"m"},null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB101","v":""},{"$f":"+Kontrafore!AA101","v":""},{"$f":"+AC24","v":""},{"$f":"IF(AA24=\"\",\"\",+AD24+0.5)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ24","v":1.4000010999999999},{"$f":"+AR23","v":1.5999999999999999},null,{"$f":"+AT24","v":{"$error":"#VALUE!"}},{"$f":"+AU23","v":{"$error":"#VALUE!"}},{"$f":"+AV24","v":0},{"$f":"+IF(Kontrafore!E1=\"\",-5,-0.4)","v":-0.4},null,{"$f":"+AY24","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$G$57=\"DA\",AZ24-0.2,-5)","v":2.64},null,{"$f":"+'Unos podataka'!I50-2","v":-0.49999899999999986},{"$f":"+'Unos podataka'!J50","v":1.7},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH16+Kontrafore!$E$8","v":10.5},1]
[null,null,null,null,null,null,null,null,null,null,null,null,"n","=",{"$f":"+'Analiza i dimenzioniranje'!E60","v":0},{"$f":"+'Analiza i dimenzioniranje'!F60","v":"m"},null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB102","v":""},{"$f":"+Kontrafore!AA102","v":""},{"$f":"+AC29","v":""},{"$f":"+AD25","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"Oznaka b2",null,null,{"$f":"+AT22-0.1","v":{"$error":"#VALUE!"}},{"$f":"+(AU23+AU22)/2","v":{"$error":"#VALUE!"}},{"$f":"+AQ13-0.1","v":-1.1000000000000001},{"$f":"+IF(Kontrafore!E1=\"\",-5,(AW24+AW25)/2+0.05)","v":-0.25000000000000006},null,{"$f":"IF('Unos podataka'!$G$57=\"DA\",BB5,-5)","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$G$57=\"DA\",AZ24,-5)","v":2.8400000000000003},null,{"$f":"+'Unos podataka'!I51-2","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!J51","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH17+Kontrafore!$E$8","v":10.5},2]
[null,null,null,null,null,null,null,null,null,null,null,null,"B","=",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m",null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB103","v":""},{"$f":"+Kontrafore!AA103","v":""},{"$f":"+AC25","v":""},{"$f":"+AD26","v":""},null,null,null,null,null,null,null,null,null,null,null,null,-0.1,{"$f":"+(AR22+AR23)/2","v":1.5},null,{"$f":"+AT25+0.1","v":{"$error":"#VALUE!"}},{"$f":"+AU26","v":{"$error":"#VALUE!"}},{"$f":"+IF(Kontrafore!E1=\"\",-5,0.1)","v":0.1},{"$f":"+AW26","v":-0.25000000000000006},null,{"$f":"+AY26","v":{"$error":"#VALUE!"}},{"$f":"+AZ25","v":2.64},null,{"$f":"+'Unos podataka'!I52-2","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!J52","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH18+Kontrafore!$E$8","v":12},2]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!A82=\"\",\"\", \"B+L\")","v":"B+L"},{"$f":"+IF('Analiza i dimenzioniranje'!A82=\"\",\"\",\"kf   =\")","v":"kf   ="},null,{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",\"\",+'Analiza i dimenzioniranje'!E61+Kontrafore!$E$3)","v":3.9000021999999994},{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",\"\",+'Analiza i dimenzioniranje'!F61)","v":"m"},null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB104","v":""},{"$f":"+Kontrafore!AA104","v":""},{"$f":"+AC27","v":""},{"$f":"+IF(AA24=\"\",\"\",O13-0.5)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ19","v":3.0000021999999995},{"$f":"+AR27","v":1.5},null,"oznaka d",null,{"$f":"+IF(Kontrafore!$E$1=\"\",-5,AQ13)","v":-1},{"$f":"+IF(Kontrafore!$E$1=\"\",-5,AR13+0.2)","v":-0.2},null,{"$f":"IF('Unos podataka'!$G$57=\"DA\",+AY24-0.1,-5)","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$G$57=\"DA\",(AZ24+AZ25)/2,-5)","v":2.74},null,{"$f":"+'Unos podataka'!I53-2","v":1.4000000999999997},{"$f":"+'Unos podataka'!J53","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH19+Kontrafore!$E$8","v":12},4.9000021999999994]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E80=\"\",\"\",\"Konzola\")","v":"Konzola"},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB105","v":""},{"$f":"+Kontrafore!AA105","v":""},{"$f":"+AA27","v":""},{"$f":"+AD28","v":""},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(O25<0.0001,-5,+AQ24/2)","v":0.70000054999999994},{"$f":"IF(AQ29=-5,-5,+(AR24+AR25)/2)","v":1.5},null,{"$f":"+(BB9+BB10)/2","v":{"$error":"#VALUE!"}},{"$f":"+(AU22+AU23)/2","v":{"$error":"#VALUE!"}},{"$f":"IF(Kontrafore!$E$1=\"\",-5,AQ14)","v":-1},{"$f":"+IF(Kontrafore!$E$1=\"\",-5,-0.1)","v":-0.1},null,{"$f":"IF('Unos podataka'!$G$57=\"DA\",BB5+0.1,-5)","v":{"$error":"#VALUE!"}},{"$f":"+AZ28","v":2.74},null,{"$f":"+'Unos podataka'!I54-2","v":-0.49999899999999986},{"$f":"+'Unos podataka'!J54","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,{"$f":"+CH20+Kontrafore!$E$8","v":16},{"$f":"IF(CH29>'Analiza i dimenzioniranje'!$E$30,0,Kontrafore!W$75)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!A77=\"\",\"\",\"b\")","v":"b"},{"$f":"+IF('Analiza i dimenzioniranje'!A77=\"\",\"\",\"k\")","v":"k"},{"$f":"+IF('Analiza i dimenzioniranje'!A77=\"\",\"\",\"=\")","v":"="},{"$f":"+'Analiza i dimenzioniranje'!E80","v":1},{"$f":"+IF('Analiza i dimenzioniranje'!D78=\"\",\"\",\"m\")","v":"m"},null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB106","v":""},{"$f":"+Kontrafore!AA106","v":""},{"$f":"+AA28","v":""},{"$f":"+AD24","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"oznaka d1",null,null,"Oznaka b1",null,0.5,null,null,"lkonz",null,null,"Oznaka n1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH21+Kontrafore!$E$8","v":12},{"$f":"IF(CH29=0,0,CI3)","v":4.9000021999999994}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!A77=\"\",\"\",\"d\")","v":"d"},{"$f":"+IF('Analiza i dimenzioniranje'!A77=\"\",\"\",\"k\")","v":"k"},{"$f":"+IF('Analiza i dimenzioniranje'!A77=\"\",\"\",\"=\")","v":"="},{"$f":"+'Analiza i dimenzioniranje'!E81","v":0.3},{"$f":"+IF('Analiza i dimenzioniranje'!D78=\"\",\"\",\"m\")","v":"m"},null,null,null,null,null,null,null,null,null,5,{"$f":"+Kontrafore!AB109","v":""},{"$f":"+Kontrafore!AA109","v":""},{"$f":"+AA32","v":""},{"$f":"IF(AA31=\"\",\"\",+$O$18)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"0+O24+O21/2","v":1.100001},{"$f":"+AR22","v":1.4},null,{"$f":"+AQ16","v":2.9000021999999994},{"$f":"+AR31","v":1.4},{"$f":"+IF(Kontrafore!$E$1=\"\",-5,BB20/2)","v":-0.125},{"$f":"+AW27","v":-0.25000000000000006},null,{"$f":"IF('Unos podataka'!$G$57=\"DA\",+(BB5+BB6)/2,-5)","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$G$57=\"\",-5,+(AZ24+AZ25)/2+0.05)","v":2.79},null,{"$f":"+(BB10+BB11)/2+0.1","v":{"$error":"#VALUE!"}},{"$f":"+(BC10+BC11)/2","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH22+Kontrafore!$E$8","v":12},{"$f":"IF(CH30=0,0,CI4)","v":2}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!A83=\"\",\"\",\"Kontrafore\")","v":"Kontrafore"},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB110","v":""},{"$f":"+Kontrafore!AA110","v":""},{"$f":"+AC31","v":""},{"$f":"IF(AA31=\"\",\"\",+AD31+0.5)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ31","v":1.100001},{"$f":"+AR23","v":1.5999999999999999},null,{"$f":"+AT31","v":2.9000021999999994},{"$f":"+AR32","v":1.5999999999999999},null,null,null,"bk",null,null,"Oznaka n2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH23+Kontrafore!$E$8","v":13.5},{"$f":"IF(CH31=0,0,CI5)","v":2}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!A83=\"\",\"\",\"L kontr =\")","v":"L kontr ="},null,null,{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",\"\",+'Analiza i dimenzioniranje'!D83)","v":1},{"$f":"+IF('Analiza i dimenzioniranje'!A82=\"\",\"\",\"m\")","v":"m"},null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB111","v":""},{"$f":"+Kontrafore!AA111","v":""},{"$f":"+AC36","v":""},{"$f":"+AD32","v":""},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ31+AQ24/2","v":1.80000155},{"$f":"+(AR28+AR29)/2","v":1.5},null,{"$f":"O24+O21+O25/2","v":2.20000105},{"$f":"+AR33+0.05","v":1.55},"Kotna za hA",null,null,{"$f":"IF('Analiza i dimenzioniranje'!E80=\"\",-5,+BB5+0.2)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E80=\"\",-5,+BC5-0.1)","v":3.04},null,{"$f":"+'Analiza i dimenzioniranje'!E61/2","v":1.4500010999999997},{"$f":"+(+BC22+BC15)/2-0.1","v":0.21410257560814314},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH24+Kontrafore!$E$8","v":13.5},{"$f":"IF(CH32=0,0,CI6)","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!A83=\"\",\"\",\"h kontr =\")","v":"h kontr ="},null,null,{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",\"\",+'Analiza i dimenzioniranje'!H85)","v":4.3},{"$f":"+IF('Analiza i dimenzioniranje'!A82=\"\",\"\",\"m\")","v":"m"},null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB112","v":""},{"$f":"+Kontrafore!AA112","v":""},{"$f":"+AC32","v":""},{"$f":"+AD33","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"Kut b",null,null,"k.c za ",null,{"$f":"+A141-0.1","v":-0.1},{"$f":"+AZ11","v":1.2},null,{"$f":"+AY33","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E80=\"\",-5,BC8+0.1)","v":3.54},null,"Oznaka n3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH25+Kontrafore!$E$8","v":14.5},1]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!A83=\"\",\"\",\"d kontr =\")","v":"d kontr ="},null,null,{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",\"\",+'Analiza i dimenzioniranje'!H83)","v":1.9000001},{"$f":"+IF('Analiza i dimenzioniranje'!A82=\"\",\"\",\"m\")","v":"m"},null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB113","v":""},{"$f":"+Kontrafore!AA113","v":""},{"$f":"+AC34","v":""},{"$f":"+IF(AA31=\"\",\"\",O13-0.5)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+BB9-0.02","v":{"$error":"#VALUE!"}},{"$f":"+BC9","v":"A"},null,{"$f":"+AZ16","v":0.79999999999999993},{"$f":"+O18+0.2","v":1.4},{"$f":"+AV34+0.2","v":0.1},{"$f":"+AW34","v":1.2},null,{"$f":"IF('Analiza i dimenzioniranje'!E80=\"\",-5,+AY33-0.1)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Analiza i dimenzioniranje'!E80=\"\",-5,BC6)","v":3.14},null,{"$f":"+BB4-0.21","v":1.1900010999999999},{"$f":"+BC4+1","v":2.2000000000000002},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH26+Kontrafore!$E$8","v":14.5},2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB114","v":""},{"$f":"+Kontrafore!AA114","v":""},{"$f":"+AA34","v":""},{"$f":"+AD35","v":""},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ35","v":{"$error":"#VALUE!"}},{"$f":"+AR35-0.4","v":{"$error":"#VALUE!"}},null,{"$f":"+AT35","v":0.79999999999999993},{"$f":"+AU32","v":1.5999999999999999},{"$f":"+AV34","v":-0.1},{"$f":"+AW34-O16","v":0.5},null,{"$f":"IF('Analiza i dimenzioniranje'!E80=\"\",-5,+AY33+0.1)","v":{"$error":"#VALUE!"}},{"$f":"+AZ35","v":3.14},null,"Oznaka n",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH27+Kontrafore!$E$8","v":16},2]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},null,null,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB115","v":""},{"$f":"+Kontrafore!AA115","v":""},{"$f":"+AA35","v":""},{"$f":"+AD31","v":""},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ36-0.2","v":{"$error":"#VALUE!"}},{"$f":"+AR35-0.2","v":{"$error":"#VALUE!"}},null,"oznaka h lijevo",null,{"$f":"+AV35","v":0.1},{"$f":"+AW36","v":0.5},null,{"$f":"+AY35","v":{"$error":"#VALUE!"}},{"$f":"+IF('Analiza i dimenzioniranje'!E80=\"\",-5,+BC7)","v":3.44},null,{"$f":"IF(O26=0,-0.05,O26/2-0.1)","v":-0.05},{"$f":"BC13/2","v":0.6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH28+Kontrafore!$E$8","v":16},4.9000021999999994]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,{"$f":"+Kontrafore!AB118","v":""},{"$f":"+Kontrafore!AA118","v":""},{"$f":"+AA39","v":""},{"$f":"IF(AA38=\"\",\"\",+$O$18)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AT6","v":-0.45},{"$f":"+AU35/2","v":0.7},"Oznaka hA",null,null,{"$f":"+AY36","v":{"$error":"#VALUE!"}},{"$f":"+AZ37","v":3.44},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+CH29+Kontrafore!$E$8","v":20},{"$f":"IF(CH38>'Analiza i dimenzioniranje'!$E$30,0,$CI$2)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB119","v":""},{"$f":"+Kontrafore!AA119","v":""},{"$f":"+AC38","v":""},{"$f":"IF(AA38=\"\",\"\",+AD38+0.5)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AT32+0.5","v":3.4000021999999994},{"$f":"(O18-O16)+(AW34-(O18-O16))/2","v":0.85},null,"Oznaka h0",null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E80=\"\",-5,(AZ36+AZ37)/2)","v":3.29},{"$f":"+IF('Analiza i dimenzioniranje'!E80=\"\",-5,AY34)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH30+Kontrafore!$E$8","v":16},{"$f":"IF(CI38=0,0,CI21)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB120","v":""},{"$f":"+Kontrafore!AA120","v":""},{"$f":"+AC43","v":""},{"$f":"+AD39","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oznaka hB",null,null,{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",-5,-1-0.01)","v":-1.01},{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",\"\",+'Analiza i dimenzioniranje'!E52/2)","v":0.6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH31+Kontrafore!$E$8","v":16},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB121","v":""},{"$f":"+Kontrafore!AA121","v":""},{"$f":"+AC39","v":""},{"$f":"+AD40","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"0-0.01","v":-0.01},{"$f":"+'Analiza i dimenzioniranje'!E52/2","v":0.6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH32+Kontrafore!$E$8","v":17.5},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB122","v":""},{"$f":"+Kontrafore!AA122","v":""},{"$f":"+AC41","v":""},{"$f":"+IF(AA38=\"\",\"\",O13-0.5)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH33+Kontrafore!$E$8","v":17.5},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB123","v":""},{"$f":"+Kontrafore!AA123","v":""},{"$f":"+AA41","v":""},{"$f":"+AD42","v":""},null,null,null,null,null,null,null,null,null,null,null,"k.c u b2 lijevo",null,"k.c-b2 desno",null,"k.c-d1 lijevo",null,"k.c d1 desno",null,"k.c  za n lijevo",null,"k.c  za n lijevo",null,"kc za hA dole",null,"kc ha hB dole",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH34+Kontrafore!$E$8","v":18.5},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB124","v":""},{"$f":"+Kontrafore!AA124","v":""},{"$f":"+AA42","v":""},{"$f":"+AD38","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ22","v":0},{"$f":"+AR22","v":1.4},{"$f":"+AP44+O25","v":1.4000001},{"$f":"+AQ44","v":1.4},{"$f":"+AR44+O21","v":2.2000001},{"$f":"+AS44","v":1.4},{"$f":"+AT44+O24","v":2.9000010999999999},{"$f":"+AU44","v":1.4},{"$f":"+IF('Analiza i dimenzioniranje'!E60=0,-5,0)","v":-5},-0.2,{"$f":"IF('Analiza i dimenzioniranje'!E60=0,-5,+'Analiza i dimenzioniranje'!E60)","v":-5},{"$f":"+AY44","v":-0.2},{"$f":"+BB45-0.2","v":3.0000010999999995},{"$f":"+BC51+0.1","v":0.5},-0.1,{"$f":"+'Unos podataka'!$L$41","v":0.12820515121628623},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH35+Kontrafore!$E$8","v":18.5},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,{"$f":"+Kontrafore!AB127","v":""},{"$f":"+Kontrafore!AA127","v":""},{"$f":"+AA46","v":""},{"$f":"IF(AA45=\"\",\"\",+$O$18)","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ23","v":0},{"$f":"+AR23","v":1.5999999999999999},{"$f":"+AQ25","v":1.4000010999999999},{"$f":"+AQ45","v":1.5999999999999999},{"$f":"+AT44","v":2.2000001},{"$f":"+AS45","v":1.5999999999999999},{"$f":"+AV44","v":2.9000010999999999},{"$f":"+AU45","v":1.5999999999999999},{"$f":"+AX44","v":-5},-0.4,{"$f":"+AZ44","v":-5},{"$f":"+AY45","v":-0.4},{"$f":"+AV45+0.3","v":3.2000010999999997},{"$f":"+BC44","v":0.5},-0.3,{"$f":"+BE44","v":0.12820515121628623},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH36+Kontrafore!$E$8","v":20},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB128","v":""},{"$f":"+Kontrafore!AA128","v":""},{"$f":"+AC45","v":""},{"$f":"IF(AA45=\"\",\"\",+AD45+0.5)","v":""},null,null,null,null,null,null,null,null,null,null,null,"oznaka b 2",null,"oznaka d1",null,"oznaka b1",null,"k.c preko svega",null,"k.c za n",null,"Oznaka n",null,"kc ha hA gore",null,"kc ha hB gore",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH37+Kontrafore!$E$8","v":20},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB129","v":""},{"$f":"+Kontrafore!AA129","v":""},{"$f":"+AC50","v":""},{"$f":"+AD46","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(O25=0,-5,+(AP44+AR44)/2)","v":0.70000004999999998},{"$f":"IF(AP47=\"\",-5,+AW48+0.01)","v":1.51},{"$f":"+(AR44+AT44)/2","v":1.8000001000000001},{"$f":"+AQ47","v":1.51},{"$f":"IF(O24<0.0001,-5,+(AV44+AT44)/2)","v":2.5500005999999997},{"$f":"IF(O24<0.0001,-5,+AS47)","v":1.51},{"$f":"+AP44-0.1","v":-0.1},{"$f":"+(AQ45+AQ44)/2","v":1.5},{"$f":"IF('Analiza i dimenzioniranje'!E60=0,-5,+AR44-0.1)","v":-5},-0.3,{"$f":"+(AX47+AX48)/2","v":-5},{"$f":"+AY47+0.01","v":-0.28999999999999998},{"$f":"+BB44","v":3.0000010999999995},{"$f":"+O18","v":1.2},{"$f":"+BD44","v":-0.1},{"$f":"+O18","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,{"$f":"+CH38+Kontrafore!$E$8","v":24},{"$f":"IF(CH47>='Analiza i dimenzioniranje'!$E$30,0,CI$3)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB130","v":""},{"$f":"+Kontrafore!AA130","v":""},{"$f":"+AC46","v":""},{"$f":"+AD47","v":""},null,null,null,null,null,null,null,null,null,null,null,"Kot za O,5 na vrhu zida",null,null,null,null,null,{"$f":"+AV45+0.1","v":3.0000011},{"$f":"+AW47","v":1.5},{"$f":"IF('Analiza i dimenzioniranje'!E60=0,-5,+O26+0.1)","v":-5},{"$f":"+AY47","v":-0.3},null,null,{"$f":"+BB45","v":3.2000010999999997},{"$f":"+BC47","v":1.2},{"$f":"+BD45","v":-0.3},{"$f":"+BE47","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH39+Kontrafore!$E$8","v":20},{"$f":"IF(CI47=0,0,CI30)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB131","v":""},{"$f":"+Kontrafore!AA131","v":""},{"$f":"+AC48","v":""},{"$f":"+IF(AA45=\"\",\"\",O13-0.5)","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AT31+0.3","v":3.2000021999999992},{"$f":"+AR2-0.6","v":{"$error":"#VALUE!"}},"oznaka za h0",null,"k.c vert.za h0",null,"k.c .za h0 gore",null,"k.c .za h0 dole",null,"oznaka za hB",null,"kc za hA",null,"kc za hB",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH40+Kontrafore!$E$8","v":20},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB132","v":""},{"$f":"+Kontrafore!AA132","v":""},{"$f":"+AA48","v":""},{"$f":"+AD49","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AP49","v":3.2000021999999992},{"$f":"+AQ49+0.7","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",-5,+AT50-0.01)","v":-1.21},{"$f":"+AW50/2","v":0.6},{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",-5,+AZ52-0.2+0.01)","v":-1.2},-0.1,{"$f":"+AT50-0.1","v":-1.3},{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",-5,+O18)","v":1.2},{"$f":"+AV50","v":-1.3},{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",-5,+G503)","v":0},{"$f":"-0.2-0.01","v":-0.21000000000000002},{"$f":"+BE51/2","v":0.65},{"$f":"+(BB47+BB48)/2","v":3.1000010999999996},{"$f":"+BC48+0.1","v":1.3},-0.2,{"$f":"+IF('Analiza i dimenzioniranje'!A83=\"\",-0.1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH41+Kontrafore!$E$8","v":21.5},{"$f":"IF(CI49=0,0,CI32)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB133","v":""},{"$f":"+Kontrafore!AA133","v":""},{"$f":"+AA49","v":""},{"$f":"+AD45","v":""},null,null,null,null,null,null,null,null,null,null,null,"Kct za-O,5 od vrha zida",null,"oznaka 0,5",null,{"$f":"+AT50","v":-1.2},{"$f":"+O18+0.1","v":1.3},{"$f":"+AT51+0.1","v":-1.0999999999999999},{"$f":"+AW50","v":1.2},{"$f":"+AV51","v":-1.0999999999999999},0,"oznaka za h0",null,{"$f":"+BB50","v":3.1000010999999996},{"$f":"+(O18-O16-0.1)","v":0.4},{"$f":"+BD50","v":-0.2},{"$f":"+O18+0.1","v":1.3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH42+Kontrafore!$E$8","v":21.5},{"$f":"IF(CI50=0,0,CI33)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,{"$f":"+Kontrafore!AB136","v":""},{"$f":"+Kontrafore!AA136","v":""},{"$f":"+AA53","v":""},{"$f":"IF(AA52=\"\",\"\",+$O$18)","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AP49-0.1","v":3.1000021999999992},{"$f":"+O13-0.5","v":5.5},{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",-5,+AP52)","v":3.1000021999999992},{"$f":"+(AQ49+AQ50)/2","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",-5,-'Analiza i dimenzioniranje'!D83-0.01)","v":-1.01},{"$f":"+P53/2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH43+Kontrafore!$E$8","v":22.5},{"$f":"IF(CI51=0,0,CI34)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB137","v":""},{"$f":"+Kontrafore!AA137","v":""},{"$f":"+AC52","v":""},{"$f":"IF(AA52=\"\",\"\",+AD52+0.5)","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AP50+0.1","v":3.3000021999999993},{"$f":"+AQ52","v":5.5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH44+Kontrafore!$E$8","v":22.5},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB138","v":""},{"$f":"+Kontrafore!AA138","v":""},{"$f":"+AC57","v":""},{"$f":"+AD53","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH45+Kontrafore!$E$8","v":24},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB139","v":""},{"$f":"+Kontrafore!AA139","v":""},{"$f":"+AC53","v":""},{"$f":"+AD54","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH46+Kontrafore!$E$8","v":24},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB140","v":""},{"$f":"+Kontrafore!AA140","v":""},{"$f":"+AC55","v":""},{"$f":"+IF(AA52=\"\",\"\",O13-0.5)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,{"$f":"+CH47+Kontrafore!$E$8","v":28},{"$f":"IF(CH56>='Analiza i dimenzioniranje'!$E$30,0,CI$3)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB141","v":""},{"$f":"+Kontrafore!AA141","v":""},{"$f":"+AA55","v":""},{"$f":"+AD56","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH48+Kontrafore!$E$8","v":24},{"$f":"IF(CI56=0,0,CI39)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB142","v":""},{"$f":"+Kontrafore!AA142","v":""},{"$f":"+AA56","v":""},{"$f":"+AD52","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH49+Kontrafore!$E$8","v":24},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,{"$f":"+Kontrafore!AB145","v":""},{"$f":"+Kontrafore!AA145","v":""},{"$f":"+AA60","v":""},{"$f":"IF(AA59=\"\",\"\",+$O$18)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH50+Kontrafore!$E$8","v":25.5},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB146","v":""},{"$f":"+Kontrafore!AA146","v":""},{"$f":"+AC59","v":""},{"$f":"IF(AA59=\"\",\"\",+AD59+0.5)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH51+Kontrafore!$E$8","v":25.5},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB147","v":""},{"$f":"+Kontrafore!AA147","v":""},{"$f":"+AC64","v":""},{"$f":"+AD60","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH52+Kontrafore!$E$8","v":26.5},{"$f":"IF(CI60=0,0,CI43)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB148","v":""},{"$f":"+Kontrafore!AA148","v":""},{"$f":"+AC60","v":""},{"$f":"+AD61","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH53+Kontrafore!$E$8","v":26.5},{"$f":"IF(CI61=0,0,CI44)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB149","v":""},{"$f":"+Kontrafore!AA149","v":""},{"$f":"+AC62","v":""},{"$f":"+IF(AA59=\"\",\"\",O13-0.5)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH54+Kontrafore!$E$8","v":28},{"$f":"IF(CI62=0,0,CI45)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB150","v":""},{"$f":"+Kontrafore!AA150","v":""},{"$f":"+AA62","v":""},{"$f":"+AD63","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH55+Kontrafore!$E$8","v":28},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB151","v":""},{"$f":"+Kontrafore!AA151","v":""},{"$f":"+AA63","v":""},{"$f":"+AD59","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,{"$f":"+CH56+Kontrafore!$E$8","v":32},{"$f":"IF(CH65>'Analiza i dimenzioniranje'!$E$30,0,CI47)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,{"$f":"+Kontrafore!AB154","v":""},{"$f":"+Kontrafore!AA154","v":""},{"$f":"+AA67","v":""},{"$f":"IF(AA66=\"\",\"\",+$O$18)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH57+Kontrafore!$E$8","v":28},{"$f":"IF(CI65=0,0,CI48)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB155","v":""},{"$f":"+Kontrafore!AA155","v":""},{"$f":"+AC66","v":""},{"$f":"IF(AA66=\"\",\"\",+AD66+0.5)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH58+Kontrafore!$E$8","v":28},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB156","v":""},{"$f":"+Kontrafore!AA156","v":""},{"$f":"+AC71","v":""},{"$f":"+AD67","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH59+Kontrafore!$E$8","v":29.5},{"$f":"IF(CI67=0,0,CI50)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB157","v":""},{"$f":"+Kontrafore!AA157","v":""},{"$f":"+AC67","v":""},{"$f":"+AD68","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH60+Kontrafore!$E$8","v":29.5},{"$f":"IF(CI68=0,0,CI51)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB158","v":""},{"$f":"+Kontrafore!AA158","v":""},{"$f":"+AC69","v":""},{"$f":"+IF(AA66=\"\",\"\",O13-0.5)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH61+Kontrafore!$E$8","v":30.5},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB159","v":""},{"$f":"+Kontrafore!AA159","v":""},{"$f":"+AA69","v":""},{"$f":"+AD70","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH62+Kontrafore!$E$8","v":30.5},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AB160","v":""},{"$f":"+Kontrafore!AA160","v":""},{"$f":"+AA70","v":""},{"$f":"+AD66","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH63+Kontrafore!$E$8","v":32},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pogled na zid",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH64+Kontrafore!$E$8","v":32},{"$f":"IF(CI72=0,0,CI55)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,{"$f":"+CH65+Kontrafore!$E$8","v":36},{"$f":"IF(CL74>'Analiza i dimenzioniranje'!$E$30,0,CI56)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!E48","v":6},0,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH66+Kontrafore!$E$8","v":32},{"$f":"IF(CM74=0,0,CI57)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},{"$f":"+AE75","v":6},10,{"$f":"+AG75","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH67+Kontrafore!$E$8","v":32},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,0,{"$f":"+AF76","v":10},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH68+Kontrafore!$E$8","v":33.5},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Linija zida na temelju",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH69+Kontrafore!$E$8","v":33.5},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",\"\",2+'Analiza i dimenzioniranje'!E59+'Analiza i dimenzioniranje'!E55)","v":4.2000000999999996},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH70+Kontrafore!$E$8","v":34.5},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",\"\",+'Analiza i dimenzioniranje'!E49)","v":12},{"$f":"+AE79","v":4.2000000999999996},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH71+Kontrafore!$E$8","v":34.5},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CH72+Kontrafore!$E$8","v":36},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CL73+Kontrafore!$E$8","v":36},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,{"$f":"+CL74+Kontrafore!$E$8","v":40},{"$f":"IF(CL83>'Analiza i dimenzioniranje'!$E$30,0,Kontrafore!W$75)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CL75+Kontrafore!$E$8","v":36},{"$f":"IF(CM83=0,0,CI66)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CL76+Kontrafore!$E$8","v":36},{"$f":"IF(CM84=0,0,CI67)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CL77+Kontrafore!$E$8","v":37.5},{"$f":"IF(CM85=0,0,CI68)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CL78+Kontrafore!$E$8","v":37.5},{"$f":"IF(CM86=0,0,CI69)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CL79+Kontrafore!$E$8","v":38.5},{"$f":"IF(CM87=0,0,CI70)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CL80+Kontrafore!$E$8","v":38.5},{"$f":"IF(CM88=0,0,CI71)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CL81+Kontrafore!$E$8","v":40},{"$f":"IF(CD89=0,0,CI72)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+CL82+Kontrafore!$E$8","v":40},{"$f":"IF(CC90=0,0,CM73)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"0.5*+((CI2*CH3-CI3*CH2)+(CI3*CH4-CI4*CH3)+(CI4*CH5-CI5*CH4)+(CI5*CH6-CI6*CH5)+(CI6*CH7-CI7*CH6)+(CI7*CH8-CI8*CH7)+(CI8*CH9-CI9*CH8)+(CI9*CH10-CI10*CH9)+(CI10*CH11-CI11*CH10)+(CI11*CH12-CI12*CH11)+(CI12*CH13-CI13*CH12)+(CI13*CH14-CI14*CH13)+(CI14*CH15-CI15*CH14)+(CI15*CH16-CI16*CH15)+(CI16*CH17-CI17*CH16)+(CI17*CH18-CI18*CH17)+(CI18*CH19-CI19*CH18)+(CI19*CH20-CI20*CH19)+(CI20*CH21-CI21*CH20)+(CI21*CH22-CI22*CH21)+(CI22*CH23-CI23*CH22)+(CI23*CH24-CI24*CH23)+(CI24*CH25-CI25*CH24)+(CI25*CH26-CI26*CH25)+(CI26*CH27-CI27*CH26)+(CI27*CH28-CI28*CH27)+(CI28*CH29-CI29*CH28)+(CI29*CH30-CI30*CH29)+(CI30*CH31-CI31*CH30)+(CI31*CH32-CI32*CH31)+(CI32*CH33-CI33*CH32)+(CI33*CH34-CI34*CH33)+(CI34*CH35-CI35*CH34)+(CI35*CH36-CI36*CH35)+(CI36*CH37-CI37*CH36)+(CI37*CH38-CI38*CH37)+(CI38*CH39-CI39*CH38)+(CI39*CH40-CI40*CH39)+(CI40*CH41-CI41*CH40)+(CI41*CH42-CI42*CH41)+(CI42*CH43-CI43*CH42)+(CI43*CH44-CI44*CH43)+(CI44*CH45-CI45*CH44)+(CI45*CH46-CI46*CH45)+(CI46*CH47-CI47*CH46)+(CI47*CH48-CI48*CH47)+(CI48*CH49-CI49*CH48)+(CI49*CH50-CI50*CH49)+(CI50*CH51-CI51*CH50)+(CI51*CH52-CI52*CH51)+(CI52*CH53-CI53*CH52)+(CI53*CH54-CI54*CH53)+(CI54*CH55-CI55*CH54)+(CI55*CH56-CI56*CH55)+(CI56*CH57-CI57*CH56)+(CI57*CH58-CI58*CH57)+(CI58*CH59-CI59*CH58)+(CI59*CH60-CI60*CH59)+(CI60*CH61-CI61*CH60)+(CI61*CH62-CI62*CH61)+(CI62*CH63-CI63*CH62)+(CI63*CH64-CI64*CH63)+(CI64*CH65-CI65*CH64)+(CI65*CH66-CI66*CH65)+(CI66*CH67-CI67*CH66)+(CI67*CH68-CI68*CH67)+(CI68*CH69-CI69*CH68)+(CI69*CH70-CI70*CH69)+(CI70*CH71-CI71*CH70)+(CI71*CH72-CI72*CH71)+(CI72*CL73-CM73*CH72)+(CM73*CL74-CM74*CL73)+(CM74*CL75-CM75*CL74)+(CM75*CL76-CM76*CL75)+(CM76*CL77-CM77*CL76)+(CM77*CL78-CM78*CL77)+(CM78*CL79-CM79*CL78)+(CM79*CL80-CM80*CL79)+(CM80*CL81-CM81*CL80)+(CM81*CL82-CM82*CL81)+(CM82*CL83-CM83*CL82)+(CM83*CL84-CM84*CL83)+(CM84*CL85-CM85*CL84)+(CM85*CL86-CM86*CL85)+(CM86*CL87-CM87*CL86)+(CM87*CL88-CM88*CL87)+(CM88*CC89-CD89*CL88)+(CD89*CB90-CC90*CC89)+(CC90*CL91-CM91*CB90))","v":28}]
[null,null,null,"Preporuča se da, zbog konstruktivnih i estetskih razloga, sidra svih redova budu u istim vertikalama. To se postiže povećanjem ili smanjenjem nosivosti sidara, povećavanjem ili smanjivanjem sidrišne dionice, prilikom unosa podataka o sidrima, u Formi 4, kao ovdje u programu."]
[0,0,0,{"$f":"+D96","v":12},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!E49*0.8","v":9.6000000000000014},{"$f":"+'Analiza i dimenzioniranje'!E48","v":6}]
[0,{"$f":"+D97","v":6},0,0,null,"red 1. ",null,"red 2.",null,"red 3.",null,"red 4.",null,null,null,null,null,null,null,null,null,{"$f":"0.8*'Analiza i dimenzioniranje'!E49","v":9.6000000000000014},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2}]
[0,{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},{"$f":"+B96","v":12},{"$f":"+C96","v":12},null,"položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra",null,null,null,null,null,null,null,null,{"$f":"+V95","v":9.6000000000000014},{"$f":"0","v":0}]
[{"$f":"+W95","v":1.2},{"$f":"+A97","v":1.2},{"$f":"+A96","v":0},{"$f":"+'Analiza i dimenzioniranje'!E48","v":6},"vertikala","I.red",null,"II.red",null,"III.red",null,"IV.red"]
[null,null,null,null,1,{"$f":"+B111","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!D71","v":5},{"$f":"+B112","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E71","v":3},{"$f":"+B113","v":-1},{"$f":"+'Analiza i dimenzioniranje'!F71","v":""},{"$f":"+B114","v":-1},{"$f":"+'Analiza i dimenzioniranje'!G71","v":""},{"$f":"+'Analiza i dimenzioniranje'!E49","v":12}]
[null,null,null,null,2,{"$f":"+D111","v":{"$error":"#VALUE!"}},{"$f":"+G98","v":5},{"$f":"+D112","v":{"$error":"#VALUE!"}},{"$f":"+I98","v":3},{"$f":"+D113","v":-1},{"$f":"+K98","v":""},{"$f":"IF(A114=\"\",-1,+D114)","v":-1},{"$f":"+M98","v":""},{"$f":"+N98","v":12}]
[null,null,null,null,3,{"$f":"IF(+F111>A110,\"\",F111)","v":{"$error":"#VALUE!"}},{"$f":"+G99","v":5},{"$f":"+F112","v":{"$error":"#VALUE!"}},{"$f":"+I99","v":3},{"$f":"+F$113","v":-1},{"$f":"+K99","v":""},{"$f":"IF(A110=\"\",-1,+F114)","v":-1},{"$f":"+M99","v":""},{"$f":"+N99","v":12}]
[null,null,null,null,4,{"$f":"IF($A$110>+H111,H111,\"\")","v":{"$error":"#VALUE!"}},5,{"$f":"IF($A$110>+H112,H112,\"\")","v":{"$error":"#VALUE!"}},3,{"$f":"IF($A$110>+H113,H113,\"\")","v":-1},"",{"$f":"IF(A110>+H114,H114,-1)","v":-1},"",{"$f":"+N100","v":12}]
[null,null,null,null,5,{"$f":"IF($A$110>+J111,J111,-1)","v":{"$error":"#VALUE!"}},5,{"$f":"IF($A$110>+J112,J112,-1)","v":{"$error":"#VALUE!"}},3,{"$f":"IF(+J113>$A$110,-1,J113)","v":-1},"",{"$f":"IF(A110>J114,J114,-1)","v":-1},"",12,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AA70","v":4.2000000999999996},{"$f":"+Kontrafore!AB70","v":0}]
[null,null,null,null,6,{"$f":"IF(A110>+L111,L111,-1)","v":{"$error":"#VALUE!"}},5,{"$f":"IF($A$110>+L$112,L112,-1)","v":{"$error":"#VALUE!"}},3,{"$f":"IF(+L113>$A$110,-1,L113)","v":-1},"",{"$f":"IF($A$110>L$114,L$114,-1)","v":-1},"",12,null,null,null,null,null,null,null,{"$f":"+Kontrafore!AA71","v":4.2000000999999996},{"$f":"+Kontrafore!AB71","v":12}]
[null,null,null,null,7,{"$f":"IF(A110>+N111,N111,-1)","v":{"$error":"#VALUE!"}},5,{"$f":"IF(A110>N$112,N112,-1)","v":{"$error":"#VALUE!"}},3,{"$f":"IF(+N113>$A$110,-1,N113)","v":-1},"",{"$f":"IF($A$110>N$114,N$114,-1)","v":-1},"",12]
[null,null,null,null,8,{"$f":"IF(A110>+P111,P111,-1)","v":{"$error":"#VALUE!"}},5,{"$f":"IF(A110>P$112,P112,-1)","v":{"$error":"#VALUE!"}},3,{"$f":"IF(A110>P113,P113,-1)","v":-1},"",{"$f":"IF($A$110>P114,P114,-1)","v":-1},"",12]
[null,null,null,null,9,{"$f":"IF($A$110>+R111,R111,-1)","v":{"$error":"#VALUE!"}},5,{"$f":"IF(A110>R$112,R112,-1)","v":{"$error":"#VALUE!"}},3,{"$f":"IF(A110>R113,R113,-1)","v":-1},"",{"$f":"IF($A$110>R114,R114,-1)","v":-1},"",12]
[null,null,null,null,10,{"$f":"IF($A$110>+T111,T111,-1)","v":{"$error":"#VALUE!"}},{"$f":"+G106","v":5},{"$f":"IF(A110>T112,T112,-1)","v":{"$error":"#VALUE!"}},{"$f":"+I106","v":3},{"$f":"IF(A110>T113,T113,-1)","v":-1},{"$f":"+K106","v":""},{"$f":"IF($A$110>T113,T113,-1)","v":-1},"",{"$f":"+N106","v":12}]
[null,null,null,null,11,{"$f":"IF($A$110>+T112,T112,-1)","v":{"$error":"#VALUE!"}},{"$f":"+G107","v":5},{"$f":"+F108","v":{"$error":"#VALUE!"}},{"$f":"+I107","v":3},{"$f":"IF(A111>T114,T114,-1)","v":-1},{"$f":"+K107","v":""},{"$f":"IF($A$110>T114,T114,-1)","v":-1},"",{"$f":"+N107","v":12}]
["duljina zida (m)","vertikala 1",null,"razmaci sidara",null,{"$f":"+'Iskaz armature'!V54-1","v":{"$error":"#VALUE!"}},"kom","vertikala 4",null,"vertikala 5",null,"vertikala 6",null,"vertikala 7",null,"vertikala 8",null,"vertikala 9",null,"vertikala 10"]
[{"$f":"+'Analiza i dimenzioniranje'!$E$49","v":12},"položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra",null,null,null,"visina sidra"]
[{"$f":"+IF('Analiza i dimenzioniranje'!D70=\"\",\"\",\"I. Red\")","v":"I. Red"},{"$f":"+IF(A111=\"\",-1,('Analiza i dimenzioniranje'!E49-'Poprečni presjek zida'!F109*'Analiza i dimenzioniranje'!D76)/2)","v":{"$error":"#VALUE!"}},{"$f":"IF(A111=\"\",-1,+'Analiza i dimenzioniranje'!D71)","v":5},{"$f":"IF(B111=-1,-1,+B111+'Analiza i dimenzioniranje'!D$76)","v":{"$error":"#VALUE!"}},{"$f":"+C111","v":5},{"$f":"IF(D111=-1,-1,+D111+'Analiza i dimenzioniranje'!D76)","v":{"$error":"#VALUE!"}},{"$f":"+E111","v":5},{"$f":"IF(F111=-1,-1,+F111+'Analiza i dimenzioniranje'!D$76)","v":{"$error":"#VALUE!"}},{"$f":"+G111","v":5},{"$f":"IF(H111=-1,-1,+H111+'Analiza i dimenzioniranje'!D$76)","v":{"$error":"#VALUE!"}},{"$f":"IF(J111=\"\",\"\",+I111)","v":{"$error":"#VALUE!"}},{"$f":"IF(J111=-1,-1,+J111+'Analiza i dimenzioniranje'!D$76)","v":{"$error":"#VALUE!"}},{"$f":"IF(L111=\"\",\"\",+K111)","v":{"$error":"#VALUE!"}},{"$f":"IF(L111=-1,-1,+L111+'Analiza i dimenzioniranje'!D$76)","v":{"$error":"#VALUE!"}},{"$f":"IF(N111=\"\",\"\",+M111)","v":{"$error":"#VALUE!"}},{"$f":"+IF(N111=-1,-1,N111+'Analiza i dimenzioniranje'!D76)","v":{"$error":"#VALUE!"}},{"$f":"IF(P111=\"\",\"\",+O111)","v":{"$error":"#VALUE!"}},{"$f":"+IF(P111=-1,-1,P111+'Analiza i dimenzioniranje'!D$76)","v":{"$error":"#VALUE!"}},{"$f":"IF(R111=\"\",\"\",+Q111)","v":{"$error":"#VALUE!"}},{"$f":"IF(R111=-1,-1,R111+'Analiza i dimenzioniranje'!D$76)","v":{"$error":"#VALUE!"}},{"$f":"IF(T111=\"\",\"\",+S111)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"IF(W111=\"\",\"\",+V111)","v":""}]
[{"$f":"+IF('Analiza i dimenzioniranje'!E70=\"\",\"\",\"II. Red\")","v":"II. Red"},{"$f":"+IF($A$112=\"\",-1,B111)","v":{"$error":"#VALUE!"}},{"$f":"IF(A112=\"\",-1,+'Analiza i dimenzioniranje'!E71)","v":3},{"$f":"+IF($A$112=\"\",-1,B112+'Analiza i dimenzioniranje'!$E$76)","v":{"$error":"#VALUE!"}},{"$f":"+C112","v":3},{"$f":"+IF($A$112=\"\",-1,D112+'Analiza i dimenzioniranje'!$E$76)","v":{"$error":"#VALUE!"}},{"$f":"+E112","v":3},{"$f":"+IF($A$112=\"\",-1,F112+'Analiza i dimenzioniranje'!$E$76)","v":{"$error":"#VALUE!"}},{"$f":"+G112","v":3},{"$f":"+IF($A$112=\"\",-1,H112+'Analiza i dimenzioniranje'!$E$76)","v":{"$error":"#VALUE!"}},{"$f":"IF(J112=\"\",\"\",+I112)","v":{"$error":"#VALUE!"}},{"$f":"+IF($A$112=\"\",-1,J112+'Analiza i dimenzioniranje'!$E$76)","v":{"$error":"#VALUE!"}},{"$f":"IF(L112=\"\",\"\",+K112)","v":{"$error":"#VALUE!"}},{"$f":"+IF($A$112=\"\",-1,L112+'Analiza i dimenzioniranje'!$E$76)","v":{"$error":"#VALUE!"}},{"$f":"+M112","v":{"$error":"#VALUE!"}},{"$f":"+IF($A$112=\"\",-1,N112+'Analiza i dimenzioniranje'!$E$76)","v":{"$error":"#VALUE!"}},{"$f":"+O112","v":{"$error":"#VALUE!"}},{"$f":"+IF($A$112=\"\",-1,P112+'Analiza i dimenzioniranje'!$E$76)","v":{"$error":"#VALUE!"}},{"$f":"+Q112","v":{"$error":"#VALUE!"}},{"$f":"+IF($A$112=\"\",-1,R112+'Analiza i dimenzioniranje'!$E$76)","v":{"$error":"#VALUE!"}},{"$f":"+S112","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"IF(W112=\"\",\"\",+V112)","v":""}]
[{"$f":"+IF('Analiza i dimenzioniranje'!F70=\"\",\"\",\"III. Red\")","v":""},{"$f":"+IF(A113=\"\",-1,B111)","v":-1},{"$f":"IF(A113=\"\",-1,+'Analiza i dimenzioniranje'!F71)","v":-1},{"$f":"IF($A$113=\"\",-1,+B113+'Analiza i dimenzioniranje'!$F$76)","v":-1},{"$f":"+C113","v":-1},{"$f":"IF($A$113=\"\",-1,+D113+'Analiza i dimenzioniranje'!$F$76)","v":-1},{"$f":"+E113","v":-1},{"$f":"IF($A$113=\"\",-1,+F113+'Analiza i dimenzioniranje'!$F$76)","v":-1},{"$f":"+G113","v":-1},{"$f":"IF($A$113=\"\",-1,+H113+'Analiza i dimenzioniranje'!$F$76)","v":-1},{"$f":"+I113","v":-1},{"$f":"IF($A$113=\"\",-1,+J113+'Analiza i dimenzioniranje'!$F$76)","v":-1},{"$f":"IF(L113=\"\",\"\",+K113)","v":-1},{"$f":"IF($A$113=\"\",-1,+L113+'Analiza i dimenzioniranje'!$F$76)","v":-1},{"$f":"+M113","v":-1},{"$f":"IF($A$113=\"\",-1,+N113+'Analiza i dimenzioniranje'!$F$76)","v":-1},{"$f":"+O113","v":-1},{"$f":"IF($A$113=\"\",-1,+P113+'Analiza i dimenzioniranje'!$F$76)","v":-1},{"$f":"+Q113","v":-1},{"$f":"IF($A$113=\"\",-1,+R113+'Analiza i dimenzioniranje'!$F$76)","v":-1},{"$f":"+S113","v":-1},null,null,null,{"$f":"+V113","v":0}]
[{"$f":"+IF('Analiza i dimenzioniranje'!G70=\"\",\"\",\"IV. Red\")","v":""},{"$f":"+IF(A114=\"\",-1,B111)","v":-1},{"$f":"IF(A114=\"\",-1,+'Analiza i dimenzioniranje'!G71)","v":-1},{"$f":"IF($A$114=\"\",-1,+B114+'Analiza i dimenzioniranje'!$G$76)","v":-1},{"$f":"+C114","v":-1},{"$f":"IF($A$114=\"\",-1,+D114+'Analiza i dimenzioniranje'!$G$76)","v":-1},{"$f":"+E114","v":-1},{"$f":"IF($A$114=\"\",-1,+F114+'Analiza i dimenzioniranje'!$G$76)","v":-1},{"$f":"+G114","v":-1},{"$f":"IF($A$114=\"\",-1,IF(+H114+'Analiza i dimenzioniranje'!$G$76>$A$110,-1,H114+'Analiza i dimenzioniranje'!$G$76))","v":-1},{"$f":"+I114","v":-1},{"$f":"IF($A$114=\"\",-1,IF(+J114=-1,-1,J114+'Analiza i dimenzioniranje'!$G$76))","v":-1},{"$f":"IF(L114=\"\",\"\",+K114)","v":-1},{"$f":"IF($A$114=\"\",-1,IF(+L114=-1,-1,L114+'Analiza i dimenzioniranje'!$G$76))","v":-1},{"$f":"+M114","v":-1},{"$f":"IF($A$114=\"\",-1,IF(+N114=-1,-1,N114+'Analiza i dimenzioniranje'!$G$76))","v":-1},{"$f":"+O114","v":-1},{"$f":"IF($A$114=\"\",-1,IF(+P114=-1,-1,P114+'Analiza i dimenzioniranje'!$G$76))","v":-1},{"$f":"+Q114","v":-1},{"$f":"IF(A114=\"\",-1,R114+'Analiza i dimenzioniranje'!G76)","v":-1},{"$f":"+S114","v":-1},null,null,null,{"$f":"+V114","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+V115","v":0}]
[]
["Duljina zida (m)","Koordinate procjednica (barbakane) razmak procjecnica",null,null,null,null,null,null,null,"d=",{"$f":"+'Tlocrt temelja i pogled na zid'!$M$27","v":2},"m","Razmak procjednica (barbakana) upisati u čeliju K86"]
[{"$f":"+'Analiza i dimenzioniranje'!$E$49","v":12},"položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra","položaj od ruba zida","visina sidra","položaj od ruba zida",null,"vertikala 7",null,"vertikala 8",null,"vertikala 9",null,null,null,null,"vertikala 10"]
[{"$f":"+'Tlocrt temelja i pogled na zid'!$C$28","v":1},{"$f":"+K117/2","v":1},{"$f":"+B119+$K$117","v":3},{"$f":"+C119+$K$117","v":5},{"$f":"IF(D119+$K$117>A118,-1,D119+$K$117)","v":7},{"$f":"IF(E119=-1,-1,IF(E119+$K$117>$A$118,-1,E119+$K$117))","v":9},11,-1,-1,-1,-1,{"$f":"IF(K119=-1,-1,IF(K119+$K$117>$A$118,-1,K119+$K$117))","v":-1},null,null,null,null,null,null,null,null,null,"visina sidra","položaj od ruba zida",null,"visina sidra"]
[{"$f":"+B120","v":1.5},{"$f":"+'Analiza i dimenzioniranje'!E52+0.3","v":1.5},{"$f":"+B120","v":1.5},1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,{"$f":"+K120","v":1.5}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"POVRŠINA TEMELJA"]
[null,null,"kontraf","x","y"]
[null,null,1,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,+CH3)","v":0},{"$f":"+CI3","v":4.9000021999999994}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,+CH4)","v":0},2]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,CH5)","v":1.5},2]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,CH6)","v":1.5},1]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,IF('Analiza i dimenzioniranje'!D83=\"\",0,CH7))","v":2.5},1]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,CH8)","v":2.5},2]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,CH9)","v":4},2]
[null,null,2,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,+CH13)","v":4},{"$f":"+CI13","v":2}]
[null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!D83=\"\",0,CH14)","v":5.5},2]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,CH15)","v":5.5},1]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,CH16)","v":6.5},1]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,CH17)","v":6.5},2]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,CH18)","v":8},2]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,+IF('Analiza i dimenzioniranje'!D83=\"\",0,IF(D150<'Analiza i dimenzioniranje'!$E$49,D150,'Analiza i dimenzioniranje'!$E$49)))","v":8},{"$f":"+IF(D151='Analiza i dimenzioniranje'!$E$49,'Poprečni presjek zida'!$E$138,'Poprečni presjek zida'!E150)","v":2}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,IF(D151='Analiza i dimenzioniranje'!$E$49,0,'Poprečni presjek zida'!D151))","v":8},{"$f":"+IF(D152=0,$E$138,E150)","v":2}]
[null,null,3,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,IF(D150='Analiza i dimenzioniranje'!E49,0,+D145+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85))","v":8},{"$f":"IF(D152=0,0,E152)","v":2}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,D146+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":9.5},{"$f":"IF(E153=0,0,E146)","v":2}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,D147+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":9.5},{"$f":"IF(E154=0,0,+E147)","v":1}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,+D148+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":10.5},{"$f":"IF(E155=0,0,+E148)","v":1}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,D149+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":10.5},{"$f":"IF(E156=0,0,E149)","v":2}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,D150+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":12},{"$f":"IF(E157=0,0,E150)","v":2}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,+IF(D158<'Analiza i dimenzioniranje'!$E$49,D158,'Analiza i dimenzioniranje'!$E$49))","v":12},{"$f":"+IF(D159='Analiza i dimenzioniranje'!$E$49,'Poprečni presjek zida'!$E$138,'Poprečni presjek zida'!E158)","v":4.9000021999999994}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,IF(D159='Analiza i dimenzioniranje'!$E$49,0,'Poprečni presjek zida'!D159))","v":0},{"$f":"+IF(D160=0,$E$138,E158)","v":4.9000021999999994}]
[null,null,4,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,IF(E161=0,0,+D153+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85))","v":0},{"$f":"IF(D160=0,0,E160)","v":0}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,IF(D161=0,0,D154+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85))","v":0},{"$f":"IF(E161=0,0,E154)","v":0}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,IF(D162=0,0,D155+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85))","v":0},{"$f":"IF(E162=0,0,+E155)","v":0}]
[null,null,null,{"$f":"IF(D163=0,0,D156+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E163=0,0,+E156)","v":0}]
[null,null,null,{"$f":"IF(D164=0,0,D157+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E164=0,0,E157)","v":0}]
[null,null,null,{"$f":"IF(D165=0,0,D158+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E165=0,0,E158)","v":0}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,+IF(D166<'Analiza i dimenzioniranje'!$E$49,D166,'Analiza i dimenzioniranje'!$E$49))","v":0},{"$f":"+IF(D167='Analiza i dimenzioniranje'!$E$49,'Poprečni presjek zida'!$E$138,'Poprečni presjek zida'!E166)","v":0}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,+IF(D167='Analiza i dimenzioniranje'!E49,0,'Poprečni presjek zida'!D167))","v":0},{"$f":"+IF(D168=0,$E$138,E167)","v":4.9000021999999994}]
[null,null,5,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,IF(E169=0,0,+D161+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85))","v":0},{"$f":"IF(D168=0,0,E168)","v":0}]
[null,null,null,{"$f":"IF(D169=0,0,+D162+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E169=0,0,E162)","v":0}]
[null,null,null,{"$f":"IF(D170=0,0,+D163+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E170=0,0,+E163)","v":0}]
[null,null,null,{"$f":"IF(D171=0,0,D164+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E171=0,0,+E164)","v":0}]
[null,null,null,{"$f":"IF(D172=0,0,D165+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E172=0,0,E165)","v":0}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,IF(E174=0,0,D166+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85))","v":0},{"$f":"IF(E173=0,0,E166)","v":0}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,+IF(D174<'Analiza i dimenzioniranje'!$E$49,D174,'Analiza i dimenzioniranje'!$E$49))","v":0},{"$f":"+IF(D175='Analiza i dimenzioniranje'!$E$49,'Poprečni presjek zida'!$E$138,'Poprečni presjek zida'!E174)","v":0}]
[null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,+IF(D175='Analiza i dimenzioniranje'!$E$49,0,'Poprečni presjek zida'!D175))","v":0},{"$f":"+IF(D176=0,$E$138,E175)","v":4.9000021999999994}]
[null,null,6,{"$f":"IF(E177=0,0,+D169+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(D176=0,0,E176)","v":0}]
[null,null,null,{"$f":"IF(D177=0,0,+D170+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E177=0,0,E170)","v":0}]
[null,null,null,{"$f":"IF(D178=0,0,+D171+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E178=0,0,+E171)","v":0}]
[null,null,null,{"$f":"IF(D179=0,0,D172+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E179=0,0,+E172)","v":0}]
[null,null,null,{"$f":"IF(D180=0,0,D173+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E180=0,0,E173)","v":0}]
[null,null,null,{"$f":"IF(E182=0,0,D174+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E181=0,0,E174)","v":0}]
[null,null,null,{"$f":"+IF(D182<'Analiza i dimenzioniranje'!$E$49,D182,'Analiza i dimenzioniranje'!$E$49)","v":0},{"$f":"+IF(D183='Analiza i dimenzioniranje'!$E$49,'Poprečni presjek zida'!$E$138,'Poprečni presjek zida'!E182)","v":0}]
[null,null,null,{"$f":"+IF(D183='Analiza i dimenzioniranje'!$E$49,0,'Poprečni presjek zida'!D183)","v":0},{"$f":"+IF(D184=0,$E$138,E183)","v":4.9000021999999994}]
[null,null,7,{"$f":"IF(E185=0,0,+D177+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(D184=0,0,E184)","v":0}]
[null,null,null,{"$f":"IF(D185=0,0,+D178+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E185=0,0,E178)","v":0}]
[null,null,null,{"$f":"IF(D186=0,0,+D179+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E186=0,0,+E179)","v":0}]
[null,null,null,{"$f":"IF(D187=0,0,D180+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E187=0,0,+E180)","v":0}]
[null,null,null,{"$f":"IF(D188=0,0,D181+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E188=0,0,E181)","v":0}]
[null,null,null,{"$f":"IF(E190=0,0,D182+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E189=0,0,E182)","v":0}]
[null,null,null,{"$f":"+IF(D190<'Analiza i dimenzioniranje'!$E$49,D190,'Analiza i dimenzioniranje'!$E$49)","v":0},{"$f":"+IF(D191='Analiza i dimenzioniranje'!$E$49,'Poprečni presjek zida'!$E$138,'Poprečni presjek zida'!E190)","v":0}]
[null,null,null,{"$f":"+IF(D191='Analiza i dimenzioniranje'!$E$49,0,'Poprečni presjek zida'!D191)","v":0},{"$f":"+IF(D192=0,$E$138,E191)","v":4.9000021999999994}]
[null,null,8,{"$f":"IF(E193=0,0,+D185+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(D192=0,0,E192)","v":0}]
[null,null,null,{"$f":"IF(D193=0,0,+D186+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E193=0,0,E186)","v":0}]
[null,null,null,{"$f":"IF(D194=0,0,+D187+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E194=0,0,+E187)","v":0}]
[null,null,null,{"$f":"IF(D195=0,0,D188+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E195=0,0,+E188)","v":0}]
[null,null,null,{"$f":"IF(D196=0,0,D189+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E196=0,0,E189)","v":0}]
[null,null,null,{"$f":"IF(E198=0,0,D190+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E197=0,0,E190)","v":0}]
[null,null,null,{"$f":"+IF(D198<'Analiza i dimenzioniranje'!$E$49,D198,'Analiza i dimenzioniranje'!$E$49)","v":0},{"$f":"+IF(D199='Analiza i dimenzioniranje'!$E$49,'Poprečni presjek zida'!$E$138,'Poprečni presjek zida'!E198)","v":0}]
[null,null,null,{"$f":"+IF(D199='Analiza i dimenzioniranje'!$E$49,0,'Poprečni presjek zida'!D199)","v":0},{"$f":"+IF(D200=0,$E$138,E199)","v":4.9000021999999994}]
[null,null,9,{"$f":"IF(E201=0,0,+D193+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(D200=0,0,E200)","v":0}]
[null,null,null,{"$f":"IF(D201=0,0,+D194+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E201=0,0,E194)","v":0}]
[null,null,null,{"$f":"IF(D202=0,0,+D195+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E202=0,0,+E195)","v":0}]
[null,null,null,{"$f":"IF(D203=0,0,D196+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E203=0,0,+E196)","v":0}]
[null,null,null,{"$f":"IF(D204=0,0,D197+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E204=0,0,E197)","v":0}]
[null,null,null,{"$f":"IF(E206=0,0,D198+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E205=0,0,E198)","v":0}]
[null,null,null,{"$f":"+IF(D206<'Analiza i dimenzioniranje'!$E$49,D206,'Analiza i dimenzioniranje'!$E$49)","v":0},{"$f":"+IF(D207='Analiza i dimenzioniranje'!$E$49,'Poprečni presjek zida'!$E$138,'Poprečni presjek zida'!E206)","v":0}]
[null,null,null,{"$f":"+IF(D207='Analiza i dimenzioniranje'!$E$49,0,'Poprečni presjek zida'!D207)","v":0},{"$f":"+IF(D208=0,$E$138,E207)","v":4.9000021999999994}]
[null,null,10,{"$f":"IF(E209=0,0,+D201+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(D208=0,0,E208)","v":0}]
[null,null,null,{"$f":"IF(D209=0,0,+D202+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E209=0,0,E202)","v":0}]
[null,null,null,{"$f":"IF(D210=0,0,+D203+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E210=0,0,+E203)","v":0}]
[null,null,null,{"$f":"IF(D211=0,0,D204+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E211=0,0,+E204)","v":0}]
[null,null,null,{"$f":"IF(D212=0,0,D205+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E212=0,0,E205)","v":0}]
[null,null,null,{"$f":"IF(E214=0,0,D206+'Analiza i dimenzioniranje'!$E$49/'Analiza i dimenzioniranje'!$D$85)","v":0},{"$f":"IF(E213=0,0,E206)","v":0}]
[null,null,null,{"$f":"+IF(D214<'Analiza i dimenzioniranje'!$E$49,D214,'Analiza i dimenzioniranje'!$E$49)","v":0},{"$f":"+IF(D215='Analiza i dimenzioniranje'!$E$49,'Poprečni presjek zida'!$E$138,'Poprečni presjek zida'!E214)","v":0}]
[null,null,null,{"$f":"+IF(D215='Analiza i dimenzioniranje'!$E$49,0,'Poprečni presjek zida'!D215)","v":0},{"$f":"+IF(D216=0,$E$138,E215)","v":4.9000021999999994}]
[null,null,null,{"$f":"0.5*+((E138*D139-E139*D138)+(E139*D140-E140*D139)+(E140*D141-E141*D140)+(E141*D142-E142*D141)+(E142*D143-E143*D142)+(E143*D144-E144*D143)+(E144*D145-E145*D144)+(E145*D146-E146*D145)+(E146*D147-E147*D146)+(E147*D148-E148*D147)+(E148*D149-E149*D148)+(E149*D150-E150*D149)+(E150*D153-E153*D150)+(E153*D154-E154*D153)+(E154*D155-E155*D154)+(E155*D156-E156*D155)+(E156*D157-E157*D156)+(E157*D158-E158*D157)+(E158*D159-E159*D158)+(E159*D160-E160*D159)+(E160*D161-E161*D160)+(E161*D162-E162*D161)+(E162*D163-E163*D162)+(E163*D164-E164*D163)+(E164*D165-E165*D164)+(E165*D166-E166*D165)+(E166*D167-E167*D166)+(E167*D168-E168*D167)+(E168*D169-E169*D168)+(E169*D170-E170*D169)+(E170*D171-E171*D170)+(E171*D172-E172*D171)+(E172*D173-E173*D172)+(E173*D174-E174*D173)+(E174*D175-E175*D174)+(E175*D176-E176*D175)+(E176*D177-E177*D176)+(E177*D178-E178*D177)+(E178*D179-E179*D178)+(E179*D180-E180*D179)+(E180*D181-E181*D180)+(E181*D182-E182*D181)+(E182*D183-E183*D182)+(E183*D184-E184*D183)+(E184*D185-E185*D184)+(E185*D186-E186*D185)+(E186*D187-E187*D186)+(E187*D188-E188*D187)+(E188*D189-E189*D188)+(E189*D190-E190*D189)+(E190*D191-E191*D190)+(E191*D192-E192*D191)+(E192*D193-E193*D192)+(E193*D194-E194*D193)+(E194*D195-E195*D194)+(E195*D196-E196*D195)+(E196*D197-E197*D196)+(E197*D198-E198*D197)+(E198*D199-E199*D198)+(E199*D200-E200*D199)+(E200*D201-E201*D200)+(E201*D202-E202*D201)+(E202*D203-E203*D202)+(E203*D204-E204*D203)+(E204*D205-E205*D204)+(E205*D206-E206*D205)+(E206*D207-E207*D206)+(E207*D208-E208*D207)+(E208*D209-E209*D208)+(E209*D210-E210*D209)+(E210*D211-E211*D210)+(E211*D212-E212*D211)+(E212*D213-E213*D212)+(E213*D214-E214*D213)+(E214*D215-E215*D214)+(E215*D216-E216*D215))","v":-37.800026399999993}]

{"sheet":"Tlocrt temelja i pogled na zid","index":9,"n_rows":28,"n_cols":21,"rows_kept":28,"cut":false,"hidden":false,"merged":[[3,9,3,10],[24,0,25,16],[26,4,26,10]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!A82=\"\",0,\"\")","v":""},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+T1","v":""},{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",'Analiza i dimenzioniranje'!E60+'Analiza i dimenzioniranje'!E61,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",+'Analiza i dimenzioniranje'!E49,\"\")","v":""},{"$f":"+U2","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+T3","v":""},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+T3","v":""},{"$f":"+'Analiza i dimenzioniranje'!E60","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+T1","v":""},{"$f":"+U5","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+IF('Analiza i dimenzioniranje'!D83>0,0,2)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},{"$f":"+T8","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+S9","v":12},{"$f":"IF('Analiza i dimenzioniranje'!D83>0,0,+T9+'Analiza i dimenzioniranje'!E59)","v":0},{"$f":"+'Analiza i dimenzioniranje'!E48","v":6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+T10","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+T11+'Analiza i dimenzioniranje'!E55","v":0.8}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+S9","v":12},{"$f":"+T13","v":0.8}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+S8","v":0},{"$f":"+T8","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+R18-1.5","v":9.1999999999999993},{"$f":"+'Analiza i dimenzioniranje'!E48+0.1","v":6.1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+R18-0.5","v":10.199999999999999},{"$f":"+S18-0.1","v":6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!E49-1.3","v":10.7},{"$f":"+'Analiza i dimenzioniranje'!E48+0.1","v":6.1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+R16","v":9.1999999999999993},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.199999999999999,{"$f":"+S19","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.7,{"$f":"+S20","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9.1999999999999993,{"$f":"0+0.1","v":0.1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.199999999999999,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.7,{"$f":"+S22","v":0.1}]
["Preporuča se da, zbog konstruktivnih i estetskih razloga, sidra svih redova budu u istim vertikalama (kao na crtežu, napr. na razmaku od 2,0 m). To se postiže povećanjem ili smanjenjem nosivosti sidara (povećavanjem ili smanjivanjem sidrišne dionice), u Formi 4, kao u originalu u programu.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.2,{"$f":"ROUNDUP('Analiza i dimenzioniranje'!E48,)-0.5","v":5.5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!E49-0.2","v":11.8},0.2]
[{"$f":"ROUNDDOWN(+'Analiza i dimenzioniranje'!E49/'Poprečni presjek zida'!K117,0)","v":6},null,"razmaka između procjednica",null,"Razmak procjednica (barbakana) upisati u čeliju M27",null,null,null,null,null,null,"d=",2,"m",null,null,null,{"$f":"+'Analiza i dimenzioniranje'!E49/2","v":6},{"$f":"+'Analiza i dimenzioniranje'!E48+0.2","v":6.2}]
[null,"Koord. 1 procj. x",{"$f":"IF(+('Analiza i dimenzioniranje'!E49-'Tlocrt temelja i pogled na zid'!A27*'Tlocrt temelja i pogled na zid'!M27)/2=0,M27/2,('Analiza i dimenzioniranje'!E49-'Tlocrt temelja i pogled na zid'!A27*'Tlocrt temelja i pogled na zid'!M27)/2)","v":1},"m","Napomena: Crtanje sidara i procjednica predviđeno je za zidove dužine do 20 m. "]

{"sheet":"Dijagram momenata","index":10,"n_rows":33,"n_cols":22,"rows_kept":33,"cut":false,"hidden":true,"merged":[[2,15,3,15],[2,16,3,16],[2,17,3,17],[2,18,3,18],[0,0,0,4],[0,15,0,18]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Momenti savijanja"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek i oznaka momenta savijanja","Visina   presjeka \n\n (m)"," Moment savijanja    MEd             (kNm/m')","Računski moment savijanja MEds         (kNm/m')   "]
[null,null,null,null,null,null,null,null,null,0,9,null,null,null,null,null,null,null,null,"Presjek"]
[28.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Q5=$Q$21,\"Mmin\",IF(Q5=$Q$22,\"Mmax\",\"XX-XX\"))","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!F9>0,+'Unos podataka'!$T$55-'Unos podataka'!F9,'Unos podataka'!T55)","v":6},0,{"$f":"+'Analiza i dimenzioniranje'!AK$52","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Q6=$Q$21,\"Mmin\",IF(Q6=$Q$22,\"Mmax\",\"XIX-XIX\"))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U66","v":5.6800000000000006},{"$f":"+'Analiza i dimenzioniranje'!AI$47","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AI$50","v":{"$error":"#VALUE!"}},null,0,{"$f":"+'C III-V'!C9","v":"A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Q7=$Q$21,\"Mmin\",IF(Q7=$Q$22,\"Mmax\",\"XVIII-XVIII\"))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U65","v":5.36},{"$f":"+'Analiza i dimenzioniranje'!AH$47","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AH$50","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,"00:00:00",null,null,{"$f":"+IF(Q8=$Q$21,\"Mmin\",IF(Q8=$Q$22,\"Mmax\",\"XVII-XVII\"))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U64","v":5.04},{"$f":"+'Analiza i dimenzioniranje'!AG$47","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AG$50","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Q9=$Q$21,\"Mmin\",IF(Q9=$Q$22,\"Mmax\",\"XVI-XVI\"))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U63","v":4.72},{"$f":"+'Analiza i dimenzioniranje'!AF$47","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AF$50","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Q10=$Q$21,\"Mmin\",IF(Q10=$Q$22,\"Mmax\",\"XV-XV\"))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U62","v":4.4000000000000004},{"$f":"+'Analiza i dimenzioniranje'!AE$47","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE$50","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Q11=$Q$21,\"Mmin\",IF(Q11=$Q$22,\"Mmax\",\"XIV-XIV\"))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U61","v":4.08},{"$f":"+'Analiza i dimenzioniranje'!AD$47","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD$50","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Q12=$Q$21,\"Mmin\",IF(Q12=$Q$22,\"Mmax\",\"XIII-XIII\"))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U60","v":3.76},{"$f":"+'Analiza i dimenzioniranje'!AC$47","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC$50","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Q13=$Q$21,\"Mmin\",IF(Q13=$Q$22,\"Mmax\",\"XII-XII\"))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U59","v":3.44},{"$f":"+'Analiza i dimenzioniranje'!AB$47","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB$50","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Q14=$Q$21,\"Mmin\",IF(Q14=$Q$22,\"Mmax\",\"XI-XI\"))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U58","v":3.14},{"$f":"+'Analiza i dimenzioniranje'!AA$47","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA$50","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Q15=$Q$21,\"Mmin\",IF(Q15=$Q$22,\"Mmax\",\"X-X\"))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U57","v":2.8},{"$f":"+'Analiza i dimenzioniranje'!Z$47","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z$50","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Q16=$Q$21,\"Mmin\",IF(Q16=$Q$22,\"Mmax\",\"IX-IX\"))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U56","v":2.48},{"$f":"+'Analiza i dimenzioniranje'!Y$47","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y$50","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Q17=$Q$21,\"Mmin\",IF(Q17=$Q$22,\"Mmax\",\"VIII-VIII\"))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U55","v":2.16},{"$f":"+'Analiza i dimenzioniranje'!X$47","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X$50","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Q18=$Q$21,\"Mmin\",IF(Q18=$Q$22,\"Mmax\",\"VII-VII\"))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U54","v":1.84},{"$f":"+'Analiza i dimenzioniranje'!W$47","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W$50","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Q19=$Q$21,\"Mmin\",IF(Q19=$Q$22,\"Mmax\",\"VII-VII\"))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U53","v":1.52},{"$f":"+'Analiza i dimenzioniranje'!V$47","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V$50","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(Q20=$Q$21,\"Mmin\",IF(Q20=$Q$22,\"Mmax\",\"III-III\"))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U52","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!U$47","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U$50","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mmin",{"$f":"IF(S6=S21,Q6,IF(S7=S21,Q7,IF(S8=S21,Q8,IF(S9=S21,Q9,IF(S10=S21,Q10,IF(S11=S21,Q11,IF(S12=S21,Q12,IF(S13=S21,Q13,IF(S14=S21,Q14,IF(S15=S21,Q15,IF(S16=S21,Q16,IF(S17=S21,Q17,IF(S18=S21,Q18,Q19)))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+MIN(R5:R19)","v":{"$error":"#VALUE!"}},{"$f":"+MIN(S6:S19)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mmax ",{"$f":"IF(S19=S22,Q19,IF(S18=S22,Q18,IF(S17=S22,Q17,IF(S16=S22,Q16,IF(S15=S22,Q15,IF(S14=S22,Q14,IF(S13=S22,Q13,IF(S12=S22,Q12,IF(S11=S22,Q11,IF(S10=S22,Q10,IF(S9=S22,Q9,IF(S8=S22,Q8,IF(S7=S22,Q7,Q6)))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"+MAX(R6:R19)","v":{"$error":"#VALUE!"}},{"$f":"+MAX(S5:S19)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!AO47","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(P27=S10,Q10,IF(P27=S11,Q11,IF(P27=S12,Q12,IF(P27=S13,Q13,IF(P27=S14,Q14)))))","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+MIN(R5:R14)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+MIN(S5:S14)","v":{"$error":"#VALUE!"}}]
[]
[]
[]
[]
[]
[null,null,null,null,null,{"$f":"+'Unos podataka'!B106","v":-8},{"$f":"+'Unos podataka'!C106","v":6.2644906473896782}]

{"sheet":"Sidra","index":11,"n_rows":23,"n_cols":25,"rows_kept":23,"cut":false,"hidden":true,"merged":[[12,0,13,0]]}
[]
["Proračun izduženja"]
[]
["Izduženje sidra kod ispitivanja odgovara izduženju \"stvarne\" slobodne dionice",null,null,null,null,null,null,null,null,"Presjek s 5 redova sidara"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
["Lapp=","Stvarna slobodna dionica",null,null,null,null,null,"Red 1.","Red 2.","Red 3.","Red 4.","Red 5.",null,{"$f":"+N8","v":4.858209496089601},{"$f":"+O8","v":5},null,"jedno sidro   x",{"$f":"+N13","v":0},{"$f":"+N8","v":4.858209496089601}]
["Le=","duljina sidrišne dionice sidra, potrebna za montažu preše",null,null,null,null,null,0.75,0.75,0.75,0.75,0.75,null,{"$f":"+IF(I12>0,V12,IF(H12>0,V8,\"\"))","v":5.3318849219583369},{"$f":"+'Analiza i dimenzioniranje'!E48","v":6},null,"y",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+O8","v":5},null,"y=",{"$f":"+'Analiza i dimenzioniranje'!E48","v":6}]
["Ltf=","duljina slobodne dionice sidra",null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!D72","v":5.9},{"$f":"+'Analiza i dimenzioniranje'!E72","v":4.9000000000000004},{"$f":"+'Analiza i dimenzioniranje'!F72","v":""},{"$f":"+'Analiza i dimenzioniranje'!G72","v":""},{"$f":"+'Analiza i dimenzioniranje'!H71","v":0},"sidro 1",{"$f":"+H13","v":4.858209496089601},{"$f":"IF(N8=0,O13,'Analiza i dimenzioniranje'!D71)","v":5},null,"Y=",{"$f":"(S7-R7)/(S6-R6)","v":0.78218117252017239},"*x    +",{"$f":"-R8*R6+R7","v":1.2},"x=",{"$f":"+(V7-T8)/R8","v":6.1366856792710749},"mm",{"$f":"+V8/1000","v":6.1366856792710745E-3},"m"]
["Ltb=","duljina sidrišne dionice sidra",null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!D73","v":6.7},{"$f":"+'Analiza i dimenzioniranje'!E73","v":4.8},{"$f":"+'Analiza i dimenzioniranje'!F73","v":""},{"$f":"+'Analiza i dimenzioniranje'!G73","v":""},{"$f":"+'Analiza i dimenzioniranje'!H72","v":0},"sidro 2",{"$f":"IF(I12=\"\",0,I13)","v":3.9108586443521296},{"$f":"IF(N9=O13,O13,'Analiza i dimenzioniranje'!E71)","v":3}]
["Et=","Modul elastičnosti čelika        =",null,null,"2,1*108","MPa",null,{"$f":"2.1*100000000","v":210000000},{"$f":"2.1*100000000","v":210000000},{"$f":"2.1*100000000","v":210000000},{"$f":"2.1*100000000","v":210000000},{"$f":"2.1*100000000","v":210000000},"sidro 3",null,null,null,"dva sidra      x",{"$f":"+N9","v":3.9108586443521296},{"$f":"+N8","v":4.858209496089601}]
["DP =","razlika između unešene sile i početne sile",null,null,null,null,null,{"$f":"+F14","v":490.08845396000771},{"$f":"+H11","v":490.08845396000771},{"$f":"+I11","v":490.08845396000771},{"$f":"+J11","v":490.08845396000771},{"$f":"+K11","v":490.08845396000771},"sidro 4",null,null,null,"y",{"$f":"+O9","v":3},{"$f":"+S7","v":5},null,"y=",{"$f":"+'Analiza i dimenzioniranje'!E48","v":6}]
["At=","površina sidra u mm2    Fvanjski=",null,null,32,{"$f":"+E12*E12*PI()/4","v":804.24771931898704},"mm2",{"$f":"+'Analiza i dimenzioniranje'!D75","v":50},{"$f":"+'Analiza i dimenzioniranje'!E75","v":50},{"$f":"+'Analiza i dimenzioniranje'!F75","v":""},{"$f":"+'Analiza i dimenzioniranje'!G75","v":""},{"$f":"+'Analiza i dimenzioniranje'!H74","v":0},"sidro 5",null,null,null,"Y=",{"$f":"(S11-R11)/(S10-R10)","v":2.1111502632123429},"*x    +",{"$f":"-R12*R10+R11","v":-5.2564102564102644},"x=",{"$f":"+(V11-T12)/R12","v":5.3318849219583369},"mm",{"$f":"+V12/1000","v":5.3318849219583372E-3},"m"]
["Ds=","Lapp*DP",null,"funutra=",20,{"$f":"+E13*E13*PI()/4","v":314.15926535897933},"Ds (mm)=",{"$f":"+H23*H12/H10/H11*1000000*1000","v":4.858209496089601},{"$f":"+I23*I12/I10/I11*1000000*1000","v":3.9108586443521296},{"$f":"+J23*J12/J10/J11*1000000*1000","v":{"$error":"#VALUE!"}},{"$f":"+K24*K12/K10/K11*1000000*1000","v":{"$error":"#VALUE!"}},{"$f":"+L24*L12/L10/L11*1000000*1000","v":0},"zid-temelj",0,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,"nastavak do vrha1 sidro"]
[null,"Et*At",null,null,null,{"$f":"+F12-F13","v":490.08845396000771},"mm2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+S6","v":4.858209496089601},{"$f":"+S7","v":5}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Zid",null,null,null,null,null,{"$f":"+V8","v":6.1366856792710749},{"$f":"+V7","v":6},null,{"$f":"+IF(I13>0,V12,V8)","v":5.3318849219583369},null,{"$f":"+V15/1000","v":5.3318849219583372E-3}]
["                                      Granične vrijednosti izduženja definirane su kao:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nastavak do vrha2 sidro"]
["Gornja granična linija (veća vrijednost od):",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+R10","v":3.9108586443521296},{"$f":"+R11","v":3}]
[null,"Lapp≤","Ltf+Le+0,5*Ltb",null,null,null,"Lapp≤",{"$f":"+H8+H7+0.5*H9","v":10},{"$f":"+I8+I7+0.5*I9","v":8.0500000000000007},null,null,null,null,null,null,null,null,null,{"$f":"+V11","v":6},1]
[null,"Lapp≤","1,1*Ltf+Le",null,null,null,"Lapp≤",{"$f":"1.1*H8+H7","v":7.2400000000000011},{"$f":"1.1*I8+I7","v":6.1400000000000006}]
[null,null,null,null,null,"Usvaja se:","Lapp=",{"$f":"+IF(H18>H19,H18,H19)","v":10},{"$f":"+IF(I18>I19,I18,I19)","v":8.0500000000000007}]
["Donja granična linija:"]
[null,"Lapp≥","0,8*Ltf+Le",null,null,null,"Lapp≥",{"$f":"0.8*H8+H7","v":5.4700000000000006},{"$f":"0.8*I8+I7","v":4.67}]
[null,null,null,null,null,"Mjerodavno:","Lapp=",{"$f":"+IF(H22>H20,H22,H20)","v":10},{"$f":"+IF(I22>I20,I22,I20)","v":8.0500000000000007}]

{"sheet":"Iskaz armature","index":12,"n_rows":119,"n_cols":51,"rows_kept":119,"cut":false,"hidden":false,"merged":[[106,0,107,23],[24,48,24,50],[21,23,23,23],[21,22,23,22],[33,23,35,23],[47,23,49,23],[24,23,26,23],[40,23,43,23],[47,22,49,22],[44,22,46,22],[40,22,43,22],[33,22,35,22],[29,29,30,29],[29,30,30,30],[28,35,30,35],[27,23,29,23],[29,28,30,28],[27,22,29,22],[28,33,30,33],[28,34,30,34],[27,26,27,35],[28,27,28,28],[28,29,28,30],[29,26,31,26],[29,27,30,27],[1,42,1,43],[15,29,15,30],[15,31,15,32],[15,27,15,28],[30,23,32,23],[1,22,1,23],[21,45,21,46],[28,31,29,32],[14,26,14,30],[17,22,20,22],[24,22,26,22],[30,22,32,22],[13,22,16,22],[16,26,17,26],[15,33,16,33],[15,34,16,34],[15,35,16,35],[74,47,74,48],[74,45,74,46],[52,20,52,21],[60,21,61,21],[64,21,65,21],[62,21,63,21],[66,21,69,21],[72,21,80,21],[44,23,46,23],[44,20,46,20],[62,45,62,46],[72,22,80,22],[52,24,53,27],[50,21,51,21],[50,22,51,22],[50,23,51,23],[50,20,51,20],[66,22,69,22],[60,22,60,23],[64,22,65,22],[64,23,65,23],[62,22,63,22],[66,23,69,23],[44,21,46,21],[81,23,84,23],[88,45,88,46],[83,45,83,46],[72,23,80,23],[70,21,71,21],[70,22,71,22],[62,20,63,20],[100,21,102,21],[100,22,102,22],[100,23,102,23],[94,22,99,22],[94,21,99,21],[85,21,87,21],[85,22,87,22],[88,20,93,20],[88,21,93,21],[88,22,93,22],[62,23,63,23],[88,19,93,19],[103,20,103,21],[104,20,104,21],[81,21,84,21],[81,22,84,22],[88,0,93,1],[88,2,93,3],[85,2,87,3],[85,4,87,5],[88,4,93,5],[93,11,93,12],[88,10,88,11],[91,10,91,11],[81,0,84,1],[85,11,85,12],[87,11,87,12],[81,19,84,19],[81,20,84,20],[81,2,84,3],[81,4,84,5],[84,11,84,12],[82,9,83,11],[85,0,87,1],[100,0,102,1],[100,19,102,19],[100,20,102,20],[100,2,102,3],[100,4,102,5],[94,0,99,1],[94,2,99,3],[94,4,99,5],[102,11,102,12],[98,8,98,9],[94,20,99,20],[99,9,99,10],[96,9,96,10],[94,11,94,12],[100,11,100,12],[94,19,99,19],[85,19,87,19],[85,20,87,20],[86,9,86,10],[64,19,65,19],[76,9,76,10],[73,10,73,11],[73,12,73,13],[62,19,63,19],[73,8,73,9],[74,9,74,11],[72,20,80,20],[67,8,68,9],[47,0,49,1],[64,2,65,3],[64,4,65,5],[62,2,63,3],[62,4,63,5],[50,0,51,1],[50,2,51,3],[50,4,51,5],[47,2,49,3],[60,0,61,1],[60,2,61,3],[60,4,61,5],[52,2,52,5],[64,0,65,1],[62,0,63,1],[47,4,49,5],[40,4,43,5],[38,8,38,9],[28,9,29,15],[31,9,32,15],[40,19,43,19],[40,2,43,3],[40,18,41,18],[40,0,43,1],[44,0,46,1],[44,2,46,3],[44,4,46,5],[33,0,35,1],[45,9,46,16],[34,9,35,15],[38,12,38,13],[40,12,40,14],[44,19,46,19],[33,19,35,19],[30,19,32,19],[27,19,29,19],[36,10,36,11],[36,19,39,19],[42,12,42,13],[24,4,26,5],[24,0,26,1],[24,2,26,3],[30,0,32,1],[27,0,29,1],[36,2,39,3],[36,0,39,1],[33,2,35,3],[36,4,39,5],[27,2,29,3],[30,2,32,3],[33,4,35,5],[27,4,29,5],[30,4,32,5],[13,2,16,3],[10,7,11,9],[21,0,23,1],[17,2,20,3],[17,4,20,5],[18,6,18,7],[19,9,19,10],[17,0,20,1],[21,2,23,3],[21,4,23,5],[20,10,20,12],[17,8,17,9],[18,8,18,9],[9,2,12,3],[13,11,13,12],[16,11,16,12],[22,11,23,12],[6,20,8,20],[9,23,12,23],[6,22,8,22],[3,23,5,23],[3,21,5,21],[6,21,8,21],[9,21,12,21],[3,22,5,22],[9,22,12,22],[3,20,5,20],[6,23,8,23],[9,20,12,20],[1,20,2,20],[1,21,2,21],[0,0,0,19],[13,4,16,5],[1,6,2,18],[1,4,2,5],[1,19,2,19],[3,19,5,19],[7,10,8,15],[4,10,5,15],[1,0,2,1],[1,2,2,3],[3,4,5,5],[3,2,5,3],[6,2,8,3],[3,0,5,1],[6,0,8,1],[6,4,8,5],[6,19,8,19],[9,4,12,5],[9,9,9,11],[10,11,10,12],[9,0,12,1],[13,0,16,1],[66,0,69,1],[66,10,66,11],[66,19,69,19],[72,0,80,1],[66,2,69,3],[66,4,69,5],[70,4,71,5],[77,10,79,11],[78,12,79,12],[72,11,72,12],[71,11,71,13],[70,0,71,1],[70,11,70,12],[70,19,71,19],[70,2,71,3],[72,19,80,19],[72,2,80,3],[74,12,74,13],[80,10,80,12],[72,4,80,5],[73,6,74,7],[80,8,80,9],[72,8,72,9],[47,12,47,13],[48,9,48,10],[47,10,47,11],[47,19,49,19],[50,11,50,12],[51,9,51,10],[79,8,79,9],[64,20,65,20],[53,10,57,10],[69,9,69,11],[70,20,71,20],[66,20,69,20],[60,19,61,19],[60,20,61,20],[54,14,54,17],[55,14,55,17],[56,14,56,17],[53,13,56,13],[57,13,57,19],[51,13,51,15],[50,19,51,19],[53,14,53,17],[17,14,17,15],[25,11,25,12],[17,12,17,13],[12,9,12,11],[27,20,29,20],[14,13,15,13],[24,19,26,19],[24,20,26,20],[21,20,23,20],[21,19,23,19],[17,20,20,20],[18,14,18,15],[19,14,19,15],[9,19,12,19],[36,20,39,20],[49,12,49,13],[47,8,47,9],[48,12,48,13],[49,8,49,9],[49,10,49,11],[36,21,39,21],[36,22,39,22],[13,20,16,20],[13,19,16,19],[47,21,49,21],[30,21,32,21],[33,20,35,20],[33,21,35,21],[27,21,29,21],[40,21,43,21],[30,20,32,20],[47,20,49,20],[21,21,23,21],[17,19,20,19],[13,21,16,21],[40,20,43,20],[24,21,26,21],[17,21,20,21]]}
[{"$f":"+IF(W58=0,\"ISKAZ ARMATURE za zid duljine     L=\",\"ISKAZ ARMATURE I SIDARA    za zid duljine  L=\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m",null,null,null,null,null,null,null,null,null,null,null,"  T A B L I C A   R E B R A S T E   A R M A T U R E",null,null,null,null,null,null,null,null,null,null,null,"Poz 3."]
["Poz.",null,"vrsta armature  B500B",null,"f ili oznaka mreže",null,"OBLIK ARMATURE",null,null,null,null,null,null,null,null,null,null,null,null,"m'/kom","kom/m'       ili kom","Ukupno kom","Ukupno kg",null,"mase",null,"PROFIL","cm2/kom",null,null,null,null,null,"Površina presjeka za komada",null,null,null,null,null,null,null,null,"   (kg/m)",null,null,{"$f":"+IF(C10=\"\",-5,0.5)","v":0.5},{"$f":"IF('Unos podataka'!$O$48=\"DA\",-5,+H11)","v":0.97317416566836989}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"šipka","mreža",null,null,"F",1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,"RA 400-1","RA 400-2",null,{"$f":"+IF(A10=\"\",-5,)","v":0},{"$f":"+AU2","v":0.97317416566836989}]
[{"$f":"+IF('Unos podataka'!$O$48=\"\",1,\"\")","v":1},null,{"$f":"IF('Unos podataka'!O48=\"\",+'Analiza i dimenzioniranje'!M538,\"\")","v":"šipka"},null,{"$f":"IF(A4=\"\",\"\",IF('Analiza i dimenzioniranje'!H50=\"mreža\",'Analiza i dimenzioniranje'!N538,'Analiza i dimenzioniranje'!O538))","v":14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(A4=\"\",\"\",+K5)","v":2.8427899619247099},{"$f":"IF(E4=\"\",\"\",IF(E4>100,'Analiza i dimenzioniranje'!AC114,IF('Unos podataka'!O48=\"DA\",\"\",IF(E4>100,AC113,+'Analiza i dimenzioniranje'!B270))))","v":{"$error":"#VALUE!"}},{"$f":"IF(E4=\"\",\"\",IF(E4>100,'Analiza i dimenzioniranje'!AC115,IF('Unos podataka'!O48=\"DA\",\"\",ROUNDUP(IF(E4>100,U4*U1,+U4*U1+1),0))))","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!O48=\"DA\",\"\",IF(E4>=100,\"\",+T4*V4*Y4))","v":{"$error":"#VALUE!"}},{"$f":"IF(A4=\"\",\"\",IF(E4>100,+Y5*V4,\"\"))","v":""},{"$f":"+IF(E4=8,$AR$5,IF(E4=10,$AR$6,IF(E4=12,$AR$7,IF(E4=14,$AR$8,IF(E4=16,$AR$9,IF(E4=18,$AR$10,IF(E4=20,$AR$11,$AR$12)))))))","v":1.242},null,6,{"$f":"+AA4*AA4*3.14/4/100","v":0.28260000000000002},{"$f":"+$AB$4*AC3","v":0.56520000000000004},0.84780000000000011,1.1304000000000001,1.413,1.6956000000000002,1.9782000000000002,2.2608000000000001,2.5434000000000001,2.8260000000000001,3.1086,3.3912000000000004,3.6738000000000004,3.9564000000000004,4.2389999999999999,0.23,0.22800000000000001,null,{"$f":"IF(A10=\"\",-5,+'Unos podataka'!G49)","v":0},{"$f":"+IF('Unos podataka'!$O$48=\"DA\",-5,'Analiza i dimenzioniranje'!E551)","v":0.20682583433163007}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Unos podataka'!O48=\"DA\",\"\",+'Analiza i dimenzioniranje'!M99-2*'Analiza i dimenzioniranje'!Q58)","v":2.8427899619247099},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(E4=283,$AJ$39,IF(E4=335,$AJ$40,IF(E4=378,$AJ$41,IF(E4=385,$AJ$42,IF(E4=424,$AJ$43,IF(E4=503,$AJ$44,IF(E4=524,$AJ$45,IF(E4=636,$AJ$46,IF(E4=785,$AJ$47,\"\")))))))))","v":""},null,8,0.50240000000000007,{"$f":"+$AB5*AC3","v":1.0048000000000001},1.5072000000000001,2.0096000000000003,2.5120000000000005,3.0144000000000002,3.5168000000000004,4.0192000000000005,4.5216000000000003,5.0240000000000009,5.5264000000000006,6.0288000000000004,6.531200000000001,7.0336000000000007,7.5360000000000014,0.40899999999999997,0.40500000000000003,null,{"$f":"IF('Unos podataka'!$O$48=\"DA\",-5,+AT2+AT4)","v":0.5},{"$f":"IF('Unos podataka'!$O$48=\"DA\",-5,+AU4+H11*TAN('Analiza i dimenzioniranje'!F217*PI()/180))","v":0.33159168262632721}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(E4=188,$AJ$19,IF(E4=221,$AJ$20,IF(E4=257,$AJ$21,IF(E4=283,$AJ$22,IF(E4=335,$AJ$23,IF(E4=503,$AJ$24,IF(E4=636,$AJ$25,IF(E4=785,$AJ$26,\"\"))))))))","v":""},null,10,0.78500000000000003,{"$f":"+$AB6*AC3","v":1.57},2.355,3.14,3.9250000000000003,4.71,5.4950000000000001,6.28,7.0650000000000004,7.8500000000000005,8.6349999999999998,9.42,10.205,10.99,11.775,0.64900000000000002,0.63300000000000001,null,"Poz 4."]
[{"$f":"+IF('Unos podataka'!$O$48=\"\",2,\"\")","v":2},null,{"$f":"IF('Unos podataka'!O48=\"\",+'Analiza i dimenzioniranje'!M537,\"\")","v":"šipka"},null,{"$f":"IF(A7=\"\",\"\",IF('Analiza i dimenzioniranje'!H50=\"mreža\",'Analiza i dimenzioniranje'!N538,'Analiza i dimenzioniranje'!O55))","v":14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(A7=\"\",\"\",+K8)","v":2.8000021999999993},{"$f":"IF(E7=\"\",\"\",IF(E7>100,'Analiza i dimenzioniranje'!AC114,IF('Unos podataka'!O48=\"DA\",\"\",IF(E7>100,AC14,+'Analiza i dimenzioniranje'!B270))))","v":{"$error":"#VALUE!"}},{"$f":"IF(E7=\"\",\"\",IF(E7>100,'Analiza i dimenzioniranje'!AC115,IF('Unos podataka'!O48=\"DA\",\"\",ROUNDUP(IF(E7>100,U7*U1,+U7*U1+1),0))))","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!O48=\"DA\",\"\",IF(E7>=100,\"\",+T7*V7*Y7))","v":{"$error":"#VALUE!"}},{"$f":"IF(A7=\"\",\"\",IF(E7>100,+Y8*V7,\"\"))","v":""},{"$f":"+IF(E7=8,$AR$5,IF(E7=10,$AR$6,IF(E7=12,$AR$7,IF(E7=14,$AR$8,IF(E7=16,$AR$9,IF(E7=18,$AR$10,IF(E7=20,$AR$11,$AR$12)))))))","v":1.242},null,12,1.1304000000000001,{"$f":"+$AB7*AC3","v":2.2608000000000001},3.3912000000000004,4.5216000000000003,5.6520000000000001,6.7824000000000009,7.9128000000000007,9.0432000000000006,10.1736,11.304,12.4344,13.564800000000002,14.695200000000002,15.825600000000001,16.956,0.92,0.91100000000000003,null,{"$f":"IF(A14=\"\",-5,+'Analiza i dimenzioniranje'!F544-AW11)","v":0},{"$f":"IF('Unos podataka'!$O$48=\"DA\",-5,+'Analiza i dimenzioniranje'!G544-AV11+0.05)","v":0.73946059119973684},{"$f":"+'Analiza i dimenzioniranje'!G544","v":1.1399999999999999},{"$f":"+'Analiza i dimenzioniranje'!F544","v":4.3500021999999996}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Unos podataka'!O48=\"DA\",\"\",+'Analiza i dimenzioniranje'!M100-2*'Analiza i dimenzioniranje'!Q58)","v":2.8000021999999993},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(E7=283,$AJ$39,IF(E7=335,$AJ$40,IF(E7=378,$AJ$41,IF(E7=385,$AJ$42,IF(E7=424,$AJ$43,IF(E7=503,$AJ$44,IF(E7=524,$AJ$45,IF(E7=636,$AJ$46,IF(E7=785,$AJ$47,\"\")))))))))","v":""},null,14,1.5386000000000002,{"$f":"+$AB8*AC3","v":3.0772000000000004},4.6158000000000001,6.1544000000000008,7.6930000000000014,9.2316000000000003,10.770200000000001,12.308800000000002,13.847400000000002,15.386000000000003,16.924600000000002,18.463200000000001,20.001800000000003,21.540400000000002,23.079000000000004,1.252,1.242,null,{"$f":"IF(A14=\"\",-5,+'Analiza i dimenzioniranje'!F545-AW11)","v":0.5},{"$f":"IF('Unos podataka'!$O$48=\"DA\",-5,+'Analiza i dimenzioniranje'!G545-AV11+0.05)","v":0.73946059119973684},{"$f":"+'Analiza i dimenzioniranje'!G545","v":1.1399999999999999},{"$f":"+'Analiza i dimenzioniranje'!F545","v":4.8500021999999996}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(E7=188,$AJ$19,IF(E7=221,$AJ$20,IF(E7=257,$AJ$21,IF(E7=283,$AJ$22,IF(E7=335,$AJ$23,IF(E7=503,$AJ$24,IF(E7=636,$AJ$25,IF(E7=785,$AJ$26,\"\"))))))))","v":""},null,16,2.0096000000000003,{"$f":"+$AB9*AC3","v":4.0192000000000005},6.0288000000000004,8.0384000000000011,10.048000000000002,12.057600000000001,14.067200000000001,16.076800000000002,18.086400000000001,20.096000000000004,22.105600000000003,24.115200000000002,26.124800000000004,28.134400000000003,30.144000000000005,null,1.621,null,{"$f":"IF(A14=\"\",-5,+'Analiza i dimenzioniranje'!F546-AW11-0.01)","v":0.49999999999999978},{"$f":"+IF('Unos podataka'!$O$48=\"DA\",-5,'Analiza i dimenzioniranje'!G546-AV11+0.05)","v":0.15256404470746193},{"$f":"+'Analiza i dimenzioniranje'!G546","v":0.55310345350772505},{"$f":"+'Analiza i dimenzioniranje'!F546","v":4.8600021999999994}]
[{"$f":"+IF('Unos podataka'!$O$48=\"\",3,\"\")","v":3},null,{"$f":"IF('Unos podataka'!$O$48=\"\",+'Analiza i dimenzioniranje'!M539,\"\")","v":"šipka"},null,{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",+'Analiza i dimenzioniranje'!H720)","v":10},null,null,null,null,{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",+'Analiza i dimenzioniranje'!H723)","v":0.5},null,null,null,null,null,null,null,null,null,{"$f":"IF(A10=\"\",\"\",+'Analiza i dimenzioniranje'!R539+0.01)","v":1.9731741656683699},{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",IF(E7>100,4,'Analiza i dimenzioniranje'!Q539))","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",ROUNDUP(IF(E7>100,U10*U1,IF(K60=\"\",+'Analiza i dimenzioniranje'!S537,+'Analiza i dimenzioniranje'!S537)),0))","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",IF(C1>100,\"\",+T10*V10*Y10))","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(E10=8,$AR$5,IF(E10=10,$AR$6,IF(E10=12,$AR$7,IF(E10=14,$AR$8,IF(E10=16,$AR$9,IF(E10=18,$AR$10,AR11))))))","v":0.63300000000000001},null,18,2.5434000000000001,{"$f":"+$AB10*AC3","v":5.0868000000000002},7.6302000000000003,10.1736,12.717000000000001,15.260400000000001,17.803800000000003,20.347200000000001,22.890599999999999,25.434000000000001,27.977400000000003,30.520800000000001,33.0642,35.607600000000005,38.151000000000003,null,2.2879999999999998,null,{"$f":"IF(A14=\"\",-5,+'Analiza i dimenzioniranje'!F547-AW11-0.01)","v":-2.1337098754514727E-16},{"$f":"IF('Unos podataka'!$O$48=\"DA\",-5,+'Analiza i dimenzioniranje'!G547-AV11+0.05)","v":0.05},{"$f":"+'Analiza i dimenzioniranje'!G547","v":0.45053940880026311},{"$f":"+'Analiza i dimenzioniranje'!F547","v":4.3600021999999994}]
[null,null,null,null,null,null,null,{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",+'Analiza i dimenzioniranje'!H724+0.01)","v":0.97317416566836989},null,null,{"$f":"+IF(A10=\"\",\"\",\"a3\")","v":"a3"},null,null,null,{"$f":"+IF(A10=\"\",\"\",\"a\")","v":"a"},{"$f":"+IF(A10=\"\",\"\",\"3=\")","v":"3="},null,{"$f":"IF(A10=\"\",\"\",+'Analiza i dimenzioniranje'!H725)","v":90},{"$f":"IF(A10=\"\",\"\",+'Analiza i dimenzioniranje'!I726)","v":"°"},null,null,null,null,null,null,null,20,3.14,{"$f":"+$AB11*AC3","v":6.28},9.42,12.56,15.700000000000001,18.84,21.98,25.12,28.26,31.400000000000002,34.54,37.68,40.82,43.96,47.1,null,2.5154700000000001,"Novi crtež ","Poz 5.",null,{"$f":"+MIN(AV7:AV10)","v":0.45053940880026311},{"$f":"+MIN(AW7:AW10)","v":4.3500021999999996}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(A10=\"\",\"\",\"b3\")","v":"b3"},null,null,null,{"$f":"+IF(A10=\"\",\"\",\"b\")","v":"b"},{"$f":"+IF(A10=\"\",\"\",\"3=\")","v":"3="},null,{"$f":"IF(A10=\"\",\"\",+'Analiza i dimenzioniranje'!H726)","v":82.694244543359446},{"$f":"IF(A10=\"\",\"\",+'Analiza i dimenzioniranje'!I726)","v":"°"},null,null,null,null,null,null,null,22,3.7993999999999999,{"$f":"+$AB12*AC3","v":7.5987999999999998},11.398199999999999,15.1976,18.997,22.796399999999998,26.595800000000001,30.395199999999999,34.194600000000001,37.994,41.793399999999998,45.592799999999997,49.392199999999995,53.191600000000001,56.991,null,3.0579999999999998,null,{"$f":"+(0-AU12-AU13)/'Analiza i dimenzioniranje'!E57","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$E$52+0.012*50-0.05","v":1.7499999999999998}]
[null,null,null,null,null,null,null,null,null,{"$f":"+J10","v":0.5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,4.90625,{"$f":"+$AB13*AC3","v":9.8125},14.71875,19.625,24.53125,29.4375,34.34375,39.25,44.15625,49.0625,53.96875,58.875,63.78125,68.6875,73.59375,null,3.9510000000000001,{"$f":"+'Analiza i dimenzioniranje'!B548-2-AV13","v":{"$error":"#VALUE!"}},0,{"$f":"+'Analiza i dimenzioniranje'!C548-AW19+0.1","v":{"$error":"#VALUE!"}},null,{"$f":"+'Analiza i dimenzioniranje'!C545","v":1.6923077248520526},{"$f":"+SQRT((AU13-AU14)*(AU13-AU14)+(AV15-AV14)*(AV15-AV14))","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF('Unos podataka'!$O$48=\"\",4,\"\")","v":4},null,{"$f":"IF(C10=\"\",\"\",+'Analiza i dimenzioniranje'!M540)","v":"šipka"},null,{"$f":"IF(E10=\"\",\"\",'Analiza i dimenzioniranje'!B731)","v":10},null,null,null,null,null,null,{"$f":"+L17","v":0.5},null,null,null,null,null,null,null,{"$f":"IF(T10=\"\",\"\",+'Analiza i dimenzioniranje'!R540+0.01)","v":1.5968965464922749},{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",IF(E7>100,4,+'Analiza i dimenzioniranje'!Q540))","v":{"$error":"#VALUE!"}},{"$f":"IF(V10=\"\",\"\",ROUNDUP(+U14*U1+1,0))","v":{"$error":"#VALUE!"}},{"$f":"IF(W10=\"\",\"\",IF(C8>100,\"\",+T14*V14*Y14))","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(E14=8,$AR$5,IF(E14=10,$AR$6,IF(E14=12,$AR$7,IF(E14=14,$AR$8,IF(E14=16,$AR$9,IF(E14=18,$AR$10,AR11))))))","v":0.63300000000000001},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!$B$547-2-$AV$13-AS13","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C547-AW19+0.1","v":{"$error":"#VALUE!"}},null,{"$f":"+'Analiza i dimenzioniranje'!C546","v":1.2},{"$f":"+SQRT((AU14-AU15)*(AU14-AU15)+(AV16-AV15)*(AV16-AV15))","v":{"$error":"#VALUE!"}},{"$f":"+AX14+50*1.2/100","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(A14=\"\",\"\",\"a4\")","v":"a4"},{"$f":"IF(A14=\"\",\"\",+'Analiza i dimenzioniranje'!B735+0.01)","v":0.59689654649227486},{"$f":"+IF(A14=\"\",\"\",\"a\")","v":"a"},{"$f":"+IF(A14=\"\",\"\",\"4=\")","v":"4="},null,{"$f":"+IF(A14=\"\",\"\",90)","v":90},{"$f":"IF(A14=\"\",\"\",+'Analiza i dimenzioniranje'!C734)","v":"°"},null,null,null,null,null,null,null,"      MREŽE NOSIVE U DVA SMJERA   (Q mreže)   š=2150 mm",null,null,null,null,"2150  mm",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AT14-(AU15-AU14)/'Analiza i dimenzioniranje'!E56","v":{"$error":"#VALUE!"}},{"$f":"+AU12","v":1.7499999999999998},null,{"$f":"+'Analiza i dimenzioniranje'!C547","v":{"$error":"#VALUE!"}},{"$f":"+SQRT((AU13-AU15)^2+(AV14-AV16)^2)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(A14=\"\",\"\",\"b4\")","v":"b4"},null,{"$f":"+IF(A14=\"\",\"\",\"b\")","v":"b"},{"$f":"+IF(A14=\"\",\"\",\"4=\")","v":"4="},null,{"$f":"IF(A14=\"\",\"\",+'Analiza i dimenzioniranje'!B736)","v":97.305755456640554},{"$f":"IF(A14=\"\",\"\",+'Analiza i dimenzioniranje'!C734)","v":"°"},null,null,null,null,null,null,null,null,"Promjer žica  (mm)",null,"Razmak žica (mm)",null,"Površina presjeka žica (cm2/m')",null,"Duljina mreže    (mm)","Masa     (kg/m2)","Masa kg/kom    (toler. 1%)",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!E42>'Analiza i dimenzioniranje'!E52,+AT14-(AU16-AU14)/'Analiza i dimenzioniranje'!E56,'Iskaz armature'!AT15)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E42>'Analiza i dimenzioniranje'!E52,+AU15+1,AU15)","v":1.7499999999999998},null,{"$f":"+'Analiza i dimenzioniranje'!C548","v":{"$error":"#VALUE!"}},{"$f":"+SQRT((AU16-AU18)*(AU16-AU18)+(AV17-AV19)*(AV17-AV19))","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(A14=\"\",\"\",+'Analiza i dimenzioniranje'!B734)","v":0.5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oznaka mreže","uzdužne","poprečne","uzdužno","poprečno","uzdužnih","poprečnih",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!B549-2-AV13","v":1.4550000999999995},{"$f":"+'Analiza i dimenzioniranje'!C549-AW19+0.1","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!B548-2","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C549","v":1.2},{"$f":"+MIN(AU13:AU18)","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF('Analiza i dimenzioniranje'!$M$569=\"\",1,5)","v":5},null,{"$f":"+'Analiza i dimenzioniranje'!M541","v":"šipka"},null,{"$f":"+IF('Analiza i dimenzioniranje'!C320=\"\",E4,'Analiza i dimenzioniranje'!C320)","v":12},null,null,null,{"$f":"+IF('Unos podataka'!$O$48=\"\",\"\",0.8)","v":""},null,null,null,null,null,{"$f":"+IF(A18=\"\",\"\",\"a =\")","v":"a ="},null,null,{"$f":"+'Analiza i dimenzioniranje'!E736","v":86.694244543359446},{"$f":"+'Analiza i dimenzioniranje'!$F$736","v":"°"},{"$f":"+J20+K21+N20","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$O$48=\"\",+'Analiza i dimenzioniranje'!Q541,10)","v":{"$error":"#VALUE!"}},{"$f":"+U18*U1+1","v":{"$error":"#VALUE!"}},{"$f":"IF(C6>100,\"\",+T18*V18*Y18)","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(E18=8,$AR$5,IF(E18=10,$AR$6,IF(E18=12,$AR$7,IF(E18=14,$AR$8,IF(E18=16,$AR$9,IF(E18=18,$AR$10,AR21))))))","v":0.91100000000000003},{"$f":"+IF(F18=8,$AB$5,IF(E18=10,$AB$6,IF(E18=12,$AB$7,IF(E18=14,$AB$8,IF(E18=16,$AB$9,IF(E18=18,$AB$10,AB25))))))","v":1.1304000000000001},null,"D","d","a","t",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!B550-2-AV13","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C550-AW19+0.1","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!B549-2","v":1.4550000999999995},{"$f":"+'Analiza i dimenzioniranje'!C550","v":1.6923077248520526},{"$f":"+SQRT('Analiza i dimenzioniranje'!E60^2+'Analiza i dimenzioniranje'!E52^2)-0.05","v":1.1499999999999999}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(A18=\"\",\"\",\"b =\")","v":"b ="},null,null,{"$f":"+'Analiza i dimenzioniranje'!E735","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$F$736","v":"°"},null,null,null,null,null,null,null,"Q-188",6,6,150,{"$f":"+AD19","v":150},1.88,1.88,6000,3.05,33.44,null,null,null,null,null,null,null,null,null,"Poz 6a.",null,{"$f":"+'Analiza i dimenzioniranje'!B550-2","v":{"$error":"#VALUE!"}},{"$f":"+MIN(AW13:AW18)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,{"$f":"+AU12-AU13","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"AU16-AU14","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,"Q-221",6.5,6.5,150,150,2.21,2.21,6000,3.6,39.47,null,null,null,null,null,null,null,null,null,{"$f":"+IF(A22=\"\",\"\",0)","v":0},{"$f":"IF(A22=\"\",\"\",+IF('Unos podataka'!G63=\"\",\"\",1))","v":1}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!E733","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Q-257",7,7,150,150,2.57,2.57,6000,4.16,45.61,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E38=0,\"\",7)","v":7},{"$f":"IF(A22=\"\",\"\",+IF('Unos podataka'!G63=\"\",\"\",1))","v":1}]
[{"$f":"+IF('Analiza i dimenzioniranje'!$M$569=\"\",\"2\",6)","v":6},null,{"$f":"IF(A22=\"\",\"\",+'Analiza i dimenzioniranje'!M542)","v":"šipka"},null,{"$f":"IF(A22=\"\",\"\",+'Unos podataka'!E94)","v":8},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(A22=\"\",\"\",'Analiza i dimenzioniranje'!R542)","v":11.9},{"$f":"IF('Unos podataka'!$O$48=\"DA\",9,'Analiza i dimenzioniranje'!AB414)","v":{"$error":"#VALUE!"}},{"$f":"+U22","v":{"$error":"#VALUE!"}},{"$f":"IF(E22>=100,\"\",+T22*V22*Y22)","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(E22=8,$AR$5,IF(E22=10,$AR$6,IF(E22=12,$AR$7,IF(E22=14,$AR$8,IF(E22=16,$AR$9,IF(E22=18,$AR$10,AR11))))))","v":0.40500000000000003},null,"Q-283",6,6,100,100,2.83,2.83,6000,4.4400000000000004,49.68,null,null,null,null,null,null,null,null,null,"Poz 7'"]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(A22=\"\",\"\",+'Analiza i dimenzioniranje'!H731)","v":11.9},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Q-335",8,8,150,150,3.35,3.35,6000,5.44,59.65,null,null,null,null,null,null,null,null,null,{"$f":"+IF(A31=\"\",-5,0)","v":{"$error":"#VALUE!"}},{"$f":"+IF(A31=\"\",-5,3)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Q-503",8,8,100,100,5.03,5.03,6000,7.9,88.49,null,null,null,null,null,null,null,null,null,{"$f":"IF(A31=\"\",-5,IF('Analiza i dimenzioniranje'!B377=\"\",-2,0.5))","v":{"$error":"#VALUE!"}},{"$f":"IF(A31=\"\",-5,+IF('Analiza i dimenzioniranje'!B377=\"\",-2,0.5))","v":{"$error":"#VALUE!"}}]
[{"$f":"IF('Unos podataka'!$O$48=\"\",+IF('Unos podataka'!G63=\"\",\"\",\"6a\"),\"\")","v":"6a"},null,{"$f":"IF(A25=\"\",\"\",IF('Unos podataka'!G63=\"\",\"\",'Analiza i dimenzioniranje'!M543))","v":"šipka"},null,{"$f":"IF(A25=\"\",\"\",IF('Unos podataka'!G63=\"\",\"\",'Analiza i dimenzioniranje'!H739))","v":14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",IF('Unos podataka'!G63=\"\",\"\",'Analiza i dimenzioniranje'!R543))","v":11.9},{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",IF('Unos podataka'!G63=\"\",\"\",'Analiza i dimenzioniranje'!S541))","v":8},{"$f":"+U25","v":8},{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",IF(E25>=100,\"\",+T25*U25*Y25))","v":118.2384},null,{"$f":"+IF(E25=8,$AR$5,IF(E25=10,$AR$6,IF(E25=12,$AR$7,IF(E25=14,$AR$8,IF(E25=16,$AR$9,IF(E25=18,$AR$10,AR11))))))","v":1.242},null,"Q-636",9,9,100,100,6.86,6.86,6000,9.98,131.69999999999999,null,null,null,null,null,null,null,null,null,"Poz 9",null,null,"Površina mreža"]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",IF('Unos podataka'!G63=\"\",\"\",'Analiza i dimenzioniranje'!H740))","v":11.9},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Q-785",10,10,100,{"$f":"+AD26","v":100},7.85,7.85,6000,12.34,138.18,null,null,null,null,null,null,null,null,null,{"$f":"IF(A37=\"\",-5,+'Analiza i dimenzioniranje'!B560-AV30+0.01)","v":{"$error":"#VALUE!"}},{"$f":"+IF(A37=\"\",-5,0)","v":0},{"$f":"+'Analiza i dimenzioniranje'!B560","v":{"$error":"#VALUE!"}},"Q mreža=",{"$f":"5.1*2.15","v":10.964999999999998},"m2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(A37=\"\",-5,+'Analiza i dimenzioniranje'!B561-AV30+0.01)","v":{"$error":"#VALUE!"}},{"$f":"+IF(A37=\"\",-5,0.5)","v":0.5},{"$f":"+'Analiza i dimenzioniranje'!B561","v":{"$error":"#VALUE!"}},"R mreža=",{"$f":"6*2.15","v":12.899999999999999},"m2"]
[{"$f":"+IF('Unos podataka'!$O$48=\"\",7,\"\")","v":7},null,{"$f":"IF(A28=\"\",\"\",+'Analiza i dimenzioniranje'!M544)","v":"šipka"},null,{"$f":"IF('Analiza i dimenzioniranje'!$M$569=\"\",\"\",IF('Analiza i dimenzioniranje'!H54=\"šipka\",'Analiza i dimenzioniranje'!C320,+'Analiza i dimenzioniranje'!G322))","v":12},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",IF('Analiza i dimenzioniranje'!H54=\"RA\",T34,+'Analiza i dimenzioniranje'!R544))","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",IF(E28>100,AW37/U1,IF('Analiza i dimenzioniranje'!H54=\"mreža\",'Iskaz armature'!U34,+'Analiza i dimenzioniranje'!AD109)))","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",IF(E28>100,AW37,IF('Analiza i dimenzioniranje'!H54=\"MA\",+U34*'Iskaz armature'!U1,'Analiza i dimenzioniranje'!AD111*U1+1)))","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",IF(E28>=100,\"\",+T28*V28*Y28))","v":{"$error":"#VALUE!"}},{"$f":"IF(A28=\"\",\"\",IF(E28>100,+Y29*V28,\"\"))","v":""},{"$f":"+IF(E28=8,$AR$5,IF(E28=10,$AR$6,IF(E28=12,$AR$7,IF(E28=14,$AR$8,IF(E28=16,$AR$9,IF(E28=18,$AR$10,AR11))))))","v":0.91100000000000003},null,"    MREŽE NOSIVE U JEDNOM SMJERU (R mreže)   š=2150  mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(A37=\"\",-5,+'Analiza i dimenzioniranje'!A562-AV30+0.01)","v":{"$error":"#VALUE!"}},{"$f":"+IF(A37=\"\",-5,0.5)","v":0.5},{"$f":"+'Analiza i dimenzioniranje'!A562","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,{"$f":"IF('Unos podataka'!$O$48=\"DA\",\"\",IF('Analiza i dimenzioniranje'!H54=\"RA\",'Iskaz armature'!T28,'Analiza i dimenzioniranje'!R544))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(E28=283,AJ39,IF(E28=335,AJ40,IF(E28=378,AJ41,IF(E28=385,AJ42,IF(E28=424,AJ43,IF(E28=503,AJ44,IF(E28=524,AJ45,IF(E28=636,AJ46,IF(E28=785,AJ47,\"\")))))))))","v":""},null,null,"Promjer žica  (mm)",null,"Razmak žica (mm)",null,"Površina presjeka žica (cm2/m')",null,"Duljina mreže    (mm)","Masa     (kg/m2)","Masa kg/kom    (toler. 1%)",null,null,null,null,null,null,null,null,null,{"$f":"IF(A37=\"\",-5,+'Analiza i dimenzioniranje'!B563-AV30+0.01)","v":{"$error":"#VALUE!"}},{"$f":"+AU26","v":0},{"$f":"+'Analiza i dimenzioniranje'!B563","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oznaka mreže","uzdužne","poprečne","uzdužno","poprečno",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poz 10",null,{"$f":"+MIN(AV26:AV29)","v":{"$error":"#VALUE!"}}]
[{"$f":"IF(A28=\"\",\"\",IF('Analiza i dimenzioniranje'!AD109=0,\"\",IF('Analiza i dimenzioniranje'!AD109<'Analiza i dimenzioniranje'!AD110,\"7'\",\"\")))","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(A31=\"\",\"\",+C28)","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(A31=\"\",\"\",E28)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(A31=\"\",\"\",IF('Analiza i dimenzioniranje'!B321=\"\",\"\",'Analiza i dimenzioniranje'!AB97-'Analiza i dimenzioniranje'!E52+0.2))","v":{"$error":"#VALUE!"}},{"$f":"+IF('Analiza i dimenzioniranje'!AD109='Analiza i dimenzioniranje'!AD110,\"\",'Analiza i dimenzioniranje'!AD111)","v":{"$error":"#VALUE!"}},{"$f":"IF(A31=\"\",\"\",+U31*U1)","v":{"$error":"#VALUE!"}},{"$f":"IF(A31=\"\",\"\",+T31*V31*Y31)","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(E31=8,$AR$5,IF(E31=10,$AR$6,IF(E31=12,$AR$7,IF(E31=14,$AR$8,IF(E31=16,$AR$9,IF(E31=18,$AR$10,AR11))))))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,"uzdužnih","poprečnih",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-IF('Analiza i dimenzioniranje'!E78=\"\",\"\",M41+AT32)-AV44","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E79=0,0,AU32)","v":{"$error":"#VALUE!"}},"Mreže"]
[null,null,null,null,null,null,null,null,null,{"$f":"+T31","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D","d","a","t",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E78=\"\",\"\",0.1)","v":0.1},{"$f":"+IF('Analiza i dimenzioniranje'!E79=0,0,'Analiza i dimenzioniranje'!E751)","v":{"$error":"#VALUE!"}},"Poz. 1","potrebno"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R-131",5,4,150,250,1.31,0.5,5000,1.52,16.34,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E78=\"\",\"\",AT32+AU32/'Analiza i dimenzioniranje'!E56)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Analiza i dimenzioniranje'!E79=0,AU32,0)","v":0},"AR=",{"$f":"+K8*U1*1.1","v":36.960029039999995},"m2"]
[{"$f":"+IF('Unos podataka'!O48=\"\",8,\"\")","v":8},null,{"$f":"IF(A34=\"\",\"\",+'Analiza i dimenzioniranje'!M545)","v":"mreža Q"},null,{"$f":"IF(A34=\"\",\"\",+'Analiza i dimenzioniranje'!N545)","v":335},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(A34=\"\",\"\",+IF('Analiza i dimenzioniranje'!R545=0,'Analiza i dimenzioniranje'!Q545,'Analiza i dimenzioniranje'!R545))","v":{"$error":"#VALUE!"}},{"$f":"IF(A34=\"\",\"\",IF(E34>100,V34/U1,+IF('Analiza i dimenzioniranje'!Q545=0,'Analiza i dimenzioniranje'!P545,'Analiza i dimenzioniranje'!Q545)))","v":{"$error":"#VALUE!"}},{"$f":"IF(A34=\"\",\"\",IF(E34>100,AW40,+IF('Analiza i dimenzioniranje'!S543=0,'Analiza i dimenzioniranje'!R545,'Analiza i dimenzioniranje'!S543)))","v":{"$error":"#VALUE!"}},null,{"$f":"IF(A34=\"\",\"\",+V34*Y36)","v":{"$error":"#VALUE!"}},null,null,"R-139",4.2,4.2,100,250,1.39,0.55000000000000004,5000,1.53,16.829999999999998,null,null,null,null,null,null,null,null,null,"Poz 11",null,"kom=",{"$f":"ROUNDUP(AW33/AX27,0)","v":3}]
[null,null,null,null,null,null,null,null,null,{"$f":"IF(A34=\"\",\"\",+'Analiza i dimenzioniranje'!R545)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R-166",4.5999999999999996,4.2,100,250,1.66,0.55000000000000004,5000,1.74,19.14,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!H77=0,\"\",0)","v":0},{"$f":"+IF('Analiza i dimenzioniranje'!H77=0,\"\",1)","v":1},"Poz. 7","potrebno"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(E34=188,$AJ$19,IF(E34=221,$AJ$20,IF(E34=257,$AJ$21,IF(E34=283,$AJ$22,IF(E34=335,$AJ$23,IF(E34=503,$AJ$24,IF(E34=636,$AJ$25,IF(E34=785,$AJ$26,\"\"))))))))","v":59.65},null,"R-196",5,4.2,100,250,1.96,0.55000000000000004,5000,1.98,21.89,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!H77=0,\"\",7)","v":7},{"$f":"+IF('Analiza i dimenzioniranje'!H77=0,\"\",1)","v":1},"AR=",{"$f":"+J29*U1*1.1","v":{"$error":"#VALUE!"}},"m2"]
[{"$f":"+IF('Unos podataka'!O48=\"\",9,\"\")","v":9},null,{"$f":"IF(A37=\"\",\"\",\"šipka\")","v":"šipka"},null,{"$f":"IF(A37=\"\",\"\",+'Analiza i dimenzioniranje'!B749)","v":10},null,null,null,null,null,{"$f":"IF(A37=\"\",\"\",+'Analiza i dimenzioniranje'!B753)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"IF(A37=\"\",\"\",+'Analiza i dimenzioniranje'!R546)","v":{"$error":"#VALUE!"}},{"$f":"IF(A37=\"\",\"\",IF(E37>100,4,+U18))","v":{"$error":"#VALUE!"}},{"$f":"IF(A37=\"\",\"\",+U37*U1+1)","v":{"$error":"#VALUE!"}},{"$f":"IF(E37>100,\"\",+T37*V37*Y37)","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(E37=8,$AR$5,IF(E37=10,$AR$6,IF(E37=12,$AR$7,IF(E37=14,$AR$8,IF(E37=16,$AR$9,IF(E37=18,$AR$10,AR11))))))","v":0.63300000000000001},null,"R-221",6.5,4.2,150,250,2.21,0.66,6000,2.27,30.57,null,null,null,null,null,null,null,null,null,"Poz.12",null,"kom=",{"$f":"ROUNDUP(AW36/AX27,0)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(A37=\"\",\"\",\"a9\")","v":"a9"},null,{"$f":"+IF('Unos podataka'!$O$48=\"DA\",\"\",\"b9\")","v":"b9"},null,{"$f":"+IF(A37=\"\",\"\",\"a\")","v":"a"},{"$f":"+IF(A37=\"\",\"\",\"9=\")","v":"9="},null,{"$f":"IF(A37=\"\",\"\",'Analiza i dimenzioniranje'!B755)","v":86},{"$f":"IF(A37=\"\",\"\",+'Analiza i dimenzioniranje'!C752)","v":"°"},null,null,null,null,null,null,null,"R-238",5.5,4.2,100,250,2.38,0.55000000000000004,6000,2.31,30.61,null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!E78=\"\",\"\",+'Analiza i dimenzioniranje'!K476+0.03-0.8)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E78=\"\",\"\",+'Analiza i dimenzioniranje'!L476+0.1-1.5)","v":1.79},"Poz. 8","potrebno"]
[null,null,null,null,null,null,null,null,{"$f":"IF(A37=\"\",\"\",+'Analiza i dimenzioniranje'!B752)","v":0.4},null,null,null,{"$f":"IF(A37=\"\",\"\",+'Analiza i dimenzioniranje'!B752)","v":0.4},null,{"$f":"+IF(A37=\"\",\"\",\"b\")","v":"b"},{"$f":"+IF(A37=\"\",\"\",\"9=\")","v":"9="},null,{"$f":"IF(A37=\"\",\"\",+'Analiza i dimenzioniranje'!B754)","v":{"$error":"#VALUE!"}},{"$f":"IF(A37=\"\",\"\",+'Analiza i dimenzioniranje'!C753)","v":"°"},null,null,null,null,null,null,null,"R-283",6,4.2,100,250,2.83,0.55000000000000004,6000,2.66,35.229999999999997,null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!E78=\"\",\"\",+'Analiza i dimenzioniranje'!K477-0.8)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E78=\"\",\"\",+'Analiza i dimenzioniranje'!L477+0.8-1)","v":3.1900000000000004},"AR=",{"$f":"+J35*U1*1.1","v":{"$error":"#VALUE!"}},"m2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R-335",8,5,150,250,3.35,0.78,6000,3.41,43.99,null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!E78=\"\",\"\",+'Analiza i dimenzioniranje'!K478-0.8)","v":{"$error":"#VALUE!"}},{"$f":"+AU39","v":3.1900000000000004},"kom=",{"$f":"ROUNDUP(AW39/AX27,0)","v":{"$error":"#VALUE!"}}]
[{"$f":"+'Analiza i dimenzioniranje'!L547","v":10},null,{"$f":"+'Analiza i dimenzioniranje'!M547","v":"šipka"},null,{"$f":"+'Analiza i dimenzioniranje'!C403","v":12},null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!H77=0,\"\",+'Analiza i dimenzioniranje'!$E$750)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!H77=0,\"\",+'Analiza i dimenzioniranje'!F752)","v":"°"},{"$f":"+'Analiza i dimenzioniranje'!R547","v":{"$error":"#VALUE!"}},{"$f":"IF(A41=\"\",\"\",+'Analiza i dimenzioniranje'!B405)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!S545","v":{"$error":"#VALUE!"}},{"$f":"IF(A41=\"\",\"\",+T41*V41*Y41)","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(E41=8,$AR$5,IF(E41=10,$AR$6,IF(E41=12,$AR$7,IF(E41=14,$AR$8,IF(E41=16,$AR$9,IF(E41=18,$AR$10,AR11))))))","v":0.91100000000000003},null,"R-378",8.5,5,150,250,3.78,0.78,6000,3.77,48.63,null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!E78=\"\",\"\",+'Analiza i dimenzioniranje'!K479-0.8)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E78=\"\",\"\",+'Analiza i dimenzioniranje'!L479-1.6)","v":1.5899999999999999}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!H78=0,\"\",\"a\")","v":"a"},{"$f":"+IF('Analiza i dimenzioniranje'!H77=0,\"\",\"10=\")","v":"10="},{"$f":"IF('Analiza i dimenzioniranje'!H77=0,\"\",+'Analiza i dimenzioniranje'!E752)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"R-385",7,5,100,250,3.85,0.78,6000,3.64,48.3,null,null,null,null,null,null,null,null,null,{"$f":"IF(AT38=\"\",\"\",IF('Analiza i dimenzioniranje'!E78=\"\",\"\",+'Analiza i dimenzioniranje'!K480-0.8))","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E78=\"\",\"\",+'Analiza i dimenzioniranje'!L480-1.6)","v":1.5899999999999999}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!H77=0,\"\",+'Analiza i dimenzioniranje'!$E$751)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,"R-424",9,6,150,250,4.24,1.1299999999999999,6000,4.22,57.02,null,null,null,null,null,null,null,null,null,{"$f":"IF(AT38=\"\",\"\",+AT42-J49)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E78=\"\",\"\",+AU40-0.1)","v":3.0900000000000003}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R-503",8,6,100,250,5.03,1.1299999999999999,6000,4.84,64.209999999999994,null,null,null,null,null,null,null,null,null,"Poz. 13"]
[{"$f":"+'Analiza i dimenzioniranje'!L548","v":11},null,{"$f":"+'Analiza i dimenzioniranje'!M548","v":"šipka"},null,{"$f":"+'Analiza i dimenzioniranje'!I748","v":8},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!R548","v":11.9},{"$f":"+V45","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!S546","v":{"$error":"#VALUE!"}},{"$f":"IF(E45>=100,\"\",+T45*V45*Y45)","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(E45=8,$AR$5,IF(E45=10,$AR$6,IF(E45=12,$AR$7,IF(E45=14,$AR$8,IF(E45=16,$AR$9,IF(E45=18,$AR$10,AR11))))))","v":0.40500000000000003},null,"R-524",10,6,150,250,5.24,1.1299999999999999,6000,5.24,67.599999999999994,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!AH84=\"\",-10,0.1)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Analiza i dimenzioniranje'!AH84=\"\",\"\",0)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!H77=0,\"\",+'Analiza i dimenzioniranje'!H749)","v":11.9},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R-636",9,6,100,250,6.36,1.1299999999999999,6000,5.88,78.069999999999993,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!AH84=\"\",-10,0.1)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AH84=\"\",\"\",+J52)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R-785",10,6,100,250,7.85,1.1299999999999999,6000,7.06,93.76,null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AH84=\"\",-10,+N51+0.1)","v":{"$error":"#VALUE!"}},{"$f":"+AU46","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF('Analiza i dimenzioniranje'!E78=\"\",\"\",12)","v":12},null,{"$f":"+IF(A48=12,\"šipka\",\"\")","v":"šipka"},null,{"$f":"+IF(A48=12,8,\"\")","v":8},null,null,null,null,null,null,null,{"$f":"IF(A48=\"\",\"\",+'Analiza i dimenzioniranje'!K478-'Analiza i dimenzioniranje'!K477)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+IF('Analiza i dimenzioniranje'!H77=0,\"\",\"a\")","v":"a"},{"$f":"+IF('Analiza i dimenzioniranje'!H77=0,\"\",\"12=\")","v":"12="},{"$f":"IF('Analiza i dimenzioniranje'!E78=\"\",\"\",+R42)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Analiza i dimenzioniranje'!E78=\"\",\"\",\"o\")","v":"o"},{"$f":"IF(A48=12,2*J49+P49+M48+M50,\"\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(A48=12,TRUNC(1/'Unos podataka'!F97*100),\"\")","v":2},{"$f":"IF(A48=12,TRUNC(U48*U1+1),\"\")","v":25},{"$f":"IF(E48>=100,\"\",+T48*V48*Y48)","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(E48=8,$AR$5,IF(E48=10,$AR$6,IF(E48=12,$AR$7,IF(E48=14,$AR$8,IF(E48=16,$AR$9,IF(E48=18,$AR$10,AR11))))))","v":0.40500000000000003},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AT47","v":{"$error":"#VALUE!"}},{"$f":"+AU45","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,{"$f":"IF(A48=\"\",\"\",'Analiza i dimenzioniranje'!E81-2*'Unos podataka'!C99/100)","v":0.19999999999999998},null,null,null,null,null,{"$f":"+J49","v":0.19999999999999998},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Unos podataka'!$O$48=\"DA\",\"\",0)","v":0},{"$f":"+IF(AC49=\"\",\"\",0.2)","v":0.2},0,0.2]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(A48=\"\",\"\",'Analiza i dimenzioniranje'!K479-'Analiza i dimenzioniranje'!K480)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+IF('Analiza i dimenzioniranje'!H77=0,\"\",\"b\")","v":"b"},{"$f":"+IF('Analiza i dimenzioniranje'!H77=0,\"\",\"12=\")","v":"12="},{"$f":"IF('Analiza i dimenzioniranje'!E78=\"\",\"\",180-R48)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Analiza i dimenzioniranje'!E78=\"\",\"\",\"o\")","v":"o"},null,null,null,null,null,null,null,null,null,{"$f":"+IF('Unos podataka'!$O$48=\"DA\",\"\",3)","v":3},{"$f":"+AD49","v":0.2},3,0.2]
[{"$f":"+IF('Analiza i dimenzioniranje'!B334=\"\",\"\",13)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(A51=\"\",\"\",+IF('Analiza i dimenzioniranje'!AD86>'Analiza i dimenzioniranje'!AD70,\"\",\"šipka\"))","v":{"$error":"#VALUE!"}},null,{"$f":"IF(A51=\"\",\"\",IF('Analiza i dimenzioniranje'!AD86>'Analiza i dimenzioniranje'!AD70,\"\",+E22))","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AH84=\"\",\"\",+('Analiza i dimenzioniranje'!V49-2*'Analiza i dimenzioniranje'!B315)/100)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AH84=\"\",\"\",+IF('Analiza i dimenzioniranje'!D439<'Analiza i dimenzioniranje'!G439,\"\",\" do\"))","v":{"$error":"#VALUE!"}},null,{"$f":"IF('Analiza i dimenzioniranje'!AH84=\"\",\"\",IF('Analiza i dimenzioniranje'!D439<'Analiza i dimenzioniranje'!G439,\"\",(+'Analiza i dimenzioniranje'!U49-2*'Analiza i dimenzioniranje'!Q52*100)/100))","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AH84=\"\",\"\",+J52+N52+N51)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AF90","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AH84=\"\",\"\",IF('Analiza i dimenzioniranje'!AD86>'Analiza i dimenzioniranje'!AD70,\"\",U1*U51))","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AH84=\"\",\"\",IF('Analiza i dimenzioniranje'!AD86>'Analiza i dimenzioniranje'!AD70,\"\",+IF(E51=10,'Analiza i dimenzioniranje'!AD460*T51*V51,IF('Iskaz armature'!E51=8,'Analiza i dimenzioniranje'!AD459)*V51)))","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(E51=8,$AR$5,IF(E51=10,$AR$6,IF(E51=12,$AR$7,IF(E51=14,$AR$8,IF(E51=16,$AR$9,IF(E51=18,$AR$10,AR11))))))","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AH84=\"\",\"\",+IF('Analiza i dimenzioniranje'!AD86>'Analiza i dimenzioniranje'!AD70,\"\",0.15))","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AH84=\"\",\"\",+IF('Analiza i dimenzioniranje'!AD86>'Analiza i dimenzioniranje'!AD70,\"\",0.15))","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ukupno zid i temelj:","        S (kg)",null,{"$f":"SUM(W4:W51)","v":{"$error":"#VALUE!"}},{"$f":"IF(X28=\"?\",\"?\",SUM(X4:X51))","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!A67=\"\",\"\",+IF('Analiza i dimenzioniranje'!A67=\"    SIDRA\",\"SIDRA\",\"\"))","v":"SIDRA"},{"$f":"+IF('Analiza i dimenzioniranje'!D70=\"\",\"\",\"I. red:\")","v":"I. red:"},null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!D70=\"\",\"\",\"m'\")","v":"m'"},{"$f":"IF('Analiza i dimenzioniranje'!D70=\"\",\"\",ROUNDUP(('Analiza i dimenzioniranje'!P$23+'Analiza i dimenzioniranje'!P$24),0))","v":13},{"$f":"+IF(T54=\"\",\"\",\"kom\")","v":"kom"},{"$f":"IF(T54=\"\",\"\",ROUNDUP(($U$1/'Analiza i dimenzioniranje'!$D$76),0))","v":{"$error":"#VALUE!"}},{"$f":"+IF(V54=\"\",\"\",\"Σm'\")","v":{"$error":"#VALUE!"}},{"$f":"IF(V54=\"\",\"\",T54*V54)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E70=\"\",\"\",\"II. red:\")","v":"II. red:"},null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E70=\"\",\"\",\"m'\")","v":"m'"},{"$f":"IF('Analiza i dimenzioniranje'!E70=\"\",\"\",ROUNDUP(('Analiza i dimenzioniranje'!Q$23+'Analiza i dimenzioniranje'!Q$24),0))","v":10},{"$f":"+IF(T55=\"\",\"\",\"kom\")","v":"kom"},{"$f":"IF(T55=\"\",\"\",ROUNDUP(($U$1/'Analiza i dimenzioniranje'!$D$76),0))","v":{"$error":"#VALUE!"}},{"$f":"+IF(V55=\"\",\"\",\"Σm'\")","v":{"$error":"#VALUE!"}},{"$f":"IF(V55=\"\",\"\",T55*V55)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!F70=\"\",\"\",\"III. red:\")","v":""},null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!F70=\"\",\"\",\"m'\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!F70=\"\",\"\",ROUNDUP(('Analiza i dimenzioniranje'!R$23+'Analiza i dimenzioniranje'!R$24),0))","v":""},{"$f":"+IF(T56=\"\",\"\",\"kom\")","v":""},{"$f":"IF(T56=\"\",\"\",ROUNDUP(($U$1/'Analiza i dimenzioniranje'!$D$76),0))","v":""},{"$f":"+IF(V56=\"\",\"\",\"Σm'\")","v":""},{"$f":"IF(V56=\"\",\"\",T56*V56)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!G70=\"\",\"\",\"IV. red:\")","v":""},null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!G70=\"\",\"\",\"m'\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!G70=\"\",\"\",IF(V57=\"\",\"\",ROUNDUP(('Analiza i dimenzioniranje'!S$23+'Analiza i dimenzioniranje'!S$24),0)))","v":""},{"$f":"+IF(T57=\"\",\"\",\"kom\")","v":""},{"$f":"IF(T57=\"\",\"\",ROUNDUP(($U$1/'Analiza i dimenzioniranje'!$D$76),0))","v":""},{"$f":"+IF(V57=\"\",\"\",\"Σm'\")","v":""},{"$f":"IF(V57=\"\",\"\",T57*V57)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(N54=\"\",\"\",\"Ukupno sidra:\")","v":"Ukupno sidra:"},null,null,null,null,null,null,{"$f":"+IF(V54=\"\",\"\",\"kom\")","v":{"$error":"#VALUE!"}},{"$f":"IF(V54=\"\",\"\",SUM(V54:V57))","v":{"$error":"#VALUE!"}},{"$f":"+IF(V54=\"\",\"\",\"m'\")","v":{"$error":"#VALUE!"}},{"$f":"IF(V54=\"\",\"\",SUM(X54:X57))","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+IF('Unos podataka'!$AB$11=\"\",\"\",\"ISKAZ ARMATURE  ZA:\")","v":"ISKAZ ARMATURE  ZA:"},{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",\"\",+'Unos podataka'!$AB$5)","v":3},{"$f":"IF(K60=\"\",\"\",+IF(K60=1,\"KONTRAFORU\",IF(K60<5,\"KONTRAFORE\",\"KONTRAFORA\")))","v":"KONTRAFORE"},null,null,null,null,null,null,null,null,{"$f":"+IF(V60=\"\",\"\",\"duljina kontrafore  l=\")","v":"duljina kontrafore  l="},{"$f":"IF(K60=\"\",\"\",+'Unos podataka'!AB4)","v":1},{"$f":"+IF(K60=\"\",\"\",\"m\")","v":"m"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!A571","v":1.05},{"$f":"+'Analiza i dimenzioniranje'!B571","v":0.05}]
["Poz.",null,"vrsta armature",null,"f ili oznaka mreže",null,"OBLIK ARMATURE",null,null,null,null,null,null,null,null,null,null,null,null,"m'/kom \nili kom","kom/m'  ili kom a'  rebru","Ukupno kom","Ukupno kg",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!A572","v":4.8600021999999994},{"$f":"+'Analiza i dimenzioniranje'!B572","v":0.54310345350772504}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"šipka","mreža",{"$f":"+IF(E63=8,$AR$5,IF(E63=10,$AR$6,IF(E63=12,$AR$7,IF(E63=14,$AR$8,IF(E63=16,$AR$9,IF(E63=18,$AR$10,AR$11))))))","v":1.242},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"l=",{"$f":"+SQRT((AT61-AT60)^2+(AU61-AU60)^2)","v":3.8417792466337888}]
[{"$f":"+IF(K60=\"\",\"\",\"1'\")","v":"1'"},null,{"$f":"+IF(K60=\"\",\"\",\"šipka\")","v":"šipka"},null,{"$f":"IF($K$60=\"\",\"\",+E4)","v":14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+K64","v":1.48},{"$f":"IF(A63=\"\",\"\",+U4)","v":{"$error":"#VALUE!"}},{"$f":"IF(K60=\"\",\"\",+U63*K60)","v":{"$error":"#VALUE!"}},{"$f":"IF(E63>100,\"\",+T63*V63*Y62)","v":{"$error":"#VALUE!"}},{"$f":"+IF(C63=\"MA\",V63*Y62,\"\")","v":""},{"$f":"+IF(E63=283,AJ39,IF(E63=335,AJ40,IF(E63=378,AJ41,IF(E63=385,AJ42,IF(E63=424,AJ43,IF(E63=503,AJ44,IF(E63=524,AJ45,IF(E63=636,AJ46,IF(E63=785,AJ47,\"\")))))))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poz 2'"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(A63=\"\",\"\",+'Analiza i dimenzioniranje'!D83+40*'Analiza i dimenzioniranje'!C428/1000)","v":1.48},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(E65=8,$AR$5,IF(E65=10,$AR$6,IF(E65=12,$AR$7,IF(E65=14,$AR$8,IF(E65=16,$AR$9,IF(E65=18,$AR$10,AR$11))))))","v":1.242},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!A568","v":1.05},{"$f":"+'Analiza i dimenzioniranje'!B568","v":1.1399999999999999}]
[{"$f":"+IF(K60=\"\",\"\",\"2'\")","v":"2'"},null,{"$f":"+IF(K60=\"\",\"\",\"šipka\")","v":"šipka"},null,{"$f":"IF($K$60=\"\",\"\",+E7)","v":14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+K66","v":1.48},{"$f":"+U63","v":{"$error":"#VALUE!"}},{"$f":"+V63","v":{"$error":"#VALUE!"}},{"$f":"IF(E65>100,\"\",+T65*V65*Y64)","v":{"$error":"#VALUE!"}},{"$f":"+IF(C65=\"MA\",V65*Y64,\"\")","v":""},{"$f":"+IF(E65=283,AJ39,IF(E65=335,AJ40,IF(E65=378,AJ41,IF(E65=385,AJ42,IF(E65=424,AJ43,IF(E65=503,AJ44,IF(E65=524,AJ45,IF(E65=636,AJ46,IF(E65=785,AJ4944,\"\")))))))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!A569","v":4.8500021999999996},{"$f":"+'Analiza i dimenzioniranje'!B569","v":1.1399999999999999}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(A63=\"\",\"\",+'Analiza i dimenzioniranje'!D83+40*'Analiza i dimenzioniranje'!C428/1000)","v":1.48},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(E67=8,$AR$5,IF(E67=10,$AR$6,IF(E67=12,$AR$7,IF(E67=14,$AR$8,IF(E67=16,$AR$9,IF(E67=18,$AR$10,AR$11))))))","v":0.63300000000000001},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"l=",{"$f":"+SQRT((AT65-AT64)^2+(AU65-AU64)^2)","v":3.8000021999999998}]
[{"$f":"+IF(K60=\"\",\"\",\"3'\")","v":"3'"},null,{"$f":"+IF(K60=\"\",\"\",\"šipka\")","v":"šipka"},null,{"$f":"IF(K60=\"\",\"\",+E10)","v":10},null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+'Analiza i dimenzioniranje'!C568-'Analiza i dimenzioniranje'!C569)","v":0.99999999999999978},null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+K67+J70+I68)","v":3.0999999999999996},{"$f":"IF(A67=\"\",\"\",IF(E67>100,4,+U63))","v":{"$error":"#VALUE!"}},{"$f":"IF(K60=\"\",\"\",+U67*K60)","v":{"$error":"#VALUE!"}},{"$f":"IF(K60=\"\",\"\",+T67*V67*Y66)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poz 3' "]
[null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+'Analiza i dimenzioniranje'!E52-2*'Analiza i dimenzioniranje'!B315/100)","v":1.0999999999999999},null,null,null,null,null,null,{"$f":"+IF(A67=\"\",\"\",\"a\")","v":"a"},{"$f":"+IF(A67=\"\",\"\",\"3=\")","v":"3="},{"$f":"IF(K60=\"\",\"\",+AU74)","v":90},{"$f":"+IF(A67=\"\",\"\",\"°\")","v":"°"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C568-0.5","v":1.5499999999999998},{"$f":"+'Analiza i dimenzioniranje'!D568+0.01-2*'Analiza i dimenzioniranje'!B315/100","v":1.0499999999999998}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(A67=\"\",\"\",\"b\")","v":"b"},{"$f":"+IF(A67=\"\",\"\",\"3=\")","v":"3="},{"$f":"IF(K60=\"\",\"\",+AU73)","v":82.694244543359446},{"$f":"+IF(A67=\"\",\"\",\"°\")","v":"°"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C569-0.5","v":0.55000000000000004},{"$f":"+AU68","v":1.0499999999999998}]
[null,null,null,null,null,null,null,null,null,{"$f":"+K67","v":0.99999999999999978},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(E71=8,$AR$5,IF(E71=10,$AR$6,IF(E71=12,$AR$7,IF(E71=14,$AR$8,IF(E71=16,$AR$9,IF(E71=18,$AR$10,AR$11))))))","v":0.40500000000000003},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C570-0.5","v":0.55000000000000004},{"$f":"+'Analiza i dimenzioniranje'!D570","v":0.05}]
[{"$f":"+IF(K60=\"\",\"\",\"6'\")","v":"6'"},null,{"$f":"+IF(K60=\"\",\"\",\"šipka\")","v":"šipka"},null,{"$f":"IF($K$60=\"\",\"\",+E22)","v":8},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+L72","v":0.9},{"$f":"IF(K60=\"\",\"\",+IF('Analiza i dimenzioniranje'!A82=\"\",0,+'Analiza i dimenzioniranje'!K569))","v":9},{"$f":"IF(K60=\"\",\"\",+U71*K60)","v":27},{"$f":"IF(K60=\"\",\"\",+T71*V71*Y70)","v":9.8415000000000017},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C571-0.5","v":1.5499999999999998},{"$f":"+'Analiza i dimenzioniranje'!D571","v":0.17820505588432745}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+'Unos podataka'!AB4-2*'Unos podataka'!C99/100)","v":0.9},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"l=",{"$f":"+SQRT((AT71-AT70)^2+(AU71-AU70)^2)","v":1.0081847729232489}]
[{"$f":"+IF(K60=\"\",\"\",\"14\")","v":"14"},null,{"$f":"+IF(K60=\"\",\"\",\"mreža Q\")","v":"mreža Q"},null,{"$f":"+IF(K60=\"\",\"\",335)","v":335},null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+'Analiza i dimenzioniranje'!G577-'Analiza i dimenzioniranje'!G576)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+AW89)","v":{"$error":"#VALUE!"}},{"$f":"IF(V60=\"\",\"\",2*AW89)","v":{"$error":"#VALUE!"}},{"$f":"IF(K60=\"\",\"\",+U73*K60)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(K60=\"\",\"\",+V73*Y73)","v":{"$error":"#VALUE!"}},{"$f":"+IF(E73=283,'Analiza i dimenzioniranje'!$W$427,IF(E73=335,'Analiza i dimenzioniranje'!$W$428,IF(E73=378,'Analiza i dimenzioniranje'!$W$429,IF(E73=385,'Analiza i dimenzioniranje'!$W$430,IF(E73=424,'Analiza i dimenzioniranje'!$W$431,IF(E73=503,'Analiza i dimenzioniranje'!$W$432,IF(E73=524,'Analiza i dimenzioniranje'!$W$433,IF(E73=636,'Analiza i dimenzioniranje'!$W$434,IF(E73=785,'Analiza i dimenzioniranje'!$W$435,\"\")))))))))","v":43.99},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"a3 =",{"$f":"90+ATAN('Analiza i dimenzioniranje'!E60/'Analiza i dimenzioniranje'!E52)*180/(PI())-'Analiza i dimenzioniranje'!F217","v":82.694244543359446}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"b3 =",{"$f":"90-ATAN('Analiza i dimenzioniranje'!E60/'Analiza i dimenzioniranje'!E52)*180/(PI())","v":90}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poz.14",null,"Koordinate točaka"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(K81)*N77","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!G574","v":1.5500010000000002},{"$f":"+AU80","v":1.22},"x","y"]
[null,null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+AU78-AU76-0.5)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"IF(K60=\"\",\"\",+AU82)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"6*2.15","v":12.899999999999999},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!G575","v":1.5500010000000002},{"$f":"+'Analiza i dimenzioniranje'!H575","v":1.65},{"$f":"+AT76","v":1.5500010000000002},1.22]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(A73=\"\",\"\",\"a\")","v":"a"},{"$f":"+IF(A73=\"\",\"\",\"14=\")","v":"14="},{"$f":"+IF(K60=\"\",\"\",90)","v":90},{"$f":"+IF(A73=\"\",\"\",\"°\")","v":"°"},null,null,null,null,null,null,{"$f":"+IF(Z77>1.2*Z76,1,2)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!G576","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!H576","v":{"$error":"#VALUE!"}},1.5500010000000002,1.65]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(A73=\"\",\"\",\"b\")","v":"b"},{"$f":"+IF(A73=\"\",\"\",\"14=\")","v":"14="},{"$f":"IF(K60=\"\",\"\",90-ATAN(1/'Analiza i dimenzioniranje'!E56)*180/PI())","v":{"$error":"#VALUE!"}},{"$f":"+IF(A73=\"\",\"\",\"°\")","v":"°"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!G577","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!H577","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(A73=\"\",\"\",\"g\")","v":"g"},{"$f":"+IF(A73=\"\",\"\",\"14=\")","v":"14="},{"$f":"IF(K60=\"\",\"\",+AU83)","v":{"$error":"#VALUE!"}},{"$f":"+IF(A73=\"\",\"\",\"°\")","v":"°"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!G578","v":4.1500010999999999},{"$f":"+'Analiza i dimenzioniranje'!H578","v":1.22},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,{"$f":"+IF(K60=\"\",\"\",0.5)","v":0.5},null,{"$f":"IF(K60=\"\",\"\",+AT80-AT76)","v":2.6000000999999999},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(E82=8,$AR$5,IF(E82=10,$AR$6,IF(E82=12,$AR$7,IF(E82=14,$AR$8,IF(E82=16,$AR$9,IF(E82=18,$AR$10,AR$11))))))","v":0.91100000000000003},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!G579","v":1.5500010000000002},{"$f":"+'Analiza i dimenzioniranje'!H579","v":1.22},4.1500010999999999,1.22]
[{"$f":"+IF(K60=\"\",\"\",15)","v":15},null,{"$f":"+IF(K60=\"\",\"\",\"šipka\")","v":"šipka"},null,{"$f":"IF(K60=\"\",\"\",+E18)","v":12},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",IF('Analiza i dimenzioniranje'!A82=\"\",0,+J83*2+L85))","v":3.55},{"$f":"IF(K60=\"\",\"\",+'Analiza i dimenzioniranje'!K607)","v":7},{"$f":"IF(K60=\"\",\"\",+U82*K60)","v":21},{"$f":"IF(K60=\"\",\"\",+T82*V82*Y81)","v":67.915049999999994},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"l=",{"$f":"+SQRT((AT80-AT79)^2+(AU80-AU79)^2)","v":{"$error":"#VALUE!"}},1.5500010000000002,1.22]
[null,null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+'Analiza i dimenzioniranje'!B588-'Analiza i dimenzioniranje'!B587)","v":1.7},null,null,null,{"$f":"+J83","v":1.7},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"g14=",{"$f":"180+ATAN((AT77-AT78)/(AU78-AU77))*180/PI()","v":{"$error":"#VALUE!"}},{"$f":"+MAX(AV77:AV82)","v":{"$error":"#VALUE!"}},{"$f":"+MAX(AW77:AW82)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poz.17",null,"    Površina Poz 14."]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+'Analiza i dimenzioniranje'!D86-2*'Unos podataka'!$C$99/100)","v":0.15},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(E86=8,$AR$5,IF(E86=10,$AR$6,IF(E86=12,$AR$7,IF(E86=14,$AR$8,IF(E86=16,$AR$9,IF(E86=18,$AR$10,AR$11))))))","v":0.91100000000000003},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!A638","v":4.8500021999999996},{"$f":"+'Analiza i dimenzioniranje'!B638","v":0.56130921946894219},"Q mreža=",{"$f":"5.1*2.15","v":10.964999999999998},"m2"]
[{"$f":"+IF(K60=\"\",\"\",16)","v":16},null,{"$f":"+IF(K60=\"\",\"\",\"šipka\")","v":"šipka"},null,{"$f":"+IF(K60=\"\",\"\",12)","v":12},null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+'Analiza i dimenzioniranje'!F588-'Analiza i dimenzioniranje'!F587)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+L86+J87+L88)","v":{"$error":"#VALUE!"}},{"$f":"IF(K60=\"\",\"\",+U101)","v":{"$error":"#VALUE!"}},{"$f":"+IF(K60=\"\",\"\",+U86*K60)","v":{"$error":"#VALUE!"}},{"$f":"+IF(K60=\"\",\"\",T86*V86*Y85)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!A639","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!B639","v":{"$error":"#VALUE!"}},"R mreža=",{"$f":"6*2.15","v":12.899999999999999},"m2"]
[null,null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+'Unos podataka'!$AB$6-2*'Unos podataka'!$C$99/100)","v":0.15},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!A640","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!B640","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(K60=\"\",\"\",0.5)","v":0.5},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(E89=8,$AR$5,IF(E89=10,$AR$6,IF(E89=12,$AR$7,IF(E89=14,$AR$8,IF(E89=16,$AR$9,IF(E89=18,$AR$10,AR$11))))))","v":0.91100000000000003},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!A641","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!B641","v":{"$error":"#VALUE!"}},"  A=",{"$f":"-0.5*((AV77*AW78-AV78*AW77)+(AV78*AW79-AV79*AW78)+(AV79*AW80-AV80*AW79)+(AV80*AW81-AV81*AW80)+(AV81*AW82-AV82*AW81))*1.2","v":{"$error":"#VALUE!"}},"m2"]
[{"$f":"+IF(K60=\"\",\"\",17)","v":17},null,{"$f":"+IF(K60=\"\",\"\",\"šipka\")","v":"šipka"},null,{"$f":"+IF(K60=\"\",\"\",12)","v":12},null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+AT87-AT88)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",IF('Analiza i dimenzioniranje'!A82=\"\",0,+K89+K92+L94))","v":{"$error":"#VALUE!"}},{"$f":"IF(K60=\"\",\"\",IF('Analiza i dimenzioniranje'!A82=\"\",0,+U95*V60))","v":3},{"$f":"IF(K60=\"\",\"\",+U89*K60)","v":9},{"$f":"IF(K60=\"\",\"\",+T89*V89*Y88)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poz.18",null,null,{"$f":"ROUNDUP(AW88/AW85,0)","v":{"$error":"#VALUE!"}},"kom"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",0,+'Analiza i dimenzioniranje'!A655-0.03)","v":2.0500010000000004},{"$f":"IF(K60=\"\",\"\",+'Analiza i dimenzioniranje'!B661)","v":0.20320505588432747},null,null,"kom"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(A89=\"\",\"\",\"a\")","v":"a"},{"$f":"+IF(A86=\"\",\"\",\"17=\")","v":"17="},{"$f":"IF(K60=\"\",\"\",90+ATAN(1/'Analiza i dimenzioniranje'!$H$581)*180/PI())","v":{"$error":"#VALUE!"}},{"$f":"+IF(A89=\"\",\"\",\"°\")","v":"°"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(V60=\"\",0,+'Analiza i dimenzioniranje'!A656)","v":1.5500010000000002},{"$f":"IF(K60=\"\",\"\",+'Analiza i dimenzioniranje'!B655)","v":0.13461530867854385}]
[null,null,"RA",null,12,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+SQRT((AT86-AT87)^2+(AU87-AU86)^2))","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+IF(A89=\"\",\"\",\"b\")","v":"b"},{"$f":"+IF(A89=\"\",\"\",\"17=\")","v":"17="},{"$f":"IF(K60=\"\",\"\",90+ATAN(1/'Analiza i dimenzioniranje'!$H$581)*180/PI()-'Analiza i dimenzioniranje'!F217)","v":{"$error":"#VALUE!"}},{"$f":"+IF(A89=\"\",\"\",\"°\")","v":"°"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",0,+'Analiza i dimenzioniranje'!A657)","v":1.5500010000000002},{"$f":"IF(K60=\"\",\"\",+'Analiza i dimenzioniranje'!B657)","v":1.65}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",0,+'Analiza i dimenzioniranje'!A658)","v":{"$error":"#VALUE!"}},{"$f":"IF(K60=\"\",\"\",+'Analiza i dimenzioniranje'!B658)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+AT85-AT86)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(E95=8,$AR$5,IF(E95=10,$AR$6,IF(E95=12,$AR$7,IF(E95=14,$AR$8,IF(E95=16,$AR$9,IF(E95=18,$AR$10,AR$11))))))","v":0.91100000000000003},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",0,+'Analiza i dimenzioniranje'!A659)","v":{"$error":"#VALUE!"}},{"$f":"IF(K60=\"\",\"\",+'Analiza i dimenzioniranje'!B659)","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(K60=\"\",\"\",18)","v":18},null,{"$f":"+IF(K60=\"\",\"\",\"šipka\")","v":"šipka"},null,{"$f":"IF(K60=\"\",\"\",+'Analiza i dimenzioniranje'!C428)","v":12},null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+AT94-AT93)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+IF('Analiza i dimenzioniranje'!A82=\"\",0,L95+J97+I99+J100))","v":{"$error":"#VALUE!"}},{"$f":"IF(A95=\"\",\"\",+('Analiza i dimenzioniranje'!D86-'Analiza i dimenzioniranje'!B290/100)/0.1+1)","v":3},{"$f":"IF(K60=\"\",\"\",+U95*K60)","v":9},{"$f":"IF(K60=\"\",\"\",+T95*V95*Y94)","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+AU93-AU92)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+IF(A95=\"\",\"\",\"a\")","v":"a"},{"$f":"+IF(A95=\"\",\"\",\"18=\")","v":"18="},{"$f":"IF(K60=\"\",\"\",90+ATAN((J97-I99)/'Analiza i dimenzioniranje'!J585)*180/PI())","v":{"$error":"#VALUE!"}},{"$f":"+IF(A95=\"\",\"\",\"°\")","v":"°"}]
[null,null,"RA",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(A95=\"\",\"\",\"b\")","v":"b"},{"$f":"+IF(A95=\"\",\"\",\"18=\")","v":"18="},{"$f":"IF(K60=\"\",\"\",180-ATAN((AT93-AT92)/(AU93-AU92))*180/PI())","v":{"$error":"#VALUE!"}},{"$f":"+IF(A95=\"\",\"\",\"°\")","v":"°"}]
[null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+AU92-AU91)","v":1.5153846913214561},null,null,null,null,null,null,{"$f":"+IF(A95=\"\",\"\",\"g\")","v":"g"},{"$f":"+IF(A95=\"\",\"\",\"18=\")","v":"18="},{"$f":"IF(K60=\"\",\"\",90-'Analiza i dimenzioniranje'!F217)","v":82.694244543359446},{"$f":"+IF(A95=\"\",\"\",\"°\")","v":"°"}]
[null,null,null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",+AT90-AT91)","v":0.50000000000000022},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(E101=8,$AR$5,IF(E101=10,$AR$6,IF(E101=12,$AR$7,IF(E101=14,$AR$8,IF(E101=16,$AR$9,IF(E101=18,$AR$10,AR$11))))))","v":0.91100000000000003}]
[{"$f":"+IF(K60=\"\",\"\",19)","v":19},null,{"$f":"+IF(K60=\"\",\"\",\"šipka\")","v":"šipka"},null,{"$f":"+IF(K60=\"\",\"\",12)","v":12},null,null,null,null,null,null,{"$f":"+L86","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"IF(K60=\"\",\"\",IF('Analiza i dimenzioniranje'!A82=\"\",0,+L101+N102+L103))","v":{"$error":"#VALUE!"}},{"$f":"IF(K60=\"\",\"\",+'Analiza i dimenzioniranje'!L627)","v":{"$error":"#VALUE!"}},{"$f":"IF(K60=\"\",\"\",+U101*K60)","v":{"$error":"#VALUE!"}},{"$f":"IF(K60=\"\",\"\",+T101*V101*Y100)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+J87","v":0.15}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+L101","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(K60=\"\",\"\",\"Ukupno kontrafore:\")","v":"Ukupno kontrafore:"},"        S (kg)",null,{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",0,SUM(W61:W103))","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!A82=\"\",0,IF(X78=\"?\",\"?\",SUM(X63:X101)))","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SVEUKUPNO:","        S (kg)",null,{"$f":"+W104+W53","v":{"$error":"#VALUE!"}},{"$f":"+X104+X53","v":{"$error":"#VALUE!"}}]
["Napomena: Kada nema kontrafora i sidara, ne treba printati dio stranice 1 i stranicu 2. Za to treba postupiti po donjim uputama:"]
["    ZID BEZ KONTRAFORA:             Kliknite na \"View\" zatim \"Page Break Preview\" (Ispod Home) a zatim postavite \"Mouse\"  \n  na liniju  između redova 105 i 106 i podignite plavu liniju ispod reda 59.\n    \n   ZID BEZ SIDARA I KONZOLE:    Ponovite postupak i podignite liniju ispod reda 53."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]

{"sheet":"Dopušteno","index":13,"n_rows":88,"n_cols":24,"rows_kept":88,"cut":false,"hidden":true,"merged":[[23,14,24,14],[26,13,27,13],[27,1,27,2],[29,11,29,12],[5,13,6,13],[10,5,10,6],[20,11,20,12],[21,12,22,12],[23,12,24,12],[5,12,6,12]]}
[]
["MJERODAVNI PRORAČUN",null,null,null,null,null,null,null,null,null,null,null,"Shema opterećenja"]
[null,null,null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null," y"]
[null,null,null,"     j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18},"°            Hx =",0,"kN                 j'=",{"$f":"ATAN(TAN(E5*3.14159/180)/E14)*180/3.14159","v":14.5707680719339},"°        ex=",null,3,"L  ",null,1,{"$f":"IF(G9=0,E9,+E9-ABS(2*P19))","v":{"$error":"#VALUE!"}}]
[null,null,"          ","       c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"kPa       Hy =",{"$f":"+'Analiza i dimenzioniranje'!B167*E9","v":{"$error":"#VALUE!"}},"kN                c' =",{"$f":"E6/E15","v":20},"kPa    ey=",null,null,"      Hy ","Hx","        x  ",{"$f":"IF(G9=0,E8,+E8-ABS(2*P20))","v":{"$error":"#VALUE!"}}]
[null,null,"q=g*Df","g =",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"kN/m3     Mx =",{"$f":"V28*E9","v":{"$error":"#VALUE!"}},"kNm",null,"           L'=",null,"  B",null,null,"                     ",{"$f":"I5*3.14159/180","v":0.2543076625950379}]
[null,null,null,"   kraća stranica u smjer osi (y)    B =",{"$f":"+MT!G13","v":3.1500021999999994},"m          My =",0,"kNm             H =",{"$f":"SQRT(G5*G5+G6*G6)","v":{"$error":"#VALUE!"}},"kN      B'=",null,null,null,null,"   + Mx"]
[null,null,null,"      dulja stranica u smjeru osi(x)    L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m            V =",{"$f":"+V26*E9","v":{"$error":"#VALUE!"}},"kN                V =",{"$f":"IF(K3=2,G9,G9+E8*E9*E11*24)","v":{"$error":"#VALUE!"}},"kPa  FMr=",null,4," ",null,2,null,null,null,null,null,"MJERODAVNI PRORAČUN"]
[null,null,null," dubina temeljenja    Df =",{"$f":"+'Analiza i dimenzioniranje'!E52+'Analiza i dimenzioniranje'!E65","v":1.5000009999999999},"m"," ","     Mx =",{"$f":"IF(K3=2,G7-G9*G13,G7-G9*G13+G6*E11)","v":{"$error":"#VALUE!"}},"kNm  Al=",null,null,null,"  +My",null,null,null,null,null,null,"Gtem ..........................",{"$f":"+'Analiza i dimenzioniranje'!B135","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C135","v":{"$error":"#VALUE!"}},{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!X10,'Dopušteno Vs-'!X10)","v":{"$error":"#VALUE!"}}]
[null,null,null,"  visina temelja    ht =",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m   ",null,"     My =",{"$f":"IF(K3=2,G8+G9*G12,+G9*G12+G5*E11)","v":{"$error":"#VALUE!"}},"kNm   iq=",null,null,"Kontaktni naponi",null,null,null,null,null,null,null,"Gzid+konz ...................",{"$f":"+'Analiza i dimenzioniranje'!B136","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C136","v":{"$error":"#VALUE!"}},{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!X11,'Dopušteno Vs-'!X11)","v":{"$error":"#VALUE!"}}]
[null,null,null,"   nagib dna temelja    a =",{"$f":"ATAN(Q30)*180/PI()","v":7.3057554566405489},"°        ex° =",0,"    pa =",{"$f":"D68","v":{"$error":"#VALUE!"}},"kPa    ig=",null,null,"s1=   ",{"$f":"+(N16+I11/N17+I10/N18)","v":{"$error":"#VALUE!"}},"KPa ",null,"ic",null,null,null,"Grebra kontrafora ............",{"$f":"+'Analiza i dimenzioniranje'!B137","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C137","v":{"$error":"#VALUE!"}},{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!X12,'Dopušteno Vs-'!X12)","v":{"$error":"#VALUE!"}}]
[null,null,"Ako nema vode g'=g","g' =",{"$f":"+'Analiza i dimenzioniranje'!H18","v":10},"kN/m3  ey°=",0,"    Vdop=",{"$f":"I12*P5*P6","v":{"$error":"#VALUE!"}},"kN      ic=",null,null,"s2=   ",{"$f":"N16+I11/N17-I10/N18","v":{"$error":"#VALUE!"}},"KPa ",null,"ig",null,null,null,"Gnasip na konzoli ............",{"$f":"+'Analiza i dimenzioniranje'!B138","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C138","v":{"$error":"#VALUE!"}},{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!X13,'Dopušteno Vs-'!X13)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"I5*3.14159/180","v":0.2543076625950379},"Faktori:","     gj =",{"$f":"+'Analiza i dimenzioniranje'!M27","v":1.25},null,null,null,null,null,null,null,"s3=   ",{"$f":"N16-I11/N17+I10/N18","v":{"$error":"#VALUE!"}},"KPa ",null,null,null,null,null,"Gnasipa iza zida .............",{"$f":"+'Analiza i dimenzioniranje'!B139","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C139","v":{"$error":"#VALUE!"}},{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!X14,'Dopušteno Vs-'!X14)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"45*PI()/180","v":0.78539816339744828},{"$f":"B15+B17","v":0.91255199469496717},"      gc =",{"$f":"+'Analiza i dimenzioniranje'!M28","v":1.25},{"$f":"IF(E14*P17>10,\"Fkl >\",\"Fkl =\")","v":{"$error":"#VALUE!"}},{"$f":"IF(E14*P17>10,10,R16)","v":{"$error":"#VALUE!"}},{"$f":"B16*B16","v":1.672279875125072},{"$f":"TAN(B14)","v":0.25993552228740757},{"$f":"3.14159*I15","v":0.81661083746289675},null,null,"s4=   ",{"$f":"N16-I11/N17-I10/N18","v":{"$error":"#VALUE!"}},"KPa ",{"$f":"IF(P5<P6,P5,P6)","v":{"$error":"#VALUE!"}},null,null,null,null,"Gnasipa ispred zida .........",{"$f":"+'Analiza i dimenzioniranje'!B140","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C140","v":{"$error":"#VALUE!"}},{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!X15,'Dopušteno Vs-'!X15)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"TAN(C15)","v":1.293166607643838},"     Ng=",{"$f":"2*(H16-1)*TAN(I5*PI()/180)","v":1.4473558577295844},"      Nc=",{"$f":"(H16-1)/I15","v":10.710596970300873},"      Nq=",{"$f":"EXP(J15)*H15","v":3.7840646174850825},null,null,null,null,"     V/F=",{"$f":"I9/(E9*E8)","v":{"$error":"#VALUE!"}},"KN/m2",{"$f":"P5*P6","v":{"$error":"#VALUE!"}},"A'",{"$f":"IF(P17<1,\"temelj klizi\",E14*P17)","v":{"$error":"#VALUE!"}},null,null,"PPrometno ...................",{"$f":"+'Analiza i dimenzioniranje'!B141","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C141","v":{"$error":"#VALUE!"}},{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!X16,'Dopušteno Vs-'!X16)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"B14/2","v":0.12715383129751895},"Tekst:"," za stalno + dopunsko  opterećenje",null,null,null,null,null," ",null,null,"      Wy=",{"$f":"E9*E9*E8/6","v":75.600052799999986},"m3",{"$f":"IF(I8=0,100,TAN(I5*3.14159/180)*G9/I8)","v":{"$error":"#VALUE!"}},null,null,null,null,"PTočkasto ....................",{"$f":"+'Analiza i dimenzioniranje'!B142","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C142","v":{"$error":"#VALUE!"}},{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!X17,'Dopušteno Vs-'!X17)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"Q18","v":{"$error":"#VALUE!"}},{"$f":"IF(N15<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(N14<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(N12<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(N13<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}},null,null,null,"      Wx=",{"$f":"E9*E8*E8/6","v":19.845027720009671},"m3",null,{"$f":"IF((((P19/E9)*(P19/E9))+((P20/E8)*(P20/E8)))>=0.11111,\"PROMJENA DIMENZIJA TEMELJA\",((P19/E9)*(P19/E9))+((P20/E8)*(P20/E8)))","v":{"$error":"#VALUE!"}},null,null,null,"PLinijsko ......................",{"$f":"+'Analiza i dimenzioniranje'!B143","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C143","v":{"$error":"#VALUE!"}},{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!X18,'Dopušteno Vs-'!X18)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"G8/G9+G12","v":{"$error":"#VALUE!"}},"ex",null,null,null,"QTemelj ili vozilo.....................",{"$f":"+'Analiza i dimenzioniranje'!B144","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C144","v":{"$error":"#VALUE!"}},{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!X19,'Dopušteno Vs-'!X19)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-(G7/G9)+G13","v":{"$error":"#VALUE!"}},"ey",null,null,null,"VSidro ........................",{"$f":"+'Analiza i dimenzioniranje'!B145","v":25.881904536133977},{"$f":"+'Analiza i dimenzioniranje'!C145","v":{"$error":"#VALUE!"}},{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!X20,'Dopušteno Vs-'!X20)","v":{"$error":"#VALUE!"}}]
[null,"                  P R O J E K T N A   O T P O R N O S T     T L A    ",null,null,null,null,null,{"$f":"+D17","v":" za stalno + dopunsko  opterećenje"},null,null,null,null,null,null,null,null,null,null,null,null,"Ev1 ...........................",{"$f":"+'Analiza i dimenzioniranje'!B146","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C146","v":{"$error":"#VALUE!"}},{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!X21,'Dopušteno Vs-'!X21)","v":{"$error":"#VALUE!"}}]
[null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ev2  ..........................",{"$f":"+'Analiza i dimenzioniranje'!B147","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C147","v":{"$error":"#VALUE!"}},{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!X22,'Dopušteno Vs-'!X22)","v":{"$error":"#VALUE!"}}]
[null," Proračun projektne otpornosti tla provodi se prema EUROCODU 7, prema izrazu:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ev3  ..........................",{"$f":"+'Analiza i dimenzioniranje'!B148","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C148","v":{"$error":"#VALUE!"}},{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!X23,'Dopušteno Vs-'!X23)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vpotres (vert.sila)........................",0,{"$f":"+'Analiza i dimenzioniranje'!C149","v":0},1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Uzgon ….......................",{"$f":"+'Analiza i dimenzioniranje'!B150","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C150","v":{"$error":"#VALUE!"}},{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!X26,'Dopušteno Vs-'!X26)","v":{"$error":"#VALUE!"}}]
[null,null,"  pa=R/A'= c' *Nc*bc*sc*ic+q' *Nq*bq*sq*iq+0,5*g' *B' *Ng*bg*sg*ig",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"V=",{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!V26,'Dopušteno Vs-'!V26)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"M=",{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!V27,'Dopušteno Vs-'!V27)","v":{"$error":"#VALUE!"}}]
[null,"gdje je:",null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     Ms =",{"$f":"+IF('Dopušteno Vs+'!$H$87>'Dopušteno Vs-'!$H$87,'Dopušteno Vs+'!V28,'Dopušteno Vs-'!V28)","v":{"$error":"#VALUE!"}},"kNm/m'"]
[null,"g.........................................",null,"prostorna efektivna težina"]
[null,"B'.............................................",null,"širina temelja (efektivna)",null,null,null,null,null,null,null,null,null,null,null,"tana=",{"$f":"+('Analiza i dimenzioniranje'!E52-'Analiza i dimenzioniranje'!E51)/('Analiza i dimenzioniranje'!E61+Kontrafore!$E$3)","v":0.12820505588432746}]
[null,"Nc, Nq, Ng................................",null,"faktori nosivosti"]
[null,"ic, iq, ig ...................................",null,"faktori nagiba opterećenja"]
[null,"sc,sq, sg .......................................",null,"faktori oblika temelja"]
[null,"bc,bq, bg  ..............................................",null,"faktori nagiba dna temelja"]
[null,"c',j'  .........................................................",null,"mobilizirani parametri čvrstoće tla"]
[null,"dc .........................................",null,"faktor dubine temeljenja"]
[null,"q ...............................................",null,"opterećenje tla u razini temeljenja"]
[null,"A ...........................................",null,"reducirana površina temelja"]
[]
[]
[null,"Karakteristike tla:",null,null,null,"           Dimenzije temelja:"]
[]
[null,"      j =",{"$f":"E5","v":18},"°  ",null,"     B =",{"$f":"E8","v":3.1500021999999994},"m (širina temelja)"]
[null,"       c =",{"$f":"E6","v":25},"kPa",null,"     L =",{"$f":"E9","v":12},"m (dužina temelja)"]
[null,"    g =",{"$f":"E7","v":20},"kN/m3",null,"     Df =",{"$f":"E10","v":1.5000009999999999},"m (dubina temeljenja)"]
[null,null,null,null,null,"a =",{"$f":"+E12","v":7.3057554566405489},"o   (kut nagiba temelja)"]
[]
[null,"Parcijalni faktori svojstava tla:"]
[null,null," "]
[null,"   gj =",{"$f":"E14","v":1.25},"    gc =",{"$f":"E15","v":1.25}]
[null,null," ",null," "," "," "]
[null,"Mobilizirani parametri čvrstoće tla:"]
[null,null," ",null,null," "," "," "," "]
[null,null,"   tgjm  =  tgj/gj  =",{"$f":"TAN(E5*3.14159/180)/E14","v":0.25993552228740757},"------>  j' =",{"$f":"I5","v":14.5707680719339},"° ----> Nq =  ",{"$f":"+H16","v":3.7840646174850825},"  => FIm=",{"$f":"I5","v":14.5707680719339},"m=mB=",{"$f":"+(2+(P6/P5))/(1+(P6/P5))","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(G5=0,100000,(G6/G5))","v":100000}]
[null,null,"c' = c/gc =",{"$f":"I6","v":20},null," ","    Nc=",{"$f":"F16","v":10.710596970300873},null,null,"m=mL=",{"$f":"+(2+(P5/P6))/(1+(P5/P6))","v":{"$error":"#VALUE!"}},null,{"$f":"ATAN(N54)*180/PI()","v":89.999427042204886}]
[null,null,null,null,null,null,"Ng=",{"$f":"D16","v":1.4473558577295844},null,null,"m=",{"$f":"+L55*N56+L54*N57","v":{"$error":"#VALUE!"}},null,{"$f":"+COS(N55*PI()/180)*COS(N55*PI()/180)","v":9.9999999990320259E-11}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+((1-I8/(I9+P5*P6*I6/TAN(I5*PI()/180))))","v":{"$error":"#VALUE!"}},null,{"$f":"+SIN(N55*PI()/180)*SIN(N55*PI()/180)","v":0.99999999989999999}]
[null,"Faktori :"]
[null,"sq=1+(B'/L')*sinj '=",null,{"$f":"1+(P6/P5)*SIN(I5*PI()/180)","v":{"$error":"#VALUE!"}},"    iq =",{"$f":"POWER(L57,L56)","v":{"$error":"#VALUE!"}},"    bq =",{"$f":"+POWER(J60,2)","v":0.93480999420900812},null,{"$f":"RADIANS(G46)","v":0.1275094870639194}]
[null,"sg = 1 - 0.30*B'/L' =",null,{"$f":"IF(P5<P6,1-0.3*P5/P6,1-0.3*P6/P5)","v":{"$error":"#VALUE!"}},"    ig =",{"$f":"POWER(L57,(L56+1))","v":{"$error":"#VALUE!"}},"    bg =",{"$f":"+H59","v":0.93480999420900812},null,{"$f":"+(1-J59*TAN(I5*PI()/180))","v":0.96685572564318412}]
[null,"sc=(sq*Nq-1)/(Nq-1)=",null,{"$f":"(D59*H54-1)/(H54-1)","v":{"$error":"#VALUE!"}},"    ic =",{"$f":"F59-(1-F59)/(H55*TAN(I5*PI()/180))","v":{"$error":"#VALUE!"}},"    bc =",{"$f":"+H59-(1-H59)/(H55*TAN(I5*PI()/180))","v":0.91139460798908856}]
[null,null,"q=g*Df =",{"$f":"+'Analiza i dimenzioniranje'!C232","v":17.000019999999999},"kPa"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"cos2*teta"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sin2*teta"]
[null,"Projektna otpornost tla za glavno + dopunsko opterećenje iznosi :"]
[]
[null,null,"   pa =",{"$f":"D55*H55*H61*D61*F61+D62*H54*H59*D59*F59+0.5*E13*P6*H56*H60*D60*F60","v":{"$error":"#VALUE!"}},"kPa"]
[]
[]
[]
[]
[]
[null,{"$f":"+IF(K3=1,\"Opterećenje na vrhu temelja:\",\"Opterećenje na dnu temelja\")","v":"Opterećenje na dnu temelja"}]
[]
[null,"       V=",{"$f":"G9","v":{"$error":"#VALUE!"}},"kN  -Vertikalna sila"]
[null,"      Hx=",{"$f":"G5","v":0},"kN   komponenta u smjeru x"]
[null,"      Hy=",{"$f":"G6","v":{"$error":"#VALUE!"}},"kN   komponenta u smjeru y"]
[null,"      Mx=",{"$f":"G7","v":{"$error":"#VALUE!"}},"kNm  moment oko osi x"]
[null,"      My=",{"$f":"G8","v":0},"kNm  moment oko osi y"]
[]
[null,"Reducirana površina temelja:"]
[]
[null,null,"B'=B-2.ey=",{"$f":"P6","v":{"$error":"#VALUE!"}},"m","      DOPUŠTENA VERTIKALNA SILA:"]
[null,null,"        L'=L-2.ex=",{"$f":"P5","v":{"$error":"#VALUE!"}},"m"]
[null,null,"        A' = L'.B' =",{"$f":"P16","v":{"$error":"#VALUE!"}},"m2","    Vdop=",{"$f":"D68*D86/'Analiza i dimenzioniranje'!M38","v":{"$error":"#VALUE!"}},{"$f":"IF(G86>C76,\"kN   >  V  =\",\"kN   <   V =\")","v":{"$error":"#VALUE!"}},{"$f":"+C76","v":{"$error":"#VALUE!"}},"kN"]
[null,null,null,null,null,null,"Iskorištenost:  ",{"$f":"+I86/G86","v":{"$error":"#VALUE!"}},{"$f":"+IF(H87<=100%,\"(Zadovoljava)\",\"(Ne zadovoljava\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,"Priredio: Nikola SAPUNAR, dipl. ing. građ."]

{"sheet":"P III-III","index":14,"n_rows":180,"n_cols":75,"rows_kept":180,"cut":false,"hidden":true,"merged":[[162,1,162,2],[29,10,29,11],[29,38,29,39],[30,10,30,11],[33,10,33,11],[60,10,60,11],[34,10,34,11],[64,11,64,12],[13,38,13,39],[15,10,15,11],[24,10,24,11],[22,38,22,39],[18,38,18,39],[18,10,18,11],[16,38,16,39],[21,38,21,39],[21,10,21,11],[20,10,20,11],[23,10,23,11],[22,10,22,11],[7,38,7,39],[8,10,8,11],[12,10,12,11],[7,10,7,11],[9,10,9,11],[9,38,9,39],[27,38,27,39],[28,10,28,11],[25,10,25,11],[26,10,26,11],[27,10,27,11],[10,47,10,48],[12,38,12,39],[10,50,10,51],[11,10,11,11],[10,10,10,11],[5,35,5,36],[19,10,19,11],[5,21,5,22],[5,26,5,27],[5,29,5,30],[5,32,5,33],[13,10,13,11],[16,10,16,11],[14,10,14,11],[2,0,2,8],[3,0,3,8],[5,0,5,7],[7,0,7,9],[6,0,6,8]]}
[null,null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z18/M18","v":{"$error":"#VALUE!"}}]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  ","krak                  y  ","Moment destabilnosti i stabilnosti","za Mzida                                              krakovi                             x                  y",null,"Moment zida III-III","za M u                           presjeku II-II                                                   krakovi                                x               y",null,"Moment      II-II","za M u                           temelju ispod zida                     krakovi                             x                  y",null,"Moment  ","za M u                           presjeku I-I                                              krakovi                             x                  y",null,"Moment      I-I"]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5},null,null,null,{"$f":"2+E57-E54-E51/2","v":3.8000010999999998},{"$f":"+E48","v":1.2},null,{"$f":"2+E55","v":3.4000010999999999},{"$f":"'C III-V'!AC46+(E48-'C III-V'!AC46)/2","v":0.75384613757397367},null,{"$f":"2+E55+E51/2","v":3.8000010999999998},{"$f":"'C III-V'!AC49","v":0.41025631985540933},null,{"$f":"2+E55+E51","v":4.2000010999999997},{"$f":"'C III-V'!AC49+(E48-'C III-V'!AC49)/2","v":0.8051281599277047}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#VALUE!"}},null,null,{"$f":"+H108","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$W$7","v":{"$error":"#VALUE!"}},{"$f":"+M8*Y8","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$AB$7","v":{"$error":"#VALUE!"}},{"$f":"T8*AB8","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null," Eh1 ....................................................."]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,null,{"$f":"+M9","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$f":"+W9-$AB$7","v":{"$error":"#VALUE!"}},{"$f":"AB9*T9","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null," Eh2 ............................................."," "]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null,null,null,{"$f":"-B110","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"-B110","v":{"$error":"#VALUE!"}}]
[null,null,"GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$f":"+W11-$AB$7","v":{"$error":"#REF!"}},{"$f":"AB11*T11","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null," EPrometno ...................................."," "]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," "]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"},null,null,null,null,null,null,null,null,null," EPLinijsko ................................"]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ...................................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,null,null,null,null,null,null,null,null," EQTemelj ...................................................."]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":2.2699256917793105},null,null,null,null,null,null,{"$f":"+M15","v":2.2699256917793105},null,null,170.21276595744681,null,169.71276595744681,{"$f":"-M15*Y15","v":-385.23536766973763},null,169.01276595744682,383.64641968549216,null,null,null,null,null,null,null,null,null," HSidro ..............................."," "]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":0},null,null,null,null,null,null,0,null,null,0,null,-0.5,0,null,-1.2,0,null,null,null,null,null,null,null,null,null," HPotres ........................................."," "]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"+'Analiza i dimenzioniranje'!D17","v":2},{"$f":"+'Analiza i dimenzioniranje'!E17","v":2.8},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)","voda",null,0,null,null,null,null,null,null,0]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":0},{"$f":"SUM(S8:S17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T8:T17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U8:U17)","v":0},null,null,"x",null,{"$f":"SUM(Z8:Z17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC8:AC17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF8:AF17)","v":0},null,null,{"$f":"SUM(AI8:AI17)","v":0},null,null,{"$f":"SUM(AL8:AL17)","v":0}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M20","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+H127","v":{"$error":"#VALUE!"}},null,{"$f":"+$V$7-V20","v":{"$error":"#VALUE!"}},null,{"$f":"+M20*X20","v":{"$error":"#VALUE!"}},{"$f":"+$AA$7-V20","v":{"$error":"#VALUE!"}},null,{"$f":"+P20*AA20","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null," Gzid+konz ...................................."," "]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli............................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M21","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V21","v":{"$error":"#VALUE!"}},null,{"$f":"+P21*AA21","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null," Gnasip na konzoli............................."," "]
[]
[null,null,"OPTEREĆENJE ZIDA:"]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X24","v":{"$error":"#VALUE!"}},null,{"$f":"+M24*AD24","v":{"$error":"#VALUE!"}},null,null,null,null,null,null," PPrometno ......................."," "]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X25","v":{"$error":"#VALUE!"}},null,{"$f":"+M25*AD25","v":{"$error":"#VALUE!"}},null,null,null,null,null,null," PTočkasto ......................"," "]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X26","v":{"$error":"#VALUE!"}},null,{"$f":"+M26*AD26","v":{"$error":"#VALUE!"}},null,null,null,null,null,null," PLinijsko ........................."," "]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X27","v":{"$error":"#VALUE!"}},null,{"$f":"+M27*AD27","v":{"$error":"#VALUE!"}},null,null,null,null,null,null," QTemelj .............................."," "]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",0.60822475599092374,null,null,{"$f":"+M28","v":0.60822475599092374},null,null,null,null,null,0,null,{"$f":"+$V$7-V28","v":4.9000021999999994},null,2.9803026424499892,{"$f":"+$AA$7-V28","v":3.8000010999999998},null,{"$f":"P28*AA28","v":2.3112547418127418},null,null,null,null,null,null,null,null,null," VSidro .............................."]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M29","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V29","v":{"$error":"#VALUE!"}},null,{"$f":"+P29*AA29","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null," Ev1 ...................................."," "]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M30","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V30","v":{"$error":"#VALUE!"}},null,{"$f":"+P30*AA30","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null," Ev2  .........................."]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m"]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":0},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":0},null,null,null,null,null,null,null,null,{"$f":"SUM(Z19:Z31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC19:AC31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF19:AF31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI19:AI31)","v":0},{"$f":"SUM(AJ19:AJ31)","v":0},{"$f":"SUM(AK19:AK31)","v":0},{"$f":"SUM(AL19:AL31)","v":0}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m"]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"omega"]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,{"$f":"+M32","v":{"$error":"#VALUE!"}},{"$f":"+N32","v":0},{"$f":"+O32","v":{"$error":"#VALUE!"}},{"$f":"+P32","v":{"$error":"#VALUE!"}},{"$f":"+Q32","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," a°","   b°","   b-a","   eta°"]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,"EUROCOD 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BB37=0,0,ATAN(BC37/BB37)*180/PI())","v":0},{"$f":"IF(BB37=0,0,ATAN(BE37/BB37)*180/PI())","v":0},{"$f":"BO37-BN37","v":0},{"$f":"BN37+BP37/2","v":0}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!U40","v":2.35},"kN/m'",null,null,null,null,"Marka betona",15,20,25,30,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AZ38=0,0,ATAN(BA38/AZ38)*180/PI())","v":0},{"$f":"IF(AZ38=0,0,ATAN(BC38/AZ38)*180/PI())","v":0},{"$f":"BM38-BL38","v":0},{"$f":"BL38+BN38/2","v":0}]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"IF(E38=0,0,'Analiza i dimenzioniranje'!E39)","v":15},"°    ",null,null,null,null,"Klasa betona C","12/15","16/20","20/25","25/30","30/37"]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"IF(E38=0,0,+'Analiza i dimenzioniranje'!U42)","v":170.21276595744681},"m",null,null,null,null,"fcm (N/mm2)",20,24,28,33,38]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*C42*'C III-V'!AA136/B42","v":0},"kN/m'",null,null,null,null,"ecu  (%0)",-3.6,-3.5,-3.4,-3.3,-3.2]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'Unos podataka'!H34","v":1},null,null,null,null,null,null,null,"fck valjak (N/mm2)",12,16,20,25,30]
[null,null,"DIMENZIJE ZIDA:",null,null,null,"          GRADIVO TEMELJA I ZIDA:",null,null,null,"fck kocka (N/mm2)",15,20,25,30,37]
[null,null,null,null,null,null,null,null,500,500,"Ecm (N/mm2)",26000,27500,29000,30500,32000]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":6},"m",null,"TEMELJ:",{"$f":"+IF(I46=\"RA\",\"\",IF(M173>7.85,\"KORISTITI  RA\",\"\"))","v":""},null,null,null,null,500]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m",{"$f":"+'Analiza i dimenzioniranje'!H48","v":"C"},{"$f":"IF(H47=20,16,IF(H47=25,20,IF(H47=30,25,IF(H47=37,30,\"?\"))))","v":25},{"$f":"+'Analiza i dimenzioniranje'!H50","v":"šipka"},"B500B"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    ",null,{"$f":"+'Analiza i dimenzioniranje'!I49","v":30},null,560]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m",{"$f":"E47+0.0000000000001","v":4.0000000000001004},"ZID:",{"$f":"IF(I49=\"RA\",\"\",IF(#REF!>7.85,\"KORISTITI  RA\",IF(#REF!>7.85,\"KORISTI  RA\",\"\")))","v":{"$error":"#REF!"}}]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m",{"$f":"+'Analiza i dimenzioniranje'!H52","v":"C"},{"$f":"IF(H50=20,16,IF(H50=25,20,IF(H50=30,25,IF(H50=37,30,\"?\"))))","v":30},{"$f":"+'Analiza i dimenzioniranje'!H54","v":"šipka"},"B500B"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m",null,{"$f":"+'Analiza i dimenzioniranje'!I53","v":37},null,560]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C III-V'!B10-'C III-V'!B11=0,\">100\",IF('C III-V'!C10-'C III-V'!C11/(0.00000000000001+'C III-V'!B11-'C III-V'!B10)>100,\">100\",('C III-V'!C10-'C III-V'!C11)/('C III-V'!B11-'C III-V'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C III-V'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C III-V'!E64","v":1.4000010999999999},"m",{"$f":"+IF(E32=0,\"\",IF(G54>AP88+E36,\"PAZI POLOŽAJ TEMELJA\",\"\"))","v":""}]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zaloge .........................................................................   "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 "]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m",null,null,null,null,"MOMENTI SAVIJANJA (kNm/m')"]
[" zapreminska težina nasipa ...............................",null,null,"      gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,"Moment na koti +",null,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,"M="," -  "]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+#REF!","v":{"$error":"#REF!"}},null,"     v=","+"]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"+#REF!","v":{"$error":"#REF!"}},null,"     h=","-"]
[null,null,{"$f":"IF(I20=0,\"\",+#REF!)","v":{"$error":"#REF!"}},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+'Dijagram momenata'!Q20","v":1.2},null,{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"-'P III-III'!B116*'P III-III'!C116","v":0},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota od dna temlja",null,"krak od presjeka do sile","     v11=",{"$f":"B130+'C III-V'!Z61+'C III-V'!Z76","v":{"$error":"#VALUE!"}}]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c111",{"$f":"IF(+L66-'Dijagram momenata'!$Q$20>0,+L66-'Dijagram momenata'!$Q$20,0)","v":{"$error":"#REF!"}},"     h11=",{"$f":"+B118*E54/E57-B117","v":{"$error":"#VALUE!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c112",{"$f":"IF(+L67-'Dijagram momenata'!$Q$20>0,+L67-'Dijagram momenata'!$Q$20,0)","v":{"$error":"#REF!"}},"     v22=",{"$f":"+B129+B131+B132+B133+B134+B138+'C III-V'!V76+'C III-V'!V61","v":{"$error":"#VALUE!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c113",{"$f":"IF(+L68-'Dijagram momenata'!$Q$20>0,+L68-'Dijagram momenata'!$Q$20,0)","v":{"$error":"#REF!"}},"     h22=",{"$f":"+B118*E55/E57-B110","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c114",{"$f":"IF(+L69-'Dijagram momenata'!$Q$20>0,+L69-'Dijagram momenata'!$Q$20,0)","v":{"$error":"#REF!"}},"     v33=",{"$f":"B127+B128+B135+B136+B137","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     h33=",{"$f":"-B108-B109-B111-B112-B113-B114+B115-B116","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko"," -koeficijent mirnog pritiska",null,null,"     vtem=",{"$f":"+'C III-V'!X61+'C III-V'!X76","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko1=","1-sinj1=",{"$f":"1-SIN(E14*PI()/180)","v":0.62539340658408804},"varijanta","     htem=",{"$f":"+B118*E51/E57","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko2=","1-sinj2=",{"$f":"1-SIN(F14*PI()/180)","v":0.69098300562505255},"n","    MI-I",{"$f":"+K62","v":0}]
[null,null,null,null,null,null,null,null,null,null,"Ko3=","1-sinj3=",{"$f":"1-SIN(G14*PI()/180)","v":0.65797985667433134},null,"MII-II",{"$f":"+L62","v":0}]
[null,null,null,null,null,null,null,null,null,null,"Ko=","n/(1-n) =",{"$f":"+N75/(1-N75)","v":0.66666666666666674},0.4,"Mzida",{"$f":"+M62","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mtem",{"$f":"+AI37","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,"Napomena:"]
[null,null,null,null,null,null,null,null,null,null,"Za crtež u mjerilu 1:50"]
[null,null,null,null,null,null,null,null,null,null,"Apcisa treba biti ukupne duljine 16"]
[null,null,null,null,null,null,null,null,null,null,"a ordinata 10. Okvir ne dirati !"]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+'C III-V'!B85","v":{"$error":"#VALUE!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+'C III-V'!D85","v":{"$error":"#VALUE!"}},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658},null,null,null,{"$f":"+IF(G56<=AP88,0,G56)","v":1.400001101}]
[" sloj 3. ..............................",{"$f":"+'Analiza i dimenzioniranje'!B112","v":{"$error":"#VALUE!"}},{"$f":"+B99*COS((G18)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B99*SIN((G18)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#VALUE!"}},{"$f":"IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF(I5=\"Y\",TAN(G14*PI()/180)^2,\"\")","v":""}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"Proraćun momenta savijanja za presjek III-III",null,null,null,null,null,null,null,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#VALUE!"}},{"$f":"IF(B108<=0,0,+'C III-V'!N87-'Analiza i dimenzioniranje'!E52)","v":{"$error":"#VALUE!"}},{"$f":"+B108*C108","v":{"$error":"#VALUE!"}},1.35,null,null,{"$f":"+C108+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}}]
[" Eh2 .............................................",{"$f":"+C98","v":{"$error":"#VALUE!"}},{"$f":"H109-'Analiza i dimenzioniranje'!E52","v":{"$error":"#VALUE!"}},{"$f":"+B109*C109","v":{"$error":"#VALUE!"}},1.35,null,null,{"$f":"+'C III-V'!D87","v":{"$error":"#VALUE!"}}]
[" Eh3 .....................................................",{"$f":"+C99","v":{"$error":"#VALUE!"}},{"$f":"IF(B110<=0,0,'C III-V'!F87-'C III-V'!C15)","v":{"$error":"#VALUE!"}},{"$f":"+B110*C110","v":{"$error":"#VALUE!"}},1.35,null,null,{"$f":"+C110+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}}]
[" EPrometno ....................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"B111*C111","v":{"$error":"#REF!"}},1.5,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}}]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"B112*C112","v":{"$error":"#REF!"}},1.35,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEv2="]
[" EPLinijsko ................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"IF(E30=0,0,+#REF!)","v":{"$error":"#REF!"}},{"$error":"#REF!"},1.35]
[" EQTemelj ....................................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$error":"#REF!"},1.35,null,null,{"$f":"+C114+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,null,{"$f":"+'C III-V'!$AI$44","v":1.5001009999999999},{"$f":"+'C III-V'!$AH$44","v":5.4000021999999994}]
[" HSidro ...............................",{"$f":"-E38*COS(E39*PI()/180)","v":-2.2699256917793105},{"$f":"IF(H115<E48,0,H115-E48)","v":169.01276595744682},-383.64641968549216,1.35,null,null,{"$f":"+E40","v":170.21276595744681},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":7.4000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":0},{"$f":"+H116-'Analiza i dimenzioniranje'!E52","v":-1.2},0,1,"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AA135","v":0}]
[null,null,{"$f":"IF(F101=0,0,E49/3)","v":0},0,1.35,null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}}," S MHA =",{"$f":"SUM(D108:D117)","v":{"$error":"#VALUE!"}},"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C III-V'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C III-V'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},1,null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C III-V'!H61","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C III-V'!H59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},1,null,null,{"$f":"2+$E$57-C127","v":{"$error":"#VALUE!"}}]
[" Gnasip na konzoli.............................",{"$f":"'C III-V'!J61","v":{"$error":"#VALUE!"}},{"$f":"IF(B128=0,0,2+E57-'C III-V'!J59)","v":{"$error":"#VALUE!"}},{"$f":"B128*C128","v":{"$error":"#VALUE!"}},1,null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C III-V'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},1,null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},1,null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C III-V'!W14<'C III-V'!B7,0,('C III-V'!W14-'C III-V'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C III-V'!W14+'C III-V'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},1,null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C III-V'!W23>'C III-V'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C III-V'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1,null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C III-V'!W28>'C III-V'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C III-V'!W27)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1,null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C III-V'!W35>'C III-V'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C III-V'!W37-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1,null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF('Analiza i dimenzioniranje'!E40<'Analiza i dimenzioniranje'!E52,0,E38*SIN(E39*PI()/180))","v":0.60822475599092374},{"$f":"2+E57-'C III-V'!AD28-E54-'Analiza i dimenzioniranje'!U49/2/100","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C III-V'!A93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1,null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C III-V'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1,null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C III-V'!E93","v":2.9000021999999994},{"$error":"#VALUE!"},1,null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]
[]
[]
[]
[" Rezultanta sila .........................................",null,"      R =",{"$f":"SQRT(B118^2+B139^2)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" sila uzduž temelja ..................................................",null,{"$f":"IF(E48=E49,\"     RH =\",\"     RT =\")","v":"     RT ="},{"$f":"D144*SIN((D148-D149)*PI()/180)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" sila okomita na temelj .................................",null,"    RN =",{"$f":"D144*COS((D148-D149)*PI()/180)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" moment oko osi temelja.....................................",null,"     Ms =",{"$f":"+B118*(I118-'C III-V'!AC50)-'Analiza i dimenzioniranje'!B168*(F139-E57/2)","v":{"$error":"#VALUE!"}},"kNm/m'"]
[" otklon rezultante od vertikale .....................................",null,"a =",{"$f":"ATAN(B118/B139)*180/PI()","v":{"$error":"#VALUE!"}},"°"]
[" nagib temelja ..........................................",null,"b =",{"$f":"ATAN('C III-V'!C15/E57)*180/PI()","v":9.7823997540577476},"°"]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"crtanje zida"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B2","v":2},{"$f":"+'C III-V'!C2","v":0.12820515121628623}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B3","v":2},{"$f":"+'C III-V'!C3","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B4","v":3.4000010999999999},{"$f":"+'C III-V'!C4","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B10","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C10","v":"A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B11","v":4.2000010999999997},{"$f":"+'C III-V'!C11","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C5","v":3.14}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B6","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C6","v":3.14}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B14","v":4.9000021999999994},{"$f":"+'C III-V'!C14","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B15","v":4.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B16","v":2},{"$f":"+'C III-V'!C16","v":0.12820515121628623}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!B25","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C25","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"IF(E49=E48,\"\",+D167*COS(D149*PI()/180))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ARM I-I"]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ARM II-II"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ankeri"]

{"sheet":"P Mmin","index":15,"n_rows":140,"n_cols":38,"rows_kept":140,"cut":false,"hidden":true,"merged":[[18,10,18,11],[45,11,46,11],[20,10,20,11],[29,10,29,11],[30,10,30,11],[21,10,21,11],[22,10,22,11],[28,10,28,11],[23,10,23,11],[24,10,24,11],[7,10,7,11],[8,10,8,11],[9,10,9,11],[16,10,16,11],[15,10,15,11],[14,10,14,11],[10,10,10,11],[11,10,11,11],[12,10,12,11],[13,10,13,11],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[7,0,7,9],[47,14,47,15],[48,14,49,14],[48,11,49,11],[47,11,47,12],[19,10,19,11],[33,10,33,11],[27,10,27,11],[25,10,25,11],[26,10,26,11],[34,10,34,11],[45,14,46,14],[45,23,46,23],[47,23,47,24],[48,23,49,23],[48,17,49,17],[45,20,46,20],[47,20,47,21],[48,20,49,20],[47,17,47,18],[45,17,46,17],[45,29,46,29],[45,26,46,26],[47,26,47,27],[48,26,49,26],[47,29,47,30],[48,29,49,29],[44,38,45,38],[46,38,46,39],[47,38,48,38],[45,32,46,32],[47,32,47,33],[48,32,49,32],[44,35,45,35],[46,35,46,36],[47,35,48,35]]}
[null,null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z18/M18","v":{"$error":"#VALUE!"}}]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  ","krak                  y  ","Moment destabilnosti i stabilnosti","za Mzida                                              krakovi                             x                  y",null,"Moment zida II","za M u                           presjeku II-II                                                   krakovi                                x               y",null,"Moment      II-II","za M u                           temelju ispod zida                     krakovi                             x                  y",null,"Moment  ","za M u                           presjeku I-I                                              krakovi                             x                  y",null,"Moment      I-I"]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5},null,null,null,{"$f":"2+E57-E54-E51/2","v":3.8000010999999998},{"$f":"+E48","v":1.2},null,{"$f":"2+E55","v":3.4000010999999999},{"$f":"'C III-V'!AC46+(E48-'C III-V'!AC46)/2","v":0.75384613757397367},null,{"$f":"2+E55+E51/2","v":3.8000010999999998},{"$f":"'C III-V'!AC49+(E48-'C III-V'!AF47)/2","v":1.0102563198554093},null,{"$f":"2+E55+E51","v":4.2000010999999997},{"$f":"'C III-V'!AC49+(E48-'C III-V'!AC49)/2","v":0.8051281599277047}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":0},null,null,null,null,null,null,{"$f":"+M8","v":0},null,null,{"$f":"+H108","v":0},null,{"$f":"+W8-$W$7","v":-0.5},{"$f":"+M8*Y8","v":0},null,{"$f":"+W8-$AB$7","v":-1.2},{"$f":"T8*AB8","v":0}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",0,null,null,null,null,null,null,{"$f":"+M9","v":0},null,null,0,null,-0.5,0,null,{"$f":"+W9-$AB$7","v":-1.2},{"$f":"AB9*T9","v":0}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"+M10","v":{"$error":"#VALUE!"}},null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,{"$f":"+AE7-'C III-V'!F93","v":{"$error":"#VALUE!"}},{"$f":"+AE10*S10","v":{"$error":"#VALUE!"}}]
[null,null,"GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}},null,null,1.2,null,0.7,{"$error":"#REF!"},null,{"$f":"+W11-$AB$7","v":0},{"$f":"AB11*T11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,1.2,null,0.7,{"$error":"#REF!"},null,0,{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ...................................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+E38","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"-M15*Y15","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":{"$error":"#REF!"}},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":{"$error":"#VALUE!"}},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-'P Mmin'!M61)","v":{"$error":"#VALUE!"}},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#REF!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#REF!"}},null,null,null,null,1.2,null,0.7,{"$error":"#REF!"},null,null,null,null,null,null,null,null,null,null,{"$f":"+AK7-C117","v":0.8051281599277047},{"$f":"+M17*AK17","v":{"$error":"#REF!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#REF!"}},{"$f":"SUM(S8:S17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T8:T17)","v":{"$error":"#REF!"}},{"$f":"SUM(U8:U17)","v":0},null,null,"x",null,{"$f":"SUM(Z8:Z17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC8:AC17)","v":{"$error":"#REF!"}},null,null,{"$f":"SUM(AF8:AF17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI8:AI17)","v":0},null,null,{"$f":"SUM(AL8:AL17)","v":{"$error":"#REF!"}}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C III-V'!V61+'C III-V'!X61+'C III-V'!Z61","v":92.625052249999968},{"$f":"+'C III-V'!Z61","v":13.03527768524077},{"$f":"+'C III-V'!V61","v":62.769260514792791},null,{"$f":"+'C III-V'!X61","v":16.820514049966405},null,null,null,null,{"$f":"+H126","v":3.3485779696489133},null,{"$f":"+$V$7-V19","v":1.5514242303510861},null,{"$f":"+M19*X19","v":143.70075039818533},null,null,null,{"$f":"AD7-'C III-V'!V59","v":1.2588240992358712},null,{"$f":"+AD19*O19","v":79.015457827235778},{"$f":"+AG7-'C III-V'!X59","v":8.1300761203646488E-3},null,{"$f":"+'C III-V'!X61*'Analiza i dimenzioniranje'!AQ13","v":0.13675205960988993},{"$f":"AJ7-'C III-V'!Z59","v":-0.34297241985289872},null,{"$f":"+'C III-V'!Z61*'Analiza i dimenzioniranje'!AT13","v":-4.470740731161519}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":"G="},null,null,{"$f":"+M20","v":"G="},null,null,null,null,null,"xt=",null,{"$f":"+$V$7-V20","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V20","v":{"$error":"#VALUE!"}},null,{"$f":"+P20*AA20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli............................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M21","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V21","v":{"$error":"#VALUE!"}},null,{"$f":"+P21*AA21","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza............."," ",0,null,{"$f":"+M22","v":0},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+AD7-V22","v":{"$error":"#VALUE!"}},null,{"$f":"+M22*AD22","v":{"$error":"#VALUE!"}}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0},null,null,null,null,null,null,null,4.5500016499999996,null,0.35000054999999985,null,0,null,null,null,null,null,null,null,null,null,{"$f":"AJ7-(2+E57-E54/2)","v":-0.35000054999999985},null,{"$f":"+AJ23*N23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X24","v":{"$error":"#VALUE!"}},null,{"$f":"+M24*AD24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X25","v":{"$error":"#VALUE!"}},null,{"$f":"+M25*AD25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X26","v":{"$error":"#VALUE!"}},null,{"$f":"+M26*AD26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X27","v":{"$error":"#VALUE!"}},null,{"$f":"+M27*AD27","v":{"$error":"#VALUE!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M28","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V28","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V28","v":{"$error":"#VALUE!"}},null,{"$f":"P28*AA28","v":{"$error":"#VALUE!"}}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",0,null,null,{"$f":"+M29","v":0},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V29","v":{"$error":"#VALUE!"}},null,{"$f":"+P29*AA29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",0,null,null,{"$f":"+M30","v":0},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V30","v":{"$error":"#VALUE!"}},null,{"$f":"+P30*AA30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",{"$error":"#VALUE!"},null,{"$f":"+M31","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,2,null,2.9000021999999994,null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-'C III-V'!E93","v":1.4000010999999999},null,{"$f":"+M31*AD31","v":{"$error":"#VALUE!"}},{"$f":"+$AD$7-AD31","v":2}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.03527768524077},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":16.820514049966405},null,null,null,null,null,null,null,null,{"$f":"SUM(Z19:Z31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC19:AC31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF19:AF31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI19:AI31)","v":0.13675205960988993},null,null,{"$f":"SUM(AL19:AL31)","v":-4.470740731161519}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"II-II","sredina","I-I"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C III-V'!V76+'C III-V'!X76+'C III-V'!Z76","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!X76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+'C III-V'!V76","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X76","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z76","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"$AD$7-'C III-V'!V77","v":{"$error":"#VALUE!"}},null,{"$f":"+X34*AD34","v":{"$error":"#VALUE!"}},{"$f":"$AG$7-'C III-V'!X77","v":{"$error":"#VALUE!"}},null,{"$f":"-Y34*AG34","v":{"$error":"#VALUE!"}},{"$f":"+AJ7-'C III-V'!Z77","v":{"$error":"#VALUE!"}},null,{"$f":"+Z34*AJ34","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+Z35","v":{"$error":"#VALUE!"}},{"$f":"+X35","v":{"$error":"#VALUE!"}},null,{"$f":"+Y35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M35*E55/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E51/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E54/E57","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AE7-'C III-V'!AC44","v":{"$error":"#VALUE!"}},{"$f":"-S35*AE35","v":{"$error":"#VALUE!"}},null,{"$f":"+AH7-'C III-V'!AC48","v":{"$error":"#VALUE!"}},{"$f":"Y35*AH35","v":{"$error":"#VALUE!"}},null,{"$f":"+AK7-'C III-V'!AC52","v":{"$error":"#VALUE!"}},{"$f":"-Z35*AK35","v":{"$error":"#VALUE!"}}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},{"$f":"R18+R35","v":{"$error":"#REF!"}},{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#REF!"}},{"$f":"+U18+U35","v":{"$error":"#VALUE!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"SUM(R36:U36)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,{"$f":"+AC18+AC32+AC34+AC35","v":{"$error":"#REF!"}},null,null,{"$f":"+AF18+AF32+AF34+AF35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AI18+AI32+AI34+AI35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AL18+AL32+AL34+AL35","v":{"$error":"#REF!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!S40","v":{"$error":"#VALUE!"}},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y","x"]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"+'Analiza i dimenzioniranje'!E39","v":15},"°    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD7","v":3.4000010999999999},{"$f":"+AE7","v":0.75384613757397367}]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!S42","v":{"$error":"#VALUE!"}},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'C III-V'!V61*('Analiza i dimenzioniranje'!AI33-'C III-V'!V59)+B129*(AD39-H129)+B138*(AD39-H138)+B138*(AD39-H138)+'C III-V'!V76*('Analiza i dimenzioniranje'!AI33-'C III-V'!V77)+S35*(AE39-'C III-V'!AC65)+B110*(AE39-H110)","v":{"$error":"#VALUE!"}}]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*C42*'C III-V'!#REF!/B42","v":{"$error":"#REF!"}},"kN/m'"]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'Unos podataka'!H34","v":1}]
[null,null,"DIMENZIJE ZIDA:"]
[]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":{"$error":"#VALUE!"}},"m"]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C III-V'!B10-'C III-V'!B11=0,\">100\",IF('C III-V'!C10-'C III-V'!C11/(0.00000000000001+'C III-V'!B11-'C III-V'!B10)>100,\">100\",('C III-V'!C10-'C III-V'!C11)/('C III-V'!B11-'C III-V'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C III-V'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C III-V'!E64","v":1.4000010999999999},"m"]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 "]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m"]
[" zapreminska težina nasipa ...............................",null,null,"      gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!AN44","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AN44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C III-V'!I87-'C III-V'!Q17)-B109*('C III-V'!K87-'C III-V'!Q17)-B112*#REF!-B113*#REF!-B114*#REF!-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C III-V'!Q16-'C III-V'!N59)+B136*('C III-V'!Q16-'C III-V'!H92)+B137*('C III-V'!Q16-'C III-V'!C93)+B135*(C135),-B116*C116/1.35-B108*('C III-V'!I87-'C III-V'!Q17)-B109*('C III-V'!K87-'C III-V'!Q17)-B112*#REF!-B113*#REF!-B114*#REF!-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C III-V'!Q16-'C III-V'!H92)+B137*('C III-V'!Q16-'C III-V'!C93)+B135*(C135))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+#REF!)","v":{"$error":"#REF!"}},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,null,null,null,{"$f":"+#REF!*#REF!","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":{"$error":"#REF!"}},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m"]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m"]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m"]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+'C III-V'!I85","v":0},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":0},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":0},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+'C III-V'!K88","v":0},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":0},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":0},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658}]
[" sloj 3. ..............................",{"$f":"+'P III-III'!B99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!C99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!D99","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#REF!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#REF!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,null,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":0},null,null,{"$f":"+'Analiza i dimenzioniranje'!I120","v":1},null,null,{"$f":"+'C III-V'!N87","v":0}]
[" Eh2 .............................................",{"$f":"+C98","v":0},null,null,{"$f":"+'Analiza i dimenzioniranje'!I121","v":1},null,null,{"$f":"+'C III-V'!K87","v":0}]
[" Eh3 .....................................................",{"$f":"+C99","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I122","v":1},null,null,{"$f":"+C110+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPrometno ....................................",{"$f":"#REF!","v":{"$error":"#REF!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I124","v":1.3},null,null,{"$f":"+C111+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I125","v":1},null,null,{"$f":"+C112+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPLinijsko ................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+B113*C113","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I126","v":1}]
[" EQTemelj ....................................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I127","v":1},null,null,{"$f":"+C114+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,null,{"$f":"+'C III-V'!$AI$44","v":1.5001009999999999},{"$f":"+'C III-V'!$AH$44","v":5.4000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"IF(H115<'Analiza i dimenzioniranje'!AN44,0,H115-'Analiza i dimenzioniranje'!AN44)","v":{"$error":"#VALUE!"}},{"$f":"+B115*C115","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I129","v":0},null,null,{"$f":"+E40","v":{"$error":"#VALUE!"}},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":7.4000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":{"$error":"#REF!"}},{"$f":"+H116-'Analiza i dimenzioniranje'!Q44","v":{"$error":"#REF!"}},{"$f":"B116*C116","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I150","v":0},"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C III-V'!#REF!","v":{"$error":"#REF!"}}]
[{"$f":"+A101","v":{"$error":"#REF!"}},{"$f":"-B101","v":{"$error":"#REF!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!E116","v":0},null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}},null,null,"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C III-V'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C III-V'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},{"$f":"+'Analiza i dimenzioniranje'!I135","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C III-V'!L61","v":"G="},{"$f":"2+E57-'C III-V'!D59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I136","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!L59","v":"xt="}]
[" Gnasip na konzoli.............................",{"$f":"IF(M61>=E67+E68,0,'C III-V'!N61)","v":{"$error":"#VALUE!"}},{"$f":"IF(B128=0,0,2+E57-'C III-V'!J59)","v":{"$error":"#VALUE!"}},{"$f":"B128*C128","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I138","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C128","v":{"$error":"#VALUE!"}}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C III-V'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I139","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},{"$f":"+'Analiza i dimenzioniranje'!I140","v":{"$error":"#VALUE!"}},null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C III-V'!W14<'C III-V'!B7,0,('C III-V'!W14-'C III-V'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C III-V'!W14+'C III-V'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I141","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C III-V'!W23>'C III-V'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C III-V'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I142","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C III-V'!W28>'C III-V'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C III-V'!W27)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I143","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C III-V'!W35>'C III-V'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C III-V'!W37-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I144","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C III-V'!AB28-E54-'Analiza i dimenzioniranje'!AN49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I145","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":0},{"$f":"2+E57-'C III-V'!H92","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I146","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":0},{"$f":"2+E57-'C III-V'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I147","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C III-V'!E93","v":2.9000021999999994},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I148","v":1},null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]

{"sheet":"P Mmax","index":16,"n_rows":140,"n_cols":38,"rows_kept":140,"cut":false,"hidden":true,"merged":[[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[26,10,26,11],[20,10,20,11],[21,10,21,11],[15,10,15,11],[16,10,16,11],[18,10,18,11],[19,10,19,11],[22,10,22,11],[23,10,23,11],[24,10,24,11],[25,10,25,11],[14,10,14,11],[7,0,7,9],[13,10,13,11],[7,10,7,11],[8,10,8,11],[12,10,12,11],[9,10,9,11],[10,10,10,11],[11,10,11,11],[34,10,34,11],[27,10,27,11],[30,10,30,11],[33,10,33,11],[28,10,28,11],[29,10,29,11],[44,38,45,38],[45,11,46,11],[45,14,46,14],[45,17,46,17],[45,20,46,20],[46,38,46,39],[45,29,46,29],[45,32,46,32],[46,35,46,36],[44,35,45,35],[45,26,46,26],[45,23,46,23],[47,11,47,12],[47,14,47,15],[47,17,47,18],[47,20,47,21],[48,11,49,11],[48,14,49,14],[48,17,49,17],[48,20,49,20],[48,23,49,23],[47,38,48,38],[48,29,49,29],[48,32,49,32],[47,32,47,33],[47,35,48,35],[48,26,49,26],[47,23,47,24],[47,26,47,27],[47,29,47,30]]}
["milenium",null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
["milenium",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z18/M18","v":{"$error":"#VALUE!"}}]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  ","krak                  y  ","Moment destabilnosti i stabilnosti","za Mzida                                              krakovi                             x                  y",null,"Moment zida II","za M u                           presjeku II-II                                                   krakovi                                x               y",null,"Moment      II-II","za M u                           temelju ispod zida                     krakovi                             x                  y",null,"Moment  ","za M u                           presjeku I-I                                              krakovi                             x                  y",null,"Moment      I-I"]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5},null,null,null,{"$f":"2+E57-E54-E51/2","v":3.8000010999999998},{"$f":"+E48","v":1.2},null,{"$f":"2+E55","v":3.4000010999999999},{"$f":"'C III-V'!AC46+(E48-'C III-V'!AC46)/2","v":0.75384613757397367},null,{"$f":"2+E55+E51/2","v":3.8000010999999998},{"$f":"'C III-V'!AC49+(E48-'C III-V'!AF47)/2","v":1.0102563198554093},null,{"$f":"2+E55+E51","v":4.2000010999999997},{"$f":"'C III-V'!AC49+(E48-'C III-V'!AC49)/2","v":0.8051281599277047}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":0},null,null,null,null,null,null,{"$f":"+M8","v":0},null,null,{"$f":"+H108","v":0},null,{"$f":"+W8-$W$7","v":-0.5},{"$f":"+M8*Y8","v":0},null,{"$f":"+W8-$AB$7","v":-1.2},{"$f":"T8*AB8","v":0}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",0,null,null,null,null,null,null,{"$f":"+M9","v":0},null,null,0,null,-0.5,0,null,{"$f":"+W9-$AB$7","v":-1.2},{"$f":"AB9*T9","v":0}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"+M10","v":{"$error":"#VALUE!"}},null,null,null,0,null,-0.5,{"$error":"#VALUE!"},null,null,null,null,{"$f":"+AE7-'C III-V'!F93","v":{"$error":"#VALUE!"}},{"$f":"+AE10*S10","v":{"$error":"#VALUE!"}}]
[null,null,"GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}},null,null,0,null,-0.5,{"$error":"#REF!"},null,{"$f":"+W11-$AB$7","v":-1.2},{"$f":"AB11*T11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ...................................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+E38","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"-M15*Y15","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,null,6.2644906473896782,null,5.7644906473896782,{"$error":"#VALUE!"},null,5.064490647389678,{"$error":"#VALUE!"}]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":{"$error":"#VALUE!"}},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-'P Mmax'!M61)","v":{"$error":"#VALUE!"}},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#REF!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#REF!"}},null,null,null,null,1.2,null,0.7,{"$error":"#REF!"},null,null,null,null,null,null,null,null,null,null,{"$f":"+AK7-C117","v":0.8051281599277047},{"$f":"+M17*AK17","v":{"$error":"#REF!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#REF!"}},{"$f":"SUM(S8:S17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T8:T17)","v":{"$error":"#REF!"}},{"$f":"SUM(U8:U17)","v":0},null,null,"x",null,{"$f":"SUM(Z8:Z17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC8:AC17)","v":{"$error":"#REF!"}},null,null,{"$f":"SUM(AF8:AF17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI8:AI17)","v":0},null,null,{"$f":"SUM(AL8:AL17)","v":{"$error":"#REF!"}}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C III-V'!V61+'C III-V'!X61+'C III-V'!Z61","v":92.625052249999968},{"$f":"+'C III-V'!Z61","v":13.03527768524077},{"$f":"+'C III-V'!V61","v":62.769260514792791},null,{"$f":"+'C III-V'!X61","v":16.820514049966405},null,null,null,null,{"$f":"+H126","v":3.3485779696489133},null,{"$f":"+$V$7-V19","v":1.5514242303510861},null,{"$f":"+M19*X19","v":143.70075039818533},null,null,null,{"$f":"AD7-'C III-V'!V59","v":1.2588240992358712},null,{"$f":"+AD19*O19","v":79.015457827235778},{"$f":"+AG7-'C III-V'!X59","v":8.1300761203646488E-3},null,{"$f":"+'C III-V'!X61*'Analiza i dimenzioniranje'!AQ13","v":0.13675205960988993},{"$f":"AJ7-'C III-V'!Z59","v":-0.34297241985289872},null,{"$f":"+'C III-V'!Z61*'Analiza i dimenzioniranje'!AT13","v":-4.470740731161519}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":0},null,null,{"$f":"+M20","v":0},null,null,null,null,null,"xt=",null,{"$f":"+$V$7-V20","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V20","v":{"$error":"#VALUE!"}},null,{"$f":"+P20*AA20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli............................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M21","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V21","v":{"$error":"#VALUE!"}},null,{"$f":"+P21*AA21","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza............."," ",0,null,{"$f":"+M22","v":0},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+AD7-V22","v":{"$error":"#VALUE!"}},null,{"$f":"+M22*AD22","v":{"$error":"#VALUE!"}}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0},null,null,null,null,null,null,null,4.5500016499999996,null,0.35000054999999985,null,0,null,null,null,null,null,null,null,null,null,{"$f":"AJ7-(2+E57-E54/2)","v":-0.35000054999999985},null,{"$f":"+AJ23*N23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X24","v":{"$error":"#VALUE!"}},null,{"$f":"+M24*AD24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X25","v":{"$error":"#VALUE!"}},null,{"$f":"+M25*AD25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X26","v":{"$error":"#VALUE!"}},null,{"$f":"+M26*AD26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X27","v":{"$error":"#VALUE!"}},null,{"$f":"+M27*AD27","v":{"$error":"#VALUE!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M28","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V28","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V28","v":{"$error":"#VALUE!"}},null,{"$f":"P28*AA28","v":{"$error":"#VALUE!"}}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",0,null,null,{"$f":"+M29","v":0},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V29","v":{"$error":"#VALUE!"}},null,{"$f":"+P29*AA29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",0,null,null,{"$f":"+M30","v":0},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V30","v":{"$error":"#VALUE!"}},null,{"$f":"+P30*AA30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",{"$error":"#VALUE!"},null,{"$f":"+M31","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,2,null,2.9000021999999994,null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-'C III-V'!E93","v":1.4000010999999999},null,{"$f":"+M31*AD31","v":{"$error":"#VALUE!"}},{"$f":"+$AD$7-AD31","v":2}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.03527768524077},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":16.820514049966405},null,null,null,null,null,null,null,null,{"$f":"SUM(Z19:Z31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC19:AC31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF19:AF31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI19:AI31)","v":0.13675205960988993},null,null,{"$f":"SUM(AL19:AL31)","v":-4.470740731161519}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"II-II","sredina","I-I"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C III-V'!V76+'C III-V'!X76+'C III-V'!Z76","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!X76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+'C III-V'!V76","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X76","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z76","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"$AD$7-'C III-V'!V77","v":{"$error":"#VALUE!"}},null,{"$f":"+X34*AD34","v":{"$error":"#VALUE!"}},{"$f":"$AG$7-'C III-V'!X77","v":{"$error":"#VALUE!"}},null,{"$f":"-Y34*AG34","v":{"$error":"#VALUE!"}},{"$f":"+AJ7-'C III-V'!Z77","v":{"$error":"#VALUE!"}},null,{"$f":"+Z34*AJ34","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+Z35","v":{"$error":"#VALUE!"}},{"$f":"+X35","v":{"$error":"#VALUE!"}},null,{"$f":"+Y35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M35*E55/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E51/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E54/E57","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AE7-'C III-V'!AC44","v":{"$error":"#VALUE!"}},{"$f":"-S35*AE35","v":{"$error":"#VALUE!"}},null,{"$f":"+AH7-'C III-V'!AC48","v":{"$error":"#VALUE!"}},{"$f":"Y35*AH35","v":{"$error":"#VALUE!"}},null,{"$f":"+AK7-'C III-V'!AC52","v":{"$error":"#VALUE!"}},{"$f":"-Z35*AK35","v":{"$error":"#VALUE!"}}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},{"$f":"R18+R35","v":{"$error":"#REF!"}},{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#REF!"}},{"$f":"+U18+U35","v":{"$error":"#VALUE!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"SUM(R36:U36)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,{"$f":"+AC18+AC32+AC34+AC35","v":{"$error":"#REF!"}},null,null,{"$f":"+AF18+AF32+AF34+AF35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AI18+AI32+AI34+AI35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AL18+AL32+AL34+AL35","v":{"$error":"#REF!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!T40","v":{"$error":"#VALUE!"}},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y","x"]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"+'Analiza i dimenzioniranje'!E39","v":15},"°    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD7","v":3.4000010999999999},{"$f":"+AE7","v":0.75384613757397367}]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!T42","v":{"$error":"#VALUE!"}},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'C III-V'!V61*('Analiza i dimenzioniranje'!AI33-'C III-V'!V59)+B129*(AD39-H129)+B138*(AD39-H138)+B138*(AD39-H138)+'C III-V'!V76*('Analiza i dimenzioniranje'!AI33-'C III-V'!V77)+S35*(AE39-'C III-V'!AC65)+B110*(AE39-H110)","v":{"$error":"#VALUE!"}}]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*'C III-V'!AI119*C42/B42","v":{"$error":"#VALUE!"}},"kN/m'"]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'Unos podataka'!H34","v":1}]
[null,null,"DIMENZIJE ZIDA:"]
[]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":{"$error":"#VALUE!"}},"m"]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C III-V'!B10-'C III-V'!B11=0,\">100\",IF('C III-V'!C10-'C III-V'!C11/(0.00000000000001+'C III-V'!B11-'C III-V'!B10)>100,\">100\",('C III-V'!C10-'C III-V'!C11)/('C III-V'!B11-'C III-V'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C III-V'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C III-V'!E64","v":1.4000010999999999},"m"]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 "]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m"]
[" zapreminska težina nasipa ...............................",null,null,"      gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!R44","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+ IF(M61='Analiza i dimenzioniranje'!E48,0,M64+M63)","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF(M61='Analiza i dimenzioniranje'!E48,0,IF('Analiza i dimenzioniranje'!AO44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C III-V'!N87-'C III-V'!P17)-B109*('C III-V'!P87-'C III-V'!P17)-B112*#REF!-B113*#REF!-B114*#REF!-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C III-V'!P16-'C III-V'!R59)+B136*('C III-V'!P16-'C III-V'!H93)+B137*('C III-V'!P16-'C III-V'!C93)+B135*(C135),-B116*C116/1.35-B108*('C III-V'!N87-'C III-V'!P17)-B109*('C III-V'!P87-'C III-V'!P17)-B112*#REF!-B113*#REF!-B114*#REF!-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C III-V'!P16-'C III-V'!H93)+B137*('C III-V'!P16-'C III-V'!C93)+B135*(C135)))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+#REF!)","v":{"$error":"#REF!"}},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,null,null,null,{"$f":"-IF(M61='Analiza i dimenzioniranje'!E48,0,#REF!*#REF!)","v":{"$error":"#VALUE!"}},{"$f":"-B116*C116","v":{"$error":"#VALUE!"}},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m"]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m"]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m"]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+'C III-V'!N85","v":0},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":0},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":0},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+'C III-V'!P88","v":0},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":0},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":0},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658}]
[" sloj 3. ..............................",{"$f":"+'P III-III'!B99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!C99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!D99","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#REF!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#REF!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,null,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":0},null,null,{"$f":"+'Analiza i dimenzioniranje'!I120","v":1}]
[" Eh2 .............................................",{"$f":"+C98","v":0},null,null,{"$f":"+'Analiza i dimenzioniranje'!I121","v":1}]
[" Eh3 .....................................................",{"$f":"+C99","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I122","v":1}]
[" EPrometno ....................................",{"$f":"#REF!","v":{"$error":"#REF!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I124","v":1.3}]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I125","v":1}]
[" EPLinijsko ................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+B113*C113","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I126","v":1}]
[" EQTemelj ....................................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I127","v":1},null,null,null,null,null,{"$f":"+'C III-V'!$AI$44","v":1.5001009999999999},{"$f":"+'C III-V'!$AH$44","v":5.4000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"IF(H115<'Analiza i dimenzioniranje'!R44,0,H115-'Analiza i dimenzioniranje'!R44)","v":{"$error":"#VALUE!"}},{"$f":"+B115*C115","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I129","v":0},null,null,{"$f":"+E40","v":{"$error":"#VALUE!"}},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":7.4000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":{"$error":"#VALUE!"}},{"$f":"+H116-'Analiza i dimenzioniranje'!R44","v":{"$error":"#VALUE!"}},{"$f":"B116*C116","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I150","v":0},"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C III-V'!AI117","v":6.2644906473896782}]
[{"$f":"+A101","v":{"$error":"#REF!"}},{"$f":"-B101","v":{"$error":"#REF!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!E116","v":0},null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}},null,null,"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C III-V'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C III-V'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},{"$f":"+'Analiza i dimenzioniranje'!I135","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C III-V'!P61","v":0},{"$f":"2+E57-'C III-V'!D59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I136","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!L59","v":"xt="}]
[" Gnasip na konzoli.............................",{"$f":"IF(M61>=E67+E68,0,'C III-V'!R61)","v":{"$error":"#VALUE!"}},{"$f":"IF(B128=0,0,2+E57-'C III-V'!J59)","v":{"$error":"#VALUE!"}},{"$f":"B128*C128","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I138","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C128","v":{"$error":"#VALUE!"}}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C III-V'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I139","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},{"$f":"+'Analiza i dimenzioniranje'!I140","v":{"$error":"#VALUE!"}},null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C III-V'!W14<'C III-V'!B7,0,('C III-V'!W14-'C III-V'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C III-V'!W14+'C III-V'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I141","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C III-V'!W23>'C III-V'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C III-V'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I142","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C III-V'!W28>'C III-V'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C III-V'!W27)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I143","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C III-V'!W35>'C III-V'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C III-V'!W37-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I144","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C III-V'!AC28-E54-'Analiza i dimenzioniranje'!AO49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I145","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":0},{"$f":"2+E57-'C III-V'!H93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I146","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":0},{"$f":"2+E57-'C III-V'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I147","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C III-V'!E93","v":2.9000021999999994},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I148","v":1},null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]

{"sheet":"P VI-VI","index":17,"n_rows":145,"n_cols":38,"rows_kept":145,"cut":false,"hidden":true,"merged":[[9,10,9,11],[10,10,10,11],[11,10,11,11],[12,10,12,11],[18,10,18,11],[13,10,13,11],[14,10,14,11],[15,10,15,11],[21,10,21,11],[19,10,19,11],[20,10,20,11],[16,10,16,11],[47,32,47,33],[33,10,33,11],[26,10,26,11],[27,10,27,11],[28,10,28,11],[22,10,22,11],[23,10,23,11],[24,10,24,11],[25,10,25,11],[47,29,47,30],[45,20,46,20],[47,23,47,24],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[7,10,7,11],[7,0,7,9],[8,10,8,11],[45,17,46,17],[47,26,47,27],[48,23,49,23],[44,38,45,38],[47,35,48,35],[47,38,48,38],[48,26,49,26],[46,38,46,39],[48,29,49,29],[46,35,46,36],[44,35,45,35],[45,26,46,26],[45,29,46,29],[48,32,49,32],[45,32,46,32],[64,11,64,12],[45,23,46,23],[48,14,49,14],[29,10,29,11],[30,10,30,11],[48,17,49,17],[48,11,49,11],[48,20,49,20],[34,10,34,11],[47,11,47,12],[47,14,47,15],[47,17,47,18],[47,20,47,21],[45,11,46,11],[45,14,46,14]]}
[" UPUTE ZA RAD: - Ispuniti sve podatke u čelijama s plavom bojom. Ispuniti i za izbor armature u kolonama L,N i O",null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z18/M18","v":{"$error":"#VALUE!"}}]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11",null,"v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  ","krak                  y  ","Moment destabilnosti i stabilnosti","za Mzida                                              krakovi                             x                  y",null,"Moment zida II","za M u                           presjeku II-II                                                   krakovi                                x               y",null,"Moment      II-II","za M u                           temelju ispod zida                     krakovi                             x                  y",null,"Moment  ","za M u                           presjeku I-I                                              krakovi                             x                  y",null,"Moment      I-I"]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C VI-VII'!C15","v":0.5},null,null,null,{"$f":"2+E57-E54-E51/2","v":3.8000010999999998},{"$f":"+E48","v":1.2},null,{"$f":"2+E55","v":3.4000010999999999},{"$f":"'C VI-VII'!AC47+(E48-'C VI-VII'!AC47)/2","v":0.72068965844232813},null,{"$f":"2+E55+E51/2","v":3.8000010999999998},{"$f":"'C VI-VII'!AC49+(E48-'C VI-VII'!AF47)/2","v":0.97931024673015765},null,{"$f":"2+E55+E51","v":4.2000010999999997},{"$f":"'C VI-VII'!AC49+(E48-'C VI-VII'!AC49)/2","v":0.78965512336507881}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#VALUE!"}},null,null,{"$f":"+H108","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$W$7","v":{"$error":"#VALUE!"}},{"$f":"+M8*Y8","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$AB$7","v":{"$error":"#VALUE!"}},{"$f":"T8*AB8","v":{"$error":"#VALUE!"}}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,null,{"$f":"+M9","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$f":"+W9-$AB$7","v":{"$error":"#VALUE!"}},{"$f":"AB9*T9","v":{"$error":"#VALUE!"}}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"+M10","v":{"$error":"#VALUE!"}},null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,{"$f":"+AE7-'C VI-VII'!F93","v":{"$error":"#VALUE!"}},{"$f":"+AE10*S10","v":{"$error":"#VALUE!"}}]
[null,null,"GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$f":"+W11-$AB$7","v":{"$error":"#REF!"}},{"$f":"AB11*T11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ...................................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":2.2699256917793105},null,null,null,null,null,null,2.2699256917793105,null,null,170.21276595744681,null,169.71276595744681,{"$f":"-M15*Y15","v":-385.23536766973763},null,169.01276595744682,383.64641968549216]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":0},null,null,null,null,null,null,0,null,null,0,null,-0.5,0,null,-1.2,0]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":2},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-'P VI-VI'!M61)","v":2.48},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#VALUE!"}},null,null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,{"$f":"+AK7-C117","v":0.78965512336507881},{"$f":"+M17*AK17","v":{"$error":"#VALUE!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S8:S17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T8:T17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U8:U17)","v":0},null,null,"x",null,{"$f":"SUM(Z8:Z17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC8:AC17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF8:AF17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI8:AI17)","v":0},null,null,{"$f":"SUM(AL8:AL17)","v":{"$error":"#VALUE!"}}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C VI-VII'!V61+'C VI-VII'!X61+'C VI-VII'!Z61","v":68.875052249999982},{"$f":"+'C VI-VII'!Z61","v":13.306056250595223},{"$f":"+'C VI-VII'!V61","v":37.77589163555291},null,{"$f":"+'C VI-VII'!X61","v":17.793104363851846},null,null,null,null,{"$f":"+H126","v":3.3485779696489133},null,{"$f":"+$V$7-V19","v":1.5514242303510861},null,{"$f":"+M19*X19","v":106.85442492734707},null,null,null,{"$f":"AD7-'C VI-VII'!V59","v":0.72609215808095717},null,{"$f":"+AD19*O19","v":27.428778681090989},{"$f":"+AG7-'C VI-VII'!X59","v":1.0335908939774985E-2},null,{"$f":"+'C VI-VII'!X61*'Analiza i dimenzioniranje'!AQ13","v":0.14465929289570792},{"$f":"AJ7-'C VI-VII'!Z59","v":-0.34074126926177506},null,{"$f":"+'C VI-VII'!Z61*'Analiza i dimenzioniranje'!AT13","v":-4.5636103109654318}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M20","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V20","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V20","v":{"$error":"#VALUE!"}},null,{"$f":"+P20*AA20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli............................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M21","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V21","v":{"$error":"#VALUE!"}},null,{"$f":"+P21*AA21","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza............."," ",0,null,{"$f":"+M22","v":0},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+AD7-V22","v":{"$error":"#VALUE!"}},null,{"$f":"+M22*AD22","v":{"$error":"#VALUE!"}}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0},null,null,null,null,null,null,null,4.5500016499999996,null,0.35000054999999985,null,0,null,null,null,null,null,null,null,null,null,{"$f":"AJ7-(2+E57-E54/2)","v":-0.35000054999999985},null,{"$f":"+AJ23*N23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X24","v":{"$error":"#VALUE!"}},null,{"$f":"+M24*AD24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X25","v":{"$error":"#VALUE!"}},null,{"$f":"+M25*AD25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X26","v":{"$error":"#VALUE!"}},null,{"$f":"+M26*AD26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X27","v":{"$error":"#VALUE!"}},null,{"$f":"+M27*AD27","v":{"$error":"#VALUE!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",0.60822475599092374,null,null,{"$f":"+M28","v":0.60822475599092374},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V28","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V28","v":{"$error":"#VALUE!"}},null,{"$f":"P28*AA28","v":{"$error":"#VALUE!"}}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M29","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V29","v":{"$error":"#VALUE!"}},null,{"$f":"+P29*AA29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M30","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V30","v":{"$error":"#VALUE!"}},null,{"$f":"+P30*AA30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",{"$error":"#VALUE!"},null,{"$f":"+M31","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,2,null,2.9000021999999994,null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-'C VI-VII'!E93","v":1.4000010999999999},null,{"$f":"+M31*AD31","v":{"$error":"#VALUE!"}},{"$f":"+$AD$7-AD31","v":2}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.306056250595223},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":17.793104363851846},null,null,null,null,null,null,null,null,{"$f":"SUM(Z19:Z31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC19:AC31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF19:AF31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI19:AI31)","v":0.14465929289570792},null,null,{"$f":"SUM(AL19:AL31)","v":-4.5636103109654318}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"II-II","sredina","I-I"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C VI-VII'!Z76+'C VI-VII'!AB76+'C VI-VII'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":{"$error":"#VALUE!"}},null,{"$f":"+'C VI-VII'!AB76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+'C VI-VII'!Z76","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!AB76","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!AD76","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"$AD$7-'C VI-VII'!Z77","v":{"$error":"#VALUE!"}},null,{"$f":"+X34*AD34","v":{"$error":"#VALUE!"}},{"$f":"$AG$7-'C VI-VII'!AB77","v":{"$error":"#VALUE!"}},null,{"$f":"-Y34*AG34","v":{"$error":"#VALUE!"}},{"$f":"+AJ7-'C VI-VII'!AD77","v":{"$error":"#VALUE!"}},null,{"$f":"+Z34*AJ34","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+Z35","v":{"$error":"#VALUE!"}},{"$f":"+X35","v":{"$error":"#VALUE!"}},null,{"$f":"+Y35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M35*E55/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E51/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E54/E57","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AE7-'C VI-VII'!AC45","v":{"$error":"#VALUE!"}},{"$f":"-S35*AE35","v":{"$error":"#VALUE!"}},null,{"$f":"+AH7-'C VI-VII'!AC48","v":{"$error":"#VALUE!"}},{"$f":"Y35*AH35","v":{"$error":"#VALUE!"}},null,{"$f":"+AK7-'C VI-VII'!AC52","v":{"$error":"#VALUE!"}},{"$f":"-Z35*AK35","v":{"$error":"#VALUE!"}}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},{"$f":"R18+R35","v":{"$error":"#VALUE!"}},{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#VALUE!"}},{"$f":"+U18+U35","v":{"$error":"#VALUE!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"SUM(R36:U36)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+AC18+AC32+AC34+AC35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AF18+AF32+AF34+AF35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AI18+AI32+AI34+AI35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AL18+AL32+AL34+AL35","v":{"$error":"#VALUE!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!V40","v":2.35},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y","x"]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"+'Analiza i dimenzioniranje'!E39","v":15},"°    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD7","v":3.4000010999999999},{"$f":"+AE7","v":0.72068965844232813}]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!V42","v":170.21276595744681},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'C VI-VII'!V61*('Analiza i dimenzioniranje'!AI33-'C VI-VII'!V59)+B129*(AD39-H129)+B138*(AD39-H138)+B138*(AD39-H138)+'C VI-VII'!Z76*('Analiza i dimenzioniranje'!AI33-'C VI-VII'!Z77)+S35*(AE39-'C VI-VII'!AG66)+B110*(AE39-H110)","v":{"$error":"#VALUE!"}}]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*'C VI-VII'!AC118*C42/B42","v":0},"kN/m'"]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'P Mmax'!C42","v":1}]
[null,null,"DIMENZIJE ZIDA:"]
[]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":5.6800000000000006},"m"]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C VI-VII'!B10-'C VI-VII'!B11=0,\">100\",IF('C VI-VII'!C10-'C VI-VII'!C11/(0.00000000000001+'C VI-VII'!B11-'C VI-VII'!B10)>100,\">100\",('C VI-VII'!C10-'C VI-VII'!C11)/('C VI-VII'!B11-'C VI-VII'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C VI-VII'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C VI-VII'!E64","v":1.4000010999999999},"m"]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 "]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m"]
[" zapreminska težina nasipa ...............................",null,null,"      gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!V44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C VI-VII'!I87-'C VI-VII'!Q17)-B109*('C VI-VII'!K87-'C VI-VII'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C VI-VII'!Q16-'C VI-VII'!N59)+B136*('C VI-VII'!Q16-'C VI-VII'!M93)+B137*('C VI-VII'!Q16-'C VI-VII'!C93)+B135*(C135),-B116*C116/1.35-B108*('C VI-VII'!I87-'C VI-VII'!Q17)-B109*('C VI-VII'!K87-'C VI-VII'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C VI-VII'!Q16-'C VI-VII'!M93)+B137*('C VI-VII'!Q16-'C VI-VII'!C93)+B135*(C135))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+#REF!)","v":{"$error":"#REF!"}},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+'Dijagram momenata'!Q19","v":1.52},null,{"$f":"-'HT III-XX'!#REF!*N66","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":0},{"$f":"-B111*'HT III-XX'!#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota",null,"krak od presjeka do sile"]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c111",{"$f":"IF(+L66-'Dijagram momenata'!$Q$19>0,+L66-'Dijagram momenata'!$Q$19,0)","v":{"$error":"#REF!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c112",{"$f":"IF(+L67-'Dijagram momenata'!$Q$19>0,+L67-'Dijagram momenata'!$Q$19,0)","v":{"$error":"#REF!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c113",{"$f":"IF(+L68-'Dijagram momenata'!$Q$19>0,+L68-'Dijagram momenata'!$Q$19,0)","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c114",{"$f":"IF(+L69-'Dijagram momenata'!$Q$19>0,+L69-'Dijagram momenata'!$Q$19,0)","v":{"$error":"#REF!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')",null,null,"Ka"]
[" sloj 1. ..........................................",{"$f":"+'C VI-VII'!I85","v":{"$error":"#VALUE!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213},{"$f":"COS((-G48-E14)*PI()/180)^2","v":0.85966990016932565},{"$f":"COS((-G48-F14)*PI()/180)^2","v":0.90450849718747361},{"$f":"COS((-G48-G14)*PI()/180)^2","v":0.88302222155948906}]
[" sloj 2. ..............................",{"$f":"+'C VI-VII'!K88","v":{"$error":"#VALUE!"}},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658},{"$f":"IF(E18=0,COS((-G48)*PI()/180)^2*COS((-G48)*PI()/180),COS((-G48)*PI()/180)^2*COS((-G48+E18)*PI()/180))","v":1},{"$f":"IF(G18=0,COS((-G48)*PI()/180)^2*COS((-G48)*PI()/180),COS((-G48)*PI()/180)^2*COS((-G48+F18)*PI()/180))","v":1},{"$f":"IF(F18=0,COS((-G48)*PI()/180)^2*COS((-G48)*PI()/180),COS((-G48)*PI()/180)^2*COS((-G48+G18)*PI()/180))","v":1}]
[" sloj 3. ..............................",{"$f":"+'P III-III'!B99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!C99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!D99","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527},{"$f":"IF(E18=0,SIN((E14)*PI()/180)*SIN((E14-E19)*PI()/180),SIN((E14+E18)*PI()/180)*SIN((E14-E19)*PI()/180))","v":0.10325557088077568},{"$f":"IF(G18=0,SIN((F14)*PI()/180)*SIN((F14-F19)*PI()/180),SIN((F14+F18)*PI()/180)*SIN((F14-F19)*PI()/180))","v":7.4757977051699134E-2},{"$f":"IF(F18=0,SIN((G14)*PI()/180)*SIN((G14-G19)*PI()/180),SIN((G14+G18)*PI()/180)*SIN((G14-G19)*PI()/180))","v":0.10569003670618687}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(E18=0,COS((-G48)*PI()/180)*COS((E19+G48)*PI()/180),COS((-G48+E18)*PI()/180)*COS((E19+G48)*PI()/180))","v":0.99452189536827329},{"$f":"IF(G18=0,COS((-G48)*PI()/180)*COS((F19+G48)*PI()/180),COS((-G48+F18)*PI()/180)*COS((F19+G48)*PI()/180))","v":0.9975640502598242},{"$f":"IF(I18=0,COS((-G48)*PI()/180)*COS((G19+G48)*PI()/180),COS((-G48+G18)*PI()/180)*COS((G19+G48)*PI()/180))","v":0.99939082701909576},{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0},{"$f":"SQRT(G99/G100)","v":0.32221783226829248},{"$f":"SQRT(H99/H100)","v":0.27375267745250276},{"$f":"SQRT(I99/I100)","v":0.32519910741806074}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0},{"$f":"(1+G101)^2","v":1.7482599959682625},{"$f":"(1+H101)^2","v":1.6224458833174196},{"$f":"(1+I101)^2","v":1.7561526743016247}]
[null,null,null,null,null,null,{"$f":"(G97/G98)/G102","v":0.49172886307062297},{"$f":"(H97/H98)/H102","v":0.55749686722248182},{"$f":"(I97/I98)/I102","v":0.50281631801212479}]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,0,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I120","v":1},null,null,{"$f":"+'C VI-VII'!N87","v":{"$error":"#VALUE!"}}]
[" Eh2 .............................................",{"$f":"+C98","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I121","v":1},null,null,{"$f":"+'C VI-VII'!K87","v":{"$error":"#VALUE!"}}]
[" Eh3 .....................................................",{"$f":"+C99","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I122","v":1},null,null,{"$f":"+C110+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPrometno ....................................",{"$f":"'HT III-XX'!#REF!","v":{"$error":"#REF!"}},{"$f":"'HT III-XX'!#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I124","v":1.3},null,null,{"$f":"+C111+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPTočkasto ......................................",{"$f":"+'HT III-XX'!#REF!","v":{"$error":"#REF!"}},{"$f":"+'HT III-XX'!#REF!","v":{"$error":"#REF!"}},{"$f":"+B112*C112","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I125","v":1},null,null,{"$f":"+C112+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPLinijsko ................................",{"$f":"'HT III-XX'!#REF!","v":{"$error":"#REF!"}},{"$f":"'HT III-XX'!#REF!","v":{"$error":"#REF!"}},{"$f":"+B113*C113","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I126","v":1}]
[" EQTemelj ....................................................",{"$f":"+'HT III-XX'!#REF!","v":{"$error":"#REF!"}},{"$f":"+'HT III-XX'!#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I127","v":1},null,null,{"$f":"+C114+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,null,{"$f":"+'C VI-VII'!$AI$44","v":1.5001009999999999},{"$f":"+'C VI-VII'!$AH$44","v":4.9000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":-2.2699256917793105},{"$f":"IF(H115<'Analiza i dimenzioniranje'!V44,0,H115-'Analiza i dimenzioniranje'!V44)","v":168.6927659574468},{"$f":"+B115*C115","v":-382.92004346412273},{"$f":"+'Analiza i dimenzioniranje'!I129","v":0},null,null,{"$f":"+E40","v":170.21276595744681},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":6.9000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":0},{"$f":"+H116-'Analiza i dimenzioniranje'!V44","v":-1.52},{"$f":"B116*C116","v":0},{"$f":"+'Analiza i dimenzioniranje'!I150","v":0},"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C VI-VII'!AC117","v":0}]
[{"$f":"+A101","v":{"$error":"#VALUE!"}},{"$f":"-B101","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!E116","v":0},null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}},null,null,"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C VI-VII'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C VI-VII'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},{"$f":"+'Analiza i dimenzioniranje'!I135","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C VI-VII'!L61","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VI-VII'!L59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I136","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C VI-VII'!L59","v":{"$error":"#VALUE!"}}]
[" Gnasip na konzoli.............................",{"$f":"IF(M61>=E67+E68,0,'C VI-VII'!N61)","v":{"$error":"#VALUE!"}},{"$f":"IF(B128=0,0,2+E57-'C VI-VII'!N59)","v":{"$error":"#VALUE!"}},{"$f":"B128*C128","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I138","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C128","v":{"$error":"#VALUE!"}}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C VI-VII'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I139","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},{"$f":"+'Analiza i dimenzioniranje'!I140","v":{"$error":"#VALUE!"}},null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C VI-VII'!W18<'C VI-VII'!B7,0,('C VI-VII'!W18-'C VI-VII'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C VI-VII'!W18+'C VI-VII'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I141","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C VI-VII'!W23>'C VI-VII'!E21,'Analiza i dimenzioniranje'!E36,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C VI-VII'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I142","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C VI-VII'!W26>'C VI-VII'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C VI-VII'!W25)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I143","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C VI-VII'!W31>'C VI-VII'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VI-VII'!W33-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I144","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":0.60822475599092374},{"$f":"2+E57-'C VI-VII'!AB24-E54-'Analiza i dimenzioniranje'!V49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I145","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VI-VII'!M93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I146","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VI-VII'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I147","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VI-VII'!E93","v":2.9000021999999994},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I148","v":1},null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]
[]
[]
[null,null,null,{"$f":"+'C VI-VII'!W23","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,{"$f":"'C VI-VII'!E23","v":0}]

{"sheet":"P VII-VII","index":18,"n_rows":175,"n_cols":24,"rows_kept":175,"cut":false,"hidden":true,"merged":[[13,10,13,11],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[7,0,7,9],[162,1,162,2],[46,0,46,2],[34,10,34,11],[28,0,28,2],[71,0,71,7],[72,0,72,8],[73,0,73,9],[95,6,95,8],[56,10,56,18],[57,10,57,18],[68,0,68,8],[69,0,69,8],[64,11,64,12],[28,10,28,11],[29,10,29,11],[30,10,30,11],[33,10,33,11],[20,10,20,11],[21,10,21,11],[24,0,24,2],[25,0,25,2],[27,0,27,2],[27,10,27,11]]}
[" UPUTE ZA RAD: - Ispuniti sve podatke u čelijama s plavom bojom. Ispuniti i za izbor armature u kolonama L,N i O",null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  "]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C VI-VII'!C15","v":0.5}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#VALUE!"}}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,null,{"$f":"+M9","v":{"$error":"#VALUE!"}}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"+M10","v":{"$error":"#VALUE!"}}]
[null,"milenium","GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ....................................................",null,{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":2.2699256917793105},null,null,null,null,null,null,{"$f":"M15","v":2.2699256917793105}]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":0.5},null,null,null,null,null,null,0.5]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":2},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-'P VII-VII'!M61)","v":2.16},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#VALUE!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S8:S17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T8:T17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U8:U17)","v":0}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C VI-VII'!V61+'C VI-VII'!X61+'C VI-VII'!Z61","v":68.875052249999982},{"$f":"+'C VI-VII'!Z61","v":13.306056250595223},{"$f":"+'C VI-VII'!V61","v":37.77589163555291},null,{"$f":"+'C VI-VII'!X61","v":17.793104363851846}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli.............................",null,{"$error":"#VALUE!"},null,null,{"$f":"+M21","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza.............",null,0,null,{"$f":"+M22","v":0}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",0,null,{"$f":"+M27","v":0}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",0.60822475599092374,null,null,{"$f":"+M28","v":0.60822475599092374}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",{"$error":"#VALUE!"},null,{"$f":"+M31","v":{"$error":"#VALUE!"}}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.306056250595223},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":17.793104363851846}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C VI-VII'!Z76+'C VI-VII'!AB76+'C VI-VII'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":0},null,{"$f":"+'C VI-VII'!AB76","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+X35","v":0}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},null,{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#VALUE!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,"EUROCOD 2",null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!W40","v":2.35},"kN/m'",null,null,null,null,"Marka betona",15,20,25,30,40]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"IF(E38=0,0,'Analiza i dimenzioniranje'!E39)","v":15},"°    ",null,null,null,null,"Klasa betona C","12/15","16/20","20/25","25/30","30/37"]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!W42","v":170.21276595744681},"m",null,null,null,null,"fcm (N/mm2)",20,24,28,33,38]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*'C VI-VII'!AI118*C42/B42","v":-0.5},"kN/m'",null,null,null,null,"ecu  (%0)",-3.6,-3.5,-3.4,-3.3,-3.2]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'P VI-VI'!C42","v":1},null,null,null,null,null,null,null,"fck valjak (N/mm2)",12,16,20,25,30]
[null,null,"DIMENZIJE ZIDA:",null,null,null,"          GRADIVO TEMELJA I ZIDA:",null,null,null,"fck kocka (N/mm2)",15,20,25,30,37]
[null,null,null,null,null,null,null,null,500,500,"Ecm (N/mm2)",26000,27500,29000,30500,32000]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":5.36},"m",null,null,null,null,"ARMATURA",null,null,500]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C VI-VII'!B10-'C VI-VII'!B11=0,\">100\",IF('C VI-VII'!C10-'C VI-VII'!C11/(0.00000000000001+'C VI-VII'!B11-'C VI-VII'!B10)>100,\">100\",('C VI-VII'!C10-'C VI-VII'!C11)/('C VI-VII'!B11-'C VI-VII'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C VI-VII'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C VI-VII'!E64","v":1.4000010999999999},"m",{"$f":"+IF(E32=0,\"\",IF(G54>#REF!+E36,\"PAZI POLOŽAJ TEMELJA\",\"\"))","v":{"$error":"#REF!"}}]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m",null,null,null,null,"FAKTORI STABILNOSTI I KONTAKTNI NAPONI"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 ",null,null,null,null,null,null,null,null,"M="," -  "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 ",null,null,null,null,null,null,null,null,"     v=","+"]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m",null,null,null,null,"MOMENTI SAVIJANJA (kNm/m')",null,null,null,"     h=","-"]
[" zapreminska težina nasipa ...............................",null,null,"gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,"Moment na koti +",null,{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},"Mkonzole"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!D63","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!V44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C VI-VII'!I87-'C VI-VII'!Q17)-B109*('C VI-VII'!K87-'C VI-VII'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C VI-VII'!Q16-'C VI-VII'!N59)+B136*('C VI-VII'!Q16-'C VI-VII'!M93)+B137*('C VI-VII'!Q16-'C VI-VII'!C93)+B135*(C135),-B116*C116/1.35-B108*('C VI-VII'!I87-'C VI-VII'!Q17)-B109*('C VI-VII'!K87-'C VI-VII'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C VI-VII'!Q16-'C VI-VII'!M93)+B137*('C VI-VII'!Q16-'C VI-VII'!C93)+B135*(C135))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+E592)","v":0},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+'Dijagram momenata'!Q18","v":1.84},null,{"$f":"-'HT III-XX'!#REF!*N66","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":2.2122453236948392},{"$f":"-B111*'HT III-XX'!#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota",null,"krak od presjeka do sile","     v11=",{"$f":"B130+'C VI-VII'!Z61+'C VI-VII'!AD76","v":{"$error":"#VALUE!"}}]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c111",{"$f":"IF(+L66-'Dijagram momenata'!$Q$18>0,+L66-'Dijagram momenata'!$Q$18,0)","v":{"$error":"#REF!"}},"     h11=",{"$f":"+B118*E54/E57-B117","v":{"$error":"#VALUE!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c112",{"$f":"IF(+L67-'Dijagram momenata'!$Q$18>0,+L67-'Dijagram momenata'!$Q$18,0)","v":{"$error":"#REF!"}},"     v22=",{"$f":"+B129+B131+B132+B133+B134+B138+'C VI-VII'!Z76+'C VI-VII'!V61","v":{"$error":"#VALUE!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c113",{"$f":"IF(+L68-'Dijagram momenata'!$Q$18>0,+L68-'Dijagram momenata'!$Q$18,0)","v":{"$error":"#REF!"}},"     h22=",{"$f":"+B118*E55/E57-B110","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c114",{"$f":"IF(+L69-'Dijagram momenata'!$Q$18>0,+L69-'Dijagram momenata'!$Q$18,0)","v":{"$error":"#REF!"}},"     v33=",{"$f":"B127+B128+B135+B136+B137","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     h33=",{"$f":"-B108-B109-B111-B112-B113-B114+B115-B116","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko"," -koeficijent mirnog pritiska",null,null,"     vtem=",{"$f":"+'C VI-VII'!X61+'C VI-VII'!AB76","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko1=","1-sinj1=",{"$f":"1-SIN(E14*PI()/180)","v":0.62539340658408804},"varijanta","     htem=",{"$f":"+B118*E51/E57","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko2=","1-sinj2=",{"$f":"1-SIN(F14*PI()/180)","v":0.69098300562505255},"n","    MI-I",{"$f":"+K62","v":0}]
[null,null,null,null,null,null,null,null,null,null,"Ko3=","1-sinj3=",{"$f":"1-SIN(G14*PI()/180)","v":0.65797985667433134},null,"MII-II",{"$f":"+L62","v":0}]
[null,null,null,null,null,null,null,null,null,null,"Ko=","n/(1-n) =",{"$f":"+N75/(1-N75)","v":0.66666666666666674},0.4,"Mzida",{"$f":"+M62","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+(B172*E51*E58)","v":0},{"$f":"+E51/2","v":0.4},{"$f":"+K76*L76","v":0}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+'C VI-VII'!N85","v":{"$error":"#VALUE!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+'C VI-VII'!P88","v":{"$error":"#VALUE!"}},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658}]
[" sloj 3. ..............................",{"$f":"+'P III-III'!B99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!C99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!D99","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,null,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#VALUE!"}},null,null,1.35,null,null,{"$f":"+'C VI-VII'!N87","v":{"$error":"#VALUE!"}}]
[" Eh2 .............................................",{"$f":"+C98","v":{"$error":"#VALUE!"}},null,null,1.35,null,null,{"$f":"+'C VI-VII'!P87","v":{"$error":"#VALUE!"}}]
[" Eh3 .....................................................",{"$f":"+C99","v":{"$error":"#VALUE!"}},null,null,1.35,null,null,{"$f":"+C110+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPrometno ....................................",{"$f":"'HT III-XX'!#REF!","v":{"$error":"#REF!"}},{"$f":"'HT III-XX'!#REF!","v":{"$error":"#REF!"}},null,1.5]
[" EPTočkasto ......................................",{"$f":"+'HT III-XX'!#REF!","v":{"$error":"#REF!"}},{"$f":"+'HT III-XX'!#REF!","v":{"$error":"#REF!"}},{"$f":"B112*C112","v":{"$error":"#REF!"}},1.35,null,null,{"$f":"+C112+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPLinijsko ................................",{"$f":"'HT III-XX'!#REF!","v":{"$error":"#REF!"}},{"$f":"'HT III-XX'!#REF!","v":{"$error":"#REF!"}},{"$f":"B113*C113","v":{"$error":"#REF!"}},1.35,null,null,{"$f":"+C113+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EQTemelj ....................................................",{"$f":"'HT III-XX'!#REF!","v":{"$error":"#REF!"}},{"$f":"'HT III-XX'!#REF!","v":{"$error":"#REF!"}},null,1.35,null,null,{"$f":"+C114+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,null,{"$f":"+'C VI-VII'!$AI$44","v":1.5001009999999999},{"$f":"+'C VI-VII'!$AH$44","v":4.9000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":-2.2699256917793105},{"$f":"IF(H115<'Analiza i dimenzioniranje'!W44,0,H115-'Analiza i dimenzioniranje'!W44)","v":168.3727659574468},null,1.35,null,null,{"$f":"+E40","v":170.21276595744681},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":6.9000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":-0.5},{"$f":"+H116-'Analiza i dimenzioniranje'!W44","v":4.4244906473896783},{"$f":"B116*C116","v":-2.2122453236948392},1,"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C VI-VII'!AI117","v":6.2644906473896782}]
[{"$f":"+A101","v":{"$error":"#VALUE!"}},{"$f":"-B101","v":{"$error":"#VALUE!"}},{"$f":"IF(F101=0,0,E49/3)","v":0},{"$f":"B117*C117","v":{"$error":"#VALUE!"}},1.35,null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}}," S MHA =",{"$f":"SUM(D108:D117)","v":{"$error":"#REF!"}},"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C VI-VII'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C VI-VII'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},1.35,null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C VI-VII'!P61","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VI-VII'!P59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},1.35,null,null,{"$f":"2+$E$57-C127","v":{"$error":"#VALUE!"}}]
[" Gnasip na konzoli.............................",{"$f":"'C VI-VII'!R61","v":{"$error":"#VALUE!"}},{"$f":"IF(B128=0,0,2+E57-'C VI-VII'!R59)","v":{"$error":"#VALUE!"}},{"$f":"B128*C128","v":{"$error":"#VALUE!"}},1.35,null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C VI-VII'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},1.35,null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},1.35,null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C VI-VII'!W18<'C VI-VII'!B7,0,('C VI-VII'!W18-'C VI-VII'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C VI-VII'!W18+'C VI-VII'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},1.5,null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C VI-VII'!W23>'C VI-VII'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C VI-VII'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C VI-VII'!W26>'C VI-VII'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C VI-VII'!W25)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",0,{"$f":"+'Rasprostiranje vertikalnog opt'!#REF!","v":{"$error":"#REF!"}},{"$error":"#REF!"},1.35,null,null,{"$error":"#REF!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":0.60822475599092374},{"$f":"2+E57-'C VI-VII'!AC24-E54-'Analiza i dimenzioniranje'!W49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VI-VII'!H93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VI-VII'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VI-VII'!E93","v":2.9000021999999994},{"$error":"#VALUE!"},1.35,null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]
[]
[]
[]
[" Rezultanta sila .........................................",null,"      R =",{"$f":"SQRT(B118^2+B139^2)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" sila uzduž temelja ..................................................",null,{"$f":"IF(E48=E49,\"     RH =\",\"     RT =\")","v":"     RT ="},{"$f":"D144*SIN((D148-D149)*PI()/180)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" sila okomita na temelj .................................",null,"    RN =",{"$f":"D144*COS((D148-D149)*PI()/180)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" moment oko osi temelja.....................................",null,"     Ms =",{"$f":"+B118*(I118-'C VI-VII'!AC50)-'Analiza i dimenzioniranje'!B168*(F139-E57/2)","v":{"$error":"#VALUE!"}},"kNm/m'"]
[" otklon rezultante od vertikale .....................................",null,"a =",{"$f":"ATAN(B118/B139)*180/PI()","v":{"$error":"#VALUE!"}},"°"]
[" nagib temelja ..........................................",null,"b =",{"$f":"ATAN('C VI-VII'!C15/E57)*180/PI()","v":9.7823997540577476},"°"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,{"$f":"IF(E49=E48,\"\",+D167*COS(D149*PI()/180))","v":0}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"za Presjeke I-I i II-II"]
[null,null,null,null,null,null,null,null,null,null,"     As,min=",{"$f":"+MAX(E251,E269)","v":0},{"$f":"+MAX(L174:L175)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"     As,1 mjer =",{"$f":"+IF(E255>L173/2,E255,L173/2)","v":0},{"$f":"+L174-7.85","v":-7.85}]
[null,null,null,null,null,null,null,null,null,null,"     As,2 mjer =",{"$f":"+IF(E273>L173/2,E273,L173/2)","v":0},{"$f":"+L175-7.85","v":-7.85}]

{"sheet":"P VIII-VIII","index":19,"n_rows":140,"n_cols":38,"rows_kept":140,"cut":false,"hidden":true,"merged":[[46,38,46,39],[46,35,46,36],[45,32,46,32],[44,38,45,38],[47,38,48,38],[48,32,49,32],[47,35,48,35],[45,20,46,20],[45,23,46,23],[47,29,47,30],[44,35,45,35],[48,20,49,20],[47,23,47,24],[48,23,49,23],[48,26,49,26],[48,29,49,29],[45,26,46,26],[45,29,46,29],[48,11,49,11],[47,32,47,33],[47,11,47,12],[47,14,47,15],[47,17,47,18],[47,20,47,21],[48,14,49,14],[48,17,49,17],[47,26,47,27],[45,11,46,11],[45,14,46,14],[45,17,46,17],[20,10,20,11],[28,10,28,11],[29,10,29,11],[30,10,30,11],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[16,10,16,11],[7,10,7,11],[8,10,8,11],[9,10,9,11],[10,10,10,11],[11,10,11,11],[12,10,12,11],[64,11,64,12],[7,0,7,9],[13,10,13,11],[14,10,14,11],[15,10,15,11],[18,10,18,11],[19,10,19,11],[34,10,34,11],[21,10,21,11],[22,10,22,11],[23,10,23,11],[24,10,24,11],[25,10,25,11],[26,10,26,11],[27,10,27,11],[33,10,33,11]]}
[" UPUTE ZA RAD: - Ispuniti sve podatke u čelijama s plavom bojom. Ispuniti i za izbor armature u kolonama L,N i O",null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z18/M18","v":{"$error":"#VALUE!"}}]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  ","krak                  y  ","Moment destabilnosti i stabilnosti","za Mzida                                              krakovi                             x                  y",null,"Moment zida II","za M u                           presjeku II-II                                                   krakovi                                x               y",null,"Moment      II-II","za M u                           temelju ispod zida                     krakovi                             x                  y",null,"Moment  ","za M u                           presjeku I-I                                              krakovi                             x                  y",null,"Moment      I-I"]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C VIII-IX'!C15","v":0.5},null,null,null,{"$f":"2+E57-E54-E51/2","v":3.8000010999999998},{"$f":"+E48","v":1.2},null,{"$f":"2+E55","v":3.4000010999999999},{"$f":"'C VIII-IX'!AC47+(E48-'C VIII-IX'!AC47)/2","v":0.72068965844232813},null,{"$f":"2+E55+E51/2","v":3.8000010999999998},{"$f":"'C VIII-IX'!AC49+(E48-'C VIII-IX'!AF47)/2","v":0.97931024673015765},null,{"$f":"2+E55+E51","v":4.2000010999999997},{"$f":"'C VIII-IX'!AC49+(E48-'C VIII-IX'!AC49)/2","v":0.78965512336507881}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#VALUE!"}},null,null,{"$f":"+H108","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$W$7","v":{"$error":"#VALUE!"}},{"$f":"+M8*Y8","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$AB$7","v":{"$error":"#VALUE!"}},{"$f":"T8*AB8","v":{"$error":"#VALUE!"}}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,null,{"$f":"+M9","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$f":"+W9-$AB$7","v":{"$error":"#VALUE!"}},{"$f":"AB9*T9","v":{"$error":"#VALUE!"}}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"+M10","v":{"$error":"#VALUE!"}},null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,{"$f":"+AE7-'C VIII-IX'!F93","v":{"$error":"#VALUE!"}},{"$f":"+AE10*S10","v":{"$error":"#VALUE!"}}]
[null,null,"GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$f":"+W11-$AB$7","v":{"$error":"#REF!"}},{"$f":"AB11*T11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ...................................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":2.2699256917793105},null,null,null,null,null,null,{"$f":"M15","v":2.2699256917793105},null,null,170.21276595744681,null,169.71276595744681,{"$f":"-M15*Y15","v":-385.23536766973763},null,169.01276595744682,383.64641968549216]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":2},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-'P VIII-VIII'!M61)","v":1.8399999999999999},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#VALUE!"}},null,null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,{"$f":"+AK7-C117","v":0.78965512336507881},{"$f":"+M17*AK17","v":{"$error":"#VALUE!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S8:S17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T8:T17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U8:U17)","v":0},null,null,"x",null,{"$f":"SUM(Z8:Z17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC8:AC17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF8:AF17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI8:AI17)","v":0},null,null,{"$f":"SUM(AL8:AL17)","v":{"$error":"#VALUE!"}}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C VIII-IX'!V61+'C VIII-IX'!X61+'C VIII-IX'!Z61","v":68.875052249999982},{"$f":"+'C VIII-IX'!Z61","v":13.306056250595223},{"$f":"+'C VIII-IX'!V61","v":37.77589163555291},null,{"$f":"+'C VIII-IX'!X61","v":17.793104363851846},null,null,null,null,{"$f":"+H126","v":3.3485779696489133},null,{"$f":"+$V$7-V19","v":1.5514242303510861},null,{"$f":"+M19*X19","v":106.85442492734707},null,null,null,{"$f":"AD7-'C VIII-IX'!V59","v":0.72609215808095717},null,{"$f":"+AD19*O19","v":27.428778681090989},{"$f":"+AG7-'C VIII-IX'!X59","v":1.0335908939774985E-2},null,{"$f":"+'C VIII-IX'!X61*'Analiza i dimenzioniranje'!AQ13","v":0.14465929289570792},{"$f":"AJ7-'C VIII-IX'!Z59","v":-0.34074126926177506},null,{"$f":"+'C VIII-IX'!Z61*'Analiza i dimenzioniranje'!AT13","v":-4.5636103109654318}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M20","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V20","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V20","v":{"$error":"#VALUE!"}},null,{"$f":"+P20*AA20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli............................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M21","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V21","v":{"$error":"#VALUE!"}},null,{"$f":"+P21*AA21","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza............."," ",0,null,{"$f":"+M22","v":0},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+AD7-V22","v":{"$error":"#VALUE!"}},null,{"$f":"+M22*AD22","v":{"$error":"#VALUE!"}}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0},null,null,null,null,null,null,null,4.5500016499999996,null,0.35000054999999985,null,0,null,null,null,null,null,null,null,null,null,{"$f":"AJ7-(2+E57-E54/2)","v":-0.35000054999999985},null,{"$f":"+AJ23*N23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X24","v":{"$error":"#VALUE!"}},null,{"$f":"+M24*AD24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X25","v":{"$error":"#VALUE!"}},null,{"$f":"+M25*AD25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X26","v":{"$error":"#VALUE!"}},null,{"$f":"+M26*AD26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X27","v":{"$error":"#VALUE!"}},null,{"$f":"+M27*AD27","v":{"$error":"#VALUE!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",0.60822475599092374,null,null,{"$f":"+M28","v":0.60822475599092374},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V28","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V28","v":{"$error":"#VALUE!"}},null,{"$f":"P28*AA28","v":{"$error":"#VALUE!"}}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M29","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V29","v":{"$error":"#VALUE!"}},null,{"$f":"+P29*AA29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M30","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V30","v":{"$error":"#VALUE!"}},null,{"$f":"+P30*AA30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",{"$error":"#VALUE!"},null,{"$f":"+M31","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,2,null,2.9000021999999994,null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-'C VIII-IX'!E93","v":1.4000010999999999},null,{"$f":"+M31*AD31","v":{"$error":"#VALUE!"}},{"$f":"+$AD$7-AD31","v":2}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.306056250595223},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":17.793104363851846},null,null,null,null,null,null,null,null,{"$f":"SUM(Z19:Z31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC19:AC31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF19:AF31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI19:AI31)","v":0.14465929289570792},null,null,{"$f":"SUM(AL19:AL31)","v":-4.5636103109654318}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"II-II","sredina","I-I"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C VIII-IX'!Z76+'C VIII-IX'!AB76+'C VIII-IX'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":{"$error":"#VALUE!"}},null,{"$f":"+'C VIII-IX'!AB76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+'C VIII-IX'!Z76","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!AB76","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!AD76","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"$AD$7-'C VIII-IX'!Z77","v":{"$error":"#VALUE!"}},null,{"$f":"+X34*AD34","v":{"$error":"#VALUE!"}},{"$f":"$AG$7-'C VIII-IX'!AB77","v":{"$error":"#VALUE!"}},null,{"$f":"-Y34*AG34","v":{"$error":"#VALUE!"}},{"$f":"+AJ7-'C VIII-IX'!AD77","v":{"$error":"#VALUE!"}},null,{"$f":"+Z34*AJ34","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+Z35","v":{"$error":"#VALUE!"}},{"$f":"+X35","v":{"$error":"#VALUE!"}},null,{"$f":"+Y35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M35*E55/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E51/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E54/E57","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AE7-'C VIII-IX'!AC45","v":{"$error":"#VALUE!"}},{"$f":"-S35*AE35","v":{"$error":"#VALUE!"}},null,{"$f":"+AH7-'C VIII-IX'!AC48","v":{"$error":"#VALUE!"}},{"$f":"Y35*AH35","v":{"$error":"#VALUE!"}},null,{"$f":"+AK7-'C VIII-IX'!AC52","v":{"$error":"#VALUE!"}},{"$f":"-Z35*AK35","v":{"$error":"#VALUE!"}}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},{"$f":"R18+R35","v":{"$error":"#VALUE!"}},{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#VALUE!"}},{"$f":"+U18+U35","v":{"$error":"#VALUE!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"SUM(R36:U36)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+AC18+AC32+AC34+AC35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AF18+AF32+AF34+AF35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AI18+AI32+AI34+AI35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AL18+AL32+AL34+AL35","v":{"$error":"#VALUE!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!X40","v":2.35},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y","x"]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"+'Analiza i dimenzioniranje'!E39","v":15},"°    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD7","v":3.4000010999999999},{"$f":"+AE7","v":0.72068965844232813}]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!X42","v":170.21276595744681},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'C VIII-IX'!V61*('Analiza i dimenzioniranje'!AI33-'C VIII-IX'!V59)+B129*(AD39-H129)+B138*(AD39-H138)+B138*(AD39-H138)+'C VIII-IX'!Z76*('Analiza i dimenzioniranje'!AI33-'C VIII-IX'!Z77)+S35*(AE39-'C VIII-IX'!AG66)+B110*(AE39-H110)","v":{"$error":"#VALUE!"}}]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*'C VIII-IX'!AC118*C42/B42","v":{"$error":"#VALUE!"}},"kN/m'"]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'P VII-VII'!C42","v":1}]
[null,null,"DIMENZIJE ZIDA:"]
[]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":5.04},"m"]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C VIII-IX'!B10-'C VIII-IX'!B11=0,\">100\",IF('C VIII-IX'!C10-'C VIII-IX'!C11/(0.00000000000001+'C VIII-IX'!B11-'C VIII-IX'!B10)>100,\">100\",('C VIII-IX'!C10-'C VIII-IX'!C11)/('C VIII-IX'!B11-'C VIII-IX'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C VIII-IX'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C VIII-IX'!E64","v":1.4000010999999999},"m"]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 "]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m"]
[" zapreminska težina nasipa ...............................",null,null,"      gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!X44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C VIII-IX'!I87-'C VIII-IX'!Q17)-B109*('C VIII-IX'!K87-'C VIII-IX'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C VIII-IX'!Q16-'C VIII-IX'!N59)+B136*('C VIII-IX'!Q16-'C VIII-IX'!M93)+B137*('C VIII-IX'!Q16-'C VIII-IX'!C93)+B135*(C135),-B116*C116/1.35-B108*('C VIII-IX'!I87-'C VIII-IX'!Q17)-B109*('C VIII-IX'!K87-'C VIII-IX'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C VIII-IX'!Q16-'C VIII-IX'!M93)+B137*('C VIII-IX'!Q16-'C VIII-IX'!C93)+B135*(C135))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+#REF!)","v":{"$error":"#REF!"}},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+'Dijagram momenata'!Q17","v":2.16},null,{"$f":"-#REF!*N66","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":{"$error":"#VALUE!"}},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota",null,"krak od presjeka do sile"]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c111",{"$f":"IF(+L66-'Dijagram momenata'!$Q$17>0,+L66-'Dijagram momenata'!$Q$17,0)","v":{"$error":"#REF!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c112",{"$f":"IF(+L67-'Dijagram momenata'!$Q$17>0,+L67-'Dijagram momenata'!$Q$17,0)","v":{"$error":"#REF!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c113",{"$f":"IF(+L68-'Dijagram momenata'!$Q$17>0,+L68-'Dijagram momenata'!$Q$17,0)","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c114",{"$f":"IF(+L69-'Dijagram momenata'!$Q$17>0,+L69-'Dijagram momenata'!$Q$17,0)","v":{"$error":"#REF!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+'C VIII-IX'!I85","v":{"$error":"#VALUE!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+'C VIII-IX'!K88","v":{"$error":"#VALUE!"}},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658}]
[" sloj 3. ..............................",{"$f":"+'P III-III'!B99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!C99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!D99","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,null,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I120","v":1},null,null,{"$f":"+'C VIII-IX'!N87","v":{"$error":"#VALUE!"}}]
[" Eh2 .............................................",{"$f":"+C98","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I121","v":1},null,null,{"$f":"+'C VIII-IX'!K87","v":{"$error":"#VALUE!"}}]
[" Eh3 .....................................................",{"$f":"+C99","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I122","v":1},null,null,{"$f":"+C110+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPrometno ....................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I124","v":1.3},null,null,{"$f":"+C111+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+B112*C112","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I125","v":1},null,null,{"$f":"+C112+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPLinijsko ................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"+B113*C113","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I126","v":1}]
[" EQTemelj ....................................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I127","v":1},null,null,{"$f":"+C114+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,null,{"$f":"+'C VIII-IX'!$AI$44","v":1.5001009999999999},{"$f":"+'C VIII-IX'!$AH$44","v":4.9000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":-2.2699256917793105},{"$f":"IF(H115<'Analiza i dimenzioniranje'!X44,0,H115-'Analiza i dimenzioniranje'!X44)","v":168.05276595744681},{"$f":"+B115*C115","v":-381.46729102138403},{"$f":"+'Analiza i dimenzioniranje'!I129","v":0},null,null,{"$f":"+E40","v":170.21276595744681},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":6.9000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":{"$error":"#VALUE!"}},{"$f":"+H116-'Analiza i dimenzioniranje'!X44","v":{"$error":"#VALUE!"}},{"$f":"B116*C116","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I150","v":0},"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C VIII-IX'!AC117","v":{"$error":"#VALUE!"}}]
[{"$f":"+A101","v":{"$error":"#VALUE!"}},{"$f":"-B101","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!E116","v":0},null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}},null,null,"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C VIII-IX'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C VIII-IX'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},{"$f":"+'Analiza i dimenzioniranje'!I135","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C VIII-IX'!L61","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VIII-IX'!L59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I136","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C VIII-IX'!L59","v":{"$error":"#VALUE!"}}]
[" Gnasip na konzoli.............................",{"$f":"IF(M61>=E67+E68,0,'C VIII-IX'!R61)","v":{"$error":"#VALUE!"}},{"$f":"IF(B128=0,0,2+E57-'C VIII-IX'!R59)","v":{"$error":"#VALUE!"}},{"$f":"B128*C128","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I138","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C128","v":{"$error":"#VALUE!"}}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C VIII-IX'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I139","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},{"$f":"+'Analiza i dimenzioniranje'!I140","v":{"$error":"#VALUE!"}},null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C VIII-IX'!W18<'C VIII-IX'!B7,0,('C VIII-IX'!W18-'C VIII-IX'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C VIII-IX'!W18+'C VIII-IX'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I141","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C VIII-IX'!W23>'C VIII-IX'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C VIII-IX'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I142","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C VIII-IX'!W26>'C VIII-IX'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C VIII-IX'!W25)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I143","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C VIII-IX'!W31>'C VIII-IX'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VIII-IX'!W33-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I144","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":0.60822475599092374},{"$f":"2+E57-'C VIII-IX'!AB24-E54-'Analiza i dimenzioniranje'!X49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I145","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VIII-IX'!M93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I146","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VIII-IX'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I147","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VIII-IX'!E93","v":2.9000021999999994},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I148","v":1},null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]

{"sheet":"P IX-IX","index":20,"n_rows":175,"n_cols":24,"rows_kept":175,"cut":false,"hidden":true,"merged":[[30,10,30,11],[95,6,95,8],[33,10,33,11],[56,10,56,18],[73,0,73,9],[64,11,64,12],[57,10,57,18],[34,10,34,11],[162,1,162,2],[46,0,46,2],[68,0,68,8],[69,0,69,8],[71,0,71,7],[72,0,72,8],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[7,0,7,9],[13,10,13,11],[20,10,20,11],[21,10,21,11],[29,10,29,11],[27,0,27,2],[27,10,27,11],[28,0,28,2],[28,10,28,11],[24,0,24,2],[25,0,25,2]]}
[" UPUTE ZA RAD: - Ispuniti sve podatke u čelijama s plavom bojom. Ispuniti i za izbor armature u kolonama L,N i O",null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  "]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C VIII-IX'!C15","v":0.5}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#VALUE!"}}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,null,{"$f":"+M9","v":{"$error":"#VALUE!"}}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"+M10","v":{"$error":"#VALUE!"}}]
[null,"milenium","GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ....................................................",null,{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":2.2699256917793105},null,null,null,null,null,null,{"$f":"M15","v":2.2699256917793105}]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"}]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":2},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-'P IX-IX'!M61)","v":1.52},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#VALUE!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S8:S17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T8:T17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U8:U17)","v":0}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C VIII-IX'!V61+'C VIII-IX'!X61+'C VIII-IX'!Z61","v":68.875052249999982},{"$f":"+'C VIII-IX'!Z61","v":13.306056250595223},{"$f":"+'C VIII-IX'!V61","v":37.77589163555291},null,{"$f":"+'C VIII-IX'!X61","v":17.793104363851846}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli.............................",null,{"$error":"#VALUE!"},null,null,{"$f":"+M21","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza.............",null,0,null,{"$f":"+M22","v":0}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",0.60822475599092374,null,null,{"$f":"+M28","v":0.60822475599092374}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",{"$error":"#VALUE!"},null,{"$f":"+M31","v":{"$error":"#VALUE!"}}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.306056250595223},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":17.793104363851846}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C VIII-IX'!Z76+'C VIII-IX'!AB76+'C VIII-IX'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":0},null,{"$f":"+'C VIII-IX'!AB76","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+X35","v":0}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},null,{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#VALUE!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,"EUROCOD 2",null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!Y40","v":2.35},"kN/m'",null,null,null,null,"Marka betona",15,20,25,30,40]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"IF(E38=0,0,'Analiza i dimenzioniranje'!E39)","v":15},"°    ",null,null,null,null,"Klasa betona C","12/15","16/20","20/25","25/30","30/37"]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!Y42","v":170.21276595744681},"m",null,null,null,null,"fcm (N/mm2)",20,24,28,33,38]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*'C VIII-IX'!AE118*C42/B42","v":{"$error":"#VALUE!"}},"kN/m'",null,null,null,null,"ecu  (%0)",-3.6,-3.5,-3.4,-3.3,-3.2]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'P VIII-VIII'!C42","v":1},null,null,null,null,null,null,null,"fck valjak (N/mm2)",12,16,20,25,30]
[null,null,"DIMENZIJE ZIDA:",null,null,null,"          GRADIVO TEMELJA I ZIDA:",null,null,null,"fck kocka (N/mm2)",15,20,25,30,37]
[null,null,null,null,null,null,null,null,500,500,"Ecm (N/mm2)",26000,27500,29000,30500,32000]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":4.72},"m",null,null,null,null,"ARMATURA",null,null,500]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C VIII-IX'!B10-'C VIII-IX'!B11=0,\">100\",IF('C VIII-IX'!C10-'C VIII-IX'!C11/(0.00000000000001+'C VIII-IX'!B11-'C VIII-IX'!B10)>100,\">100\",('C VIII-IX'!C10-'C VIII-IX'!C11)/('C VIII-IX'!B11-'C VIII-IX'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C VIII-IX'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C VIII-IX'!E64","v":1.4000010999999999},"m"]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m",null,null,null,null,"FAKTORI STABILNOSTI I KONTAKTNI NAPONI"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 ",null,null,null,null,null,null,null,null,"M="," -  "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 ",null,null,null,null,null,null,null,null,"     v=","+"]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m",null,null,null,null,"MOMENTI SAVIJANJA (kNm/m')",null,null,null,"     h=","-"]
[" zapreminska težina nasipa ...............................",null,null,"gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,"Moment na koti +",null,{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},"Mkonzole"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!D63","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!Y44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C VIII-IX'!N87-'C VIII-IX'!P17)-B109*('C VIII-IX'!P87-'C VIII-IX'!P17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C VIII-IX'!P16-'C VIII-IX'!R59)+B136*('C VIII-IX'!P16-'C VIII-IX'!H93)+B137*('C VIII-IX'!P16-'C VIII-IX'!C93)+B135*(C135),-B116*C116/1.35-B108*('C VIII-IX'!N87-'C VIII-IX'!P17)-B109*('C VIII-IX'!P87-'C VIII-IX'!P17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C VIII-IX'!P16-'C VIII-IX'!H93)+B137*('C VIII-IX'!P16-'C VIII-IX'!C93)+B135*(C135))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+E592)","v":0},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+M61","v":2.48},null,{"$f":"-#REF!*N66","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":{"$error":"#VALUE!"}},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota",null,"krak od presjeka do sile","     v11=",{"$f":"B130+'C VIII-IX'!Z61+'C VIII-IX'!AD76","v":{"$error":"#VALUE!"}}]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c111",{"$f":"IF(+L66-'Dijagram momenata'!$Q$16>0,+L66-'Dijagram momenata'!$Q$16,0)","v":{"$error":"#REF!"}},"     h11=",{"$f":"+B118*E54/E57-B117","v":{"$error":"#VALUE!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c112",{"$f":"IF(+L67-'Dijagram momenata'!$Q$16>0,+L67-'Dijagram momenata'!$Q$16,0)","v":{"$error":"#REF!"}},"     v22=",{"$f":"+B129+B131+B132+B133+B134+B138+'C VIII-IX'!Z76+'C VIII-IX'!V61","v":{"$error":"#VALUE!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c113",{"$f":"IF(+L68-'Dijagram momenata'!$Q$16>0,+L68-'Dijagram momenata'!$Q$16,0)","v":{"$error":"#REF!"}},"     h22=",{"$f":"+B118*E55/E57-B110","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c114",{"$f":"IF(+L69-'Dijagram momenata'!$Q$16>0,+L69-'Dijagram momenata'!$Q$16,0)","v":{"$error":"#REF!"}},"     v33=",{"$f":"B127+B128+B135+B136+B137","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     h33=",{"$f":"-B108-B109-B111-B112-B113-B114+B115-B116","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko"," -koeficijent mirnog pritiska",null,null,"     vtem=",{"$f":"+'C VIII-IX'!X61+'C VIII-IX'!AB76","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko1=","1-sinj1=",{"$f":"1-SIN(E14*PI()/180)","v":0.62539340658408804},"varijanta","     htem=",{"$f":"+B118*E51/E57","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko2=","1-sinj2=",{"$f":"1-SIN(F14*PI()/180)","v":0.69098300562505255},"n","    MI-I",{"$f":"+K62","v":0}]
[null,null,null,null,null,null,null,null,null,null,"Ko3=","1-sinj3=",{"$f":"1-SIN(G14*PI()/180)","v":0.65797985667433134},null,"MII-II",{"$f":"+L62","v":0}]
[null,null,null,null,null,null,null,null,null,null,"Ko=","n/(1-n) =",{"$f":"+N75/(1-N75)","v":0.66666666666666674},0.4,"Mzida",{"$f":"+M62","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+(B172*E51*E58)","v":0},{"$f":"+E51/2","v":0.4},{"$f":"+K76*L76","v":0}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+'C VIII-IX'!N85","v":{"$error":"#VALUE!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+'C VIII-IX'!P88","v":{"$error":"#VALUE!"}},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658}]
[" sloj 3. ..............................",{"$f":"+'P III-III'!B99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!C99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!D99","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,null,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#VALUE!"}},null,null,1.35,null,null,{"$f":"+'C VIII-IX'!N87","v":{"$error":"#VALUE!"}}]
[" Eh2 .............................................",{"$f":"+C98","v":{"$error":"#VALUE!"}},null,null,1.35,null,null,{"$f":"+'C VIII-IX'!P87","v":{"$error":"#VALUE!"}}]
[" Eh3 .....................................................",{"$f":"+C99","v":{"$error":"#VALUE!"}},null,null,1.35,null,null,{"$f":"+C110+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPrometno ....................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,1.5]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"B112*C112","v":{"$error":"#REF!"}},1.35,null,null,{"$f":"+C112+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPLinijsko ................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"B113*C113","v":{"$error":"#REF!"}},1.35,null,null,{"$f":"+C113+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EQTemelj ....................................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,1.35,null,null,{"$f":"+C114+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,null,{"$f":"+'C VIII-IX'!$AI$44","v":1.5001009999999999},{"$f":"+'C VIII-IX'!$AH$44","v":4.9000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":-2.2699256917793105},{"$f":"IF(H115<'Analiza i dimenzioniranje'!Y44,0,H115-'Analiza i dimenzioniranje'!Y44)","v":167.73276595744682},null,1.35,null,null,{"$f":"+E40","v":170.21276595744681},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":6.9000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":{"$error":"#VALUE!"}},{"$f":"+H116-'Analiza i dimenzioniranje'!Y44","v":{"$error":"#VALUE!"}},{"$f":"B116*C116","v":{"$error":"#VALUE!"}},1,"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C VIII-IX'!AE117","v":{"$error":"#VALUE!"}}]
[{"$f":"+A101","v":{"$error":"#VALUE!"}},{"$f":"-B101","v":{"$error":"#VALUE!"}},{"$f":"IF(F101=0,0,E49/3)","v":0},{"$f":"B117*C117","v":{"$error":"#VALUE!"}},1.35,null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}}," S MHA =",null,"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C VIII-IX'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C VIII-IX'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},1.35,null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C VIII-IX'!P61","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VIII-IX'!P59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},1.35,null,null,{"$f":"2+$E$57-C127","v":{"$error":"#VALUE!"}}]
[" Gnasip na konzoli.............................",{"$f":"+'C VIII-IX'!R61","v":{"$error":"#VALUE!"}},{"$f":"IF(B128=0,0,2+E57-'C VIII-IX'!R59)","v":{"$error":"#VALUE!"}},{"$f":"B128*C128","v":{"$error":"#VALUE!"}},1.35,null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C VIII-IX'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},1.35,null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},1.35,null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C VIII-IX'!W18<'C VIII-IX'!B7,0,('C VIII-IX'!W18-'C VIII-IX'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C VIII-IX'!W18+'C VIII-IX'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},1.5,null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C VIII-IX'!W23>'C VIII-IX'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C VIII-IX'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C VIII-IX'!W26>'C VIII-IX'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C VIII-IX'!W25)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C VIII-IX'!W31>'C VIII-IX'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VIII-IX'!W33-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":0.60822475599092374},{"$f":"2+E57-'C VIII-IX'!AC24-E54-'Analiza i dimenzioniranje'!Y49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VIII-IX'!H93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VIII-IX'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C VIII-IX'!E93","v":2.9000021999999994},{"$error":"#VALUE!"},1.35,null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]
[]
[]
[]
[" Rezultanta sila .........................................",null,"      R =",{"$f":"SQRT(B118^2+B139^2)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" sila uzduž temelja ..................................................",null,{"$f":"IF(E48=E49,\"     RH =\",\"     RT =\")","v":"     RT ="},{"$f":"D144*SIN((D148-D149)*PI()/180)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" sila okomita na temelj .................................",null,"    RN =",{"$f":"D144*COS((D148-D149)*PI()/180)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" moment oko osi temelja.....................................",null,"     Ms =",{"$f":"+B118*(I118-'C VIII-IX'!AC50)-'Analiza i dimenzioniranje'!B168*(F139-E57/2)","v":{"$error":"#VALUE!"}},"kNm/m'"]
[" otklon rezultante od vertikale .....................................",null,"a =",{"$f":"ATAN(B118/B139)*180/PI()","v":{"$error":"#VALUE!"}},"°"]
[" nagib temelja ..........................................",null,"b =",{"$f":"ATAN('C VIII-IX'!C15/E57)*180/PI()","v":9.7823997540577476},"°"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,{"$f":"IF(E49=E48,\"\",+D167*COS(D149*PI()/180))","v":0}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"za Presjeke I-I i II-II"]
[null,null,null,null,null,null,null,null,null,null,"     As,min=",{"$f":"+MAX(E251,E269)","v":0},{"$f":"+MAX(L174:L175)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"     As,1 mjer =",{"$f":"+IF(E255>L173/2,E255,L173/2)","v":0},{"$f":"+L174-7.85","v":-7.85}]
[null,null,null,null,null,null,null,null,null,null,"     As,2 mjer =",{"$f":"+IF(E273>L173/2,E273,L173/2)","v":0},{"$f":"+L175-7.85","v":-7.85}]

{"sheet":"P X-X","index":21,"n_rows":140,"n_cols":38,"rows_kept":140,"cut":false,"hidden":true,"merged":[[46,38,46,39],[46,35,46,36],[45,32,46,32],[44,38,45,38],[47,38,48,38],[48,32,49,32],[47,35,48,35],[45,20,46,20],[45,23,46,23],[47,29,47,30],[44,35,45,35],[48,20,49,20],[47,23,47,24],[48,23,49,23],[48,26,49,26],[48,29,49,29],[45,26,46,26],[45,29,46,29],[48,11,49,11],[47,32,47,33],[47,11,47,12],[47,14,47,15],[47,17,47,18],[47,20,47,21],[48,14,49,14],[48,17,49,17],[47,26,47,27],[45,11,46,11],[45,14,46,14],[45,17,46,17],[20,10,20,11],[28,10,28,11],[29,10,29,11],[30,10,30,11],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[16,10,16,11],[7,10,7,11],[8,10,8,11],[9,10,9,11],[10,10,10,11],[11,10,11,11],[12,10,12,11],[64,11,64,12],[7,0,7,9],[13,10,13,11],[14,10,14,11],[15,10,15,11],[18,10,18,11],[19,10,19,11],[34,10,34,11],[21,10,21,11],[22,10,22,11],[23,10,23,11],[24,10,24,11],[25,10,25,11],[26,10,26,11],[27,10,27,11],[33,10,33,11]]}
[" UPUTE ZA RAD: - Ispuniti sve podatke u čelijama s plavom bojom. Ispuniti i za izbor armature u kolonama L,N i O",null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789},null,"ABC"]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z18/M18","v":{"$error":"#VALUE!"}}]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,"aalokinranupass",null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"aalokinranupass",null,null,null,"Koordinate","V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  ","krak                  y  ","Moment destabilnosti i stabilnosti","za Mzida                                              krakovi                             x                  y",null,"Moment zida II","za M u                           presjeku II-II                                                   krakovi                                x               y",null,"Moment      II-II","za M u                           temelju ispod zida                     krakovi                             x                  y",null,"Moment  ","za M u                           presjeku I-I                                              krakovi                             x                  y",null,"Moment      I-I"]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C X-XI'!C15","v":0.5},null,null,null,{"$f":"2+E57-E54-E51/2","v":3.8000010999999998},{"$f":"+E48","v":1.2},null,{"$f":"2+E55","v":3.4000010999999999},{"$f":"'C X-XI'!AC47+(E48-'C X-XI'!AC47)/2","v":0.72068965844232813},null,{"$f":"2+E55+E51/2","v":3.8000010999999998},{"$f":"'C X-XI'!AC49+(E48-'C X-XI'!AF47)/2","v":0.97931024673015765},null,{"$f":"2+E55+E51","v":4.2000010999999997},{"$f":"'C X-XI'!AC49+(E48-'C X-XI'!AC49)/2","v":0.78965512336507881}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#VALUE!"}},null,null,{"$f":"+H108","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$W$7","v":{"$error":"#VALUE!"}},{"$f":"+M8*Y8","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$AB$7","v":{"$error":"#VALUE!"}},{"$f":"T8*AB8","v":{"$error":"#VALUE!"}}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,null,{"$f":"+M9","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$f":"+W9-$AB$7","v":{"$error":"#VALUE!"}},{"$f":"AB9*T9","v":{"$error":"#VALUE!"}}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"+M10","v":{"$error":"#VALUE!"}},null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,{"$f":"+AE7-'C X-XI'!F93","v":{"$error":"#VALUE!"}},{"$f":"+AE10*S10","v":{"$error":"#VALUE!"}}]
[null,null,"GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$f":"+W11-$AB$7","v":{"$error":"#REF!"}},{"$f":"AB11*T11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ...................................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":2.2699256917793105},null,null,null,null,null,null,{"$f":"+M15","v":2.2699256917793105},null,null,170.21276595744681,null,169.71276595744681,{"$f":"-M15*Y15","v":-385.23536766973763},null,169.01276595744682,383.64641968549216]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":0},null,null,null,null,null,null,0,null,null,0,null,-0.5,0,null,-1.2,0]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":2},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-'P X-X'!M61)","v":1.2000000000000002},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#VALUE!"}},null,null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,{"$f":"+AK7-C117","v":0.78965512336507881},{"$f":"+M17*AK17","v":{"$error":"#VALUE!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S8:S17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T8:T17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U8:U17)","v":0},null,null,"x",null,{"$f":"SUM(Z8:Z17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC8:AC17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF8:AF17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI8:AI17)","v":0},null,null,{"$f":"SUM(AL8:AL17)","v":{"$error":"#VALUE!"}}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C X-XI'!V61+'C X-XI'!X61+'C X-XI'!Z61","v":68.875052249999982},{"$f":"+'C X-XI'!Z61","v":13.306056250595223},{"$f":"+'C X-XI'!V61","v":37.77589163555291},null,{"$f":"+'C X-XI'!X61","v":17.793104363851846},null,null,null,null,{"$f":"+H126","v":3.3485779696489133},null,{"$f":"+$V$7-V19","v":1.5514242303510861},null,{"$f":"+M19*X19","v":106.85442492734707},null,null,null,{"$f":"AD7-'C X-XI'!V59","v":0.72609215808095717},null,{"$f":"+AD19*O19","v":27.428778681090989},{"$f":"+AG7-'C X-XI'!X59","v":1.0335908939774985E-2},null,{"$f":"+'C X-XI'!X61*'Analiza i dimenzioniranje'!AQ13","v":0.14465929289570792},{"$f":"AJ7-'C X-XI'!Z59","v":-0.34074126926177506},null,{"$f":"+'C X-XI'!Z61*'Analiza i dimenzioniranje'!AT13","v":-4.5636103109654318}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M20","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V20","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V20","v":{"$error":"#VALUE!"}},null,{"$f":"+P20*AA20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli............................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M21","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V21","v":{"$error":"#VALUE!"}},null,{"$f":"+P21*AA21","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza............."," ",0,null,{"$f":"+M22","v":0},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+AD7-V22","v":{"$error":"#VALUE!"}},null,{"$f":"+M22*AD22","v":{"$error":"#VALUE!"}}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0},null,null,null,null,null,null,null,4.5500016499999996,null,0.35000054999999985,null,0,null,null,null,null,null,null,null,null,null,{"$f":"AJ7-(2+E57-E54/2)","v":-0.35000054999999985},null,{"$f":"+AJ23*N23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X24","v":{"$error":"#VALUE!"}},null,{"$f":"+M24*AD24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X25","v":{"$error":"#VALUE!"}},null,{"$f":"+M25*AD25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X26","v":{"$error":"#VALUE!"}},null,{"$f":"+M26*AD26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X27","v":{"$error":"#VALUE!"}},null,{"$f":"+M27*AD27","v":{"$error":"#VALUE!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",0.60822475599092374,null,null,{"$f":"+M28","v":0.60822475599092374},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V28","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V28","v":{"$error":"#VALUE!"}},null,{"$f":"P28*AA28","v":{"$error":"#VALUE!"}}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M29","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V29","v":{"$error":"#VALUE!"}},null,{"$f":"+P29*AA29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M30","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V30","v":{"$error":"#VALUE!"}},null,{"$f":"+P30*AA30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",{"$error":"#VALUE!"},null,{"$f":"+M31","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,2,null,2.9000021999999994,null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-'C X-XI'!E93","v":1.4000010999999999},null,{"$f":"+M31*AD31","v":{"$error":"#VALUE!"}},{"$f":"+$AD$7-AD31","v":2}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.306056250595223},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":17.793104363851846},null,null,null,null,null,null,null,null,{"$f":"SUM(Z19:Z31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC19:AC31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF19:AF31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI19:AI31)","v":0.14465929289570792},null,null,{"$f":"SUM(AL19:AL31)","v":-4.5636103109654318}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"II-II","sredina","I-I"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C X-XI'!Z76+'C X-XI'!AB76+'C X-XI'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":{"$error":"#VALUE!"}},null,{"$f":"+'C X-XI'!AB76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+'C X-XI'!Z76","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!AB76","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!AD76","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"$AD$7-'C X-XI'!Z77","v":{"$error":"#VALUE!"}},null,{"$f":"+X34*AD34","v":{"$error":"#VALUE!"}},{"$f":"$AG$7-'C X-XI'!AB77","v":{"$error":"#VALUE!"}},null,{"$f":"-Y34*AG34","v":{"$error":"#VALUE!"}},{"$f":"+AJ7-'C X-XI'!AD77","v":{"$error":"#VALUE!"}},null,{"$f":"+Z34*AJ34","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+Z35","v":{"$error":"#VALUE!"}},{"$f":"+X35","v":{"$error":"#VALUE!"}},null,{"$f":"+Y35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M35*E55/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E51/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E54/E57","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AE7-'C X-XI'!AC45","v":{"$error":"#VALUE!"}},{"$f":"-S35*AE35","v":{"$error":"#VALUE!"}},null,{"$f":"+AH7-'C X-XI'!AC48","v":{"$error":"#VALUE!"}},{"$f":"Y35*AH35","v":{"$error":"#VALUE!"}},null,{"$f":"+AK7-'C X-XI'!AC52","v":{"$error":"#VALUE!"}},{"$f":"-Z35*AK35","v":{"$error":"#VALUE!"}}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},{"$f":"R18+R35","v":{"$error":"#VALUE!"}},{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#VALUE!"}},{"$f":"+U18+U35","v":{"$error":"#VALUE!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"SUM(R36:U36)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+AC18+AC32+AC34+AC35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AF18+AF32+AF34+AF35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AI18+AI32+AI34+AI35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AL18+AL32+AL34+AL35","v":{"$error":"#VALUE!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!Z40","v":2.35},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y","x"]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"+'Analiza i dimenzioniranje'!E39","v":15},"°    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD7","v":3.4000010999999999},{"$f":"+AE7","v":0.72068965844232813}]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!Z42","v":170.21276595744681},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'C X-XI'!V61*('Analiza i dimenzioniranje'!AI33-'C X-XI'!V59)+B129*(AD39-H129)+B138*(AD39-H138)+B138*(AD39-H138)+'C X-XI'!Z76*('Analiza i dimenzioniranje'!AI33-'C X-XI'!Z77)+S35*(AE39-'C X-XI'!AG66)+B110*(AE39-H110)","v":{"$error":"#VALUE!"}}]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*'C X-XI'!AC118*C42/B42","v":0},"kN/m'"]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'P IX-IX'!C42","v":1}]
[null,null,"DIMENZIJE ZIDA:"]
[]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":4.4000000000000004},"m"]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C X-XI'!B10-'C X-XI'!B11=0,\">100\",IF('C X-XI'!C10-'C X-XI'!C11/(0.00000000000001+'C X-XI'!B11-'C X-XI'!B10)>100,\">100\",('C X-XI'!C10-'C X-XI'!C11)/('C X-XI'!B11-'C X-XI'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C X-XI'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C X-XI'!E64","v":1.4000010999999999},"m"]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 "]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m"]
[" zapreminska težina nasipa ...............................",null,null,"      gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!Z44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C X-XI'!I87-'C X-XI'!Q17)-B109*('C X-XI'!K87-'C X-XI'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C X-XI'!Q16-'C X-XI'!N59)+B136*('C X-XI'!Q16-'C X-XI'!M93)+B137*('C X-XI'!Q16-'C X-XI'!C93)+B135*(C135),-B116*C116/1.35-B108*('C X-XI'!I87-'C X-XI'!Q17)-B109*('C X-XI'!K87-'C X-XI'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C X-XI'!Q16-'C X-XI'!M93)+B137*('C X-XI'!Q16-'C X-XI'!C93)+B135*(C135))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+#REF!)","v":{"$error":"#REF!"}},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+'Dijagram momenata'!Q15","v":2.8},null,{"$f":"-B111*N66","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":0},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota",null,"krak od presjeka do sile"]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c111",{"$f":"IF(+L66-'Dijagram momenata'!$Q$15>0,+L66-'Dijagram momenata'!$Q$15,0)","v":{"$error":"#REF!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c112",{"$f":"IF(+L67-'Dijagram momenata'!$Q$15>0,+L67-'Dijagram momenata'!$Q$15,0)","v":{"$error":"#REF!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c113",{"$f":"IF(+L68-'Dijagram momenata'!$Q$15>0,+L68-'Dijagram momenata'!$Q$15,0)","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c114",{"$f":"IF(+L69-'Dijagram momenata'!$Q$15>0,+L69-'Dijagram momenata'!$Q$15,0)","v":{"$error":"#REF!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+'C X-XI'!I85","v":{"$error":"#VALUE!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+'C X-XI'!K88","v":{"$error":"#VALUE!"}},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658}]
[" sloj 3. ..............................",{"$f":"+'P III-III'!B99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!C99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!D99","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,null,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I120","v":1},null,null,{"$f":"+'C X-XI'!N87","v":{"$error":"#VALUE!"}}]
[" Eh2 .............................................",{"$f":"+C98","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I121","v":1},null,null,{"$f":"+'C X-XI'!K87","v":{"$error":"#VALUE!"}}]
[" Eh3 .....................................................",{"$f":"+C99","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I122","v":1},null,null,{"$f":"+C110+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPrometno ....................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I124","v":1.3},null,null,{"$f":"+C111+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+B112*C112","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I125","v":1},null,null,{"$f":"+C112+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPLinijsko ................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"+B113*C113","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I126","v":1}]
[" EQTemelj ....................................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I127","v":1},null,null,{"$f":"+C114+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,null,{"$f":"+'C X-XI'!$AI$44","v":1.5001009999999999},{"$f":"+'C X-XI'!$AH$44","v":4.9000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":-2.2699256917793105},{"$f":"IF(H115<'Analiza i dimenzioniranje'!Z44,0,H115-'Analiza i dimenzioniranje'!Z44)","v":167.41276595744679},{"$f":"+B115*C115","v":-380.01453857864522},{"$f":"+'Analiza i dimenzioniranje'!I129","v":0},null,null,{"$f":"+E40","v":170.21276595744681},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":6.9000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":0},{"$f":"+H116-'Analiza i dimenzioniranje'!Z44","v":-2.8},{"$f":"B116*C116","v":0},{"$f":"+'Analiza i dimenzioniranje'!I150","v":0},"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C X-XI'!AC117","v":0}]
[{"$f":"+A101","v":{"$error":"#VALUE!"}},{"$f":"-B101","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!E116","v":0},null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}},null,null,"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C X-XI'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C X-XI'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},{"$f":"+'Analiza i dimenzioniranje'!I135","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C X-XI'!L61","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C X-XI'!L59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I136","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C X-XI'!L59","v":{"$error":"#VALUE!"}}]
[" Gnasip na konzoli.............................",{"$f":"IF(M61>=E67+E68,0,'C X-XI'!N61)","v":{"$error":"#VALUE!"}},{"$f":"IF(B128=0,0,2+E57-'C X-XI'!N59)","v":{"$error":"#VALUE!"}},{"$f":"B128*C128","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I138","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C128","v":{"$error":"#VALUE!"}}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C X-XI'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I139","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},{"$f":"+'Analiza i dimenzioniranje'!I140","v":{"$error":"#VALUE!"}},null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C X-XI'!W18<'C X-XI'!B7,0,('C X-XI'!W18-'C X-XI'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C X-XI'!W18+'C X-XI'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I141","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C X-XI'!W23>'C X-XI'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C X-XI'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I142","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C X-XI'!W26>'C X-XI'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C X-XI'!W25)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I143","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C X-XI'!W31>'C X-XI'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C X-XI'!W33-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I144","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":0.60822475599092374},{"$f":"2+E57-'C X-XI'!AB24-E54-'Analiza i dimenzioniranje'!Z49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I145","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C X-XI'!M93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I146","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C X-XI'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I147","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C X-XI'!E93","v":2.9000021999999994},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I148","v":1},null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]

{"sheet":"P XI-XI","index":22,"n_rows":175,"n_cols":24,"rows_kept":175,"cut":false,"hidden":true,"merged":[[30,10,30,11],[95,6,95,8],[33,10,33,11],[56,10,56,18],[73,0,73,9],[64,11,64,12],[57,10,57,18],[34,10,34,11],[162,1,162,2],[46,0,46,2],[68,0,68,8],[69,0,69,8],[71,0,71,7],[72,0,72,8],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[7,0,7,9],[13,10,13,11],[20,10,20,11],[21,10,21,11],[29,10,29,11],[27,0,27,2],[27,10,27,11],[28,0,28,2],[28,10,28,11],[24,0,24,2],[25,0,25,2]]}
[" UPUTE ZA RAD: - Ispuniti sve podatke u čelijama s plavom bojom. Ispuniti i za izbor armature u kolonama L,N i O",null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  "]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C X-XI'!C15","v":0.5}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#VALUE!"}}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,null,{"$f":"+M9","v":{"$error":"#VALUE!"}}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"+M10","v":{"$error":"#VALUE!"}}]
[null,"milenium","GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ....................................................",null,{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":48.296291314453413},null,null,null,null,null,null,{"$f":"M15","v":48.296291314453413}]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":0},null,null,null,null,null,null,0]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":2},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-'P XI-XI'!M61)","v":0.85999999999999988},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#VALUE!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S8:S17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T8:T17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U8:U17)","v":0}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!F21","v":10},{"$f":"+'Analiza i dimenzioniranje'!F22","v":10},{"$f":"+'Analiza i dimenzioniranje'!J22","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C X-XI'!V61+'C X-XI'!X61+'C X-XI'!Z61","v":68.875052249999982},{"$f":"+'C X-XI'!Z61","v":13.306056250595223},{"$f":"+'C X-XI'!V61","v":37.77589163555291},null,{"$f":"+'C X-XI'!X61","v":17.793104363851846}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli.............................",null,{"$error":"#VALUE!"},null,null,{"$f":"+M21","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza.............",null,0,null,{"$f":"+M22","v":0}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",12.940952255126037,null,null,{"$f":"+M28","v":12.940952255126037}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",{"$error":"#VALUE!"},null,{"$f":"+M31","v":{"$error":"#VALUE!"}}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.306056250595223},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":17.793104363851846}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C X-XI'!Z76+'C X-XI'!AB76+'C X-XI'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":0},null,{"$f":"+'C X-XI'!AB76","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+X35","v":0},null,{"$f":"+#REF!","v":{"$error":"#REF!"}}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},null,{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#VALUE!"}},{"$f":"+U18+U35","v":{"$error":"#REF!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,"EUROCOD 2",null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"SUM(R36:U36)","v":{"$error":"#VALUE!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!AA40","v":50},"kN/m'",null,null,null,null,"Marka betona",15,20,25,30,40]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"IF(E38=0,0,'Analiza i dimenzioniranje'!E39)","v":15},"°    ",null,null,null,null,"Klasa betona C","12/15","16/20","20/25","25/30","30/37"]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!AA42","v":5},"m",null,null,null,null,"fcm (N/mm2)",20,24,28,33,38]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*'C X-XI'!AE118*C42/B42","v":0},"kN/m'",null,null,null,null,"ecu  (%0)",-3.6,-3.5,-3.4,-3.3,-3.2]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'P X-X'!C42","v":1},null,null,null,null,null,null,null,"fck valjak (N/mm2)",12,16,20,25,30]
[null,null,"DIMENZIJE ZIDA:",null,null,null,"          GRADIVO TEMELJA I ZIDA:",null,null,null,"fck kocka (N/mm2)",15,20,25,30,37]
[null,null,null,null,null,null,null,null,500,500,"Ecm (N/mm2)",26000,27500,29000,30500,32000]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":4.0599999999999996},"m",null,null,null,null,"ARMATURA",null,null,500]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C X-XI'!B10-'C X-XI'!B11=0,\">100\",IF('C X-XI'!C10-'C X-XI'!C11/(0.00000000000001+'C X-XI'!B11-'C X-XI'!B10)>100,\">100\",('C X-XI'!C10-'C X-XI'!C11)/('C X-XI'!B11-'C X-XI'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C X-XI'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22=",null,null,{"$f":"+'C X-XI'!N87-'C X-XI'!P17","v":{"$error":"#VALUE!"}}]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C X-XI'!E64","v":1.4000010999999999},"m"]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m",null,null,null,null,"FAKTORI STABILNOSTI I KONTAKTNI NAPONI"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 ",null,null,null,null,null,null,null,null,"M="," -  "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 ",null,null,null,null,null,null,null,null,"     v=","+"]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m",null,null,null,null,"MOMENTI SAVIJANJA (kNm/m')",null,null,null,"     h=","-"]
[" zapreminska težina nasipa ...............................",null,null,"gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,"Moment na koti +",null,{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},"Mkonzole"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!D63","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AA44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C X-XI'!N87-'C X-XI'!P17)-B109*('C X-XI'!P87-'C X-XI'!P17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C X-XI'!P16-'C X-XI'!R59)+B136*('C X-XI'!P16-'C X-XI'!H93)+B137*('C X-XI'!P16-'C X-XI'!C93)+B135*(C135),-B116*C116/1.35-B108*('C X-XI'!N87-'C X-XI'!P17)-B109*('C X-XI'!P87-'C X-XI'!P17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C X-XI'!P16-'C X-XI'!H93)+B137*('C X-XI'!P16-'C X-XI'!C93)+B135*(C135))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+E592)","v":0},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+'Dijagram momenata'!Q14","v":3.14},null,{"$f":"-#REF!*N66","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":0},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota",null,"krak od presjeka do sile","     v11=",{"$f":"B130+'C X-XI'!Z61+'C X-XI'!AD76","v":{"$error":"#VALUE!"}}]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c111",{"$f":"IF(+L66-'Dijagram momenata'!$Q$14>0,+L66-'Dijagram momenata'!$Q$14,0)","v":{"$error":"#REF!"}},"     h11=",{"$f":"+B118*E54/E57-B117","v":{"$error":"#VALUE!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c112",{"$f":"IF(+L67-'Dijagram momenata'!$Q$14>0,+L67-'Dijagram momenata'!$Q$14,0)","v":{"$error":"#REF!"}},"     v22=",{"$f":"+B129+B131+B132+B133+B134+B138+'C X-XI'!Z76+'C X-XI'!V61","v":{"$error":"#VALUE!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c113",{"$f":"IF(+L68-'Dijagram momenata'!$Q$14>0,+L68-'Dijagram momenata'!$Q$14,0)","v":{"$error":"#REF!"}},"     h22=",{"$f":"+B118*E55/E57-B110","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c114",{"$f":"IF(+L69-'Dijagram momenata'!$Q$14>0,+L69-'Dijagram momenata'!$Q$14,0)","v":{"$error":"#REF!"}},"     v33=",{"$f":"B127+B128+B135+B136+B137","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     h33=",{"$f":"-B108-B109-B111-B112-B113-B114+B115-B116","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko"," -koeficijent mirnog pritiska",null,null,"     vtem=",{"$f":"+'C X-XI'!X61+'C X-XI'!AB76","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko1=","1-sinj1=",{"$f":"1-SIN(E14*PI()/180)","v":0.62539340658408804},"varijanta","     htem=",{"$f":"+B118*E51/E57","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko2=","1-sinj2=",{"$f":"1-SIN(F14*PI()/180)","v":0.69098300562505255},"n","    MI-I",{"$f":"+K62","v":0}]
[null,null,null,null,null,null,null,null,null,null,"Ko3=","1-sinj3=",{"$f":"1-SIN(G14*PI()/180)","v":0.65797985667433134},null,"MII-II",{"$f":"+L62","v":0}]
[null,null,null,null,null,null,null,null,null,null,"Ko=","n/(1-n) =",{"$f":"+N75/(1-N75)","v":0.66666666666666674},0.4,"Mzida",{"$f":"+M62","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+(B172*E51*E58)","v":0},{"$f":"+E51/2","v":0.4},{"$f":"+K76*L76","v":0}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+'C X-XI'!N85","v":{"$error":"#VALUE!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+'C X-XI'!P88","v":{"$error":"#VALUE!"}},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658}]
[" sloj 3. ..............................",{"$f":"+'P III-III'!B99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!C99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!D99","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,null,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#VALUE!"}},null,null,1.35,null,null,{"$f":"+'C X-XI'!N87","v":{"$error":"#VALUE!"}}]
[" Eh2 .............................................",{"$f":"+C98","v":{"$error":"#VALUE!"}},null,null,1.35,null,null,{"$f":"+'C X-XI'!P87","v":{"$error":"#VALUE!"}}]
[" Eh3 .....................................................",{"$f":"+C99","v":{"$error":"#VALUE!"}},null,null,1.35,null,null,{"$f":"+C110+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPrometno ....................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,1.5]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"B112*C112","v":{"$error":"#REF!"}},1.35,null,null,{"$f":"+C112+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,{"$f":"+C112*B112","v":{"$error":"#REF!"}}]
[" EPLinijsko ................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"B113*C113","v":{"$error":"#REF!"}},1.35,null,null,{"$f":"+C113+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EQTemelj ....................................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,1.35,null,null,{"$f":"+C114+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,{"$f":"+C114*B114","v":{"$error":"#REF!"}},{"$f":"+'C X-XI'!$AI$44","v":1.5001009999999999},{"$f":"+'C X-XI'!$AH$44","v":4.9000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":-48.296291314453413},{"$f":"IF(H115<'Analiza i dimenzioniranje'!AA44,0,H115-'Analiza i dimenzioniranje'!AA44)","v":1.8599999999999999},null,1.35,null,null,{"$f":"+E40","v":5},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":6.9000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":0},{"$f":"+H116-'Analiza i dimenzioniranje'!AA44","v":-3.14},{"$f":"B116*C116","v":0},1,"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C X-XI'!AE117","v":0}]
[{"$f":"+A101","v":{"$error":"#VALUE!"}},{"$f":"-B101","v":{"$error":"#VALUE!"}},{"$f":"IF(F101=0,0,E49/3)","v":0},{"$f":"B117*C117","v":{"$error":"#VALUE!"}},1.35,null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}}," S MHA =",{"$f":"SUM(D108:D117)","v":{"$error":"#REF!"}},"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C X-XI'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C X-XI'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},1.35,null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C X-XI'!P61","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C X-XI'!P59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},1.35,null,null,{"$f":"2+$E$57-C127","v":{"$error":"#VALUE!"}}]
[" Gnasip na konzoli.............................",{"$f":"'C X-XI'!R61","v":{"$error":"#VALUE!"}},{"$f":"IF(B128=0,0,2+E57-'C X-XI'!R59)","v":{"$error":"#VALUE!"}},{"$f":"B128*C128","v":{"$error":"#VALUE!"}},1.35,null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C X-XI'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},1.35,null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},1.35,null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C X-XI'!W18<'C X-XI'!B7,0,('C X-XI'!W18-'C X-XI'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C X-XI'!W18+'C X-XI'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},1.5,null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C X-XI'!W23>'C X-XI'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C X-XI'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C X-XI'!W26>'C X-XI'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C X-XI'!W25)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C X-XI'!W31>'C X-XI'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C X-XI'!W33-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":12.940952255126037},{"$f":"2+E57-'C X-XI'!AC24-E54-'Analiza i dimenzioniranje'!AA49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C X-XI'!H93-E54/'Analiza i dimenzioniranje'!AA49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C X-XI'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C X-XI'!E93","v":2.9000021999999994},{"$error":"#VALUE!"},1.35,null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]
[]
[]
[]
[" Rezultanta sila .........................................",null,"      R =",{"$f":"SQRT(B118^2+B139^2)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" sila uzduž temelja ..................................................",null,{"$f":"IF(E48=E49,\"     RH =\",\"     RT =\")","v":"     RT ="},{"$f":"D144*SIN((D148-D149)*PI()/180)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" sila okomita na temelj .................................",null,"    RN =",{"$f":"D144*COS((D148-D149)*PI()/180)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" moment oko osi temelja.....................................",null,"     Ms =",{"$f":"+B118*(I118-'C X-XI'!AC50)-'Analiza i dimenzioniranje'!B168*(F139-E57/2)","v":{"$error":"#VALUE!"}},"kNm/m'"]
[" otklon rezultante od vertikale .....................................",null,"a =",{"$f":"ATAN(B118/B139)*180/PI()","v":{"$error":"#VALUE!"}},"°"]
[" nagib temelja ..........................................",null,"b =",{"$f":"ATAN('C X-XI'!C15/E57)*180/PI()","v":9.7823997540577476},"°"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,{"$f":"IF(E49=E48,\"\",+D167*COS(D149*PI()/180))","v":0}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"za Presjeke I-I i II-II"]
[null,null,null,null,null,null,null,null,null,null,"     As,min=",{"$f":"+MAX(E251,E269)","v":0},{"$f":"+MAX(L174:L175)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"     As,1 mjer =",{"$f":"+IF(E255>L173/2,E255,L173/2)","v":0},{"$f":"+L174-7.85","v":-7.85}]
[null,null,null,null,null,null,null,null,null,null,"     As,2 mjer =",{"$f":"+IF(E273>L173/2,E273,L173/2)","v":0},{"$f":"+L175-7.85","v":-7.85}]

{"sheet":"P XII-XII","index":23,"n_rows":140,"n_cols":38,"rows_kept":140,"cut":false,"hidden":true,"merged":[[46,38,46,39],[46,35,46,36],[45,32,46,32],[44,38,45,38],[47,38,48,38],[48,32,49,32],[47,35,48,35],[45,20,46,20],[45,23,46,23],[47,29,47,30],[44,35,45,35],[48,20,49,20],[47,23,47,24],[48,23,49,23],[48,26,49,26],[48,29,49,29],[45,26,46,26],[45,29,46,29],[48,11,49,11],[47,32,47,33],[47,11,47,12],[47,14,47,15],[47,17,47,18],[47,20,47,21],[48,14,49,14],[48,17,49,17],[47,26,47,27],[45,11,46,11],[45,14,46,14],[45,17,46,17],[20,10,20,11],[28,10,28,11],[29,10,29,11],[30,10,30,11],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[16,10,16,11],[7,10,7,11],[8,10,8,11],[9,10,9,11],[10,10,10,11],[11,10,11,11],[12,10,12,11],[64,11,64,12],[7,0,7,9],[13,10,13,11],[14,10,14,11],[15,10,15,11],[18,10,18,11],[19,10,19,11],[34,10,34,11],[21,10,21,11],[22,10,22,11],[23,10,23,11],[24,10,24,11],[25,10,25,11],[26,10,26,11],[27,10,27,11],[33,10,33,11]]}
[" UPUTE ZA RAD: - Ispuniti sve podatke u čelijama s plavom bojom. Ispuniti i za izbor armature u kolonama L,N i O",null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z18/M18","v":{"$error":"#VALUE!"}}]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  ","krak                  y  ","Moment destabilnosti i stabilnosti","za Mzida                                              krakovi                             x                  y",null,"Moment zida II","za M u                           presjeku II-II                                                   krakovi                                x               y",null,"Moment      II-II","za M u                           temelju ispod zida                     krakovi                             x                  y",null,"Moment  ","za M u                           presjeku I-I                                              krakovi                             x                  y",null,"Moment      I-I"]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C XII-XIII'!C15","v":0.5},null,null,null,{"$f":"2+E57-E54-E51/2","v":3.8000010999999998},{"$f":"+E48","v":1.2},null,{"$f":"2+E55","v":3.4000010999999999},{"$f":"'C XII-XIII'!AC47+(E48-'C XII-XIII'!AC47)/2","v":0.72068965844232813},null,{"$f":"2+E55+E51/2","v":3.8000010999999998},{"$f":"'C XII-XIII'!AC49+(E48-'C XII-XIII'!AF47)/2","v":0.97931024673015765},null,{"$f":"2+E55+E51","v":4.2000010999999997},{"$f":"'C XII-XIII'!AC49+(E48-'C XII-XIII'!AC49)/2","v":0.78965512336507881}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#VALUE!"}},null,null,{"$f":"+H108","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$W$7","v":{"$error":"#VALUE!"}},{"$f":"+M8*Y8","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$AB$7","v":{"$error":"#VALUE!"}},{"$f":"T8*AB8","v":{"$error":"#VALUE!"}}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,null,{"$f":"+M9","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$f":"+W9-$AB$7","v":{"$error":"#VALUE!"}},{"$f":"AB9*T9","v":{"$error":"#VALUE!"}}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"+M10","v":{"$error":"#VALUE!"}},null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,{"$f":"+AE7-'C XII-XIII'!F93","v":{"$error":"#VALUE!"}},{"$f":"+AE10*S10","v":{"$error":"#VALUE!"}}]
[null,null,"GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$f":"+W11-$AB$7","v":{"$error":"#REF!"}},{"$f":"AB11*T11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ...................................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":48.296291314453413},null,null,null,null,null,null,{"$f":"+M15","v":48.296291314453413},null,null,5,null,4.5,{"$f":"-M15*Y15","v":-217.33331091504036},null,3.8,183.52590699492296]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":0},null,null,null,null,null,null,0,null,null,0,null,-0.5,0,null,-1.2,0]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":2},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-'P XII-XII'!M61)","v":0.56000000000000005},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#VALUE!"}},null,null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,{"$f":"+AK7-C117","v":0.78965512336507881},{"$f":"+M17*AK17","v":{"$error":"#VALUE!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S8:S17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T8:T17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U8:U17)","v":0},null,null,"x",null,{"$f":"SUM(Z8:Z17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC8:AC17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF8:AF17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI8:AI17)","v":0},null,null,{"$f":"SUM(AL8:AL17)","v":{"$error":"#VALUE!"}}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C XII-XIII'!V61+'C XII-XIII'!X61+'C XII-XIII'!Z61","v":68.875052249999982},{"$f":"+'C XII-XIII'!Z61","v":13.306056250595223},{"$f":"+'C XII-XIII'!V61","v":37.77589163555291},null,{"$f":"+'C XII-XIII'!X61","v":17.793104363851846},null,null,null,null,{"$f":"+H126","v":3.3485779696489133},null,{"$f":"+$V$7-V19","v":1.5514242303510861},null,{"$f":"+M19*X19","v":106.85442492734707},null,null,null,{"$f":"AD7-'C XII-XIII'!V59","v":0.72609215808095717},null,{"$f":"+AD19*O19","v":27.428778681090989},{"$f":"+AG7-'C XII-XIII'!X59","v":1.0335908939774985E-2},null,{"$f":"+'C XII-XIII'!X61*'Analiza i dimenzioniranje'!AQ13","v":0.14465929289570792},{"$f":"AJ7-'C XII-XIII'!Z59","v":-0.34074126926177506},null,{"$f":"+'C XII-XIII'!Z61*'Analiza i dimenzioniranje'!AT13","v":-4.5636103109654318}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M20","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V20","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V20","v":{"$error":"#VALUE!"}},null,{"$f":"+P20*AA20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli............................."," ",0,null,null,{"$f":"+M21","v":0},null,null,null,null,null,4.9000021999999994,null,0,null,0,{"$f":"+$AA$7-V21","v":-1.1000010999999996},null,{"$f":"+P21*AA21","v":0}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza............."," ",0,null,{"$f":"+M22","v":0},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+AD7-V22","v":{"$error":"#VALUE!"}},null,{"$f":"+M22*AD22","v":{"$error":"#VALUE!"}}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0},null,null,null,null,null,null,null,4.5500016499999996,null,0.35000054999999985,null,0,null,null,null,null,null,null,null,null,null,{"$f":"AJ7-(2+E57-E54/2)","v":-0.35000054999999985},null,{"$f":"+AJ23*N23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X24","v":{"$error":"#VALUE!"}},null,{"$f":"+M24*AD24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X25","v":{"$error":"#VALUE!"}},null,{"$f":"+M25*AD25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X26","v":{"$error":"#VALUE!"}},null,{"$f":"+M26*AD26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X27","v":{"$error":"#VALUE!"}},null,{"$f":"+M27*AD27","v":{"$error":"#VALUE!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",12.940952255126037,null,null,{"$f":"+M28","v":12.940952255126037},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V28","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V28","v":{"$error":"#VALUE!"}},null,{"$f":"P28*AA28","v":{"$error":"#VALUE!"}}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M29","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V29","v":{"$error":"#VALUE!"}},null,{"$f":"+P29*AA29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M30","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V30","v":{"$error":"#VALUE!"}},null,{"$f":"+P30*AA30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",{"$error":"#VALUE!"},null,{"$f":"+M31","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,2,null,2.9000021999999994,null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-'C XII-XIII'!E93","v":1.4000010999999999},null,{"$f":"+M31*AD31","v":{"$error":"#VALUE!"}},{"$f":"+$AD$7-AD31","v":2}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.306056250595223},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":17.793104363851846},null,null,null,null,null,null,null,null,{"$f":"SUM(Z19:Z31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC19:AC31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF19:AF31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI19:AI31)","v":0.14465929289570792},null,null,{"$f":"SUM(AL19:AL31)","v":-4.5636103109654318}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"II-II","sredina","I-I"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C XII-XIII'!Z76+'C XII-XIII'!AB76+'C XII-XIII'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":{"$error":"#VALUE!"}},null,{"$f":"+'C XII-XIII'!AB76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+'C XII-XIII'!Z76","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!AB76","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!AD76","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"$AD$7-'C XII-XIII'!Z77","v":{"$error":"#VALUE!"}},null,{"$f":"+X34*AD34","v":{"$error":"#VALUE!"}},{"$f":"$AG$7-'C XII-XIII'!AB77","v":{"$error":"#VALUE!"}},null,{"$f":"-Y34*AG34","v":{"$error":"#VALUE!"}},{"$f":"+AJ7-'C XII-XIII'!AD77","v":{"$error":"#VALUE!"}},null,{"$f":"+Z34*AJ34","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+Z35","v":{"$error":"#VALUE!"}},{"$f":"+X35","v":{"$error":"#VALUE!"}},null,{"$f":"+Y35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M35*E55/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E51/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E54/E57","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AE7-'C XII-XIII'!AC45","v":{"$error":"#VALUE!"}},{"$f":"-S35*AE35","v":{"$error":"#VALUE!"}},null,{"$f":"+AH7-'C XII-XIII'!AC48","v":{"$error":"#VALUE!"}},{"$f":"Y35*AH35","v":{"$error":"#VALUE!"}},null,{"$f":"+AK7-'C XII-XIII'!AC52","v":{"$error":"#VALUE!"}},{"$f":"-Z35*AK35","v":{"$error":"#VALUE!"}}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},{"$f":"R18+R35","v":{"$error":"#VALUE!"}},{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#VALUE!"}},{"$f":"+U18+U35","v":{"$error":"#VALUE!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"SUM(R36:U36)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+AC18+AC32+AC34+AC35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AF18+AF32+AF34+AF35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AI18+AI32+AI34+AI35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AL18+AL32+AL34+AL35","v":{"$error":"#VALUE!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!AB40","v":50},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y","x"]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"+'Analiza i dimenzioniranje'!E39","v":15},"°    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD7","v":3.4000010999999999},{"$f":"+AE7","v":0.72068965844232813}]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!AB42","v":5},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'C XII-XIII'!V61*('Analiza i dimenzioniranje'!AI33-'C XII-XIII'!V59)+B129*(AD39-H129)+B138*(AD39-H138)+B138*(AD39-H138)+'C XII-XIII'!Z76*('Analiza i dimenzioniranje'!AI33-'C XII-XIII'!Z77)+S35*(AE39-'C XII-XIII'!AG66)+B110*(AE39-H110)","v":{"$error":"#VALUE!"}}]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*'C XII-XIII'!AC118*C42/B42","v":0},"kN/m'"]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'P XI-XI'!C42","v":1}]
[null,null,"DIMENZIJE ZIDA:"]
[]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":3.76},"m"]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C XII-XIII'!B10-'C XII-XIII'!B11=0,\">100\",IF('C XII-XIII'!C10-'C XII-XIII'!C11/(0.00000000000001+'C XII-XIII'!B11-'C XII-XIII'!B10)>100,\">100\",('C XII-XIII'!C10-'C XII-XIII'!C11)/('C XII-XIII'!B11-'C XII-XIII'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C XII-XIII'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C XII-XIII'!E64","v":1.4000010999999999},"m"]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 "]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m"]
[" zapreminska težina nasipa ...............................",null,null,"      gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AB44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C XII-XIII'!I87-'C XII-XIII'!Q17)-B109*('C XII-XIII'!K87-'C XII-XIII'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C XII-XIII'!Q16-'C XII-XIII'!N59)+B136*('C XII-XIII'!Q16-'C XII-XIII'!M93)+B137*('C XII-XIII'!Q16-'C XII-XIII'!C93)+B135*(C135),-B116*C116/1.35-B108*('C XII-XIII'!I87-'C XII-XIII'!Q17)-B109*('C XII-XIII'!K87-'C XII-XIII'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C XII-XIII'!Q16-'C XII-XIII'!M93)+B137*('C XII-XIII'!Q16-'C XII-XIII'!C93)+B135*(C135))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+#REF!)","v":{"$error":"#REF!"}},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+'Dijagram momenata'!Q13","v":3.44},null,{"$f":"-#REF!*N66","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":0},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota",null,"krak od presjeka do sile"]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c111",{"$f":"IF(+L66-'Dijagram momenata'!$Q$13>0,+L66-'Dijagram momenata'!$Q$13,0)","v":{"$error":"#REF!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c112",{"$f":"IF(+L67-'Dijagram momenata'!$Q$13>0,+L67-'Dijagram momenata'!$Q$13,0)","v":{"$error":"#REF!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c113",{"$f":"IF(+L68-'Dijagram momenata'!$Q$13>0,+L68-'Dijagram momenata'!$Q$13,0)","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c114",{"$f":"IF(+L69-'Dijagram momenata'!$Q$13>0,+L69-'Dijagram momenata'!$Q$13,0)","v":{"$error":"#REF!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+'C XII-XIII'!I85","v":{"$error":"#VALUE!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+'C XII-XIII'!K88","v":{"$error":"#VALUE!"}},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658}]
[" sloj 3. ..............................",{"$f":"+'P III-III'!B99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!C99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!D99","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,null,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I120","v":1},null,null,{"$f":"+'C XII-XIII'!N87","v":{"$error":"#VALUE!"}}]
[" Eh2 .............................................",{"$f":"+C98","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I121","v":1},null,null,{"$f":"+'C XII-XIII'!K87","v":{"$error":"#VALUE!"}}]
[" Eh3 .....................................................",{"$f":"+C99","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I122","v":1},null,null,{"$f":"+C110+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPrometno ....................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I124","v":1.3},null,null,{"$f":"+C111+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+B112*C112","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I125","v":1},null,null,{"$f":"+C112+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPLinijsko ................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"+B113*C113","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I126","v":1}]
[" EQTemelj ....................................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I127","v":1},null,null,{"$f":"+C114+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,null,{"$f":"+'C XII-XIII'!$AI$44","v":1.5001009999999999},{"$f":"+'C XII-XIII'!$AH$44","v":4.9000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":-48.296291314453413},{"$f":"IF(H115<'Analiza i dimenzioniranje'!AB44,0,H115-'Analiza i dimenzioniranje'!AB44)","v":1.56},{"$f":"+B115*C115","v":-75.342214450547331},{"$f":"+'Analiza i dimenzioniranje'!I129","v":0},null,null,{"$f":"+E40","v":5},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":6.9000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":0},{"$f":"+H116-'Analiza i dimenzioniranje'!AB44","v":-3.44},{"$f":"B116*C116","v":0},{"$f":"+'Analiza i dimenzioniranje'!I150","v":0},"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C XII-XIII'!AC117","v":0}]
[{"$f":"+A101","v":{"$error":"#VALUE!"}},{"$f":"-B101","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!E116","v":0},null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}},null,null,"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C XII-XIII'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C XII-XIII'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},{"$f":"+'Analiza i dimenzioniranje'!I135","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C XII-XIII'!L61","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XII-XIII'!L59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I136","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C XII-XIII'!L59","v":{"$error":"#VALUE!"}}]
[" Gnasip na konzoli.............................",{"$f":"IF(M61>=E67+E68,0,'C XII-XIII'!N61)","v":0},{"$f":"IF(B128=0,0,2+E57-'C XII-XIII'!N59)","v":0},{"$f":"B128*C128","v":0},{"$f":"+'Analiza i dimenzioniranje'!I138","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C128","v":4.9000021999999994}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C XII-XIII'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I139","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},{"$f":"+'Analiza i dimenzioniranje'!I140","v":{"$error":"#VALUE!"}},null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C XII-XIII'!W18<'C XII-XIII'!B7,0,('C XII-XIII'!W18-'C XII-XIII'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C XII-XIII'!W18+'C XII-XIII'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I141","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C XII-XIII'!W23>'C XII-XIII'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C XII-XIII'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I142","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C XII-XIII'!W26>'C XII-XIII'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C XII-XIII'!W25)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I143","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C XII-XIII'!W31>'C XII-XIII'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XII-XIII'!W33-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I144","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":12.940952255126037},{"$f":"2+E57-'C XII-XIII'!AB24-E54-'Analiza i dimenzioniranje'!AB49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I145","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XII-XIII'!M93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I146","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XII-XIII'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I147","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XII-XIII'!E93","v":2.9000021999999994},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I148","v":1},null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]

{"sheet":"P XIII-XIII","index":24,"n_rows":175,"n_cols":24,"rows_kept":175,"cut":false,"hidden":true,"merged":[[30,10,30,11],[95,6,95,8],[33,10,33,11],[56,10,56,18],[73,0,73,9],[64,11,64,12],[57,10,57,18],[34,10,34,11],[162,1,162,2],[46,0,46,2],[68,0,68,8],[69,0,69,8],[71,0,71,7],[72,0,72,8],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[7,0,7,9],[13,10,13,11],[20,10,20,11],[21,10,21,11],[29,10,29,11],[27,0,27,2],[27,10,27,11],[28,0,28,2],[28,10,28,11],[24,0,24,2],[25,0,25,2]]}
[" UPUTE ZA RAD: - Ispuniti sve podatke u čelijama s plavom bojom. Ispuniti i za izbor armature u kolonama L,N i O",null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","milenium","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  "]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C XII-XIII'!C15","v":0.5}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#VALUE!"}}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,null,{"$f":"+M9","v":{"$error":"#VALUE!"}}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"+M10","v":{"$error":"#VALUE!"}}]
[null,"milenium","GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ....................................................",null,{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":48.296291314453413},null,null,null,null,null,null,{"$f":"M15","v":48.296291314453413}]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":0},null,null,null,null,null,null,0]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":2},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-'P XIII-XIII'!M61)","v":0.24000000000000021},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#VALUE!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S8:S17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T8:T17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U8:U17)","v":0}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C XII-XIII'!V61+'C XII-XIII'!X61+'C XII-XIII'!Z61","v":68.875052249999982},{"$f":"+'C XII-XIII'!Z61","v":13.306056250595223},{"$f":"+'C XII-XIII'!V61","v":37.77589163555291},null,{"$f":"+'C XII-XIII'!X61","v":17.793104363851846}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli.............................",null,{"$error":"#VALUE!"},null,null,{"$f":"+M21","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza.............",null,0,null,{"$f":"+M22","v":0}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",12.940952255126037,null,null,{"$f":"+M28","v":12.940952255126037}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",{"$error":"#VALUE!"},null,{"$f":"+M31","v":{"$error":"#VALUE!"}}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.306056250595223},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":17.793104363851846}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C XII-XIII'!Z76+'C XII-XIII'!AB76+'C XII-XIII'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":0},null,{"$f":"+'C XII-XIII'!AB76","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+X35","v":0}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},null,{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#VALUE!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,"EUROCOD 2",null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!AC40","v":50},"kN/m'",null,null,null,null,"Marka betona",15,20,25,30,40]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"IF(E38=0,0,'Analiza i dimenzioniranje'!E39)","v":15},"°    ",null,null,null,null,"Klasa betona C","12/15","16/20","20/25","25/30","30/37"]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!AC42","v":5},"m",null,null,null,null,"fcm (N/mm2)",20,24,28,33,38]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*'C XII-XIII'!AE118*C42/B42","v":0},"kN/m'",null,null,null,null,"ecu  (%0)",-3.6,-3.5,-3.4,-3.3,-3.2]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'P XII-XII'!C42","v":1},null,null,null,null,null,null,null,"fck valjak (N/mm2)",12,16,20,25,30]
[null,null,"DIMENZIJE ZIDA:",null,null,null,"          GRADIVO TEMELJA I ZIDA:",null,null,null,"fck kocka (N/mm2)",15,20,25,30,37]
[null,null,null,null,null,null,null,null,500,500,"Ecm (N/mm2)",26000,27500,29000,30500,32000]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":3.4400000000000004},"m",null,null,null,null,"ARMATURA",null,null,500]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C XII-XIII'!B10-'C XII-XIII'!B11=0,\">100\",IF('C XII-XIII'!C10-'C XII-XIII'!C11/(0.00000000000001+'C XII-XIII'!B11-'C XII-XIII'!B10)>100,\">100\",('C XII-XIII'!C10-'C XII-XIII'!C11)/('C XII-XIII'!B11-'C XII-XIII'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C XII-XIII'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C XII-XIII'!E64","v":1.4000010999999999},"m",{"$f":"+IF(E32=0,\"\",IF(G54>#REF!+E36,\"PAZI POLOŽAJ TEMELJA\",\"\"))","v":{"$error":"#REF!"}}]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m",null,null,null,null,"FAKTORI STABILNOSTI I KONTAKTNI NAPONI"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 ",null,null,null,null,null,null,null,null,"M="," -  "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 ",null,null,null,null,null,null,null,null,"     v=","+"]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m",null,null,null,null,"MOMENTI SAVIJANJA (kNm/m')",null,null,null,"     h=","-"]
[" zapreminska težina nasipa ...............................",null,null,"gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,"Moment na koti +",null,{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},"Mkonzole"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!D63","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AC44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C XII-XIII'!N87-'C XII-XIII'!P17)-B109*('C XII-XIII'!P87-'C XII-XIII'!P17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C XII-XIII'!P16-'C XII-XIII'!R59)+B136*('C XII-XIII'!P16-'C XII-XIII'!H93)+B137*('C XII-XIII'!P16-'C XII-XIII'!C93)+B135*(C135),-B116*C116/1.35-B108*('C XII-XIII'!N87-'C XII-XIII'!P17)-B109*('C XII-XIII'!P87-'C XII-XIII'!P17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C XII-XIII'!P16-'C XII-XIII'!H93)+B137*('C XII-XIII'!P16-'C XII-XIII'!C93)+B135*(C135))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+E592)","v":0},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+'Dijagram momenata'!Q12","v":3.76},null,{"$f":"-#REF!*N66","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":0},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota",null,"krak od presjeka do sile","     v11=",{"$f":"B130+'C XII-XIII'!Z61+'C XII-XIII'!AD76","v":{"$error":"#VALUE!"}}]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c111",{"$f":"IF(+L66-'Dijagram momenata'!$Q$12>0,+L66-'Dijagram momenata'!$Q$12,0)","v":{"$error":"#REF!"}},"     h11=",{"$f":"+B118*E54/E57-B117","v":{"$error":"#VALUE!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c112",{"$f":"IF(+L67-'Dijagram momenata'!$Q$12>0,+L67-'Dijagram momenata'!$Q$12,0)","v":{"$error":"#REF!"}},"     v22=",{"$f":"+B129+B131+B132+B133+B134+B138+'C XII-XIII'!Z76+'C XII-XIII'!V61","v":{"$error":"#VALUE!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c113",{"$f":"IF(+L68-'Dijagram momenata'!$Q$12>0,+L68-'Dijagram momenata'!$Q$12,0)","v":{"$error":"#REF!"}},"     h22=",{"$f":"+B118*E55/E57-B110","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c114",{"$f":"IF(+L69-'Dijagram momenata'!$Q$12>0,+L69-'Dijagram momenata'!$Q$12,0)","v":{"$error":"#REF!"}},"     v33=",{"$f":"B127+B128+B135+B136+B137","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     h33=",{"$f":"-B108-B109-B111-B112-B113-B114+B115-B116","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko"," -koeficijent mirnog pritiska",null,null,"     vtem=",{"$f":"+'C XII-XIII'!X61+'C XII-XIII'!AB76","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko1=","1-sinj1=",{"$f":"1-SIN(E14*PI()/180)","v":0.62539340658408804},"varijanta","     htem=",{"$f":"+B118*E51/E57","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko2=","1-sinj2=",{"$f":"1-SIN(F14*PI()/180)","v":0.69098300562505255},"n","    MI-I",{"$f":"+K62","v":0}]
[null,null,null,null,null,null,null,null,null,null,"Ko3=","1-sinj3=",{"$f":"1-SIN(G14*PI()/180)","v":0.65797985667433134},null,"MII-II",{"$f":"+L62","v":0}]
[null,null,null,null,null,null,null,null,null,null,"Ko=","n/(1-n) =",{"$f":"+N75/(1-N75)","v":0.66666666666666674},0.4,"Mzida",{"$f":"+M62","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+(B172*E51*E58)","v":0},{"$f":"+E51/2","v":0.4},{"$f":"+K76*L76","v":0}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+'C XII-XIII'!N85","v":{"$error":"#VALUE!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+'C XII-XIII'!P88","v":{"$error":"#VALUE!"}},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658}]
[" sloj 3. ..............................",{"$f":"+'P III-III'!B99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!C99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!D99","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,null,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#VALUE!"}},null,null,1.35,null,null,{"$f":"+'C XII-XIII'!N87","v":{"$error":"#VALUE!"}}]
[" Eh2 .............................................",{"$f":"+C98","v":{"$error":"#VALUE!"}},null,null,1.35,null,null,{"$f":"+'C XII-XIII'!P87","v":{"$error":"#VALUE!"}}]
[" Eh3 .....................................................",{"$f":"+C99","v":{"$error":"#VALUE!"}},null,null,1.35,null,null,{"$f":"+C110+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPrometno ....................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,1.5]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"B112*C112","v":{"$error":"#REF!"}},1.35,null,null,{"$f":"+C112+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPLinijsko ................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"B113*C113","v":{"$error":"#REF!"}},1.35,null,null,{"$f":"+C113+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EQTemelj ....................................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,1.35,null,null,{"$f":"+C114+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,null,{"$f":"+'C XII-XIII'!$AI$44","v":1.5001009999999999},{"$f":"+'C XII-XIII'!$AH$44","v":4.9000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":-48.296291314453413},{"$f":"IF(H115<'Analiza i dimenzioniranje'!AC44,0,H115-'Analiza i dimenzioniranje'!AC44)","v":1.2400000000000002},null,1.35,null,null,{"$f":"+E40","v":5},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":6.9000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":0},{"$f":"+H116-'Analiza i dimenzioniranje'!AC44","v":-3.76},{"$f":"B116*C116","v":0},1,"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C XII-XIII'!AE117","v":0}]
[{"$f":"+A101","v":{"$error":"#VALUE!"}},{"$f":"-B101","v":{"$error":"#VALUE!"}},{"$f":"IF(F101=0,0,E49/3)","v":0},{"$f":"B117*C117","v":{"$error":"#VALUE!"}},1.35,null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}}," S MHA =",{"$f":"SUM(D108:D117)","v":{"$error":"#REF!"}},"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C XII-XIII'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C XII-XIII'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},1.35,null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C XII-XIII'!P61","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XII-XIII'!P59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},1.35,null,null,{"$f":"2+$E$57-C127","v":{"$error":"#VALUE!"}}]
[" Gnasip na konzoli.............................",{"$f":"'C XII-XIII'!R61","v":{"$error":"#VALUE!"}},{"$f":"IF(B128=0,0,2+E57-'C XII-XIII'!R59)","v":{"$error":"#VALUE!"}},{"$f":"B128*C128","v":{"$error":"#VALUE!"}},1.35,null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C XII-XIII'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},1.35,null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},1.35,null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C XII-XIII'!W18<'C XII-XIII'!B7,0,('C XII-XIII'!W18-'C XII-XIII'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C XII-XIII'!W18+'C XII-XIII'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},1.5,null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C XII-XIII'!W23>'C XII-XIII'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C XII-XIII'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C XII-XIII'!W26>'C XII-XIII'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C XII-XIII'!W25)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C XII-XIII'!W31>'C XII-XIII'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XII-XIII'!W33-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":12.940952255126037},{"$f":"2+E57-'C XII-XIII'!AC24-E54-'Analiza i dimenzioniranje'!AC49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XII-XIII'!H93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XII-XIII'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XII-XIII'!E93","v":2.9000021999999994},{"$error":"#VALUE!"},1.35,null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]
[]
[]
[]
[" Rezultanta sila .........................................",null,"      R =",{"$f":"SQRT(B118^2+B139^2)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" sila uzduž temelja ..................................................",null,{"$f":"IF(E48=E49,\"     RH =\",\"     RT =\")","v":"     RT ="},{"$f":"D144*SIN((D148-D149)*PI()/180)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" sila okomita na temelj .................................",null,"    RN =",{"$f":"D144*COS((D148-D149)*PI()/180)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" moment oko osi temelja.....................................",null,"     Ms =",{"$f":"+B118*(I118-'C XII-XIII'!AC50)-'Analiza i dimenzioniranje'!B168*(F139-E57/2)","v":{"$error":"#VALUE!"}},"kNm/m'"]
[" otklon rezultante od vertikale .....................................",null,"a =",{"$f":"ATAN(B118/B139)*180/PI()","v":{"$error":"#VALUE!"}},"°"]
[" nagib temelja ..........................................",null,"b =",{"$f":"ATAN('C XII-XIII'!C15/E57)*180/PI()","v":9.7823997540577476},"°"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,{"$f":"IF(E49=E48,\"\",+D167*COS(D149*PI()/180))","v":0}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"za Presjeke I-I i II-II"]
[null,null,null,null,null,null,null,null,null,null,"     As,min=",{"$f":"+MAX(E251,E269)","v":0},{"$f":"+MAX(L174:L175)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"     As,1 mjer =",{"$f":"+IF(E255>L173/2,E255,L173/2)","v":0},{"$f":"+L174-7.85","v":-7.85}]
[null,null,null,null,null,null,null,null,null,null,"     As,2 mjer =",{"$f":"+IF(E273>L173/2,E273,L173/2)","v":0},{"$f":"+L175-7.85","v":-7.85}]

{"sheet":"P XIV-XIV","index":25,"n_rows":140,"n_cols":38,"rows_kept":140,"cut":false,"hidden":true,"merged":[[46,38,46,39],[46,35,46,36],[45,32,46,32],[44,38,45,38],[47,38,48,38],[48,32,49,32],[47,35,48,35],[45,20,46,20],[45,23,46,23],[47,29,47,30],[44,35,45,35],[48,20,49,20],[47,23,47,24],[48,23,49,23],[48,26,49,26],[48,29,49,29],[45,26,46,26],[45,29,46,29],[48,11,49,11],[47,32,47,33],[47,11,47,12],[47,14,47,15],[47,17,47,18],[47,20,47,21],[48,14,49,14],[48,17,49,17],[47,26,47,27],[45,11,46,11],[45,14,46,14],[45,17,46,17],[20,10,20,11],[28,10,28,11],[29,10,29,11],[30,10,30,11],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[16,10,16,11],[7,10,7,11],[8,10,8,11],[9,10,9,11],[10,10,10,11],[11,10,11,11],[12,10,12,11],[64,11,64,12],[7,0,7,9],[13,10,13,11],[14,10,14,11],[15,10,15,11],[18,10,18,11],[19,10,19,11],[34,10,34,11],[21,10,21,11],[22,10,22,11],[23,10,23,11],[24,10,24,11],[25,10,25,11],[26,10,26,11],[27,10,27,11],[33,10,33,11]]}
[" UPUTE ZA RAD: - Ispuniti sve podatke u čelijama s plavom bojom. Ispuniti i za izbor armature u kolonama L,N i O",null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z18/M18","v":{"$error":"#VALUE!"}}]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  ","krak                  y  ","Moment destabilnosti i stabilnosti","za Mzida                                              krakovi                             x                  y",null,"Moment zida II","za M u                           presjeku II-II                                                   krakovi                                x               y",null,"Moment      II-II","za M u                           temelju ispod zida                     krakovi                             x                  y",null,"Moment  ","za M u                           presjeku I-I                                              krakovi                             x                  y",null,"Moment      I-I"]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C XIV-XV'!C15","v":0.5},null,null,null,{"$f":"2+E57-E54-E51/2","v":3.8000010999999998},{"$f":"+E48","v":1.2},null,{"$f":"2+E55","v":3.4000010999999999},{"$f":"'C XIV-XV'!AC47+(E48-'C XIV-XV'!AC47)/2","v":0.72068965844232813},null,{"$f":"2+E55+E51/2","v":3.8000010999999998},{"$f":"'C XIV-XV'!AC49+(E48-'C XIV-XV'!AF47)/2","v":0.97931024673015765},null,{"$f":"2+E55+E51","v":4.2000010999999997},{"$f":"'C XIV-XV'!AC49+(E48-'C XIV-XV'!AC49)/2","v":0.78965512336507881}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#VALUE!"}},null,null,{"$f":"+H108","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$W$7","v":{"$error":"#VALUE!"}},{"$f":"+M8*Y8","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$AB$7","v":{"$error":"#VALUE!"}},{"$f":"T8*AB8","v":{"$error":"#VALUE!"}}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,null,{"$f":"+M9","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$f":"+W9-$AB$7","v":{"$error":"#VALUE!"}},{"$f":"AB9*T9","v":{"$error":"#VALUE!"}}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"+M10","v":{"$error":"#VALUE!"}},null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,{"$f":"+AE7-'C XIV-XV'!F93","v":{"$error":"#VALUE!"}},{"$f":"+AE10*S10","v":{"$error":"#VALUE!"}}]
[null,null,"GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$f":"+W11-$AB$7","v":{"$error":"#REF!"}},{"$f":"AB11*T11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ...................................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":48.296291314453413},null,null,null,null,null,null,{"$f":"+M15","v":48.296291314453413},null,null,5,null,4.5,{"$f":"-M15*Y15","v":-217.33331091504036},null,3.8,183.52590699492296]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":0},null,null,null,null,null,null,0,null,null,0,null,-0.5,0,null,-1.2,0]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":{"$error":"#VALUE!"}},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-'P XIV-XIV'!M61)","v":0},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#VALUE!"}},null,null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,{"$f":"+AK7-C117","v":0.78965512336507881},{"$f":"+M17*AK17","v":{"$error":"#VALUE!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S8:S17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T8:T17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U8:U17)","v":0},null,null,"x",null,{"$f":"SUM(Z8:Z17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC8:AC17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF8:AF17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI8:AI17)","v":0},null,null,{"$f":"SUM(AL8:AL17)","v":{"$error":"#VALUE!"}}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C XIV-XV'!V61+'C XIV-XV'!X61+'C XIV-XV'!Z61","v":68.875052249999982},{"$f":"+'C XIV-XV'!Z61","v":13.306056250595223},{"$f":"+'C XIV-XV'!V61","v":37.77589163555291},null,{"$f":"+'C XIV-XV'!X61","v":17.793104363851846},null,null,null,null,{"$f":"+H126","v":3.3485779696489133},null,{"$f":"+$V$7-V19","v":1.5514242303510861},null,{"$f":"+M19*X19","v":106.85442492734707},null,null,null,{"$f":"AD7-'C XIV-XV'!V59","v":0.72609215808095717},null,{"$f":"+AD19*O19","v":27.428778681090989},{"$f":"+AG7-'C XIV-XV'!X59","v":1.0335908939774985E-2},null,{"$f":"+'C XIV-XV'!X61*'Analiza i dimenzioniranje'!AQ13","v":0.14465929289570792},{"$f":"AJ7-'C XIV-XV'!Z59","v":-0.34074126926177506},null,{"$f":"+'C XIV-XV'!Z61*'Analiza i dimenzioniranje'!AT13","v":-4.5636103109654318}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M20","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V20","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V20","v":{"$error":"#VALUE!"}},null,{"$f":"+P20*AA20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli............................."," ",0,null,null,{"$f":"+M21","v":0},null,null,null,null,null,4.9000021999999994,null,0,null,0,{"$f":"+$AA$7-V21","v":-1.1000010999999996},null,{"$f":"+P21*AA21","v":0}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza............."," ",0,null,{"$f":"+M22","v":0},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+AD7-V22","v":{"$error":"#VALUE!"}},null,{"$f":"+M22*AD22","v":{"$error":"#VALUE!"}}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0},null,null,null,null,null,null,null,4.5500016499999996,null,0.35000054999999985,null,0,null,null,null,null,null,null,null,null,null,{"$f":"AJ7-(2+E57-E54/2)","v":-0.35000054999999985},null,{"$f":"+AJ23*N23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X24","v":{"$error":"#VALUE!"}},null,{"$f":"+M24*AD24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X25","v":{"$error":"#VALUE!"}},null,{"$f":"+M25*AD25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X26","v":{"$error":"#VALUE!"}},null,{"$f":"+M26*AD26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X27","v":{"$error":"#VALUE!"}},null,{"$f":"+M27*AD27","v":{"$error":"#VALUE!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",12.940952255126037,null,null,{"$f":"+M28","v":12.940952255126037},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V28","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V28","v":{"$error":"#VALUE!"}},null,{"$f":"P28*AA28","v":{"$error":"#VALUE!"}}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M29","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V29","v":{"$error":"#VALUE!"}},null,{"$f":"+P29*AA29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M30","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V30","v":{"$error":"#VALUE!"}},null,{"$f":"+P30*AA30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",{"$error":"#VALUE!"},null,{"$f":"+M31","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,2,null,2.9000021999999994,null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-'C XIV-XV'!E93","v":1.4000010999999999},null,{"$f":"+M31*AD31","v":{"$error":"#VALUE!"}},{"$f":"+$AD$7-AD31","v":2}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.306056250595223},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":17.793104363851846},null,null,null,null,null,null,null,null,{"$f":"SUM(Z19:Z31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC19:AC31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF19:AF31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI19:AI31)","v":0.14465929289570792},null,null,{"$f":"SUM(AL19:AL31)","v":-4.5636103109654318}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"II-II","sredina","I-I"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C XIV-XV'!Z76+'C XIV-XV'!AB76+'C XIV-XV'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":{"$error":"#VALUE!"}},null,{"$f":"+'C XIV-XV'!AB76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+'C XIV-XV'!Z76","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!AB76","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!AD76","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"$AD$7-'C XIV-XV'!Z77","v":{"$error":"#VALUE!"}},null,{"$f":"+X34*AD34","v":{"$error":"#VALUE!"}},{"$f":"$AG$7-'C XIV-XV'!AB77","v":{"$error":"#VALUE!"}},null,{"$f":"-Y34*AG34","v":{"$error":"#VALUE!"}},{"$f":"+AJ7-'C XIV-XV'!AD77","v":{"$error":"#VALUE!"}},null,{"$f":"+Z34*AJ34","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+Z35","v":{"$error":"#VALUE!"}},{"$f":"+X35","v":{"$error":"#VALUE!"}},null,{"$f":"+Y35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M35*E55/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E51/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E54/E57","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AE7-'C XIV-XV'!AC45","v":{"$error":"#VALUE!"}},{"$f":"-S35*AE35","v":{"$error":"#VALUE!"}},null,{"$f":"+AH7-'C XIV-XV'!AC48","v":{"$error":"#VALUE!"}},{"$f":"Y35*AH35","v":{"$error":"#VALUE!"}},null,{"$f":"+AK7-'C XIV-XV'!AC52","v":{"$error":"#VALUE!"}},{"$f":"-Z35*AK35","v":{"$error":"#VALUE!"}}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},{"$f":"R18+R35","v":{"$error":"#VALUE!"}},{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#VALUE!"}},{"$f":"+U18+U35","v":{"$error":"#VALUE!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"SUM(R36:U36)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+AC18+AC32+AC34+AC35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AF18+AF32+AF34+AF35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AI18+AI32+AI34+AI35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AL18+AL32+AL34+AL35","v":{"$error":"#VALUE!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!AD40","v":50},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y","x"]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"+'Analiza i dimenzioniranje'!E39","v":15},"°    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD7","v":3.4000010999999999},{"$f":"+AE7","v":0.72068965844232813}]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!AD42","v":5},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'C XIV-XV'!V61*('Analiza i dimenzioniranje'!AI33-'C XIV-XV'!V59)+B129*(AD39-H129)+B138*(AD39-H138)+B138*(AD39-H138)+'C XIV-XV'!Z76*('Analiza i dimenzioniranje'!AI33-'C XIV-XV'!Z77)+S35*(AE39-'C XIV-XV'!AG66)+B110*(AE39-H110)","v":{"$error":"#VALUE!"}}]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*'C XIV-XV'!AC118*C42/B42","v":0},"kN/m'"]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'P XIII-XIII'!C42","v":1}]
[null,null,"DIMENZIJE ZIDA:"]
[]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":{"$error":"#VALUE!"}},"m"]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C XIV-XV'!B10-'C XIV-XV'!B11=0,\">100\",IF('C XIV-XV'!C10-'C XIV-XV'!C11/(0.00000000000001+'C XIV-XV'!B11-'C XIV-XV'!B10)>100,\">100\",('C XIV-XV'!C10-'C XIV-XV'!C11)/('C XIV-XV'!B11-'C XIV-XV'!B10)))","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+('C XIV-XV'!I87-'C XIV-XV'!Q17)","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C XIV-XV'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C XIV-XV'!E64","v":1.4000010999999999},"m"]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 "]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m"]
[" zapreminska težina nasipa ...............................",null,null,"      gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AD44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C XIV-XV'!I87-'C XIV-XV'!Q17)-B109*('C XIV-XV'!K87-'C XIV-XV'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C XIV-XV'!Q16-'C XIV-XV'!N59)+B136*('C XIV-XV'!Q16-'C XIV-XV'!M93)+B137*('C XIV-XV'!Q16-'C XIV-XV'!C93)+B135*(C135),-B116*C116/1.35-B108*('C XIV-XV'!I87-'C XIV-XV'!Q17)-B109*('C XIV-XV'!K87-'C XIV-XV'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C XIV-XV'!Q16-'C XIV-XV'!M93)+B137*('C XIV-XV'!Q16-'C XIV-XV'!C93)+B135*(C135))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+#REF!)","v":{"$error":"#REF!"}},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+'Dijagram momenata'!Q11","v":4.08},null,{"$f":"-#REF!*N66","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":0},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota",null,"krak od presjeka do sile"]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c111",{"$f":"IF(+L66-'Dijagram momenata'!$Q$11>0,+L66-'Dijagram momenata'!$Q$11,0)","v":{"$error":"#REF!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c112",{"$f":"IF(+L67-'Dijagram momenata'!$Q$11>0,+L67-'Dijagram momenata'!$Q$11,0)","v":{"$error":"#REF!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c113",{"$f":"IF(+L68-'Dijagram momenata'!$Q$11>0,+L68-'Dijagram momenata'!$Q$11,0)","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c114",{"$f":"IF(+L69-'Dijagram momenata'!$Q$11>0,+L69-'Dijagram momenata'!$Q$11,0)","v":{"$error":"#REF!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+'C XIV-XV'!I85","v":{"$error":"#VALUE!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213},null,null,{"$f":"COS((-G48-G14)*PI()/180)^2","v":0.88302222155948906}]
[" sloj 2. ..............................",{"$f":"+'C XIV-XV'!K88","v":{"$error":"#VALUE!"}},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658},null,null,{"$f":"IF(F18=0,COS((-G48)*PI()/180)^2*COS((-G48)*PI()/180),COS((-G48)*PI()/180)^2*COS((-G48+G18)*PI()/180))","v":1}]
[" sloj 3. ..............................",{"$f":"+'P III-III'!B99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!C99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!D99","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527},null,null,{"$f":"IF(F18=0,SIN((G14)*PI()/180)*SIN((G14-G19)*PI()/180),SIN((G14+G18)*PI()/180)*SIN((G14-G19)*PI()/180))","v":0.10569003670618687}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"IF(I18=0,COS((-G48)*PI()/180)*COS((G19+G48)*PI()/180),COS((-G48+G18)*PI()/180)*COS((G19+G48)*PI()/180))","v":0.99939082701909576},{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0},null,null,{"$f":"SQRT(I99/I100)","v":0.32519910741806074}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0},null,null,{"$f":"(1+I101)^2","v":1.7561526743016247}]
[null,null,null,null,null,null,null,null,{"$f":"(I97/I98)/I102","v":0.50281631801212479}]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,0,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I120","v":1},null,null,{"$f":"+'C XIV-XV'!N87","v":{"$error":"#VALUE!"}}]
[" Eh2 .............................................",{"$f":"+C98","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I121","v":1},null,null,{"$f":"+'C XIV-XV'!K87","v":{"$error":"#VALUE!"}}]
[" Eh3 .....................................................",{"$f":"+C99","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I122","v":1},null,null,{"$f":"+C110+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPrometno ....................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I124","v":1.3},null,null,{"$f":"+C111+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+B112*C112","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I125","v":1},null,null,{"$f":"+C112+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPLinijsko ................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"+B113*C113","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I126","v":1}]
[" EQTemelj ....................................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I127","v":1},null,null,{"$f":"+C114+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,null,{"$f":"+'C XIV-XV'!$AI$44","v":1.5001009999999999},{"$f":"+'C XIV-XV'!$AH$44","v":4.9000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":-48.296291314453413},{"$f":"IF(H115<'Analiza i dimenzioniranje'!AD44,0,H115-'Analiza i dimenzioniranje'!AD44)","v":0.91999999999999993},{"$f":"+B115*C115","v":-44.432588009297135},{"$f":"+'Analiza i dimenzioniranje'!I129","v":0},null,null,{"$f":"+E40","v":5},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":6.9000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":0},{"$f":"+H116-'Analiza i dimenzioniranje'!AD44","v":-4.08},{"$f":"B116*C116","v":0},{"$f":"+'Analiza i dimenzioniranje'!I150","v":0},"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C XIV-XV'!AC117","v":0}]
[{"$f":"+A101","v":{"$error":"#VALUE!"}},{"$f":"-B101","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!E116","v":0},null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}},null,null,"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C XIV-XV'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C XIV-XV'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},{"$f":"+'Analiza i dimenzioniranje'!I135","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C XIV-XV'!L61","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XIV-XV'!L59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I136","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C XIV-XV'!L59","v":{"$error":"#VALUE!"}}]
[" Gnasip na konzoli.............................",{"$f":"IF(M61>=E67+E68,0,'C XIV-XV'!N61)","v":0},{"$f":"IF(B128=0,0,2+E57-'C XIV-XV'!N59)","v":0},{"$f":"B128*C128","v":0},{"$f":"+'Analiza i dimenzioniranje'!I138","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C128","v":4.9000021999999994}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C XIV-XV'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I139","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},{"$f":"+'Analiza i dimenzioniranje'!I140","v":{"$error":"#VALUE!"}},null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C XIV-XV'!W18<'C XIV-XV'!B7,0,('C XIV-XV'!W18-'C XIV-XV'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C XIV-XV'!W18+'C XIV-XV'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I141","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C XIV-XV'!W23>'C XIV-XV'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C XIV-XV'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I142","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C XIV-XV'!W26>'C XIV-XV'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C XIV-XV'!W25)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I143","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C XIV-XV'!W31>'C XIV-XV'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XIV-XV'!W33-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I144","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":12.940952255126037},{"$f":"2+E57-'C XIV-XV'!AB24-E54-'Analiza i dimenzioniranje'!AD49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I145","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XIV-XV'!M93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I146","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XIV-XV'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I147","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XIV-XV'!E93","v":2.9000021999999994},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I148","v":1},null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]

{"sheet":"P XV-XV","index":26,"n_rows":175,"n_cols":24,"rows_kept":175,"cut":false,"hidden":true,"merged":[[30,10,30,11],[95,6,95,8],[33,10,33,11],[56,10,56,18],[73,0,73,9],[64,11,64,12],[57,10,57,18],[34,10,34,11],[162,1,162,2],[46,0,46,2],[68,0,68,8],[69,0,69,8],[71,0,71,7],[72,0,72,8],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[7,0,7,9],[13,10,13,11],[20,10,20,11],[21,10,21,11],[29,10,29,11],[27,0,27,2],[27,10,27,11],[28,0,28,2],[28,10,28,11],[24,0,24,2],[25,0,25,2]]}
[" UPUTE ZA RAD: - Ispuniti sve podatke u čelijama s plavom bojom. Ispuniti i za izbor armature u kolonama L,N i O",null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  "]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C XIV-XV'!C15","v":0.5}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#VALUE!"}}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,null,{"$f":"+M9","v":{"$error":"#VALUE!"}}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"+M10","v":{"$error":"#VALUE!"}}]
[null,"milenium","GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ....................................................",null,{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":48.296291314453413},null,null,null,null,null,null,{"$f":"M15","v":48.296291314453413}]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":0},null,null,null,null,null,null,0]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":{"$error":"#VALUE!"}},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-'P XV-XV'!M61)","v":0},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#VALUE!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S8:S17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T8:T17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U8:U17)","v":0}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C XIV-XV'!V61+'C XIV-XV'!X61+'C XIV-XV'!Z61","v":68.875052249999982},{"$f":"+'C XIV-XV'!Z61","v":13.306056250595223},{"$f":"+'C XIV-XV'!V61","v":37.77589163555291},null,{"$f":"+'C XIV-XV'!X61","v":17.793104363851846}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli.............................",null,{"$error":"#VALUE!"},null,null,{"$f":"+M21","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza.............",null,0,null,{"$f":"+M22","v":0}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",12.940952255126037,null,null,{"$f":"+M28","v":12.940952255126037}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",{"$error":"#VALUE!"},null,{"$f":"+M31","v":{"$error":"#VALUE!"}}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.306056250595223},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":17.793104363851846}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C XIV-XV'!Z76+'C XIV-XV'!AB76+'C XIV-XV'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":0},null,{"$f":"+'C XIV-XV'!AB76","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+X35","v":0},null,{"$f":"+#REF!","v":{"$error":"#REF!"}}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},null,{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#VALUE!"}},{"$f":"+U18+U35","v":{"$error":"#REF!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,"EUROCOD 2",null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"SUM(R36:U36)","v":{"$error":"#VALUE!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!AE40","v":50},"kN/m'",null,null,null,null,"Marka betona",15,20,25,30,40]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"IF(E38=0,0,'Analiza i dimenzioniranje'!E39)","v":15},"°    ",null,null,null,null,"Klasa betona C","12/15","16/20","20/25","25/30","30/37"]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!AE42","v":5},"m",null,null,null,null,"fcm (N/mm2)",20,24,28,33,38]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*'C XIV-XV'!AE118*C42/B42","v":0},"kN/m'",null,null,null,null,"ecu  (%0)",-3.6,-3.5,-3.4,-3.3,-3.2]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'P XIV-XIV'!C42","v":1},null,null,null,null,null,null,null,"fck valjak (N/mm2)",12,16,20,25,30]
[null,null,"DIMENZIJE ZIDA:",null,null,null,"          GRADIVO TEMELJA I ZIDA:",null,null,null,"fck kocka (N/mm2)",15,20,25,30,37]
[null,null,null,null,null,null,null,null,500,500,"Ecm (N/mm2)",26000,27500,29000,30500,32000]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":{"$error":"#VALUE!"}},"m",null,null,null,null,"ARMATURA",null,null,500]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C XIV-XV'!B10-'C XIV-XV'!B11=0,\">100\",IF('C XIV-XV'!C10-'C XIV-XV'!C11/(0.00000000000001+'C XIV-XV'!B11-'C XIV-XV'!B10)>100,\">100\",('C XIV-XV'!C10-'C XIV-XV'!C11)/('C XIV-XV'!B11-'C XIV-XV'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C XIV-XV'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C XIV-XV'!E64","v":1.4000010999999999},"m",{"$f":"+IF(E32=0,\"\",IF(G54>#REF!+E36,\"PAZI POLOŽAJ TEMELJA\",\"\"))","v":{"$error":"#REF!"}}]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m",null,null,null,null,"FAKTORI STABILNOSTI I KONTAKTNI NAPONI"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 ",null,null,null,null,null,null,null,null,"M="," -  "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 ",null,null,null,null,null,null,null,null,"     v=","+"]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m",null,null,null,null,"MOMENTI SAVIJANJA (kNm/m')",null,null,null,"     h=","-"]
[" zapreminska težina nasipa ...............................",null,null,"gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,"Moment na koti +",null,{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},"Mkonzole"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!D63","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AE44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C XIV-XV'!N87-'C XIV-XV'!P17)-B109*('C XIV-XV'!P87-'C XIV-XV'!P17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C XIV-XV'!P16-'C XIV-XV'!R59)+B136*('C XIV-XV'!P16-'C XIV-XV'!H93)+B137*('C XIV-XV'!P16-'C XIV-XV'!C93)+B135*(C135),-B116*C116/1.35-B108*('C XIV-XV'!N87-'C XIV-XV'!P17)-B109*('C XIV-XV'!P87-'C XIV-XV'!P17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C XIV-XV'!P16-'C XIV-XV'!H93)+B137*('C XIV-XV'!P16-'C XIV-XV'!C93)+B135*(C135))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+E592)","v":0},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+'Dijagram momenata'!Q10","v":4.4000000000000004},null,{"$f":"-#REF!*N66","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":0},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota",null,"krak od presjeka do sile","     v11=",{"$f":"B130+'C XIV-XV'!Z61+'C XIV-XV'!AD76","v":{"$error":"#VALUE!"}}]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c111",{"$f":"IF(+L66-'Dijagram momenata'!$Q$10>0,+L66-'Dijagram momenata'!$Q$10,0)","v":{"$error":"#REF!"}},"     h11=",{"$f":"+B118*E54/E57-B117","v":{"$error":"#VALUE!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c112",{"$f":"IF(+L67-'Dijagram momenata'!$Q$10>0,+L67-'Dijagram momenata'!$Q$10,0)","v":{"$error":"#REF!"}},"     v22=",{"$f":"+B129+B131+B132+B133+B134+B138+'C XIV-XV'!Z76+'C XIV-XV'!V61","v":{"$error":"#VALUE!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c113",{"$f":"IF(+L68-'Dijagram momenata'!$Q$10>0,+L68-'Dijagram momenata'!$Q$10,0)","v":{"$error":"#REF!"}},"     h22=",{"$f":"+B118*E55/E57-B110","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c114",{"$f":"IF(+L69-'Dijagram momenata'!$Q$10>0,+L69-'Dijagram momenata'!$Q$10,0)","v":{"$error":"#REF!"}},"     v33=",{"$f":"B127+B128+B135+B136+B137","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     h33=",{"$f":"-B108-B109-B111-B112-B113-B114+B115-B116","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko"," -koeficijent mirnog pritiska",null,null,"     vtem=",{"$f":"+'C XIV-XV'!X61+'C XIV-XV'!AB76","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko1=","1-sinj1=",{"$f":"1-SIN(E14*PI()/180)","v":0.62539340658408804},"varijanta","     htem=",{"$f":"+B118*E51/E57","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Ko2=","1-sinj2=",{"$f":"1-SIN(F14*PI()/180)","v":0.69098300562505255},"n","    MI-I",{"$f":"+K62","v":0}]
[null,null,null,null,null,null,null,null,null,null,"Ko3=","1-sinj3=",{"$f":"1-SIN(G14*PI()/180)","v":0.65797985667433134},null,"MII-II",{"$f":"+L62","v":0}]
[null,null,null,null,null,null,null,null,null,null,"Ko=","n/(1-n) =",{"$f":"+N75/(1-N75)","v":0.66666666666666674},0.4,"Mzida",{"$f":"+M62","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+(B172*E51*E58)","v":0},{"$f":"+E51/2","v":0.4},{"$f":"+K76*L76","v":0}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+'C XIV-XV'!N85","v":{"$error":"#VALUE!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+'C XIV-XV'!P88","v":{"$error":"#VALUE!"}},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658}]
[" sloj 3. ..............................",{"$f":"+'P III-III'!B99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!C99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!D99","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,null,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#VALUE!"}},null,null,1.35,null,null,{"$f":"+'C XIV-XV'!N87","v":{"$error":"#VALUE!"}}]
[" Eh2 .............................................",{"$f":"+C98","v":{"$error":"#VALUE!"}},null,null,1.35,null,null,{"$f":"+'C XIV-XV'!P87","v":{"$error":"#VALUE!"}}]
[" Eh3 .....................................................",{"$f":"+C99","v":{"$error":"#VALUE!"}},null,null,1.35,null,null,{"$f":"+C110+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPrometno ....................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,1.5]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,1.35,null,null,{"$f":"+C112+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPLinijsko ................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"B113*C113","v":{"$error":"#REF!"}},1.35,null,null,{"$f":"+C113+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EQTemelj ....................................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,1.35,null,null,{"$f":"+C114+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,null,{"$f":"+'C XIV-XV'!$AI$44","v":1.5001009999999999},{"$f":"+'C XIV-XV'!$AH$44","v":4.9000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":-48.296291314453413},{"$f":"IF(H115<'Analiza i dimenzioniranje'!AE44,0,H115-'Analiza i dimenzioniranje'!AE44)","v":0.59999999999999964},null,1.35,null,null,{"$f":"+E40","v":5},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":6.9000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":0},{"$f":"+H116-'Analiza i dimenzioniranje'!AE44","v":-4.4000000000000004},{"$f":"B116*C116","v":0},1,"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C XIV-XV'!AE117","v":0}]
[{"$f":"+A101","v":{"$error":"#VALUE!"}},{"$f":"-B101","v":{"$error":"#VALUE!"}},{"$f":"IF(F101=0,0,E49/3)","v":0},{"$f":"B117*C117","v":{"$error":"#VALUE!"}},1.35,null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}}," S MHA =",{"$f":"SUM(D108:D117)","v":{"$error":"#REF!"}},"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C XIV-XV'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C XIV-XV'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},1.35,null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C XIV-XV'!P61","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XIV-XV'!D59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},1.35,null,null,{"$f":"2+$E$57-C127","v":{"$error":"#VALUE!"}}]
[" Gnasip na konzoli.............................",{"$f":"'C XIV-XV'!R61","v":{"$error":"#VALUE!"}},{"$f":"IF(B128=0,0,2+E57-'C XIV-XV'!J59)","v":{"$error":"#VALUE!"}},{"$f":"B128*C128","v":{"$error":"#VALUE!"}},1.35,null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C XIV-XV'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},1.35,null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},1.35,null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C XIV-XV'!W18<'C XIV-XV'!B7,0,('C XIV-XV'!W18-'C XIV-XV'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C XIV-XV'!W18+'C XIV-XV'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},1.5,null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C XIV-XV'!W23>'C XIV-XV'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C XIV-XV'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C XIV-XV'!W26>'C XIV-XV'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C XIV-XV'!W25)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C XIV-XV'!W31>'C XIV-XV'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XIV-XV'!W33-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":12.940952255126037},{"$f":"2+E57-'C XIV-XV'!AC24-E54-'Analiza i dimenzioniranje'!AE49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XIV-XV'!H93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XIV-XV'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},1.35,null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XIV-XV'!E93","v":2.9000021999999994},{"$error":"#VALUE!"},1.35,null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]
[]
[]
[]
[" Rezultanta sila .........................................",null,"      R =",{"$f":"SQRT(B118^2+B139^2)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" sila uzduž temelja ..................................................",null,{"$f":"IF(E48=E49,\"     RH =\",\"     RT =\")","v":"     RT ="},{"$f":"D144*SIN((D148-D149)*PI()/180)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" sila okomita na temelj .................................",null,"    RN =",{"$f":"D144*COS((D148-D149)*PI()/180)","v":{"$error":"#VALUE!"}},"kN/m'"]
[" moment oko osi temelja.....................................",null,"     Ms =",{"$f":"+B118*(I118-'C XIV-XV'!AC50)-'Analiza i dimenzioniranje'!B168*(F139-E57/2)","v":{"$error":"#VALUE!"}},"kNm/m'"]
[" otklon rezultante od vertikale .....................................",null,"a =",{"$f":"ATAN(B118/B139)*180/PI()","v":{"$error":"#VALUE!"}},"°"]
[" nagib temelja ..........................................",null,"b =",{"$f":"ATAN('C XIV-XV'!C15/E57)*180/PI()","v":9.7823997540577476},"°"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,{"$f":"IF(E49=E48,\"\",+D167*COS(D149*PI()/180))","v":0}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"za Presjeke I-I i II-II"]
[null,null,null,null,null,null,null,null,null,null,"     As,min=",{"$f":"+MAX(E251,E269)","v":0},{"$f":"+MAX(L174:L175)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"     As,1 mjer =",{"$f":"+IF(E255>L173/2,E255,L173/2)","v":0},{"$f":"+L174-7.85","v":-7.85}]
[null,null,null,null,null,null,null,null,null,null,"     As,2 mjer =",{"$f":"+IF(E273>L173/2,E273,L173/2)","v":0},{"$f":"+L175-7.85","v":-7.85}]

{"sheet":"P XVI-XVI","index":27,"n_rows":140,"n_cols":38,"rows_kept":140,"cut":false,"hidden":true,"merged":[[46,38,46,39],[46,35,46,36],[45,32,46,32],[44,38,45,38],[47,38,48,38],[48,32,49,32],[47,35,48,35],[45,20,46,20],[45,23,46,23],[47,29,47,30],[44,35,45,35],[48,20,49,20],[47,23,47,24],[48,23,49,23],[48,26,49,26],[48,29,49,29],[45,26,46,26],[45,29,46,29],[48,11,49,11],[47,32,47,33],[47,11,47,12],[47,14,47,15],[47,17,47,18],[47,20,47,21],[48,14,49,14],[48,17,49,17],[47,26,47,27],[45,11,46,11],[45,14,46,14],[45,17,46,17],[20,10,20,11],[28,10,28,11],[29,10,29,11],[30,10,30,11],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[16,10,16,11],[7,10,7,11],[8,10,8,11],[9,10,9,11],[10,10,10,11],[11,10,11,11],[12,10,12,11],[64,11,64,12],[7,0,7,9],[13,10,13,11],[14,10,14,11],[15,10,15,11],[18,10,18,11],[19,10,19,11],[34,10,34,11],[21,10,21,11],[22,10,22,11],[23,10,23,11],[24,10,24,11],[25,10,25,11],[26,10,26,11],[27,10,27,11],[33,10,33,11]]}
[" UPUTE ZA RAD: - Ispuniti sve podatke u čelijama s plavom bojom. Ispuniti i za izbor armature u kolonama L,N i O",null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z18/M18","v":{"$error":"#VALUE!"}}]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  ","krak                  y  ","Moment destabilnosti i stabilnosti","za Mzida                                              krakovi                             x                  y",null,"Moment zida II","za M u                           presjeku II-II                                                   krakovi                                x               y",null,"Moment      II-II","za M u                           temelju ispod zida                     krakovi                             x                  y",null,"Moment  ","za M u                           presjeku I-I                                              krakovi                             x                  y",null,"Moment      I-I"]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C XVI-XVII'!C15","v":0.5},null,null,null,{"$f":"2+E57-E54-E51/2","v":3.8000010999999998},{"$f":"+E48","v":1.2},null,{"$f":"2+E55","v":3.4000010999999999},{"$f":"'C XVI-XVII'!AC47+(E48-'C XVI-XVII'!AC47)/2","v":0.72068965844232813},null,{"$f":"2+E55+E51/2","v":3.8000010999999998},{"$f":"'C XVI-XVII'!AC49+(E48-'C XVI-XVII'!AF47)/2","v":0.97931024673015765},null,{"$f":"2+E55+E51","v":4.2000010999999997},{"$f":"'C XVI-XVII'!AC49+(E48-'C XVI-XVII'!AC49)/2","v":0.78965512336507881}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#VALUE!"}},null,null,{"$f":"+H108","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$W$7","v":{"$error":"#VALUE!"}},{"$f":"+M8*Y8","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$AB$7","v":{"$error":"#VALUE!"}},{"$f":"T8*AB8","v":{"$error":"#VALUE!"}}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,null,{"$f":"+M9","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$f":"+W9-$AB$7","v":{"$error":"#VALUE!"}},{"$f":"AB9*T9","v":{"$error":"#VALUE!"}}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"+M10","v":{"$error":"#VALUE!"}},null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,{"$f":"+AE7-'C XVI-XVII'!F93","v":{"$error":"#VALUE!"}},{"$f":"+AE10*S10","v":{"$error":"#VALUE!"}}]
[null,null,"GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$f":"+W11-$AB$7","v":{"$error":"#REF!"}},{"$f":"AB11*T11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ...................................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":48.296291314453413},null,null,null,null,null,null,{"$f":"+M15","v":48.296291314453413},null,null,5,null,4.5,{"$f":"-M15*Y15","v":-217.33331091504036},null,3.8,183.52590699492296]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":0},null,null,null,null,null,null,0,null,null,0,null,-0.5,0,null,-1.2,0]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":{"$error":"#VALUE!"}},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-M61)","v":0},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#VALUE!"}},null,null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,{"$f":"+AK7-C117","v":0.78965512336507881},{"$f":"+M17*AK17","v":{"$error":"#VALUE!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S8:S17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(T8:T17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U8:U17)","v":0},null,null,"x",null,{"$f":"SUM(Z8:Z17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC8:AC17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF8:AF17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI8:AI17)","v":0},null,null,{"$f":"SUM(AL8:AL17)","v":{"$error":"#VALUE!"}}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C XVI-XVII'!V61+'C XVI-XVII'!X61+'C XVI-XVII'!Z61","v":68.875052249999982},{"$f":"+'C XVI-XVII'!Z61","v":13.306056250595223},{"$f":"+'C XVI-XVII'!V61","v":37.77589163555291},null,{"$f":"+'C XVI-XVII'!X61","v":17.793104363851846},null,null,null,null,{"$f":"+H126","v":3.3485779696489133},null,{"$f":"+$V$7-V19","v":1.5514242303510861},null,{"$f":"+M19*X19","v":106.85442492734707},null,null,null,{"$f":"AD7-'C XVI-XVII'!V59","v":0.72609215808095717},null,{"$f":"+AD19*O19","v":27.428778681090989},{"$f":"+AG7-'C XVI-XVII'!X59","v":1.0335908939774985E-2},null,{"$f":"+'C XVI-XVII'!X61*'Analiza i dimenzioniranje'!AQ13","v":0.14465929289570792},{"$f":"AJ7-'C XVI-XVII'!Z59","v":-0.34074126926177506},null,{"$f":"+'C XVI-XVII'!Z61*'Analiza i dimenzioniranje'!AT13","v":-4.5636103109654318}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M20","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V20","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V20","v":{"$error":"#VALUE!"}},null,{"$f":"+P20*AA20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli............................."," ",0,null,null,{"$f":"+M21","v":0},null,null,null,null,null,4.9000021999999994,null,0,null,0,{"$f":"+$AA$7-V21","v":-1.1000010999999996},null,{"$f":"+P21*AA21","v":0}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza............."," ",0,null,{"$f":"+M22","v":0},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+AD7-V22","v":{"$error":"#VALUE!"}},null,{"$f":"+M22*AD22","v":{"$error":"#VALUE!"}}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0},null,null,null,null,null,null,null,4.5500016499999996,null,0.35000054999999985,null,0,null,null,null,null,null,null,null,null,null,{"$f":"AJ7-(2+E57-E54/2)","v":-0.35000054999999985},null,{"$f":"+AJ23*N23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X24","v":{"$error":"#VALUE!"}},null,{"$f":"+M24*AD24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X25","v":{"$error":"#VALUE!"}},null,{"$f":"+M25*AD25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X26","v":{"$error":"#VALUE!"}},null,{"$f":"+M26*AD26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X27","v":{"$error":"#VALUE!"}},null,{"$f":"+M27*AD27","v":{"$error":"#VALUE!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",12.940952255126037,null,null,{"$f":"+M28","v":12.940952255126037},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V28","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V28","v":{"$error":"#VALUE!"}},null,{"$f":"P28*AA28","v":{"$error":"#VALUE!"}}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M29","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V29","v":{"$error":"#VALUE!"}},null,{"$f":"+P29*AA29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M30","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V30","v":{"$error":"#VALUE!"}},null,{"$f":"+P30*AA30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",{"$error":"#VALUE!"},null,{"$f":"+M31","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,2,null,2.9000021999999994,null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-'C XVI-XVII'!E93","v":1.4000010999999999},null,{"$f":"+M31*AD31","v":{"$error":"#VALUE!"}},{"$f":"+$AD$7-AD31","v":2}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.306056250595223},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":17.793104363851846},null,null,null,null,null,null,null,null,{"$f":"SUM(Z19:Z31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC19:AC31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF19:AF31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI19:AI31)","v":0.14465929289570792},null,null,{"$f":"SUM(AL19:AL31)","v":-4.5636103109654318}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"II-II","sredina","I-I"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C XVI-XVII'!Z76+'C XVI-XVII'!AB76+'C XVI-XVII'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":{"$error":"#VALUE!"}},null,{"$f":"+'C XVI-XVII'!AB76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+'C XVI-XVII'!Z76","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!AB76","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!AD76","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"$AD$7-'C XVI-XVII'!Z77","v":{"$error":"#VALUE!"}},null,{"$f":"+X34*AD34","v":{"$error":"#VALUE!"}},{"$f":"$AG$7-'C XVI-XVII'!AB77","v":{"$error":"#VALUE!"}},null,{"$f":"-Y34*AG34","v":{"$error":"#VALUE!"}},{"$f":"+AJ7-'C XVI-XVII'!AD77","v":{"$error":"#VALUE!"}},null,{"$f":"+Z34*AJ34","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+Z35","v":{"$error":"#VALUE!"}},{"$f":"+X35","v":{"$error":"#VALUE!"}},null,{"$f":"+Y35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M35*E55/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E51/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E54/E57","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AE7-'C XVI-XVII'!AC45","v":{"$error":"#VALUE!"}},{"$f":"-S35*AE35","v":{"$error":"#VALUE!"}},null,{"$f":"+AH7-'C XVI-XVII'!AC48","v":{"$error":"#VALUE!"}},{"$f":"Y35*AH35","v":{"$error":"#VALUE!"}},null,{"$f":"+AK7-'C XVI-XVII'!AC52","v":{"$error":"#VALUE!"}},{"$f":"-Z35*AK35","v":{"$error":"#VALUE!"}}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},{"$f":"R18+R35","v":{"$error":"#VALUE!"}},{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#VALUE!"}},{"$f":"+U18+U35","v":{"$error":"#VALUE!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"SUM(R36:U36)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+AC18+AC32+AC34+AC35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AF18+AF32+AF34+AF35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AI18+AI32+AI34+AI35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AL18+AL32+AL34+AL35","v":{"$error":"#VALUE!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!AF40","v":50},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y","x"]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"+'Analiza i dimenzioniranje'!E39","v":15},"°    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD7","v":3.4000010999999999},{"$f":"+AE7","v":0.72068965844232813}]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!AF42","v":5},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'C XVI-XVII'!V61*('Analiza i dimenzioniranje'!AI33-'C XVI-XVII'!V59)+B129*(AD39-H129)+B138*(AD39-H138)+B138*(AD39-H138)+'C XVI-XVII'!Z76*('Analiza i dimenzioniranje'!AI33-'C XVI-XVII'!Z77)+S35*(AE39-'C XVI-XVII'!AG66)+B110*(AE39-H110)","v":{"$error":"#VALUE!"}}]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*'C XVI-XVII'!AC118*C42/B42","v":0},"kN/m'"]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'P XV-XV'!C42","v":1}]
[null,null,"DIMENZIJE ZIDA:"]
[]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":{"$error":"#VALUE!"}},"m"]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C XVI-XVII'!B10-'C XVI-XVII'!B11=0,\">100\",IF('C XVI-XVII'!C10-'C XVI-XVII'!C11/(0.00000000000001+'C XVI-XVII'!B11-'C XVI-XVII'!B10)>100,\">100\",('C XVI-XVII'!C10-'C XVI-XVII'!C11)/('C XVI-XVII'!B11-'C XVI-XVII'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C XVI-XVII'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C XVI-XVII'!E64","v":1.4000010999999999},"m"]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 "]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m"]
[" zapreminska težina nasipa ...............................",null,null,"      gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AF44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C XVI-XVII'!I87-'C XVI-XVII'!Q17)-B109*('C XVI-XVII'!K87-'C XVI-XVII'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C XVI-XVII'!Q16-'C XVI-XVII'!N59)+B136*('C XVI-XVII'!Q16-'C XVI-XVII'!M93)+B137*('C XVI-XVII'!Q16-'C XVI-XVII'!C93)+B135*(C135),-B116*C116/1.35-B108*('C XVI-XVII'!I87-'C XVI-XVII'!Q17)-B109*('C XVI-XVII'!K87-'C XVI-XVII'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C XVI-XVII'!Q16-'C XVI-XVII'!M93)+B137*('C XVI-XVII'!Q16-'C XVI-XVII'!C93)+B135*(C135))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+#REF!)","v":{"$error":"#REF!"}},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+'Dijagram momenata'!Q9","v":4.72},null,{"$f":"-#REF!*N66","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":0},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota",null,"krak od presjeka do sile"]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c111",{"$f":"IF(+L66-'Dijagram momenata'!$Q$9>0,+L66-'Dijagram momenata'!$Q$9,0)","v":{"$error":"#REF!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c112",{"$f":"IF(+L67-'Dijagram momenata'!$Q$9>0,+L67-'Dijagram momenata'!$Q$9,0)","v":{"$error":"#REF!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c113",{"$f":"IF(+L68-'Dijagram momenata'!$Q$9>0,+L68-'Dijagram momenata'!$Q$9,0)","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c114",{"$f":"IF(+L69-'Dijagram momenata'!$Q$9>0,+L69-'Dijagram momenata'!$Q$9,0)","v":{"$error":"#REF!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')",null,null,"Ka"]
[" sloj 1. ..........................................",{"$f":"+'C XVI-XVII'!I85","v":{"$error":"#VALUE!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+'C XVI-XVII'!K88","v":{"$error":"#VALUE!"}},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658}]
[" sloj 3. ..............................",{"$f":"+'P III-III'!B99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!C99","v":{"$error":"#VALUE!"}},{"$f":"+'P III-III'!D99","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,null,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I120","v":1},null,null,{"$f":"+'C XVI-XVII'!N87","v":{"$error":"#VALUE!"}}]
[" Eh2 .............................................",{"$f":"+C98","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I121","v":1},null,null,{"$f":"+'C XVI-XVII'!K87","v":{"$error":"#VALUE!"}}]
[" Eh3 .....................................................",{"$f":"+C99","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I122","v":1},null,null,{"$f":"+C110+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPrometno ....................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I124","v":1.3},null,null,{"$f":"+C111+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I125","v":1},null,null,{"$f":"+C112+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPLinijsko ................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"+B113*C113","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I126","v":1}]
[" EQTemelj ....................................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I127","v":1},null,null,{"$f":"+C114+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,null,{"$f":"+'C XVI-XVII'!$AI$44","v":1.5001009999999999},{"$f":"+'C XVI-XVII'!$AH$44","v":4.9000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":-48.296291314453413},{"$f":"IF(H115<'Analiza i dimenzioniranje'!AF44,0,H115-'Analiza i dimenzioniranje'!AF44)","v":0.28000000000000025},{"$f":"+B115*C115","v":-13.522961568046968},{"$f":"+'Analiza i dimenzioniranje'!I129","v":0},null,null,{"$f":"+E40","v":5},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":6.9000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":0},{"$f":"+H116-'Analiza i dimenzioniranje'!AF44","v":-4.72},{"$f":"B116*C116","v":0},{"$f":"+'Analiza i dimenzioniranje'!I150","v":0},"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C XVI-XVII'!AC117","v":0}]
[{"$f":"+A101","v":{"$error":"#VALUE!"}},{"$f":"-B101","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!E116","v":0},null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}},null,null,"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C XVI-XVII'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C XVI-XVII'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},{"$f":"+'Analiza i dimenzioniranje'!I135","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C XVI-XVII'!L61","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVI-XVII'!D59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I136","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C XVI-XVII'!L59","v":{"$error":"#VALUE!"}}]
[" Gnasip na konzoli.............................",{"$f":"IF(M61>=E67+E68,0,'C XVI-XVII'!N61)","v":0},{"$f":"IF(B128=0,0,2+E57-'C XVI-XVII'!J59)","v":0},{"$f":"B128*C128","v":0},{"$f":"+'Analiza i dimenzioniranje'!I138","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C128","v":4.9000021999999994}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C XVI-XVII'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I139","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},{"$f":"+'Analiza i dimenzioniranje'!I140","v":{"$error":"#VALUE!"}},null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C XVI-XVII'!W18<'C XVI-XVII'!B7,0,('C XVI-XVII'!W18-'C XVI-XVII'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C XVI-XVII'!W18+'C XVI-XVII'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I141","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C XVI-XVII'!W23>'C XVI-XVII'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C XVI-XVII'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I142","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C XVI-XVII'!W26>'C XVI-XVII'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C XVI-XVII'!W25)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I143","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C XVI-XVII'!W31>'C XVI-XVII'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVI-XVII'!W33-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I144","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":12.940952255126037},{"$f":"2+E57-'C XVI-XVII'!AB24-E54-'Analiza i dimenzioniranje'!AF49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I145","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVI-XVII'!M93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I146","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVI-XVII'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I147","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVI-XVII'!E93","v":2.9000021999999994},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I148","v":1},null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]

{"sheet":"P XVII-XVII","index":28,"n_rows":140,"n_cols":38,"rows_kept":140,"cut":false,"hidden":true,"merged":[[46,38,46,39],[46,35,46,36],[45,32,46,32],[44,38,45,38],[47,38,48,38],[48,32,49,32],[47,35,48,35],[45,20,46,20],[45,23,46,23],[47,29,47,30],[44,35,45,35],[48,20,49,20],[47,23,47,24],[48,23,49,23],[48,26,49,26],[48,29,49,29],[45,26,46,26],[45,29,46,29],[48,11,49,11],[47,32,47,33],[47,11,47,12],[47,14,47,15],[47,17,47,18],[47,20,47,21],[48,14,49,14],[48,17,49,17],[47,26,47,27],[45,11,46,11],[45,14,46,14],[45,17,46,17],[20,10,20,11],[28,10,28,11],[29,10,29,11],[30,10,30,11],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[16,10,16,11],[7,10,7,11],[8,10,8,11],[9,10,9,11],[10,10,10,11],[11,10,11,11],[12,10,12,11],[64,11,64,12],[7,0,7,9],[13,10,13,11],[14,10,14,11],[15,10,15,11],[18,10,18,11],[19,10,19,11],[34,10,34,11],[21,10,21,11],[22,10,22,11],[23,10,23,11],[24,10,24,11],[25,10,25,11],[26,10,26,11],[27,10,27,11],[33,10,33,11]]}
[{"$f":"+'Analiza i dimenzioniranje'!#REF!","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!#REF!","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!#REF!","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z18/M18","v":{"$error":"#VALUE!"}}]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","milenium","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  ","krak                  y  ","Moment destabilnosti i stabilnosti","za Mzida                                              krakovi                             x                  y",null,"Moment zida II","za M u                           presjeku II-II                                                   krakovi                                x               y",null,"Moment      II-II","za M u                           temelju ispod zida                     krakovi                             x                  y",null,"Moment  ","za M u                           presjeku I-I                                              krakovi                             x                  y",null,"Moment      I-I"]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C XVI-XVII'!C15","v":0.5},null,null,null,{"$f":"2+E57-E54-E51/2","v":3.8000010999999998},{"$f":"+E48","v":1.2},null,{"$f":"2+E55","v":3.4000010999999999},{"$f":"'C XVI-XVII'!AC47+(E48-'C XVI-XVII'!AC47)/2","v":0.72068965844232813},null,{"$f":"2+E55+E51/2","v":3.8000010999999998},{"$f":"'C XVI-XVII'!AC49+(E48-'C XVI-XVII'!AF47)/2","v":0.97931024673015765},null,{"$f":"2+E55+E51","v":4.2000010999999997},{"$f":"'C XVI-XVII'!AC49+(E48-'C XVI-XVII'!AC49)/2","v":0.78965512336507881}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#VALUE!"}},null,null,{"$f":"+H108","v":0},null,{"$f":"+W8-$W$7","v":-0.5},{"$f":"+M8*Y8","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$AB$7","v":-1.2},{"$f":"T8*AB8","v":{"$error":"#VALUE!"}}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,null,{"$f":"+M9","v":{"$error":"#VALUE!"}},null,null,0,null,-0.5,{"$error":"#VALUE!"},null,{"$f":"+W9-$AB$7","v":-1.2},{"$f":"AB9*T9","v":{"$error":"#VALUE!"}}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",0,null,null,null,null,null,{"$f":"+M10","v":0},null,null,null,0,null,-0.5,0,null,null,null,null,{"$f":"+AE7-'C XVI-XVII'!F93","v":{"$error":"#VALUE!"}},{"$f":"+AE10*S10","v":{"$error":"#VALUE!"}}]
[null,null,"GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}},null,null,0,null,-0.5,{"$error":"#REF!"},null,{"$f":"+W11-$AB$7","v":-1.2},{"$f":"AB11*T11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ...................................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":0},null,null,null,null,null,null,{"$f":"+M15","v":0},null,null,0,null,-0.5,{"$f":"-M15*Y15","v":0},null,-1.2,0]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":0},null,null,null,null,null,null,0,null,null,0,null,-0.5,0,null,-1.2,0]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":{"$error":"#VALUE!"}},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-M61)","v":0},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#VALUE!"}},null,null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,{"$f":"+AK7-C117","v":0.78965512336507881},{"$f":"+M17*AK17","v":{"$error":"#VALUE!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S8:S17)","v":0},{"$f":"SUM(T8:T17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U8:U17)","v":0},null,null,"x",null,{"$f":"SUM(Z8:Z17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC8:AC17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF8:AF17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI8:AI17)","v":0},null,null,{"$f":"SUM(AL8:AL17)","v":{"$error":"#VALUE!"}}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C XVI-XVII'!V61+'C XVI-XVII'!X61+'C XVI-XVII'!Z61","v":68.875052249999982},{"$f":"+'C XVI-XVII'!Z61","v":13.306056250595223},{"$f":"+'C XVI-XVII'!V61","v":37.77589163555291},null,{"$f":"+'C XVI-XVII'!X61","v":17.793104363851846},null,null,null,null,{"$f":"+H126","v":3.3485779696489133},null,{"$f":"+$V$7-V19","v":1.5514242303510861},null,{"$f":"+M19*X19","v":106.85442492734707},null,null,null,{"$f":"AD7-'C XVI-XVII'!V59","v":0.72609215808095717},null,{"$f":"+AD19*O19","v":27.428778681090989},{"$f":"+AG7-'C XVI-XVII'!X59","v":1.0335908939774985E-2},null,{"$f":"+'C XVI-XVII'!X61*'Analiza i dimenzioniranje'!AQ13","v":0.14465929289570792},{"$f":"AJ7-'C XVI-XVII'!Z59","v":-0.34074126926177506},null,{"$f":"+'C XVI-XVII'!Z61*'Analiza i dimenzioniranje'!AT13","v":-4.5636103109654318}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M20","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V20","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V20","v":{"$error":"#VALUE!"}},null,{"$f":"+P20*AA20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli............................."," ",0,null,null,{"$f":"+M21","v":0},null,null,null,null,null,4.9000021999999994,null,0,null,0,{"$f":"+$AA$7-V21","v":-1.1000010999999996},null,{"$f":"+P21*AA21","v":0}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza............."," ",0,null,{"$f":"+M22","v":0},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+AD7-V22","v":{"$error":"#VALUE!"}},null,{"$f":"+M22*AD22","v":{"$error":"#VALUE!"}}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0},null,null,null,null,null,null,null,4.5500016499999996,null,0.35000054999999985,null,0,null,null,null,null,null,null,null,null,null,{"$f":"AJ7-(2+E57-E54/2)","v":-0.35000054999999985},null,{"$f":"+AJ23*N23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X24","v":{"$error":"#VALUE!"}},null,{"$f":"+M24*AD24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X25","v":{"$error":"#VALUE!"}},null,{"$f":"+M25*AD25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X26","v":{"$error":"#VALUE!"}},null,{"$f":"+M26*AD26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X27","v":{"$error":"#VALUE!"}},null,{"$f":"+M27*AD27","v":{"$error":"#VALUE!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",0,null,null,{"$f":"+M28","v":0},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V28","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V28","v":{"$error":"#VALUE!"}},null,{"$f":"P28*AA28","v":{"$error":"#VALUE!"}}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M29","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V29","v":{"$error":"#VALUE!"}},null,{"$f":"+P29*AA29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M30","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V30","v":{"$error":"#VALUE!"}},null,{"$f":"+P30*AA30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",0,null,{"$f":"+M31","v":0},null,null,null,null,null,null,2,null,2.9000021999999994,null,0,null,null,null,{"$f":"+$AD$7-'C XVI-XVII'!E93","v":1.4000010999999999},null,{"$f":"+M31*AD31","v":0},{"$f":"+$AD$7-AD31","v":2}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.306056250595223},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":17.793104363851846},null,null,null,null,null,null,null,null,{"$f":"SUM(Z19:Z31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC19:AC31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF19:AF31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI19:AI31)","v":0.14465929289570792},null,null,{"$f":"SUM(AL19:AL31)","v":-4.5636103109654318}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"II-II","sredina","I-I"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C XVI-XVII'!Z76+'C XVI-XVII'!AB76+'C XVI-XVII'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":{"$error":"#VALUE!"}},null,{"$f":"+'C XVI-XVII'!AB76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+'C XVI-XVII'!Z76","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!AB76","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!AD76","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"$AD$7-'C XVI-XVII'!Z77","v":{"$error":"#VALUE!"}},null,{"$f":"+X34*AD34","v":{"$error":"#VALUE!"}},{"$f":"$AG$7-'C XVI-XVII'!AB77","v":{"$error":"#VALUE!"}},null,{"$f":"-Y34*AG34","v":{"$error":"#VALUE!"}},{"$f":"+AJ7-'C XVI-XVII'!AD77","v":{"$error":"#VALUE!"}},null,{"$f":"+Z34*AJ34","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+Z35","v":{"$error":"#VALUE!"}},{"$f":"+X35","v":{"$error":"#VALUE!"}},null,{"$f":"+Y35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M35*E55/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E51/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E54/E57","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AE7-'C XVI-XVII'!AC45","v":{"$error":"#VALUE!"}},{"$f":"-S35*AE35","v":{"$error":"#VALUE!"}},null,{"$f":"+AH7-'C XVI-XVII'!AC48","v":{"$error":"#VALUE!"}},{"$f":"Y35*AH35","v":{"$error":"#VALUE!"}},null,{"$f":"+AK7-'C XVI-XVII'!AC52","v":{"$error":"#VALUE!"}},{"$f":"-Z35*AK35","v":{"$error":"#VALUE!"}}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},{"$f":"R18+R35","v":{"$error":"#VALUE!"}},{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#VALUE!"}},{"$f":"+U18+U35","v":{"$error":"#VALUE!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"SUM(R36:U36)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+AC18+AC32+AC34+AC35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AF18+AF32+AF34+AF35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AI18+AI32+AI34+AI35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AL18+AL32+AL34+AL35","v":{"$error":"#VALUE!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!AG40","v":0},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y","x"]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"+'Analiza i dimenzioniranje'!E39","v":15},"°    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD7","v":3.4000010999999999},{"$f":"+AE7","v":0.72068965844232813}]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!AG42","v":0},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'C XVI-XVII'!V61*('Analiza i dimenzioniranje'!AI33-'C XVI-XVII'!V59)+B129*(AD39-H129)+B138*(AD39-H138)+B138*(AD39-H138)+'C XVI-XVII'!Z76*('Analiza i dimenzioniranje'!AI33-'C XVI-XVII'!Z77)+S35*(AE39-'C XVI-XVII'!AG66)+B110*(AE39-H110)","v":{"$error":"#VALUE!"}}]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*'C XVI-XVII'!AE118*C42/B42","v":0},"kN/m'"]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'P XVI-XVI'!C42","v":1}]
[null,null,"DIMENZIJE ZIDA:"]
[]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":{"$error":"#VALUE!"}},"m"]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C XVI-XVII'!B10-'C XVI-XVII'!B11=0,\">100\",IF('C XVI-XVII'!C10-'C XVI-XVII'!C11/(0.00000000000001+'C XVI-XVII'!B11-'C XVI-XVII'!B10)>100,\">100\",('C XVI-XVII'!C10-'C XVI-XVII'!C11)/('C XVI-XVII'!B11-'C XVI-XVII'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C XVI-XVII'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C XVI-XVII'!E64","v":1.4000010999999999},"m"]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 "]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m"]
[" zapreminska težina nasipa ...............................",null,null,"      gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!AG44","v":5.04}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AG44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C XVI-XVII'!N87-'C XVI-XVII'!P17)-B109*('C XVI-XVII'!P87-'C XVI-XVII'!P17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C XVI-XVII'!P16-'C XVI-XVII'!R59)+B136*('C XVI-XVII'!P16-'C XVI-XVII'!H93)+B137*('C XVI-XVII'!P16-'C XVI-XVII'!C93)+B135*(C135),-B116*C116/1.35-B108*('C XVI-XVII'!N87-'C XVI-XVII'!P17)-B109*('C XVI-XVII'!P87-'C XVI-XVII'!P17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C XVI-XVII'!P16-'C XVI-XVII'!H93)+B137*('C XVI-XVII'!P16-'C XVI-XVII'!C93)+B135*(C135))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+#REF!)","v":{"$error":"#REF!"}},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+'Dijagram momenata'!Q8","v":5.04},null,{"$f":"-#REF!*N66","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":0},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota",null,"krak od presjeka do sile"]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},{"$f":"+C111","v":{"$error":"#REF!"}},{"$f":"IF(+L66-'Dijagram momenata'!$Q$8>0,+L66-'Dijagram momenata'!$Q$8,0)","v":{"$error":"#REF!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},{"$f":"+C112","v":{"$error":"#REF!"}},{"$f":"IF(+L67-'Dijagram momenata'!$Q$8>0,+L67-'Dijagram momenata'!$Q$8,0)","v":{"$error":"#REF!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},{"$f":"+C113","v":{"$error":"#REF!"}},{"$f":"IF(+L68-'Dijagram momenata'!$Q$8>0,+L68-'Dijagram momenata'!$Q$8,0)","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},{"$f":"+C114","v":{"$error":"#REF!"}},{"$f":"IF(+L69-'Dijagram momenata'!$Q$8>0,+L69-'Dijagram momenata'!$Q$8,0)","v":{"$error":"#REF!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+'C XVI-XVII'!N85","v":{"$error":"#VALUE!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+'C XVI-XVII'!P88","v":{"$error":"#VALUE!"}},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658}]
[" sloj 3. ..............................",0,{"$f":"+B99*COS((G18-E47)*PI()/180)","v":0},{"$f":"+B99*SIN((G18-E47)*PI()/180)","v":0},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,null,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I120","v":1}]
[" Eh2 .............................................",{"$f":"+C98","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I121","v":1}]
[" Eh3 .....................................................",{"$f":"+C99","v":0},null,null,{"$f":"+'Analiza i dimenzioniranje'!I122","v":1}]
[" EPrometno ....................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I124","v":1.3}]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I125","v":1}]
[" EPLinijsko ................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"+B113*C113","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I126","v":1}]
[" EQTemelj ....................................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I127","v":1},null,null,null,null,null,{"$f":"+'C XVI-XVII'!$AI$44","v":1.5001009999999999},{"$f":"+'C XVI-XVII'!$AH$44","v":4.9000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":0},{"$f":"IF(H115<'Analiza i dimenzioniranje'!AG44,0,H115-'Analiza i dimenzioniranje'!AG44)","v":0},{"$f":"+B115*C115","v":0},{"$f":"+'Analiza i dimenzioniranje'!I129","v":0},null,null,{"$f":"+E40","v":0},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":6.9000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":0},{"$f":"+H116-'Analiza i dimenzioniranje'!AG44","v":-5.04},{"$f":"B116*C116","v":0},{"$f":"+'Analiza i dimenzioniranje'!I150","v":0},"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C XVI-XVII'!AE117","v":0}]
[{"$f":"+A101","v":{"$error":"#VALUE!"}},{"$f":"-B101","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!E116","v":0},null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}},null,null,"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C XVI-XVII'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C XVI-XVII'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},{"$f":"+'Analiza i dimenzioniranje'!I135","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C XVI-XVII'!P61","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVI-XVII'!P59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I136","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C XVI-XVII'!L59","v":{"$error":"#VALUE!"}}]
[" Gnasip na konzoli.............................",{"$f":"IF(M61>=E67+E68,0,'C XVI-XVII'!R61)","v":0},{"$f":"IF(B128=0,0,2+E57-'C XVI-XVII'!R59)","v":0},{"$f":"B128*C128","v":0},{"$f":"+'Analiza i dimenzioniranje'!I138","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C128","v":4.9000021999999994}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C XVI-XVII'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I139","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},{"$f":"+'Analiza i dimenzioniranje'!I140","v":{"$error":"#VALUE!"}},null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C XVI-XVII'!W18<'C XVI-XVII'!B7,0,('C XVI-XVII'!W18-'C XVI-XVII'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C XVI-XVII'!W18+'C XVI-XVII'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I141","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C XVI-XVII'!W23>'C XVI-XVII'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C XVI-XVII'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I142","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C XVI-XVII'!W26>'C XVI-XVII'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C XVI-XVII'!W25)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I143","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C XVI-XVII'!W31>'C XVI-XVII'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVI-XVII'!W33-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I144","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":0},{"$f":"2+E57-'C XVI-XVII'!AC24-E54-'Analiza i dimenzioniranje'!AG49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I145","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVI-XVII'!H93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I146","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVI-XVII'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I147","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":0},{"$f":"2+E57-'C XVI-XVII'!E93","v":2.9000021999999994},0,{"$f":"+'Analiza i dimenzioniranje'!I148","v":1},null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]

{"sheet":"P XVIII-XVIII","index":29,"n_rows":140,"n_cols":38,"rows_kept":140,"cut":false,"hidden":true,"merged":[[9,10,9,11],[10,10,10,11],[11,10,11,11],[12,10,12,11],[18,10,18,11],[13,10,13,11],[14,10,14,11],[15,10,15,11],[21,10,21,11],[19,10,19,11],[20,10,20,11],[16,10,16,11],[47,32,47,33],[33,10,33,11],[26,10,26,11],[27,10,27,11],[28,10,28,11],[22,10,22,11],[23,10,23,11],[24,10,24,11],[25,10,25,11],[47,29,47,30],[45,20,46,20],[47,23,47,24],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[7,10,7,11],[7,0,7,9],[8,10,8,11],[45,17,46,17],[47,26,47,27],[48,23,49,23],[44,38,45,38],[47,35,48,35],[47,38,48,38],[48,26,49,26],[46,38,46,39],[48,29,49,29],[46,35,46,36],[44,35,45,35],[45,26,46,26],[45,29,46,29],[48,32,49,32],[45,32,46,32],[64,11,64,12],[45,23,46,23],[48,14,49,14],[29,10,29,11],[30,10,30,11],[48,17,49,17],[48,11,49,11],[48,20,49,20],[34,10,34,11],[47,11,47,12],[47,14,47,15],[47,17,47,18],[47,20,47,21],[45,11,46,11],[45,14,46,14]]}
[" UPUTE ZA RAD: - Ispuniti sve podatke u čelijama s plavom bojom. Ispuniti i za izbor armature u kolonama L,N i O",null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z18/M18","v":{"$error":"#VALUE!"}}]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  ","krak                  y  ","Moment destabilnosti i stabilnosti","za Mzida                                              krakovi                             x                  y",null,"Moment zida II","za M u                           presjeku II-II                                                   krakovi                                x               y",null,"Moment      II-II","za M u                           temelju ispod zida                     krakovi                             x                  y",null,"Moment  ","za M u                           presjeku I-I                                              krakovi                             x                  y",null,"Moment      I-I"]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C XVIII-XIX'!C15","v":0.5},null,null,null,{"$f":"2+E57-E54-E51/2","v":3.8000010999999998},{"$f":"+E48","v":1.2},null,{"$f":"2+E55","v":3.4000010999999999},{"$f":"'C XVIII-XIX'!AC47+(E48-'C XVIII-XIX'!AC47)/2","v":0.72068965844232813},null,{"$f":"2+E55+E51/2","v":3.8000010999999998},{"$f":"'C XVIII-XIX'!AC49+(E48-'C XVIII-XIX'!AF47)/2","v":0.97931024673015765},null,{"$f":"2+E55+E51","v":4.2000010999999997},{"$f":"'C XVIII-XIX'!AC49+(E48-'C XVIII-XIX'!AC49)/2","v":0.78965512336507881}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#VALUE!"}},null,null,{"$f":"+H108","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$W$7","v":{"$error":"#VALUE!"}},{"$f":"+M8*Y8","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$AB$7","v":{"$error":"#VALUE!"}},{"$f":"T8*AB8","v":{"$error":"#VALUE!"}}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",0,null,null,null,null,null,null,{"$f":"+M9","v":0},null,null,0,null,-0.5,0,null,{"$f":"+W9-$AB$7","v":-1.2},{"$f":"AB9*T9","v":0}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",0,null,null,null,null,null,{"$f":"+M10","v":0},null,null,null,1.2,null,0.7,0,null,null,null,null,{"$f":"+AE7-'C XVIII-XIX'!F93","v":{"$error":"#VALUE!"}},{"$f":"+AE10*S10","v":{"$error":"#VALUE!"}}]
[null,null,"GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$f":"+W11-$AB$7","v":{"$error":"#REF!"}},{"$f":"AB11*T11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ...................................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":0},null,null,null,null,null,null,{"$f":"+E38","v":0},null,null,0,null,-0.5,{"$f":"-M15*Y15","v":0},null,-1.2,0]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":0},null,null,null,null,null,null,0,null,null,0,null,-0.5,0,null,-1.2,0]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":{"$error":"#VALUE!"}},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-M61)","v":0},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#VALUE!"}},null,null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,{"$f":"+AK7-C117","v":0.78965512336507881},{"$f":"+M17*AK17","v":{"$error":"#VALUE!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S8:S17)","v":0},{"$f":"SUM(T8:T17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U8:U17)","v":0},null,null,"x",null,{"$f":"SUM(Z8:Z17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC8:AC17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF8:AF17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI8:AI17)","v":0},null,null,{"$f":"SUM(AL8:AL17)","v":{"$error":"#VALUE!"}}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C XVIII-XIX'!V61+'C XVIII-XIX'!X61+'C XVIII-XIX'!Z61","v":68.875052249999982},{"$f":"+'C XVIII-XIX'!Z61","v":13.306056250595223},{"$f":"+'C XVIII-XIX'!V61","v":37.77589163555291},null,{"$f":"+'C XVIII-XIX'!X61","v":17.793104363851846},null,null,null,null,{"$f":"+H126","v":3.3485779696489133},null,{"$f":"+$V$7-V19","v":1.5514242303510861},null,{"$f":"+M19*X19","v":106.85442492734707},null,null,null,{"$f":"AD7-'C XVIII-XIX'!V59","v":0.72609215808095717},null,{"$f":"+AD19*O19","v":27.428778681090989},{"$f":"+AG7-'C XVIII-XIX'!X59","v":1.0335908939774985E-2},null,{"$f":"+'C XVIII-XIX'!X61*'Analiza i dimenzioniranje'!AQ13","v":0.14465929289570792},{"$f":"AJ7-'C XVIII-XIX'!Z59","v":-0.34074126926177506},null,{"$f":"+'C XVIII-XIX'!Z61*'Analiza i dimenzioniranje'!AT13","v":-4.5636103109654318}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M20","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V20","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V20","v":{"$error":"#VALUE!"}},null,{"$f":"+P20*AA20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli............................."," ",0,null,null,{"$f":"+M21","v":0},null,null,null,null,null,4.9000021999999994,null,0,null,0,{"$f":"+$AA$7-V21","v":-1.1000010999999996},null,{"$f":"+P21*AA21","v":0}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza............."," ",0,null,{"$f":"+M22","v":0},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+AD7-V22","v":{"$error":"#VALUE!"}},null,{"$f":"+M22*AD22","v":{"$error":"#VALUE!"}}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0},null,null,null,null,null,null,null,4.5500016499999996,null,0.35000054999999985,null,0,null,null,null,null,null,null,null,null,null,{"$f":"AJ7-(2+E57-E54/2)","v":-0.35000054999999985},null,{"$f":"+AJ23*N23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X24","v":{"$error":"#VALUE!"}},null,{"$f":"+M24*AD24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X25","v":{"$error":"#VALUE!"}},null,{"$f":"+M25*AD25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X26","v":{"$error":"#VALUE!"}},null,{"$f":"+M26*AD26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X27","v":{"$error":"#VALUE!"}},null,{"$f":"+M27*AD27","v":{"$error":"#VALUE!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",0,null,null,{"$f":"+M28","v":0},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V28","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V28","v":{"$error":"#VALUE!"}},null,{"$f":"P28*AA28","v":{"$error":"#VALUE!"}}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M29","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V29","v":{"$error":"#VALUE!"}},null,{"$f":"+P29*AA29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",0,null,null,{"$f":"+M30","v":0},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V30","v":{"$error":"#VALUE!"}},null,{"$f":"+P30*AA30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",0,null,{"$f":"+M31","v":0},null,null,null,null,null,null,2,null,2.9000021999999994,null,0,null,null,null,{"$f":"+$AD$7-'C XVIII-XIX'!E93","v":1.4000010999999999},null,{"$f":"+M31*AD31","v":0},{"$f":"+$AD$7-AD31","v":2}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.306056250595223},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":17.793104363851846},null,null,null,null,null,null,null,null,{"$f":"SUM(Z19:Z31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC19:AC31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF19:AF31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI19:AI31)","v":0.14465929289570792},null,null,{"$f":"SUM(AL19:AL31)","v":-4.5636103109654318}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"II-II","sredina","I-I"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C XVIII-XIX'!Z76+'C XVIII-XIX'!AB76+'C XVIII-XIX'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+'C XVIII-XIX'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":{"$error":"#VALUE!"}},null,{"$f":"+'C XVIII-XIX'!AB76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+'C XVIII-XIX'!Z76","v":{"$error":"#VALUE!"}},{"$f":"+'C XVIII-XIX'!AB76","v":{"$error":"#VALUE!"}},{"$f":"+'C XVIII-XIX'!AD76","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"$AD$7-'C XVIII-XIX'!Z77","v":{"$error":"#VALUE!"}},null,{"$f":"+X34*AD34","v":{"$error":"#VALUE!"}},{"$f":"$AG$7-'C XVIII-XIX'!AB77","v":{"$error":"#VALUE!"}},null,{"$f":"-Y34*AG34","v":{"$error":"#VALUE!"}},{"$f":"+AJ7-'C XVIII-XIX'!AD77","v":{"$error":"#VALUE!"}},null,{"$f":"+Z34*AJ34","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+Z35","v":{"$error":"#VALUE!"}},{"$f":"+X35","v":{"$error":"#VALUE!"}},null,{"$f":"+Y35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M35*E55/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E51/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E54/E57","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AE7-'C XVIII-XIX'!AC45","v":{"$error":"#VALUE!"}},{"$f":"-S35*AE35","v":{"$error":"#VALUE!"}},null,{"$f":"+AH7-'C XVIII-XIX'!AC48","v":{"$error":"#VALUE!"}},{"$f":"Y35*AH35","v":{"$error":"#VALUE!"}},null,{"$f":"+AK7-'C XVIII-XIX'!AC52","v":{"$error":"#VALUE!"}},{"$f":"-Z35*AK35","v":{"$error":"#VALUE!"}}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},{"$f":"R18+R35","v":{"$error":"#VALUE!"}},{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#VALUE!"}},{"$f":"+U18+U35","v":{"$error":"#VALUE!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"SUM(R36:U36)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+AC18+AC32+AC34+AC35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AF18+AF32+AF34+AF35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AI18+AI32+AI34+AI35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AL18+AL32+AL34+AL35","v":{"$error":"#VALUE!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!AH40","v":0},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y","x"]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"+'Analiza i dimenzioniranje'!E39","v":15},"°    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD7","v":3.4000010999999999},{"$f":"+AE7","v":0.72068965844232813}]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!AH42","v":0},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'C XVIII-XIX'!V61*('Analiza i dimenzioniranje'!AI33-'C XVIII-XIX'!V59)+B129*(AD39-H129)+B138*(AD39-H138)+B138*(AD39-H138)+'C XVIII-XIX'!Z76*('Analiza i dimenzioniranje'!AI33-'C XVIII-XIX'!Z77)+S35*(AE39-'C XVIII-XIX'!AG66)+B110*(AE39-H110)","v":{"$error":"#VALUE!"}}]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*'C XVIII-XIX'!AC118*C42/B42","v":0},"kN/m'"]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'P XVII-XVII'!C42","v":1}]
[null,null,"DIMENZIJE ZIDA:"]
[]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":{"$error":"#VALUE!"}},"m"]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C XVIII-XIX'!B10-'C XVIII-XIX'!B11=0,\">100\",IF('C XVIII-XIX'!C10-'C XVIII-XIX'!C11/(0.00000000000001+'C XVIII-XIX'!B11-'C XVIII-XIX'!B10)>100,\">100\",('C XVIII-XIX'!C10-'C XVIII-XIX'!C11)/('C XVIII-XIX'!B11-'C XVIII-XIX'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C XVIII-XIX'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C XVIII-XIX'!E64","v":1.4000010999999999},"m"]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 "]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m"]
[" zapreminska težina nasipa ...............................",null,null,"      gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!AH44","v":5.36}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AH44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C XVIII-XIX'!I87-'C XVIII-XIX'!Q17)-B109*('C XVIII-XIX'!K87-'C XVIII-XIX'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C XVIII-XIX'!Q16-'C XVIII-XIX'!N59)+B136*('C XVIII-XIX'!Q16-'C XVIII-XIX'!M93)+B137*('C XVIII-XIX'!Q16-'C XVIII-XIX'!C93)+B135*(C135),-B116*C116/1.35-B108*('C XVIII-XIX'!I87-'C XVIII-XIX'!Q17)-B109*('C XVIII-XIX'!K87-'C XVIII-XIX'!Q17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C XVIII-XIX'!Q16-'C XVIII-XIX'!M93)+B137*('C XVIII-XIX'!Q16-'C XVIII-XIX'!C93)+B135*(C135))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+#REF!)","v":{"$error":"#REF!"}},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+'Dijagram momenata'!Q7","v":5.36},null,{"$f":"-#REF!*N66","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":0},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota",null,"krak od presjeka do sile"]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},{"$f":"+C111","v":{"$error":"#REF!"}},{"$f":"IF(+L66-'Dijagram momenata'!$Q$7>0,+L66-'Dijagram momenata'!$Q$7,0)","v":{"$error":"#REF!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},{"$f":"+C112","v":{"$error":"#REF!"}},{"$f":"IF(+L67-'Dijagram momenata'!$Q$7>0,+L67-'Dijagram momenata'!$Q$7,0)","v":{"$error":"#REF!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},{"$f":"+C113","v":{"$error":"#REF!"}},{"$f":"IF(+L68-'Dijagram momenata'!$Q$7>0,+L68-'Dijagram momenata'!$Q$7,0)","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},{"$f":"+C114","v":{"$error":"#REF!"}},{"$f":"IF(+L69-'Dijagram momenata'!$Q$7>0,+L69-'Dijagram momenata'!$Q$7,0)","v":{"$error":"#REF!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+'C XVIII-XIX'!I85","v":{"$error":"#VALUE!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+'C XVIII-XIX'!K88","v":0},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":0},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":0},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658}]
[" sloj 3. ..............................",0,{"$f":"+B99*COS((G18-E47)*PI()/180)","v":0},{"$f":"+B99*SIN((G18-E47)*PI()/180)","v":0},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,null,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I120","v":1},null,null,{"$f":"+'C XVIII-XIX'!N87","v":{"$error":"#VALUE!"}}]
[" Eh2 .............................................",{"$f":"+C98","v":0},null,null,{"$f":"+'Analiza i dimenzioniranje'!I121","v":1},null,null,{"$f":"+'C XVIII-XIX'!K87","v":0}]
[" Eh3 .....................................................",{"$f":"+C99","v":0},null,null,{"$f":"+'Analiza i dimenzioniranje'!I122","v":1},null,null,{"$f":"+C110+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPrometno ....................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I124","v":1.3},null,null,{"$f":"+C111+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I125","v":1},null,null,{"$f":"+C112+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPLinijsko ................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"+B113*C113","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I126","v":1}]
[" EQTemelj ....................................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I127","v":1},null,null,{"$f":"+C114+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,null,{"$f":"+'C XVIII-XIX'!$AI$44","v":1.5001009999999999},{"$f":"+'C XVIII-XIX'!$AH$44","v":4.9000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":0},{"$f":"IF(H115<'Analiza i dimenzioniranje'!AH44,0,H115-'Analiza i dimenzioniranje'!AH44)","v":0},{"$f":"+B115*C115","v":0},{"$f":"+'Analiza i dimenzioniranje'!I129","v":0},null,null,{"$f":"+E40","v":0},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":6.9000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":0},{"$f":"+H116-'Analiza i dimenzioniranje'!AH44","v":-5.36},{"$f":"B116*C116","v":0},{"$f":"+'Analiza i dimenzioniranje'!I150","v":0},"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C XVIII-XIX'!AC117","v":0}]
[{"$f":"+A101","v":{"$error":"#VALUE!"}},{"$f":"-B101","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!E116","v":0},null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}},null,null,"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C XVIII-XIX'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C XVIII-XIX'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},{"$f":"+'Analiza i dimenzioniranje'!I135","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C XVIII-XIX'!L61","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVIII-XIX'!L59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I136","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C XVIII-XIX'!L59","v":{"$error":"#VALUE!"}}]
[" Gnasip na konzoli.............................",{"$f":"IF(M61>=E67+E68,0,'C XVIII-XIX'!N61)","v":0},{"$f":"IF(B128=0,0,2+E57-'C XVIII-XIX'!N59)","v":0},{"$f":"B128*C128","v":0},{"$f":"+'Analiza i dimenzioniranje'!I138","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C128","v":4.9000021999999994}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C XVIII-XIX'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I139","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},{"$f":"+'Analiza i dimenzioniranje'!I140","v":{"$error":"#VALUE!"}},null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C XVIII-XIX'!W18<'C XVIII-XIX'!B7,0,('C XVIII-XIX'!W18-'C XVIII-XIX'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C XVIII-XIX'!W18+'C XVIII-XIX'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I141","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C XVIII-XIX'!W23>'C XVIII-XIX'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C XVIII-XIX'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I142","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C XVIII-XIX'!W26>'C XVIII-XIX'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C XVIII-XIX'!W25)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I143","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C XVIII-XIX'!W31>'C XVIII-XIX'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVIII-XIX'!W33-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I144","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":0},{"$f":"2+E57-'C XVIII-XIX'!AB24-E54-'Analiza i dimenzioniranje'!AH49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I145","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVIII-XIX'!M93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I146","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":0},{"$f":"2+E57-'C XVIII-XIX'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I147","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":0},{"$f":"2+E57-'C XVIII-XIX'!E93","v":2.9000021999999994},0,{"$f":"+'Analiza i dimenzioniranje'!I148","v":1},null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]

{"sheet":"P XIX-XIX","index":30,"n_rows":140,"n_cols":38,"rows_kept":140,"cut":false,"hidden":true,"merged":[[9,10,9,11],[10,10,10,11],[11,10,11,11],[12,10,12,11],[18,10,18,11],[13,10,13,11],[14,10,14,11],[15,10,15,11],[21,10,21,11],[19,10,19,11],[20,10,20,11],[16,10,16,11],[47,32,47,33],[33,10,33,11],[26,10,26,11],[27,10,27,11],[28,10,28,11],[22,10,22,11],[23,10,23,11],[24,10,24,11],[25,10,25,11],[47,29,47,30],[45,20,46,20],[47,23,47,24],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[7,10,7,11],[7,0,7,9],[8,10,8,11],[45,17,46,17],[47,26,47,27],[48,23,49,23],[44,38,45,38],[47,35,48,35],[47,38,48,38],[48,26,49,26],[46,38,46,39],[48,29,49,29],[46,35,46,36],[44,35,45,35],[45,26,46,26],[45,29,46,29],[48,32,49,32],[45,32,46,32],[64,11,64,12],[45,23,46,23],[48,14,49,14],[29,10,29,11],[30,10,30,11],[48,17,49,17],[48,11,49,11],[48,20,49,20],[34,10,34,11],[47,11,47,12],[47,14,47,15],[47,17,47,18],[47,20,47,21],[45,11,46,11],[45,14,46,14]]}
[" UPUTE ZA RAD: - Ispuniti sve podatke u čelijama s plavom bojom. Ispuniti i za izbor armature u kolonama L,N i O",null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z18/M18","v":{"$error":"#VALUE!"}}]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  ","krak                  y  ","Moment destabilnosti i stabilnosti","za Mzida                                              krakovi                             x                  y",null,"Moment zida II","za M u                           presjeku II-II                                                   krakovi                                x               y",null,"Moment      II-II","za M u                           temelju ispod zida                     krakovi                             x                  y",null,"Moment  ","za M u                           presjeku I-I                                              krakovi                             x                  y",null,"Moment      I-I"]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+'C XVIII-XIX'!C15","v":0.5},null,null,null,{"$f":"2+E57-E54-E51/2","v":3.8000010999999998},{"$f":"+E48","v":1.2},null,{"$f":"2+E55","v":3.4000010999999999},{"$f":"'C XVIII-XIX'!AC47+(E48-'C XVIII-XIX'!AC47)/2","v":0.72068965844232813},null,{"$f":"2+E55+E51/2","v":3.8000010999999998},{"$f":"'C XVIII-XIX'!AC49+(E48-'C XVIII-XIX'!AF47)/2","v":0.97931024673015765},null,{"$f":"2+E55+E51","v":4.2000010999999997},{"$f":"'C XVIII-XIX'!AC49+(E48-'C XVIII-XIX'!AC49)/2","v":0.78965512336507881}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#VALUE!"}},null,null,{"$f":"+H108","v":0},null,{"$f":"+W8-$W$7","v":-0.5},{"$f":"+M8*Y8","v":{"$error":"#VALUE!"}},null,{"$f":"+W8-$AB$7","v":-1.2},{"$f":"T8*AB8","v":{"$error":"#VALUE!"}}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",{"$error":"#VALUE!"},null,null,null,null,null,null,{"$f":"+M9","v":{"$error":"#VALUE!"}},null,null,0,null,-0.5,{"$error":"#VALUE!"},null,{"$f":"+W9-$AB$7","v":-1.2},{"$f":"AB9*T9","v":{"$error":"#VALUE!"}}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",0,null,null,null,null,null,{"$f":"+M10","v":0},null,null,null,0,null,-0.5,0,null,null,null,null,{"$f":"+AE7-'C XVIII-XIX'!F93","v":{"$error":"#VALUE!"}},{"$f":"+AE10*S10","v":{"$error":"#VALUE!"}}]
[null,null,"GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}},null,null,0,null,-0.5,{"$error":"#REF!"},null,{"$f":"+W11-$AB$7","v":-1.2},{"$f":"AB11*T11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ...................................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,-0.5,{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":0},null,null,null,null,null,null,{"$f":"+E38","v":0},null,null,0,null,-0.5,{"$f":"-M15*Y15","v":0},null,-1.2,0]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":0},null,null,null,null,null,null,0,null,null,0,null,-0.5,0,null,-1.2,0]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":{"$error":"#VALUE!"}},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-M61)","v":0},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)"," Ep..............................................."," ",{"$f":"+B117","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-M17","v":{"$error":"#VALUE!"}},null,null,null,null,1.2,null,0.7,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,{"$f":"+AK7-C117","v":0.78965512336507881},{"$f":"+M17*AK17","v":{"$error":"#VALUE!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(S8:S17)","v":0},{"$f":"SUM(T8:T17)","v":{"$error":"#VALUE!"}},{"$f":"SUM(U8:U17)","v":0},null,null,"x",null,{"$f":"SUM(Z8:Z17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC8:AC17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF8:AF17)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI8:AI17)","v":0},null,null,{"$f":"SUM(AL8:AL17)","v":{"$error":"#VALUE!"}}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+'C XVIII-XIX'!V61+'C XVIII-XIX'!X61+'C XVIII-XIX'!Z61","v":68.875052249999982},{"$f":"+'C XVIII-XIX'!Z61","v":13.306056250595223},{"$f":"+'C XVIII-XIX'!V61","v":37.77589163555291},null,{"$f":"+'C XVIII-XIX'!X61","v":17.793104363851846},null,null,null,null,{"$f":"+H126","v":3.3485779696489133},null,{"$f":"+$V$7-V19","v":1.5514242303510861},null,{"$f":"+M19*X19","v":106.85442492734707},null,null,null,{"$f":"AD7-'C XVIII-XIX'!V59","v":0.72609215808095717},null,{"$f":"+AD19*O19","v":27.428778681090989},{"$f":"+AG7-'C XVIII-XIX'!X59","v":1.0335908939774985E-2},null,{"$f":"+'C XVIII-XIX'!X61*'Analiza i dimenzioniranje'!AQ13","v":0.14465929289570792},{"$f":"AJ7-'C XVIII-XIX'!Z59","v":-0.34074126926177506},null,{"$f":"+'C XVIII-XIX'!Z61*'Analiza i dimenzioniranje'!AT13","v":-4.5636103109654318}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},"(°)"," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M20","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V20","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V20","v":{"$error":"#VALUE!"}},null,{"$f":"+P20*AA20","v":{"$error":"#VALUE!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli............................."," ",0,null,null,{"$f":"+M21","v":0},null,null,null,null,null,4.9000021999999994,null,0,null,0,{"$f":"+$AA$7-V21","v":-1.1000010999999996},null,{"$f":"+P21*AA21","v":0}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza............."," ",0,null,{"$f":"+M22","v":0},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+AD7-V22","v":{"$error":"#VALUE!"}},null,{"$f":"+M22*AD22","v":{"$error":"#VALUE!"}}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0},null,null,null,null,null,null,null,4.5500016499999996,null,0.35000054999999985,null,0,null,null,null,null,null,null,null,null,null,{"$f":"AJ7-(2+E57-E54/2)","v":-0.35000054999999985},null,{"$f":"+AJ23*N23","v":0}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#VALUE!"},null,{"$f":"+M24","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X24","v":{"$error":"#VALUE!"}},null,{"$f":"+M24*AD24","v":{"$error":"#VALUE!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#VALUE!"},null,{"$f":"+M25","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X25","v":{"$error":"#VALUE!"}},null,{"$f":"+M25*AD25","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#VALUE!"},null,{"$f":"+M26","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X26","v":{"$error":"#VALUE!"}},null,{"$f":"+M26*AD26","v":{"$error":"#VALUE!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#VALUE!"},null,{"$f":"+M27","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,null,null,{"$f":"+$AD$7-X27","v":{"$error":"#VALUE!"}},null,{"$f":"+M27*AD27","v":{"$error":"#VALUE!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",0,null,null,{"$f":"+M28","v":0},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+$V$7-V28","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V28","v":{"$error":"#VALUE!"}},null,{"$f":"P28*AA28","v":{"$error":"#VALUE!"}}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M29","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V29","v":{"$error":"#VALUE!"}},null,{"$f":"+P29*AA29","v":{"$error":"#VALUE!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",{"$error":"#VALUE!"},null,null,{"$f":"+M30","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+$AA$7-V30","v":{"$error":"#VALUE!"}},null,{"$f":"+P30*AA30","v":{"$error":"#VALUE!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",0,null,{"$f":"+M31","v":0},null,null,null,null,null,null,2,null,2.9000021999999994,null,0,null,null,null,{"$f":"+$AD$7-'C XVIII-XIX'!E93","v":1.4000010999999999},null,{"$f":"+M31*AD31","v":0},{"$f":"+$AD$7-AD31","v":2}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(N19:N31)","v":13.306056250595223},{"$f":"SUM(O19:O31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#VALUE!"}},{"$f":"SUM(Q19:Q31)","v":17.793104363851846},null,null,null,null,null,null,null,null,{"$f":"SUM(Z19:Z31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AC19:AC31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AF19:AF31)","v":{"$error":"#VALUE!"}},null,null,{"$f":"SUM(AI19:AI31)","v":0.14465929289570792},null,null,{"$f":"SUM(AL19:AL31)","v":-4.5636103109654318}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"II-II","sredina","I-I"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+'C XVIII-XIX'!Z76+'C XVIII-XIX'!AB76+'C XVIII-XIX'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+'C XVIII-XIX'!AD76","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":{"$error":"#VALUE!"}},null,{"$f":"+'C XVIII-XIX'!AB76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+'C XVIII-XIX'!Z76","v":{"$error":"#VALUE!"}},{"$f":"+'C XVIII-XIX'!AB76","v":{"$error":"#VALUE!"}},{"$f":"+'C XVIII-XIX'!AD76","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"$AD$7-'C XVIII-XIX'!Z77","v":{"$error":"#VALUE!"}},null,{"$f":"+X34*AD34","v":{"$error":"#VALUE!"}},{"$f":"$AG$7-'C XVIII-XIX'!AB77","v":{"$error":"#VALUE!"}},null,{"$f":"-Y34*AG34","v":{"$error":"#VALUE!"}},{"$f":"+AJ7-'C XVIII-XIX'!AD77","v":{"$error":"#VALUE!"}},null,{"$f":"+Z34*AJ34","v":{"$error":"#VALUE!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+Z35","v":{"$error":"#VALUE!"}},{"$f":"+X35","v":{"$error":"#VALUE!"}},null,{"$f":"+Y35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+M35*E55/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E51/E57","v":{"$error":"#VALUE!"}},{"$f":"+M35*E54/E57","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AE7-'C XVIII-XIX'!AC45","v":{"$error":"#VALUE!"}},{"$f":"-S35*AE35","v":{"$error":"#VALUE!"}},null,{"$f":"+AH7-'C XVIII-XIX'!AC48","v":{"$error":"#VALUE!"}},{"$f":"Y35*AH35","v":{"$error":"#VALUE!"}},null,{"$f":"+AK7-'C XVIII-XIX'!AC52","v":{"$error":"#VALUE!"}},{"$f":"-Z35*AK35","v":{"$error":"#VALUE!"}}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#VALUE!"}},{"$f":"+O32+O34","v":{"$error":"#VALUE!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#VALUE!"}},{"$f":"+Q32+Q34","v":{"$error":"#VALUE!"}},{"$f":"R18+R35","v":{"$error":"#VALUE!"}},{"$f":"S18+S35","v":{"$error":"#VALUE!"}},{"$f":"T18+T34+T35","v":{"$error":"#VALUE!"}},{"$f":"+U18+U35","v":{"$error":"#VALUE!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"SUM(R36:U36)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+AC18+AC32+AC34+AC35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AF18+AF32+AF34+AF35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AI18+AI32+AI34+AI35","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AL18+AL32+AL34+AL35","v":{"$error":"#VALUE!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!AI40","v":0},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y","x"]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"+'Analiza i dimenzioniranje'!E39","v":15},"°    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD7","v":3.4000010999999999},{"$f":"+AE7","v":0.72068965844232813}]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!AI42","v":0},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'C XVIII-XIX'!V61*('Analiza i dimenzioniranje'!AI33-'C XVIII-XIX'!V59)+B129*(AD39-H129)+B138*(AD39-H138)+B138*(AD39-H138)+'C XVIII-XIX'!Z76*('Analiza i dimenzioniranje'!AI33-'C XVIII-XIX'!Z77)+S35*(AE39-'C XVIII-XIX'!AG66)+B110*(AE39-H110)","v":{"$error":"#VALUE!"}}]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*'C XVIII-XIX'!AE118*C42/B42","v":0},"kN/m'"]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'P XVIII-XVIII'!C42","v":1}]
[null,null,"DIMENZIJE ZIDA:"]
[]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":{"$error":"#VALUE!"}},"m"]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF('C XVIII-XIX'!B10-'C XVIII-XIX'!B11=0,\">100\",IF('C XVIII-XIX'!C10-'C XVIII-XIX'!C11/(0.00000000000001+'C XVIII-XIX'!B11-'C XVIII-XIX'!B10)>100,\">100\",('C XVIII-XIX'!C10-'C XVIII-XIX'!C11)/('C XVIII-XIX'!B11-'C XVIII-XIX'!B10)))","v":{"$error":"#VALUE!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/('C XVIII-XIX'!C15))","v":5.8000043999999988}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":0.70000109999999949},"m",{"$f":"+E55+0.000000001","v":1.400001101},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+'C XVIII-XIX'!E64","v":1.4000010999999999},"m"]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":1.400001101}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 "]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m"]
[" zapreminska težina nasipa ...............................",null,null,"      gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!AI44","v":5.6800000000000006}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#VALUE!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AI44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*('C XVIII-XIX'!N87-'C XVIII-XIX'!P17)-B109*('C XVIII-XIX'!P87-'C XVIII-XIX'!P17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B128*('C XVIII-XIX'!P16-'C XVIII-XIX'!R59)+B136*('C XVIII-XIX'!P16-'C XVIII-XIX'!H93)+B137*('C XVIII-XIX'!P16-'C XVIII-XIX'!C93)+B135*(C135),-B116*C116/1.35-B108*('C XVIII-XIX'!N87-'C XVIII-XIX'!P17)-B109*('C XVIII-XIX'!P87-'C XVIII-XIX'!P17)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B136*('C XVIII-XIX'!P16-'C XVIII-XIX'!H93)+B137*('C XVIII-XIX'!P16-'C XVIII-XIX'!C93)+B135*(C135))","v":{"$error":"#VALUE!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+#REF!)","v":{"$error":"#REF!"}},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+'Dijagram momenata'!Q6","v":5.6800000000000006},null,{"$f":"-#REF!*N66","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":0},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota",null,"krak od presjeka do sile"]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c111",{"$f":"IF(+L66-'Dijagram momenata'!$Q$6>0,+L66-'Dijagram momenata'!$Q$6,0)","v":{"$error":"#REF!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c112",{"$f":"IF(+L67-'Dijagram momenata'!$Q$6>0,+L67-'Dijagram momenata'!$Q$6,0)","v":{"$error":"#REF!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c113",{"$f":"IF(+L68-'Dijagram momenata'!$Q$6>0,+L68-'Dijagram momenata'!$Q$6,0)","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c114",{"$f":"IF(+L69-'Dijagram momenata'!$Q$6>0,+L69-'Dijagram momenata'!$Q$6,0)","v":{"$error":"#REF!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+'C XVIII-XIX'!N85","v":{"$error":"#VALUE!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+'C XVIII-XIX'!P88","v":{"$error":"#VALUE!"}},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658}]
[" sloj 3. ..............................",0,{"$f":"+B99*COS((G18-E47)*PI()/180)","v":0},{"$f":"+B99*SIN((G18-E47)*PI()/180)","v":0},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#VALUE!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":1.40000110101}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#VALUE!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,null,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I120","v":1}]
[" Eh2 .............................................",{"$f":"+C98","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I121","v":1}]
[" Eh3 .....................................................",{"$f":"+C99","v":0},null,null,{"$f":"+'Analiza i dimenzioniranje'!I122","v":1}]
[" EPrometno ....................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I124","v":1.3}]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I125","v":1}]
[" EPLinijsko ................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"+B113*C113","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I126","v":1}]
[" EQTemelj ....................................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I127","v":1},null,null,null,null,null,{"$f":"+'C XVIII-XIX'!$AI$44","v":1.5001009999999999},{"$f":"+'C XVIII-XIX'!$AH$44","v":4.9000021999999994}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":0},{"$f":"IF(H115<'Analiza i dimenzioniranje'!AI44,0,H115-'Analiza i dimenzioniranje'!AI44)","v":0},{"$f":"+B115*C115","v":0},{"$f":"+'Analiza i dimenzioniranje'!I129","v":0},null,null,{"$f":"+E40","v":0},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":1.14744703858307},{"$f":"+L114+2","v":6.9000021999999994}]
[" HPotres .........................................",{"$f":"+E41","v":0},{"$f":"+H116-'Analiza i dimenzioniranje'!AI44","v":-5.6800000000000006},{"$f":"B116*C116","v":0},{"$f":"+'Analiza i dimenzioniranje'!I150","v":0},"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+'C XVIII-XIX'!AE117","v":0}]
[{"$f":"+A101","v":{"$error":"#VALUE!"}},{"$f":"-B101","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!E116","v":0},null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#VALUE!"}},null,null,"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#VALUE!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+'C XVIII-XIX'!$AA$1","v":0}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-'C XVIII-XIX'!B59","v":1.5514242303510861},{"$f":"B126*C126","v":0},{"$f":"+'Analiza i dimenzioniranje'!I135","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C126","v":3.3485779696489133}]
[" Gzid+konz ....................................",{"$f":"+'C XVIII-XIX'!P61","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVIII-XIX'!P59","v":{"$error":"#VALUE!"}},{"$f":"B127*C127","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I136","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C XVIII-XIX'!L59","v":{"$error":"#VALUE!"}}]
[" Gnasip na konzoli.............................",{"$f":"IF(M61>=E67+E68,0,'C XVIII-XIX'!R61)","v":0},{"$f":"IF(B128=0,0,2+E57-'C XVIII-XIX'!R59)","v":0},{"$f":"B128*C128","v":0},{"$f":"+'Analiza i dimenzioniranje'!I138","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C128","v":4.9000021999999994}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-'C XVIII-XIX'!F59","v":{"$error":"#VALUE!"}},{"$f":"B129*C129","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I139","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":0.35000054999999974},{"$f":"B130*C130","v":0},{"$f":"+'Analiza i dimenzioniranje'!I140","v":{"$error":"#VALUE!"}},null,null,4.5500016499999996]
[" PPrometno .......................",{"$f":"+IF('C XVIII-XIX'!W18<'C XVIII-XIX'!B7,0,('C XVIII-XIX'!W18-'C XVIII-XIX'!B7)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#VALUE!"}},{"$f":"IF(B131=0,0,2+E57-('C XVIII-XIX'!W18+'C XVIII-XIX'!H8)/2)","v":{"$error":"#VALUE!"}},{"$f":"B131*C131","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I141","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PTočkasto ......................",{"$f":"IF('C XVIII-XIX'!W23>'C XVIII-XIX'!E21,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B132=0,0,2+E57-'C XVIII-XIX'!W23)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I142","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" PLinijsko .........................",{"$f":"IF('C XVIII-XIX'!W26>'C XVIII-XIX'!E21,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#VALUE!"}},{"$f":"IF(B133=0,0,2+E57-'C XVIII-XIX'!W25)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I143","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" QTemelj ..............................",{"$f":"IF('C XVIII-XIX'!W31>'C XVIII-XIX'!E21,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVIII-XIX'!W33-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I144","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":0},{"$f":"2+E57-'C XVIII-XIX'!AC24-E54-'Analiza i dimenzioniranje'!AI49/200","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I145","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVIII-XIX'!H93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I146","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev2  ..........................",{"$f":"+D98","v":{"$error":"#VALUE!"}},{"$f":"2+E57-'C XVIII-XIX'!C93","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!I147","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":0},{"$f":"2+E57-'C XVIII-XIX'!E93","v":2.9000021999999994},0,{"$f":"+'Analiza i dimenzioniranje'!I148","v":1},null,null,2]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#VALUE!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#VALUE!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#VALUE!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#VALUE!"}},{"$f":"D139/B139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]

{"sheet":"P XX-XX","index":31,"n_rows":140,"n_cols":38,"rows_kept":140,"cut":false,"hidden":true,"merged":[[9,10,9,11],[10,10,10,11],[11,10,11,11],[12,10,12,11],[18,10,18,11],[13,10,13,11],[14,10,14,11],[15,10,15,11],[21,10,21,11],[19,10,19,11],[20,10,20,11],[16,10,16,11],[47,32,47,33],[33,10,33,11],[26,10,26,11],[27,10,27,11],[28,10,28,11],[22,10,22,11],[23,10,23,11],[24,10,24,11],[25,10,25,11],[47,29,47,30],[45,20,46,20],[47,23,47,24],[2,0,2,8],[3,0,3,8],[5,0,5,7],[6,0,6,8],[7,10,7,11],[7,0,7,9],[8,10,8,11],[45,17,46,17],[47,26,47,27],[48,23,49,23],[44,38,45,38],[47,35,48,35],[47,38,48,38],[48,26,49,26],[46,38,46,39],[48,29,49,29],[46,35,46,36],[44,35,45,35],[45,26,46,26],[45,29,46,29],[48,32,49,32],[45,32,46,32],[64,11,64,12],[45,23,46,23],[48,14,49,14],[29,10,29,11],[30,10,30,11],[48,17,49,17],[48,11,49,11],[48,20,49,20],[34,10,34,11],[47,11,47,12],[47,14,47,15],[47,17,47,18],[47,20,47,21],[45,11,46,11],[45,14,46,14]]}
[" UPUTE ZA RAD: - Ispuniti sve podatke u čelijama s plavom bojom. Ispuniti i za izbor armature u kolonama L,N i O",null,null,null,null,null,null,null,null,null,{"$f":"+K3-K2","v":168.84210526315789}]
[" - Ukoliko nosivost tla ili klizanje ne zadovoljava, treba promijeniti dimenzije temeljne stope",null,null,null,null,null,null,null,null,null,{"$f":"70*0.18796992481203","v":13.157894736842101}]
[" - Za privremene objekte mobilizirani faktori mogu biti minimalni:   Fjmin=1,2  (I19) i   Fcmin=1,8 (I20)                                                ",null,null,null,null,null,null,null,null,null,182,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z18/M18","v":{"$error":"#REF!"}}]
[" - Udaljenost temelja od iskopa x (E 37) treba biti veća od širine temelja iza zida b2 (E 56)."]
[" - Ukoliko će se u proračunu koristiti i pasivni otpor, u čeliju I 5 upiši Y a ako ne onda N",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!C9","v":"Ka"},null,null,null,null,null,null,null,null,null,null,null,"koordinate","Kordinate svih opterećenja"]
["  - Ukoliko se tlak na zid računa sa Ka, u čeliju I 6 upiši Ka a ako sa Ko, upiši Ko (Ko - slova).                                                                                                                                                                                 - Ukoliko se za armiranje koristi rebrasta armatura, u čelije I47 i I50 upiši RA (za mreže MA) a u čelije L44, L45, L47 i L51 upiši profil armature, a za razdjelnu armaturu i razmak armature u čeliju O 45. Debljinu zaštitnog sloja upiši u čeliju N44 i N51.",null,null,null,null,null,null,null,"Ka",null,null,null,"Koordinate","V11","v22","v33","Vtem","h11","h22","h33","Htem","Za stabilnost oko toćke A                                                                                                                 x              y",null,"krak                  x  ","krak                  y  ","Moment destabilnosti i stabilnosti","za Mzida                                              krakovi                             x                  y",null,"Moment zida II","za M u                           presjeku II-II                                                   krakovi                                x               y",null,"Moment      II-II","za M u                           temelju ispod zida                     krakovi                             x                  y",null,"Moment  ","za M u                           presjeku I-I                                              krakovi                             x                  y",null,"Moment      I-I"]
[" - Za izračun iskopa treba upisati koordinate postojećeg terena u tablici od G513 do H525",null,null,null,null,null,null,null,null,null,"Naziv opterećenja",null,"Opterećenje",null,null,null,null,null,null,null,null,{"$f":"2+E57","v":4.9000021999999994},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,null,null,{"$f":"2+E57-E54-E51/2","v":{"$error":"#REF!"}},{"$f":"+E48","v":1.2},null,{"$f":"2+E55","v":{"$error":"#REF!"}},{"$f":"#REF!+(E48-#REF!)/2","v":{"$error":"#REF!"}},null,{"$f":"2+E55+E51/2","v":{"$error":"#REF!"}},{"$f":"#REF!+(E48-#REF!)/2","v":{"$error":"#REF!"}},null,{"$f":"2+E55+E51","v":{"$error":"#REF!"}},{"$f":"#REF!+(E48-#REF!)/2","v":{"$error":"#REF!"}}]
[" - Ovaj program može, po odobrenju autora programa, koristiti isključivo....................................                                                                     - Korištenje programa bez odobrenja autora je kažnjivo. - Ime autora i vlasnika programa navedeno je u čeliji A 10.",null,null,null,null,null,null,null,null,null," Eh1 .....................................................",null,{"$f":"-B108","v":{"$error":"#REF!"}},null,null,null,null,null,null,{"$f":"+M8","v":{"$error":"#REF!"}},null,null,{"$f":"+H108","v":{"$error":"#REF!"}},null,{"$f":"+W8-$W$7","v":{"$error":"#REF!"}},{"$f":"+M8*Y8","v":{"$error":"#REF!"}},null,{"$f":"+W8-$AB$7","v":{"$error":"#REF!"}},{"$f":"T8*AB8","v":{"$error":"#REF!"}}]
[null,"ANALIZA STABILNOSTI I DIMENZIONIRANJE POTPORNOG ZIDA  ",null,null,null,null,null,null,null,null," Eh2 ............................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M9","v":{"$error":"#REF!"}},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$f":"+W9-$AB$7","v":{"$error":"#REF!"}},{"$f":"AB9*T9","v":{"$error":"#REF!"}}]
["Nikola Sapunar, Zagreb, Gundulićeva 36, tel. 098 213 632",null,null,null,null,null,null,null,null,null," Eh3 ....................................................."," ",0,null,null,null,null,null,{"$f":"+M10","v":0},null,null,null,1.2,null,{"$error":"#REF!"},{"$error":"#REF!"},null,null,null,null,{"$f":"+AE7-#REF!","v":{"$error":"#REF!"}},{"$f":"+AE10*S10","v":{"$error":"#REF!"}}]
[null,null,"GEOMEHANIČKE KARAKTERISTIKE TLA",null,null,null,null,null,null,null," EPrometno ...................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$f":"+M11","v":{"$error":"#REF!"}},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$f":"+W11-$AB$7","v":{"$error":"#REF!"}},{"$f":"AB11*T11","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," EPTočkasto ......................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[null,null,null,null,"     1. Sloj","   2. Sloj","     3. Sloj",null,"  Tlo ispod temelja",null," EPLinijsko ................................"," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,0,null,{"$error":"#REF!"},{"$error":"#REF!"},null,-1.2,{"$error":"#REF!"}]
[" kut unutrašnjeg trenja: ......................................",null," j","(°)",{"$f":"+'Analiza i dimenzioniranje'!D14","v":22},{"$f":"+'Analiza i dimenzioniranje'!E14","v":18},{"$f":"+'Analiza i dimenzioniranje'!F14","v":20}," j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18}," (°)"," EQTemelj ...................................................."," ",{"$error":"#REF!"},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[" kohezija: ...............................................................",null,"c","(kPa)",{"$f":"+'Analiza i dimenzioniranje'!D15","v":10},{"$f":"+'Analiza i dimenzioniranje'!F12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C12","v":{"$error":"#VALUE!"}},"c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"(kPa)"," HSidro ..............................."," ",{"$f":"-B115","v":2.2699256917793105},null,null,null,null,null,null,{"$f":"+M15","v":2.2699256917793105},null,null,170.21276595744681,null,{"$error":"#REF!"},{"$f":"-M15*Y15","v":{"$error":"#REF!"}},null,169.01276595744682,383.64641968549216]
[" zapreminska težina: ..............................................",null,"g   ","(kN/m3)",{"$f":"+'Analiza i dimenzioniranje'!D16","v":20},{"$f":"+'Analiza i dimenzioniranje'!E16","v":20},{"$f":"+'Analiza i dimenzioniranje'!F16","v":20},"g =   ",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"(kN/m3)"," HPotres ........................................."," ",{"$f":"-B116","v":{"$error":"#REF!"}},null,null,null,null,null,null,{"$error":"#REF!"},null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"},null,{"$error":"#REF!"},{"$error":"#REF!"}]
[" debljina sloja: .....................................................",null,"h","(m)",{"$f":"IF(M61>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!E47-M61,'Analiza i dimenzioniranje'!D17)","v":{"$error":"#VALUE!"}},{"$f":"+IF(M61>='Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,0,'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17-'P XX-XX'!M61)","v":0},{"$f":"+E48","v":1.2},"g' =  ",{"$f":"+'Analiza i dimenzioniranje'!H17","v":10},"(kN/m3)","Voda"," ",{"$f":"-'Analiza i dimenzioniranje'!B123","v":-1.7999999999999998},null,null,null,null,{"$f":"-M17","v":1.7999999999999998},null,{"$f":"+M17","v":-1.7999999999999998},null,null,1.2,null,{"$error":"#REF!"},{"$error":"#REF!"},null,null,null,null,null,null,null,null,null,null,{"$f":"+AK7-C117","v":{"$error":"#REF!"}},{"$f":"+M17*AK17","v":{"$error":"#REF!"}}]
[" trenje zid-tlo: .........................................................",null,"d","(°)",{"$f":"+'Analiza i dimenzioniranje'!D19","v":0},{"$f":"+'Analiza i dimenzioniranje'!E19","v":0},{"$f":"+'Analiza i dimenzioniranje'!F19","v":0},"Fj =",{"$f":"+'Analiza i dimenzioniranje'!J27","v":1.25},null,null,null,{"$f":"SUM(M8:M17)","v":{"$error":"#REF!"}},null,null,null,null,{"$f":"SUM(R8:R17)","v":1.7999999999999998},{"$f":"SUM(S8:S17)","v":0},{"$f":"SUM(T8:T17)","v":{"$error":"#REF!"}},{"$f":"SUM(U8:U17)","v":0},null,null,"x",null,{"$f":"SUM(Z8:Z17)","v":{"$error":"#REF!"}},null,null,{"$f":"SUM(AC8:AC17)","v":{"$error":"#REF!"}},null,null,{"$f":"SUM(AF8:AF17)","v":{"$error":"#REF!"}},null,null,{"$f":"SUM(AI8:AI17)","v":0},null,null,{"$f":"SUM(AL8:AL17)","v":{"$error":"#REF!"}}]
[" nagib pokosa ili sloja: ....................................................",null,"e","(°)",{"$f":"+'Analiza i dimenzioniranje'!D18","v":6},{"$f":"+'Analiza i dimenzioniranje'!E18","v":4},{"$f":"+'Analiza i dimenzioniranje'!F18","v":2},"Fc =",{"$f":"+'Analiza i dimenzioniranje'!J28","v":1.25},null," Gtem .......N61+P61+R61............................."," ",{"$f":"+#REF!+#REF!+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+#REF!","v":{"$error":"#REF!"}},null,null,null,null,{"$f":"+H126","v":{"$error":"#REF!"}},null,{"$f":"+$V$7-V19","v":{"$error":"#REF!"}},null,{"$f":"+M19*X19","v":{"$error":"#REF!"}},null,null,null,{"$f":"AD7-#REF!","v":{"$error":"#REF!"}},null,{"$f":"+AD19*O19","v":{"$error":"#REF!"}},{"$f":"+AG7-#REF!","v":{"$error":"#REF!"}},null,{"$f":"+#REF!*'Analiza i dimenzioniranje'!AQ13","v":{"$error":"#REF!"}},{"$f":"AJ7-#REF!","v":{"$error":"#REF!"}},null,{"$f":"+#REF!*'Analiza i dimenzioniranje'!AT13","v":{"$error":"#REF!"}}]
[" nadvišenje tla iznad zida: ..........................................",null,"v","(m)",{"$f":"+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,"nagib padine   e =",{"$f":"+'Unos podataka'!F10","v":10},null," Gzid+konz ...................................."," ",{"$f":"+B127","v":{"$error":"#REF!"}},null,null,{"$f":"+M20","v":{"$error":"#REF!"}},null,null,null,null,null,{"$error":"#REF!"},null,{"$f":"+$V$7-V20","v":{"$error":"#REF!"}},null,{"$error":"#REF!"},{"$f":"+$AA$7-V20","v":{"$error":"#REF!"}},null,{"$f":"+P20*AA20","v":{"$error":"#REF!"}}]
[" Poissonov koeficijent: .......................",null,"n",null,{"$f":"+'Analiza i dimenzioniranje'!D21","v":0.3},null,null,null,null,null," Gnasip na konzoli............................."," ",0,null,null,{"$f":"+M21","v":0},null,null,null,null,null,4.9000021999999994,null,0,null,0,{"$f":"+$AA$7-V21","v":{"$error":"#REF!"}},null,{"$f":"+P21*AA21","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null," Gnasipa na temelju iza............."," ",0,null,{"$f":"+M22","v":0},null,null,null,null,null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,null,null,{"$f":"+AD7-V22","v":{"$error":"#REF!"}},null,{"$f":"+M22*AD22","v":{"$error":"#REF!"}}]
[null,null,"OPTEREĆENJE ZIDA:",null,null,null,null,null,null,null," Gnasipa na temelju ispred ........................"," ",0,{"$f":"+M23","v":0},null,null,null,null,null,null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,null,null,null,null,null,null,null,null,{"$f":"AJ7-(2+E57-E54/2)","v":{"$error":"#REF!"}},null,{"$f":"+AJ23*N23","v":{"$error":"#REF!"}}]
["PROMETNO OPTEREĆENJE...............................................................",null,null,"Pp =",{"$f":"+'Analiza i dimenzioniranje'!E24","v":10},"kN/m2 ",null,null,null,null," PPrometno ......................."," ",{"$error":"#REF!"},null,{"$f":"+M24","v":{"$error":"#REF!"}},null,null,null,null,null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,null,null,{"$f":"+$AD$7-X24","v":{"$error":"#REF!"}},null,{"$f":"+M24*AD24","v":{"$error":"#REF!"}}]
[" širina opterećenja.............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E25","v":3},"m",{"$f":"+E26-E27","v":2.9999989999999999},null,null,null," PTočkasto ......................"," ",{"$error":"#REF!"},null,{"$f":"+M25","v":{"$error":"#REF!"}},null,null,null,null,null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,null,null,{"$f":"+$AD$7-X25","v":{"$error":"#REF!"}},null,{"$f":"+M25*AD25","v":{"$error":"#REF!"}}]
[" udaljenost opterećenja od zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E26","v":4.5},"m",{"$f":"+G27+G25","v":4.5000009999999993},null,null,null," PLinijsko ........................."," ",{"$error":"#REF!"},null,{"$f":"+M26","v":{"$error":"#REF!"}},null,null,null,null,null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,null,null,{"$f":"+$AD$7-X26","v":{"$error":"#REF!"}},null,{"$f":"+M26*AD26","v":{"$error":"#REF!"}}]
[{"$f":"+IF(E19>0,\" udaljenost vrha pokosa od zida......................................................\",\"\")","v":" udaljenost vrha pokosa od zida......................................................"},null,null,{"$f":"+IF(E19>0,\"b =\",\"\")","v":"b ="},{"$f":"+'Analiza i dimenzioniranje'!E27","v":1.5000009999999999},{"$f":"+IF(E19>0,\"m\",\"\")","v":"m"},{"$f":"+E27+0.000001","v":1.5000019999999998},null,null,null," QTemelj .............................."," ",{"$error":"#REF!"},null,{"$f":"+M27","v":{"$error":"#REF!"}},null,null,null,null,null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,null,null,{"$f":"+$AD$7-X27","v":{"$error":"#REF!"}},null,{"$f":"+M27*AD27","v":{"$error":"#REF!"}}]
["TOČKASTO OPTEREĆENJE ................................................",null,null,"PT =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/100 cm2",null,{"$f":"+E28+0.00001","v":20.000011000000001},{"$f":"0.1+0.0000000001","v":0.1000000001},{"$f":"0.1+0.0000000001","v":0.1000000001}," VSidro .............................."," ",0.60822475599092374,null,null,{"$f":"+M28","v":0.60822475599092374},null,null,null,null,null,{"$error":"#REF!"},null,{"$f":"+$V$7-V28","v":{"$error":"#REF!"}},null,{"$error":"#REF!"},{"$f":"+$AA$7-V28","v":{"$error":"#REF!"}},null,{"$f":"P28*AA28","v":{"$error":"#REF!"}}]
[" udaljenost centra opterećenja od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E37","v":1.5},"m",null,null,null,null," Ev1 ...................................."," ",{"$error":"#REF!"},null,null,{"$f":"+M29","v":{"$error":"#REF!"}},null,null,null,null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$f":"+$AA$7-V29","v":{"$error":"#REF!"}},null,{"$f":"+P29*AA29","v":{"$error":"#REF!"}}]
["LINIJSKO IZA ZIDA ................................................................",null,null,"PL =",{"$f":"+'Analiza i dimenzioniranje'!E34","v":20.000001000000001},"kN/m'/10 cm",null,{"$f":"+E30+0.00001","v":20.000011000000001},null,null," Ev2  .........................."," ",{"$error":"#REF!"},null,null,{"$f":"+M30","v":{"$error":"#REF!"}},null,null,null,null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,{"$error":"#REF!"},{"$f":"+$AA$7-V30","v":{"$error":"#REF!"}},null,{"$f":"+P30*AA30","v":{"$error":"#REF!"}}]
[" udaljenost opterećenja od vrha zida ......................................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!K28","v":2.5},"m",null,null,null,null," Ev3 (na temelj) ........................................"," ",0,null,{"$f":"+M31","v":0},null,null,null,null,null,null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,{"$error":"#REF!"},null,null,null,{"$f":"+$AD$7-#REF!","v":{"$error":"#REF!"}},null,{"$f":"+M31*AD31","v":{"$error":"#REF!"}},{"$f":"+$AD$7-AD31","v":{"$error":"#REF!"}}]
["OPTEREĆENJE TEMELJEM ..............................................",null,null,"QT =",{"$f":"+'Analiza i dimenzioniranje'!E28","v":120},"kN/m2 ",null,null,null,null,null,null,{"$f":"SUM(M19:M31)","v":{"$error":"#REF!"}},{"$f":"SUM(N19:N31)","v":{"$error":"#REF!"}},{"$f":"SUM(O19:O31)","v":{"$error":"#REF!"}},{"$f":"SUM(P19:P31)","v":{"$error":"#REF!"}},{"$f":"SUM(Q19:Q31)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,{"$f":"SUM(Z19:Z31)","v":{"$error":"#REF!"}},null,null,{"$f":"SUM(AC19:AC31)","v":{"$error":"#REF!"}},null,null,{"$f":"SUM(AF19:AF31)","v":{"$error":"#REF!"}},null,null,{"$f":"SUM(AI19:AI31)","v":{"$error":"#REF!"}},null,null,{"$f":"SUM(AL19:AL31)","v":{"$error":"#REF!"}}]
[" širina temelja (opterećenja).............................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"II-II","sredina","I-I"]
[" duljina temelja (opterećenja)....................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E30","v":10},"m",null,null,null,null,"Kont naponi N76, P76, R76.....................",null,{"$f":"+#REF!+#REF!+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+X34","v":{"$error":"#REF!"}},null,{"$f":"+#REF!","v":{"$error":"#REF!"}},null,null,null,null,null,null,{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,null,null,{"$f":"$AD$7-#REF!","v":{"$error":"#REF!"}},null,{"$f":"+X34*AD34","v":{"$error":"#REF!"}},{"$f":"$AG$7-#REF!","v":{"$error":"#REF!"}},null,{"$f":"-Y34*AG34","v":{"$error":"#REF!"}},{"$f":"+AJ7-#REF!","v":{"$error":"#REF!"}},null,{"$f":"+Z34*AJ34","v":{"$error":"#REF!"}}]
[" visina temelja ..........................................................",null,null,"h =",{"$f":"+'Analiza i dimenzioniranje'!E33","v":1},"m",null,null,null,null,"Trenje ...................................",null,{"$f":"B118","v":{"$error":"#REF!"}},null,null,null,null,{"$f":"+Z35","v":{"$error":"#REF!"}},{"$f":"+X35","v":{"$error":"#REF!"}},null,{"$f":"+Y35","v":{"$error":"#REF!"}},null,null,{"$f":"+M35*E55/E57","v":{"$error":"#REF!"}},{"$f":"+M35*E51/E57","v":{"$error":"#REF!"}},{"$f":"+M35*E54/E57","v":{"$error":"#REF!"}},null,null,null,null,{"$f":"+AE7-#REF!","v":{"$error":"#REF!"}},{"$f":"-S35*AE35","v":{"$error":"#REF!"}},null,{"$f":"+AH7-#REF!","v":{"$error":"#REF!"}},{"$f":"Y35*AH35","v":{"$error":"#REF!"}},null,{"$f":"+AK7-#REF!","v":{"$error":"#REF!"}},{"$f":"-Z35*AK35","v":{"$error":"#REF!"}}]
[" udaljenost temelja (opterećenja) od zida ..........................................",null,null,"x =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m",null,null,null,null,null,null,"S",{"$f":"N32+N34","v":{"$error":"#REF!"}},{"$f":"+O32+O34","v":{"$error":"#REF!"}},{"$f":"SUM(P32:P35)","v":{"$error":"#REF!"}},{"$f":"+Q32+Q34","v":{"$error":"#REF!"}},{"$f":"R18+R35","v":{"$error":"#REF!"}},{"$f":"S18+S35","v":{"$error":"#REF!"}},{"$f":"T18+T34+T35","v":{"$error":"#REF!"}},{"$f":"+U18+U35","v":{"$error":"#REF!"}}]
[" dubina temeljenja (u odnosu na vrh zida)..................................................",null,null,"Df =",{"$f":"+'Analiza i dimenzioniranje'!K31","v":1},"m",null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N36:Q36)","v":{"$error":"#REF!"}},null,null,null,{"$f":"SUM(R36:U36)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,{"$f":"+AC18+AC32+AC34+AC35","v":{"$error":"#REF!"}},null,null,{"$f":"+AF18+AF32+AF34+AF35","v":{"$error":"#REF!"}},null,null,{"$f":"+AI18+AI32+AI34+AI35","v":{"$error":"#REF!"}},null,null,{"$f":"+AL18+AL32+AL34+AL35","v":{"$error":"#REF!"}}]
["SILA U SIDRU (u smjeru sidra) ..............................................",null,null,"PS =",{"$f":"+'Analiza i dimenzioniranje'!AJ40","v":2.35},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y","x"]
[" otklon sidra od horizontale ...................................................",null,null,"a=",{"$f":"+'Analiza i dimenzioniranje'!E39","v":15},"°    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD7","v":{"$error":"#REF!"}},{"$f":"+AE7","v":{"$error":"#REF!"}}]
[" hvatište sidra od dna temelja ..................................................",null,null,"hs =",{"$f":"+'Analiza i dimenzioniranje'!AJ42","v":170.21276595744681},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!*('Analiza i dimenzioniranje'!AI33-#REF!)+B129*(AD39-H129)+B138*(AD39-H138)+B138*(AD39-H138)+#REF!*('Analiza i dimenzioniranje'!AI33-#REF!)+S35*(AE39-#REF!)+B110*(AE39-H110)","v":{"$error":"#REF!"}}]
[" POTRES...........S V *",{"$f":"+'Analiza i dimenzioniranje'!E44","v":0.1},"..................................................","HP =",{"$f":"+B41*#REF!*C42/B42","v":{"$error":"#REF!"}},"kN/m'"]
[null,{"$f":"+'Analiza i dimenzioniranje'!E45","v":1},{"$f":"+'P XIX-XIX'!C42","v":1}]
[null,null,"DIMENZIJE ZIDA:"]
[]
[" visina zida i temelja.........................................................",null,null,"H =",{"$f":"+E17+F17+G17","v":{"$error":"#VALUE!"}},"m"]
[" dužina zida .......................................................",null,null,"L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m"]
[" otklon zida uz tlo od vertikale.........................................",null,null,"b =",{"$f":"+'Analiza i dimenzioniranje'!H51","v":4},"°    "]
[" visina temelja prema zasipu .............................",null,null,"hB=",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m"]
[" visina temelja prema padini ........................................",null,null,"hA=",{"$f":"+'Analiza i dimenzioniranje'!E51","v":0.7},"m"]
[" širina zida u kruni .............................................................",null,null,"d =",{"$f":"+'Analiza i dimenzioniranje'!E54","v":0.6},"m"]
[" širina zida na temelju .......................................",null,null,"d1=",{"$f":"+'Analiza i dimenzioniranje'!E55","v":0.8},"m"]
[" nagib lica zida .............................   n1: 1",null,null,"n1 =",{"$f":"IF(#REF!-#REF!=0,\">100\",IF(#REF!-#REF!/(0.00000000000001+#REF!-#REF!)>100,\">100\",(#REF!-#REF!)/(#REF!-#REF!)))","v":{"$error":"#REF!"}}]
[" nagib dna temelja ........................   n2: 1",null,null,"n2 =",{"$f":"IF(E48=E49,\">100\",E57/(#REF!))","v":{"$error":"#REF!"}}]
[" širina temelja ispred zida ................................",null,null,"b1=",{"$f":"+E57-E55-E51","v":{"$error":"#REF!"}},"m",{"$f":"+E55+0.000000001","v":{"$error":"#REF!"}},null,null,"     v22="]
[" širina temelja iza zida .............................................................",null,null,"b2=",{"$f":"+#REF!","v":{"$error":"#REF!"}},"m"]
[" širina zaloge na temelju.............................................................",null,null,"b3=",0,"m  ",{"$f":"+E55+0.000000001","v":{"$error":"#REF!"}}]
[" ukupna širina temelja .....................................................",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m"]
[" zapreminska težina zida i temelja........................................",null,null,"gb=",{"$f":"+'Analiza i dimenzioniranje'!E62","v":25},"kN/m3 "]
[{"$f":"IF(J98=0,\" zapreminska težina zasipa ................................................ \",\" zapreminska težina zaloge .........................................................................   \")","v":" zapreminska težina zasipa ................................................ "},null,null,"gz=",{"$f":"+'Analiza i dimenzioniranje'!E63","v":20},"kN/m3 "]
[" visina nasipa ispred zida .........................................................................",null,null,"hn=",{"$f":"+'Analiza i dimenzioniranje'!H76","v":0.30010099999999995},"m"]
[" zapreminska težina nasipa ...............................",null,null,"      gn=",{"$f":"+'Analiza i dimenzioniranje'!E66","v":20},"kN/m3 ",null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!U68","v":6.0000000000000009}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M63+M64","v":{"$error":"#REF!"}}]
[null,null,"KONZOLA:",null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!U44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,-B116*C116/1.35-B108*(#REF!-#REF!)-B109*(#REF!-#REF!)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B128*(#REF!-#REF!)+B136*(#REF!-#REF!)+B137*(#REF!-#REF!)+B135*(C135),-B116*C116/1.35-B108*(#REF!-#REF!)-B109*(#REF!-#REF!)-B112*N67-B113*N68-B114*N69-B115*C115+B127*(C127-(E54+0.5*E51))+B136*(#REF!-#REF!)+B137*(#REF!-#REF!)+B135*(C135))","v":{"$error":"#REF!"}}]
[null,null,{"$f":"IF(I20=0,\"\",+#REF!)","v":{"$error":"#REF!"}},null,{"$f":"+E65+0.0000001","v":1.0000001000000001},null,null,null,null,"Visina presjeka",{"$f":"+'Dijagram momenata'!Q5","v":6},null,{"$f":"-#REF!*N66","v":{"$error":"#REF!"}},{"$f":"-B116*C116","v":{"$error":"#REF!"}},{"$f":"-B111*#REF!","v":{"$error":"#REF!"}}]
[" širina konzole  ............................................................",null,null,"bk=",{"$f":"+'Analiza i dimenzioniranje'!G78","v":1},"m",null,null,null,"Presjek i Krak od vrha zida","krakovi od vrha zida","krak kota",null,"krak od presjeka do sile"]
[" duljina konzole  ............................................................",null,null,"Lk=",{"$f":"+'Analiza i dimenzioniranje'!E78","v":12},"m",null,null,null," Eprometno",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C111","v":{"$error":"#REF!"}},{"$f":"+C111+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c111",{"$f":"IF(+L66-'Dijagram momenata'!$Q$5>0,+L66-'Dijagram momenata'!$Q$5,0)","v":{"$error":"#REF!"}}]
[" visina konzole od dna temelja ...............................",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},"m",null,null,null," EPTočkasto",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C112","v":{"$error":"#REF!"}},{"$f":"+C112+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c112",{"$f":"IF(+L67-'Dijagram momenata'!$Q$5>0,+L67-'Dijagram momenata'!$Q$5,0)","v":{"$error":"#REF!"}}]
[" visina konzole  ............................................................",null,null,"dk=",{"$f":"+'Analiza i dimenzioniranje'!C77","v":0.3},"m",null,null,null," EPLinijsko",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C113","v":{"$error":"#REF!"}},{"$f":"+C113+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c113",{"$f":"IF(+L68-'Dijagram momenata'!$Q$5>0,+L68-'Dijagram momenata'!$Q$5,0)","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null," EQTemelj ",{"$f":"(+'Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)-C114","v":{"$error":"#REF!"}},{"$f":"+C114+'Dijagram momenata'!$Q$20","v":{"$error":"#REF!"}},"c114",{"$f":"IF(+L69-'Dijagram momenata'!$Q$5>0,+L69-'Dijagram momenata'!$Q$5,0)","v":{"$error":"#REF!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,4]
[]
[]
[]
[null,{"$f":"+IF(I5=\"y\",\"AKTIVNI TLAK I PASIVNI OTPOR\",\"AKTIVNI TLAK\")","v":"AKTIVNI TLAK"}]
[null,"(Coulomb - Poncelet)"]
[]
[null,"Ea(kN/m')","Eh(kN/m')","Ev(kN/m')"]
[" sloj 1. ..........................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+B97*COS((E18-E47)*PI()/180)","v":{"$error":"#REF!"}},{"$f":"+B97*SIN((E18-E47)*PI()/180)","v":{"$error":"#REF!"}},{"$f":"+IF(I6=\"ko\",\"Ko1=\",\"Ka1 =\")","v":"Ka1 ="},{"$f":"+'Analiza i dimenzioniranje'!F110","v":0.59693740409312213}]
[" sloj 2. ..............................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+B98*COS((F18-E47)*PI()/180)","v":{"$error":"#REF!"}},{"$f":"+B98*SIN((F18-E47)*PI()/180)","v":{"$error":"#REF!"}},{"$f":"+IF(I6=\"ko\",\"Ko2=\",\"Ka2 =\")","v":"Ka2 ="},{"$f":"+'Analiza i dimenzioniranje'!F111","v":0.78849922516973658}]
[" sloj 3. ..............................",0,{"$f":"+B99*COS((G18-E47)*PI()/180)","v":0},{"$f":"+B99*SIN((G18-E47)*PI()/180)","v":0},{"$f":"+IF(I6=\"ko\",\"Ko3=\",\"Ka3 =\")","v":"Ka3 ="},{"$f":"+'Analiza i dimenzioniranje'!F112","v":0.71000444573298527}]
["S Ea =",{"$f":"SUM(B97:B99)","v":{"$error":"#REF!"}},{"$f":"SUM(C97:C99)","v":{"$error":"#REF!"}},{"$f":"SUM(D97:D99)","v":{"$error":"#REF!"}},null,null,null,null,null,{"$f":"G54+0.00000000001","v":{"$error":"#REF!"}}]
[{"$f":"+IF(B101>B108+B109+B111+B112+B113+B114+B115+B116,\"Epmax =\",\"Ep =\")","v":{"$error":"#REF!"}},{"$f":"+IF(0.5*E61*(E49+E60)*(E49+E60)*F101>B108+B109+B111+B112+B113+B114+B115+B116,B108+B109+B111+B112+B113+B114+B115+B116+0.0000011,0.5*(E61*(E49+E60)*(E49+E60)*F102))","v":{"$error":"#REF!"}},"kN/m'",null,{"$f":"+IF(I5=\"Y\",\"Kp =\",\"\")","v":""},{"$f":"IF('Analiza i dimenzioniranje'!C9=\"y\",TAN(G14*PI()/180)^2,0)","v":0}]
[null,null,null,null,null,{"$f":"+IF(F101=\"\",0,F101)","v":0}]
[]
[null,"KONTROLA STABILNOSTI  (Prevrtanje oko točke A)",null,null,null,null,null,null,0,{"$f":"IF(J97=0,COS((-K90)*PI()/180)^2*COS((-K90)*PI()/180),COS((-K90)*PI()/180)^2*COS((-K90+J97)*PI()/180))","v":1}]
[]
[null,"Horizontalno opterećenje",null,"Moment destabilnosti"]
[null,"(kN/m')"," krak(m)","MH(kNm/m')","Faktor",null,null,"koordinata"]
[" Eh1 .....................................................",{"$f":"+C97","v":{"$error":"#REF!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I120","v":1},null,null,{"$f":"+#REF!","v":{"$error":"#REF!"}}]
[" Eh2 .............................................",{"$f":"+C98","v":{"$error":"#REF!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!I121","v":1},null,null,{"$f":"+#REF!","v":{"$error":"#REF!"}}]
[" Eh3 .....................................................",{"$f":"+C99","v":0},null,null,{"$f":"+'Analiza i dimenzioniranje'!I122","v":1},null,null,{"$f":"+C110+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
[" EPrometno ....................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I124","v":1.3},null,null,{"$f":"+C111+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPTočkasto ......................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I125","v":1},null,null,{"$f":"+C112+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}}]
[" EPLinijsko ................................",{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"+B113*C113","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I126","v":1}]
[" EQTemelj ....................................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}},null,{"$f":"+'Analiza i dimenzioniranje'!I127","v":1},null,null,{"$f":"+C114+'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#REF!"}},null,null,{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}}]
[" HSidro ...............................",{"$f":"IF(E40<M61,0,-E38*COS(E39*PI()/180))","v":-2.2699256917793105},{"$f":"IF(H115<'Analiza i dimenzioniranje'!U44,0,H115-'Analiza i dimenzioniranje'!U44)","v":169.01276595744682},{"$f":"+B115*C115","v":-383.64641968549216},{"$f":"+'Analiza i dimenzioniranje'!I129","v":0},null,null,{"$f":"+E40","v":170.21276595744681},null,null,{"$f":"+K114-TAN(I20*PI()/180)*2","v":{"$error":"#REF!"}},{"$f":"+L114+2","v":{"$error":"#REF!"}}]
[" HPotres .........................................",{"$f":"+E41","v":{"$error":"#REF!"}},{"$f":"+H116-'Analiza i dimenzioniranje'!U44","v":{"$error":"#REF!"}},{"$f":"B116*C116","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I150","v":0},"hp =",{"$f":"+(D108+D109+D110+D111+D112+D113+D114+D115+D117)/(B108+B109+B110+B111+B112+B113+B114+B115+B117)","v":{"$error":"#REF!"}},{"$f":"+#REF!","v":{"$error":"#REF!"}}]
[{"$f":"+A101","v":{"$error":"#REF!"}},{"$f":"-B101","v":{"$error":"#REF!"}},null,null,{"$f":"+'Analiza i dimenzioniranje'!E116","v":0},null,null,{"$f":"+C117+'Analiza i dimenzioniranje'!$E$52","v":1.2}]
["S Eh =",{"$f":"SUM(B108:B117)","v":{"$error":"#REF!"}},null,null,"      za = ",{"$f":"IF(B118=0,0,D118/B118)","v":{"$error":"#REF!"}},"m"]
[null,null,null,null,"       / za - krak horizontalne komponente /"]
[]
[]
[]
[]
[null,"Vertikalno opterećenje",null,"Moment stabilnosti",null,null,null,null,null,{"$f":"+#REF!","v":{"$error":"#REF!"}}]
[" ","  (kN/m')"," krak(m)","MV(kNm/m')","Faktor",null,null,"koordinata"]
[" Gtem ....................................",0,{"$f":"2+E57-#REF!","v":{"$error":"#REF!"}},{"$f":"B126*C126","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I135","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C126","v":{"$error":"#REF!"}}]
[" Gzid+konz ....................................",{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"2+E57-#REF!","v":{"$error":"#REF!"}},{"$f":"B127*C127","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I136","v":{"$error":"#VALUE!"}},null,null,{"$f":"+#REF!","v":{"$error":"#REF!"}}]
[" Gnasip na konzoli.............................",{"$f":"IF(M61>=E67+E68,0,#REF!)","v":0},{"$f":"IF(B128=0,0,2+E57-#REF!)","v":0},{"$f":"B128*C128","v":0},{"$f":"+'Analiza i dimenzioniranje'!I138","v":{"$error":"#VALUE!"}},null,null,{"$f":"2+$E$57-C128","v":4.9000021999999994}]
[" Gnasipa na temelju iza.............",{"$f":"0","v":0},{"$f":"2+E57-#REF!","v":{"$error":"#REF!"}},{"$f":"B129*C129","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I139","v":{"$error":"#VALUE!"}},null,null,{"$error":"#REF!"}]
[" Gnasipa na temelju ispred ........................",0,{"$f":"E54/2","v":{"$error":"#REF!"}},{"$f":"B130*C130","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I140","v":{"$error":"#VALUE!"}},null,null,{"$error":"#REF!"}]
[" PPrometno .......................",{"$f":"+IF(#REF!<#REF!,0,(#REF!-#REF!)*'Analiza i dimenzioniranje'!E24)","v":{"$error":"#REF!"}},{"$f":"IF(B131=0,0,2+E57-(#REF!+#REF!)/2)","v":{"$error":"#REF!"}},{"$f":"B131*C131","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!I141","v":{"$error":"#VALUE!"}},null,null,{"$error":"#REF!"}]
[" PTočkasto ......................",{"$f":"IF(#REF!>#REF!,'Analiza i dimenzioniranje'!E36/100,0)","v":{"$error":"#REF!"}},{"$f":"IF(B132=0,0,2+E57-#REF!)","v":{"$error":"#REF!"}},{"$error":"#REF!"},{"$f":"+'Analiza i dimenzioniranje'!I142","v":{"$error":"#VALUE!"}},null,null,{"$error":"#REF!"}]
[" PLinijsko .........................",{"$f":"IF(#REF!>#REF!,'Analiza i dimenzioniranje'!E34,0)","v":{"$error":"#REF!"}},{"$f":"IF(B133=0,0,2+E57-#REF!)","v":{"$error":"#REF!"}},{"$error":"#REF!"},{"$f":"+'Analiza i dimenzioniranje'!I143","v":{"$error":"#VALUE!"}},null,null,{"$error":"#REF!"}]
[" QTemelj ..............................",{"$f":"IF(#REF!>#REF!,'Analiza i dimenzioniranje'!E28,0)","v":{"$error":"#REF!"}},{"$f":"2+E57-#REF!-'Analiza i dimenzioniranje'!E29/2","v":{"$error":"#REF!"}},{"$error":"#REF!"},{"$f":"+'Analiza i dimenzioniranje'!I144","v":{"$error":"#VALUE!"}},null,null,{"$error":"#REF!"}]
[" VSidro ..............................",{"$f":"IF(E40<M61,0,E38*SIN(E39*PI()/180))","v":0.60822475599092374},{"$f":"2+E57-#REF!-E54-'Analiza i dimenzioniranje'!U49/200","v":{"$error":"#REF!"}},{"$error":"#REF!"},{"$f":"+'Analiza i dimenzioniranje'!I145","v":{"$error":"#VALUE!"}},null,null,{"$error":"#REF!"}]
[" Ev1 ....................................",{"$f":"+D97","v":{"$error":"#REF!"}},{"$f":"2+E57-#REF!","v":{"$error":"#REF!"}},{"$error":"#REF!"},{"$f":"+'Analiza i dimenzioniranje'!I146","v":{"$error":"#VALUE!"}},null,null,{"$error":"#REF!"}]
[" Ev2  ..........................",{"$f":"+D98","v":{"$error":"#REF!"}},{"$f":"2+E57-#REF!","v":{"$error":"#REF!"}},{"$error":"#REF!"},{"$f":"+'Analiza i dimenzioniranje'!I147","v":{"$error":"#VALUE!"}},null,null,{"$error":"#REF!"}]
[" Ev3 (na temelj) ........................................",{"$f":"+D99","v":0},{"$f":"2+E57-#REF!","v":{"$error":"#REF!"}},{"$error":"#REF!"},{"$f":"+'Analiza i dimenzioniranje'!I148","v":1},null,null,{"$error":"#REF!"}]
[" S V =",{"$f":"SUM(B126:B138)","v":{"$error":"#REF!"}}," S MVA =",{"$f":"SUM(D126:D138)","v":{"$error":"#REF!"}},"      xa = ",{"$f":"+I139","v":{"$error":"#REF!"}},"m",{"$f":"2+E57-F139","v":{"$error":"#REF!"}},{"$f":"D139/B139","v":{"$error":"#REF!"}}]
[null,null,null,null,"       / xa - krak vertikalne komponente /"]

{"sheet":"Slijeganje","index":32,"n_rows":143,"n_cols":29,"rows_kept":143,"cut":false,"hidden":true,"merged":[[14,21,14,22],[14,23,14,24],[16,25,16,26],[72,12,73,12],[72,13,73,13],[132,4,132,5],[0,0,0,12],[11,0,11,2],[12,0,13,2],[17,0,18,2],[19,0,21,2],[56,5,56,12]]}
[" -Program omogućava proračun slijegavanja od utjecaja 8 temelja u 8 odabranih točaka, (TS1 do TS8), bilo gdje unutar ili izvan temelja. Svi temelji imaju istu dubinu temeljenja."]
[" -Zadaju se slijedeće vrijednosti:"]
[" -Dubina temeljenja Df  upisuje se u čeliji E15, slojevi tla do dna temelja u čelije D28 i D29 a ispod temelja u čelije H28 do H32."]
[" -Koordinate točaka u kojima se želi izračunati slijegavanje TS1 do TS8"]
[" -Opterećenje pojedinog temelja dati na nivou dubine temeljenja"]
[" -Debljina, zapreminska težina i modul stišljivosti pojedinog sloja (Hi , g i Msi) "]
[" -Upisati nivo podzemne vode"]
[null,"  PRORAČUN SLIJEGANJA GRUPE TEMELJA U ODABRANIM TOČKAMA"]
[null,null,null,null,null,null,null,"rasterećenje"]
["  ULAZNI PODACI",null,null,null,"sB=",{"$f":"+'Analiza i dimenzioniranje'!F193","v":{"$error":"#VALUE!"}},"K1","g*h=",{"$f":"+('Analiza i dimenzioniranje'!E65+X30)*'Analiza i dimenzioniranje'!H18","v":13.243681064918412}]
[null,null,null,null,"sA=",{"$f":"+'Analiza i dimenzioniranje'!F190","v":{"$error":"#VALUE!"}},"K2","g*h=",{"$f":"+('Analiza i dimenzioniranje'!E65+X31)*'Analiza i dimenzioniranje'!H18","v":10.484696480964821}]
["OZNAKA TEMELJA",null,null,null,"T1","T2"]
["DIMENZIJE TEMELJA",null,null,"L",{"$f":"+'Unos podataka'!$F$38","v":12},{"$f":"+E13","v":12}]
[null,null,null,"B",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},{"$f":"+E14","v":2.9000021999999994},null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+S15","v":3.1500021999999994}]
["DUBINA TEMELJENJA",null,null,"Df",{"$f":"+'Analiza i dimenzioniranje'!$F$216","v":1.5001009999999999},{"$f":"+E15","v":1.5001009999999999},null,null,null,null,null,null,null,null,null,null,"sA",{"$f":"+'Analiza i dimenzioniranje'!F190","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C185","v":3.1500021999999994},null,"Točke","pravca 1",null,"visina temelja"]
["OPTEREĆENJE TEMELJEM",null,null,"p",{"$f":"+X25","v":{"$error":"#VALUE!"}},{"$f":"+X26","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"sB",{"$f":"+'Analiza i dimenzioniranje'!F193","v":{"$error":"#VALUE!"}},0,null,null,"T1  ","T2","T3","T4"]
["DOPUNSKO OPTEREĆENJE  p-y*h",null,null,"Dp",{"$f":"IF(E16-I10<0,0,E16-I10)","v":{"$error":"#VALUE!"}},{"$f":"+F16-I11","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,0,0,null,"x=",{"$f":"+R15","v":{"$error":"#VALUE!"}},{"$f":"+R16","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C190*100","v":70},{"$f":"+'Analiza i dimenzioniranje'!C193*100","v":107.28357545883233},"Kontrola"]
["KOORDINATE TEŽIŠTA TEMELJA",null,null,"X",{"$f":"+E13/2","v":6},{"$f":"+E18","v":6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+S15","v":3.1500021999999994},{"$f":"+S16","v":0},{"$f":"+V18","v":3.1500021999999994},{"$f":"+W18","v":0},"x","y"]
[null,null,null,"Y",{"$f":"+E14/2","v":1.4500010999999997},{"$f":"+F14/2","v":1.4500010999999997},null,null,null,null,null,null,null,null,null,null,"K1",0,{"$f":"0.26*S15/2","v":0.40950028599999994},null,"Y=",{"$f":"(W18-V18)/(W17-V17)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-V19*V17+V18","v":{"$error":"#VALUE!"}}," ",-4,{"$f":"V19*Z19+X19","v":{"$error":"#VALUE!"}}]
["OZNAKE TOČAKA I KOORDINATE TOČAKA U KOJIMA SE RAČUNA SLIJEGANJE",null,null,null,"K1","K2",null,null,null,null,null,null,null,null,null,null,"K2",0,{"$f":"+S14-S19","v":2.7405019139999993},null,"Y=",{"$f":"-(Y18-X18)/(X17-Y17)","v":-8.4487664105020177E-2},"*x    +",{"$f":"-(X17*V20-X18)","v":9.0641386873514129}," ",{"$f":"+Z19","v":-4},{"$f":"V20*Z20+X20","v":9.4020893437714932}]
[null,null,null,"X",{"$f":"0.26*E13/2","v":1.56},{"$f":"+E21","v":1.56},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(X20-X19)/(V19-V20)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+V20*V21+X20","v":{"$error":"#VALUE!"}}]
[null,null,null,"Y",{"$f":"+(0.26*E14/2)","v":0.37700028599999996},{"$f":"(E14-0.26*E14/2)","v":2.5230019139999995}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"               Vrijednosti s na pravcu napona",null,null,null,"Slijeganje u karak. točkama"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y","x"]
[null,null,"SLOJEVI TLA DO DNA TEMELJA",null,null,null,"KARAKTERISTIKE SLOJEVA ISPOD TEMELJA",null,null,null,null,null,null,"x","y",null,null,null,null,null,null,"K1",{"$f":"+S19","v":0.40950028599999994},{"$f":"-X19/V19+W25/V19","v":{"$error":"#VALUE!"}},null,null,"K1",{"$f":"+F66","v":{"$error":"#VALUE!"}},"cm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"K2",{"$f":"+S20","v":2.7405019139999993},{"$f":"-X19/V19+W26/V19","v":{"$error":"#VALUE!"}},null,null,"K2",{"$f":"+G66","v":{"$error":"#VALUE!"}},"cm"]
[null,null,"Sloj"," Hi (m)","g (kN/m3)","pg (kPa)","Sloj"," Hi (m)","g (kN/m3)","Msi (kN/m2)",null,null,"T1",{"$f":"+E18-E13/2","v":0},{"$f":"+E19-E14/2","v":0},null,null,null,null,null,null,"Ds=",{"$f":"+W26-W25","v":2.3310016279999992},{"$f":"+X26-X25","v":{"$error":"#VALUE!"}},null,null,"temelj  Dw=",{"$f":"+AB26-AB25","v":{"$error":"#VALUE!"}},"cm"]
[null,null,1,{"$f":"+('Analiza i dimenzioniranje'!$E$52+'Unos podataka'!$F$54)/2","v":0.75},{"$f":"+'Analiza i dimenzioniranje'!$F$16","v":20},{"$f":"+D28*E28","v":15},3,1,{"$f":"+'Analiza i dimenzioniranje'!$G$16","v":20},{"$f":"+'Unos podataka'!F12","v":8000},null,null,null,{"$f":"+E18+E13/2","v":12},{"$f":"+O27","v":0},null,null,null,null,null,null,"               Visine temelja u tokama K1 i K2"]
[null,null,2,{"$f":"+D28","v":0.75},{"$f":"+E28","v":20},null,4,1,{"$f":"+'Analiza i dimenzioniranje'!$H$17","v":10},{"$f":"+J28","v":8000},null,null,null,{"$f":"+N28","v":12},{"$f":"+E19+E14/2","v":2.9000021999999994},null,null,null,null,null,null,null,"Y","x",null,null,"pomak na vrhu zida Dw=",{"$f":"IF('Analiza i dimenzioniranje'!D71=\"\",+AB27*('Analiza i dimenzioniranje'!E48)/'Analiza i dimenzioniranje'!G240,+AB27*('Analiza i dimenzioniranje'!E48-'Analiza i dimenzioniranje'!D71)/'Analiza i dimenzioniranje'!G240)","v":{"$error":"#VALUE!"}},"cm"]
[null,null,null,"g*h=",{"$f":"+D28*E28+D29*E29","v":30},null,5,2,{"$f":"+I29","v":10},{"$f":"+J29","v":8000},null,null,null,{"$f":"+N31","v":0},{"$f":"+O29","v":2.9000021999999994},null,null,null,null,null,null,"K1",{"$f":"+W25","v":0.40950028599999994},{"$f":"IF('Analiza i dimenzioniranje'!E52='Analiza i dimenzioniranje'!E51,'Analiza i dimenzioniranje'!E52,(-X20/V20+W25/V20)/100)","v":1.0243671064918414},null,"rastezanje sidara",null,{"$f":"IF(Sidra!H12=\"\",0,+IF(Sidra!H12>0,Sidra!H13,IF(Sidra!I12>0,Sidra!I13,IF(Sidra!J12>0,Sidra!J13,IF(Sidra!K12>0,Sidra!K13,IF(Sidra!L12>0,Sidra!L13))))))/10","v":0.48582094960896011},"cm"]
[null,null,null,"NIVO PODZEMNE VODE -",{"$f":"+'Analiza i dimenzioniranje'!E41","v":0.6},"m",6,2,{"$f":"+I30","v":10},{"$f":"+J30","v":8000},null,null,null,{"$f":"+N27","v":0},{"$f":"+O27","v":0},null,null,null,null,null,null,"K2",{"$f":"+W26","v":2.7405019139999993},{"$f":"IF('Analiza i dimenzioniranje'!E52='Analiza i dimenzioniranje'!E51,'Analiza i dimenzioniranje'!E52,(-X20/V20+W26/V20)/100)","v":0.74846864809648228},null,"Ukupno",null,{"$f":"+AB29+AB30","v":{"$error":"#VALUE!"}},"cm"]
[null,null,null,null,null,null,7,2,{"$f":"+I31","v":10},{"$f":"+J31","v":8000}]
[null,null,null,null,null,null,8,0.01,{"$f":"+I32","v":10},{"$f":"+J32","v":8000}]
[]
["  SHEMATSKI TLOCRT TEMELJA I TOČAKA U KOJIMA SE RAČUNA SLIJEGANJE"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"  SLIJEGANJE TLA U ODABRANIM TOČKAMA (cm)"]
[]
[null,"SLOJ","pg (kPa)","0,2 pg ","zi (m)","K1","K2","TS3","TS4","TS5","TS6","TS7","TS8"]
[null,3,{"$f":"+'T1'!G23","v":40},{"$f":"+'T1'!J23","v":8},{"$f":"+'T1'!F23","v":0.5},{"$f":"+($H$28*C74/$J$28)*100","v":{"$error":"#VALUE!"}},{"$f":"+$H$28*D74/$J$28*100","v":{"$error":"#VALUE!"}}]
[null,4,{"$f":"+'T1'!G24","v":55},{"$f":"+'T1'!J24","v":11},{"$f":"+'T1'!F24","v":1.5},{"$f":"+$H$29*C75/$J$29*100","v":{"$error":"#VALUE!"}},{"$f":"+$H$29*D75/$J$29*100","v":{"$error":"#VALUE!"}}]
[null,5,{"$f":"+'T1'!G25","v":70},{"$f":"+'T1'!J25","v":14},{"$f":"+'T1'!F25","v":3},{"$f":"+$H$30*C76/$J$30*100","v":{"$error":"#VALUE!"}},{"$f":"+$H$30*D76/$J$30*100","v":{"$error":"#VALUE!"}}]
[null,6,{"$f":"+'T1'!G26","v":90},{"$f":"+'T1'!J26","v":18},{"$f":"+'T1'!F26","v":5},{"$f":"+$H$31*C77/$J$31*100","v":{"$error":"#VALUE!"}},{"$f":"+$H$31*D77/$J$31*100","v":{"$error":"#VALUE!"}}]
[null,7,{"$f":"+'T1'!G27","v":110},{"$f":"+'T1'!J27","v":22},{"$f":"+'T1'!F27","v":7},{"$f":"+$H$32*C78/$J$32*100","v":{"$error":"#VALUE!"}},{"$f":"+$H$32*D78/$J$32*100","v":{"$error":"#VALUE!"}}]
[null,8,{"$f":"+'T1'!G28","v":120.05},{"$f":"+'T1'!J28","v":24.01},{"$f":"+'T1'!F28","v":8.0050000000000008},{"$f":"+$H$33*C79/$J$33*100","v":{"$error":"#VALUE!"}},{"$f":"+$H$33*D79/$J$33*100","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"SW =",{"$f":"SUM(F60:F65)","v":{"$error":"#VALUE!"}},{"$f":"SUM(G60:G65)","v":{"$error":"#VALUE!"}}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+E15","v":1.5001009999999999}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+O69","v":1.5001009999999999}]
["  DODATNA NAPREZANJA U SREDINI SLOJA (kPa)",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+O69","v":1.5001009999999999}]
[null,null,null,null,null,null,null,null,null,null,null,"Slijeg ","razmak","Ds"]
[null,"SLOJ","TS1","TS2","TS3","TS4","TS5","TS6","TS7","TS8","K1",{"$f":"+F66","v":{"$error":"#VALUE!"}},{"$f":"'Analiza i dimenzioniranje'!C185*100","v":315.00021999999996},{"$f":"+L74-L73","v":{"$error":"#VALUE!"}}]
[null,3,{"$f":"+'T1'!H23","v":{"$error":"#VALUE!"}},{"$f":"+'T2'!H23","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,"K2",{"$f":"+G66","v":{"$error":"#VALUE!"}}]
[null,4,{"$f":"+'T1'!H24","v":{"$error":"#VALUE!"}},{"$f":"+'T2'!H24","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"tgj",{"$f":"N73/M73","v":{"$error":"#VALUE!"}}]
[null,5,{"$f":"+'T1'!H25","v":{"$error":"#VALUE!"}},{"$f":"+'T2'!H25","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"j",{"$f":"IF(ATAN(M75)*180/PI()<0,0,ATAN(M75)*180/PI())","v":{"$error":"#VALUE!"}},"⁰"]
[null,6,{"$f":"+'T1'!H26","v":{"$error":"#VALUE!"}},{"$f":"+'T2'!H26","v":{"$error":"#VALUE!"}}]
[null,7,{"$f":"+'T1'!H27","v":{"$error":"#VALUE!"}},{"$f":"+'T2'!H27","v":{"$error":"#VALUE!"}}]
[null,8,{"$f":"+'T1'!H28","v":{"$error":"#VALUE!"}},{"$f":"+'T2'!H28","v":{"$error":"#VALUE!"}}]
[]
[]
["  DIJAGRAM DODATNIH NAPREZANJA ISPOD ODABRANIH TOČAKA"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Df"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+N89/2","v":100}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,200]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"z"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+O115+D28","v":0.75}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+O116+D29","v":1.5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+O117+H28","v":2.5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5]
["TS1","TS2","TS3","TS4","TS5","TS6","TS7","Priredio:","Nikola SAPUNAR, dipl. ing. građ.",null,null,null,null,null,9.5]
[null,null,null,null,null,null,null,null,0,{"$f":"+I123*0.2","v":0},0,0,0,null,9.51]
[null,null,null,null,null,null,null,null,{"$f":"+F28","v":15},3,{"$f":"+D28","v":0.75},{"$f":"+D28*E28","v":15},{"$f":"+D28","v":0.75}]
[{"$f":"+E17","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},0,0,0,0,0,0,{"$f":"+E30","v":30},6,{"$f":"+E15","v":1.5001009999999999},{"$f":"+L124+D29*E29","v":30},{"$f":"+K125","v":1.5001009999999999}]
[{"$f":"+C74","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},0,0,0,0,0,0,{"$f":"+C60","v":40},8,{"$f":"+E60+$K$125","v":2.0001009999999999},{"$f":"+L125+H28*I28","v":50},2.0001009999999999]
[{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,0,0,0,0,55,11,3.0001009999999999,60,3.0001009999999999]
[{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,0,0,0,0,70,14,4.5001009999999999,80,4.5001009999999999]
[{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,0,0,0,0,90,18,6.5001009999999999,100,6.5001009999999999]
[{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,0,0,0,0,110,22,8.5001010000000008,120,8.5001010000000008]
[{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,0,0,0,0,120.05,24.01,9.5051009999999998,120.1,9.5051009999999998]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"0,2*pg"]
[null,null,null,null,"NPV",null,null,null,null,null,null,null,null,{"$f":"+L123*0.2","v":0}]
[null,null,null,null,0,{"$f":"+E31","v":0.6},null,null,null,null,null,null,null,3]
[null,null,null,null,{"$f":"+E17+50","v":{"$error":"#VALUE!"}},{"$f":"+F134","v":0.6},null,null,null,null,null,null,null,6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,10]
["Sloj 1",null,"Sloj 2 ",null,"Sloj 3",null,"Sloj 4",null,"Sloj 5",null,"Sloj 6",null,null,12]
[0,{"$f":"+D28","v":0.75},0,{"$f":"+D28+D29","v":1.5},0,{"$f":"+D138+H28","v":2.5},{"$f":"+E138","v":0},{"$f":"+F138+H29","v":3.5},{"$f":"+G138","v":0},{"$f":"+H138+H30","v":5.5},{"$f":"+I138","v":0},{"$f":"+J138+H31","v":7.5},null,16]
[{"$f":"+E135","v":{"$error":"#VALUE!"}},{"$f":"+B138","v":0.75},{"$f":"+A139","v":{"$error":"#VALUE!"}},{"$f":"+D138","v":1.5},{"$f":"+C139","v":{"$error":"#VALUE!"}},{"$f":"+F138","v":2.5},{"$f":"+E139","v":{"$error":"#VALUE!"}},{"$f":"+H138","v":3.5},{"$f":"+G139","v":{"$error":"#VALUE!"}},{"$f":"+J138","v":5.5},{"$f":"+I139","v":{"$error":"#VALUE!"}},{"$f":"+L138","v":7.5},null,20]
[",",null,null,null,null,null,null,null,null,null,null,null,null,24]
[null,null,null,null,null,null,null,null,"Sloj 7",null,"Sloj 8",null,null,24.02]
[null,null,null,null,null,null,null,null,{"$f":"+I138","v":0},{"$f":"+L138+H32","v":9.5},{"$f":"+K138","v":0},{"$f":"+J142+H33","v":9.51}]
[null,null,null,null,null,null,null,null,{"$f":"+I139","v":{"$error":"#VALUE!"}},{"$f":"+J142","v":9.5},{"$f":"+K139","v":{"$error":"#VALUE!"}},{"$f":"+L142","v":9.51}]

{"sheet":"T1","index":33,"n_rows":378,"n_cols":22,"rows_kept":378,"cut":false,"hidden":true,"merged":[[292,2,292,3],[292,4,292,5],[338,2,338,3],[338,4,338,5],[154,2,154,3],[154,4,154,5],[200,2,200,3],[200,4,200,5],[246,2,246,3],[246,4,246,5],[16,2,16,3],[16,4,16,5],[62,2,62,3],[62,4,62,5],[108,2,108,3],[108,4,108,5]]}
["Dimenzije temelja:",null,"T1","T2","T3","T4","T5","T6","T7","T8"]
[null,"L",{"$f":"+Slijeganje!E13","v":12},{"$f":"+Slijeganje!F13","v":12},{"$f":"+Slijeganje!G13","v":0},{"$f":"+Slijeganje!H13","v":0},{"$f":"+Slijeganje!I13","v":0},{"$f":"+Slijeganje!J13","v":0},{"$f":"+Slijeganje!K13","v":0},{"$f":"+Slijeganje!L13","v":0}]
[null,"B",{"$f":"+Slijeganje!E14","v":2.9000021999999994},{"$f":"+Slijeganje!F14","v":2.9000021999999994},{"$f":"+Slijeganje!G14","v":0},{"$f":"+Slijeganje!H14","v":0},{"$f":"+Slijeganje!I14","v":0},{"$f":"+Slijeganje!J14","v":0},{"$f":"+Slijeganje!K14","v":0},{"$f":"+Slijeganje!L14","v":0}]
[null,"Df=",{"$f":"+Slijeganje!E15","v":1.5001009999999999},{"$f":"+Slijeganje!F15","v":1.5001009999999999},{"$f":"+Slijeganje!G15","v":0},{"$f":"+Slijeganje!H15","v":0},{"$f":"+Slijeganje!I15","v":0},{"$f":"+Slijeganje!J15","v":0},{"$f":"+Slijeganje!K15","v":0},{"$f":"+Slijeganje!L15","v":0}]
["opterećenje: /kn/m2/",null,{"$f":"+Slijeganje!E17","v":{"$error":"#VALUE!"}},{"$f":"+Slijeganje!F17","v":{"$error":"#VALUE!"}},{"$f":"+Slijeganje!G17","v":0},{"$f":"+Slijeganje!H17","v":0},{"$f":"+Slijeganje!I17","v":0},{"$f":"+Slijeganje!J17","v":0},{"$f":"+Slijeganje!K17","v":0},{"$f":"+Slijeganje!L17","v":0}]
["Težište temelja      x",null,{"$f":"+Slijeganje!E18","v":6},{"$f":"+Slijeganje!F18","v":6},{"$f":"+Slijeganje!G18","v":0},{"$f":"+Slijeganje!H18","v":0},{"$f":"+Slijeganje!I18","v":0},{"$f":"+Slijeganje!J18","v":0},{"$f":"+Slijeganje!K18","v":0},{"$f":"+Slijeganje!L18","v":0}]
[null,"y",{"$f":"+Slijeganje!E19","v":1.4500010999999997},{"$f":"+Slijeganje!F19","v":1.4500010999999997},{"$f":"+Slijeganje!G19","v":0},{"$f":"+Slijeganje!H19","v":0},{"$f":"+Slijeganje!I19","v":0},{"$f":"+Slijeganje!J19","v":0},{"$f":"+Slijeganje!K19","v":0},{"$f":"+Slijeganje!L19","v":0}]
["Točka u kojoj se",null,"TS1"]
["računa slijeganje    x",null,{"$f":"+Slijeganje!E21","v":1.56}]
[null,"y",{"$f":"+Slijeganje!E22","v":0.37700028599999996}]
[null,"xL",{"$f":"+ABS($C$9-C6)/C2*2","v":0.73999999999999988},{"$f":"+ABS($C$9-D6)/D2*2","v":0.73999999999999988}]
[null,"yB",{"$f":"ABS($C$10-C7)/C3*2","v":0.74},{"$f":"ABS($C$10-D7)/D3*2","v":0.74}]
[]
[]
[null,null,"SLIJEGANJE TOČKE K1 OD TEMELJA T1",null,null,null,null,null,"       x=L/2*",{"$f":"+C11","v":0.73999999999999988},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"+C12","v":0.74}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!E13","v":12},"m         Dpa'=",{"$f":"+Slijeganje!E17","v":{"$error":"#VALUE!"}},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!E14","v":2.9000021999999994},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O41*O41)+(O42*O42)+(H43*H43))","v":10.752169021088147},{"$f":"SQRT((O41*O41)+(O46*O46)+(H43*H43))","v":10.458763273716643},{"$f":"SQRT((O45*O45)+(O46*O46)+(H43*H43))","v":1.6809905459710603},{"$f":"SQRT((O45*O45)+(O42*O42)+(H43*H43))","v":3.0081786280152416},{"$f":"H43*O41*O42*((O41*O41)+(O42*O42)+(2*H43*H43))/(((O41*O41)+(H43*H43))*((O42*O42)+(H43*H43))*O19)","v":0.19636364301930606},{"$f":"H43*O41*O46*((O41*O41)+(O46*O46)+(2*H43*H43))/(((O41*O41)+(H43*H43))*((O46*O46)+(H43*H43))*P19)","v":-0.48156925795510397},{"$f":"H43*O45*O46*((O45*O45)+(O46*O46)+(2*H43*H43))/(((O45*O45)+(H43*H43))*((O46*O46)+(H43*H43))*Q19)","v":0.51129568251091073},{"$f":"H43*O45*O42*((O45*O45)+(O42*O42)+(2*H43*H43))/(((O45*O45)+(H43*H43))*((O42*O42)+(H43*H43))*R19)","v":-0.34266384985112436}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!E15","v":1.5001009999999999},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O41*O41)+(O42*O42)+(H44*H44))","v":10.844774716795534},{"$f":"SQRT((O41*O41)+(O46*O46)+(H44*H44))","v":10.553943775463468},{"$f":"SQRT((O45*O45)+(O46*O46)+(H44*H44))","v":2.1967542456187683},{"$f":"SQRT((O45*O45)+(O42*O42)+(H44*H44))","v":3.3240244671253043},{"$f":"H44*O41*O42*((O41*O41)+(O42*O42)+(2*H44*H44))/(((O41*O41)+(H44*H44))*((O42*O42)+(H44*H44))*O20)","v":0.45561969101701461},{"$f":"H44*O41*O46*((O41*O41)+(O46*O46)+(2*H44*H44))/(((O41*O41)+(H44*H44))*((O46*O46)+(H44*H44))*P20)","v":-0.23887675696849342},{"$f":"H44*O45*O46*((O45*O45)+(O46*O46)+(2*H44*H44))/(((O45*O45)+(H44*H44))*((O46*O46)+(H44*H44))*Q20)","v":0.25361961236358982},{"$f":"H44*O45*O42*((O45*O45)+(O42*O42)+(2*H44*H44))/(((O45*O45)+(H44*H44))*((O42*O42)+(H44*H44))*R20)","v":-0.5853700614304056}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O41*O41)+(O42*O42)+(H45*H45))","v":11.151642868118026},{"$f":"SQRT((O41*O41)+(O46*O46)+(H45*H45))","v":10.869026139247438},{"$f":"SQRT((O45*O45)+(O46*O46)+(H45*H45))","v":3.4023123336407672},{"$f":"SQRT((O45*O45)+(O42*O42)+(H45*H45))","v":4.2189025418996895},{"$f":"H45*O41*O42*((O41*O41)+(O42*O42)+(2*H45*H45))/(((O41*O41)+(H45*H45))*((O42*O42)+(H45*H45))*O21)","v":0.52121513855296753},{"$f":"H45*O41*O46*((O41*O41)+(O46*O46)+(2*H45*H45))/(((O41*O41)+(H45*H45))*((O46*O46)+(H45*H45))*P21)","v":-0.12803674097832882},{"$f":"H45*O45*O46*((O45*O45)+(O46*O46)+(2*H45*H45))/(((O45*O45)+(H45*H45))*((O46*O46)+(H45*H45))*Q21)","v":0.1020794306640232},{"$f":"H45*O45*O42*((O45*O45)+(O42*O42)+(2*H45*H45))/(((O45*O45)+(H45*H45))*((O42*O42)+(H45*H45))*R21)","v":-0.42692736365192813}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O41*O41)+(O42*O42)+(H46*H46))","v":11.847326224007155},{"$f":"SQRT((O41*O41)+(O46*O46)+(H46*H46))","v":11.581698028166857},{"$f":"SQRT((O45*O45)+(O46*O46)+(H46*H46))","v":5.2512597741536347},{"$f":"SQRT((O45*O45)+(O42*O42)+(H46*H46))","v":5.8137026633676117},{"$f":"H46*O41*O42*((O41*O41)+(O42*O42)+(2*H46*H46))/(((O41*O41)+(H46*H46))*((O42*O42)+(H46*H46))*O22)","v":0.43738021268409849},{"$f":"H46*O41*O46*((O41*O41)+(O46*O46)+(2*H46*H46))/(((O41*O41)+(H46*H46))*((O46*O46)+(H46*H46))*P22)","v":-8.0264135870411507E-2},{"$f":"H46*O45*O46*((O45*O45)+(O46*O46)+(2*H46*H46))/(((O45*O45)+(H46*H46))*((O46*O46)+(H46*H46))*Q22)","v":4.2684797783968532E-2},{"$f":"H46*O45*O42*((O45*O45)+(O42*O42)+(2*H46*H46))/(((O45*O45)+(H46*H46))*((O42*O42)+(H46*H46))*R22)","v":-0.23131019679513548}]
[null,1,{"$f":"+Slijeganje!H28","v":1},{"$f":"+Slijeganje!I28","v":20},{"$f":"+Slijeganje!J28","v":8000},{"$f":"IF(H43=0,\"   \",+H43)","v":0.5},{"$f":"IF(D50=0,\"       \",+D50)","v":40},{"$f":"F50","v":{"$error":"#VALUE!"}},{"$f":"H50","v":{"$error":"#VALUE!"}},{"$f":"+J50","v":8}]
[null,{"$f":"IF(H44=(H43+C23/2),\"\",2)","v":2},{"$f":"+Slijeganje!H29","v":1},{"$f":"+Slijeganje!I29","v":10},{"$f":"+Slijeganje!J29","v":8000},{"$f":"IF(H44=H43,\"   \",+H44)","v":1.5},{"$f":"IF(D51=D50,\"       \",+D51)","v":55},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+J51","v":11}]
[null,{"$f":"IF(H45=(H44+C24/2),\"\",3)","v":3},{"$f":"+Slijeganje!H30","v":2},{"$f":"+Slijeganje!I30","v":10},{"$f":"+Slijeganje!J30","v":8000},{"$f":"IF(H45=H44,\"   \",+H45)","v":3},{"$f":"IF(D52=D51,\"       \",+D52)","v":70},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+J52","v":14},null,null,null,null,{"$f":"SQRT((O41*O41)+(O42*O42)+(H47*H47))","v":12.820262815482669},{"$f":"SQRT((O41*O41)+(O46*O46)+(H47*H47))","v":12.575202949282531},{"$f":"SQRT((O45*O45)+(O46*O46)+(H47*H47))","v":7.1816244134348937},{"$f":"SQRT((O45*O45)+(O42*O42)+(H47*H47))","v":7.6025744756659677},{"$f":"H47*O41*O42*((O41*O41)+(O42*O42)+(2*H47*H47))/(((O41*O41)+(H47*H47))*((O42*O42)+(H47*H47))*O25)","v":0.35079340123228608},{"$f":"H47*O41*O46*((O41*O41)+(O46*O46)+(2*H47*H47))/(((O41*O41)+(H47*H47))*((O46*O46)+(H47*H47))*P25)","v":-5.845030324916508E-2},{"$f":"H47*O45*O46*((O45*O45)+(O46*O46)+(2*H47*H47))/(((O45*O45)+(H47*H47))*((O46*O46)+(H47*H47))*Q25)","v":2.2810453885631181E-2},{"$f":"H47*O45*O42*((O45*O45)+(O42*O42)+(2*H47*H47))/(((O45*O45)+(H47*H47))*((O42*O42)+(H47*H47))*R25)","v":-0.13591294801022338}]
[null,{"$f":"IF(H46=(H45+C25/2),\"\",4)","v":4},{"$f":"+Slijeganje!H31","v":2},{"$f":"+Slijeganje!I31","v":10},{"$f":"+Slijeganje!J31","v":8000},{"$f":"IF(H46=H45,\"   \",+H46)","v":5},{"$f":"IF(D53=D52,\"       \",+D53)","v":90},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D53=D52,\"\",+J53)","v":18},null,null,null,null,{"$f":"SQRT((O41*O41)+(O42*O42)+(H48*H48))","v":13.395490422453657},{"$f":"SQRT((O41*O41)+(O46*O46)+(H48*H48))","v":13.161145627020623},{"$f":"SQRT((O45*O45)+(O46*O46)+(H48*H48))","v":8.1642975335079555},{"$f":"SQRT((O45*O45)+(O42*O42)+(H48*H48))","v":8.5369294045369539},{"$f":"H48*O41*O42*((O41*O41)+(O42*O42)+(2*H48*H48))/(((O41*O41)+(H48*H48))*((O42*O42)+(H48*H48))*O26)","v":0.31439052318616756},{"$f":"H48*O41*O46*((O41*O41)+(O46*O46)+(2*H48*H48))/(((O41*O41)+(H48*H48))*((O46*O46)+(H48*H48))*P26)","v":-5.110743375621709E-2},{"$f":"H48*O45*O46*((O45*O45)+(O46*O46)+(2*H48*H48))/(((O45*O45)+(H48*H48))*((O46*O46)+(H48*H48))*Q26)","v":1.7648498562459976E-2},{"$f":"H48*O45*O42*((O45*O45)+(O42*O42)+(2*H48*H48))/(((O45*O45)+(H48*H48))*((O42*O42)+(H48*H48))*R26)","v":-0.10787696837105963}]
[null,{"$f":"IF(H47=(H46+C26/2),\"\",5)","v":5},{"$f":"+Slijeganje!H32","v":2},{"$f":"+Slijeganje!I32","v":10},{"$f":"+Slijeganje!J32","v":8000},{"$f":"IF(H47=H46,\"   \",+H47)","v":7},{"$f":"IF(D54=D53,\"       \",+D54)","v":110},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D54=D53,\"\",+J54)","v":22},null,null,null,null,{"$f":"ATAN((O41*O42)/(H43*O19))","v":1.3694593280275096},{"$f":"ATAN((O41*O46)/(H43*P19))","v":-0.64519359719234393},{"$f":"ATAN((O45*O46)/(H43*Q19))","v":0.61054528349481807},{"$f":"ATAN((O45*O42)/(H43*R19))","v":-1.2057738009809331}]
[null,{"$f":"IF(H48=(H47+C27/2),\"\",6)","v":6},{"$f":"+Slijeganje!H33","v":0.01},{"$f":"+Slijeganje!I33","v":10},{"$f":"+Slijeganje!J33","v":8000},{"$f":"IF(H48=H47,\"   \",+H48)","v":8.0050000000000008},{"$f":"IF(D55=D54,\"       \",+D55)","v":120.05},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D55=D54,\"\",+J55)","v":24.01},null,null,null,null,{"$f":"ATAN((O41*O42)/(H44*O20))","v":1.0175500375717115},{"$f":"ATAN((O41*O46)/(H44*P20))","v":-0.24367946210134675},{"$f":"ATAN((O45*O46)/(H44*Q20))","v":0.17662183950321556},{"$f":"ATAN((O45*O42)/(H44*R20))","v":-0.66823236211286796}]
[null,null,null,null,null,null,null,"  S W =",{"$error":"#VALUE!"},"m ",null,null,null,null,{"$f":"ATAN((O41*O42)/(H45*O21))","v":0.66696875500848141},{"$f":"ATAN((O41*O46)/(H45*P21))","v":-0.12012523800910783},{"$f":"ATAN((O45*O46)/(H45*Q21))","v":5.7556040648313406E-2},{"$f":"ATAN((O45*O42)/(H45*R21))","v":-0.3014923003067399}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O41*O42)/(H46*O22))","v":0.41840402748355454},{"$f":"ATAN((O41*O46)/(H46*P22))","v":-6.7862916946734964E-2},{"$f":"ATAN((O45*O46)/(H46*Q22))","v":2.2395468624673166E-2},{"$f":"ATAN((O45*O42)/(H46*R22))","v":-0.13458175982630699}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O41*O42)/(H47*O25))","v":0.28549221161305105},{"$f":"ATAN((O41*O46)/(H47*P25))","v":-4.4682757904761075E-2},{"$f":"ATAN((O45*O46)/(H47*Q25))","v":1.1698380349486639E-2},{"$f":"ATAN((O45*O42)/(H47*R25))","v":-7.3823307548584932E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O41*O42)/(H48*O26))","v":0.24087042826675767},{"$f":"ATAN((O41*O46)/(H48*P26))","v":-3.7340938551026569E-2},{"$f":"ATAN((O45*O46)/(H48*Q26))","v":8.9985885744867274E-3},{"$f":"ATAN((O45*O42)/(H48*R26))","v":-5.7530697805092901E-2}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E18","v":12},"m",null,null,null,null,{"$f":"E18/2","v":6}]
[null,null,"     širina temelja  B=",{"$f":"E19","v":2.9000021999999994},"m",null,null,null,null,{"$f":"E19/2","v":1.4500010999999997}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G18","v":{"$error":"#VALUE!"}},"kPa",null,null,null,null,{"$f":"J15*J35","v":4.4399999999999995}]
[null,null,"      dubina temeljenja Df=",{"$f":"E20","v":1.5001009999999999},"m",null,null,null,null,{"$f":"J16*J36","v":1.0730008139999998}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J37+J35","v":10.44}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J38+J36","v":2.5230019139999995}]
[1,null,"      H1=",{"$f":"IF(C23=0,\"      \",C23)","v":1},"m        Mk1=",{"$f":"IF(E23=0,\"       \",+E23)","v":8000},"KN/m2     z1=",{"$f":"C23/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C23+C24/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C23+C24+C25/2","v":3},"m",null,null,null,null,null,{"$f":"J37-J35","v":-1.5600000000000005}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C23+C24+C25+C26/2","v":5},"m",null,null,null,null,null,{"$f":"J38-J36","v":-0.37700028599999991}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C23+C24+C25+C26+C27/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C23+C24+C25+C26+C27+C28/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O27)-(P27)+(Q27)-(R27)+(S19)-(T19)+(U19)-(V19))/(2*3.14159)","v":0.85352710618381922},{"$f":"Slijeganje!E30+D23*C23/2","v":40},"kPa     Dp1=",{"$f":"(G18)*C50","v":{"$error":"#VALUE!"}},"kPa        w1=",{"$f":"IF(E23=0,\"       \",+F50*C23/E23)","v":{"$error":"#VALUE!"}},"m",{"$f":"0.2*D50","v":8}]
[null,"    I42=",{"$f":"((O28)-(P28)+(Q28)-(R28)+(S20)-(T20)+(U20)-(V20))/(2*3.14159)","v":0.57925601734609633},{"$f":"Slijeganje!E30+D23*C23+D24*C24/2","v":55},"kPa     Dp2=",{"$f":"IF(H44=H43,\"     \",(G18)*C51)","v":{"$error":"#VALUE!"}},"kPa       w2=",{"$error":"#VALUE!"},"m",11]
[null,"    I43=",{"$f":"((O29)-(P29)+(Q29)-(R29)+(S21)-(T21)+(U21)-(V21))/(2*3.14159)","v":0.36994022259745701},{"$f":"Slijeganje!E30+D23*C23+D24*C24+D25*C25/2","v":70},"kPa     Dp3=",{"$f":"IF(H45=H44,\"     \",(G18)*C52)","v":{"$error":"#VALUE!"}},"kPa       w3=",{"$error":"#VALUE!"},"m",14]
[null,"    I44=",{"$f":"((O30)-(P30)+(Q30)-(R30)+(S22)-(T22)+(U22)-(V22))/(2*3.14159)","v":0.22836899722988735},{"$f":"Slijeganje!E30+D23*C23+D24*C24+D25*C25+D26*C26/2","v":90},"kPa     Dp4=",{"$f":"IF(H46=H45,\"     \",(G18)*C53)","v":{"$error":"#VALUE!"}},"kPa       w4=",{"$error":"#VALUE!"},"m",18]
[null,"    I45=",{"$f":"((O31)-(P31)+(Q31)-(R31)+(S25)-(T25)+(U25)-(V25))/(2*3.14159)","v":0.15655508258448581},{"$f":"Slijeganje!E30+D23*C23+D24*C24+D25*C25+D26*C26+D27*C27/2","v":110},"kPa     Dp5=",{"$f":"IF(H47=H46,\"     \",(G18)*C54)","v":{"$error":"#VALUE!"}},"kPa       w5=",{"$error":"#VALUE!"},"m",22]
[null,"    I46=",{"$f":"((P32)-(Q32)+(R32)-(S32)+(S26)-(T26)+(U26)-(V26))/(2*3.14159)","v":0.13301609647873661},{"$f":"Slijeganje!E30+D23*C23+D24*C24+D25*C25+D26*C26+D27*C27+D28*C28/2","v":120.05},"kPa     Dp6=",{"$f":"IF(H48=H47,\"       \",(G18)*C55)","v":{"$error":"#VALUE!"}},"kPa       w6=",{"$error":"#VALUE!"},"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H50:H55)","v":{"$error":"#VALUE!"}},"m"]
[]
[]
[]
[]
[null,null,"SLIJEGANJE TOČKE K1 OD TEMELJA T1",null,null,null,null,null,"       x=L/2*",{"$f":"D11","v":0.73999999999999988},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"D12","v":0.74}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!F13","v":12},"m         Dpa'=",{"$f":"+Slijeganje!F17","v":{"$error":"#VALUE!"}},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!F14","v":2.9000021999999994},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O87*O87)+(O88*O88)+(H89*H89))","v":10.752169021088147},{"$f":"SQRT((O87*O87)+(O92*O92)+(H89*H89))","v":10.458763273716643},{"$f":"SQRT((O91*O91)+(O92*O92)+(H89*H89))","v":1.6809905459710603},{"$f":"SQRT((O91*O91)+(O88*O88)+(H89*H89))","v":3.0081786280152416},{"$f":"H89*O87*O88*((O87*O87)+(O88*O88)+(2*H89*H89))/(((O87*O87)+(H89*H89))*((O88*O88)+(H89*H89))*O65)","v":0.19636364301930606},{"$f":"H89*O87*O92*((O87*O87)+(O92*O92)+(2*H89*H89))/(((O87*O87)+(H89*H89))*((O92*O92)+(H89*H89))*P65)","v":-0.48156925795510397},{"$f":"H89*O91*O92*((O91*O91)+(O92*O92)+(2*H89*H89))/(((O91*O91)+(H89*H89))*((O92*O92)+(H89*H89))*Q65)","v":0.51129568251091073},{"$f":"H89*O91*O88*((O91*O91)+(O88*O88)+(2*H89*H89))/(((O91*O91)+(H89*H89))*((O88*O88)+(H89*H89))*R65)","v":-0.34266384985112436}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!F15","v":1.5001009999999999},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O87*O87)+(O88*O88)+(H90*H90))","v":10.844774716795534},{"$f":"SQRT((O87*O87)+(O92*O92)+(H90*H90))","v":10.553943775463468},{"$f":"SQRT((O91*O91)+(O92*O92)+(H90*H90))","v":2.1967542456187683},{"$f":"SQRT((O91*O91)+(O88*O88)+(H90*H90))","v":3.3240244671253043},{"$f":"H90*O87*O88*((O87*O87)+(O88*O88)+(2*H90*H90))/(((O87*O87)+(H90*H90))*((O88*O88)+(H90*H90))*O66)","v":0.45561969101701461},{"$f":"H90*O87*O92*((O87*O87)+(O92*O92)+(2*H90*H90))/(((O87*O87)+(H90*H90))*((O92*O92)+(H90*H90))*P66)","v":-0.23887675696849342},{"$f":"H90*O91*O92*((O91*O91)+(O92*O92)+(2*H90*H90))/(((O91*O91)+(H90*H90))*((O92*O92)+(H90*H90))*Q66)","v":0.25361961236358982},{"$f":"H90*O91*O88*((O91*O91)+(O88*O88)+(2*H90*H90))/(((O91*O91)+(H90*H90))*((O88*O88)+(H90*H90))*R66)","v":-0.5853700614304056}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O87*O87)+(O88*O88)+(H91*H91))","v":11.151642868118026},{"$f":"SQRT((O87*O87)+(O92*O92)+(H91*H91))","v":10.869026139247438},{"$f":"SQRT((O91*O91)+(O92*O92)+(H91*H91))","v":3.4023123336407672},{"$f":"SQRT((O91*O91)+(O88*O88)+(H91*H91))","v":4.2189025418996895},{"$f":"H91*O87*O88*((O87*O87)+(O88*O88)+(2*H91*H91))/(((O87*O87)+(H91*H91))*((O88*O88)+(H91*H91))*O67)","v":0.52121513855296753},{"$f":"H91*O87*O92*((O87*O87)+(O92*O92)+(2*H91*H91))/(((O87*O87)+(H91*H91))*((O92*O92)+(H91*H91))*P67)","v":-0.12803674097832882},{"$f":"H91*O91*O92*((O91*O91)+(O92*O92)+(2*H91*H91))/(((O91*O91)+(H91*H91))*((O92*O92)+(H91*H91))*Q67)","v":0.1020794306640232},{"$f":"H91*O91*O88*((O91*O91)+(O88*O88)+(2*H91*H91))/(((O91*O91)+(H91*H91))*((O88*O88)+(H91*H91))*R67)","v":-0.42692736365192813}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O87*O87)+(O88*O88)+(H92*H92))","v":11.847326224007155},{"$f":"SQRT((O87*O87)+(O92*O92)+(H92*H92))","v":11.581698028166857},{"$f":"SQRT((O91*O91)+(O92*O92)+(H92*H92))","v":5.2512597741536347},{"$f":"SQRT((O91*O91)+(O88*O88)+(H92*H92))","v":5.8137026633676117},{"$f":"H92*O87*O88*((O87*O87)+(O88*O88)+(2*H92*H92))/(((O87*O87)+(H92*H92))*((O88*O88)+(H92*H92))*O68)","v":0.43738021268409849},{"$f":"H92*O87*O92*((O87*O87)+(O92*O92)+(2*H92*H92))/(((O87*O87)+(H92*H92))*((O92*O92)+(H92*H92))*P68)","v":-8.0264135870411507E-2},{"$f":"H92*O91*O92*((O91*O91)+(O92*O92)+(2*H92*H92))/(((O91*O91)+(H92*H92))*((O92*O92)+(H92*H92))*Q68)","v":4.2684797783968532E-2},{"$f":"H92*O91*O88*((O91*O91)+(O88*O88)+(2*H92*H92))/(((O91*O91)+(H92*H92))*((O88*O88)+(H92*H92))*R68)","v":-0.23131019679513548}]
[null,1,{"$f":"+$C$23","v":1},{"$f":"+$D$23","v":20},{"$f":"+$E$23","v":8000},{"$f":"IF(H89=0,\"   \",+H89)","v":0.5},{"$f":"IF(D96=0,\"       \",+D96)","v":40},{"$f":"F96","v":{"$error":"#VALUE!"}},{"$f":"H96","v":{"$error":"#VALUE!"}},{"$f":"+J96","v":8}]
[null,{"$f":"IF(H90=(H89+C69/2),\"\",2)","v":2},{"$f":"+$C$24","v":1},{"$f":"+$D$24","v":10},{"$f":"+$E$24","v":8000},{"$f":"IF(H90=H89,\"   \",+H90)","v":1.5},{"$f":"IF(D97=D96,\"       \",+D97)","v":55},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+J97","v":11}]
[null,{"$f":"IF(H91=(H90+C70/2),\"\",3)","v":3},{"$f":"+$C$25","v":2},{"$f":"+$D$25","v":10},{"$f":"+$E$25","v":8000},{"$f":"IF(H91=H90,\"   \",+H91)","v":3},{"$f":"IF(D98=D97,\"       \",+D98)","v":70},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+J98","v":14},null,null,null,null,{"$f":"SQRT((O87*O87)+(O88*O88)+(H93*H93))","v":12.820262815482669},{"$f":"SQRT((O87*O87)+(O92*O92)+(H93*H93))","v":12.575202949282531},{"$f":"SQRT((O91*O91)+(O92*O92)+(H93*H93))","v":7.1816244134348937},{"$f":"SQRT((O91*O91)+(O88*O88)+(H93*H93))","v":7.6025744756659677},{"$f":"H93*O87*O88*((O87*O87)+(O88*O88)+(2*H93*H93))/(((O87*O87)+(H93*H93))*((O88*O88)+(H93*H93))*O71)","v":0.35079340123228608},{"$f":"H93*O87*O92*((O87*O87)+(O92*O92)+(2*H93*H93))/(((O87*O87)+(H93*H93))*((O92*O92)+(H93*H93))*P71)","v":-5.845030324916508E-2},{"$f":"H93*O91*O92*((O91*O91)+(O92*O92)+(2*H93*H93))/(((O91*O91)+(H93*H93))*((O92*O92)+(H93*H93))*Q71)","v":2.2810453885631181E-2},{"$f":"H93*O91*O88*((O91*O91)+(O88*O88)+(2*H93*H93))/(((O91*O91)+(H93*H93))*((O88*O88)+(H93*H93))*R71)","v":-0.13591294801022338}]
[null,{"$f":"IF(H92=(H91+C71/2),\"\",4)","v":4},{"$f":"+$C$26","v":2},{"$f":"+$D$26","v":10},{"$f":"+$E$26","v":8000},{"$f":"IF(H92=H91,\"   \",+H92)","v":5},{"$f":"IF(D99=D98,\"       \",+D99)","v":90},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D99=D98,\"\",+J99)","v":18},null,null,null,null,{"$f":"SQRT((O87*O87)+(O88*O88)+(H94*H94))","v":13.395490422453657},{"$f":"SQRT((O87*O87)+(O92*O92)+(H94*H94))","v":13.161145627020623},{"$f":"SQRT((O91*O91)+(O92*O92)+(H94*H94))","v":8.1642975335079555},{"$f":"SQRT((O91*O91)+(O88*O88)+(H94*H94))","v":8.5369294045369539},{"$f":"H94*O87*O88*((O87*O87)+(O88*O88)+(2*H94*H94))/(((O87*O87)+(H94*H94))*((O88*O88)+(H94*H94))*O72)","v":0.31439052318616756},{"$f":"H94*O87*O92*((O87*O87)+(O92*O92)+(2*H94*H94))/(((O87*O87)+(H94*H94))*((O92*O92)+(H94*H94))*P72)","v":-5.110743375621709E-2},{"$f":"H94*O91*O92*((O91*O91)+(O92*O92)+(2*H94*H94))/(((O91*O91)+(H94*H94))*((O92*O92)+(H94*H94))*Q72)","v":1.7648498562459976E-2},{"$f":"H94*O91*O88*((O91*O91)+(O88*O88)+(2*H94*H94))/(((O91*O91)+(H94*H94))*((O88*O88)+(H94*H94))*R72)","v":-0.10787696837105963}]
[null,{"$f":"IF(H93=(H92+C72/2),\"\",5)","v":5},{"$f":"+$C$27","v":2},{"$f":"+$D$27","v":10},{"$f":"+$E$27","v":8000},{"$f":"IF(H93=H92,\"   \",+H93)","v":7},{"$f":"IF(D100=D99,\"       \",+D100)","v":110},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D100=D99,\"\",+J100)","v":22},null,null,null,null,{"$f":"ATAN((O87*O88)/(H89*O65))","v":1.3694593280275096},{"$f":"ATAN((O87*O92)/(H89*P65))","v":-0.64519359719234393},{"$f":"ATAN((O91*O92)/(H89*Q65))","v":0.61054528349481807},{"$f":"ATAN((O91*O88)/(H89*R65))","v":-1.2057738009809331}]
[null,{"$f":"IF(H94=(H93+C73/2),\"\",6)","v":6},{"$f":"+$C$28","v":0.01},{"$f":"+$D$28","v":10},{"$f":"+$E$28","v":8000},{"$f":"IF(H94=H93,\"   \",+H94)","v":8.0050000000000008},{"$f":"IF(D101=D100,\"       \",+D101)","v":120.05},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D101=D100,\"\",+J101)","v":24.01},null,null,null,null,{"$f":"ATAN((O87*O88)/(H90*O66))","v":1.0175500375717115},{"$f":"ATAN((O87*O92)/(H90*P66))","v":-0.24367946210134675},{"$f":"ATAN((O91*O92)/(H90*Q66))","v":0.17662183950321556},{"$f":"ATAN((O91*O88)/(H90*R66))","v":-0.66823236211286796}]
[null,null,null,null,null,null,null,"  S W =",{"$error":"#VALUE!"},"m ",null,null,null,null,{"$f":"ATAN((O87*O88)/(H91*O67))","v":0.66696875500848141},{"$f":"ATAN((O87*O92)/(H91*P67))","v":-0.12012523800910783},{"$f":"ATAN((O91*O92)/(H91*Q67))","v":5.7556040648313406E-2},{"$f":"ATAN((O91*O88)/(H91*R67))","v":-0.3014923003067399}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O87*O88)/(H92*O68))","v":0.41840402748355454},{"$f":"ATAN((O87*O92)/(H92*P68))","v":-6.7862916946734964E-2},{"$f":"ATAN((O91*O92)/(H92*Q68))","v":2.2395468624673166E-2},{"$f":"ATAN((O91*O88)/(H92*R68))","v":-0.13458175982630699}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O87*O88)/(H93*O71))","v":0.28549221161305105},{"$f":"ATAN((O87*O92)/(H93*P71))","v":-4.4682757904761075E-2},{"$f":"ATAN((O91*O92)/(H93*Q71))","v":1.1698380349486639E-2},{"$f":"ATAN((O91*O88)/(H93*R71))","v":-7.3823307548584932E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O87*O88)/(H94*O72))","v":0.24087042826675767},{"$f":"ATAN((O87*O92)/(H94*P72))","v":-3.7340938551026569E-2},{"$f":"ATAN((O91*O92)/(H94*Q72))","v":8.9985885744867274E-3},{"$f":"ATAN((O91*O88)/(H94*R72))","v":-5.7530697805092901E-2}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E64","v":12},"m",null,null,null,null,{"$f":"E64/2","v":6}]
[null,null,"     širina temelja  B=",{"$f":"E65","v":2.9000021999999994},"m",null,null,null,null,{"$f":"E65/2","v":1.4500010999999997}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G64","v":{"$error":"#VALUE!"}},"kPa",null,null,null,null,{"$f":"J61*J81","v":4.4399999999999995}]
[null,null,"      dubina temeljenja Df=",{"$f":"E66","v":1.5001009999999999},"m",null,null,null,null,{"$f":"J62*J82","v":1.0730008139999998}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J83+J81","v":10.44}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J84+J82","v":2.5230019139999995}]
[1,null,"      H1=",{"$f":"IF(C69=0,\"      \",C69)","v":1},"m        Mk1=",{"$f":"IF(E69=0,\"       \",+E69)","v":8000},"KN/m2     z1=",{"$f":"C69/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C69+C70/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C69+C70+C71/2","v":3},"m",null,null,null,null,null,{"$f":"J83-J81","v":-1.5600000000000005}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C69+C70+C71+C72/2","v":5},"m",null,null,null,null,null,{"$f":"J84-J82","v":-0.37700028599999991}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C69+C70+C71+C72+C73/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C69+C70+C71+C72+C73+C74/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O73)-(P73)+(Q73)-(R73)+(S65)-(T65)+(U65)-(V65))/(2*3.14159)","v":0.85352710618381922},{"$f":"+D50","v":40},"kPa     Dp1=",{"$f":"(G64)*C96","v":{"$error":"#VALUE!"}},"kPa        w1=",{"$f":"IF(E69=0,\"       \",+F96*C69/E69)","v":{"$error":"#VALUE!"}},"m",{"$f":"0.2*D96","v":8}]
[null,"    I42=",{"$f":"((O74)-(P74)+(Q74)-(R74)+(S66)-(T66)+(U66)-(V66))/(2*3.14159)","v":0.57925601734609633},55,"kPa     Dp2=",{"$f":"IF(H90=H89,\"     \",(G64)*C97)","v":{"$error":"#VALUE!"}},"kPa       w2=",{"$error":"#VALUE!"},"m",11]
[null,"    I43=",{"$f":"((O75)-(P75)+(Q75)-(R75)+(S67)-(T67)+(U67)-(V67))/(2*3.14159)","v":0.36994022259745701},70,"kPa     Dp3=",{"$f":"IF(H91=H90,\"     \",(G64)*C98)","v":{"$error":"#VALUE!"}},"kPa       w3=",{"$error":"#VALUE!"},"m",14]
[null,"    I44=",{"$f":"((O76)-(P76)+(Q76)-(R76)+(S68)-(T68)+(U68)-(V68))/(2*3.14159)","v":0.22836899722988735},90,"kPa     Dp4=",{"$f":"IF(H92=H91,\"     \",(G64)*C99)","v":{"$error":"#VALUE!"}},"kPa       w4=",{"$error":"#VALUE!"},"m",18]
[null,"    I45=",{"$f":"((O77)-(P77)+(Q77)-(R77)+(S71)-(T71)+(U71)-(V71))/(2*3.14159)","v":0.15655508258448581},110,"kPa     Dp5=",{"$f":"IF(H93=H92,\"     \",(G64)*C100)","v":{"$error":"#VALUE!"}},"kPa       w5=",{"$error":"#VALUE!"},"m",22]
[null,"    I46=",{"$f":"((P78)-(Q78)+(R78)-(S78)+(S72)-(T72)+(U72)-(V72))/(2*3.14159)","v":0.13301609647873661},120.05,"kPa     Dp6=",{"$f":"IF(H94=H93,\"       \",(G64)*C101)","v":{"$error":"#VALUE!"}},"kPa       w6=",{"$error":"#VALUE!"},"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H96:H101)","v":{"$error":"#VALUE!"}},"m"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[]
[null,null,"SLIJEGANJE TOČKE K1 OD TEMELJA T3",null,null,null,null,null,"       x=L/2*",{"$f":"E11","v":0},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"E12","v":0}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!G13","v":0},"m         Dpa'=",{"$f":"+Slijeganje!G17","v":0},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!G14","v":0},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O133*O133)+(O134*O134)+(H135*H135))","v":0.5},{"$f":"SQRT((O133*O133)+(O138*O138)+(H135*H135))","v":0.5},{"$f":"SQRT((O137*O137)+(O138*O138)+(H135*H135))","v":0.5},{"$f":"SQRT((O137*O137)+(O134*O134)+(H135*H135))","v":0.5},{"$f":"H135*O133*O134*((O133*O133)+(O134*O134)+(2*H135*H135))/(((O133*O133)+(H135*H135))*((O134*O134)+(H135*H135))*O111)","v":0},{"$f":"H135*O133*O138*((O133*O133)+(O138*O138)+(2*H135*H135))/(((O133*O133)+(H135*H135))*((O138*O138)+(H135*H135))*P111)","v":0},{"$f":"H135*O137*O138*((O137*O137)+(O138*O138)+(2*H135*H135))/(((O137*O137)+(H135*H135))*((O138*O138)+(H135*H135))*Q111)","v":0},{"$f":"H135*O137*O134*((O137*O137)+(O134*O134)+(2*H135*H135))/(((O137*O137)+(H135*H135))*((O134*O134)+(H135*H135))*R111)","v":0}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!G15","v":0},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O133*O133)+(O134*O134)+(H136*H136))","v":1.5},{"$f":"SQRT((O133*O133)+(O138*O138)+(H136*H136))","v":1.5},{"$f":"SQRT((O137*O137)+(O138*O138)+(H136*H136))","v":1.5},{"$f":"SQRT((O137*O137)+(O134*O134)+(H136*H136))","v":1.5},{"$f":"H136*O133*O134*((O133*O133)+(O134*O134)+(2*H136*H136))/(((O133*O133)+(H136*H136))*((O134*O134)+(H136*H136))*O112)","v":0},{"$f":"H136*O133*O138*((O133*O133)+(O138*O138)+(2*H136*H136))/(((O133*O133)+(H136*H136))*((O138*O138)+(H136*H136))*P112)","v":0},{"$f":"H136*O137*O138*((O137*O137)+(O138*O138)+(2*H136*H136))/(((O137*O137)+(H136*H136))*((O138*O138)+(H136*H136))*Q112)","v":0},{"$f":"H136*O137*O134*((O137*O137)+(O134*O134)+(2*H136*H136))/(((O137*O137)+(H136*H136))*((O134*O134)+(H136*H136))*R112)","v":0}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O133*O133)+(O134*O134)+(H137*H137))","v":3},{"$f":"SQRT((O133*O133)+(O138*O138)+(H137*H137))","v":3},{"$f":"SQRT((O137*O137)+(O138*O138)+(H137*H137))","v":3},{"$f":"SQRT((O137*O137)+(O134*O134)+(H137*H137))","v":3},{"$f":"H137*O133*O134*((O133*O133)+(O134*O134)+(2*H137*H137))/(((O133*O133)+(H137*H137))*((O134*O134)+(H137*H137))*O113)","v":0},{"$f":"H137*O133*O138*((O133*O133)+(O138*O138)+(2*H137*H137))/(((O133*O133)+(H137*H137))*((O138*O138)+(H137*H137))*P113)","v":0},{"$f":"H137*O137*O138*((O137*O137)+(O138*O138)+(2*H137*H137))/(((O137*O137)+(H137*H137))*((O138*O138)+(H137*H137))*Q113)","v":0},{"$f":"H137*O137*O134*((O137*O137)+(O134*O134)+(2*H137*H137))/(((O137*O137)+(H137*H137))*((O134*O134)+(H137*H137))*R113)","v":0}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O133*O133)+(O134*O134)+(H138*H138))","v":5},{"$f":"SQRT((O133*O133)+(O138*O138)+(H138*H138))","v":5},{"$f":"SQRT((O137*O137)+(O138*O138)+(H138*H138))","v":5},{"$f":"SQRT((O137*O137)+(O134*O134)+(H138*H138))","v":5},{"$f":"H138*O133*O134*((O133*O133)+(O134*O134)+(2*H138*H138))/(((O133*O133)+(H138*H138))*((O134*O134)+(H138*H138))*O114)","v":0},{"$f":"H138*O133*O138*((O133*O133)+(O138*O138)+(2*H138*H138))/(((O133*O133)+(H138*H138))*((O138*O138)+(H138*H138))*P114)","v":0},{"$f":"H138*O137*O138*((O137*O137)+(O138*O138)+(2*H138*H138))/(((O137*O137)+(H138*H138))*((O138*O138)+(H138*H138))*Q114)","v":0},{"$f":"H138*O137*O134*((O137*O137)+(O134*O134)+(2*H138*H138))/(((O137*O137)+(H138*H138))*((O134*O134)+(H138*H138))*R114)","v":0}]
[null,1,{"$f":"+$C$23","v":1},{"$f":"+$D$23","v":20},{"$f":"+$E$23","v":8000},{"$f":"IF(H135=0,\"   \",+H135)","v":0.5},{"$f":"IF(D142=0,\"       \",+D142)","v":40},{"$f":"F142","v":0},{"$f":"H142","v":0},{"$f":"+J142","v":8}]
[null,{"$f":"IF(H136=(H135+C115/2),\"\",2)","v":2},{"$f":"+$C$24","v":1},{"$f":"+$D$24","v":10},{"$f":"+$E$24","v":8000},{"$f":"IF(H136=H135,\"   \",+H136)","v":1.5},{"$f":"IF(D143=D142,\"       \",+D143)","v":55},0,0,{"$f":"+J143","v":11}]
[null,{"$f":"IF(H137=(H136+C116/2),\"\",3)","v":3},{"$f":"+$C$25","v":2},{"$f":"+$D$25","v":10},{"$f":"+$E$25","v":8000},{"$f":"IF(H137=H136,\"   \",+H137)","v":3},{"$f":"IF(D144=D143,\"       \",+D144)","v":70},0,0,{"$f":"+J144","v":14},null,null,null,null,{"$f":"SQRT((O133*O133)+(O134*O134)+(H139*H139))","v":7},{"$f":"SQRT((O133*O133)+(O138*O138)+(H139*H139))","v":7},{"$f":"SQRT((O137*O137)+(O138*O138)+(H139*H139))","v":7},{"$f":"SQRT((O137*O137)+(O134*O134)+(H139*H139))","v":7},{"$f":"H139*O133*O134*((O133*O133)+(O134*O134)+(2*H139*H139))/(((O133*O133)+(H139*H139))*((O134*O134)+(H139*H139))*O117)","v":0},{"$f":"H139*O133*O138*((O133*O133)+(O138*O138)+(2*H139*H139))/(((O133*O133)+(H139*H139))*((O138*O138)+(H139*H139))*P117)","v":0},{"$f":"H139*O137*O138*((O137*O137)+(O138*O138)+(2*H139*H139))/(((O137*O137)+(H139*H139))*((O138*O138)+(H139*H139))*Q117)","v":0},{"$f":"H139*O137*O134*((O137*O137)+(O134*O134)+(2*H139*H139))/(((O137*O137)+(H139*H139))*((O134*O134)+(H139*H139))*R117)","v":0}]
[null,{"$f":"IF(H138=(H137+C117/2),\"\",4)","v":4},{"$f":"+$C$26","v":2},{"$f":"+$D$26","v":10},{"$f":"+$E$26","v":8000},{"$f":"IF(H138=H137,\"   \",+H138)","v":5},{"$f":"IF(D145=D144,\"       \",+D145)","v":90},0,0,{"$f":"IF(D145=D144,\"\",+J145)","v":18},null,null,null,null,{"$f":"SQRT((O133*O133)+(O134*O134)+(H140*H140))","v":8.0050000000000008},{"$f":"SQRT((O133*O133)+(O138*O138)+(H140*H140))","v":8.0050000000000008},{"$f":"SQRT((O137*O137)+(O138*O138)+(H140*H140))","v":8.0050000000000008},{"$f":"SQRT((O137*O137)+(O134*O134)+(H140*H140))","v":8.0050000000000008},{"$f":"H140*O133*O134*((O133*O133)+(O134*O134)+(2*H140*H140))/(((O133*O133)+(H140*H140))*((O134*O134)+(H140*H140))*O118)","v":0},{"$f":"H140*O133*O138*((O133*O133)+(O138*O138)+(2*H140*H140))/(((O133*O133)+(H140*H140))*((O138*O138)+(H140*H140))*P118)","v":0},{"$f":"H140*O137*O138*((O137*O137)+(O138*O138)+(2*H140*H140))/(((O137*O137)+(H140*H140))*((O138*O138)+(H140*H140))*Q118)","v":0},{"$f":"H140*O137*O134*((O137*O137)+(O134*O134)+(2*H140*H140))/(((O137*O137)+(H140*H140))*((O134*O134)+(H140*H140))*R118)","v":0}]
[null,{"$f":"IF(H139=(H138+C118/2),\"\",5)","v":5},{"$f":"+$C$27","v":2},{"$f":"+$D$27","v":10},{"$f":"+$E$27","v":8000},{"$f":"IF(H139=H138,\"   \",+H139)","v":7},{"$f":"IF(D146=D145,\"       \",+D146)","v":110},0,0,{"$f":"IF(D146=D145,\"\",+J146)","v":22},null,null,null,null,{"$f":"ATAN((O133*O134)/(H135*O111))","v":0},{"$f":"ATAN((O133*O138)/(H135*P111))","v":0},{"$f":"ATAN((O137*O138)/(H135*Q111))","v":0},{"$f":"ATAN((O137*O134)/(H135*R111))","v":0}]
[null,{"$f":"IF(H140=(H139+C119/2),\"\",6)","v":6},{"$f":"+$C$28","v":0.01},{"$f":"+$D$28","v":10},{"$f":"+$E$28","v":8000},{"$f":"IF(H140=H139,\"   \",+H140)","v":8.0050000000000008},{"$f":"IF(D147=D146,\"       \",+D147)","v":120.05},0,0,{"$f":"IF(D147=D146,\"\",+J147)","v":24.01},null,null,null,null,{"$f":"ATAN((O133*O134)/(H136*O112))","v":0},{"$f":"ATAN((O133*O138)/(H136*P112))","v":0},{"$f":"ATAN((O137*O138)/(H136*Q112))","v":0},{"$f":"ATAN((O137*O134)/(H136*R112))","v":0}]
[null,null,null,null,null,null,null,"  S W =",0,"m ",null,null,null,null,{"$f":"ATAN((O133*O134)/(H137*O113))","v":0},{"$f":"ATAN((O133*O138)/(H137*P113))","v":0},{"$f":"ATAN((O137*O138)/(H137*Q113))","v":0},{"$f":"ATAN((O137*O134)/(H137*R113))","v":0}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O133*O134)/(H138*O114))","v":0},{"$f":"ATAN((O133*O138)/(H138*P114))","v":0},{"$f":"ATAN((O137*O138)/(H138*Q114))","v":0},{"$f":"ATAN((O137*O134)/(H138*R114))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O133*O134)/(H139*O117))","v":0},{"$f":"ATAN((O133*O138)/(H139*P117))","v":0},{"$f":"ATAN((O137*O138)/(H139*Q117))","v":0},{"$f":"ATAN((O137*O134)/(H139*R117))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O133*O134)/(H140*O118))","v":0},{"$f":"ATAN((O133*O138)/(H140*P118))","v":0},{"$f":"ATAN((O137*O138)/(H140*Q118))","v":0},{"$f":"ATAN((O137*O134)/(H140*R118))","v":0}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E110","v":0},"m",null,null,null,null,{"$f":"E110/2","v":0}]
[null,null,"     širina temelja  B=",{"$f":"E111","v":0},"m",null,null,null,null,{"$f":"E111/2","v":0}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G110","v":0},"kPa",null,null,null,null,{"$f":"J107*J127","v":0}]
[null,null,"      dubina temeljenja Df=",{"$f":"E112","v":0},"m",null,null,null,null,{"$f":"J108*J128","v":0}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J129+J127","v":0}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J130+J128","v":0}]
[1,null,"      H1=",{"$f":"IF(C115=0,\"      \",C115)","v":1},"m        Mk1=",{"$f":"IF(E115=0,\"       \",+E115)","v":8000},"KN/m2     z1=",{"$f":"C115/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C115+C116/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C115+C116+C117/2","v":3},"m",null,null,null,null,null,{"$f":"J129-J127","v":0}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C115+C116+C117+C118/2","v":5},"m",null,null,null,null,null,{"$f":"J130-J128","v":0}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C115+C116+C117+C118+C119/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C115+C116+C117+C118+C119+C120/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O119)-(P119)+(Q119)-(R119)+(S111)-(T111)+(U111)-(V111))/(2*3.14159)","v":0},{"$f":"+D96","v":40},"kPa     Dp1=",{"$f":"(G110)*C142","v":0},"kPa        w1=",{"$f":"IF(E115=0,\"       \",+F142*C115/E115)","v":0},"m",{"$f":"0.2*D142","v":8}]
[null,"    I42=",{"$f":"((O120)-(P120)+(Q120)-(R120)+(S112)-(T112)+(U112)-(V112))/(2*3.14159)","v":0},55,"kPa     Dp2=",{"$f":"IF(H136=H135,\"     \",(G110)*C143)","v":0},"kPa       w2=",0,"m",11]
[null,"    I43=",{"$f":"((O121)-(P121)+(Q121)-(R121)+(S113)-(T113)+(U113)-(V113))/(2*3.14159)","v":0},70,"kPa     Dp3=",{"$f":"IF(H137=H136,\"     \",(G110)*C144)","v":0},"kPa       w3=",0,"m",14]
[null,"    I44=",{"$f":"((O122)-(P122)+(Q122)-(R122)+(S114)-(T114)+(U114)-(V114))/(2*3.14159)","v":0},90,"kPa     Dp4=",{"$f":"IF(H138=H137,\"     \",(G110)*C145)","v":0},"kPa       w4=",0,"m",18]
[null,"    I45=",{"$f":"((O123)-(P123)+(Q123)-(R123)+(S117)-(T117)+(U117)-(V117))/(2*3.14159)","v":0},110,"kPa     Dp5=",{"$f":"IF(H139=H138,\"     \",(G110)*C146)","v":0},"kPa       w5=",0,"m",22]
[null,"    I46=",{"$f":"((P124)-(Q124)+(R124)-(S124)+(S118)-(T118)+(U118)-(V118))/(2*3.14159)","v":0},120.05,"kPa     Dp6=",{"$f":"IF(H140=H139,\"       \",(G110)*C147)","v":0},"kPa       w6=",0,"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H142:H147)","v":0},"m"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[]
[null,null,"SLIJEGANJE TOČKE K1 OD TEMELJA T4",null,null,null,null,null,"       x=L/2*",{"$f":"F11","v":0},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"F12","v":0}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!H13","v":0},"m         Dpa'=",{"$f":"+Slijeganje!H17","v":0},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!H14","v":0},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O179*O179)+(O180*O180)+(H181*H181))","v":0.5},{"$f":"SQRT((O179*O179)+(O184*O184)+(H181*H181))","v":0.5},{"$f":"SQRT((O183*O183)+(O184*O184)+(H181*H181))","v":0.5},{"$f":"SQRT((O183*O183)+(O180*O180)+(H181*H181))","v":0.5},{"$f":"H181*O179*O180*((O179*O179)+(O180*O180)+(2*H181*H181))/(((O179*O179)+(H181*H181))*((O180*O180)+(H181*H181))*O157)","v":0},{"$f":"H181*O179*O184*((O179*O179)+(O184*O184)+(2*H181*H181))/(((O179*O179)+(H181*H181))*((O184*O184)+(H181*H181))*P157)","v":0},{"$f":"H181*O183*O184*((O183*O183)+(O184*O184)+(2*H181*H181))/(((O183*O183)+(H181*H181))*((O184*O184)+(H181*H181))*Q157)","v":0},{"$f":"H181*O183*O180*((O183*O183)+(O180*O180)+(2*H181*H181))/(((O183*O183)+(H181*H181))*((O180*O180)+(H181*H181))*R157)","v":0}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!H15","v":0},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O179*O179)+(O180*O180)+(H182*H182))","v":1.5},{"$f":"SQRT((O179*O179)+(O184*O184)+(H182*H182))","v":1.5},{"$f":"SQRT((O183*O183)+(O184*O184)+(H182*H182))","v":1.5},{"$f":"SQRT((O183*O183)+(O180*O180)+(H182*H182))","v":1.5},{"$f":"H182*O179*O180*((O179*O179)+(O180*O180)+(2*H182*H182))/(((O179*O179)+(H182*H182))*((O180*O180)+(H182*H182))*O158)","v":0},{"$f":"H182*O179*O184*((O179*O179)+(O184*O184)+(2*H182*H182))/(((O179*O179)+(H182*H182))*((O184*O184)+(H182*H182))*P158)","v":0},{"$f":"H182*O183*O184*((O183*O183)+(O184*O184)+(2*H182*H182))/(((O183*O183)+(H182*H182))*((O184*O184)+(H182*H182))*Q158)","v":0},{"$f":"H182*O183*O180*((O183*O183)+(O180*O180)+(2*H182*H182))/(((O183*O183)+(H182*H182))*((O180*O180)+(H182*H182))*R158)","v":0}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O179*O179)+(O180*O180)+(H183*H183))","v":3},{"$f":"SQRT((O179*O179)+(O184*O184)+(H183*H183))","v":3},{"$f":"SQRT((O183*O183)+(O184*O184)+(H183*H183))","v":3},{"$f":"SQRT((O183*O183)+(O180*O180)+(H183*H183))","v":3},{"$f":"H183*O179*O180*((O179*O179)+(O180*O180)+(2*H183*H183))/(((O179*O179)+(H183*H183))*((O180*O180)+(H183*H183))*O159)","v":0},{"$f":"H183*O179*O184*((O179*O179)+(O184*O184)+(2*H183*H183))/(((O179*O179)+(H183*H183))*((O184*O184)+(H183*H183))*P159)","v":0},{"$f":"H183*O183*O184*((O183*O183)+(O184*O184)+(2*H183*H183))/(((O183*O183)+(H183*H183))*((O184*O184)+(H183*H183))*Q159)","v":0},{"$f":"H183*O183*O180*((O183*O183)+(O180*O180)+(2*H183*H183))/(((O183*O183)+(H183*H183))*((O180*O180)+(H183*H183))*R159)","v":0}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O179*O179)+(O180*O180)+(H184*H184))","v":5},{"$f":"SQRT((O179*O179)+(O184*O184)+(H184*H184))","v":5},{"$f":"SQRT((O183*O183)+(O184*O184)+(H184*H184))","v":5},{"$f":"SQRT((O183*O183)+(O180*O180)+(H184*H184))","v":5},{"$f":"H184*O179*O180*((O179*O179)+(O180*O180)+(2*H184*H184))/(((O179*O179)+(H184*H184))*((O180*O180)+(H184*H184))*O160)","v":0},{"$f":"H184*O179*O184*((O179*O179)+(O184*O184)+(2*H184*H184))/(((O179*O179)+(H184*H184))*((O184*O184)+(H184*H184))*P160)","v":0},{"$f":"H184*O183*O184*((O183*O183)+(O184*O184)+(2*H184*H184))/(((O183*O183)+(H184*H184))*((O184*O184)+(H184*H184))*Q160)","v":0},{"$f":"H184*O183*O180*((O183*O183)+(O180*O180)+(2*H184*H184))/(((O183*O183)+(H184*H184))*((O180*O180)+(H184*H184))*R160)","v":0}]
[null,1,{"$f":"+$C$23","v":1},{"$f":"+$D$23","v":20},{"$f":"+$E$23","v":8000},{"$f":"IF(H181=0,\"   \",+H181)","v":0.5},{"$f":"IF(D188=0,\"       \",+D188)","v":40},{"$f":"F188","v":0},{"$f":"H188","v":0},{"$f":"+J188","v":8}]
[null,{"$f":"IF(H182=(H181+C161/2),\"\",2)","v":2},{"$f":"+$C$24","v":1},{"$f":"+$D$24","v":10},{"$f":"+$E$24","v":8000},{"$f":"IF(H182=H181,\"   \",+H182)","v":1.5},{"$f":"IF(D189=D188,\"       \",+D189)","v":55},0,0,{"$f":"+J189","v":11}]
[null,{"$f":"IF(H183=(H182+C162/2),\"\",3)","v":3},{"$f":"+$C$25","v":2},{"$f":"+$D$25","v":10},{"$f":"+$E$25","v":8000},{"$f":"IF(H183=H182,\"   \",+H183)","v":3},{"$f":"IF(D190=D189,\"       \",+D190)","v":70},0,0,{"$f":"+J190","v":14},null,null,null,null,{"$f":"SQRT((O179*O179)+(O180*O180)+(H185*H185))","v":7},{"$f":"SQRT((O179*O179)+(O184*O184)+(H185*H185))","v":7},{"$f":"SQRT((O183*O183)+(O184*O184)+(H185*H185))","v":7},{"$f":"SQRT((O183*O183)+(O180*O180)+(H185*H185))","v":7},{"$f":"H185*O179*O180*((O179*O179)+(O180*O180)+(2*H185*H185))/(((O179*O179)+(H185*H185))*((O180*O180)+(H185*H185))*O163)","v":0},{"$f":"H185*O179*O184*((O179*O179)+(O184*O184)+(2*H185*H185))/(((O179*O179)+(H185*H185))*((O184*O184)+(H185*H185))*P163)","v":0},{"$f":"H185*O183*O184*((O183*O183)+(O184*O184)+(2*H185*H185))/(((O183*O183)+(H185*H185))*((O184*O184)+(H185*H185))*Q163)","v":0},{"$f":"H185*O183*O180*((O183*O183)+(O180*O180)+(2*H185*H185))/(((O183*O183)+(H185*H185))*((O180*O180)+(H185*H185))*R163)","v":0}]
[null,{"$f":"IF(H184=(H183+C163/2),\"\",4)","v":4},{"$f":"+$C$26","v":2},{"$f":"+$D$26","v":10},{"$f":"+$E$26","v":8000},{"$f":"IF(H184=H183,\"   \",+H184)","v":5},{"$f":"IF(D191=D190,\"       \",+D191)","v":90},0,0,{"$f":"IF(D191=D190,\"\",+J191)","v":18},null,null,null,null,{"$f":"SQRT((O179*O179)+(O180*O180)+(H186*H186))","v":8.0050000000000008},{"$f":"SQRT((O179*O179)+(O184*O184)+(H186*H186))","v":8.0050000000000008},{"$f":"SQRT((O183*O183)+(O184*O184)+(H186*H186))","v":8.0050000000000008},{"$f":"SQRT((O183*O183)+(O180*O180)+(H186*H186))","v":8.0050000000000008},{"$f":"H186*O179*O180*((O179*O179)+(O180*O180)+(2*H186*H186))/(((O179*O179)+(H186*H186))*((O180*O180)+(H186*H186))*O164)","v":0},{"$f":"H186*O179*O184*((O179*O179)+(O184*O184)+(2*H186*H186))/(((O179*O179)+(H186*H186))*((O184*O184)+(H186*H186))*P164)","v":0},{"$f":"H186*O183*O184*((O183*O183)+(O184*O184)+(2*H186*H186))/(((O183*O183)+(H186*H186))*((O184*O184)+(H186*H186))*Q164)","v":0},{"$f":"H186*O183*O180*((O183*O183)+(O180*O180)+(2*H186*H186))/(((O183*O183)+(H186*H186))*((O180*O180)+(H186*H186))*R164)","v":0}]
[null,{"$f":"IF(H185=(H184+C164/2),\"\",5)","v":5},{"$f":"+$C$27","v":2},{"$f":"+$D$27","v":10},{"$f":"+$E$27","v":8000},{"$f":"IF(H185=H184,\"   \",+H185)","v":7},{"$f":"IF(D192=D191,\"       \",+D192)","v":110},0,0,{"$f":"IF(D192=D191,\"\",+J192)","v":22},null,null,null,null,{"$f":"ATAN((O179*O180)/(H181*O157))","v":0},{"$f":"ATAN((O179*O184)/(H181*P157))","v":0},{"$f":"ATAN((O183*O184)/(H181*Q157))","v":0},{"$f":"ATAN((O183*O180)/(H181*R157))","v":0}]
[null,{"$f":"IF(H186=(H185+C165/2),\"\",6)","v":6},{"$f":"+$C$28","v":0.01},{"$f":"+$D$28","v":10},{"$f":"+$E$28","v":8000},{"$f":"IF(H186=H185,\"   \",+H186)","v":8.0050000000000008},{"$f":"IF(D193=D192,\"       \",+D193)","v":120.05},0,0,{"$f":"IF(D193=D192,\"\",+J193)","v":24.01},null,null,null,null,{"$f":"ATAN((O179*O180)/(H182*O158))","v":0},{"$f":"ATAN((O179*O184)/(H182*P158))","v":0},{"$f":"ATAN((O183*O184)/(H182*Q158))","v":0},{"$f":"ATAN((O183*O180)/(H182*R158))","v":0}]
[null,null,null,null,null,null,null,"  S W =",0,"m ",null,null,null,null,{"$f":"ATAN((O179*O180)/(H183*O159))","v":0},{"$f":"ATAN((O179*O184)/(H183*P159))","v":0},{"$f":"ATAN((O183*O184)/(H183*Q159))","v":0},{"$f":"ATAN((O183*O180)/(H183*R159))","v":0}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O179*O180)/(H184*O160))","v":0},{"$f":"ATAN((O179*O184)/(H184*P160))","v":0},{"$f":"ATAN((O183*O184)/(H184*Q160))","v":0},{"$f":"ATAN((O183*O180)/(H184*R160))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O179*O180)/(H185*O163))","v":0},{"$f":"ATAN((O179*O184)/(H185*P163))","v":0},{"$f":"ATAN((O183*O184)/(H185*Q163))","v":0},{"$f":"ATAN((O183*O180)/(H185*R163))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O179*O180)/(H186*O164))","v":0},{"$f":"ATAN((O179*O184)/(H186*P164))","v":0},{"$f":"ATAN((O183*O184)/(H186*Q164))","v":0},{"$f":"ATAN((O183*O180)/(H186*R164))","v":0}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E156","v":0},"m",null,null,null,null,{"$f":"E156/2","v":0}]
[null,null,"     širina temelja  B=",{"$f":"E157","v":0},"m",null,null,null,null,{"$f":"E157/2","v":0}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G156","v":0},"kPa",null,null,null,null,{"$f":"J153*J173","v":0}]
[null,null,"      dubina temeljenja Df=",{"$f":"E158","v":0},"m",null,null,null,null,{"$f":"J154*J174","v":0}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J175+J173","v":0}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J176+J174","v":0}]
[1,null,"      H1=",{"$f":"IF(C161=0,\"      \",C161)","v":1},"m        Mk1=",{"$f":"IF(E161=0,\"       \",+E161)","v":8000},"KN/m2     z1=",{"$f":"C161/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C161+C162/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C161+C162+C163/2","v":3},"m",null,null,null,null,null,{"$f":"J175-J173","v":0}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C161+C162+C163+C164/2","v":5},"m",null,null,null,null,null,{"$f":"J176-J174","v":0}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C161+C162+C163+C164+C165/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C161+C162+C163+C164+C165+C166/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O165)-(P165)+(Q165)-(R165)+(S157)-(T157)+(U157)-(V157))/(2*3.14159)","v":0},{"$f":"+D142","v":40},"kPa     Dp1=",{"$f":"(G156)*C188","v":0},"kPa        w1=",{"$f":"IF(E161=0,\"       \",+F188*C161/E161)","v":0},"m",{"$f":"0.2*D188","v":8}]
[null,"    I42=",{"$f":"((O166)-(P166)+(Q166)-(R166)+(S158)-(T158)+(U158)-(V158))/(2*3.14159)","v":0},55,"kPa     Dp2=",{"$f":"IF(H182=H181,\"     \",(G156)*C189)","v":0},"kPa       w2=",0,"m",11]
[null,"    I43=",{"$f":"((O167)-(P167)+(Q167)-(R167)+(S159)-(T159)+(U159)-(V159))/(2*3.14159)","v":0},70,"kPa     Dp3=",{"$f":"IF(H183=H182,\"     \",(G156)*C190)","v":0},"kPa       w3=",0,"m",14]
[null,"    I44=",{"$f":"((O168)-(P168)+(Q168)-(R168)+(S160)-(T160)+(U160)-(V160))/(2*3.14159)","v":0},90,"kPa     Dp4=",{"$f":"IF(H184=H183,\"     \",(G156)*C191)","v":0},"kPa       w4=",0,"m",18]
[null,"    I45=",{"$f":"((O169)-(P169)+(Q169)-(R169)+(S163)-(T163)+(U163)-(V163))/(2*3.14159)","v":0},110,"kPa     Dp5=",{"$f":"IF(H185=H184,\"     \",(G156)*C192)","v":0},"kPa       w5=",0,"m",22]
[null,"    I46=",{"$f":"((P170)-(Q170)+(R170)-(S170)+(S164)-(T164)+(U164)-(V164))/(2*3.14159)","v":0},120.05,"kPa     Dp6=",{"$f":"IF(H186=H185,\"       \",(G156)*C193)","v":0},"kPa       w6=",0,"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H188:H193)","v":0},"m"]
[]
[]
[]
[]
[null,null,"SLIJEGANJE TOČKE TS1 OD TEMELJA T5",null,null,null,null,null,"       x=L/2*",{"$f":"G11","v":0},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"G12","v":0}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!I13","v":0},"m         Dpa'=",{"$f":"+Slijeganje!I17","v":0},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!I14","v":0},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O225*O225)+(O226*O226)+(H227*H227))","v":0.5},{"$f":"SQRT((O225*O225)+(O230*O230)+(H227*H227))","v":0.5},{"$f":"SQRT((O229*O229)+(O230*O230)+(H227*H227))","v":0.5},{"$f":"SQRT((O229*O229)+(O226*O226)+(H227*H227))","v":0.5},{"$f":"H227*O225*O226*((O225*O225)+(O226*O226)+(2*H227*H227))/(((O225*O225)+(H227*H227))*((O226*O226)+(H227*H227))*O203)","v":0},{"$f":"H227*O225*O230*((O225*O225)+(O230*O230)+(2*H227*H227))/(((O225*O225)+(H227*H227))*((O230*O230)+(H227*H227))*P203)","v":0},{"$f":"H227*O229*O230*((O229*O229)+(O230*O230)+(2*H227*H227))/(((O229*O229)+(H227*H227))*((O230*O230)+(H227*H227))*Q203)","v":0},{"$f":"H227*O229*O226*((O229*O229)+(O226*O226)+(2*H227*H227))/(((O229*O229)+(H227*H227))*((O226*O226)+(H227*H227))*R203)","v":0}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!I15","v":0},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O225*O225)+(O226*O226)+(H228*H228))","v":1.5},{"$f":"SQRT((O225*O225)+(O230*O230)+(H228*H228))","v":1.5},{"$f":"SQRT((O229*O229)+(O230*O230)+(H228*H228))","v":1.5},{"$f":"SQRT((O229*O229)+(O226*O226)+(H228*H228))","v":1.5},{"$f":"H228*O225*O226*((O225*O225)+(O226*O226)+(2*H228*H228))/(((O225*O225)+(H228*H228))*((O226*O226)+(H228*H228))*O204)","v":0},{"$f":"H228*O225*O230*((O225*O225)+(O230*O230)+(2*H228*H228))/(((O225*O225)+(H228*H228))*((O230*O230)+(H228*H228))*P204)","v":0},{"$f":"H228*O229*O230*((O229*O229)+(O230*O230)+(2*H228*H228))/(((O229*O229)+(H228*H228))*((O230*O230)+(H228*H228))*Q204)","v":0},{"$f":"H228*O229*O226*((O229*O229)+(O226*O226)+(2*H228*H228))/(((O229*O229)+(H228*H228))*((O226*O226)+(H228*H228))*R204)","v":0}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O225*O225)+(O226*O226)+(H229*H229))","v":3},{"$f":"SQRT((O225*O225)+(O230*O230)+(H229*H229))","v":3},{"$f":"SQRT((O229*O229)+(O230*O230)+(H229*H229))","v":3},{"$f":"SQRT((O229*O229)+(O226*O226)+(H229*H229))","v":3},{"$f":"H229*O225*O226*((O225*O225)+(O226*O226)+(2*H229*H229))/(((O225*O225)+(H229*H229))*((O226*O226)+(H229*H229))*O205)","v":0},{"$f":"H229*O225*O230*((O225*O225)+(O230*O230)+(2*H229*H229))/(((O225*O225)+(H229*H229))*((O230*O230)+(H229*H229))*P205)","v":0},{"$f":"H229*O229*O230*((O229*O229)+(O230*O230)+(2*H229*H229))/(((O229*O229)+(H229*H229))*((O230*O230)+(H229*H229))*Q205)","v":0},{"$f":"H229*O229*O226*((O229*O229)+(O226*O226)+(2*H229*H229))/(((O229*O229)+(H229*H229))*((O226*O226)+(H229*H229))*R205)","v":0}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O225*O225)+(O226*O226)+(H230*H230))","v":5},{"$f":"SQRT((O225*O225)+(O230*O230)+(H230*H230))","v":5},{"$f":"SQRT((O229*O229)+(O230*O230)+(H230*H230))","v":5},{"$f":"SQRT((O229*O229)+(O226*O226)+(H230*H230))","v":5},{"$f":"H230*O225*O226*((O225*O225)+(O226*O226)+(2*H230*H230))/(((O225*O225)+(H230*H230))*((O226*O226)+(H230*H230))*O206)","v":0},{"$f":"H230*O225*O230*((O225*O225)+(O230*O230)+(2*H230*H230))/(((O225*O225)+(H230*H230))*((O230*O230)+(H230*H230))*P206)","v":0},{"$f":"H230*O229*O230*((O229*O229)+(O230*O230)+(2*H230*H230))/(((O229*O229)+(H230*H230))*((O230*O230)+(H230*H230))*Q206)","v":0},{"$f":"H230*O229*O226*((O229*O229)+(O226*O226)+(2*H230*H230))/(((O229*O229)+(H230*H230))*((O226*O226)+(H230*H230))*R206)","v":0}]
[null,1,{"$f":"+$C$23","v":1},{"$f":"+$D$23","v":20},{"$f":"+$E$23","v":8000},{"$f":"IF(H227=0,\"   \",+H227)","v":0.5},{"$f":"IF(D234=0,\"       \",+D234)","v":40},{"$f":"F234","v":0},{"$f":"H234","v":0},{"$f":"+J234","v":8}]
[null,{"$f":"IF(H228=(H227+C207/2),\"\",2)","v":2},{"$f":"+$C$24","v":1},{"$f":"+$D$24","v":10},{"$f":"+$E$24","v":8000},{"$f":"IF(H228=H227,\"   \",+H228)","v":1.5},{"$f":"IF(D235=D234,\"       \",+D235)","v":55},0,0,{"$f":"+J235","v":11}]
[null,{"$f":"IF(H229=(H228+C208/2),\"\",3)","v":3},{"$f":"+$C$25","v":2},{"$f":"+$D$25","v":10},{"$f":"+$E$25","v":8000},{"$f":"IF(H229=H228,\"   \",+H229)","v":3},{"$f":"IF(D236=D235,\"       \",+D236)","v":70},0,0,{"$f":"+J236","v":14},null,null,null,null,{"$f":"SQRT((O225*O225)+(O226*O226)+(H231*H231))","v":7},{"$f":"SQRT((O225*O225)+(O230*O230)+(H231*H231))","v":7},{"$f":"SQRT((O229*O229)+(O230*O230)+(H231*H231))","v":7},{"$f":"SQRT((O229*O229)+(O226*O226)+(H231*H231))","v":7},{"$f":"H231*O225*O226*((O225*O225)+(O226*O226)+(2*H231*H231))/(((O225*O225)+(H231*H231))*((O226*O226)+(H231*H231))*O209)","v":0},{"$f":"H231*O225*O230*((O225*O225)+(O230*O230)+(2*H231*H231))/(((O225*O225)+(H231*H231))*((O230*O230)+(H231*H231))*P209)","v":0},{"$f":"H231*O229*O230*((O229*O229)+(O230*O230)+(2*H231*H231))/(((O229*O229)+(H231*H231))*((O230*O230)+(H231*H231))*Q209)","v":0},{"$f":"H231*O229*O226*((O229*O229)+(O226*O226)+(2*H231*H231))/(((O229*O229)+(H231*H231))*((O226*O226)+(H231*H231))*R209)","v":0}]
[null,{"$f":"IF(H230=(H229+C209/2),\"\",4)","v":4},{"$f":"+$C$26","v":2},{"$f":"+$D$26","v":10},{"$f":"+$E$26","v":8000},{"$f":"IF(H230=H229,\"   \",+H230)","v":5},{"$f":"IF(D237=D236,\"       \",+D237)","v":90},0,0,{"$f":"IF(D237=D236,\"\",+J237)","v":18},null,null,null,null,{"$f":"SQRT((O225*O225)+(O226*O226)+(H232*H232))","v":8.0050000000000008},{"$f":"SQRT((O225*O225)+(O230*O230)+(H232*H232))","v":8.0050000000000008},{"$f":"SQRT((O229*O229)+(O230*O230)+(H232*H232))","v":8.0050000000000008},{"$f":"SQRT((O229*O229)+(O226*O226)+(H232*H232))","v":8.0050000000000008},{"$f":"H232*O225*O226*((O225*O225)+(O226*O226)+(2*H232*H232))/(((O225*O225)+(H232*H232))*((O226*O226)+(H232*H232))*O210)","v":0},{"$f":"H232*O225*O230*((O225*O225)+(O230*O230)+(2*H232*H232))/(((O225*O225)+(H232*H232))*((O230*O230)+(H232*H232))*P210)","v":0},{"$f":"H232*O229*O230*((O229*O229)+(O230*O230)+(2*H232*H232))/(((O229*O229)+(H232*H232))*((O230*O230)+(H232*H232))*Q210)","v":0},{"$f":"H232*O229*O226*((O229*O229)+(O226*O226)+(2*H232*H232))/(((O229*O229)+(H232*H232))*((O226*O226)+(H232*H232))*R210)","v":0}]
[null,{"$f":"IF(H231=(H230+C210/2),\"\",5)","v":5},{"$f":"+$C$27","v":2},{"$f":"+$D$27","v":10},{"$f":"+$E$27","v":8000},{"$f":"IF(H231=H230,\"   \",+H231)","v":7},{"$f":"IF(D238=D237,\"       \",+D238)","v":110},0,0,{"$f":"IF(D238=D237,\"\",+J238)","v":22},null,null,null,null,{"$f":"ATAN((O225*O226)/(H227*O203))","v":0},{"$f":"ATAN((O225*O230)/(H227*P203))","v":0},{"$f":"ATAN((O229*O230)/(H227*Q203))","v":0},{"$f":"ATAN((O229*O226)/(H227*R203))","v":0}]
[null,{"$f":"IF(H232=(H231+C211/2),\"\",6)","v":6},{"$f":"+$C$28","v":0.01},{"$f":"+$D$28","v":10},{"$f":"+$E$28","v":8000},{"$f":"IF(H232=H231,\"   \",+H232)","v":8.0050000000000008},{"$f":"IF(D239=D238,\"       \",+D239)","v":120.05},0,0,{"$f":"IF(D239=D238,\"\",+J239)","v":24.01},null,null,null,null,{"$f":"ATAN((O225*O226)/(H228*O204))","v":0},{"$f":"ATAN((O225*O230)/(H228*P204))","v":0},{"$f":"ATAN((O229*O230)/(H228*Q204))","v":0},{"$f":"ATAN((O229*O226)/(H228*R204))","v":0}]
[null,null,null,null,null,null,null,"  S W =",0,"m ",null,null,null,null,{"$f":"ATAN((O225*O226)/(H229*O205))","v":0},{"$f":"ATAN((O225*O230)/(H229*P205))","v":0},{"$f":"ATAN((O229*O230)/(H229*Q205))","v":0},{"$f":"ATAN((O229*O226)/(H229*R205))","v":0}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O225*O226)/(H230*O206))","v":0},{"$f":"ATAN((O225*O230)/(H230*P206))","v":0},{"$f":"ATAN((O229*O230)/(H230*Q206))","v":0},{"$f":"ATAN((O229*O226)/(H230*R206))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O225*O226)/(H231*O209))","v":0},{"$f":"ATAN((O225*O230)/(H231*P209))","v":0},{"$f":"ATAN((O229*O230)/(H231*Q209))","v":0},{"$f":"ATAN((O229*O226)/(H231*R209))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O225*O226)/(H232*O210))","v":0},{"$f":"ATAN((O225*O230)/(H232*P210))","v":0},{"$f":"ATAN((O229*O230)/(H232*Q210))","v":0},{"$f":"ATAN((O229*O226)/(H232*R210))","v":0}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E202","v":0},"m",null,null,null,null,{"$f":"E202/2","v":0}]
[null,null,"     širina temelja  B=",{"$f":"E203","v":0},"m",null,null,null,null,{"$f":"E203/2","v":0}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G202","v":0},"kPa",null,null,null,null,{"$f":"J199*J219","v":0}]
[null,null,"      dubina temeljenja Df=",{"$f":"E204","v":0},"m",null,null,null,null,{"$f":"J200*J220","v":0}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J221+J219","v":0}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J222+J220","v":0}]
[1,null,"      H1=",{"$f":"IF(C207=0,\"      \",C207)","v":1},"m        Mk1=",{"$f":"IF(E207=0,\"       \",+E207)","v":8000},"KN/m2     z1=",{"$f":"C207/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C207+C208/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C207+C208+C209/2","v":3},"m",null,null,null,null,null,{"$f":"J221-J219","v":0}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C207+C208+C209+C210/2","v":5},"m",null,null,null,null,null,{"$f":"J222-J220","v":0}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C207+C208+C209+C210+C211/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C207+C208+C209+C210+C211+C212/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O211)-(P211)+(Q211)-(R211)+(S203)-(T203)+(U203)-(V203))/(2*3.14159)","v":0},{"$f":"+D188","v":40},"kPa     Dp1=",{"$f":"(G202)*C234","v":0},"kPa        w1=",{"$f":"IF(E207=0,\"       \",+F234*C207/E207)","v":0},"m",{"$f":"0.2*D234","v":8}]
[null,"    I42=",{"$f":"((O212)-(P212)+(Q212)-(R212)+(S204)-(T204)+(U204)-(V204))/(2*3.14159)","v":0},55,"kPa     Dp2=",{"$f":"IF(H228=H227,\"     \",(G202)*C235)","v":0},"kPa       w2=",0,"m",11]
[null,"    I43=",{"$f":"((O213)-(P213)+(Q213)-(R213)+(S205)-(T205)+(U205)-(V205))/(2*3.14159)","v":0},70,"kPa     Dp3=",{"$f":"IF(H229=H228,\"     \",(G202)*C236)","v":0},"kPa       w3=",0,"m",14]
[null,"    I44=",{"$f":"((O214)-(P214)+(Q214)-(R214)+(S206)-(T206)+(U206)-(V206))/(2*3.14159)","v":0},90,"kPa     Dp4=",{"$f":"IF(H230=H229,\"     \",(G202)*C237)","v":0},"kPa       w4=",0,"m",18]
[null,"    I45=",{"$f":"((O215)-(P215)+(Q215)-(R215)+(S209)-(T209)+(U209)-(V209))/(2*3.14159)","v":0},110,"kPa     Dp5=",{"$f":"IF(H231=H230,\"     \",(G202)*C238)","v":0},"kPa       w5=",0,"m",22]
[null,"    I46=",{"$f":"((P216)-(Q216)+(R216)-(S216)+(S210)-(T210)+(U210)-(V210))/(2*3.14159)","v":0},120.05,"kPa     Dp6=",{"$f":"IF(H232=H231,\"       \",(G202)*C239)","v":0},"kPa       w6=",0,"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H234:H239)","v":0},"m"]
[]
[]
[]
[]
[null,null,"SLIJEGANJE TOČKE TS1 OD TEMELJA T6",null,null,null,null,null,"       x=L/2*",{"$f":"H11","v":0},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"H12","v":0}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!J13","v":0},"m         Dpa'=",{"$f":"+Slijeganje!J17","v":0},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!J14","v":0},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O271*O271)+(O272*O272)+(H273*H273))","v":0.5},{"$f":"SQRT((O271*O271)+(O276*O276)+(H273*H273))","v":0.5},{"$f":"SQRT((O275*O275)+(O276*O276)+(H273*H273))","v":0.5},{"$f":"SQRT((O275*O275)+(O272*O272)+(H273*H273))","v":0.5},{"$f":"H273*O271*O272*((O271*O271)+(O272*O272)+(2*H273*H273))/(((O271*O271)+(H273*H273))*((O272*O272)+(H273*H273))*O249)","v":0},{"$f":"H273*O271*O276*((O271*O271)+(O276*O276)+(2*H273*H273))/(((O271*O271)+(H273*H273))*((O276*O276)+(H273*H273))*P249)","v":0},{"$f":"H273*O275*O276*((O275*O275)+(O276*O276)+(2*H273*H273))/(((O275*O275)+(H273*H273))*((O276*O276)+(H273*H273))*Q249)","v":0},{"$f":"H273*O275*O272*((O275*O275)+(O272*O272)+(2*H273*H273))/(((O275*O275)+(H273*H273))*((O272*O272)+(H273*H273))*R249)","v":0}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!J15","v":0},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O271*O271)+(O272*O272)+(H274*H274))","v":1.5},{"$f":"SQRT((O271*O271)+(O276*O276)+(H274*H274))","v":1.5},{"$f":"SQRT((O275*O275)+(O276*O276)+(H274*H274))","v":1.5},{"$f":"SQRT((O275*O275)+(O272*O272)+(H274*H274))","v":1.5},{"$f":"H274*O271*O272*((O271*O271)+(O272*O272)+(2*H274*H274))/(((O271*O271)+(H274*H274))*((O272*O272)+(H274*H274))*O250)","v":0},{"$f":"H274*O271*O276*((O271*O271)+(O276*O276)+(2*H274*H274))/(((O271*O271)+(H274*H274))*((O276*O276)+(H274*H274))*P250)","v":0},{"$f":"H274*O275*O276*((O275*O275)+(O276*O276)+(2*H274*H274))/(((O275*O275)+(H274*H274))*((O276*O276)+(H274*H274))*Q250)","v":0},{"$f":"H274*O275*O272*((O275*O275)+(O272*O272)+(2*H274*H274))/(((O275*O275)+(H274*H274))*((O272*O272)+(H274*H274))*R250)","v":0}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O271*O271)+(O272*O272)+(H275*H275))","v":3},{"$f":"SQRT((O271*O271)+(O276*O276)+(H275*H275))","v":3},{"$f":"SQRT((O275*O275)+(O276*O276)+(H275*H275))","v":3},{"$f":"SQRT((O275*O275)+(O272*O272)+(H275*H275))","v":3},{"$f":"H275*O271*O272*((O271*O271)+(O272*O272)+(2*H275*H275))/(((O271*O271)+(H275*H275))*((O272*O272)+(H275*H275))*O251)","v":0},{"$f":"H275*O271*O276*((O271*O271)+(O276*O276)+(2*H275*H275))/(((O271*O271)+(H275*H275))*((O276*O276)+(H275*H275))*P251)","v":0},{"$f":"H275*O275*O276*((O275*O275)+(O276*O276)+(2*H275*H275))/(((O275*O275)+(H275*H275))*((O276*O276)+(H275*H275))*Q251)","v":0},{"$f":"H275*O275*O272*((O275*O275)+(O272*O272)+(2*H275*H275))/(((O275*O275)+(H275*H275))*((O272*O272)+(H275*H275))*R251)","v":0}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O271*O271)+(O272*O272)+(H276*H276))","v":5},{"$f":"SQRT((O271*O271)+(O276*O276)+(H276*H276))","v":5},{"$f":"SQRT((O275*O275)+(O276*O276)+(H276*H276))","v":5},{"$f":"SQRT((O275*O275)+(O272*O272)+(H276*H276))","v":5},{"$f":"H276*O271*O272*((O271*O271)+(O272*O272)+(2*H276*H276))/(((O271*O271)+(H276*H276))*((O272*O272)+(H276*H276))*O252)","v":0},{"$f":"H276*O271*O276*((O271*O271)+(O276*O276)+(2*H276*H276))/(((O271*O271)+(H276*H276))*((O276*O276)+(H276*H276))*P252)","v":0},{"$f":"H276*O275*O276*((O275*O275)+(O276*O276)+(2*H276*H276))/(((O275*O275)+(H276*H276))*((O276*O276)+(H276*H276))*Q252)","v":0},{"$f":"H276*O275*O272*((O275*O275)+(O272*O272)+(2*H276*H276))/(((O275*O275)+(H276*H276))*((O272*O272)+(H276*H276))*R252)","v":0}]
[null,1,{"$f":"+$C$23","v":1},{"$f":"+$D$23","v":20},{"$f":"+$E$23","v":8000},{"$f":"IF(H273=0,\"   \",+H273)","v":0.5},{"$f":"IF(D280=0,\"       \",+D280)","v":40},{"$f":"F280","v":0},{"$f":"H280","v":0},{"$f":"+J280","v":8}]
[null,{"$f":"IF(H274=(H273+C253/2),\"\",2)","v":2},{"$f":"+$C$24","v":1},{"$f":"+$D$24","v":10},{"$f":"+$E$24","v":8000},{"$f":"IF(H274=H273,\"   \",+H274)","v":1.5},{"$f":"IF(D281=D280,\"       \",+D281)","v":55},0,0,{"$f":"+J281","v":11}]
[null,{"$f":"IF(H275=(H274+C254/2),\"\",3)","v":3},{"$f":"+$C$25","v":2},{"$f":"+$D$25","v":10},{"$f":"+$E$25","v":8000},{"$f":"IF(H275=H274,\"   \",+H275)","v":3},{"$f":"IF(D282=D281,\"       \",+D282)","v":70},0,0,{"$f":"+J282","v":14},null,null,null,null,{"$f":"SQRT((O271*O271)+(O272*O272)+(H277*H277))","v":7},{"$f":"SQRT((O271*O271)+(O276*O276)+(H277*H277))","v":7},{"$f":"SQRT((O275*O275)+(O276*O276)+(H277*H277))","v":7},{"$f":"SQRT((O275*O275)+(O272*O272)+(H277*H277))","v":7},{"$f":"H277*O271*O272*((O271*O271)+(O272*O272)+(2*H277*H277))/(((O271*O271)+(H277*H277))*((O272*O272)+(H277*H277))*O255)","v":0},{"$f":"H277*O271*O276*((O271*O271)+(O276*O276)+(2*H277*H277))/(((O271*O271)+(H277*H277))*((O276*O276)+(H277*H277))*P255)","v":0},{"$f":"H277*O275*O276*((O275*O275)+(O276*O276)+(2*H277*H277))/(((O275*O275)+(H277*H277))*((O276*O276)+(H277*H277))*Q255)","v":0},{"$f":"H277*O275*O272*((O275*O275)+(O272*O272)+(2*H277*H277))/(((O275*O275)+(H277*H277))*((O272*O272)+(H277*H277))*R255)","v":0}]
[null,{"$f":"IF(H276=(H275+C255/2),\"\",4)","v":4},{"$f":"+$C$26","v":2},{"$f":"+$D$26","v":10},{"$f":"+$E$26","v":8000},{"$f":"IF(H276=H275,\"   \",+H276)","v":5},{"$f":"IF(D283=D282,\"       \",+D283)","v":90},0,0,{"$f":"IF(D283=D282,\"\",+J283)","v":18},null,null,null,null,{"$f":"SQRT((O271*O271)+(O272*O272)+(H278*H278))","v":8.0050000000000008},{"$f":"SQRT((O271*O271)+(O276*O276)+(H278*H278))","v":8.0050000000000008},{"$f":"SQRT((O275*O275)+(O276*O276)+(H278*H278))","v":8.0050000000000008},{"$f":"SQRT((O275*O275)+(O272*O272)+(H278*H278))","v":8.0050000000000008},{"$f":"H278*O271*O272*((O271*O271)+(O272*O272)+(2*H278*H278))/(((O271*O271)+(H278*H278))*((O272*O272)+(H278*H278))*O256)","v":0},{"$f":"H278*O271*O276*((O271*O271)+(O276*O276)+(2*H278*H278))/(((O271*O271)+(H278*H278))*((O276*O276)+(H278*H278))*P256)","v":0},{"$f":"H278*O275*O276*((O275*O275)+(O276*O276)+(2*H278*H278))/(((O275*O275)+(H278*H278))*((O276*O276)+(H278*H278))*Q256)","v":0},{"$f":"H278*O275*O272*((O275*O275)+(O272*O272)+(2*H278*H278))/(((O275*O275)+(H278*H278))*((O272*O272)+(H278*H278))*R256)","v":0}]
[null,{"$f":"IF(H277=(H276+C256/2),\"\",5)","v":5},{"$f":"+$C$27","v":2},{"$f":"+$D$27","v":10},{"$f":"+$E$27","v":8000},{"$f":"IF(H277=H276,\"   \",+H277)","v":7},{"$f":"IF(D284=D283,\"       \",+D284)","v":110},0,0,{"$f":"IF(D284=D283,\"\",+J284)","v":22},null,null,null,null,{"$f":"ATAN((O271*O272)/(H273*O249))","v":0},{"$f":"ATAN((O271*O276)/(H273*P249))","v":0},{"$f":"ATAN((O275*O276)/(H273*Q249))","v":0},{"$f":"ATAN((O275*O272)/(H273*R249))","v":0}]
[null,{"$f":"IF(H278=(H277+C257/2),\"\",6)","v":6},{"$f":"+$C$28","v":0.01},{"$f":"+$D$28","v":10},{"$f":"+$E$28","v":8000},{"$f":"IF(H278=H277,\"   \",+H278)","v":8.0050000000000008},{"$f":"IF(D285=D284,\"       \",+D285)","v":120.05},0,0,{"$f":"IF(D285=D284,\"\",+J285)","v":24.01},null,null,null,null,{"$f":"ATAN((O271*O272)/(H274*O250))","v":0},{"$f":"ATAN((O271*O276)/(H274*P250))","v":0},{"$f":"ATAN((O275*O276)/(H274*Q250))","v":0},{"$f":"ATAN((O275*O272)/(H274*R250))","v":0}]
[null,null,null,null,null,null,null,"  S W =",0,"m ",null,null,null,null,{"$f":"ATAN((O271*O272)/(H275*O251))","v":0},{"$f":"ATAN((O271*O276)/(H275*P251))","v":0},{"$f":"ATAN((O275*O276)/(H275*Q251))","v":0},{"$f":"ATAN((O275*O272)/(H275*R251))","v":0}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O271*O272)/(H276*O252))","v":0},{"$f":"ATAN((O271*O276)/(H276*P252))","v":0},{"$f":"ATAN((O275*O276)/(H276*Q252))","v":0},{"$f":"ATAN((O275*O272)/(H276*R252))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O271*O272)/(H277*O255))","v":0},{"$f":"ATAN((O271*O276)/(H277*P255))","v":0},{"$f":"ATAN((O275*O276)/(H277*Q255))","v":0},{"$f":"ATAN((O275*O272)/(H277*R255))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O271*O272)/(H278*O256))","v":0},{"$f":"ATAN((O271*O276)/(H278*P256))","v":0},{"$f":"ATAN((O275*O276)/(H278*Q256))","v":0},{"$f":"ATAN((O275*O272)/(H278*R256))","v":0}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E248","v":0},"m",null,null,null,null,{"$f":"E248/2","v":0}]
[null,null,"     širina temelja  B=",{"$f":"E249","v":0},"m",null,null,null,null,{"$f":"E249/2","v":0}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G248","v":0},"kPa",null,null,null,null,{"$f":"J245*J265","v":0}]
[null,null,"      dubina temeljenja Df=",{"$f":"E250","v":0},"m",null,null,null,null,{"$f":"J246*J266","v":0}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J267+J265","v":0}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J268+J266","v":0}]
[1,null,"      H1=",{"$f":"IF(C253=0,\"      \",C253)","v":1},"m        Mk1=",{"$f":"IF(E253=0,\"       \",+E253)","v":8000},"KN/m2     z1=",{"$f":"C253/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C253+C254/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C253+C254+C255/2","v":3},"m",null,null,null,null,null,{"$f":"J267-J265","v":0}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C253+C254+C255+C256/2","v":5},"m",null,null,null,null,null,{"$f":"J268-J266","v":0}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C253+C254+C255+C256+C257/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C253+C254+C255+C256+C257+C258/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O257)-(P257)+(Q257)-(R257)+(S249)-(T249)+(U249)-(V249))/(2*3.14159)","v":0},{"$f":"+D234","v":40},"kPa     Dp1=",{"$f":"(G248)*C280","v":0},"kPa        w1=",{"$f":"IF(E253=0,\"       \",+F280*C253/E253)","v":0},"m",{"$f":"0.2*D280","v":8}]
[null,"    I42=",{"$f":"((O258)-(P258)+(Q258)-(R258)+(S250)-(T250)+(U250)-(V250))/(2*3.14159)","v":0},55,"kPa     Dp2=",{"$f":"IF(H274=H273,\"     \",(G248)*C281)","v":0},"kPa       w2=",0,"m",11]
[null,"    I43=",{"$f":"((O259)-(P259)+(Q259)-(R259)+(S251)-(T251)+(U251)-(V251))/(2*3.14159)","v":0},70,"kPa     Dp3=",{"$f":"IF(H275=H274,\"     \",(G248)*C282)","v":0},"kPa       w3=",0,"m",14]
[null,"    I44=",{"$f":"((O260)-(P260)+(Q260)-(R260)+(S252)-(T252)+(U252)-(V252))/(2*3.14159)","v":0},90,"kPa     Dp4=",{"$f":"IF(H276=H275,\"     \",(G248)*C283)","v":0},"kPa       w4=",0,"m",18]
[null,"    I45=",{"$f":"((O261)-(P261)+(Q261)-(R261)+(S255)-(T255)+(U255)-(V255))/(2*3.14159)","v":0},110,"kPa     Dp5=",{"$f":"IF(H277=H276,\"     \",(G248)*C284)","v":0},"kPa       w5=",0,"m",22]
[null,"    I46=",{"$f":"((P262)-(Q262)+(R262)-(S262)+(S256)-(T256)+(U256)-(V256))/(2*3.14159)","v":0},120.05,"kPa     Dp6=",{"$f":"IF(H278=H277,\"       \",(G248)*C285)","v":0},"kPa       w6=",0,"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H280:H285)","v":0},"m"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[]
[null,null,"SLIJEGANJE TOČKE TS1 OD TEMELJA T7",null,null,null,null,null,"       x=L/2*",{"$f":"I11","v":0},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"I12","v":0}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!K13","v":0},"m         Dpa'=",{"$f":"+Slijeganje!K17","v":0},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!K14","v":0},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O317*O317)+(O318*O318)+(H319*H319))","v":0.5},{"$f":"SQRT((O317*O317)+(O322*O322)+(H319*H319))","v":0.5},{"$f":"SQRT((O321*O321)+(O322*O322)+(H319*H319))","v":0.5},{"$f":"SQRT((O321*O321)+(O318*O318)+(H319*H319))","v":0.5},{"$f":"H319*O317*O318*((O317*O317)+(O318*O318)+(2*H319*H319))/(((O317*O317)+(H319*H319))*((O318*O318)+(H319*H319))*O295)","v":0},{"$f":"H319*O317*O322*((O317*O317)+(O322*O322)+(2*H319*H319))/(((O317*O317)+(H319*H319))*((O322*O322)+(H319*H319))*P295)","v":0},{"$f":"H319*O321*O322*((O321*O321)+(O322*O322)+(2*H319*H319))/(((O321*O321)+(H319*H319))*((O322*O322)+(H319*H319))*Q295)","v":0},{"$f":"H319*O321*O318*((O321*O321)+(O318*O318)+(2*H319*H319))/(((O321*O321)+(H319*H319))*((O318*O318)+(H319*H319))*R295)","v":0}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!K15","v":0},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O317*O317)+(O318*O318)+(H320*H320))","v":1.5},{"$f":"SQRT((O317*O317)+(O322*O322)+(H320*H320))","v":1.5},{"$f":"SQRT((O321*O321)+(O322*O322)+(H320*H320))","v":1.5},{"$f":"SQRT((O321*O321)+(O318*O318)+(H320*H320))","v":1.5},{"$f":"H320*O317*O318*((O317*O317)+(O318*O318)+(2*H320*H320))/(((O317*O317)+(H320*H320))*((O318*O318)+(H320*H320))*O296)","v":0},{"$f":"H320*O317*O322*((O317*O317)+(O322*O322)+(2*H320*H320))/(((O317*O317)+(H320*H320))*((O322*O322)+(H320*H320))*P296)","v":0},{"$f":"H320*O321*O322*((O321*O321)+(O322*O322)+(2*H320*H320))/(((O321*O321)+(H320*H320))*((O322*O322)+(H320*H320))*Q296)","v":0},{"$f":"H320*O321*O318*((O321*O321)+(O318*O318)+(2*H320*H320))/(((O321*O321)+(H320*H320))*((O318*O318)+(H320*H320))*R296)","v":0}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O317*O317)+(O318*O318)+(H321*H321))","v":3},{"$f":"SQRT((O317*O317)+(O322*O322)+(H321*H321))","v":3},{"$f":"SQRT((O321*O321)+(O322*O322)+(H321*H321))","v":3},{"$f":"SQRT((O321*O321)+(O318*O318)+(H321*H321))","v":3},{"$f":"H321*O317*O318*((O317*O317)+(O318*O318)+(2*H321*H321))/(((O317*O317)+(H321*H321))*((O318*O318)+(H321*H321))*O297)","v":0},{"$f":"H321*O317*O322*((O317*O317)+(O322*O322)+(2*H321*H321))/(((O317*O317)+(H321*H321))*((O322*O322)+(H321*H321))*P297)","v":0},{"$f":"H321*O321*O322*((O321*O321)+(O322*O322)+(2*H321*H321))/(((O321*O321)+(H321*H321))*((O322*O322)+(H321*H321))*Q297)","v":0},{"$f":"H321*O321*O318*((O321*O321)+(O318*O318)+(2*H321*H321))/(((O321*O321)+(H321*H321))*((O318*O318)+(H321*H321))*R297)","v":0}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O317*O317)+(O318*O318)+(H322*H322))","v":5},{"$f":"SQRT((O317*O317)+(O322*O322)+(H322*H322))","v":5},{"$f":"SQRT((O321*O321)+(O322*O322)+(H322*H322))","v":5},{"$f":"SQRT((O321*O321)+(O318*O318)+(H322*H322))","v":5},{"$f":"H322*O317*O318*((O317*O317)+(O318*O318)+(2*H322*H322))/(((O317*O317)+(H322*H322))*((O318*O318)+(H322*H322))*O298)","v":0},{"$f":"H322*O317*O322*((O317*O317)+(O322*O322)+(2*H322*H322))/(((O317*O317)+(H322*H322))*((O322*O322)+(H322*H322))*P298)","v":0},{"$f":"H322*O321*O322*((O321*O321)+(O322*O322)+(2*H322*H322))/(((O321*O321)+(H322*H322))*((O322*O322)+(H322*H322))*Q298)","v":0},{"$f":"H322*O321*O318*((O321*O321)+(O318*O318)+(2*H322*H322))/(((O321*O321)+(H322*H322))*((O318*O318)+(H322*H322))*R298)","v":0}]
[null,1,{"$f":"+$C$23","v":1},{"$f":"+$D$23","v":20},{"$f":"+$E$23","v":8000},{"$f":"IF(H319=0,\"   \",+H319)","v":0.5},{"$f":"IF(D326=0,\"       \",+D326)","v":40},{"$f":"F326","v":0},{"$f":"H326","v":0},{"$f":"+J326","v":8}]
[null,{"$f":"IF(H320=(H319+C299/2),\"\",2)","v":2},{"$f":"+$C$24","v":1},{"$f":"+$D$24","v":10},{"$f":"+$E$24","v":8000},{"$f":"IF(H320=H319,\"   \",+H320)","v":1.5},{"$f":"IF(D327=D326,\"       \",+D327)","v":55},0,0,{"$f":"+J327","v":11}]
[null,{"$f":"IF(H321=(H320+C300/2),\"\",3)","v":3},{"$f":"+$C$25","v":2},{"$f":"+$D$25","v":10},{"$f":"+$E$25","v":8000},{"$f":"IF(H321=H320,\"   \",+H321)","v":3},{"$f":"IF(D328=D327,\"       \",+D328)","v":70},0,0,{"$f":"+J328","v":14},null,null,null,null,{"$f":"SQRT((O317*O317)+(O318*O318)+(H323*H323))","v":7},{"$f":"SQRT((O317*O317)+(O322*O322)+(H323*H323))","v":7},{"$f":"SQRT((O321*O321)+(O322*O322)+(H323*H323))","v":7},{"$f":"SQRT((O321*O321)+(O318*O318)+(H323*H323))","v":7},{"$f":"H323*O317*O318*((O317*O317)+(O318*O318)+(2*H323*H323))/(((O317*O317)+(H323*H323))*((O318*O318)+(H323*H323))*O301)","v":0},{"$f":"H323*O317*O322*((O317*O317)+(O322*O322)+(2*H323*H323))/(((O317*O317)+(H323*H323))*((O322*O322)+(H323*H323))*P301)","v":0},{"$f":"H323*O321*O322*((O321*O321)+(O322*O322)+(2*H323*H323))/(((O321*O321)+(H323*H323))*((O322*O322)+(H323*H323))*Q301)","v":0},{"$f":"H323*O321*O318*((O321*O321)+(O318*O318)+(2*H323*H323))/(((O321*O321)+(H323*H323))*((O318*O318)+(H323*H323))*R301)","v":0}]
[null,{"$f":"IF(H322=(H321+C301/2),\"\",4)","v":4},{"$f":"+$C$26","v":2},{"$f":"+$D$26","v":10},{"$f":"+$E$26","v":8000},{"$f":"IF(H322=H321,\"   \",+H322)","v":5},{"$f":"IF(D329=D328,\"       \",+D329)","v":90},0,0,{"$f":"IF(D329=D328,\"\",+J329)","v":18},null,null,null,null,{"$f":"SQRT((O317*O317)+(O318*O318)+(H324*H324))","v":8.0050000000000008},{"$f":"SQRT((O317*O317)+(O322*O322)+(H324*H324))","v":8.0050000000000008},{"$f":"SQRT((O321*O321)+(O322*O322)+(H324*H324))","v":8.0050000000000008},{"$f":"SQRT((O321*O321)+(O318*O318)+(H324*H324))","v":8.0050000000000008},{"$f":"H324*O317*O318*((O317*O317)+(O318*O318)+(2*H324*H324))/(((O317*O317)+(H324*H324))*((O318*O318)+(H324*H324))*O302)","v":0},{"$f":"H324*O317*O322*((O317*O317)+(O322*O322)+(2*H324*H324))/(((O317*O317)+(H324*H324))*((O322*O322)+(H324*H324))*P302)","v":0},{"$f":"H324*O321*O322*((O321*O321)+(O322*O322)+(2*H324*H324))/(((O321*O321)+(H324*H324))*((O322*O322)+(H324*H324))*Q302)","v":0},{"$f":"H324*O321*O318*((O321*O321)+(O318*O318)+(2*H324*H324))/(((O321*O321)+(H324*H324))*((O318*O318)+(H324*H324))*R302)","v":0}]
[null,{"$f":"IF(H323=(H322+C302/2),\"\",5)","v":5},{"$f":"+$C$27","v":2},{"$f":"+$D$27","v":10},{"$f":"+$E$27","v":8000},{"$f":"IF(H323=H322,\"   \",+H323)","v":7},{"$f":"IF(D330=D329,\"       \",+D330)","v":110},0,0,{"$f":"IF(D330=D329,\"\",+J330)","v":22},null,null,null,null,{"$f":"ATAN((O317*O318)/(H319*O295))","v":0},{"$f":"ATAN((O317*O322)/(H319*P295))","v":0},{"$f":"ATAN((O321*O322)/(H319*Q295))","v":0},{"$f":"ATAN((O321*O318)/(H319*R295))","v":0}]
[null,{"$f":"IF(H324=(H323+C303/2),\"\",6)","v":6},{"$f":"+$C$28","v":0.01},{"$f":"+$D$28","v":10},{"$f":"+$E$28","v":8000},{"$f":"IF(H324=H323,\"   \",+H324)","v":8.0050000000000008},{"$f":"IF(D331=D330,\"       \",+D331)","v":120.05},0,0,{"$f":"IF(D331=D330,\"\",+J331)","v":24.01},null,null,null,null,{"$f":"ATAN((O317*O318)/(H320*O296))","v":0},{"$f":"ATAN((O317*O322)/(H320*P296))","v":0},{"$f":"ATAN((O321*O322)/(H320*Q296))","v":0},{"$f":"ATAN((O321*O318)/(H320*R296))","v":0}]
[null,null,null,null,null,null,null,"  S W =",0,"m ",null,null,null,null,{"$f":"ATAN((O317*O318)/(H321*O297))","v":0},{"$f":"ATAN((O317*O322)/(H321*P297))","v":0},{"$f":"ATAN((O321*O322)/(H321*Q297))","v":0},{"$f":"ATAN((O321*O318)/(H321*R297))","v":0}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O317*O318)/(H322*O298))","v":0},{"$f":"ATAN((O317*O322)/(H322*P298))","v":0},{"$f":"ATAN((O321*O322)/(H322*Q298))","v":0},{"$f":"ATAN((O321*O318)/(H322*R298))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O317*O318)/(H323*O301))","v":0},{"$f":"ATAN((O317*O322)/(H323*P301))","v":0},{"$f":"ATAN((O321*O322)/(H323*Q301))","v":0},{"$f":"ATAN((O321*O318)/(H323*R301))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O317*O318)/(H324*O302))","v":0},{"$f":"ATAN((O317*O322)/(H324*P302))","v":0},{"$f":"ATAN((O321*O322)/(H324*Q302))","v":0},{"$f":"ATAN((O321*O318)/(H324*R302))","v":0}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E294","v":0},"m",null,null,null,null,{"$f":"E294/2","v":0}]
[null,null,"     širina temelja  B=",{"$f":"E295","v":0},"m",null,null,null,null,{"$f":"E295/2","v":0}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G294","v":0},"kPa",null,null,null,null,{"$f":"J291*J311","v":0}]
[null,null,"      dubina temeljenja Df=",{"$f":"E296","v":0},"m",null,null,null,null,{"$f":"J292*J312","v":0}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J313+J311","v":0}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J314+J312","v":0}]
[1,null,"      H1=",{"$f":"IF(C299=0,\"      \",C299)","v":1},"m        Mk1=",{"$f":"IF(E299=0,\"       \",+E299)","v":8000},"KN/m2     z1=",{"$f":"C299/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C299+C300/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C299+C300+C301/2","v":3},"m",null,null,null,null,null,{"$f":"J313-J311","v":0}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C299+C300+C301+C302/2","v":5},"m",null,null,null,null,null,{"$f":"J314-J312","v":0}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C299+C300+C301+C302+C303/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C299+C300+C301+C302+C303+C304/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O303)-(P303)+(Q303)-(R303)+(S295)-(T295)+(U295)-(V295))/(2*3.14159)","v":0},{"$f":"+D280","v":40},"kPa     Dp1=",{"$f":"(G294)*C326","v":0},"kPa        w1=",{"$f":"IF(E299=0,\"       \",+F326*C299/E299)","v":0},"m",{"$f":"0.2*D326","v":8}]
[null,"    I42=",{"$f":"((O304)-(P304)+(Q304)-(R304)+(S296)-(T296)+(U296)-(V296))/(2*3.14159)","v":0},55,"kPa     Dp2=",{"$f":"IF(H320=H319,\"     \",(G294)*C327)","v":0},"kPa       w2=",0,"m",11]
[null,"    I43=",{"$f":"((O305)-(P305)+(Q305)-(R305)+(S297)-(T297)+(U297)-(V297))/(2*3.14159)","v":0},70,"kPa     Dp3=",{"$f":"IF(H321=H320,\"     \",(G294)*C328)","v":0},"kPa       w3=",0,"m",14]
[null,"    I44=",{"$f":"((O306)-(P306)+(Q306)-(R306)+(S298)-(T298)+(U298)-(V298))/(2*3.14159)","v":0},90,"kPa     Dp4=",{"$f":"IF(H322=H321,\"     \",(G294)*C329)","v":0},"kPa       w4=",0,"m",18]
[null,"    I45=",{"$f":"((O307)-(P307)+(Q307)-(R307)+(S301)-(T301)+(U301)-(V301))/(2*3.14159)","v":0},110,"kPa     Dp5=",{"$f":"IF(H323=H322,\"     \",(G294)*C330)","v":0},"kPa       w5=",0,"m",22]
[null,"    I46=",{"$f":"((P308)-(Q308)+(R308)-(S308)+(S302)-(T302)+(U302)-(V302))/(2*3.14159)","v":0},120.05,"kPa     Dp6=",{"$f":"IF(H324=H323,\"       \",(G294)*C331)","v":0},"kPa       w6=",0,"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H326:H331)","v":0},"m"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[]
[null,null,"SLIJEGANJE TOČKE TS1 OD TEMELJA T8",null,null,null,null,null,"       x=L/2*",{"$f":"J11","v":0},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"J12","v":0}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!L13","v":0},"m         Dpa'=",{"$f":"+Slijeganje!L17","v":0},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!L14","v":0},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O363*O363)+(O364*O364)+(H365*H365))","v":0.5},{"$f":"SQRT((O363*O363)+(O368*O368)+(H365*H365))","v":0.5},{"$f":"SQRT((O367*O367)+(O368*O368)+(H365*H365))","v":0.5},{"$f":"SQRT((O367*O367)+(O364*O364)+(H365*H365))","v":0.5},{"$f":"H365*O363*O364*((O363*O363)+(O364*O364)+(2*H365*H365))/(((O363*O363)+(H365*H365))*((O364*O364)+(H365*H365))*O341)","v":0},{"$f":"H365*O363*O368*((O363*O363)+(O368*O368)+(2*H365*H365))/(((O363*O363)+(H365*H365))*((O368*O368)+(H365*H365))*P341)","v":0},{"$f":"H365*O367*O368*((O367*O367)+(O368*O368)+(2*H365*H365))/(((O367*O367)+(H365*H365))*((O368*O368)+(H365*H365))*Q341)","v":0},{"$f":"H365*O367*O364*((O367*O367)+(O364*O364)+(2*H365*H365))/(((O367*O367)+(H365*H365))*((O364*O364)+(H365*H365))*R341)","v":0}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!L15","v":0},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O363*O363)+(O364*O364)+(H366*H366))","v":1.5},{"$f":"SQRT((O363*O363)+(O368*O368)+(H366*H366))","v":1.5},{"$f":"SQRT((O367*O367)+(O368*O368)+(H366*H366))","v":1.5},{"$f":"SQRT((O367*O367)+(O364*O364)+(H366*H366))","v":1.5},{"$f":"H366*O363*O364*((O363*O363)+(O364*O364)+(2*H366*H366))/(((O363*O363)+(H366*H366))*((O364*O364)+(H366*H366))*O342)","v":0},{"$f":"H366*O363*O368*((O363*O363)+(O368*O368)+(2*H366*H366))/(((O363*O363)+(H366*H366))*((O368*O368)+(H366*H366))*P342)","v":0},{"$f":"H366*O367*O368*((O367*O367)+(O368*O368)+(2*H366*H366))/(((O367*O367)+(H366*H366))*((O368*O368)+(H366*H366))*Q342)","v":0},{"$f":"H366*O367*O364*((O367*O367)+(O364*O364)+(2*H366*H366))/(((O367*O367)+(H366*H366))*((O364*O364)+(H366*H366))*R342)","v":0}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O363*O363)+(O364*O364)+(H367*H367))","v":3},{"$f":"SQRT((O363*O363)+(O368*O368)+(H367*H367))","v":3},{"$f":"SQRT((O367*O367)+(O368*O368)+(H367*H367))","v":3},{"$f":"SQRT((O367*O367)+(O364*O364)+(H367*H367))","v":3},{"$f":"H367*O363*O364*((O363*O363)+(O364*O364)+(2*H367*H367))/(((O363*O363)+(H367*H367))*((O364*O364)+(H367*H367))*O343)","v":0},{"$f":"H367*O363*O368*((O363*O363)+(O368*O368)+(2*H367*H367))/(((O363*O363)+(H367*H367))*((O368*O368)+(H367*H367))*P343)","v":0},{"$f":"H367*O367*O368*((O367*O367)+(O368*O368)+(2*H367*H367))/(((O367*O367)+(H367*H367))*((O368*O368)+(H367*H367))*Q343)","v":0},{"$f":"H367*O367*O364*((O367*O367)+(O364*O364)+(2*H367*H367))/(((O367*O367)+(H367*H367))*((O364*O364)+(H367*H367))*R343)","v":0}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O363*O363)+(O364*O364)+(H368*H368))","v":5},{"$f":"SQRT((O363*O363)+(O368*O368)+(H368*H368))","v":5},{"$f":"SQRT((O367*O367)+(O368*O368)+(H368*H368))","v":5},{"$f":"SQRT((O367*O367)+(O364*O364)+(H368*H368))","v":5},{"$f":"H368*O363*O364*((O363*O363)+(O364*O364)+(2*H368*H368))/(((O363*O363)+(H368*H368))*((O364*O364)+(H368*H368))*O344)","v":0},{"$f":"H368*O363*O368*((O363*O363)+(O368*O368)+(2*H368*H368))/(((O363*O363)+(H368*H368))*((O368*O368)+(H368*H368))*P344)","v":0},{"$f":"H368*O367*O368*((O367*O367)+(O368*O368)+(2*H368*H368))/(((O367*O367)+(H368*H368))*((O368*O368)+(H368*H368))*Q344)","v":0},{"$f":"H368*O367*O364*((O367*O367)+(O364*O364)+(2*H368*H368))/(((O367*O367)+(H368*H368))*((O364*O364)+(H368*H368))*R344)","v":0}]
[null,1,{"$f":"+$C$23","v":1},{"$f":"+$D$23","v":20},{"$f":"+$E$23","v":8000},{"$f":"IF(H365=0,\"   \",+H365)","v":0.5},{"$f":"IF(D372=0,\"       \",+D372)","v":40},{"$f":"F372","v":0},{"$f":"H372","v":0},{"$f":"+J372","v":8}]
[null,{"$f":"IF(H366=(H365+C345/2),\"\",2)","v":2},{"$f":"+$C$24","v":1},{"$f":"+$D$24","v":10},{"$f":"+$E$24","v":8000},{"$f":"IF(H366=H365,\"   \",+H366)","v":1.5},{"$f":"IF(D373=D372,\"       \",+D373)","v":55},0,0,{"$f":"+J373","v":11}]
[null,{"$f":"IF(H367=(H366+C346/2),\"\",3)","v":3},{"$f":"+$C$25","v":2},{"$f":"+$D$25","v":10},{"$f":"+$E$25","v":8000},{"$f":"IF(H367=H366,\"   \",+H367)","v":3},{"$f":"IF(D374=D373,\"       \",+D374)","v":70},0,0,{"$f":"+J374","v":14},null,null,null,null,{"$f":"SQRT((O363*O363)+(O364*O364)+(H369*H369))","v":7},{"$f":"SQRT((O363*O363)+(O368*O368)+(H369*H369))","v":7},{"$f":"SQRT((O367*O367)+(O368*O368)+(H369*H369))","v":7},{"$f":"SQRT((O367*O367)+(O364*O364)+(H369*H369))","v":7},{"$f":"H369*O363*O364*((O363*O363)+(O364*O364)+(2*H369*H369))/(((O363*O363)+(H369*H369))*((O364*O364)+(H369*H369))*O347)","v":0},{"$f":"H369*O363*O368*((O363*O363)+(O368*O368)+(2*H369*H369))/(((O363*O363)+(H369*H369))*((O368*O368)+(H369*H369))*P347)","v":0},{"$f":"H369*O367*O368*((O367*O367)+(O368*O368)+(2*H369*H369))/(((O367*O367)+(H369*H369))*((O368*O368)+(H369*H369))*Q347)","v":0},{"$f":"H369*O367*O364*((O367*O367)+(O364*O364)+(2*H369*H369))/(((O367*O367)+(H369*H369))*((O364*O364)+(H369*H369))*R347)","v":0}]
[null,{"$f":"IF(H368=(H367+C347/2),\"\",4)","v":4},{"$f":"+$C$26","v":2},{"$f":"+$D$26","v":10},{"$f":"+$E$26","v":8000},{"$f":"IF(H368=H367,\"   \",+H368)","v":5},{"$f":"IF(D375=D374,\"       \",+D375)","v":90},0,0,{"$f":"IF(D375=D374,\"\",+J375)","v":18},null,null,null,null,{"$f":"SQRT((O363*O363)+(O364*O364)+(H370*H370))","v":8.0050000000000008},{"$f":"SQRT((O363*O363)+(O368*O368)+(H370*H370))","v":8.0050000000000008},{"$f":"SQRT((O367*O367)+(O368*O368)+(H370*H370))","v":8.0050000000000008},{"$f":"SQRT((O367*O367)+(O364*O364)+(H370*H370))","v":8.0050000000000008},{"$f":"H370*O363*O364*((O363*O363)+(O364*O364)+(2*H370*H370))/(((O363*O363)+(H370*H370))*((O364*O364)+(H370*H370))*O348)","v":0},{"$f":"H370*O363*O368*((O363*O363)+(O368*O368)+(2*H370*H370))/(((O363*O363)+(H370*H370))*((O368*O368)+(H370*H370))*P348)","v":0},{"$f":"H370*O367*O368*((O367*O367)+(O368*O368)+(2*H370*H370))/(((O367*O367)+(H370*H370))*((O368*O368)+(H370*H370))*Q348)","v":0},{"$f":"H370*O367*O364*((O367*O367)+(O364*O364)+(2*H370*H370))/(((O367*O367)+(H370*H370))*((O364*O364)+(H370*H370))*R348)","v":0}]
[null,{"$f":"IF(H369=(H368+C348/2),\"\",5)","v":5},{"$f":"+$C$27","v":2},{"$f":"+$D$27","v":10},{"$f":"+$E$27","v":8000},{"$f":"IF(H369=H368,\"   \",+H369)","v":7},{"$f":"IF(D376=D375,\"       \",+D376)","v":110},0,0,{"$f":"IF(D376=D375,\"\",+J376)","v":22},null,null,null,null,{"$f":"ATAN((O363*O364)/(H365*O341))","v":0},{"$f":"ATAN((O363*O368)/(H365*P341))","v":0},{"$f":"ATAN((O367*O368)/(H365*Q341))","v":0},{"$f":"ATAN((O367*O364)/(H365*R341))","v":0}]
[null,{"$f":"IF(H370=(H369+C349/2),\"\",6)","v":6},{"$f":"+$C$28","v":0.01},{"$f":"+$D$28","v":10},{"$f":"+$E$28","v":8000},{"$f":"IF(H370=H369,\"   \",+H370)","v":8.0050000000000008},{"$f":"IF(D377=D376,\"       \",+D377)","v":120.05},0,0,{"$f":"IF(D377=D376,\"\",+J377)","v":24.01},null,null,null,null,{"$f":"ATAN((O363*O364)/(H366*O342))","v":0},{"$f":"ATAN((O363*O368)/(H366*P342))","v":0},{"$f":"ATAN((O367*O368)/(H366*Q342))","v":0},{"$f":"ATAN((O367*O364)/(H366*R342))","v":0}]
[null,null,null,null,null,null,null,"  S W =",0,"m ",null,null,null,null,{"$f":"ATAN((O363*O364)/(H367*O343))","v":0},{"$f":"ATAN((O363*O368)/(H367*P343))","v":0},{"$f":"ATAN((O367*O368)/(H367*Q343))","v":0},{"$f":"ATAN((O367*O364)/(H367*R343))","v":0}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O363*O364)/(H368*O344))","v":0},{"$f":"ATAN((O363*O368)/(H368*P344))","v":0},{"$f":"ATAN((O367*O368)/(H368*Q344))","v":0},{"$f":"ATAN((O367*O364)/(H368*R344))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O363*O364)/(H369*O347))","v":0},{"$f":"ATAN((O363*O368)/(H369*P347))","v":0},{"$f":"ATAN((O367*O368)/(H369*Q347))","v":0},{"$f":"ATAN((O367*O364)/(H369*R347))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O363*O364)/(H370*O348))","v":0},{"$f":"ATAN((O363*O368)/(H370*P348))","v":0},{"$f":"ATAN((O367*O368)/(H370*Q348))","v":0},{"$f":"ATAN((O367*O364)/(H370*R348))","v":0}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E340","v":0},"m",null,null,null,null,{"$f":"E340/2","v":0}]
[null,null,"     širina temelja  B=",{"$f":"E341","v":0},"m",null,null,null,null,{"$f":"E341/2","v":0}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G340","v":0},"kPa",null,null,null,null,{"$f":"J337*J357","v":0}]
[null,null,"      dubina temeljenja Df=",{"$f":"E342","v":0},"m",null,null,null,null,{"$f":"J338*J358","v":0}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J359+J357","v":0}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J360+J358","v":0}]
[1,null,"      H1=",{"$f":"IF(C345=0,\"      \",C345)","v":1},"m        Mk1=",{"$f":"IF(E345=0,\"       \",+E345)","v":8000},"KN/m2     z1=",{"$f":"C345/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C345+C346/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C345+C346+C347/2","v":3},"m",null,null,null,null,null,{"$f":"J359-J357","v":0}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C345+C346+C347+C348/2","v":5},"m",null,null,null,null,null,{"$f":"J360-J358","v":0}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C345+C346+C347+C348+C349/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C345+C346+C347+C348+C349+C350/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O349)-(P349)+(Q349)-(R349)+(S341)-(T341)+(U341)-(V341))/(2*3.14159)","v":0},{"$f":"+D326","v":40},"kPa     Dp1=",{"$f":"(G340)*C372","v":0},"kPa        w1=",{"$f":"IF(E345=0,\"       \",+F372*C345/E345)","v":0},"m",{"$f":"0.2*D372","v":8}]
[null,"    I42=",{"$f":"((O350)-(P350)+(Q350)-(R350)+(S342)-(T342)+(U342)-(V342))/(2*3.14159)","v":0},55,"kPa     Dp2=",{"$f":"IF(H366=H365,\"     \",(G340)*C373)","v":0},"kPa       w2=",0,"m",11]
[null,"    I43=",{"$f":"((O351)-(P351)+(Q351)-(R351)+(S343)-(T343)+(U343)-(V343))/(2*3.14159)","v":0},70,"kPa     Dp3=",{"$f":"IF(H367=H366,\"     \",(G340)*C374)","v":0},"kPa       w3=",0,"m",14]
[null,"    I44=",{"$f":"((O352)-(P352)+(Q352)-(R352)+(S344)-(T344)+(U344)-(V344))/(2*3.14159)","v":0},90,"kPa     Dp4=",{"$f":"IF(H368=H367,\"     \",(G340)*C375)","v":0},"kPa       w4=",0,"m",18]
[null,"    I45=",{"$f":"((O353)-(P353)+(Q353)-(R353)+(S347)-(T347)+(U347)-(V347))/(2*3.14159)","v":0},110,"kPa     Dp5=",{"$f":"IF(H369=H368,\"     \",(G340)*C376)","v":0},"kPa       w5=",0,"m",22]
[null,"    I46=",{"$f":"((P354)-(Q354)+(R354)-(S354)+(S348)-(T348)+(U348)-(V348))/(2*3.14159)","v":0},120.05,"kPa     Dp6=",{"$f":"IF(H370=H369,\"       \",(G340)*C377)","v":0},"kPa       w6=",0,"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H372:H377)","v":0},"m"]

{"sheet":"T2","index":34,"n_rows":378,"n_cols":22,"rows_kept":378,"cut":false,"hidden":true,"merged":[[108,2,108,3],[108,4,108,5],[8,0,8,1],[292,2,292,3],[292,4,292,5],[16,2,16,3],[16,4,16,5],[62,2,62,3],[62,4,62,5],[338,2,338,3],[338,4,338,5],[154,2,154,3],[154,4,154,5],[200,2,200,3],[200,4,200,5],[246,2,246,3],[246,4,246,5]]}
["Dimenzije temelja:",null,"T1","T2"]
[null,"L",{"$f":"+Slijeganje!E13","v":12},{"$f":"+Slijeganje!F13","v":12}]
[null,"B",{"$f":"+Slijeganje!E14","v":2.9000021999999994},{"$f":"+Slijeganje!F14","v":2.9000021999999994}]
[null,"Df=",{"$f":"+Slijeganje!E15","v":1.5001009999999999},{"$f":"+Slijeganje!F15","v":1.5001009999999999}]
["opterećenje: /kn/m2/",null,{"$f":"+Slijeganje!E17","v":{"$error":"#VALUE!"}},{"$f":"+Slijeganje!F17","v":{"$error":"#VALUE!"}}]
["Težište temelja      x",null,{"$f":"+Slijeganje!E18","v":6},{"$f":"+Slijeganje!F18","v":6}]
[null,"y",{"$f":"+Slijeganje!E19","v":1.4500010999999997},{"$f":"+Slijeganje!F19","v":1.4500010999999997}]
["Točka u kojoj se",null,"TS2"]
["računa slijeganje              x",null,{"$f":"+Slijeganje!F21","v":1.56}]
[null,"y",{"$f":"+Slijeganje!F22","v":2.5230019139999995}]
[null,"xL",{"$f":"ABS($C$9-C6)/C2*2","v":0.73999999999999988},{"$f":"ABS($C$9-D6)/D2*2","v":0.73999999999999988}]
[null,"yB",{"$f":"+ABS($C$10-C7)/C3*2","v":0.74},{"$f":"+ABS($C$10-D7)/D3*2","v":0.74}]
[]
[]
[null,null,"SLIJEGANJE TOČKE TS2 OD TEMELJA T1",null,null,null,null,null,"       x=L/2*",{"$f":"+C11","v":0.73999999999999988},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"+C12","v":0.74}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!E13","v":12},"m         Dpa'=",{"$f":"+Slijeganje!F17","v":{"$error":"#VALUE!"}},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!E14","v":2.9000021999999994},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O41*O41)+(O42*O42)+(H43*H43))","v":10.752169021088147},{"$f":"SQRT((O41*O41)+(O46*O46)+(H43*H43))","v":10.458763273716643},{"$f":"SQRT((O45*O45)+(O46*O46)+(H43*H43))","v":1.6809905459710603},{"$f":"SQRT((O45*O45)+(O42*O42)+(H43*H43))","v":3.0081786280152416},{"$f":"H43*O41*O42*((O41*O41)+(O42*O42)+(2*H43*H43))/(((O41*O41)+(H43*H43))*((O42*O42)+(H43*H43))*O19)","v":0.19636364301930606},{"$f":"H43*O41*O46*((O41*O41)+(O46*O46)+(2*H43*H43))/(((O41*O41)+(H43*H43))*((O46*O46)+(H43*H43))*P19)","v":-0.48156925795510397},{"$f":"H43*O45*O46*((O45*O45)+(O46*O46)+(2*H43*H43))/(((O45*O45)+(H43*H43))*((O46*O46)+(H43*H43))*Q19)","v":0.51129568251091073},{"$f":"H43*O45*O42*((O45*O45)+(O42*O42)+(2*H43*H43))/(((O45*O45)+(H43*H43))*((O42*O42)+(H43*H43))*R19)","v":-0.34266384985112436}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!E15","v":1.5001009999999999},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O41*O41)+(O42*O42)+(H44*H44))","v":10.844774716795534},{"$f":"SQRT((O41*O41)+(O46*O46)+(H44*H44))","v":10.553943775463468},{"$f":"SQRT((O45*O45)+(O46*O46)+(H44*H44))","v":2.1967542456187683},{"$f":"SQRT((O45*O45)+(O42*O42)+(H44*H44))","v":3.3240244671253043},{"$f":"H44*O41*O42*((O41*O41)+(O42*O42)+(2*H44*H44))/(((O41*O41)+(H44*H44))*((O42*O42)+(H44*H44))*O20)","v":0.45561969101701461},{"$f":"H44*O41*O46*((O41*O41)+(O46*O46)+(2*H44*H44))/(((O41*O41)+(H44*H44))*((O46*O46)+(H44*H44))*P20)","v":-0.23887675696849342},{"$f":"H44*O45*O46*((O45*O45)+(O46*O46)+(2*H44*H44))/(((O45*O45)+(H44*H44))*((O46*O46)+(H44*H44))*Q20)","v":0.25361961236358982},{"$f":"H44*O45*O42*((O45*O45)+(O42*O42)+(2*H44*H44))/(((O45*O45)+(H44*H44))*((O42*O42)+(H44*H44))*R20)","v":-0.5853700614304056}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O41*O41)+(O42*O42)+(H45*H45))","v":11.151642868118026},{"$f":"SQRT((O41*O41)+(O46*O46)+(H45*H45))","v":10.869026139247438},{"$f":"SQRT((O45*O45)+(O46*O46)+(H45*H45))","v":3.4023123336407672},{"$f":"SQRT((O45*O45)+(O42*O42)+(H45*H45))","v":4.2189025418996895},{"$f":"H45*O41*O42*((O41*O41)+(O42*O42)+(2*H45*H45))/(((O41*O41)+(H45*H45))*((O42*O42)+(H45*H45))*O21)","v":0.52121513855296753},{"$f":"H45*O41*O46*((O41*O41)+(O46*O46)+(2*H45*H45))/(((O41*O41)+(H45*H45))*((O46*O46)+(H45*H45))*P21)","v":-0.12803674097832882},{"$f":"H45*O45*O46*((O45*O45)+(O46*O46)+(2*H45*H45))/(((O45*O45)+(H45*H45))*((O46*O46)+(H45*H45))*Q21)","v":0.1020794306640232},{"$f":"H45*O45*O42*((O45*O45)+(O42*O42)+(2*H45*H45))/(((O45*O45)+(H45*H45))*((O42*O42)+(H45*H45))*R21)","v":-0.42692736365192813}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O41*O41)+(O42*O42)+(H46*H46))","v":11.847326224007155},{"$f":"SQRT((O41*O41)+(O46*O46)+(H46*H46))","v":11.581698028166857},{"$f":"SQRT((O45*O45)+(O46*O46)+(H46*H46))","v":5.2512597741536347},{"$f":"SQRT((O45*O45)+(O42*O42)+(H46*H46))","v":5.8137026633676117},{"$f":"H46*O41*O42*((O41*O41)+(O42*O42)+(2*H46*H46))/(((O41*O41)+(H46*H46))*((O42*O42)+(H46*H46))*O22)","v":0.43738021268409849},{"$f":"H46*O41*O46*((O41*O41)+(O46*O46)+(2*H46*H46))/(((O41*O41)+(H46*H46))*((O46*O46)+(H46*H46))*P22)","v":-8.0264135870411507E-2},{"$f":"H46*O45*O46*((O45*O45)+(O46*O46)+(2*H46*H46))/(((O45*O45)+(H46*H46))*((O46*O46)+(H46*H46))*Q22)","v":4.2684797783968532E-2},{"$f":"H46*O45*O42*((O45*O45)+(O42*O42)+(2*H46*H46))/(((O45*O45)+(H46*H46))*((O42*O42)+(H46*H46))*R22)","v":-0.23131019679513548}]
[null,1,{"$f":"+Slijeganje!H28","v":1},{"$f":"+Slijeganje!I28","v":20},{"$f":"+Slijeganje!J28","v":8000},{"$f":"IF(H43=0,\"   \",+H43)","v":0.5},{"$f":"IF(D50=0,\"       \",+D50)","v":40},{"$f":"F50","v":{"$error":"#VALUE!"}},{"$f":"H50","v":{"$error":"#VALUE!"}},{"$f":"+J50","v":8}]
[null,{"$f":"IF(H44=(H43+C23/2),\"\",2)","v":2},{"$f":"+Slijeganje!H29","v":1},{"$f":"+Slijeganje!I29","v":10},{"$f":"+Slijeganje!J29","v":8000},{"$f":"IF(H44=H43,\"   \",+H44)","v":1.5},{"$f":"IF(D51=D50,\"       \",+D51)","v":55},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+J51","v":11}]
[null,{"$f":"IF(H45=(H44+C24/2),\"\",3)","v":3},{"$f":"+Slijeganje!H30","v":2},{"$f":"+Slijeganje!I30","v":10},{"$f":"+Slijeganje!J30","v":8000},{"$f":"IF(H45=H44,\"   \",+H45)","v":3},{"$f":"IF(D52=D51,\"       \",+D52)","v":70},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+J52","v":14},null,null,null,null,{"$f":"SQRT((O41*O41)+(O42*O42)+(H47*H47))","v":12.820262815482669},{"$f":"SQRT((O41*O41)+(O46*O46)+(H47*H47))","v":12.575202949282531},{"$f":"SQRT((O45*O45)+(O46*O46)+(H47*H47))","v":7.1816244134348937},{"$f":"SQRT((O45*O45)+(O42*O42)+(H47*H47))","v":7.6025744756659677},{"$f":"H47*O41*O42*((O41*O41)+(O42*O42)+(2*H47*H47))/(((O41*O41)+(H47*H47))*((O42*O42)+(H47*H47))*O25)","v":0.35079340123228608},{"$f":"H47*O41*O46*((O41*O41)+(O46*O46)+(2*H47*H47))/(((O41*O41)+(H47*H47))*((O46*O46)+(H47*H47))*P25)","v":-5.845030324916508E-2},{"$f":"H47*O45*O46*((O45*O45)+(O46*O46)+(2*H47*H47))/(((O45*O45)+(H47*H47))*((O46*O46)+(H47*H47))*Q25)","v":2.2810453885631181E-2},{"$f":"H47*O45*O42*((O45*O45)+(O42*O42)+(2*H47*H47))/(((O45*O45)+(H47*H47))*((O42*O42)+(H47*H47))*R25)","v":-0.13591294801022338}]
[null,{"$f":"IF(H46=(H45+C25/2),\"\",4)","v":4},{"$f":"+Slijeganje!H31","v":2},{"$f":"+Slijeganje!I31","v":10},{"$f":"+Slijeganje!J31","v":8000},{"$f":"IF(H46=H45,\"   \",+H46)","v":5},{"$f":"IF(D53=D52,\"       \",+D53)","v":90},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D53=D52,\"\",+J53)","v":18},null,null,null,null,{"$f":"SQRT((O41*O41)+(O42*O42)+(H48*H48))","v":13.395490422453657},{"$f":"SQRT((O41*O41)+(O46*O46)+(H48*H48))","v":13.161145627020623},{"$f":"SQRT((O45*O45)+(O46*O46)+(H48*H48))","v":8.1642975335079555},{"$f":"SQRT((O45*O45)+(O42*O42)+(H48*H48))","v":8.5369294045369539},{"$f":"H48*O41*O42*((O41*O41)+(O42*O42)+(2*H48*H48))/(((O41*O41)+(H48*H48))*((O42*O42)+(H48*H48))*O26)","v":0.31439052318616756},{"$f":"H48*O41*O46*((O41*O41)+(O46*O46)+(2*H48*H48))/(((O41*O41)+(H48*H48))*((O46*O46)+(H48*H48))*P26)","v":-5.110743375621709E-2},{"$f":"H48*O45*O46*((O45*O45)+(O46*O46)+(2*H48*H48))/(((O45*O45)+(H48*H48))*((O46*O46)+(H48*H48))*Q26)","v":1.7648498562459976E-2},{"$f":"H48*O45*O42*((O45*O45)+(O42*O42)+(2*H48*H48))/(((O45*O45)+(H48*H48))*((O42*O42)+(H48*H48))*R26)","v":-0.10787696837105963}]
[null,{"$f":"IF(H47=(H46+C26/2),\"\",5)","v":5},{"$f":"+Slijeganje!H32","v":2},{"$f":"+Slijeganje!I32","v":10},{"$f":"+Slijeganje!J32","v":8000},{"$f":"IF(H47=H46,\"   \",+H47)","v":7},{"$f":"IF(D54=D53,\"       \",+D54)","v":110},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D54=D53,\"\",+J54)","v":22},null,null,null,null,{"$f":"ATAN((O41*O42)/(H43*O19))","v":1.3694593280275096},{"$f":"ATAN((O41*O46)/(H43*P19))","v":-0.64519359719234393},{"$f":"ATAN((O45*O46)/(H43*Q19))","v":0.61054528349481807},{"$f":"ATAN((O45*O42)/(H43*R19))","v":-1.2057738009809331}]
[null,{"$f":"IF(H48=(H47+C27/2),\"\",6)","v":6},{"$f":"+Slijeganje!H33","v":0.01},{"$f":"+Slijeganje!I33","v":10},{"$f":"+Slijeganje!J33","v":8000},{"$f":"IF(H48=H47,\"   \",+H48)","v":8.0050000000000008},{"$f":"IF(D55=D54,\"       \",+D55)","v":120.05},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D55=D54,\"\",+J55)","v":24.01},null,null,null,null,{"$f":"ATAN((O41*O42)/(H44*O20))","v":1.0175500375717115},{"$f":"ATAN((O41*O46)/(H44*P20))","v":-0.24367946210134675},{"$f":"ATAN((O45*O46)/(H44*Q20))","v":0.17662183950321556},{"$f":"ATAN((O45*O42)/(H44*R20))","v":-0.66823236211286796}]
[null,null,null,null,null,null,null,"  S W =",{"$error":"#VALUE!"},"m ",null,null,null,null,{"$f":"ATAN((O41*O42)/(H45*O21))","v":0.66696875500848141},{"$f":"ATAN((O41*O46)/(H45*P21))","v":-0.12012523800910783},{"$f":"ATAN((O45*O46)/(H45*Q21))","v":5.7556040648313406E-2},{"$f":"ATAN((O45*O42)/(H45*R21))","v":-0.3014923003067399}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O41*O42)/(H46*O22))","v":0.41840402748355454},{"$f":"ATAN((O41*O46)/(H46*P22))","v":-6.7862916946734964E-2},{"$f":"ATAN((O45*O46)/(H46*Q22))","v":2.2395468624673166E-2},{"$f":"ATAN((O45*O42)/(H46*R22))","v":-0.13458175982630699}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O41*O42)/(H47*O25))","v":0.28549221161305105},{"$f":"ATAN((O41*O46)/(H47*P25))","v":-4.4682757904761075E-2},{"$f":"ATAN((O45*O46)/(H47*Q25))","v":1.1698380349486639E-2},{"$f":"ATAN((O45*O42)/(H47*R25))","v":-7.3823307548584932E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O41*O42)/(H48*O26))","v":0.24087042826675767},{"$f":"ATAN((O41*O46)/(H48*P26))","v":-3.7340938551026569E-2},{"$f":"ATAN((O45*O46)/(H48*Q26))","v":8.9985885744867274E-3},{"$f":"ATAN((O45*O42)/(H48*R26))","v":-5.7530697805092901E-2}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E18","v":12},"m",null,null,null,null,{"$f":"E18/2","v":6}]
[null,null,"     širina temelja  B=",{"$f":"E19","v":2.9000021999999994},"m",null,null,null,null,{"$f":"E19/2","v":1.4500010999999997}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G18","v":{"$error":"#VALUE!"}},"kPa",null,null,null,null,{"$f":"J15*J35","v":4.4399999999999995}]
[null,null,"      dubina temeljenja Df=",{"$f":"E20","v":1.5001009999999999},"m",null,null,null,null,{"$f":"J16*J36","v":1.0730008139999998}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J37+J35","v":10.44}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J38+J36","v":2.5230019139999995}]
[1,null,"      H1=",{"$f":"IF(C23=0,\"      \",C23)","v":1},"m        Mk1=",{"$f":"IF(E23=0,\"       \",+E23)","v":8000},"KN/m2     z1=",{"$f":"C23/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C23+C24/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C23+C24+C25/2","v":3},"m",null,null,null,null,null,{"$f":"J37-J35","v":-1.5600000000000005}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C23+C24+C25+C26/2","v":5},"m",null,null,null,null,null,{"$f":"J38-J36","v":-0.37700028599999991}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C23+C24+C25+C26+C27/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C23+C24+C25+C26+C27+C28/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O27)-(P27)+(Q27)-(R27)+(S19)-(T19)+(U19)-(V19))/(2*3.14159)","v":0.85352710618381922},{"$f":"+'T1'!D50","v":40},"kPa     Dp1=",{"$f":"(G18)*C50","v":{"$error":"#VALUE!"}},"kPa        w1=",{"$f":"IF(E23=0,\"       \",+F50*C23/E23)","v":{"$error":"#VALUE!"}},"m",{"$f":"0.2*D50","v":8}]
[null,"    I42=",{"$f":"((O28)-(P28)+(Q28)-(R28)+(S20)-(T20)+(U20)-(V20))/(2*3.14159)","v":0.57925601734609633},{"$f":"+'T1'!D51","v":55},"kPa     Dp2=",{"$f":"IF(H44=H43,\"     \",(G18)*C51)","v":{"$error":"#VALUE!"}},"kPa       w2=",{"$error":"#VALUE!"},"m",11]
[null,"    I43=",{"$f":"((O29)-(P29)+(Q29)-(R29)+(S21)-(T21)+(U21)-(V21))/(2*3.14159)","v":0.36994022259745701},{"$f":"+'T1'!D52","v":70},"kPa     Dp3=",{"$f":"IF(H45=H44,\"     \",(G18)*C52)","v":{"$error":"#VALUE!"}},"kPa       w3=",{"$error":"#VALUE!"},"m",14]
[null,"    I44=",{"$f":"((O30)-(P30)+(Q30)-(R30)+(S22)-(T22)+(U22)-(V22))/(2*3.14159)","v":0.22836899722988735},{"$f":"+'T1'!D53","v":90},"kPa     Dp4=",{"$f":"IF(H46=H45,\"     \",(G18)*C53)","v":{"$error":"#VALUE!"}},"kPa       w4=",{"$error":"#VALUE!"},"m",18]
[null,"    I45=",{"$f":"((O31)-(P31)+(Q31)-(R31)+(S25)-(T25)+(U25)-(V25))/(2*3.14159)","v":0.15655508258448581},{"$f":"+'T1'!D54","v":110},"kPa     Dp5=",{"$f":"IF(H47=H46,\"     \",(G18)*C54)","v":{"$error":"#VALUE!"}},"kPa       w5=",{"$error":"#VALUE!"},"m",22]
[null,"    I46=",{"$f":"((P32)-(Q32)+(R32)-(S32)+(S26)-(T26)+(U26)-(V26))/(2*3.14159)","v":0.13301609647873661},{"$f":"+'T1'!D55","v":120.05},"kPa     Dp6=",{"$f":"IF(H48=H47,\"       \",(G18)*C55)","v":{"$error":"#VALUE!"}},"kPa       w6=",{"$error":"#VALUE!"},"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H50:H55)","v":{"$error":"#VALUE!"}},"m"]
[]
[]
[]
[]
[null,null,"SLIJEGANJE TOČKE TS2 OD TEMELJA T2",null,null,null,null,null,"       x=L/2*",{"$f":"D11","v":0.73999999999999988},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"D12","v":0.74}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!F13","v":12},"m         Dpa'=",{"$f":"+Slijeganje!F17","v":{"$error":"#VALUE!"}},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!F14","v":2.9000021999999994},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O87*O87)+(O88*O88)+(H89*H89))","v":10.752169021088147},{"$f":"SQRT((O87*O87)+(O92*O92)+(H89*H89))","v":10.458763273716643},{"$f":"SQRT((O91*O91)+(O92*O92)+(H89*H89))","v":1.6809905459710603},{"$f":"SQRT((O91*O91)+(O88*O88)+(H89*H89))","v":3.0081786280152416},{"$f":"H89*O87*O88*((O87*O87)+(O88*O88)+(2*H89*H89))/(((O87*O87)+(H89*H89))*((O88*O88)+(H89*H89))*O65)","v":0.19636364301930606},{"$f":"H89*O87*O92*((O87*O87)+(O92*O92)+(2*H89*H89))/(((O87*O87)+(H89*H89))*((O92*O92)+(H89*H89))*P65)","v":-0.48156925795510397},{"$f":"H89*O91*O92*((O91*O91)+(O92*O92)+(2*H89*H89))/(((O91*O91)+(H89*H89))*((O92*O92)+(H89*H89))*Q65)","v":0.51129568251091073},{"$f":"H89*O91*O88*((O91*O91)+(O88*O88)+(2*H89*H89))/(((O91*O91)+(H89*H89))*((O88*O88)+(H89*H89))*R65)","v":-0.34266384985112436}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!F15","v":1.5001009999999999},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O87*O87)+(O88*O88)+(H90*H90))","v":10.844774716795534},{"$f":"SQRT((O87*O87)+(O92*O92)+(H90*H90))","v":10.553943775463468},{"$f":"SQRT((O91*O91)+(O92*O92)+(H90*H90))","v":2.1967542456187683},{"$f":"SQRT((O91*O91)+(O88*O88)+(H90*H90))","v":3.3240244671253043},{"$f":"H90*O87*O88*((O87*O87)+(O88*O88)+(2*H90*H90))/(((O87*O87)+(H90*H90))*((O88*O88)+(H90*H90))*O66)","v":0.45561969101701461},{"$f":"H90*O87*O92*((O87*O87)+(O92*O92)+(2*H90*H90))/(((O87*O87)+(H90*H90))*((O92*O92)+(H90*H90))*P66)","v":-0.23887675696849342},{"$f":"H90*O91*O92*((O91*O91)+(O92*O92)+(2*H90*H90))/(((O91*O91)+(H90*H90))*((O92*O92)+(H90*H90))*Q66)","v":0.25361961236358982},{"$f":"H90*O91*O88*((O91*O91)+(O88*O88)+(2*H90*H90))/(((O91*O91)+(H90*H90))*((O88*O88)+(H90*H90))*R66)","v":-0.5853700614304056}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O87*O87)+(O88*O88)+(H91*H91))","v":11.151642868118026},{"$f":"SQRT((O87*O87)+(O92*O92)+(H91*H91))","v":10.869026139247438},{"$f":"SQRT((O91*O91)+(O92*O92)+(H91*H91))","v":3.4023123336407672},{"$f":"SQRT((O91*O91)+(O88*O88)+(H91*H91))","v":4.2189025418996895},{"$f":"H91*O87*O88*((O87*O87)+(O88*O88)+(2*H91*H91))/(((O87*O87)+(H91*H91))*((O88*O88)+(H91*H91))*O67)","v":0.52121513855296753},{"$f":"H91*O87*O92*((O87*O87)+(O92*O92)+(2*H91*H91))/(((O87*O87)+(H91*H91))*((O92*O92)+(H91*H91))*P67)","v":-0.12803674097832882},{"$f":"H91*O91*O92*((O91*O91)+(O92*O92)+(2*H91*H91))/(((O91*O91)+(H91*H91))*((O92*O92)+(H91*H91))*Q67)","v":0.1020794306640232},{"$f":"H91*O91*O88*((O91*O91)+(O88*O88)+(2*H91*H91))/(((O91*O91)+(H91*H91))*((O88*O88)+(H91*H91))*R67)","v":-0.42692736365192813}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O87*O87)+(O88*O88)+(H92*H92))","v":11.847326224007155},{"$f":"SQRT((O87*O87)+(O92*O92)+(H92*H92))","v":11.581698028166857},{"$f":"SQRT((O91*O91)+(O92*O92)+(H92*H92))","v":5.2512597741536347},{"$f":"SQRT((O91*O91)+(O88*O88)+(H92*H92))","v":5.8137026633676117},{"$f":"H92*O87*O88*((O87*O87)+(O88*O88)+(2*H92*H92))/(((O87*O87)+(H92*H92))*((O88*O88)+(H92*H92))*O68)","v":0.43738021268409849},{"$f":"H92*O87*O92*((O87*O87)+(O92*O92)+(2*H92*H92))/(((O87*O87)+(H92*H92))*((O92*O92)+(H92*H92))*P68)","v":-8.0264135870411507E-2},{"$f":"H92*O91*O92*((O91*O91)+(O92*O92)+(2*H92*H92))/(((O91*O91)+(H92*H92))*((O92*O92)+(H92*H92))*Q68)","v":4.2684797783968532E-2},{"$f":"H92*O91*O88*((O91*O91)+(O88*O88)+(2*H92*H92))/(((O91*O91)+(H92*H92))*((O88*O88)+(H92*H92))*R68)","v":-0.23131019679513548}]
[null,1,{"$f":"+$C$23","v":1},{"$f":"+$D$23","v":20},{"$f":"+$E$23","v":8000},{"$f":"IF(H89=0,\"   \",+H89)","v":0.5},{"$f":"IF(D96=0,\"       \",+D96)","v":40},{"$f":"F96","v":{"$error":"#VALUE!"}},{"$f":"H96","v":{"$error":"#VALUE!"}},{"$f":"+J96","v":8}]
[null,{"$f":"IF(H90=(H89+C69/2),\"\",2)","v":2},{"$f":"+$C$24","v":1},{"$f":"+$D$24","v":10},{"$f":"+$E$24","v":8000},{"$f":"IF(H90=H89,\"   \",+H90)","v":1.5},{"$f":"IF(D97=D96,\"       \",+D97)","v":55},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+J97","v":11}]
[null,{"$f":"IF(H91=(H90+C70/2),\"\",3)","v":3},{"$f":"+$C$25","v":2},{"$f":"+$D$25","v":10},{"$f":"+$E$25","v":8000},{"$f":"IF(H91=H90,\"   \",+H91)","v":3},{"$f":"IF(D98=D97,\"       \",+D98)","v":70},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+J98","v":14},null,null,null,null,{"$f":"SQRT((O87*O87)+(O88*O88)+(H93*H93))","v":12.820262815482669},{"$f":"SQRT((O87*O87)+(O92*O92)+(H93*H93))","v":12.575202949282531},{"$f":"SQRT((O91*O91)+(O92*O92)+(H93*H93))","v":7.1816244134348937},{"$f":"SQRT((O91*O91)+(O88*O88)+(H93*H93))","v":7.6025744756659677},{"$f":"H93*O87*O88*((O87*O87)+(O88*O88)+(2*H93*H93))/(((O87*O87)+(H93*H93))*((O88*O88)+(H93*H93))*O71)","v":0.35079340123228608},{"$f":"H93*O87*O92*((O87*O87)+(O92*O92)+(2*H93*H93))/(((O87*O87)+(H93*H93))*((O92*O92)+(H93*H93))*P71)","v":-5.845030324916508E-2},{"$f":"H93*O91*O92*((O91*O91)+(O92*O92)+(2*H93*H93))/(((O91*O91)+(H93*H93))*((O92*O92)+(H93*H93))*Q71)","v":2.2810453885631181E-2},{"$f":"H93*O91*O88*((O91*O91)+(O88*O88)+(2*H93*H93))/(((O91*O91)+(H93*H93))*((O88*O88)+(H93*H93))*R71)","v":-0.13591294801022338}]
[null,{"$f":"IF(H92=(H91+C71/2),\"\",4)","v":4},{"$f":"+$C$26","v":2},{"$f":"+$D$26","v":10},{"$f":"+$E$26","v":8000},{"$f":"IF(H92=H91,\"   \",+H92)","v":5},{"$f":"IF(D99=D98,\"       \",+D99)","v":90},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D99=D98,\"\",+J99)","v":18},null,null,null,null,{"$f":"SQRT((O87*O87)+(O88*O88)+(H94*H94))","v":13.395490422453657},{"$f":"SQRT((O87*O87)+(O92*O92)+(H94*H94))","v":13.161145627020623},{"$f":"SQRT((O91*O91)+(O92*O92)+(H94*H94))","v":8.1642975335079555},{"$f":"SQRT((O91*O91)+(O88*O88)+(H94*H94))","v":8.5369294045369539},{"$f":"H94*O87*O88*((O87*O87)+(O88*O88)+(2*H94*H94))/(((O87*O87)+(H94*H94))*((O88*O88)+(H94*H94))*O72)","v":0.31439052318616756},{"$f":"H94*O87*O92*((O87*O87)+(O92*O92)+(2*H94*H94))/(((O87*O87)+(H94*H94))*((O92*O92)+(H94*H94))*P72)","v":-5.110743375621709E-2},{"$f":"H94*O91*O92*((O91*O91)+(O92*O92)+(2*H94*H94))/(((O91*O91)+(H94*H94))*((O92*O92)+(H94*H94))*Q72)","v":1.7648498562459976E-2},{"$f":"H94*O91*O88*((O91*O91)+(O88*O88)+(2*H94*H94))/(((O91*O91)+(H94*H94))*((O88*O88)+(H94*H94))*R72)","v":-0.10787696837105963}]
[null,{"$f":"IF(H93=(H92+C72/2),\"\",5)","v":5},{"$f":"+$C$27","v":2},{"$f":"+$D$27","v":10},{"$f":"+$E$27","v":8000},{"$f":"IF(H93=H92,\"   \",+H93)","v":7},{"$f":"IF(D100=D99,\"       \",+D100)","v":110},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D100=D99,\"\",+J100)","v":22},null,null,null,null,{"$f":"ATAN((O87*O88)/(H89*O65))","v":1.3694593280275096},{"$f":"ATAN((O87*O92)/(H89*P65))","v":-0.64519359719234393},{"$f":"ATAN((O91*O92)/(H89*Q65))","v":0.61054528349481807},{"$f":"ATAN((O91*O88)/(H89*R65))","v":-1.2057738009809331}]
[null,{"$f":"IF(H94=(H93+C73/2),\"\",6)","v":6},{"$f":"+$C$28","v":0.01},{"$f":"+$D$28","v":10},{"$f":"+$E$28","v":8000},{"$f":"IF(H94=H93,\"   \",+H94)","v":8.0050000000000008},{"$f":"IF(D101=D100,\"       \",+D101)","v":120.05},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D101=D100,\"\",+J101)","v":24.01},null,null,null,null,{"$f":"ATAN((O87*O88)/(H90*O66))","v":1.0175500375717115},{"$f":"ATAN((O87*O92)/(H90*P66))","v":-0.24367946210134675},{"$f":"ATAN((O91*O92)/(H90*Q66))","v":0.17662183950321556},{"$f":"ATAN((O91*O88)/(H90*R66))","v":-0.66823236211286796}]
[null,null,null,null,null,null,null,"  S W =",{"$error":"#VALUE!"},"m ",null,null,null,null,{"$f":"ATAN((O87*O88)/(H91*O67))","v":0.66696875500848141},{"$f":"ATAN((O87*O92)/(H91*P67))","v":-0.12012523800910783},{"$f":"ATAN((O91*O92)/(H91*Q67))","v":5.7556040648313406E-2},{"$f":"ATAN((O91*O88)/(H91*R67))","v":-0.3014923003067399}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O87*O88)/(H92*O68))","v":0.41840402748355454},{"$f":"ATAN((O87*O92)/(H92*P68))","v":-6.7862916946734964E-2},{"$f":"ATAN((O91*O92)/(H92*Q68))","v":2.2395468624673166E-2},{"$f":"ATAN((O91*O88)/(H92*R68))","v":-0.13458175982630699}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O87*O88)/(H93*O71))","v":0.28549221161305105},{"$f":"ATAN((O87*O92)/(H93*P71))","v":-4.4682757904761075E-2},{"$f":"ATAN((O91*O92)/(H93*Q71))","v":1.1698380349486639E-2},{"$f":"ATAN((O91*O88)/(H93*R71))","v":-7.3823307548584932E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O87*O88)/(H94*O72))","v":0.24087042826675767},{"$f":"ATAN((O87*O92)/(H94*P72))","v":-3.7340938551026569E-2},{"$f":"ATAN((O91*O92)/(H94*Q72))","v":8.9985885744867274E-3},{"$f":"ATAN((O91*O88)/(H94*R72))","v":-5.7530697805092901E-2}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E64","v":12},"m",null,null,null,null,{"$f":"E64/2","v":6}]
[null,null,"     širina temelja  B=",{"$f":"E65","v":2.9000021999999994},"m",null,null,null,null,{"$f":"E65/2","v":1.4500010999999997}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G64","v":{"$error":"#VALUE!"}},"kPa",null,null,null,null,{"$f":"J61*J81","v":4.4399999999999995}]
[null,null,"      dubina temeljenja Df=",{"$f":"E66","v":1.5001009999999999},"m",null,null,null,null,{"$f":"J62*J82","v":1.0730008139999998}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J83+J81","v":10.44}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J84+J82","v":2.5230019139999995}]
[1,null,"      H1=",{"$f":"IF(C69=0,\"      \",C69)","v":1},"m        Mk1=",{"$f":"IF(E69=0,\"       \",+E69)","v":8000},"KN/m2     z1=",{"$f":"C69/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C69+C70/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C69+C70+C71/2","v":3},"m",null,null,null,null,null,{"$f":"J83-J81","v":-1.5600000000000005}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C69+C70+C71+C72/2","v":5},"m",null,null,null,null,null,{"$f":"J84-J82","v":-0.37700028599999991}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C69+C70+C71+C72+C73/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C69+C70+C71+C72+C73+C74/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O73)-(P73)+(Q73)-(R73)+(S65)-(T65)+(U65)-(V65))/(2*3.14159)","v":0.85352710618381922},{"$f":"+'T1'!D96","v":40},"kPa     Dp1=",{"$f":"(G64)*C96","v":{"$error":"#VALUE!"}},"kPa        w1=",{"$f":"IF(E69=0,\"       \",+F96*C69/E69)","v":{"$error":"#VALUE!"}},"m",{"$f":"0.2*D96","v":8}]
[null,"    I42=",{"$f":"((O74)-(P74)+(Q74)-(R74)+(S66)-(T66)+(U66)-(V66))/(2*3.14159)","v":0.57925601734609633},{"$f":"+'T1'!D97","v":55},"kPa     Dp2=",{"$f":"IF(H90=H89,\"     \",(G64)*C97)","v":{"$error":"#VALUE!"}},"kPa       w2=",{"$error":"#VALUE!"},"m",11]
[null,"    I43=",{"$f":"((O75)-(P75)+(Q75)-(R75)+(S67)-(T67)+(U67)-(V67))/(2*3.14159)","v":0.36994022259745701},{"$f":"+'T1'!D98","v":70},"kPa     Dp3=",{"$f":"IF(H91=H90,\"     \",(G64)*C98)","v":{"$error":"#VALUE!"}},"kPa       w3=",{"$error":"#VALUE!"},"m",14]
[null,"    I44=",{"$f":"((O76)-(P76)+(Q76)-(R76)+(S68)-(T68)+(U68)-(V68))/(2*3.14159)","v":0.22836899722988735},{"$f":"+'T1'!D99","v":90},"kPa     Dp4=",{"$f":"IF(H92=H91,\"     \",(G64)*C99)","v":{"$error":"#VALUE!"}},"kPa       w4=",{"$error":"#VALUE!"},"m",18]
[null,"    I45=",{"$f":"((O77)-(P77)+(Q77)-(R77)+(S71)-(T71)+(U71)-(V71))/(2*3.14159)","v":0.15655508258448581},{"$f":"+'T1'!D100","v":110},"kPa     Dp5=",{"$f":"IF(H93=H92,\"     \",(G64)*C100)","v":{"$error":"#VALUE!"}},"kPa       w5=",{"$error":"#VALUE!"},"m",22]
[null,"    I46=",{"$f":"((P78)-(Q78)+(R78)-(S78)+(S72)-(T72)+(U72)-(V72))/(2*3.14159)","v":0.13301609647873661},{"$f":"+'T1'!D101","v":120.05},"kPa     Dp6=",{"$f":"IF(H94=H93,\"       \",(G64)*C101)","v":{"$error":"#VALUE!"}},"kPa       w6=",{"$error":"#VALUE!"},"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H96:H101)","v":{"$error":"#VALUE!"}},"m"]
[]
[]
[]
[]
[null,null,"SLIJEGANJE TOČKE TS2 OD TEMELJA T3",null,null,null,null,null,"       x=L/2*",{"$f":"E11","v":0},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"E12","v":0}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!G13","v":0},"m         Dpa'=",{"$f":"+Slijeganje!G17","v":0},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!G14","v":0},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O133*O133)+(O134*O134)+(H135*H135))","v":0.5},{"$f":"SQRT((O133*O133)+(O138*O138)+(H135*H135))","v":0.5},{"$f":"SQRT((O137*O137)+(O138*O138)+(H135*H135))","v":0.5},{"$f":"SQRT((O137*O137)+(O134*O134)+(H135*H135))","v":0.5},{"$f":"H135*O133*O134*((O133*O133)+(O134*O134)+(2*H135*H135))/(((O133*O133)+(H135*H135))*((O134*O134)+(H135*H135))*O111)","v":0},{"$f":"H135*O133*O138*((O133*O133)+(O138*O138)+(2*H135*H135))/(((O133*O133)+(H135*H135))*((O138*O138)+(H135*H135))*P111)","v":0},{"$f":"H135*O137*O138*((O137*O137)+(O138*O138)+(2*H135*H135))/(((O137*O137)+(H135*H135))*((O138*O138)+(H135*H135))*Q111)","v":0},{"$f":"H135*O137*O134*((O137*O137)+(O134*O134)+(2*H135*H135))/(((O137*O137)+(H135*H135))*((O134*O134)+(H135*H135))*R111)","v":0}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!G15","v":0},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O133*O133)+(O134*O134)+(H136*H136))","v":1.5},{"$f":"SQRT((O133*O133)+(O138*O138)+(H136*H136))","v":1.5},{"$f":"SQRT((O137*O137)+(O138*O138)+(H136*H136))","v":1.5},{"$f":"SQRT((O137*O137)+(O134*O134)+(H136*H136))","v":1.5},{"$f":"H136*O133*O134*((O133*O133)+(O134*O134)+(2*H136*H136))/(((O133*O133)+(H136*H136))*((O134*O134)+(H136*H136))*O112)","v":0},{"$f":"H136*O133*O138*((O133*O133)+(O138*O138)+(2*H136*H136))/(((O133*O133)+(H136*H136))*((O138*O138)+(H136*H136))*P112)","v":0},{"$f":"H136*O137*O138*((O137*O137)+(O138*O138)+(2*H136*H136))/(((O137*O137)+(H136*H136))*((O138*O138)+(H136*H136))*Q112)","v":0},{"$f":"H136*O137*O134*((O137*O137)+(O134*O134)+(2*H136*H136))/(((O137*O137)+(H136*H136))*((O134*O134)+(H136*H136))*R112)","v":0}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O133*O133)+(O134*O134)+(H137*H137))","v":3},{"$f":"SQRT((O133*O133)+(O138*O138)+(H137*H137))","v":3},{"$f":"SQRT((O137*O137)+(O138*O138)+(H137*H137))","v":3},{"$f":"SQRT((O137*O137)+(O134*O134)+(H137*H137))","v":3},{"$f":"H137*O133*O134*((O133*O133)+(O134*O134)+(2*H137*H137))/(((O133*O133)+(H137*H137))*((O134*O134)+(H137*H137))*O113)","v":0},{"$f":"H137*O133*O138*((O133*O133)+(O138*O138)+(2*H137*H137))/(((O133*O133)+(H137*H137))*((O138*O138)+(H137*H137))*P113)","v":0},{"$f":"H137*O137*O138*((O137*O137)+(O138*O138)+(2*H137*H137))/(((O137*O137)+(H137*H137))*((O138*O138)+(H137*H137))*Q113)","v":0},{"$f":"H137*O137*O134*((O137*O137)+(O134*O134)+(2*H137*H137))/(((O137*O137)+(H137*H137))*((O134*O134)+(H137*H137))*R113)","v":0}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O133*O133)+(O134*O134)+(H138*H138))","v":5},{"$f":"SQRT((O133*O133)+(O138*O138)+(H138*H138))","v":5},{"$f":"SQRT((O137*O137)+(O138*O138)+(H138*H138))","v":5},{"$f":"SQRT((O137*O137)+(O134*O134)+(H138*H138))","v":5},{"$f":"H138*O133*O134*((O133*O133)+(O134*O134)+(2*H138*H138))/(((O133*O133)+(H138*H138))*((O134*O134)+(H138*H138))*O114)","v":0},{"$f":"H138*O133*O138*((O133*O133)+(O138*O138)+(2*H138*H138))/(((O133*O133)+(H138*H138))*((O138*O138)+(H138*H138))*P114)","v":0},{"$f":"H138*O137*O138*((O137*O137)+(O138*O138)+(2*H138*H138))/(((O137*O137)+(H138*H138))*((O138*O138)+(H138*H138))*Q114)","v":0},{"$f":"H138*O137*O134*((O137*O137)+(O134*O134)+(2*H138*H138))/(((O137*O137)+(H138*H138))*((O134*O134)+(H138*H138))*R114)","v":0}]
[null,1,{"$f":"+$C$23","v":1},{"$f":"+$D$23","v":20},{"$f":"+$E$23","v":8000},{"$f":"IF(H135=0,\"   \",+H135)","v":0.5},{"$f":"IF(D142=0,\"       \",+D142)","v":40},{"$f":"F142","v":0},{"$f":"H142","v":0},{"$f":"+J142","v":8}]
[null,{"$f":"IF(H136=(H135+C115/2),\"\",2)","v":2},{"$f":"+$C$24","v":1},{"$f":"+$D$24","v":10},{"$f":"+$E$24","v":8000},{"$f":"IF(H136=H135,\"   \",+H136)","v":1.5},{"$f":"IF(D143=D142,\"       \",+D143)","v":55},0,0,{"$f":"+J143","v":11}]
[null,{"$f":"IF(H137=(H136+C116/2),\"\",3)","v":3},{"$f":"+$C$25","v":2},{"$f":"+$D$25","v":10},{"$f":"+$E$25","v":8000},{"$f":"IF(H137=H136,\"   \",+H137)","v":3},{"$f":"IF(D144=D143,\"       \",+D144)","v":70},0,0,{"$f":"+J144","v":14},null,null,null,null,{"$f":"SQRT((O133*O133)+(O134*O134)+(H139*H139))","v":7},{"$f":"SQRT((O133*O133)+(O138*O138)+(H139*H139))","v":7},{"$f":"SQRT((O137*O137)+(O138*O138)+(H139*H139))","v":7},{"$f":"SQRT((O137*O137)+(O134*O134)+(H139*H139))","v":7},{"$f":"H139*O133*O134*((O133*O133)+(O134*O134)+(2*H139*H139))/(((O133*O133)+(H139*H139))*((O134*O134)+(H139*H139))*O117)","v":0},{"$f":"H139*O133*O138*((O133*O133)+(O138*O138)+(2*H139*H139))/(((O133*O133)+(H139*H139))*((O138*O138)+(H139*H139))*P117)","v":0},{"$f":"H139*O137*O138*((O137*O137)+(O138*O138)+(2*H139*H139))/(((O137*O137)+(H139*H139))*((O138*O138)+(H139*H139))*Q117)","v":0},{"$f":"H139*O137*O134*((O137*O137)+(O134*O134)+(2*H139*H139))/(((O137*O137)+(H139*H139))*((O134*O134)+(H139*H139))*R117)","v":0}]
[null,{"$f":"IF(H138=(H137+C117/2),\"\",4)","v":4},{"$f":"+$C$26","v":2},{"$f":"+$D$26","v":10},{"$f":"+$E$26","v":8000},{"$f":"IF(H138=H137,\"   \",+H138)","v":5},{"$f":"IF(D145=D144,\"       \",+D145)","v":90},0,0,{"$f":"IF(D145=D144,\"\",+J145)","v":18},null,null,null,null,{"$f":"SQRT((O133*O133)+(O134*O134)+(H140*H140))","v":8.0050000000000008},{"$f":"SQRT((O133*O133)+(O138*O138)+(H140*H140))","v":8.0050000000000008},{"$f":"SQRT((O137*O137)+(O138*O138)+(H140*H140))","v":8.0050000000000008},{"$f":"SQRT((O137*O137)+(O134*O134)+(H140*H140))","v":8.0050000000000008},{"$f":"H140*O133*O134*((O133*O133)+(O134*O134)+(2*H140*H140))/(((O133*O133)+(H140*H140))*((O134*O134)+(H140*H140))*O118)","v":0},{"$f":"H140*O133*O138*((O133*O133)+(O138*O138)+(2*H140*H140))/(((O133*O133)+(H140*H140))*((O138*O138)+(H140*H140))*P118)","v":0},{"$f":"H140*O137*O138*((O137*O137)+(O138*O138)+(2*H140*H140))/(((O137*O137)+(H140*H140))*((O138*O138)+(H140*H140))*Q118)","v":0},{"$f":"H140*O137*O134*((O137*O137)+(O134*O134)+(2*H140*H140))/(((O137*O137)+(H140*H140))*((O134*O134)+(H140*H140))*R118)","v":0}]
[null,{"$f":"IF(H139=(H138+C118/2),\"\",5)","v":5},{"$f":"+$C$27","v":2},{"$f":"+$D$27","v":10},{"$f":"+$E$27","v":8000},{"$f":"IF(H139=H138,\"   \",+H139)","v":7},{"$f":"IF(D146=D145,\"       \",+D146)","v":110},0,0,{"$f":"IF(D146=D145,\"\",+J146)","v":22},null,null,null,null,{"$f":"ATAN((O133*O134)/(H135*O111))","v":0},{"$f":"ATAN((O133*O138)/(H135*P111))","v":0},{"$f":"ATAN((O137*O138)/(H135*Q111))","v":0},{"$f":"ATAN((O137*O134)/(H135*R111))","v":0}]
[null,{"$f":"IF(H140=(H139+C119/2),\"\",6)","v":6},{"$f":"+$C$28","v":0.01},{"$f":"+$D$28","v":10},{"$f":"+$E$28","v":8000},{"$f":"IF(H140=H139,\"   \",+H140)","v":8.0050000000000008},{"$f":"IF(D147=D146,\"       \",+D147)","v":120.05},0,0,{"$f":"IF(D147=D146,\"\",+J147)","v":24.01},null,null,null,null,{"$f":"ATAN((O133*O134)/(H136*O112))","v":0},{"$f":"ATAN((O133*O138)/(H136*P112))","v":0},{"$f":"ATAN((O137*O138)/(H136*Q112))","v":0},{"$f":"ATAN((O137*O134)/(H136*R112))","v":0}]
[null,null,null,null,null,null,null,"  S W =",0,"m ",null,null,null,null,{"$f":"ATAN((O133*O134)/(H137*O113))","v":0},{"$f":"ATAN((O133*O138)/(H137*P113))","v":0},{"$f":"ATAN((O137*O138)/(H137*Q113))","v":0},{"$f":"ATAN((O137*O134)/(H137*R113))","v":0}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O133*O134)/(H138*O114))","v":0},{"$f":"ATAN((O133*O138)/(H138*P114))","v":0},{"$f":"ATAN((O137*O138)/(H138*Q114))","v":0},{"$f":"ATAN((O137*O134)/(H138*R114))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O133*O134)/(H139*O117))","v":0},{"$f":"ATAN((O133*O138)/(H139*P117))","v":0},{"$f":"ATAN((O137*O138)/(H139*Q117))","v":0},{"$f":"ATAN((O137*O134)/(H139*R117))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O133*O134)/(H140*O118))","v":0},{"$f":"ATAN((O133*O138)/(H140*P118))","v":0},{"$f":"ATAN((O137*O138)/(H140*Q118))","v":0},{"$f":"ATAN((O137*O134)/(H140*R118))","v":0}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E110","v":0},"m",null,null,null,null,{"$f":"E110/2","v":0}]
[null,null,"     širina temelja  B=",{"$f":"E111","v":0},"m",null,null,null,null,{"$f":"E111/2","v":0}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G110","v":0},"kPa",null,null,null,null,{"$f":"J107*J127","v":0}]
[null,null,"      dubina temeljenja Df=",{"$f":"E112","v":0},"m",null,null,null,null,{"$f":"J108*J128","v":0}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J129+J127","v":0}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J130+J128","v":0}]
[1,null,"      H1=",{"$f":"IF(C115=0,\"      \",C115)","v":1},"m        Mk1=",{"$f":"IF(E115=0,\"       \",+E115)","v":8000},"KN/m2     z1=",{"$f":"C115/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C115+C116/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C115+C116+C117/2","v":3},"m",null,null,null,null,null,{"$f":"J129-J127","v":0}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C115+C116+C117+C118/2","v":5},"m",null,null,null,null,null,{"$f":"J130-J128","v":0}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C115+C116+C117+C118+C119/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C115+C116+C117+C118+C119+C120/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O119)-(P119)+(Q119)-(R119)+(S111)-(T111)+(U111)-(V111))/(2*3.14159)","v":0},{"$f":"+'T1'!D142","v":40},"kPa     Dp1=",{"$f":"(G110)*C142","v":0},"kPa        w1=",{"$f":"IF(E115=0,\"       \",+F142*C115/E115)","v":0},"m",{"$f":"0.2*D142","v":8}]
[null,"    I42=",{"$f":"((O120)-(P120)+(Q120)-(R120)+(S112)-(T112)+(U112)-(V112))/(2*3.14159)","v":0},{"$f":"+'T1'!D143","v":55},"kPa     Dp2=",{"$f":"IF(H136=H135,\"     \",(G110)*C143)","v":0},"kPa       w2=",0,"m",11]
[null,"    I43=",{"$f":"((O121)-(P121)+(Q121)-(R121)+(S113)-(T113)+(U113)-(V113))/(2*3.14159)","v":0},{"$f":"+'T1'!D144","v":70},"kPa     Dp3=",{"$f":"IF(H137=H136,\"     \",(G110)*C144)","v":0},"kPa       w3=",0,"m",14]
[null,"    I44=",{"$f":"((O122)-(P122)+(Q122)-(R122)+(S114)-(T114)+(U114)-(V114))/(2*3.14159)","v":0},{"$f":"+'T1'!D145","v":90},"kPa     Dp4=",{"$f":"IF(H138=H137,\"     \",(G110)*C145)","v":0},"kPa       w4=",0,"m",18]
[null,"    I45=",{"$f":"((O123)-(P123)+(Q123)-(R123)+(S117)-(T117)+(U117)-(V117))/(2*3.14159)","v":0},{"$f":"+'T1'!D146","v":110},"kPa     Dp5=",{"$f":"IF(H139=H138,\"     \",(G110)*C146)","v":0},"kPa       w5=",0,"m",22]
[null,"    I46=",{"$f":"((P124)-(Q124)+(R124)-(S124)+(S118)-(T118)+(U118)-(V118))/(2*3.14159)","v":0},{"$f":"+'T1'!D147","v":120.05},"kPa     Dp6=",{"$f":"IF(H140=H139,\"       \",(G110)*C147)","v":0},"kPa       w6=",0,"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H142:H147)","v":0},"m"]
[]
[]
[]
[]
[null,null,"SLIJEGANJE TOČKE TS3 OD TEMELJA T4",null,null,null,null,null,"       x=L/2*",{"$f":"F11","v":0},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"F12","v":0}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!H13","v":0},"m         Dpa'=",{"$f":"+Slijeganje!H17","v":0},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!H14","v":0},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O179*O179)+(O180*O180)+(H181*H181))","v":0.5},{"$f":"SQRT((O179*O179)+(O184*O184)+(H181*H181))","v":0.5},{"$f":"SQRT((O183*O183)+(O184*O184)+(H181*H181))","v":0.5},{"$f":"SQRT((O183*O183)+(O180*O180)+(H181*H181))","v":0.5},{"$f":"H181*O179*O180*((O179*O179)+(O180*O180)+(2*H181*H181))/(((O179*O179)+(H181*H181))*((O180*O180)+(H181*H181))*O157)","v":0},{"$f":"H181*O179*O184*((O179*O179)+(O184*O184)+(2*H181*H181))/(((O179*O179)+(H181*H181))*((O184*O184)+(H181*H181))*P157)","v":0},{"$f":"H181*O183*O184*((O183*O183)+(O184*O184)+(2*H181*H181))/(((O183*O183)+(H181*H181))*((O184*O184)+(H181*H181))*Q157)","v":0},{"$f":"H181*O183*O180*((O183*O183)+(O180*O180)+(2*H181*H181))/(((O183*O183)+(H181*H181))*((O180*O180)+(H181*H181))*R157)","v":0}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!H15","v":0},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O179*O179)+(O180*O180)+(H182*H182))","v":1.5},{"$f":"SQRT((O179*O179)+(O184*O184)+(H182*H182))","v":1.5},{"$f":"SQRT((O183*O183)+(O184*O184)+(H182*H182))","v":1.5},{"$f":"SQRT((O183*O183)+(O180*O180)+(H182*H182))","v":1.5},{"$f":"H182*O179*O180*((O179*O179)+(O180*O180)+(2*H182*H182))/(((O179*O179)+(H182*H182))*((O180*O180)+(H182*H182))*O158)","v":0},{"$f":"H182*O179*O184*((O179*O179)+(O184*O184)+(2*H182*H182))/(((O179*O179)+(H182*H182))*((O184*O184)+(H182*H182))*P158)","v":0},{"$f":"H182*O183*O184*((O183*O183)+(O184*O184)+(2*H182*H182))/(((O183*O183)+(H182*H182))*((O184*O184)+(H182*H182))*Q158)","v":0},{"$f":"H182*O183*O180*((O183*O183)+(O180*O180)+(2*H182*H182))/(((O183*O183)+(H182*H182))*((O180*O180)+(H182*H182))*R158)","v":0}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O179*O179)+(O180*O180)+(H183*H183))","v":3},{"$f":"SQRT((O179*O179)+(O184*O184)+(H183*H183))","v":3},{"$f":"SQRT((O183*O183)+(O184*O184)+(H183*H183))","v":3},{"$f":"SQRT((O183*O183)+(O180*O180)+(H183*H183))","v":3},{"$f":"H183*O179*O180*((O179*O179)+(O180*O180)+(2*H183*H183))/(((O179*O179)+(H183*H183))*((O180*O180)+(H183*H183))*O159)","v":0},{"$f":"H183*O179*O184*((O179*O179)+(O184*O184)+(2*H183*H183))/(((O179*O179)+(H183*H183))*((O184*O184)+(H183*H183))*P159)","v":0},{"$f":"H183*O183*O184*((O183*O183)+(O184*O184)+(2*H183*H183))/(((O183*O183)+(H183*H183))*((O184*O184)+(H183*H183))*Q159)","v":0},{"$f":"H183*O183*O180*((O183*O183)+(O180*O180)+(2*H183*H183))/(((O183*O183)+(H183*H183))*((O180*O180)+(H183*H183))*R159)","v":0}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O179*O179)+(O180*O180)+(H184*H184))","v":5},{"$f":"SQRT((O179*O179)+(O184*O184)+(H184*H184))","v":5},{"$f":"SQRT((O183*O183)+(O184*O184)+(H184*H184))","v":5},{"$f":"SQRT((O183*O183)+(O180*O180)+(H184*H184))","v":5},{"$f":"H184*O179*O180*((O179*O179)+(O180*O180)+(2*H184*H184))/(((O179*O179)+(H184*H184))*((O180*O180)+(H184*H184))*O160)","v":0},{"$f":"H184*O179*O184*((O179*O179)+(O184*O184)+(2*H184*H184))/(((O179*O179)+(H184*H184))*((O184*O184)+(H184*H184))*P160)","v":0},{"$f":"H184*O183*O184*((O183*O183)+(O184*O184)+(2*H184*H184))/(((O183*O183)+(H184*H184))*((O184*O184)+(H184*H184))*Q160)","v":0},{"$f":"H184*O183*O180*((O183*O183)+(O180*O180)+(2*H184*H184))/(((O183*O183)+(H184*H184))*((O180*O180)+(H184*H184))*R160)","v":0}]
[null,1,{"$f":"+$C$23","v":1},{"$f":"+$D$23","v":20},{"$f":"+$E$23","v":8000},{"$f":"IF(H181=0,\"   \",+H181)","v":0.5},{"$f":"IF(D188=0,\"       \",+D188)","v":40},{"$f":"F188","v":0},{"$f":"H188","v":0},{"$f":"+J188","v":8}]
[null,{"$f":"IF(H182=(H181+C161/2),\"\",2)","v":2},{"$f":"+$C$24","v":1},{"$f":"+$D$24","v":10},{"$f":"+$E$24","v":8000},{"$f":"IF(H182=H181,\"   \",+H182)","v":1.5},{"$f":"IF(D189=D188,\"       \",+D189)","v":55},0,0,{"$f":"+J189","v":11}]
[null,{"$f":"IF(H183=(H182+C162/2),\"\",3)","v":3},{"$f":"+$C$25","v":2},{"$f":"+$D$25","v":10},{"$f":"+$E$25","v":8000},{"$f":"IF(H183=H182,\"   \",+H183)","v":3},{"$f":"IF(D190=D189,\"       \",+D190)","v":70},0,0,{"$f":"+J190","v":14},null,null,null,null,{"$f":"SQRT((O179*O179)+(O180*O180)+(H185*H185))","v":7},{"$f":"SQRT((O179*O179)+(O184*O184)+(H185*H185))","v":7},{"$f":"SQRT((O183*O183)+(O184*O184)+(H185*H185))","v":7},{"$f":"SQRT((O183*O183)+(O180*O180)+(H185*H185))","v":7},{"$f":"H185*O179*O180*((O179*O179)+(O180*O180)+(2*H185*H185))/(((O179*O179)+(H185*H185))*((O180*O180)+(H185*H185))*O163)","v":0},{"$f":"H185*O179*O184*((O179*O179)+(O184*O184)+(2*H185*H185))/(((O179*O179)+(H185*H185))*((O184*O184)+(H185*H185))*P163)","v":0},{"$f":"H185*O183*O184*((O183*O183)+(O184*O184)+(2*H185*H185))/(((O183*O183)+(H185*H185))*((O184*O184)+(H185*H185))*Q163)","v":0},{"$f":"H185*O183*O180*((O183*O183)+(O180*O180)+(2*H185*H185))/(((O183*O183)+(H185*H185))*((O180*O180)+(H185*H185))*R163)","v":0}]
[null,{"$f":"IF(H184=(H183+C163/2),\"\",4)","v":4},{"$f":"+$C$26","v":2},{"$f":"+$D$26","v":10},{"$f":"+$E$26","v":8000},{"$f":"IF(H184=H183,\"   \",+H184)","v":5},{"$f":"IF(D191=D190,\"       \",+D191)","v":90},0,0,{"$f":"IF(D191=D190,\"\",+J191)","v":18},null,null,null,null,{"$f":"SQRT((O179*O179)+(O180*O180)+(H186*H186))","v":8.0050000000000008},{"$f":"SQRT((O179*O179)+(O184*O184)+(H186*H186))","v":8.0050000000000008},{"$f":"SQRT((O183*O183)+(O184*O184)+(H186*H186))","v":8.0050000000000008},{"$f":"SQRT((O183*O183)+(O180*O180)+(H186*H186))","v":8.0050000000000008},{"$f":"H186*O179*O180*((O179*O179)+(O180*O180)+(2*H186*H186))/(((O179*O179)+(H186*H186))*((O180*O180)+(H186*H186))*O164)","v":0},{"$f":"H186*O179*O184*((O179*O179)+(O184*O184)+(2*H186*H186))/(((O179*O179)+(H186*H186))*((O184*O184)+(H186*H186))*P164)","v":0},{"$f":"H186*O183*O184*((O183*O183)+(O184*O184)+(2*H186*H186))/(((O183*O183)+(H186*H186))*((O184*O184)+(H186*H186))*Q164)","v":0},{"$f":"H186*O183*O180*((O183*O183)+(O180*O180)+(2*H186*H186))/(((O183*O183)+(H186*H186))*((O180*O180)+(H186*H186))*R164)","v":0}]
[null,{"$f":"IF(H185=(H184+C164/2),\"\",5)","v":5},{"$f":"+$C$27","v":2},{"$f":"+$D$27","v":10},{"$f":"+$E$27","v":8000},{"$f":"IF(H185=H184,\"   \",+H185)","v":7},{"$f":"IF(D192=D191,\"       \",+D192)","v":110},0,0,{"$f":"IF(D192=D191,\"\",+J192)","v":22},null,null,null,null,{"$f":"ATAN((O179*O180)/(H181*O157))","v":0},{"$f":"ATAN((O179*O184)/(H181*P157))","v":0},{"$f":"ATAN((O183*O184)/(H181*Q157))","v":0},{"$f":"ATAN((O183*O180)/(H181*R157))","v":0}]
[null,{"$f":"IF(H186=(H185+C165/2),\"\",6)","v":6},{"$f":"+$C$28","v":0.01},{"$f":"+$D$28","v":10},{"$f":"+$E$28","v":8000},{"$f":"IF(H186=H185,\"   \",+H186)","v":8.0050000000000008},{"$f":"IF(D193=D192,\"       \",+D193)","v":120.05},0,0,{"$f":"IF(D193=D192,\"\",+J193)","v":24.01},null,null,null,null,{"$f":"ATAN((O179*O180)/(H182*O158))","v":0},{"$f":"ATAN((O179*O184)/(H182*P158))","v":0},{"$f":"ATAN((O183*O184)/(H182*Q158))","v":0},{"$f":"ATAN((O183*O180)/(H182*R158))","v":0}]
[null,null,null,null,null,null,null,"  S W =",0,"m ",null,null,null,null,{"$f":"ATAN((O179*O180)/(H183*O159))","v":0},{"$f":"ATAN((O179*O184)/(H183*P159))","v":0},{"$f":"ATAN((O183*O184)/(H183*Q159))","v":0},{"$f":"ATAN((O183*O180)/(H183*R159))","v":0}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O179*O180)/(H184*O160))","v":0},{"$f":"ATAN((O179*O184)/(H184*P160))","v":0},{"$f":"ATAN((O183*O184)/(H184*Q160))","v":0},{"$f":"ATAN((O183*O180)/(H184*R160))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O179*O180)/(H185*O163))","v":0},{"$f":"ATAN((O179*O184)/(H185*P163))","v":0},{"$f":"ATAN((O183*O184)/(H185*Q163))","v":0},{"$f":"ATAN((O183*O180)/(H185*R163))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O179*O180)/(H186*O164))","v":0},{"$f":"ATAN((O179*O184)/(H186*P164))","v":0},{"$f":"ATAN((O183*O184)/(H186*Q164))","v":0},{"$f":"ATAN((O183*O180)/(H186*R164))","v":0}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E156","v":0},"m",null,null,null,null,{"$f":"E156/2","v":0}]
[null,null,"     širina temelja  B=",{"$f":"E157","v":0},"m",null,null,null,null,{"$f":"E157/2","v":0}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G156","v":0},"kPa",null,null,null,null,{"$f":"J153*J173","v":0}]
[null,null,"      dubina temeljenja Df=",{"$f":"E158","v":0},"m",null,null,null,null,{"$f":"J154*J174","v":0}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J175+J173","v":0}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J176+J174","v":0}]
[1,null,"      H1=",{"$f":"IF(C161=0,\"      \",C161)","v":1},"m        Mk1=",{"$f":"IF(E161=0,\"       \",+E161)","v":8000},"KN/m2     z1=",{"$f":"C161/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C161+C162/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C161+C162+C163/2","v":3},"m",null,null,null,null,null,{"$f":"J175-J173","v":0}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C161+C162+C163+C164/2","v":5},"m",null,null,null,null,null,{"$f":"J176-J174","v":0}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C161+C162+C163+C164+C165/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C161+C162+C163+C164+C165+C166/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O165)-(P165)+(Q165)-(R165)+(S157)-(T157)+(U157)-(V157))/(2*3.14159)","v":0},{"$f":"+'T1'!D188","v":40},"kPa     Dp1=",{"$f":"(G156)*C188","v":0},"kPa        w1=",{"$f":"IF(E161=0,\"       \",+F188*C161/E161)","v":0},"m",{"$f":"0.2*D188","v":8}]
[null,"    I42=",{"$f":"((O166)-(P166)+(Q166)-(R166)+(S158)-(T158)+(U158)-(V158))/(2*3.14159)","v":0},{"$f":"+'T1'!D189","v":55},"kPa     Dp2=",{"$f":"IF(H182=H181,\"     \",(G156)*C189)","v":0},"kPa       w2=",0,"m",11]
[null,"    I43=",{"$f":"((O167)-(P167)+(Q167)-(R167)+(S159)-(T159)+(U159)-(V159))/(2*3.14159)","v":0},{"$f":"+'T1'!D190","v":70},"kPa     Dp3=",{"$f":"IF(H183=H182,\"     \",(G156)*C190)","v":0},"kPa       w3=",0,"m",14]
[null,"    I44=",{"$f":"((O168)-(P168)+(Q168)-(R168)+(S160)-(T160)+(U160)-(V160))/(2*3.14159)","v":0},{"$f":"+'T1'!D191","v":90},"kPa     Dp4=",{"$f":"IF(H184=H183,\"     \",(G156)*C191)","v":0},"kPa       w4=",0,"m",18]
[null,"    I45=",{"$f":"((O169)-(P169)+(Q169)-(R169)+(S163)-(T163)+(U163)-(V163))/(2*3.14159)","v":0},{"$f":"+'T1'!D192","v":110},"kPa     Dp5=",{"$f":"IF(H185=H184,\"     \",(G156)*C192)","v":0},"kPa       w5=",0,"m",22]
[null,"    I46=",{"$f":"((P170)-(Q170)+(R170)-(S170)+(S164)-(T164)+(U164)-(V164))/(2*3.14159)","v":0},{"$f":"+'T1'!D193","v":120.05},"kPa     Dp6=",{"$f":"IF(H186=H185,\"       \",(G156)*C193)","v":0},"kPa       w6=",0,"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H188:H193)","v":0},"m"]
[]
[]
[]
[]
[null,null,"SLIJEGANJE TOČKE TS2 OD TEMELJA T5",null,null,null,null,null,"       x=L/2*",{"$f":"G11","v":0},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"G12","v":0}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!I13","v":0},"m         Dpa'=",{"$f":"+Slijeganje!I17","v":0},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!I14","v":0},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O225*O225)+(O226*O226)+(H227*H227))","v":0.5},{"$f":"SQRT((O225*O225)+(O230*O230)+(H227*H227))","v":0.5},{"$f":"SQRT((O229*O229)+(O230*O230)+(H227*H227))","v":0.5},{"$f":"SQRT((O229*O229)+(O226*O226)+(H227*H227))","v":0.5},{"$f":"H227*O225*O226*((O225*O225)+(O226*O226)+(2*H227*H227))/(((O225*O225)+(H227*H227))*((O226*O226)+(H227*H227))*O203)","v":0},{"$f":"H227*O225*O230*((O225*O225)+(O230*O230)+(2*H227*H227))/(((O225*O225)+(H227*H227))*((O230*O230)+(H227*H227))*P203)","v":0},{"$f":"H227*O229*O230*((O229*O229)+(O230*O230)+(2*H227*H227))/(((O229*O229)+(H227*H227))*((O230*O230)+(H227*H227))*Q203)","v":0},{"$f":"H227*O229*O226*((O229*O229)+(O226*O226)+(2*H227*H227))/(((O229*O229)+(H227*H227))*((O226*O226)+(H227*H227))*R203)","v":0}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!I15","v":0},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O225*O225)+(O226*O226)+(H228*H228))","v":1.5},{"$f":"SQRT((O225*O225)+(O230*O230)+(H228*H228))","v":1.5},{"$f":"SQRT((O229*O229)+(O230*O230)+(H228*H228))","v":1.5},{"$f":"SQRT((O229*O229)+(O226*O226)+(H228*H228))","v":1.5},{"$f":"H228*O225*O226*((O225*O225)+(O226*O226)+(2*H228*H228))/(((O225*O225)+(H228*H228))*((O226*O226)+(H228*H228))*O204)","v":0},{"$f":"H228*O225*O230*((O225*O225)+(O230*O230)+(2*H228*H228))/(((O225*O225)+(H228*H228))*((O230*O230)+(H228*H228))*P204)","v":0},{"$f":"H228*O229*O230*((O229*O229)+(O230*O230)+(2*H228*H228))/(((O229*O229)+(H228*H228))*((O230*O230)+(H228*H228))*Q204)","v":0},{"$f":"H228*O229*O226*((O229*O229)+(O226*O226)+(2*H228*H228))/(((O229*O229)+(H228*H228))*((O226*O226)+(H228*H228))*R204)","v":0}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O225*O225)+(O226*O226)+(H229*H229))","v":3},{"$f":"SQRT((O225*O225)+(O230*O230)+(H229*H229))","v":3},{"$f":"SQRT((O229*O229)+(O230*O230)+(H229*H229))","v":3},{"$f":"SQRT((O229*O229)+(O226*O226)+(H229*H229))","v":3},{"$f":"H229*O225*O226*((O225*O225)+(O226*O226)+(2*H229*H229))/(((O225*O225)+(H229*H229))*((O226*O226)+(H229*H229))*O205)","v":0},{"$f":"H229*O225*O230*((O225*O225)+(O230*O230)+(2*H229*H229))/(((O225*O225)+(H229*H229))*((O230*O230)+(H229*H229))*P205)","v":0},{"$f":"H229*O229*O230*((O229*O229)+(O230*O230)+(2*H229*H229))/(((O229*O229)+(H229*H229))*((O230*O230)+(H229*H229))*Q205)","v":0},{"$f":"H229*O229*O226*((O229*O229)+(O226*O226)+(2*H229*H229))/(((O229*O229)+(H229*H229))*((O226*O226)+(H229*H229))*R205)","v":0}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O225*O225)+(O226*O226)+(H230*H230))","v":5},{"$f":"SQRT((O225*O225)+(O230*O230)+(H230*H230))","v":5},{"$f":"SQRT((O229*O229)+(O230*O230)+(H230*H230))","v":5},{"$f":"SQRT((O229*O229)+(O226*O226)+(H230*H230))","v":5},{"$f":"H230*O225*O226*((O225*O225)+(O226*O226)+(2*H230*H230))/(((O225*O225)+(H230*H230))*((O226*O226)+(H230*H230))*O206)","v":0},{"$f":"H230*O225*O230*((O225*O225)+(O230*O230)+(2*H230*H230))/(((O225*O225)+(H230*H230))*((O230*O230)+(H230*H230))*P206)","v":0},{"$f":"H230*O229*O230*((O229*O229)+(O230*O230)+(2*H230*H230))/(((O229*O229)+(H230*H230))*((O230*O230)+(H230*H230))*Q206)","v":0},{"$f":"H230*O229*O226*((O229*O229)+(O226*O226)+(2*H230*H230))/(((O229*O229)+(H230*H230))*((O226*O226)+(H230*H230))*R206)","v":0}]
[null,1,{"$f":"+$C$23","v":1},{"$f":"+$D$23","v":20},{"$f":"+$E$23","v":8000},{"$f":"IF(H227=0,\"   \",+H227)","v":0.5},{"$f":"IF(D234=0,\"       \",+D234)","v":40},{"$f":"F234","v":0},{"$f":"H234","v":0},{"$f":"+J234","v":8}]
[null,{"$f":"IF(H228=(H227+C207/2),\"\",2)","v":2},{"$f":"+$C$24","v":1},{"$f":"+$D$24","v":10},{"$f":"+$E$24","v":8000},{"$f":"IF(H228=H227,\"   \",+H228)","v":1.5},{"$f":"IF(D235=D234,\"       \",+D235)","v":55},0,0,{"$f":"+J235","v":11}]
[null,{"$f":"IF(H229=(H228+C208/2),\"\",3)","v":3},{"$f":"+$C$25","v":2},{"$f":"+$D$25","v":10},{"$f":"+$E$25","v":8000},{"$f":"IF(H229=H228,\"   \",+H229)","v":3},{"$f":"IF(D236=D235,\"       \",+D236)","v":70},0,0,{"$f":"+J236","v":14},null,null,null,null,{"$f":"SQRT((O225*O225)+(O226*O226)+(H231*H231))","v":7},{"$f":"SQRT((O225*O225)+(O230*O230)+(H231*H231))","v":7},{"$f":"SQRT((O229*O229)+(O230*O230)+(H231*H231))","v":7},{"$f":"SQRT((O229*O229)+(O226*O226)+(H231*H231))","v":7},{"$f":"H231*O225*O226*((O225*O225)+(O226*O226)+(2*H231*H231))/(((O225*O225)+(H231*H231))*((O226*O226)+(H231*H231))*O209)","v":0},{"$f":"H231*O225*O230*((O225*O225)+(O230*O230)+(2*H231*H231))/(((O225*O225)+(H231*H231))*((O230*O230)+(H231*H231))*P209)","v":0},{"$f":"H231*O229*O230*((O229*O229)+(O230*O230)+(2*H231*H231))/(((O229*O229)+(H231*H231))*((O230*O230)+(H231*H231))*Q209)","v":0},{"$f":"H231*O229*O226*((O229*O229)+(O226*O226)+(2*H231*H231))/(((O229*O229)+(H231*H231))*((O226*O226)+(H231*H231))*R209)","v":0}]
[null,{"$f":"IF(H230=(H229+C209/2),\"\",4)","v":4},{"$f":"+$C$26","v":2},{"$f":"+$D$26","v":10},{"$f":"+$E$26","v":8000},{"$f":"IF(H230=H229,\"   \",+H230)","v":5},{"$f":"IF(D237=D236,\"       \",+D237)","v":90},0,0,{"$f":"IF(D237=D236,\"\",+J237)","v":18},null,null,null,null,{"$f":"SQRT((O225*O225)+(O226*O226)+(H232*H232))","v":8.0050000000000008},{"$f":"SQRT((O225*O225)+(O230*O230)+(H232*H232))","v":8.0050000000000008},{"$f":"SQRT((O229*O229)+(O230*O230)+(H232*H232))","v":8.0050000000000008},{"$f":"SQRT((O229*O229)+(O226*O226)+(H232*H232))","v":8.0050000000000008},{"$f":"H232*O225*O226*((O225*O225)+(O226*O226)+(2*H232*H232))/(((O225*O225)+(H232*H232))*((O226*O226)+(H232*H232))*O210)","v":0},{"$f":"H232*O225*O230*((O225*O225)+(O230*O230)+(2*H232*H232))/(((O225*O225)+(H232*H232))*((O230*O230)+(H232*H232))*P210)","v":0},{"$f":"H232*O229*O230*((O229*O229)+(O230*O230)+(2*H232*H232))/(((O229*O229)+(H232*H232))*((O230*O230)+(H232*H232))*Q210)","v":0},{"$f":"H232*O229*O226*((O229*O229)+(O226*O226)+(2*H232*H232))/(((O229*O229)+(H232*H232))*((O226*O226)+(H232*H232))*R210)","v":0}]
[null,{"$f":"IF(H231=(H230+C210/2),\"\",5)","v":5},{"$f":"+$C$27","v":2},{"$f":"+$D$27","v":10},{"$f":"+$E$27","v":8000},{"$f":"IF(H231=H230,\"   \",+H231)","v":7},{"$f":"IF(D238=D237,\"       \",+D238)","v":110},0,0,{"$f":"IF(D238=D237,\"\",+J238)","v":22},null,null,null,null,{"$f":"ATAN((O225*O226)/(H227*O203))","v":0},{"$f":"ATAN((O225*O230)/(H227*P203))","v":0},{"$f":"ATAN((O229*O230)/(H227*Q203))","v":0},{"$f":"ATAN((O229*O226)/(H227*R203))","v":0}]
[null,{"$f":"IF(H232=(H231+C211/2),\"\",6)","v":6},{"$f":"+$C$28","v":0.01},{"$f":"+$D$28","v":10},{"$f":"+$E$28","v":8000},{"$f":"IF(H232=H231,\"   \",+H232)","v":8.0050000000000008},{"$f":"IF(D239=D238,\"       \",+D239)","v":120.05},0,0,{"$f":"IF(D239=D238,\"\",+J239)","v":24.01},null,null,null,null,{"$f":"ATAN((O225*O226)/(H228*O204))","v":0},{"$f":"ATAN((O225*O230)/(H228*P204))","v":0},{"$f":"ATAN((O229*O230)/(H228*Q204))","v":0},{"$f":"ATAN((O229*O226)/(H228*R204))","v":0}]
[null,null,null,null,null,null,null,"  S W =",0,"m ",null,null,null,null,{"$f":"ATAN((O225*O226)/(H229*O205))","v":0},{"$f":"ATAN((O225*O230)/(H229*P205))","v":0},{"$f":"ATAN((O229*O230)/(H229*Q205))","v":0},{"$f":"ATAN((O229*O226)/(H229*R205))","v":0}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O225*O226)/(H230*O206))","v":0},{"$f":"ATAN((O225*O230)/(H230*P206))","v":0},{"$f":"ATAN((O229*O230)/(H230*Q206))","v":0},{"$f":"ATAN((O229*O226)/(H230*R206))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O225*O226)/(H231*O209))","v":0},{"$f":"ATAN((O225*O230)/(H231*P209))","v":0},{"$f":"ATAN((O229*O230)/(H231*Q209))","v":0},{"$f":"ATAN((O229*O226)/(H231*R209))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O225*O226)/(H232*O210))","v":0},{"$f":"ATAN((O225*O230)/(H232*P210))","v":0},{"$f":"ATAN((O229*O230)/(H232*Q210))","v":0},{"$f":"ATAN((O229*O226)/(H232*R210))","v":0}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E202","v":0},"m",null,null,null,null,{"$f":"E202/2","v":0}]
[null,null,"     širina temelja  B=",{"$f":"E203","v":0},"m",null,null,null,null,{"$f":"E203/2","v":0}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G202","v":0},"kPa",null,null,null,null,{"$f":"J199*J219","v":0}]
[null,null,"      dubina temeljenja Df=",{"$f":"E204","v":0},"m",null,null,null,null,{"$f":"J200*J220","v":0}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J221+J219","v":0}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J222+J220","v":0}]
[1,null,"      H1=",{"$f":"IF(C207=0,\"      \",C207)","v":1},"m        Mk1=",{"$f":"IF(E207=0,\"       \",+E207)","v":8000},"KN/m2     z1=",{"$f":"C207/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C207+C208/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C207+C208+C209/2","v":3},"m",null,null,null,null,null,{"$f":"J221-J219","v":0}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C207+C208+C209+C210/2","v":5},"m",null,null,null,null,null,{"$f":"J222-J220","v":0}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C207+C208+C209+C210+C211/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C207+C208+C209+C210+C211+C212/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O211)-(P211)+(Q211)-(R211)+(S203)-(T203)+(U203)-(V203))/(2*3.14159)","v":0},{"$f":"+'T1'!D234","v":40},"kPa     Dp1=",{"$f":"(G202)*C234","v":0},"kPa        w1=",{"$f":"IF(E207=0,\"       \",+F234*C207/E207)","v":0},"m",{"$f":"0.2*D234","v":8}]
[null,"    I42=",{"$f":"((O212)-(P212)+(Q212)-(R212)+(S204)-(T204)+(U204)-(V204))/(2*3.14159)","v":0},{"$f":"+'T1'!D235","v":55},"kPa     Dp2=",{"$f":"IF(H228=H227,\"     \",(G202)*C235)","v":0},"kPa       w2=",0,"m",11]
[null,"    I43=",{"$f":"((O213)-(P213)+(Q213)-(R213)+(S205)-(T205)+(U205)-(V205))/(2*3.14159)","v":0},{"$f":"+'T1'!D236","v":70},"kPa     Dp3=",{"$f":"IF(H229=H228,\"     \",(G202)*C236)","v":0},"kPa       w3=",0,"m",14]
[null,"    I44=",{"$f":"((O214)-(P214)+(Q214)-(R214)+(S206)-(T206)+(U206)-(V206))/(2*3.14159)","v":0},{"$f":"+'T1'!D237","v":90},"kPa     Dp4=",{"$f":"IF(H230=H229,\"     \",(G202)*C237)","v":0},"kPa       w4=",0,"m",18]
[null,"    I45=",{"$f":"((O215)-(P215)+(Q215)-(R215)+(S209)-(T209)+(U209)-(V209))/(2*3.14159)","v":0},{"$f":"+'T1'!D238","v":110},"kPa     Dp5=",{"$f":"IF(H231=H230,\"     \",(G202)*C238)","v":0},"kPa       w5=",0,"m",22]
[null,"    I46=",{"$f":"((P216)-(Q216)+(R216)-(S216)+(S210)-(T210)+(U210)-(V210))/(2*3.14159)","v":0},{"$f":"+'T1'!D239","v":120.05},"kPa     Dp6=",{"$f":"IF(H232=H231,\"       \",(G202)*C239)","v":0},"kPa       w6=",0,"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H234:H239)","v":0},"m"]
[]
[]
[]
[]
[null,null,"SLIJEGANJE TOČKE TS2 OD TEMELJA T6",null,null,null,null,null,"       x=L/2*",{"$f":"H11","v":0},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"H12","v":0}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!J13","v":0},"m         Dpa'=",{"$f":"+Slijeganje!J17","v":0},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!J14","v":0},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O271*O271)+(O272*O272)+(H273*H273))","v":0.5},{"$f":"SQRT((O271*O271)+(O276*O276)+(H273*H273))","v":0.5},{"$f":"SQRT((O275*O275)+(O276*O276)+(H273*H273))","v":0.5},{"$f":"SQRT((O275*O275)+(O272*O272)+(H273*H273))","v":0.5},{"$f":"H273*O271*O272*((O271*O271)+(O272*O272)+(2*H273*H273))/(((O271*O271)+(H273*H273))*((O272*O272)+(H273*H273))*O249)","v":0},{"$f":"H273*O271*O276*((O271*O271)+(O276*O276)+(2*H273*H273))/(((O271*O271)+(H273*H273))*((O276*O276)+(H273*H273))*P249)","v":0},{"$f":"H273*O275*O276*((O275*O275)+(O276*O276)+(2*H273*H273))/(((O275*O275)+(H273*H273))*((O276*O276)+(H273*H273))*Q249)","v":0},{"$f":"H273*O275*O272*((O275*O275)+(O272*O272)+(2*H273*H273))/(((O275*O275)+(H273*H273))*((O272*O272)+(H273*H273))*R249)","v":0}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!J15","v":0},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O271*O271)+(O272*O272)+(H274*H274))","v":1.5},{"$f":"SQRT((O271*O271)+(O276*O276)+(H274*H274))","v":1.5},{"$f":"SQRT((O275*O275)+(O276*O276)+(H274*H274))","v":1.5},{"$f":"SQRT((O275*O275)+(O272*O272)+(H274*H274))","v":1.5},{"$f":"H274*O271*O272*((O271*O271)+(O272*O272)+(2*H274*H274))/(((O271*O271)+(H274*H274))*((O272*O272)+(H274*H274))*O250)","v":0},{"$f":"H274*O271*O276*((O271*O271)+(O276*O276)+(2*H274*H274))/(((O271*O271)+(H274*H274))*((O276*O276)+(H274*H274))*P250)","v":0},{"$f":"H274*O275*O276*((O275*O275)+(O276*O276)+(2*H274*H274))/(((O275*O275)+(H274*H274))*((O276*O276)+(H274*H274))*Q250)","v":0},{"$f":"H274*O275*O272*((O275*O275)+(O272*O272)+(2*H274*H274))/(((O275*O275)+(H274*H274))*((O272*O272)+(H274*H274))*R250)","v":0}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O271*O271)+(O272*O272)+(H275*H275))","v":3},{"$f":"SQRT((O271*O271)+(O276*O276)+(H275*H275))","v":3},{"$f":"SQRT((O275*O275)+(O276*O276)+(H275*H275))","v":3},{"$f":"SQRT((O275*O275)+(O272*O272)+(H275*H275))","v":3},{"$f":"H275*O271*O272*((O271*O271)+(O272*O272)+(2*H275*H275))/(((O271*O271)+(H275*H275))*((O272*O272)+(H275*H275))*O251)","v":0},{"$f":"H275*O271*O276*((O271*O271)+(O276*O276)+(2*H275*H275))/(((O271*O271)+(H275*H275))*((O276*O276)+(H275*H275))*P251)","v":0},{"$f":"H275*O275*O276*((O275*O275)+(O276*O276)+(2*H275*H275))/(((O275*O275)+(H275*H275))*((O276*O276)+(H275*H275))*Q251)","v":0},{"$f":"H275*O275*O272*((O275*O275)+(O272*O272)+(2*H275*H275))/(((O275*O275)+(H275*H275))*((O272*O272)+(H275*H275))*R251)","v":0}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O271*O271)+(O272*O272)+(H276*H276))","v":5},{"$f":"SQRT((O271*O271)+(O276*O276)+(H276*H276))","v":5},{"$f":"SQRT((O275*O275)+(O276*O276)+(H276*H276))","v":5},{"$f":"SQRT((O275*O275)+(O272*O272)+(H276*H276))","v":5},{"$f":"H276*O271*O272*((O271*O271)+(O272*O272)+(2*H276*H276))/(((O271*O271)+(H276*H276))*((O272*O272)+(H276*H276))*O252)","v":0},{"$f":"H276*O271*O276*((O271*O271)+(O276*O276)+(2*H276*H276))/(((O271*O271)+(H276*H276))*((O276*O276)+(H276*H276))*P252)","v":0},{"$f":"H276*O275*O276*((O275*O275)+(O276*O276)+(2*H276*H276))/(((O275*O275)+(H276*H276))*((O276*O276)+(H276*H276))*Q252)","v":0},{"$f":"H276*O275*O272*((O275*O275)+(O272*O272)+(2*H276*H276))/(((O275*O275)+(H276*H276))*((O272*O272)+(H276*H276))*R252)","v":0}]
[null,1,{"$f":"+$C$23","v":1},{"$f":"+$D$23","v":20},{"$f":"+$E$23","v":8000},{"$f":"IF(H273=0,\"   \",+H273)","v":0.5},{"$f":"IF(D280=0,\"       \",+D280)","v":40},{"$f":"F280","v":0},{"$f":"H280","v":0},{"$f":"+J280","v":8}]
[null,{"$f":"IF(H274=(H273+C253/2),\"\",2)","v":2},{"$f":"+$C$24","v":1},{"$f":"+$D$24","v":10},{"$f":"+$E$24","v":8000},{"$f":"IF(H274=H273,\"   \",+H274)","v":1.5},{"$f":"IF(D281=D280,\"       \",+D281)","v":55},0,0,{"$f":"+J281","v":11}]
[null,{"$f":"IF(H275=(H274+C254/2),\"\",3)","v":3},{"$f":"+$C$25","v":2},{"$f":"+$D$25","v":10},{"$f":"+$E$25","v":8000},{"$f":"IF(H275=H274,\"   \",+H275)","v":3},{"$f":"IF(D282=D281,\"       \",+D282)","v":70},0,0,{"$f":"+J282","v":14},null,null,null,null,{"$f":"SQRT((O271*O271)+(O272*O272)+(H277*H277))","v":7},{"$f":"SQRT((O271*O271)+(O276*O276)+(H277*H277))","v":7},{"$f":"SQRT((O275*O275)+(O276*O276)+(H277*H277))","v":7},{"$f":"SQRT((O275*O275)+(O272*O272)+(H277*H277))","v":7},{"$f":"H277*O271*O272*((O271*O271)+(O272*O272)+(2*H277*H277))/(((O271*O271)+(H277*H277))*((O272*O272)+(H277*H277))*O255)","v":0},{"$f":"H277*O271*O276*((O271*O271)+(O276*O276)+(2*H277*H277))/(((O271*O271)+(H277*H277))*((O276*O276)+(H277*H277))*P255)","v":0},{"$f":"H277*O275*O276*((O275*O275)+(O276*O276)+(2*H277*H277))/(((O275*O275)+(H277*H277))*((O276*O276)+(H277*H277))*Q255)","v":0},{"$f":"H277*O275*O272*((O275*O275)+(O272*O272)+(2*H277*H277))/(((O275*O275)+(H277*H277))*((O272*O272)+(H277*H277))*R255)","v":0}]
[null,{"$f":"IF(H276=(H275+C255/2),\"\",4)","v":4},{"$f":"+$C$26","v":2},{"$f":"+$D$26","v":10},{"$f":"+$E$26","v":8000},{"$f":"IF(H276=H275,\"   \",+H276)","v":5},{"$f":"IF(D283=D282,\"       \",+D283)","v":90},0,0,{"$f":"IF(D283=D282,\"\",+J283)","v":18},null,null,null,null,{"$f":"SQRT((O271*O271)+(O272*O272)+(H278*H278))","v":8.0050000000000008},{"$f":"SQRT((O271*O271)+(O276*O276)+(H278*H278))","v":8.0050000000000008},{"$f":"SQRT((O275*O275)+(O276*O276)+(H278*H278))","v":8.0050000000000008},{"$f":"SQRT((O275*O275)+(O272*O272)+(H278*H278))","v":8.0050000000000008},{"$f":"H278*O271*O272*((O271*O271)+(O272*O272)+(2*H278*H278))/(((O271*O271)+(H278*H278))*((O272*O272)+(H278*H278))*O256)","v":0},{"$f":"H278*O271*O276*((O271*O271)+(O276*O276)+(2*H278*H278))/(((O271*O271)+(H278*H278))*((O276*O276)+(H278*H278))*P256)","v":0},{"$f":"H278*O275*O276*((O275*O275)+(O276*O276)+(2*H278*H278))/(((O275*O275)+(H278*H278))*((O276*O276)+(H278*H278))*Q256)","v":0},{"$f":"H278*O275*O272*((O275*O275)+(O272*O272)+(2*H278*H278))/(((O275*O275)+(H278*H278))*((O272*O272)+(H278*H278))*R256)","v":0}]
[null,{"$f":"IF(H277=(H276+C256/2),\"\",5)","v":5},{"$f":"+$C$27","v":2},{"$f":"+$D$27","v":10},{"$f":"+$E$27","v":8000},{"$f":"IF(H277=H276,\"   \",+H277)","v":7},{"$f":"IF(D284=D283,\"       \",+D284)","v":110},0,0,{"$f":"IF(D284=D283,\"\",+J284)","v":22},null,null,null,null,{"$f":"ATAN((O271*O272)/(H273*O249))","v":0},{"$f":"ATAN((O271*O276)/(H273*P249))","v":0},{"$f":"ATAN((O275*O276)/(H273*Q249))","v":0},{"$f":"ATAN((O275*O272)/(H273*R249))","v":0}]
[null,{"$f":"IF(H278=(H277+C257/2),\"\",6)","v":6},{"$f":"+$C$28","v":0.01},{"$f":"+$D$28","v":10},{"$f":"+$E$28","v":8000},{"$f":"IF(H278=H277,\"   \",+H278)","v":8.0050000000000008},{"$f":"IF(D285=D284,\"       \",+D285)","v":120.05},0,0,{"$f":"IF(D285=D284,\"\",+J285)","v":24.01},null,null,null,null,{"$f":"ATAN((O271*O272)/(H274*O250))","v":0},{"$f":"ATAN((O271*O276)/(H274*P250))","v":0},{"$f":"ATAN((O275*O276)/(H274*Q250))","v":0},{"$f":"ATAN((O275*O272)/(H274*R250))","v":0}]
[null,null,null,null,null,null,null,"  S W =",0,"m ",null,null,null,null,{"$f":"ATAN((O271*O272)/(H275*O251))","v":0},{"$f":"ATAN((O271*O276)/(H275*P251))","v":0},{"$f":"ATAN((O275*O276)/(H275*Q251))","v":0},{"$f":"ATAN((O275*O272)/(H275*R251))","v":0}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O271*O272)/(H276*O252))","v":0},{"$f":"ATAN((O271*O276)/(H276*P252))","v":0},{"$f":"ATAN((O275*O276)/(H276*Q252))","v":0},{"$f":"ATAN((O275*O272)/(H276*R252))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O271*O272)/(H277*O255))","v":0},{"$f":"ATAN((O271*O276)/(H277*P255))","v":0},{"$f":"ATAN((O275*O276)/(H277*Q255))","v":0},{"$f":"ATAN((O275*O272)/(H277*R255))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O271*O272)/(H278*O256))","v":0},{"$f":"ATAN((O271*O276)/(H278*P256))","v":0},{"$f":"ATAN((O275*O276)/(H278*Q256))","v":0},{"$f":"ATAN((O275*O272)/(H278*R256))","v":0}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E248","v":0},"m",null,null,null,null,{"$f":"E248/2","v":0}]
[null,null,"     širina temelja  B=",{"$f":"E249","v":0},"m",null,null,null,null,{"$f":"E249/2","v":0}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G248","v":0},"kPa",null,null,null,null,{"$f":"J245*J265","v":0}]
[null,null,"      dubina temeljenja Df=",{"$f":"E250","v":0},"m",null,null,null,null,{"$f":"J246*J266","v":0}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J267+J265","v":0}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J268+J266","v":0}]
[1,null,"      H1=",{"$f":"IF(C253=0,\"      \",C253)","v":1},"m        Mk1=",{"$f":"IF(E253=0,\"       \",+E253)","v":8000},"KN/m2     z1=",{"$f":"C253/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C253+C254/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C253+C254+C255/2","v":3},"m",null,null,null,null,null,{"$f":"J267-J265","v":0}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C253+C254+C255+C256/2","v":5},"m",null,null,null,null,null,{"$f":"J268-J266","v":0}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C253+C254+C255+C256+C257/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C253+C254+C255+C256+C257+C258/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O257)-(P257)+(Q257)-(R257)+(S249)-(T249)+(U249)-(V249))/(2*3.14159)","v":0},{"$f":"+'T1'!D280","v":40},"kPa     Dp1=",{"$f":"(G248)*C280","v":0},"kPa        w1=",{"$f":"IF(E253=0,\"       \",+F280*C253/E253)","v":0},"m",{"$f":"0.2*D280","v":8}]
[null,"    I42=",{"$f":"((O258)-(P258)+(Q258)-(R258)+(S250)-(T250)+(U250)-(V250))/(2*3.14159)","v":0},{"$f":"+'T1'!D281","v":55},"kPa     Dp2=",{"$f":"IF(H274=H273,\"     \",(G248)*C281)","v":0},"kPa       w2=",0,"m",11]
[null,"    I43=",{"$f":"((O259)-(P259)+(Q259)-(R259)+(S251)-(T251)+(U251)-(V251))/(2*3.14159)","v":0},{"$f":"+'T1'!D282","v":70},"kPa     Dp3=",{"$f":"IF(H275=H274,\"     \",(G248)*C282)","v":0},"kPa       w3=",0,"m",14]
[null,"    I44=",{"$f":"((O260)-(P260)+(Q260)-(R260)+(S252)-(T252)+(U252)-(V252))/(2*3.14159)","v":0},{"$f":"+'T1'!D283","v":90},"kPa     Dp4=",{"$f":"IF(H276=H275,\"     \",(G248)*C283)","v":0},"kPa       w4=",0,"m",18]
[null,"    I45=",{"$f":"((O261)-(P261)+(Q261)-(R261)+(S255)-(T255)+(U255)-(V255))/(2*3.14159)","v":0},{"$f":"+'T1'!D284","v":110},"kPa     Dp5=",{"$f":"IF(H277=H276,\"     \",(G248)*C284)","v":0},"kPa       w5=",0,"m",22]
[null,"    I46=",{"$f":"((P262)-(Q262)+(R262)-(S262)+(S256)-(T256)+(U256)-(V256))/(2*3.14159)","v":0},{"$f":"+'T1'!D285","v":120.05},"kPa     Dp6=",{"$f":"IF(H278=H277,\"       \",(G248)*C285)","v":0},"kPa       w6=",0,"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H280:H285)","v":0},"m"]
[]
[]
[]
[]
[null,null,"SLIJEGANJE TOČKE TS2 OD TEMELJA T7",null,null,null,null,null,"       x=L/2*",{"$f":"I11","v":0},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"I12","v":0}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!K13","v":0},"m         Dpa'=",{"$f":"+Slijeganje!K17","v":0},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!K14","v":0},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O317*O317)+(O318*O318)+(H319*H319))","v":0.5},{"$f":"SQRT((O317*O317)+(O322*O322)+(H319*H319))","v":0.5},{"$f":"SQRT((O321*O321)+(O322*O322)+(H319*H319))","v":0.5},{"$f":"SQRT((O321*O321)+(O318*O318)+(H319*H319))","v":0.5},{"$f":"H319*O317*O318*((O317*O317)+(O318*O318)+(2*H319*H319))/(((O317*O317)+(H319*H319))*((O318*O318)+(H319*H319))*O295)","v":0},{"$f":"H319*O317*O322*((O317*O317)+(O322*O322)+(2*H319*H319))/(((O317*O317)+(H319*H319))*((O322*O322)+(H319*H319))*P295)","v":0},{"$f":"H319*O321*O322*((O321*O321)+(O322*O322)+(2*H319*H319))/(((O321*O321)+(H319*H319))*((O322*O322)+(H319*H319))*Q295)","v":0},{"$f":"H319*O321*O318*((O321*O321)+(O318*O318)+(2*H319*H319))/(((O321*O321)+(H319*H319))*((O318*O318)+(H319*H319))*R295)","v":0}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!K15","v":0},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O317*O317)+(O318*O318)+(H320*H320))","v":1.5},{"$f":"SQRT((O317*O317)+(O322*O322)+(H320*H320))","v":1.5},{"$f":"SQRT((O321*O321)+(O322*O322)+(H320*H320))","v":1.5},{"$f":"SQRT((O321*O321)+(O318*O318)+(H320*H320))","v":1.5},{"$f":"H320*O317*O318*((O317*O317)+(O318*O318)+(2*H320*H320))/(((O317*O317)+(H320*H320))*((O318*O318)+(H320*H320))*O296)","v":0},{"$f":"H320*O317*O322*((O317*O317)+(O322*O322)+(2*H320*H320))/(((O317*O317)+(H320*H320))*((O322*O322)+(H320*H320))*P296)","v":0},{"$f":"H320*O321*O322*((O321*O321)+(O322*O322)+(2*H320*H320))/(((O321*O321)+(H320*H320))*((O322*O322)+(H320*H320))*Q296)","v":0},{"$f":"H320*O321*O318*((O321*O321)+(O318*O318)+(2*H320*H320))/(((O321*O321)+(H320*H320))*((O318*O318)+(H320*H320))*R296)","v":0}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O317*O317)+(O318*O318)+(H321*H321))","v":3},{"$f":"SQRT((O317*O317)+(O322*O322)+(H321*H321))","v":3},{"$f":"SQRT((O321*O321)+(O322*O322)+(H321*H321))","v":3},{"$f":"SQRT((O321*O321)+(O318*O318)+(H321*H321))","v":3},{"$f":"H321*O317*O318*((O317*O317)+(O318*O318)+(2*H321*H321))/(((O317*O317)+(H321*H321))*((O318*O318)+(H321*H321))*O297)","v":0},{"$f":"H321*O317*O322*((O317*O317)+(O322*O322)+(2*H321*H321))/(((O317*O317)+(H321*H321))*((O322*O322)+(H321*H321))*P297)","v":0},{"$f":"H321*O321*O322*((O321*O321)+(O322*O322)+(2*H321*H321))/(((O321*O321)+(H321*H321))*((O322*O322)+(H321*H321))*Q297)","v":0},{"$f":"H321*O321*O318*((O321*O321)+(O318*O318)+(2*H321*H321))/(((O321*O321)+(H321*H321))*((O318*O318)+(H321*H321))*R297)","v":0}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O317*O317)+(O318*O318)+(H322*H322))","v":5},{"$f":"SQRT((O317*O317)+(O322*O322)+(H322*H322))","v":5},{"$f":"SQRT((O321*O321)+(O322*O322)+(H322*H322))","v":5},{"$f":"SQRT((O321*O321)+(O318*O318)+(H322*H322))","v":5},{"$f":"H322*O317*O318*((O317*O317)+(O318*O318)+(2*H322*H322))/(((O317*O317)+(H322*H322))*((O318*O318)+(H322*H322))*O298)","v":0},{"$f":"H322*O317*O322*((O317*O317)+(O322*O322)+(2*H322*H322))/(((O317*O317)+(H322*H322))*((O322*O322)+(H322*H322))*P298)","v":0},{"$f":"H322*O321*O322*((O321*O321)+(O322*O322)+(2*H322*H322))/(((O321*O321)+(H322*H322))*((O322*O322)+(H322*H322))*Q298)","v":0},{"$f":"H322*O321*O318*((O321*O321)+(O318*O318)+(2*H322*H322))/(((O321*O321)+(H322*H322))*((O318*O318)+(H322*H322))*R298)","v":0}]
[null,1,{"$f":"+$C$23","v":1},{"$f":"+$D$23","v":20},{"$f":"+$E$23","v":8000},{"$f":"IF(H319=0,\"   \",+H319)","v":0.5},{"$f":"IF(D326=0,\"       \",+D326)","v":40},{"$f":"F326","v":0},{"$f":"H326","v":0},{"$f":"+J326","v":8}]
[null,{"$f":"IF(H320=(H319+C299/2),\"\",2)","v":2},{"$f":"+$C$24","v":1},{"$f":"+$D$24","v":10},{"$f":"+$E$24","v":8000},{"$f":"IF(H320=H319,\"   \",+H320)","v":1.5},{"$f":"IF(D327=D326,\"       \",+D327)","v":55},0,0,{"$f":"+J327","v":11}]
[null,{"$f":"IF(H321=(H320+C300/2),\"\",3)","v":3},{"$f":"+$C$25","v":2},{"$f":"+$D$25","v":10},{"$f":"+$E$25","v":8000},{"$f":"IF(H321=H320,\"   \",+H321)","v":3},{"$f":"IF(D328=D327,\"       \",+D328)","v":70},0,0,{"$f":"+J328","v":14},null,null,null,null,{"$f":"SQRT((O317*O317)+(O318*O318)+(H323*H323))","v":7},{"$f":"SQRT((O317*O317)+(O322*O322)+(H323*H323))","v":7},{"$f":"SQRT((O321*O321)+(O322*O322)+(H323*H323))","v":7},{"$f":"SQRT((O321*O321)+(O318*O318)+(H323*H323))","v":7},{"$f":"H323*O317*O318*((O317*O317)+(O318*O318)+(2*H323*H323))/(((O317*O317)+(H323*H323))*((O318*O318)+(H323*H323))*O301)","v":0},{"$f":"H323*O317*O322*((O317*O317)+(O322*O322)+(2*H323*H323))/(((O317*O317)+(H323*H323))*((O322*O322)+(H323*H323))*P301)","v":0},{"$f":"H323*O321*O322*((O321*O321)+(O322*O322)+(2*H323*H323))/(((O321*O321)+(H323*H323))*((O322*O322)+(H323*H323))*Q301)","v":0},{"$f":"H323*O321*O318*((O321*O321)+(O318*O318)+(2*H323*H323))/(((O321*O321)+(H323*H323))*((O318*O318)+(H323*H323))*R301)","v":0}]
[null,{"$f":"IF(H322=(H321+C301/2),\"\",4)","v":4},{"$f":"+$C$26","v":2},{"$f":"+$D$26","v":10},{"$f":"+$E$26","v":8000},{"$f":"IF(H322=H321,\"   \",+H322)","v":5},{"$f":"IF(D329=D328,\"       \",+D329)","v":90},0,0,{"$f":"IF(D329=D328,\"\",+J329)","v":18},null,null,null,null,{"$f":"SQRT((O317*O317)+(O318*O318)+(H324*H324))","v":8.0050000000000008},{"$f":"SQRT((O317*O317)+(O322*O322)+(H324*H324))","v":8.0050000000000008},{"$f":"SQRT((O321*O321)+(O322*O322)+(H324*H324))","v":8.0050000000000008},{"$f":"SQRT((O321*O321)+(O318*O318)+(H324*H324))","v":8.0050000000000008},{"$f":"H324*O317*O318*((O317*O317)+(O318*O318)+(2*H324*H324))/(((O317*O317)+(H324*H324))*((O318*O318)+(H324*H324))*O302)","v":0},{"$f":"H324*O317*O322*((O317*O317)+(O322*O322)+(2*H324*H324))/(((O317*O317)+(H324*H324))*((O322*O322)+(H324*H324))*P302)","v":0},{"$f":"H324*O321*O322*((O321*O321)+(O322*O322)+(2*H324*H324))/(((O321*O321)+(H324*H324))*((O322*O322)+(H324*H324))*Q302)","v":0},{"$f":"H324*O321*O318*((O321*O321)+(O318*O318)+(2*H324*H324))/(((O321*O321)+(H324*H324))*((O318*O318)+(H324*H324))*R302)","v":0}]
[null,{"$f":"IF(H323=(H322+C302/2),\"\",5)","v":5},{"$f":"+$C$27","v":2},{"$f":"+$D$27","v":10},{"$f":"+$E$27","v":8000},{"$f":"IF(H323=H322,\"   \",+H323)","v":7},{"$f":"IF(D330=D329,\"       \",+D330)","v":110},0,0,{"$f":"IF(D330=D329,\"\",+J330)","v":22},null,null,null,null,{"$f":"ATAN((O317*O318)/(H319*O295))","v":0},{"$f":"ATAN((O317*O322)/(H319*P295))","v":0},{"$f":"ATAN((O321*O322)/(H319*Q295))","v":0},{"$f":"ATAN((O321*O318)/(H319*R295))","v":0}]
[null,{"$f":"IF(H324=(H323+C303/2),\"\",6)","v":6},{"$f":"+$C$28","v":0.01},{"$f":"+$D$28","v":10},{"$f":"+$E$28","v":8000},{"$f":"IF(H324=H323,\"   \",+H324)","v":8.0050000000000008},{"$f":"IF(D331=D330,\"       \",+D331)","v":120.05},0,0,{"$f":"IF(D331=D330,\"\",+J331)","v":24.01},null,null,null,null,{"$f":"ATAN((O317*O318)/(H320*O296))","v":0},{"$f":"ATAN((O317*O322)/(H320*P296))","v":0},{"$f":"ATAN((O321*O322)/(H320*Q296))","v":0},{"$f":"ATAN((O321*O318)/(H320*R296))","v":0}]
[null,null,null,null,null,null,null,"  S W =",0,"m ",null,null,null,null,{"$f":"ATAN((O317*O318)/(H321*O297))","v":0},{"$f":"ATAN((O317*O322)/(H321*P297))","v":0},{"$f":"ATAN((O321*O322)/(H321*Q297))","v":0},{"$f":"ATAN((O321*O318)/(H321*R297))","v":0}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O317*O318)/(H322*O298))","v":0},{"$f":"ATAN((O317*O322)/(H322*P298))","v":0},{"$f":"ATAN((O321*O322)/(H322*Q298))","v":0},{"$f":"ATAN((O321*O318)/(H322*R298))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O317*O318)/(H323*O301))","v":0},{"$f":"ATAN((O317*O322)/(H323*P301))","v":0},{"$f":"ATAN((O321*O322)/(H323*Q301))","v":0},{"$f":"ATAN((O321*O318)/(H323*R301))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O317*O318)/(H324*O302))","v":0},{"$f":"ATAN((O317*O322)/(H324*P302))","v":0},{"$f":"ATAN((O321*O322)/(H324*Q302))","v":0},{"$f":"ATAN((O321*O318)/(H324*R302))","v":0}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E294","v":0},"m",null,null,null,null,{"$f":"E294/2","v":0}]
[null,null,"     širina temelja  B=",{"$f":"E295","v":0},"m",null,null,null,null,{"$f":"E295/2","v":0}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G294","v":0},"kPa",null,null,null,null,{"$f":"J291*J311","v":0}]
[null,null,"      dubina temeljenja Df=",{"$f":"E296","v":0},"m",null,null,null,null,{"$f":"J292*J312","v":0}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J313+J311","v":0}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J314+J312","v":0}]
[1,null,"      H1=",{"$f":"IF(C299=0,\"      \",C299)","v":1},"m        Mk1=",{"$f":"IF(E299=0,\"       \",+E299)","v":8000},"KN/m2     z1=",{"$f":"C299/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C299+C300/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C299+C300+C301/2","v":3},"m",null,null,null,null,null,{"$f":"J313-J311","v":0}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C299+C300+C301+C302/2","v":5},"m",null,null,null,null,null,{"$f":"J314-J312","v":0}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C299+C300+C301+C302+C303/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C299+C300+C301+C302+C303+C304/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O303)-(P303)+(Q303)-(R303)+(S295)-(T295)+(U295)-(V295))/(2*3.14159)","v":0},{"$f":"+'T1'!D326","v":40},"kPa     Dp1=",{"$f":"(G294)*C326","v":0},"kPa        w1=",{"$f":"IF(E299=0,\"       \",+F326*C299/E299)","v":0},"m",{"$f":"0.2*D326","v":8}]
[null,"    I42=",{"$f":"((O304)-(P304)+(Q304)-(R304)+(S296)-(T296)+(U296)-(V296))/(2*3.14159)","v":0},{"$f":"+'T1'!D327","v":55},"kPa     Dp2=",{"$f":"IF(H320=H319,\"     \",(G294)*C327)","v":0},"kPa       w2=",0,"m",11]
[null,"    I43=",{"$f":"((O305)-(P305)+(Q305)-(R305)+(S297)-(T297)+(U297)-(V297))/(2*3.14159)","v":0},{"$f":"+'T1'!D328","v":70},"kPa     Dp3=",{"$f":"IF(H321=H320,\"     \",(G294)*C328)","v":0},"kPa       w3=",0,"m",14]
[null,"    I44=",{"$f":"((O306)-(P306)+(Q306)-(R306)+(S298)-(T298)+(U298)-(V298))/(2*3.14159)","v":0},{"$f":"+'T1'!D329","v":90},"kPa     Dp4=",{"$f":"IF(H322=H321,\"     \",(G294)*C329)","v":0},"kPa       w4=",0,"m",18]
[null,"    I45=",{"$f":"((O307)-(P307)+(Q307)-(R307)+(S301)-(T301)+(U301)-(V301))/(2*3.14159)","v":0},{"$f":"+'T1'!D330","v":110},"kPa     Dp5=",{"$f":"IF(H323=H322,\"     \",(G294)*C330)","v":0},"kPa       w5=",0,"m",22]
[null,"    I46=",{"$f":"((P308)-(Q308)+(R308)-(S308)+(S302)-(T302)+(U302)-(V302))/(2*3.14159)","v":0},{"$f":"+'T1'!D331","v":120.05},"kPa     Dp6=",{"$f":"IF(H324=H323,\"       \",(G294)*C331)","v":0},"kPa       w6=",0,"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H326:H331)","v":0},"m"]
[]
[]
[]
[]
[null,null,"SLIJEGANJE TOČKE TS2 OD TEMELJA T8",null,null,null,null,null,"       x=L/2*",{"$f":"J11","v":0},null,null,null,null," "]
[null,null,null,null,null,null,null,null,"       y=B/2*",{"$f":"J12","v":0}]
[]
[null,null,null,"      dužina temelja  L=",{"$f":"+Slijeganje!L13","v":0},"m         Dpa'=",{"$f":"+Slijeganje!L17","v":0},"kPa"]
[null,null,null,"     širina temelja  B=",{"$f":"+Slijeganje!L14","v":0},"m       ",null,null,null,null,null,null,null,null,{"$f":"SQRT((O363*O363)+(O364*O364)+(H365*H365))","v":0.5},{"$f":"SQRT((O363*O363)+(O368*O368)+(H365*H365))","v":0.5},{"$f":"SQRT((O367*O367)+(O368*O368)+(H365*H365))","v":0.5},{"$f":"SQRT((O367*O367)+(O364*O364)+(H365*H365))","v":0.5},{"$f":"H365*O363*O364*((O363*O363)+(O364*O364)+(2*H365*H365))/(((O363*O363)+(H365*H365))*((O364*O364)+(H365*H365))*O341)","v":0},{"$f":"H365*O363*O368*((O363*O363)+(O368*O368)+(2*H365*H365))/(((O363*O363)+(H365*H365))*((O368*O368)+(H365*H365))*P341)","v":0},{"$f":"H365*O367*O368*((O367*O367)+(O368*O368)+(2*H365*H365))/(((O367*O367)+(H365*H365))*((O368*O368)+(H365*H365))*Q341)","v":0},{"$f":"H365*O367*O364*((O367*O367)+(O364*O364)+(2*H365*H365))/(((O367*O367)+(H365*H365))*((O364*O364)+(H365*H365))*R341)","v":0}]
[null,null,null,"      dubina temeljenja Df=",{"$f":"+Slijeganje!L15","v":0},"m     ispod površine terena",null,null,null,null,null,null,null,null,{"$f":"SQRT((O363*O363)+(O364*O364)+(H366*H366))","v":1.5},{"$f":"SQRT((O363*O363)+(O368*O368)+(H366*H366))","v":1.5},{"$f":"SQRT((O367*O367)+(O368*O368)+(H366*H366))","v":1.5},{"$f":"SQRT((O367*O367)+(O364*O364)+(H366*H366))","v":1.5},{"$f":"H366*O363*O364*((O363*O363)+(O364*O364)+(2*H366*H366))/(((O363*O363)+(H366*H366))*((O364*O364)+(H366*H366))*O342)","v":0},{"$f":"H366*O363*O368*((O363*O363)+(O368*O368)+(2*H366*H366))/(((O363*O363)+(H366*H366))*((O368*O368)+(H366*H366))*P342)","v":0},{"$f":"H366*O367*O368*((O367*O367)+(O368*O368)+(2*H366*H366))/(((O367*O367)+(H366*H366))*((O368*O368)+(H366*H366))*Q342)","v":0},{"$f":"H366*O367*O364*((O367*O367)+(O364*O364)+(2*H366*H366))/(((O367*O367)+(H366*H366))*((O364*O364)+(H366*H366))*R342)","v":0}]
[null," ",null,null,null,null,null,null," ",null,null,null,null,null,{"$f":"SQRT((O363*O363)+(O364*O364)+(H367*H367))","v":3},{"$f":"SQRT((O363*O363)+(O368*O368)+(H367*H367))","v":3},{"$f":"SQRT((O367*O367)+(O368*O368)+(H367*H367))","v":3},{"$f":"SQRT((O367*O367)+(O364*O364)+(H367*H367))","v":3},{"$f":"H367*O363*O364*((O363*O363)+(O364*O364)+(2*H367*H367))/(((O363*O363)+(H367*H367))*((O364*O364)+(H367*H367))*O343)","v":0},{"$f":"H367*O363*O368*((O363*O363)+(O368*O368)+(2*H367*H367))/(((O363*O363)+(H367*H367))*((O368*O368)+(H367*H367))*P343)","v":0},{"$f":"H367*O367*O368*((O367*O367)+(O368*O368)+(2*H367*H367))/(((O367*O367)+(H367*H367))*((O368*O368)+(H367*H367))*Q343)","v":0},{"$f":"H367*O367*O364*((O367*O367)+(O364*O364)+(2*H367*H367))/(((O367*O367)+(H367*H367))*((O364*O364)+(H367*H367))*R343)","v":0}]
[null,"sloj"," Hi (m)","g (kN/m3)","Mki (kN/m2)","zi (m)","pg (kPa)"," Dp (kPa)","wi (m)","0,2*pg (kPa)",null,null,null,null,{"$f":"SQRT((O363*O363)+(O364*O364)+(H368*H368))","v":5},{"$f":"SQRT((O363*O363)+(O368*O368)+(H368*H368))","v":5},{"$f":"SQRT((O367*O367)+(O368*O368)+(H368*H368))","v":5},{"$f":"SQRT((O367*O367)+(O364*O364)+(H368*H368))","v":5},{"$f":"H368*O363*O364*((O363*O363)+(O364*O364)+(2*H368*H368))/(((O363*O363)+(H368*H368))*((O364*O364)+(H368*H368))*O344)","v":0},{"$f":"H368*O363*O368*((O363*O363)+(O368*O368)+(2*H368*H368))/(((O363*O363)+(H368*H368))*((O368*O368)+(H368*H368))*P344)","v":0},{"$f":"H368*O367*O368*((O367*O367)+(O368*O368)+(2*H368*H368))/(((O367*O367)+(H368*H368))*((O368*O368)+(H368*H368))*Q344)","v":0},{"$f":"H368*O367*O364*((O367*O367)+(O364*O364)+(2*H368*H368))/(((O367*O367)+(H368*H368))*((O364*O364)+(H368*H368))*R344)","v":0}]
[null,1,{"$f":"+$C$23","v":1},{"$f":"+$D$23","v":20},{"$f":"+$E$23","v":8000},{"$f":"IF(H365=0,\"   \",+H365)","v":0.5},{"$f":"IF(D372=0,\"       \",+D372)","v":40},{"$f":"F372","v":0},{"$f":"H372","v":0},{"$f":"+J372","v":8}]
[null,{"$f":"IF(H366=(H365+C345/2),\"\",2)","v":2},{"$f":"+$C$24","v":1},{"$f":"+$D$24","v":10},{"$f":"+$E$24","v":8000},{"$f":"IF(H366=H365,\"   \",+H366)","v":1.5},{"$f":"IF(D373=D372,\"       \",+D373)","v":55},0,0,{"$f":"+J373","v":11}]
[null,{"$f":"IF(H367=(H366+C346/2),\"\",3)","v":3},{"$f":"+$C$25","v":2},{"$f":"+$D$25","v":10},{"$f":"+$E$25","v":8000},{"$f":"IF(H367=H366,\"   \",+H367)","v":3},{"$f":"IF(D374=D373,\"       \",+D374)","v":70},0,0,{"$f":"+J374","v":14},null,null,null,null,{"$f":"SQRT((O363*O363)+(O364*O364)+(H369*H369))","v":7},{"$f":"SQRT((O363*O363)+(O368*O368)+(H369*H369))","v":7},{"$f":"SQRT((O367*O367)+(O368*O368)+(H369*H369))","v":7},{"$f":"SQRT((O367*O367)+(O364*O364)+(H369*H369))","v":7},{"$f":"H369*O363*O364*((O363*O363)+(O364*O364)+(2*H369*H369))/(((O363*O363)+(H369*H369))*((O364*O364)+(H369*H369))*O347)","v":0},{"$f":"H369*O363*O368*((O363*O363)+(O368*O368)+(2*H369*H369))/(((O363*O363)+(H369*H369))*((O368*O368)+(H369*H369))*P347)","v":0},{"$f":"H369*O367*O368*((O367*O367)+(O368*O368)+(2*H369*H369))/(((O367*O367)+(H369*H369))*((O368*O368)+(H369*H369))*Q347)","v":0},{"$f":"H369*O367*O364*((O367*O367)+(O364*O364)+(2*H369*H369))/(((O367*O367)+(H369*H369))*((O364*O364)+(H369*H369))*R347)","v":0}]
[null,{"$f":"IF(H368=(H367+C347/2),\"\",4)","v":4},{"$f":"+$C$26","v":2},{"$f":"+$D$26","v":10},{"$f":"+$E$26","v":8000},{"$f":"IF(H368=H367,\"   \",+H368)","v":5},{"$f":"IF(D375=D374,\"       \",+D375)","v":90},0,0,{"$f":"IF(D375=D374,\"\",+J375)","v":18},null,null,null,null,{"$f":"SQRT((O363*O363)+(O364*O364)+(H370*H370))","v":8.0050000000000008},{"$f":"SQRT((O363*O363)+(O368*O368)+(H370*H370))","v":8.0050000000000008},{"$f":"SQRT((O367*O367)+(O368*O368)+(H370*H370))","v":8.0050000000000008},{"$f":"SQRT((O367*O367)+(O364*O364)+(H370*H370))","v":8.0050000000000008},{"$f":"H370*O363*O364*((O363*O363)+(O364*O364)+(2*H370*H370))/(((O363*O363)+(H370*H370))*((O364*O364)+(H370*H370))*O348)","v":0},{"$f":"H370*O363*O368*((O363*O363)+(O368*O368)+(2*H370*H370))/(((O363*O363)+(H370*H370))*((O368*O368)+(H370*H370))*P348)","v":0},{"$f":"H370*O367*O368*((O367*O367)+(O368*O368)+(2*H370*H370))/(((O367*O367)+(H370*H370))*((O368*O368)+(H370*H370))*Q348)","v":0},{"$f":"H370*O367*O364*((O367*O367)+(O364*O364)+(2*H370*H370))/(((O367*O367)+(H370*H370))*((O364*O364)+(H370*H370))*R348)","v":0}]
[null,{"$f":"IF(H369=(H368+C348/2),\"\",5)","v":5},{"$f":"+$C$27","v":2},{"$f":"+$D$27","v":10},{"$f":"+$E$27","v":8000},{"$f":"IF(H369=H368,\"   \",+H369)","v":7},{"$f":"IF(D376=D375,\"       \",+D376)","v":110},0,0,{"$f":"IF(D376=D375,\"\",+J376)","v":22},null,null,null,null,{"$f":"ATAN((O363*O364)/(H365*O341))","v":0},{"$f":"ATAN((O363*O368)/(H365*P341))","v":0},{"$f":"ATAN((O367*O368)/(H365*Q341))","v":0},{"$f":"ATAN((O367*O364)/(H365*R341))","v":0}]
[null,{"$f":"IF(H370=(H369+C349/2),\"\",6)","v":6},{"$f":"+$C$28","v":0.01},{"$f":"+$D$28","v":10},{"$f":"+$E$28","v":8000},{"$f":"IF(H370=H369,\"   \",+H370)","v":8.0050000000000008},{"$f":"IF(D377=D376,\"       \",+D377)","v":120.05},0,0,{"$f":"IF(D377=D376,\"\",+J377)","v":24.01},null,null,null,null,{"$f":"ATAN((O363*O364)/(H366*O342))","v":0},{"$f":"ATAN((O363*O368)/(H366*P342))","v":0},{"$f":"ATAN((O367*O368)/(H366*Q342))","v":0},{"$f":"ATAN((O367*O364)/(H366*R342))","v":0}]
[null,null,null,null,null,null,null,"  S W =",0,"m ",null,null,null,null,{"$f":"ATAN((O363*O364)/(H367*O343))","v":0},{"$f":"ATAN((O363*O368)/(H367*P343))","v":0},{"$f":"ATAN((O367*O368)/(H367*Q343))","v":0},{"$f":"ATAN((O367*O364)/(H367*R343))","v":0}]
[null,null,null,null,null,null,null,null,null,"N. Sapunar",null,null,null,null,{"$f":"ATAN((O363*O364)/(H368*O344))","v":0},{"$f":"ATAN((O363*O368)/(H368*P344))","v":0},{"$f":"ATAN((O367*O368)/(H368*Q344))","v":0},{"$f":"ATAN((O367*O364)/(H368*R344))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O363*O364)/(H369*O347))","v":0},{"$f":"ATAN((O363*O368)/(H369*P347))","v":0},{"$f":"ATAN((O367*O368)/(H369*Q347))","v":0},{"$f":"ATAN((O367*O364)/(H369*R347))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ATAN((O363*O364)/(H370*O348))","v":0},{"$f":"ATAN((O363*O368)/(H370*P348))","v":0},{"$f":"ATAN((O367*O368)/(H370*Q348))","v":0},{"$f":"ATAN((O367*O364)/(H370*R348))","v":0}]
[]
[null,null,"PODACI O TEMELJU: "]
[null,null,"      dužina temelja  L=",{"$f":"E340","v":0},"m",null,null,null,null,{"$f":"E340/2","v":0}]
[null,null,"     širina temelja  B=",{"$f":"E341","v":0},"m",null,null,null,null,{"$f":"E341/2","v":0}]
[null,null," spec. opter. temeljem pa'=",{"$f":"G340","v":0},"kPa",null,null,null,null,{"$f":"J337*J357","v":0}]
[null,null,"      dubina temeljenja Df=",{"$f":"E342","v":0},"m",null,null,null,null,{"$f":"J338*J358","v":0}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"J359+J357","v":0}]
["sloj",null,null,null,"PODACI O TLU: ",null,null,null,null,null,null,null,null,null,{"$f":"J360+J358","v":0}]
[1,null,"      H1=",{"$f":"IF(C345=0,\"      \",C345)","v":1},"m        Mk1=",{"$f":"IF(E345=0,\"       \",+E345)","v":8000},"KN/m2     z1=",{"$f":"C345/2","v":0.5},"m"]
[2,null,"      H2=",1,"m        Mk2=",8000,"KN/m2     z2=",{"$f":"C345+C346/2","v":1.5},"m"]
[3,null,"      H3=",2,"m        Mk3=",8000,"KN/m2     z3=",{"$f":"C345+C346+C347/2","v":3},"m",null,null,null,null,null,{"$f":"J359-J357","v":0}]
[4,null,"      H4=",2,"m        Mk4=",8000,"KN/m2     z4=",{"$f":"C345+C346+C347+C348/2","v":5},"m",null,null,null,null,null,{"$f":"J360-J358","v":0}]
[5,null,"      H5=",2,"m        Mk5=",8000,"KN/m2     z5=",{"$f":"C345+C346+C347+C348+C349/2","v":7},"m"]
[6,null,"      H6=",0.01,"m        Mk6=",8000,"KN/m2     z6=",{"$f":"C345+C346+C347+C348+C349+C350/2","v":8.0050000000000008},"m"]
[null,null,null,null,null," "]
[null,"    I41=",{"$f":"((O349)-(P349)+(Q349)-(R349)+(S341)-(T341)+(U341)-(V341))/(2*3.14159)","v":0},{"$f":"+'T1'!D372","v":40},"kPa     Dp1=",{"$f":"(G340)*C372","v":0},"kPa        w1=",{"$f":"IF(E345=0,\"       \",+F372*C345/E345)","v":0},"m",{"$f":"0.2*D372","v":8}]
[null,"    I42=",{"$f":"((O350)-(P350)+(Q350)-(R350)+(S342)-(T342)+(U342)-(V342))/(2*3.14159)","v":0},{"$f":"+'T1'!D373","v":55},"kPa     Dp2=",{"$f":"IF(H366=H365,\"     \",(G340)*C373)","v":0},"kPa       w2=",0,"m",11]
[null,"    I43=",{"$f":"((O351)-(P351)+(Q351)-(R351)+(S343)-(T343)+(U343)-(V343))/(2*3.14159)","v":0},{"$f":"+'T1'!D374","v":70},"kPa     Dp3=",{"$f":"IF(H367=H366,\"     \",(G340)*C374)","v":0},"kPa       w3=",0,"m",14]
[null,"    I44=",{"$f":"((O352)-(P352)+(Q352)-(R352)+(S344)-(T344)+(U344)-(V344))/(2*3.14159)","v":0},{"$f":"+'T1'!D375","v":90},"kPa     Dp4=",{"$f":"IF(H368=H367,\"     \",(G340)*C375)","v":0},"kPa       w4=",0,"m",18]
[null,"    I45=",{"$f":"((O353)-(P353)+(Q353)-(R353)+(S347)-(T347)+(U347)-(V347))/(2*3.14159)","v":0},{"$f":"+'T1'!D376","v":110},"kPa     Dp5=",{"$f":"IF(H369=H368,\"     \",(G340)*C376)","v":0},"kPa       w5=",0,"m",22]
[null,"    I46=",{"$f":"((P354)-(Q354)+(R354)-(S354)+(S348)-(T348)+(U348)-(V348))/(2*3.14159)","v":0},{"$f":"+'T1'!D377","v":120.05},"kPa     Dp6=",{"$f":"IF(H370=H369,\"       \",(G340)*C377)","v":0},"kPa       w6=",0,"m",24.01]
[null,null,null,null,null,null," S W=",{"$f":"SUM(H372:H377)","v":0},"m"]

{"sheet":"Dopušteno Vs+","index":35,"n_rows":87,"n_cols":25,"rows_kept":87,"cut":false,"hidden":true,"merged":[[23,14,24,14],[26,13,27,13],[27,1,27,2],[29,11,29,12],[5,12,6,12],[5,13,6,13],[10,5,10,6],[20,11,20,12],[21,12,22,12],[23,12,24,12]]}
[]
["PRORAČUN AKO VERTIKALNE SILE DJELUJU POZITIVNO NA NOSIVOST",null,null,null,null,null,null,null,null,null,null,null,"Shema opterećenja"]
[null,null,null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null," y"]
[null,null,null,"     j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18},"°            Hx =",0,"kN                 j'=",{"$f":"ATAN(TAN(E5*3.14159/180)/E14)*180/3.14159","v":14.5707680719339},"°        ex=",null,3,"L  ",null,1,{"$f":"IF(G9=0,E9,+E9-ABS(2*P19))","v":{"$error":"#VALUE!"}}]
[null,null,"          ","       c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"kPa       Hy =",{"$f":"+'Analiza i dimenzioniranje'!B167*E9","v":{"$error":"#VALUE!"}},"kN                c' =",{"$f":"E6/E15","v":20},"kPa    ey=",null,null,"      Hy ","Hx","        x  ",{"$f":"IF(G9=0,E8,+E8-ABS(2*P20))","v":{"$error":"#VALUE!"}}]
[null,null,"q=g*Df","g =",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"kN/m3     Mx =",{"$f":"V28*E9","v":{"$error":"#VALUE!"}},"kNm",null,"           L'=",null,"  B",null,null,"                     ",{"$f":"I5*3.14159/180","v":0.2543076625950379}]
[null,null,null,"   kraća stranica u smjer osi (y)    B =",{"$f":"+MT!G13","v":3.1500021999999994},"m          My =",0,"kNm             H =",{"$f":"SQRT(G5*G5+G6*G6)","v":{"$error":"#VALUE!"}},"kN      B'=",null,null,null,null,"   + Mx"]
[null,null,null,"      dulja stranica u smjeru osi(x)    L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m            V =",{"$f":"+V26*E9","v":{"$error":"#VALUE!"}},"kN                V =",{"$f":"IF(K3=2,G9,G9+E8*E9*E11*24)","v":{"$error":"#VALUE!"}},"kPa  FMr=",null,4," ",null,2,null,null,null,null,null,"VERTIKALNE SILE DJELUJU POZITIVNO NA NOSIVOST"]
[null,null,null," dubina temeljenja    Df =",{"$f":"+'Analiza i dimenzioniranje'!E52+'Analiza i dimenzioniranje'!E65","v":1.5000009999999999},"m"," ","     Mx =",{"$f":"IF(K3=2,G7-G9*G13,G7-G9*G13+G6*E11)","v":{"$error":"#VALUE!"}},"kNm  Al=",null,null,null,"  +My",null,null,null,null,null,null,"Gtem ..........................",{"$f":"+'Analiza i dimenzioniranje'!B135","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C135","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$I$32","v":1}]
[null,null,null,"  visina temelja    ht =",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m   ",null,"     My =",{"$f":"IF(K3=2,G8+G9*G12,+G9*G12+G5*E11)","v":{"$error":"#VALUE!"}},"kNm   iq=",null,null,"Kontaktni naponi",null,null,null,null,null,null,null,"Gzid+konz ...................",{"$f":"+'Analiza i dimenzioniranje'!B136","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C136","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$I$32","v":1}]
[null,null,null,"   nagib dna temelja    a =",{"$f":"ATAN(Q30)*180/PI()","v":7.3057554566405489},"°        ex° =",0,"    pa =",{"$f":"D68","v":{"$error":"#VALUE!"}},"kPa    ig=",null,null,"s1=   ",{"$f":"+(N16+I11/N17+I10/N18)","v":{"$error":"#VALUE!"}},"KPa ",null,"ic",null,null,null,"Grebra kontrafora ............",{"$f":"+'Analiza i dimenzioniranje'!B137","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C137","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$I$32","v":1}]
[null,null,"Ako nema vode g'=g","g' =",{"$f":"+'Analiza i dimenzioniranje'!H18","v":10},"kN/m3  ey°=",0,"    Vdop=",{"$f":"I12*P5*P6","v":{"$error":"#VALUE!"}},"kN      ic=",null,null,"s2=   ",{"$f":"N16+I11/N17-I10/N18","v":{"$error":"#VALUE!"}},"KPa ",null,"ig",null,null,null,"Gnasip na konzoli ............",{"$f":"+'Analiza i dimenzioniranje'!B138","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C138","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$I$32","v":1}]
[null,{"$f":"I5*3.14159/180","v":0.2543076625950379},"Faktori:","     gj =",{"$f":"+'Analiza i dimenzioniranje'!M27","v":1.25},null,null,null,null,null,null,null,"s3=   ",{"$f":"N16-I11/N17+I10/N18","v":{"$error":"#VALUE!"}},"KPa ",null,null,null,null,null,"Gnasipa iza zida .............",{"$f":"+'Analiza i dimenzioniranje'!B139","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C139","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$I$32","v":1}]
[null,{"$f":"45*PI()/180","v":0.78539816339744828},{"$f":"B15+B17","v":0.91255199469496717},"      gc =",{"$f":"+'Analiza i dimenzioniranje'!M28","v":1.25},{"$f":"IF(E14*P17>10,\"Fkl >\",\"Fkl =\")","v":{"$error":"#VALUE!"}},{"$f":"IF(E14*P17>10,10,R16)","v":{"$error":"#VALUE!"}},{"$f":"B16*B16","v":1.672279875125072},{"$f":"TAN(B14)","v":0.25993552228740757},{"$f":"3.14159*I15","v":0.81661083746289675},null,null,"s4=   ",{"$f":"N16-I11/N17-I10/N18","v":{"$error":"#VALUE!"}},"KPa ",{"$f":"IF(P5<P6,P5,P6)","v":{"$error":"#VALUE!"}},null,null,null,null,"Gnasipa ispred zida .........",{"$f":"+'Analiza i dimenzioniranje'!B140","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C140","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$I$32","v":1}]
[null,{"$f":"TAN(C15)","v":1.293166607643838},"     Ng=",{"$f":"2*(H16-1)*TAN(I5*PI()/180)","v":1.4473558577295844},"      Nc=",{"$f":"(H16-1)/I15","v":10.710596970300873},"      Nq=",{"$f":"EXP(J15)*H15","v":3.7840646174850825},null,null,null,null,"     V/F=",{"$f":"I9/(E9*E8)","v":{"$error":"#VALUE!"}},"KN/m2",{"$f":"P5*P6","v":{"$error":"#VALUE!"}},"A'",{"$f":"IF(P17<1,\"temelj klizi\",E14*P17)","v":{"$error":"#VALUE!"}},null,null,"PPrometno ...................",{"$f":"+'Analiza i dimenzioniranje'!B141","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C141","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$J$34","v":0}]
[null,{"$f":"B14/2","v":0.12715383129751895},"Tekst:"," za stalno + dopunsko  opterećenje",null,null,null,null,null," ",null,null,"      Wy=",{"$f":"E9*E9*E8/6","v":75.600052799999986},"m3",{"$f":"IF(I8=0,100,TAN(I5*3.14159/180)*G9/I8)","v":{"$error":"#VALUE!"}},null,null,null,null,"PTočkasto ....................",{"$f":"+'Analiza i dimenzioniranje'!B142","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C142","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$J$32","v":1}]
[null,{"$f":"Q18","v":{"$error":"#VALUE!"}},{"$f":"IF(N15<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(N14<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(N12<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(N13<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}},null,null,null,"      Wx=",{"$f":"E9*E8*E8/6","v":19.845027720009671},"m3",null,{"$f":"IF((((P19/E9)*(P19/E9))+((P20/E8)*(P20/E8)))>=0.11111,\"PROMJENA DIMENZIJA TEMELJA\",((P19/E9)*(P19/E9))+((P20/E8)*(P20/E8)))","v":{"$error":"#VALUE!"}},null,null,null,"PLinijsko ......................",{"$f":"+'Analiza i dimenzioniranje'!B143","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C143","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$J$32","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"G8/G9+G12","v":{"$error":"#VALUE!"}},"ex",null,null,null,"QTemelj ili vozilo.....................",{"$f":"+'Analiza i dimenzioniranje'!B144","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C144","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!D31=\"VV=\",'Analiza i dimenzioniranje'!$J$34,'Analiza i dimenzioniranje'!$J$32)","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-(G7/G9)+G13","v":{"$error":"#VALUE!"}},"ey",null,null,null,"VSidro ........................",{"$f":"+'Analiza i dimenzioniranje'!B145","v":25.881904536133977},{"$f":"+'Analiza i dimenzioniranje'!C145","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$J$32","v":1}]
[null,"                  P R O J E K T N A   O T P O R N O S T     T L A    ",null,null,null,null,null,{"$f":"+D17","v":" za stalno + dopunsko  opterećenje"},null,null,null,null,null,null,null,null,null,null,null,null,"Ev1 ...........................",{"$f":"+'Analiza i dimenzioniranje'!B146","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C146","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$J$32","v":1}]
[null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ev2  ..........................",{"$f":"+'Analiza i dimenzioniranje'!B147","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C147","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$J$32","v":1}]
[null," Proračun projektne otpornosti tla provodi se prema EUROCODU 7, prema izrazu:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ev3  ..........................",{"$f":"+'Analiza i dimenzioniranje'!B148","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C148","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$J$32","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vpotres (vert.sila)........................",0,{"$f":"+'Analiza i dimenzioniranje'!C149","v":0},1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Uzgon ….......................",{"$f":"+'Analiza i dimenzioniranje'!B150","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C150","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$I$33","v":1.5}]
[null,null,"  pa=R/A'= c' *Nc*bc*sc*ic+q' *Nq*bq*sq*iq+0,5*g' *B' *Ng*bg*sg*ig",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"V=",{"$f":"+V10*X10+V11*X11+V12*X12+V13*X13+V14*X14+V15*X15+V16*X16+V17*X17+V18*X18+V19*X19+V20*X20+V21*X21+V22*X22+V23*X23+V24*X24-V25*X25","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"M=",{"$f":"+V10*W10*X10+V11*W11*X11+V12*W12*X12+V13*W13*X13+V14*W14*X14+V15*W15*X15+V16*W16*X16+V17*W17*X17+V18*W18*X18+V19*W19*X19+V20*W20*X20+V21*W21*X21+V22*W22*X22+V23*W23*X23+V24*W24*X24+V25*W25*X25","v":{"$error":"#VALUE!"}},"x=",{"$f":"+V27/V26","v":{"$error":"#VALUE!"}}]
[null,"gdje je:",null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     Ms =",{"$f":"IF('Analiza i dimenzioniranje'!A83=\"\",X37,Y37)","v":{"$error":"#VALUE!"}},"kNm/m'"]
[null,"g.........................................",null,"prostorna efektivna težina"]
[null,"B'.............................................",null,"širina temelja (efektivna)",null,null,null,null,null,null,null,null,null,null,null,"tana=",{"$f":"+('Analiza i dimenzioniranje'!E52-'Analiza i dimenzioniranje'!E51)/('Analiza i dimenzioniranje'!E61+Kontrafore!$E$3)","v":0.12820505588432746}]
[null,"Nc, Nq, Ng................................",null,"faktori nosivosti",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOMENT OKO OSI TEMELJA KOD NOSIVOSTI"]
[null,"ic, iq, ig ...................................",null,"faktori nagiba opterećenja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Točka A",null,"Krak rezultante do osi temelja"]
[null,"sc,sq, sg .......................................",null,"faktori oblika temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+'Sile i krakovi'!M8","v":0},null,"bez kont","s kont"]
[null,"bc,bq, bg  ..............................................",null,"faktori nagiba dna temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+'Sile i krakovi'!N8","v":0},"Vert. Rez x=",{"$f":"+'Analiza i dimenzioniranje'!E61/2-'Dopušteno Vs+'!X27","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C185/2-'Dopušteno Vs+'!X27","v":{"$error":"#VALUE!"}}]
[null,"c',j'  .........................................................",null,"mobilizirani parametri čvrstoće tla",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Horiz. Rez y=",{"$f":"+IF('Analiza i dimenzioniranje'!E53=\"0,00\",0,'Analiza i dimenzioniranje'!E61/2/'Analiza i dimenzioniranje'!E53)+'Analiza i dimenzioniranje'!H167","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!H167++IF('Analiza i dimenzioniranje'!E53=\"0,00\",0,'Analiza i dimenzioniranje'!C185/2/'Analiza i dimenzioniranje'!E53)","v":{"$error":"#VALUE!"}}]
[null,"dc .........................................",null,"faktor dubine temeljenja"]
[null,"q ...............................................",null,"opterećenje tla u razini temeljenja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Moment oko osi temelja",null,{"$f":"+V26*X34+'Analiza i dimenzioniranje'!B167*X35","v":{"$error":"#VALUE!"}},{"$f":"+V26*Y34+'Analiza i dimenzioniranje'!B167*Y35","v":{"$error":"#VALUE!"}}]
[null,"A ...........................................",null,"reducirana površina temelja"]
[]
[]
[null,"Karakteristike tla:",null,null,null,"           Dimenzije temelja:"]
[]
[null,"      j =",{"$f":"E5","v":18},"°  ",null,"     B =",{"$f":"E8","v":3.1500021999999994},"m (širina temelja)"]
[null,"       c =",{"$f":"E6","v":25},"kPa",null,"     L =",{"$f":"E9","v":12},"m (dužina temelja)"]
[null,"    g =",{"$f":"E7","v":20},"kN/m3",null,"     Df =",{"$f":"E10","v":1.5000009999999999},"m (dubina temeljenja)"]
[null,null,null,null,null,"a =",{"$f":"+E12","v":7.3057554566405489},"o   (kut nagiba temelja)"]
[]
[null,"Parcijalni faktori svojstava tla:"]
[null,null," "]
[null,"   gj =",{"$f":"E14","v":1.25},"    gc =",{"$f":"E15","v":1.25}]
[null,null," ",null," "," "," "]
[null,"Mobilizirani parametri čvrstoće tla:"]
[null,null," ",null,null," "," "," "," "]
[null,null,"   tgjm  =  tgj/gj  =",{"$f":"TAN(E5*3.14159/180)/E14","v":0.25993552228740757},"------>  j' =",{"$f":"I5","v":14.5707680719339},"° ----> Nq =  ",{"$f":"+H16","v":3.7840646174850825},"  => FIm=",{"$f":"I5","v":14.5707680719339},"m=mB=",{"$f":"+(2+(P6/P5))/(1+(P6/P5))","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(G5=0,100000,(G6/G5))","v":100000}]
[null,null,"c' = c/gc =",{"$f":"I6","v":20},null," ","    Nc=",{"$f":"F16","v":10.710596970300873},null,null,"m=mL=",{"$f":"+(2+(P5/P6))/(1+(P5/P6))","v":{"$error":"#VALUE!"}},null,{"$f":"ATAN(N54)*180/PI()","v":89.999427042204886}]
[null,null,null,null,null,null,"Ng=",{"$f":"D16","v":1.4473558577295844},null,null,"m=",{"$f":"+L55*N56+L54*N57","v":{"$error":"#VALUE!"}},null,{"$f":"+COS(N55*PI()/180)*COS(N55*PI()/180)","v":9.9999999990320259E-11}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+((1-I8/(I9+P5*P6*I6/TAN(I5*PI()/180))))","v":{"$error":"#VALUE!"}},null,{"$f":"+SIN(N55*PI()/180)*SIN(N55*PI()/180)","v":0.99999999989999999}]
[null,"Faktori :"]
[null,"sq=1+(B'/L')*sinj '=",null,{"$f":"1+(P6/P5)*SIN(I5*PI()/180)","v":{"$error":"#VALUE!"}},"    iq =",{"$f":"POWER(L57,L56)","v":{"$error":"#VALUE!"}},"    bq =",{"$f":"+POWER(J60,2)","v":0.93480999420900812},null,{"$f":"RADIANS(G46)","v":0.1275094870639194}]
[null,"sg = 1 - 0.30*B'/L' =",null,{"$f":"IF(P5<P6,1-0.3*P5/P6,1-0.3*P6/P5)","v":{"$error":"#VALUE!"}},"    ig =",{"$f":"POWER(L57,(L56+1))","v":{"$error":"#VALUE!"}},"    bg =",{"$f":"+H59","v":0.93480999420900812},null,{"$f":"+(1-J59*TAN(I5*PI()/180))","v":0.96685572564318412}]
[null,"sc=(sq*Nq-1)/(Nq-1)=",null,{"$f":"(D59*H54-1)/(H54-1)","v":{"$error":"#VALUE!"}},"    ic =",{"$f":"F59-(1-F59)/(H55*TAN(I5*PI()/180))","v":{"$error":"#VALUE!"}},"    bc =",{"$f":"+H59-(1-H59)/(H55*TAN(I5*PI()/180))","v":0.91139460798908856}]
[null,null,"q=g*Df =",{"$f":"+'Analiza i dimenzioniranje'!C232","v":17.000019999999999},"kPa"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"cos2*teta"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sin2*teta"]
[null,"Projektna otpornost tla za glavno + dopunsko opterećenje iznosi :"]
[]
[null,null,"   pa =",{"$f":"D55*H55*H61*D61*F61+D62*H54*H59*D59*F59+0.5*E13*P6*H56*H60*D60*F60","v":{"$error":"#VALUE!"}},"kPa"]
[]
[]
[]
[]
[]
[null,{"$f":"+IF(K3=1,\"Opterećenje na vrhu temelja:\",\"Opterećenje na dnu temelja\")","v":"Opterećenje na dnu temelja"}]
[]
[null,"       V=",{"$f":"G9","v":{"$error":"#VALUE!"}},"kN  -Vertikalna sila"]
[null,"      Hx=",{"$f":"G5","v":0},"kN   komponenta u smjeru x"]
[null,"      Hy=",{"$f":"G6","v":{"$error":"#VALUE!"}},"kN   komponenta u smjeru y"]
[null,"      Mx=",{"$f":"G7","v":{"$error":"#VALUE!"}},"kNm  moment oko osi x"]
[null,"      My=",{"$f":"G8","v":0},"kNm  moment oko osi y"]
[]
[null,"Reducirana površina temelja:"]
[]
[null,null,"B'=B-2.ey=",{"$f":"P6","v":{"$error":"#VALUE!"}},"m","      DOPUŠTENA VERTIKALNA SILA:"]
[null,null,"        L'=L-2.ex=",{"$f":"P5","v":{"$error":"#VALUE!"}},"m"]
[null,null,"        A' = L'.B' =",{"$f":"P16","v":{"$error":"#VALUE!"}},"m2","    Vdop=",{"$f":"D68*D86/'Analiza i dimenzioniranje'!M38","v":{"$error":"#VALUE!"}},{"$f":"IF(G86>C76,\"kN   >  V  =\",\"kN   <   V =\")","v":{"$error":"#VALUE!"}},{"$f":"+C76","v":{"$error":"#VALUE!"}},"kN"]
[null,null,null,null,null,null,"Iskorištenost:  ",{"$f":"+I86/G86","v":{"$error":"#VALUE!"}},{"$f":"+IF(H87<=100%,\"(Zadovoljava)\",\"(Ne zadovoljava\")","v":{"$error":"#VALUE!"}}]

{"sheet":"Dopušteno Vs-","index":36,"n_rows":87,"n_cols":25,"rows_kept":87,"cut":false,"hidden":true,"merged":[[23,14,24,14],[26,13,27,13],[27,1,27,2],[29,11,29,12],[5,12,6,12],[5,13,6,13],[10,5,10,6],[20,11,20,12],[21,12,22,12],[23,12,24,12]]}
[]
["PRORAČUN AKO VERTIKALNE SILE DJELUJU NEGATIVNO NA NOSIVOST",null,null,null,null,null,null,null,null,null,null,null,"Shema opterećenja"]
[null,null,null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null," y"]
[null,null,null,"     j =",{"$f":"+'Analiza i dimenzioniranje'!G14","v":18},"°            Hx =",0,"kN                 j'=",{"$f":"ATAN(TAN(E5*3.14159/180)/E14)*180/3.14159","v":14.5707680719339},"°        ex=",null,3,"L  ",null,1,{"$f":"IF(G9=0,E9,+E9-ABS(2*P19))","v":{"$error":"#VALUE!"}}]
[null,null,"          ","       c =",{"$f":"+'Analiza i dimenzioniranje'!G15","v":25},"kPa       Hy =",{"$f":"+'Analiza i dimenzioniranje'!B167*E9","v":{"$error":"#VALUE!"}},"kN                c' =",{"$f":"E6/E15","v":20},"kPa    ey=",null,null,"      Hy ","Hx","        x  ",{"$f":"IF(G9=0,E8,+E8-ABS(2*P20))","v":{"$error":"#VALUE!"}}]
[null,null,"q=g*Df","g =",{"$f":"+'Analiza i dimenzioniranje'!G16","v":20},"kN/m3     Mx =",{"$f":"V28*E9","v":{"$error":"#VALUE!"}},"kNm",null,"           L'=",null,"  B",null,null,"                     ",{"$f":"I5*3.14159/180","v":0.2543076625950379}]
[null,null,null,"   kraća stranica u smjer osi (y)    B =",{"$f":"+MT!G13","v":3.1500021999999994},"m          My =",0,"kNm             H =",{"$f":"SQRT(G5*G5+G6*G6)","v":{"$error":"#VALUE!"}},"kN      B'=",null,null,null,null,"   + Mx"]
[null,null,null,"      dulja stranica u smjeru osi(x)    L =",{"$f":"+'Analiza i dimenzioniranje'!E49","v":12},"m            V =",{"$f":"+V26*E9","v":{"$error":"#VALUE!"}},"kN                V =",{"$f":"IF(K3=2,G9,G9+E8*E9*E11*24)","v":{"$error":"#VALUE!"}},"kPa  FMr=",null,4," ",null,2,null,null,null,null,null,"VERTIKALNE SILE DJELUJU NEGATIVNO NA NOSIVOST"]
[null,null,null," dubina temeljenja    Df =",{"$f":"+'Analiza i dimenzioniranje'!E52+'Analiza i dimenzioniranje'!E65","v":1.5000009999999999},"m"," ","     Mx =",{"$f":"IF(K3=2,G7-G9*G13,G7-G9*G13+G6*E11)","v":{"$error":"#VALUE!"}},"kNm  Al=",null,null,null,"  +My",null,null,null,null,null,null,"Gtem ..........................",{"$f":"+'Analiza i dimenzioniranje'!B135","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C135","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$I$31","v":1.35}]
[null,null,null,"  visina temelja    ht =",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"m   ",null,"     My =",{"$f":"IF(K3=2,G8+G9*G12,+G9*G12+G5*E11)","v":{"$error":"#VALUE!"}},"kNm   iq=",null,null,"Kontaktni naponi",null,null,null,null,null,null,null,"Gzid+konz ...................",{"$f":"+'Analiza i dimenzioniranje'!B136","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C136","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$I$31","v":1.35}]
[null,null,null,"   nagib dna temelja    a =",{"$f":"ATAN(Q30)*180/PI()","v":7.3057554566405489},"°        ex° =",0,"    pa =",{"$f":"D68","v":{"$error":"#VALUE!"}},"kPa    ig=",null,null,"s1=   ",{"$f":"+(N16+I11/N17+I10/N18)","v":{"$error":"#VALUE!"}},"KPa ",null,"ic",null,null,null,"Grebra kontrafora ............",{"$f":"+'Analiza i dimenzioniranje'!B137","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C137","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$I$31","v":1.35}]
[null,null,"Ako nema vode g'=g","g' =",{"$f":"+'Analiza i dimenzioniranje'!H18","v":10},"kN/m3  ey°=",0,"    Vdop=",{"$f":"I12*P5*P6","v":{"$error":"#VALUE!"}},"kN      ic=",null,null,"s2=   ",{"$f":"N16+I11/N17-I10/N18","v":{"$error":"#VALUE!"}},"KPa ",null,"ig",null,null,null,"Gnasip na konzoli ............",{"$f":"+'Analiza i dimenzioniranje'!B138","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C138","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$I$31","v":1.35}]
[null,{"$f":"I5*3.14159/180","v":0.2543076625950379},"Faktori:","     gj =",{"$f":"+'Analiza i dimenzioniranje'!M27","v":1.25},null,null,null,null,null,null,null,"s3=   ",{"$f":"N16-I11/N17+I10/N18","v":{"$error":"#VALUE!"}},"KPa ",null,null,null,null,null,"Gnasipa iza zida .............",{"$f":"+'Analiza i dimenzioniranje'!B139","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C139","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$I$31","v":1.35}]
[null,{"$f":"45*PI()/180","v":0.78539816339744828},{"$f":"B15+B17","v":0.91255199469496717},"      gc =",{"$f":"+'Analiza i dimenzioniranje'!M28","v":1.25},{"$f":"IF(E14*P17>10,\"Fkl >\",\"Fkl =\")","v":{"$error":"#VALUE!"}},{"$f":"IF(E14*P17>10,10,R16)","v":{"$error":"#VALUE!"}},{"$f":"B16*B16","v":1.672279875125072},{"$f":"TAN(B14)","v":0.25993552228740757},{"$f":"3.14159*I15","v":0.81661083746289675},null,null,"s4=   ",{"$f":"N16-I11/N17-I10/N18","v":{"$error":"#VALUE!"}},"KPa ",{"$f":"IF(P5<P6,P5,P6)","v":{"$error":"#VALUE!"}},null,null,null,null,"Gnasipa ispred zida .........",{"$f":"+'Analiza i dimenzioniranje'!B140","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C140","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$I$31","v":1.35}]
[null,{"$f":"TAN(C15)","v":1.293166607643838},"     Ng=",{"$f":"2*(H16-1)*TAN(I5*PI()/180)","v":1.4473558577295844},"      Nc=",{"$f":"(H16-1)/I15","v":10.710596970300873},"      Nq=",{"$f":"EXP(J15)*H15","v":3.7840646174850825},null,null,null,null,"     V/F=",{"$f":"I9/(E9*E8)","v":{"$error":"#VALUE!"}},"KN/m2",{"$f":"P5*P6","v":{"$error":"#VALUE!"}},"A'",{"$f":"IF(P17<1,\"temelj klizi\",E14*P17)","v":{"$error":"#VALUE!"}},null,null,"PPrometno ...................",{"$f":"+'Analiza i dimenzioniranje'!B141","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C141","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$J$33","v":1.3}]
[null,{"$f":"B14/2","v":0.12715383129751895},"Tekst:"," za stalno + dopunsko  opterećenje",null,null,null,null,null," ",null,null,"      Wy=",{"$f":"E9*E9*E8/6","v":75.600052799999986},"m3",{"$f":"IF(I8=0,100,TAN(I5*3.14159/180)*G9/I8)","v":{"$error":"#VALUE!"}},null,null,null,null,"PTočkasto ....................",{"$f":"+'Analiza i dimenzioniranje'!B142","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C142","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$J$31","v":1}]
[null,{"$f":"Q18","v":{"$error":"#VALUE!"}},{"$f":"IF(N15<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(N14<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(N12<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(N13<0,\"VLAK U TEMELJU\",\"\")","v":{"$error":"#VALUE!"}},null,null,null,"      Wx=",{"$f":"E9*E8*E8/6","v":19.845027720009671},"m3",null,{"$f":"IF((((P19/E9)*(P19/E9))+((P20/E8)*(P20/E8)))>=0.11111,\"PROMJENA DIMENZIJA TEMELJA\",((P19/E9)*(P19/E9))+((P20/E8)*(P20/E8)))","v":{"$error":"#VALUE!"}},null,null,null,"PLinijsko ......................",{"$f":"+'Analiza i dimenzioniranje'!B143","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C143","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$J$31","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"G8/G9+G12","v":{"$error":"#VALUE!"}},"ex",null,null,null,"QTemelj ili vozilo.....................",{"$f":"+'Analiza i dimenzioniranje'!B144","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C144","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!D31=\"VV=\",'Analiza i dimenzioniranje'!$J$33,'Analiza i dimenzioniranje'!$J$31)","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-(G7/G9)+G13","v":{"$error":"#VALUE!"}},"ey",null,null,null,"VSidro ........................",{"$f":"+'Analiza i dimenzioniranje'!B145","v":25.881904536133977},{"$f":"+'Analiza i dimenzioniranje'!C145","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$J$31","v":1}]
[null,"                  P R O J E K T N A   O T P O R N O S T     T L A    ",null,null,null,null,null,{"$f":"+D17","v":" za stalno + dopunsko  opterećenje"},null,null,null,null,null,null,null,null,null,null,null,null,"Ev1 ...........................",{"$f":"+'Analiza i dimenzioniranje'!B146","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C146","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$J$31","v":1}]
[null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ev2  ..........................",{"$f":"+'Analiza i dimenzioniranje'!B147","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C147","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$J$31","v":1}]
[null," Proračun projektne otpornosti tla provodi se prema EUROCODU 7, prema izrazu:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ev3  ..........................",{"$f":"+'Analiza i dimenzioniranje'!B148","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C148","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$J$31","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vpotres (vert.sila)........................",0,{"$f":"+'Analiza i dimenzioniranje'!C149","v":0},1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Uzgon ….......................",{"$f":"+'Analiza i dimenzioniranje'!B150","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C150","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!I34","v":0}]
[null,null,"  pa=R/A'= c' *Nc*bc*sc*ic+q' *Nq*bq*sq*iq+0,5*g' *B' *Ng*bg*sg*ig",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"V=",{"$f":"+V10*X10+V11*X11+V12*X12+V13*X13+V14*X14+V15*X15+V16*X16+V17*X17+V18*X18+V19*X19+V20*X20+V21*X21+V22*X22+V23*X23+V24*X24","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"M=",{"$f":"+V10*W10*X10+V11*W11*X11+V12*W12*X12+V13*W13*X13+V14*W14*X14+V15*W15*X15+V16*W16*X16+V17*W17*X17+V18*W18*X18+V19*W19*X19+V20*W20*X20+V21*W21*X21+V22*W22*X22+V23*W23*X23","v":{"$error":"#VALUE!"}},"x=",{"$f":"+V27/V26","v":{"$error":"#VALUE!"}}]
[null,"gdje je:",null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     Ms =",{"$f":"IF('Analiza i dimenzioniranje'!A83=\"\",X37,Y37)","v":{"$error":"#VALUE!"}},"kNm/m'"]
[null,"g.........................................",null,"prostorna efektivna težina"]
[null,"B'.............................................",null,"širina temelja (efektivna)",null,null,null,null,null,null,null,null,null,null,null,"tana=",{"$f":"+('Analiza i dimenzioniranje'!E52-'Analiza i dimenzioniranje'!E51)/('Analiza i dimenzioniranje'!E61+Kontrafore!$E$3)","v":0.12820505588432746}]
[null,"Nc, Nq, Ng................................",null,"faktori nosivosti",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOMENT OKO OSI TEMELJA KOD NOSIVOSTI"]
[null,"ic, iq, ig ...................................",null,"faktori nagiba opterećenja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Točka A",null,"Krak rezultante do osi temelja"]
[null,"sc,sq, sg .......................................",null,"faktori oblika temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+'Sile i krakovi'!M8","v":0},null,"bez kont","s kont"]
[null,"bc,bq, bg  ..............................................",null,"faktori nagiba dna temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+'Sile i krakovi'!N8","v":0},"Vert. Rez x=",{"$f":"+'Analiza i dimenzioniranje'!E61/2-'Dopušteno Vs-'!X27","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C185/2-'Dopušteno Vs-'!X27","v":{"$error":"#VALUE!"}}]
[null,"c',j'  .........................................................",null,"mobilizirani parametri čvrstoće tla",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Horiz. Rez y=",{"$f":"+IF('Analiza i dimenzioniranje'!E53=\"0,00\",0,'Analiza i dimenzioniranje'!E61/2/'Analiza i dimenzioniranje'!E53)+'Analiza i dimenzioniranje'!H167","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!H167++IF('Analiza i dimenzioniranje'!E53=\"0,00\",0,'Analiza i dimenzioniranje'!C185/2/'Analiza i dimenzioniranje'!E53)","v":{"$error":"#VALUE!"}}]
[null,"dc .........................................",null,"faktor dubine temeljenja"]
[null,"q ...............................................",null,"opterećenje tla u razini temeljenja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Moment oko osi temelja",null,{"$f":"+V26*X34+'Analiza i dimenzioniranje'!B167*X35","v":{"$error":"#VALUE!"}},{"$f":"+V26*Y34+'Analiza i dimenzioniranje'!B167*Y35","v":{"$error":"#VALUE!"}}]
[null,"A ...........................................",null,"reducirana površina temelja"]
[]
[]
[null,"Karakteristike tla:",null,null,null,"           Dimenzije temelja:"]
[]
[null,"      j =",{"$f":"E5","v":18},"°  ",null,"     B =",{"$f":"E8","v":3.1500021999999994},"m (širina temelja)"]
[null,"       c =",{"$f":"E6","v":25},"kPa",null,"     L =",{"$f":"E9","v":12},"m (dužina temelja)"]
[null,"    g =",{"$f":"E7","v":20},"kN/m3",null,"     Df =",{"$f":"E10","v":1.5000009999999999},"m (dubina temeljenja)"]
[null,null,null,null,null,"a =",{"$f":"+E12","v":7.3057554566405489},"o   (kut nagiba temelja)"]
[]
[null,"Parcijalni faktori svojstava tla:"]
[null,null," "]
[null,"   gj =",{"$f":"E14","v":1.25},"    gc =",{"$f":"E15","v":1.25}]
[null,null," ",null," "," "," "]
[null,"Mobilizirani parametri čvrstoće tla:"]
[null,null," ",null,null," "," "," "," "]
[null,null,"   tgjm  =  tgj/gj  =",{"$f":"TAN(E5*3.14159/180)/E14","v":0.25993552228740757},"------>  j' =",{"$f":"I5","v":14.5707680719339},"° ----> Nq =  ",{"$f":"+H16","v":3.7840646174850825},"  => FIm=",{"$f":"I5","v":14.5707680719339},"m=mB=",{"$f":"+(2+(P6/P5))/(1+(P6/P5))","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(G5=0,100000,(G6/G5))","v":100000}]
[null,null,"c' = c/gc =",{"$f":"I6","v":20},null," ","    Nc=",{"$f":"F16","v":10.710596970300873},null,null,"m=mL=",{"$f":"+(2+(P5/P6))/(1+(P5/P6))","v":{"$error":"#VALUE!"}},null,{"$f":"ATAN(N54)*180/PI()","v":89.999427042204886}]
[null,null,null,null,null,null,"Ng=",{"$f":"D16","v":1.4473558577295844},null,null,"m=",{"$f":"+L55*N56+L54*N57","v":{"$error":"#VALUE!"}},null,{"$f":"+COS(N55*PI()/180)*COS(N55*PI()/180)","v":9.9999999990320259E-11}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+((1-I8/(I9+P5*P6*I6/TAN(I5*PI()/180))))","v":{"$error":"#VALUE!"}},null,{"$f":"+SIN(N55*PI()/180)*SIN(N55*PI()/180)","v":0.99999999989999999}]
[null,"Faktori :"]
[null,"sq=1+(B'/L')*sinj '=",null,{"$f":"1+(P6/P5)*SIN(I5*PI()/180)","v":{"$error":"#VALUE!"}},"    iq =",{"$f":"POWER(L57,L56)","v":{"$error":"#VALUE!"}},"    bq =",{"$f":"+POWER(J60,2)","v":0.93480999420900812},null,{"$f":"RADIANS(G46)","v":0.1275094870639194}]
[null,"sg = 1 - 0.30*B'/L' =",null,{"$f":"IF(P5<P6,1-0.3*P5/P6,1-0.3*P6/P5)","v":{"$error":"#VALUE!"}},"    ig =",{"$f":"POWER(L57,(L56+1))","v":{"$error":"#VALUE!"}},"    bg =",{"$f":"+H59","v":0.93480999420900812},null,{"$f":"+(1-J59*TAN(I5*PI()/180))","v":0.96685572564318412}]
[null,"sc=(sq*Nq-1)/(Nq-1)=",null,{"$f":"(D59*H54-1)/(H54-1)","v":{"$error":"#VALUE!"}},"    ic =",{"$f":"F59-(1-F59)/(H55*TAN(I5*PI()/180))","v":{"$error":"#VALUE!"}},"    bc =",{"$f":"+H59-(1-H59)/(H55*TAN(I5*PI()/180))","v":0.91139460798908856}]
[null,null,"q=g*Df =",{"$f":"+'Analiza i dimenzioniranje'!C232","v":17.000019999999999},"kPa"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"cos2*teta"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sin2*teta"]
[null,"Projektna otpornost tla za glavno + dopunsko opterećenje iznosi :"]
[]
[null,null,"   pa =",{"$f":"D55*H55*H61*D61*F61+D62*H54*H59*D59*F59+0.5*E13*P6*H56*H60*D60*F60","v":{"$error":"#VALUE!"}},"kPa"]
[]
[]
[]
[]
[]
[null,{"$f":"+IF(K3=1,\"Opterećenje na vrhu temelja:\",\"Opterećenje na dnu temelja\")","v":"Opterećenje na dnu temelja"}]
[]
[null,"       V=",{"$f":"G9","v":{"$error":"#VALUE!"}},"kN  -Vertikalna sila"]
[null,"      Hx=",{"$f":"G5","v":0},"kN   komponenta u smjeru x"]
[null,"      Hy=",{"$f":"G6","v":{"$error":"#VALUE!"}},"kN   komponenta u smjeru y"]
[null,"      Mx=",{"$f":"G7","v":{"$error":"#VALUE!"}},"kNm  moment oko osi x"]
[null,"      My=",{"$f":"G8","v":0},"kNm  moment oko osi y"]
[]
[null,"Reducirana površina temelja:"]
[]
[null,null,"B'=B-2.ey=",{"$f":"P6","v":{"$error":"#VALUE!"}},"m","      DOPUŠTENA VERTIKALNA SILA:"]
[null,null,"        L'=L-2.ex=",{"$f":"P5","v":{"$error":"#VALUE!"}},"m"]
[null,null,"        A' = L'.B' =",{"$f":"P16","v":{"$error":"#VALUE!"}},"m2","    Vdop=",{"$f":"D68*D86/'Analiza i dimenzioniranje'!M38","v":{"$error":"#VALUE!"}},{"$f":"IF(G86>C76,\"kN   >  V  =\",\"kN   <   V =\")","v":{"$error":"#VALUE!"}},{"$f":"+C76","v":{"$error":"#VALUE!"}},"kN"]
[null,null,null,null,null,null,"Iskorištenost:  ",{"$f":"+I86/G86","v":{"$error":"#VALUE!"}},{"$f":"+IF(H87<=100%,\"(Zadovoljava)\",\"(Ne zadovoljava\")","v":{"$error":"#VALUE!"}}]

{"sheet":"ProjektniPristupi","index":37,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":true,"merged":[[47,4,47,6],[4,4,6,5],[4,6,5,7],[18,4,20,5],[18,6,19,7],[43,4,43,6],[44,4,44,6]]}
[]
[]
[null,"Odabrani pristup"]
[null,{"$f":"+'Unos podataka'!L11","v":3}]
[null,null,null,null,"PARCIJALNI KOEFICIJENTI ZA SVE PROJEKTNE PRISTUPE ZA PREVRTANJE (EQU PROBLEM)"]
[]
[]
[null,"Parcijalni koeficijenti za sve pristupe",null,null,"     Parcijalni koeficijenti za svojstva tla:  M"]
[null,{"$f":"+G9","v":1.25},null,null,"za kut unutr. trenja    gj=",null,1.25]
[null,{"$f":"+G10","v":1.25},null,null,"za koheziju            gc =",null,1.25]
[null,null,null,null,"     Parcijalni koeficijenti djelovanja:         A"]
[null,null,null,null,"EQU"]
[null,{"$f":"+G13","v":1.1000000000000001},null,null,"          Trajna nepovoljna ",null,1.1000000000000001]
[null,0.9,null,null,"         Trajna povoljna           ",null,0.9]
[null,1.5,null,null,"           Promjenjiva nepovoljna     ",null,1.5]
[null,0,null,null,"           Promjenjiva povoljna        ",null,0]
[]
[]
[null,null,null,null,"PARCIJALNI KOEFICIJENTI ZA PROJEKTNE PRISTUPE ZA KLIZANJE I NOSIVOST (GEO PROBLEM)",null,"PP1"]
[null,null,null,null,null,null,null,null,"PP2","PP3"]
[null,null,null,null,null,null,"1K1","1K2"]
[null,"Parcijalni koeficijenti za odabrani pristup",null,null,"     Parcijalni koeficijenti za svojstva tla:  M"]
[null,{"$f":"+IF(B$4=\"1K1\",G23,IF(B$4=\"1K2\",H23,IF(B$4=2,I23,IF(B$4=\"EQU\",1.25,J23))))","v":1.25},null,null,"za kut unutr. trenja    gj=",null,1,1.25,1,1.25]
[null,{"$f":"+IF(B$4=\"1K1\",G24,IF(B$4=\"1K2\",H24,IF(B$4=2,I24,IF(B$4=\"EQU\",1.25,J24))))","v":1.25},null,null,"za koheziju            gc =",null,1,1.25,1,1.25]
[null,null,null,null,"     Parcijalni koeficijenti djelovanja:         A"]
[]
[null,null,null,null,"STR"]
[null,{"$f":"+IF(B$4=\"1K1\",G28,IF(B$4=\"1K2\",H28,IF(B$4=2,I28,IF(B$4=\"EQU\",1,J28))))","v":1.35},null,null,"          Trajna nepovoljna ",null,1.35,1,1.35,1.35]
[null,{"$f":"+IF(B$4=\"1K1\",G29,IF(B$4=\"1K2\",H29,IF(B$4=2,I29,IF(B$4=\"EQU\",1,J29))))","v":1},null,null,"         Trajna povoljna           ",null,1,1,1,1]
[null,1.5,null,null,"           Promjenjiva nepovoljna     ",null,1.5,1.3,1.5,1.5]
[null,{"$f":"+IF(B$4=\"1K1\",G31,IF(B$4=\"1K2\",H31,IF(B$4=2,I31,IF(B$4=\"EQU\",0,J31))))","v":0},null,null,"           Promjenjiva povoljna        ",null,0,0,0,0]
[]
[null,null,null,null,"GEO"]
[null,{"$f":"+IF(B$4=\"1K1\",G34,IF(B$4=\"1K2\",H34,IF(B$4=2,I34,IF(B$4=\"EQU\",1,J34))))","v":1},null,null,"          Trajna nepovoljna ",null,1.35,1,1.35,1]
[null,{"$f":"+IF(B$4=\"1K1\",G35,IF(B$4=\"1K2\",H35,IF(B$4=2,I35,IF(B$4=\"EQU\",1,J35))))","v":1},null,null,"         Trajna povoljna           ",null,1,1,1,1]
[null,1.3,null,null,"           Promjenjiva nepovoljna     ",null,1.5,1.3,1.5,1.3]
[null,{"$f":"+IF(B$4=\"1K1\",G37,IF(B$4=\"1K2\",H37,IF(B$4=2,I37,IF(B$4=\"EQU\",0,J37))))","v":0},null,null,"           Promjenjiva povoljna        ",null,0,0,0,0]
[]
[null,null,null,null,"     Parcijalni koeficijenti za otpornost:      R"]
[null,{"$f":"+IF(B$4=\"1K1\",G40,IF(B$4=\"1K2\",H40,IF(B$4=2,I40,J40)))","v":1},null,null,"Prevrtanje              gR =",null,1,1,1,1]
[null,1,null,null,"Klizanje                   gRh=",null,1,1,1.1000000000000001,1]
[null,1,null,null,"Nosivost                gRv=",null,1,1,1.4,1]

{"sheet":"Troškovnik","index":38,"n_rows":77,"n_cols":45,"rows_kept":77,"cut":false,"hidden":false,"merged":[[42,12,43,12],[43,1,43,11],[39,1,39,2],[41,3,41,11],[42,1,42,11],[40,1,40,2],[39,3,39,11],[30,1,30,11],[52,10,52,12],[46,2,46,13],[48,10,48,12],[49,10,49,12],[50,10,50,12],[51,10,51,12],[47,10,47,12],[38,1,38,2],[38,3,38,11],[33,13,37,13],[32,1,32,11],[30,12,32,12],[30,13,32,13],[44,7,44,12],[40,3,40,11],[56,35,59,39],[56,22,59,26],[68,32,68,33],[71,27,71,33],[42,13,43,13],[42,15,43,15],[44,14,44,15],[42,14,43,14],[30,15,32,15],[30,14,32,14],[3,1,3,15],[6,14,9,14],[6,15,9,15],[6,12,9,12],[4,7,4,12],[10,15,11,15],[12,1,12,11],[13,1,13,11],[14,1,14,11],[15,14,15,15],[17,15,18,15],[19,15,20,15],[20,1,20,11],[18,1,18,11],[33,14,37,14],[33,15,37,15],[17,13,18,13],[19,12,20,12],[17,12,18,12],[17,14,18,14],[19,14,20,14],[23,7,23,12],[25,1,25,11],[26,1,26,11],[35,1,37,11],[33,1,33,11],[31,5,31,6],[33,12,37,12],[19,13,20,13],[19,8,19,11],[21,0,22,0],[21,13,22,13],[22,1,22,11],[21,12,22,12],[29,1,29,11],[0,17,1,21],[15,7,15,12],[27,14,27,15],[23,14,23,15],[27,7,27,12],[21,14,22,14],[21,15,22,15],[0,0,0,15],[10,1,10,11],[6,13,9,13],[1,1,1,11],[9,1,9,11],[10,13,11,13],[10,14,11,14],[10,12,11,12],[2,17,12,21]]}
["TROŠKOVNIK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tekst Troškovnika nije protektiran i može se u potpunosti izmijeniti osim Rekapitulacije i kolona N i P"]
["St. ","OPIS RADOVA",null,null,null,null,null,null,null,null,null,null,"jed. mjere","količina","jedinična cijena","cijena"]
["0.","   Pripremni radovi",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  \n   Program je predviđen za Analizu i dimenzioniranje, kada su:  \n   Zidovi iste visine i izvode se u istom profilu terena\n  Količine u stavci Zemljani radovi određene su prema zadanim koordinatama i nije potrebna nikakva intervencija u količinama u Troškovniku.\n  \n  Ali, ako su:\n  1. Zidovi iste visine a izvode se u različitom profilu terena\n  Za dobivanje preciznijih količina, preporučam izvesti analizu i dimenzioniranje za 2 ili više segmenata zida bitno različitih profila terena \n  U ovom slučaju pritaju se samo troškovnici i u osnovni proračun u sheetu Troškovnik, upiše se zbroj količina svakog zida. Radi ujednačavanja armature u čitavom zidu preporučam te vrijednosti upisati su proračun zida sa najnepovoljnijim profilom terena.\nPrimjer: 4 različitih profila terena = 1 ili 2 proračuna ukoliko je bitna razlika u profilu terena ili 1 proračun uz izbor najnepovoljnijeg profila.\n  \n Ili, ako su:\n  2. Zidovi različite visine a izvode se i u različitom profilu terena\n  Budući da se u ovom slučaju mijenja količina betona i oblik armature svakog dijela zida, kao i vrijednosti količina u Zemljanim radovima, potrebno je printati sve proračune. \n  Za svaku visinu zida napraviti postupak kao u prethodnom tekstu.\n  Ukupnu količinu materijala za više zidova treba prikazati u skupnom Troškovniku.\n "]
[null,"     Izvoditelj je dužan prije početka građevinskih radova napraviti tehničku priprema gradilišta i opreme za rad  i dostavi Nadzornom inženjeru dinamički plan radova i popis mehanizacije.\n     Priprema obuhvaća i izvedbu privremenih gradilišnih objekata i puteva, privremenih gradilišnih  deponija i instalacija, te nabavu i dopremu potrebne opreme. Troškove snosi Izvođač."]
[null,null,null,null,null,null,null,"    Pripremni radovi             Paušalno:",null,null,null,null,null,{"$f":"+Q53","v":"€"},700,{"$f":"+O5","v":700}]
["1.","   Zemljani radovi"]
["1.1.","    Strojni iskop tla",null,null,"III.","  kategorije  sa utovarom u kamion i odvozom",null,null,null,null,null,null,"m3",{"$f":"+'Analiza i dimenzioniranje'!M526*E9/100","v":{"$error":"#VALUE!"}},3,{"$f":"+N7*O7","v":{"$error":"#VALUE!"}}]
[null,"na deponiju na udaljenosti cca",null,null,null,null,20,"km. Predviđena količina strojnog"]
[null,"iskopa iznosi cca",null,null,95,"% ukupne količine."]
[null,"     Obračun količina izvodi se prema stvarnim izmjerama, ovjerenim po nadzornom inžinjeru."]
["1.2.","     Ručni iskop u zoni temelja, utovar i odvoz tla na istu deponiju.",null,null,null,null,null,null,null,null,null,null,"m3",{"$f":"+'Analiza i dimenzioniranje'!M526*Troškovnik!H12","v":{"$error":"#VALUE!"}},30,{"$f":"+N11*O11","v":{"$error":"#VALUE!"}}]
[null," Predviđena količina ručnog iskopa cca",null,null,null,null,null,{"$f":"+(100-E9)%","v":0.05},"ukupnog iskopa."]
["1.3.","     Ručno planiranje dna iskopa za temelj sa tolerancijom do   ±3  cm.  \n    Prekop iznad ovih vrijednosti se ne priznaje kao VTR ali u svakom slučaju iskop treba imati odgovarajući nagib, prema projektu.   \n Obračun se provodi prema stvarno izvedenim količinama.   ",null,null,null,null,null,null,null,null,null,null,"m2",{"$f":"+'Analiza i dimenzioniranje'!T521*('Analiza i dimenzioniranje'!E61+Kontrafore!E3)","v":46.800026399999993},10,{"$f":"+N13*O13","v":468.0002639999999}]
["1.4.","      Ugradnja zasipa iza zida. Kao materijal za zasip može se koristiti materijal iz iskopa ili odgovarajući materijal koji se ugrađuje u slojevima max debljine 40 cm, uz odgovarajuće zbijanje. Modul stišljivost ugrađenog materijala treba biti minimalno kao i modul stišljivosti prirodnog tlo iza zasipa. Materijal se ugrađuje nakon završetka betoniranja svake etaže zida (max visina 2,5 m) i dostignute čvrstoće (cca 80 %) betona. Istovremeno se po visini ugrađuje drenažni sloj i zasip (nakon ugradnje drenaže). \n U cijenu radova uključiti nabavu, prijevoz i ugradnju materijala. \n Obračun se provodi prema stvarno izvedenim količinama.                                                   ",null,null,null,null,null,null,null,null,null,null,"m3",{"$f":"+'Analiza i dimenzioniranje'!P526","v":{"$error":"#VALUE!"}},16,{"$f":"+N14*O14","v":{"$error":"#VALUE!"}}]
["1.5.","     Ugradnja drenažnog materijala iza zida. Za izradu drenažnog sloja ugrađuje se prirodni šljunak ili drobljeni materijal. Modul stišljivost ugrađenog materijala treba biti minimalno kao i modul stišljivosti prirodnog tlo iza zasipa. Materijal se ugrađuje nakon završetka betoniranja zida i dostignute čvrstoće (cca 80 %) betona. Drenažni materijal ugrađuje se, po visini, istovremeno sa zasipom (nakon ugradnje drenaže). \n U cijenu radova uključiti nabavu, prijevoz i ugradnju materijala.\n Obračun se provodi prema stavci troškovnika.                                                  ",null,null,null,null,null,null,null,null,null,null,"m3",{"$f":"+'Analiza i dimenzioniranje'!S529","v":{"$error":"#VALUE!"}},20,{"$f":"+N15*O15","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null," Zemljani radovi                Ukupno:",null,null,null,null,null,{"$f":"+Q53","v":"€"},{"$f":"SUM(P7:P15)","v":{"$error":"#VALUE!"}}]
["2.","   Betonski radovi"]
["2.1.","     Nabava i ugradnja betona  razreda",null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!M12","v":"16/20"}," visine cca ",null,10,"cm na ","m3",{"$f":"+'Analiza i dimenzioniranje'!E49*('Analiza i dimenzioniranje'!E61+Kontrafore!E3)*1.1*0.1","v":5.1480029040000002},120,{"$f":"+N18*O18","v":617.76034848000006}]
[null,"isplaniranu temeljnu plohu (podložni beton). \n  Obračun se izvodi prema stvarno izvedenim količinama"]
["2.2.","     Nabava i ugradnja betona razreda",null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!I49=20,'Analiza i dimenzioniranje'!M12,IF('Analiza i dimenzioniranje'!I49=25,'Analiza i dimenzioniranje'!N12,IF('Analiza i dimenzioniranje'!I49=30,'Analiza i dimenzioniranje'!O12,IF('Analiza i dimenzioniranje'!I49=37,'Analiza i dimenzioniranje'!P12,IF('Analiza i dimenzioniranje'!I49=45,'Analiza i dimenzioniranje'!Q21,'Analiza i dimenzioniranje'!R21)))))","v":"25/30"}," za temelj.",null,null,null,"m3",{"$f":"IF('Unos podataka'!$O$48=\"DA\",'Poprečni presjek zida'!BF7*'Iskaz armature'!U1,+'Analiza i dimenzioniranje'!E49*(Kontrafore!AC32+Kontrafore!AE32))","v":{"$error":"#VALUE!"}},135,{"$f":"+N20*O20","v":{"$error":"#VALUE!"}}]
[null,"    Ugradnja betona izvodi se u iskop, bez oplate, nakon postavljanja armature. Razred izloženosti betona XF2. \n Obračun se provodi prema stavci troškovnika."]
["2.3.","     Nabava i ugradnja betona razreda",null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!I53=20,'Analiza i dimenzioniranje'!M12,IF('Analiza i dimenzioniranje'!I53=25,'Analiza i dimenzioniranje'!N12,IF('Analiza i dimenzioniranje'!I53=30,'Analiza i dimenzioniranje'!O12,IF('Analiza i dimenzioniranje'!I53=37,'Analiza i dimenzioniranje'!P12,IF('Analiza i dimenzioniranje'!I53=45,'Analiza i dimenzioniranje'!Q12,'Analiza i dimenzioniranje'!R12)))))","v":"30/37"}," za zid. Ugradnja se izvodi",null,null,null,"m3",{"$f":"+'Analiza i dimenzioniranje'!P531","v":{"$error":"#VALUE!"}},155,{"$f":"+N22*O22","v":{"$error":"#VALUE!"}}]
[null,"u dvostranoj dobro učvršćenoj oplati kako bi se izbjeglo izdizanje oplate prilikom betoniranja. Ugradnja betona razreda izloženosti XF2, ne smije se izvoditi sa visine veće od 1,5 m ili se ugradnja izvodi kontraktorom. \nMaksimalna visina jedne etaže betoniranja ne smije biti veća od 2,5 m. Slijedeća etaže može se izvoditi nakon završetka vezanja betona. Prije ugradnje betona, ugrađenu armaturu treba pregledati nadzorni inžinjer i upisom u Građevinski dnevnik odobriti betoniranje. \n  U cijenu radova uključiti i izradu i demontažu oplate uz višestruko korištenje. \n  Obračun se provodi prema stavci troškovnika."]
[null,null,null,null,null,null,null,"    Betonski radovi                Ukupno:",null,null,null,null,null,{"$f":"+Q53","v":"€"},{"$f":"SUM(P18:P23)","v":{"$error":"#VALUE!"}}]
["3.","   Armirački radovi"]
["3.1.","     Nabava, doprema, rezanje i ugradnja rebraste armature - šipki, B500B u temelje i zid.  ",null,null,null,null,null,null,null,null,null,null,"kg",{"$f":"IF('Unos podataka'!$O$48=\"\",+'Iskaz armature'!W105,'Iskaz armature'!W18)","v":{"$error":"#VALUE!"}},1.5,{"$f":"+N26*O26","v":{"$error":"#VALUE!"}}]
["3.2.","  Nabava, doprema, rezanje i ugradnja armaturnih mreža B500B u zid.  ",null,null,null,null,null,null,null,null,null,null,"kg",{"$f":"+'Iskaz armature'!X105","v":{"$error":"#VALUE!"}},1.5,{"$f":"+N27*O27","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,"    Armirački radovi                Ukupno:",null,null,null,null,null,{"$f":"Q53","v":"€"},{"$f":"SUM(P26:P27)","v":{"$error":"#VALUE!"}}]
["4.","Ostali radovi"]
["4.1.","Drenaža"]
[null," Izvedba drenaže od \"Raudril\" cijevi promjera 15 cm s odvodom u gradsku kanalizaciju ili otvorenu odvodnju. Cijev se ugrađuje po čitavoj duljini zida na betonskoj tajači i zaštićuje drenažnim materijalom (granulirani šljunak). Osim drenaže iza zida u izvedbu treba uključiti i kanalizaciju do gradske kanalizacije ili otvorenog vodotoka, s kanalizacionim cijevima F 20 cm. ",null,null,null,null,null,null,null,null,null,null,"m'",{"$f":"+'Analiza i dimenzioniranje'!E49+F32","v":37},45,{"$f":"+N31*O31","v":1665}]
[null," Duljina ovog priključka iznosi",null,null,null,25,null,"m."]
[null," U cijenu radova uključiti nabavu, dopremu i ugradnju svih materijala za izvedbu drenaže i odvodnje u gradsku kanalizaciju ili otvoreni vodotok. \n Obračun se provodi prema stvarno izvedenim količinama."]
["4.2.","Sidra"]
[null,"   Nabava i ugradnja samobušivih (IBO ili IBI) sidara ",null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!J74","v":{"$error":"#VALUE!"}}]
[null," Pri injektiranju treba voditi računa da se injektiranje izvede dominantno u sidrišnoj zoni. Duljina sidrišne zone prikazana je u projektu. \n  Izvođač treba nadzornom inženjeru dostaviti dokaz nosivosti sklopa šipke+matica+podložna ploča, kao i za spojnice za nastavljanje (produljivanje) sidra. Sidra se tretiraju kao stalna.\n  U cijenu radova uključiti nabavu šipki, matica, podložnih pločica i kompletnog pribora za ugradnju, dopremu, ugradnju, injektiranje i sve pripremne radove kao i selidbu do lokacije i po lokaciji. \n Samobušiva sidra su razlićite duljine prema specifikaciji u projektu i sastavljaju se od komada duljine 2, 3 ili 4 m.\n Obračun se provodi prema ukupnoj duljini sidara a za st. 4.2.3. uključujući i otpadni dio koji ostaje pri rezanju sidara.\n"]
[]
[]
[null,"4.2.1.   ",null,"Generalni i lokalni transport garniture ",null,null,null,null,null,null,null,null,"pauš.",{"$f":"+IF('Analiza i dimenzioniranje'!P22=0,0,1)","v":1},2500,{"$f":"+N39*O39","v":2500}]
[null,"4.2.2.",null,"Komplet spojnica, matica i podložnih pločica",null,null,null,null,null,null,null,null,"kom.",{"$f":"IF('Iskaz armature'!N54=\"\",\"\",'Iskaz armature'!V58)","v":{"$error":"#VALUE!"}},20,{"$f":"+N40*O40","v":{"$error":"#VALUE!"}}]
[null,"4.2.3.   ",null,"Nabava i ugradnja sidara",null,null,null,null,null,null,null,null,"m'",{"$f":"IF('Iskaz armature'!X58=\"\",0,+'Iskaz armature'!X58)","v":{"$error":"#VALUE!"}},28,{"$f":"+N41*O41","v":{"$error":"#VALUE!"}}]
[null,"4.2.4.",null,"Injektiranje",null,null,null,null,null,null,null,null,"m'",{"$f":"+'Analiza i dimenzioniranje'!H73","v":11.5},28,{"$f":"+N42*O42","v":322}]
["4.3.","Procjednice",null,null,null,null,null,null,null,null,null,null,"kom",{"$f":"+'Analiza i dimenzioniranje'!E49/2","v":6},15,{"$f":"+N43*O43","v":90}]
[null," Procjednice (barbakane) se izvode na razmaku od 2 m i na visini cca 0,3 m iznad vrha drenažnih cijevi. Promjer procjednica iznosi minimalno 5 cm. Izvode se ugradnjom \"Juvidur\" cijevi prije betoniranja zida. \n U cijenu radova uključena je nabava, priprema i ugradnja \"Juvidur\" cijevi unutar dvostrane oplate."]
[null,null,null,null,null,null,null,"   Ostali radovi:                   Ukupno:",null,null,null,null,null,{"$f":"+Q53","v":"€"},{"$f":"SUM(P31:P44)","v":{"$error":"#VALUE!"}}]
[]
[null,null,"REKAPITULACIJA"]
[null,null,null,null,"0.","Pripremni radovi",null,null,null,null,{"$f":"+P5","v":700},null,{"$f":"+P5","v":700},{"$f":"+Q53","v":"€"}]
[null,null,null,null,"1. ","Zemljani radovi",null,null,null,null,{"$f":"+O16","v":{"$error":"#VALUE!"}},null,null,{"$f":"+Q53","v":"€"}]
[null,null,null,null,"2.","Betonski radovi",null,null,null,null,{"$f":"+O24","v":{"$error":"#VALUE!"}},null,null,{"$f":"+Q53","v":"€"}]
[null,null,null,null,"3.","Armirački radovi",null,null,null,null,{"$f":"+O28","v":{"$error":"#VALUE!"}},null,null,{"$f":"+Q53","v":"€"}]
[null,null,null,null,"4.","Ostali radovi",null,null,null,null,{"$f":"+O45","v":{"$error":"#VALUE!"}},null,null,{"$f":"+Q53","v":"€"}]
[null,null,null,null,null,null,null,null,"Sveukupno:",null,{"$f":"+SUM(K48:M52)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+Q53","v":"€"},null,null,"€","Izbor valute"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HRK"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"€"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KM"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RSD"]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!AA446","v":"Vrh zida"},{"$f":"+'Analiza i dimenzioniranje'!AB446","v":"T2"},{"$f":"+'Analiza i dimenzioniranje'!AC446","v":"T3"},{"$f":"+'Analiza i dimenzioniranje'!AD446","v":"T4"},{"$f":"+'Analiza i dimenzioniranje'!AE446","v":0},{"$f":"+'Analiza i dimenzioniranje'!AF446","v":"Vrh zida"},{"$f":"+'Analiza i dimenzioniranje'!AG446","v":"T2"},{"$f":"+'Analiza i dimenzioniranje'!AH446","v":"vrh temelja"},null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!AU448","v":0},{"$f":"+'Analiza i dimenzioniranje'!AV446","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!Z447","v":"x="},{"$f":"+'Analiza i dimenzioniranje'!AA447","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!K113","v":-21.16},{"$f":"+'Analiza i dimenzioniranje'!AC447","v":-15},{"$f":"+'Analiza i dimenzioniranje'!AD447","v":-10},{"$f":"+'Analiza i dimenzioniranje'!AE447","v":"x="},{"$f":"+'Analiza i dimenzioniranje'!AF447","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AG447","v":-21.16},{"$f":"+'Analiza i dimenzioniranje'!AH447","v":-1},null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!AU449","v":0},{"$f":"+'Analiza i dimenzioniranje'!AV447","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!Z448","v":"Y="},{"$f":"+'Analiza i dimenzioniranje'!AA448","v":0},{"$f":"+'Analiza i dimenzioniranje'!AB448","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC448","v":9.5},{"$f":"+'Analiza i dimenzioniranje'!AD448","v":9},{"$f":"+'Analiza i dimenzioniranje'!AE448","v":"Y="},{"$f":"+'Analiza i dimenzioniranje'!AF448","v":0},{"$f":"+'Analiza i dimenzioniranje'!AG448","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AH448","v":1.2},null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!AU450","v":0},{"$f":"+'Analiza i dimenzioniranje'!AV448","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!Z449","v":"Y="},{"$f":"+'Analiza i dimenzioniranje'!AA449","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB449","v":"*x    +"},{"$f":"+'Analiza i dimenzioniranje'!AC449","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD449","v":"Jednadžba pravca proj. kosine od vrha"},{"$f":"+'Analiza i dimenzioniranje'!AE449","v":"Y="},{"$f":"+'Analiza i dimenzioniranje'!AF449","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AG449","v":"*x    +"},{"$f":"+'Analiza i dimenzioniranje'!AH449","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!AU451","v":0},{"$f":"+'Analiza i dimenzioniranje'!AV449","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!Z450","v":"Y="},{"$f":"+'Analiza i dimenzioniranje'!AA450","v":-0.1},{"$f":"+'Analiza i dimenzioniranje'!AB450","v":"*x    +"},{"$f":"+'Analiza i dimenzioniranje'!AC450","v":8},{"$f":"+'Analiza i dimenzioniranje'!AD450","v":"Jednadžba pravca terena od 3-4"},{"$f":"+'Analiza i dimenzioniranje'!AE450","v":"Y="},{"$f":"+'Analiza i dimenzioniranje'!AF450","v":-1.2},{"$f":"+'Analiza i dimenzioniranje'!AG450","v":"*x    +"},{"$f":"+'Analiza i dimenzioniranje'!AH450","v":0},null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!AU452","v":0},{"$f":"+'Analiza i dimenzioniranje'!AV450","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!Z451","v":"X="},{"$f":"+AD64","v":-21.16},{"$f":"+'Analiza i dimenzioniranje'!AB451","v":"Y="},{"$f":"+'Analiza i dimenzioniranje'!AC451","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD451","v":"sjecište"},{"$f":"+'Analiza i dimenzioniranje'!AE451","v":"X="},{"$f":"+'Analiza i dimenzioniranje'!AF451","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AG451","v":"Y="},{"$f":"+'Analiza i dimenzioniranje'!AH451","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!AU453","v":0},{"$f":"+'Analiza i dimenzioniranje'!AV451","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!Z452","v":"Pravac 1-2"},{"$f":"+'Analiza i dimenzioniranje'!AA452","v":"T2"},{"$f":"+'Analiza i dimenzioniranje'!AB452","v":"T1"},{"$f":"+'Analiza i dimenzioniranje'!AC452","v":"sredina"},null,{"$f":"+'Analiza i dimenzioniranje'!AD452","v":"privremani iskop"},null,"sredina"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!Z453","v":"x="},{"$f":"+AD64","v":-21.16},{"$f":"+'Analiza i dimenzioniranje'!AB453","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC453","v":{"$error":"#VALUE!"}},{"$f":"+AE70-1","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD453","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE453","v":-1},{"$f":"+(AD70+AH70)/2","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!Z454","v":"Y="},{"$f":"+'Analiza i dimenzioniranje'!AA454","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB454","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC454","v":{"$error":"#VALUE!"}},{"$f":"+AE71-2","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD454","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE454","v":1.2},{"$f":"+(AD71+AH71)/2","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sjecište  projektiranog pokosa terena i pokosa prometa"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AB70","v":"x="},{"$f":"+AD64","v":-21.16},{"$error":"#VALUE!"},{"$f":"+'Unos podataka'!Q74","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!Q75","v":{"$error":"#VALUE!"}},{"$f":"+AD64","v":-21.16},{"$f":"+AD64","v":-21.16}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+'Unos podataka'!S74","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!S75","v":6.2644906473896782},{"$f":"+AE77","v":{"$error":"#VALUE!"}},{"$f":"+AC74","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"(AD74-AC74)/(AD73-AC73)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AC75*AC73+AC74","v":{"$error":"#VALUE!"}},null,{"$f":"+'Unos podataka'!$Q$91","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!$Q$92","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"IF(AE73=AF73,0,-(AF74-AE74)/(AE73-AF73))","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-(AE73*AC76-AE74)","v":{"$error":"#VALUE!"}},null,{"$f":"+AD64","v":-21.16},{"$f":"+'Unos podataka'!$R$92","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"IF(AC74=AE74,0,+(AE76-AE75)/(AC75-AC76))","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AC76*AC77+AE76","v":{"$error":"#VALUE!"}}]

{"sheet":"C III-V","index":39,"n_rows":166,"n_cols":65,"rows_kept":166,"cut":false,"hidden":true,"merged":[[90,4,90,5],[73,1,73,2],[67,3,67,4],[67,5,67,6],[73,3,73,6],[67,1,67,2],[8,61,9,62],[8,63,9,64],[8,57,9,58],[37,45,38,45],[8,59,9,60],[19,45,20,45],[25,45,26,45],[31,45,32,45],[11,33,11,34],[25,38,26,38],[31,38,32,38],[37,38,38,38],[13,45,14,45],[13,38,14,38],[19,38,20,38],[21,22,21,23],[25,22,25,23],[116,53,116,55],[99,34,99,35],[99,36,99,37],[96,36,98,37],[112,40,113,40],[41,33,41,34],[112,39,113,39],[17,12,17,16],[42,15,43,18],[40,27,40,28],[44,25,44,26],[42,11,43,14],[103,9,103,12],[53,27,53,28],[106,20,106,21],[73,13,73,14],[73,10,73,11],[70,17,70,18],[67,10,67,11],[67,15,67,16],[21,24,21,25],[67,13,67,14],[0,1,0,2],[0,3,0,4],[42,7,43,10],[11,3,11,4],[42,5,42,6],[42,1,42,2],[0,9,0,10],[10,3,10,4],[1,5,1,8],[0,5,0,7],[42,3,42,4],[12,3,12,4],[0,35,0,36],[1,27,1,28],[11,27,11,28],[26,31,26,32],[11,29,11,30],[3,27,3,30],[7,29,7,30],[8,27,8,28],[8,29,8,30],[0,29,0,30],[7,27,7,28],[7,35,7,36],[7,31,7,32],[8,35,8,36],[11,35,11,36],[8,31,8,32],[11,31,11,32],[5,20,5,21],[10,20,10,21],[13,20,13,21],[16,20,16,21],[13,12,13,16],[44,15,44,16],[44,9,44,10],[44,19,44,20],[44,17,44,18],[44,13,44,14],[44,11,44,12],[125,45,125,48],[135,15,135,17],[110,38,113,38],[110,39,111,40],[80,24,81,25],[112,19,113,20],[96,20,98,21],[105,9,105,12],[74,19,75,19],[105,14,105,17],[109,14,109,17],[99,14,99,17],[98,9,99,12],[96,22,97,23],[112,9,112,13],[112,14,112,18],[114,38,116,39],[117,38,117,39],[98,18,98,19],[77,13,77,14],[109,9,109,12],[79,20,79,21],[79,18,79,19],[84,24,84,25],[121,45,121,48],[96,34,98,35],[114,34,114,35],[114,36,114,37],[96,24,99,25],[35,24,35,25],[73,8,73,9],[66,8,66,11],[67,8,67,9],[70,19,70,20],[77,15,77,16],[104,14,104,17],[44,7,44,8],[99,30,99,31],[58,31,58,32],[62,27,62,28],[99,32,99,33],[96,32,98,33],[59,31,59,32],[77,8,77,9],[77,10,77,11],[73,15,73,16],[66,13,66,16],[122,0,122,1],[122,2,122,3],[146,30,146,33],[153,30,153,33],[139,30,139,33],[140,25,140,28],[145,25,145,28],[150,25,150,28],[22,24,22,25],[117,2,117,5],[111,2,111,5],[96,1,96,2],[96,3,96,4],[96,5,96,6],[90,0,90,1],[90,2,90,3],[77,1,77,2],[145,2,145,3],[135,5,135,6],[127,1,127,2],[127,3,127,4],[137,2,137,3],[77,3,77,4],[77,5,77,6]]}
["Točke","ZID I TEMELJ",null,"NASIP NA TEMELJU IZA",null,"ZID, KONZOLA I NASIP NA KONZOLI",null,null,null,null,null,null,null,null,"Presjek XV",{"$f":"+($B$9-$B$4)*(Q1-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},null,null,null,"Točka A",null,"Presjek I-I",null,null,null,null,null,null,"1. sloj",null,null,null,null,null,"2. sloj klizna ploha",null,null,"Jednadžba klizne plohe 2. sloja"]
[1,{"$f":"2+'Unos podataka'!G49","v":2},{"$f":"'Analiza i dimenzioniranje'!BG9+'Unos podataka'!J41","v":0.12820515121628623},null,null,"ZA BILO KOJI PRESJEK ",null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(Q2-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+Q1","v":4.4000000000000004},"Presjek zid Iv",{"$f":"+($B$9-$B$4)*(T2-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AN44","v":{"$error":"#VALUE!"}},{"$f":"+B15","v":4.9000021999999994},{"$f":"+C15","v":0.5},{"$f":"+'C III-V'!B10+0.05","v":{"$error":"#VALUE!"}},-0.5,null,null,null,"Rsidra",null,{"$f":"+U9","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782},null,"Jednadžba površine terena",null,null,{"$f":"+$U$85","v":2},{"$f":"+$V$85","v":0}]
[2,{"$f":"+B2-'Unos podataka'!$G$49","v":2},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,null,null,null,null,null,null,null,"Presjek Xvi",{"$f":"+($B$9-$B$4)*(Q3-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72},null,{"$f":"+($B$11-$B$10)*(T3-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AN44","v":{"$error":"#VALUE!"}},"Točka B",null,{"$f":"+W2","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C10+0.5","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,20,AB11)","v":20},{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,0,AC11)","v":0},{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782},"Y=",{"$f":"+(AE3-AE2)/(AD3-AD2)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AG3*AD2+AE2","v":{"$error":"#VALUE!"}},{"$f":"+$X$85","v":1.1597509541483482},{"$f":"+$X$86","v":1.2},"Y=",{"$f":"+($AK$3-$AK$2)/($AJ$3-$AJ$2)","v":-1.4281480067421144},"*x              +",{"$f":"-$AM$3*$AJ$2+$AK$2","v":2.8562960134842288}]
[3,{"$f":"+B3+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+C3","v":1.2},{"$f":"+B19","v":2},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>C4,B21,B4)","v":3.4000010999999999},{"$f":"IF(E20>C4,E20,C4)","v":1.2},{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(Q4-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+Q3","v":4.72},"Presjek V",{"$f":"+($B$9-$B$4)*(T4-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!R44","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!B2","v":2},{"$f":"+'C III-V'!C2","v":0.12820515121628623},"Presjek II-II",null,null,null,null,"Os rezultante sidara Ukupna računska sila u sidrima",null,null,null,null,"Jednadžba najdonjeg sloja",null,"Y=",{"$f":"+(AK3-AK2)/(AJ3-AJ2)","v":-1.4281480067421144},"*x             +",{"$f":"-AJ3*AJ2+AK2","v":-2.3195019082966963},null,"x","y",null,null,null,null,null,null,null,null,null,null,null,"x",null,null,"x"]
[4,{"$f":"IF('Analiza i dimenzioniranje'!E50=0,B4,B4-(C5-C12)/'Analiza i dimenzioniranje'!E57)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},{"$f":"IF('Analiza i dimenzioniranje'!E59=0,'C III-V'!B5,+D4)","v":2},{"$f":"IF(B6<2,'Analiza i dimenzioniranje'!F45,IF(B9>2,'Analiza i dimenzioniranje'!E47+'Unos podataka'!G10+(B9-2)*TAN('Analiza i dimenzioniranje'!F21*PI()/180),C19))","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,B21,B5)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,E20,C5)","v":3.14},{"$f":"+F8","v":{"$error":"#VALUE!"}},{"$f":"+G8","v":3.44},null,null,null,null,null,"Presjek Xvii",{"$f":"+($B$9-$B$4)*(Q5-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AG44","v":5.04},null,{"$f":"+($B$11-$B$10)*(T5-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!R44","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!B15-0.05","v":4.8500021999999996},{"$f":"+'C III-V'!X2","v":-0.5},null,null,"Nasip na zidu iza",null,null,null,null,null,null,null,"Y=",{"$f":"+($AK$3-$AK$2)/($AJ$3-$AJ$2)","v":-1.4281480067421144},"*x             +",{"$f":"-$AM$3*$AJ$2+$AK$2","v":2.8562960134842288},null,{"$f":"+AJ2","v":2},{"$f":"+AK2","v":0},{"$f":"+'Analiza i dimenzioniranje'!F97","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!G96","v":6.2644906473896782},null,null,null,null,null,null,null,null,null,"y",null,null,"y"]
[5,{"$f":"+B5-'Analiza i dimenzioniranje'!G78","v":{"$error":"#VALUE!"}},{"$f":"+C5","v":3.14},{"$f":"IF('Analiza i dimenzioniranje'!E59=0,'C III-V'!B5,+'Unos podataka'!S56)","v":{"$error":"#VALUE!"}},{"$f":"IF(B6<B3,C5,C9+'Unos podataka'!G10)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C7,B21,B6)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C6,E20,C6)","v":3.14},{"$f":"IF(F7>F9,H5,F9)","v":{"$error":"#VALUE!"}},{"$f":"IF(F7>F9,I5,IF(E20>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C III-V'!E20,G9))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(Q6-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+Q5","v":5.04},"Presjek VI",{"$f":"+($B$9-$B$4)*(T6-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},"TLO 1. kosina",null,{"$f":"+'C III-V'!B15-0.05","v":4.8500021999999996},{"$f":"+'C III-V'!X3","v":{"$error":"#VALUE!"}},null,2,{"$f":"IF('Analiza i dimenzioniranje'!AW26>'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AW26)","v":0},"za x=",{"$f":"+AB14","v":{"$error":"#VALUE!"}},null,{"$f":"+AD14","v":{"$error":"#VALUE!"}},null,{"$f":"+AF14","v":-20},null,{"$f":"+AH14","v":-20},null,{"$f":"+AJ14","v":-25.75},null,null,{"$f":"+AA143","v":-1.0572404418349119},{"$f":"+AB143","v":4},{"$f":"+'Analiza i dimenzioniranje'!F98","v":-8},{"$f":"+'Analiza i dimenzioniranje'!G97","v":6.2644906473896782},null,null,null,null,null,null,null,null,null,"Jednadžba  pravca za sidrišne dionice"]
[6,{"$f":"IF('Analiza i dimenzioniranje'!G78=0,'C III-V'!B8,B6)","v":{"$error":"#VALUE!"}},{"$f":"C6+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+B4","v":3.4000010999999999},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>=C7,B21,B7)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C7,E20,C7)","v":3.44},{"$f":"+D17","v":{"$error":"#VALUE!"}},{"$f":"+E17","v":"A"},null,null,null,null,null,"Presjek Xviii",{"$f":"+($B$9-$B$4)*(Q7-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AH44","v":5.36},null,{"$f":"+($B$11-$B$10)*(T7-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"'Analiza i dimenzioniranje'!D17+'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17+'Unos podataka'!F9","v":6},"Presjek ZID",null,"Horizontala",2,{"$f":"'Analiza i dimenzioniranje'!BF28","v":0},"y=",{"$f":"+$AG$3*AC6+$AI$3","v":{"$error":"#VALUE!"}},null,{"$f":"+$AG$3*AE6+$AI$3","v":{"$error":"#VALUE!"}},null,{"$f":"+$AG$3*AG6+$AI$3","v":{"$error":"#VALUE!"}},null,{"$f":"+$AG$3*AI6+$AI$3","v":{"$error":"#VALUE!"}},null,{"$f":"+$AG$3*AK6+$AI$3","v":{"$error":"#VALUE!"}},null,"Y=",{"$f":"+(AO6-AO5)/(AN6-AN5)","v":-1.3083694515041995},"*x      +",{"$f":"-AN7*AN5+AO5","v":2.616738903008399},"jed aktivnog klina",null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!L97","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!M97","v":{"$error":"#VALUE!"}}]
[7,{"$f":"+B22","v":{"$error":"#VALUE!"}},{"$f":"+C7","v":3.44},{"$f":"+D4","v":2},{"$f":"+E4","v":1.2},{"$f":"IF(E20>C8,B21,B8)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C8,E20,C8)","v":3.44},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$H$15=0,I7+(H7-H8)*'Unos podataka'!R57,IF('C III-V'!H9>'Unos podataka'!$B$105,I7+(H7-H8)*'Unos podataka'!$R$55,'Unos podataka'!$T$57))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(Q8-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+Q7","v":5.36},"Presjek VII",{"$f":"+($B$9-$B$4)*(T8-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+V7","v":6},{"$f":"+'C III-V'!B15-0.5","v":4.4000021999999994},{"$f":"+'C III-V'!C10+0.1","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C5","v":3.14},null,"Sidro I",null,"Sidro II",null,"Sidro III",null,"Sidro IV",null,"Sidro V",null,null,"Y=",{"$f":"+(AQ6-AQ5)/(AP6-AP5)","v":{"$error":"#VALUE!"}},"*x      +",{"$f":"-AN8*AP5+AQ5","v":{"$error":"#VALUE!"}},"jed prirodnog terena",null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!L98","v":0.54999999999999982},{"$f":"+'Analiza i dimenzioniranje'!N98","v":0}]
[8,{"$f":"B4-TAN('Analiza i dimenzioniranje'!H51*PI()/180)*('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},{"$f":"+D4","v":2},{"$f":"+E4","v":1.2},{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"+I4","v":3.44},null,null,null,null,null,"Presjek Xix",{"$f":"+($B$9-$B$4)*(Q9-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AI44","v":5.6800000000000006},null,{"$f":"+($B$11-$B$10)*(T9-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},{"$f":"+U8-'Analiza i dimenzioniranje'!E27","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E24>0,V10,V8+'Analiza i dimenzioniranje'!E27*TAN('Unos podataka'!F8*PI()/180))","v":6.2644906473896782},{"$f":"+'C III-V'!B10+0.5","v":{"$error":"#VALUE!"}},{"$f":"+X8","v":{"$error":"#VALUE!"}},{"$f":"+IF('Analiza i dimenzioniranje'!$E$24=0,0,'C III-V'!Y4)","v":0},{"$f":"+Z8","v":3.14},null,"Slobodna  zona.",null,"Slobodna  zona.",null,"Slobodna  zona.",null,"Slobodna  zona.",null,"Slobodna  zona.",null,null,null,"X=",{"$f":"+(AP8-AP7)/(AN7-AN8)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(BC8-BC7)/(BB8-BB7)","v":{"$error":"#VALUE!"}},"*x             +",{"$f":"-BB9*BB7+BC7","v":{"$error":"#VALUE!"}},null,"Koordinate sjecišta sidra i pravca kliznog tijela u visini sidra",null,"Koordinate sjecišta pravsa sidra i lica zida",null,"Dulijna slobodne dionice",null,"Koordinate kraja slobodne zone"]
[9,{"$f":"+B9+'Analiza i dimenzioniranje'!E54","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},null,null,{"$f":"+B10","v":{"$error":"#VALUE!"}},{"$f":"+C10","v":"A"},null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(Q10-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+Q9","v":5.6800000000000006},"Presjek VIII",{"$f":"+($B$9-$B$4)*(T10-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},-8,{"$f":"+'Unos podataka'!$T$58","v":6.2644906473896782},"Pad terena niz padinu",null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!$K$39=0,0,'Analiza i dimenzioniranje'!P100)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$K$39=0,0,'Analiza i dimenzioniranje'!P22)","v":5},{"$f":"IF('Analiza i dimenzioniranje'!$K$39=0,0,'Analiza i dimenzioniranje'!P105)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$K$39=0,0,'Analiza i dimenzioniranje'!Q22)","v":3},{"$f":"IF('Analiza i dimenzioniranje'!$K$39=0,0,'Analiza i dimenzioniranje'!P110)","v":-20},{"$f":"IF('Analiza i dimenzioniranje'!$K$39=0,0,'Analiza i dimenzioniranje'!R22)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$K$39=0,0,'Analiza i dimenzioniranje'!P115)","v":-20},{"$f":"IF('Analiza i dimenzioniranje'!$K$39=0,0,'Analiza i dimenzioniranje'!S22)","v":0},{"$f":"IF('Analiza i dimenzioniranje'!$K$39=0,0,'Analiza i dimenzioniranje'!P120)","v":-20},{"$f":"IF('Analiza i dimenzioniranje'!$K$39=0,0,'Analiza i dimenzioniranje'!T22)","v":0},null,null,"Y=",{"$f":"+AN7*AO9+AP7","v":{"$error":"#VALUE!"}}]
[10,{"$f":"+B4+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+C3","v":1.2},null,null,{"$f":"+F12+E65","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C11,E20,C11)","v":1.2},null,null,null,null,null,null,null,"Presjek Xx",{"$f":"+($B$9-$B$4)*(Q11-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U44","v":1.2},null,{"$f":"+($B$11-$B$10)*(T11-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},"TLO 1 dno sloja",null,{"$f":"+'Analiza i dimenzioniranje'!Q105","v":3},{"$f":"+'Analiza i dimenzioniranje'!P105","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"AB10-'Analiza i dimenzioniranje'!P23","v":{"$error":"#VALUE!"}},{"$f":"+AC10-(AB10-AB11)*TAN('Analiza i dimenzioniranje'!$E$39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"AD10-'Analiza i dimenzioniranje'!Q23","v":{"$error":"#VALUE!"}},{"$f":"+AE10-(AD10-AD11)*TAN('Analiza i dimenzioniranje'!$E$39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"AF10-'Analiza i dimenzioniranje'!R23","v":-20},{"$f":"+AG10-(AF10-AF11)*TAN('Analiza i dimenzioniranje'!$E$39*PI()/180)","v":0},{"$f":"AH10-'Analiza i dimenzioniranje'!S23","v":-20},{"$f":"+AI10-(AH10-AH11)*TAN('Analiza i dimenzioniranje'!$E$39*PI()/180)","v":0},{"$f":"AJ10-'Analiza i dimenzioniranje'!T23","v":-20},{"$f":"+AK10-(AJ10-AJ11)*TAN('Analiza i dimenzioniranje'!$E$39*PI()/180)","v":0},null,"Jednadžbe",null,null,null,null,"klizno tijelo II Sloj",null,"Jednadžbe",null,null,null,null,"klizno tijelo I Sloj",null,"sjecišta sidara i klizne plohe"]
[11,{"$f":"+B11","v":4.2000010999999997},{"$f":"+C11","v":1.2},"NASIP NA KONZOLI",null,{"$f":"+F4","v":3.4000010999999999},{"$f":"+G4","v":1.2},null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(Q12-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+Q11","v":1.2},"Presjek IX",{"$f":"+($B$9-$B$4)*(T12-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"IF(('Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17)<'Analiza i dimenzioniranje'!$F$45,2,(IF(B7<B24,B7,IF('Analiza i dimenzioniranje'!G78=0,'C III-V'!B24,2))))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17","v":4},{"$f":"+'Analiza i dimenzioniranje'!O130","v":7.1000021999999996},{"$f":"+'Analiza i dimenzioniranje'!N130","v":1.5001009999999999},null,null,{"$f":"3.99/2.65","v":1.5056603773584907},"Sidrena dionica",null,"Sidrena dionica",null,"Sidrena dionica",null,"Sidrena dionica",null,"Sidrena dionica",null,null,"Sidro 1",{"$f":"+AU12","v":"Y="},{"$f":"+AV12","v":{"$error":"#VALUE!"}},{"$f":"+AW12","v":"*x             +"},{"$f":"+AX12","v":{"$error":"#VALUE!"}},{"$f":"+AE103","v":-1.0572404418349119},{"$f":"+AF103","v":4},"Sidro 1","Y=",{"$f":"+AB17","v":{"$error":"#VALUE!"}},{"$f":"+AC17","v":"*x             +"},{"$f":"+AD17","v":{"$error":"#VALUE!"}},{"$f":"+AE102","v":0.97707863658009864},{"$f":"+AF102","v":1.2},{"$f":"+BA9","v":"Y="},{"$f":"+BB9","v":{"$error":"#VALUE!"}},{"$f":"+BC9","v":"*x             +"},{"$f":"+BD9","v":{"$error":"#VALUE!"}},null,null,null,null,null,"x1-x=",{"$f":"+BI14-BG14","v":{"$error":"#VALUE!"}},"X=",{"$f":"+BK12*BK12/BK14","v":{"$error":"#VALUE!"}}]
[12,{"$f":"+B12","v":4.2000010999999997},{"$f":"+C12","v":1.2},"za stabilnost",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T13-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},-8,{"$f":"+V12+(U12-U13)*TAN('Analiza i dimenzioniranje'!$E$18*PI()/180)","v":{"$error":"#VALUE!"}},"Prometno opterećenje",null,null,null,null,{"$f":"+AB11","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},-20,0,-20,0,-20,0,null,"kliz tijelo I sloj","Y=",{"$f":"+(AS13-AS12)/(AR13-AR12)","v":{"$error":"#VALUE!"}},"*x             +",{"$f":"-AO13*AR12+AS12","v":{"$error":"#VALUE!"}},{"$f":"+AE104","v":{"$error":"#VALUE!"}},{"$f":"+AF104","v":{"$error":"#VALUE!"}},"kliz tijelo II sloj","Y=",{"$f":"+(AZ13-AZ12)/(AY13-AY12)","v":-1.3763819204711734},"*x             +",{"$f":"-AV13*AY12+AZ12","v":2.5448333702674715},{"$f":"+AE103","v":-1.0572404418349119},{"$f":"+AF103","v":4},{"$f":"+AU12","v":"Y="},{"$f":"+AV12","v":{"$error":"#VALUE!"}},{"$f":"+AW12","v":"*x             +"},{"$f":"+AX12","v":{"$error":"#VALUE!"}},null,null,null,null,null,"y1-y=",{"$f":"+BI15-BG15","v":{"$error":"#VALUE!"}},"y=",{"$f":"+BK13*BK13/BK14","v":{"$error":"#VALUE!"}}]
[13,{"$f":"+B11+'Analiza i dimenzioniranje'!G57","v":4.9000021999999994},{"$f":"+C13","v":1.2},{"$f":"+B7","v":{"$error":"#VALUE!"}},3.44,null,null,null,null,"Linija presjeka",null,null," Koordinata sredine presjeka",null,null,null,null,"Presjek X",{"$f":"+($B$9-$B$4)*(T14-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},null,null,{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,+'C III-V'!B9-'Analiza i dimenzioniranje'!E26)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,'C III-V'!V9)","v":6.2644906473896782},null,"centralna točka sidr zone",null,{"$f":"+(AB15+AB13)/2","v":{"$error":"#VALUE!"}},{"$f":"+(AC13+AC15)/2","v":{"$error":"#VALUE!"}},{"$f":"+(AD15+AD13)/2","v":{"$error":"#VALUE!"}},{"$f":"+(AE13+AE15)/2","v":{"$error":"#VALUE!"}},{"$f":"+(AF15+AF13)/2","v":-20},{"$f":"+(AG13+AG15)/2","v":-1},{"$f":"+(AH15+AH13)/2","v":-20},{"$f":"+(AI13+AI15)/2","v":-1},{"$f":"+(AJ15+AJ13)/2","v":-25.75},{"$f":"+(AK13+AK15)/2","v":-1.5407078564789556},null,"sjecište","X=",{"$f":"+(AQ13-AQ12)/(AO12-AO13)","v":{"$error":"#VALUE!"}},null,null,null,null,"sjecište","X=",{"$f":"+(AX13-AX12)/(AV12-AV13)","v":{"$error":"#VALUE!"}},null,null,null,null,"X=",{"$f":"+(BD13-BD12)/(BB12-BB13)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!P100","v":{"$error":"#VALUE!"}},"d=",{"$f":"IF(BC14=-20,\"\",SQRT((BB14-BC14)*(BB14-BC14)+(BB15-BC15)*(BB15-BC15)))","v":{"$error":"#VALUE!"}},"X=",{"$f":"+IF(BG15=AO15,AO14,AV14)","v":{"$error":"#VALUE!"}},"X1=",{"$f":"+Z35","v":{"$error":"#VALUE!"}},"ls1=",{"$f":"+SQRT(BK12*BK12+BK13*BK13)","v":{"$error":"#VALUE!"}}]
[14,{"$f":"+B14","v":4.9000021999999994},{"$f":"+C14-'Analiza i dimenzioniranje'!E51","v":0.5},{"$error":"#VALUE!"},3.44,{"$f":"IF((B4-B9)=0,0,+(C9-C4)/(B4-B9))","v":{"$error":"#VALUE!"}},"n  Nagib zida u tlu",null,null,0,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,"III-III","konzola","Presjek v","Presjek Iv",null,{"$f":"+($B$11-$B$10)*(T15-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},null,null,{"$f":"+W14","v":{"$error":"#VALUE!"}},{"$f":"+X14+'Analiza i dimenzioniranje'!E24/50","v":6.4644906473896784},null,"Koord. Sidra na kraju sidr zone",null,{"$f":"+AB13-'Analiza i dimenzioniranje'!P24","v":{"$error":"#VALUE!"}},{"$f":"IF(AC13-(AB13-AB15)*TAN('Analiza i dimenzioniranje'!$E$39*PI()/180)=0,-2,AC13-(AB13-AB15)*TAN('Analiza i dimenzioniranje'!$E$39*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"+AD13-'Analiza i dimenzioniranje'!Q24","v":{"$error":"#VALUE!"}},{"$f":"IF(AE13-(AD13-AD15)*TAN('Analiza i dimenzioniranje'!$E$39*PI()/180)=0,-2,AE13-(AD13-AD15)*TAN('Analiza i dimenzioniranje'!$E$39*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!P112","v":-20},{"$f":"IF(AG13-(AF13-AF15)*TAN('Analiza i dimenzioniranje'!$E$39*PI()/180)=0,-2,AG13-(AF13-AF15)*TAN('Analiza i dimenzioniranje'!$E$39*PI()/180))","v":-2},{"$f":"+AH13-'Analiza i dimenzioniranje'!S24","v":-20},{"$f":"IF(AI13-(AH13-AH15)*TAN('Analiza i dimenzioniranje'!$E$39*PI()/180)=0,-2,AI13-(AH13-AH15)*TAN('Analiza i dimenzioniranje'!$E$39*PI()/180))","v":-2},{"$f":"+AJ13-'Analiza i dimenzioniranje'!T24","v":-31.5},{"$f":"IF(AK13-(AJ13-AJ15)*TAN('Analiza i dimenzioniranje'!$E$39*PI()/180)=0,-2,AK13-(AJ13-AJ15)*TAN('Analiza i dimenzioniranje'!$E$39*PI()/180))","v":-3.0814157129579112},null,null,"Y=",{"$f":"+AO12*AO14+AQ12","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Y=",{"$f":"+AV12*AV14+AX12","v":{"$error":"#VALUE!"}},null,null,null,null,"Y=",{"$f":"+BB12*BB14+BD12","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Q100","v":5},null,null,"Y=",{"$f":"+IF(AV15<AZ13,AV15,AO15)","v":{"$error":"#VALUE!"}},"Y1=",{"$f":"+Z34","v":5}]
[15,{"$f":"+B2","v":2},{"$f":"+C2","v":0.12820515121628623},{"$error":"#VALUE!"},"A",null,"Nema prometa",null,null,3,{"$f":"+K15","v":1.2},null,"x",{"$f":"+(F12+F11)/2","v":{"$error":"#VALUE!"}},{"$f":"(B8+(B11-B10)*(O17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U29+(B11-B10)*(P17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U34+(B11-B10)*(Q17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},"Presjek XI",{"$f":"+($B$9-$B$4)*(T16-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},null,null,{"$f":"IF('Unos podataka'!$H$15=0,0,W14-'Analiza i dimenzioniranje'!E25)","v":{"$error":"#VALUE!"}},{"$f":"+X15","v":6.4644906473896784},null,"Koord. Sidra na zidu ",null,{"$f":"+AB10","v":{"$error":"#VALUE!"}},{"$f":"IF(AC10=0,-2,AC10)","v":5},{"$f":"+AD10","v":{"$error":"#VALUE!"}},{"$f":"IF(AE10=0,-2,AE10)","v":3},{"$f":"+'Analiza i dimenzioniranje'!P110","v":-20},{"$f":"IF(AG10=0,-2,AG10)","v":-2},{"$f":"+AH10","v":-20},{"$f":"IF(AI10=0,-2,AI10)","v":-2},{"$f":"+AJ10","v":-20},{"$f":"IF(AK10=0,-2,AK10)","v":-2}]
[null,null,"Jednadžba pravca zida uz tlo",{"$f":"+D16","v":{"$error":"#VALUE!"}},{"$f":"+C10","v":"A"},null,"Y=",{"$f":"+I7+('Unos podataka'!$V$69-H7)*'Unos podataka'!$R$57","v":{"$error":"#VALUE!"}},null,"Sloj 2 gore",null,null,"y",{"$f":"+G11","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+'Analiza i dimenzioniranje'!R44","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AN44","v":{"$error":"#VALUE!"}},null,{"$f":"+($B$11-$B$10)*(T17-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},null,null,{"$f":"+W16","v":{"$error":"#VALUE!"}},{"$f":"+X14","v":6.2644906473896782},"Jednadžbe sidara I, III i V",null,"Y=",{"$f":"+(AC16-AC15)/(AB16-AB15)","v":{"$error":"#VALUE!"}},"*x             +",{"$f":"-AB17*AB16+AC16","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+(AG16-AG15)/(AF16-AF15)","v":{"$error":"#DIV/0!"}},"*x             +",{"$f":"-AF17*AF15+AG15","v":{"$error":"#DIV/0!"}},"Y=",{"$f":"+(AK16-AK15)/(AJ16-AJ15)","v":9.4036148952861845E-2},"*x             +",{"$f":"-AJ17*AJ15+AK15","v":-0.11927702094276293},null,null,null,null,null,{"$f":"+AR11","v":"klizno tijelo II Sloj"},null,null,null,null,null,null,"klizno tijelo I Sloj"]
[null,"x","y",{"$f":"+D4","v":2},{"$f":"+E4","v":1.2},null,null,null,null,{"$f":"+'Unos podataka'!B107","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!C107","v":4},null,null,null,null,null,null,"Presjek XII",{"$f":"+($B$9-$B$4)*(T18-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},null,null,null,null,"Jedn. Klizn plohe ",null,"Y=",{"$f":"+(AO6-AK2)/(AN6-AN5)","v":-1.3083694515041995},"*x             +",{"$f":"-AN7*AN5+AO5","v":2.616738903008399},"Y=",{"$f":"+($AK$3-$AK$2)/($AJ$3-$AJ$2)","v":-1.4281480067421144},"*x             +",{"$f":"-$AM$3*$AJ$2+$AK$2","v":2.8562960134842288},"Y=",{"$f":"+($AK$3-$AK$2)/($AJ$3-$AJ$2)","v":-1.4281480067421144},"*x             +",{"$f":"-$AM$3*$AJ$2+$AK$2","v":2.8562960134842288},"Sidro 2",{"$f":"+AU18","v":"Y="},{"$f":"+AV18","v":{"$error":"#VALUE!"}},{"$f":"+AW18","v":"*x             +"},{"$f":"+AX18","v":{"$error":"#VALUE!"}},{"$f":"+AR12","v":-1.0572404418349119},{"$f":"+AS12","v":4},"Sidro 2","Y=",{"$f":"+AD19","v":{"$error":"#VALUE!"}},{"$f":"+AE19","v":"*x             +"},{"$f":"+AF19","v":{"$error":"#VALUE!"}},{"$f":"+AY12","v":0.97707863658009864},1.2,"Y=",{"$error":"#VALUE!"},"*x             +",{"$error":"#VALUE!"},null,null,null,null,null,"x1-x=",{"$f":"+BI20-BG20","v":{"$error":"#VALUE!"}},"X=",{"$f":"+BK18*BK18/BK20","v":{"$error":"#VALUE!"}}]
[null,2,{"$f":"+B19*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+'Unos podataka'!B108","v":-8},{"$f":"+'Unos podataka'!C108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T19-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},null,null,null,null,"Jednadžbe sidara Ii i IV",null,null,null,"Y=",{"$f":"+(AE16-AE15)/(AD16-AD15)","v":{"$error":"#VALUE!"}},"*x             +",{"$f":"-AD19*AD16+AE16","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+(AI16-AI15)/(AH16-AH15)","v":{"$error":"#DIV/0!"}},"*x             +",{"$f":"-AH19*AH16+AI16","v":{"$error":"#DIV/0!"}},null,null,{"$f":"+AM13","v":"kliz tijelo I sloj"},"Y=",{"$f":"+(AS19-AS18)/(AR19-AR18)","v":{"$error":"#VALUE!"}},"*x             +",{"$f":"-AO19*AR18+AS18","v":{"$error":"#VALUE!"}},{"$f":"+AR13","v":{"$error":"#VALUE!"}},{"$f":"+AS13","v":{"$error":"#VALUE!"}},{"$f":"+AT13","v":"kliz tijelo II sloj"},"Y=",-1.3763819204711734,"*x             +",2.5448333702674715,-1.0572404418349119,4,{"$f":"+AU18","v":"Y="},{"$f":"+AV18","v":{"$error":"#VALUE!"}},{"$f":"+AW18","v":"*x             +"},{"$f":"+AX18","v":{"$error":"#VALUE!"}},null,null,null,null,null,"y1-y=",{"$f":"+BI21-BG21","v":{"$error":"#VALUE!"}},"y=",{"$f":"+BK19*BK19/BK20","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+H8","v":{"$error":"#VALUE!"}},{"$f":"+B20*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},"M na koti",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,"Sloj 1 ili2 dole",null,null,null,null,null,null,{"$f":"+(B11-B10)*(Q21-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},"Presjek XIII",{"$f":"+($B$9-$B$4)*(T20-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},"KONTAKTNI NAPONI",null,null,null,"Jedn. Klizn plohe ",null,null,null,"Y=",{"$f":"+AB18","v":-1.3083694515041995},"*x             +",{"$f":"+AD18","v":2.616738903008399},"Y=",{"$f":"+($AK$3-$AK$2)/($AJ$3-$AJ$2)","v":-1.4281480067421144},"*x             +",{"$f":"-$AM$3*$AJ$2+$AK$2","v":2.8562960134842288},null,null,"sjecište","X=",{"$f":"+(AQ19-AQ18)/(AO18-AO19)","v":{"$error":"#VALUE!"}},null,null,null,null,"sjecište","X=",{"$f":"+(AX19-AX18)/(AV18-AV19)","v":{"$error":"#VALUE!"}},null,null,null,null,"X=",{"$f":"+(BD19-BD18)/(BB18-BB19)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!P105","v":{"$error":"#VALUE!"}},"d=",{"$f":"IF(BC20=-20,\"\",SQRT((BB20-BC20)*(BB20-BC20)+(BB21-BC21)*(BB21-BC21)))","v":{"$error":"#VALUE!"}},"X=",{"$f":"+IF(BG21=AO21,AO20,AV20)","v":{"$error":"#VALUE!"}},"X2=",{"$f":"+Z33","v":{"$error":"#VALUE!"}},"ls1=",{"$f":"+SQRT(BK18*BK18+BK19*BK19)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C21-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,{"$f":"+IF('Analiza i dimenzioniranje'!G78=0,D8,H8)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+F95","v":0},{"$f":"+G12","v":1.2},null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,{"$f":"+($B$11-$B$10)*(T21-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},{"$f":"+B2-Kontrafore!E3","v":1},0,"x","y","Visina nadsloja iznad središta sidrene zone do vrha tla (za sg)",null,null,null,{"$f":"+AC7-AC14","v":{"$error":"#VALUE!"}},null,{"$f":"+AE7-AE14","v":{"$error":"#VALUE!"}},null,{"$f":"+AG7-AG14","v":{"$error":"#VALUE!"}},null,{"$f":"+AI7-AI14","v":{"$error":"#VALUE!"}},null,{"$f":"+AK7-AK14","v":{"$error":"#VALUE!"}},null,null,"Y=",{"$f":"+AO18*AO20+AQ18","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Y=",{"$f":"+AV18*AV20+AX18","v":{"$error":"#VALUE!"}},null,null,null,null,"Y=",{"$f":"+BB18*BB20+BD18","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Q105","v":3},null,null,"Y=",{"$f":"+IF(AV21<AZ19,AV21,AO21)","v":{"$error":"#VALUE!"}},"Y2=",{"$f":"+Z32","v":3}]
[null,{"$f":"+(B9-B4)*(C22-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+C23+'Analiza i dimenzioniranje'!C77","v":3.44},null,null,null,null,null,null,{"$f":"+'Unos podataka'!B110","v":-8},{"$f":"+K21","v":1.2},null,null,null,null,null,null,"Presjek XIV",{"$f":"+($B$9-$B$4)*(T22-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"+U21","v":1},{"$f":"IF(Kontrafore!E1=\"DA\",-'Analiza i dimenzioniranje'!$F$194/100,-'Analiza i dimenzioniranje'!$F$193/100)","v":{"$error":"#VALUE!"}},"Točkasto",null,null,null,null,"Koordinate sjecišta pravca sidra i klizne plohe u trećem sloju"]
[null,{"$f":"+(B9-B4)*(C23-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T23-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"+B15","v":4.9000021999999994},{"$f":"-'Analiza i dimenzioniranje'!$F$190/100","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E36=0,-5,B9-'Analiza i dimenzioniranje'!E37)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Unos podataka'!C105-'Unos podataka'!C106,'C III-V'!X24,'C III-V'!X25)","v":{"$error":"#VALUE!"}},"sjecište slojeva II i III",null,null,"X=",{"$f":"+(AD18-AD17)/(AB17-AB18)","v":{"$error":"#VALUE!"}},"X=",{"$f":"+(AF20-AF19)/(AD19-AD20)","v":{"$error":"#VALUE!"}},"X=",{"$f":"+(AH18-AH17)/(AF17-AF18)","v":{"$error":"#DIV/0!"}},"X=",{"$f":"+(AJ20-AJ19)/(AH19-AH20)","v":{"$error":"#DIV/0!"}},"X=",{"$f":"+(AL18-AL17)/(AJ17-AJ18)","v":1.9548048922296453},null,null,null,null,null,null,{"$f":"+AR17","v":"klizno tijelo II Sloj"},null,null,null,null,null,null,{"$f":"+AY17","v":"klizno tijelo I Sloj"}]
[null,{"$f":"+(B9-B4)*(C24-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V12","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek XV",{"$f":"+($B$9-$B$4)*(T24-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U23","v":4.9000021999999994},0,null,{"$f":"+C9+('Analiza i dimenzioniranje'!$E$37*TAN('Analiza i dimenzioniranje'!$H$20*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"+AE103","v":-1.0572404418349119},{"$f":"+AF103","v":4},null,"Y=",{"$f":"+AB17*AC23+AD17","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AD19*AE23+AF19","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AF17*AG23+AH17","v":{"$error":"#DIV/0!"}},"Y=",{"$f":"+AH19*AI23+AJ19","v":{"$error":"#DIV/0!"}},"Y=",{"$f":"+AJ17*AK23+AL17","v":6.454530307672704E-2},null,"Sidro 3",{"$f":"+AU24","v":"Y="},{"$f":"+AV24","v":{"$error":"#DIV/0!"}},{"$f":"+AW24","v":"*x             +"},{"$f":"+AX24","v":{"$error":"#DIV/0!"}},{"$f":"+AR18","v":-1.0572404418349119},{"$f":"+AS18","v":4},"Sidro 3","Y=",{"$f":"+AF17","v":{"$error":"#DIV/0!"}},{"$f":"+AG17","v":"*x             +"},{"$f":"+AH17","v":{"$error":"#DIV/0!"}},{"$f":"+AY18","v":0.97707863658009864},{"$f":"+AZ18","v":1.2},{"$f":"+BA9","v":"Y="},{"$f":"+BB9","v":{"$error":"#VALUE!"}},{"$f":"+BC9","v":"*x             +"},{"$f":"+BD9","v":{"$error":"#VALUE!"}},null,null,null,null,null,"x1-x=",{"$f":"+BI26-BG26","v":{"$error":"#VALUE!"}},"X=",{"$f":"+BK24*BK24/BK26","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C25-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!R44","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U21","v":1},0,null,{"$f":"+IF('Analiza i dimenzioniranje'!$E$37<'Unos podataka'!B105,'C III-V'!X24,'Unos podataka'!C105)","v":{"$error":"#VALUE!"}},null,null,null,"duljina slob",{"$f":"+SQRT((AB16-AC23)*(AB16-AC23)+(AC16-AC24)*(AC16-AC24))","v":{"$error":"#VALUE!"}},null,{"$f":"+SQRT((AD16-AE23)*(AD16-AE23)+(AE16-AE24)*(AE16-AE24))","v":{"$error":"#VALUE!"}},null,{"$f":"+SQRT((AF16-AG23)*(AF16-AG23)+(AG16-AG24)*(AG16-AG24))","v":{"$error":"#DIV/0!"}},null,{"$f":"+SQRT((AH16-AI23)*(AH16-AI23)+(AI16-AI24)*(AI16-AI24))","v":{"$error":"#DIV/0!"}},null,{"$f":"+SQRT((AJ16-AK23)*(AJ16-AK23)+(AK16-AK24)*(AK16-AK24))","v":22.051662185974259},null,{"$f":"+AM19","v":"kliz tijelo I sloj"},"Y=",{"$f":"+(AS25-AS24)/(AR25-AR24)","v":{"$error":"#VALUE!"}},"*x             +",{"$f":"-AO25*AR24+AS24","v":{"$error":"#VALUE!"}},{"$f":"+AR19","v":{"$error":"#VALUE!"}},{"$f":"+AS19","v":{"$error":"#VALUE!"}},{"$f":"+AT19","v":"kliz tijelo II sloj"},{"$f":"+AU19","v":"Y="},{"$f":"+AV19","v":-1.3763819204711734},{"$f":"+AW19","v":"*x             +"},{"$f":"+AX19","v":2.5448333702674715},{"$f":"+AY19","v":-1.0572404418349119},{"$f":"+AZ19","v":4},{"$f":"+AU24","v":"Y="},{"$f":"+AV24","v":{"$error":"#DIV/0!"}},{"$f":"+AW24","v":"*x             +"},{"$f":"+AX24","v":{"$error":"#DIV/0!"}},null,null,null,null,null,"y1-y=",{"$f":"+BI27-BG27","v":{"$error":"#DIV/0!"}},"y=",{"$f":"+BK25*BK25/BK26","v":{"$error":"#DIV/0!"}}]
[null,{"$f":"+(B9-B4)*(C26-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Q44","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid v-v",{"$f":"+'Analiza i dimenzioniranje'!R44","v":{"$error":"#VALUE!"}},"Linijsko iza zida",null,"y=",{"$f":"+'Analiza i dimenzioniranje'!T22","v":0},null,"dionice",null,null,null,null,null,null,null,null,null,null,"sjecište","X=",{"$f":"+(AQ25-AQ24)/(AO24-AO25)","v":{"$error":"#VALUE!"}},null,null,null,null,"sjecište","X=",{"$f":"+(AX25-AX24)/(AV24-AV25)","v":{"$error":"#DIV/0!"}},null,null,null,null,"X=",{"$f":"+(BD25-BD24)/(BB24-BB25)","v":{"$error":"#DIV/0!"}},{"$f":"+'Analiza i dimenzioniranje'!P110","v":-20},"d=",{"$f":"IF(BC26=-20,\"\",SQRT((BB26-BC26)*(BB26-BC26)+(BB27-BC27)*(BB27-BC27)))","v":""},"X=",{"$f":"+IF(BG27=AO27,AO26,AV26)","v":{"$error":"#DIV/0!"}},"X3=",{"$f":"+Z31","v":{"$error":"#VALUE!"}},"ls1=",{"$f":"+SQRT(BK24*BK24+BK25*BK25)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C27-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!R44","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!R44","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$34=0,0,B9-'Analiza i dimenzioniranje'!K28)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Unos podataka'!C105-'Unos podataka'!C106,X29,X30)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z26-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"Jednadžba  lica zida ",null,null,null,"Rez. Sidra na zidu",null,null,null,null,null,null,null,"Y=",{"$f":"+AO24*AO26+AQ24","v":{"$error":"#DIV/0!"}},null,null,null,null,null,"Y=",{"$f":"+AV24*AV26+AX24","v":{"$error":"#DIV/0!"}},null,null,null,null,"Y=",{"$f":"+BB24*BB26+BD24","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Q110","v":0},null,null,"Y=",{"$f":"+IF(AV27<AZ25,AV27,AO27)","v":{"$error":"#DIV/0!"}},"Y3=",{"$f":"+Z30","v":0}]
[null,{"$f":"+(B9-B4)*(C28-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Q44","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V27","v":{"$error":"#VALUE!"}},{"$f":"+W27","v":{"$error":"#VALUE!"}},{"$f":"+X27+0.5","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!S22","v":0},"x=",{"$f":"+($B$11-$B$10)*(AB29-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+($B$11-$B$10)*(AC29-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+($B$11-$B$10)*(AD29-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AE29-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C29-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!C107","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V29-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":{"$error":"#VALUE!"}},null,{"$f":"+C9+('Analiza i dimenzioniranje'!$E$35*TAN('Analiza i dimenzioniranje'!$H$20*PI()/180))","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z28-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!S42","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!T42","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!U42","v":170.21276595744681},{"$f":"+'Analiza i dimenzioniranje'!H76+'Analiza i dimenzioniranje'!E52","v":1.5001009999999999},{"$f":"+($B$11-$B$10)*(AG29-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E40","v":3.9999999960000001},{"$f":"+AF29+0.4","v":{"$error":"#VALUE!"}},{"$f":"+AG29+(AH29-AF29)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"+AR23","v":"klizno tijelo II Sloj"},null,null,null,null,null,null,{"$f":"+AY23","v":"klizno tijelo I Sloj"}]
["Sjecište s dnom temelja",null,null,null,null,null,null,null,null,null,null,"MOMENT NA KOZOLI OD NASIPA",null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V30-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":{"$error":"#VALUE!"}},null,{"$f":"+IF('Analiza i dimenzioniranje'!$E$35<'Unos podataka'!B105,'C III-V'!X29,'Unos podataka'!C105)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!R22","v":0},null,"IV","V","III",{"$f":"+B14-AE28","v":{"$error":"#VALUE!"}},null,null,{"$f":"+AF29-1","v":{"$error":"#VALUE!"}},{"$f":"+AG29-(AF29-AH30)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}},null,null,null,"Sidro 4",{"$f":"+AU30","v":"Y="},{"$f":"+AV30","v":{"$error":"#DIV/0!"}},{"$f":"+AW30","v":"*x             +"},{"$f":"+AX30","v":{"$error":"#DIV/0!"}},{"$f":"+AR24","v":-1.0572404418349119},{"$f":"+AS24","v":4},"Sidro 4",{"$f":"+AG19","v":"Y="},{"$f":"+AH19","v":{"$error":"#DIV/0!"}},{"$f":"+AI19","v":"*x             +"},{"$f":"+AJ19","v":{"$error":"#DIV/0!"}},{"$f":"+AY24","v":0.97707863658009864},{"$f":"+AZ24","v":1.2},{"$f":"+BA9","v":"Y="},{"$f":"+BB9","v":{"$error":"#VALUE!"}},{"$f":"+BC9","v":"*x             +"},{"$f":"+BD9","v":{"$error":"#VALUE!"}},null,null,null,null,null,"x1-x=",{"$f":"+BI32-BG32","v":{"$error":"#VALUE!"}},"X=",{"$f":"+BK30*BK30/BK32","v":{"$error":"#VALUE!"}}]
["zid",{"$f":"+B20","v":{"$error":"#VALUE!"}},{"$f":"+B31*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid Iv",{"$f":"+'Analiza i dimenzioniranje'!Q44","v":{"$error":"#VALUE!"}},"TEMELJ -opterećenje",null,"x=",{"$f":"+($B$11-$B$10)*(Z30-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"Koordinate kliznog I sloja",null,"Koordinate kliznog II sloja",null,null,null,null,null,null,null,null,{"$f":"+AM25","v":"kliz tijelo I sloj"},"Y=",{"$f":"+(AS31-AS30)/(AR31-AR30)","v":{"$error":"#VALUE!"}},"*x             +",{"$f":"-AO31*AR30+AS30","v":{"$error":"#VALUE!"}},{"$f":"+AR25","v":{"$error":"#VALUE!"}},{"$f":"+AS25","v":{"$error":"#VALUE!"}},{"$f":"+AT25","v":"kliz tijelo II sloj"},{"$f":"+AU25","v":"Y="},{"$f":"+AV25","v":-1.3763819204711734},{"$f":"+AW25","v":"*x             +"},{"$f":"+AX25","v":2.5448333702674715},{"$f":"+AY25","v":-1.0572404418349119},{"$f":"+AZ25","v":4},{"$f":"+AU30","v":"Y="},{"$f":"+AV30","v":{"$error":"#DIV/0!"}},{"$f":"+AW30","v":"*x             +"},{"$f":"+AX30","v":{"$error":"#DIV/0!"}},null,null,null,null,null,"y1-y=",{"$f":"+BI33-BG33","v":{"$error":"#DIV/0!"}},"y=",{"$f":"+BK31*BK31/BK32","v":{"$error":"#DIV/0!"}}]
["Vrh zida",{"$f":"+(B9-B4)*(C32-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C558","v":-0.45},null,null,null,null,null,null,null,null,{"$f":"-J61*(B8-J59)","v":{"$error":"#VALUE!"}},"kNm/m'",null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!AN44","v":{"$error":"#VALUE!"}},{"$f":"+IF('Analiza i dimenzioniranje'!E28=0,0,W33)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9+'Analiza i dimenzioniranje'!F20+1.5)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q22","v":3},null,null,null,null,null,null,null,null,null,null,null,null,"sjecište","X=",{"$f":"+(AQ31-AQ30)/(AO30-AO31)","v":{"$error":"#VALUE!"}},null,null,null,null,"sjecište","X=",{"$f":"+(AX31-AX30)/(AV30-AV31)","v":{"$error":"#DIV/0!"}},null,null,null,null,"X=",{"$f":"+(BD31-BD30)/(BB30-BB31)","v":{"$error":"#DIV/0!"}},{"$f":"+'Analiza i dimenzioniranje'!P115","v":-20},"d=",{"$f":"IF(BC32=-20,\"\",SQRT((BB32-BC32)*(BB32-BC32)+(BB33-BC33)*(BB33-BC33)))","v":""},"X=",{"$f":"+IF(BG33=AO33,AO32,AV32)","v":{"$error":"#DIV/0!"}},"X4=",{"$f":"+Z29","v":{"$error":"#VALUE!"}},"ls1=",{"$f":"+SQRT(BK30*BK30+BK31*BK31)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V32","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W34-0.3)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X34)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z32-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+AO30*AO32+AQ30","v":{"$error":"#DIV/0!"}},null,null,null,null,null,"Y=",{"$f":"+AV30*AV32+AX30","v":{"$error":"#DIV/0!"}},null,null,null,null,"Y=",{"$f":"+BB30*BB32+BD30","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Q115","v":0},null,null,"Y=",{"$f":"+IF(AV33<AZ31,AV33,AO33)","v":{"$error":"#DIV/0!"}},"Y4=",{"$f":"+Z28","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V34-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V33","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,B9-'Analiza i dimenzioniranje'!$E$32)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X35+'Analiza i dimenzioniranje'!E33)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q20","v":5},null,"nagib lica zida","tan",{"$f":"+(B13-B10)/(C10-C13)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V35-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V34","v":{"$error":"#VALUE!"}},{"$f":"+W34","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9-'Analiza i dimenzioniranje'!K31)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z34-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"kut",{"$f":"+ATAN(AD34)*180/PI()","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AR29","v":"klizno tijelo II Sloj"},null,null,null,null,null,null,{"$f":"+AY29","v":"klizno tijelo I Sloj"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SIDRO za presjek",null,{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,W35-'Analiza i dimenzioniranje'!$E$29)","v":{"$error":"#VALUE!"}},{"$f":"+X35","v":{"$error":"#VALUE!"}},"Jednadžba pravca lica zida",null,null,"Sjecište a arm konzole",null,"vrh zida","Anker armatura uz lice",null,"arm dno",null,"Y=",{"$f":"IF(AE38=AE37,1000000,(AF38-AF37)/(AE38-AE37))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AJ36*AE37+AF37","v":{"$error":"#VALUE!"}},"Sidro 5",{"$f":"+AU36","v":"Y="},{"$f":"+AV36","v":9.4036148952861845E-2},{"$f":"+AW36","v":"*x             +"},{"$f":"+AX36","v":-0.11927702094276293},{"$f":"+AR30","v":-1.0572404418349119},{"$f":"+AS30","v":4},"Sidro 5",{"$f":"+AI17","v":"Y="},{"$f":"+AJ17","v":9.4036148952861845E-2},{"$f":"+AK17","v":"*x             +"},{"$f":"+AL17","v":-0.11927702094276293},{"$f":"+AY30","v":0.97707863658009864},{"$f":"+AZ30","v":1.2},{"$f":"+BA9","v":"Y="},{"$f":"+BB9","v":{"$error":"#VALUE!"}},{"$f":"+BC9","v":"*x             +"},{"$f":"+BD9","v":{"$error":"#VALUE!"}},null,null,null,null,null,"x1-x=",{"$f":"+BI38-BG38","v":{"$error":"#VALUE!"}},"X=",{"$f":"+BK36*BK36/BK38","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+H52","v":{"$error":"#VALUE!"}},{"$f":"+B47","v":3.4000010999999999},{"$f":"IF('Analiza i dimenzioniranje'!AN44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!Q44,K47)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB10)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC10)","v":5},{"$f":"+W36","v":{"$error":"#VALUE!"}},{"$f":"+X34","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!O475","v":0},null,{"$f":"+(B11-B10)*(AB38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AC38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AD38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AF37-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!B545","v":{"$error":"#VALUE!"}},{"$f":"+U81","v":2.0499999999999998},{"$f":"+V81","v":0.18682583433163008},"X=",{"$f":"+(-AL36+AL39)/(AJ36-AJ39)","v":{"$error":"#VALUE!"}},"sjeište",null,{"$f":"+AM31","v":"kliz tijelo I sloj"},"Y=",{"$f":"+(AS37-AS36)/(AR37-AR36)","v":{"$error":"#VALUE!"}},"*x             +",{"$f":"-AO37*AR36+AS36","v":{"$error":"#VALUE!"}},{"$f":"+AR31","v":{"$error":"#VALUE!"}},{"$f":"+AS31","v":{"$error":"#VALUE!"}},{"$f":"+AT31","v":"kliz tijelo II sloj"},{"$f":"+AU31","v":"Y="},{"$f":"+AV31","v":-1.3763819204711734},{"$f":"+AW31","v":"*x             +"},{"$f":"+AX31","v":2.5448333702674715},{"$f":"+AY31","v":-1.0572404418349119},{"$f":"+AZ31","v":4},{"$f":"+AU36","v":"Y="},{"$f":"+AV36","v":9.4036148952861845E-2},{"$f":"+AW36","v":"*x             +"},{"$f":"+AX36","v":-0.11927702094276293},null,null,null,null,null,"y1-y=",{"$f":"+BI39-BG39","v":-5.1098117110894653E-2},"y=",{"$f":"+BK37*BK37/BK38","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+I52","v":"A"},{"$f":"+C47","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!AN44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!Q44,K48)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB11)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC11)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W37+0.3)","v":{"$error":"#VALUE!"}},{"$f":"+X33","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z37-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+'Analiza i dimenzioniranje'!E555","v":3.39},{"$f":"+AB38-'Analiza i dimenzioniranje'!#REF!","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!C558","v":-0.45},{"$f":"+(B11-B10)*(AF38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+U82","v":4.8600021999999994},{"$f":"+V82","v":0.54310345350772504},"Y=",{"$f":"+AJ36*AJ37+AL36","v":{"$error":"#VALUE!"}},null,null,"sjecište","X=",{"$f":"+(AQ37-AQ36)/(AO36-AO37)","v":{"$error":"#VALUE!"}},null,null,null,null,"sjecište","X=",{"$f":"+(AX37-AX36)/(AV36-AV37)","v":1.8118047150044683},null,null,null,null,"X=",{"$f":"+(BD37-BD36)/(BB36-BB37)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!P120","v":-20},"d=",{"$f":"IF(BC38=-20,\"\",SQRT((BB38-BC38)*(BB38-BC38)+(BB39-BC39)*(BB39-BC39)))","v":""},"X=",{"$f":"+IF(BG39=AO39,AO38,AV38)","v":{"$error":"#VALUE!"}},"X5=",{"$f":"+Z27","v":{"$error":"#VALUE!"}},"ls1=",{"$f":"+SQRT(BK36*BK36+BK37*BK37)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"(M38-L38)/(M37-L37)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-L39*L37+L38","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"+W38","v":{"$error":"#VALUE!"}},{"$f":"+X32","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!S593-0.2","v":1.2923077248520527},null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AH38-AH37)/(AG38-AG37)","v":0.12678908905341604},"*x",{"$f":"-AJ39*AG37+AH37","v":-7.3091798227872762E-2},null,"Y=",{"$f":"+AO36*AO38+AQ36","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Y=",{"$f":"+AV36*AV38+AX36","v":5.1098117110894653E-2},null,null,null,null,"Y=",{"$f":"+BB36*BB38+BD36","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Q120","v":0},null,null,"Y=",{"$f":"+IF(AV39<AZ37,AV39,AO39)","v":5.1098117110894653E-2},"Y5=",{"$f":"+Z26","v":0}]
[null,null,null,null,null,null,null,null,null,null,"iz jedn Y=   X=",{"$f":"-($N$39-N40)/$L$39","v":{"$error":"#VALUE!"}},"za",{"$f":"+K50","v":6},null,null,null,null,null,null,null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!O474","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z39-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},"koord Pr II",null,null,null,"SIDRO",null,null,null,null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!$C$545","v":1.6923077248520526}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!AN44>'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C III-V'!B28,B8)","v":{"$error":"#VALUE!"}},{"$f":"-($N$39-N41)/$L$39","v":{"$error":"#VALUE!"}},"za",{"$f":"+K51","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+P58-L58","v":{"$error":"#VALUE!"}},null,null,null,null,"x=",{"$f":"+($B$11-$B$10)*(X40-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"lice",{"$f":"+B8","v":{"$error":"#VALUE!"}},"Koordinate dna temelja",null,null,{"$f":"+AB10","v":{"$error":"#VALUE!"}},{"$f":"+AC10","v":5},null,null,null,null,"x=",{"$f":"+(AL40-AL36)/AJ36","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+K37","v":"X="},{"$f":"+L38","v":"A"},null,null,null,null,null,{"$f":"+P59-L59","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,"x=",{"$f":"+(B11-B10)*(Z43-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+Z43","v":3.44},{"$f":"+B2-Kontrafore!E3","v":1},0,null,{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,AB10-0.5)","v":{"$error":"#VALUE!"}},{"$f":"+AF41-(AE41-AE42)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},null,"Nasip ispred zida"]
["Oznaka","temelj",null,"Zid i konzola za pr. ZID",null,"Nasip na temelju iza zida",null,"      Za momente u presjeku zid-temelj          ",null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},null,{"$f":"2+'Analiza i dimenzioniranje'!E61/2","v":3.4500010999999997},{"$f":"+(AC46+AC49)/2","v":0.35897429750167836},null,null,null,null,{"$f":"+AE28","v":{"$error":"#VALUE!"}},{"$f":"+C11+'Analiza i dimenzioniranje'!$H$76","v":1.5001009999999999}]
["točke","x","y","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - BETON",null,null,null,null,null,{"$f":"+V77","v":{"$error":"#VALUE!"}},{"$f":"(AB44*(AC53-AC42)/(AB53-AB42)-AB42*(AC53-AC42)/(AB53-AB42)+AC42)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!$E$61+0.5","v":5.4000021999999994},{"$f":"+AI43","v":1.5001009999999999}]
[1,{"$f":"+'C III-V'!B2","v":2},{"$f":"+'C III-V'!C2","v":0.12820515121628623},null,null,null,null,"ZID I KONZOLA",null,"Nasip na konzoli",null,null,null,null,null,null,null,null,null,"Kontaktni naponi za stab",null,"Beton do presjeka II-II",null,"Beton sredine temelja",null,"Beton do presjeka I-I",null,{"$f":"+(AB42+AB46)/2","v":2.2000005499999999},{"$f":"(AB45*(AC53-AC42)/(AB53-AB42)-AB42*(AC53-AC42)/(AB53-AB42)+AC42)","v":0.1538461375739737},null,null,null,null,{"$f":"+AH44+1.6","v":7.0000021999999991},{"$f":"+AI44-(AH45-AH44)*TAN('Analiza i dimenzioniranje'!H22*PI()/180)","v":1.5001009999999999}]
[2,{"$f":"+'C III-V'!B3","v":2},{"$f":"+'C III-V'!C3","v":1.2},null,null,{"$f":"IF('Analiza i dimenzioniranje'!E$75=\"\",0,D4)","v":2},{"$f":"+E4","v":1.2},"x","y","x","y",null,null,null,null,null,null,null,null,"x","y",null,null,"x","y","x","y",{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"(AB46*(AC53-AC42)/(AB53-AB42)-AB42*(AC53-AC42)/(AB53-AB42)+AC42)","v":0.30769227514794739},null,null,null,null,"x","y"]
[3,{"$f":"+'C III-V'!B4","v":3.4000010999999999},{"$f":"+'C III-V'!C4","v":1.2},{"$f":"+B4","v":3.4000010999999999},1.2,{"$f":"IF('Analiza i dimenzioniranje'!E$75=\"\",0,D5)","v":2},{"$error":"#VALUE!"},{"$f":"+F4","v":3.4000010999999999},{"$f":"+G4","v":1.2},{"$f":"+'C VI-VII'!N47","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!O47","v":3.44},null,null,null,null,null,null,null,null,{"$f":"+U21","v":1},{"$f":"+V21*100","v":0},{"$f":"+B2-Kontrafore!E3","v":1},0,{"$f":"+B4","v":3.4000010999999999},{"$f":"+W49","v":1.2},{"$f":"+B11","v":4.2000010999999997},1.2,{"$f":"+AB46+'Analiza i dimenzioniranje'!Q58","v":3.4500010999999997},{"$f":"(AB47*(AC53-AC42)/(AB53-AB42)-AB42*(AC53-AC42)/(AB53-AB42)+AC42)","v":0.31410252794216376},"Presjek II-II",null,null,null,{"$f":"+'C III-V'!B11","v":4.2000010999999997},{"$f":"+C11","v":1.2}]
[4,{"$f":"+B11","v":4.2000010999999997},1.2,{"$error":"#VALUE!"},3.14,{"$f":"IF('Analiza i dimenzioniranje'!E$75=\"\",0,D6)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.14,{"$f":"+'C VI-VII'!N48","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!O48","v":3.44},null,null,null,null,null,null,null,null,{"$f":"+U22","v":1},{"$f":"+V22*100","v":{"$error":"#VALUE!"}},{"$f":"+V47-'Unos podataka'!$G$49","v":1},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+X47+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+Y47","v":1.2},4.2000010999999997,1.2,{"$f":"+X77","v":{"$error":"#VALUE!"}},{"$f":"(AB48*(AC53-AC42)/(AB53-AB42)-AB42*(AC53-AC42)/(AB53-AB42)+AC42)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47+'Analiza i dimenzioniranje'!H76","v":1.5001009999999999}]
[5,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.14,{"$f":"IF('Analiza i dimenzioniranje'!E$75=\"\",0,D7)","v":3.4000010999999999},1.2,{"$error":"#VALUE!"},3.14,{"$f":"+J50","v":{"$error":"#VALUE!"}},{"$f":"+K50","v":6},null,null,null,null,null,null,null,null,{"$f":"+U23","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},{"$f":"+V48+'Analiza i dimenzioniranje'!F46+Kontrafore!E3","v":3.4000010999999999},{"$f":"+W48","v":1.2},{"$f":"+AB49","v":4.2000010999999997},{"$f":"+AC49","v":0.41025631985540933},4.2000010999999997,1.2,{"$f":"+AB46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+(AB49*(AC42-AC53)/(AB42-AB53)-AB53*(AC42-AC53)/(AB42-AB53)+AC53)","v":0.41025631985540933},"Presjek I-I",null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+AI48","v":1.5001009999999999}]
[6,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.44,{"$f":"IF('Analiza i dimenzioniranje'!E$75=\"\",0,D8)","v":2},1.2,{"$error":"#VALUE!"},3.44,{"$f":"+'Unos podataka'!$S$56","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!$T$56","v":6},null,null,null,null,null,null,null,null,{"$f":"+U24","v":4.9000021999999994},{"$f":"+V24*100","v":0},{"$f":"+V49","v":3.4000010999999999},{"$f":"+AC46","v":0.30769227514794739},{"$f":"+X47","v":3.4000010999999999},{"$f":"+AC46","v":0.30769227514794739},4.9000021999999994,1.2,{"$f":"B2+('Analiza i dimenzioniranje'!E61+Kontrafore!E3)/2-Kontrafore!E3","v":2.9500010999999997},{"$f":"(AB50*(AC53-AC42)/(AB53-AB42)-AB42*(AC53-AC42)/(AB53-AB42)+AC42)","v":0.25},null,null,null,null,{"$f":"+AH49","v":4.9000021999999994},{"$f":"+C14","v":1.2}]
[7,4.9000021999999994,1.2,{"$error":"#VALUE!"},3.44,{"$f":"IF('Analiza i dimenzioniranje'!E$75=\"\",0,D9)","v":2},1.2,{"$error":"#VALUE!"},3.44,{"$f":"+'C VI-VII'!N51","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!O51","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"+U25","v":1},{"$f":"+V25*100","v":0},{"$f":"+V47","v":1},{"$f":"+W47","v":0},{"$f":"+X47","v":3.4000010999999999},{"$f":"+Y47","v":1.2},4.9000021999999994,0.5,{"$f":"+(AB49+AB53)/2","v":4.5500016499999996},{"$f":"(AB51*(AC53-AC42)/(AB53-AB42)-AB42*(AC53-AC42)/(AB53-AB42)+AC42)","v":0.45512815992770467},null,null,null,null,{"$f":"+B13","v":4.2000010999999997},{"$f":"+C13","v":1.2}]
[8,4.9000021999999994,0.5,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",{"$f":"+'C VI-VII'!N52","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!O52","v":3.44},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AC49","v":0.41025631985540933},{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"(AB52*(AC53-AC42)/(AB53-AB42)-AB42*(AC53-AC42)/(AB53-AB42)+AC42)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH51","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[9,2,0.12820515121628623,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AA47","v":1.2},{"$f":"B2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+C15","v":0.5},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[10,null,null,4.2000010999999997,1.2,null,null,{"$error":"#VALUE!"},1.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate s naprezanjem"]
[11,null,null,{"$f":"+D47","v":3.4000010999999999},{"$f":"+E47","v":1.2},null,null,3.4000010999999999,1.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U22","v":1},{"$f":"+V22*100","v":{"$error":"#VALUE!"}}]
[12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+AB56*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
[13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AB57*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
["  A=",{"$f":"-0.5*((B45*C46-B46*C45)+(B46*C47-B47*C46)+(B47*C48-B48*C47)+(B48*C49-B49*C48)+(B49*C50-B50*C49)+(B50*C51-B51*C50)+(B51*C52-B52*C51)+(B52*C53-B53*C52))","v":2.5691044797107181},"m2",{"$f":"-0.5*((D45*E46-D46*E45)+(D46*E47-D47*E46)+(D47*E48-D48*E47)+(D48*E49-D49*E48)+(D49*E50-D50*E49)+(D50*E51-D51*E50)+(D51*E52-D52*E51)+(D52*E53-D53*E52)+(D53*E54-D54*E53)+(D54*E55-D55*E54)+(D55*E56-D56*E55)+(D56*E57-D57*E56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((F45*G46-F46*G45)+(F46*G47-F47*G46)+(F47*G48-F48*G47)+(F48*G49-F49*G48)+(F49*G50-F50*G49)+(F50*G51-F51*G50)+(F51*G52-F52*G51)+(F52*G53-F53*G52)+(F53*G54-F54*G53)+(F54*G55-F55*G54)+(F55*G56-F56*G55)+(F56*G57-F57*G56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((H47*I48-H48*I47)+(H48*I49-H49*I48)+(H49*I50-H50*I49)+(H50*I51-H51*I50)+(H51*I52-H52*I51)+(H52*I53-H53*I52)+(H53*I54-H54*I53)+(H54*I55-H55*I54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((J47*K48-J48*K47)+(J48*K49-J49*K48)+(J49*K50-J50*K49)+(J50*K51-J51*K50)+(J51*K52-J52*K51)+(J52*K53-J53*K52)+(J53*K54-J54*K53)+(J54*K55-J55*K54))","v":{"$error":"#VALUE!"}},"m2","  A=",null,null,null,null,null,null,null,{"$f":"0.5*((T47*U48-T48*U47)+(T48*U49-T49*U48)+(T49*U50-T50*U49)+(T50*U51-T51*U50)+(T51*U52-T52*U51)+(T52*U53-T53*U52)+(T53*U54-T54*U53)+(T54*U55-T55*U54))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((V47*W48-V48*W47)+(V48*W49-V49*W48)+(V49*W50-V50*W49)+(V50*W51-V51*W50))","v":2.5107704205917116},"m2",{"$f":"-0.5*((X47*Y48-X48*Y47)+(X48*Y49-X49*Y48)+(X49*Y50-X50*Y49)+(X50*Y51-X51*Y50))","v":0.67282056199865625},"m2",{"$f":"-0.5*((Z47*AA48-Z48*AA47)+(Z48*AA49-Z49*AA48)+(Z49*AA50-Z50*AA49)+(Z50*AA51-Z51*AA50)+(Z51*AA52-Z52*AA51)+(Z52*AA53-Z53*AA52)+(Z53*AA54-Z54*AA53)+(Z54*AA55-Z55*AA54))","v":0.52141110740963081},"m2",{"$f":"B2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-0.5*((AH47*AI48-AH48*AI47)+(AH48*AI49-AH49*AI48)+(AH49*AI50-AH50*AI49)+(AH50*AI51-AH51*AI50)+(AH51*AI52-AH52*AI51)+(AH52*AI53-AH53*AI52)+(AH53*AI54-AH54*AI53)+(AH54*AI55-AH55*AI54))","v":0.21007103011109951},"m2"]
["xt=",{"$f":"-((B45*C46-B46*C45)*(B45+B46)+(B46*C47-B47*C46)*(B46+B47)+(B47*C48-B48*C47)*(B47+B48)+(B48*C49-B49*C48)*(B48+B49)+(B49*C50-B50*C49)*(B49+B50)+(B50*C51-B51*C50)*(B50+B51)+(B51*C52-B52*C51)*(B51+B52)+(B52*C53-B53*C52)*(B52+B53)+(B53*C54-B54*C53)*(B53+B54)+(B54*C55-B55*C54)*(B54+B55)+(B55*C56-B56*C55)*(B55+B56)+(B56*C57-B57*C56)*(B56+B57))/6/B58","v":3.3485779696489133},"m",{"$f":"-((D45*E46-D46*E45)*(D45+D46)+(D46*E47-D47*E46)*(D46+D47)+(D47*E48-D48*E47)*(D47+D48)+(D48*E49-D49*E48)*(D48+D49)+(D49*E50-D50*E49)*(D49+D50)+(D50*E51-D51*E50)*(D50+D51)+(D51*E52-D52*E51)*(D51+D52)+(D52*E53-D53*E52)*(D52+D53)+(D53*E54-D54*E53)*(D53+D54)+(D54*E55-D55*E54)*(D54+D55)+(D55*E56-D56*E55)*(D55+D56)+(D56*E57-D57*E56)*(D56+D57))/6/D58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(F58=0,0,-((F45*G46-F46*G45)*(F45+F46)+(F46*G47-F47*G46)*(F46+F47)+(F47*G48-F48*G47)*(F47+F48)+(F48*G49-F49*G48)*(F48+F49)+(F49*G50-F50*G49)*(F49+F50)+(F50*G51-F51*G50)*(F50+F51))/6/F58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(H47*I48-H48*I47)*(H47+H48)+(H48*I49-H49*I48)*(H48+H49)+(H49*I50-H50*I49)*(H49+H50)+(H50*I51-H51*I50)*(H50+H51)+(H51*I52-H52*I51)*(H51+H52)+(H52*I53-H53*I52)*(H52+H53)+(H53*I54-H54*I53)*(H53+H54)+(H54*I55-H55*I54)*(H54+H55))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(J47+J48)+(J48*K49-J49*K48)*(J48+J49)+(J49*K50-J50*K49)*(J49+J50)+(J50*K51-J51*K50)*(J50+J51)+(J51*K52-J52*K51)*(J51+J52)+(J52*K53-J53*K52)*(J52+J53)+(J53*K54-J54*K53)*(J53+J54)+(J54*K55-J55*K54)*(J54+J55)+(J55*K56-J56*K55)*(J55+J56)+(J56*K57-J57*K56)*(J56+J57))/6/J58)","v":{"$error":"#VALUE!"}},"m","xt=",null,null,null,null,null,null,null,{"$f":"IF(T58=0,0,(+(T47*U48-T48*U47)*(T47+T48)+(T48*U49-T49*U48)*(T48+T49)+(T49*U50-T50*U49)*(T49+T50)+(T50*U51-T51*U50)*(T50+T51)+(T51*U52-T52*U51)*(T51+T52)+(T52*U53-T53*U52)*(T52+T53)+(T53*U54-T54*U53)*(T53+T54)+(T54*U55-T55*U54)*(T54+T55)+(T55*U56-T56*U55)*(T55+T56)+(T56*U57-T57*U56)*(T56+T57))/6/T58)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(V58=0,0,-(+(V47*W48-V48*W47)*(V47+V48)+(V48*W49-V49*W48)*(V48+V49)+(V49*W50-V50*W49)*(V49+V50)+(V50*W51-V51*W50)*(V50+V51))/6/V58)","v":2.1411770007641286},"m",{"$f":"IF(X58=0,0,-(+(X47*Y48-X48*Y47)*(X47+X48)+(X48*Y49-X49*Y48)*(X48+X49)+(X49*Y50-X50*Y49)*(X49+X50)+(X50*Y51-X51*Y50)*(X50+X51))/6/X58)","v":3.7918710238796351},"m",{"$f":"-(+(Z47*AA48-Z48*AA47)*(Z47+Z48)+(Z48*AA49-Z49*AA48)*(Z48+Z49)+(Z49*AA50-Z50*AA49)*(Z49+Z50)+(Z50*AA51-Z51*AA50)*(Z50+Z51)+(Z51*AA52-Z52*AA51)*(Z51+Z52)+(Z52*AA53-Z53*AA52)*(Z52+Z53)+(Z53*AA54-Z54*AA53)*(Z53+Z54)+(Z54*AA55-Z55*AA54)*(Z54+Z55)+(Z55*AA56-Z56*AA55)*(Z55+Z56)+(Z56*AA57-Z57*AA56)*(Z56+Z57))/6/Z58","v":4.5429735198528984},"m",null,null,null,null,"   Koordinate težišta presjeka",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AH47+AH48)+(AH48*AI49-AH49*AI48)*(AH48+AH49)+(AH49*AI50-AH50*AI49)*(AH49+AH50)+(AH50*AI51-AH51*AI50)*(AH50+AH51)+(AH51*AI52-AH52*AI51)*(AH51+AH52)+(AH52*AI53-AH53*AI52)*(AH52+AH53)+(AH53*AI54-AH54*AI53)*(AH53+AH54)+(AH54*AI55-AH55*AI54)*(AH54+AH55)+(AH55*AI56-AH56*AI55)*(AH55+AH56)+(AH56*AI57-AH57*AI56)*(AH56+AH57))/6/AH58","v":4.550001650000004},"m"]
["yt=",{"$f":"-((B45*C46-B46*C45)*(C45+C46)+(B46*C47-B47*C46)*(C46+C47)+(B47*C48-B48*C47)*(C47+C48)+(B48*C49-B49*C48)*(C48+C49)+(B49*C50-B50*C49)*(C49+C50)+(B50*C51-B51*C50)*(C50+C51)+(B51*C52-B52*C51)*(C51+C52)+(B52*C53-B53*C52)*(C52+C53)+(B53*C54-B54*C53)*(C53+C54)+(B54*C55-B55*C54)*(C54+C55)+(B55*C56-B56*C55)*(C55+C56)+(B56*C57-B57*C56)*(C56+C57))/6/B58","v":0.75054981042380386},"m",{"$f":"-((D45*E46-D46*E45)*(E45+E46)+(D46*E47-D47*E46)*(E46+E47)+(D47*E48-D48*E47)*(E47+E48)+(D48*E49-D49*E48)*(E48+E49)+(D49*E50-D50*E49)*(E49+E50)+(D50*E51-D51*E50)*(E50+E51)+(D51*E52-D52*E51)*(E51+E52)+(D52*E53-D53*E52)*(E52+E53)+(D53*E54-D54*E53)*(E53+E54)+(D54*E55-D55*E54)*(E54+E55)+(D55*E56-D56*E55)*(E55+E56)+(D56*E57-D57*E56)*(E56+E57))/6/D58","v":{"$error":"#VALUE!"}},"m",null,"m",{"$f":"-(+(H47*I48-H48*I47)*(I47+I48)+(H48*I49-H49*I48)*(I48+I49)+(H49*I50-H50*I49)*(I49+I50)+(H50*I51-H51*I50)*(I50+I51)+(H51*I52-H52*I51)*(I51+I52)+(H52*I53-H53*I52)*(I52+I53)+(H53*I54-H54*I53)*(I53+I54)+(H54*I55-H55*I54)*(I54+I55)+(H55*I56-H56*I55)*(I55+I56)+(H56*I57-H57*I56)*(I56+I57))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(K47+K48)+(J48*K49-J49*K48)*(K48+K49)+(J49*K50-J50*K49)*(K49+K50)+(J50*K51-J51*K50)*(K50+K51)+(J51*K52-J52*K51)*(K51+K52)+(J52*K53-J53*K52)*(K52+K53)+(J53*K54-J54*K53)*(K53+K54)+(J54*K55-J55*K54)*(K54+K55)+(J55*K56-J56*K55)*(K55+K56)+(J56*K57-J57*K56)*(K56+K57))/6/J58)","v":{"$error":"#VALUE!"}},"m","yt=",null,null,null,null,null,null,null,{"$f":"-IF(T58=0,0,(+(T47*U48-T48*U47)*(U47+U48)+(T48*U49-T49*U48)*(U48+U49)+(T49*U50-T50*U49)*(U49+U50)+(T50*U51-T51*U50)*(U50+U51)+(T51*U52-T52*U51)*(U51+U52)+(T52*U53-T53*U52)*(U52+U53)+(T53*U54-T54*U53)*(U53+U54)+(T54*U55-T55*U54)*(U54+U55)+(T55*U56-T56*U55)*(U55+U56)+(T56*U57-T57*U56)*(U56+U57))/6/T58)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((V47*W48-V48*W47)*(W47+W48)+(V48*W49-V49*W48)*(W48+W49)+(V49*W50-V50*W49)*(W49+W50)+(V50*W51-V51*W50)*(W50+W51))/6/V58","v":0.67315233057843704},"kN",{"$f":"-((X47*Y48-X48*Y47)*(Y47+Y48)+(X48*Y49-X49*Y48)*(Y48+Y49)+(X49*Y50-X50*Y49)*(Y49+Y50)+(X50*Y51-X51*Y50)*(Y50+Y51))/6/X58","v":0.77896599031916203},"kN",{"$f":"-(+(Z47*AA48-Z48*AA47)*(AA47+AA48)+(Z48*AA49-Z49*AA48)*(AA48+AA49)+(Z49*AA50-Z50*AA49)*(AA49+AA50)+(Z50*AA51-Z51*AA50)*(AA50+AA51)+(Z51*AA52-Z52*AA51)*(AA51+AA52)+(Z52*AA53-Z53*AA52)*(AA52+AA53)+(Z53*AA54-Z54*AA53)*(AA53+AA54)+(Z54*AA55-Z55*AA54)*(AA54+AA55)+(Z55*AA56-Z56*AA55)*(AA55+AA56)+(Z56*AA57-Z57*AA56)*(AA56+AA57))/6/Z58","v":0.8271135590547164},"m",null,null,null,null,"II-II i I-I",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AI47+AI48)+(AH48*AI49-AH49*AI48)*(AI48+AI49)+(AH49*AI50-AH50*AI49)*(AI49+AI50)+(AH50*AI51-AH51*AI50)*(AI50+AI51)+(AH51*AI52-AH52*AI51)*(AI51+AI52)+(AH52*AI53-AH53*AI52)*(AI52+AI53)+(AH53*AI54-AH54*AI53)*(AI53+AI54)+(AH54*AI55-AH55*AI54)*(AI54+AI55)+(AH55*AI56-AH56*AI55)*(AI55+AI56)+(AH56*AI57-AH57*AI56)*(AI56+AI57))/6/AH58","v":1.3500505000000005},"m"]
["G=",{"$f":"+B58*'Analiza i dimenzioniranje'!E62","v":64.227611992767947},"kN",{"$f":"+D58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",null,"kN",{"$f":"+H58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(J58*'Analiza i dimenzioniranje'!E63<0,0,J58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN","G=",null,null,null,null,null,null,null,{"$f":"+T58*'Analiza i dimenzioniranje'!E49","v":{"$error":"#VALUE!"}},"kN (za L)",{"$f":"+V58*'Analiza i dimenzioniranje'!E62","v":62.769260514792791},"kN",{"$f":"+X58*'Analiza i dimenzioniranje'!E62","v":16.820514049966405},"kN",{"$f":"+Z58*'Analiza i dimenzioniranje'!E62","v":13.03527768524077},"kN",null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},"       ",{"$f":"+AH58*'Analiza i dimenzioniranje'!E62","v":5.2517757527774878},"kN"]
["Vertikala nasipa na konzoli",null,null,"Moment na konzoli",null,"Pokos na vrhu zida",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - NAPONI ",null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+'C III-V'!AC49+('Analiza i dimenzioniranje'!C191/2)","v":0.8051281599277047}]
[null,"x","y",{"$f":"IF('Analiza i dimenzioniranje'!G78=0,0,'Analiza i dimenzioniranje'!G78*'Analiza i dimenzioniranje'!C77*'Analiza i dimenzioniranje'!E62*(Q20-B5+'Analiza i dimenzioniranje'!G78/2)+J61*(O16-J59))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"+F64","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"naponi za presjek II-II",null,"naponi za srednji dio ",null,"naponi za presjek I-I",null,"Koordinate dna temelja"]
[null,{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},"b1=",{"$f":"+H47-2","v":1.4000010999999999},{"$f":"+B52","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y","x","y","x","y",{"$f":"+B2","v":2},0]
[null,{"$f":"+B64","v":{"$error":"#VALUE!"}},{"$f":"IF(B65>J49,C19,+C20+'Analiza i dimenzioniranje'!F20+(H52-H50)*TAN('Analiza i dimenzioniranje'!F21*PI()/180))","v":{"$error":"#VALUE!"}},"b2=",{"$f":"'Analiza i dimenzioniranje'!E54+('Analiza i dimenzioniranje'!E55-'Analiza i dimenzioniranje'!E54)*(('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)/(C9-C4))","v":{"$error":"#VALUE!"}},{"$f":"+B65","v":{"$error":"#VALUE!"}},{"$f":"+G64+(F64-F65)*TAN('Analiza i dimenzioniranje'!F21*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B2-Kontrafore!E3","v":1},0,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},0,{"$f":"+'C III-V'!B11","v":4.2000010999999997},{"$f":"-U47","v":0},{"$f":"+V77","v":{"$error":"#VALUE!"}},{"$f":"(AB65*(AC70-AC64)/(AB70-AB64)-AB64*(AC70-AC64)/(AB70-AB64)+AC64)","v":{"$error":"#VALUE!"}}]
[null,"AKTIVNI TLAKOVI za stabilnost zida oko točke A          ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+V65","v":1},{"$f":"AC55","v":{"$error":"#VALUE!"}},{"$f":"+X65","v":3.4000010999999999},{"$f":"+W67","v":{"$error":"#VALUE!"}},{"$f":"+AB57","v":4.2000010999999997},{"$f":"AC57","v":{"$error":"#VALUE!"}},2.5,{"$f":"+AC46","v":0.30769227514794739}]
[null,"AKTIVNI TLAKOVI za Presjek III-III ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"AC56","v":{"$error":"#VALUE!"}},{"$f":"+X66+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AA66","v":{"$error":"#VALUE!"}},{"$f":"+AB58","v":4.9000021999999994},{"$f":"+AC58","v":{"$error":"#VALUE!"}},{"$f":"+X77","v":{"$error":"#VALUE!"}},{"$f":"+(AB67*(AC64-AC70)/(AB64-AB70)-AB70*(AC64-AC70)/(AB64-AB70)+AC70)","v":{"$error":"#VALUE!"}}]
[null,"E1",null,"E2",null,"E3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+V67","v":3.4000010999999999},0,{"$f":"+X67","v":4.2000010999999997},0,{"$f":"+Z67","v":4.9000021999999994},{"$f":"+U50","v":0},{"$f":"+X67","v":4.2000010999999997},{"$f":"+(AB68*(AC64-AC70)/(AB64-AB70)-AB70*(AC64-AC70)/(AB64-AB70)+AC70)","v":0.37931024673015767}]
[null,0,{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C71","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+V65","v":1},{"$f":"+W65","v":0},{"$f":"+X65","v":3.4000010999999999},0,{"$f":"+Z65","v":4.2000010999999997},{"$f":"+U51","v":0},{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"+(AB69*(AC65-AC70)/(AB65-AB70)-AB70*(AC65-AC70)/(AB65-AB70)+AC70)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+B69","v":0},{"$f":"+C69-'Analiza i dimenzioniranje'!D17-'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+D69+'Analiza i dimenzioniranje'!E16*'Analiza i dimenzioniranje'!E17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+E69-'Analiza i dimenzioniranje'!E17","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"sjecište  armature uz tlo i armature dna temelja",null,null,null,null,null,null,null,null,null,{"$f":"+AB53","v":4.9000021999999994},{"$f":"+AC53","v":0.5}]
[null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('Analiza i dimenzioniranje'!D17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},0,{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F70+'Analiza i dimenzioniranje'!F16*'Analiza i dimenzioniranje'!F17*'Analiza i dimenzioniranje'!F112","v":{"$error":"#VALUE!"}},0,null,null,null,null,null,null,null,null,null,null,"Jedn pravca zida uz tlo",null,"Jedn pravca arm dno "]
[null,{"$f":"+B69","v":0},{"$f":"+C69","v":{"$error":"#VALUE!"}},0,{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F69","v":0},0,null,null,null,null,null,null,null,null,null,null,{"$f":"+S81+0.055","v":3.4550011},{"$f":"+T81","v":1.2},{"$f":"+U81+0.01","v":2.0599999999999996},{"$f":"+V81","v":0.18682583433163008}]
[null,null,null,{"$f":"+D69","v":{"$error":"#VALUE!"}},{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F72","v":0},{"$f":"+G70","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"+S82+0.055","v":{"$error":"#VALUE!"}},{"$f":"+T82","v":"A"},{"$f":"+U82+0.01","v":4.8700021999999992},{"$f":"+V82+0.02","v":0.56310345350772506}]
[null,"Koord. vertikale kohezije    sjecišta kohezije s pravcem od tlaka",null,"Koord. kohezije s pravcem od tlaka",null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(S73-S72)/(R73-R72)","v":{"$error":"#VALUE!"}}," *X",{"$f":"-S74*R72+S72","v":{"$error":"#VALUE!"}}]
[null,"X","y","X","y","X","y",null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(-U74+U77)/(S74-S77)","v":{"$error":"#VALUE!"}},"sjecište"]
[null,{"$f":"2*'Analiza i dimenzioniranje'!D15/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F110)","v":12.361875887090893},{"$f":"B76*(C71-C72)/(B71-B72)-B72*(C71-C72)/(B71-B72)+C72","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!F12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F111)","v":{"$error":"#VALUE!"}},{"$f":"IF(D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69>'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69)","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!C12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F112)","v":{"$error":"#VALUE!"}},{"$f":"IF((F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70)>'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!F17,(F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+S74*S75+U74","v":{"$error":"#VALUE!"}},null,null,{"$f":"-0.5*((V65*W66-V66*W65)+(V66*W67-V67*W66)+(V67*W68-V68*W67)+(V68*W69-V69*W68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((X65*Y66-X66*Y65)+(X66*Y67-X67*Y66)+(X67*Y68-X68*Y67)+(X68*Y69-X69*Y68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((Z65*AA66-Z66*AA65)+(Z66*AA67-Z67*AA66)+(Z67*AA68-Z68*AA67)+(Z68*AA69-Z69*AA68))","v":{"$error":"#VALUE!"}},"kN/m'"]
[null,{"$f":"+B76","v":12.361875887090893},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(U73-U72)/(T73-T72)","v":0.13390652120346919}," *X",{"$f":"-S77*T72+U72","v":-8.9021599347516411E-2},{"$f":"IF(V76=0,0,-(+(V65*W66-V66*W65)*(V65+V66)+(V66*W67-V67*W66)*(V66+V67)+(V67*W68-V68*W67)*(V67+V68)+(V68*W69-V69*W68)*(V68+V69))/6/V76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(X76=0,0,-(+(X65*Y66-X66*Y65)*(X65+X66)+(X66*Y67-X67*Y66)*(X66+X67)+(X67*Y68-X68*Y67)*(X67+X68)+(X68*Y69-X69*Y68)*(X68+X69))/6/X76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(Z76=0,0,-(+(Z65*AA66-Z66*AA65)*(Z65+Z66)+(Z66*AA67-Z67*AA66)*(Z66+Z67)+(Z67*AA68-Z68*AA67)*(Z67+Z68)+(Z68*AA69-Z69*AA68)*(Z68+Z69))/6/Z76)","v":{"$error":"#VALUE!"}},"m"]
["Oznaka","E1",null,"E2",null,"E3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-((V65*W66-V66*W65)*(W65+W66)+(V66*W67-V67*W66)*(W66+W67)+(V67*W68-V68*W67)*(W67+W68)+(V68*W69-V69*W68)*(W68+W69))/6/V76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((X65*Y66-X66*Y65)*(Y65+Y66)+(X66*Y67-X67*Y66)*(Y66+Y67)+(X67*Y68-X68*Y67)*(Y67+Y68)+(X68*Y69-X69*Y68)*(Y68+Y69))/6/X76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((Z65*AA66-Z66*AA65)*(AA65+AA66)+(Z66*AA67-Z67*AA66)*(AA66+AA67)+(Z67*AA68-Z68*AA67)*(AA67+AA68)+(Z68*AA69-Z69*AA68)*(AA68+AA69))/6/Z76","v":{"$error":"#VALUE!"}},"kN/m'"]
["točke","x","y","x","y","x","y"]
[1,{"$f":"+B77","v":12.361875887090893},{"$f":"+C77","v":{"$error":"#VALUE!"}},{"$f":"+D77","v":{"$error":"#VALUE!"}},{"$f":"+E77","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G77","v":0},null,null,null,null,null,null,null,null,null,null,null,"Jedn pravca zida uz tlo",null,"Jedn pravca arm dno ",null,"Y=",{"$f":"IF(S82=S81,1000000,(T82-T81)/(S82-S81))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X80*S81+T81","v":{"$error":"#VALUE!"}}]
[2,{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G70","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Unos podataka'!$O$48=\"\",+B4,B4+'Analiza i dimenzioniranje'!$E$60)","v":3.4000010999999999},{"$f":"+IF('Unos podataka'!$O$48=\"\",C4,0)","v":1.2},{"$f":"IF('Unos podataka'!$O$48=\"\",'Analiza i dimenzioniranje'!T593,+S81)","v":2.0499999999999998},{"$f":"IF('Unos podataka'!O48=\"\",'Analiza i dimenzioniranje'!U593,+T81)","v":0.18682583433163008},"X=",{"$f":"+(-Z80+Z83)/(X80-X83)","v":{"$error":"#VALUE!"}},"sjecište"]
[3,{"$f":"+B80","v":12.361875887090893},{"$f":"+C76","v":{"$error":"#VALUE!"}},{"$f":"IF(D76>D69,D81,D69)","v":{"$error":"#VALUE!"}},{"$f":"+E81","v":{"$error":"#VALUE!"}},{"$f":"IF(F77>F70,F77,F70)","v":{"$error":"#VALUE!"}},{"$f":"+G81","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!O48=\"\",C9,+C4)","v":"A"},{"$f":"IF('Unos podataka'!O48=\"\",'Analiza i dimenzioniranje'!T594,+'Unos podataka'!M125)","v":4.8600021999999994},{"$f":"IF('Unos podataka'!O48=\"\",'Analiza i dimenzioniranje'!U594,'Unos podataka'!N125)","v":0.54310345350772504},"Y=",{"$f":"+X80*X81+Z80","v":{"$error":"#VALUE!"}}]
[4,{"$f":"+B80","v":12.361875887090893},{"$f":"+C80","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F71","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(V82-V81)/(U82-U81)","v":0.12678908905341604},"*x",{"$f":"-X83*U81+V81","v":-7.3091798227872762E-2},"CRTANJE"]
[5,null,null,{"$f":"+D80","v":{"$error":"#VALUE!"}},{"$f":"+E80","v":{"$error":"#VALUE!"}},{"$f":"+F80","v":{"$error":"#VALUE!"}},{"$f":"+G80","v":0},null,null,null,null,null,null,null,null,null,null,null,"Jedn pravca sloja 3",null,"Jedn pravca sloja 3 klizno",null,"Y=",{"$f":"+(T86-T85)/(S86-S85)","v":-6.9926811943510428E-2},"*x",{"$f":"-X84*S85+T85","v":1.3398536238870209},"Jedn pravca sloja 3 klizno",null,"sjecište 1/2 sidra sa vrhom 1. sloja"]
["  A=",{"$f":"IF(B77>B71,0,-IF(B84>B83,0,-0.5*((B80*C81-B81*C80)+(B81*C82-B82*C81)+(B82*C83-B83*C82)+(B83*C84-B84*C83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D77>D70,0,IF(D84>D83,0,-0.5*((D80*E81-D81*E80)+(D81*E82-D82*E81)+(D82*E83-D83*E82)+(D83*E84-D84*E83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F77>F71,0,IF(F84>F83,0,-0.5*((F80*G81-F81*G80)+(F81*G82-F82*G81)+(F82*G83-F83*G82)+(F83*G84-F84*G83))))","v":{"$error":"#VALUE!"}},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Unos podataka'!B109","v":2},{"$f":"+'Unos podataka'!C109","v":1.2},{"$f":"+W100","v":2},0,"X=",{"$f":"+AB156","v":1.1597509541483482},"sjecište ",null,{"$f":"+U85","v":2},{"$f":"+V85","v":0},"Y=",{"$f":"+X92","v":{"$error":"#VALUE!"}},"*x",{"$f":"+Z92","v":{"$error":"#VALUE!"}}]
["xt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(B80+B81)+(B81*C82-B82*C81)*(B81+B82)+(B82*C83-B83*C82)*(B82+B83)+(B83*C84-B84*C83)*(B83+B84))/6/B85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(D80+D81)+(D81*E82-D82*E81)*(D81+D82)+(D82*E83-D83*E82)*(D82+D83)+(D83*E84-D84*E83)*(D83+D84))/6/D85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(F80+F81)+(F81*G82-F82*G81)*(F81+F82)+(F82*G83-F83*G82)*(F82+F83)+(F83*G84-F84*G83)*(F83+F84))/6/F85)","v":{"$error":"#VALUE!"}},"kN/m'",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Unos podataka'!B110","v":-8},{"$f":"+'Unos podataka'!C110","v":1.8992681194351042},-5,{"$f":"+V85+(U85-U86)*TAN((45+'Analiza i dimenzioniranje'!F14/2)*PI()/180)","v":9.9970360471948005},"Y=",{"$f":"+X101","v":1.2},3,null,{"$f":"+X85","v":1.1597509541483482},{"$f":"+X86","v":1.2}]
["yt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(C80+C81)+(B81*C82-B82*C81)*(C81+C82)+(B82*C83-B83*C82)*(C82+C83)+(B83*C84-B84*C83)*(C83+C84))/6/B85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(E80+E81)+(D81*E82-D82*E81)*(E81+E82)+(D82*E83-D83*E82)*(E82+E83)+(D83*E84-D84*E83)*(E83+E84))/6/D85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(G80+G81)+(F81*G82-F82*G81)*(G81+G82)+(F82*G83-F83*G82)*(G82+G83)+(F83*G84-F84*G83)*(G83+G84))/6/F85)","v":{"$error":"#VALUE!"}},"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(V86-V85)/(U86-U85)","v":-1.4281480067421144},"*x",{"$f":"-X87*U85+V85","v":2.8562960134842288},"y=2       x=",{"$f":"+('Analiza i dimenzioniranje'!E52-'C III-V'!Z87)/'C III-V'!X87","v":1.1597509541483482}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(K85<0,0,K85)","v":0},null,null,null,null,{"$f":"+IF(P85<0,0,P85)","v":0},null,null,"Jedn pravca sloja 2",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(T90-T89)/(S90-S89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X88*S89+T89","v":{"$error":"#VALUE!"}},"Jedn pravca sloja 2 klizno",null,"Jednadžba pravca sidra",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(AD90-AD89)/(AC90-AC89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AH88*AC89+AD89","v":{"$error":"#VALUE!"}}]
["X koordinata položaja rezultante aktivnog tlaka na stražnjoj strani zida za  Ev1, Ev2 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U12","v":{"$error":"#VALUE!"}},{"$f":"+V12","v":4},{"$f":"+X85","v":1.1597509541483482},{"$f":"+X86","v":1.2},"X=",{"$f":"+(-Z88+Z91)/(X88-X91)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U89","v":1.1597509541483482},{"$f":"+V89","v":1.2},{"$f":"+U37","v":{"$error":"#VALUE!"}},{"$f":"+V37","v":5},{"$f":"+U89","v":1.1597509541483482},{"$f":"+V89","v":1.2},"X=",{"$f":"+(-AJ88+AJ91)/(AH88-AH91)","v":{"$error":"#VALUE!"}},"sjecište"]
["Jednadžba pravca zida uz tlo",null,null,null,null,"Za Ev3 x=2",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U13","v":-8},{"$f":"+V13","v":{"$error":"#VALUE!"}},-5,{"$f":"+V89+(U89-U90)*TAN((45+'Analiza i dimenzioniranje'!E14/2)*PI()/180)","v":9.6781698478948464},"Y=",{"$f":"+X88*X89+Z88","v":{"$error":"#VALUE!"}},2,null,{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},{"$f":"+U38","v":{"$error":"#VALUE!"}},{"$f":"+V38","v":{"$error":"#VALUE!"}},{"$f":"+U90","v":-5},{"$f":"+V90","v":9.6781698478948464},"Y=",{"$f":"+AH88*AH89+AJ88","v":{"$error":"#VALUE!"}},2]
["E1",null,"E2",null,"E3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(V90-V89)/(U90-U89)","v":-1.3763819204711734},"*x",{"$f":"-X91*U89+V89","v":2.7962602455389791},null,null,null,null,null,null,"Y=",{"$f":"+(AF90-AF89)/(AE90-AE89)","v":-1.3763819204711734},"*x",{"$f":"-AH91*AE89+AF89","v":2.7962602455389791}]
["x","y","x","y","x","y",null,{"$f":"+(B8-B4)*(I92-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+I87","v":0},null,null,null,null,null,null,null,null,null,"Jedn pravca sloja 1",null,"Jedn pravca sloja 1 klizno",null,"Y=",{"$f":"+(T95-T94)/(S95-S94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X92*S94+T94","v":{"$error":"#VALUE!"}},"Jedan pravca sloja 1 klizno",null,"Slobodna dionica ls>=",{"$f":"+SQRT((AC94-AC93)*(AC94-AC93)+(AD94-AD93)*(AD94-AD93))","v":{"$error":"#VALUE!"}}]
[{"$f":"+(B8-B4)*(B93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+B87","v":{"$error":"#VALUE!"}},{"$f":"+(B8-B4)*(D93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+D87","v":{"$error":"#VALUE!"}},2,{"$f":"+F87","v":{"$error":"#VALUE!"}},null,{"$f":"+(B8-B4)*(I93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+N87","v":0},null,null,null,null,null,null,null,null,null,{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+V7","v":6},null,null,"X=",{"$f":"+(-Z92+Z95)/(X92-X95)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U94","v":{"$error":"#VALUE!"}},{"$f":"+V94","v":{"$error":"#VALUE!"}},{"$f":"+AC89","v":{"$error":"#VALUE!"}},{"$f":"+AD89","v":5},null,null,null,null,null,null,null,null,"Gornja klizna ploha",null,null,null,"Donja klizna ploha"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U8","v":{"$error":"#VALUE!"}},{"$f":"+V8","v":6},{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+X92*X93+Z92","v":{"$error":"#VALUE!"}},1,null,{"$f":"+X93","v":{"$error":"#VALUE!"}},{"$f":"+X94","v":{"$error":"#VALUE!"}},{"$f":"+AH89","v":{"$error":"#VALUE!"}},{"$f":"+AH90","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782},-5,{"$f":"+V94+(U94-U95)*TAN((45+'Analiza i dimenzioniranje'!D14/2)*PI()/180)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+(V95-V94)/(U95-U94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X95*U94+V94","v":{"$error":"#VALUE!"}},{"$f":"+(AB95-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782},null,null,null,null,null,null,null,null,null,null,{"$f":"+T131","v":"x="},1.75,-1.0572404418349119,null,{"$f":"+AK136","v":{"$error":"#VALUE!"}},{"$f":"+AK103","v":-1.0572404418349119}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(AB96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!R44","v":{"$error":"#VALUE!"}},{"$f":"+(AD96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Q44","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"y=",0,4,null,{"$f":"+AL136","v":{"$error":"#VALUE!"}},{"$f":"+AL103","v":4}]
[{"$f":"+A78","v":"Oznaka"},{"$f":"+B78","v":"E1"},null,{"$f":"+D78","v":"E2"},null,{"$f":"+F78","v":"E3"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Linija klizne plohe za potres kada su kontrafore ",null,"Zid",null,"POTRES sa kliznim tijelom Uključen proporcionalmi dio kontrafora). U originalu 3/10.",null,"x","y","x","y","x","y","POTRES bez kontrafora",null,"Ovaj račun potresa sa kontraforama služi samo za dobivanje računskog potresa kada iskop za temelje kontrafore nije pojedinačni nego je po čitavoj duljini isti  kao i za temelj zida. ",null,"Računski potres s ukljućenim dijelom temelja za kontrafore",null,"Y=",{"$f":"(AO96-AN96)/(AO95-AN95)","v":-1.4248868534344206},"*x    +",{"$f":"-AN97*AN95+AN96","v":2.4935519935102359},{"$f":"(AR96-AQ96)/(AR95-AQ95)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AQ97*AQ95+AQ96","v":{"$error":"#VALUE!"}}]
[{"$f":"+A79","v":"točke"},{"$f":"+B79","v":"x"},{"$f":"+C79","v":"y"},{"$f":"+D79","v":"x"},{"$f":"+E79","v":"y"},{"$f":"+F79","v":"x"},{"$f":"+G79","v":"y"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(B9-B4)*(AB98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Q44","v":{"$error":"#VALUE!"}},{"$f":"+(B9-B4)*(AD98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Dijagram momenata'!$Q$22","v":{"$error":"#VALUE!"}},2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,null,null,"X=",{"$f":"-($AP$97-AO98)/$AN$97","v":0.90782786744952648},{"$f":"+AR102","v":1.2}]
[{"$f":"+A80","v":1},{"$f":"+B80*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":12.331762978735648},{"$f":"+C80*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+D80*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+E80*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+F80*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+G80*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":0},null,null,"Jednadžba UREĐENOG TERENA KADA JE KOSINA IZA ZIDA (bez prometa)",null,null,null,null,null,null,null,null,"uređeni teren ",null,null,null,{"$f":"+B2","v":2},0.12820515121628623,null,null,{"$f":"+AB116","v":-2.2362814274055753},{"$f":"+AC116","v":5.6800000000000006},{"$f":"+AB103","v":0.68324863210273346},{"$f":"+AC103","v":1.52},{"$f":"+(Z95-AF99)/(-X91)","v":{"$error":"#VALUE!"}},{"$f":"+AF98","v":1.2},null,null,null,null,null,null,null,null,null,"Srednja klizna ploha","Gornja klizna ploha"]
[2,{"$f":"+B81*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+C81*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+D81*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+E81*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+F81*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+G81*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"Jednadžba terena s prometnim",null,null,null,"x","y","x","y",2,1.2,null,null,"oznaka","X","Y",null,"Presjek III-III",null,null,null,null,null,"Potresna sila za stabilnost ",null,null,null,null,"y","x",{"$f":"+AC100","v":"Y"},"X"]
[3,{"$f":"+B82*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":12.331762978735648},{"$f":"+C82*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+D82*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+E82*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+F82*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+G82*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},null,null,"x=",{"$f":"+S101","v":-8},{"$f":"+S105","v":{"$error":"#VALUE!"}},null,null,{"$f":"+J101","v":"x="},{"$f":"+D114","v":{"$error":"#VALUE!"}},{"$f":"+D115","v":-8},null,{"$f":"+'Unos podataka'!S58","v":-8},{"$f":"+'Unos podataka'!T58","v":6.2644906473896782},{"$f":"+'Analiza i dimenzioniranje'!$A94","v":1.75},{"$f":"+'Analiza i dimenzioniranje'!$B94","v":0},3.4000010999999999,1.2,{"$f":"2+AN113+'Analiza i dimenzioniranje'!E60","v":1.75},{"$f":"+'Sile i krakovi'!B218","v":9.6153895463470418E-2},"Y=0",{"$f":"+AC101/$K$109-$M$109/$K$109","v":1.75},0,null,null,null,null,null,null,null,{"$f":"+Y101","v":1.75},9.6153895463470418E-2,null,null,null,{"$f":"-($AP$97-AR101)/$AN$97","v":1.75},{"$f":"-($AS$97-AR101)/$AQ$97","v":{"$error":"#VALUE!"}},0,{"$f":"+IF(AQ101<=$AN$105,AP101,AQ101)","v":{"$error":"#VALUE!"}}]
[4,{"$f":"+B83*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":12.331762978735648},{"$f":"+C83*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+D83*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+E83*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+F83*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+G83*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":0},null,null,"Y=",{"$f":"+T101","v":6.2644906473896782},{"$f":"+T105","v":"A"},null,null,{"$f":"+J102","v":"Y="},{"$f":"+E114","v":6.2644906473896782},{"$f":"+E115","v":6.2644906473896782},null,{"$f":"+'Unos podataka'!$V$68","v":{"$error":"#VALUE!"}},{"$f":"+T101","v":6.2644906473896782},{"$f":"+'Analiza i dimenzioniranje'!$A95","v":0.97707863658009864},{"$f":"+'Analiza i dimenzioniranje'!$B95","v":1.2},{"$error":"#VALUE!"},3.14,{"$f":"+Y101-(Z102-Z101)/TAN(W119*PI()/180)","v":0.97707863658009864},{"$f":"+AC102","v":1.2},"PIII",{"$f":"+Y102","v":0.97707863658009864},{"$f":"+'Analiza i dimenzioniranje'!U52","v":1.2},null,{"$f":"+Y102","v":0.97707863658009864},{"$f":"+Z102","v":1.2},null,null,null,null,0.97707863658009864,1.2,null,null,null,0.90782786744952648,{"$error":"#VALUE!"},1.2,{"$error":"#VALUE!"}]
[5,{"$f":"+B84*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":0},{"$f":"+C84*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":0},{"$f":"+D84*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+E84*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+F84*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+G84*COS(('Analiza i dimenzioniranje'!$D$19+'Analiza i dimenzioniranje'!$H$51)*PI()/180)","v":0},null,null,"Y=",{"$f":"(L102-K102)/(L101-K101)","v":{"$error":"#VALUE!"}},"*x             +",{"$f":"-K103*K101+K102","v":{"$error":"#VALUE!"}},null,"Y=",{"$f":"(Q102-P102)/(Q101-P101)","v":{"$error":"#VALUE!"}},"*x             +",{"$f":"-P103*P101+P102","v":{"$error":"#VALUE!"}},{"$f":"+D121","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!W68","v":6.2644906473896782},{"$f":"+'Analiza i dimenzioniranje'!$A96","v":-1.0572404418349119},{"$f":"+'Analiza i dimenzioniranje'!$B96","v":4},{"$error":"#VALUE!"},3.14,{"$f":"+Y102-(Z103-Z102)/TAN(W118*PI()/180)","v":-1.0572404418349119},{"$f":"+'Analiza i dimenzioniranje'!$E$17+'Analiza i dimenzioniranje'!$F$17","v":4},"PVI",{"$f":"-($W$133-AC103)/$U$133","v":0.68324863210273346},{"$f":"+'Analiza i dimenzioniranje'!U53","v":1.52},null,-1.0572404418349119,{"$f":"+AN105","v":4},null,null,null,null,-1.0572404418349119,4,null,null,null,0.68324863210273346,{"$error":"#VALUE!"},1.52,{"$error":"#VALUE!"}]
["  A=",{"$f":"IF(B99>B100,0,IF(-0.5*((B99*C100-B100*C99)+(B100*C101-B101*C100)+(B101*C102-B102*C101)+(B102*C103-B103*C102))<0,0.5*((B99*C100-B100*C99)+(B100*C101-B101*C100)+(B101*C102-B102*C101)+(B102*C103-B103*C102)),0))","v":{"$error":"#VALUE!"}},{"$f":"+C85","v":"kN/m'"},{"$f":"IF(D103>D102,0,-0.5*((D99*E100-D100*E99)+(D100*E101-D101*E100)+(D101*E102-D102*E101)+(D102*E103-D103*E102)))","v":{"$error":"#VALUE!"}},{"$f":"+E85","v":"kN/m'"},{"$f":"IF(F103>F102,0,-0.5*((F99*G100-F100*G99)+(F100*G101-F101*G100)+(F101*G102-F102*G101)+(F102*G103-F103*G102)))","v":{"$error":"#VALUE!"}},{"$f":"+G85","v":"kN/m'"},null,null,"Vrijednosti X za poznati Y",null,null,null,null,"X=",{"$f":"+Q112/$K$109-$M$109/$K$109","v":{"$error":"#VALUE!"}},6.2," =Y",{"$f":"+'Unos podataka'!V69","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!W69","v":6},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$B97","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},3.44,{"$f":"+Y103-(Z104-Z103)/TAN(W117*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+AL136","v":{"$error":"#VALUE!"}},"PVII",0.45866939675594048,{"$f":"+'Analiza i dimenzioniranje'!U54","v":1.84},null,{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+AL136","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AE104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},null,null,null,0.45866939675594048,{"$error":"#VALUE!"},1.84,{"$error":"#VALUE!"}]
["xt=",{"$f":"IF(B104=0,0,((B99*C100-B100*C99)*(B99+B100)+(B100*C101-B101*C100)*(B100+B101)+(B101*C102-B102*C101)*(B101+B102)+(B102*C103-B103*C102)*(B102+B103))/6/B104)","v":{"$error":"#VALUE!"}},{"$f":"+C86","v":"kN/m'"},{"$f":"IF(D104=0,0,-((D99*E100-D100*E99)*(D99+D100)+(D100*E101-D101*E100)*(D100+D101)+(D101*E102-D102*E101)*(D101+D102)+(D102*E103-D103*E102)*(D102+D103))/6/D104)","v":{"$error":"#VALUE!"}},{"$f":"+E86","v":"kN/m'"},{"$f":"IF(F104=0,0,-((F99*G100-F100*G99)*(F99+F100)+(F100*G101-F101*G100)*(F100+F101)+(F101*G102-F102*G101)*(F101+F102)+(F102*G103-F103*G102)*(F102+F103))/6/F104)","v":{"$error":"#VALUE!"}},{"$f":"+G86","v":"kN/m'"},null,null,"X=",{"$f":"+L112/$K$109-$M$109/$K$109","v":{"$error":"#VALUE!"}},6.2," =Y",null,{"$f":"+J104","v":"Vrijednosti X za poznati Y"},null,null,null,{"$f":"+'Unos podataka'!V70","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!W70","v":"A"},null,null,{"$error":"#VALUE!"},3.44,{"$f":"+'Unos podataka'!B105","v":{"$error":"#VALUE!"}},{"$f":"+V110","v":6.2644906473896782},"PVIII",0.23409016140914748,{"$f":"+'Analiza i dimenzioniranje'!U55","v":2.16},null,{"$error":"#VALUE!"},6.2644906473896782,{"$f":"+AM105","v":" H="},{"$f":"+AN105","v":4},null,null,{"$f":"+Y105","v":{"$error":"#VALUE!"}},6.2644906473896782," H=",{"$f":"+'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17+'Unos podataka'!$F$9","v":4},null,0.23409016140914748,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"}]
["yt=",{"$f":"IF(B104=0,0,((B99*C100-B100*C99)*(C99+C100)+(B100*C101-B101*C100)*(C100+C101)+(B101*C102-B102*C101)*(C101+C102)+(B102*C103-B103*C102)*(C102+C103))/6/B104)","v":{"$error":"#VALUE!"}},{"$f":"+C87","v":"m"},{"$f":"IF(D104=0,0,-((D99*E100-D100*E99)*(E99+E100)+(D100*E101-D101*E100)*(E100+E101)+(D101*E102-D102*E101)*(E101+E102)+(D102*E103-D103*E102)*(E102+E103))/6/D104)","v":{"$error":"#VALUE!"}},{"$f":"+E87","v":"m"},{"$f":"IF(F104=0,0,-((F99*G100-F100*G99)*(G99+G100)+(F100*G101-F101*G100)*(G100+G101)+(F101*G102-F102*G101)*(G101+G102)+(F102*G103-F103*G102)*(G102+G103))/6/F104)","v":{"$error":"#VALUE!"}},{"$f":"+G87","v":"m"},null,null,"Jednadžba kizne ploha  ",null,null,null,null,{"$f":"+J106","v":"Jednadžba kizne ploha  "},{"$f":"+K106","v":0},{"$f":"+L106","v":0},{"$f":"+M106","v":0},null,null,null,null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+X107","v":"A"},{"$f":"+'Unos podataka'!S56","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!$T$55","v":6},"PIX",9.5109260623546556E-3,{"$f":"+'Analiza i dimenzioniranje'!U56","v":2.48},null,{"$error":"#VALUE!"},6,null,null,null,null,{"$error":"#VALUE!"},6,null,null,null,9.5109260623546556E-3,{"$error":"#VALUE!"},2.48,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,"x=",{"$f":"+AK103","v":-1.0572404418349119},{"$f":"+AV123","v":1.75},null,null,{"$f":"+J107","v":"x="},{"$f":"+AK103","v":-1.0572404418349119},{"$f":"+AV123","v":1.75},null,null,null,"Profil terena",null,{"$f":"+B10","v":{"$error":"#VALUE!"}},{"$f":"+C10","v":"A"},{"$f":"+'Unos podataka'!S56","v":{"$error":"#VALUE!"}},{"$f":"+Z106","v":6},"PX",-0.21506830928443818,{"$f":"+'Analiza i dimenzioniranje'!U57","v":2.8},null,{"$error":"#VALUE!"},6,null,null,null,null,{"$error":"#VALUE!"},6,null,null,null,-0.21506830928443818,{"$error":"#VALUE!"},2.8,{"$error":"#VALUE!"}]
["Jednadžba dna konzole",null,"Y=",{"$f":"+AA150","v":-1.3763819204711734}," *X      +",{"$f":"+AC149","v":2.5448333702674724},null,null,null,"Y=",{"$f":"+AL103","v":4},{"$f":"+AV124","v":0},null,null,{"$f":"+J108","v":"Y="},{"$f":"+AL103","v":4},{"$f":"+AV124","v":0},null,null,null,{"$f":"+'Unos podataka'!B103","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!C103","v":6},{"$f":"+W107","v":{"$error":"#VALUE!"}},{"$f":"+X107","v":"A"},{"$f":"2+'Analiza i dimenzioniranje'!E59","v":3.4000000999999997},{"$f":"+Z102","v":1.2},"PXI",-0.45368374684040591,{"$f":"+'Analiza i dimenzioniranje'!U58","v":3.14},null,3.4000000999999997,1.2,null,null,null,null,3.4000000999999997,1.2,null,"visina 2 donja sloja   h=",{"$f":"+'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17+'Unos podataka'!F9","v":4},-0.45368374684040591,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"}]
["Jednadžba klizne plohe II. Sloja           X=",null,null,{"$f":"+(F108-E109)/(-D108)","v":-0.43241386775030138},{"$f":"+'C III-V'!C6","v":3.14}," =Y",null,null,null,"Y=",{"$f":"(L108-K108)/(L107-K107)","v":-1.4248868534344206},"*x    +",{"$f":"-K109*K107+K108","v":2.4935519935102359},null,"Y=",{"$f":"(Q108-P108)/(Q107-P107)","v":-1.4248868534344206},"*x    +",{"$f":"-P109*P107+P108","v":2.4935519935102359},null,null,{"$f":"+'Unos podataka'!B104","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!C104","v":6},{"$f":"+B11","v":4.2000010999999997},1.2,{"$f":"IF('Unos podataka'!$O$48=\"DA\",2,+Y110)","v":1.75},{"$f":"+Z108","v":1.2},"PXII",-0.66422677997802415,{"$f":"+'Analiza i dimenzioniranje'!U59","v":3.44},null,{"$f":"+AE102","v":0.97707863658009864},{"$f":"+AF102","v":1.2},null,null,null,null,1.75,1.2,null,null,null,-0.66422677997802415,{"$error":"#VALUE!"},3.44,{"$error":"#VALUE!"}]
[null,null,null,{"$f":"+IF('Unos podataka'!H59>=('Unos podataka'!H7+'Unos podataka'!J7),'C III-V'!E110,'C III-V'!D109)","v":-0.43241386775030138},{"$f":"+(AC144-E109)/(-AA145)","v":-0.4771631173504251},null,null,null,null,"Vrijednosti X za poznati Y",null,null,null,null,"Vrijednosti X za poznati Y",null,null,null,null,null,{"$f":"+'Unos podataka'!B105","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!C105","v":6.2644906473896782},4.2000010999999997,1.2,{"$f":"+Y101","v":1.75},{"$f":"+Z101","v":9.6153895463470418E-2},"PXIII",-0.88880601532481696,{"$f":"+'Analiza i dimenzioniranje'!U60","v":3.76},null,null,null,null,null,null,null,1.75,{"$f":"+AL101","v":9.6153895463470418E-2},null,null,null,-0.88880601532481696,{"$error":"#VALUE!"},3.76,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,"X=",{"$f":"+L111/$K$109-$M$109/$K$109","v":-3.7311369626826654},7.81," =Y",null,"X=",{"$f":"+Q111/$K$109-$M$109/$K$109","v":-3.7311369626826654},7.81," =Y",null,null,{"$f":"+'Unos podataka'!B106","v":-8},{"$f":"+'Unos podataka'!C106","v":6.2644906473896782},4.2000010999999997,1.2,{"$f":"-0.5*((Y101*Z102-Y102*Z101)+(Y102*Z103-Y103*Z102)+(Y103*Z104-Y104*Z103)+(Y104*Z105-Y105*Z104)+(Y105*Z106-Y106*Z105)+(Y106*Z107-Y107*Z106)+(Y107*Z108-Y108*Z107)+(Y108*Z109-Y109*Z108)+(Y109*Z110-Y110*Z109))","v":{"$error":"#VALUE!"}},"m2","PXIV",-1.1133852506716102,{"$f":"+'Analiza i dimenzioniranje'!U61","v":4.08},null,{"$f":"-0.5*((AE101*AF102-AE102*AF101)+(AE102*AF103-AE103*AF102)+(AE103*AF104-AE104*AF103)+(AE104*AF105-AE105*AF104)+(AE105*AF106-AE106*AF105)+(AE106*AF107-AE107*AF106)+(AE107*AF108-AE108*AF107)+(AE108*AF109-AE109*AF108)+(AE109*AF110-AE110*AF109))","v":{"$error":"#VALUE!"}},"m2",null,null,null,null,{"$f":"-0.5*((AK101*AL102-AK102*AL101)+(AK102*AL103-AK103*AL102)+(AK103*AL104-AK104*AL103)+(AK104*AL105-AK105*AL104)+(AK105*AL106-AK106*AL105)+(AK106*AL107-AK107*AL106)+(AK107*AL108-AK108*AL107)+(AK108*AL109-AK109*AL108)+(AK109*AL110-AK110*AL109))","v":{"$error":"#VALUE!"}},"m2","OK","prosječna površina temelja od temelja kontrafore duž čitavog zida",null,-1.1133852506716102,{"$error":"#VALUE!"},4.08,{"$error":"#VALUE!"}]
[null,null,"Jednadžba terena s prometnim",null,null,null,null,null,null,null,{"$f":"+L112/$K$109-$M$109/$K$109","v":{"$error":"#VALUE!"}},{"$f":"+G64","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+K112","v":{"$error":"#VALUE!"}},{"$f":"+L112","v":{"$error":"#VALUE!"}},null,null,null,null,null,4.9000021999999994,1.2,{"$f":"-((Y101*Z102-Y102*Z101)*(Y101+Y102)+(Y102*Z103-Y103*Z102)*(Y102+Y103)+(Y103*Z104-Y104*Z103)*(Y103+Y104)+(Y104*Z105-Y105*Z104)*(Y104+Y105)+(Y105*Z106-Y106*Z105)*(Y105+Y106)+(Y106*Z107-Y107*Z106)*(Y106+Y107)+(Y107*Z108-Y108*Z107)*(Y107+Y108)+(Y108*Z109-Y109*Z108)*(Y108+Y109)+(Y109*Z110-Y110*Z109)*(Y109+Y110))/6/Y111","v":{"$error":"#VALUE!"}},"m  ","PXV",-1.3379644860184032,{"$f":"+'Analiza i dimenzioniranje'!U62","v":4.4000000000000004},null,{"$f":"-((AE101*AF102-AE102*AF101)*(AE101+AE102)+(AE102*AF103-AE103*AF102)*(AE102+AE103)+(AE103*AF104-AE104*AF103)*(AE103+AE104)+(AE104*AF105-AE105*AF104)*(AE104+AE105)+(AE105*AF106-AE106*AF105)*(AE105+AE106)+(AE106*AF107-AE107*AF106)*(AE106+AE107)+(AE107*AF108-AE108*AF107)*(AE107+AE108)+(AE108*AF109-AE109*AF108)*(AE108+AE109)+(AE109*AF110-AE110*AF109)*(AE109+AE110))/6/AE111","v":{"$error":"#VALUE!"}},"m  ","x",null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AK101+AK102)+(AK102*AL103-AK103*AL102)*(AK102+AK103)+(AK103*AL104-AK104*AL103)*(AK103+AK104)+(AK104*AL105-AK105*AL104)*(AK104+AK105)+(AK105*AL106-AK106*AL105)*(AK105+AK106)+(AK106*AL107-AK107*AL106)*(AK106+AK107)+(AK107*AL108-AK108*AL107)*(AK107+AK108)+(AK108*AL109-AK109*AL108)*(AK108+AK109)+(AK109*AL110-AK110*AL109)*(AK109+AK110))/6/AK111","v":{"$error":"#VALUE!"}},"m  ",null,null,null,-1.3379644860184032,{"$error":"#VALUE!"},4.4000000000000004,{"$error":"#VALUE!"}]
[null,null,null,"x","y",null,null,null,null,"sjecište klizne plohe s  terenom bez prometa ",null,null,null,null,"sjecište klizne plohe s terenom sa prometom ",null,null,null,null,"koordinate težišta mase za h22",null,null,4.9000021999999994,0.5,{"$f":"-((Y101*Z102-Y102*Z101)*(Z101+Z102)+(Y102*Z103-Y103*Z102)*(Z102+Z103)+(Y103*Z104-Y104*Z103)*(Z103+Z104)+(Y104*Z105-Y105*Z104)*(Z104+Z105)+(Y105*Z106-Y106*Z105)*(Z105+Z106)+(Y106*Z107-Y107*Z106)*(Z106+Z107)+(Y107*Z108-Y108*Z107)*(Z107+Z108)+(Y108*Z109-Y109*Z108)*(Z108+Z109)+(Y109*Z110-Y110*Z109)*(Z109+Z110))/6/Y111","v":{"$error":"#VALUE!"}},"m    ","PXVI",-1.5625437213651958,{"$f":"+'Analiza i dimenzioniranje'!U63","v":4.72},null,{"$f":"-((AE101*AF102-AE102*AF101)*(AF101+AF102)+(AE102*AF103-AE103*AF102)*(AF102+AF103)+(AE103*AF104-AE104*AF103)*(AF103+AF104)+(AE104*AF105-AE105*AF104)*(AF104+AF105)+(AE105*AF106-AE106*AF105)*(AF105+AF106)+(AE106*AF107-AE107*AF106)*(AF106+AF107)+(AE107*AF108-AE108*AF107)*(AF107+AF108)+(AE108*AF109-AE109*AF108)*(AF108+AF109)+(AE109*AF110-AE110*AF109)*(AF109+AF110))/6/AE111","v":{"$error":"#VALUE!"}},"m    ","y",null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AL101+AL102)+(AK102*AL103-AK103*AL102)*(AL102+AL103)+(AK103*AL104-AK104*AL103)*(AL103+AL104)+(AK104*AL105-AK105*AL104)*(AL104+AL105)+(AK105*AL106-AK106*AL105)*(AL105+AL106)+(AK106*AL107-AK107*AL106)*(AL106+AL107)+(AK107*AL108-AK108*AL107)*(AL107+AL108)+(AK108*AL109-AK109*AL108)*(AL108+AL109)+(AK109*AL110-AK110*AL109)*(AL109+AL110))/6/AK111","v":{"$error":"#VALUE!"}},"m    ",null,{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,BC124)","v":-0.25},{"$f":"IF('Analiza i dimenzioniranje'!D83=\"\",0,'Analiza i dimenzioniranje'!D83+'C III-V'!AN113)","v":0.75},-1.5625437213651958,{"$error":"#VALUE!"},4.72,{"$error":"#VALUE!"}]
[null,null,null,{"$f":"+U110","v":{"$error":"#VALUE!"}},{"$f":"+V110","v":6.2644906473896782},null,null,null,null,"x=",{"$f":"+L101","v":{"$error":"#VALUE!"}},-6,{"$f":"+R114","v":-1.0572404418349119},{"$f":"+S114","v":-3.7552745092046185},"x=",{"$f":"+P101","v":{"$error":"#VALUE!"}},{"$f":"+Q101","v":-8},{"$f":"+P107","v":-1.0572404418349119},{"$f":"+R114-(S115-R115)/TAN(W117*PI()/180)","v":-3.7552745092046185},null,null,null,2,0.12820515121628623,{"$f":"+Y111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN","PXVII",-1.7871229567119888,{"$f":"+'Analiza i dimenzioniranje'!U64","v":5.04},null,{"$f":"+AE111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,{"$f":"+AK111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",null,null,null,-1.7871229567119888,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"}]
[null,null,null,{"$f":"+U111","v":-8},{"$f":"+V111","v":6.2644906473896782},null,null,null,null,"Y=",{"$f":"+L102","v":"A"},{"$f":"(K115+(-L114+K114)*TAN('Analiza i dimenzioniranje'!H20*PI()/180))","v":{"$error":"#VALUE!"}},{"$f":"+R115","v":4},{"$f":"+S115","v":8},"Y=",{"$f":"+P102","v":6.2644906473896782},{"$f":"+Q102","v":6.2644906473896782},{"$f":"+P108","v":4},8,{"$f":"(AA124-AA125)/3","v":0},{"$f":"+AF102*0.666666666666667","v":0.80000000000000038},null,null,null,null,null,"PXVIII",-2.0117021920587819,{"$f":"+'Analiza i dimenzioniranje'!U65","v":5.36},null,null,null,null,null,"Teren  ",null,"Klizna ploha",null,"Potres za Masivni zid",null,null,-2.0117021920587819,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"}]
[null,null,"Y=",{"$f":"+(E115-E114)/(D115-D114)","v":{"$error":"#VALUE!"}},"*x      +",{"$f":"-D116*D114+E114","v":{"$error":"#VALUE!"}},null,null,null,"Y=",{"$f":"(L115-K115)/(L114-K114)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-K116*K114+K115","v":{"$error":"#VALUE!"}}," ","Y=",{"$f":"(Q115-P115)/(Q114-P114)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-P116*P114+P115","v":{"$error":"#VALUE!"}}," ",null,null," j","h",null,null,null,"PXIX",-2.2362814274055753,{"$f":"+'Analiza i dimenzioniranje'!U66","v":5.6800000000000006},null,null,null,null,null,{"$f":"+Y105","v":{"$error":"#VALUE!"}},{"$f":"+Y106","v":{"$error":"#VALUE!"}},{"$f":"+U131","v":1.75},{"$f":"+AK136","v":{"$error":"#VALUE!"}},null,null,null,-2.2362814274055753,{"$error":"#VALUE!"},5.6800000000000006,{"$error":"#VALUE!"},"x=",{"$f":"+AK102","v":0.97707863658009864},{"$f":"+AL102","v":1.2},null,null,"Omjer površine"]
[null,null,null,null,null,null,null,null,null,"Y=",{"$f":"-(N115-M115)/(M114-N114)","v":-1.4825609685127403},"*x    +",{"$f":"-(M114*K117-M115)","v":2.4325765866023952}," ","Y=",{"$f":"-(S115-R115)/(R114-S114)","v":-1.4825609685127403},"*x    +",{"$f":"-(R114*P117-R115)","v":2.4325765866023952}," ",null,"1.sloj",{"$f":"+'Unos podataka'!F4","v":22},{"$f":"45+V117/2","v":56},null,null,null,"PXX",0,{"$f":"+'Analiza i dimenzioniranje'!U67","v":6.0000000000000009},null,null,null,null,null,{"$f":"+Z105","v":6.2644906473896782},{"$f":"+Z106","v":6},{"$f":"+U132","v":0},{"$f":"+AL136","v":{"$error":"#VALUE!"}},null,null,null,-2.4608606627523684,{"$error":"#VALUE!"},6.0000000000000009,{"$error":"#VALUE!"},null,{"$f":"+AU127","v":{"$error":"#VALUE!"}},{"$f":"+AV116","v":1.2},null,"        sa kontraforama: bez kontrafora",null,null,null,"Potresna sila-prosječna"]
[null,null,"Sjecište I. sloja i terena",null,null,null,null,null,null,"X=",{"$f":"+((M117-M116)/(K116-K117))","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+K117*K118+M117","v":{"$error":"#VALUE!"}},null,"X=",{"$f":"+((R117-R116)/(P116-P117))","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+P117*P118+R117","v":{"$error":"#VALUE!"}},null,null,"2.sloj",{"$f":"+'Unos podataka'!G4","v":18},{"$f":"45+V118/2","v":54},null,null,null,null,{"$f":"+AE104","v":{"$error":"#VALUE!"}},{"$f":"+AF104","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!D116,AI117)","v":-5},{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!E116,-8)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},"Y=",{"$f":"(AV117-AU117)/(AV116-AU116)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AU118*AU116+AU117","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Potresna sila","F","G"]
[null,null,"Y=",{"$f":"+AA145","v":-1.4825609685127401},"*x      +",{"$f":"+AC144","v":2.4325765866023956},null,null,null,null,null,null,null,"x","Y",null,null,null,null,null,"3. sloj",{"$f":"+'Unos podataka'!H4","v":20},{"$f":"45+V119/2","v":55},null,null,null,null,{"$f":"-($W$133-AC119)/$U$133","v":-3.3802319074533012},7.31,null,null,null,null,"Y=",{"$f":"(AJ117-AI117)/(AJ116-AI116)","v":{"$error":"#VALUE!"}},"*x            +",{"$f":"-AI119*AI116+AI117","v":{"$error":"#VALUE!"}}," ",{"$f":"+Y101","v":1.75},{"$f":"+AL101","v":9.6153895463470418E-2},null,-3.3802319074533012,{"$error":"#VALUE!"},7.31,{"$error":"#VALUE!"},"Vrijednosti X za poznati Y",null,null,null,null,"Ukupna duljina zida",null,{"$f":"+Kontrafore!E13","v":12},"m",{"$f":"+BA119","v":12},{"$f":"+AE111","v":{"$error":"#VALUE!"}},{"$f":"+AE114","v":{"$error":"#VALUE!"}}]
[null,null,"Y=",{"$f":"+D116","v":{"$error":"#VALUE!"}},"*x      +",{"$f":"+F116","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'C III-V'!P118,'C III-V'!K118)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'C III-V'!R118,'C III-V'!M118)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!D17-'Unos podataka'!$F$9","v":2},null,null,null,null,{"$f":"-($W$133-AC120)/$U$133","v":-3.520593929545047},7.51,null,null,null,null,{"$f":"+T133","v":"Y="},{"$f":"+U133","v":-1.4248868534344206},{"$f":"+V133","v":"*x    +"},{"$f":"+W133","v":2.4935519935102359}," ",{"$f":"+AK102","v":0.97707863658009864},{"$f":"+AL102","v":1.2},null,-3.520593929545047,{"$error":"#VALUE!"},7.51,{"$error":"#VALUE!"},"X=",{"$f":"+AW120/AU118-AW118/AU118","v":{"$error":"#VALUE!"}},"y=",0,null,"ukupna duljina kontrafora",null,{"$f":"+Kontrafore!E5*Kontrafore!E4","v":3},"m",{"$f":"+BA120","v":3},{"$f":"+BD119-BD121","v":{"$error":"#VALUE!"}},{"$f":"IF(BA120=BA119,0,BE119-BE121)","v":{"$error":"#VALUE!"}}]
[null,null,"X=",{"$f":"+(F120-F119)/(D119-D120)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+D119*D121+F119","v":{"$error":"#VALUE!"}},null,null,null,"Jednadžbe pravaca slojeva",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!E17","v":2.8},null,null,null,null,{"$f":"-($W$133-AC121)/$U$133","v":-3.8644808836698235},8,null,null,null,null,"X=",{"$f":"+(AK120-AK119)/(AI119-AI120)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AI120*AI121+AK120","v":{"$error":"#VALUE!"}},null,{"$f":"+AK103","v":-1.0572404418349119},{"$f":"+AL103","v":4},null,-3.8644808836698235,{"$error":"#VALUE!"},8,{"$error":"#VALUE!"},null,null,null,null,null,"ukupna duljina bez kontrafora",null,{"$f":"+BA119-BA120","v":9},"m",{"$f":"+BC119-BC120","v":9},{"$f":"+AC133","v":0},{"$f":"+IF(BC121=0,0,AC136)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!F17","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AK104","v":{"$error":"#VALUE!"}},{"$f":"+AL104","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Jednadžba kombi klizne plohe",null,null,null,null,"površina s kontraforama",null,{"$f":"+BA120/BA119","v":0.25}]
["Presjek kroz zid I",null,"Presjek kroz zid II",null,null,null,null,null,"sloj1.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($AK$119-$AK$123)/AI119","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AK121","v":{"$error":"#VALUE!"}},null,{"$f":"+AK105","v":{"$error":"#VALUE!"}},6.2644906473896782,null,null,null,null,null,null,{"$f":"+AK105","v":{"$error":"#VALUE!"}},{"$f":"+AK101","v":1.75},null,null,"površina bez kontrafora",null,{"$f":"+BA121/BA119","v":0.75},null,{"$f":"-($BC$120/$BC$119)*'Analiza i dimenzioniranje'!$D$83","v":-0.25}]
["x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},6,null,null,null,null,null,null,{"$f":"+AL105","v":6.2644906473896782},0,null,null,null,null,"odnos",null,{"$f":"-($BC$120/$BC$119)*'Analiza i dimenzioniranje'!$D$83","v":-0.25}]
[0,{"$f":"+'Analiza i dimenzioniranje'!R44","v":{"$error":"#VALUE!"}},{"$f":"+A125","v":0},{"$f":"+'Analiza i dimenzioniranje'!Q44","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},6,null,null,null,null,null,"Y=",{"$f":"(AV124-AU124)/(AV123-AU123)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AU125*AU123+AU124","v":{"$error":"#VALUE!"}},null,null,"krak",{"$f":"+AE113","v":{"$error":"#VALUE!"}},{"$f":"+BE119","v":{"$error":"#VALUE!"}},{"$f":"+BE120*BA122","v":{"$error":"#VALUE!"}},null,{"$f":"+BE119-BC126","v":{"$error":"#VALUE!"}}]
[{"$f":"+F83","v":{"$error":"#VALUE!"}},{"$f":"+B125","v":{"$error":"#VALUE!"}},{"$f":"+A126","v":{"$error":"#VALUE!"}},{"$f":"+D125","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($AK$120-AK126)/$AI$120","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AK121","v":{"$error":"#VALUE!"}},null,3.4000000999999997,1.2,null,null,null,null,null,"Vrijednosti X za poznati Y",null,null,null,null,null,null,{"$f":"+AC135","v":0},{"$f":"+BE121","v":0},{"$f":"+BE120*BA123","v":{"$error":"#VALUE!"}},null,{"$f":"+BE121+BC125","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-($AK$120-AK127)/$AI$120","v":-1.1976024639266576},null,4.2,null,{"$f":"+AK109","v":1.75},1.2,null,null,null,null,null,"X=",{"$f":"+AW127/$AU$125-$AW$125/$AU$125","v":{"$error":"#VALUE!"}},"y=",0,null,null,null,null,"Prosječna masa za potres:",null,{"$f":"IF(IF(BA130=BB130,AE114,+BE126)=0,BE125,IF(BA130=BB130,AE114,+BE126))","v":{"$error":"#VALUE!"}},"kn"]
[null,"E1",null,"E2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-($AK$120-AK128)/$AI$120","v":0.90782786744952648},null,1.2,null,{"$f":"+AM119","v":1.75},{"$f":"+AN119","v":9.6153895463470418E-2}]
["x=",{"$f":"+B80","v":12.361875887090893},{"$f":"+C80","v":{"$error":"#VALUE!"}},{"$f":"+D80","v":{"$error":"#VALUE!"}},{"$f":"+E80","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-($AK$120-AK129)/$AI$120","v":{"$error":"#VALUE!"}},null,{"$f":"+AF104","v":{"$error":"#VALUE!"}},null,{"$f":"-0.5*((AM119*AN120-AM120*AN119)+(AM120*AN121-AM121*AN120)+(AM121*AN122-AM122*AN121)+(AM122*AN123-AM123*AN122)+(AM123*AN124-AM124*AN123)+(AM124*AN125-AM125*AN124)+(AM125*AN126-AM126*AN125)+(AM126*AN127-AM127*AN126)+(AM127*AN128-AM128*AN127))","v":{"$error":"#VALUE!"}},"m2"]
["y=",{"$f":"+B81","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+D83","v":{"$error":"#VALUE!"}},{"$f":"+E83","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba pravca klizne plohe",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-($AK$120-AK130)/$AI$120","v":-2.6464828732122183},null,{"$f":"+AI117","v":6.2644906473896782},null,{"$f":"-((AM119*AN120-AM120*AN119)*(AM119+AM120)+(AM120*AN121-AM121*AN120)*(AM120+AM121)+(AM121*AN122-AM122*AN121)*(AM121+AM122)+(AM122*AN123-AM123*AN122)*(AM122+AM123)+(AM123*AN124-AM124*AN123)*(AM123+AM124)+(AM124*AN125-AM125*AN124)*(AM124+AM125)+(AM125*AN126-AM126*AN125)*(AM125+AM126)+(AM126*AN127-AM127*AN126)*(AM126+AM127)+(AM127*AN128-AM128*AN127)*(AM127+AM128))/6/AM129","v":{"$error":"#VALUE!"}},"m  "]
[null,12.361875887090893,{"$error":"#VALUE!"},{"$f":"+D82","v":{"$error":"#VALUE!"}},{"$f":"+E82","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"2+AN113","v":1.75},{"$f":"+AF142","v":-1.0572404418349119},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-((AM119*AN120-AM120*AN119)*(AN119+AN120)+(AM120*AN121-AM121*AN120)*(AN120+AN121)+(AM121*AN122-AM122*AN121)*(AN121+AN122)+(AM122*AN123-AM123*AN122)*(AN122+AN123)+(AM123*AN124-AM124*AN123)*(AN123+AN124)+(AM124*AN125-AM125*AN124)*(AN124+AN125)+(AM125*AN126-AM126*AN125)*(AN125+AN126)+(AM126*AN127-AM127*AN126)*(AN126+AN127)+(AM127*AN128-AM128*AN127)*(AN127+AN128))/6/AM129","v":{"$error":"#VALUE!"}},"m    "]
[null,12.361875887090893,{"$error":"#VALUE!"},{"$f":"+D81","v":{"$error":"#VALUE!"}},{"$f":"+E81","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y=",0,{"$f":"+Z103","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AM129*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"(V132-U132)/(V131-U131)","v":-1.4248868534344206},"*x    +",{"$f":"-U133*U131+U132","v":2.4935519935102359}]
["Jednadžba pravca sloja 1",null,"od",">+",{"$f":"+C129","v":{"$error":"#VALUE!"}},null,">",null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($W$133-V134)/$U$133","v":-1.1133852506716102},{"$f":"+AC111","v":4.08},"y=",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+AK113","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+B130","v":{"$error":"#VALUE!"}},{"$f":"+B132","v":12.361875887090893},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Primjeri;",{"$f":"-($W$133-V135)/$U$133","v":0.76746584535778084},1.4,null,"Položaj djelovanje vert. Sile potresa",null,null,null,null,null,null,null,null,"Dio potresa koji  otpada na temelj:      Ps=",{"$f":"AK114-AE114","v":{"$error":"#VALUE!"}},"kN     y     krak=",{"$f":"+AN119+(AN120-AN119)*0.666666666666667","v":0.83205129848782378},"x","Y",null,null,null,null,null,null,null,null,null,null,null,null,null,"xstv=",{"$f":"+BA134-X113","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+C130","v":{"$error":"#VALUE!"}},{"$f":"+C131","v":{"$error":"#VALUE!"}},null,null,"Visina presjeka",null,"Intezitet",null,null,null,null,null,null,null,"Zid s ili bez kontrafora",null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!E25=0,'C III-V'!AB118,-($W$133-V136)/$U$133)","v":{"$error":"#VALUE!"}},{"$f":"+AC118","v":{"$error":"#VALUE!"}},null,"x","y","koord na zidu",null,null,null,{"$f":"+AE104","v":{"$error":"#VALUE!"}},{"$f":"+AK129","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"+N120","v":{"$error":"#VALUE!"}},{"$f":"+O120","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,"            Masa da se dobije prosječni potres iz čelije AT125=",null,null,null,{"$f":"+BE125","v":{"$error":"#VALUE!"}}]
["Y=",{"$f":"(C136-B136)/(C135-B135)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-B137*B135+B136","v":{"$error":"#VALUE!"}},null,"III",{"$f":"+'Rasprostiranje vertikalnog opt'!V15","v":1.2},{"$f":"IF(G137<C130,+G137/$B$137-$D$137/$B$137,G137/$B$137-$D$137/$B$137)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!H194","v":1.75},{"$f":"+'Unos podataka'!J46","v":9.6153895463470418E-2},null,null,{"$f":"-($W$133-V137)/$U$133","v":-2.4608606627523679},6,null,"koord tećišta",{"$f":"+Y113","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AF104","v":{"$error":"#VALUE!"}},{"$f":"+AH116","v":0}]
["Vrijednosti X za poznati Y",null,"naprimjer za  +c 115",null,null,"VI",{"$f":"+'Rasprostiranje vertikalnog opt'!V16","v":1.52},{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,{"$f":"+Q137","v":1.75},{"$f":"+'Sile i krakovi'!C3","v":1.2},null,null,{"$f":"IF('Analiza i dimenzioniranje'!E27=0,'C III-V'!AB120,-($W$133-V138)/$U$133)","v":-3.1626707732110959},7,null,{"$f":"+'Sile i krakovi'!B99","v":{"$error":"#VALUE!"}},{"$f":"-(Z138-Y137)/X138","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!D99","v":{"$error":"#VALUE!"}},null,null,"Y=",{"$f":"(AE137-AD137)/(AE136-AD136)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AD138*AD136+AD137","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"razlika¸površina",{"$f":"+AE111-AI111","v":{"$error":"#VALUE!"}}]
["X=",{"$f":"+D139/$B$137-$D$137/$B$137","v":{"$error":"#VALUE!"}},"za        y=",3.7,null,"VII",{"$f":"+'Rasprostiranje vertikalnog opt'!V17","v":1.84},{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,{"$f":"+'Sile i krakovi'!B4","v":2},{"$f":"+'Sile i krakovi'!C4","v":1.2},null,null,{"$f":"IF('Analiza i dimenzioniranje'!E28=0,'C III-V'!AB121,-($W$133-V139)/$U$133)","v":-3.8644808836698235},8,null,"razmak od ",{"$f":"2+'Analiza i dimenzioniranje'!E61-'C III-V'!Y138","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"Mmax",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"duljina segmenta",{"$f":"++AJ105","v":0}]
[null,null,null,null,null,"VIII",{"$f":"+'Rasprostiranje vertikalnog opt'!V18","v":2.16},{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,{"$f":"+'Sile i krakovi'!B5","v":2},{"$f":"+'Sile i krakovi'!C5","v":0.12820515121628623},null,null,{"$f":"IF('Analiza i dimenzioniranje'!E29=0,'C III-V'!AB122,-($W$133-V140)/$U$133)","v":-1.0572404418349119},{"$f":"+V132","v":4},null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina I. sloja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"okomito na kliz. Plohu",null,{"$f":"+BA143/BA139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,"IX",{"$f":"+'Rasprostiranje vertikalnog opt'!V19","v":2.48},{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,{"$f":"+'Sile i krakovi'!B6","v":1},{"$f":"+'Sile i krakovi'!C6","v":0},null,null,null,null,null,null,null,"Jednadžba aktivnog klina I. sloja",null,null,null,null,null,"x","y",null,"X=",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"d=","dodatak",{"$f":"+BA140/COS(BA142*PI()/180)","v":{"$error":"#VALUE!"}}]
["Jednadžba pravca sloja 2",null,"od",">+",{"$f":"+E134","v":{"$error":"#VALUE!"}},"X",{"$f":"+'Rasprostiranje vertikalnog opt'!V20","v":2.8},{"$error":"#VALUE!"},null,null,null,null,null,null,null,1,{"$f":"+'Sile i krakovi'!B7","v":2},{"$f":"+'Sile i krakovi'!C7","v":0.12820515121628623},null,null,null,null,null,"koordinate na sjecištu slojeva",null,null,"x","y",null,null,null,{"$f":"+AE103","v":-1.0572404418349119},{"$f":"+AF103","v":4},null,"Y=",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"          kut nagiba klizne plohe za potres   a= ",null,{"$f":"ATAN((-AE104+AE101)/(AF104-AF101))*180/PI()","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+D130","v":{"$error":"#VALUE!"}},{"$f":"+D131","v":{"$error":"#VALUE!"}},null,null,"XI",{"$f":"+'Rasprostiranje vertikalnog opt'!V21","v":3.14},{"$error":"#VALUE!"},null,null,null,null,null,null,null,2,{"$f":"+'Sile i krakovi'!B8","v":2},{"$f":"+'Sile i krakovi'!C8","v":1.2},null,"Jednadžba pravca kosine iza zida",null,null,null,"koordinate na sjecištu s terenom",null,null,{"$f":"+AF142","v":-1.0572404418349119},{"$f":"+'Unos podataka'!$H$7+'Unos podataka'!$J$7","v":4},null,null,null,{"$f":"+AE104","v":{"$error":"#VALUE!"}},{"$f":"+AF104","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dodatna površina",{"$f":"+BA144/'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+E130","v":{"$error":"#VALUE!"}},{"$f":"+E131","v":{"$error":"#VALUE!"}},null,null,"XIII",{"$f":"+'Rasprostiranje vertikalnog opt'!V22","v":3.44},{"$error":"#VALUE!"},null,null,null,null,null,null,null,3,{"$f":"+'Sile i krakovi'!B9","v":3.4000010999999999},{"$f":"+'Sile i krakovi'!C9","v":1.2},null,"x=",{"$f":"+Y107","v":{"$error":"#VALUE!"}},{"$f":"+AE105","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AA143+(AB143-AB144)/TAN((45+'Unos podataka'!F4/2)*PI()/180)","v":-2.5846586698092704},{"$f":"+T102","v":6.2644906473896782},{"$f":"-AA145*AA144+AB144","v":2.4325765866023956},null,"Y=",{"$f":"+(AG143-AG142)/(AF143-AF142)","v":{"$error":"#VALUE!"}},"*x      +",{"$f":"-AF144*AF142+AG142","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"G=",{"$f":"+BC126","v":{"$error":"#VALUE!"}}]
["Y=",{"$f":"(C144-B144)/(C143-B143)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-B145*B143+B144","v":{"$error":"#VALUE!"}},null,"XIII",{"$f":"+'Rasprostiranje vertikalnog opt'!V23","v":3.76},{"$error":"#VALUE!"},null,null,null,null,null,null,null,4,{"$f":"+'Sile i krakovi'!B10","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!C10","v":3.14},null,"y=",{"$f":"+Z107","v":6},{"$f":"U145+(U144-V144)*TAN('Analiza i dimenzioniranje'!$H$20*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,"Y=",{"$f":"+(AB143-AB144)/(AA143-AA144)","v":-1.4825609685127401},"*x      +",null,null,null,"X=",{"$f":"+(AH144-AG146)/(-AF144)","v":{"$error":"#VALUE!"}}]
["Vrijednosti X za poznati Y",null,"naprimjer za  +c 115",null,null,"XIV",{"$f":"+'Rasprostiranje vertikalnog opt'!V24","v":4.08},{"$error":"#VALUE!"},null,null,null,null,null,null,null,5,{"$f":"+'Sile i krakovi'!B11","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!C11","v":3.14},null,"Y=",{"$f":"(V145-U145)/(V144-U144)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-U146*U144+U145","v":{"$error":"#VALUE!"}},null,null,"Jednadžba aktivnog klina II. sloja",null,null,null,null,null,"Y=",{"$f":"+AG153","v":0}]
["X=",{"$f":"+D147/$B$145-$D$145/$B$145","v":{"$error":"#VALUE!"}},"za        y=",3.7,null,"XV",{"$f":"+'Rasprostiranje vertikalnog opt'!V25","v":4.4000000000000004},{"$error":"#VALUE!"},null,null,null,null,null,null,null,6,{"$f":"+'Sile i krakovi'!B12","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!C12","v":3.44},null,"Y=",{"$f":"+U146*V147+W146","v":{"$error":"#VALUE!"}},{"$f":"+Y105","v":{"$error":"#VALUE!"}},null,null,null,null,"x","y",null,null,"Jednadžba aktivnog klina II. sloja"]
[null,null,null,null,null,"XVI",{"$f":"+'Rasprostiranje vertikalnog opt'!V26","v":4.72},{"$error":"#VALUE!"},null,null,null,null,null,null,null,7,{"$f":"+'Sile i krakovi'!B13","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!C13","v":3.44},null,"X=",{"$f":"+U146*W148+W146","v":{"$error":"#VALUE!"}},"y=",-0.56999999999999995,null,null,null,{"$f":"+AA143","v":-1.0572404418349119},{"$f":"+AB143","v":4},null,null,null,"x","y"]
[null,null,null,null,null,"XVII",{"$f":"+'Rasprostiranje vertikalnog opt'!V27","v":5.04},{"$error":"#VALUE!"},null,null,null,null,null,null,null,8,{"$f":"+'Sile i krakovi'!B14","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!C14","v":"A"},null,"sjecište terena i kosine",null,null,null,null,null,null,{"$f":"+AE102","v":0.97707863658009864},{"$f":"+AB157","v":1.2},{"$f":"-AA150*AA148+AB148","v":2.5448333702674724},null,null,{"$f":"+AE102","v":0.97707863658009864},{"$f":"+AF102","v":1.2}]
[null,null,null,null,null,"XVIII",{"$f":"+'Rasprostiranje vertikalnog opt'!V28","v":5.36},{"$error":"#VALUE!"},null,null,null,null,null,null,null,9,{"$f":"+'Sile i krakovi'!B15","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!C15","v":"A"},null,{"$f":"+T133","v":"Y="},{"$f":"+U133","v":-1.4248868534344206},{"$f":"+V133","v":"*x    +"},{"$f":"+W133","v":2.4935519935102359},null,null,"Y=",{"$f":"+(AB149-AB148)/(AA149-AA148)","v":-1.3763819204711734},"*x      +",null,null,null,{"$f":"+AE103","v":-1.0572404418349119},{"$f":"+AF103","v":4}]
[null,null,null,null,null,"XIX",{"$f":"+'Rasprostiranje vertikalnog opt'!V29","v":5.6800000000000006},{"$error":"#VALUE!"},null,null,null,null,null,null,null,10,{"$f":"+'Sile i krakovi'!B16","v":4.2000010999999997},{"$f":"+'Sile i krakovi'!C16","v":1.2},null,{"$f":"+T146","v":"Y="},{"$f":"+U146","v":{"$error":"#VALUE!"}},{"$f":"+V146","v":"*x    +"},{"$f":"+W146","v":{"$error":"#VALUE!"}},null,null,"Jednadžba aktivnog klina III. sloja",null,null,null,null,"Y=",{"$f":"+(AG150-AG149)/(AF150-AF149)","v":-1.3763819204711734},"*x      +",{"$f":"-AF151*AF149+AG149","v":2.5448333702674715}]
[null,null,null,null,null,"XX",{"$f":"+'Rasprostiranje vertikalnog opt'!V30","v":6},{"$error":"#VALUE!"},null,null,null,null,null,null,null,11,{"$f":"+'Sile i krakovi'!B17","v":4.2000010999999997},{"$f":"+'Sile i krakovi'!C17","v":1.2},null,"X=",{"$f":"+(W151-W150)/(U150-U151)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+U151*U152+W151","v":{"$error":"#VALUE!"}},null,null,null,"x","y",null,null,null,"X=",{"$f":"+(AH151-AG153)/(-AF151)","v":1.8489296701865316}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,{"$f":"+'Sile i krakovi'!B18","v":4.2000010999999997},{"$f":"+'Sile i krakovi'!C18","v":1.2},null,null,null,null,null,null,null,null,{"$f":"+B2","v":2},0,null,null,null,"Y=",{"$f":"+AH102","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,{"$f":"+'Sile i krakovi'!B19","v":4.9000021999999994},{"$f":"+'Sile i krakovi'!C19","v":1.2},"Izračun ","y=",{"$f":"+U146*W154+W151","v":{"$error":"#VALUE!"}},"x=",{"$f":"+AE105","v":{"$error":"#VALUE!"}},null,null,null,-5,{"$f":"+(AA153-AA154)*TAN((45+'Unos podataka'!E106/2)*PI()/180)","v":9.9970360471948005},{"$f":"-AA155*AA153+AB153","v":2.8562960134842288},null,"Jednadžba aktivnog klina III. sloja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,{"$f":"+'Sile i krakovi'!B20","v":4.9000021999999994},{"$f":"+'Sile i krakovi'!C20","v":0.5},null,null,{"$f":"+U147*W155+W152","v":{"$error":"#VALUE!"}},"x=",-0.56999999999999995,null,null,"Y=",{"$f":"+(AB154-AB153)/(AA154-AA153)","v":-1.4281480067421144},"*x      +",null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,{"$f":"+'Sile i krakovi'!B21","v":2},{"$f":"+'Sile i krakovi'!C21","v":0.12820515121628623},null,null,null,null,null,null,null,null,"X=",{"$f":"+(AC154-AB157)/(-AA155)","v":1.1597509541483482},null,null,null,{"$f":"+AE101","v":0},{"$f":"+AF101","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rub dna konzole uz aktivni klin","Y=",{"$f":"+AF102","v":1.2},null,null,null,{"$f":"+AE102","v":0.97707863658009864},{"$f":"+AF102","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B6","v":{"$error":"#VALUE!"}},{"$f":"+C6","v":3.14},null,null,"Y=",{"$f":"+(AG157-AG156)/(AF157-AF156)","v":1.2281508929518252},"*x      +",{"$f":"-AF158*AF156+AG156","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AH158-AG160)/(-AF158)","v":0.97707863658009853}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AC144","v":2.4325765866023956},null,null,"Y=",{"$f":"+AF102","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1. sloj    Y=",{"$f":"+AA145","v":-1.4825609685127401},{"$f":"+AB145","v":"*x      +"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+AB98","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AC160-AB162)/(-AA161)","v":{"$error":"#VALUE!"}},{"$f":"+AC149","v":2.5448333702674724}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2. sloj    Y=",{"$f":"+AA150","v":-1.3763819204711734},{"$f":"+AB150","v":"*x      +"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+AB162","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AC163-AB165)/(-AA164)","v":{"$error":"#VALUE!"}}]

{"sheet":"C VI-VII","index":40,"n_rows":157,"n_cols":61,"rows_kept":157,"cut":false,"hidden":true,"merged":[[125,45,125,48],[139,37,139,38],[115,42,116,42],[116,55,116,57],[96,24,97,25],[96,32,98,33],[96,34,98,35],[96,36,98,37],[99,32,99,33],[99,34,99,35],[99,36,99,37],[110,38,113,38],[110,39,111,40],[112,39,113,39],[112,40,113,40],[114,34,114,35],[10,27,10,28],[11,3,11,4],[12,27,12,28],[17,27,17,28],[16,27,16,28],[0,9,0,10],[1,5,1,8],[10,3,10,4],[42,1,42,2],[42,3,42,4],[42,5,42,6],[0,1,0,2],[0,3,0,4],[0,5,0,7],[42,7,43,10],[44,7,44,8],[13,29,13,30],[13,12,13,16],[26,27,26,28],[44,21,44,22],[42,15,43,18],[44,15,44,16],[44,17,44,18],[17,12,17,16],[13,27,13,28],[44,9,44,10],[44,11,44,12],[44,13,44,14],[42,11,43,14],[151,27,151,30],[77,1,77,2],[90,1,90,2],[90,3,90,4],[90,5,90,6],[77,3,77,4],[77,5,77,6],[77,8,77,9],[77,10,77,11],[77,15,77,16],[99,24,99,25],[99,30,99,31],[112,5,112,6],[139,27,139,30],[99,26,99,27],[99,28,99,29],[94,0,94,1],[77,13,77,14],[114,36,114,37],[62,29,62,30],[146,27,146,30],[67,15,67,16],[67,20,67,21],[67,22,67,23],[62,27,62,28],[96,22,97,23],[67,1,67,2],[67,3,67,4],[67,5,67,6],[67,8,67,9],[67,13,67,14],[67,10,67,11],[98,9,99,12],[103,9,103,12],[105,9,105,12],[109,9,109,12],[96,20,98,21]]}
["Točke","ZID I TEMELJ",null,"NASIP NA TEMELJU IZA",null,"ZID, KONZOLA I NASIP NA KONZOLI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Točka A",null,"Presjek I-I"]
[1,2,{"$f":"+'C III-V'!$C$2","v":0.12820515121628623},null,null," ZA BILO KOJI PRESJEK ",null,null,null,null,null,null,null,null,null,null,null,"Presjek zid Iv",{"$f":"+($B$9-$B$4)*(T2-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},{"$f":"+B15","v":4.9000021999999994},{"$f":"+C15","v":0.5},{"$f":"+'C VI-VII'!B10+0.05","v":{"$error":"#VALUE!"}},-0.5]
[2,2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T3-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},"Točka B",null,{"$f":"+W2","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!C10+0.5","v":{"$error":"#VALUE!"}}]
[3,{"$f":"+B3+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+C3","v":1.2},{"$f":"+B19","v":2},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>C4,B21,B4)","v":3.4000010999999999},{"$f":"IF(E20>C4,E20,C4)","v":1.2},{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},null,null,null,null,null,null,null,null,"Presjek V",{"$f":"+($B$9-$B$4)*(T4-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},{"$f":"+'C VI-VII'!B2","v":2},{"$f":"+'C VI-VII'!C2","v":0.12820515121628623}]
[4,{"$f":"+B23","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},{"$f":"+D4","v":2},{"$f":"+'C III-V'!E5","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,B21,B5)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,E20,C5)","v":3.14},{"$f":"+F8","v":{"$error":"#VALUE!"}},{"$f":"+G8","v":3.44},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T5-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},null,null,"Presjek II-II",null,null,null,"Nasip na zidu iza"]
[5,{"$f":"+B5-'Analiza i dimenzioniranje'!G78","v":{"$error":"#VALUE!"}},{"$f":"+C5","v":3.14},{"$f":"IF(B6<2,B5,IF(B9>2,B9,D5))","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!E6","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C7,B21,B6)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C6,E20,C6)","v":3.14},{"$f":"IF(F7>F9,H5,F9)","v":{"$error":"#VALUE!"}},{"$f":"IF(F7>F9,I5,IF(E20>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C VI-VII'!E20,G9))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"Presjek VI",{"$f":"+($B$9-$B$4)*(T6-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},"TLO 1. sloj",null,{"$f":"+'C VI-VII'!B15-0.05","v":4.8500021999999996},{"$f":"+'C VI-VII'!X2","v":-0.5},null,null,2,{"$f":"IF('Analiza i dimenzioniranje'!AW26>'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AW26)","v":0}]
[6,{"$f":"IF('Analiza i dimenzioniranje'!G78=0,'C VI-VII'!B8,B6)","v":{"$error":"#VALUE!"}},{"$f":"C6+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+B4","v":3.4000010999999999},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>=C7,B21,B7)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C7,E20,C7)","v":3.44},{"$f":"IF(F7>F9,H6,H6)","v":{"$error":"#VALUE!"}},{"$f":"+I6","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T7-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},{"$f":"+'C VI-VII'!B15-0.05","v":4.8500021999999996},{"$f":"+'C VI-VII'!X3","v":{"$error":"#VALUE!"}},"Horizontala",null,2,{"$f":"'Analiza i dimenzioniranje'!BF28","v":0}]
[7,{"$f":"+B22","v":{"$error":"#VALUE!"}},{"$f":"+C7","v":3.44},{"$f":"+D4","v":2},{"$f":"+E4","v":1.2},{"$f":"IF(E20>C8,B21,B8)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C8,E20,C8)","v":3.44},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$H$15=0,I7+(H7-H8)*'Unos podataka'!R57,IF('C III-V'!H9>'Unos podataka'!$B$105,I7+(H7-H8)*'Unos podataka'!$R$55,'Unos podataka'!$T$57))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"Presjek VII",{"$f":"+($B$9-$B$4)*(T8-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!V8","v":6},null,null,{"$f":"+'C VI-VII'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!C5","v":3.14}]
[8,{"$f":"B4-TAN('Analiza i dimenzioniranje'!H51*PI()/180)*('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},null,null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"+I4","v":3.44},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T9-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},{"$f":"+U8-'Analiza i dimenzioniranje'!E27","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!V9","v":6.2644906473896782},"Presjek ZID",null,{"$f":"+IF('Analiza i dimenzioniranje'!$E$24=0,0,'C VI-VII'!Y4)","v":0},{"$f":"+Z8","v":3.14}]
[9,{"$f":"+B9+'Analiza i dimenzioniranje'!E54","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},null,null,{"$f":"+B10","v":{"$error":"#VALUE!"}},{"$f":"+C10","v":"A"},null,null,null,null,null,null,null,null,null,null,"Presjek VIII",{"$f":"+($B$9-$B$4)*(T10-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},-8,{"$f":"+'C III-V'!V10","v":6.2644906473896782},{"$f":"+'C VI-VII'!B15-0.5","v":4.4000021999999994},{"$f":"+'C VI-VII'!C10+0.1","v":{"$error":"#VALUE!"}}]
[10,{"$f":"+B4+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+C3","v":1.2},"NASIP NA KONZOLI",null,{"$f":"+F12+E65","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C11,E20,C11)","v":1.2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T11-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},"x","y",{"$f":"+'C VI-VII'!B10+0.5","v":{"$error":"#VALUE!"}},{"$f":"+X10","v":{"$error":"#VALUE!"}},null,null,null,"Rsidra"]
[11,{"$f":"+B11","v":4.2000010999999997},{"$f":"+C11","v":1.2},"za stabilnost",null,{"$f":"+F4","v":3.4000010999999999},{"$f":"+G4","v":1.2},null,null,null,null,null,null,null,null,null,null,"Presjek IX",{"$f":"+($B$9-$B$4)*(T12-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+W23","v":{"$error":"#VALUE!"}},{"$f":"+U12*(V9-V8)/(U9-U8)-U8*(V9-V8)/(U9-U8)+V8","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,20,AB16)","v":20},{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,0,AC16)","v":0}]
[12,{"$f":"+B12","v":4.2000010999999997},{"$f":"+C12","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T13-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+W25","v":{"$error":"#VALUE!"}},{"$f":"+U13*(V9-V8)/(U9-U8)-U8*(V9-V8)/(U9-U8)+V8","v":{"$error":"#VALUE!"}},"Pad terena niz padinu",null,null,null,null,"Os rezultante sidara Ukupna računska sila u sidrima"]
[13,{"$f":"+B11+'Analiza i dimenzioniranje'!G57","v":4.9000021999999994},{"$f":"+C13","v":1.2},{"$f":"+H4","v":{"$error":"#VALUE!"}},3.44,null,null,null,null,"Linija presjeka",null,null," Koordinata sredine presjeka",null,null,null,null,"Presjek X",{"$f":"+($B$9-$B$4)*(T14-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},"TLO 2. sloj",null,{"$f":"+'Analiza i dimenzioniranje'!Q105","v":3},{"$f":"+'Analiza i dimenzioniranje'!P105","v":{"$error":"#VALUE!"}},null,null,null,"Slobodna  zona.",null,"1. sloj"]
[14,{"$f":"+B14","v":4.9000021999999994},{"$f":"+C14-'Analiza i dimenzioniranje'!E51","v":0.5},{"$error":"#VALUE!"},3.44,{"$f":"IF((B4-B9)=0,0,+(C9-C4)/(B4-B9))","v":{"$error":"#VALUE!"}},"n  Nagib zida u tlu",null,null,0,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,"III-III","konzola","Presjek I","Presjek II",null,{"$f":"+($B$11-$B$10)*(T15-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},{"$f":"IF(('Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17)<'Analiza i dimenzioniranje'!$F$45,2,(IF(B7<B24,B7,IF('Analiza i dimenzioniranje'!G78=0,'C VI-VII'!B24,2))))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17","v":4},{"$f":"+'Analiza i dimenzioniranje'!O130","v":7.1000021999999996},{"$f":"+'Analiza i dimenzioniranje'!N130","v":1.5001009999999999},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,AB24)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,'Analiza i dimenzioniranje'!P22)","v":5},{"$f":"+U9","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782}]
[15,{"$f":"+B2","v":2},{"$f":"+C2","v":0.12820515121628623},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,null,3,{"$f":"+K15","v":1.2},null,"x",{"$f":"+(F12+F11)/2","v":{"$error":"#VALUE!"}},{"$f":"(B8+(B11-B10)*(O17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U29+(B11-B10)*(P17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U34+(B11-B10)*(Q17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},"Presjek XI",{"$f":"+($B$9-$B$4)*(T16-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},-8,{"$f":"+V15+(U15-U16)*TAN('Analiza i dimenzioniranje'!$E$18*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"AB15-'Analiza i dimenzioniranje'!P23","v":{"$error":"#VALUE!"}},{"$f":"+AC15-(AB15-AB16)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782}]
[null,null,"Jednadžba pravca zida uz tlo",{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,null,"Sloj 2 gore",null,null,"y",{"$f":"+G11","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},null,{"$f":"+($B$11-$B$10)*(T17-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},"TLO 3. sloj",null,"Prometno opterećenje",null,null,null,null,"Sidrena dionica",null,"Jednadžba površine terena"]
[null,"x","y",{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,null,{"$f":"+F94","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E52>=G94,0,G94)","v":4},null,null,null,null,null,null,"Presjek XII",{"$f":"+($B$9-$B$4)*(T18-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},2,{"$f":"+'Analiza i dimenzioniranje'!$F$17","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,+'C VI-VII'!B9-'Analiza i dimenzioniranje'!E26)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,'C VI-VII'!V9)","v":6.2644906473896782},null,null,null,"                   Y=",null,{"$f":"+(AE16-AE15)/(AD16-AD15)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AD18*AD15+AE15","v":{"$error":"#VALUE!"}}]
[null,2,{"$f":"+B19*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},3.44,null,null,null,null,{"$f":"U16","v":-8},{"$f":"+K18","v":4},null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T19-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},-8,{"$f":"+V18+(U18-U19)*TAN('Analiza i dimenzioniranje'!$F$18*PI()/180)","v":1.5492076949174773},{"$f":"+W18","v":{"$error":"#VALUE!"}},{"$f":"+X18+'Analiza i dimenzioniranje'!E24/50","v":6.4644906473896784},null,null,null,{"$f":"+AB16","v":{"$error":"#VALUE!"}},{"$f":"+AC16","v":{"$error":"#VALUE!"}},"za x=",{"$f":"+AB20","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+H8","v":{"$error":"#VALUE!"}},{"$f":"+B20*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},"M na koti",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,"Sloj 1 ili2 dole",null,null,null,null,null,null,{"$f":"+(B11-B10)*(Q21-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},"Presjek XIII",{"$f":"+($B$9-$B$4)*(T20-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},"KONTAKTNI NAPONI",null,{"$f":"+W18-'Analiza i dimenzioniranje'!E25","v":{"$error":"#VALUE!"}},{"$f":"+X19","v":6.4644906473896784},null,null,null,{"$f":"+(AB21+AB19)/2","v":{"$error":"#VALUE!"}},{"$f":"+(AC19+AC21)/2","v":{"$error":"#VALUE!"}},"y=",{"$f":"+AD18*AE19+AF18","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C21-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,{"$f":"+IF('Analiza i dimenzioniranje'!G78=0,D8,H8)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+F95","v":{"$error":"#VALUE!"}},{"$f":"+G12","v":1.2},null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,{"$f":"+($B$11-$B$10)*(T21-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},2,0,{"$f":"+W20","v":{"$error":"#VALUE!"}},{"$f":"+X18","v":6.2644906473896782},null,null,null,{"$f":"+AB19-'Analiza i dimenzioniranje'!P24","v":{"$error":"#VALUE!"}},{"$f":"+AC19-(AB19-AB21)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},"visina sloja iznad centra sidra"]
[null,{"$f":"+(B9-B4)*(C22-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+C23+'Analiza i dimenzioniranje'!C77","v":3.44},null,null,null,null,null,null,{"$f":"+U19","v":-8},{"$f":"+K21","v":1.2},null,null,null,null,null,null,"Presjek XIV",{"$f":"+($B$9-$B$4)*(T22-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},2,{"$f":"-'Analiza i dimenzioniranje'!$F$193/100","v":{"$error":"#VALUE!"}},"Točkasto",null,null,null,null,null,null,{"$f":"+AE20-AC20","v":{"$error":"#VALUE!"}},"m"]
[null,{"$f":"+(B9-B4)*(C23-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T23-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"2+'Analiza i dimenzioniranje'!$E$61","v":4.9000021999999994},{"$f":"-'Analiza i dimenzioniranje'!$F$190/100","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E36=0,-10,B9-'Analiza i dimenzioniranje'!E37)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X23","v":{"$error":"#VALUE!"}},null,null,null,"Jednadžba  lica zida "]
[null,{"$f":"+(B9-B4)*(C24-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V15","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek XV",{"$f":"+($B$9-$B$4)*(T24-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U23","v":4.9000021999999994},0,"Linijsko iza zida",null,null,null,"x=",{"$f":"+($B$11-$B$10)*(AB25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+($B$11-$B$10)*(AC25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+(B11-B10)*(AE25-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C25-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U21","v":2},0,{"$f":"IF('Analiza i dimenzioniranje'!$E$34=0,0,B9-'Analiza i dimenzioniranje'!K28)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X27","v":{"$error":"#VALUE!"}},null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!V42","v":170.21276595744681},{"$f":"+'Analiza i dimenzioniranje'!W42","v":170.21276595744681},null,{"$f":"+'Analiza i dimenzioniranje'!H76+'Analiza i dimenzioniranje'!E52","v":1.5001009999999999}]
[null,{"$f":"+(B9-B4)*(C26-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid VII-VII",{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},{"$f":"+W25","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$34=0,0,X25+1)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!T22","v":0},null,null,null,null,{"$f":"+B14-AE24","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C27-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},"TEMELJ -opterećenje",null,"x=",{"$f":"+($B$11-$B$10)*(Z26-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"Rez. Sidra na zidu"]
[null,{"$f":"+(B9-B4)*(C26-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V27","v":1.84},{"$f":"+IF('Analiza i dimenzioniranje'!E28=0,0,W29)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9+'Analiza i dimenzioniranje'!F20+1.5)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!S22","v":0}]
["Sjecište s dnom temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V29-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":1.84},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W30-0.3)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X30)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z28-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+($B$11-$B$10)*(AC29-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E40","v":3.9999999960000001},{"$f":"+AB29+0.4","v":{"$error":"#VALUE!"}},{"$f":"+AC29+(AD29-AB29)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}}]
["zid",{"$f":"+B20","v":{"$error":"#VALUE!"}},{"$f":"+B30*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V30-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":1.84},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,B9-'Analiza i dimenzioniranje'!$E$32)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X31+'Analiza i dimenzioniranje'!E33)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!R22","v":0},null,null,null,{"$f":"+AB29-1","v":{"$error":"#VALUE!"}},{"$f":"+AC29-(AB29-AD30)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}}]
["Vrh zida",{"$f":"+(B9-B4)*(C31-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C558","v":-0.45},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid Iv",{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},{"$f":"+W30","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9-'Analiza i dimenzioniranje'!K31)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z30-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"nagib lica"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,W31-'Analiza i dimenzioniranje'!$E$29)","v":{"$error":"#VALUE!"}},{"$f":"+X31","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q22","v":3},null,"tan"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V32","v":1.52},{"$f":"+W32","v":{"$error":"#VALUE!"}},{"$f":"+X30","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z32-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+(B13-B10)/(C10-C13)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V34-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V33","v":1.52},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W33+0.3)","v":{"$error":"#VALUE!"}},{"$f":"+X29","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q20","v":5},null,"kut"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V35-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V34","v":1.52},{"$f":"+W34","v":{"$error":"#VALUE!"}},{"$f":"+X28","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z34-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+ATAN(AB33)*180/PI()","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SIDRO za presjek",null,null,null,"Jednadžba pravca lica zida ",null,null,"Sjecište a arm konzole",null,"vrh zida","Anker armatura uz lice",null,"arm dno",null,"Y=",{"$f":"IF(AE38=AE37,1000000,(AF38-AF37)/(AE38-AE37))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AJ36*AE37+AF37","v":{"$error":"#VALUE!"}},null,null,null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!$C$545","v":1.6923077248520526}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB15)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC15)","v":5},null,null,"x=",null,null,{"$f":"+(B11-B10)*(AB38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},null,{"$f":"+(B11-B10)*(AD38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AF37-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!B545","v":{"$error":"#VALUE!"}},{"$f":"+U81","v":2.0499999999999998},{"$f":"+V81","v":0.18682583433163008},"X=",{"$f":"+(-AL36+AL39)/(AJ36-AJ39)","v":{"$error":"#VALUE!"}},"sjeište",null,null,null,null,null,"x=",{"$f":"+(AR36-AL36)/AJ36","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB16)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC16)","v":{"$error":"#VALUE!"}},null,null,"y=",null,null,{"$f":"+'Analiza i dimenzioniranje'!E555","v":3.39},null,{"$f":"+'Analiza i dimenzioniranje'!C558","v":-0.45},{"$f":"+(B11-B10)*(AF38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+U82","v":4.8600021999999994},{"$f":"+V82","v":0.54310345350772504},"Y=",{"$f":"+AJ36*AJ37+AL36","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate dna temelja",null,null,null,null,null,null,"Y=",{"$f":"+(AH38-AH37)/(AG38-AG37)","v":0.12678908905341604},"*x",{"$f":"-AJ39*AG37+AH37","v":-7.3091798227872762E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"lice","koord Pr II",{"$f":"+AB47+'Analiza i dimenzioniranje'!Q58","v":3.4500010999999997},{"$f":"(AB40*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24999999999999994},null,"SIDRO"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+(B11-B10)*(Z42-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+B8","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+AB15","v":{"$error":"#VALUE!"}},{"$f":"+AC15","v":5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+P59-L59","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+Z42","v":3.44},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,AB15-0.5)","v":{"$error":"#VALUE!"}},{"$f":"+AF41-(AE41-AE42)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},null,"Nasip ispred zida"]
["Oznaka","temelj",null,"Zid i konzola za pr. ZID",null,"Nasip na temelju iza zida",null,"      Za momente u presjeku zid-temelj          ",null,null,null,"      Za momente u presjeku VI-VI",null,null,null,"         Za momente u presjeku VII-VII",null,null,null,null,1,null,null,null,null,null,null,2,0,null,null,null,null,{"$f":"+AE24","v":{"$error":"#VALUE!"}},{"$f":"+C11+'Analiza i dimenzioniranje'!$H$76","v":1.5001009999999999}]
["točke","x","y","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - BETON",null,null,null,null,null,2.65,{"$f":"+(AC47+AC49)/2","v":0.31034478180740688},null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!$E$61","v":4.9000021999999994},{"$f":"+AI43","v":1.5001009999999999}]
[1,{"$f":"+'C VI-VII'!B2","v":2},{"$f":"+'C VI-VII'!C2","v":0.12820515121628623},null,null,null,null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"Kontaktni naponi za stab",null,"Beton do presjeka II-II",null,"Beton sredine temelja",null,"Beton do presjeka I-I",null,{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"(AB45*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH44+1.6","v":6.5000021999999991},{"$f":"+AI44-(AH45-AH44)*TAN('Analiza i dimenzioniranje'!H22*PI()/180)","v":1.5001009999999999}]
[2,{"$f":"+'C VI-VII'!B3","v":2},{"$f":"+'C VI-VII'!C3","v":1.2},null,null,null,null,"x","y","x","y","x","y","x","y","x","y","x","y","x","y",null,null,"x","y","x","y",{"$f":"+(AB43+AB47)/2","v":2.7000005499999999},{"$f":"(AB46*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.1206896584423281},null,null,null,null,"x","y"]
[3,{"$f":"+'C VI-VII'!B4","v":3.4000010999999999},{"$f":"+'C VI-VII'!C4","v":1.2},{"$f":"+B4","v":3.4000010999999999},1.2,2,1.2,3.4000010999999999,1.2,{"$f":"+D14","v":{"$error":"#VALUE!"}},3.44,{"$f":"+U34","v":{"$error":"#VALUE!"}},{"$f":"+V34","v":1.52},{"$f":"+J47","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!V44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!V44,K47)","v":3.44},{"$f":"+U29","v":{"$error":"#VALUE!"}},{"$f":"+V29","v":1.84},{"$f":"+J47","v":{"$error":"#VALUE!"}},{"$f":"+S48","v":3.44},{"$f":"+U21","v":2},{"$f":"+V21*100","v":0},2,0,{"$f":"+B4","v":3.4000010999999999},{"$f":"+W49","v":1.2},{"$f":"+B11","v":4.2000010999999997},1.2,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"(AB47*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24137931688465614},"Presjek II-II",null,null,null,{"$f":"+'C VI-VII'!B11","v":4.2000010999999997},{"$f":"+C11","v":1.2}]
[4,{"$f":"+B11","v":4.2000010999999997},1.2,{"$error":"#VALUE!"},3.14,2,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.44,{"$f":"+H48","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!V44<'Analiza i dimenzioniranje'!F45,I48,'C VI-VII'!V34)","v":3.14},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!V44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!V44,K48)","v":3.44},{"$f":"+H48","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!W44<'Analiza i dimenzioniranje'!F45,I48,V29)","v":3.14},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!W44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!W44,K48)","v":3.44},{"$f":"+U22","v":2},{"$f":"+V22*100","v":{"$error":"#VALUE!"}},2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+X47+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+Y47","v":1.2},4.2000010999999997,1.2,{"$f":"+AB77","v":{"$error":"#VALUE!"}},{"$f":"(AB48*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47+'Analiza i dimenzioniranje'!H76","v":1.5001009999999999}]
[5,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.14,{"$f":"+'Unos podataka'!$B$104","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.14,{"$f":"+F49","v":{"$error":"#VALUE!"}},{"$f":"+E16+'Unos podataka'!$F9","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!V44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C VI-VII'!L47,'C VI-VII'!B6)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!V44<'Analiza i dimenzioniranje'!F45,I49,'C VI-VII'!V34)","v":3.14},{"$f":"+J49","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!V44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!V44,K49)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!W44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C VI-VII'!B6,P47)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!W44<'Analiza i dimenzioniranje'!F45,'C VI-VII'!I49,Q48)","v":3.14},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!W44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!W44,K49)","v":{"$error":"#VALUE!"}},{"$f":"+U23","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},{"$f":"+V48+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+W48","v":1.2},{"$f":"+AB49","v":4.2000010999999997},{"$f":"+AC49","v":0.37931024673015767},4.2000010999999997,1.2,{"$f":"+AB47+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+(AB49*(AC43-AC53)/(AB43-AB53)-AB53*(AC43-AC53)/(AB43-AB53)+AC53)","v":0.37931024673015767},"Presjek I-I",null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+AI48","v":1.5001009999999999}]
[6,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.44,3.4000010999999999,1.2,{"$error":"#VALUE!"},3.44,{"$f":"IF('Unos podataka'!$B$105>J47,'Unos podataka'!$B$105,J47)","v":{"$error":"#VALUE!"}},{"$f":"+K51","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!V44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C VI-VII'!L48,'C VI-VII'!B7)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!V44<='Analiza i dimenzioniranje'!F45,I50,'C VI-VII'!V34)","v":3.44},{"$f":"IF('Unos podataka'!$B$105>N47,'Unos podataka'!$B$105,N47)","v":{"$error":"#VALUE!"}},{"$f":"+O51","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!W44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C VI-VII'!P47,H50)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!W44<='Analiza i dimenzioniranje'!F45,I50,V29)","v":3.44},{"$f":"IF('Unos podataka'!$B$105>R47,'Unos podataka'!$B$105,R47)","v":{"$error":"#VALUE!"}},{"$f":"+S51","v":{"$error":"#VALUE!"}},{"$f":"+U24","v":4.9000021999999994},{"$f":"+V24*100","v":0},{"$f":"+V49","v":3.4000010999999999},{"$f":"+AC47","v":0.24137931688465614},{"$f":"+X47","v":3.4000010999999999},{"$f":"+AC47","v":0.24137931688465614},4.9000021999999994,1.2,{"$f":"2+'Analiza i dimenzioniranje'!E61/2","v":3.4500010999999997},{"$f":"(AB50*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24999999999999994},null,null,null,null,{"$f":"+AH49","v":4.9000021999999994},{"$f":"+C14","v":1.2}]
[7,4.9000021999999994,1.2,{"$error":"#VALUE!"},3.44,2,1.2,{"$error":"#VALUE!"},3.44,{"$error":"#VALUE!"},{"$f":"+E18+'Unos podataka'!$F9","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!V44>'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C VI-VII'!B28,B8)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!V44>='Analiza i dimenzioniranje'!I75+'Analiza i dimenzioniranje'!G67,'C VI-VII'!M50,Z26)","v":3.44},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!V44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!V44,K51)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!W44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C VI-VII'!B25,H51)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!W44<='Analiza i dimenzioniranje'!F45,I51,V29)","v":3.44},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!W44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!W44,K51)","v":{"$error":"#VALUE!"}},{"$f":"+U25","v":2},{"$f":"+V25*100","v":0},{"$f":"+V47","v":2},{"$f":"+W47","v":0},{"$f":"+X47","v":3.4000010999999999},{"$f":"+Y47","v":1.2},4.9000021999999994,0.5,{"$f":"+(AB49+AB53)/2","v":4.5500016499999996},{"$f":"(AB51*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.43965512336507878},null,null,null,null,{"$f":"+B13","v":4.2000010999999997},{"$f":"+C13","v":1.2}]
[8,4.9000021999999994,0.5,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",{"$error":"#VALUE!"},3.44,{"$f":"+H52","v":{"$error":"#VALUE!"}},{"$f":"+Q52","v":"A"},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!V44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!V44,K52)","v":3.44},{"$f":"+H52","v":{"$error":"#VALUE!"}},{"$f":"+I52","v":"A"},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!W44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!W44,K52)","v":3.44},null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AC49","v":0.37931024673015767},{"$f":"+AD77","v":{"$error":"#VALUE!"}},{"$f":"(AB52*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH51","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[9,2,0.12820515121628623,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",null,null,{"$f":"+H53","v":{"$error":"#VALUE!"}},{"$f":"+Q53","v":"A"},null,null,{"$f":"+H53","v":{"$error":"#VALUE!"}},{"$f":"+I53","v":"A"},null,null,null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AA47","v":1.2},{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+C15","v":0.5},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[10,null,null,4.2000010999999997,1.2,null,null,{"$error":"#VALUE!"},1.2,null,null,{"$f":"+U35","v":{"$error":"#VALUE!"}},{"$f":"+M47","v":1.52},null,null,{"$f":"+U30","v":{"$error":"#VALUE!"}},{"$f":"+V30","v":1.84},null,null,null,null,null,null,null,null,null,null,"Koordinate s","naprezanjem"]
[11,null,null,{"$f":"+D47","v":3.4000010999999999},{"$f":"+E47","v":1.2},null,null,3.4000010999999999,1.2,null,null,{"$f":"+L47","v":{"$error":"#VALUE!"}},{"$f":"+M47","v":1.52},null,null,{"$f":"+P47","v":{"$error":"#VALUE!"}},{"$f":"+Q47","v":1.84},null,null,null,null,null,null,null,null,null,null,{"$f":"+U22","v":2},{"$f":"+V22*100","v":{"$error":"#VALUE!"}}]
[12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+AB56*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
[13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AB57*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
["  A=",{"$f":"-0.5*((B45*C46-B46*C45)+(B46*C47-B47*C46)+(B47*C48-B48*C47)+(B48*C49-B49*C48)+(B49*C50-B50*C49)+(B50*C51-B51*C50)+(B51*C52-B52*C51)+(B52*C53-B53*C52))","v":2.5691044797107181},"m2",{"$f":"-0.5*((D45*E46-D46*E45)+(D46*E47-D47*E46)+(D47*E48-D48*E47)+(D48*E49-D49*E48)+(D49*E50-D50*E49)+(D50*E51-D51*E50)+(D51*E52-D52*E51)+(D52*E53-D53*E52)+(D53*E54-D54*E53)+(D54*E55-D55*E54)+(D55*E56-D56*E55)+(D56*E57-D57*E56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((F45*G46-F46*G45)+(F46*G47-F47*G46)+(F47*G48-F48*G47)+(F48*G49-F49*G48)+(F49*G50-F50*G49)+(F50*G51-F51*G50)+(F51*G52-F52*G51)+(F52*G53-F53*G52)+(F53*G54-F54*G53)+(F54*G55-F55*G54)+(F55*G56-F56*G55)+(F56*G57-F57*G56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((H47*I48-H48*I47)+(H48*I49-H49*I48)+(H49*I50-H50*I49)+(H50*I51-H51*I50)+(H51*I52-H52*I51)+(H52*I53-H53*I52)+(H53*I54-H54*I53)+(H54*I55-H55*I54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((J47*K48-J48*K47)+(J48*K49-J49*K48)+(J49*K50-J50*K49)+(J50*K51-J51*K50)+(J51*K52-J52*K51)+(J52*K53-J53*K52)+(J53*K54-J54*K53)+(J54*K55-J55*K54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((L47*M48-L48*M47)+(L48*M49-L49*M48)+(L49*M50-L50*M49)+(L50*M51-L51*M50)+(L51*M52-L52*M51)+(L52*M53-L53*M52)+(L53*M54-L54*M53)+(L54*M55-L55*M54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((N47*O48-N48*O47)+(N48*O49-N49*O48)+(N49*O50-N50*O49)+(N50*O51-N51*O50)+(N51*O52-N52*O51)+(N52*O53-N53*O52)+(N53*O54-N54*O53)+(N54*O55-N55*O54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((P47*Q48-P48*Q47)+(P48*Q49-P49*Q48)+(P49*Q50-P50*Q49)+(P50*Q51-P51*Q50)+(P51*Q52-P52*Q51)+(P52*Q53-P53*Q52)+(P53*Q54-P54*Q53)+(P54*Q55-P55*Q54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((R47*S48-R48*S47)+(R48*S49-R49*S48)+(R49*S50-R50*S49)+(R50*S51-R51*S50)+(R51*S52-R52*S51)+(R52*S53-R53*S52)+(R53*S54-R54*S53)+(R54*S55-R55*S54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((T47*U48-T48*U47)+(T48*U49-T49*U48)+(T49*U50-T50*U49)+(T50*U51-T51*U50)+(T51*U52-T52*U51)+(T52*U53-T53*U52)+(T53*U54-T54*U53)+(T54*U55-T55*U54))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((V47*W48-V48*W47)+(V48*W49-V49*W48)+(V49*W50-V50*W49)+(V50*W51-V51*W50))","v":1.5110356654221164},"m2",{"$f":"-0.5*((X47*Y48-X48*Y47)+(X48*Y49-X49*Y48)+(X49*Y50-X50*Y49)+(X50*Y51-X51*Y50))","v":0.71172417455407389},"m2",{"$f":"-0.5*((Z47*AA48-Z48*AA47)+(Z48*AA49-Z49*AA48)+(Z49*AA50-Z50*AA49)+(Z50*AA51-Z51*AA50)+(Z51*AA52-Z52*AA51)+(Z52*AA53-Z53*AA52)+(Z53*AA54-Z54*AA53)+(Z54*AA55-Z55*AA54))","v":0.53224225002380887},"m2",{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-0.5*((AH47*AI48-AH48*AI47)+(AH48*AI49-AH49*AI48)+(AH49*AI50-AH50*AI49)+(AH50*AI51-AH51*AI50)+(AH51*AI52-AH52*AI51)+(AH52*AI53-AH53*AI52)+(AH53*AI54-AH54*AI53)+(AH54*AI55-AH55*AI54))","v":0.21007103011109951},"m2"]
["xt=",{"$f":"-((B45*C46-B46*C45)*(B45+B46)+(B46*C47-B47*C46)*(B46+B47)+(B47*C48-B48*C47)*(B47+B48)+(B48*C49-B49*C48)*(B48+B49)+(B49*C50-B50*C49)*(B49+B50)+(B50*C51-B51*C50)*(B50+B51)+(B51*C52-B52*C51)*(B51+B52)+(B52*C53-B53*C52)*(B52+B53)+(B53*C54-B54*C53)*(B53+B54)+(B54*C55-B55*C54)*(B54+B55)+(B55*C56-B56*C55)*(B55+B56)+(B56*C57-B57*C56)*(B56+B57))/6/B58","v":3.3485779696489133},"m",{"$f":"-((D45*E46-D46*E45)*(D45+D46)+(D46*E47-D47*E46)*(D46+D47)+(D47*E48-D48*E47)*(D47+D48)+(D48*E49-D49*E48)*(D48+D49)+(D49*E50-D50*E49)*(D49+D50)+(D50*E51-D51*E50)*(D50+D51)+(D51*E52-D52*E51)*(D51+D52)+(D52*E53-D53*E52)*(D52+D53)+(D53*E54-D54*E53)*(D53+D54)+(D54*E55-D55*E54)*(D54+D55)+(D55*E56-D56*E55)*(D55+D56)+(D56*E57-D57*E56)*(D56+D57))/6/D58","v":{"$error":"#VALUE!"}},"m",{"$f":"-((F45*G46-F46*G45)*(F45+F46)+(F46*G47-F47*G46)*(F46+F47)+(F47*G48-F48*G47)*(F47+F48)+(F48*G49-F49*G48)*(F48+F49)+(F49*G50-F50*G49)*(F49+F50)+(F50*G51-F51*G50)*(F50+F51)+(F51*G52-F52*G51)*(F51+F52)+(F52*G53-F53*G52)*(F52+F53)+(F53*G54-F54*G53)*(F53+F54)+(F54*G55-F55*G54)*(F54+F55)+(F55*G56-F56*G55)*(F55+F56)+(F56*G57-F57*G56)*(F56+F57))/6/F58","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(H47*I48-H48*I47)*(H47+H48)+(H48*I49-H49*I48)*(H48+H49)+(H49*I50-H50*I49)*(H49+H50)+(H50*I51-H51*I50)*(H50+H51)+(H51*I52-H52*I51)*(H51+H52)+(H52*I53-H53*I52)*(H52+H53)+(H53*I54-H54*I53)*(H53+H54)+(H54*I55-H55*I54)*(H54+H55))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(J47+J48)+(J48*K49-J49*K48)*(J48+J49)+(J49*K50-J50*K49)*(J49+J50)+(J50*K51-J51*K50)*(J50+J51)+(J51*K52-J52*K51)*(J51+J52)+(J52*K53-J53*K52)*(J52+J53)+(J53*K54-J54*K53)*(J53+J54)+(J54*K55-J55*K54)*(J54+J55)+(J55*K56-J56*K55)*(J55+J56)+(J56*K57-J57*K56)*(J56+J57))/6/J58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(L47*M48-L48*M47)*(L47+L48)+(L48*M49-L49*M48)*(L48+L49)+(L49*M50-L50*M49)*(L49+L50)+(L50*M51-L51*M50)*(L50+L51)+(L51*M52-L52*M51)*(L51+L52)+(L52*M53-L53*M52)*(L52+L53)+(L53*M54-L54*M53)*(L53+L54)+(L54*M55-L55*M54)*(L54+L55))/6/L58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(N58=0,0,(+(N47*O48-N48*O47)*(N47+N48)+(N48*O49-N49*O48)*(N48+N49)+(N49*O50-N50*O49)*(N49+N50)+(N50*O51-N51*O50)*(N50+N51)+(N51*O52-N52*O51)*(N51+N52)+(N52*O53-N53*O52)*(N52+N53)+(N53*O54-N54*O53)*(N53+N54)+(N54*O55-N55*O54)*(N54+N55)+(N55*O56-N56*O55)*(N55+N56)+(N56*O57-N57*O56)*(N56+N57))/6/N58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(P47*Q48-P48*Q47)*(P47+P48)+(P48*Q49-P49*Q48)*(P48+P49)+(P49*Q50-P50*Q49)*(P49+P50)+(P50*Q51-P51*Q50)*(P50+P51)+(P51*Q52-P52*Q51)*(P51+P52)+(P52*Q53-P53*Q52)*(P52+P53)+(P53*Q54-P54*Q53)*(P53+P54)+(P54*Q55-P55*Q54)*(P54+P55))/6/P58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(R58=0,0,(+(R47*S48-R48*S47)*(R47+R48)+(R48*S49-R49*S48)*(R48+R49)+(R49*S50-R50*S49)*(R49+R50)+(R50*S51-R51*S50)*(R50+R51)+(R51*S52-R52*S51)*(R51+R52)+(R52*S53-R53*S52)*(R52+R53)+(R53*S54-R54*S53)*(R53+R54)+(R54*S55-R55*S54)*(R54+R55)+(R55*S56-R56*S55)*(R55+R56)+(R56*S57-R57*S56)*(R56+R57))/6/R58)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(T58=0,0,(+(T47*U48-T48*U47)*(T47+T48)+(T48*U49-T49*U48)*(T48+T49)+(T49*U50-T50*U49)*(T49+T50)+(T50*U51-T51*U50)*(T50+T51)+(T51*U52-T52*U51)*(T51+T52)+(T52*U53-T53*U52)*(T52+T53)+(T53*U54-T54*U53)*(T53+T54)+(T54*U55-T55*U54)*(T54+T55)+(T55*U56-T56*U55)*(T55+T56)+(T56*U57-T57*U56)*(T56+T57))/6/T58)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(V58=0,0,-(+(V47*W48-V48*W47)*(V47+V48)+(V48*W49-V49*W48)*(V48+V49)+(V49*W50-V50*W49)*(V49+V50)+(V50*W51-V51*W50)*(V50+V51))/6/V58)","v":2.6739089419190427},"m",{"$f":"IF(X58=0,0,-(+(X47*Y48-X48*Y47)*(X47+X48)+(X48*Y49-X49*Y48)*(X48+X49)+(X49*Y50-X50*Y49)*(X49+X50)+(X50*Y51-X51*Y50)*(X50+X51))/6/X58)","v":3.7896651910602248},"m",{"$f":"-(+(Z47*AA48-Z48*AA47)*(Z47+Z48)+(Z48*AA49-Z49*AA48)*(Z48+Z49)+(Z49*AA50-Z50*AA49)*(Z49+Z50)+(Z50*AA51-Z51*AA50)*(Z50+Z51)+(Z51*AA52-Z52*AA51)*(Z51+Z52)+(Z52*AA53-Z53*AA52)*(Z52+Z53)+(Z53*AA54-Z54*AA53)*(Z53+Z54)+(Z54*AA55-Z55*AA54)*(Z54+Z55)+(Z55*AA56-Z56*AA55)*(Z55+Z56)+(Z56*AA57-Z57*AA56)*(Z56+Z57))/6/Z58","v":4.5407423692617748},"m",null,null,null,null,"   Koordinate presjeka",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AH47+AH48)+(AH48*AI49-AH49*AI48)*(AH48+AH49)+(AH49*AI50-AH50*AI49)*(AH49+AH50)+(AH50*AI51-AH51*AI50)*(AH50+AH51)+(AH51*AI52-AH52*AI51)*(AH51+AH52)+(AH52*AI53-AH53*AI52)*(AH52+AH53)+(AH53*AI54-AH54*AI53)*(AH53+AH54)+(AH54*AI55-AH55*AI54)*(AH54+AH55)+(AH55*AI56-AH56*AI55)*(AH55+AH56)+(AH56*AI57-AH57*AI56)*(AH56+AH57))/6/AH58","v":4.550001650000004},"m"]
["yt=",{"$f":"-((B45*C46-B46*C45)*(C45+C46)+(B46*C47-B47*C46)*(C46+C47)+(B47*C48-B48*C47)*(C47+C48)+(B48*C49-B49*C48)*(C48+C49)+(B49*C50-B50*C49)*(C49+C50)+(B50*C51-B51*C50)*(C50+C51)+(B51*C52-B52*C51)*(C51+C52)+(B52*C53-B53*C52)*(C52+C53)+(B53*C54-B54*C53)*(C53+C54)+(B54*C55-B55*C54)*(C54+C55)+(B55*C56-B56*C55)*(C55+C56)+(B56*C57-B57*C56)*(C56+C57))/6/B58","v":0.75054981042380386},"m",{"$f":"-((D45*E46-D46*E45)*(E45+E46)+(D46*E47-D47*E46)*(E46+E47)+(D47*E48-D48*E47)*(E47+E48)+(D48*E49-D49*E48)*(E48+E49)+(D49*E50-D50*E49)*(E49+E50)+(D50*E51-D51*E50)*(E50+E51)+(D51*E52-D52*E51)*(E51+E52)+(D52*E53-D53*E52)*(E52+E53)+(D53*E54-D54*E53)*(E53+E54)+(D54*E55-D55*E54)*(E54+E55)+(D55*E56-D56*E55)*(E55+E56)+(D56*E57-D57*E56)*(E56+E57))/6/D58","v":{"$error":"#VALUE!"}},"m",{"$f":"-((F45*G46-F46*G45)*(G45+G46)+(F46*G47-F47*G46)*(G46+G47)+(F47*G48-F48*G47)*(G47+G48)+(F48*G49-F49*G48)*(G48+G49)+(F49*G50-F50*G49)*(G49+G50)+(F50*G51-F51*G50)*(G50+G51)+(F51*G52-F52*G51)*(G51+G52)+(F52*G53-F53*G52)*(G52+G53)+(F53*G54-F54*G53)*(G53+G54)+(F54*G55-F55*G54)*(G54+G55)+(F55*G56-F56*G55)*(G55+G56)+(F56*G57-F57*G56)*(G56+G57))/6/F58","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(H47*I48-H48*I47)*(I47+I48)+(H48*I49-H49*I48)*(I48+I49)+(H49*I50-H50*I49)*(I49+I50)+(H50*I51-H51*I50)*(I50+I51)+(H51*I52-H52*I51)*(I51+I52)+(H52*I53-H53*I52)*(I52+I53)+(H53*I54-H54*I53)*(I53+I54)+(H54*I55-H55*I54)*(I54+I55)+(H55*I56-H56*I55)*(I55+I56)+(H56*I57-H57*I56)*(I56+I57))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(K47+K48)+(J48*K49-J49*K48)*(K48+K49)+(J49*K50-J50*K49)*(K49+K50)+(J50*K51-J51*K50)*(K50+K51)+(J51*K52-J52*K51)*(K51+K52)+(J52*K53-J53*K52)*(K52+K53)+(J53*K54-J54*K53)*(K53+K54)+(J54*K55-J55*K54)*(K54+K55)+(J55*K56-J56*K55)*(K55+K56)+(J56*K57-J57*K56)*(K56+K57))/6/J58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(L47*M48-L48*M47)*(M47+M48)+(L48*M49-L49*M48)*(M48+M49)+(L49*M50-L50*M49)*(M49+M50)+(L50*M51-L51*M50)*(M50+M51)+(L51*M52-L52*M51)*(M51+M52)+(L52*M53-L53*M52)*(M52+M53)+(L53*M54-L54*M53)*(M53+M54)+(L54*M55-L55*M54)*(M54+M55))/6/L58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(N58=0,0,(+(N47*O48-N48*O47)*(O47+O48)+(N48*O49-N49*O48)*(O48+O49)+(N49*O50-N50*O49)*(O49+O50)+(N50*O51-N51*O50)*(O50+O51)+(N51*O52-N52*O51)*(O51+O52)+(N52*O53-N53*O52)*(O52+O53)+(N53*O54-N54*O53)*(O53+O54)+(N54*O55-N55*O54)*(O54+O55)+(N55*O56-N56*O55)*(O55+O56)+(N56*O57-N57*O56)*(O56+O57))/6/N58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(P47*Q48-P48*Q47)*(Q47+Q48)+(P48*Q49-P49*Q48)*(Q48+Q49)+(P49*Q50-P50*Q49)*(Q49+Q50)+(P50*Q51-P51*Q50)*(Q50+Q51)+(P51*Q52-P52*Q51)*(Q51+Q52)+(P52*Q53-P53*Q52)*(Q52+Q53)+(P53*Q54-P54*Q53)*(Q53+Q54)+(P54*Q55-P55*Q54)*(Q54+Q55))/6/P58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(R58=0,0,(+(R47*S48-R48*S47)*(S47+S48)+(R48*S49-R49*S48)*(S48+S49)+(R49*S50-R50*S49)*(S49+S50)+(R50*S51-R51*S50)*(S50+S51)+(R51*S52-R52*S51)*(S51+S52)+(R52*S53-R53*S52)*(S52+S53)+(R53*S54-R54*S53)*(S53+S54)+(R54*S55-R55*S54)*(S54+S55)+(R55*S56-R56*S55)*(S55+S56)+(R56*S57-R57*S56)*(S56+S57))/6/R58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-IF(T58=0,0,(+(T47*U48-T48*U47)*(U47+U48)+(T48*U49-T49*U48)*(U48+U49)+(T49*U50-T50*U49)*(U49+U50)+(T50*U51-T51*U50)*(U50+U51)+(T51*U52-T52*U51)*(U51+U52)+(T52*U53-T53*U52)*(U52+U53)+(T53*U54-T54*U53)*(U53+U54)+(T54*U55-T55*U54)*(U54+U55)+(T55*U56-T56*U55)*(U55+U56)+(T56*U57-T57*U56)*(U56+U57))/6/T58)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((V47*W48-V48*W47)*(W47+W48)+(V48*W49-V49*W48)*(W48+W49)+(V49*W50-V50*W49)*(W49+W50)+(V50*W51-V51*W50)*(W50+W51))/6/V58","v":0.65809555436880718},"kN",{"$f":"-((X47*Y48-X48*Y47)*(Y47+Y48)+(X48*Y49-X49*Y48)*(Y48+Y49)+(X49*Y50-X50*Y49)*(Y49+Y50)+(X50*Y51-X51*Y50)*(Y50+Y51))/6/X58","v":0.75428136494691478},"kN",{"$f":"-(+(Z47*AA48-Z48*AA47)*(AA47+AA48)+(Z48*AA49-Z49*AA48)*(AA48+AA49)+(Z49*AA50-Z50*AA49)*(AA49+AA50)+(Z50*AA51-Z51*AA50)*(AA50+AA51)+(Z51*AA52-Z52*AA51)*(AA51+AA52)+(Z52*AA53-Z53*AA52)*(AA52+AA53)+(Z53*AA54-Z54*AA53)*(AA53+AA54)+(Z54*AA55-Z55*AA54)*(AA54+AA55)+(Z55*AA56-Z56*AA55)*(AA55+AA56)+(Z56*AA57-Z57*AA56)*(AA56+AA57))/6/Z58","v":0.81902934843133712},"m",null,null,null,null,"II-II i I-I",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AI47+AI48)+(AH48*AI49-AH49*AI48)*(AI48+AI49)+(AH49*AI50-AH50*AI49)*(AI49+AI50)+(AH50*AI51-AH51*AI50)*(AI50+AI51)+(AH51*AI52-AH52*AI51)*(AI51+AI52)+(AH52*AI53-AH53*AI52)*(AI52+AI53)+(AH53*AI54-AH54*AI53)*(AI53+AI54)+(AH54*AI55-AH55*AI54)*(AI54+AI55)+(AH55*AI56-AH56*AI55)*(AI55+AI56)+(AH56*AI57-AH57*AI56)*(AI56+AI57))/6/AH58","v":1.3500505000000005},"m"]
["G=",{"$f":"+B58*'Analiza i dimenzioniranje'!E62","v":64.227611992767947},"kN",{"$f":"+D58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"+F58*'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}},"kN",{"$f":"+H58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(J58*'Analiza i dimenzioniranje'!E63<0,0,J58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+L58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(N58*'Analiza i dimenzioniranje'!U41<0,0,N58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+P58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(R58<=0,0,R58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",null,"kN (za L)",{"$f":"+V58*'Analiza i dimenzioniranje'!E62","v":37.77589163555291},"kN",{"$f":"+X58*'Analiza i dimenzioniranje'!E62","v":17.793104363851846},"kN",{"$f":"+Z58*'Analiza i dimenzioniranje'!E62","v":13.306056250595223},"kN",null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"AC47+'Analiza i dimenzioniranje'!C192/2","v":0.68753317931068247},{"$f":"+AH58*'Analiza i dimenzioniranje'!E62","v":5.2517757527774878},"kN"]
["Vertikala nasipa na konzoli",null,null,"Moment na konzoli",null,"Pokos na vrhu zida",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - NAPONI ",null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+'C VI-VII'!AC49+('Analiza i dimenzioniranje'!C191/2)","v":0.77418208680245293}]
[null,"x","y",{"$f":"IF('Analiza i dimenzioniranje'!G78=0,0,'Analiza i dimenzioniranje'!G78*'Analiza i dimenzioniranje'!C77*'Analiza i dimenzioniranje'!E62*(Q20-B5+'Analiza i dimenzioniranje'!G78/2)+J61*(O16-J59))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"+F64","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"naponi za presjek II-II",null,"naponi za srednji dio ",null,"naponi za presjek I-I"]
[null,{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},"b1=",{"$f":"+H47-2","v":1.4000010999999999},{"$f":"+B52","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y","x","y","x","y","Koordinate dna temelja"]
[null,{"$f":"+B64","v":{"$error":"#VALUE!"}},{"$f":"IF(B65>J49,C19,+C20+'Analiza i dimenzioniranje'!F20+(H52-H50)*TAN('Analiza i dimenzioniranje'!F21*PI()/180))","v":{"$error":"#VALUE!"}},"b2=",{"$f":"'Analiza i dimenzioniranje'!E54+('Analiza i dimenzioniranje'!E55-'Analiza i dimenzioniranje'!E54)*(('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)/(C9-C4))","v":{"$error":"#VALUE!"}},{"$f":"+B65","v":{"$error":"#VALUE!"}},{"$f":"+G64+(F64-F65)*TAN('Analiza i dimenzioniranje'!F21*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,0,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},0,{"$f":"+'C VI-VII'!B11","v":4.2000010999999997},{"$f":"-U47","v":0},2,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z65","v":2},{"$f":"AC55","v":{"$error":"#VALUE!"}},{"$f":"+AB65","v":3.4000010999999999},{"$f":"+AA67","v":{"$error":"#VALUE!"}},{"$f":"+AB57","v":4.2000010999999997},{"$f":"AC57","v":{"$error":"#VALUE!"}},{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"(AF66*(AG70-AG65)/(AF70-AF65)-AF65*(AG70-AG65)/(AF70-AF65)+AG65)","v":{"$error":"#VALUE!"}}]
[null,"AKTIVNI TLAKOVI za stabilnost i Presjek III-III (bez E3)",null,null,null,null,null,null,"  AKTIVNI TLAKOVI za presjek kroz zid VI-VI",null,null,null,null,"    AKTIVNI TLAKOVI za presjek kroz zid VII-VII",null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"AC56","v":{"$error":"#VALUE!"}},{"$f":"+AB66+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AE66","v":{"$error":"#VALUE!"}},{"$f":"+AB58","v":4.9000021999999994},{"$f":"+AC58","v":{"$error":"#VALUE!"}},{"$f":"+AB77","v":{"$error":"#VALUE!"}},{"$f":"+(AF67*(AG65-AG70)/(AF65-AF70)-AF70*(AG65-AG70)/(AF65-AF70)+AG70)","v":{"$error":"#VALUE!"}}]
[null,"E1",null,"E2",null,"E3",null,null,"E1",null,"E2 do presjeka kroz zid II",null,null,"E1",null,"E2",null,null,null,null,null,null,null,null,null,{"$f":"+Z67","v":3.4000010999999999},0,{"$f":"+AB67","v":4.2000010999999997},0,{"$f":"+AD67","v":4.9000021999999994},{"$f":"+U50","v":0},{"$f":"+AB67","v":4.2000010999999997},{"$f":"+(AF68*(AG65-AG70)/(AF65-AF70)-AF70*(AG65-AG70)/(AF65-AF70)+AG70)","v":0.37931024673015767}]
[null,0,{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C71","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,{"$f":"+N69","v":0},{"$f":"+O69","v":{"$error":"#VALUE!"}},{"$f":"+I71","v":{"$error":"#VALUE!"}},{"$f":"+J71","v":{"$error":"#VALUE!"}},null,{"$f":"+B69","v":0},{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+N71","v":{"$error":"#VALUE!"}},{"$f":"+O71","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"+Z65","v":2},0,{"$f":"+AB65","v":3.4000010999999999},0,{"$f":"+AD65","v":4.2000010999999997},{"$f":"+U51","v":0},{"$f":"+AD77","v":{"$error":"#VALUE!"}},{"$f":"+(AF69*(AG66-AG70)/(AF66-AF70)-AF70*(AG66-AG70)/(AF66-AF70)+AG70)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+B69","v":0},{"$f":"+C69-'Analiza i dimenzioniranje'!D17-'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+D69+'Analiza i dimenzioniranje'!E16*'Analiza i dimenzioniranje'!E17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+E69-'Analiza i dimenzioniranje'!E17","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},null,{"$f":"+N70","v":0},{"$f":"+J69-('Analiza i dimenzioniranje'!F20+'P VI-VI'!E17)","v":{"$error":"#VALUE!"}},{"$f":"+K69+'P VI-VI'!F16*'P VI-VI'!F17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},null,{"$f":"+B70","v":0},{"$f":"+O69-('Analiza i dimenzioniranje'!F20+'P VII-VII'!E17)","v":{"$error":"#VALUE!"}},{"$f":"+P69+'P VII-VII'!F16*'P VII-VII'!F17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AB53","v":4.9000021999999994},{"$f":"+AC53","v":0.5}]
[null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('Analiza i dimenzioniranje'!D17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},0,{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F70+'Analiza i dimenzioniranje'!F16*'Analiza i dimenzioniranje'!F17*'Analiza i dimenzioniranje'!F112","v":{"$error":"#VALUE!"}},0,null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('P VI-VI'!E17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+J70","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+L70","v":1.52},null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('P VII-VII'!E17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+Q70","v":1.84}]
[null,{"$f":"+B69","v":0},{"$f":"+C69","v":{"$error":"#VALUE!"}},0,{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F69","v":0},0,null,{"$f":"+N72","v":0},{"$f":"+O72","v":{"$error":"#VALUE!"}},{"$f":"+D72","v":0},{"$f":"+L69","v":{"$error":"#VALUE!"}},null,{"$f":"+N69","v":0},{"$f":"+O69","v":{"$error":"#VALUE!"}},{"$f":"+D72","v":0},{"$f":"+Q69","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+D69","v":{"$error":"#VALUE!"}},{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F72","v":0},{"$f":"+G70","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+K69","v":{"$error":"#VALUE!"}},{"$f":"+L69","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+P69","v":{"$error":"#VALUE!"}},{"$f":"+Q69","v":{"$error":"#VALUE!"}}]
["Jednadžba vertikale kohezije    Određivanje sjecišta kohezije s pravcem od tlaka",null,null,null,null,null,null,{"$f":"+M74","v":"Jednadžba vertikale kohezije  -  sjecišta kohezije s pravcem od tlaka"},null,null,null,null,"Jednadžba vertikale kohezije  -  sjecišta kohezije s pravcem od tlaka"]
[null,"X","y","X","y","X","y",null,{"$f":"+N75","v":"X"},{"$f":"+O75","v":"y"},"X","y",null,"X","y","X","y"]
[null,{"$f":"2*'Analiza i dimenzioniranje'!D15/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F110)","v":12.361875887090893},{"$f":"B76*(C71-C72)/(B71-B72)-B72*(C71-C72)/(B71-B72)+C72","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!F12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F111)","v":{"$error":"#VALUE!"}},{"$f":"IF(D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69>'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69)","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!C12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F112)","v":{"$error":"#VALUE!"}},{"$f":"IF((F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70)>'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!F17,(F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70))","v":{"$error":"#VALUE!"}},null,{"$f":"+N76","v":12.361875887090893},{"$f":"I76*(J71-J72)/(I71-I72)-I72*(J71-J72)/(I71-I72)+J72","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},null,{"$f":"+B76","v":12.361875887090893},{"$f":"N76*(O71-O72)/(N71-N72)-N72*(O71-O72)/(N71-N72)+O72","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"-0.5*((Z65*AA66-Z66*AA65)+(Z66*AA67-Z67*AA66)+(Z67*AA68-Z68*AA67)+(Z68*AA69-Z69*AA68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((AB65*AC66-AB66*AC65)+(AB66*AC67-AB67*AC66)+(AB67*AC68-AB68*AC67)+(AB68*AC69-AB69*AC68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((AD65*AE66-AD66*AE65)+(AD66*AE67-AD67*AE66)+(AD67*AE68-AD68*AE67)+(AD68*AE69-AD69*AE68)+(AD69*AE70-AD70*AE69)+(AD70*AE71-AD71*AE70)+(AD71*AE72-AD72*AE71)+(AD72*AE73-AD73*AE72))","v":{"$error":"#VALUE!"}},"kN/m'"]
[null,{"$f":"+B76","v":12.361875887090893},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},null,{"$f":"+N77","v":12.361875887090893},{"$f":"+O77","v":{"$error":"#VALUE!"}},{"$f":"+K76","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},null,{"$f":"+N76","v":12.361875887090893},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+P76","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},null,null,null,null,null,null,null,null,{"$f":"IF(Z76=0,0,-(+(Z65*AA66-Z66*AA65)*(Z65+Z66)+(Z66*AA67-Z67*AA66)*(Z66+Z67)+(Z67*AA68-Z68*AA67)*(Z67+Z68)+(Z68*AA69-Z69*AA68)*(Z68+Z69))/6/Z76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(AB76=0,0,-(+(AB65*AC66-AB66*AC65)*(AB65+AB66)+(AB66*AC67-AB67*AC66)*(AB66+AB67)+(AB67*AC68-AB68*AC67)*(AB67+AB68)+(AB68*AC69-AB69*AC68)*(AB68+AB69))/6/AB76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(AD76=0,0,-(+(AD65*AE66-AD66*AE65)*(AD65+AD66)+(AD66*AE67-AD67*AE66)*(AD66+AD67)+(AD67*AE68-AD68*AE67)*(AD67+AD68)+(AD68*AE69-AD69*AE68)*(AD68+AD69))/6/AD76)","v":{"$error":"#VALUE!"}},"m"]
["Oznaka","E1",null,"E2",null,"E3",null,{"$f":"+M78","v":"Oznaka"},{"$f":"+N78","v":"E1"},null,"E2",null,"Oznaka","E1",null,"E2",null,null,null,null,null,null,null,null,null,{"$f":"-((Z65*AA66-Z66*AA65)*(AA65+AA66)+(Z66*AA67-Z67*AA66)*(AA66+AA67)+(Z67*AA68-Z68*AA67)*(AA67+AA68)+(Z68*AA69-Z69*AA68)*(AA68+AA69))/6/Z76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((AB65*AC66-AB66*AC65)*(AC65+AC66)+(AB66*AC67-AB67*AC66)*(AC66+AC67)+(AB67*AC68-AB68*AC67)*(AC67+AC68)+(AB68*AC69-AB69*AC68)*(AC68+AC69))/6/AB76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((AD65*AE66-AD66*AE65)*(AE65+AE66)+(AD66*AE67-AD67*AE66)*(AE66+AE67)+(AD67*AE68-AD68*AE67)*(AE67+AE68)+(AD68*AE69-AD69*AE68)*(AE68+AE69))/6/AD76","v":{"$error":"#VALUE!"}},"kN/m'"]
["točke","x","y","x","y","x","y","točke",{"$f":"+N79","v":"x"},{"$f":"+O79","v":"y"},"x","y","točke","x","y","x","y"]
[1,{"$f":"+'C III-V'!B80","v":12.361875887090893},{"$f":"+C77","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,{"$f":"+I76","v":12.361875887090893},{"$f":"+J76","v":{"$error":"#VALUE!"}},{"$f":"+K76","v":{"$error":"#VALUE!"}},{"$f":"+L76","v":{"$error":"#VALUE!"}},{"$f":"+R80","v":0},12.361875887090893,{"$f":"+O77","v":{"$error":"#VALUE!"}},{"$f":"+P76","v":{"$error":"#VALUE!"}},{"$f":"+Q76","v":{"$error":"#VALUE!"}},null,"Jedn pravca zida uz tlo",null,"Jedn pravca arm dno ",null,"Y=",{"$f":"IF(S82=S81,1000000,(T82-T81)/(S82-S81))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X80*S81+T81","v":{"$error":"#VALUE!"}}]
[2,{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G76","v":{"$error":"#VALUE!"}},0,{"$f":"+I71","v":{"$error":"#VALUE!"}},{"$f":"+J71","v":{"$error":"#VALUE!"}},{"$f":"+K69","v":{"$error":"#VALUE!"}},{"$f":"+L69","v":{"$error":"#VALUE!"}},{"$f":"+R81","v":0},{"$f":"+N71","v":{"$error":"#VALUE!"}},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+P69","v":{"$error":"#VALUE!"}},{"$f":"+Q69","v":{"$error":"#VALUE!"}},null,{"$f":"+B4","v":3.4000010999999999},{"$f":"+C4","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!T593","v":2.0499999999999998},{"$f":"+'Analiza i dimenzioniranje'!U593","v":0.18682583433163008},"X=",{"$f":"+(-Z80+Z83)/(X80-X83)","v":{"$error":"#VALUE!"}},"sjeište"]
[3,{"$f":"+B80","v":12.361875887090893},{"$f":"+C76","v":{"$error":"#VALUE!"}},{"$f":"IF(D76>D69,D81,D69)","v":{"$error":"#VALUE!"}},{"$f":"+E81","v":{"$error":"#VALUE!"}},{"$f":"IF(F77>F70,F77,F70)","v":{"$error":"#VALUE!"}},{"$f":"IF(F77>F70,G76,G70)","v":{"$error":"#VALUE!"}},0,{"$f":"+I77","v":12.361875887090893},{"$f":"+J77","v":{"$error":"#VALUE!"}},{"$f":"+K70","v":{"$error":"#VALUE!"}},{"$f":"+L70","v":1.52},{"$f":"+R82","v":0},{"$f":"+N80","v":12.361875887090893},{"$f":"+O76","v":{"$error":"#VALUE!"}},{"$f":"+P70","v":{"$error":"#VALUE!"}},{"$f":"+Q70","v":1.84},null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},{"$f":"+'Analiza i dimenzioniranje'!T594","v":4.8600021999999994},{"$f":"+'Analiza i dimenzioniranje'!U594","v":0.54310345350772504},"Y=",{"$f":"+X80*X81+Z80","v":{"$error":"#VALUE!"}}]
[4,{"$f":"+B80","v":12.361875887090893},{"$f":"+C80","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F71","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},0,{"$f":"+I76","v":12.361875887090893},{"$f":"+J76","v":{"$error":"#VALUE!"}},{"$f":"+K76","v":{"$error":"#VALUE!"}},{"$f":"+L82","v":1.52},{"$f":"+R83","v":0},{"$f":"+N80","v":12.361875887090893},{"$f":"+O80","v":{"$error":"#VALUE!"}},{"$f":"+P84","v":{"$error":"#VALUE!"}},{"$f":"+IF('Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17<'Analiza i dimenzioniranje'!W44,0,'C VI-VII'!Q82)","v":1.84},null,null,null,null,null,"Y=",{"$f":"+(V82-V81)/(U82-U81)","v":0.12678908905341604},"*x",{"$f":"-X83*U81+V81","v":-7.3091798227872762E-2},"CRTANJE"]
[5,null,null,{"$f":"+D80","v":{"$error":"#VALUE!"}},{"$f":"+E80","v":{"$error":"#VALUE!"}},{"$f":"+F80","v":{"$error":"#VALUE!"}},{"$f":"+G80","v":0},5,null,null,{"$f":"+K80","v":{"$error":"#VALUE!"}},{"$f":"+L80","v":{"$error":"#VALUE!"}},5,null,null,{"$f":"+P80","v":{"$error":"#VALUE!"}},{"$f":"+Q80","v":{"$error":"#VALUE!"}},null,"Jedn pravca sloja 3",null,"Jedn pravca sloja 3 klizno",null,"Y=",{"$f":"+(T86-T85)/(S86-S85)","v":-3.4920769491747737E-2},"*x",{"$f":"-X84*S85+T85","v":1.2698415389834954},"Jedn pravca sloja 3 klizno",null,"sjecište 1/2 sidra sa vrhom 1. sloja"]
["  A=",{"$f":"IF(B77>B71,0,-IF(B84>B83,0,-0.5*((B80*C81-B81*C80)+(B81*C82-B82*C81)+(B82*C83-B83*C82)+(B83*C84-B84*C83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D77>D70,0,IF(D84>D83,0,-0.5*((D80*E81-D81*E80)+(D81*E82-D82*E81)+(D82*E83-D83*E82)+(D83*E84-D84*E83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F77>F71,0,IF(F84>F83,0,-0.5*((F80*G81-F81*G80)+(F81*G82-F82*G81)+(F82*G83-F83*G82)+(F83*G84-F84*G83))))","v":{"$error":"#VALUE!"}},"kN/m'","  A=",{"$f":"IF(J77>J76,0,-0.5*((I80*J81-I81*J80)+(I81*J82-I82*J81)+(I82*J83-I83*J82)+(I83*J84-I84*J83)))","v":{"$error":"#VALUE!"}},{"$f":"+O85","v":"kN/m'"},{"$f":"IF(L77>L76,0,-0.5*((K80*L81-K81*L80)+(K81*L82-K82*L81)+(K82*L83-K83*L82)+(K83*L84-K84*L83)))","v":{"$error":"#VALUE!"}},"kN/m'","  A=",{"$f":"IF(O77>O76,0,0.5*((N80*O81-N81*O80)+(N81*O82-N82*O81)+(N82*O83-N83*O82)+(N83*O84-N84*O83)))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(Q77>Q76,0,-0.5*((P80*Q81-P81*Q80)+(P81*Q82-P82*Q81)+(P82*Q83-P83*Q82)+(P83*Q84-P84*Q83)))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+U18","v":2},{"$f":"+V18","v":1.2},{"$f":"+W100","v":2},0,"X=",{"$f":"+(-Z84+Z87)/(X84-X87)","v":1.1386903959986558},"sjecište ",null,{"$f":"+U85","v":2},{"$f":"+V85","v":0},"Y=",{"$f":"+X92","v":{"$error":"#VALUE!"}},"*x",{"$f":"+Z92","v":{"$error":"#VALUE!"}}]
["xt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(B80+B81)+(B81*C82-B82*C81)*(B81+B82)+(B82*C83-B83*C82)*(B82+B83)+(B83*C84-B84*C83)*(B83+B84))/6/B85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(D80+D81)+(D81*E82-D82*E81)*(D81+D82)+(D82*E83-D83*E82)*(D82+D83)+(D83*E84-D84*E83)*(D83+D84))/6/D85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(F80+F81)+(F81*G82-F82*G81)*(F81+F82)+(F82*G83-F83*G82)*(F82+F83)+(F83*G84-F84*G83)*(F83+F84))/6/F85)","v":{"$error":"#VALUE!"}},"kN/m'","xt=",{"$f":"IF(I85=0,0,-((I80*J81-I81*J80)*(I80+I81)+(I81*J82-I82*J81)*(I81+I82)+(I82*J83-I83*J82)*(I82+I83)+(I83*J84-I84*J83)*(I83+I84))/6/I85)","v":{"$error":"#VALUE!"}},{"$f":"+O86","v":"kN/m'"},{"$f":"IF(K85=0,0,-((K80*L81-K81*L80)*(K80+K81)+(K81*L82-K82*L81)*(K81+K82)+(K82*L83-K83*L82)*(K82+K83)+(K83*L84-K84*L83)*(K83+K84))/6/K85)","v":{"$error":"#VALUE!"}},"kN/m'","xt=",{"$f":"IF(N85=0,0,((N80*O81-N81*O80)*(N80+N81)+(N81*O82-N82*O81)*(N81+N82)+(N82*O83-N83*O82)*(N82+N83)+(N83*O84-N84*O83)*(N83+N84))/6/N85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(P85=0,0,-((P80*Q81-P81*Q80)*(P80+P81)+(P81*Q82-P82*Q81)*(P81+P82)+(P82*Q83-P83*Q82)*(P82+P83)+(P83*Q84-P84*Q83)*(P83+P84))/6/P85)","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+U19","v":-8},{"$f":"+V19","v":1.5492076949174773},-5,{"$f":"+V85+(U85-U86)*TAN((45+'Analiza i dimenzioniranje'!F14/2)*PI()/180)","v":9.9970360471948005},"Y=",{"$f":"+X84*X85+Z84","v":1.2300775941423594},3,null,{"$f":"+X85","v":1.1386903959986558},{"$f":"+X86","v":1.2300775941423594}]
["yt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(C80+C81)+(B81*C82-B82*C81)*(C81+C82)+(B82*C83-B83*C82)*(C82+C83)+(B83*C84-B84*C83)*(C83+C84))/6/B85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(E80+E81)+(D81*E82-D82*E81)*(E81+E82)+(D82*E83-D83*E82)*(E82+E83)+(D83*E84-D84*E83)*(E83+E84))/6/D85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(G80+G81)+(F81*G82-F82*G81)*(G81+G82)+(F82*G83-F83*G82)*(G82+G83)+(F83*G84-F84*G83)*(G83+G84))/6/F85)","v":{"$error":"#VALUE!"}},"m","yt=",{"$f":"IF(I85=0,0,-((I80*J81-I81*J80)*(J80+J81)+(I81*J82-I82*J81)*(J81+J82)+(I82*J83-I83*J82)*(J82+J83)+(I83*J84-I84*J83)*(J83+J84))/6/I85)","v":{"$error":"#VALUE!"}},{"$f":"+O87","v":"m"},{"$f":"IF(K85=0,0,-((K80*L81-K81*L80)*(L80+L81)+(K81*L82-K82*L81)*(L81+L82)+(K82*L83-K83*L82)*(L82+L83)+(K83*L84-K84*L83)*(L83+L84))/6/K85)","v":{"$error":"#VALUE!"}},"m","yt=",{"$f":"IF(N85=0,0,((N80*O81-N81*O80)*(O80+O81)+(N81*O82-N82*O81)*(O81+O82)+(N82*O83-N83*O82)*(O82+O83)+(N83*O84-N84*O83)*(O83+O84))/6/N85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(P85=0,0,-((P80*Q81-P81*Q80)*(Q80+Q81)+(P81*Q82-P82*Q81)*(Q81+Q82)+(P82*Q83-P83*Q82)*(Q82+Q83)+(P83*Q84-P84*Q83)*(Q83+Q84))/6/P85)","v":{"$error":"#VALUE!"}},"m",null,null,null,null,null,"Y=",{"$f":"+(V86-V85)/(U86-U85)","v":-1.4281480067421144},"*x",{"$f":"-X87*U85+V85","v":2.8562960134842288},"y=2       x=",{"$f":"+('Analiza i dimenzioniranje'!E52-'C VI-VII'!Z87)/'C VI-VII'!X87","v":1.1597509541483482}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(K85<0,0,K85)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+IF(P85<0,0,P85)","v":{"$error":"#VALUE!"}},null,null,"Jedn pravca sloja 2",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(T90-T89)/(S90-S89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X88*S89+T89","v":{"$error":"#VALUE!"}},"Jedn pravca sloja 2 klizno",null,"Jednadžba pravca sidra",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(AD90-AD89)/(AC90-AC89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AH88*AC89+AD89","v":{"$error":"#VALUE!"}}]
["X koordinata položaja rezultante aktivnog tlaka na stražnjoj strani zida za  Ev1, Ev2 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U15","v":{"$error":"#VALUE!"}},{"$f":"+V15","v":4},{"$f":"+X85","v":1.1386903959986558},{"$f":"+X86","v":1.2300775941423594},"X=",{"$f":"+(-Z88+Z91)/(X88-X91)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U89","v":1.1386903959986558},{"$f":"+V89","v":1.2300775941423594},{"$f":"+U37","v":{"$error":"#VALUE!"}},{"$f":"+V37","v":5},{"$f":"+U89","v":1.1386903959986558},{"$f":"+V89","v":1.2300775941423594},"X=",{"$f":"+(-AJ88+AJ91)/(AH88-AH91)","v":{"$error":"#VALUE!"}},"sjecište"]
["Jednadžba pravca zida uz tlo",null,null,null,null,"Za Ev3 x=2",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U16","v":-8},{"$f":"+V16","v":{"$error":"#VALUE!"}},-5,{"$f":"+V89+(U89-U90)*TAN((45+'Analiza i dimenzioniranje'!E14/2)*PI()/180)","v":9.6792600705649363},"Y=",{"$f":"+X88*X89+Z88","v":{"$error":"#VALUE!"}},2,null,{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},{"$f":"+U38","v":{"$error":"#VALUE!"}},{"$f":"+V38","v":{"$error":"#VALUE!"}},{"$f":"+U90","v":-5},{"$f":"+V90","v":9.6792600705649363},"Y=",{"$f":"+AH88*AH89+AJ88","v":{"$error":"#VALUE!"}},2]
[null,"E1",null,"E2",null,"E3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(V90-V89)/(U90-U89)","v":-1.3763819204711731},"*x",{"$f":"-X91*U89+V89","v":2.79735046820907},null,null,null,null,null,null,"Y=",{"$f":"+(AF90-AF89)/(AE90-AE89)","v":-1.3763819204711731},"*x",{"$f":"-AH91*AE89+AF89","v":2.79735046820907}]
["x","y","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,"Jedn pravca sloja 1",null,null,null,"Y=",{"$f":"+(T95-T94)/(S95-S94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X92*S94+T94","v":{"$error":"#VALUE!"}},"Jednaž pravca sloja 1 klizno",null,"Slobodna dionica ls>=",{"$f":"+SQRT((AC94-AC93)*(AC94-AC93)+(AD94-AD93)*(AD94-AD93))","v":{"$error":"#VALUE!"}}]
[{"$f":"+(B8-B4)*(B93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+B87","v":{"$error":"#VALUE!"}},{"$f":"+(B8-B4)*(D93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+D87","v":{"$error":"#VALUE!"}},2,{"$f":"+F87","v":{"$error":"#VALUE!"}},null,{"$f":"+(B8-B4)*(I93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+N87","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+(B8-B4)*(N93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+I87","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+V7","v":"A"},null,null,"X=",{"$f":"+(-Z92+Z95)/(X92-X95)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U94","v":{"$error":"#VALUE!"}},{"$f":"+V94","v":{"$error":"#VALUE!"}},{"$f":"+AC89","v":{"$error":"#VALUE!"}},{"$f":"+AD89","v":5}]
[null,null,null,null,"Sloj2",{"$f":"+(B8-B4)*(G94-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!V15","v":4},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U8","v":{"$error":"#VALUE!"}},{"$f":"+V8","v":6},{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+X92*X93+Z92","v":{"$error":"#VALUE!"}},1,null,{"$f":"+X93","v":{"$error":"#VALUE!"}},{"$f":"+X94","v":{"$error":"#VALUE!"}},{"$f":"+AH89","v":{"$error":"#VALUE!"}},{"$f":"+AH90","v":{"$error":"#VALUE!"}}]
[{"$f":"+F113","v":"Visina presjeka"},null,{"$f":"+'C III-V'!C118:D118","v":"Sjecište I. sloja i terena"},null,null,{"$f":"+(B8-B4)*(G95-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+K21","v":1.2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782},-5,{"$f":"+V94+(U94-U95)*TAN((45+'Analiza i dimenzioniranje'!D14/2)*PI()/180)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+(V95-V94)/(U95-U94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X95*U94+V94","v":{"$error":"#VALUE!"}},{"$f":"+(AB95-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782}]
[{"$f":"+F114","v":"III"},{"$f":"+G114","v":1.2},{"$f":"+H114","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(AB96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},{"$f":"+(AD96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52}]
[{"$f":"+F115","v":"VI"},{"$f":"+G115","v":1.52},{"$f":"+H115","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Linija klizne plohe za potres kada su kontrafore ",null,"Geometrija zida",null,"POTRES",null,"x","y","x","y","x","y",null,null,null,null,"Masa za potres s prosjekom kontrafore i bez kontrafora"]
["VII",1.84,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+(B9-B4)*(AD98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},{"$f":"+(B9-B4)*(AF98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84}]
["VIII",2.16,{"$error":"#VALUE!"},null,null,null,null,null,null,"Jednadžba UREĐENOG TERENA KADA JE KOSINA IZA ZIDA (bez prometa)",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W99","v":2},{"$f":"+'C III-V'!X99","v":0.12820515121628623},null,null,{"$f":"+(Z95-AB99)/(-X91)","v":{"$error":"#VALUE!"}},{"$f":"+AB98","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!V44>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'C VI-VII'!AC96,(Z91-AD99)/(-X91))","v":0.92804943832144926},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},{"$f":"IF('Analiza i dimenzioniranje'!W44>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'C VI-VII'!AA96,(Z91-AF99)/(-X91))","v":0.6955558293597337},{"$f":"+AF98","v":1.84}]
["IX",2.48,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y",{"$f":"+'C III-V'!W100","v":2},{"$f":"+'C III-V'!X100","v":1.2},"Površina kliznog tijela od računske kontrafore",null,"Klizno tijelo za potres za presjek III-III",null,"Klizno tijelo za potres za presjek   VI-VI   ",null,"Klizno tijelo za potres za presjek   VII-VII",null,null,null,null,null,"Potresna sila za stabilnost "]
["X",2.8,{"$error":"#VALUE!"},null,null,null,null,null,null,"x=",{"$f":"+S101","v":0},{"$f":"+S105","v":0},null,null,null,null,null,null,null,null,{"$f":"2+AN113","v":1.75},0,{"$f":"+'C III-V'!W101","v":3.4000010999999999},{"$f":"+'C III-V'!X101","v":1.2},{"$f":"+'C III-V'!Y101","v":1.75},{"$f":"+'C III-V'!Z101","v":9.6153895463470418E-2},{"$f":"+Y102","v":0.97707863658009864},{"$f":"+Z102","v":1.2},{"$f":"+AC98","v":{"$error":"#VALUE!"}},{"$f":"+AD98","v":1.52},{"$f":"+AE98","v":{"$error":"#VALUE!"}},{"$f":"+AF98","v":1.84},null,null,null,null,{"$f":"+'C III-V'!Y101","v":1.75},{"$f":"+'C III-V'!Z101","v":9.6153895463470418E-2}]
["XI",3.14,{"$error":"#VALUE!"},null,null,null,null,null,null,"Y=",{"$f":"+T101","v":0},{"$f":"+T105","v":0},null,null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!$A$82=\"\",AC101,+AK102)","v":0.97707863658009864},{"$f":"+AL102","v":1.2},{"$f":"+'C III-V'!W102","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X102","v":3.14},{"$f":"+'C III-V'!Y102","v":0.97707863658009864},{"$f":"+'C III-V'!Z102","v":1.2},{"$f":"+Y103","v":-1.0572404418349119},{"$f":"+Z103","v":4},{"$f":"+AA101","v":0.97707863658009864},{"$f":"+AP120","v":1.52},{"$f":"+AO121","v":0.45866939675594048},{"$f":"+AP121","v":1.84},null,null,null,null,{"$f":"+'C III-V'!Y102","v":0.97707863658009864},{"$f":"+'C III-V'!Z102","v":1.2}]
["XIII",3.44,{"$error":"#VALUE!"},null,null,null,null,null,null,"Y=",{"$f":"(L102-K102)/(L101-K101)","v":{"$error":"#DIV/0!"}},"*x             +",{"$f":"-K103*K101+K102","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!$A$82=\"\",AC102,+AK103)","v":-1.0572404418349119},{"$f":"+AL103","v":4},{"$f":"+'C III-V'!W103","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X103","v":3.14},{"$f":"+'C III-V'!Y103","v":-1.0572404418349119},{"$f":"+'C III-V'!Z103","v":4},{"$f":"+Y103","v":-1.0572404418349119},4,-1.0572404418349119,4,-1.0572404418349119,4,null,null,null,null,{"$f":"+'C III-V'!Y103","v":-1.0572404418349119},{"$f":"+'C III-V'!Z103","v":4}]
["XIII",3.76,{"$error":"#VALUE!"},null,null,null,null,null,null,"Vrijednosti X za poznati Y",null,null,null,null,null,null,null,null,null,null,{"$f":"+AK136","v":{"$error":"#VALUE!"}},{"$f":"+AL136","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!W104","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X104","v":3.44},{"$f":"+'C III-V'!Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z104","v":{"$error":"#VALUE!"}},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+'C III-V'!Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z104","v":{"$error":"#VALUE!"}}]
["XIV",4.08,{"$error":"#VALUE!"},null,null,null,null,null,null,"X=",{"$f":"+L112/$K$109-$M$109/$K$109","v":{"$error":"#VALUE!"}},6.2," =Y",null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W105","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X105","v":3.44},{"$f":"+'C III-V'!Y105","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z105","v":6.2644906473896782},{"$f":"+Y105","v":{"$error":"#VALUE!"}},{"$f":"+Z105","v":6.2644906473896782},{"$f":"+AA105","v":{"$error":"#VALUE!"}},{"$f":"IF(AA105=AC105,AB105,AB95)","v":{"$error":"#VALUE!"}},{"$f":"+AC105","v":{"$error":"#VALUE!"}},{"$f":"+AD105","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AG105","v":" H="},{"$f":"+'C III-V'!AH105","v":4},null,null,{"$f":"+'C III-V'!Y105","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z105","v":6.2644906473896782}]
["XV",4.4000000000000004,{"$error":"#VALUE!"},null,null,null,null,null,null,"Jednadžba kizne ploha  ",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W106","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X106","v":"A"},{"$f":"+'C III-V'!Y106","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z106","v":6},{"$f":"+Y106","v":{"$error":"#VALUE!"}},6,{"$f":"+AE106","v":{"$error":"#VALUE!"}},{"$f":"+AF106","v":6},{"$f":"+AA106","v":{"$error":"#VALUE!"}},{"$f":"+AB106","v":6},null,null,null,null,{"$f":"+'C III-V'!Y106","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z106","v":6}]
["XVI",4.72,{"$error":"#VALUE!"},null,null,null,null,null,null,"x=",{"$f":"+AK103","v":-1.0572404418349119},{"$f":"+AU123","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W107","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X107","v":"A"},{"$f":"+'C III-V'!Y107","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z107","v":6},{"$error":"#VALUE!"},6,{"$f":"+AE107","v":{"$error":"#VALUE!"}},{"$f":"+AF107","v":6},{"$f":"+AA107","v":{"$error":"#VALUE!"}},{"$f":"+AB107","v":6},null,null,null,null,{"$f":"+'C III-V'!Y107","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z107","v":6}]
["XVII",5.04,{"$error":"#VALUE!"},null,null,null,null,null,null,"Y=",{"$f":"+AL103","v":4},{"$f":"+AU124","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W108","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X108","v":"A"},{"$f":"+'C III-V'!Y108","v":3.4000000999999997},{"$f":"+'C III-V'!Z108","v":1.2},3.4000000999999997,1.2,{"$f":"+AC109","v":{"$error":"#VALUE!"}},{"$f":"+AD109","v":1.52},{"$f":"+AE109","v":{"$error":"#VALUE!"}},{"$f":"+AF109","v":1.84},null,null,null,null,{"$f":"+'C III-V'!Y108","v":3.4000000999999997},{"$f":"+'C III-V'!Z108","v":1.2}]
["XVIII",5.36,{"$error":"#VALUE!"},null,null,null,null,null,null,"Y=",{"$f":"(L108-K108)/(L107-K107)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-K109*K107+K108","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W109","v":4.2000010999999997},{"$f":"+'C III-V'!X109","v":1.2},{"$f":"+'C III-V'!Y109","v":1.75},{"$f":"+'C III-V'!Z109","v":1.2},{"$f":"+AA101","v":0.97707863658009864},{"$f":"+AB101","v":1.2},{"$f":"+AC98","v":{"$error":"#VALUE!"}},{"$f":"+AD98","v":1.52},{"$f":"+AE101","v":{"$error":"#VALUE!"}},{"$f":"+AP121","v":1.84},null,null,null,null,{"$f":"+'C III-V'!Y109","v":1.75},{"$f":"+'C III-V'!Z109","v":1.2}]
["XIX",5.6800000000000006,{"$error":"#VALUE!"},null,null,null,null,null,null,"Vrijednosti X za poznati Y",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W110","v":4.2000010999999997},{"$f":"+'C III-V'!X110","v":1.2},{"$f":"+'C III-V'!Y110","v":1.75},{"$f":"+'C III-V'!Z110","v":9.6153895463470418E-2},null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!Y110","v":1.75},{"$f":"+'C III-V'!Z110","v":9.6153895463470418E-2}]
[{"$f":"+F129","v":"XX"},6,{"$error":"#VALUE!"},null,null,null,null,null,null,"X=",{"$f":"+L111/$K$109-$M$109/$K$109","v":{"$error":"#VALUE!"}},7.81," =Y",null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W111","v":4.2000010999999997},{"$f":"+'C III-V'!X111","v":1.2},{"$f":"-0.5*((Y101*Z102-Y102*Z101)+(Y102*Z103-Y103*Z102)+(Y103*Z104-Y104*Z103)+(Y104*Z105-Y105*Z104)+(Y105*Z106-Y106*Z105)+(Y106*Z107-Y107*Z106)+(Y107*Z108-Y108*Z107)+(Y108*Z109-Y109*Z108)+(Y109*Z110-Y110*Z109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AA101*AB102-AA102*AB101)+(AA102*AB103-AA103*AB102)+(AA103*AB104-AA104*AB103)+(AA104*AB105-AA105*AB104)+(AA105*AB106-AA106*AB105)+(AA106*AB107-AA107*AB106)+(AA107*AB108-AA108*AB107)+(AA108*AB109-AA109*AB108)+(AA109*AB110-AA110*AB109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AC101*AD102-AC102*AD101)+(AC102*AD103-AC103*AD102)+(AC103*AD104-AC104*AD103)+(AC104*AD105-AC105*AD104)+(AC105*AD106-AC106*AD105)+(AC106*AD107-AC107*AD106)+(AC107*AD108-AC108*AD107)+(AC108*AD109-AC109*AD108)+(AC109*AD110-AC110*AD109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AE101*AF102-AE102*AF101)+(AE102*AF103-AE103*AF102)+(AE103*AF104-AE104*AF103)+(AE104*AF105-AE105*AF104)+(AE105*AF106-AE106*AF105)+(AE106*AF107-AE107*AF106)+(AE107*AF108-AE108*AF107)+(AE108*AF109-AE109*AF108)+(AE109*AF110-AE110*AF109))","v":{"$error":"#VALUE!"}},"m2",null,null,null,null,{"$f":"-0.5*((AK101*AL102-AK102*AL101)+(AK102*AL103-AK103*AL102)+(AK103*AL104-AK104*AL103)+(AK104*AL105-AK105*AL104)+(AK105*AL106-AK106*AL105)+(AK106*AL107-AK107*AL106)+(AK107*AL108-AK108*AL107)+(AK108*AL109-AK109*AL108)+(AK109*AL110-AK110*AL109))","v":{"$error":"#VALUE!"}},"m2","OK","prosječna površina temelja od temelja kontrafore duž čitavog zida"]
[null,null,null,null,null,null,"Tlakovi",null,null,null,{"$f":"+L112/$K$109-$M$109/$K$109","v":{"$error":"#VALUE!"}},{"$f":"+G64","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W112","v":4.9000021999999994},{"$f":"+'C III-V'!X112","v":1.2},{"$f":"-((Y101*Z102-Y102*Z101)*(Y101+Y102)+(Y102*Z103-Y103*Z102)*(Y102+Y103)+(Y103*Z104-Y104*Z103)*(Y103+Y104)+(Y104*Z105-Y105*Z104)*(Y104+Y105)+(Y105*Z106-Y106*Z105)*(Y105+Y106)+(Y106*Z107-Y107*Z106)*(Y106+Y107)+(Y107*Z108-Y108*Z107)*(Y107+Y108)+(Y108*Z109-Y109*Z108)*(Y108+Y109)+(Y109*Z110-Y110*Z109)*(Y109+Y110))/6/Y111","v":{"$error":"#VALUE!"}},"m  ",{"$f":"-((AA101*AB102-AA102*AB101)*(AA101+AA102)+(AA102*AB103-AA103*AB102)*(AA102+AA103)+(AA103*AB104-AA104*AB103)*(AA103+AA104)+(AA104*AB105-AA105*AB104)*(AA104+AA105)+(AA105*AB106-AA106*AB105)*(AA105+AA106)+(AA106*AB107-AA107*AB106)*(AA106+AA107)+(AA107*AB108-AA108*AB107)*(AA107+AA108)+(AA108*AB109-AA109*AB108)*(AA108+AA109)+(AA109*AB110-AA110*AB109)*(AA109+AA110))/6/AA111","v":{"$error":"#VALUE!"}},"m  ",{"$f":"-((AC101*AD102-AC102*AD101)*(AC101+AC102)+(AC102*AD103-AC103*AD102)*(AC102+AC103)+(AC103*AD104-AC104*AD103)*(AC103+AC104)+(AC104*AD105-AC105*AD104)*(AC104+AC105)+(AC105*AD106-AC106*AD105)*(AC105+AC106)+(AC106*AD107-AC107*AD106)*(AC106+AC107)+(AC107*AD108-AC108*AD107)*(AC107+AC108)+(AC108*AD109-AC109*AD108)*(AC108+AC109)+(AC109*AD110-AC110*AD109)*(AC109+AC110))/6/AC111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AE101*AF102-AE102*AF101)*(AE101+AE102)+(AE102*AF103-AE103*AF102)*(AE102+AE103)+(AE103*AF104-AE104*AF103)*(AE103+AE104)+(AE104*AF105-AE105*AF104)*(AE104+AE105)+(AE105*AF106-AE106*AF105)*(AE105+AE106)+(AE106*AF107-AE107*AF106)*(AE106+AE107)+(AE107*AF108-AE108*AF107)*(AE107+AE108)+(AE108*AF109-AE109*AF108)*(AE108+AE109)+(AE109*AF110-AE110*AF109)*(AE109+AE110))/6/AE111","v":{"$error":"#VALUE!"}},"m",null,null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AK101+AK102)+(AK102*AL103-AK103*AL102)*(AK102+AK103)+(AK103*AL104-AK104*AL103)*(AK103+AK104)+(AK104*AL105-AK105*AL104)*(AK104+AK105)+(AK105*AL106-AK106*AL105)*(AK105+AK106)+(AK106*AL107-AK107*AL106)*(AK106+AK107)+(AK107*AL108-AK108*AL107)*(AK107+AK108)+(AK108*AL109-AK109*AL108)*(AK108+AK109)+(AK109*AL110-AK110*AL109)*(AK109+AK110))/6/AK111","v":{"$error":"#VALUE!"}},"m  "]
[null,null,null,null,null,{"$f":"+'C III-V'!F136:G136","v":"Visina presjeka"},null,{"$f":"+'C III-V'!H136:I136","v":"Intezitet"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W113","v":4.9000021999999994},{"$f":"+'C III-V'!X113","v":0.5},{"$f":"-((Y101*Z102-Y102*Z101)*(Z101+Z102)+(Y102*Z103-Y103*Z102)*(Z102+Z103)+(Y103*Z104-Y104*Z103)*(Z103+Z104)+(Y104*Z105-Y105*Z104)*(Z104+Z105)+(Y105*Z106-Y106*Z105)*(Z105+Z106)+(Y106*Z107-Y107*Z106)*(Z106+Z107)+(Y107*Z108-Y108*Z107)*(Z107+Z108)+(Y108*Z109-Y109*Z108)*(Z108+Z109)+(Y109*Z110-Y110*Z109)*(Z109+Z110))/6/Y111","v":{"$error":"#VALUE!"}},"m    ",{"$f":"-((AA101*AB102-AA102*AB101)*(AB101+AB102)+(AA102*AB103-AA103*AB102)*(AB102+AB103)+(AA103*AB104-AA104*AB103)*(AB103+AB104)+(AA104*AB105-AA105*AB104)*(AB104+AB105)+(AA105*AB106-AA106*AB105)*(AB105+AB106)+(AA106*AB107-AA107*AB106)*(AB106+AB107)+(AA107*AB108-AA108*AB107)*(AB107+AB108)+(AA108*AB109-AA109*AB108)*(AB108+AB109)+(AA109*AB110-AA110*AB109)*(AB109+AB110))/6/AA111","v":{"$error":"#VALUE!"}},"m    ",{"$f":"-((AC101*AD102-AC102*AD101)*(AD101+AD102)+(AC102*AD103-AC103*AD102)*(AD102+AD103)+(AC103*AD104-AC104*AD103)*(AD103+AD104)+(AC104*AD105-AC105*AD104)*(AD104+AD105)+(AC105*AD106-AC106*AD105)*(AD105+AD106)+(AC106*AD107-AC107*AD106)*(AD106+AD107)+(AC107*AD108-AC108*AD107)*(AD107+AD108)+(AC108*AD109-AC109*AD108)*(AD108+AD109)+(AC109*AD110-AC110*AD109)*(AD109+AD110))/6/AC111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AE101*AF102-AE102*AF101)*(AF101+AF102)+(AE102*AF103-AE103*AF102)*(AF102+AF103)+(AE103*AF104-AE104*AF103)*(AF103+AF104)+(AE104*AF105-AE105*AF104)*(AF104+AF105)+(AE105*AF106-AE106*AF105)*(AF105+AF106)+(AE106*AF107-AE107*AF106)*(AF106+AF107)+(AE107*AF108-AE108*AF107)*(AF107+AF108)+(AE108*AF109-AE109*AF108)*(AF108+AF109)+(AE109*AF110-AE110*AF109)*(AF109+AF110))/6/AE111","v":{"$error":"#VALUE!"}},"m",null,null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AL101+AL102)+(AK102*AL103-AK103*AL102)*(AL102+AL103)+(AK103*AL104-AK104*AL103)*(AL103+AL104)+(AK104*AL105-AK105*AL104)*(AL104+AL105)+(AK105*AL106-AK106*AL105)*(AL105+AL106)+(AK106*AL107-AK107*AL106)*(AL106+AL107)+(AK107*AL108-AK108*AL107)*(AL107+AL108)+(AK108*AL109-AK109*AL108)*(AL108+AL109)+(AK109*AL110-AK110*AL109)*(AL109+AL110))/6/AK111","v":{"$error":"#VALUE!"}},"m    ",null,{"$f":"+'C III-V'!AN113","v":-0.25},{"$f":"IF('Analiza i dimenzioniranje'!D84=\"\",0,'Analiza i dimenzioniranje'!D83+'C III-V'!AN113)","v":0.75}]
[null,null,null,null,null,{"$f":"+'C III-V'!F137","v":"III"},{"$f":"+'C III-V'!G137:H137","v":1.2},{"$f":"+'C III-V'!H137:I137","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!W114","v":2},{"$f":"+'C III-V'!X114","v":0.12820515121628623},{"$f":"+Y111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AA111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AC111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AE111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,{"$f":"+AK111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN"]
[null,null,null,null,null,{"$f":"+'C III-V'!F138","v":"VI"},{"$f":"+'C III-V'!G138:H138","v":1.52},{"$f":"+'C III-V'!H138:I138","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Teren  kosina",null,"Klizna ploha"]
[null,null,null,null,null,{"$f":"+'C III-V'!F139","v":"VII"},{"$f":"+'C III-V'!G139:H139","v":1.84},{"$f":"+'C III-V'!H139:I139","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AI116","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AJ116","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AK116","v":1.75},{"$f":"+'C III-V'!AL116","v":{"$error":"#VALUE!"}},null,"sjecišta  presjeka na kliznoj plohi i s leđima zida",null,null,null,null,null,null,null,null,null,null,null,null,null,"Omjer površine"]
[null,null,null,null,null,{"$f":"+'C III-V'!F140","v":"VIII"},{"$f":"+'C III-V'!G140:H140","v":2.16},{"$f":"+'C III-V'!H140:I140","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koord. Težište mase  za h22",null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AI117","v":6.2644906473896782},{"$f":"+'C III-V'!AJ117","v":6},{"$f":"+'C III-V'!AK117","v":0},{"$f":"+'C III-V'!AL117","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA100","v":"oznaka"},{"$f":"+'C III-V'!AB100","v":"X"},{"$f":"+'C III-V'!AC100","v":"Y"},null,null,null,null,null,null,null,null,null,null,"        sa kontraforama: bez kontrafora",null,null,"Potresna sila-prosječna"]
[null,null,null,null,null,{"$f":"+'C III-V'!F141","v":"IX"},{"$f":"+'C III-V'!G141:H141","v":2.48},{"$f":"+'C III-V'!H141:I141","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(AA101-AA102)/3","v":0.67810635947167019},{"$f":"+Z103*0.666666666666667","v":2.6666666666666679},null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!D116,AI117)","v":-5},{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!E116,'C III-V'!AJ117)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+'C III-V'!AA101","v":"Y=0"},{"$f":"+AP118/$K$109-$M$109/$K$109","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AC101","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Potresna sila","F","G"]
[null,null,null,null,null,{"$f":"+'C III-V'!F142","v":"X"},{"$f":"+'C III-V'!G142:H142","v":2.8},{"$f":"+'C III-V'!H142:I142","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"(AJ117-AI117)/(AJ116-AI116)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AI119*AI116+AI117","v":{"$error":"#VALUE!"}}," ",null,{"$f":"+'C III-V'!AA102","v":"PIII"},{"$f":"+'C III-V'!AB102","v":0.97707863658009864},{"$f":"+'C III-V'!AC102","v":1.2},null,null,null,null,null,null,null,null,null,null,null,"Ukupna duljina zida",null,{"$f":"+Kontrafore!E13","v":12},"m",{"$f":"+BD119","v":12},{"$f":"+Y111","v":{"$error":"#VALUE!"}},{"$f":"+Y114","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F143","v":"XI"},{"$f":"+'C III-V'!G143:H143","v":3.14},{"$f":"+'C III-V'!H143:I143","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"-(AL117-AK117)/(AK116-AL116)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-(AK116*AI120-AK117)","v":{"$error":"#VALUE!"}}," ",null,{"$f":"+'C III-V'!AA103","v":"PVI"},{"$f":"+'C III-V'!AB103","v":0.68324863210273346},{"$f":"+'C III-V'!AC103","v":1.52},null,null,null,null,null,null,null,null,null,null,null,"ukupna duljina kontrafora",null,{"$f":"+Kontrafore!E5*Kontrafore!E4","v":3},"m",{"$f":"+BD120","v":3},{"$f":"+BG119-BG121","v":{"$error":"#VALUE!"}},{"$f":"IF(BD120=BD119,0,BH119-BH121)","v":{"$error":"#VALUE!"}}]
["Presjek kroz zid I",null,"Presjek kroz zid II",null,null,{"$f":"+'C III-V'!F144","v":"XIII"},{"$f":"+'C III-V'!G144:H144","v":3.44},{"$f":"+'C III-V'!H144:I144","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AK120-AK119)/(AI119-AI120)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AI120*AI121+AK120","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!AA104","v":"PVII"},{"$f":"+'C III-V'!AB104","v":0.45866939675594048},{"$f":"+'C III-V'!AC104","v":1.84},null,null,null,null,null,null,null,null,null,null,null,"ukupna duljina bez kontrafora",null,{"$f":"+BD119-BD120","v":9},"m",{"$f":"+BF119-BF120","v":9},{"$f":"+AG111","v":0},{"$f":"+IF(BF121=0,0,AG114)","v":0}]
["x","y","x","y",null,{"$f":"+'C III-V'!F145","v":"XIII"},{"$f":"+'C III-V'!G145:H145","v":3.76},{"$f":"+'C III-V'!H145:I145","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA105","v":"PVIII"},{"$f":"+'C III-V'!AB105","v":0.23409016140914748},{"$f":"+'C III-V'!AC105","v":2.16},null,null,null,null,{"$f":"+'C III-V'!AT122","v":"Jednadžba kombi klizne plohe"},null,null,null,null,null,null,"površina s kontraforama",null,{"$f":"+BD120/BD119","v":0.25}]
[0,{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},{"$f":"+A123","v":0},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},null,{"$f":"+'C III-V'!F146","v":"XIV"},{"$f":"+'C III-V'!G146:H146","v":4.08},{"$f":"+'C III-V'!H146:I146","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA106","v":"PIX"},{"$f":"+'C III-V'!AB106","v":9.5109260623546556E-3},{"$f":"+'C III-V'!AC106","v":2.48},null,null,null,null,{"$f":"+AK104","v":{"$error":"#VALUE!"}},{"$f":"+AK101","v":1.75},null,null,null,null,null,"površina bez kontrafora",null,{"$f":"+BD121/BD119","v":0.75}]
[{"$f":"+F83","v":{"$error":"#VALUE!"}},{"$f":"+B123","v":1.84},{"$f":"+A124","v":{"$error":"#VALUE!"}},{"$f":"+D123","v":1.52},null,{"$f":"+'C III-V'!F147","v":"XV"},{"$f":"+'C III-V'!G147:H147","v":4.4000000000000004},{"$f":"+'C III-V'!H147:I147","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA107","v":"PX"},{"$f":"+'C III-V'!AB107","v":-0.21506830928443818},{"$f":"+'C III-V'!AC107","v":2.8},null,null,null,null,{"$f":"+AL104","v":{"$error":"#VALUE!"}},0,null,null,null,null,null,null,null,"odnos",null,{"$f":"-(BF120/BF119)*'Analiza i dimenzioniranje'!D83","v":-0.25}]
[null,null,null,null,null,{"$f":"+'C III-V'!F148","v":"XVI"},{"$f":"+'C III-V'!G148:H148","v":4.72},{"$f":"+'C III-V'!H148:I148","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA108","v":"PXI"},{"$f":"+'C III-V'!AB108","v":-0.45368374684040591},{"$f":"+'C III-V'!AC108","v":3.14},null,null,null,{"$f":"+'C III-V'!AT125","v":"Y="},{"$f":"(AV124-AU124)/(AV123-AU123)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AU125*AU123+AU124","v":{"$error":"#VALUE!"}},null,null,null,null,null,"krak",{"$f":"+Y113","v":{"$error":"#VALUE!"}},{"$f":"+BH119","v":{"$error":"#VALUE!"}},{"$f":"+BH120*BD122","v":{"$error":"#VALUE!"}},null,{"$f":"+BH119-BF126","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F149","v":"XVII"},{"$f":"+'C III-V'!G149:H149","v":5.04},{"$f":"+'C III-V'!H149:I149","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($AK$120-AK126)/$AI$120","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AK121","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!AA109","v":"PXII"},{"$f":"+'C III-V'!AB109","v":-0.66422677997802415},{"$f":"+'C III-V'!AC109","v":3.44},null,null,null,"Vrijednosti X za poznati Y",null,null,null,null,null,null,null,null,null,{"$f":"+AG113","v":0},{"$f":"+BH121","v":0},{"$f":"+BH120*BD123","v":{"$error":"#VALUE!"}},null,{"$f":"+BH121+BF125","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F150","v":"XVIII"},{"$f":"+'C III-V'!G150:H150","v":5.36},{"$f":"+'C III-V'!H150:I150","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},null,4.2,null,null,{"$f":"+'C III-V'!AA110","v":"PXIII"},{"$f":"+'C III-V'!AB110","v":-0.88880601532481696},{"$f":"+'C III-V'!AC110","v":3.76},null,null,null,"X=",{"$f":"+AL109","v":1.2},{"$f":"+AU127/$AU$125-$AW$125/$AU$125","v":{"$error":"#VALUE!"}}," = Y",null,null,null,null,null,null,null,null,"Prosječna masa za potres:",null,{"$f":"IF(IF(BC130=BD130,Y114,+BH126)=0,BH125,IF(BC130=BD130,Y114,+BH126))","v":{"$error":"#VALUE!"}},"kn"]
[null,null,null,null,null,{"$f":"+'C III-V'!F151","v":"XIX"},{"$f":"+'C III-V'!G151:H151","v":5.6800000000000006},{"$f":"+'C III-V'!H151:I151","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},null,1.2,null,null,{"$f":"+'C III-V'!AA111","v":"PXIV"},{"$f":"+'C III-V'!AB111","v":-1.1133852506716102},{"$f":"+'C III-V'!AC111","v":4.08}]
[null,null,null,null,null,{"$f":"+'C III-V'!F152","v":"XX"},{"$f":"+'C III-V'!G152:H152","v":6},{"$f":"+'C III-V'!H152:I152","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+AB104","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!AA112","v":"PXV"},{"$f":"+'C III-V'!AB112","v":-1.3379644860184032},{"$f":"+'C III-V'!AC112","v":4.4000000000000004}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+AD109","v":1.52},null,null,{"$f":"+'C III-V'!AA113","v":"PXVI"},{"$f":"+'C III-V'!AB113","v":-1.5625437213651958},{"$f":"+'C III-V'!AC113","v":4.72},null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+AG113","v":0},{"$f":"+Y113","v":{"$error":"#VALUE!"}},null,{"$f":"+AI109","v":0},{"$f":"+AI106","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+AF109","v":1.84},null,null,{"$f":"+'C III-V'!AA114","v":"PXVII"},{"$f":"+'C III-V'!AB114","v":-1.7871229567119888},{"$f":"+'C III-V'!AC114","v":5.04},null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+AG114","v":0},{"$f":"+Y114","v":{"$error":"#VALUE!"}},null,{"$f":"+AJ109","v":0},{"$f":"+AJ106","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+AI117","v":6.2644906473896782},null,null,{"$f":"+'C III-V'!AA115","v":"PXVIII"},{"$f":"+'C III-V'!AB115","v":-2.0117021920587819},{"$f":"+'C III-V'!AC115","v":5.36},null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"(BC131-BD131)/(BC130-BD130)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-BC132*BD130+BD131","v":{"$error":"#VALUE!"}},{"$f":"(BF131-BG131)/(BF130-BG130)","v":{"$error":"#DIV/0!"}},"*x    +",{"$f":"-BF132*BG130+BG131","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA116","v":"PXIX"},{"$f":"+'C III-V'!AB116","v":-2.2362814274055753},{"$f":"+'C III-V'!AC116","v":5.6800000000000006}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA117","v":"PXX"},{"$f":"+'C III-V'!AB117","v":0},{"$f":"+'C III-V'!AC117","v":6.0000000000000009},null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+AK113","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","Y",null,null,{"$f":"+AK136","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AC118","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,"xstv=",{"$f":"+BC134-X113","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AK136","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AL136","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,"            Masa da se dobije prosječni potres iz čelije AT125=",null,null,null,null,{"$f":"+BH125","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+AF104","v":{"$error":"#VALUE!"}},{"$f":"+AD102","v":1.52},{"$f":"+AF102","v":1.84},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"razlika¸površina",{"$f":"+Y111-AI111","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AE144-AC138)/(-AC144)","v":{"$error":"#VALUE!"}},{"$f":"IF(AD138<AC138,(AE151-AD138)/(-AC151),(AE156-AD138)/(-AC156))","v":{"$error":"#VALUE!"}},{"$f":"IF(AE138<AC138,(AE151-AE138)/(-AC151),(AE156-AE138)/(-AC156))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"duljina segmenta",{"$f":"++AJ105","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina III. sloja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"okomito na kliz. Plohu",null,{"$f":"+AY143/AY139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"d=","dodatak",{"$f":"+AY140/COS(AY142*PI()/180)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B2","v":2},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"          kut nagiba klizne plohe za potres   a= ",null,{"$f":"ATAN((-Y104+Y101)/(Z104-Z101))*180/PI()","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-5,{"$f":"+'C III-V'!AB154","v":9.9970360471948005},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dodatna površina",{"$f":"+AY144/'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+'C III-V'!AA155","v":-1.4281480067421144},"*x      +",{"$f":"+'C III-V'!AC154","v":2.8562960134842288},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"G=",{"$f":"+BF126","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AE144-AD146)/(-AC144)","v":1.1597509541483482}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+Z102","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina II. sloja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B9","v":{"$error":"#VALUE!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA149","v":0.97707863658009864},{"$f":"+'C III-V'!AB149","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+'C III-V'!AA150","v":-1.3763819204711734},"*x      +",{"$f":"+'C III-V'!AC149","v":2.5448333702674724}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina I. sloja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koordinate na sjecištu s terenom",null,null,{"$f":"+'C III-V'!AA144","v":-2.5846586698092704},{"$f":"+'C III-V'!AB144","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koordinate na sjecištu slojeva",null,null,{"$f":"+'C III-V'!AA143","v":-1.0572404418349119},{"$f":"+'C III-V'!AB143","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+'C III-V'!AA145","v":-1.4825609685127401},"*x      +",{"$f":"-AC156*AC154+AD154","v":2.4325765866023956}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rub dna konzole uz aktivni klin",null,null,{"$f":"+B6","v":{"$error":"#VALUE!"}},{"$f":"+C6","v":3.14}]

{"sheet":"C VIII-IX","index":41,"n_rows":157,"n_cols":50,"rows_kept":157,"cut":false,"hidden":true,"merged":[[94,0,94,4],[96,5,96,6],[116,44,116,46],[96,32,98,33],[96,34,98,35],[96,36,98,37],[99,32,99,33],[99,34,99,35],[99,36,99,37],[115,38,115,40],[110,38,113,38],[110,39,111,40],[112,39,113,39],[112,40,113,40],[114,34,114,35],[114,36,114,37],[90,1,90,2],[90,3,90,4],[90,5,90,6],[77,1,77,2],[77,8,77,9],[77,10,77,11],[77,15,77,16],[67,1,67,2],[67,3,67,4],[67,5,67,6],[67,8,67,9],[77,13,77,14],[67,22,67,23],[67,20,67,21],[67,15,67,16],[67,13,67,14],[67,10,67,11],[42,1,42,2],[42,3,42,4],[42,5,42,6],[42,7,43,10],[44,11,44,12],[44,7,44,8],[44,9,44,10],[42,11,43,14],[10,27,10,28],[11,3,11,4],[13,27,13,28],[17,12,17,16],[17,27,17,28],[10,3,10,4],[13,12,13,16],[12,27,12,28],[0,1,0,2],[0,3,0,4],[0,5,0,7],[0,9,0,10],[1,5,1,8],[42,15,43,18],[16,27,16,28],[44,21,44,22],[13,29,13,30],[63,15,63,16],[63,17,63,18],[26,27,26,28],[43,21,43,22],[63,13,63,14],[63,11,63,12],[44,13,44,14],[44,15,44,16],[62,29,62,30],[61,15,62,18],[61,11,62,14],[62,27,62,28],[44,17,44,18],[44,23,44,24],[44,25,44,26],[99,28,99,29],[99,30,99,31],[77,18,77,19],[99,26,99,27],[84,18,84,19],[96,22,97,23],[99,24,99,25]]}
["Točke","ZID I TEMELJ",null,"NASIP NA TEMELJU IZA",null,"ZID, KONZOLA I NASIP NA KONZOLI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Točka A",null,"Presjek VIII-VIII"]
[1,2,{"$f":"+'C III-V'!$C$2","v":0.12820515121628623},null,null,"ZA BILO KOJI PRESJEK ",null,null,null,null,null,null,null,null,null,null,null,"Presjek zid Iv",{"$f":"+($B$9-$B$4)*(T2-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},{"$f":"+B15","v":4.9000021999999994},{"$f":"+C15","v":0.5},{"$f":"+'C VIII-IX'!B10+0.05","v":{"$error":"#VALUE!"}},-0.5]
[2,2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T3-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},"Točka B",null,{"$f":"+W2","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!C10+0.5","v":{"$error":"#VALUE!"}}]
[3,{"$f":"+B3+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+C3","v":1.2},{"$f":"+B19","v":2},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>C4,B21,B4)","v":3.4000010999999999},{"$f":"IF(E20>C4,E20,C4)","v":1.2},{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},null,null,null,null,null,null,null,null,"Presjek V",{"$f":"+($B$9-$B$4)*(T4-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+'C VIII-IX'!B2","v":2},{"$f":"+'C VIII-IX'!C2","v":0.12820515121628623}]
[4,{"$f":"+B23","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},{"$f":"+D4","v":2},{"$f":"+'C VI-VII'!E5","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,B21,B5)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,E20,C5)","v":3.14},{"$f":"+F8","v":{"$error":"#VALUE!"}},{"$f":"+G8","v":3.44},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T5-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},null,null,"Presjek IX-IX",null,null,null,"Nasip na zidu iza"]
[5,{"$f":"+B5-'Analiza i dimenzioniranje'!G78","v":{"$error":"#VALUE!"}},{"$f":"+C5","v":3.14},{"$f":"IF(B6<2,B5,IF(B9>2,B9,D5))","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!E6","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C7,B21,B6)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C6,E20,C6)","v":3.14},{"$f":"IF(F7>F9,H5,F9)","v":{"$error":"#VALUE!"}},{"$f":"IF(F7>F9,I5,IF(E20>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C VIII-IX'!E20,G9))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"Presjek VI",{"$f":"+($B$9-$B$4)*(T6-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},"TLO 1. sloj",null,{"$f":"+'C VIII-IX'!B15-0.05","v":4.8500021999999996},{"$f":"+'C VIII-IX'!X2","v":-0.5},null,null,2,{"$f":"IF('Analiza i dimenzioniranje'!AW26>'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AW26)","v":0}]
[6,{"$f":"IF('Analiza i dimenzioniranje'!G78=0,'C VIII-IX'!B8,B6)","v":{"$error":"#VALUE!"}},{"$f":"C6+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+B4","v":3.4000010999999999},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>=C7,B21,B7)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C7,E20,C7)","v":3.44},{"$f":"IF(F7>F9,H6,H6)","v":{"$error":"#VALUE!"}},{"$f":"+I6","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T7-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},{"$f":"+'C VIII-IX'!B15-0.05","v":4.8500021999999996},{"$f":"+'C VIII-IX'!X3","v":{"$error":"#VALUE!"}},"Horizontala",null,2,{"$f":"'Analiza i dimenzioniranje'!BF28","v":0}]
[7,{"$f":"+B22","v":{"$error":"#VALUE!"}},{"$f":"+C7","v":3.44},{"$f":"+D4","v":2},{"$f":"+E4","v":1.2},{"$f":"IF(E20>C8,B21,B8)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C8,E20,C8)","v":3.44},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$H$15=0,I7+(H7-H8)*'Unos podataka'!R57,IF('C III-V'!H9>'Unos podataka'!$B$105,I7+(H7-H8)*'Unos podataka'!$R$55,'Unos podataka'!$T$57))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"Presjek VII",{"$f":"+($B$9-$B$4)*(T8-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!V8","v":6},null,null,{"$f":"+'C VIII-IX'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!C5","v":3.14}]
[8,{"$f":"B4-TAN('Analiza i dimenzioniranje'!H51*PI()/180)*('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},null,null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"+I4","v":3.44},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T9-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+U8-'Analiza i dimenzioniranje'!E27","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!V9","v":6.2644906473896782},"Presjek ZID",null,{"$f":"+IF('Analiza i dimenzioniranje'!$E$24=0,0,'C VIII-IX'!Y4)","v":0},{"$f":"+Z8","v":3.14}]
[9,{"$f":"+B9+'Analiza i dimenzioniranje'!E54","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},null,null,{"$f":"+B10","v":{"$error":"#VALUE!"}},{"$f":"+C10","v":"A"},null,null,null,null,null,null,null,null,null,null,"Presjek VIII",{"$f":"+($B$9-$B$4)*(T10-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},-8,{"$f":"+'C III-V'!V10","v":6.2644906473896782},{"$f":"+'C VIII-IX'!B15-0.5","v":4.4000021999999994},{"$f":"+'C VIII-IX'!C10+0.1","v":{"$error":"#VALUE!"}}]
[10,{"$f":"+B4+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+C3","v":1.2},"NASIP NA KONZOLI",null,{"$f":"+F12+E65","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C11,E20,C11)","v":1.2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T11-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},"x","y",{"$f":"+'C VIII-IX'!B10+0.5","v":{"$error":"#VALUE!"}},{"$f":"+X10","v":{"$error":"#VALUE!"}},null,null,null,"Rsidra"]
[11,{"$f":"+B11","v":4.2000010999999997},{"$f":"+C11","v":1.2},"za stabilnost",null,{"$f":"+F4","v":3.4000010999999999},{"$f":"+G4","v":1.2},null,null,null,null,null,null,null,null,null,null,"Presjek IX",{"$f":"+($B$9-$B$4)*(T12-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+W23","v":{"$error":"#VALUE!"}},{"$f":"+U12*(V9-V8)/(U9-U8)-U8*(V9-V8)/(U9-U8)+V8","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,20,AB16)","v":20},{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,0,AC16)","v":0}]
[12,{"$f":"+B12","v":4.2000010999999997},{"$f":"+C12","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T13-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+W25","v":{"$error":"#VALUE!"}},{"$f":"+U13*(V9-V8)/(U9-U8)-U8*(V9-V8)/(U9-U8)+V8","v":{"$error":"#VALUE!"}},"Pad terena niz padinu",null,null,null,null,"Os rezultante sidara Ukupna računska sila u sidrima"]
[13,{"$f":"+B11+'Analiza i dimenzioniranje'!G57","v":4.9000021999999994},{"$f":"+C13","v":1.2},{"$f":"+B7","v":{"$error":"#VALUE!"}},3.44,null,null,null,null,"Linija presjeka",null,null," Koordinata sredine presjeka",null,null,null,null,"Presjek X",{"$f":"+($B$9-$B$4)*(T14-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},"TLO 2. sloj",null,{"$f":"+'Analiza i dimenzioniranje'!Q105","v":3},{"$f":"+'Analiza i dimenzioniranje'!P105","v":{"$error":"#VALUE!"}},null,null,null,"Slobodna  zona.",null,"1. sloj"]
[14,{"$f":"+B14","v":4.9000021999999994},{"$f":"+C14-'Analiza i dimenzioniranje'!E51","v":0.5},{"$error":"#VALUE!"},3.44,{"$f":"IF((B4-B9)=0,0,+(C9-C4)/(B4-B9))","v":{"$error":"#VALUE!"}},"n  Nagib zida u tlu",null,null,0,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,"III-III","konzola","Presjek VIII-VIII","Presjek IX",null,{"$f":"+($B$11-$B$10)*(T15-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},{"$f":"IF(('Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17)<'Analiza i dimenzioniranje'!$F$45,2,(IF(B7<B24,B7,IF('Analiza i dimenzioniranje'!G78=0,'C VIII-IX'!B24,2))))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17","v":4},{"$f":"+'Analiza i dimenzioniranje'!O130","v":7.1000021999999996},{"$f":"+'Analiza i dimenzioniranje'!N130","v":1.5001009999999999},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,AB24)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,'Analiza i dimenzioniranje'!P22)","v":5},{"$f":"+U9","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782}]
[15,{"$f":"+B2","v":2},{"$f":"+C2","v":0.12820515121628623},{"$error":"#VALUE!"},"A",null,null,null,null,3,{"$f":"+K15","v":1.2},null,"x",{"$f":"+(F12+F11)/2","v":{"$error":"#VALUE!"}},{"$f":"(B8+(B11-B10)*(O17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U29+(B11-B10)*(P17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U34+(B11-B10)*(Q17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},"Presjek XI",{"$f":"+($B$9-$B$4)*(T16-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},-8,{"$f":"+V15+(U15-U16)*TAN('Analiza i dimenzioniranje'!$E$18*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"AB15-'Analiza i dimenzioniranje'!P23","v":{"$error":"#VALUE!"}},{"$f":"+AC15-(AB15-AB16)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782}]
[null,null,"Jednadžba pravca zida uz tlo",{"$f":"+D16","v":{"$error":"#VALUE!"}},{"$f":"+I7","v":{"$error":"#VALUE!"}},null,null,null,null,"Sloj 2 gore",null,null,"y",{"$f":"+G11","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},null,{"$f":"+($B$11-$B$10)*(T17-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},"TLO 3. sloj",null,"Prometno opterećenje",null,null,null,null,"Sidrena dionica",null,"Jednadžba površine terena"]
[null,"x","y",{"$f":"+D14","v":{"$error":"#VALUE!"}},{"$f":"+I8","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+F94","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E52>=G94,0,G94)","v":4},null,null,null,null,null,null,"Presjek XII",{"$f":"+($B$9-$B$4)*(T18-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},2,{"$f":"+'Analiza i dimenzioniranje'!$F$17","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,+'C VIII-IX'!B9-'Analiza i dimenzioniranje'!E26)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,'C VIII-IX'!V9)","v":6.2644906473896782},null,null,null,"                   Y=",null,{"$f":"+(AE16-AE15)/(AD16-AD15)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AD18*AD15+AE15","v":{"$error":"#VALUE!"}}]
[null,2,{"$f":"+B19*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},{"$f":"+D14","v":{"$error":"#VALUE!"}},{"$f":"+E14","v":3.44},null,null,null,null,{"$f":"U16","v":-8},{"$f":"+K18","v":4},null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T19-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},-8,{"$f":"+V18+(U18-U19)*TAN('Analiza i dimenzioniranje'!$F$18*PI()/180)","v":1.5492076949174773},{"$f":"+W18","v":{"$error":"#VALUE!"}},{"$f":"+X18+'Analiza i dimenzioniranje'!E24/50","v":6.4644906473896784},null,null,null,{"$f":"+AB16","v":{"$error":"#VALUE!"}},{"$f":"+AC16","v":{"$error":"#VALUE!"}},"za x=",{"$f":"+AB20","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+H8","v":{"$error":"#VALUE!"}},{"$f":"+B20*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},"M na koti",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,"Sloj 1 ili2 dole",null,null,null,null,null,null,{"$f":"+(B11-B10)*(Q21-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},"Presjek XIII",{"$f":"+($B$9-$B$4)*(T20-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},"KONTAKTNI NAPONI",null,{"$f":"+W18-'Analiza i dimenzioniranje'!E25","v":{"$error":"#VALUE!"}},{"$f":"+X19","v":6.4644906473896784},null,null,null,{"$f":"+(AB21+AB19)/2","v":{"$error":"#VALUE!"}},{"$f":"+(AC19+AC21)/2","v":{"$error":"#VALUE!"}},"y=",{"$f":"+AD18*AE19+AF18","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C21-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,{"$f":"+IF('Analiza i dimenzioniranje'!G78=0,D8,H8)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+F95","v":{"$error":"#VALUE!"}},{"$f":"+G12","v":1.2},null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,{"$f":"+($B$11-$B$10)*(T21-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},2,0,{"$f":"+W20","v":{"$error":"#VALUE!"}},{"$f":"+X18","v":6.2644906473896782},null,null,null,{"$f":"+AB19-'Analiza i dimenzioniranje'!P24","v":{"$error":"#VALUE!"}},{"$f":"+AC19-(AB19-AB21)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},"visina sloja iznad centra sidra"]
[null,{"$f":"+(B9-B4)*(C22-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+C23+'Analiza i dimenzioniranje'!C77","v":3.44},null,null,null,null,null,null,{"$f":"+U19","v":-8},{"$f":"+K21","v":1.2},null,null,null,null,null,null,"Presjek XIV",{"$f":"+($B$9-$B$4)*(T22-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},2,{"$f":"-'Analiza i dimenzioniranje'!$F$193/100","v":{"$error":"#VALUE!"}},"Točkasto",null,null,null,null,null,null,{"$f":"+AE20-AC20","v":{"$error":"#VALUE!"}},"m"]
[null,{"$f":"+(B9-B4)*(C23-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T23-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"2+'Analiza i dimenzioniranje'!$E$61","v":4.9000021999999994},{"$f":"-'Analiza i dimenzioniranje'!$F$190/100","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E36=0,-10,B9-'Analiza i dimenzioniranje'!E37)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X23","v":{"$error":"#VALUE!"}},null,null,null,"Jednadžba  lica zida "]
[null,{"$f":"+(B9-B4)*(C24-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V15","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek XV",{"$f":"+($B$9-$B$4)*(T24-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U23","v":4.9000021999999994},0,"Linijsko iza zida",null,null,null,"x=",{"$f":"+($B$11-$B$10)*(AB25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+($B$11-$B$10)*(AC25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+(B11-B10)*(AE25-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C25-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U21","v":2},0,{"$f":"IF('Analiza i dimenzioniranje'!$E$34=0,0,B9-'Analiza i dimenzioniranje'!K28)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X27","v":{"$error":"#VALUE!"}},null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!X42","v":170.21276595744681},{"$f":"+'Analiza i dimenzioniranje'!Y42","v":170.21276595744681},null,{"$f":"+'Analiza i dimenzioniranje'!H76+'Analiza i dimenzioniranje'!E52","v":1.5001009999999999}]
[null,{"$f":"+(B9-B4)*(C26-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid IX-IX",{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+W25","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$34=0,0,X25+1)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!T22","v":0},null,null,null,null,{"$f":"+B14-AE24","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C27-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},"TEMELJ -opterećenje",null,"x=",{"$f":"+($B$11-$B$10)*(Z26-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"Rez. Sidra na zidu"]
[null,{"$f":"+(B9-B4)*(C26-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},null,null,"+",null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V27","v":2.48},{"$f":"+IF('Analiza i dimenzioniranje'!E28=0,0,W29)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9+'Analiza i dimenzioniranje'!F20+1.5)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!S22","v":0}]
["Sjecište s dnom temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V29-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":2.48},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W30-0.3)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X30)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z28-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+($B$11-$B$10)*(AC29-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E40","v":3.9999999960000001},{"$f":"+AB29+0.4","v":{"$error":"#VALUE!"}},{"$f":"+AC29+(AD29-AB29)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}}]
["zid",{"$f":"+B20","v":{"$error":"#VALUE!"}},{"$f":"+B30*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V30-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":2.48},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,B9-'Analiza i dimenzioniranje'!$E$32)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X31+'Analiza i dimenzioniranje'!E33)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!R22","v":0},null,null,null,{"$f":"+AB29-1","v":{"$error":"#VALUE!"}},{"$f":"+AC29-(AB29-AD30)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}}]
["Vrh zida",{"$f":"+(B9-B4)*(C31-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C558","v":-0.45},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid Iv",{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},{"$f":"+W30","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9-'Analiza i dimenzioniranje'!K31)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z30-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"nagib lica"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,W31-'Analiza i dimenzioniranje'!$E$29)","v":{"$error":"#VALUE!"}},{"$f":"+X31","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q22","v":3},null,"tan"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V32","v":2.16},{"$f":"+W32","v":{"$error":"#VALUE!"}},{"$f":"+X30","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z32-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+(B13-B10)/(C10-C13)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V34-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V33","v":2.16},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W33+0.3)","v":{"$error":"#VALUE!"}},{"$f":"+X29","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q20","v":5},null,"kut"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V35-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V34","v":2.16},{"$f":"+W34","v":{"$error":"#VALUE!"}},{"$f":"+X28","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z34-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+ATAN(AB33)*180/PI()","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SIDRO za presjek",null,null,null,"Jednadžba pravca lica zida ",null,null,"Sjecište a arm konzole",null,"vrh zida","Anker armatura uz lice",null,"arm dno",null,"Y=",{"$f":"IF(AE38=AE37,1000000,(AF38-AF37)/(AE38-AE37))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AJ36*AE37+AF37","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!$C$545","v":1.6923077248520526}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB15)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC15)","v":5},null,null,"x=",null,null,{"$f":"+(B11-B10)*(AB38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AC38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AD38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AF37-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!B545","v":{"$error":"#VALUE!"}},{"$f":"+U81","v":2.0499999999999998},{"$f":"+V81","v":0.18682583433163008},"X=",{"$f":"+(-AL36+AL39)/(AJ36-AJ39)","v":{"$error":"#VALUE!"}},"sjeište",null,"x=",{"$f":"+(AN36-AL36)/AJ36","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB16)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC16)","v":{"$error":"#VALUE!"}},null,null,"y=",null,null,{"$f":"+'Analiza i dimenzioniranje'!E555","v":3.39},{"$f":"+AB38-'Analiza i dimenzioniranje'!#REF!","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!C558","v":-0.45},{"$f":"+(B11-B10)*(AF38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+U82","v":4.8600021999999994},{"$f":"+V82","v":0.54310345350772504},"Y=",{"$f":"+AJ36*AJ37+AL36","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate dna temelja",null,null,null,null,null,null,"Y=",{"$f":"+(AH38-AH37)/(AG38-AG37)","v":0.12678908905341604},"*x",{"$f":"-AJ39*AG37+AH37","v":-7.3091798227872762E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"lice","koord Pr II",{"$f":"+AB47+'Analiza i dimenzioniranje'!Q58","v":3.4500010999999997},{"$f":"(AB40*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24999999999999994},null,"SIDRO"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+(B11-B10)*(Z42-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+B8","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+AB15","v":{"$error":"#VALUE!"}},{"$f":"+AC15","v":5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+Z42","v":3.44},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,AB15-0.5)","v":{"$error":"#VALUE!"}},{"$f":"+AF41-(AE41-AE42)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},null,"Nasip ispred zida"]
["Oznaka","temelj",null,"Zid i konzola za pr. ZID",null,"Nasip na temelju iza zida",null,"      Za momente u presjeku zid-temelj    III-III      ",null,null,null,"      Za momente u presjeku VIII-VIII",null,null,null,"         Za momente u presjeku IX-IX",null,null,null,null,null,null,null,null,null,null,null,2,0,null,null,null,null,{"$f":"+AE24","v":{"$error":"#VALUE!"}},{"$f":"+C11+'Analiza i dimenzioniranje'!$H$76","v":1.5001009999999999}]
["točke","x","y","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - BETON",null,null,null,null,null,2.65,{"$f":"+(AC47+AC49)/2","v":0.31034478180740688},null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!$E$61","v":4.9000021999999994},{"$f":"+AI43","v":1.5001009999999999}]
[1,{"$f":"+'C VIII-IX'!B2","v":2},{"$f":"+'C VIII-IX'!C2","v":0.12820515121628623},null,null,null,null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"Kontaktni naponi za stab",null,"Beton do presjeka II-II",null,"Beton sredine temelja",null,"Beton do presjeka I-I",null,{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"(AB45*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH44+1.6","v":6.5000021999999991},{"$f":"+AI44-(AH45-AH44)*TAN('Analiza i dimenzioniranje'!H22*PI()/180)","v":1.5001009999999999}]
[2,{"$f":"+'C VIII-IX'!B3","v":2},{"$f":"+'C VIII-IX'!C3","v":1.2},null,null,null,null,"x","y","x","y","x","y","x","y","x","y","x","y","x","y",null,null,"x","y","x","y",{"$f":"+(AB43+AB47)/2","v":2.7000005499999999},{"$f":"(AB46*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.1206896584423281},null,null,null,null,"x","y"]
[3,{"$f":"+'C VIII-IX'!B4","v":3.4000010999999999},{"$f":"+'C VIII-IX'!C4","v":1.2},{"$f":"+B4","v":3.4000010999999999},1.2,2,1.2,3.4000010999999999,1.2,{"$f":"+D14","v":{"$error":"#VALUE!"}},3.44,{"$f":"+U34","v":{"$error":"#VALUE!"}},{"$f":"+V34","v":2.16},{"$f":"+J47","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!X44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!X44,K47)","v":3.44},{"$f":"+U29","v":{"$error":"#VALUE!"}},{"$f":"+V29","v":2.48},{"$f":"+J47","v":{"$error":"#VALUE!"}},{"$f":"+S48","v":3.44},{"$f":"+U21","v":2},{"$f":"+V21*100","v":0},2,0,{"$f":"+B4","v":3.4000010999999999},{"$f":"+W49","v":1.2},{"$f":"+B11","v":4.2000010999999997},1.2,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"(AB47*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24137931688465614},"Presjek IX-IX",null,null,null,{"$f":"+'C VIII-IX'!B11","v":4.2000010999999997},{"$f":"+C11","v":1.2}]
[4,{"$f":"+B11","v":4.2000010999999997},1.2,{"$error":"#VALUE!"},3.14,2,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.44,{"$f":"+H48","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!X44<'Analiza i dimenzioniranje'!F45,I48,'C VIII-IX'!V34)","v":3.14},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!X44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!X44,K48)","v":3.44},{"$f":"+H48","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!Y44<'Analiza i dimenzioniranje'!F45,I48,V29)","v":3.14},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!Y44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!Y44,K48)","v":3.44},{"$f":"+U22","v":2},{"$f":"+V22*100","v":{"$error":"#VALUE!"}},2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+X47+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+Y47","v":1.2},4.2000010999999997,1.2,{"$f":"+AB77","v":{"$error":"#VALUE!"}},{"$f":"(AB48*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47+'Analiza i dimenzioniranje'!H76","v":1.5001009999999999}]
[5,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.14,{"$f":"+D16","v":{"$error":"#VALUE!"}},{"$f":"+E16+'Unos podataka'!$F9","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!X44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C VIII-IX'!L47,'C VIII-IX'!B6)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!X44<'Analiza i dimenzioniranje'!F45,I49,'C VIII-IX'!V34)","v":3.14},{"$f":"+D16","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!X44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!X44,K49)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!Y44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C VIII-IX'!B6,P47)","v":{"$error":"#VALUE!"}},{"$f":"+Q48","v":3.14},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!Y44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!Y44,K49)","v":{"$error":"#VALUE!"}},{"$f":"+U23","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},{"$f":"+V48+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+W48","v":1.2},{"$f":"+AB49","v":4.2000010999999997},{"$f":"+AC49","v":0.37931024673015767},4.2000010999999997,1.2,{"$f":"+AB47+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+(AB49*(AC43-AC53)/(AB43-AB53)-AB53*(AC43-AC53)/(AB43-AB53)+AC53)","v":0.37931024673015767},"Presjek VIII-VIII",null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+AI48","v":1.5001009999999999}]
[6,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.44,3.4000010999999999,1.2,{"$error":"#VALUE!"},3.44,{"$f":"IF('Unos podataka'!$B$105>J47,'Unos podataka'!$B$105,J47)","v":{"$error":"#VALUE!"}},{"$f":"+K51","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!X44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C VIII-IX'!L48,'C VIII-IX'!B7)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!X44<='Analiza i dimenzioniranje'!F45,I50,'C VIII-IX'!V34)","v":3.44},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!X44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!X44,K50)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!Y44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C VIII-IX'!P47,H50)","v":{"$error":"#VALUE!"}},{"$f":"+S47","v":3.44},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!Y44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!Y44,K50)","v":{"$error":"#VALUE!"}},{"$f":"+U24","v":4.9000021999999994},{"$f":"+V24*100","v":0},{"$f":"+V49","v":3.4000010999999999},{"$f":"+AC47","v":0.24137931688465614},{"$f":"+X47","v":3.4000010999999999},{"$f":"+AC47","v":0.24137931688465614},4.9000021999999994,1.2,{"$f":"2+'Analiza i dimenzioniranje'!E61/2","v":3.4500010999999997},{"$f":"(AB50*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24999999999999994},null,null,null,null,{"$f":"+AH49","v":4.9000021999999994},{"$f":"+C14","v":1.2}]
[7,4.9000021999999994,1.2,{"$error":"#VALUE!"},3.44,2,1.2,{"$error":"#VALUE!"},3.44,{"$error":"#VALUE!"},{"$f":"+E18+'Unos podataka'!$F9","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!X44>'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C VIII-IX'!B28,B8)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!X44>='Analiza i dimenzioniranje'!I75+'Analiza i dimenzioniranje'!G67,'C VIII-IX'!M50,Z26)","v":3.44},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!X44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!X44,K51)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!Y44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C VIII-IX'!B25,H51)","v":{"$error":"#VALUE!"}},{"$f":"+Q50","v":3.44},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!Y44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!Y44,K51)","v":{"$error":"#VALUE!"}},{"$f":"+U25","v":2},{"$f":"+V25*100","v":0},{"$f":"+V47","v":2},{"$f":"+W47","v":0},{"$f":"+X47","v":3.4000010999999999},{"$f":"+Y47","v":1.2},4.9000021999999994,0.5,{"$f":"+(AB49+AB53)/2","v":4.5500016499999996},{"$f":"(AB51*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.43965512336507878},null,null,null,null,{"$f":"+B13","v":4.2000010999999997},{"$f":"+C13","v":1.2}]
[8,4.9000021999999994,0.5,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",{"$error":"#VALUE!"},3.44,{"$f":"+H52","v":{"$error":"#VALUE!"}},{"$f":"+Q52","v":"A"},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!X44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!X44,K52)","v":3.44},{"$f":"+H52","v":{"$error":"#VALUE!"}},{"$f":"+I52","v":"A"},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!Y44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!Y44,K52)","v":3.44},null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AC49","v":0.37931024673015767},{"$f":"+AD77","v":{"$error":"#VALUE!"}},{"$f":"(AB52*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH51","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[9,2,0.12820515121628623,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",null,null,{"$f":"+H53","v":{"$error":"#VALUE!"}},{"$f":"+Q53","v":"A"},null,null,{"$f":"+H53","v":{"$error":"#VALUE!"}},{"$f":"+I53","v":"A"},null,null,null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AA47","v":1.2},{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+C15","v":0.5},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[10,null,null,4.2000010999999997,1.2,null,null,{"$error":"#VALUE!"},1.2,null,null,{"$f":"+U35","v":{"$error":"#VALUE!"}},{"$f":"+M47","v":2.16},null,null,{"$f":"+U30","v":{"$error":"#VALUE!"}},{"$f":"+V30","v":2.48},null,null,null,null,null,null,null,null,null,null,"Koordinate s","naprezanjem"]
[11,null,null,{"$f":"+D47","v":3.4000010999999999},{"$f":"+E47","v":1.2},null,null,3.4000010999999999,1.2,null,null,{"$f":"+L47","v":{"$error":"#VALUE!"}},{"$f":"+M47","v":2.16},null,null,{"$f":"+P47","v":{"$error":"#VALUE!"}},{"$f":"+Q47","v":2.48},null,null,null,null,null,null,null,null,null,null,{"$f":"+U22","v":2},{"$f":"+V22*100","v":{"$error":"#VALUE!"}}]
[12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+AB56*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
[13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AB57*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
["  A=",{"$f":"-0.5*((B45*C46-B46*C45)+(B46*C47-B47*C46)+(B47*C48-B48*C47)+(B48*C49-B49*C48)+(B49*C50-B50*C49)+(B50*C51-B51*C50)+(B51*C52-B52*C51)+(B52*C53-B53*C52))","v":2.5691044797107181},"m2",{"$f":"-0.5*((D45*E46-D46*E45)+(D46*E47-D47*E46)+(D47*E48-D48*E47)+(D48*E49-D49*E48)+(D49*E50-D50*E49)+(D50*E51-D51*E50)+(D51*E52-D52*E51)+(D52*E53-D53*E52)+(D53*E54-D54*E53)+(D54*E55-D55*E54)+(D55*E56-D56*E55)+(D56*E57-D57*E56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((F45*G46-F46*G45)+(F46*G47-F47*G46)+(F47*G48-F48*G47)+(F48*G49-F49*G48)+(F49*G50-F50*G49)+(F50*G51-F51*G50)+(F51*G52-F52*G51)+(F52*G53-F53*G52)+(F53*G54-F54*G53)+(F54*G55-F55*G54)+(F55*G56-F56*G55)+(F56*G57-F57*G56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((H47*I48-H48*I47)+(H48*I49-H49*I48)+(H49*I50-H50*I49)+(H50*I51-H51*I50)+(H51*I52-H52*I51)+(H52*I53-H53*I52)+(H53*I54-H54*I53)+(H54*I55-H55*I54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((J47*K48-J48*K47)+(J48*K49-J49*K48)+(J49*K50-J50*K49)+(J50*K51-J51*K50)+(J51*K52-J52*K51)+(J52*K53-J53*K52)+(J53*K54-J54*K53)+(J54*K55-J55*K54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((L47*M48-L48*M47)+(L48*M49-L49*M48)+(L49*M50-L50*M49)+(L50*M51-L51*M50)+(L51*M52-L52*M51)+(L52*M53-L53*M52)+(L53*M54-L54*M53)+(L54*M55-L55*M54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"IF(0.5*((N47*O48-N48*O47)+(N48*O49-N49*O48)+(N49*O50-N50*O49)+(N50*O51-N51*O50)+(N51*O52-N52*O51)+(N52*O53-N53*O52)+(N53*O54-N54*O53)+(N54*O55-N55*O54))<0,0,0.5*((N47*O48-N48*O47)+(N48*O49-N49*O48)+(N49*O50-N50*O49)+(N50*O51-N51*O50)+(N51*O52-N52*O51)+(N52*O53-N53*O52)+(N53*O54-N54*O53)+(N54*O55-N55*O54)))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((P47*Q48-P48*Q47)+(P48*Q49-P49*Q48)+(P49*Q50-P50*Q49)+(P50*Q51-P51*Q50)+(P51*Q52-P52*Q51)+(P52*Q53-P53*Q52)+(P53*Q54-P54*Q53)+(P54*Q55-P55*Q54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((R47*S48-R48*S47)+(R48*S49-R49*S48)+(R49*S50-R50*S49)+(R50*S51-R51*S50)+(R51*S52-R52*S51)+(R52*S53-R53*S52)+(R53*S54-R54*S53)+(R54*S55-R55*S54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((T47*U48-T48*U47)+(T48*U49-T49*U48)+(T49*U50-T50*U49)+(T50*U51-T51*U50)+(T51*U52-T52*U51)+(T52*U53-T53*U52)+(T53*U54-T54*U53)+(T54*U55-T55*U54))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((V47*W48-V48*W47)+(V48*W49-V49*W48)+(V49*W50-V50*W49)+(V50*W51-V51*W50))","v":1.5110356654221164},"m2",{"$f":"-0.5*((X47*Y48-X48*Y47)+(X48*Y49-X49*Y48)+(X49*Y50-X50*Y49)+(X50*Y51-X51*Y50))","v":0.71172417455407389},"m2",{"$f":"-0.5*((Z47*AA48-Z48*AA47)+(Z48*AA49-Z49*AA48)+(Z49*AA50-Z50*AA49)+(Z50*AA51-Z51*AA50)+(Z51*AA52-Z52*AA51)+(Z52*AA53-Z53*AA52)+(Z53*AA54-Z54*AA53)+(Z54*AA55-Z55*AA54))","v":0.53224225002380887},"m2",{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-0.5*((AH47*AI48-AH48*AI47)+(AH48*AI49-AH49*AI48)+(AH49*AI50-AH50*AI49)+(AH50*AI51-AH51*AI50)+(AH51*AI52-AH52*AI51)+(AH52*AI53-AH53*AI52)+(AH53*AI54-AH54*AI53)+(AH54*AI55-AH55*AI54))","v":0.21007103011109951},"m2"]
["xt=",{"$f":"-((B45*C46-B46*C45)*(B45+B46)+(B46*C47-B47*C46)*(B46+B47)+(B47*C48-B48*C47)*(B47+B48)+(B48*C49-B49*C48)*(B48+B49)+(B49*C50-B50*C49)*(B49+B50)+(B50*C51-B51*C50)*(B50+B51)+(B51*C52-B52*C51)*(B51+B52)+(B52*C53-B53*C52)*(B52+B53)+(B53*C54-B54*C53)*(B53+B54)+(B54*C55-B55*C54)*(B54+B55)+(B55*C56-B56*C55)*(B55+B56)+(B56*C57-B57*C56)*(B56+B57))/6/B58","v":3.3485779696489133},"m",{"$f":"-((D45*E46-D46*E45)*(D45+D46)+(D46*E47-D47*E46)*(D46+D47)+(D47*E48-D48*E47)*(D47+D48)+(D48*E49-D49*E48)*(D48+D49)+(D49*E50-D50*E49)*(D49+D50)+(D50*E51-D51*E50)*(D50+D51)+(D51*E52-D52*E51)*(D51+D52)+(D52*E53-D53*E52)*(D52+D53)+(D53*E54-D54*E53)*(D53+D54)+(D54*E55-D55*E54)*(D54+D55)+(D55*E56-D56*E55)*(D55+D56)+(D56*E57-D57*E56)*(D56+D57))/6/D58","v":{"$error":"#VALUE!"}},"m",{"$f":"-((F45*G46-F46*G45)*(F45+F46)+(F46*G47-F47*G46)*(F46+F47)+(F47*G48-F48*G47)*(F47+F48)+(F48*G49-F49*G48)*(F48+F49)+(F49*G50-F50*G49)*(F49+F50)+(F50*G51-F51*G50)*(F50+F51)+(F51*G52-F52*G51)*(F51+F52)+(F52*G53-F53*G52)*(F52+F53)+(F53*G54-F54*G53)*(F53+F54)+(F54*G55-F55*G54)*(F54+F55)+(F55*G56-F56*G55)*(F55+F56)+(F56*G57-F57*G56)*(F56+F57))/6/F58","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(H47*I48-H48*I47)*(H47+H48)+(H48*I49-H49*I48)*(H48+H49)+(H49*I50-H50*I49)*(H49+H50)+(H50*I51-H51*I50)*(H50+H51)+(H51*I52-H52*I51)*(H51+H52)+(H52*I53-H53*I52)*(H52+H53)+(H53*I54-H54*I53)*(H53+H54)+(H54*I55-H55*I54)*(H54+H55))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(J47+J48)+(J48*K49-J49*K48)*(J48+J49)+(J49*K50-J50*K49)*(J49+J50)+(J50*K51-J51*K50)*(J50+J51)+(J51*K52-J52*K51)*(J51+J52)+(J52*K53-J53*K52)*(J52+J53)+(J53*K54-J54*K53)*(J53+J54)+(J54*K55-J55*K54)*(J54+J55)+(J55*K56-J56*K55)*(J55+J56)+(J56*K57-J57*K56)*(J56+J57))/6/J58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(L47*M48-L48*M47)*(L47+L48)+(L48*M49-L49*M48)*(L48+L49)+(L49*M50-L50*M49)*(L49+L50)+(L50*M51-L51*M50)*(L50+L51)+(L51*M52-L52*M51)*(L51+L52)+(L52*M53-L53*M52)*(L52+L53)+(L53*M54-L54*M53)*(L53+L54)+(L54*M55-L55*M54)*(L54+L55))/6/L58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(N58=0,0,(+(N47*O48-N48*O47)*(N47+N48)+(N48*O49-N49*O48)*(N48+N49)+(N49*O50-N50*O49)*(N49+N50)+(N50*O51-N51*O50)*(N50+N51)+(N51*O52-N52*O51)*(N51+N52))/6/N58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(P47*Q48-P48*Q47)*(P47+P48)+(P48*Q49-P49*Q48)*(P48+P49)+(P49*Q50-P50*Q49)*(P49+P50)+(P50*Q51-P51*Q50)*(P50+P51)+(P51*Q52-P52*Q51)*(P51+P52)+(P52*Q53-P53*Q52)*(P52+P53)+(P53*Q54-P54*Q53)*(P53+P54)+(P54*Q55-P55*Q54)*(P54+P55))/6/P58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(R58=0,0,(+(R47*S48-R48*S47)*(R47+R48)+(R48*S49-R49*S48)*(R48+R49)+(R49*S50-R50*S49)*(R49+R50)+(R50*S51-R51*S50)*(R50+R51)+(R51*S52-R52*S51)*(R51+R52))/6/R58)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(T58=0,0,(+(T47*U48-T48*U47)*(T47+T48)+(T48*U49-T49*U48)*(T48+T49)+(T49*U50-T50*U49)*(T49+T50)+(T50*U51-T51*U50)*(T50+T51)+(T51*U52-T52*U51)*(T51+T52)+(T52*U53-T53*U52)*(T52+T53)+(T53*U54-T54*U53)*(T53+T54)+(T54*U55-T55*U54)*(T54+T55)+(T55*U56-T56*U55)*(T55+T56)+(T56*U57-T57*U56)*(T56+T57))/6/T58)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(V58=0,0,-(+(V47*W48-V48*W47)*(V47+V48)+(V48*W49-V49*W48)*(V48+V49)+(V49*W50-V50*W49)*(V49+V50)+(V50*W51-V51*W50)*(V50+V51))/6/V58)","v":2.6739089419190427},"m",{"$f":"IF(X58=0,0,-(+(X47*Y48-X48*Y47)*(X47+X48)+(X48*Y49-X49*Y48)*(X48+X49)+(X49*Y50-X50*Y49)*(X49+X50)+(X50*Y51-X51*Y50)*(X50+X51))/6/X58)","v":3.7896651910602248},"m",{"$f":"-(+(Z47*AA48-Z48*AA47)*(Z47+Z48)+(Z48*AA49-Z49*AA48)*(Z48+Z49)+(Z49*AA50-Z50*AA49)*(Z49+Z50)+(Z50*AA51-Z51*AA50)*(Z50+Z51)+(Z51*AA52-Z52*AA51)*(Z51+Z52)+(Z52*AA53-Z53*AA52)*(Z52+Z53)+(Z53*AA54-Z54*AA53)*(Z53+Z54)+(Z54*AA55-Z55*AA54)*(Z54+Z55)+(Z55*AA56-Z56*AA55)*(Z55+Z56)+(Z56*AA57-Z57*AA56)*(Z56+Z57))/6/Z58","v":4.5407423692617748},"m",null,null,null,null,"   Koordinate presjeka",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AH47+AH48)+(AH48*AI49-AH49*AI48)*(AH48+AH49)+(AH49*AI50-AH50*AI49)*(AH49+AH50)+(AH50*AI51-AH51*AI50)*(AH50+AH51)+(AH51*AI52-AH52*AI51)*(AH51+AH52)+(AH52*AI53-AH53*AI52)*(AH52+AH53)+(AH53*AI54-AH54*AI53)*(AH53+AH54)+(AH54*AI55-AH55*AI54)*(AH54+AH55)+(AH55*AI56-AH56*AI55)*(AH55+AH56)+(AH56*AI57-AH57*AI56)*(AH56+AH57))/6/AH58","v":4.550001650000004},"m"]
["yt=",{"$f":"-((B45*C46-B46*C45)*(C45+C46)+(B46*C47-B47*C46)*(C46+C47)+(B47*C48-B48*C47)*(C47+C48)+(B48*C49-B49*C48)*(C48+C49)+(B49*C50-B50*C49)*(C49+C50)+(B50*C51-B51*C50)*(C50+C51)+(B51*C52-B52*C51)*(C51+C52)+(B52*C53-B53*C52)*(C52+C53)+(B53*C54-B54*C53)*(C53+C54)+(B54*C55-B55*C54)*(C54+C55)+(B55*C56-B56*C55)*(C55+C56)+(B56*C57-B57*C56)*(C56+C57))/6/B58","v":0.75054981042380386},"m",{"$f":"-((D45*E46-D46*E45)*(E45+E46)+(D46*E47-D47*E46)*(E46+E47)+(D47*E48-D48*E47)*(E47+E48)+(D48*E49-D49*E48)*(E48+E49)+(D49*E50-D50*E49)*(E49+E50)+(D50*E51-D51*E50)*(E50+E51)+(D51*E52-D52*E51)*(E51+E52)+(D52*E53-D53*E52)*(E52+E53)+(D53*E54-D54*E53)*(E53+E54)+(D54*E55-D55*E54)*(E54+E55)+(D55*E56-D56*E55)*(E55+E56)+(D56*E57-D57*E56)*(E56+E57))/6/D58","v":{"$error":"#VALUE!"}},"m",{"$f":"-((F45*G46-F46*G45)*(G45+G46)+(F46*G47-F47*G46)*(G46+G47)+(F47*G48-F48*G47)*(G47+G48)+(F48*G49-F49*G48)*(G48+G49)+(F49*G50-F50*G49)*(G49+G50)+(F50*G51-F51*G50)*(G50+G51)+(F51*G52-F52*G51)*(G51+G52)+(F52*G53-F53*G52)*(G52+G53)+(F53*G54-F54*G53)*(G53+G54)+(F54*G55-F55*G54)*(G54+G55)+(F55*G56-F56*G55)*(G55+G56)+(F56*G57-F57*G56)*(G56+G57))/6/F58","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(H47*I48-H48*I47)*(I47+I48)+(H48*I49-H49*I48)*(I48+I49)+(H49*I50-H50*I49)*(I49+I50)+(H50*I51-H51*I50)*(I50+I51)+(H51*I52-H52*I51)*(I51+I52)+(H52*I53-H53*I52)*(I52+I53)+(H53*I54-H54*I53)*(I53+I54)+(H54*I55-H55*I54)*(I54+I55)+(H55*I56-H56*I55)*(I55+I56)+(H56*I57-H57*I56)*(I56+I57))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(K47+K48)+(J48*K49-J49*K48)*(K48+K49)+(J49*K50-J50*K49)*(K49+K50)+(J50*K51-J51*K50)*(K50+K51)+(J51*K52-J52*K51)*(K51+K52)+(J52*K53-J53*K52)*(K52+K53)+(J53*K54-J54*K53)*(K53+K54)+(J54*K55-J55*K54)*(K54+K55)+(J55*K56-J56*K55)*(K55+K56)+(J56*K57-J57*K56)*(K56+K57))/6/J58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(L47*M48-L48*M47)*(M47+M48)+(L48*M49-L49*M48)*(M48+M49)+(L49*M50-L50*M49)*(M49+M50)+(L50*M51-L51*M50)*(M50+M51)+(L51*M52-L52*M51)*(M51+M52)+(L52*M53-L53*M52)*(M52+M53)+(L53*M54-L54*M53)*(M53+M54)+(L54*M55-L55*M54)*(M54+M55))/6/L58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(N58=0,0,(+(N47*O48-N48*O47)*(O47+O48)+(N48*O49-N49*O48)*(O48+O49)+(N49*O50-N50*O49)*(O49+O50)+(N50*O51-N51*O50)*(O50+O51)+(N51*O52-N52*O51)*(O51+O52)+(N52*O53-N53*O52)*(O52+O53)+(N53*O54-N54*O53)*(O53+O54)+(N54*O55-N55*O54)*(O54+O55)+(N55*O56-N56*O55)*(O55+O56)+(N56*O57-N57*O56)*(O56+O57))/6/N58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(P47*Q48-P48*Q47)*(Q47+Q48)+(P48*Q49-P49*Q48)*(Q48+Q49)+(P49*Q50-P50*Q49)*(Q49+Q50)+(P50*Q51-P51*Q50)*(Q50+Q51)+(P51*Q52-P52*Q51)*(Q51+Q52)+(P52*Q53-P53*Q52)*(Q52+Q53)+(P53*Q54-P54*Q53)*(Q53+Q54)+(P54*Q55-P55*Q54)*(Q54+Q55))/6/P58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(R58=0,0,(+(R47*S48-R48*S47)*(S47+S48)+(R48*S49-R49*S48)*(S48+S49)+(R49*S50-R50*S49)*(S49+S50)+(R50*S51-R51*S50)*(S50+S51)+(R51*S52-R52*S51)*(S51+S52)+(R52*S53-R53*S52)*(S52+S53)+(R53*S54-R54*S53)*(S53+S54)+(R54*S55-R55*S54)*(S54+S55)+(R55*S56-R56*S55)*(S55+S56)+(R56*S57-R57*S56)*(S56+S57))/6/R58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-IF(T58=0,0,(+(T47*U48-T48*U47)*(U47+U48)+(T48*U49-T49*U48)*(U48+U49)+(T49*U50-T50*U49)*(U49+U50)+(T50*U51-T51*U50)*(U50+U51)+(T51*U52-T52*U51)*(U51+U52)+(T52*U53-T53*U52)*(U52+U53)+(T53*U54-T54*U53)*(U53+U54)+(T54*U55-T55*U54)*(U54+U55)+(T55*U56-T56*U55)*(U55+U56)+(T56*U57-T57*U56)*(U56+U57))/6/T58)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((V47*W48-V48*W47)*(W47+W48)+(V48*W49-V49*W48)*(W48+W49)+(V49*W50-V50*W49)*(W49+W50)+(V50*W51-V51*W50)*(W50+W51))/6/V58","v":0.65809555436880718},"kN",{"$f":"-((X47*Y48-X48*Y47)*(Y47+Y48)+(X48*Y49-X49*Y48)*(Y48+Y49)+(X49*Y50-X50*Y49)*(Y49+Y50)+(X50*Y51-X51*Y50)*(Y50+Y51))/6/X58","v":0.75428136494691478},"kN",{"$f":"-(+(Z47*AA48-Z48*AA47)*(AA47+AA48)+(Z48*AA49-Z49*AA48)*(AA48+AA49)+(Z49*AA50-Z50*AA49)*(AA49+AA50)+(Z50*AA51-Z51*AA50)*(AA50+AA51)+(Z51*AA52-Z52*AA51)*(AA51+AA52)+(Z52*AA53-Z53*AA52)*(AA52+AA53)+(Z53*AA54-Z54*AA53)*(AA53+AA54)+(Z54*AA55-Z55*AA54)*(AA54+AA55)+(Z55*AA56-Z56*AA55)*(AA55+AA56)+(Z56*AA57-Z57*AA56)*(AA56+AA57))/6/Z58","v":0.81902934843133712},"m",null,null,null,null,"II-II i I-I",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AI47+AI48)+(AH48*AI49-AH49*AI48)*(AI48+AI49)+(AH49*AI50-AH50*AI49)*(AI49+AI50)+(AH50*AI51-AH51*AI50)*(AI50+AI51)+(AH51*AI52-AH52*AI51)*(AI51+AI52)+(AH52*AI53-AH53*AI52)*(AI52+AI53)+(AH53*AI54-AH54*AI53)*(AI53+AI54)+(AH54*AI55-AH55*AI54)*(AI54+AI55)+(AH55*AI56-AH56*AI55)*(AI55+AI56)+(AH56*AI57-AH57*AI56)*(AI56+AI57))/6/AH58","v":1.3500505000000005},"m"]
["G=",{"$f":"+B58*'Analiza i dimenzioniranje'!E62","v":64.227611992767947},"kN",{"$f":"+D58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"+F58*'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}},"kN",{"$f":"+H58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(J58*'Analiza i dimenzioniranje'!E63<0,0,J58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+L58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(N58*'Analiza i dimenzioniranje'!U41<0,0,N58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+P58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(R58<=0,0,R58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+T58*'Analiza i dimenzioniranje'!E49","v":{"$error":"#VALUE!"}},"kN (za L)",{"$f":"+V58*'Analiza i dimenzioniranje'!E62","v":37.77589163555291},"kN",{"$f":"+X58*'Analiza i dimenzioniranje'!E62","v":17.793104363851846},"kN",{"$f":"+Z58*'Analiza i dimenzioniranje'!E62","v":13.306056250595223},"kN",null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"AC47+'Analiza i dimenzioniranje'!C192/2","v":0.68753317931068247},{"$f":"+AH58*'Analiza i dimenzioniranje'!E62","v":5.2517757527774878},"kN"]
["Vertikala nasipa na konzoli",null,null,"Moment na konzoli",null,"Pokos na vrhu zida",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - NAPONI ",null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+'C VIII-IX'!AC49+('Analiza i dimenzioniranje'!C191/2)","v":0.77418208680245293}]
[null,"x","y",{"$f":"IF('Analiza i dimenzioniranje'!G78=0,0,'Analiza i dimenzioniranje'!G78*'Analiza i dimenzioniranje'!C77*'Analiza i dimenzioniranje'!E62*(Q20-B5+'Analiza i dimenzioniranje'!G78/2)+J61*(O16-J59))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"+F64","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"naponi za Presjek IX-IX",null,"naponi za srednji dio ",null,"naponi za Presjek VIII-VIII"]
[null,{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},"b1=",{"$f":"+H47-2","v":1.4000010999999999},{"$f":"+B52","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y","x","y","x","y","Koordinate dna temelja"]
[null,{"$f":"+B64","v":{"$error":"#VALUE!"}},{"$f":"IF(B65>J49,C19,+C20+'Analiza i dimenzioniranje'!F20+(H52-H50)*TAN('Analiza i dimenzioniranje'!F21*PI()/180))","v":{"$error":"#VALUE!"}},"b2=",{"$f":"'Analiza i dimenzioniranje'!E54+('Analiza i dimenzioniranje'!E55-'Analiza i dimenzioniranje'!E54)*(('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)/(C9-C4))","v":{"$error":"#VALUE!"}},{"$f":"+B65","v":{"$error":"#VALUE!"}},{"$f":"+G64+(F64-F65)*TAN('Analiza i dimenzioniranje'!F21*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,0,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},0,{"$f":"+'C VIII-IX'!B11","v":4.2000010999999997},{"$f":"-U47","v":0},2,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z65","v":2},{"$f":"AC55","v":{"$error":"#VALUE!"}},{"$f":"+AB65","v":3.4000010999999999},{"$f":"+AA67","v":{"$error":"#VALUE!"}},{"$f":"+AB57","v":4.2000010999999997},{"$f":"AC57","v":{"$error":"#VALUE!"}},{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"(AF66*(AG70-AG65)/(AF70-AF65)-AF65*(AG70-AG65)/(AF70-AF65)+AG65)","v":{"$error":"#VALUE!"}}]
[null,"AKTIVNI TLAKOVI za stabilnost i Presjek III-III (bez E3)",null,null,null,null,null,null,"  AKTIVNI TLAKOVI za presjek kroz zid VIII-VIII",null,null,null,null,"    AKTIVNI TLAKOVI za presjek kroz zid IX-IX",null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"AC56","v":{"$error":"#VALUE!"}},{"$f":"+AB66+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AE66","v":{"$error":"#VALUE!"}},{"$f":"+AB58","v":4.9000021999999994},{"$f":"+AC58","v":{"$error":"#VALUE!"}},{"$f":"+AB77","v":{"$error":"#VALUE!"}},{"$f":"+(AF67*(AG65-AG70)/(AF65-AF70)-AF70*(AG65-AG70)/(AF65-AF70)+AG70)","v":{"$error":"#VALUE!"}}]
[null,"E1",null,"E2",null,"E3",null,null,"E1",null,"E2 do presjeka kroz zid II",null,null,"E1",null,"E2",null,null,null,null,null,null,null,null,null,{"$f":"+Z67","v":3.4000010999999999},0,{"$f":"+AB67","v":4.2000010999999997},0,{"$f":"+AD67","v":4.9000021999999994},{"$f":"+U50","v":0},{"$f":"+AB67","v":4.2000010999999997},{"$f":"+(AF68*(AG65-AG70)/(AF65-AF70)-AF70*(AG65-AG70)/(AF65-AF70)+AG70)","v":0.37931024673015767}]
[null,0,{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C71","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,{"$f":"+N69","v":0},{"$f":"+O69","v":{"$error":"#VALUE!"}},{"$f":"+D69","v":{"$error":"#VALUE!"}},{"$f":"+J71","v":{"$error":"#VALUE!"}},null,{"$f":"+B69","v":0},{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+K69","v":{"$error":"#VALUE!"}},{"$f":"+O71","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"+Z65","v":2},0,{"$f":"+AB65","v":3.4000010999999999},0,{"$f":"+AD65","v":4.2000010999999997},{"$f":"+U51","v":0},{"$f":"+AD77","v":{"$error":"#VALUE!"}},{"$f":"+(AF69*(AG66-AG70)/(AF66-AF70)-AF70*(AG66-AG70)/(AF66-AF70)+AG70)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+B69","v":0},{"$f":"+C69-'Analiza i dimenzioniranje'!D17-'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+D69+'Analiza i dimenzioniranje'!E16*'Analiza i dimenzioniranje'!E17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+E69-'Analiza i dimenzioniranje'!E17","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},null,{"$f":"+N70","v":0},{"$f":"+J69-('Analiza i dimenzioniranje'!F20+'P VIII-VIII'!E17)","v":{"$error":"#VALUE!"}},{"$f":"+K69+'P VIII-VIII'!F16*'P VIII-VIII'!F17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},null,{"$f":"+B70","v":0},{"$f":"+O69-('Analiza i dimenzioniranje'!F20+'P IX-IX'!E17)","v":{"$error":"#VALUE!"}},{"$f":"+P69+'P IX-IX'!F16*'P IX-IX'!F17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AB53","v":4.9000021999999994},{"$f":"+AC53","v":0.5}]
[null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('Analiza i dimenzioniranje'!D17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},0,{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F70+'Analiza i dimenzioniranje'!F16*'Analiza i dimenzioniranje'!F17*'Analiza i dimenzioniranje'!F112","v":{"$error":"#VALUE!"}},0,null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('P VIII-VIII'!E17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+J70","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+L70","v":2.16},null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('P IX-IX'!E17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+Q70","v":2.48}]
[null,{"$f":"+B69","v":0},{"$f":"+C69","v":{"$error":"#VALUE!"}},0,{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F69","v":0},0,null,{"$f":"+N72","v":0},{"$f":"+O72","v":{"$error":"#VALUE!"}},{"$f":"+D72","v":0},{"$f":"+L69","v":{"$error":"#VALUE!"}},null,{"$f":"+N69","v":0},{"$f":"+O69","v":{"$error":"#VALUE!"}},{"$f":"+D72","v":0},{"$f":"+Q69","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+D69","v":{"$error":"#VALUE!"}},{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F72","v":0},{"$f":"+G70","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+K69","v":{"$error":"#VALUE!"}},{"$f":"+L69","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+P69","v":{"$error":"#VALUE!"}},{"$f":"+Q69","v":{"$error":"#VALUE!"}}]
["Jednadžba vertikale kohezije    Određivanje sjecišta kohezije s pravcem od tlaka",null,null,null,null,null,null,{"$f":"+M74","v":"Jednadžba vertikale kohezije  -  sjecišta kohezije s pravcem od tlaka"},null,null,null,null,"Jednadžba vertikale kohezije  -  sjecišta kohezije s pravcem od tlaka"]
[null,"X","y","X","y","X","y",null,{"$f":"+N75","v":"X"},{"$f":"+O75","v":"y"},"X","y",null,"X","y","X","y"]
[null,{"$f":"2*'Analiza i dimenzioniranje'!D15/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F110)","v":12.361875887090893},{"$f":"B76*(C71-C72)/(B71-B72)-B72*(C71-C72)/(B71-B72)+C72","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!F12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F111)","v":{"$error":"#VALUE!"}},{"$f":"IF(D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69>'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69)","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!C12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F112)","v":{"$error":"#VALUE!"}},{"$f":"IF((F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70)>'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!F17,(F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70))","v":{"$error":"#VALUE!"}},null,{"$f":"+N76","v":12.361875887090893},{"$f":"I76*(J71-J72)/(I71-I72)-I72*(J71-J72)/(I71-I72)+J72","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},null,{"$f":"+B76","v":12.361875887090893},{"$f":"N76*(O71-O72)/(N71-N72)-N72*(O71-O72)/(N71-N72)+O72","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"-0.5*((Z65*AA66-Z66*AA65)+(Z66*AA67-Z67*AA66)+(Z67*AA68-Z68*AA67)+(Z68*AA69-Z69*AA68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((AB65*AC66-AB66*AC65)+(AB66*AC67-AB67*AC66)+(AB67*AC68-AB68*AC67)+(AB68*AC69-AB69*AC68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((AD65*AE66-AD66*AE65)+(AD66*AE67-AD67*AE66)+(AD67*AE68-AD68*AE67)+(AD68*AE69-AD69*AE68)+(AD69*AE70-AD70*AE69)+(AD70*AE71-AD71*AE70)+(AD71*AE72-AD72*AE71)+(AD72*AE73-AD73*AE72))","v":{"$error":"#VALUE!"}},"kN/m'"]
[null,{"$f":"+B76","v":12.361875887090893},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},null,{"$f":"+N77","v":12.361875887090893},{"$f":"+O77","v":{"$error":"#VALUE!"}},{"$f":"+K76","v":{"$error":"#VALUE!"}},{"$f":"+G101","v":2.16},null,{"$f":"+N76","v":12.361875887090893},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+P76","v":{"$error":"#VALUE!"}},{"$f":"+G102","v":2.48},null,null,null,null,null,null,null,null,{"$f":"IF(Z76=0,0,-(+(Z65*AA66-Z66*AA65)*(Z65+Z66)+(Z66*AA67-Z67*AA66)*(Z66+Z67)+(Z67*AA68-Z68*AA67)*(Z67+Z68)+(Z68*AA69-Z69*AA68)*(Z68+Z69))/6/Z76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(AB76=0,0,-(+(AB65*AC66-AB66*AC65)*(AB65+AB66)+(AB66*AC67-AB67*AC66)*(AB66+AB67)+(AB67*AC68-AB68*AC67)*(AB67+AB68)+(AB68*AC69-AB69*AC68)*(AB68+AB69))/6/AB76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(AD76=0,0,-(+(AD65*AE66-AD66*AE65)*(AD65+AD66)+(AD66*AE67-AD67*AE66)*(AD66+AD67)+(AD67*AE68-AD68*AE67)*(AD67+AD68)+(AD68*AE69-AD69*AE68)*(AD68+AD69))/6/AD76)","v":{"$error":"#VALUE!"}},"m"]
["Oznaka","E1",null,"E2",null,"E3",null,{"$f":"+M78","v":"Oznaka"},{"$f":"+N78","v":"E1"},null,"E2",null,"Oznaka","E1",null,"E2",null,null,null,null,null,null,null,null,null,{"$f":"-((Z65*AA66-Z66*AA65)*(AA65+AA66)+(Z66*AA67-Z67*AA66)*(AA66+AA67)+(Z67*AA68-Z68*AA67)*(AA67+AA68)+(Z68*AA69-Z69*AA68)*(AA68+AA69))/6/Z76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((AB65*AC66-AB66*AC65)*(AC65+AC66)+(AB66*AC67-AB67*AC66)*(AC66+AC67)+(AB67*AC68-AB68*AC67)*(AC67+AC68)+(AB68*AC69-AB69*AC68)*(AC68+AC69))/6/AB76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((AD65*AE66-AD66*AE65)*(AE65+AE66)+(AD66*AE67-AD67*AE66)*(AE66+AE67)+(AD67*AE68-AD68*AE67)*(AE67+AE68)+(AD68*AE69-AD69*AE68)*(AE68+AE69))/6/AD76","v":{"$error":"#VALUE!"}},"kN/m'"]
["točke","x","y","x","y","x","y","točke",{"$f":"+N79","v":"x"},{"$f":"+O79","v":"y"},"x","y","točke","x","y","x","y"]
[1,{"$f":"+B77","v":12.361875887090893},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,1,{"$f":"+I76","v":12.361875887090893},{"$f":"+J76","v":{"$error":"#VALUE!"}},{"$f":"+K76","v":{"$error":"#VALUE!"}},{"$f":"+L76","v":{"$error":"#VALUE!"}},1,{"$f":"+N76","v":12.361875887090893},{"$f":"+O76","v":{"$error":"#VALUE!"}},{"$f":"+P76","v":{"$error":"#VALUE!"}},{"$f":"+Q76","v":{"$error":"#VALUE!"}},null,"Jedn pravca zida uz tlo",null,"Jedn pravca arm dno ",null,"Y=",{"$f":"IF(S82=S81,1000000,(T82-T81)/(S82-S81))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X80*S81+T81","v":{"$error":"#VALUE!"}}]
[2,{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G76","v":{"$error":"#VALUE!"}},2,{"$f":"+I71","v":{"$error":"#VALUE!"}},{"$f":"+J71","v":{"$error":"#VALUE!"}},{"$f":"+K69","v":{"$error":"#VALUE!"}},{"$f":"+L69","v":{"$error":"#VALUE!"}},2,{"$f":"+N71","v":{"$error":"#VALUE!"}},{"$f":"+O71","v":{"$error":"#VALUE!"}},{"$f":"+P69","v":{"$error":"#VALUE!"}},{"$f":"+Q69","v":{"$error":"#VALUE!"}},null,{"$f":"+B4","v":3.4000010999999999},{"$f":"+C4","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!T593","v":2.0499999999999998},{"$f":"+'Analiza i dimenzioniranje'!U593","v":0.18682583433163008},"X=",{"$f":"+(-Z80+Z83)/(X80-X83)","v":{"$error":"#VALUE!"}},"sjeište"]
[3,{"$f":"+B80","v":12.361875887090893},{"$f":"+C76","v":{"$error":"#VALUE!"}},{"$f":"IF(D76>D69,D81,D69)","v":{"$error":"#VALUE!"}},{"$f":"+E81","v":{"$error":"#VALUE!"}},{"$f":"IF(F77>F70,F77,F70)","v":{"$error":"#VALUE!"}},{"$f":"IF(F77>F70,G76,G70)","v":{"$error":"#VALUE!"}},3,{"$f":"+I80","v":12.361875887090893},{"$f":"+J81","v":{"$error":"#VALUE!"}},{"$f":"+K70","v":{"$error":"#VALUE!"}},{"$f":"+L70","v":2.16},3,{"$f":"+N77","v":12.361875887090893},{"$f":"+O77","v":{"$error":"#VALUE!"}},{"$f":"+P70","v":{"$error":"#VALUE!"}},{"$f":"+Q70","v":2.48},null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},{"$f":"+'Analiza i dimenzioniranje'!T594","v":4.8600021999999994},{"$f":"+'Analiza i dimenzioniranje'!U594","v":0.54310345350772504},"Y=",{"$f":"+X80*X81+Z80","v":{"$error":"#VALUE!"}}]
[4,{"$f":"+B80","v":12.361875887090893},{"$f":"+C80","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F71","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},4,{"$f":"+I76","v":12.361875887090893},{"$f":"+J76","v":{"$error":"#VALUE!"}},{"$f":"+K77","v":{"$error":"#VALUE!"}},{"$f":"+L77","v":2.16},4,{"$f":"+N76","v":12.361875887090893},{"$f":"+O76","v":{"$error":"#VALUE!"}},{"$f":"+P84","v":{"$error":"#VALUE!"}},{"$f":"+IF('Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17<'Analiza i dimenzioniranje'!Y44,0,'C VIII-IX'!Q82)","v":2.48},null,null,null,null,null,"Y=",{"$f":"+(V82-V81)/(U82-U81)","v":0.12678908905341604},"*x",{"$f":"-X83*U81+V81","v":-7.3091798227872762E-2},"CRTANJE"]
[5,null,null,{"$f":"+D80","v":{"$error":"#VALUE!"}},{"$f":"+E80","v":{"$error":"#VALUE!"}},{"$f":"+F80","v":{"$error":"#VALUE!"}},{"$f":"+G80","v":0},5,null,null,{"$f":"+K76","v":{"$error":"#VALUE!"}},{"$f":"+L76","v":{"$error":"#VALUE!"}},5,null,null,{"$f":"+P80","v":{"$error":"#VALUE!"}},{"$f":"+Q80","v":{"$error":"#VALUE!"}},null,"Jedn pravca sloja 3",null,"Jedn pravca sloja 3 klizno",null,"Y=",{"$f":"+(T86-T85)/(S86-S85)","v":-3.4920769491747737E-2},"*x",{"$f":"-X84*S85+T85","v":1.2698415389834954},"Jedn pravca sloja 3 klizno",null,"sjecište 1/2 sidra sa vrhom 1. sloja"]
["  A=",{"$f":"IF(B77>B71,0,-IF(B84>B83,0,-0.5*((B80*C81-B81*C80)+(B81*C82-B82*C81)+(B82*C83-B83*C82)+(B83*C84-B84*C83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D77>D70,0,IF(D84>D83,0,-0.5*((D80*E81-D81*E80)+(D81*E82-D82*E81)+(D82*E83-D83*E82)+(D83*E84-D84*E83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F77>F71,0,IF(F84>F83,0,-0.5*((F80*G81-F81*G80)+(F81*G82-F82*G81)+(F82*G83-F83*G82)+(F83*G84-F84*G83))))","v":{"$error":"#VALUE!"}},"kN/m'","  A=",{"$f":"IF(J77>J76,0,-0.5*((I80*J81-I81*J80)+(I81*J82-I82*J81)+(I82*J83-I83*J82)+(I83*J84-I84*J83)))","v":{"$error":"#VALUE!"}},{"$f":"+O85","v":"kN/m'"},{"$f":"IF(L77>L76,0,-0.5*((K80*L81-K81*L80)+(K81*L82-K82*L81)+(K82*L83-K83*L82)+(K83*L84-K84*L83)))","v":{"$error":"#VALUE!"}},"kN/m'","  A=",{"$f":"IF(O77>O76,0,-0.5*((N80*O81-N81*O80)+(N81*O82-N82*O81)+(N82*O83-N83*O82)+(N83*O84-N84*O83)))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(Q77>Q76,0,-0.5*((P80*Q81-P81*Q80)+(P81*Q82-P82*Q81)+(P82*Q83-P83*Q82)+(P83*Q84-P84*Q83)))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+U18","v":2},{"$f":"+V18","v":1.2},{"$f":"+W100","v":2},0,"X=",{"$f":"+(-Z84+Z87)/(X84-X87)","v":1.1386903959986558},"sjecište ",null,{"$f":"+U85","v":2},{"$f":"+V85","v":0},"Y=",{"$f":"+X92","v":{"$error":"#VALUE!"}},"*x",{"$f":"+Z92","v":{"$error":"#VALUE!"}}]
["xt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(B80+B81)+(B81*C82-B82*C81)*(B81+B82)+(B82*C83-B83*C82)*(B82+B83)+(B83*C84-B84*C83)*(B83+B84))/6/B85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(D80+D81)+(D81*E82-D82*E81)*(D81+D82)+(D82*E83-D83*E82)*(D82+D83)+(D83*E84-D84*E83)*(D83+D84))/6/D85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(F80+F81)+(F81*G82-F82*G81)*(F81+F82)+(F82*G83-F83*G82)*(F82+F83)+(F83*G84-F84*G83)*(F83+F84))/6/F85)","v":{"$error":"#VALUE!"}},"kN/m'","xt=",{"$f":"IF(I85=0,0,-((I80*J81-I81*J80)*(I80+I81)+(I81*J82-I82*J81)*(I81+I82)+(I82*J83-I83*J82)*(I82+I83)+(I83*J84-I84*J83)*(I83+I84))/6/I85)","v":{"$error":"#VALUE!"}},{"$f":"+O86","v":"kN/m'"},{"$f":"IF(K85=0,0,((K80*L83-K83*L80)*(K80+K83)+(K83*L82-K82*L83)*(K83+K82)+(K82*L81-K81*L82)*(K82+K81)+(K81*L84-K84*L81)*(K81+K84))/6/K85)","v":{"$error":"#VALUE!"}},"kN/m'","xt=",{"$f":"IF(N85=0,0,-((N80*O81-N81*O80)*(N80+N81)+(N81*O82-N82*O81)*(N81+N82)+(N82*O83-N83*O82)*(N82+N83)+(N83*O84-N84*O83)*(N83+N84))/6/N85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(P85=0,0,-((P80*Q81-P81*Q80)*(P80+P81)+(P81*Q82-P82*Q81)*(P81+P82)+(P82*Q83-P83*Q82)*(P82+P83)+(P83*Q84-P84*Q83)*(P83+P84))/6/P85)","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+U19","v":-8},{"$f":"+V19","v":1.5492076949174773},-5,{"$f":"+V85+(U85-U86)*TAN((45+'Analiza i dimenzioniranje'!F14/2)*PI()/180)","v":9.9970360471948005},"Y=",{"$f":"+X84*X85+Z84","v":1.2300775941423594},3,null,{"$f":"+X85","v":1.1386903959986558},{"$f":"+X86","v":1.2300775941423594}]
["yt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(C80+C81)+(B81*C82-B82*C81)*(C81+C82)+(B82*C83-B83*C82)*(C82+C83)+(B83*C84-B84*C83)*(C83+C84))/6/B85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(E80+E81)+(D81*E82-D82*E81)*(E81+E82)+(D82*E83-D83*E82)*(E82+E83)+(D83*E84-D84*E83)*(E83+E84))/6/D85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(G80+G81)+(F81*G82-F82*G81)*(G81+G82)+(F82*G83-F83*G82)*(G82+G83)+(F83*G84-F84*G83)*(G83+G84))/6/F85)","v":{"$error":"#VALUE!"}},"m","yt=",{"$f":"IF(I85=0,0,-((I80*J81-I81*J80)*(J80+J81)+(I81*J82-I82*J81)*(J81+J82)+(I82*J83-I83*J82)*(J82+J83)+(I83*J84-I84*J83)*(J83+J84))/6/I85)","v":{"$error":"#VALUE!"}},{"$f":"+O87","v":"m"},{"$f":"IF(K85=0,0,((K80*L83-K83*L80)*(L80+L83)+(K83*L82-K82*L83)*(L83+L82)+(K82*L81-K81*L82)*(L82+L81)+(K81*L84-K84*L81)*(L81+L84))/6/K85)","v":{"$error":"#VALUE!"}},"m","yt=",{"$f":"IF(N85=0,0,-((N80*O81-N81*O80)*(O80+O81)+(N81*O82-N82*O81)*(O81+O82)+(N82*O83-N83*O82)*(O82+O83)+(N83*O84-N84*O83)*(O83+O84))/6/N85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(P85=0,0,-((P80*Q81-P81*Q80)*(Q80+Q81)+(P81*Q82-P82*Q81)*(Q81+Q82)+(P82*Q83-P83*Q82)*(Q82+Q83)+(P83*Q84-P84*Q83)*(Q83+Q84))/6/P85)","v":{"$error":"#VALUE!"}},"m",null,null,null,null,null,"Y=",{"$f":"+(V86-V85)/(U86-U85)","v":-1.4281480067421144},"*x",{"$f":"-X87*U85+V85","v":2.8562960134842288},"y=2       x=",{"$f":"+('Analiza i dimenzioniranje'!E52-'C VIII-IX'!Z87)/'C VIII-IX'!X87","v":1.1597509541483482}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(K85<0,0,K85)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+IF(P85<0,0,P85)","v":{"$error":"#VALUE!"}},null,null,"Jedn pravca sloja 2",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(T90-T89)/(S90-S89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X88*S89+T89","v":{"$error":"#VALUE!"}},"Jedn pravca sloja 2 klizno",null,"Jednadžba pravca sidra",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(AD90-AD89)/(AC90-AC89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AH88*AC89+AD89","v":{"$error":"#VALUE!"}}]
["X koordinata položaja rezultante aktivnog tlaka na stražnjoj strani zida za  Ev1, Ev2 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U15","v":{"$error":"#VALUE!"}},{"$f":"+V15","v":4},{"$f":"+X85","v":1.1386903959986558},{"$f":"+X86","v":1.2300775941423594},"X=",{"$f":"+(-Z88+Z91)/(X88-X91)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U89","v":1.1386903959986558},{"$f":"+V89","v":1.2300775941423594},{"$f":"+U37","v":{"$error":"#VALUE!"}},{"$f":"+V37","v":5},{"$f":"+U89","v":1.1386903959986558},{"$f":"+V89","v":1.2300775941423594},"X=",{"$f":"+(-AJ88+AJ91)/(AH88-AH91)","v":{"$error":"#VALUE!"}},"sjecište"]
["Jednadžba pravca zida uz tlo",null,null,null,null,"Za Ev3 x=2",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U16","v":-8},{"$f":"+V16","v":{"$error":"#VALUE!"}},-5,{"$f":"+V89+(U89-U90)*TAN((45+'Analiza i dimenzioniranje'!E14/2)*PI()/180)","v":9.6792600705649363},"Y=",{"$f":"+X88*X89+Z88","v":{"$error":"#VALUE!"}},2,null,{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},{"$f":"+U38","v":{"$error":"#VALUE!"}},{"$f":"+V38","v":{"$error":"#VALUE!"}},{"$f":"+U90","v":-5},{"$f":"+V90","v":9.6792600705649363},"Y=",{"$f":"+AH88*AH89+AJ88","v":{"$error":"#VALUE!"}},2]
[null,"E1",null,"E2",null,"E3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(V90-V89)/(U90-U89)","v":-1.3763819204711731},"*x",{"$f":"-X91*U89+V89","v":2.79735046820907},null,null,null,null,null,null,"Y=",{"$f":"+(AF90-AF89)/(AE90-AE89)","v":-1.3763819204711731},"*x",{"$f":"-AH91*AE89+AF89","v":2.79735046820907}]
["x","y","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,"Jedn pravca sloja 1",null,null,null,"Y=",{"$f":"+(T95-T94)/(S95-S94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X92*S94+T94","v":{"$error":"#VALUE!"}},"Jedan pravca sloja 1 klizno",null,"Slobodna dionica ls>=",{"$f":"+SQRT((AC94-AC93)*(AC94-AC93)+(AD94-AD93)*(AD94-AD93))","v":{"$error":"#VALUE!"}}]
[{"$f":"+(B8-B4)*(B93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+B87","v":{"$error":"#VALUE!"}},{"$f":"+(B8-B4)*(D93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+D87","v":{"$error":"#VALUE!"}},2,{"$f":"+F87","v":{"$error":"#VALUE!"}},null,{"$f":"+(B8-B4)*(I93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+N87","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+(B8-B4)*(N93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+I87","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+V7","v":"A"},null,null,"X=",{"$f":"+(-Z92+Z95)/(X92-X95)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U94","v":{"$error":"#VALUE!"}},{"$f":"+V94","v":{"$error":"#VALUE!"}},{"$f":"+AC89","v":{"$error":"#VALUE!"}},{"$f":"+AD89","v":5}]
[{"$f":"+I76","v":12.361875887090893},{"$f":"+J76","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+(B8-B4)*(G94-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!V15","v":4},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U8","v":{"$error":"#VALUE!"}},{"$f":"+V8","v":6},{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+X92*X93+Z92","v":{"$error":"#VALUE!"}},1,null,{"$f":"+X93","v":{"$error":"#VALUE!"}},{"$f":"+X94","v":{"$error":"#VALUE!"}},{"$f":"+AH89","v":{"$error":"#VALUE!"}},{"$f":"+AH90","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+(B8-B4)*(G95-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+K21","v":1.2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782},-5,{"$f":"+V94+(U94-U95)*TAN((45+'Analiza i dimenzioniranje'!D14/2)*PI()/180)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+(V95-V94)/(U95-U94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X95*U94+V94","v":{"$error":"#VALUE!"}},{"$f":"+(AB95-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(AB96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+(AD96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16}]
[null,null,null,null,null,{"$f":"+'C III-V'!F136:G136","v":"Visina presjeka"},null,{"$f":"+'C III-V'!H136:I136","v":"Intezitet"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zid",null,"POTRES",null,"x","y","x","y","x","y",null,null,null,null,"Masa za potres s prosjekom kontrafore i bez kontrafora"]
[null,null,null,null,null,{"$f":"+'C III-V'!F137:G137","v":"III"},{"$f":"+'C III-V'!G137:H137","v":1.2},{"$f":"+'C III-V'!H137:I137","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+(B9-B4)*(AD98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},{"$f":"+(B9-B4)*(AF98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48}]
[null,null,null,null,null,{"$f":"+'C III-V'!F138:G138","v":"VI"},{"$f":"+'C III-V'!G138:H138","v":1.52},{"$f":"+'C III-V'!H138:I138","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B2","v":2},0.12820515121628623,null,null,{"$f":"+(Z95-AB99)/(-X91)","v":{"$error":"#VALUE!"}},{"$f":"+AB98","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!X44>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'C VIII-IX'!AC96,(Z91-AD99)/(-X91))","v":0.46306222039801814},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},{"$f":"IF('Analiza i dimenzioniranje'!Y44>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'C VIII-IX'!AA96,(Z91-AF99)/(-X91))","v":0.2305686114363027},{"$f":"+AO123","v":2.48}]
[null,null,null,null,null,{"$f":"+'C III-V'!F139:G139","v":"VII"},{"$f":"+'C III-V'!G139:H139","v":1.84},{"$f":"+'C III-V'!H139:I139","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,1.2,"Potresna sila za stabilnost",null,"Klizno tijelo za potres za presjek III-III",null,"Klizno tijelo za potres za presjek  VIII-VIII",null,"Klizno tijelo za potres za presjek    IX-IX",null,null,null,null,null,"Potresna sila za stabilnost "]
[null,null,null,null,null,{"$f":"+'C III-V'!F140:G140","v":"VIII"},{"$f":"+'C III-V'!G140:H140","v":2.16},{"$f":"+'C III-V'!H140:I140","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.4000010999999999,1.2,{"$f":"+'C III-V'!Y101","v":1.75},{"$f":"+'C III-V'!Z101","v":9.6153895463470418E-2},null,null,{"$f":"+AC98","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AC105","v":2.16},{"$f":"+AE98","v":{"$error":"#VALUE!"}},{"$f":"+AF98","v":2.48},null,null,null,null,{"$f":"+'C III-V'!Y101","v":1.75},{"$f":"+'C III-V'!Z101","v":9.6153895463470418E-2}]
[null,null,null,null,null,{"$f":"+'C III-V'!F141:G141","v":"IX"},{"$f":"+'C III-V'!G141:H141","v":2.48},{"$f":"+'C III-V'!H141:I141","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.14,{"$f":"+'C III-V'!Y102","v":0.97707863658009864},{"$f":"+'C III-V'!Z102","v":1.2},{"$f":"+Y102","v":0.97707863658009864},1.2,{"$f":"+AN122","v":0.23409016140914748},{"$f":"+AO122","v":2.16},{"$f":"+AN123","v":9.5109260623546556E-3},{"$f":"+AO123","v":2.48},null,null,null,null,{"$f":"+'C III-V'!Y102","v":0.97707863658009864},{"$f":"+'C III-V'!Z102","v":1.2}]
[null,null,null,null,null,{"$f":"+'C III-V'!F142:G142","v":"X"},{"$f":"+'C III-V'!G142:H142","v":2.8},{"$f":"+'C III-V'!H142:I142","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.14,{"$f":"+'C III-V'!Y103","v":-1.0572404418349119},{"$f":"+'C III-V'!Z103","v":4},-1.0572404418349119,4,{"$f":"IF(AD103=AD102,AC102,+AA103)","v":-1.0572404418349119},{"$f":"IF($AH$105<=AD102,AD102,$AH$105)","v":4},{"$f":"IF(AF103=AF102,AE102,+AC103)","v":-1.0572404418349119},{"$f":"IF($AH$105<=AF102,AF102,$AH$105)","v":4},null,null,null,null,{"$f":"+'C III-V'!Y103","v":-1.0572404418349119},{"$f":"+'C III-V'!Z103","v":4}]
[null,null,null,null,null,{"$f":"+'C III-V'!F143:G143","v":"XI"},{"$f":"+'C III-V'!G143:H143","v":3.14},{"$f":"+'C III-V'!H143:I143","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.44,{"$f":"+'C III-V'!Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z104","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+'C III-V'!Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z104","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F144:G144","v":"XIII"},{"$f":"+'C III-V'!G144:H144","v":3.44},{"$f":"+'C III-V'!H144:I144","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.44,{"$f":"+'C III-V'!Y105","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z105","v":6.2644906473896782},{"$error":"#VALUE!"},6.2644906473896782,{"$f":"+AA105","v":{"$error":"#VALUE!"}},{"$f":"IF(AA105=AC105,AB105,AB95)","v":{"$error":"#VALUE!"}},{"$f":"+AA105","v":{"$error":"#VALUE!"}},{"$f":"+IF(AA105=AE105,AB105,AB95)","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!AG105","v":" H="},{"$f":"+'C III-V'!AH105","v":4},null,null,{"$f":"+'C III-V'!Y105","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z105","v":6.2644906473896782}]
[null,null,null,null,null,{"$f":"+'C III-V'!F145:G145","v":"XIII"},{"$f":"+'C III-V'!G145:H145","v":3.76},{"$f":"+'C III-V'!H145:I145","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},"A",{"$f":"+'C III-V'!Y106","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z106","v":6},{"$error":"#VALUE!"},6,{"$f":"+AE106","v":{"$error":"#VALUE!"}},{"$f":"+AF106","v":6},{"$f":"+AA106","v":{"$error":"#VALUE!"}},{"$f":"+AB106","v":6},null,null,null,null,{"$f":"+'C III-V'!Y106","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z106","v":6}]
[null,null,null,null,null,{"$f":"+'C III-V'!F146:G146","v":"XIV"},{"$f":"+'C III-V'!G146:H146","v":4.08},{"$f":"+'C III-V'!H146:I146","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},"A",{"$f":"+'C III-V'!Y107","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z107","v":6},{"$error":"#VALUE!"},6,{"$f":"+AE107","v":{"$error":"#VALUE!"}},{"$f":"+AF107","v":6},{"$f":"+AA107","v":{"$error":"#VALUE!"}},{"$f":"+AB107","v":6},null,null,null,null,{"$f":"+'C III-V'!Y107","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z107","v":6}]
[null,null,null,null,null,{"$f":"+'C III-V'!F147:G147","v":"XV"},{"$f":"+'C III-V'!G147:H147","v":4.4000000000000004},{"$f":"+'C III-V'!H147:I147","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+W107","v":{"$error":"#VALUE!"}},{"$f":"+X107","v":"A"},{"$f":"+'C III-V'!Y108","v":3.4000000999999997},{"$f":"+'C III-V'!Z108","v":1.2},3.4000000999999997,1.2,{"$f":"+AC109","v":{"$error":"#VALUE!"}},{"$f":"+AD109","v":2.16},{"$f":"+AE109","v":{"$error":"#VALUE!"}},{"$f":"+AF109","v":2.48},null,null,null,null,{"$f":"+'C III-V'!Y108","v":3.4000000999999997},{"$f":"+'C III-V'!Z108","v":1.2}]
[null,null,null,null,null,{"$f":"+'C III-V'!F148:G148","v":"XVI"},{"$f":"+'C III-V'!G148:H148","v":4.72},{"$f":"+'C III-V'!H148:I148","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B11","v":4.2000010999999997},1.2,{"$f":"+'C III-V'!Y109","v":1.75},{"$f":"+'C III-V'!Z109","v":1.2},{"$f":"+AA102","v":0.97707863658009864},{"$f":"+AB102","v":1.2},{"$f":"+AC98","v":{"$error":"#VALUE!"}},{"$f":"+AD98","v":2.16},{"$f":"+AE101","v":{"$error":"#VALUE!"}},{"$f":"+AF101","v":2.48},null,null,null,null,{"$f":"+'C III-V'!Y109","v":1.75},{"$f":"+'C III-V'!Z109","v":1.2}]
[null,null,null,null,null,{"$f":"+'C III-V'!F149:G149","v":"XVII"},{"$f":"+'C III-V'!G149:H149","v":5.04},{"$f":"+'C III-V'!H149:I149","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2000010999999997,1.2,{"$f":"+'C III-V'!Y110","v":1.75},{"$f":"+'C III-V'!Z110","v":9.6153895463470418E-2},null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!Y110","v":1.75},{"$f":"+'C III-V'!Z110","v":9.6153895463470418E-2}]
[null,null,null,null,null,{"$f":"+'C III-V'!F150:G150","v":"XVIII"},{"$f":"+'C III-V'!G150:H150","v":5.36},{"$f":"+'C III-V'!H150:I150","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2000010999999997,1.2,{"$f":"-0.5*((Y101*Z102-Y102*Z101)+(Y102*Z103-Y103*Z102)+(Y103*Z104-Y104*Z103)+(Y104*Z105-Y105*Z104)+(Y105*Z106-Y106*Z105)+(Y106*Z107-Y107*Z106)+(Y107*Z108-Y108*Z107)+(Y108*Z109-Y109*Z108)+(Y109*Z110-Y110*Z109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AA101*AB102-AA102*AB101)+(AA102*AB103-AA103*AB102)+(AA103*AB104-AA104*AB103)+(AA104*AB105-AA105*AB104)+(AA105*AB106-AA106*AB105)+(AA106*AB107-AA107*AB106)+(AA107*AB108-AA108*AB107)+(AA108*AB109-AA109*AB108)+(AA109*AB110-AA110*AB109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AC101*AD102-AC102*AD101)+(AC102*AD103-AC103*AD102)+(AC103*AD104-AC104*AD103)+(AC104*AD105-AC105*AD104)+(AC105*AD106-AC106*AD105)+(AC106*AD107-AC107*AD106)+(AC107*AD108-AC108*AD107)+(AC108*AD109-AC109*AD108)+(AC109*AD110-AC110*AD109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AE101*AF102-AE102*AF101)+(AE102*AF103-AE103*AF102)+(AE103*AF104-AE104*AF103)+(AE104*AF105-AE105*AF104)+(AE105*AF106-AE106*AF105)+(AE106*AF107-AE107*AF106)+(AE107*AF108-AE108*AF107)+(AE108*AF109-AE109*AF108)+(AE109*AF110-AE110*AF109))","v":{"$error":"#VALUE!"}},"m2",null,null,null,null,{"$f":"-0.5*((AK101*AL102-AK102*AL101)+(AK102*AL103-AK103*AL102)+(AK103*AL104-AK104*AL103)+(AK104*AL105-AK105*AL104)+(AK105*AL106-AK106*AL105)+(AK106*AL107-AK107*AL106)+(AK107*AL108-AK108*AL107)+(AK108*AL109-AK109*AL108)+(AK109*AL110-AK110*AL109))","v":{"$error":"#VALUE!"}},"m2","OK","prosječna površina temelja od temelja kontrafore duž čitavog zida"]
[null,null,null,null,null,{"$f":"+'C III-V'!F151:G151","v":"XIX"},{"$f":"+'C III-V'!G151:H151","v":5.6800000000000006},{"$f":"+'C III-V'!H151:I151","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.9000021999999994,1.2,{"$f":"-((Y101*Z102-Y102*Z101)*(Y101+Y102)+(Y102*Z103-Y103*Z102)*(Y102+Y103)+(Y103*Z104-Y104*Z103)*(Y103+Y104)+(Y104*Z105-Y105*Z104)*(Y104+Y105)+(Y105*Z106-Y106*Z105)*(Y105+Y106)+(Y106*Z107-Y107*Z106)*(Y106+Y107)+(Y107*Z108-Y108*Z107)*(Y107+Y108)+(Y108*Z109-Y109*Z108)*(Y108+Y109)+(Y109*Z110-Y110*Z109)*(Y109+Y110))/6/Y111","v":{"$error":"#VALUE!"}},"m  ",{"$f":"-((AA101*AB102-AA102*AB101)*(AA101+AA102)+(AA102*AB103-AA103*AB102)*(AA102+AA103)+(AA103*AB104-AA104*AB103)*(AA103+AA104)+(AA104*AB105-AA105*AB104)*(AA104+AA105)+(AA105*AB106-AA106*AB105)*(AA105+AA106)+(AA106*AB107-AA107*AB106)*(AA106+AA107)+(AA107*AB108-AA108*AB107)*(AA107+AA108)+(AA108*AB109-AA109*AB108)*(AA108+AA109)+(AA109*AB110-AA110*AB109)*(AA109+AA110))/6/AA111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AC101*AD102-AC102*AD101)*(AC101+AC102)+(AC102*AD103-AC103*AD102)*(AC102+AC103)+(AC103*AD104-AC104*AD103)*(AC103+AC104)+(AC104*AD105-AC105*AD104)*(AC104+AC105)+(AC105*AD106-AC106*AD105)*(AC105+AC106)+(AC106*AD107-AC107*AD106)*(AC106+AC107)+(AC107*AD108-AC108*AD107)*(AC107+AC108)+(AC108*AD109-AC109*AD108)*(AC108+AC109)+(AC109*AD110-AC110*AD109)*(AC109+AC110))/6/AC111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AE101*AF102-AE102*AF101)*(AE101+AE102)+(AE102*AF103-AE103*AF102)*(AE102+AE103)+(AE103*AF104-AE104*AF103)*(AE103+AE104)+(AE104*AF105-AE105*AF104)*(AE104+AE105)+(AE105*AF106-AE106*AF105)*(AE105+AE106)+(AE106*AF107-AE107*AF106)*(AE106+AE107)+(AE107*AF108-AE108*AF107)*(AE107+AE108)+(AE108*AF109-AE109*AF108)*(AE108+AE109)+(AE109*AF110-AE110*AF109)*(AE109+AE110))/6/AE111","v":{"$error":"#VALUE!"}},"m",null,null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AK101+AK102)+(AK102*AL103-AK103*AL102)*(AK102+AK103)+(AK103*AL104-AK104*AL103)*(AK103+AK104)+(AK104*AL105-AK105*AL104)*(AK104+AK105)+(AK105*AL106-AK106*AL105)*(AK105+AK106)+(AK106*AL107-AK107*AL106)*(AK106+AK107)+(AK107*AL108-AK108*AL107)*(AK107+AK108)+(AK108*AL109-AK109*AL108)*(AK108+AK109)+(AK109*AL110-AK110*AL109)*(AK109+AK110))/6/AK111","v":{"$error":"#VALUE!"}},"m  "]
[null,null,null,null,null,{"$f":"+'C III-V'!F152:G152","v":"XX"},{"$f":"+'C III-V'!G152:H152","v":6},{"$f":"+'C III-V'!H152:I152","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.9000021999999994,0.5,{"$f":"-((Y101*Z102-Y102*Z101)*(Z101+Z102)+(Y102*Z103-Y103*Z102)*(Z102+Z103)+(Y103*Z104-Y104*Z103)*(Z103+Z104)+(Y104*Z105-Y105*Z104)*(Z104+Z105)+(Y105*Z106-Y106*Z105)*(Z105+Z106)+(Y106*Z107-Y107*Z106)*(Z106+Z107)+(Y107*Z108-Y108*Z107)*(Z107+Z108)+(Y108*Z109-Y109*Z108)*(Z108+Z109)+(Y109*Z110-Y110*Z109)*(Z109+Z110))/6/Y111","v":{"$error":"#VALUE!"}},"m    ",{"$f":"-((AA101*AB102-AA102*AB101)*(AB101+AB102)+(AA102*AB103-AA103*AB102)*(AB102+AB103)+(AA103*AB104-AA104*AB103)*(AB103+AB104)+(AA104*AB105-AA105*AB104)*(AB104+AB105)+(AA105*AB106-AA106*AB105)*(AB105+AB106)+(AA106*AB107-AA107*AB106)*(AB106+AB107)+(AA107*AB108-AA108*AB107)*(AB107+AB108)+(AA108*AB109-AA109*AB108)*(AB108+AB109)+(AA109*AB110-AA110*AB109)*(AB109+AB110))/6/AA111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AC101*AD102-AC102*AD101)*(AD101+AD102)+(AC102*AD103-AC103*AD102)*(AD102+AD103)+(AC103*AD104-AC104*AD103)*(AD103+AD104)+(AC104*AD105-AC105*AD104)*(AD104+AD105)+(AC105*AD106-AC106*AD105)*(AD105+AD106)+(AC106*AD107-AC107*AD106)*(AD106+AD107)+(AC107*AD108-AC108*AD107)*(AD107+AD108)+(AC108*AD109-AC109*AD108)*(AD108+AD109)+(AC109*AD110-AC110*AD109)*(AD109+AD110))/6/AC111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AE101*AF102-AE102*AF101)*(AF101+AF102)+(AE102*AF103-AE103*AF102)*(AF102+AF103)+(AE103*AF104-AE104*AF103)*(AF103+AF104)+(AE104*AF105-AE105*AF104)*(AF104+AF105)+(AE105*AF106-AE106*AF105)*(AF105+AF106)+(AE106*AF107-AE107*AF106)*(AF106+AF107)+(AE107*AF108-AE108*AF107)*(AF107+AF108)+(AE108*AF109-AE109*AF108)*(AF108+AF109)+(AE109*AF110-AE110*AF109)*(AF109+AF110))/6/AE111","v":{"$error":"#VALUE!"}},"m",null,null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AL101+AL102)+(AK102*AL103-AK103*AL102)*(AL102+AL103)+(AK103*AL104-AK104*AL103)*(AL103+AL104)+(AK104*AL105-AK105*AL104)*(AL104+AL105)+(AK105*AL106-AK106*AL105)*(AL105+AL106)+(AK106*AL107-AK107*AL106)*(AL106+AL107)+(AK107*AL108-AK108*AL107)*(AL107+AL108)+(AK108*AL109-AK109*AL108)*(AL108+AL109)+(AK109*AL110-AK110*AL109)*(AL109+AL110))/6/AK111","v":{"$error":"#VALUE!"}},"m    ",null,{"$f":"+'C III-V'!AN113:AN114","v":-0.25},{"$f":"IF('Analiza i dimenzioniranje'!D84=\"\",0,'Analiza i dimenzioniranje'!D83+'C III-V'!AN113)","v":0.75}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,0.12820515121628623,{"$f":"+Y111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AA111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AC111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AE111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,{"$f":"+AK111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(W99:W114)","v":{"$error":"#VALUE!"}},{"$f":"SUM(X99:X114)","v":21.11641030243257},null,null,null,null,{"$f":"+AC111","v":{"$error":"#VALUE!"}},null,{"$f":"'C VIII-IX'!AE111","v":{"$error":"#VALUE!"}},null,null,null,"Teren  kosina",null,"Klizna ploha"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AC112","v":{"$error":"#VALUE!"}},null,{"$f":"'C VIII-IX'!AE112","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+'C VI-VII'!AI116","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!AJ116","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!AK116","v":1.75},{"$f":"+AN128","v":-1.1133852506716102},"sjecišta ravnine presjeka na kliznoj plohi"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koord. Težište mase  za h22",null,null,null,{"$f":"+AC113","v":{"$error":"#VALUE!"}},null,{"$f":"'C VIII-IX'!AE113","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+'C VI-VII'!AI117","v":6.2644906473896782},{"$f":"+'C VI-VII'!AJ117","v":6},{"$f":"+'C VI-VII'!AK117","v":0},{"$f":"+AO128","v":4.08},{"$f":"+'C III-V'!AA100","v":"oznaka"},{"$f":"+'C III-V'!AB100","v":"X"},{"$f":"+'C III-V'!AC100","v":"Y"},"        sa kontraforama: bez kontrafora",null,null,"Potresna sila-prosječna"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(AA102-AA103)/3","v":0.67810635947167019},{"$f":"+Z103*0.666666666666667","v":2.6666666666666679},null,null,{"$f":"+AC114","v":{"$error":"#VALUE!"}},null,{"$f":"'C VIII-IX'!AE114","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!D116,AI117)","v":-5},{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!E116,'C III-V'!AJ117)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!AA101","v":"Y=0"},{"$f":"+'C III-V'!AB101","v":1.75},{"$f":"+'C III-V'!AC101","v":0},{"$f":"+'C VI-VII'!AQ118","v":0},null,null,null,null,"Potresna sila","F","G"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"(AJ117-AI117)/(AJ116-AI116)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AI119*AI116+AI117","v":{"$error":"#VALUE!"}}," ",{"$f":"+'C III-V'!AA102","v":"PIII"},{"$f":"+'C III-V'!AB102","v":0.97707863658009864},{"$f":"+'C III-V'!AC102","v":1.2},{"$f":"+'C VI-VII'!AQ119","v":0},null,null,{"$f":"+Kontrafore!E13","v":12},"m",{"$f":"+AS119","v":12},{"$f":"+Y111","v":{"$error":"#VALUE!"}},{"$f":"+Y114","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"-(AL117-AK117)/(AK116-AL116)","v":-1.4248868534344206},"*x    +",{"$f":"-(AK116*AI120-AK117)","v":2.4935519935102359}," ",{"$f":"+'C III-V'!AA103","v":"PVI"},{"$f":"+'C III-V'!AB103","v":0.68324863210273346},{"$f":"+'C III-V'!AC103","v":1.52},{"$f":"+'C VI-VII'!AQ120","v":0},null,null,{"$f":"+Kontrafore!E5*Kontrafore!E4","v":3},"m",{"$f":"+AS120","v":3},{"$f":"+AV119-AV121","v":{"$error":"#VALUE!"}},{"$f":"IF(AS120=AS119,0,AW119-AW121)","v":{"$error":"#VALUE!"}}]
["Presjek kroz zid I",null,"Presjek kroz zid II",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AK120-AK119)/(AI119-AI120)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AI120*AI121+AK120","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA104","v":"PVII"},{"$f":"+'C III-V'!AB104","v":0.45866939675594048},{"$f":"+'C III-V'!AC104","v":1.84},{"$f":"+'C VI-VII'!AQ121","v":0},null,null,{"$f":"+AS119-AS120","v":9},"m",{"$f":"+AU119-AU120","v":9},{"$f":"+AG111","v":0},{"$f":"+IF(AU121=0,0,AG114)","v":0}]
["x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA105","v":"PVIII"},{"$f":"+'C III-V'!AB105","v":0.23409016140914748},{"$f":"+'C III-V'!AC105","v":2.16},{"$f":"+'C VI-VII'!AQ122","v":0},null,null,{"$f":"+AS120/AS119","v":0.25}]
[0,{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+A123","v":0},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($AK$119-$AK$123)/AI119","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AK121","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA106","v":"PIX"},{"$f":"+'C III-V'!AB106","v":9.5109260623546556E-3},{"$f":"+'C III-V'!AC106","v":2.48},{"$f":"+'C VI-VII'!AQ123","v":0},null,null,{"$f":"+AS121/AS119","v":0.75}]
[{"$f":"+F83","v":{"$error":"#VALUE!"}},{"$f":"+B123","v":2.48},{"$f":"+A124","v":{"$error":"#VALUE!"}},{"$f":"+D123","v":2.16},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA107","v":"PX"},{"$f":"+'C III-V'!AB107","v":-0.21506830928443818},{"$f":"+'C III-V'!AC107","v":2.8},{"$f":"+'C VI-VII'!AQ124","v":0},null,null,"odnos",null,{"$f":"-(AU120/AU119)*'Analiza i dimenzioniranje'!D83","v":-0.25}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA108","v":"PXI"},{"$f":"+'C III-V'!AB108","v":-0.45368374684040591},{"$f":"+'C III-V'!AC108","v":3.14},{"$f":"+'C VI-VII'!AQ125","v":0},null,"krak",{"$f":"+Y113","v":{"$error":"#VALUE!"}},{"$f":"+AW119","v":{"$error":"#VALUE!"}},{"$f":"+AW120*AS122","v":{"$error":"#VALUE!"}},null,{"$f":"+AW119-AU126","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($AK$120-AK126)/$AI$120","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AK121","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA109","v":"PXII"},{"$f":"+'C III-V'!AB109","v":-0.66422677997802415},{"$f":"+'C III-V'!AC109","v":3.44},{"$f":"+'C VI-VII'!AQ126","v":0},null,null,{"$f":"+AG113","v":0},{"$f":"+AW121","v":0},{"$f":"+AW120*AS123","v":{"$error":"#VALUE!"}},null,{"$f":"+AW121+AU125","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-1.1976024639266576,null,4.2,null,{"$f":"+'C III-V'!AA110","v":"PXIII"},{"$f":"+'C III-V'!AB110","v":-0.88880601532481696},{"$f":"+'C III-V'!AC110","v":3.76},{"$f":"+'C VI-VII'!AQ127","v":0},null,null,null,null,"Prosječna masa za potres:",null,{"$f":"IF(IF(AS130=AT130,Y114,+AW126)=0,AW125,IF(AS130=AT130,Y114,+AW126))","v":{"$error":"#VALUE!"}},"kn"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.90782786744952648,null,1.2,null,{"$f":"+'C III-V'!AA111","v":"PXIV"},{"$f":"+'C III-V'!AB111","v":-1.1133852506716102},{"$f":"+'C III-V'!AC111","v":4.08},{"$f":"+'C VI-VII'!AQ128","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+Z104","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA112","v":"PXV"},{"$f":"+'C III-V'!AB112","v":-1.3379644860184032},{"$f":"+'C III-V'!AC112","v":4.4000000000000004},{"$f":"+'C VI-VII'!AQ129","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.23409016140914748,null,{"$f":"+AD109","v":2.16},null,{"$f":"+'C III-V'!AA113","v":"PXVI"},{"$f":"+'C III-V'!AB113","v":-1.5625437213651958},{"$f":"+'C III-V'!AC113","v":4.72},{"$f":"+'C VI-VII'!AQ130","v":0},null,"x=",{"$f":"+AG113","v":0},{"$f":"+Y113","v":{"$error":"#VALUE!"}},null,{"$f":"+AI109","v":0},{"$f":"+AI106","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9.5109260623546556E-3,null,{"$f":"+AF109","v":2.48},null,{"$f":"+'C III-V'!AA114","v":"PXVII"},{"$f":"+'C III-V'!AB114","v":-1.7871229567119888},{"$f":"+'C III-V'!AC114","v":5.04},{"$f":"+'C VI-VII'!AQ131","v":0},null,"Y=",{"$f":"+AG114","v":0},{"$f":"+Y114","v":{"$error":"#VALUE!"}},null,{"$f":"+AJ109","v":0},{"$f":"+AJ106","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.6464828732122183,null,{"$f":"+AI117","v":6.2644906473896782},null,{"$f":"+'C III-V'!AA115","v":"PXVIII"},{"$f":"+'C III-V'!AB115","v":-2.0117021920587819},{"$f":"+'C III-V'!AC115","v":5.36},{"$f":"+'C VI-VII'!AQ132","v":0},null,"Y=",{"$f":"(AS131-AT131)/(AS130-AT130)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AS132*AT130+AT131","v":{"$error":"#VALUE!"}},{"$f":"(AV131-AW131)/(AV130-AW130)","v":{"$error":"#DIV/0!"}},"*x    +",{"$f":"-AV132*AW130+AW131","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA116","v":"PXIX"},{"$f":"+'C III-V'!AB116","v":-2.2362814274055753},{"$f":"+'C III-V'!AC116","v":5.6800000000000006},{"$f":"+'C VI-VII'!AQ133","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA117","v":"PXX"},{"$f":"+'C III-V'!AB117","v":0},{"$f":"+'C III-V'!AC117","v":6.0000000000000009},{"$f":"+'C VI-VII'!AQ134","v":0},null,"x=",{"$f":"+AK113","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","Y",null,{"$f":"+AK104","v":{"$error":"#VALUE!"}},{"$f":"+AL104","v":{"$error":"#VALUE!"}},{"$f":"+'C VI-VII'!AQ135","v":0},null,"xstv=",{"$f":"+AS134-X113","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AK136","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AL136","v":{"$error":"#VALUE!"}},null,null,null,null,null,"            Masa da se dobije prosječni potres iz čelije AT125=",null,null,null,null,{"$f":"+AW125","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+AF104","v":{"$error":"#VALUE!"}},{"$f":"+AD102","v":2.16},{"$f":"+AF102","v":2.48},null,null,null,null,null,null,null,null,null,null,null,null,"razlika¸površina",{"$f":"+Y111-AI111","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AE144-AC138)/(-AC144)","v":{"$error":"#VALUE!"}},{"$f":"IF(AD138<AC138,(AE151-AD138)/(-AC151),(AE156-AD138)/(-AC156))","v":{"$error":"#VALUE!"}},{"$f":"IF(AE138<AC138,(AE151-AE138)/(-AC151),(AE156-AE138)/(-AC156))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,"duljina segmenta",{"$f":"++AJ105","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina III. sloja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"okomito na kliz. Plohu",null,{"$f":"+AS143/AS139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y",null,null,null,null,null,null,null,null,null,null,null,null,"d=","dodatak",{"$f":"+AS140/COS(AS142*PI()/180)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B2","v":2},0,null,null,null,null,null,null,null,null,null,null,null,null,"          kut nagiba klizne plohe za potres   a= ",null,{"$f":"ATAN((-Y104+Y101)/(Z104-Z101))*180/PI()","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA154","v":-5},{"$f":"+'C III-V'!AB154","v":9.9970360471948005},null,null,null,null,null,null,null,null,null,null,null,null,null,"dodatna površina",{"$f":"+AS144/'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+'C III-V'!AA155","v":-1.4281480067421144},"*x      +",{"$f":"+'C III-V'!AC154","v":2.8562960134842288},null,null,null,null,null,null,null,null,null,null,null,null,"G=",{"$f":"+AU126","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AE144-AD146)/(-AC144)","v":1.1597509541483482}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+Z102","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina II. sloja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B9","v":{"$error":"#VALUE!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-5,{"$f":"+'C III-V'!AB149","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+'C III-V'!AA150","v":-1.3763819204711734},"*x      +",{"$f":"+'C III-V'!AC149","v":2.5448333702674724}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina I. sloja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koordinate na sjecištu s terenom",null,null,{"$f":"+'C III-V'!AA144","v":-2.5846586698092704},{"$f":"+'C III-V'!AB144","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koordinate na sjecištu slojeva",null,null,{"$f":"+'C III-V'!AA143","v":-1.0572404418349119},{"$f":"+'C III-V'!AB143","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+'C III-V'!AA145","v":-1.4825609685127401},"*x      +",{"$f":"-AC156*AC154+AD154","v":2.4325765866023956}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rub dna konzole uz aktivni klin",null,null,{"$f":"+B6","v":{"$error":"#VALUE!"}},{"$f":"+C6","v":3.14}]

{"sheet":"C X-XI","index":42,"n_rows":157,"n_cols":53,"rows_kept":157,"cut":false,"hidden":true,"merged":[[112,5,112,6],[116,47,116,49],[96,32,98,33],[96,34,98,35],[96,36,98,37],[99,32,99,33],[99,34,99,35],[99,36,99,37],[115,38,115,40],[110,38,113,38],[110,39,111,40],[112,39,113,39],[112,40,113,40],[99,28,99,29],[99,30,99,31],[114,34,114,35],[77,13,77,14],[77,10,77,11],[99,26,99,27],[67,20,67,21],[77,15,77,16],[67,15,67,16],[67,22,67,23],[67,10,67,11],[67,13,67,14],[90,1,90,2],[90,3,90,4],[90,5,90,6],[96,22,97,23],[99,24,99,25],[44,7,44,8],[44,17,44,18],[42,1,42,2],[42,3,42,4],[42,5,42,6],[42,7,43,10],[44,9,44,10],[44,11,44,12],[77,1,77,2],[77,3,77,4],[77,5,77,6],[77,8,77,9],[67,1,67,2],[67,3,67,4],[67,5,67,6],[67,8,67,9],[44,23,44,24],[44,25,44,26],[16,27,16,28],[17,12,17,16],[17,27,17,28],[26,27,26,28],[42,11,43,14],[42,15,43,18],[44,21,44,22],[44,13,44,14],[44,15,44,16],[43,21,43,22],[10,3,10,4],[10,27,10,28],[11,3,11,4],[12,27,12,28],[13,12,13,16],[13,27,13,28],[0,1,0,2],[0,3,0,4],[0,5,0,7],[0,9,0,10],[1,5,1,8],[114,36,114,37],[139,27,139,30],[146,27,146,30],[151,27,151,30],[13,29,13,30],[62,29,62,30],[62,27,62,28]]}
["Točke","ZID I TEMELJ",null,"NASIP NA TEMELJU IZA",null,"ZID, KONZOLA I NASIP NA KONZOLI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Točka A",null,"Presjek I-I"]
[1,2,{"$f":"+'C III-V'!$C$2","v":0.12820515121628623},null,null,"ZA BILO KOJI PRESJEK ",null,null,null,null,null,null,null,null,null,null,null,"Presjek zid Iv",{"$f":"+($B$9-$B$4)*(T2-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},{"$f":"+B15","v":4.9000021999999994},{"$f":"+C15","v":0.5},{"$f":"+'C X-XI'!B10+0.05","v":{"$error":"#VALUE!"}},-0.5]
[2,2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T3-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},"Točka B",null,{"$f":"+W2","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!C10+0.5","v":{"$error":"#VALUE!"}}]
[3,{"$f":"+B3+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+C3","v":1.2},{"$f":"+B19","v":2},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>C4,B21,B4)","v":3.4000010999999999},{"$f":"IF(E20>C4,E20,C4)","v":1.2},{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},null,null,null,null,null,null,null,null,"Presjek V",{"$f":"+($B$9-$B$4)*(T4-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},{"$f":"+'C X-XI'!B2","v":2},{"$f":"+'C X-XI'!C2","v":0.12820515121628623}]
[4,{"$f":"+B23","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},{"$f":"+D4","v":2},{"$f":"+'C III-V'!E5","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,B21,B5)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,E20,C5)","v":3.14},{"$f":"+F8","v":{"$error":"#VALUE!"}},{"$f":"+G8","v":3.44},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T5-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},null,null,"Presjek II-II",null,null,null,"Nasip na zidu iza"]
[5,{"$f":"+B5-'Analiza i dimenzioniranje'!G78","v":{"$error":"#VALUE!"}},{"$f":"+C5","v":3.14},{"$f":"IF(B6<2,B5,IF(B9>2,B9,D5))","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!E6","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C7,B21,B6)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C6,E20,C6)","v":3.14},{"$f":"IF(F7>F9,H5,F9)","v":{"$error":"#VALUE!"}},{"$f":"IF(F7>F9,I5,IF(E20>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C X-XI'!E20,G9))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"Presjek VI",{"$f":"+($B$9-$B$4)*(T6-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},"TLO 1. sloj",null,{"$f":"+'C X-XI'!B15-0.05","v":4.8500021999999996},{"$f":"+'C X-XI'!X2","v":-0.5},null,null,2,{"$f":"IF('Analiza i dimenzioniranje'!AW26>'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AW26)","v":0}]
[6,{"$f":"IF('Analiza i dimenzioniranje'!G78=0,'C X-XI'!B8,B6)","v":{"$error":"#VALUE!"}},{"$f":"C6+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+B4","v":3.4000010999999999},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>=C7,B21,B7)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C7,E20,C7)","v":3.44},{"$f":"IF(F7>F9,H6,H6)","v":{"$error":"#VALUE!"}},{"$f":"+I6","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T7-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},{"$f":"+'C X-XI'!B15-0.05","v":4.8500021999999996},{"$f":"+'C X-XI'!X3","v":{"$error":"#VALUE!"}},"Horizontala",null,2,{"$f":"'Analiza i dimenzioniranje'!BF28","v":0}]
[7,{"$f":"+B22","v":{"$error":"#VALUE!"}},{"$f":"+C7","v":3.44},{"$f":"+D4","v":2},{"$f":"+E4","v":1.2},{"$f":"IF(E20>C8,B21,B8)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C8,E20,C8)","v":3.44},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$H$15=0,I7+(H7-H8)*'Unos podataka'!R57,IF('C III-V'!H9>'Unos podataka'!$B$105,I7+(H7-H8)*'Unos podataka'!$R$55,'Unos podataka'!$T$57))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"Presjek VII",{"$f":"+($B$9-$B$4)*(T8-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!V8","v":6},null,null,{"$f":"+'C X-XI'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!C5","v":3.14}]
[8,{"$f":"B4-TAN('Analiza i dimenzioniranje'!H51*PI()/180)*('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},null,null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"+I4","v":3.44},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T9-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},{"$f":"+U8-'Analiza i dimenzioniranje'!E27","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!V9","v":6.2644906473896782},"Presjek ZID",null,{"$f":"+IF('Analiza i dimenzioniranje'!$E$24=0,0,'C X-XI'!Y4)","v":0},{"$f":"+Z8","v":3.14}]
[9,{"$f":"+B9+'Analiza i dimenzioniranje'!E54","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},null,null,{"$f":"+B10","v":{"$error":"#VALUE!"}},{"$f":"+C10","v":"A"},null,null,null,null,null,null,null,null,null,null,"Presjek VIII",{"$f":"+($B$9-$B$4)*(T10-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},-8,{"$f":"+'C III-V'!V10","v":6.2644906473896782},{"$f":"+'C X-XI'!B15-0.5","v":4.4000021999999994},{"$f":"+'C X-XI'!C10+0.1","v":{"$error":"#VALUE!"}}]
[10,{"$f":"+B4+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+C3","v":1.2},"NASIP NA KONZOLI",null,{"$f":"+F12+E65","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C11,E20,C11)","v":1.2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T11-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},"x","y",{"$f":"+'C X-XI'!B10+0.5","v":{"$error":"#VALUE!"}},{"$f":"+X10","v":{"$error":"#VALUE!"}},null,null,null,"Rsidra"]
[11,{"$f":"+B11","v":4.2000010999999997},{"$f":"+C11","v":1.2},"za stabilnost",null,{"$f":"+F4","v":3.4000010999999999},{"$f":"+G4","v":1.2},null,null,null,null,null,null,null,null,null,null,"Presjek IX",{"$f":"+($B$9-$B$4)*(T12-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+W23","v":{"$error":"#VALUE!"}},{"$f":"+U12*(V9-V8)/(U9-U8)-U8*(V9-V8)/(U9-U8)+V8","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,20,AB16)","v":20},{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,0,AC16)","v":0}]
[12,{"$f":"+B12","v":4.2000010999999997},{"$f":"+C12","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T13-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+W25","v":{"$error":"#VALUE!"}},{"$f":"+U13*(V9-V8)/(U9-U8)-U8*(V9-V8)/(U9-U8)+V8","v":{"$error":"#VALUE!"}},"Pad terena niz padinu",null,null,null,null,"Os rezultante sidara Ukupna računska sila u sidrima"]
[13,{"$f":"+B11+'Analiza i dimenzioniranje'!G57","v":4.9000021999999994},{"$f":"+C13","v":1.2},{"$f":"+B7","v":{"$error":"#VALUE!"}},3.44,null,null,null,null,"Linija presjeka",null,null," Koordinata sredine presjeka",null,null,null,null,"Presjek X",{"$f":"+($B$9-$B$4)*(T14-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},"TLO 2. sloj",null,{"$f":"+'Analiza i dimenzioniranje'!Q105","v":3},{"$f":"+'Analiza i dimenzioniranje'!P105","v":{"$error":"#VALUE!"}},null,null,null,"Slobodna  zona.",null,"1. sloj"]
[14,{"$f":"+B14","v":4.9000021999999994},{"$f":"+C14-'Analiza i dimenzioniranje'!E51","v":0.5},{"$error":"#VALUE!"},3.44,{"$f":"IF((B4-B9)=0,0,+(C9-C4)/(B4-B9))","v":{"$error":"#VALUE!"}},"n  Nagib zida u tlu",null,null,0,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,"III-III","konzola","Presjek I","Presjek II",null,{"$f":"+($B$11-$B$10)*(T15-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},{"$f":"IF(('Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17)<'Analiza i dimenzioniranje'!$F$45,2,(IF(B7<B24,B7,IF('Analiza i dimenzioniranje'!G78=0,'C X-XI'!B24,2))))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17","v":4},{"$f":"+'Analiza i dimenzioniranje'!O130","v":7.1000021999999996},{"$f":"+'Analiza i dimenzioniranje'!N130","v":1.5001009999999999},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,AB24)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,'Analiza i dimenzioniranje'!P22)","v":5},{"$f":"+U9","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782}]
[15,{"$f":"+B2","v":2},{"$f":"+C2","v":0.12820515121628623},{"$error":"#VALUE!"},"A",null,null,null,null,3,{"$f":"+K15","v":1.2},null,"x",{"$f":"+(F12+F11)/2","v":{"$error":"#VALUE!"}},{"$f":"(B8+(B11-B10)*(O17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U29+(B11-B10)*(P17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U34+(B11-B10)*(Q17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},"Presjek XI",{"$f":"+($B$9-$B$4)*(T16-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},-8,{"$f":"+V15+(U15-U16)*TAN('Analiza i dimenzioniranje'!$E$18*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"AB15-'Analiza i dimenzioniranje'!P23","v":{"$error":"#VALUE!"}},{"$f":"+AC15-(AB15-AB16)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782}]
[null,null,"Jednadžba pravca zida uz tlo",{"$f":"+D16","v":{"$error":"#VALUE!"}},{"$f":"+I7","v":{"$error":"#VALUE!"}},null,null,null,null,"Sloj 2 gore",null,null,"y",{"$f":"+G11","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},null,{"$f":"+($B$11-$B$10)*(T17-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},"TLO 3. sloj",null,"Prometno opterećenje",null,null,null,null,"Sidrena dionica",null,"Jednadžba površine terena"]
[null,"x","y",{"$f":"+D14","v":{"$error":"#VALUE!"}},{"$f":"+I8","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+F94","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E52>=G94,0,G94)","v":4},null,null,null,null,null,null,"Presjek XII",{"$f":"+($B$9-$B$4)*(T18-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},2,{"$f":"+'Analiza i dimenzioniranje'!$F$17","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,+'C X-XI'!B9-'Analiza i dimenzioniranje'!E26)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,'C X-XI'!V9)","v":6.2644906473896782},null,null,null,"                   Y=",null,{"$f":"+(AE16-AE15)/(AD16-AD15)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AD18*AD15+AE15","v":{"$error":"#VALUE!"}}]
[null,2,{"$f":"+B19*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},{"$f":"+D14","v":{"$error":"#VALUE!"}},{"$f":"+E14","v":3.44},null,null,null,null,{"$f":"U16","v":-8},{"$f":"+K18","v":4},null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T19-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},-8,{"$f":"+V18+(U18-U19)*TAN('Analiza i dimenzioniranje'!$F$18*PI()/180)","v":1.5492076949174773},{"$f":"+W18","v":{"$error":"#VALUE!"}},{"$f":"+X18+'Analiza i dimenzioniranje'!E24/20","v":6.7644906473896782},null,null,null,{"$f":"+AB16","v":{"$error":"#VALUE!"}},{"$f":"+AC16","v":{"$error":"#VALUE!"}},"za x=",{"$f":"+AB20","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+H8","v":{"$error":"#VALUE!"}},{"$f":"+B20*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},"M na koti",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,"Sloj 1 ili2 dole",null,null,null,null,null,null,{"$f":"+(B11-B10)*(Q21-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},"Presjek XIII",{"$f":"+($B$9-$B$4)*(T20-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},"KONTAKTNI NAPONI",null,{"$f":"+W18-'Analiza i dimenzioniranje'!E25","v":{"$error":"#VALUE!"}},{"$f":"+X19","v":6.7644906473896782},null,null,null,{"$f":"+(AB21+AB19)/2","v":{"$error":"#VALUE!"}},{"$f":"+(AC19+AC21)/2","v":{"$error":"#VALUE!"}},"y=",{"$f":"+AD18*AE19+AF18","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C21-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,{"$f":"+IF('Analiza i dimenzioniranje'!G78=0,D8,H8)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+F95","v":{"$error":"#VALUE!"}},{"$f":"+G12","v":1.2},null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,{"$f":"+($B$11-$B$10)*(T21-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},2,0,{"$f":"+W20","v":{"$error":"#VALUE!"}},{"$f":"+X18","v":6.2644906473896782},null,null,null,{"$f":"+AB19-'Analiza i dimenzioniranje'!P24","v":{"$error":"#VALUE!"}},{"$f":"+AC19-(AB19-AB21)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},"visina sloja iznad centra sidra"]
[null,{"$f":"+(B9-B4)*(C22-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+C23+'Analiza i dimenzioniranje'!C77","v":3.44},null,null,null,null,null,null,{"$f":"+U19","v":-8},{"$f":"+K21","v":1.2},null,null,null,null,null,null,"Presjek XIV",{"$f":"+($B$9-$B$4)*(T22-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},2,{"$f":"-'Analiza i dimenzioniranje'!$F$193/100","v":{"$error":"#VALUE!"}},"Točkasto",null,null,null,null,null,null,{"$f":"+AE20-AC20","v":{"$error":"#VALUE!"}},"m"]
[null,{"$f":"+(B9-B4)*(C23-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T23-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"2+'Analiza i dimenzioniranje'!$E$61","v":4.9000021999999994},{"$f":"-'Analiza i dimenzioniranje'!$F$190/100","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E36=0,-10,B9-'Analiza i dimenzioniranje'!E37)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X23","v":{"$error":"#VALUE!"}},null,null,null,"Jednadžba  lica zida "]
[null,{"$f":"+(B9-B4)*(C24-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V15","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek XV",{"$f":"+($B$9-$B$4)*(T24-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U23","v":4.9000021999999994},0,"Linijsko iza zida",null,null,null,"x=",{"$f":"+($B$11-$B$10)*(AB25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+($B$11-$B$10)*(AC25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+(B11-B10)*(AE25-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C25-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U21","v":2},0,{"$f":"IF('Analiza i dimenzioniranje'!$E$34=0,0,B9-'Analiza i dimenzioniranje'!K28)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X27","v":{"$error":"#VALUE!"}},null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!Z42","v":170.21276595744681},{"$f":"+'Analiza i dimenzioniranje'!AA42","v":5},null,{"$f":"+'Analiza i dimenzioniranje'!H76+'Analiza i dimenzioniranje'!E52","v":1.5001009999999999}]
[null,{"$f":"+(B9-B4)*(C26-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid XI-XI",{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},{"$f":"+W25","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$34=0,0,X25+1)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!T22","v":0},null,null,null,null,{"$f":"+B14-AE24","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C27-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},"TEMELJ -opterećenje",null,"x=",{"$f":"+($B$11-$B$10)*(Z26-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"Rez. Sidra na zidu"]
[null,{"$f":"+(B9-B4)*(C26-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V27","v":3.14},{"$f":"+IF('Analiza i dimenzioniranje'!E28=0,0,W29)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9+'Analiza i dimenzioniranje'!F20+1.5)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!S22","v":0}]
["Sjecište s dnom temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V29-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":3.14},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W30-0.3)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X30)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z28-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+($B$11-$B$10)*(AC29-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E40","v":3.9999999960000001},{"$f":"+AB29+0.4","v":{"$error":"#VALUE!"}},{"$f":"+AC29+(AD29-AB29)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}}]
["zid",{"$f":"+B20","v":{"$error":"#VALUE!"}},{"$f":"+B30*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V30-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":3.14},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,B9-'Analiza i dimenzioniranje'!$E$32)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X31+'Analiza i dimenzioniranje'!E33)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!R22","v":0},null,null,null,{"$f":"+AB29-1","v":{"$error":"#VALUE!"}},{"$f":"+AC29-(AB29-AD30)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}}]
["Vrh zida",{"$f":"+(B9-B4)*(C31-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C558","v":-0.45},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid Iv",{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},{"$f":"+W30","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9-'Analiza i dimenzioniranje'!K31)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z30-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"nagib lica"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,W31-'Analiza i dimenzioniranje'!$E$29)","v":{"$error":"#VALUE!"}},{"$f":"+X31","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q22","v":3},null,"tan"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V32","v":2.8},{"$f":"+W32","v":{"$error":"#VALUE!"}},{"$f":"+X30","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z32-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+(B13-B10)/(C10-C13)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V34-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V33","v":2.8},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W33+0.3)","v":{"$error":"#VALUE!"}},{"$f":"+X29","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q20","v":5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V35-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V34","v":2.8},{"$f":"+W34","v":{"$error":"#VALUE!"}},{"$f":"+X28","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z34-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SIDRO za presjek",null,null,null,"Jednadžba pravca lica zida ",null,null,null,null,null,"Anker armatura uz lice",null,"arm dno",null,"Y=",{"$f":"IF(AE38=AE37,1000000,(AF38-AF37)/(AE38-AE37))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AJ36*AE37+AF37","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!$C$545","v":1.6923077248520526}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB15)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC15)","v":5},null,null,"x=",null,null,null,null,null,{"$f":"+(B11-B10)*(AF37-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!B545","v":{"$error":"#VALUE!"}},{"$f":"+U81","v":2.0499999999999998},{"$f":"+V81","v":0.18682583433163008},"X=",{"$f":"+(-AL36+AL39)/(AJ36-AJ39)","v":{"$error":"#VALUE!"}},"sjeište",null,"x=",{"$f":"+(AN36-AL36)/AJ36","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB16)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC16)","v":{"$error":"#VALUE!"}},null,null,"y=",null,null,null,null,null,{"$f":"+(B11-B10)*(AF38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+U82","v":4.8600021999999994},{"$f":"+V82","v":0.54310345350772504},"Y=",{"$f":"+AJ36*AJ37+AL36","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate dna temelja",null,null,null,null,null,null,"Y=",{"$f":"+(AH38-AH37)/(AG38-AG37)","v":0.12678908905341604},"*x",{"$f":"-AJ39*AG37+AH37","v":-7.3091798227872762E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"lice","koord Pr II",{"$f":"+AB47+'Analiza i dimenzioniranje'!Q58","v":3.4500010999999997},{"$f":"(AB40*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24999999999999994},null,"SIDRO"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+(B11-B10)*(Z42-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+B8","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+AB15","v":{"$error":"#VALUE!"}},{"$f":"+AC15","v":5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+Z42","v":3.44},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,AB15-0.5)","v":{"$error":"#VALUE!"}},{"$f":"+AF41-(AE41-AE42)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},null,"Nasip ispred zida"]
["Oznaka","temelj",null,"Zid i konzola za pr. ZID",null,"Nasip na temelju iza zida",null,"      Za momente u presjeku zid-temelj          ",null,null,null,"      Za momente u presjeku X-X",null,null,null,"         Za momente u presjeku XI-XI",null,null,null,null,null,null,null,null,null,null,null,2,0,null,null,null,null,{"$f":"+AE24","v":{"$error":"#VALUE!"}},{"$f":"+C11+'Analiza i dimenzioniranje'!$H$76","v":1.5001009999999999}]
["točke","x","y","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - BETON",null,null,null,null,null,2.65,{"$f":"+(AC47+AC49)/2","v":0.31034478180740688},null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!$E$61","v":4.9000021999999994},{"$f":"+AI43","v":1.5001009999999999}]
[1,{"$f":"+'C X-XI'!B2","v":2},{"$f":"+'C X-XI'!C2","v":0.12820515121628623},null,null,null,null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"Kontaktni naponi za stab",null,"Beton do presjeka II-II",null,"Beton sredine temelja",null,"Beton do presjeka I-I",null,{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"(AB45*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH44+1.6","v":6.5000021999999991},{"$f":"+AI44-(AH45-AH44)*TAN('Analiza i dimenzioniranje'!H22*PI()/180)","v":1.5001009999999999}]
[2,{"$f":"+'C X-XI'!B3","v":2},{"$f":"+'C X-XI'!C3","v":1.2},null,null,null,null,"x","y","x","y","x","y","x","y","x","y","x","y","x","y",null,null,"x","y","x","y",{"$f":"+(AB43+AB47)/2","v":2.7000005499999999},{"$f":"(AB46*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.1206896584423281},null,null,null,null,"x","y"]
[3,{"$f":"+'C X-XI'!B4","v":3.4000010999999999},{"$f":"+'C X-XI'!C4","v":1.2},{"$f":"+B4","v":3.4000010999999999},1.2,2,1.2,3.4000010999999999,1.2,{"$f":"+D14","v":{"$error":"#VALUE!"}},3.44,{"$f":"+U34","v":{"$error":"#VALUE!"}},{"$f":"+V34","v":2.8},{"$f":"+J47","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!Z44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!Z44,K47)","v":3.44},{"$f":"+U29","v":{"$error":"#VALUE!"}},{"$f":"+V29","v":3.14},{"$f":"+J47","v":{"$error":"#VALUE!"}},{"$f":"+S48","v":3.44},{"$f":"+U21","v":2},{"$f":"+V21*100","v":0},2,0,{"$f":"+B4","v":3.4000010999999999},{"$f":"+W49","v":1.2},{"$f":"+B11","v":4.2000010999999997},1.2,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"(AB47*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24137931688465614},"Presjek II-II",null,null,null,{"$f":"+'C X-XI'!B11","v":4.2000010999999997},{"$f":"+C11","v":1.2}]
[4,{"$f":"+B11","v":4.2000010999999997},1.2,{"$error":"#VALUE!"},3.14,2,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.44,{"$f":"+H48","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!Z44<'Analiza i dimenzioniranje'!F45,I48,'C X-XI'!V34)","v":3.14},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!Z44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!Z44,K48)","v":3.44},{"$f":"+H48","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AA44<'Analiza i dimenzioniranje'!F45,I48,V29)","v":3.14},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AA44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AA44,K48)","v":3.44},{"$f":"+U22","v":2},{"$f":"+V22*100","v":{"$error":"#VALUE!"}},2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+X47+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+Y47","v":1.2},4.2000010999999997,1.2,{"$f":"+AB77","v":{"$error":"#VALUE!"}},{"$f":"(AB48*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47+'Analiza i dimenzioniranje'!H76","v":1.5001009999999999}]
[5,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.14,{"$f":"+D16","v":{"$error":"#VALUE!"}},{"$f":"+E16+'Unos podataka'!$F9","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!Z44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C X-XI'!L47,'C X-XI'!B6)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!Z44<'Analiza i dimenzioniranje'!F45,I49,'C X-XI'!V34)","v":3.14},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!Z44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!Z44,K49)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AA44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C X-XI'!B6,P47)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AA44<'Analiza i dimenzioniranje'!F45,'C X-XI'!I49,Q48)","v":3.14},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AA44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AA44,K49)","v":{"$error":"#VALUE!"}},{"$f":"+U23","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},{"$f":"+V48+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+W48","v":1.2},{"$f":"+AB49","v":4.2000010999999997},{"$f":"+AC49","v":0.37931024673015767},4.2000010999999997,1.2,{"$f":"+AB47+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+(AB49*(AC43-AC53)/(AB43-AB53)-AB53*(AC43-AC53)/(AB43-AB53)+AC53)","v":0.37931024673015767},"Presjek I-I",null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+AI48","v":1.5001009999999999}]
[6,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.44,3.4000010999999999,1.2,{"$error":"#VALUE!"},3.44,{"$f":"IF('Unos podataka'!$B$105>J47,'Unos podataka'!$B$105,J47)","v":{"$error":"#VALUE!"}},{"$f":"+K51","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!Z44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C X-XI'!L48,'C X-XI'!B7)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!Z44<='Analiza i dimenzioniranje'!F45,I50,'C X-XI'!V34)","v":3.44},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!Z44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!Z44,K50)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AA44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C X-XI'!P47,H50)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AA44<='Analiza i dimenzioniranje'!F45,I50,V29)","v":3.44},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AA44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AA44,K50)","v":{"$error":"#VALUE!"}},{"$f":"+U24","v":4.9000021999999994},{"$f":"+V24*100","v":0},{"$f":"+V49","v":3.4000010999999999},{"$f":"+AC47","v":0.24137931688465614},{"$f":"+X47","v":3.4000010999999999},{"$f":"+AC47","v":0.24137931688465614},4.9000021999999994,1.2,{"$f":"2+'Analiza i dimenzioniranje'!E61/2","v":3.4500010999999997},{"$f":"(AB50*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24999999999999994},null,null,null,null,{"$f":"+AH49","v":4.9000021999999994},{"$f":"+C14","v":1.2}]
[7,4.9000021999999994,1.2,{"$error":"#VALUE!"},3.44,2,1.2,{"$error":"#VALUE!"},3.44,{"$f":"+D18","v":{"$error":"#VALUE!"}},{"$f":"+E18+'Unos podataka'!$F9","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!Z44>'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C X-XI'!B28,B8)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!Z44>='Analiza i dimenzioniranje'!I75+'Analiza i dimenzioniranje'!G67,'C X-XI'!M50,Z26)","v":3.44},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!Z44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!Z44,K51)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AA44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C X-XI'!B25,H51)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AA44<='Analiza i dimenzioniranje'!F45,I51,V29)","v":3.44},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AA44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AA44,K51)","v":{"$error":"#VALUE!"}},{"$f":"+U25","v":2},{"$f":"+V25*100","v":0},{"$f":"+V47","v":2},{"$f":"+W47","v":0},{"$f":"+X47","v":3.4000010999999999},{"$f":"+Y47","v":1.2},4.9000021999999994,0.5,{"$f":"+(AB49+AB53)/2","v":4.5500016499999996},{"$f":"(AB51*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.43965512336507878},null,null,null,null,{"$f":"+B13","v":4.2000010999999997},{"$f":"+C13","v":1.2}]
[8,4.9000021999999994,0.5,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",{"$error":"#VALUE!"},3.44,{"$f":"+H52","v":{"$error":"#VALUE!"}},{"$f":"+Q52","v":"A"},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!Z44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!Z44,K52)","v":3.44},{"$f":"+H52","v":{"$error":"#VALUE!"}},{"$f":"+I52","v":"A"},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AA44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AA44,K52)","v":3.44},null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AC49","v":0.37931024673015767},{"$f":"+AD77","v":{"$error":"#VALUE!"}},{"$f":"(AB52*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH51","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[9,2,0.12820515121628623,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",null,null,{"$f":"+H53","v":{"$error":"#VALUE!"}},{"$f":"+Q53","v":"A"},null,null,{"$f":"+H53","v":{"$error":"#VALUE!"}},{"$f":"+I53","v":"A"},null,null,null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AA47","v":1.2},{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+C15","v":0.5},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[10,null,null,4.2000010999999997,1.2,null,null,{"$error":"#VALUE!"},1.2,null,null,{"$f":"+U35","v":{"$error":"#VALUE!"}},{"$f":"+M47","v":2.8},null,null,{"$f":"+U30","v":{"$error":"#VALUE!"}},{"$f":"+V30","v":3.14},null,null,null,null,null,null,null,null,null,null,"Koordinate s","naprezanjem"]
[11,null,null,{"$f":"+D47","v":3.4000010999999999},{"$f":"+E47","v":1.2},null,null,3.4000010999999999,1.2,null,null,{"$f":"+L47","v":{"$error":"#VALUE!"}},{"$f":"+M47","v":2.8},null,null,{"$f":"+P47","v":{"$error":"#VALUE!"}},{"$f":"+Q47","v":3.14},null,null,null,null,null,null,null,null,null,null,{"$f":"+U22","v":2},{"$f":"+V22*100","v":{"$error":"#VALUE!"}}]
[12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+AB56*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
[13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AB57*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
["  A=",{"$f":"-0.5*((B45*C46-B46*C45)+(B46*C47-B47*C46)+(B47*C48-B48*C47)+(B48*C49-B49*C48)+(B49*C50-B50*C49)+(B50*C51-B51*C50)+(B51*C52-B52*C51)+(B52*C53-B53*C52))","v":2.5691044797107181},"m2",{"$f":"-0.5*((D45*E46-D46*E45)+(D46*E47-D47*E46)+(D47*E48-D48*E47)+(D48*E49-D49*E48)+(D49*E50-D50*E49)+(D50*E51-D51*E50)+(D51*E52-D52*E51)+(D52*E53-D53*E52)+(D53*E54-D54*E53)+(D54*E55-D55*E54)+(D55*E56-D56*E55)+(D56*E57-D57*E56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((F45*G46-F46*G45)+(F46*G47-F47*G46)+(F47*G48-F48*G47)+(F48*G49-F49*G48)+(F49*G50-F50*G49)+(F50*G51-F51*G50)+(F51*G52-F52*G51)+(F52*G53-F53*G52)+(F53*G54-F54*G53)+(F54*G55-F55*G54)+(F55*G56-F56*G55)+(F56*G57-F57*G56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((H47*I48-H48*I47)+(H48*I49-H49*I48)+(H49*I50-H50*I49)+(H50*I51-H51*I50)+(H51*I52-H52*I51)+(H52*I53-H53*I52)+(H53*I54-H54*I53)+(H54*I55-H55*I54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((J47*K48-J48*K47)+(J48*K49-J49*K48)+(J49*K50-J50*K49)+(J50*K51-J51*K50)+(J51*K52-J52*K51)+(J52*K53-J53*K52)+(J53*K54-J54*K53)+(J54*K55-J55*K54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((L47*M48-L48*M47)+(L48*M49-L49*M48)+(L49*M50-L50*M49)+(L50*M51-L51*M50)+(L51*M52-L52*M51)+(L52*M53-L53*M52)+(L53*M54-L54*M53)+(L54*M55-L55*M54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"IF(0.5*((N47*O48-N48*O47)+(N48*O49-N49*O48)+(N49*O50-N50*O49)+(N50*O51-N51*O50)+(N51*O52-N52*O51)+(N52*O53-N53*O52)+(N53*O54-N54*O53)+(N54*O55-N55*O54))<0,0,0.5*((N47*O48-N48*O47)+(N48*O49-N49*O48)+(N49*O50-N50*O49)+(N50*O51-N51*O50)+(N51*O52-N52*O51)+(N52*O53-N53*O52)+(N53*O54-N54*O53)+(N54*O55-N55*O54)))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((P47*Q48-P48*Q47)+(P48*Q49-P49*Q48)+(P49*Q50-P50*Q49)+(P50*Q51-P51*Q50)+(P51*Q52-P52*Q51)+(P52*Q53-P53*Q52)+(P53*Q54-P54*Q53)+(P54*Q55-P55*Q54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((R47*S48-R48*S47)+(R48*S49-R49*S48)+(R49*S50-R50*S49)+(R50*S51-R51*S50)+(R51*S52-R52*S51)+(R52*S53-R53*S52)+(R53*S54-R54*S53)+(R54*S55-R55*S54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((T47*U48-T48*U47)+(T48*U49-T49*U48)+(T49*U50-T50*U49)+(T50*U51-T51*U50)+(T51*U52-T52*U51)+(T52*U53-T53*U52)+(T53*U54-T54*U53)+(T54*U55-T55*U54))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((V47*W48-V48*W47)+(V48*W49-V49*W48)+(V49*W50-V50*W49)+(V50*W51-V51*W50))","v":1.5110356654221164},"m2",{"$f":"-0.5*((X47*Y48-X48*Y47)+(X48*Y49-X49*Y48)+(X49*Y50-X50*Y49)+(X50*Y51-X51*Y50))","v":0.71172417455407389},"m2",{"$f":"-0.5*((Z47*AA48-Z48*AA47)+(Z48*AA49-Z49*AA48)+(Z49*AA50-Z50*AA49)+(Z50*AA51-Z51*AA50)+(Z51*AA52-Z52*AA51)+(Z52*AA53-Z53*AA52)+(Z53*AA54-Z54*AA53)+(Z54*AA55-Z55*AA54))","v":0.53224225002380887},"m2",{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-0.5*((AH47*AI48-AH48*AI47)+(AH48*AI49-AH49*AI48)+(AH49*AI50-AH50*AI49)+(AH50*AI51-AH51*AI50)+(AH51*AI52-AH52*AI51)+(AH52*AI53-AH53*AI52)+(AH53*AI54-AH54*AI53)+(AH54*AI55-AH55*AI54))","v":0.21007103011109951},"m2"]
["xt=",{"$f":"-((B45*C46-B46*C45)*(B45+B46)+(B46*C47-B47*C46)*(B46+B47)+(B47*C48-B48*C47)*(B47+B48)+(B48*C49-B49*C48)*(B48+B49)+(B49*C50-B50*C49)*(B49+B50)+(B50*C51-B51*C50)*(B50+B51)+(B51*C52-B52*C51)*(B51+B52)+(B52*C53-B53*C52)*(B52+B53)+(B53*C54-B54*C53)*(B53+B54)+(B54*C55-B55*C54)*(B54+B55)+(B55*C56-B56*C55)*(B55+B56)+(B56*C57-B57*C56)*(B56+B57))/6/B58","v":3.3485779696489133},"m",{"$f":"-((D45*E46-D46*E45)*(D45+D46)+(D46*E47-D47*E46)*(D46+D47)+(D47*E48-D48*E47)*(D47+D48)+(D48*E49-D49*E48)*(D48+D49)+(D49*E50-D50*E49)*(D49+D50)+(D50*E51-D51*E50)*(D50+D51)+(D51*E52-D52*E51)*(D51+D52)+(D52*E53-D53*E52)*(D52+D53)+(D53*E54-D54*E53)*(D53+D54)+(D54*E55-D55*E54)*(D54+D55)+(D55*E56-D56*E55)*(D55+D56)+(D56*E57-D57*E56)*(D56+D57))/6/D58","v":{"$error":"#VALUE!"}},"m",{"$f":"-((F45*G46-F46*G45)*(F45+F46)+(F46*G47-F47*G46)*(F46+F47)+(F47*G48-F48*G47)*(F47+F48)+(F48*G49-F49*G48)*(F48+F49)+(F49*G50-F50*G49)*(F49+F50)+(F50*G51-F51*G50)*(F50+F51)+(F51*G52-F52*G51)*(F51+F52)+(F52*G53-F53*G52)*(F52+F53)+(F53*G54-F54*G53)*(F53+F54)+(F54*G55-F55*G54)*(F54+F55)+(F55*G56-F56*G55)*(F55+F56)+(F56*G57-F57*G56)*(F56+F57))/6/F58","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(H47*I48-H48*I47)*(H47+H48)+(H48*I49-H49*I48)*(H48+H49)+(H49*I50-H50*I49)*(H49+H50)+(H50*I51-H51*I50)*(H50+H51)+(H51*I52-H52*I51)*(H51+H52)+(H52*I53-H53*I52)*(H52+H53)+(H53*I54-H54*I53)*(H53+H54)+(H54*I55-H55*I54)*(H54+H55))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(J47+J48)+(J48*K49-J49*K48)*(J48+J49)+(J49*K50-J50*K49)*(J49+J50)+(J50*K51-J51*K50)*(J50+J51)+(J51*K52-J52*K51)*(J51+J52)+(J52*K53-J53*K52)*(J52+J53)+(J53*K54-J54*K53)*(J53+J54)+(J54*K55-J55*K54)*(J54+J55)+(J55*K56-J56*K55)*(J55+J56)+(J56*K57-J57*K56)*(J56+J57))/6/J58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(L47*M48-L48*M47)*(L47+L48)+(L48*M49-L49*M48)*(L48+L49)+(L49*M50-L50*M49)*(L49+L50)+(L50*M51-L51*M50)*(L50+L51)+(L51*M52-L52*M51)*(L51+L52)+(L52*M53-L53*M52)*(L52+L53)+(L53*M54-L54*M53)*(L53+L54)+(L54*M55-L55*M54)*(L54+L55))/6/L58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(N58=0,0,(+(N47*O48-N48*O47)*(N47+N48)+(N48*O49-N49*O48)*(N48+N49)+(N49*O50-N50*O49)*(N49+N50)+(N50*O51-N51*O50)*(N50+N51)+(N51*O52-N52*O51)*(N51+N52))/6/N58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(P47*Q48-P48*Q47)*(P47+P48)+(P48*Q49-P49*Q48)*(P48+P49)+(P49*Q50-P50*Q49)*(P49+P50)+(P50*Q51-P51*Q50)*(P50+P51)+(P51*Q52-P52*Q51)*(P51+P52)+(P52*Q53-P53*Q52)*(P52+P53)+(P53*Q54-P54*Q53)*(P53+P54)+(P54*Q55-P55*Q54)*(P54+P55))/6/P58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(R58=0,0,(+(R47*S48-R48*S47)*(R47+R48)+(R48*S49-R49*S48)*(R48+R49)+(R49*S50-R50*S49)*(R49+R50)+(R50*S51-R51*S50)*(R50+R51)+(R51*S52-R52*S51)*(R51+R52))/6/R58)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(T58=0,0,(+(T47*U48-T48*U47)*(T47+T48)+(T48*U49-T49*U48)*(T48+T49)+(T49*U50-T50*U49)*(T49+T50)+(T50*U51-T51*U50)*(T50+T51)+(T51*U52-T52*U51)*(T51+T52)+(T52*U53-T53*U52)*(T52+T53)+(T53*U54-T54*U53)*(T53+T54)+(T54*U55-T55*U54)*(T54+T55)+(T55*U56-T56*U55)*(T55+T56)+(T56*U57-T57*U56)*(T56+T57))/6/T58)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(V58=0,0,-(+(V47*W48-V48*W47)*(V47+V48)+(V48*W49-V49*W48)*(V48+V49)+(V49*W50-V50*W49)*(V49+V50)+(V50*W51-V51*W50)*(V50+V51))/6/V58)","v":2.6739089419190427},"m",{"$f":"IF(X58=0,0,-(+(X47*Y48-X48*Y47)*(X47+X48)+(X48*Y49-X49*Y48)*(X48+X49)+(X49*Y50-X50*Y49)*(X49+X50)+(X50*Y51-X51*Y50)*(X50+X51))/6/X58)","v":3.7896651910602248},"m",{"$f":"-(+(Z47*AA48-Z48*AA47)*(Z47+Z48)+(Z48*AA49-Z49*AA48)*(Z48+Z49)+(Z49*AA50-Z50*AA49)*(Z49+Z50)+(Z50*AA51-Z51*AA50)*(Z50+Z51)+(Z51*AA52-Z52*AA51)*(Z51+Z52)+(Z52*AA53-Z53*AA52)*(Z52+Z53)+(Z53*AA54-Z54*AA53)*(Z53+Z54)+(Z54*AA55-Z55*AA54)*(Z54+Z55)+(Z55*AA56-Z56*AA55)*(Z55+Z56)+(Z56*AA57-Z57*AA56)*(Z56+Z57))/6/Z58","v":4.5407423692617748},"m",null,null,null,null,"   Koordinate presjeka",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AH47+AH48)+(AH48*AI49-AH49*AI48)*(AH48+AH49)+(AH49*AI50-AH50*AI49)*(AH49+AH50)+(AH50*AI51-AH51*AI50)*(AH50+AH51)+(AH51*AI52-AH52*AI51)*(AH51+AH52)+(AH52*AI53-AH53*AI52)*(AH52+AH53)+(AH53*AI54-AH54*AI53)*(AH53+AH54)+(AH54*AI55-AH55*AI54)*(AH54+AH55)+(AH55*AI56-AH56*AI55)*(AH55+AH56)+(AH56*AI57-AH57*AI56)*(AH56+AH57))/6/AH58","v":4.550001650000004},"m"]
["yt=",{"$f":"-((B45*C46-B46*C45)*(C45+C46)+(B46*C47-B47*C46)*(C46+C47)+(B47*C48-B48*C47)*(C47+C48)+(B48*C49-B49*C48)*(C48+C49)+(B49*C50-B50*C49)*(C49+C50)+(B50*C51-B51*C50)*(C50+C51)+(B51*C52-B52*C51)*(C51+C52)+(B52*C53-B53*C52)*(C52+C53)+(B53*C54-B54*C53)*(C53+C54)+(B54*C55-B55*C54)*(C54+C55)+(B55*C56-B56*C55)*(C55+C56)+(B56*C57-B57*C56)*(C56+C57))/6/B58","v":0.75054981042380386},"m",{"$f":"-((D45*E46-D46*E45)*(E45+E46)+(D46*E47-D47*E46)*(E46+E47)+(D47*E48-D48*E47)*(E47+E48)+(D48*E49-D49*E48)*(E48+E49)+(D49*E50-D50*E49)*(E49+E50)+(D50*E51-D51*E50)*(E50+E51)+(D51*E52-D52*E51)*(E51+E52)+(D52*E53-D53*E52)*(E52+E53)+(D53*E54-D54*E53)*(E53+E54)+(D54*E55-D55*E54)*(E54+E55)+(D55*E56-D56*E55)*(E55+E56)+(D56*E57-D57*E56)*(E56+E57))/6/D58","v":{"$error":"#VALUE!"}},"m",{"$f":"-((F45*G46-F46*G45)*(G45+G46)+(F46*G47-F47*G46)*(G46+G47)+(F47*G48-F48*G47)*(G47+G48)+(F48*G49-F49*G48)*(G48+G49)+(F49*G50-F50*G49)*(G49+G50)+(F50*G51-F51*G50)*(G50+G51)+(F51*G52-F52*G51)*(G51+G52)+(F52*G53-F53*G52)*(G52+G53)+(F53*G54-F54*G53)*(G53+G54)+(F54*G55-F55*G54)*(G54+G55)+(F55*G56-F56*G55)*(G55+G56)+(F56*G57-F57*G56)*(G56+G57))/6/F58","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(H47*I48-H48*I47)*(I47+I48)+(H48*I49-H49*I48)*(I48+I49)+(H49*I50-H50*I49)*(I49+I50)+(H50*I51-H51*I50)*(I50+I51)+(H51*I52-H52*I51)*(I51+I52)+(H52*I53-H53*I52)*(I52+I53)+(H53*I54-H54*I53)*(I53+I54)+(H54*I55-H55*I54)*(I54+I55)+(H55*I56-H56*I55)*(I55+I56)+(H56*I57-H57*I56)*(I56+I57))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(K47+K48)+(J48*K49-J49*K48)*(K48+K49)+(J49*K50-J50*K49)*(K49+K50)+(J50*K51-J51*K50)*(K50+K51)+(J51*K52-J52*K51)*(K51+K52)+(J52*K53-J53*K52)*(K52+K53)+(J53*K54-J54*K53)*(K53+K54)+(J54*K55-J55*K54)*(K54+K55)+(J55*K56-J56*K55)*(K55+K56)+(J56*K57-J57*K56)*(K56+K57))/6/J58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(L47*M48-L48*M47)*(M47+M48)+(L48*M49-L49*M48)*(M48+M49)+(L49*M50-L50*M49)*(M49+M50)+(L50*M51-L51*M50)*(M50+M51)+(L51*M52-L52*M51)*(M51+M52)+(L52*M53-L53*M52)*(M52+M53)+(L53*M54-L54*M53)*(M53+M54)+(L54*M55-L55*M54)*(M54+M55))/6/L58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(N58=0,0,(+(N47*O48-N48*O47)*(O47+O48)+(N48*O49-N49*O48)*(O48+O49)+(N49*O50-N50*O49)*(O49+O50)+(N50*O51-N51*O50)*(O50+O51)+(N51*O52-N52*O51)*(O51+O52)+(N52*O53-N53*O52)*(O52+O53)+(N53*O54-N54*O53)*(O53+O54)+(N54*O55-N55*O54)*(O54+O55)+(N55*O56-N56*O55)*(O55+O56)+(N56*O57-N57*O56)*(O56+O57))/6/N58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(P47*Q48-P48*Q47)*(Q47+Q48)+(P48*Q49-P49*Q48)*(Q48+Q49)+(P49*Q50-P50*Q49)*(Q49+Q50)+(P50*Q51-P51*Q50)*(Q50+Q51)+(P51*Q52-P52*Q51)*(Q51+Q52)+(P52*Q53-P53*Q52)*(Q52+Q53)+(P53*Q54-P54*Q53)*(Q53+Q54)+(P54*Q55-P55*Q54)*(Q54+Q55))/6/P58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(R58=0,0,(+(R47*S48-R48*S47)*(S47+S48)+(R48*S49-R49*S48)*(S48+S49)+(R49*S50-R50*S49)*(S49+S50)+(R50*S51-R51*S50)*(S50+S51)+(R51*S52-R52*S51)*(S51+S52)+(R52*S53-R53*S52)*(S52+S53)+(R53*S54-R54*S53)*(S53+S54)+(R54*S55-R55*S54)*(S54+S55)+(R55*S56-R56*S55)*(S55+S56)+(R56*S57-R57*S56)*(S56+S57))/6/R58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-IF(T58=0,0,(+(T47*U48-T48*U47)*(U47+U48)+(T48*U49-T49*U48)*(U48+U49)+(T49*U50-T50*U49)*(U49+U50)+(T50*U51-T51*U50)*(U50+U51)+(T51*U52-T52*U51)*(U51+U52)+(T52*U53-T53*U52)*(U52+U53)+(T53*U54-T54*U53)*(U53+U54)+(T54*U55-T55*U54)*(U54+U55)+(T55*U56-T56*U55)*(U55+U56)+(T56*U57-T57*U56)*(U56+U57))/6/T58)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((V47*W48-V48*W47)*(W47+W48)+(V48*W49-V49*W48)*(W48+W49)+(V49*W50-V50*W49)*(W49+W50)+(V50*W51-V51*W50)*(W50+W51))/6/V58","v":0.65809555436880718},"kN",{"$f":"-((X47*Y48-X48*Y47)*(Y47+Y48)+(X48*Y49-X49*Y48)*(Y48+Y49)+(X49*Y50-X50*Y49)*(Y49+Y50)+(X50*Y51-X51*Y50)*(Y50+Y51))/6/X58","v":0.75428136494691478},"kN",{"$f":"-(+(Z47*AA48-Z48*AA47)*(AA47+AA48)+(Z48*AA49-Z49*AA48)*(AA48+AA49)+(Z49*AA50-Z50*AA49)*(AA49+AA50)+(Z50*AA51-Z51*AA50)*(AA50+AA51)+(Z51*AA52-Z52*AA51)*(AA51+AA52)+(Z52*AA53-Z53*AA52)*(AA52+AA53)+(Z53*AA54-Z54*AA53)*(AA53+AA54)+(Z54*AA55-Z55*AA54)*(AA54+AA55)+(Z55*AA56-Z56*AA55)*(AA55+AA56)+(Z56*AA57-Z57*AA56)*(AA56+AA57))/6/Z58","v":0.81902934843133712},"m",null,null,null,null,"II-II i I-I",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AI47+AI48)+(AH48*AI49-AH49*AI48)*(AI48+AI49)+(AH49*AI50-AH50*AI49)*(AI49+AI50)+(AH50*AI51-AH51*AI50)*(AI50+AI51)+(AH51*AI52-AH52*AI51)*(AI51+AI52)+(AH52*AI53-AH53*AI52)*(AI52+AI53)+(AH53*AI54-AH54*AI53)*(AI53+AI54)+(AH54*AI55-AH55*AI54)*(AI54+AI55)+(AH55*AI56-AH56*AI55)*(AI55+AI56)+(AH56*AI57-AH57*AI56)*(AI56+AI57))/6/AH58","v":1.3500505000000005},"m"]
["G=",{"$f":"+B58*'Analiza i dimenzioniranje'!E62","v":64.227611992767947},"kN",{"$f":"+D58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"+F58*'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}},"kN",{"$f":"+H58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(J58*'Analiza i dimenzioniranje'!E63<0,0,J58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+L58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(N58*'Analiza i dimenzioniranje'!U41<0,0,N58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+P58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(R58<=0,0,R58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+T58*'Analiza i dimenzioniranje'!E49","v":{"$error":"#VALUE!"}},"kN (za L)",{"$f":"+V58*'Analiza i dimenzioniranje'!E62","v":37.77589163555291},"kN",{"$f":"+X58*'Analiza i dimenzioniranje'!E62","v":17.793104363851846},"kN",{"$f":"+Z58*'Analiza i dimenzioniranje'!E62","v":13.306056250595223},"kN",null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"AC47+'Analiza i dimenzioniranje'!C192/2","v":0.68753317931068247},{"$f":"+AH58*'Analiza i dimenzioniranje'!E62","v":5.2517757527774878},"kN"]
["Vertikala nasipa na konzoli",null,null,"Moment na konzoli",null,"Pokos na vrhu zida",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - NAPONI ",null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+'C X-XI'!AC49+('Analiza i dimenzioniranje'!C191/2)","v":0.77418208680245293}]
[null,"x","y",{"$f":"IF('Analiza i dimenzioniranje'!G78=0,0,'Analiza i dimenzioniranje'!G78*'Analiza i dimenzioniranje'!C77*'Analiza i dimenzioniranje'!E62*(Q20-B5+'Analiza i dimenzioniranje'!G78/2)+J61*(O16-J59))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"+F64","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"naponi za presjek II-II",null,"naponi za srednji dio ",null,"naponi za presjek I-I"]
[null,{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},"b1=",{"$f":"+H47-2","v":1.4000010999999999},{"$f":"+B52","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y","x","y","x","y","Koordinate dna temelja"]
[null,{"$f":"+B64","v":{"$error":"#VALUE!"}},{"$f":"IF(B65>J49,C19,+C20+'Analiza i dimenzioniranje'!F20+(H52-H50)*TAN('Analiza i dimenzioniranje'!F21*PI()/180))","v":{"$error":"#VALUE!"}},"b2=",{"$f":"'Analiza i dimenzioniranje'!E54+('Analiza i dimenzioniranje'!E55-'Analiza i dimenzioniranje'!E54)*(('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)/(C9-C4))","v":{"$error":"#VALUE!"}},{"$f":"+B65","v":{"$error":"#VALUE!"}},{"$f":"+G64+(F64-F65)*TAN('Analiza i dimenzioniranje'!F21*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,0,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},0,{"$f":"+'C X-XI'!B11","v":4.2000010999999997},{"$f":"-U47","v":0},2,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z65","v":2},{"$f":"AC55","v":{"$error":"#VALUE!"}},{"$f":"+AB65","v":3.4000010999999999},{"$f":"+AA67","v":{"$error":"#VALUE!"}},{"$f":"+AB57","v":4.2000010999999997},{"$f":"AC57","v":{"$error":"#VALUE!"}},{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"(AF66*(AG70-AG65)/(AF70-AF65)-AF65*(AG70-AG65)/(AF70-AF65)+AG65)","v":{"$error":"#VALUE!"}}]
[null,"AKTIVNI TLAKOVI za stabilnost i Presjek III-III (bez E3)",null,null,null,null,null,null,"  AKTIVNI TLAKOVI za presjek kroz zid X-X",null,null,"X-X",null,"    AKTIVNI TLAKOVI za presjek kroz zid XI-XI",null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"AC56","v":{"$error":"#VALUE!"}},{"$f":"+AB66+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AE66","v":{"$error":"#VALUE!"}},{"$f":"+AB58","v":4.9000021999999994},{"$f":"+AC58","v":{"$error":"#VALUE!"}},{"$f":"+AB77","v":{"$error":"#VALUE!"}},{"$f":"+(AF67*(AG65-AG70)/(AF65-AF70)-AF70*(AG65-AG70)/(AF65-AF70)+AG70)","v":{"$error":"#VALUE!"}}]
[null,"E1",null,"E2",null,"E3",null,null,"E1",null,"E2 do presjeka kroz zid II",null,null,"E1",null,"E2",null,null,null,null,null,null,null,null,null,{"$f":"+Z67","v":3.4000010999999999},0,{"$f":"+AB67","v":4.2000010999999997},0,{"$f":"+AD67","v":4.9000021999999994},{"$f":"+U50","v":0},{"$f":"+AB67","v":4.2000010999999997},{"$f":"+(AF68*(AG65-AG70)/(AF65-AF70)-AF70*(AG65-AG70)/(AF65-AF70)+AG70)","v":0.37931024673015767}]
[null,0,{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C71","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,{"$f":"+N69","v":0},{"$f":"+O69","v":{"$error":"#VALUE!"}},{"$f":"+I71","v":{"$error":"#VALUE!"}},{"$f":"+J71","v":{"$error":"#VALUE!"}},null,{"$f":"+B69","v":0},{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+N71","v":{"$error":"#VALUE!"}},{"$f":"+O71","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"+Z65","v":2},0,{"$f":"+AB65","v":3.4000010999999999},0,{"$f":"+AD65","v":4.2000010999999997},{"$f":"+U51","v":0},{"$f":"+AD77","v":{"$error":"#VALUE!"}},{"$f":"+(AF69*(AG66-AG70)/(AF66-AF70)-AF70*(AG66-AG70)/(AF66-AF70)+AG70)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+B69","v":0},{"$f":"+C69-'Analiza i dimenzioniranje'!D17-'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+D69+'Analiza i dimenzioniranje'!E16*'Analiza i dimenzioniranje'!E17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+E69-'Analiza i dimenzioniranje'!E17","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},null,{"$f":"+N70","v":0},{"$f":"+J69-('Analiza i dimenzioniranje'!F20+'P X-X'!E17)","v":{"$error":"#VALUE!"}},{"$f":"+K69+'P X-X'!F16*'P X-X'!F17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},null,{"$f":"+B70","v":0},{"$f":"+O69-('Analiza i dimenzioniranje'!F20+'P XI-XI'!E17)","v":{"$error":"#VALUE!"}},{"$f":"+P69+'P XI-XI'!F16*'P XI-XI'!F17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AB53","v":4.9000021999999994},{"$f":"+AC53","v":0.5}]
[null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('Analiza i dimenzioniranje'!D17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},0,{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F70+'Analiza i dimenzioniranje'!F16*'Analiza i dimenzioniranje'!F17*'Analiza i dimenzioniranje'!F112","v":{"$error":"#VALUE!"}},0,null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('P X-X'!E17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+J70","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+L70","v":2.8},null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('P XI-XI'!E17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+Q70","v":3.14}]
[null,{"$f":"+B69","v":0},{"$f":"+C69","v":{"$error":"#VALUE!"}},0,{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F69","v":0},0,null,{"$f":"+N72","v":0},{"$f":"+O72","v":{"$error":"#VALUE!"}},{"$f":"+D72","v":0},{"$f":"+L69","v":{"$error":"#VALUE!"}},null,{"$f":"+N69","v":0},{"$f":"+O69","v":{"$error":"#VALUE!"}},{"$f":"+D72","v":0},{"$f":"+Q69","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+D69","v":{"$error":"#VALUE!"}},{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F72","v":0},{"$f":"+G70","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+K69","v":{"$error":"#VALUE!"}},{"$f":"+L69","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+P69","v":{"$error":"#VALUE!"}},{"$f":"+Q69","v":{"$error":"#VALUE!"}}]
["Jednadžba vertikale kohezije    Određivanje sjecišta kohezije s pravcem od tlaka",null,null,null,null,null,null,{"$f":"+M74","v":"Jednadžba vertikale kohezije  -  sjecišta kohezije s pravcem od tlaka"},null,null,null,null,"Jednadžba vertikale kohezije  -  sjecišta kohezije s pravcem od tlaka"]
[null,"X","y","X","y","X","y",null,{"$f":"+N75","v":"X"},{"$f":"+O75","v":"y"},"X","y",null,"X","y","X","y"]
[null,{"$f":"2*'Analiza i dimenzioniranje'!D15/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F110)","v":12.361875887090893},{"$f":"B76*(C71-C72)/(B71-B72)-B72*(C71-C72)/(B71-B72)+C72","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!F12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F111)","v":{"$error":"#VALUE!"}},{"$f":"IF(D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69>'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69)","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!C12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F112)","v":{"$error":"#VALUE!"}},{"$f":"IF((F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70)>'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!F17,(F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70))","v":{"$error":"#VALUE!"}},null,{"$f":"+N76","v":12.361875887090893},{"$f":"I76*(J71-J72)/(I71-I72)-I72*(J71-J72)/(I71-I72)+J72","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},null,{"$f":"+B76","v":12.361875887090893},{"$f":"N76*(O71-O72)/(N71-N72)-N72*(O71-O72)/(N71-N72)+O72","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"-0.5*((Z65*AA66-Z66*AA65)+(Z66*AA67-Z67*AA66)+(Z67*AA68-Z68*AA67)+(Z68*AA69-Z69*AA68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((AB65*AC66-AB66*AC65)+(AB66*AC67-AB67*AC66)+(AB67*AC68-AB68*AC67)+(AB68*AC69-AB69*AC68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((AD65*AE66-AD66*AE65)+(AD66*AE67-AD67*AE66)+(AD67*AE68-AD68*AE67)+(AD68*AE69-AD69*AE68)+(AD69*AE70-AD70*AE69)+(AD70*AE71-AD71*AE70)+(AD71*AE72-AD72*AE71)+(AD72*AE73-AD73*AE72))","v":{"$error":"#VALUE!"}},"kN/m'"]
[null,{"$f":"+B76","v":12.361875887090893},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},null,{"$f":"+N77","v":12.361875887090893},{"$f":"+O77","v":{"$error":"#VALUE!"}},{"$f":"+K76","v":{"$error":"#VALUE!"}},{"$f":"+L70","v":2.8},null,{"$f":"+N76","v":12.361875887090893},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+P76","v":{"$error":"#VALUE!"}},{"$f":"+G120","v":3.14},null,null,null,null,null,null,null,null,{"$f":"IF(Z76=0,0,-(+(Z65*AA66-Z66*AA65)*(Z65+Z66)+(Z66*AA67-Z67*AA66)*(Z66+Z67)+(Z67*AA68-Z68*AA67)*(Z67+Z68)+(Z68*AA69-Z69*AA68)*(Z68+Z69))/6/Z76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(AB76=0,0,-(+(AB65*AC66-AB66*AC65)*(AB65+AB66)+(AB66*AC67-AB67*AC66)*(AB66+AB67)+(AB67*AC68-AB68*AC67)*(AB67+AB68)+(AB68*AC69-AB69*AC68)*(AB68+AB69))/6/AB76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(AD76=0,0,-(+(AD65*AE66-AD66*AE65)*(AD65+AD66)+(AD66*AE67-AD67*AE66)*(AD66+AD67)+(AD67*AE68-AD68*AE67)*(AD67+AD68)+(AD68*AE69-AD69*AE68)*(AD68+AD69))/6/AD76)","v":{"$error":"#VALUE!"}},"m"]
["Oznaka","E1",null,"E2",null,"E3",null,{"$f":"+M78","v":"Oznaka"},{"$f":"+N78","v":"E1"},null,"E2",null,"Oznaka","E1",null,"E2",null,null,null,null,null,null,null,null,null,{"$f":"-((Z65*AA66-Z66*AA65)*(AA65+AA66)+(Z66*AA67-Z67*AA66)*(AA66+AA67)+(Z67*AA68-Z68*AA67)*(AA67+AA68)+(Z68*AA69-Z69*AA68)*(AA68+AA69))/6/Z76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((AB65*AC66-AB66*AC65)*(AC65+AC66)+(AB66*AC67-AB67*AC66)*(AC66+AC67)+(AB67*AC68-AB68*AC67)*(AC67+AC68)+(AB68*AC69-AB69*AC68)*(AC68+AC69))/6/AB76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((AD65*AE66-AD66*AE65)*(AE65+AE66)+(AD66*AE67-AD67*AE66)*(AE66+AE67)+(AD67*AE68-AD68*AE67)*(AE67+AE68)+(AD68*AE69-AD69*AE68)*(AE68+AE69))/6/AD76","v":{"$error":"#VALUE!"}},"kN/m'"]
["točke","x","y","x","y","x","y","točke",{"$f":"+N79","v":"x"},{"$f":"+O79","v":"y"},"x","y","točke","x","y","x","y"]
[1,{"$f":"+B77","v":12.361875887090893},{"$f":"+C77","v":{"$error":"#VALUE!"}},{"$f":"+D77","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,1,{"$f":"+I76","v":12.361875887090893},{"$f":"+J76","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17<'Analiza i dimenzioniranje'!Z44,0,K77)","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},1,12.361875887090893,{"$f":"+O77","v":{"$error":"#VALUE!"}},{"$f":"+K80","v":{"$error":"#VALUE!"}},{"$f":"+Q76","v":{"$error":"#VALUE!"}},null,"Jedn pravca zida uz tlo",null,"Jedn pravca arm dno ",null,"Y=",{"$f":"IF(S82=S81,1000000,(T82-T81)/(S82-S81))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X80*S81+T81","v":{"$error":"#VALUE!"}}]
[2,{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G76","v":{"$error":"#VALUE!"}},2,{"$f":"+I71","v":{"$error":"#VALUE!"}},{"$f":"+J71","v":{"$error":"#VALUE!"}},{"$f":"IF(E76<E73,D76,I81)","v":{"$error":"#VALUE!"}},{"$f":"+L76","v":{"$error":"#VALUE!"}},2,{"$f":"+N71","v":{"$error":"#VALUE!"}},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+K81","v":{"$error":"#VALUE!"}},{"$f":"+Q80","v":{"$error":"#VALUE!"}},null,{"$f":"+B4","v":3.4000010999999999},{"$f":"+C4","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!T593","v":2.0499999999999998},{"$f":"+'Analiza i dimenzioniranje'!U593","v":0.18682583433163008},"X=",{"$f":"+(-Z80+Z83)/(X80-X83)","v":{"$error":"#VALUE!"}},"sjeište"]
[3,{"$f":"+B80","v":12.361875887090893},{"$f":"+C76","v":{"$error":"#VALUE!"}},{"$f":"IF(D76>D69,D81,D69)","v":{"$error":"#VALUE!"}},{"$f":"+E81","v":{"$error":"#VALUE!"}},{"$f":"IF(F77>F70,F77,F70)","v":{"$error":"#VALUE!"}},{"$f":"IF(F77>F70,G76,G70)","v":{"$error":"#VALUE!"}},3,{"$f":"+I80","v":12.361875887090893},{"$f":"+J81","v":{"$error":"#VALUE!"}},{"$f":"+K70","v":{"$error":"#VALUE!"}},{"$f":"+L70","v":2.8},3,{"$f":"+N80","v":12.361875887090893},{"$f":"+O76","v":{"$error":"#VALUE!"}},{"$f":"+P70","v":{"$error":"#VALUE!"}},{"$f":"+Q70","v":3.14},null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},{"$f":"+'Analiza i dimenzioniranje'!T594","v":4.8600021999999994},{"$f":"+'Analiza i dimenzioniranje'!U594","v":0.54310345350772504},"Y=",{"$f":"+X80*X81+Z80","v":{"$error":"#VALUE!"}}]
[4,{"$f":"+B80","v":12.361875887090893},{"$f":"+C80","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F71","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},4,{"$f":"+I76","v":12.361875887090893},{"$f":"+J76","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17<'Analiza i dimenzioniranje'!Z44,0,K76)","v":{"$error":"#VALUE!"}},{"$f":"+L77","v":2.8},4,{"$f":"+N80","v":12.361875887090893},{"$f":"+O80","v":{"$error":"#VALUE!"}},{"$f":"+P80","v":{"$error":"#VALUE!"}},{"$f":"+Q82","v":3.14},null,null,null,null,null,"Y=",{"$f":"+(V82-V81)/(U82-U81)","v":0.12678908905341604},"*x",{"$f":"-X83*U81+V81","v":-7.3091798227872762E-2},"CRTANJE"]
[5,null,null,{"$f":"+D80","v":{"$error":"#VALUE!"}},{"$f":"+E80","v":{"$error":"#VALUE!"}},{"$f":"+F80","v":{"$error":"#VALUE!"}},{"$f":"+G80","v":0},5,null,null,{"$f":"+K80","v":{"$error":"#VALUE!"}},{"$f":"+L80","v":{"$error":"#VALUE!"}},5,null,null,{"$f":"+P80","v":{"$error":"#VALUE!"}},{"$f":"+Q80","v":{"$error":"#VALUE!"}},null,"Jedn pravca sloja 3",null,"Jedn pravca sloja 3 klizno",null,"Y=",{"$f":"+(T86-T85)/(S86-S85)","v":-3.4920769491747737E-2},"*x",{"$f":"-X84*S85+T85","v":1.2698415389834954},"Jedn pravca sloja 3 klizno",null,"sjecište 1/2 sidra sa vrhom 1. sloja"]
["  A=",{"$f":"IF(B77>B71,0,-IF(B84>B83,0,-0.5*((B80*C81-B81*C80)+(B81*C82-B82*C81)+(B82*C83-B83*C82)+(B83*C84-B84*C83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D77>D70,0,IF(D84>D83,0,-0.5*((D80*E81-D81*E80)+(D81*E82-D82*E81)+(D82*E83-D83*E82)+(D83*E84-D84*E83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F77>F71,0,IF(F84>F83,0,-0.5*((F80*G81-F81*G80)+(F81*G82-F82*G81)+(F82*G83-F83*G82)+(F83*G84-F84*G83))))","v":{"$error":"#VALUE!"}},"kN/m'","  A=",{"$f":"IF(I77>I71,0,IF(I84>I83,0,-0.5*((I80*J81-I81*J80)+(I81*J82-I82*J81)+(I82*J83-I83*J82)+(I83*J84-I84*J83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(L77>L76,0,IF(K84>K83,0,-0.5*((K80*L81-K81*L80)+(K81*L82-K82*L81)+(K82*L83-K83*L82)+(K83*L84-K84*L83))))","v":{"$error":"#VALUE!"}},"kN/m'","  A=",{"$f":"IF(O77>O76,0,0.5*((N80*O81-N81*O80)+(N81*O82-N82*O81)+(N82*O83-N83*O82)+(N83*O84-N84*O83)))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(Q77>Q76,0,-0.5*((P80*Q81-P81*Q80)+(P81*Q82-P82*Q81)+(P82*Q83-P83*Q82)+(P83*Q84-P84*Q83)))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+U18","v":2},{"$f":"+V18","v":1.2},{"$f":"+W100","v":2},0,"X=",{"$f":"+(-Z84+Z87)/(X84-X87)","v":1.1386903959986558},"sjecište ",null,{"$f":"+U85","v":2},{"$f":"+V85","v":0},"Y=",{"$f":"+X92","v":{"$error":"#VALUE!"}},"*x",{"$f":"+Z92","v":{"$error":"#VALUE!"}}]
["xt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(B80+B81)+(B81*C82-B82*C81)*(B81+B82)+(B82*C83-B83*C82)*(B82+B83)+(B83*C84-B84*C83)*(B83+B84))/6/B85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(D80+D81)+(D81*E82-D82*E81)*(D81+D82)+(D82*E83-D83*E82)*(D82+D83)+(D83*E84-D84*E83)*(D83+D84))/6/D85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(F80+F81)+(F81*G82-F82*G81)*(F81+F82)+(F82*G83-F83*G82)*(F82+F83)+(F83*G84-F84*G83)*(F83+F84))/6/F85)","v":{"$error":"#VALUE!"}},"kN/m'","xt=",{"$f":"IF(I85=0,0,-((I80*J81-I81*J80)*(I80+I81)+(I81*J82-I82*J81)*(I81+I82)+(I82*J83-I83*J82)*(I82+I83)+(I83*J84-I84*J83)*(I83+I84))/6/I85)","v":{"$error":"#VALUE!"}},{"$f":"+O86","v":"kN/m'"},{"$f":"IF(K85=0,0,((K80*L83-K83*L80)*(K80+K83)+(K83*L82-K82*L83)*(K83+K82)+(K82*L81-K81*L82)*(K82+K81)+(K81*L84-K84*L81)*(K81+K84))/6/K85)","v":{"$error":"#VALUE!"}},"kN/m'","xt=",{"$f":"IF(N85=0,0,((N80*O81-N81*O80)*(N80+N81)+(N81*O82-N82*O81)*(N81+N82)+(N82*O83-N83*O82)*(N82+N83)+(N83*O84-N84*O83)*(N83+N84))/6/N85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(P85=0,0,((P80*Q83-P83*Q80)*(P80+P83)+(P83*Q82-P82*Q83)*(P83+P82)+(P82*Q81-P81*Q82)*(P82+P81)+(P81*Q84-P84*Q81)*(P81+P84))/6/P85)","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+U19","v":-8},{"$f":"+V19","v":1.5492076949174773},-5,{"$f":"+V85+(U85-U86)*TAN((45+'Analiza i dimenzioniranje'!F14/2)*PI()/180)","v":9.9970360471948005},"Y=",{"$f":"+X84*X85+Z84","v":1.2300775941423594},3,null,{"$f":"+X85","v":1.1386903959986558},{"$f":"+X86","v":1.2300775941423594}]
["yt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(C80+C81)+(B81*C82-B82*C81)*(C81+C82)+(B82*C83-B83*C82)*(C82+C83)+(B83*C84-B84*C83)*(C83+C84))/6/B85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(E80+E81)+(D81*E82-D82*E81)*(E81+E82)+(D82*E83-D83*E82)*(E82+E83)+(D83*E84-D84*E83)*(E83+E84))/6/D85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(G80+G81)+(F81*G82-F82*G81)*(G81+G82)+(F82*G83-F83*G82)*(G82+G83)+(F83*G84-F84*G83)*(G83+G84))/6/F85)","v":{"$error":"#VALUE!"}},"m","yt=",{"$f":"IF(I85=0,0,-((I80*J81-I81*J80)*(J80+J81)+(I81*J82-I82*J81)*(J81+J82)+(I82*J83-I83*J82)*(J82+J83)+(I83*J84-I84*J83)*(J83+J84))/6/I85)","v":{"$error":"#VALUE!"}},{"$f":"+O87","v":"m"},{"$f":"IF(K85=0,0,((K80*L83-K83*L80)*(L80+L83)+(K83*L82-K82*L83)*(L83+L82)+(K82*L81-K81*L82)*(L82+L81)+(K81*L84-K84*L81)*(L81+L84))/6/K85)","v":{"$error":"#VALUE!"}},"m","yt=",{"$f":"IF(N85=0,0,((N80*O81-N81*O80)*(O80+O81)+(N81*O82-N82*O81)*(O81+O82)+(N82*O83-N83*O82)*(O82+O83)+(N83*O84-N84*O83)*(O83+O84))/6/N85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(P85=0,0,((P80*Q83-P83*Q80)*(Q80+Q83)+(P83*Q82-P82*Q83)*(Q83+Q82)+(P82*Q81-P81*Q82)*(Q82+Q81)+(P81*Q84-P84*Q81)*(Q81+Q84))/6/P85)","v":{"$error":"#VALUE!"}},"m",null,null,null,null,null,"Y=",{"$f":"+(V86-V85)/(U86-U85)","v":-1.4281480067421144},"*x",{"$f":"-X87*U85+V85","v":2.8562960134842288},"y=2       x=",{"$f":"+('Analiza i dimenzioniranje'!E52-'C X-XI'!Z87)/'C X-XI'!X87","v":1.1597509541483482}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(K85<0,0,K85)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+IF(P85<0,0,P85)","v":{"$error":"#VALUE!"}},null,null,"Jedn pravca sloja 2",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(T90-T89)/(S90-S89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X88*S89+T89","v":{"$error":"#VALUE!"}},"Jedn pravca sloja 2 klizno",null,"Jednadžba pravca sidra",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(AD90-AD89)/(AC90-AC89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AH88*AC89+AD89","v":{"$error":"#VALUE!"}}]
["X koordinata položaja rezultante aktivnog tlaka na stražnjoj strani zida za  Ev1, Ev2 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U15","v":{"$error":"#VALUE!"}},{"$f":"+V15","v":4},{"$f":"+X85","v":1.1386903959986558},{"$f":"+X86","v":1.2300775941423594},"X=",{"$f":"+(-Z88+Z91)/(X88-X91)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U89","v":1.1386903959986558},{"$f":"+V89","v":1.2300775941423594},{"$f":"+U37","v":{"$error":"#VALUE!"}},{"$f":"+V37","v":5},{"$f":"+U89","v":1.1386903959986558},{"$f":"+V89","v":1.2300775941423594},"X=",{"$f":"+(-AJ88+AJ91)/(AH88-AH91)","v":{"$error":"#VALUE!"}},"sjecište"]
["Jednadžba pravca zida uz tlo",null,null,null,null,"Za Ev3 x=2",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U16","v":-8},{"$f":"+V16","v":{"$error":"#VALUE!"}},-5,{"$f":"+V89+(U89-U90)*TAN((45+'Analiza i dimenzioniranje'!E14/2)*PI()/180)","v":9.6792600705649363},"Y=",{"$f":"+X88*X89+Z88","v":{"$error":"#VALUE!"}},2,null,{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},{"$f":"+U38","v":{"$error":"#VALUE!"}},{"$f":"+V38","v":{"$error":"#VALUE!"}},{"$f":"+U90","v":-5},{"$f":"+V90","v":9.6792600705649363},"Y=",{"$f":"+AH88*AH89+AJ88","v":{"$error":"#VALUE!"}},2]
[null,"E1",null,"E2",null,"E3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(V90-V89)/(U90-U89)","v":-1.3763819204711731},"*x",{"$f":"-X91*U89+V89","v":2.79735046820907},null,null,null,null,null,null,"Y=",{"$f":"+(AF90-AF89)/(AE90-AE89)","v":-1.3763819204711731},"*x",{"$f":"-AH91*AE89+AF89","v":2.79735046820907}]
["x","y","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,"Jedn pravca sloja 1",null,null,null,"Y=",{"$f":"+(T95-T94)/(S95-S94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X92*S94+T94","v":{"$error":"#VALUE!"}},"Jedan pravca sloja 1 klizno",null,"Slobodna dionica ls>=",{"$f":"+SQRT((AC94-AC93)*(AC94-AC93)+(AD94-AD93)*(AD94-AD93))","v":{"$error":"#VALUE!"}}]
[{"$f":"+(B8-B4)*(B93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+B87","v":{"$error":"#VALUE!"}},{"$f":"+(B8-B4)*(D93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+D87","v":{"$error":"#VALUE!"}},2,{"$f":"+F87","v":{"$error":"#VALUE!"}},null,{"$f":"+(B8-B4)*(I93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+N87","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+(B8-B4)*(N93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+I87","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+V7","v":"A"},null,null,"X=",{"$f":"+(-Z92+Z95)/(X92-X95)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U94","v":{"$error":"#VALUE!"}},{"$f":"+V94","v":{"$error":"#VALUE!"}},{"$f":"+AC89","v":{"$error":"#VALUE!"}},{"$f":"+AD89","v":5}]
[null,null,null,null,"Sloj2",{"$f":"+(B8-B4)*(G94-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!V15","v":4},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U8","v":{"$error":"#VALUE!"}},{"$f":"+V8","v":6},{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+X92*X93+Z92","v":{"$error":"#VALUE!"}},1,null,{"$f":"+X93","v":{"$error":"#VALUE!"}},{"$f":"+X94","v":{"$error":"#VALUE!"}},{"$f":"+AH89","v":{"$error":"#VALUE!"}},{"$f":"+AH90","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+(B8-B4)*(G95-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+K21","v":1.2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782},-5,{"$f":"+V94+(U94-U95)*TAN((45+'Analiza i dimenzioniranje'!D14/2)*PI()/180)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+(V95-V94)/(U95-U94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X95*U94+V94","v":{"$error":"#VALUE!"}},{"$f":"+(AB95-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(AB96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},{"$f":"+(AD96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Masa unutar kliznog tijela - za potres",null,"POTRES",null,"x","y","x","y","x","y",null,null,null,null,"Masa za potres s prosjekom kontrafore i bez kontrafora"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+(B9-B4)*(AD98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},{"$f":"+(B9-B4)*(AF98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B2","v":2},0.12820515121628623,null,null,{"$f":"+(Z95-AB99)/(-X91)","v":{"$error":"#VALUE!"}},{"$f":"+AB98","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!Z44>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'C X-XI'!AC96,(Z91-AD99)/(-X91))","v":-1.9249975254127523E-3},{"$f":"+AD98","v":2.8},{"$f":"IF('Analiza i dimenzioniranje'!AA44>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'C X-XI'!AA96,(Z91-AF99)/(-X91))","v":-0.24894945704723576},{"$f":"+AF98","v":3.14}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,1.2,"Potresna sila za stabilnost",null,"Klizno tijelo za potres za presjek III-III",null,"Klizno tijelo za potres za presjek    X-X",null,"Klizno tijelo za potres za presjek XI-XI",null,null,null,null,null,"Potresna sila za stabilnost "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.4000010999999999,1.2,{"$f":"+'C VIII-IX'!Y101","v":1.75},{"$f":"+'C VIII-IX'!Z101","v":9.6153895463470418E-2},null,null,{"$f":"+AC98","v":{"$error":"#VALUE!"}},{"$f":"+AD96","v":2.8},{"$f":"+AE98","v":{"$error":"#VALUE!"}},{"$f":"+AF98","v":3.14},null,null,null,null,{"$f":"+'C III-V'!Y101","v":1.75},{"$f":"+'C III-V'!Z101","v":9.6153895463470418E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.14,{"$f":"+'C VIII-IX'!Y102","v":0.97707863658009864},{"$f":"+'C VIII-IX'!Z102","v":1.2},{"$f":"+Y102","v":0.97707863658009864},1.2,{"$f":"+AN124","v":-0.21506830928443818},{"$f":"+AO124","v":2.8},{"$f":"+AN125","v":-0.45368374684040591},{"$f":"+AO125","v":3.14},null,null,null,null,{"$f":"+'C III-V'!Y102","v":0.97707863658009864},{"$f":"+'C III-V'!Z102","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.14,{"$f":"+'C VIII-IX'!Y103","v":-1.0572404418349119},{"$f":"+'C VIII-IX'!Z103","v":4},-1.0572404418349119,4,{"$f":"IF(AD103=AD102,AC102,+AA103)","v":-1.0572404418349119},{"$f":"IF($AH$105<=AD102,AD102,$AH$105)","v":4},{"$f":"IF(AF103=AF102,AE102,+AC103)","v":-1.0572404418349119},{"$f":"IF($AH$105<=AF102,AF102,$AH$105)","v":4},null,null,null,null,{"$f":"+'C III-V'!Y103","v":-1.0572404418349119},{"$f":"+'C III-V'!Z103","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.44,{"$f":"+'C VIII-IX'!Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!Z104","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+'C III-V'!Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z104","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.44,{"$f":"+'C VIII-IX'!Y105","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!Z105","v":6.2644906473896782},{"$error":"#VALUE!"},6.2644906473896782,{"$f":"+AA105","v":{"$error":"#VALUE!"}},{"$f":"IF(AA105=AC105,AB105,AB95)","v":{"$error":"#VALUE!"}},{"$f":"+AA105","v":{"$error":"#VALUE!"}},{"$f":"+IF(AA105=AE105,AB105,AB95)","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!AG105","v":" H="},{"$f":"+'C XIV-XV'!AH105","v":4},null,null,{"$f":"+'C III-V'!Y105","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z105","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},"A",{"$f":"+'C VIII-IX'!Y106","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!Z106","v":6},{"$error":"#VALUE!"},6,{"$f":"+AE106","v":{"$error":"#VALUE!"}},{"$f":"+AF106","v":6},{"$f":"+AA106","v":{"$error":"#VALUE!"}},{"$f":"+AB106","v":6},null,null,null,null,{"$f":"+'C III-V'!Y106","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z106","v":6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},"A",{"$f":"+'C VIII-IX'!Y107","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!Z107","v":6},{"$error":"#VALUE!"},6,{"$f":"+AE107","v":{"$error":"#VALUE!"}},{"$f":"+AF107","v":6},{"$f":"+AA107","v":{"$error":"#VALUE!"}},{"$f":"+AB107","v":6},null,null,null,null,{"$f":"+'C III-V'!Y107","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z107","v":6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+W107","v":{"$error":"#VALUE!"}},{"$f":"+X107","v":"A"},{"$f":"+'C VIII-IX'!Y108","v":3.4000000999999997},{"$f":"+'C VIII-IX'!Z108","v":1.2},3.4000000999999997,1.2,{"$f":"+AC109","v":{"$error":"#VALUE!"}},{"$f":"+AD109","v":2.8},{"$f":"+AE109","v":{"$error":"#VALUE!"}},{"$f":"+AF109","v":3.14},null,null,null,null,{"$f":"+'C III-V'!Y108","v":3.4000000999999997},{"$f":"+'C III-V'!Z108","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B11","v":4.2000010999999997},1.2,{"$f":"+'C VIII-IX'!Y109","v":1.75},{"$f":"+'C VIII-IX'!Z109","v":1.2},{"$f":"+AA102","v":0.97707863658009864},{"$f":"+AB102","v":1.2},{"$f":"+AC98","v":{"$error":"#VALUE!"}},{"$f":"+AD101","v":2.8},{"$f":"+AE101","v":{"$error":"#VALUE!"}},{"$f":"+AF101","v":3.14},null,null,null,null,{"$f":"+'C III-V'!Y109","v":1.75},{"$f":"+'C III-V'!Z109","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2000010999999997,1.2,{"$f":"+'C VIII-IX'!Y110","v":1.75},{"$f":"+'C VIII-IX'!Z110","v":9.6153895463470418E-2},null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!Y110","v":1.75},{"$f":"+'C III-V'!Z110","v":9.6153895463470418E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2000010999999997,1.2,{"$f":"-0.5*((Y101*Z102-Y102*Z101)+(Y102*Z103-Y103*Z102)+(Y103*Z104-Y104*Z103)+(Y104*Z105-Y105*Z104)+(Y105*Z106-Y106*Z105)+(Y106*Z107-Y107*Z106)+(Y107*Z108-Y108*Z107)+(Y108*Z109-Y109*Z108)+(Y109*Z110-Y110*Z109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AA101*AB102-AA102*AB101)+(AA102*AB103-AA103*AB102)+(AA103*AB104-AA104*AB103)+(AA104*AB105-AA105*AB104)+(AA105*AB106-AA106*AB105)+(AA106*AB107-AA107*AB106)+(AA107*AB108-AA108*AB107)+(AA108*AB109-AA109*AB108)+(AA109*AB110-AA110*AB109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AC101*AD102-AC102*AD101)+(AC102*AD103-AC103*AD102)+(AC103*AD104-AC104*AD103)+(AC104*AD105-AC105*AD104)+(AC105*AD106-AC106*AD105)+(AC106*AD107-AC107*AD106)+(AC107*AD108-AC108*AD107)+(AC108*AD109-AC109*AD108)+(AC109*AD110-AC110*AD109))","v":{"$error":"#VALUE!"}},null,{"$f":"-0.5*((AE101*AF102-AE102*AF101)+(AE102*AF103-AE103*AF102)+(AE103*AF104-AE104*AF103)+(AE104*AF105-AE105*AF104)+(AE105*AF106-AE106*AF105)+(AE106*AF107-AE107*AF106)+(AE107*AF108-AE108*AF107)+(AE108*AF109-AE109*AF108)+(AE109*AF110-AE110*AF109))","v":{"$error":"#VALUE!"}},"m2",null,null,null,null,{"$f":"-0.5*((AK101*AL102-AK102*AL101)+(AK102*AL103-AK103*AL102)+(AK103*AL104-AK104*AL103)+(AK104*AL105-AK105*AL104)+(AK105*AL106-AK106*AL105)+(AK106*AL107-AK107*AL106)+(AK107*AL108-AK108*AL107)+(AK108*AL109-AK109*AL108)+(AK109*AL110-AK110*AL109))","v":{"$error":"#VALUE!"}},"m2","OK","prosječna površina temelja od temelja kontrafore duž čitavog zida"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.9000021999999994,1.2,{"$f":"-((Y101*Z102-Y102*Z101)*(Y101+Y102)+(Y102*Z103-Y103*Z102)*(Y102+Y103)+(Y103*Z104-Y104*Z103)*(Y103+Y104)+(Y104*Z105-Y105*Z104)*(Y104+Y105)+(Y105*Z106-Y106*Z105)*(Y105+Y106)+(Y106*Z107-Y107*Z106)*(Y106+Y107)+(Y107*Z108-Y108*Z107)*(Y107+Y108)+(Y108*Z109-Y109*Z108)*(Y108+Y109)+(Y109*Z110-Y110*Z109)*(Y109+Y110))/6/Y111","v":{"$error":"#VALUE!"}},"m  ",{"$f":"-((AA101*AB102-AA102*AB101)*(AA101+AA102)+(AA102*AB103-AA103*AB102)*(AA102+AA103)+(AA103*AB104-AA104*AB103)*(AA103+AA104)+(AA104*AB105-AA105*AB104)*(AA104+AA105)+(AA105*AB106-AA106*AB105)*(AA105+AA106)+(AA106*AB107-AA107*AB106)*(AA106+AA107)+(AA107*AB108-AA108*AB107)*(AA107+AA108)+(AA108*AB109-AA109*AB108)*(AA108+AA109)+(AA109*AB110-AA110*AB109)*(AA109+AA110))/6/AA111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AC101*AD102-AC102*AD101)*(AC101+AC102)+(AC102*AD103-AC103*AD102)*(AC102+AC103)+(AC103*AD104-AC104*AD103)*(AC103+AC104)+(AC104*AD105-AC105*AD104)*(AC104+AC105)+(AC105*AD106-AC106*AD105)*(AC105+AC106)+(AC106*AD107-AC107*AD106)*(AC106+AC107)+(AC107*AD108-AC108*AD107)*(AC107+AC108)+(AC108*AD109-AC109*AD108)*(AC108+AC109)+(AC109*AD110-AC110*AD109)*(AC109+AC110))/6/AC111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AE101*AF102-AE102*AF101)*(AE101+AE102)+(AE102*AF103-AE103*AF102)*(AE102+AE103)+(AE103*AF104-AE104*AF103)*(AE103+AE104)+(AE104*AF105-AE105*AF104)*(AE104+AE105)+(AE105*AF106-AE106*AF105)*(AE105+AE106)+(AE106*AF107-AE107*AF106)*(AE106+AE107)+(AE107*AF108-AE108*AF107)*(AE107+AE108)+(AE108*AF109-AE109*AF108)*(AE108+AE109)+(AE109*AF110-AE110*AF109)*(AE109+AE110))/6/AE111","v":{"$error":"#VALUE!"}},"m",null,null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AK101+AK102)+(AK102*AL103-AK103*AL102)*(AK102+AK103)+(AK103*AL104-AK104*AL103)*(AK103+AK104)+(AK104*AL105-AK105*AL104)*(AK104+AK105)+(AK105*AL106-AK106*AL105)*(AK105+AK106)+(AK106*AL107-AK107*AL106)*(AK106+AK107)+(AK107*AL108-AK108*AL107)*(AK107+AK108)+(AK108*AL109-AK109*AL108)*(AK108+AK109)+(AK109*AL110-AK110*AL109)*(AK109+AK110))/6/AK111","v":{"$error":"#VALUE!"}},"m  "]
[null,null,null,null,null,{"$f":"+'C III-V'!F136:G136","v":"Visina presjeka"},null,{"$f":"+'C III-V'!H136:I136","v":"Intezitet"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.9000021999999994,0.5,{"$f":"-((Y101*Z102-Y102*Z101)*(Z101+Z102)+(Y102*Z103-Y103*Z102)*(Z102+Z103)+(Y103*Z104-Y104*Z103)*(Z103+Z104)+(Y104*Z105-Y105*Z104)*(Z104+Z105)+(Y105*Z106-Y106*Z105)*(Z105+Z106)+(Y106*Z107-Y107*Z106)*(Z106+Z107)+(Y107*Z108-Y108*Z107)*(Z107+Z108)+(Y108*Z109-Y109*Z108)*(Z108+Z109)+(Y109*Z110-Y110*Z109)*(Z109+Z110))/6/Y111","v":{"$error":"#VALUE!"}},"m    ",{"$f":"-((AA101*AB102-AA102*AB101)*(AB101+AB102)+(AA102*AB103-AA103*AB102)*(AB102+AB103)+(AA103*AB104-AA104*AB103)*(AB103+AB104)+(AA104*AB105-AA105*AB104)*(AB104+AB105)+(AA105*AB106-AA106*AB105)*(AB105+AB106)+(AA106*AB107-AA107*AB106)*(AB106+AB107)+(AA107*AB108-AA108*AB107)*(AB107+AB108)+(AA108*AB109-AA109*AB108)*(AB108+AB109)+(AA109*AB110-AA110*AB109)*(AB109+AB110))/6/AA111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AC101*AD102-AC102*AD101)*(AD101+AD102)+(AC102*AD103-AC103*AD102)*(AD102+AD103)+(AC103*AD104-AC104*AD103)*(AD103+AD104)+(AC104*AD105-AC105*AD104)*(AD104+AD105)+(AC105*AD106-AC106*AD105)*(AD105+AD106)+(AC106*AD107-AC107*AD106)*(AD106+AD107)+(AC107*AD108-AC108*AD107)*(AD107+AD108)+(AC108*AD109-AC109*AD108)*(AD108+AD109)+(AC109*AD110-AC110*AD109)*(AD109+AD110))/6/AC111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AE101*AF102-AE102*AF101)*(AF101+AF102)+(AE102*AF103-AE103*AF102)*(AF102+AF103)+(AE103*AF104-AE104*AF103)*(AF103+AF104)+(AE104*AF105-AE105*AF104)*(AF104+AF105)+(AE105*AF106-AE106*AF105)*(AF105+AF106)+(AE106*AF107-AE107*AF106)*(AF106+AF107)+(AE107*AF108-AE108*AF107)*(AF107+AF108)+(AE108*AF109-AE109*AF108)*(AF108+AF109)+(AE109*AF110-AE110*AF109)*(AF109+AF110))/6/AE111","v":{"$error":"#VALUE!"}},"m",null,null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AL101+AL102)+(AK102*AL103-AK103*AL102)*(AL102+AL103)+(AK103*AL104-AK104*AL103)*(AL103+AL104)+(AK104*AL105-AK105*AL104)*(AL104+AL105)+(AK105*AL106-AK106*AL105)*(AL105+AL106)+(AK106*AL107-AK107*AL106)*(AL106+AL107)+(AK107*AL108-AK108*AL107)*(AL107+AL108)+(AK108*AL109-AK109*AL108)*(AL108+AL109)+(AK109*AL110-AK110*AL109)*(AL109+AL110))/6/AK111","v":{"$error":"#VALUE!"}},"m    ",null,{"$f":"+'C III-V'!AN113:AN114","v":-0.25},{"$f":"IF('Analiza i dimenzioniranje'!D84=\"\",0,'Analiza i dimenzioniranje'!D83+'C III-V'!AN113)","v":0.75}]
[null,null,null,null,null,{"$f":"+'C III-V'!F137:G137","v":"III"},{"$f":"+'C III-V'!G137:H137","v":1.2},{"$f":"+'C III-V'!H137:I137","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,0.12820515121628623,{"$f":"+Y111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AA111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AC111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AE111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,{"$f":"+AK111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN"]
[null,null,null,null,null,{"$f":"+'C III-V'!F138:G138","v":"VI"},{"$f":"+'C III-V'!G138:H138","v":1.52},{"$f":"+'C III-V'!H138:I138","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Teren  kosina",null,"Klizna ploha"]
[null,null,null,null,null,{"$f":"+'C III-V'!F139:G139","v":"VII"},{"$f":"+'C III-V'!G139:H139","v":1.84},{"$f":"+'C III-V'!H139:I139","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C VIII-IX'!AI116","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!AJ116","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!AK116","v":1.75},{"$f":"+'C VIII-IX'!AL116","v":-1.1133852506716102},"sjecišta ravnine presjeka na kliznoj plohi",null,null,null,null,null,null,"Omjer površine"]
[null,null,null,null,null,{"$f":"+'C III-V'!F140:G140","v":"VIII"},{"$f":"+'C III-V'!G140:H140","v":2.16},{"$f":"+'C III-V'!H140:I140","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koord. Težište mase  za h22",null,null,null,null,null,null,null,null,null,{"$f":"+'C VIII-IX'!AI117","v":6.2644906473896782},{"$f":"+'C VIII-IX'!AJ117","v":6},{"$f":"+'C VIII-IX'!AK117","v":0},{"$f":"+'C VIII-IX'!AL117","v":4.08},{"$f":"+'C III-V'!AA100","v":"oznaka"},{"$f":"+'C III-V'!AB100","v":"X"},{"$f":"+'C III-V'!AC100","v":"Y"},null,null,null,"        sa kontraforama: bez kontrafora",null,null,"Potresna sila-prosječna"]
[null,null,null,null,null,{"$f":"+'C III-V'!F141:G141","v":"IX"},{"$f":"+'C III-V'!G141:H141","v":2.48},{"$f":"+'C III-V'!H141:I141","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(AA102-AA103)/3","v":0.67810635947167019},{"$f":"+Z103*0.666666666666667","v":2.6666666666666679},null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!D116,AI117)","v":-5},{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!E116,'C III-V'!AJ117)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!AA101","v":"Y=0"},{"$f":"+'C III-V'!AB101","v":1.75},{"$f":"+'C III-V'!AC101","v":0},null,null,null,null,null,null,null,null,"Potresna sila","F","G"]
[null,null,null,null,null,{"$f":"+'C III-V'!F142:G142","v":"X"},{"$f":"+'C III-V'!G142:H142","v":2.8},{"$f":"+'C III-V'!H142:I142","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"(AJ117-AI117)/(AJ116-AI116)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AI119*AI116+AI117","v":{"$error":"#VALUE!"}}," ",{"$f":"+'C III-V'!AA102","v":"PIII"},{"$f":"+'C III-V'!AB102","v":0.97707863658009864},{"$f":"+'C III-V'!AC102","v":1.2},null,null,null,null,"Ukupna duljina zida",null,{"$f":"+Kontrafore!E13","v":12},"m",{"$f":"+AV119","v":12},{"$f":"+Y111","v":{"$error":"#VALUE!"}},{"$f":"+Y114","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F143:G143","v":"XI"},{"$f":"+'C III-V'!G143:H143","v":3.14},{"$f":"+'C III-V'!H143:I143","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"-(AL117-AK117)/(AK116-AL116)","v":-1.4248868534344206},"*x    +",{"$f":"-(AK116*AI120-AK117)","v":2.4935519935102359}," ",{"$f":"+'C III-V'!AA103","v":"PVI"},{"$f":"+'C III-V'!AB103","v":0.68324863210273346},{"$f":"+'C III-V'!AC103","v":1.52},null,null,null,null,"ukupna duljina kontrafora",null,{"$f":"+Kontrafore!E5*Kontrafore!E4","v":3},"m",{"$f":"+AV120","v":3},{"$f":"+AY119-AY121","v":{"$error":"#VALUE!"}},{"$f":"IF(AV120=AV119,0,AZ119-AZ121)","v":{"$error":"#VALUE!"}}]
["Presjek kroz zid I",null,"Presjek kroz zid II",null,null,{"$f":"+'C III-V'!F144:G144","v":"XIII"},{"$f":"+'C III-V'!G144:H144","v":3.44},{"$f":"+'C III-V'!H144:I144","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AK120-AK119)/(AI119-AI120)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AI120*AI121+AK120","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA104","v":"PVII"},{"$f":"+'C III-V'!AB104","v":0.45866939675594048},{"$f":"+'C III-V'!AC104","v":1.84},null,null,null,null,"ukupna duljina bez kontrafora",null,{"$f":"+AV119-AV120","v":9},"m",{"$f":"+AX119-AX120","v":9},{"$f":"+AG111","v":0},{"$f":"+IF(AX121=0,0,AG114)","v":0}]
["x","y","x","y",null,{"$f":"+'C III-V'!F145:G145","v":"XIII"},{"$f":"+'C III-V'!G145:H145","v":3.76},{"$f":"+'C III-V'!H145:I145","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA105","v":"PVIII"},{"$f":"+'C III-V'!AB105","v":0.23409016140914748},{"$f":"+'C III-V'!AC105","v":2.16},null,null,null,null,"površina s kontraforama",null,{"$f":"+AV120/AV119","v":0.25}]
[0,{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},{"$f":"+A123","v":0},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},null,{"$f":"+'C III-V'!F146:G146","v":"XIV"},{"$f":"+'C III-V'!G146:H146","v":4.08},{"$f":"+'C III-V'!H146:I146","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($AK$119-$AK$123)/AI119","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AK121","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA106","v":"PIX"},{"$f":"+'C III-V'!AB106","v":9.5109260623546556E-3},{"$f":"+'C III-V'!AC106","v":2.48},null,null,null,null,"površina bez kontrafora",null,{"$f":"+AV121/AV119","v":0.75}]
[{"$f":"+F83","v":{"$error":"#VALUE!"}},{"$f":"+B123","v":3.14},{"$f":"+A124","v":{"$error":"#VALUE!"}},{"$f":"+D123","v":2.8},null,{"$f":"+'C III-V'!F147:G147","v":"XV"},{"$f":"+'C III-V'!G147:H147","v":4.4000000000000004},{"$f":"+'C III-V'!H147:I147","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA107","v":"PX"},{"$f":"+'C III-V'!AB107","v":-0.21506830928443818},{"$f":"+'C III-V'!AC107","v":2.8},null,null,null,null,null,null,"odnos",null,{"$f":"-(AX120/AX119)*'Analiza i dimenzioniranje'!D83","v":-0.25}]
[null,null,null,null,null,{"$f":"+'C III-V'!F148:G148","v":"XVI"},{"$f":"+'C III-V'!G148:H148","v":4.72},{"$f":"+'C III-V'!H148:I148","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA108","v":"PXI"},{"$f":"+'C III-V'!AB108","v":-0.45368374684040591},{"$f":"+'C III-V'!AC108","v":3.14},null,null,null,null,null,"krak",{"$f":"+Y113","v":{"$error":"#VALUE!"}},{"$f":"+AZ119","v":{"$error":"#VALUE!"}},{"$f":"+AZ120*AV122","v":{"$error":"#VALUE!"}},null,{"$f":"+AZ119-AX126","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F149:G149","v":"XVII"},{"$f":"+'C III-V'!G149:H149","v":5.04},{"$f":"+'C III-V'!H149:I149","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($AK$120-AK126)/$AI$120","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AK121","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA109","v":"PXII"},{"$f":"+'C III-V'!AB109","v":-0.66422677997802415},{"$f":"+'C III-V'!AC109","v":3.44},null,null,null,null,null,null,{"$f":"+AG113","v":0},{"$f":"+AZ121","v":0},{"$f":"+AZ120*AV123","v":{"$error":"#VALUE!"}},null,{"$f":"+AZ121+AX125","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F150:G150","v":"XVIII"},{"$f":"+'C III-V'!G150:H150","v":5.36},{"$f":"+'C III-V'!H150:I150","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-1.1976024639266576,null,4.2,null,{"$f":"+'C III-V'!AA110","v":"PXIII"},{"$f":"+'C III-V'!AB110","v":-0.88880601532481696},{"$f":"+'C III-V'!AC110","v":3.76},null,null,null,null,null,null,null,null,"Prosječna masa za potres:",null,{"$f":"IF(IF(AV130=AW130,Y114,+AZ126)=0,AZ125,IF(AV130=AW130,Y114,+AZ126))","v":{"$error":"#VALUE!"}},"kn"]
[null,null,null,null,null,{"$f":"+'C III-V'!F151:G151","v":"XIX"},{"$f":"+'C III-V'!G151:H151","v":5.6800000000000006},{"$f":"+'C III-V'!H151:I151","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.90782786744952648,null,1.2,null,{"$f":"+'C III-V'!AA111","v":"PXIV"},{"$f":"+'C III-V'!AB111","v":-1.1133852506716102},{"$f":"+'C III-V'!AC111","v":4.08}]
[null,null,null,null,null,{"$f":"+'C III-V'!F152:G152","v":"XX"},{"$f":"+'C III-V'!G152:H152","v":6},{"$f":"+'C III-V'!H152:I152","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.6464828732122183,null,{"$f":"+AI117","v":6.2644906473896782},null,{"$f":"+'C III-V'!AA112","v":"PXV"},{"$f":"+'C III-V'!AB112","v":-1.3379644860184032},{"$f":"+'C III-V'!AC112","v":4.4000000000000004}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-0.21506830928443818,null,{"$f":"+AD101","v":2.8},null,{"$f":"+'C III-V'!AA113","v":"PXVI"},{"$f":"+'C III-V'!AB113","v":-1.5625437213651958},{"$f":"+'C III-V'!AC113","v":4.72},null,null,null,null,null,"x=",{"$f":"+AG113","v":0},{"$f":"+Y113","v":{"$error":"#VALUE!"}},null,{"$f":"+AI109","v":0},{"$f":"+AI106","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-0.45368374684040591,null,{"$f":"+AF109","v":3.14},null,{"$f":"+'C III-V'!AA114","v":"PXVII"},{"$f":"+'C III-V'!AB114","v":-1.7871229567119888},{"$f":"+'C III-V'!AC114","v":5.04},null,null,null,null,null,"Y=",{"$f":"+AG114","v":0},{"$f":"+Y114","v":{"$error":"#VALUE!"}},null,{"$f":"+AJ109","v":0},{"$f":"+AJ106","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA115","v":"PXVIII"},{"$f":"+'C III-V'!AB115","v":-2.0117021920587819},{"$f":"+'C III-V'!AC115","v":5.36},null,null,null,null,null,"Y=",{"$f":"(AV131-AW131)/(AV130-AW130)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AV132*AW130+AW131","v":{"$error":"#VALUE!"}},{"$f":"(AY131-AZ131)/(AY130-AZ130)","v":{"$error":"#DIV/0!"}},"*x    +",{"$f":"-AY132*AZ130+AZ131","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA116","v":"PXIX"},{"$f":"+'C III-V'!AB116","v":-2.2362814274055753},{"$f":"+'C III-V'!AC116","v":5.6800000000000006}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA117","v":"PXX"},{"$f":"+'C III-V'!AB117","v":0},{"$f":"+'C III-V'!AC117","v":6.0000000000000009},null,null,null,null,null,"x=",{"$f":"+AK113","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","Y",null,null,null,{"$f":"+AI136","v":{"$error":"#VALUE!"}},{"$f":"+AJ136","v":{"$error":"#VALUE!"}},null,null,null,null,null,"xstv=",{"$f":"+AV134-X113","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C VIII-IX'!AK136","v":{"$error":"#VALUE!"}},{"$f":"+'C VIII-IX'!AL136","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"            Masa da se dobije prosječni potres iz čelije AT125=",null,null,null,null,{"$f":"+AZ125","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+AF104","v":{"$error":"#VALUE!"}},{"$f":"+AD102","v":2.8},{"$f":"+AF102","v":3.14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"razlika¸površina",{"$f":"+Y111-AI111","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AE144-AC138)/(-AC144)","v":{"$error":"#VALUE!"}},{"$f":"IF(AD138<AC138,(AE151-AD138)/(-AC151),(AE156-AD138)/(-AC156))","v":{"$error":"#VALUE!"}},{"$f":"IF(AE138<AC138,(AE151-AE138)/(-AC151),(AE156-AE138)/(-AC156))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"duljina segmenta",{"$f":"++AJ105","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina III. sloja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"okomito na kliz. Plohu",null,{"$f":"+AV143/AV139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"d=","dodatak",{"$f":"+AV140/COS(AV142*PI()/180)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA153","v":2},{"$f":"+'C III-V'!AB153","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"          kut nagiba klizne plohe za potres   a= ",null,{"$f":"ATAN((-Y104+Y101)/(Z104-Z101))*180/PI()","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA154","v":-5},{"$f":"+'C III-V'!AB154","v":9.9970360471948005},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dodatna površina",{"$f":"+AV144/'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AD143-AD142)/(AC143-AC142)","v":-1.4281480067421144},"*x      +",{"$f":"-AC144*AC142+AD142","v":2.8562960134842288},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"G=",{"$f":"+AX126","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AE144-AD146)/(-AC144)","v":1.1597509541483482}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+Z102","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina II. sloja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA148","v":-1.0572404418349119},{"$f":"+'C III-V'!AB148","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA149","v":0.97707863658009864},{"$f":"+'C III-V'!AB149","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AD150-AD149)/(AC150-AC149)","v":-1.3763819204711734},"*x      +",{"$f":"-AC151*AC149+AD149","v":2.5448333702674724}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina I. sloja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koordinate na sjecištu s terenom",null,null,{"$f":"+'C III-V'!AA144","v":-2.5846586698092704},{"$f":"+'C III-V'!AB144","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koordinate na sjecištu slojeva",null,null,{"$f":"+'C III-V'!AA143","v":-1.0572404418349119},{"$f":"+'C III-V'!AB143","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AD155-AD154)/(AC155-AC154)","v":-1.4825609685127401},"*x      +",{"$f":"-AC156*AC154+AD154","v":2.4325765866023956}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rub dna konzole uz aktivni klin",null,null,{"$f":"+B6","v":{"$error":"#VALUE!"}},{"$f":"+C6","v":3.14}]

{"sheet":"C XII-XIII","index":43,"n_rows":157,"n_cols":53,"rows_kept":157,"cut":false,"hidden":true,"merged":[[112,5,112,6],[116,47,116,49],[96,32,98,33],[96,34,98,35],[96,36,98,37],[99,32,99,33],[99,34,99,35],[99,36,99,37],[115,38,115,40],[110,38,113,38],[110,39,111,40],[112,39,113,39],[112,40,113,40],[99,28,99,29],[99,30,99,31],[114,34,114,35],[99,24,99,25],[67,10,67,11],[67,13,67,14],[77,13,77,14],[77,10,77,11],[67,20,67,21],[77,15,77,16],[67,15,67,16],[90,1,90,2],[90,3,90,4],[90,5,90,6],[42,11,43,14],[96,22,97,23],[67,22,67,23],[44,7,44,8],[44,17,44,18],[42,1,42,2],[42,3,42,4],[42,5,42,6],[42,7,43,10],[44,9,44,10],[44,11,44,12],[77,1,77,2],[77,3,77,4],[77,5,77,6],[77,8,77,9],[67,1,67,2],[67,3,67,4],[67,5,67,6],[67,8,67,9],[42,15,43,18],[44,21,44,22],[44,13,44,14],[44,15,44,16],[10,3,10,4],[17,12,17,16],[10,27,10,28],[11,3,11,4],[12,27,12,28],[13,12,13,16],[13,27,13,28],[0,1,0,2],[0,3,0,4],[0,5,0,7],[0,9,0,10],[1,5,1,8],[114,36,114,37],[139,27,139,30],[146,27,146,30],[151,27,151,30],[13,29,13,30],[62,29,62,30],[62,27,62,28],[16,27,16,28],[99,26,99,27],[17,27,17,28],[26,27,26,28]]}
["Točke","ZID I TEMELJ",null,"NASIP NA TEMELJU IZA",null,"ZID, KONZOLA I NASIP NA KONZOLI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Točka A",null,"Presjek I-I"]
[1,2,{"$f":"+'C III-V'!$C$2","v":0.12820515121628623},null,null,"ZA BILO KOJI PRESJEK ",null,null,null,null,null,null,null,null,null,null,null,"Presjek zid Iv",{"$f":"+($B$9-$B$4)*(T2-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},{"$f":"+B15","v":4.9000021999999994},{"$f":"+C15","v":0.5},{"$f":"+'C XII-XIII'!B10+0.05","v":{"$error":"#VALUE!"}},-0.5]
[2,2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T3-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},"Točka B",null,{"$f":"+W2","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!C10+0.5","v":{"$error":"#VALUE!"}}]
[3,{"$f":"+B3+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+C3","v":1.2},{"$f":"+B19","v":2},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>C4,B21,B4)","v":3.4000010999999999},{"$f":"IF(E20>C4,E20,C4)","v":1.2},{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},null,null,null,null,null,null,null,null,"Presjek V",{"$f":"+($B$9-$B$4)*(T4-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},{"$f":"+'C XII-XIII'!B2","v":2},{"$f":"+'C XII-XIII'!C2","v":0.12820515121628623}]
[4,{"$f":"+B23","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},{"$f":"+D4","v":2},{"$f":"+'C III-V'!E5","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,B21,B5)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,E20,C5)","v":3.14},{"$f":"+F8","v":{"$error":"#VALUE!"}},{"$f":"+G8","v":3.44},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T5-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},null,null,"Presjek II-II",null,null,null,"Nasip na zidu iza"]
[5,{"$f":"+B5-'Analiza i dimenzioniranje'!G78","v":{"$error":"#VALUE!"}},{"$f":"+C5","v":3.14},{"$f":"IF(B6<2,B5,IF(B9>2,B9,D5))","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!E6","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C7,B21,B6)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C6,E20,C6)","v":3.14},{"$f":"IF(F7>F9,H5,F9)","v":{"$error":"#VALUE!"}},{"$f":"IF(F7>F9,I5,IF(E20>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XII-XIII'!E20,G9))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"Presjek VI",{"$f":"+($B$9-$B$4)*(T6-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},"TLO 1. sloj",null,{"$f":"+'C XII-XIII'!B15-0.05","v":4.8500021999999996},{"$f":"+'C XII-XIII'!X2","v":-0.5},null,null,2,{"$f":"IF('Analiza i dimenzioniranje'!AW26>'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AW26)","v":0}]
[6,{"$f":"IF('Analiza i dimenzioniranje'!G78=0,'C XII-XIII'!B8,B6)","v":{"$error":"#VALUE!"}},{"$f":"C6+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+B4","v":3.4000010999999999},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>=C7,B21,B7)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C7,E20,C7)","v":3.44},{"$f":"IF(F7>F9,H6,H6)","v":{"$error":"#VALUE!"}},{"$f":"+I6","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T7-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},{"$f":"+'C XII-XIII'!B15-0.05","v":4.8500021999999996},{"$f":"+'C XII-XIII'!X3","v":{"$error":"#VALUE!"}},"Horizontala",null,2,{"$f":"'Analiza i dimenzioniranje'!BF28","v":0}]
[7,{"$f":"+B22","v":{"$error":"#VALUE!"}},{"$f":"+C7","v":3.44},{"$f":"+D4","v":2},{"$f":"+E4","v":1.2},{"$f":"IF(E20>C8,B21,B8)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C8,E20,C8)","v":3.44},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$H$15=0,I7+(H7-H8)*'Unos podataka'!R57,IF('C III-V'!H9>'Unos podataka'!$B$105,I7+(H7-H8)*'Unos podataka'!$R$55,'Unos podataka'!$T$57))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"Presjek VII",{"$f":"+($B$9-$B$4)*(T8-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!V8","v":6},null,null,{"$f":"+'C XII-XIII'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!C5","v":3.14}]
[8,{"$f":"B4-TAN('Analiza i dimenzioniranje'!H51*PI()/180)*('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},null,null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"+I4","v":3.44},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T9-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},{"$f":"+U8-'Analiza i dimenzioniranje'!E27","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!V9","v":6.2644906473896782},"Presjek ZID",null,{"$f":"+IF('Analiza i dimenzioniranje'!$E$24=0,0,'C XII-XIII'!Y4)","v":0},{"$f":"+Z8","v":3.14}]
[9,{"$f":"+B9+'Analiza i dimenzioniranje'!E54","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},null,null,{"$f":"+B10","v":{"$error":"#VALUE!"}},{"$f":"+C10","v":"A"},null,null,null,null,null,null,null,null,null,null,"Presjek VIII",{"$f":"+($B$9-$B$4)*(T10-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},-8,{"$f":"+'C III-V'!V10","v":6.2644906473896782},{"$f":"+'C XII-XIII'!B15-0.5","v":4.4000021999999994},{"$f":"+'C XII-XIII'!C10+0.1","v":{"$error":"#VALUE!"}}]
[10,{"$f":"+B4+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+C3","v":1.2},"NASIP NA KONZOLI",null,{"$f":"+F12+E65","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C11,E20,C11)","v":1.2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T11-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},"x","y",{"$f":"+'C XII-XIII'!B10+0.5","v":{"$error":"#VALUE!"}},{"$f":"+X10","v":{"$error":"#VALUE!"}},null,null,null,"Rsidra"]
[11,{"$f":"+B11","v":4.2000010999999997},{"$f":"+C11","v":1.2},"za stabilnost",null,{"$f":"+F4","v":3.4000010999999999},{"$f":"+G4","v":1.2},null,null,null,null,null,null,null,null,null,null,"Presjek IX",{"$f":"+($B$9-$B$4)*(T12-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+W23","v":{"$error":"#VALUE!"}},{"$f":"+U12*(V9-V8)/(U9-U8)-U8*(V9-V8)/(U9-U8)+V8","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,20,AB16)","v":20},{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,0,AC16)","v":0}]
[12,{"$f":"+B12","v":4.2000010999999997},{"$f":"+C12","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T13-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+W25","v":{"$error":"#VALUE!"}},{"$f":"+U13*(V9-V8)/(U9-U8)-U8*(V9-V8)/(U9-U8)+V8","v":{"$error":"#VALUE!"}},"Pad terena niz padinu",null,null,null,null,"Os rezultante sidara Ukupna računska sila u sidrima"]
[13,{"$f":"+B11+'Analiza i dimenzioniranje'!G57","v":4.9000021999999994},{"$f":"+C13","v":1.2},{"$f":"+B7","v":{"$error":"#VALUE!"}},3.44,null,null,null,null,"Linija presjeka",null,null," Koordinata sredine presjeka",null,null,null,null,"Presjek X",{"$f":"+($B$9-$B$4)*(T14-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},"TLO 2. sloj",null,{"$f":"+'Analiza i dimenzioniranje'!Q105","v":3},{"$f":"+'Analiza i dimenzioniranje'!P105","v":{"$error":"#VALUE!"}},null,null,null,"Slobodna  zona.",null,"1. sloj"]
[14,{"$f":"+B14","v":4.9000021999999994},{"$f":"+C14-'Analiza i dimenzioniranje'!E51","v":0.5},{"$error":"#VALUE!"},3.44,{"$f":"IF((B4-B9)=0,0,+(C9-C4)/(B4-B9))","v":{"$error":"#VALUE!"}},"n  Nagib zida u tlu",null,null,0,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,"III-III","konzola","Presjek I","Presjek II",null,{"$f":"+($B$11-$B$10)*(T15-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},{"$f":"IF(('Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17)<'Analiza i dimenzioniranje'!$F$45,2,(IF(B7<B24,B7,IF('Analiza i dimenzioniranje'!G78=0,'C XII-XIII'!B24,2))))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17","v":4},{"$f":"+'Analiza i dimenzioniranje'!O130","v":7.1000021999999996},{"$f":"+'Analiza i dimenzioniranje'!N130","v":1.5001009999999999},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,AB24)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,'Analiza i dimenzioniranje'!P22)","v":5},{"$f":"+U9","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782}]
[15,{"$f":"+B2","v":2},{"$f":"+C2","v":0.12820515121628623},{"$error":"#VALUE!"},"A",null,null,null,null,3,{"$f":"+K15","v":1.2},null,"x",{"$f":"+(F12+F11)/2","v":{"$error":"#VALUE!"}},{"$f":"(B8+(B11-B10)*(O17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U29+(B11-B10)*(P17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U34+(B11-B10)*(Q17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},"Presjek XI",{"$f":"+($B$9-$B$4)*(T16-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},-8,{"$f":"+V15+(U15-U16)*TAN('Analiza i dimenzioniranje'!$E$18*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"AB15-'Analiza i dimenzioniranje'!P23","v":{"$error":"#VALUE!"}},{"$f":"+AC15-(AB15-AB16)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782}]
[null,null,"Jednadžba pravca zida uz tlo",{"$f":"+D16","v":{"$error":"#VALUE!"}},{"$f":"+I7","v":{"$error":"#VALUE!"}},null,null,null,null,"Sloj 2 gore",null,null,"y",{"$f":"+G11","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},null,{"$f":"+($B$11-$B$10)*(T17-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},"TLO 3. sloj",null,"Prometno opterećenje",null,null,null,null,"Sidrena dionica",null,"Jednadžba površine terena"]
[null,"x","y",{"$f":"+D14","v":{"$error":"#VALUE!"}},{"$f":"+I8","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+F94","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E52>=G94,0,G94)","v":4},null,null,null,null,null,null,"Presjek XII",{"$f":"+($B$9-$B$4)*(T18-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},2,{"$f":"+'Analiza i dimenzioniranje'!$F$17","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,+'C XII-XIII'!B9-'Analiza i dimenzioniranje'!E26)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,'C XII-XIII'!V9)","v":6.2644906473896782},null,null,null,"                   Y=",null,{"$f":"+(AE16-AE15)/(AD16-AD15)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AD18*AD15+AE15","v":{"$error":"#VALUE!"}}]
[null,2,{"$f":"+B19*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},{"$f":"+D14","v":{"$error":"#VALUE!"}},{"$f":"+E14","v":3.44},null,null,null,null,{"$f":"U16","v":-8},{"$f":"+K18","v":4},null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T19-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},-8,{"$f":"+V18+(U18-U19)*TAN('Analiza i dimenzioniranje'!$F$18*PI()/180)","v":1.5492076949174773},{"$f":"+W18","v":{"$error":"#VALUE!"}},{"$f":"+X18+'Analiza i dimenzioniranje'!E24/50","v":6.4644906473896784},null,null,null,{"$f":"+AB16","v":{"$error":"#VALUE!"}},{"$f":"+AC16","v":{"$error":"#VALUE!"}},"za x=",{"$f":"+AB20","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+H8","v":{"$error":"#VALUE!"}},{"$f":"+B20*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},"M na koti",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,"Sloj 1 ili2 dole",null,null,null,null,null,null,{"$f":"+(B11-B10)*(Q21-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},"Presjek XIII",{"$f":"+($B$9-$B$4)*(T20-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},"KONTAKTNI NAPONI",null,{"$f":"+W18-'Analiza i dimenzioniranje'!E25","v":{"$error":"#VALUE!"}},{"$f":"+X19","v":6.4644906473896784},null,null,null,{"$f":"+(AB21+AB19)/2","v":{"$error":"#VALUE!"}},{"$f":"+(AC19+AC21)/2","v":{"$error":"#VALUE!"}},"y=",{"$f":"+AD18*AE19+AF18","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C21-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,{"$f":"+IF('Analiza i dimenzioniranje'!G78=0,D8,H8)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+F95","v":{"$error":"#VALUE!"}},{"$f":"+G12","v":1.2},null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,{"$f":"+($B$11-$B$10)*(T21-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},2,0,{"$f":"+W20","v":{"$error":"#VALUE!"}},{"$f":"+X18","v":6.2644906473896782},null,null,null,{"$f":"+AB19-'Analiza i dimenzioniranje'!P24","v":{"$error":"#VALUE!"}},{"$f":"+AC19-(AB19-AB21)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},"visina sloja iznad centra sidra"]
[null,{"$f":"+(B9-B4)*(C22-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+C23+'Analiza i dimenzioniranje'!C77","v":3.44},null,null,null,null,null,null,{"$f":"+U19","v":-8},{"$f":"+K21","v":1.2},null,null,null,null,null,null,"Presjek XIV",{"$f":"+($B$9-$B$4)*(T22-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},2,{"$f":"-'Analiza i dimenzioniranje'!$F$193/100","v":{"$error":"#VALUE!"}},"Točkasto",null,null,null,null,null,null,{"$f":"+AE20-AC20","v":{"$error":"#VALUE!"}},"m"]
[null,{"$f":"+(B9-B4)*(C23-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T23-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"2+'Analiza i dimenzioniranje'!$E$61","v":4.9000021999999994},{"$f":"-'Analiza i dimenzioniranje'!$F$190/100","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E36=0,-10,B9-'Analiza i dimenzioniranje'!E37)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X23","v":{"$error":"#VALUE!"}},null,null,null,"Jednadžba  lica zida "]
[null,{"$f":"+(B9-B4)*(C24-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V15","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek XV",{"$f":"+($B$9-$B$4)*(T24-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U23","v":4.9000021999999994},0,"Linijsko iza zida",null,null,null,"x=",{"$f":"+($B$11-$B$10)*(AB25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+($B$11-$B$10)*(AC25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+(B11-B10)*(AE25-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C25-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U21","v":2},0,{"$f":"IF('Analiza i dimenzioniranje'!$E$34=0,0,B9-'Analiza i dimenzioniranje'!K28)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X27","v":{"$error":"#VALUE!"}},null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!AB42","v":5},{"$f":"+'Analiza i dimenzioniranje'!AC42","v":5},null,{"$f":"+'Analiza i dimenzioniranje'!H76+'Analiza i dimenzioniranje'!E52","v":1.5001009999999999}]
[null,{"$f":"+(B9-B4)*(C26-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid XIII-XIII",{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},{"$f":"+W25","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$34=0,0,X25+1)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!T22","v":0},null,null,null,null,{"$f":"+B14-AE24","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C27-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},"TEMELJ -opterećenje",null,"x=",{"$f":"+($B$11-$B$10)*(Z26-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"Rez. Sidra na zidu"]
[null,{"$f":"+(B9-B4)*(C26-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V27","v":3.76},{"$f":"+IF('Analiza i dimenzioniranje'!E28=0,0,W29)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9+'Analiza i dimenzioniranje'!F20+1.5)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!S22","v":0}]
["Sjecište s dnom temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V29-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":3.76},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W30-0.3)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X30)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z28-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+($B$11-$B$10)*(AC29-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E40","v":3.9999999960000001},{"$f":"+AB29+0.4","v":{"$error":"#VALUE!"}},{"$f":"+AC29+(AD29-AB29)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}}]
["zid",{"$f":"+B20","v":{"$error":"#VALUE!"}},{"$f":"+B30*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V30-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":3.76},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,B9-'Analiza i dimenzioniranje'!$E$32)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X31+'Analiza i dimenzioniranje'!E33)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!R22","v":0},null,null,null,{"$f":"+AB29-1","v":{"$error":"#VALUE!"}},{"$f":"+AC29-(AB29-AD30)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}}]
["Vrh zida",{"$f":"+(B9-B4)*(C31-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C558","v":-0.45},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid Iv",{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},{"$f":"+W30","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9-'Analiza i dimenzioniranje'!K31)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z30-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"nagib lica"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,W31-'Analiza i dimenzioniranje'!$E$29)","v":{"$error":"#VALUE!"}},{"$f":"+X31","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q22","v":3},null,"tan"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V32","v":3.44},{"$f":"+W32","v":{"$error":"#VALUE!"}},{"$f":"+X30","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z32-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+(B13-B10)/(C10-C13)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V34-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V33","v":3.44},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W33+0.3)","v":{"$error":"#VALUE!"}},{"$f":"+X29","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q20","v":5},null,"kut"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V35-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V34","v":3.44},{"$f":"+W34","v":{"$error":"#VALUE!"}},{"$f":"+X28","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z34-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+ATAN(AB33)*180/PI()","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SIDRO za presjek",null,null,null,"Jednadžba pravca lica zida ",null,null,"Sjecište a arm konzole",null,"vrh zida","Anker armatura uz lice",null,"arm dno",null,"Y=",{"$f":"IF(AE38=AE37,1000000,(AF38-AF37)/(AE38-AE37))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AJ36*AE37+AF37","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!$C$545","v":1.6923077248520526}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB15)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC15)","v":5},null,null,"x=",null,null,{"$f":"+(B11-B10)*(AB38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AC38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AD38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AF37-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!B545","v":{"$error":"#VALUE!"}},{"$f":"+U81","v":2.0499999999999998},{"$f":"+V81","v":0.18682583433163008},"X=",{"$f":"+(-AL36+AL39)/(AJ36-AJ39)","v":{"$error":"#VALUE!"}},"sjeište",null,"x=",{"$f":"+(AN36-AL36)/AJ36","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB16)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC16)","v":{"$error":"#VALUE!"}},null,null,"y=",null,null,{"$f":"+'Analiza i dimenzioniranje'!E555","v":3.39},{"$f":"+AB38-'Analiza i dimenzioniranje'!#REF!","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!C558","v":-0.45},{"$f":"+(B11-B10)*(AF38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+U82","v":4.8600021999999994},{"$f":"+V82","v":0.54310345350772504},"Y=",{"$f":"+AJ36*AJ37+AL36","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate dna temelja",null,null,null,null,null,null,"Y=",{"$f":"+(AH38-AH37)/(AG38-AG37)","v":0.12678908905341604},"*x",{"$f":"-AJ39*AG37+AH37","v":-7.3091798227872762E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"lice","koord Pr II",{"$f":"+AB47+'Analiza i dimenzioniranje'!Q58","v":3.4500010999999997},{"$f":"(AB40*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24999999999999994},null,"SIDRO"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+(B11-B10)*(Z42-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+B8","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+AB15","v":{"$error":"#VALUE!"}},{"$f":"+AC15","v":5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+Z42","v":3.44},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,AB15-0.5)","v":{"$error":"#VALUE!"}},{"$f":"+AF41-(AE41-AE42)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},null,"Nasip ispred zida"]
["Oznaka","temelj",null,"Zid i konzola za pr. ZID",null,"Nasip na temelju iza zida",null,"      Za momente u presjeku zid-temelj          ",null,null,null,"      Za momente u presjeku XII-XII",null,null,null,"         Za momente u presjeku XIII-XIII",null,null,null,null,1,null,null,null,null,null,null,2,0,null,null,null,null,{"$f":"+AE24","v":{"$error":"#VALUE!"}},{"$f":"+C11+'Analiza i dimenzioniranje'!$H$76","v":1.5001009999999999}]
["točke","x","y","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - BETON",null,null,null,null,null,2.65,{"$f":"+(AC47+AC49)/2","v":0.31034478180740688},null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!$E$61","v":4.9000021999999994},{"$f":"+AI43","v":1.5001009999999999}]
[1,{"$f":"+'C XII-XIII'!B2","v":2},{"$f":"+'C XII-XIII'!C2","v":0.12820515121628623},null,null,null,null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"Kontaktni naponi za stab",null,"Beton do presjeka II-II",null,"Beton sredine temelja",null,"Beton do presjeka I-I",null,{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"(AB45*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH44+1.6","v":6.5000021999999991},{"$f":"+AI44-(AH45-AH44)*TAN('Analiza i dimenzioniranje'!H22*PI()/180)","v":1.5001009999999999}]
[2,{"$f":"+'C XII-XIII'!B3","v":2},{"$f":"+'C XII-XIII'!C3","v":1.2},null,null,null,null,"x","y","x","y","x","y","x","y","x","y","x","y","x","y",null,null,"x","y","x","y",{"$f":"+(AB43+AB47)/2","v":2.7000005499999999},{"$f":"(AB46*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.1206896584423281},null,null,null,null,"x","y"]
[3,{"$f":"+'C XII-XIII'!B4","v":3.4000010999999999},{"$f":"+'C XII-XIII'!C4","v":1.2},{"$f":"+B4","v":3.4000010999999999},1.2,2,1.2,3.4000010999999999,1.2,{"$f":"+D14","v":{"$error":"#VALUE!"}},3.44,{"$f":"+U34","v":{"$error":"#VALUE!"}},{"$f":"+V34","v":3.44},{"$f":"+J47","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AB44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AB44,K47)","v":3.44},{"$f":"+U29","v":{"$error":"#VALUE!"}},{"$f":"+V29","v":3.76},{"$f":"+J47","v":{"$error":"#VALUE!"}},{"$f":"+S48","v":3.76},{"$f":"+U21","v":2},{"$f":"+V21*100","v":0},2,0,{"$f":"+B4","v":3.4000010999999999},{"$f":"+W49","v":1.2},{"$f":"+B11","v":4.2000010999999997},1.2,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"(AB47*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24137931688465614},"Presjek II-II",null,null,null,{"$f":"+'C XII-XIII'!B11","v":4.2000010999999997},{"$f":"+C11","v":1.2}]
[4,{"$f":"+B11","v":4.2000010999999997},1.2,{"$error":"#VALUE!"},3.14,2,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.44,{"$f":"+H48","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AB44<'Analiza i dimenzioniranje'!F45,I48,'C XII-XIII'!V34)","v":3.44},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AB44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AB44,K48)","v":3.44},{"$f":"+H48","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AC44<'Analiza i dimenzioniranje'!F45,I48,V29)","v":3.76},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AC44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AC44,K48)","v":3.76},{"$f":"+U22","v":2},{"$f":"+V22*100","v":{"$error":"#VALUE!"}},2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+X47+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+Y47","v":1.2},4.2000010999999997,1.2,{"$f":"+AB77","v":{"$error":"#VALUE!"}},{"$f":"(AB48*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47+'Analiza i dimenzioniranje'!H76","v":1.5001009999999999}]
[5,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.14,{"$f":"+D16","v":{"$error":"#VALUE!"}},{"$f":"+E16+'Unos podataka'!$F9","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AB44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XII-XIII'!L47,'C XII-XIII'!B6)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AB44<'Analiza i dimenzioniranje'!F45,I49,'C XII-XIII'!V34)","v":3.44},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AB44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AB44,K49)","v":3.44},{"$f":"IF('Analiza i dimenzioniranje'!AC44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XII-XIII'!B6,P47)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AC44<'Analiza i dimenzioniranje'!F45,'C XII-XIII'!I49,Q48)","v":3.76},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AC44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AC44,K49)","v":3.76},{"$f":"+U23","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},{"$f":"+V48+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+W48","v":1.2},{"$f":"+AB49","v":4.2000010999999997},{"$f":"+AC49","v":0.37931024673015767},4.2000010999999997,1.2,{"$f":"+AB47+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+(AB49*(AC43-AC53)/(AB43-AB53)-AB53*(AC43-AC53)/(AB43-AB53)+AC53)","v":0.37931024673015767},"Presjek I-I",null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+AI48","v":1.5001009999999999}]
[6,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.44,3.4000010999999999,1.2,{"$error":"#VALUE!"},3.44,{"$f":"IF('Unos podataka'!$B$105>J47,'Unos podataka'!$B$105,J47)","v":{"$error":"#VALUE!"}},{"$f":"+K51","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AB44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XII-XIII'!L48,'C XII-XIII'!B7)","v":{"$error":"#VALUE!"}},{"$f":"+O47","v":3.44},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AB44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AB44,K50)","v":3.44},{"$f":"IF('Analiza i dimenzioniranje'!AC44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XII-XIII'!P47,H50)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AC44<='Analiza i dimenzioniranje'!F45,I50,V29)","v":3.76},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AC44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AC44,K50)","v":3.76},{"$f":"+U24","v":4.9000021999999994},{"$f":"+V24*100","v":0},{"$f":"+V49","v":3.4000010999999999},{"$f":"+AC47","v":0.24137931688465614},{"$f":"+X47","v":3.4000010999999999},{"$f":"+AC47","v":0.24137931688465614},4.9000021999999994,1.2,{"$f":"2+'Analiza i dimenzioniranje'!E61/2","v":3.4500010999999997},{"$f":"(AB50*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24999999999999994},null,null,null,null,{"$f":"+AH49","v":4.9000021999999994},{"$f":"+C14","v":1.2}]
[7,4.9000021999999994,1.2,{"$error":"#VALUE!"},3.44,2,1.2,{"$error":"#VALUE!"},3.44,{"$f":"+D18","v":{"$error":"#VALUE!"}},{"$f":"+E18+'Unos podataka'!$F9","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AB44>'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XII-XIII'!B28,B8)","v":{"$error":"#VALUE!"}},{"$f":"+M50","v":3.44},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AB44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AB44,K51)","v":3.44},{"$f":"IF('Analiza i dimenzioniranje'!AC44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XII-XIII'!B25,H51)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AC44<='Analiza i dimenzioniranje'!F45,I51,V29)","v":3.76},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AC44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AC44,K51)","v":3.76},{"$f":"+U25","v":2},{"$f":"+V25*100","v":0},{"$f":"+V47","v":2},{"$f":"+W47","v":0},{"$f":"+X47","v":3.4000010999999999},{"$f":"+Y47","v":1.2},4.9000021999999994,0.5,{"$f":"+(AB49+AB53)/2","v":4.5500016499999996},{"$f":"(AB51*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.43965512336507878},null,null,null,null,{"$f":"+B13","v":4.2000010999999997},{"$f":"+C13","v":1.2}]
[8,4.9000021999999994,0.5,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",{"$error":"#VALUE!"},3.44,{"$f":"+H52","v":{"$error":"#VALUE!"}},{"$f":"+Q52","v":"A"},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AB44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AB44,K52)","v":3.44},{"$f":"+H52","v":{"$error":"#VALUE!"}},{"$f":"+I52","v":"A"},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AC44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AC44,K52)","v":3.76},null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AC49","v":0.37931024673015767},{"$f":"+AD77","v":{"$error":"#VALUE!"}},{"$f":"(AB52*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH51","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[9,2,0.12820515121628623,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",null,null,{"$f":"+H53","v":{"$error":"#VALUE!"}},{"$f":"+Q53","v":"A"},null,null,{"$f":"+H53","v":{"$error":"#VALUE!"}},{"$f":"+I53","v":"A"},null,null,null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AA47","v":1.2},{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+C15","v":0.5},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[10,null,null,4.2000010999999997,1.2,null,null,{"$error":"#VALUE!"},1.2,null,null,{"$f":"+U35","v":{"$error":"#VALUE!"}},{"$f":"+M47","v":3.44},null,null,{"$f":"+U30","v":{"$error":"#VALUE!"}},{"$f":"+V30","v":3.76},null,null,null,null,null,null,null,null,null,null,"Koordinate s","naprezanjem"]
[11,null,null,{"$f":"+D47","v":3.4000010999999999},{"$f":"+E47","v":1.2},null,null,3.4000010999999999,1.2,null,null,{"$f":"+L47","v":{"$error":"#VALUE!"}},{"$f":"+M47","v":3.44},null,null,{"$f":"+P47","v":{"$error":"#VALUE!"}},{"$f":"+Q47","v":3.76},null,null,null,null,null,null,null,null,null,null,{"$f":"+U22","v":2},{"$f":"+V22*100","v":{"$error":"#VALUE!"}}]
[12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+AB56*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
[13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AB57*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
["  A=",{"$f":"-0.5*((B45*C46-B46*C45)+(B46*C47-B47*C46)+(B47*C48-B48*C47)+(B48*C49-B49*C48)+(B49*C50-B50*C49)+(B50*C51-B51*C50)+(B51*C52-B52*C51)+(B52*C53-B53*C52))","v":2.5691044797107181},"m2",{"$f":"-0.5*((D45*E46-D46*E45)+(D46*E47-D47*E46)+(D47*E48-D48*E47)+(D48*E49-D49*E48)+(D49*E50-D50*E49)+(D50*E51-D51*E50)+(D51*E52-D52*E51)+(D52*E53-D53*E52)+(D53*E54-D54*E53)+(D54*E55-D55*E54)+(D55*E56-D56*E55)+(D56*E57-D57*E56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((F45*G46-F46*G45)+(F46*G47-F47*G46)+(F47*G48-F48*G47)+(F48*G49-F49*G48)+(F49*G50-F50*G49)+(F50*G51-F51*G50)+(F51*G52-F52*G51)+(F52*G53-F53*G52)+(F53*G54-F54*G53)+(F54*G55-F55*G54)+(F55*G56-F56*G55)+(F56*G57-F57*G56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((H47*I48-H48*I47)+(H48*I49-H49*I48)+(H49*I50-H50*I49)+(H50*I51-H51*I50)+(H51*I52-H52*I51)+(H52*I53-H53*I52)+(H53*I54-H54*I53)+(H54*I55-H55*I54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((J47*K48-J48*K47)+(J48*K49-J49*K48)+(J49*K50-J50*K49)+(J50*K51-J51*K50)+(J51*K52-J52*K51)+(J52*K53-J53*K52)+(J53*K54-J54*K53)+(J54*K55-J55*K54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((L47*M48-L48*M47)+(L48*M49-L49*M48)+(L49*M50-L50*M49)+(L50*M51-L51*M50)+(L51*M52-L52*M51)+(L52*M53-L53*M52)+(L53*M54-L54*M53)+(L54*M55-L55*M54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((N47*O48-N48*O47)+(N48*O49-N49*O48)+(N49*O50-N50*O49)+(N50*O51-N51*O50)+(N51*O52-N52*O51)+(N52*O53-N53*O52)+(N53*O54-N54*O53)+(N54*O55-N55*O54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((P47*Q48-P48*Q47)+(P48*Q49-P49*Q48)+(P49*Q50-P50*Q49)+(P50*Q51-P51*Q50)+(P51*Q52-P52*Q51)+(P52*Q53-P53*Q52)+(P53*Q54-P54*Q53)+(P54*Q55-P55*Q54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((R47*S48-R48*S47)+(R48*S49-R49*S48)+(R49*S50-R50*S49)+(R50*S51-R51*S50)+(R51*S52-R52*S51)+(R52*S53-R53*S52)+(R53*S54-R54*S53)+(R54*S55-R55*S54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((T47*U48-T48*U47)+(T48*U49-T49*U48)+(T49*U50-T50*U49)+(T50*U51-T51*U50)+(T51*U52-T52*U51)+(T52*U53-T53*U52)+(T53*U54-T54*U53)+(T54*U55-T55*U54))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((V47*W48-V48*W47)+(V48*W49-V49*W48)+(V49*W50-V50*W49)+(V50*W51-V51*W50))","v":1.5110356654221164},"m2",{"$f":"-0.5*((X47*Y48-X48*Y47)+(X48*Y49-X49*Y48)+(X49*Y50-X50*Y49)+(X50*Y51-X51*Y50))","v":0.71172417455407389},"m2",{"$f":"-0.5*((Z47*AA48-Z48*AA47)+(Z48*AA49-Z49*AA48)+(Z49*AA50-Z50*AA49)+(Z50*AA51-Z51*AA50)+(Z51*AA52-Z52*AA51)+(Z52*AA53-Z53*AA52)+(Z53*AA54-Z54*AA53)+(Z54*AA55-Z55*AA54))","v":0.53224225002380887},"m2",{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-0.5*((AH47*AI48-AH48*AI47)+(AH48*AI49-AH49*AI48)+(AH49*AI50-AH50*AI49)+(AH50*AI51-AH51*AI50)+(AH51*AI52-AH52*AI51)+(AH52*AI53-AH53*AI52)+(AH53*AI54-AH54*AI53)+(AH54*AI55-AH55*AI54))","v":0.21007103011109951},"m2"]
["xt=",{"$f":"-((B45*C46-B46*C45)*(B45+B46)+(B46*C47-B47*C46)*(B46+B47)+(B47*C48-B48*C47)*(B47+B48)+(B48*C49-B49*C48)*(B48+B49)+(B49*C50-B50*C49)*(B49+B50)+(B50*C51-B51*C50)*(B50+B51)+(B51*C52-B52*C51)*(B51+B52)+(B52*C53-B53*C52)*(B52+B53)+(B53*C54-B54*C53)*(B53+B54)+(B54*C55-B55*C54)*(B54+B55)+(B55*C56-B56*C55)*(B55+B56)+(B56*C57-B57*C56)*(B56+B57))/6/B58","v":3.3485779696489133},"m",{"$f":"-((D45*E46-D46*E45)*(D45+D46)+(D46*E47-D47*E46)*(D46+D47)+(D47*E48-D48*E47)*(D47+D48)+(D48*E49-D49*E48)*(D48+D49)+(D49*E50-D50*E49)*(D49+D50)+(D50*E51-D51*E50)*(D50+D51)+(D51*E52-D52*E51)*(D51+D52)+(D52*E53-D53*E52)*(D52+D53)+(D53*E54-D54*E53)*(D53+D54)+(D54*E55-D55*E54)*(D54+D55)+(D55*E56-D56*E55)*(D55+D56)+(D56*E57-D57*E56)*(D56+D57))/6/D58","v":{"$error":"#VALUE!"}},"m",{"$f":"-((F45*G46-F46*G45)*(F45+F46)+(F46*G47-F47*G46)*(F46+F47)+(F47*G48-F48*G47)*(F47+F48)+(F48*G49-F49*G48)*(F48+F49)+(F49*G50-F50*G49)*(F49+F50)+(F50*G51-F51*G50)*(F50+F51)+(F51*G52-F52*G51)*(F51+F52)+(F52*G53-F53*G52)*(F52+F53)+(F53*G54-F54*G53)*(F53+F54)+(F54*G55-F55*G54)*(F54+F55)+(F55*G56-F56*G55)*(F55+F56)+(F56*G57-F57*G56)*(F56+F57))/6/F58","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(H47*I48-H48*I47)*(H47+H48)+(H48*I49-H49*I48)*(H48+H49)+(H49*I50-H50*I49)*(H49+H50)+(H50*I51-H51*I50)*(H50+H51)+(H51*I52-H52*I51)*(H51+H52)+(H52*I53-H53*I52)*(H52+H53)+(H53*I54-H54*I53)*(H53+H54)+(H54*I55-H55*I54)*(H54+H55))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(J47+J48)+(J48*K49-J49*K48)*(J48+J49)+(J49*K50-J50*K49)*(J49+J50)+(J50*K51-J51*K50)*(J50+J51)+(J51*K52-J52*K51)*(J51+J52)+(J52*K53-J53*K52)*(J52+J53)+(J53*K54-J54*K53)*(J53+J54)+(J54*K55-J55*K54)*(J54+J55)+(J55*K56-J56*K55)*(J55+J56)+(J56*K57-J57*K56)*(J56+J57))/6/J58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(L47*M48-L48*M47)*(L47+L48)+(L48*M49-L49*M48)*(L48+L49)+(L49*M50-L50*M49)*(L49+L50)+(L50*M51-L51*M50)*(L50+L51)+(L51*M52-L52*M51)*(L51+L52)+(L52*M53-L53*M52)*(L52+L53)+(L53*M54-L54*M53)*(L53+L54)+(L54*M55-L55*M54)*(L54+L55))/6/L58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(N58=0,0,(+(N47*O48-N48*O47)*(N47+N48)+(N48*O49-N49*O48)*(N48+N49)+(N49*O50-N50*O49)*(N49+N50)+(N50*O51-N51*O50)*(N50+N51)+(N51*O52-N52*O51)*(N51+N52)+(N52*O53-N53*O52)*(N52+N53)+(N53*O54-N54*O53)*(N53+N54)+(N54*O55-N55*O54)*(N54+N55)+(N55*O56-N56*O55)*(N55+N56)+(N56*O57-N57*O56)*(N56+N57))/6/N58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(P47*Q48-P48*Q47)*(P47+P48)+(P48*Q49-P49*Q48)*(P48+P49)+(P49*Q50-P50*Q49)*(P49+P50)+(P50*Q51-P51*Q50)*(P50+P51)+(P51*Q52-P52*Q51)*(P51+P52)+(P52*Q53-P53*Q52)*(P52+P53)+(P53*Q54-P54*Q53)*(P53+P54)+(P54*Q55-P55*Q54)*(P54+P55))/6/P58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(R58=0,0,(+(R47*S48-R48*S47)*(R47+R48)+(R48*S49-R49*S48)*(R48+R49)+(R49*S50-R50*S49)*(R49+R50)+(R50*S51-R51*S50)*(R50+R51)+(R51*S52-R52*S51)*(R51+R52))/6/R58)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(T58=0,0,(+(T47*U48-T48*U47)*(T47+T48)+(T48*U49-T49*U48)*(T48+T49)+(T49*U50-T50*U49)*(T49+T50)+(T50*U51-T51*U50)*(T50+T51)+(T51*U52-T52*U51)*(T51+T52)+(T52*U53-T53*U52)*(T52+T53)+(T53*U54-T54*U53)*(T53+T54)+(T54*U55-T55*U54)*(T54+T55)+(T55*U56-T56*U55)*(T55+T56)+(T56*U57-T57*U56)*(T56+T57))/6/T58)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(V58=0,0,-(+(V47*W48-V48*W47)*(V47+V48)+(V48*W49-V49*W48)*(V48+V49)+(V49*W50-V50*W49)*(V49+V50)+(V50*W51-V51*W50)*(V50+V51))/6/V58)","v":2.6739089419190427},"m",{"$f":"IF(X58=0,0,-(+(X47*Y48-X48*Y47)*(X47+X48)+(X48*Y49-X49*Y48)*(X48+X49)+(X49*Y50-X50*Y49)*(X49+X50)+(X50*Y51-X51*Y50)*(X50+X51))/6/X58)","v":3.7896651910602248},"m",{"$f":"-(+(Z47*AA48-Z48*AA47)*(Z47+Z48)+(Z48*AA49-Z49*AA48)*(Z48+Z49)+(Z49*AA50-Z50*AA49)*(Z49+Z50)+(Z50*AA51-Z51*AA50)*(Z50+Z51)+(Z51*AA52-Z52*AA51)*(Z51+Z52)+(Z52*AA53-Z53*AA52)*(Z52+Z53)+(Z53*AA54-Z54*AA53)*(Z53+Z54)+(Z54*AA55-Z55*AA54)*(Z54+Z55)+(Z55*AA56-Z56*AA55)*(Z55+Z56)+(Z56*AA57-Z57*AA56)*(Z56+Z57))/6/Z58","v":4.5407423692617748},"m",null,null,null,null,"   Koordinate presjeka",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AH47+AH48)+(AH48*AI49-AH49*AI48)*(AH48+AH49)+(AH49*AI50-AH50*AI49)*(AH49+AH50)+(AH50*AI51-AH51*AI50)*(AH50+AH51)+(AH51*AI52-AH52*AI51)*(AH51+AH52)+(AH52*AI53-AH53*AI52)*(AH52+AH53)+(AH53*AI54-AH54*AI53)*(AH53+AH54)+(AH54*AI55-AH55*AI54)*(AH54+AH55)+(AH55*AI56-AH56*AI55)*(AH55+AH56)+(AH56*AI57-AH57*AI56)*(AH56+AH57))/6/AH58","v":4.550001650000004},"m"]
["yt=",{"$f":"-((B45*C46-B46*C45)*(C45+C46)+(B46*C47-B47*C46)*(C46+C47)+(B47*C48-B48*C47)*(C47+C48)+(B48*C49-B49*C48)*(C48+C49)+(B49*C50-B50*C49)*(C49+C50)+(B50*C51-B51*C50)*(C50+C51)+(B51*C52-B52*C51)*(C51+C52)+(B52*C53-B53*C52)*(C52+C53)+(B53*C54-B54*C53)*(C53+C54)+(B54*C55-B55*C54)*(C54+C55)+(B55*C56-B56*C55)*(C55+C56)+(B56*C57-B57*C56)*(C56+C57))/6/B58","v":0.75054981042380386},"m",{"$f":"-((D45*E46-D46*E45)*(E45+E46)+(D46*E47-D47*E46)*(E46+E47)+(D47*E48-D48*E47)*(E47+E48)+(D48*E49-D49*E48)*(E48+E49)+(D49*E50-D50*E49)*(E49+E50)+(D50*E51-D51*E50)*(E50+E51)+(D51*E52-D52*E51)*(E51+E52)+(D52*E53-D53*E52)*(E52+E53)+(D53*E54-D54*E53)*(E53+E54)+(D54*E55-D55*E54)*(E54+E55)+(D55*E56-D56*E55)*(E55+E56)+(D56*E57-D57*E56)*(E56+E57))/6/D58","v":{"$error":"#VALUE!"}},"m",{"$f":"-((F45*G46-F46*G45)*(G45+G46)+(F46*G47-F47*G46)*(G46+G47)+(F47*G48-F48*G47)*(G47+G48)+(F48*G49-F49*G48)*(G48+G49)+(F49*G50-F50*G49)*(G49+G50)+(F50*G51-F51*G50)*(G50+G51)+(F51*G52-F52*G51)*(G51+G52)+(F52*G53-F53*G52)*(G52+G53)+(F53*G54-F54*G53)*(G53+G54)+(F54*G55-F55*G54)*(G54+G55)+(F55*G56-F56*G55)*(G55+G56)+(F56*G57-F57*G56)*(G56+G57))/6/F58","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(H47*I48-H48*I47)*(I47+I48)+(H48*I49-H49*I48)*(I48+I49)+(H49*I50-H50*I49)*(I49+I50)+(H50*I51-H51*I50)*(I50+I51)+(H51*I52-H52*I51)*(I51+I52)+(H52*I53-H53*I52)*(I52+I53)+(H53*I54-H54*I53)*(I53+I54)+(H54*I55-H55*I54)*(I54+I55)+(H55*I56-H56*I55)*(I55+I56)+(H56*I57-H57*I56)*(I56+I57))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(K47+K48)+(J48*K49-J49*K48)*(K48+K49)+(J49*K50-J50*K49)*(K49+K50)+(J50*K51-J51*K50)*(K50+K51)+(J51*K52-J52*K51)*(K51+K52)+(J52*K53-J53*K52)*(K52+K53)+(J53*K54-J54*K53)*(K53+K54)+(J54*K55-J55*K54)*(K54+K55)+(J55*K56-J56*K55)*(K55+K56)+(J56*K57-J57*K56)*(K56+K57))/6/J58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(L47*M48-L48*M47)*(M47+M48)+(L48*M49-L49*M48)*(M48+M49)+(L49*M50-L50*M49)*(M49+M50)+(L50*M51-L51*M50)*(M50+M51)+(L51*M52-L52*M51)*(M51+M52)+(L52*M53-L53*M52)*(M52+M53)+(L53*M54-L54*M53)*(M53+M54)+(L54*M55-L55*M54)*(M54+M55))/6/L58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(N58=0,0,(+(N47*O48-N48*O47)*(O47+O48)+(N48*O49-N49*O48)*(O48+O49)+(N49*O50-N50*O49)*(O49+O50)+(N50*O51-N51*O50)*(O50+O51)+(N51*O52-N52*O51)*(O51+O52)+(N52*O53-N53*O52)*(O52+O53)+(N53*O54-N54*O53)*(O53+O54)+(N54*O55-N55*O54)*(O54+O55)+(N55*O56-N56*O55)*(O55+O56)+(N56*O57-N57*O56)*(O56+O57))/6/N58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(P47*Q48-P48*Q47)*(Q47+Q48)+(P48*Q49-P49*Q48)*(Q48+Q49)+(P49*Q50-P50*Q49)*(Q49+Q50)+(P50*Q51-P51*Q50)*(Q50+Q51)+(P51*Q52-P52*Q51)*(Q51+Q52)+(P52*Q53-P53*Q52)*(Q52+Q53)+(P53*Q54-P54*Q53)*(Q53+Q54)+(P54*Q55-P55*Q54)*(Q54+Q55))/6/P58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(R58=0,0,(+(R47*S48-R48*S47)*(S47+S48)+(R48*S49-R49*S48)*(S48+S49)+(R49*S50-R50*S49)*(S49+S50)+(R50*S51-R51*S50)*(S50+S51)+(R51*S52-R52*S51)*(S51+S52)+(R52*S53-R53*S52)*(S52+S53)+(R53*S54-R54*S53)*(S53+S54)+(R54*S55-R55*S54)*(S54+S55)+(R55*S56-R56*S55)*(S55+S56)+(R56*S57-R57*S56)*(S56+S57))/6/R58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-IF(T58=0,0,(+(T47*U48-T48*U47)*(U47+U48)+(T48*U49-T49*U48)*(U48+U49)+(T49*U50-T50*U49)*(U49+U50)+(T50*U51-T51*U50)*(U50+U51)+(T51*U52-T52*U51)*(U51+U52)+(T52*U53-T53*U52)*(U52+U53)+(T53*U54-T54*U53)*(U53+U54)+(T54*U55-T55*U54)*(U54+U55)+(T55*U56-T56*U55)*(U55+U56)+(T56*U57-T57*U56)*(U56+U57))/6/T58)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((V47*W48-V48*W47)*(W47+W48)+(V48*W49-V49*W48)*(W48+W49)+(V49*W50-V50*W49)*(W49+W50)+(V50*W51-V51*W50)*(W50+W51))/6/V58","v":0.65809555436880718},"kN",{"$f":"-((X47*Y48-X48*Y47)*(Y47+Y48)+(X48*Y49-X49*Y48)*(Y48+Y49)+(X49*Y50-X50*Y49)*(Y49+Y50)+(X50*Y51-X51*Y50)*(Y50+Y51))/6/X58","v":0.75428136494691478},"kN",{"$f":"-(+(Z47*AA48-Z48*AA47)*(AA47+AA48)+(Z48*AA49-Z49*AA48)*(AA48+AA49)+(Z49*AA50-Z50*AA49)*(AA49+AA50)+(Z50*AA51-Z51*AA50)*(AA50+AA51)+(Z51*AA52-Z52*AA51)*(AA51+AA52)+(Z52*AA53-Z53*AA52)*(AA52+AA53)+(Z53*AA54-Z54*AA53)*(AA53+AA54)+(Z54*AA55-Z55*AA54)*(AA54+AA55)+(Z55*AA56-Z56*AA55)*(AA55+AA56)+(Z56*AA57-Z57*AA56)*(AA56+AA57))/6/Z58","v":0.81902934843133712},"m",null,null,null,null,"II-II i I-I",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AI47+AI48)+(AH48*AI49-AH49*AI48)*(AI48+AI49)+(AH49*AI50-AH50*AI49)*(AI49+AI50)+(AH50*AI51-AH51*AI50)*(AI50+AI51)+(AH51*AI52-AH52*AI51)*(AI51+AI52)+(AH52*AI53-AH53*AI52)*(AI52+AI53)+(AH53*AI54-AH54*AI53)*(AI53+AI54)+(AH54*AI55-AH55*AI54)*(AI54+AI55)+(AH55*AI56-AH56*AI55)*(AI55+AI56)+(AH56*AI57-AH57*AI56)*(AI56+AI57))/6/AH58","v":1.3500505000000005},"m"]
["G=",{"$f":"+B58*'Analiza i dimenzioniranje'!E62","v":64.227611992767947},"kN",{"$f":"+D58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"+F58*'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}},"kN",{"$f":"+H58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(J58*'Analiza i dimenzioniranje'!E63<0,0,J58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+L58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(N58*'Analiza i dimenzioniranje'!U41<0,0,N58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+P58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(R58<=0,0,R58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+T58*'Analiza i dimenzioniranje'!E49","v":{"$error":"#VALUE!"}},"kN (za L)",{"$f":"+V58*'Analiza i dimenzioniranje'!E62","v":37.77589163555291},"kN",{"$f":"+X58*'Analiza i dimenzioniranje'!E62","v":17.793104363851846},"kN",{"$f":"+Z58*'Analiza i dimenzioniranje'!E62","v":13.306056250595223},"kN",null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"AC47+'Analiza i dimenzioniranje'!C192/2","v":0.68753317931068247},{"$f":"+AH58*'Analiza i dimenzioniranje'!E62","v":5.2517757527774878},"kN"]
["Vertikala nasipa na konzoli",null,null,"Moment na konzoli",null,"Pokos na vrhu zida",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - NAPONI ",null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+'C XII-XIII'!AC49+('Analiza i dimenzioniranje'!C191/2)","v":0.77418208680245293}]
[null,"x","y",{"$f":"IF('Analiza i dimenzioniranje'!G78=0,0,'Analiza i dimenzioniranje'!G78*'Analiza i dimenzioniranje'!C77*'Analiza i dimenzioniranje'!E62*(Q20-B5+'Analiza i dimenzioniranje'!G78/2)+J61*(O16-J59))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"+F64","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"naponi za presjek II-II",null,"naponi za srednji dio ",null,"naponi za presjek I-I"]
[null,{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},"b1=",{"$f":"+H47-2","v":1.4000010999999999},{"$f":"+B52","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y","x","y","x","y","Koordinate dna temelja"]
[null,{"$f":"+B64","v":{"$error":"#VALUE!"}},{"$f":"IF(B65>J49,C19,+C20+'Analiza i dimenzioniranje'!F20+(H52-H50)*TAN('Analiza i dimenzioniranje'!F21*PI()/180))","v":{"$error":"#VALUE!"}},"b2=",{"$f":"'Analiza i dimenzioniranje'!E54+('Analiza i dimenzioniranje'!E55-'Analiza i dimenzioniranje'!E54)*(('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)/(C9-C4))","v":{"$error":"#VALUE!"}},{"$f":"+B65","v":{"$error":"#VALUE!"}},{"$f":"+G64+(F64-F65)*TAN('Analiza i dimenzioniranje'!F21*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,0,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},0,{"$f":"+'C XII-XIII'!B11","v":4.2000010999999997},{"$f":"-U47","v":0},2,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z65","v":2},{"$f":"AC55","v":{"$error":"#VALUE!"}},{"$f":"+AB65","v":3.4000010999999999},{"$f":"+AA67","v":{"$error":"#VALUE!"}},{"$f":"+AB57","v":4.2000010999999997},{"$f":"AC57","v":{"$error":"#VALUE!"}},{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"(AF66*(AG70-AG65)/(AF70-AF65)-AF65*(AG70-AG65)/(AF70-AF65)+AG65)","v":{"$error":"#VALUE!"}}]
[null,"AKTIVNI TLAKOVI za stabilnost i Presjek III-III (bez E3)",null,null,null,null,null,null,"  AKTIVNI TLAKOVI za presjek kroz zid XII-XII",null,null,null,null,"    AKTIVNI TLAKOVI za presjek kroz zid XIII-XIII",null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"AC56","v":{"$error":"#VALUE!"}},{"$f":"+AB66+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AE66","v":{"$error":"#VALUE!"}},{"$f":"+AB58","v":4.9000021999999994},{"$f":"+AC58","v":{"$error":"#VALUE!"}},{"$f":"+AB77","v":{"$error":"#VALUE!"}},{"$f":"+(AF67*(AG65-AG70)/(AF65-AF70)-AF70*(AG65-AG70)/(AF65-AF70)+AG70)","v":{"$error":"#VALUE!"}}]
[null,"E1",null,"E2",null,"E3",null,null,"E1",null,"E2 do presjeka kroz zid II",null,null,"E1",null,"E2",null,null,null,null,null,null,null,null,null,{"$f":"+Z67","v":3.4000010999999999},0,{"$f":"+AB67","v":4.2000010999999997},0,{"$f":"+AD67","v":4.9000021999999994},{"$f":"+U50","v":0},{"$f":"+AB67","v":4.2000010999999997},{"$f":"+(AF68*(AG65-AG70)/(AF65-AF70)-AF70*(AG65-AG70)/(AF65-AF70)+AG70)","v":0.37931024673015767}]
[null,0,{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C71","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,{"$f":"+N69","v":0},{"$f":"+O69","v":{"$error":"#VALUE!"}},{"$f":"+I71","v":{"$error":"#VALUE!"}},{"$f":"+J71","v":{"$error":"#VALUE!"}},null,{"$f":"+B69","v":0},{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+N71","v":{"$error":"#VALUE!"}},{"$f":"+O71","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"+Z65","v":2},0,{"$f":"+AB65","v":3.4000010999999999},0,{"$f":"+AD65","v":4.2000010999999997},{"$f":"+U51","v":0},{"$f":"+AD77","v":{"$error":"#VALUE!"}},{"$f":"+(AF69*(AG66-AG70)/(AF66-AF70)-AF70*(AG66-AG70)/(AF66-AF70)+AG70)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+B69","v":0},{"$f":"+C69-'Analiza i dimenzioniranje'!D17-'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+D69+'Analiza i dimenzioniranje'!E16*'Analiza i dimenzioniranje'!E17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+E69-'Analiza i dimenzioniranje'!E17","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},null,{"$f":"+N70","v":0},{"$f":"+J69-('Analiza i dimenzioniranje'!F20+'P XII-XII'!E17)","v":{"$error":"#VALUE!"}},{"$f":"+K69+'P XII-XII'!F16*'P XII-XII'!F17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},null,{"$f":"+B70","v":0},{"$f":"+O69-('Analiza i dimenzioniranje'!F20+'P XIII-XIII'!E17)","v":{"$error":"#VALUE!"}},{"$f":"+P69+'P XIII-XIII'!F16*'P XIII-XIII'!F17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AB53","v":4.9000021999999994},{"$f":"+AC53","v":0.5}]
[null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('Analiza i dimenzioniranje'!D17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},0,{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F70+'Analiza i dimenzioniranje'!F16*'Analiza i dimenzioniranje'!F17*'Analiza i dimenzioniranje'!F112","v":{"$error":"#VALUE!"}},0,null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('P XII-XII'!E17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+J70","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+L70","v":3.44},null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('P XIII-XIII'!E17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+Q70","v":3.76}]
[null,{"$f":"+B69","v":0},{"$f":"+C69","v":{"$error":"#VALUE!"}},0,{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F69","v":0},0,null,{"$f":"+N72","v":0},{"$f":"+O72","v":{"$error":"#VALUE!"}},{"$f":"+D72","v":0},{"$f":"+L69","v":{"$error":"#VALUE!"}},null,{"$f":"+N69","v":0},{"$f":"+O69","v":{"$error":"#VALUE!"}},{"$f":"+D72","v":0},{"$f":"+Q69","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+D69","v":{"$error":"#VALUE!"}},{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F72","v":0},{"$f":"+G70","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+K69","v":{"$error":"#VALUE!"}},{"$f":"+L69","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+P69","v":{"$error":"#VALUE!"}},{"$f":"+Q69","v":{"$error":"#VALUE!"}}]
["Jednadžba vertikale kohezije    Određivanje sjecišta kohezije s pravcem od tlaka",null,null,null,null,null,null,{"$f":"+M74","v":"Jednadžba vertikale kohezije  -  sjecišta kohezije s pravcem od tlaka"},null,null,null,null,"Jednadžba vertikale kohezije  -  sjecišta kohezije s pravcem od tlaka"]
[null,"X","y","X","y","X","y",null,{"$f":"+N75","v":"X"},{"$f":"+O75","v":"y"},"X","y",null,"X","y","X","y"]
[null,{"$f":"2*'Analiza i dimenzioniranje'!D15/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F110)","v":12.361875887090893},{"$f":"B76*(C71-C72)/(B71-B72)-B72*(C71-C72)/(B71-B72)+C72","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!F12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F111)","v":{"$error":"#VALUE!"}},{"$f":"IF(D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69>'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69)","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!C12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F112)","v":{"$error":"#VALUE!"}},{"$f":"IF((F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70)>'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!F17,(F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70))","v":{"$error":"#VALUE!"}},null,{"$f":"+N76","v":12.361875887090893},{"$f":"I76*(J71-J72)/(I71-I72)-I72*(J71-J72)/(I71-I72)+J72","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},null,{"$f":"+B76","v":12.361875887090893},{"$f":"N76*(O71-O72)/(N71-N72)-N72*(O71-O72)/(N71-N72)+O72","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"-0.5*((Z65*AA66-Z66*AA65)+(Z66*AA67-Z67*AA66)+(Z67*AA68-Z68*AA67)+(Z68*AA69-Z69*AA68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((AB65*AC66-AB66*AC65)+(AB66*AC67-AB67*AC66)+(AB67*AC68-AB68*AC67)+(AB68*AC69-AB69*AC68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((AD65*AE66-AD66*AE65)+(AD66*AE67-AD67*AE66)+(AD67*AE68-AD68*AE67)+(AD68*AE69-AD69*AE68)+(AD69*AE70-AD70*AE69)+(AD70*AE71-AD71*AE70)+(AD71*AE72-AD72*AE71)+(AD72*AE73-AD73*AE72))","v":{"$error":"#VALUE!"}},"kN/m'"]
[null,{"$f":"+B76","v":12.361875887090893},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},null,{"$f":"+N77","v":12.361875887090893},{"$f":"+O77","v":{"$error":"#VALUE!"}},{"$f":"+K76","v":{"$error":"#VALUE!"}},{"$f":"+L70","v":3.44},null,{"$f":"+N76","v":12.361875887090893},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+P76","v":{"$error":"#VALUE!"}},{"$f":"+G122","v":3.76},null,null,null,null,null,null,null,null,{"$f":"IF(Z76=0,0,-(+(Z65*AA66-Z66*AA65)*(Z65+Z66)+(Z66*AA67-Z67*AA66)*(Z66+Z67)+(Z67*AA68-Z68*AA67)*(Z67+Z68)+(Z68*AA69-Z69*AA68)*(Z68+Z69))/6/Z76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(AB76=0,0,-(+(AB65*AC66-AB66*AC65)*(AB65+AB66)+(AB66*AC67-AB67*AC66)*(AB66+AB67)+(AB67*AC68-AB68*AC67)*(AB67+AB68)+(AB68*AC69-AB69*AC68)*(AB68+AB69))/6/AB76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(AD76=0,0,-(+(AD65*AE66-AD66*AE65)*(AD65+AD66)+(AD66*AE67-AD67*AE66)*(AD66+AD67)+(AD67*AE68-AD68*AE67)*(AD67+AD68)+(AD68*AE69-AD69*AE68)*(AD68+AD69))/6/AD76)","v":{"$error":"#VALUE!"}},"m"]
["Oznaka","E1",null,"E2",null,"E3",null,{"$f":"+M78","v":"Oznaka"},{"$f":"+N78","v":"E1"},null,"E2",null,"Oznaka","E1",null,"E2",null,null,null,null,null,null,null,null,null,{"$f":"-((Z65*AA66-Z66*AA65)*(AA65+AA66)+(Z66*AA67-Z67*AA66)*(AA66+AA67)+(Z67*AA68-Z68*AA67)*(AA67+AA68)+(Z68*AA69-Z69*AA68)*(AA68+AA69))/6/Z76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((AB65*AC66-AB66*AC65)*(AC65+AC66)+(AB66*AC67-AB67*AC66)*(AC66+AC67)+(AB67*AC68-AB68*AC67)*(AC67+AC68)+(AB68*AC69-AB69*AC68)*(AC68+AC69))/6/AB76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((AD65*AE66-AD66*AE65)*(AE65+AE66)+(AD66*AE67-AD67*AE66)*(AE66+AE67)+(AD67*AE68-AD68*AE67)*(AE67+AE68)+(AD68*AE69-AD69*AE68)*(AE68+AE69))/6/AD76","v":{"$error":"#VALUE!"}},"kN/m'"]
["točke","x","y","x","y","x","y","točke",{"$f":"+N79","v":"x"},{"$f":"+O79","v":"y"},"x","y","točke","x","y","x","y"]
[1,{"$f":"+B77","v":12.361875887090893},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,1,{"$f":"+N80","v":12.361875887090893},{"$f":"+J76","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17<'Analiza i dimenzioniranje'!Z44,0,K77)","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},1,12.361875887090893,{"$f":"+O77","v":{"$error":"#VALUE!"}},{"$f":"+K80","v":{"$error":"#VALUE!"}},{"$f":"+Q76","v":{"$error":"#VALUE!"}},null,"Jedn pravca zida uz tlo",null,"Jedn pravca arm dno ",null,"Y=",{"$f":"IF(S82=S81,1000000,(T82-T81)/(S82-S81))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X80*S81+T81","v":{"$error":"#VALUE!"}}]
[2,{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G76","v":{"$error":"#VALUE!"}},2,{"$f":"+I71","v":{"$error":"#VALUE!"}},{"$f":"+J71","v":{"$error":"#VALUE!"}},{"$f":"IF(E76<E73,D76,I81)","v":{"$error":"#VALUE!"}},{"$f":"+L76","v":{"$error":"#VALUE!"}},2,{"$f":"+N71","v":{"$error":"#VALUE!"}},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+K81","v":{"$error":"#VALUE!"}},{"$f":"+Q80","v":{"$error":"#VALUE!"}},null,{"$f":"+B4","v":3.4000010999999999},{"$f":"+C4","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!T593","v":2.0499999999999998},{"$f":"+'Analiza i dimenzioniranje'!U593","v":0.18682583433163008},"X=",{"$f":"+(-Z80+Z83)/(X80-X83)","v":{"$error":"#VALUE!"}},"sjeište"]
[3,{"$f":"+B80","v":12.361875887090893},{"$f":"+C76","v":{"$error":"#VALUE!"}},{"$f":"IF(D76>D69,D81,D69)","v":{"$error":"#VALUE!"}},{"$f":"+E81","v":{"$error":"#VALUE!"}},{"$f":"IF(F77>F70,F77,F70)","v":{"$error":"#VALUE!"}},{"$f":"IF(F77>F70,G76,G70)","v":{"$error":"#VALUE!"}},3,{"$f":"+N82","v":12.361875887090893},{"$f":"+J81","v":{"$error":"#VALUE!"}},{"$f":"+K70","v":{"$error":"#VALUE!"}},{"$f":"+L70","v":3.44},3,{"$f":"+N80","v":12.361875887090893},{"$f":"+O76","v":{"$error":"#VALUE!"}},{"$f":"+P70","v":{"$error":"#VALUE!"}},{"$f":"+Q70","v":3.76},null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},{"$f":"+'Analiza i dimenzioniranje'!T594","v":4.8600021999999994},{"$f":"+'Analiza i dimenzioniranje'!U594","v":0.54310345350772504},"Y=",{"$f":"+X80*X81+Z80","v":{"$error":"#VALUE!"}}]
[4,{"$f":"+B80","v":12.361875887090893},{"$f":"+C80","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F71","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},4,{"$f":"+N83","v":12.361875887090893},{"$f":"+J80","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17<'Analiza i dimenzioniranje'!Z44,0,K76)","v":{"$error":"#VALUE!"}},{"$f":"+L77","v":3.44},4,{"$f":"+N80","v":12.361875887090893},{"$f":"+O80","v":{"$error":"#VALUE!"}},{"$f":"+P80","v":{"$error":"#VALUE!"}},{"$f":"+Q82","v":3.76},null,null,null,null,null,"Y=",{"$f":"+(V82-V81)/(U82-U81)","v":0.12678908905341604},"*x",{"$f":"-X83*U81+V81","v":-7.3091798227872762E-2},"CRTANJE"]
[5,null,null,{"$f":"+D80","v":{"$error":"#VALUE!"}},{"$f":"+E80","v":{"$error":"#VALUE!"}},{"$f":"+F80","v":{"$error":"#VALUE!"}},{"$f":"+G80","v":0},5,null,null,{"$f":"+K80","v":{"$error":"#VALUE!"}},{"$f":"+L80","v":{"$error":"#VALUE!"}},5,null,null,{"$f":"+P80","v":{"$error":"#VALUE!"}},{"$f":"+Q80","v":{"$error":"#VALUE!"}},null,"Jedn pravca sloja 3",null,"Jedn pravca sloja 3 klizno",null,"Y=",{"$f":"+(T86-T85)/(S86-S85)","v":-3.4920769491747737E-2},"*x",{"$f":"-X84*S85+T85","v":1.2698415389834954},"Jedn pravca sloja 3 klizno",null,"sjecište 1/2 sidra sa vrhom 1. sloja"]
["  A=",{"$f":"IF(B77>B71,0,-IF(B84>B83,0,-0.5*((B80*C81-B81*C80)+(B81*C82-B82*C81)+(B82*C83-B83*C82)+(B83*C84-B84*C83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D77>D70,0,IF(D84>D83,0,-0.5*((D80*E81-D81*E80)+(D81*E82-D82*E81)+(D82*E83-D83*E82)+(D83*E84-D84*E83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F77>F71,0,IF(F84>F83,0,-0.5*((F80*G81-F81*G80)+(F81*G82-F82*G81)+(F82*G83-F83*G82)+(F83*G84-F84*G83))))","v":{"$error":"#VALUE!"}},"kN/m'","  A=",{"$f":"IF(I77>I71,0,IF(I84>I83,0,-0.5*((I80*J81-I81*J80)+(I81*J82-I82*J81)+(I82*J83-I83*J82)+(I83*J84-I84*J83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-IF(L77>L76,0,-IF(K84>K83,0,-0.5*((K80*L81-K81*L80)+(K81*L82-K82*L81)+(K82*L83-K83*L82)+(K83*L84-K84*L83))))","v":{"$error":"#VALUE!"}},"kN/m'","  A=",{"$f":"IF(O77>O76,0,0.5*((N80*O81-N81*O80)+(N81*O82-N82*O81)+(N82*O83-N83*O82)+(N83*O84-N84*O83)))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(Q77>Q76,0,-0.5*((P80*Q81-P81*Q80)+(P81*Q82-P82*Q81)+(P82*Q83-P83*Q82)+(P83*Q84-P84*Q83)))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+U18","v":2},{"$f":"+V18","v":1.2},{"$f":"+W100","v":2},0,"X=",{"$f":"+(-Z84+Z87)/(X84-X87)","v":1.1386903959986558},"sjecište ",null,{"$f":"+U85","v":2},{"$f":"+V85","v":0},"Y=",{"$f":"+X92","v":{"$error":"#VALUE!"}},"*x",{"$f":"+Z92","v":{"$error":"#VALUE!"}}]
["xt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(B80+B81)+(B81*C82-B82*C81)*(B81+B82)+(B82*C83-B83*C82)*(B82+B83)+(B83*C84-B84*C83)*(B83+B84))/6/B85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(D80+D81)+(D81*E82-D82*E81)*(D81+D82)+(D82*E83-D83*E82)*(D82+D83)+(D83*E84-D84*E83)*(D83+D84))/6/D85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(F80+F81)+(F81*G82-F82*G81)*(F81+F82)+(F82*G83-F83*G82)*(F82+F83)+(F83*G84-F84*G83)*(F83+F84))/6/F85)","v":{"$error":"#VALUE!"}},"kN/m'","xt=",{"$f":"IF(I85=0,0,-+((I80*J81-I81*J80)*(I80+I81)+(I81*J82-I82*J81)*(I81+I82)+(I82*J83-I83*J82)*(I82+I83)+(I83*J84-I84*J83)*(I83+I84))/6/I85)","v":{"$error":"#VALUE!"}},{"$f":"+O86","v":"kN/m'"},{"$f":"-IF(K85=0,0,-((K80*L83-K83*L80)*(K80+K83)+(K83*L82-K82*L83)*(K83+K82)+(K82*L81-K81*L82)*(K82+K81)+(K81*L84-K84*L81)*(K81+K84))/6/K85)","v":{"$error":"#VALUE!"}},"kN/m'","xt=",{"$f":"IF(N85=0,0,((N80*O81-N81*O80)*(N80+N81)+(N81*O82-N82*O81)*(N81+N82)+(N82*O83-N83*O82)*(N82+N83)+(N83*O84-N84*O83)*(N83+N84))/6/N85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(P85=0,0,+((P80*Q83-P83*Q80)*(P80+P83)+(P83*Q82-P82*Q83)*(P83+P82)+(P82*Q81-P81*Q82)*(P82+P81)+(P81*Q84-P84*Q81)*(P81+P84))/6/P85)","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+U19","v":-8},{"$f":"+V19","v":1.5492076949174773},-5,{"$f":"+V85+(U85-U86)*TAN((45+'Analiza i dimenzioniranje'!F14/2)*PI()/180)","v":9.9970360471948005},"Y=",{"$f":"+X84*X85+Z84","v":1.2300775941423594},3,null,{"$f":"+X85","v":1.1386903959986558},{"$f":"+X86","v":1.2300775941423594}]
["yt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(C80+C81)+(B81*C82-B82*C81)*(C81+C82)+(B82*C83-B83*C82)*(C82+C83)+(B83*C84-B84*C83)*(C83+C84))/6/B85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(E80+E81)+(D81*E82-D82*E81)*(E81+E82)+(D82*E83-D83*E82)*(E82+E83)+(D83*E84-D84*E83)*(E83+E84))/6/D85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(G80+G81)+(F81*G82-F82*G81)*(G81+G82)+(F82*G83-F83*G82)*(G82+G83)+(F83*G84-F84*G83)*(G83+G84))/6/F85)","v":{"$error":"#VALUE!"}},"m","yt=",{"$f":"IF(I85=0,0,-((I80*J81-I81*J80)*(J80+J81)+(I81*J82-I82*J81)*(J81+J82)+(I82*J83-I83*J82)*(J82+J83)+(I83*J84-I84*J83)*(J83+J84))/6/I85)","v":{"$error":"#VALUE!"}},{"$f":"+O87","v":"m"},{"$f":"-IF(K85=0,0,-((K80*L83-K83*L80)*(L80+L83)+(K83*L82-K82*L83)*(L83+L82)+(K82*L81-K81*L82)*(L82+L81)+(K81*L84-K84*L81)*(L81+L84))/6/K85)","v":{"$error":"#VALUE!"}},"m","yt=",{"$f":"IF(N85=0,0,((N80*O81-N81*O80)*(O80+O81)+(N81*O82-N82*O81)*(O81+O82)+(N82*O83-N83*O82)*(O82+O83)+(N83*O84-N84*O83)*(O83+O84))/6/N85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(P85=0,0,((P80*Q83-P83*Q80)*(Q80+Q83)+(P83*Q82-P82*Q83)*(Q83+Q82)+(P82*Q81-P81*Q82)*(Q82+Q81)+(P81*Q84-P84*Q81)*(Q81+Q84))/6/P85)","v":{"$error":"#VALUE!"}},"m",null,null,null,null,null,"Y=",{"$f":"+(V86-V85)/(U86-U85)","v":-1.4281480067421144},"*x",{"$f":"-X87*U85+V85","v":2.8562960134842288},"y=2       x=",{"$f":"+('Analiza i dimenzioniranje'!E52-'C XII-XIII'!Z87)/'C XII-XIII'!X87","v":1.1597509541483482}]
[null,null,null,null,null,null,null,null,{"$f":"+I85","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(K85<0,0,K85)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+N85","v":{"$error":"#VALUE!"}},null,{"$f":"+IF(P85<0,0,P85)","v":{"$error":"#VALUE!"}},null,null,"Jedn pravca sloja 2",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(T90-T89)/(S90-S89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X88*S89+T89","v":{"$error":"#VALUE!"}},"Jedn pravca sloja 2 klizno",null,"Jednadžba pravca sidra",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(AD90-AD89)/(AC90-AC89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AH88*AC89+AD89","v":{"$error":"#VALUE!"}}]
["X koordinata položaja rezultante aktivnog tlaka na stražnjoj strani zida za  Ev1, Ev2 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U15","v":{"$error":"#VALUE!"}},{"$f":"+V15","v":4},{"$f":"+X85","v":1.1386903959986558},{"$f":"+X86","v":1.2300775941423594},"X=",{"$f":"+(-Z88+Z91)/(X88-X91)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U89","v":1.1386903959986558},{"$f":"+V89","v":1.2300775941423594},{"$f":"+U37","v":{"$error":"#VALUE!"}},{"$f":"+V37","v":5},{"$f":"+U89","v":1.1386903959986558},{"$f":"+V89","v":1.2300775941423594},"X=",{"$f":"+(-AJ88+AJ91)/(AH88-AH91)","v":{"$error":"#VALUE!"}},"sjecište"]
["Jednadžba pravca zida uz tlo",null,null,null,null,"Za Ev3 x=2",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U16","v":-8},{"$f":"+V16","v":{"$error":"#VALUE!"}},-5,{"$f":"+V89+(U89-U90)*TAN((45+'Analiza i dimenzioniranje'!E14/2)*PI()/180)","v":9.6792600705649363},"Y=",{"$f":"+X88*X89+Z88","v":{"$error":"#VALUE!"}},2,null,{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},{"$f":"+U38","v":{"$error":"#VALUE!"}},{"$f":"+V38","v":{"$error":"#VALUE!"}},{"$f":"+U90","v":-5},{"$f":"+V90","v":9.6792600705649363},"Y=",{"$f":"+AH88*AH89+AJ88","v":{"$error":"#VALUE!"}},2]
[null,"E1",null,"E2",null,"E3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(V90-V89)/(U90-U89)","v":-1.3763819204711731},"*x",{"$f":"-X91*U89+V89","v":2.79735046820907},null,null,null,null,null,null,"Y=",{"$f":"+(AF90-AF89)/(AE90-AE89)","v":-1.3763819204711731},"*x",{"$f":"-AH91*AE89+AF89","v":2.79735046820907}]
["x","y","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,"Jedn pravca sloja 1",null,null,null,"Y=",{"$f":"+(T95-T94)/(S95-S94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X92*S94+T94","v":{"$error":"#VALUE!"}},"Jedan pravca sloja 1 klizno",null,"Slobodna dionica ls>=",{"$f":"+SQRT((AC94-AC93)*(AC94-AC93)+(AD94-AD93)*(AD94-AD93))","v":{"$error":"#VALUE!"}}]
[{"$f":"+(B8-B4)*(B93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+B87","v":{"$error":"#VALUE!"}},{"$f":"+(B8-B4)*(D93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+D87","v":{"$error":"#VALUE!"}},2,{"$f":"+F87","v":{"$error":"#VALUE!"}},null,{"$f":"+(B8-B4)*(I93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+N87","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+(B8-B4)*(N93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+I87","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+V7","v":"A"},null,null,"X=",{"$f":"+(-Z92+Z95)/(X92-X95)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U94","v":{"$error":"#VALUE!"}},{"$f":"+V94","v":{"$error":"#VALUE!"}},{"$f":"+AC89","v":{"$error":"#VALUE!"}},{"$f":"+AD89","v":5}]
[null,null,null,null,"Sloj2",{"$f":"+(B8-B4)*(G94-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!V15","v":4},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U8","v":{"$error":"#VALUE!"}},{"$f":"+V8","v":6},{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+X92*X93+Z92","v":{"$error":"#VALUE!"}},1,null,{"$f":"+X93","v":{"$error":"#VALUE!"}},{"$f":"+X94","v":{"$error":"#VALUE!"}},{"$f":"+AH89","v":{"$error":"#VALUE!"}},{"$f":"+AH90","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+(B8-B4)*(G95-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+K21","v":1.2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782},-5,{"$f":"+V94+(U94-U95)*TAN((45+'Analiza i dimenzioniranje'!D14/2)*PI()/180)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+(V95-V94)/(U95-U94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X95*U94+V94","v":{"$error":"#VALUE!"}},{"$f":"+(AB95-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(AB96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},{"$f":"+(AD96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Masa unutar kliznog tijela - za potres",null,"POTRES",null,"x","y","x","y","x","y",null,null,null,null,"Masa za potres s prosjekom kontrafore i bez kontrafora"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+(B9-B4)*(AD98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},{"$f":"+(B9-B4)*(AF98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B2","v":2},0.12820515121628623,null,null,{"$f":"+(Z95-AB99)/(-X91)","v":{"$error":"#VALUE!"}},{"$f":"+AB98","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!AB44>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'C XII-XIII'!AC96,(Z91-AD99)/(-X91))","v":-0.46691221544884393},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},{"$f":"IF('Analiza i dimenzioniranje'!AC44>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'C XII-XIII'!AA96,(Z91-AF99)/(-X91))","v":-0.69940582441055943},{"$f":"+AF98","v":3.76}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,1.2,"Potresna sila za stabilnost",null,"Klizno tijelo za potres za presjek III-III",null,"Klizno tijelo za potres za presjek XII-XII",null,"Klizno tijelo za potres za presjek  XIII-XIII",null,null,null,null,null,"Potresna sila za stabilnost "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.4000010999999999,1.2,{"$f":"+'C X-XI'!Y101","v":1.75},{"$f":"+'C X-XI'!Z101","v":9.6153895463470418E-2},null,null,{"$f":"+AC98","v":{"$error":"#VALUE!"}},{"$f":"+AD96","v":3.44},{"$f":"+AE98","v":{"$error":"#VALUE!"}},{"$f":"+AF98","v":3.76},null,null,null,null,{"$f":"+'C III-V'!Y101","v":1.75},{"$f":"+'C III-V'!Z101","v":9.6153895463470418E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.14,{"$f":"+'C X-XI'!Y102","v":0.97707863658009864},{"$f":"+'C X-XI'!Z102","v":1.2},{"$f":"+Y102","v":0.97707863658009864},1.2,{"$f":"+AN126","v":-0.66422677997802415},{"$f":"+AO126","v":3.44},{"$f":"+AN127","v":-0.88880601532481696},{"$f":"+AO127","v":3.76},null,null,null,null,{"$f":"+'C III-V'!Y102","v":0.97707863658009864},{"$f":"+'C III-V'!Z102","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.14,{"$f":"+'C X-XI'!Y103","v":-1.0572404418349119},{"$f":"+'C X-XI'!Z103","v":4},{"$f":"+Y103","v":-1.0572404418349119},{"$f":"+Z103","v":4},{"$f":"IF(AD103=AD102,AC102,+AA103)","v":-1.0572404418349119},{"$f":"IF($AH$105<=AD102,AD102,$AH$105)","v":4},{"$f":"IF(AF103=AF102,AE102,+AC103)","v":-1.0572404418349119},{"$f":"IF($AH$105<=AF102,AF102,$AH$105)","v":4},null,null,null,null,{"$f":"+'C III-V'!Y103","v":-1.0572404418349119},{"$f":"+'C III-V'!Z103","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.44,{"$f":"+'C X-XI'!Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!Z104","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+'C III-V'!Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z104","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.44,{"$f":"+'C X-XI'!Y105","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!Z105","v":6.2644906473896782},{"$error":"#VALUE!"},6.2644906473896782,{"$f":"+AA105","v":{"$error":"#VALUE!"}},{"$f":"IF(AA105=AC105,AB105,AB95)","v":{"$error":"#VALUE!"}},{"$f":"+AA105","v":{"$error":"#VALUE!"}},{"$f":"+IF(AA105=AE105,AB105,AB95)","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!AG105","v":" H="},{"$f":"+'C XIV-XV'!AH105","v":4},null,null,{"$f":"+'C III-V'!Y105","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z105","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},"A",{"$f":"+'C X-XI'!Y106","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!Z106","v":6},{"$error":"#VALUE!"},6,{"$f":"+AE106","v":{"$error":"#VALUE!"}},{"$f":"+AF106","v":6},{"$f":"+AA106","v":{"$error":"#VALUE!"}},{"$f":"+AB106","v":6},null,null,null,null,{"$f":"+'C III-V'!Y106","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z106","v":6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},"A",{"$f":"+'C X-XI'!Y107","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!Z107","v":6},{"$error":"#VALUE!"},6,{"$f":"+AE107","v":{"$error":"#VALUE!"}},{"$f":"+AF107","v":6},{"$f":"+AA107","v":{"$error":"#VALUE!"}},{"$f":"+AB107","v":6},null,null,null,null,{"$f":"+'C III-V'!Y107","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z107","v":6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+W107","v":{"$error":"#VALUE!"}},{"$f":"+X107","v":"A"},{"$f":"+'C X-XI'!Y108","v":3.4000000999999997},{"$f":"+'C X-XI'!Z108","v":1.2},3.4000000999999997,1.2,{"$f":"+AC109","v":{"$error":"#VALUE!"}},{"$f":"+AD109","v":3.44},{"$f":"+AE109","v":{"$error":"#VALUE!"}},{"$f":"+AF109","v":3.76},null,null,null,null,{"$f":"+'C III-V'!Y108","v":3.4000000999999997},{"$f":"+'C III-V'!Z108","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B11","v":4.2000010999999997},1.2,{"$f":"+'C X-XI'!Y109","v":1.75},{"$f":"+'C X-XI'!Z109","v":1.2},{"$f":"+AA102","v":0.97707863658009864},{"$f":"+AB102","v":1.2},{"$f":"+AC98","v":{"$error":"#VALUE!"}},{"$f":"+AD101","v":3.44},{"$f":"+AE101","v":{"$error":"#VALUE!"}},{"$f":"+AF101","v":3.76},null,null,null,null,{"$f":"+'C III-V'!Y109","v":1.75},{"$f":"+'C III-V'!Z109","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2000010999999997,1.2,{"$f":"+'C X-XI'!Y110","v":1.75},{"$f":"+'C X-XI'!Z110","v":9.6153895463470418E-2},null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!Y110","v":1.75},{"$f":"+'C III-V'!Z110","v":9.6153895463470418E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2000010999999997,1.2,{"$f":"-0.5*((Y101*Z102-Y102*Z101)+(Y102*Z103-Y103*Z102)+(Y103*Z104-Y104*Z103)+(Y104*Z105-Y105*Z104)+(Y105*Z106-Y106*Z105)+(Y106*Z107-Y107*Z106)+(Y107*Z108-Y108*Z107)+(Y108*Z109-Y109*Z108)+(Y109*Z110-Y110*Z109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AA101*AB102-AA102*AB101)+(AA102*AB103-AA103*AB102)+(AA103*AB104-AA104*AB103)+(AA104*AB105-AA105*AB104)+(AA105*AB106-AA106*AB105)+(AA106*AB107-AA107*AB106)+(AA107*AB108-AA108*AB107)+(AA108*AB109-AA109*AB108)+(AA109*AB110-AA110*AB109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AC101*AD102-AC102*AD101)+(AC102*AD103-AC103*AD102)+(AC103*AD104-AC104*AD103)+(AC104*AD105-AC105*AD104)+(AC105*AD106-AC106*AD105)+(AC106*AD107-AC107*AD106)+(AC107*AD108-AC108*AD107)+(AC108*AD109-AC109*AD108)+(AC109*AD110-AC110*AD109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AE101*AF102-AE102*AF101)+(AE102*AF103-AE103*AF102)+(AE103*AF104-AE104*AF103)+(AE104*AF105-AE105*AF104)+(AE105*AF106-AE106*AF105)+(AE106*AF107-AE107*AF106)+(AE107*AF108-AE108*AF107)+(AE108*AF109-AE109*AF108)+(AE109*AF110-AE110*AF109))","v":{"$error":"#VALUE!"}},"m2",null,null,null,null,{"$f":"-0.5*((AK101*AL102-AK102*AL101)+(AK102*AL103-AK103*AL102)+(AK103*AL104-AK104*AL103)+(AK104*AL105-AK105*AL104)+(AK105*AL106-AK106*AL105)+(AK106*AL107-AK107*AL106)+(AK107*AL108-AK108*AL107)+(AK108*AL109-AK109*AL108)+(AK109*AL110-AK110*AL109))","v":{"$error":"#VALUE!"}},"m2","OK","prosječna površina temelja od temelja kontrafore duž čitavog zida"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.9000021999999994,1.2,{"$f":"-((Y101*Z102-Y102*Z101)*(Y101+Y102)+(Y102*Z103-Y103*Z102)*(Y102+Y103)+(Y103*Z104-Y104*Z103)*(Y103+Y104)+(Y104*Z105-Y105*Z104)*(Y104+Y105)+(Y105*Z106-Y106*Z105)*(Y105+Y106)+(Y106*Z107-Y107*Z106)*(Y106+Y107)+(Y107*Z108-Y108*Z107)*(Y107+Y108)+(Y108*Z109-Y109*Z108)*(Y108+Y109)+(Y109*Z110-Y110*Z109)*(Y109+Y110))/6/Y111","v":{"$error":"#VALUE!"}},"m  ",{"$f":"-((AA101*AB102-AA102*AB101)*(AA101+AA102)+(AA102*AB103-AA103*AB102)*(AA102+AA103)+(AA103*AB104-AA104*AB103)*(AA103+AA104)+(AA104*AB105-AA105*AB104)*(AA104+AA105)+(AA105*AB106-AA106*AB105)*(AA105+AA106)+(AA106*AB107-AA107*AB106)*(AA106+AA107)+(AA107*AB108-AA108*AB107)*(AA107+AA108)+(AA108*AB109-AA109*AB108)*(AA108+AA109)+(AA109*AB110-AA110*AB109)*(AA109+AA110))/6/AA111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AC101*AD102-AC102*AD101)*(AC101+AC102)+(AC102*AD103-AC103*AD102)*(AC102+AC103)+(AC103*AD104-AC104*AD103)*(AC103+AC104)+(AC104*AD105-AC105*AD104)*(AC104+AC105)+(AC105*AD106-AC106*AD105)*(AC105+AC106)+(AC106*AD107-AC107*AD106)*(AC106+AC107)+(AC107*AD108-AC108*AD107)*(AC107+AC108)+(AC108*AD109-AC109*AD108)*(AC108+AC109)+(AC109*AD110-AC110*AD109)*(AC109+AC110))/6/AC111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AE101*AF102-AE102*AF101)*(AE101+AE102)+(AE102*AF103-AE103*AF102)*(AE102+AE103)+(AE103*AF104-AE104*AF103)*(AE103+AE104)+(AE104*AF105-AE105*AF104)*(AE104+AE105)+(AE105*AF106-AE106*AF105)*(AE105+AE106)+(AE106*AF107-AE107*AF106)*(AE106+AE107)+(AE107*AF108-AE108*AF107)*(AE107+AE108)+(AE108*AF109-AE109*AF108)*(AE108+AE109)+(AE109*AF110-AE110*AF109)*(AE109+AE110))/6/AE111","v":{"$error":"#VALUE!"}},"m",null,null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AK101+AK102)+(AK102*AL103-AK103*AL102)*(AK102+AK103)+(AK103*AL104-AK104*AL103)*(AK103+AK104)+(AK104*AL105-AK105*AL104)*(AK104+AK105)+(AK105*AL106-AK106*AL105)*(AK105+AK106)+(AK106*AL107-AK107*AL106)*(AK106+AK107)+(AK107*AL108-AK108*AL107)*(AK107+AK108)+(AK108*AL109-AK109*AL108)*(AK108+AK109)+(AK109*AL110-AK110*AL109)*(AK109+AK110))/6/AK111","v":{"$error":"#VALUE!"}},"m  "]
[null,null,null,null,null,{"$f":"+'C III-V'!F136:G136","v":"Visina presjeka"},null,{"$f":"+'C III-V'!H136:I136","v":"Intezitet"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.9000021999999994,0.5,{"$f":"-((Y101*Z102-Y102*Z101)*(Z101+Z102)+(Y102*Z103-Y103*Z102)*(Z102+Z103)+(Y103*Z104-Y104*Z103)*(Z103+Z104)+(Y104*Z105-Y105*Z104)*(Z104+Z105)+(Y105*Z106-Y106*Z105)*(Z105+Z106)+(Y106*Z107-Y107*Z106)*(Z106+Z107)+(Y107*Z108-Y108*Z107)*(Z107+Z108)+(Y108*Z109-Y109*Z108)*(Z108+Z109)+(Y109*Z110-Y110*Z109)*(Z109+Z110))/6/Y111","v":{"$error":"#VALUE!"}},"m    ",{"$f":"-((AA101*AB102-AA102*AB101)*(AB101+AB102)+(AA102*AB103-AA103*AB102)*(AB102+AB103)+(AA103*AB104-AA104*AB103)*(AB103+AB104)+(AA104*AB105-AA105*AB104)*(AB104+AB105)+(AA105*AB106-AA106*AB105)*(AB105+AB106)+(AA106*AB107-AA107*AB106)*(AB106+AB107)+(AA107*AB108-AA108*AB107)*(AB107+AB108)+(AA108*AB109-AA109*AB108)*(AB108+AB109)+(AA109*AB110-AA110*AB109)*(AB109+AB110))/6/AA111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AC101*AD102-AC102*AD101)*(AD101+AD102)+(AC102*AD103-AC103*AD102)*(AD102+AD103)+(AC103*AD104-AC104*AD103)*(AD103+AD104)+(AC104*AD105-AC105*AD104)*(AD104+AD105)+(AC105*AD106-AC106*AD105)*(AD105+AD106)+(AC106*AD107-AC107*AD106)*(AD106+AD107)+(AC107*AD108-AC108*AD107)*(AD107+AD108)+(AC108*AD109-AC109*AD108)*(AD108+AD109)+(AC109*AD110-AC110*AD109)*(AD109+AD110))/6/AC111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AE101*AF102-AE102*AF101)*(AF101+AF102)+(AE102*AF103-AE103*AF102)*(AF102+AF103)+(AE103*AF104-AE104*AF103)*(AF103+AF104)+(AE104*AF105-AE105*AF104)*(AF104+AF105)+(AE105*AF106-AE106*AF105)*(AF105+AF106)+(AE106*AF107-AE107*AF106)*(AF106+AF107)+(AE107*AF108-AE108*AF107)*(AF107+AF108)+(AE108*AF109-AE109*AF108)*(AF108+AF109)+(AE109*AF110-AE110*AF109)*(AF109+AF110))/6/AE111","v":{"$error":"#VALUE!"}},"m",null,null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AL101+AL102)+(AK102*AL103-AK103*AL102)*(AL102+AL103)+(AK103*AL104-AK104*AL103)*(AL103+AL104)+(AK104*AL105-AK105*AL104)*(AL104+AL105)+(AK105*AL106-AK106*AL105)*(AL105+AL106)+(AK106*AL107-AK107*AL106)*(AL106+AL107)+(AK107*AL108-AK108*AL107)*(AL107+AL108)+(AK108*AL109-AK109*AL108)*(AL108+AL109)+(AK109*AL110-AK110*AL109)*(AL109+AL110))/6/AK111","v":{"$error":"#VALUE!"}},"m    ",null,{"$f":"+'C III-V'!AN113:AN114","v":-0.25},{"$f":"IF('Analiza i dimenzioniranje'!D84=\"\",0,'Analiza i dimenzioniranje'!D83+'C III-V'!AN113)","v":0.75}]
[null,null,null,null,null,{"$f":"+'C III-V'!F137:G137","v":"III"},{"$f":"+'C III-V'!G137:H137","v":1.2},{"$f":"+'C III-V'!H137:I137","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,0.12820515121628623,{"$f":"+Y111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AA111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AC111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AE111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,{"$f":"+AK111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN"]
[null,null,null,null,null,{"$f":"+'C III-V'!F138:G138","v":"VI"},{"$f":"+'C III-V'!G138:H138","v":1.52},{"$f":"+'C III-V'!H138:I138","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(W99:W114)","v":{"$error":"#VALUE!"}},{"$f":"SUM(X99:X114)","v":21.11641030243257},null,null,null,null,null,null,null,null,null,null,"Teren  kosina",null,"Klizna ploha"]
[null,null,null,null,null,{"$f":"+'C III-V'!F139:G139","v":"VII"},{"$f":"+'C III-V'!G139:H139","v":1.84},{"$f":"+'C III-V'!H139:I139","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C X-XI'!AI116","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!AJ116","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!AK116","v":1.75},{"$f":"+'C X-XI'!AL116","v":-1.1133852506716102},"sjecišta ravnine presjeka na kliznoj plohi",null,null,null,null,null,null,"Omjer površine"]
[null,null,null,null,null,{"$f":"+'C III-V'!F140:G140","v":"VIII"},{"$f":"+'C III-V'!G140:H140","v":2.16},{"$f":"+'C III-V'!H140:I140","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koord. Težište mase  za h22",null,null,null,null,null,null,null,null,null,{"$f":"+'C X-XI'!AI117","v":6.2644906473896782},{"$f":"+'C X-XI'!AJ117","v":6},{"$f":"+'C X-XI'!AK117","v":0},{"$f":"+'C X-XI'!AL117","v":4.08},{"$f":"+'C III-V'!AA100","v":"oznaka"},{"$f":"+'C III-V'!AB100","v":"X"},{"$f":"+'C III-V'!AC100","v":"Y"},null,null,null,"        sa kontraforama: bez kontrafora",null,null,"Potresna sila-prosječna"]
[null,null,null,null,null,{"$f":"+'C III-V'!F141:G141","v":"IX"},{"$f":"+'C III-V'!G141:H141","v":2.48},{"$f":"+'C III-V'!H141:I141","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(AA102-AA103)/3","v":0.67810635947167019},{"$f":"+Z103*0.666666666666667","v":2.6666666666666679},null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!D116,AI117)","v":-5},{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!E116,'C III-V'!AJ117)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!AA101","v":"Y=0"},{"$f":"+'C III-V'!AB101","v":1.75},{"$f":"+'C III-V'!AC101","v":0},{"$f":"+'C X-XI'!AP118","v":0},null,null,null,null,null,null,null,"Potresna sila","F","G"]
[null,null,null,null,null,{"$f":"+'C III-V'!F142:G142","v":"X"},{"$f":"+'C III-V'!G142:H142","v":2.8},{"$f":"+'C III-V'!H142:I142","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"(AJ117-AI117)/(AJ116-AI116)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AI119*AI116+AI117","v":{"$error":"#VALUE!"}}," ",{"$f":"+'C III-V'!AA102","v":"PIII"},{"$f":"+'C III-V'!AB102","v":0.97707863658009864},{"$f":"+'C III-V'!AC102","v":1.2},{"$f":"+'C X-XI'!AP119","v":0},null,null,null,"Ukupna duljina zida",null,{"$f":"+Kontrafore!E13","v":12},"m",{"$f":"+AV119","v":12},{"$f":"+Y111","v":{"$error":"#VALUE!"}},{"$f":"+Y114","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F143:G143","v":"XI"},{"$f":"+'C III-V'!G143:H143","v":3.14},{"$f":"+'C III-V'!H143:I143","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"-(AL117-AK117)/(AK116-AL116)","v":-1.4248868534344206},"*x    +",{"$f":"-(AK116*AI120-AK117)","v":2.4935519935102359}," ",{"$f":"+'C III-V'!AA103","v":"PVI"},{"$f":"+'C III-V'!AB103","v":0.68324863210273346},{"$f":"+'C III-V'!AC103","v":1.52},{"$f":"+'C X-XI'!AP120","v":0},null,null,null,"ukupna duljina kontrafora",null,{"$f":"+Kontrafore!E5*Kontrafore!E4","v":3},"m",{"$f":"+AV120","v":3},{"$f":"+AY119-AY121","v":{"$error":"#VALUE!"}},{"$f":"IF(AV120=AV119,0,AZ119-AZ121)","v":{"$error":"#VALUE!"}}]
["Presjek kroz zid I",null,"Presjek kroz zid II",null,null,{"$f":"+'C III-V'!F144:G144","v":"XIII"},{"$f":"+'C III-V'!G144:H144","v":3.44},{"$f":"+'C III-V'!H144:I144","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AK120-AK119)/(AI119-AI120)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AI120*AI121+AK120","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA104","v":"PVII"},{"$f":"+'C III-V'!AB104","v":0.45866939675594048},{"$f":"+'C III-V'!AC104","v":1.84},{"$f":"+'C X-XI'!AP121","v":0},null,null,null,"ukupna duljina bez kontrafora",null,{"$f":"+AV119-AV120","v":9},"m",{"$f":"+AX119-AX120","v":9},{"$f":"+AG111","v":0},{"$f":"+IF(AX121=0,0,AG114)","v":0}]
["x","y","x","y",null,{"$f":"+'C III-V'!F145:G145","v":"XIII"},{"$f":"+'C III-V'!G145:H145","v":3.76},{"$f":"+'C III-V'!H145:I145","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA105","v":"PVIII"},{"$f":"+'C III-V'!AB105","v":0.23409016140914748},{"$f":"+'C III-V'!AC105","v":2.16},{"$f":"+'C X-XI'!AP122","v":0},null,null,null,"površina s kontraforama",null,{"$f":"+AV120/AV119","v":0.25}]
[0,{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},{"$f":"+A123","v":0},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},null,{"$f":"+'C III-V'!F146:G146","v":"XIV"},{"$f":"+'C III-V'!G146:H146","v":4.08},{"$f":"+'C III-V'!H146:I146","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($AK$119-$AK$123)/AI119","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AK121","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA106","v":"PIX"},{"$f":"+'C III-V'!AB106","v":9.5109260623546556E-3},{"$f":"+'C III-V'!AC106","v":2.48},{"$f":"+'C X-XI'!AP123","v":0},null,null,null,"površina bez kontrafora",null,{"$f":"+AV121/AV119","v":0.75}]
[{"$f":"+F83","v":{"$error":"#VALUE!"}},{"$f":"+B123","v":3.76},{"$f":"+A124","v":{"$error":"#VALUE!"}},{"$f":"+D123","v":3.44},null,{"$f":"+'C III-V'!F147:G147","v":"XV"},{"$f":"+'C III-V'!G147:H147","v":4.4000000000000004},{"$f":"+'C III-V'!H147:I147","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA107","v":"PX"},{"$f":"+'C III-V'!AB107","v":-0.21506830928443818},{"$f":"+'C III-V'!AC107","v":2.8},{"$f":"+'C X-XI'!AP124","v":0},null,null,null,null,null,"odnos",null,{"$f":"-(AX120/AX119)*'Analiza i dimenzioniranje'!D83","v":-0.25}]
[null,null,null,null,null,{"$f":"+'C III-V'!F148:G148","v":"XVI"},{"$f":"+'C III-V'!G148:H148","v":4.72},{"$f":"+'C III-V'!H148:I148","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA108","v":"PXI"},{"$f":"+'C III-V'!AB108","v":-0.45368374684040591},{"$f":"+'C III-V'!AC108","v":3.14},{"$f":"+'C X-XI'!AP125","v":0},null,null,null,null,"krak",{"$f":"+Y113","v":{"$error":"#VALUE!"}},{"$f":"+AZ119","v":{"$error":"#VALUE!"}},{"$f":"+AZ120*AV122","v":{"$error":"#VALUE!"}},null,{"$f":"+AZ119-AX126","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F149:G149","v":"XVII"},{"$f":"+'C III-V'!G149:H149","v":5.04},{"$f":"+'C III-V'!H149:I149","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($AK$120-AK126)/$AI$120","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AK121","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA109","v":"PXII"},{"$f":"+'C III-V'!AB109","v":-0.66422677997802415},{"$f":"+'C III-V'!AC109","v":3.44},{"$f":"+'C X-XI'!AP126","v":0},null,null,null,null,null,{"$f":"+AG113","v":0},{"$f":"+AZ121","v":0},{"$f":"+AZ120*AV123","v":{"$error":"#VALUE!"}},null,{"$f":"+AZ121+AX125","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F150:G150","v":"XVIII"},{"$f":"+'C III-V'!G150:H150","v":5.36},{"$f":"+'C III-V'!H150:I150","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-1.1976024639266576,null,4.2,null,{"$f":"+'C III-V'!AA110","v":"PXIII"},{"$f":"+'C III-V'!AB110","v":-0.88880601532481696},{"$f":"+'C III-V'!AC110","v":3.76},{"$f":"+'C X-XI'!AP127","v":0},null,null,null,null,null,null,null,"Prosječna masa za potres:",null,{"$f":"IF(IF(AV130=AW130,Y114,+AZ126)=0,AZ125,IF(AV130=AW130,Y114,+AZ126))","v":{"$error":"#VALUE!"}},"kn"]
[null,null,null,null,null,{"$f":"+'C III-V'!F151:G151","v":"XIX"},{"$f":"+'C III-V'!G151:H151","v":5.6800000000000006},{"$f":"+'C III-V'!H151:I151","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.90782786744952648,null,1.2,null,{"$f":"+'C III-V'!AA111","v":"PXIV"},{"$f":"+'C III-V'!AB111","v":-1.1133852506716102},{"$f":"+'C III-V'!AC111","v":4.08},{"$f":"+'C X-XI'!AP128","v":0}]
[null,null,null,null,null,{"$f":"+'C III-V'!F152:G152","v":"XX"},{"$f":"+'C III-V'!G152:H152","v":6},{"$f":"+'C III-V'!H152:I152","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.6464828732122183,null,{"$f":"+AI117","v":6.2644906473896782},null,{"$f":"+'C III-V'!AA112","v":"PXV"},{"$f":"+'C III-V'!AB112","v":-1.3379644860184032},{"$f":"+'C III-V'!AC112","v":4.4000000000000004},{"$f":"+'C X-XI'!AP129","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-0.88880601532481696,null,{"$f":"+AF109","v":3.76},null,{"$f":"+'C III-V'!AA113","v":"PXVI"},{"$f":"+'C III-V'!AB113","v":-1.5625437213651958},{"$f":"+'C III-V'!AC113","v":4.72},{"$f":"+'C X-XI'!AP130","v":0},null,null,null,null,"x=",{"$f":"+AG113","v":0},{"$f":"+Y113","v":{"$error":"#VALUE!"}},null,{"$f":"+AI109","v":0},{"$f":"+AI106","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-0.66422677997802415,null,{"$f":"+AD109","v":3.44},null,{"$f":"+'C III-V'!AA114","v":"PXVII"},{"$f":"+'C III-V'!AB114","v":-1.7871229567119888},{"$f":"+'C III-V'!AC114","v":5.04},{"$f":"+'C X-XI'!AP131","v":0},null,null,null,null,"Y=",{"$f":"+AG114","v":0},{"$f":"+Y114","v":{"$error":"#VALUE!"}},null,{"$f":"+AJ109","v":0},{"$f":"+AJ106","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA115","v":"PXVIII"},{"$f":"+'C III-V'!AB115","v":-2.0117021920587819},{"$f":"+'C III-V'!AC115","v":5.36},{"$f":"+'C X-XI'!AP132","v":0},null,null,null,null,"Y=",{"$f":"(AV131-AW131)/(AV130-AW130)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AV132*AW130+AW131","v":{"$error":"#VALUE!"}},{"$f":"(AY131-AZ131)/(AY130-AZ130)","v":{"$error":"#DIV/0!"}},"*x    +",{"$f":"-AY132*AZ130+AZ131","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA116","v":"PXIX"},{"$f":"+'C III-V'!AB116","v":-2.2362814274055753},{"$f":"+'C III-V'!AC116","v":5.6800000000000006},{"$f":"+'C X-XI'!AP133","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA117","v":"PXX"},{"$f":"+'C III-V'!AB117","v":0},{"$f":"+'C III-V'!AC117","v":6.0000000000000009},{"$f":"+'C X-XI'!AP134","v":0},null,null,null,null,"x=",{"$f":"+AK113","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","Y",null,null,null,{"$f":"+AI136","v":{"$error":"#VALUE!"}},{"$f":"+AJ136","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!AP135","v":0},null,null,null,null,"xstv=",{"$f":"+AV134-X113","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C X-XI'!AI136","v":{"$error":"#VALUE!"}},{"$f":"+'C X-XI'!AJ136","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"            Masa da se dobije prosječni potres iz čelije AT125=",null,null,null,null,{"$f":"+AZ125","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+AF104","v":{"$error":"#VALUE!"}},{"$f":"+AD102","v":3.44},{"$f":"+AF102","v":3.76},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"razlika¸površina",{"$f":"+Y111-AI111","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AE144-AC138)/(-AC144)","v":{"$error":"#VALUE!"}},{"$f":"IF(AD138<AC138,(AE151-AD138)/(-AC151),(AE156-AD138)/(-AC156))","v":{"$error":"#VALUE!"}},{"$f":"IF(AE138<AC138,(AE151-AE138)/(-AC151),(AE156-AE138)/(-AC156))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"duljina segmenta",{"$f":"++AJ105","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina III. sloja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"okomito na kliz. Plohu",null,{"$f":"+AV143/AV139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"d=","dodatak",{"$f":"+AV140/COS(AV142*PI()/180)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA153","v":2},{"$f":"+'C III-V'!AB153","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"          kut nagiba klizne plohe za potres   a= ",null,{"$f":"ATAN((-Y104+Y101)/(Z104-Z101))*180/PI()","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA154","v":-5},{"$f":"+'C III-V'!AB154","v":9.9970360471948005},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dodatna površina",{"$f":"+AV144/'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AD143-AD142)/(AC143-AC142)","v":-1.4281480067421144},"*x      +",{"$f":"-AC144*AC142+AD142","v":2.8562960134842288},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"G=",{"$f":"+AX126","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AE144-AD146)/(-AC144)","v":1.1597509541483482}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+Z102","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina II. sloja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA148","v":-1.0572404418349119},{"$f":"+'C III-V'!AB148","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA149","v":0.97707863658009864},{"$f":"+'C III-V'!AB149","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AD150-AD149)/(AC150-AC149)","v":-1.3763819204711734},"*x      +",{"$f":"-AC151*AC149+AD149","v":2.5448333702674724}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina I. sloja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koordinate na sjecištu s terenom",null,null,{"$f":"+'C III-V'!AA144","v":-2.5846586698092704},{"$f":"+'C III-V'!AB144","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koordinate na sjecištu slojeva",null,null,{"$f":"+'C III-V'!AA143","v":-1.0572404418349119},{"$f":"+'C III-V'!AB143","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AD155-AD154)/(AC155-AC154)","v":-1.4825609685127401},"*x      +",{"$f":"-AC156*AC154+AD154","v":2.4325765866023956}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rub dna konzole uz aktivni klin",null,null,{"$f":"+B6","v":{"$error":"#VALUE!"}},{"$f":"+C6","v":3.14}]

{"sheet":"C XIV-XV","index":44,"n_rows":157,"n_cols":53,"rows_kept":157,"cut":false,"hidden":true,"merged":[[112,5,112,6],[99,36,99,37],[116,47,116,49],[67,10,67,11],[67,13,67,14],[77,13,77,14],[77,10,77,11],[99,26,99,27],[99,28,99,29],[99,30,99,31],[67,20,67,21],[77,15,77,16],[67,15,67,16],[96,32,98,33],[96,34,98,35],[96,36,98,37],[99,32,99,33],[99,34,99,35],[90,1,90,2],[90,3,90,4],[90,5,90,6],[96,22,97,23],[99,24,99,25],[44,7,44,8],[44,17,44,18],[42,1,42,2],[42,3,42,4],[42,5,42,6],[42,7,43,10],[44,9,44,10],[44,11,44,12],[42,11,43,14],[42,15,43,18],[67,22,67,23],[77,1,77,2],[77,3,77,4],[77,5,77,6],[77,8,77,9],[67,1,67,2],[67,3,67,4],[67,5,67,6],[67,8,67,9],[44,21,44,22],[44,13,44,14],[44,15,44,16],[16,27,16,28],[17,12,17,16],[17,27,17,28],[26,27,26,28],[114,34,114,35],[114,36,114,37],[13,29,13,30],[0,1,0,2],[0,3,0,4],[0,5,0,7],[0,9,0,10],[1,5,1,8],[10,3,10,4],[10,27,10,28],[11,3,11,4],[12,27,12,28],[13,12,13,16],[13,27,13,28],[62,29,62,30],[62,27,62,28],[110,38,113,38],[110,39,111,40],[112,39,113,39],[112,40,113,40],[115,38,115,40]]}
["Točke","ZID I TEMELJ",null,"NASIP NA TEMELJU IZA",null,"ZID, KONZOLA I NASIP NA KONZOLI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Točka A",null,"Presjek I-I"]
[1,2,{"$f":"+'C III-V'!$C$2","v":0.12820515121628623},null,null,"ZA BILO KOJI PRESJEK ",null,null,null,null,null,null,null,null,null,null,null,"Presjek zid Iv",{"$f":"+($B$9-$B$4)*(T2-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"+B15","v":4.9000021999999994},{"$f":"+C15","v":0.5},{"$f":"+'C XIV-XV'!B10+0.05","v":{"$error":"#VALUE!"}},-0.5]
[2,2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T3-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},"Točka B",null,{"$f":"+W2","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!C10+0.5","v":{"$error":"#VALUE!"}}]
[3,{"$f":"+B3+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+C3","v":1.2},{"$f":"+B19","v":2},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>C4,B21,B4)","v":3.4000010999999999},{"$f":"IF(E20>C4,E20,C4)","v":1.2},{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},null,null,null,null,null,null,null,null,"Presjek V",{"$f":"+($B$9-$B$4)*(T4-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+'C XIV-XV'!B2","v":2},{"$f":"+'C XIV-XV'!C2","v":0.12820515121628623}]
[4,{"$f":"+B23","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},{"$f":"+D4","v":2},{"$f":"+'C III-V'!E5","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,B21,B5)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,E20,C5)","v":3.14},{"$f":"+F8","v":{"$error":"#VALUE!"}},{"$f":"+G8","v":3.44},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T5-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},null,null,"Presjek II-II",null,null,null,"Nasip na zidu iza"]
[5,{"$f":"+B5-'Analiza i dimenzioniranje'!G78","v":{"$error":"#VALUE!"}},{"$f":"+C5","v":3.14},{"$f":"IF(B6<2,B5,IF(B9>2,B9,D5))","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!E6","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C7,B21,B6)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C6,E20,C6)","v":3.14},{"$f":"IF(F7>F9,H5,F9)","v":{"$error":"#VALUE!"}},{"$f":"IF(F7>F9,I5,IF(E20>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XIV-XV'!E20,G9))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"Presjek VI",{"$f":"+($B$9-$B$4)*(T6-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},"TLO 1. sloj",null,{"$f":"+'C XIV-XV'!B15-0.05","v":4.8500021999999996},{"$f":"+'C XIV-XV'!X2","v":-0.5},null,null,2,{"$f":"IF('Analiza i dimenzioniranje'!AW26>'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AW26)","v":0}]
[6,{"$f":"IF('Analiza i dimenzioniranje'!G78=0,'C XIV-XV'!B8,B6)","v":{"$error":"#VALUE!"}},{"$f":"C6+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+B4","v":3.4000010999999999},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>=C7,B21,B7)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C7,E20,C7)","v":3.44},{"$f":"IF(F7>F9,H6,H6)","v":{"$error":"#VALUE!"}},{"$f":"+I6","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T7-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},{"$f":"+'C XIV-XV'!B15-0.05","v":4.8500021999999996},{"$f":"+'C XIV-XV'!X3","v":{"$error":"#VALUE!"}},"Horizontala",null,2,{"$f":"'Analiza i dimenzioniranje'!BF28","v":0}]
[7,{"$f":"+B22","v":{"$error":"#VALUE!"}},{"$f":"+C7","v":3.44},{"$f":"+D4","v":2},{"$f":"+E4","v":1.2},{"$f":"IF(E20>C8,B21,B8)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C8,E20,C8)","v":3.44},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$H$15=0,I7+(H7-H8)*'Unos podataka'!R57,IF('C III-V'!H9>'Unos podataka'!$B$105,I7+(H7-H8)*'Unos podataka'!$R$55,'Unos podataka'!$T$57))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"Presjek VII",{"$f":"+($B$9-$B$4)*(T8-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!V8","v":6},null,null,{"$f":"+'C XIV-XV'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!C5","v":3.14}]
[8,{"$f":"B4-TAN('Analiza i dimenzioniranje'!H51*PI()/180)*('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},null,null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"+I4","v":3.44},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T9-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U8-'Analiza i dimenzioniranje'!E27","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!V9","v":6.2644906473896782},"Presjek ZID",null,{"$f":"+IF('Analiza i dimenzioniranje'!$E$24=0,0,'C XIV-XV'!Y4)","v":0},{"$f":"+Z8","v":3.14}]
[9,{"$f":"+B9+'Analiza i dimenzioniranje'!E54","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},null,null,{"$f":"+B10","v":{"$error":"#VALUE!"}},{"$f":"+C10","v":"A"},null,null,null,null,null,null,null,null,null,null,"Presjek VIII",{"$f":"+($B$9-$B$4)*(T10-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},-8,{"$f":"+'C III-V'!V10","v":6.2644906473896782},{"$f":"+'C XIV-XV'!B15-0.5","v":4.4000021999999994},{"$f":"+'C XIV-XV'!C10+0.1","v":{"$error":"#VALUE!"}}]
[10,{"$f":"+B4+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+C3","v":1.2},"NASIP NA KONZOLI",null,{"$f":"+F12+E65","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C11,E20,C11)","v":1.2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T11-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},"x","y",{"$f":"+'C XIV-XV'!B10+0.5","v":{"$error":"#VALUE!"}},{"$f":"+X10","v":{"$error":"#VALUE!"}},null,null,null,"Rsidra"]
[11,{"$f":"+B11","v":4.2000010999999997},{"$f":"+C11","v":1.2},"za stabilnost",null,{"$f":"+F4","v":3.4000010999999999},{"$f":"+G4","v":1.2},null,null,null,null,null,null,null,null,null,null,"Presjek IX",{"$f":"+($B$9-$B$4)*(T12-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+W23","v":{"$error":"#VALUE!"}},{"$f":"+U12*(V9-V8)/(U9-U8)-U8*(V9-V8)/(U9-U8)+V8","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,20,AB16)","v":20},{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,0,AC16)","v":0}]
[12,{"$f":"+B12","v":4.2000010999999997},{"$f":"+C12","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T13-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+W25","v":{"$error":"#VALUE!"}},{"$f":"+U13*(V9-V8)/(U9-U8)-U8*(V9-V8)/(U9-U8)+V8","v":{"$error":"#VALUE!"}},"Pad terena niz padinu",null,null,null,null,"Os rezultante sidara Ukupna računska sila u sidrima"]
[13,{"$f":"+B11+'Analiza i dimenzioniranje'!G57","v":4.9000021999999994},{"$f":"+C13","v":1.2},{"$f":"+B7","v":{"$error":"#VALUE!"}},3.44,null,null,null,null,"Linija presjeka",null,null," Koordinata sredine presjeka",null,null,null,null,"Presjek X",{"$f":"+($B$9-$B$4)*(T14-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},"TLO 2. sloj",null,{"$f":"+'Analiza i dimenzioniranje'!Q105","v":3},{"$f":"+'Analiza i dimenzioniranje'!P105","v":{"$error":"#VALUE!"}},null,null,null,"Slobodna  zona.",null,"1. sloj"]
[14,{"$f":"+B14","v":4.9000021999999994},{"$f":"+C14-'Analiza i dimenzioniranje'!E51","v":0.5},{"$error":"#VALUE!"},3.44,{"$f":"IF((B4-B9)=0,0,+(C9-C4)/(B4-B9))","v":{"$error":"#VALUE!"}},"n  Nagib zida u tlu",null,null,0,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,"III-III","konzola","Presjek I","Presjek II",null,{"$f":"+($B$11-$B$10)*(T15-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},{"$f":"IF(('Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17)<'Analiza i dimenzioniranje'!$F$45,2,(IF(B7<B24,B7,IF('Analiza i dimenzioniranje'!G78=0,'C XIV-XV'!B24,2))))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17","v":4},{"$f":"+'Analiza i dimenzioniranje'!O130","v":7.1000021999999996},{"$f":"+'Analiza i dimenzioniranje'!N130","v":1.5001009999999999},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,AB24)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,'Analiza i dimenzioniranje'!P22)","v":5},{"$f":"+U9","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782}]
[15,{"$f":"+B2","v":2},{"$f":"+C2","v":0.12820515121628623},{"$error":"#VALUE!"},"A",null,null,null,null,3,{"$f":"+K15","v":1.2},null,"x",{"$f":"+(F12+F11)/2","v":{"$error":"#VALUE!"}},{"$f":"(B8+(B11-B10)*(O17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U29+(B11-B10)*(P17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U34+(B11-B10)*(Q17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},"Presjek XI",{"$f":"+($B$9-$B$4)*(T16-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},-8,{"$f":"+V15+(U15-U16)*TAN('Analiza i dimenzioniranje'!$E$18*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"AB15-'Analiza i dimenzioniranje'!P23","v":{"$error":"#VALUE!"}},{"$f":"+AC15-(AB15-AB16)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782}]
[null,null,"Jednadžba pravca zida uz tlo",{"$f":"+D16","v":{"$error":"#VALUE!"}},{"$f":"+I7","v":{"$error":"#VALUE!"}},null,null,null,null,"Sloj 2 gore",null,null,"y",{"$f":"+G11","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},null,{"$f":"+($B$11-$B$10)*(T17-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},"TLO 3. sloj",null,"Prometno opterećenje",null,null,null,null,"Sidrena dionica",null,"Jednadžba površine terena"]
[null,"x","y",{"$f":"+D14","v":{"$error":"#VALUE!"}},{"$f":"+I8","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+F94","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E52>=G94,0,G94)","v":4},null,null,null,null,null,null,"Presjek XII",{"$f":"+($B$9-$B$4)*(T18-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},2,{"$f":"+'Analiza i dimenzioniranje'!$F$17","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,+'C XIV-XV'!B9-'Analiza i dimenzioniranje'!E26)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,'C XIV-XV'!V9)","v":6.2644906473896782},null,null,null,"                   Y=",null,{"$f":"+(AE16-AE15)/(AD16-AD15)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AD18*AD15+AE15","v":{"$error":"#VALUE!"}}]
[null,2,{"$f":"+B19*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},{"$f":"+D14","v":{"$error":"#VALUE!"}},{"$f":"+E14","v":3.44},null,null,null,null,{"$f":"U16","v":-8},{"$f":"+K18","v":4},null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T19-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},-8,{"$f":"+V18+(U18-U19)*TAN('Analiza i dimenzioniranje'!$F$18*PI()/180)","v":1.5492076949174773},{"$f":"+W18","v":{"$error":"#VALUE!"}},{"$f":"+X18+'Analiza i dimenzioniranje'!E24/50","v":6.4644906473896784},null,null,null,{"$f":"+AB16","v":{"$error":"#VALUE!"}},{"$f":"+AC16","v":{"$error":"#VALUE!"}},"za x=",{"$f":"+AB20","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+H8","v":{"$error":"#VALUE!"}},{"$f":"+B20*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},"M na koti",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,"Sloj 1 ili2 dole",null,null,null,null,null,null,{"$f":"+(B11-B10)*(Q21-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},"Presjek XIII",{"$f":"+($B$9-$B$4)*(T20-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},"KONTAKTNI NAPONI",null,{"$f":"+W18-'Analiza i dimenzioniranje'!E25","v":{"$error":"#VALUE!"}},{"$f":"+X19","v":6.4644906473896784},null,null,null,{"$f":"+(AB21+AB19)/2","v":{"$error":"#VALUE!"}},{"$f":"+(AC19+AC21)/2","v":{"$error":"#VALUE!"}},"y=",{"$f":"+AD18*AE19+AF18","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C21-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,{"$f":"+IF('Analiza i dimenzioniranje'!G78=0,D8,H8)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+F95","v":{"$error":"#VALUE!"}},{"$f":"+G12","v":1.2},null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,{"$f":"+($B$11-$B$10)*(T21-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},2,0,{"$f":"+W20","v":{"$error":"#VALUE!"}},{"$f":"+X18","v":6.2644906473896782},null,null,null,{"$f":"+AB19-'Analiza i dimenzioniranje'!P24","v":{"$error":"#VALUE!"}},{"$f":"+AC19-(AB19-AB21)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},"visina sloja iznad centra sidra"]
[null,{"$f":"+(B9-B4)*(C22-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+C23+'Analiza i dimenzioniranje'!C77","v":3.44},null,null,null,null,null,null,{"$f":"+U19","v":-8},{"$f":"+K21","v":1.2},null,null,null,null,null,null,"Presjek XIV",{"$f":"+($B$9-$B$4)*(T22-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},2,{"$f":"-'Analiza i dimenzioniranje'!$F$193/100","v":{"$error":"#VALUE!"}},"Točkasto",null,null,null,null,null,null,{"$f":"+AE20-AC20","v":{"$error":"#VALUE!"}},"m"]
[null,{"$f":"+(B9-B4)*(C23-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T23-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"2+'Analiza i dimenzioniranje'!$E$61","v":4.9000021999999994},{"$f":"-'Analiza i dimenzioniranje'!$F$190/100","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E36=0,-10,B9-'Analiza i dimenzioniranje'!E37)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X23","v":{"$error":"#VALUE!"}},null,null,null,"Jednadžba  lica zida "]
[null,{"$f":"+(B9-B4)*(C24-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V15","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek XV",{"$f":"+($B$9-$B$4)*(T24-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U23","v":4.9000021999999994},0,"Linijsko iza zida",null,null,null,"x=",{"$f":"+($B$11-$B$10)*(AB25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+($B$11-$B$10)*(AC25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+(B11-B10)*(AE25-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C25-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U21","v":2},0,{"$f":"IF('Analiza i dimenzioniranje'!$E$34=0,0,B9-'Analiza i dimenzioniranje'!K28)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X27","v":{"$error":"#VALUE!"}},null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!AD42","v":5},{"$f":"+'Analiza i dimenzioniranje'!AE42","v":5},null,{"$f":"+'Analiza i dimenzioniranje'!H76+'Analiza i dimenzioniranje'!E52","v":1.5001009999999999}]
[null,{"$f":"+(B9-B4)*(C26-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid VII-VII",{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+W25","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$34=0,0,X25+1)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!T22","v":0},null,null,null,null,{"$f":"+B14-AE24","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C27-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},"TEMELJ -opterećenje",null,"x=",{"$f":"+($B$11-$B$10)*(Z26-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"Rez. Sidra na zidu"]
[null,{"$f":"+(B9-B4)*(C26-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V27","v":4.4000000000000004},{"$f":"+IF('Analiza i dimenzioniranje'!E28=0,0,W29)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9+'Analiza i dimenzioniranje'!F20+1.5)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!S22","v":0}]
["Sjecište s dnom temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V29-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":4.4000000000000004},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W30-0.3)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X30)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z28-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+($B$11-$B$10)*(AC29-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E40","v":3.9999999960000001},{"$f":"+AB29+0.4","v":{"$error":"#VALUE!"}},{"$f":"+AC29+(AD29-AB29)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}}]
["zid",{"$f":"+B20","v":{"$error":"#VALUE!"}},{"$f":"+B30*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V30-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":4.4000000000000004},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,B9-'Analiza i dimenzioniranje'!$E$32)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X31+'Analiza i dimenzioniranje'!E33)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!R22","v":0},null,null,null,{"$f":"+AB29-1","v":{"$error":"#VALUE!"}},{"$f":"+AC29-(AB29-AD30)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}}]
["Vrh zida",{"$f":"+(B9-B4)*(C31-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C558","v":-0.45},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid Iv",{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"+W30","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9-'Analiza i dimenzioniranje'!K31)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z30-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"nagib lica"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,W31-'Analiza i dimenzioniranje'!$E$29)","v":{"$error":"#VALUE!"}},{"$f":"+X31","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q22","v":3},null,"tan"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V32","v":4.08},{"$f":"+W32","v":{"$error":"#VALUE!"}},{"$f":"+X30","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z32-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+(B13-B10)/(C10-C13)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V34-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V33","v":4.08},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W33+0.3)","v":{"$error":"#VALUE!"}},{"$f":"+X29","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q20","v":5},null,"kut"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V35-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V34","v":4.08},{"$f":"+W34","v":{"$error":"#VALUE!"}},{"$f":"+X28","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z34-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+ATAN(AB33)*180/PI()","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SIDRO za presjek",null,null,null,"Jednadžba pravca lica zida ",null,null,"Sjecište a arm konzole",null,"vrh zida","Anker armatura uz lice",null,"arm dno",null,"Y=",{"$f":"IF(AE38=AE37,1000000,(AF38-AF37)/(AE38-AE37))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AJ36*AE37+AF37","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!$C$545","v":1.6923077248520526}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB15)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC15)","v":5},null,null,"x=",null,null,{"$f":"+(B11-B10)*(AB38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AC38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AD38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AF37-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!B545","v":{"$error":"#VALUE!"}},{"$f":"+U81","v":2.0499999999999998},{"$f":"+V81","v":0.18682583433163008},"X=",{"$f":"+(-AL36+AL39)/(AJ36-AJ39)","v":{"$error":"#VALUE!"}},"sjeište",null,"x=",{"$f":"+(AN36-AL36)/AJ36","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB16)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC16)","v":{"$error":"#VALUE!"}},null,null,"y=",null,null,{"$f":"+'Analiza i dimenzioniranje'!E555","v":3.39},{"$f":"+AB38-'Analiza i dimenzioniranje'!#REF!","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!C558","v":-0.45},{"$f":"+(B11-B10)*(AF38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+U82","v":4.8600021999999994},{"$f":"+V82","v":0.54310345350772504},"Y=",{"$f":"+AJ36*AJ37+AL36","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate dna temelja",null,null,null,null,null,null,"Y=",{"$f":"+(AH38-AH37)/(AG38-AG37)","v":0.12678908905341604},"*x",{"$f":"-AJ39*AG37+AH37","v":-7.3091798227872762E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"lice","koord Pr II",{"$f":"+AB47+'Analiza i dimenzioniranje'!Q58","v":3.4500010999999997},{"$f":"(AB40*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24999999999999994},null,"SIDRO"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+(B11-B10)*(Z42-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+B8","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+AB15","v":{"$error":"#VALUE!"}},{"$f":"+AC15","v":5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+Z42","v":3.44},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,AB15-0.5)","v":{"$error":"#VALUE!"}},{"$f":"+AF41-(AE41-AE42)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},null,"Nasip ispred zida"]
["Oznaka","temelj",null,"Zid i konzola za pr. ZID",null,"Nasip na temelju iza zida",null,"      Za momente u presjeku zid-temelj          ",null,null,null,"      Za momente u presjeku XIV",null,null,null,"         Za momente u presjeku XV",null,null,null,null,1,null,null,null,null,null,null,2,0,null,null,null,null,{"$f":"+AE24","v":{"$error":"#VALUE!"}},{"$f":"+C11+'Analiza i dimenzioniranje'!$H$76","v":1.5001009999999999}]
["točke","x","y","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - BETON",null,null,null,null,null,2.65,{"$f":"+(AC47+AC49)/2","v":0.31034478180740688},null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!$E$61","v":4.9000021999999994},{"$f":"+AI43","v":1.5001009999999999}]
[1,{"$f":"+'C XIV-XV'!B2","v":2},{"$f":"+'C XIV-XV'!C2","v":0.12820515121628623},null,null,null,null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"Kontaktni naponi za stab",null,"Beton do presjeka II-II",null,"Beton sredine temelja",null,"Beton do presjeka I-I",null,{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"(AB45*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH44+1.6","v":6.5000021999999991},{"$f":"+AI44-(AH45-AH44)*TAN('Analiza i dimenzioniranje'!H22*PI()/180)","v":1.5001009999999999}]
[2,{"$f":"+'C XIV-XV'!B3","v":2},{"$f":"+'C XIV-XV'!C3","v":1.2},null,null,null,null,"x","y","x","y","x","y","x","y","x","y","x","y","x","y",null,null,"x","y","x","y",{"$f":"+(AB43+AB47)/2","v":2.7000005499999999},{"$f":"(AB46*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.1206896584423281},null,null,null,null,"x","y"]
[3,{"$f":"+'C XIV-XV'!B4","v":3.4000010999999999},{"$f":"+'C XIV-XV'!C4","v":1.2},{"$f":"+B4","v":3.4000010999999999},1.2,2,1.2,3.4000010999999999,1.2,{"$f":"+D14","v":{"$error":"#VALUE!"}},3.44,{"$f":"+U34","v":{"$error":"#VALUE!"}},{"$f":"+V34","v":4.08},{"$f":"+J47","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AD44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AD44,K47)","v":4.08},{"$f":"+U29","v":{"$error":"#VALUE!"}},{"$f":"+V29","v":4.4000000000000004},{"$f":"+J47","v":{"$error":"#VALUE!"}},{"$f":"+S48","v":4.4000000000000004},{"$f":"+U21","v":2},{"$f":"+V21*100","v":0},2,0,{"$f":"+B4","v":3.4000010999999999},{"$f":"+W49","v":1.2},{"$f":"+B11","v":4.2000010999999997},1.2,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"(AB47*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24137931688465614},"Presjek II-II",null,null,null,{"$f":"+'C XIV-XV'!B11","v":4.2000010999999997},{"$f":"+C11","v":1.2}]
[4,{"$f":"+B11","v":4.2000010999999997},1.2,{"$error":"#VALUE!"},3.14,2,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.44,{"$f":"+H48","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AD44<'Analiza i dimenzioniranje'!F45,I48,'C XIV-XV'!V34)","v":4.08},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AD44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AD44,K48)","v":4.08},{"$f":"+H48","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AE44<'Analiza i dimenzioniranje'!F45,I48,V29)","v":4.4000000000000004},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AE44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AE44,K48)","v":4.4000000000000004},{"$f":"+U22","v":2},{"$f":"+V22*100","v":{"$error":"#VALUE!"}},2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+X47+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+Y47","v":1.2},4.2000010999999997,1.2,{"$f":"+AB77","v":{"$error":"#VALUE!"}},{"$f":"(AB48*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47+'Analiza i dimenzioniranje'!H76","v":1.5001009999999999}]
[5,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.14,{"$f":"+D16","v":{"$error":"#VALUE!"}},{"$f":"+E16+'Unos podataka'!$F9","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AD44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XIV-XV'!L47,'C XIV-XV'!B6)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AD44<'Analiza i dimenzioniranje'!F45,I49,'C XIV-XV'!V34)","v":4.08},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AD44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AD44,K49)","v":4.08},{"$f":"IF('Analiza i dimenzioniranje'!AE44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XIV-XV'!B6,P47)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AE44<'Analiza i dimenzioniranje'!F45,'C XIV-XV'!I49,Q48)","v":4.4000000000000004},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AE44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AE44,K49)","v":4.4000000000000004},{"$f":"+U23","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},{"$f":"+V48+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+W48","v":1.2},{"$f":"+AB49","v":4.2000010999999997},{"$f":"+AC49","v":0.37931024673015767},4.2000010999999997,1.2,{"$f":"+AB47+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+(AB49*(AC43-AC53)/(AB43-AB53)-AB53*(AC43-AC53)/(AB43-AB53)+AC53)","v":0.37931024673015767},"Presjek I-I",null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+AI48","v":1.5001009999999999}]
[6,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.44,3.4000010999999999,1.2,{"$error":"#VALUE!"},3.44,{"$f":"IF('Unos podataka'!$B$105>J47,'Unos podataka'!$B$105,J47)","v":{"$error":"#VALUE!"}},{"$f":"+K51","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AD44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XIV-XV'!L48,'C XIV-XV'!B7)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AD44<='Analiza i dimenzioniranje'!F45,I50,'C XIV-XV'!V34)","v":4.08},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AD44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AD44,K50)","v":4.08},{"$f":"IF('Analiza i dimenzioniranje'!AE44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XIV-XV'!P47,H50)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AG44<='Analiza i dimenzioniranje'!F45,I50,V29)","v":4.4000000000000004},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AE44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AE44,K50)","v":4.4000000000000004},{"$f":"+U24","v":4.9000021999999994},{"$f":"+V24*100","v":0},{"$f":"+V49","v":3.4000010999999999},{"$f":"+AC47","v":0.24137931688465614},{"$f":"+X47","v":3.4000010999999999},{"$f":"+AC47","v":0.24137931688465614},4.9000021999999994,1.2,{"$f":"2+'Analiza i dimenzioniranje'!E61/2","v":3.4500010999999997},{"$f":"(AB50*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24999999999999994},null,null,null,null,{"$f":"+AH49","v":4.9000021999999994},{"$f":"+C14","v":1.2}]
[7,4.9000021999999994,1.2,{"$error":"#VALUE!"},3.44,2,1.2,{"$error":"#VALUE!"},3.44,{"$f":"+D18","v":{"$error":"#VALUE!"}},{"$f":"+E18+'Unos podataka'!$F9","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AD44>'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XIV-XV'!B28,B8)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AD44>='Analiza i dimenzioniranje'!I75+'Analiza i dimenzioniranje'!G67,'C XIV-XV'!M50,Z26)","v":4.08},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AD44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AD44,K51)","v":4.08},{"$f":"IF('Analiza i dimenzioniranje'!AE44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XIV-XV'!B25,H51)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AG44<='Analiza i dimenzioniranje'!F45,I51,V29)","v":4.4000000000000004},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AE44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AE44,K51)","v":4.4000000000000004},{"$f":"+U25","v":2},{"$f":"+V25*100","v":0},{"$f":"+V47","v":2},{"$f":"+W47","v":0},{"$f":"+X47","v":3.4000010999999999},{"$f":"+Y47","v":1.2},4.9000021999999994,0.5,{"$f":"+(AB49+AB53)/2","v":4.5500016499999996},{"$f":"(AB51*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.43965512336507878},null,null,null,null,{"$f":"+B13","v":4.2000010999999997},{"$f":"+C13","v":1.2}]
[8,4.9000021999999994,0.5,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",{"$error":"#VALUE!"},3.44,{"$f":"+H52","v":{"$error":"#VALUE!"}},{"$f":"+Q52","v":"A"},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AD44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AD44,K52)","v":4.08},{"$f":"+H52","v":{"$error":"#VALUE!"}},{"$f":"+I52","v":"A"},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AE44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AE44,K52)","v":4.4000000000000004},null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AC49","v":0.37931024673015767},{"$f":"+AD77","v":{"$error":"#VALUE!"}},{"$f":"(AB52*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH51","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[9,2,0.12820515121628623,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",null,null,{"$f":"+H53","v":{"$error":"#VALUE!"}},{"$f":"+Q53","v":"A"},null,null,{"$f":"+H53","v":{"$error":"#VALUE!"}},{"$f":"+I53","v":"A"},null,null,null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AA47","v":1.2},{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+C15","v":0.5},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[10,null,null,4.2000010999999997,1.2,null,null,{"$error":"#VALUE!"},1.2,null,null,{"$f":"+U35","v":{"$error":"#VALUE!"}},{"$f":"+M47","v":4.08},null,null,{"$f":"+U30","v":{"$error":"#VALUE!"}},{"$f":"+V30","v":4.4000000000000004},null,null,null,null,null,null,null,null,null,null,"Koordinate s","naprezanjem"]
[11,null,null,{"$f":"+D47","v":3.4000010999999999},{"$f":"+E47","v":1.2},null,null,3.4000010999999999,1.2,null,null,{"$f":"+L47","v":{"$error":"#VALUE!"}},{"$f":"+M47","v":4.08},null,null,{"$f":"+P47","v":{"$error":"#VALUE!"}},{"$f":"+Q47","v":4.4000000000000004},null,null,null,null,null,null,null,null,null,null,{"$f":"+U22","v":2},{"$f":"+V22*100","v":{"$error":"#VALUE!"}}]
[12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+AB56*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
[13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AB57*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
["  A=",{"$f":"-0.5*((B45*C46-B46*C45)+(B46*C47-B47*C46)+(B47*C48-B48*C47)+(B48*C49-B49*C48)+(B49*C50-B50*C49)+(B50*C51-B51*C50)+(B51*C52-B52*C51)+(B52*C53-B53*C52))","v":2.5691044797107181},"m2",{"$f":"-0.5*((D45*E46-D46*E45)+(D46*E47-D47*E46)+(D47*E48-D48*E47)+(D48*E49-D49*E48)+(D49*E50-D50*E49)+(D50*E51-D51*E50)+(D51*E52-D52*E51)+(D52*E53-D53*E52)+(D53*E54-D54*E53)+(D54*E55-D55*E54)+(D55*E56-D56*E55)+(D56*E57-D57*E56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((F45*G46-F46*G45)+(F46*G47-F47*G46)+(F47*G48-F48*G47)+(F48*G49-F49*G48)+(F49*G50-F50*G49)+(F50*G51-F51*G50)+(F51*G52-F52*G51)+(F52*G53-F53*G52)+(F53*G54-F54*G53)+(F54*G55-F55*G54)+(F55*G56-F56*G55)+(F56*G57-F57*G56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((H47*I48-H48*I47)+(H48*I49-H49*I48)+(H49*I50-H50*I49)+(H50*I51-H51*I50)+(H51*I52-H52*I51)+(H52*I53-H53*I52)+(H53*I54-H54*I53)+(H54*I55-H55*I54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((J47*K48-J48*K47)+(J48*K49-J49*K48)+(J49*K50-J50*K49)+(J50*K51-J51*K50)+(J51*K52-J52*K51)+(J52*K53-J53*K52)+(J53*K54-J54*K53)+(J54*K55-J55*K54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((L47*M48-L48*M47)+(L48*M49-L49*M48)+(L49*M50-L50*M49)+(L50*M51-L51*M50)+(L51*M52-L52*M51)+(L52*M53-L53*M52)+(L53*M54-L54*M53)+(L54*M55-L55*M54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"IF(0.5*((N47*O48-N48*O47)+(N48*O49-N49*O48)+(N49*O50-N50*O49)+(N50*O51-N51*O50)+(N51*O52-N52*O51)+(N52*O53-N53*O52)+(N53*O54-N54*O53)+(N54*O55-N55*O54))<0,0,0.5*((N47*O48-N48*O47)+(N48*O49-N49*O48)+(N49*O50-N50*O49)+(N50*O51-N51*O50)+(N51*O52-N52*O51)+(N52*O53-N53*O52)+(N53*O54-N54*O53)+(N54*O55-N55*O54)))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((P47*Q48-P48*Q47)+(P48*Q49-P49*Q48)+(P49*Q50-P50*Q49)+(P50*Q51-P51*Q50)+(P51*Q52-P52*Q51)+(P52*Q53-P53*Q52)+(P53*Q54-P54*Q53)+(P54*Q55-P55*Q54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((R47*S48-R48*S47)+(R48*S49-R49*S48)+(R49*S50-R50*S49)+(R50*S51-R51*S50)+(R51*S52-R52*S51)+(R52*S53-R53*S52)+(R53*S54-R54*S53)+(R54*S55-R55*S54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((T47*U48-T48*U47)+(T48*U49-T49*U48)+(T49*U50-T50*U49)+(T50*U51-T51*U50)+(T51*U52-T52*U51)+(T52*U53-T53*U52)+(T53*U54-T54*U53)+(T54*U55-T55*U54))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((V47*W48-V48*W47)+(V48*W49-V49*W48)+(V49*W50-V50*W49)+(V50*W51-V51*W50))","v":1.5110356654221164},"m2",{"$f":"-0.5*((X47*Y48-X48*Y47)+(X48*Y49-X49*Y48)+(X49*Y50-X50*Y49)+(X50*Y51-X51*Y50))","v":0.71172417455407389},"m2",{"$f":"-0.5*((Z47*AA48-Z48*AA47)+(Z48*AA49-Z49*AA48)+(Z49*AA50-Z50*AA49)+(Z50*AA51-Z51*AA50)+(Z51*AA52-Z52*AA51)+(Z52*AA53-Z53*AA52)+(Z53*AA54-Z54*AA53)+(Z54*AA55-Z55*AA54))","v":0.53224225002380887},"m2",{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-0.5*((AH47*AI48-AH48*AI47)+(AH48*AI49-AH49*AI48)+(AH49*AI50-AH50*AI49)+(AH50*AI51-AH51*AI50)+(AH51*AI52-AH52*AI51)+(AH52*AI53-AH53*AI52)+(AH53*AI54-AH54*AI53)+(AH54*AI55-AH55*AI54))","v":0.21007103011109951},"m2"]
["xt=",{"$f":"-((B45*C46-B46*C45)*(B45+B46)+(B46*C47-B47*C46)*(B46+B47)+(B47*C48-B48*C47)*(B47+B48)+(B48*C49-B49*C48)*(B48+B49)+(B49*C50-B50*C49)*(B49+B50)+(B50*C51-B51*C50)*(B50+B51)+(B51*C52-B52*C51)*(B51+B52)+(B52*C53-B53*C52)*(B52+B53)+(B53*C54-B54*C53)*(B53+B54)+(B54*C55-B55*C54)*(B54+B55)+(B55*C56-B56*C55)*(B55+B56)+(B56*C57-B57*C56)*(B56+B57))/6/B58","v":3.3485779696489133},"m",{"$f":"-((D45*E46-D46*E45)*(D45+D46)+(D46*E47-D47*E46)*(D46+D47)+(D47*E48-D48*E47)*(D47+D48)+(D48*E49-D49*E48)*(D48+D49)+(D49*E50-D50*E49)*(D49+D50)+(D50*E51-D51*E50)*(D50+D51)+(D51*E52-D52*E51)*(D51+D52)+(D52*E53-D53*E52)*(D52+D53)+(D53*E54-D54*E53)*(D53+D54)+(D54*E55-D55*E54)*(D54+D55)+(D55*E56-D56*E55)*(D55+D56)+(D56*E57-D57*E56)*(D56+D57))/6/D58","v":{"$error":"#VALUE!"}},"m",{"$f":"-((F45*G46-F46*G45)*(F45+F46)+(F46*G47-F47*G46)*(F46+F47)+(F47*G48-F48*G47)*(F47+F48)+(F48*G49-F49*G48)*(F48+F49)+(F49*G50-F50*G49)*(F49+F50)+(F50*G51-F51*G50)*(F50+F51)+(F51*G52-F52*G51)*(F51+F52)+(F52*G53-F53*G52)*(F52+F53)+(F53*G54-F54*G53)*(F53+F54)+(F54*G55-F55*G54)*(F54+F55)+(F55*G56-F56*G55)*(F55+F56)+(F56*G57-F57*G56)*(F56+F57))/6/F58","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(H47*I48-H48*I47)*(H47+H48)+(H48*I49-H49*I48)*(H48+H49)+(H49*I50-H50*I49)*(H49+H50)+(H50*I51-H51*I50)*(H50+H51)+(H51*I52-H52*I51)*(H51+H52)+(H52*I53-H53*I52)*(H52+H53)+(H53*I54-H54*I53)*(H53+H54)+(H54*I55-H55*I54)*(H54+H55))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(J47+J48)+(J48*K49-J49*K48)*(J48+J49)+(J49*K50-J50*K49)*(J49+J50)+(J50*K51-J51*K50)*(J50+J51)+(J51*K52-J52*K51)*(J51+J52)+(J52*K53-J53*K52)*(J52+J53)+(J53*K54-J54*K53)*(J53+J54)+(J54*K55-J55*K54)*(J54+J55)+(J55*K56-J56*K55)*(J55+J56)+(J56*K57-J57*K56)*(J56+J57))/6/J58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(L47*M48-L48*M47)*(L47+L48)+(L48*M49-L49*M48)*(L48+L49)+(L49*M50-L50*M49)*(L49+L50)+(L50*M51-L51*M50)*(L50+L51)+(L51*M52-L52*M51)*(L51+L52)+(L52*M53-L53*M52)*(L52+L53)+(L53*M54-L54*M53)*(L53+L54)+(L54*M55-L55*M54)*(L54+L55))/6/L58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(N58=0,0,(+(N47*O48-N48*O47)*(N47+N48)+(N48*O49-N49*O48)*(N48+N49)+(N49*O50-N50*O49)*(N49+N50)+(N50*O51-N51*O50)*(N50+N51)+(N51*O52-N52*O51)*(N51+N52))/6/N58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(P47*Q48-P48*Q47)*(P47+P48)+(P48*Q49-P49*Q48)*(P48+P49)+(P49*Q50-P50*Q49)*(P49+P50)+(P50*Q51-P51*Q50)*(P50+P51)+(P51*Q52-P52*Q51)*(P51+P52)+(P52*Q53-P53*Q52)*(P52+P53)+(P53*Q54-P54*Q53)*(P53+P54)+(P54*Q55-P55*Q54)*(P54+P55))/6/P58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(R58=0,0,(+(R47*S48-R48*S47)*(R47+R48)+(R48*S49-R49*S48)*(R48+R49)+(R49*S50-R50*S49)*(R49+R50)+(R50*S51-R51*S50)*(R50+R51)+(R51*S52-R52*S51)*(R51+R52))/6/R58)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(T58=0,0,(+(T47*U48-T48*U47)*(T47+T48)+(T48*U49-T49*U48)*(T48+T49)+(T49*U50-T50*U49)*(T49+T50)+(T50*U51-T51*U50)*(T50+T51)+(T51*U52-T52*U51)*(T51+T52)+(T52*U53-T53*U52)*(T52+T53)+(T53*U54-T54*U53)*(T53+T54)+(T54*U55-T55*U54)*(T54+T55)+(T55*U56-T56*U55)*(T55+T56)+(T56*U57-T57*U56)*(T56+T57))/6/T58)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(V58=0,0,-(+(V47*W48-V48*W47)*(V47+V48)+(V48*W49-V49*W48)*(V48+V49)+(V49*W50-V50*W49)*(V49+V50)+(V50*W51-V51*W50)*(V50+V51))/6/V58)","v":2.6739089419190427},"m",{"$f":"IF(X58=0,0,-(+(X47*Y48-X48*Y47)*(X47+X48)+(X48*Y49-X49*Y48)*(X48+X49)+(X49*Y50-X50*Y49)*(X49+X50)+(X50*Y51-X51*Y50)*(X50+X51))/6/X58)","v":3.7896651910602248},"m",{"$f":"-(+(Z47*AA48-Z48*AA47)*(Z47+Z48)+(Z48*AA49-Z49*AA48)*(Z48+Z49)+(Z49*AA50-Z50*AA49)*(Z49+Z50)+(Z50*AA51-Z51*AA50)*(Z50+Z51)+(Z51*AA52-Z52*AA51)*(Z51+Z52)+(Z52*AA53-Z53*AA52)*(Z52+Z53)+(Z53*AA54-Z54*AA53)*(Z53+Z54)+(Z54*AA55-Z55*AA54)*(Z54+Z55)+(Z55*AA56-Z56*AA55)*(Z55+Z56)+(Z56*AA57-Z57*AA56)*(Z56+Z57))/6/Z58","v":4.5407423692617748},"m",null,null,null,null,"   Koordinate presjeka",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AH47+AH48)+(AH48*AI49-AH49*AI48)*(AH48+AH49)+(AH49*AI50-AH50*AI49)*(AH49+AH50)+(AH50*AI51-AH51*AI50)*(AH50+AH51)+(AH51*AI52-AH52*AI51)*(AH51+AH52)+(AH52*AI53-AH53*AI52)*(AH52+AH53)+(AH53*AI54-AH54*AI53)*(AH53+AH54)+(AH54*AI55-AH55*AI54)*(AH54+AH55)+(AH55*AI56-AH56*AI55)*(AH55+AH56)+(AH56*AI57-AH57*AI56)*(AH56+AH57))/6/AH58","v":4.550001650000004},"m"]
["yt=",{"$f":"-((B45*C46-B46*C45)*(C45+C46)+(B46*C47-B47*C46)*(C46+C47)+(B47*C48-B48*C47)*(C47+C48)+(B48*C49-B49*C48)*(C48+C49)+(B49*C50-B50*C49)*(C49+C50)+(B50*C51-B51*C50)*(C50+C51)+(B51*C52-B52*C51)*(C51+C52)+(B52*C53-B53*C52)*(C52+C53)+(B53*C54-B54*C53)*(C53+C54)+(B54*C55-B55*C54)*(C54+C55)+(B55*C56-B56*C55)*(C55+C56)+(B56*C57-B57*C56)*(C56+C57))/6/B58","v":0.75054981042380386},"m",{"$f":"-((D45*E46-D46*E45)*(E45+E46)+(D46*E47-D47*E46)*(E46+E47)+(D47*E48-D48*E47)*(E47+E48)+(D48*E49-D49*E48)*(E48+E49)+(D49*E50-D50*E49)*(E49+E50)+(D50*E51-D51*E50)*(E50+E51)+(D51*E52-D52*E51)*(E51+E52)+(D52*E53-D53*E52)*(E52+E53)+(D53*E54-D54*E53)*(E53+E54)+(D54*E55-D55*E54)*(E54+E55)+(D55*E56-D56*E55)*(E55+E56)+(D56*E57-D57*E56)*(E56+E57))/6/D58","v":{"$error":"#VALUE!"}},"m",{"$f":"-((F45*G46-F46*G45)*(G45+G46)+(F46*G47-F47*G46)*(G46+G47)+(F47*G48-F48*G47)*(G47+G48)+(F48*G49-F49*G48)*(G48+G49)+(F49*G50-F50*G49)*(G49+G50)+(F50*G51-F51*G50)*(G50+G51)+(F51*G52-F52*G51)*(G51+G52)+(F52*G53-F53*G52)*(G52+G53)+(F53*G54-F54*G53)*(G53+G54)+(F54*G55-F55*G54)*(G54+G55)+(F55*G56-F56*G55)*(G55+G56)+(F56*G57-F57*G56)*(G56+G57))/6/F58","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(H47*I48-H48*I47)*(I47+I48)+(H48*I49-H49*I48)*(I48+I49)+(H49*I50-H50*I49)*(I49+I50)+(H50*I51-H51*I50)*(I50+I51)+(H51*I52-H52*I51)*(I51+I52)+(H52*I53-H53*I52)*(I52+I53)+(H53*I54-H54*I53)*(I53+I54)+(H54*I55-H55*I54)*(I54+I55)+(H55*I56-H56*I55)*(I55+I56)+(H56*I57-H57*I56)*(I56+I57))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(K47+K48)+(J48*K49-J49*K48)*(K48+K49)+(J49*K50-J50*K49)*(K49+K50)+(J50*K51-J51*K50)*(K50+K51)+(J51*K52-J52*K51)*(K51+K52)+(J52*K53-J53*K52)*(K52+K53)+(J53*K54-J54*K53)*(K53+K54)+(J54*K55-J55*K54)*(K54+K55)+(J55*K56-J56*K55)*(K55+K56)+(J56*K57-J57*K56)*(K56+K57))/6/J58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(L47*M48-L48*M47)*(M47+M48)+(L48*M49-L49*M48)*(M48+M49)+(L49*M50-L50*M49)*(M49+M50)+(L50*M51-L51*M50)*(M50+M51)+(L51*M52-L52*M51)*(M51+M52)+(L52*M53-L53*M52)*(M52+M53)+(L53*M54-L54*M53)*(M53+M54)+(L54*M55-L55*M54)*(M54+M55))/6/L58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(N58=0,0,(+(N47*O48-N48*O47)*(O47+O48)+(N48*O49-N49*O48)*(O48+O49)+(N49*O50-N50*O49)*(O49+O50)+(N50*O51-N51*O50)*(O50+O51)+(N51*O52-N52*O51)*(O51+O52)+(N52*O53-N53*O52)*(O52+O53)+(N53*O54-N54*O53)*(O53+O54)+(N54*O55-N55*O54)*(O54+O55)+(N55*O56-N56*O55)*(O55+O56)+(N56*O57-N57*O56)*(O56+O57))/6/N58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(P47*Q48-P48*Q47)*(Q47+Q48)+(P48*Q49-P49*Q48)*(Q48+Q49)+(P49*Q50-P50*Q49)*(Q49+Q50)+(P50*Q51-P51*Q50)*(Q50+Q51)+(P51*Q52-P52*Q51)*(Q51+Q52)+(P52*Q53-P53*Q52)*(Q52+Q53)+(P53*Q54-P54*Q53)*(Q53+Q54)+(P54*Q55-P55*Q54)*(Q54+Q55))/6/P58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(R58=0,0,(+(R47*S48-R48*S47)*(S47+S48)+(R48*S49-R49*S48)*(S48+S49)+(R49*S50-R50*S49)*(S49+S50)+(R50*S51-R51*S50)*(S50+S51)+(R51*S52-R52*S51)*(S51+S52)+(R52*S53-R53*S52)*(S52+S53)+(R53*S54-R54*S53)*(S53+S54)+(R54*S55-R55*S54)*(S54+S55)+(R55*S56-R56*S55)*(S55+S56)+(R56*S57-R57*S56)*(S56+S57))/6/R58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-IF(T58=0,0,(+(T47*U48-T48*U47)*(U47+U48)+(T48*U49-T49*U48)*(U48+U49)+(T49*U50-T50*U49)*(U49+U50)+(T50*U51-T51*U50)*(U50+U51)+(T51*U52-T52*U51)*(U51+U52)+(T52*U53-T53*U52)*(U52+U53)+(T53*U54-T54*U53)*(U53+U54)+(T54*U55-T55*U54)*(U54+U55)+(T55*U56-T56*U55)*(U55+U56)+(T56*U57-T57*U56)*(U56+U57))/6/T58)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((V47*W48-V48*W47)*(W47+W48)+(V48*W49-V49*W48)*(W48+W49)+(V49*W50-V50*W49)*(W49+W50)+(V50*W51-V51*W50)*(W50+W51))/6/V58","v":0.65809555436880718},"kN",{"$f":"-((X47*Y48-X48*Y47)*(Y47+Y48)+(X48*Y49-X49*Y48)*(Y48+Y49)+(X49*Y50-X50*Y49)*(Y49+Y50)+(X50*Y51-X51*Y50)*(Y50+Y51))/6/X58","v":0.75428136494691478},"kN",{"$f":"-(+(Z47*AA48-Z48*AA47)*(AA47+AA48)+(Z48*AA49-Z49*AA48)*(AA48+AA49)+(Z49*AA50-Z50*AA49)*(AA49+AA50)+(Z50*AA51-Z51*AA50)*(AA50+AA51)+(Z51*AA52-Z52*AA51)*(AA51+AA52)+(Z52*AA53-Z53*AA52)*(AA52+AA53)+(Z53*AA54-Z54*AA53)*(AA53+AA54)+(Z54*AA55-Z55*AA54)*(AA54+AA55)+(Z55*AA56-Z56*AA55)*(AA55+AA56)+(Z56*AA57-Z57*AA56)*(AA56+AA57))/6/Z58","v":0.81902934843133712},"m",null,null,null,null,"II-II i I-I",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AI47+AI48)+(AH48*AI49-AH49*AI48)*(AI48+AI49)+(AH49*AI50-AH50*AI49)*(AI49+AI50)+(AH50*AI51-AH51*AI50)*(AI50+AI51)+(AH51*AI52-AH52*AI51)*(AI51+AI52)+(AH52*AI53-AH53*AI52)*(AI52+AI53)+(AH53*AI54-AH54*AI53)*(AI53+AI54)+(AH54*AI55-AH55*AI54)*(AI54+AI55)+(AH55*AI56-AH56*AI55)*(AI55+AI56)+(AH56*AI57-AH57*AI56)*(AI56+AI57))/6/AH58","v":1.3500505000000005},"m"]
["G=",{"$f":"+B58*'Analiza i dimenzioniranje'!E62","v":64.227611992767947},"kN",{"$f":"+D58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"+F58*'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}},"kN",{"$f":"+H58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(J58*'Analiza i dimenzioniranje'!E63<0,0,J58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+L58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(N58*'Analiza i dimenzioniranje'!U41<0,0,N58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+P58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(R58<=0,0,R58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+T58*'Analiza i dimenzioniranje'!E49","v":{"$error":"#VALUE!"}},"kN (za L)",{"$f":"+V58*'Analiza i dimenzioniranje'!E62","v":37.77589163555291},"kN",{"$f":"+X58*'Analiza i dimenzioniranje'!E62","v":17.793104363851846},"kN",{"$f":"+Z58*'Analiza i dimenzioniranje'!E62","v":13.306056250595223},"kN",null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"AC47+'Analiza i dimenzioniranje'!C192/2","v":0.68753317931068247},{"$f":"+AH58*'Analiza i dimenzioniranje'!E62","v":5.2517757527774878},"kN"]
["Vertikala nasipa na konzoli",null,null,"Moment na konzoli",null,"Pokos na vrhu zida",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - NAPONI ",null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+'C XIV-XV'!AC49+('Analiza i dimenzioniranje'!C191/2)","v":0.77418208680245293}]
[null,"x","y",{"$f":"IF('Analiza i dimenzioniranje'!G78=0,0,'Analiza i dimenzioniranje'!G78*'Analiza i dimenzioniranje'!C77*'Analiza i dimenzioniranje'!E62*(Q20-B5+'Analiza i dimenzioniranje'!G78/2)+J61*(O16-J59))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"+F64","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"naponi za presjek II-II",null,"naponi za srednji dio ",null,"naponi za presjek I-I"]
[null,{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},"b1=",{"$f":"+H47-2","v":1.4000010999999999},{"$f":"+B52","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y","x","y","x","y","Koordinate dna temelja"]
[null,{"$f":"+B64","v":{"$error":"#VALUE!"}},{"$f":"IF(B65>J49,C19,+C20+'Analiza i dimenzioniranje'!F20+(H52-H50)*TAN('Analiza i dimenzioniranje'!F21*PI()/180))","v":{"$error":"#VALUE!"}},"b2=",{"$f":"'Analiza i dimenzioniranje'!E54+('Analiza i dimenzioniranje'!E55-'Analiza i dimenzioniranje'!E54)*(('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)/(C9-C4))","v":{"$error":"#VALUE!"}},{"$f":"+B65","v":{"$error":"#VALUE!"}},{"$f":"+G64+(F64-F65)*TAN('Analiza i dimenzioniranje'!F21*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,0,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},0,{"$f":"+'C XIV-XV'!B11","v":4.2000010999999997},{"$f":"-U47","v":0},2,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z65","v":2},{"$f":"AC55","v":{"$error":"#VALUE!"}},{"$f":"+AB65","v":3.4000010999999999},{"$f":"+AA67","v":{"$error":"#VALUE!"}},{"$f":"+AB57","v":4.2000010999999997},{"$f":"AC57","v":{"$error":"#VALUE!"}},{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"(AF66*(AG70-AG65)/(AF70-AF65)-AF65*(AG70-AG65)/(AF70-AF65)+AG65)","v":{"$error":"#VALUE!"}}]
[null,"AKTIVNI TLAKOVI za stabilnost i Presjek III-III (bez E3)",null,null,null,null,null,null,"  AKTIVNI TLAKOVI za presjek kroz zid XIV-XIV",null,null,null,null,"    AKTIVNI TLAKOVI za presjek kroz zid XV-XV",null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"AC56","v":{"$error":"#VALUE!"}},{"$f":"+AB66+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AE66","v":{"$error":"#VALUE!"}},{"$f":"+AB58","v":4.9000021999999994},{"$f":"+AC58","v":{"$error":"#VALUE!"}},{"$f":"+AB77","v":{"$error":"#VALUE!"}},{"$f":"+(AF67*(AG65-AG70)/(AF65-AF70)-AF70*(AG65-AG70)/(AF65-AF70)+AG70)","v":{"$error":"#VALUE!"}}]
[null,"E1",null,"E2",null,"E3",null,null,"E1",null,"E2 do presjeka kroz zid II",null,null,"E1",null,"E2",null,null,null,null,null,null,null,null,null,{"$f":"+Z67","v":3.4000010999999999},0,{"$f":"+AB67","v":4.2000010999999997},0,{"$f":"+AD67","v":4.9000021999999994},{"$f":"+U50","v":0},{"$f":"+AB67","v":4.2000010999999997},{"$f":"+(AF68*(AG65-AG70)/(AF65-AF70)-AF70*(AG65-AG70)/(AF65-AF70)+AG70)","v":0.37931024673015767}]
[null,0,{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C71","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,{"$f":"+N69","v":0},{"$f":"+O69","v":{"$error":"#VALUE!"}},{"$f":"+I71","v":{"$error":"#VALUE!"}},{"$f":"+J71","v":{"$error":"#VALUE!"}},null,{"$f":"+B69","v":0},{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+N71","v":{"$error":"#VALUE!"}},{"$f":"+O71","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"+Z65","v":2},0,{"$f":"+AB65","v":3.4000010999999999},0,{"$f":"+AD65","v":4.2000010999999997},{"$f":"+U51","v":0},{"$f":"+AD77","v":{"$error":"#VALUE!"}},{"$f":"+(AF69*(AG66-AG70)/(AF66-AF70)-AF70*(AG66-AG70)/(AF66-AF70)+AG70)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+B69","v":0},{"$f":"+C69-'Analiza i dimenzioniranje'!D17-'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+D69+'Analiza i dimenzioniranje'!E16*'Analiza i dimenzioniranje'!E17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+E69-'Analiza i dimenzioniranje'!E17","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},null,{"$f":"+N70","v":0},{"$f":"+J69-('Analiza i dimenzioniranje'!F20+'P XIV-XIV'!E17)","v":{"$error":"#VALUE!"}},{"$f":"+K69+'P XIV-XIV'!F16*'P XIV-XIV'!F17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},null,{"$f":"+B70","v":0},{"$f":"+O69-('Analiza i dimenzioniranje'!F20+'P XV-XV'!E17)","v":{"$error":"#VALUE!"}},{"$f":"+P69+'P XV-XV'!F16*'P XV-XV'!F17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AB53","v":4.9000021999999994},{"$f":"+AC53","v":0.5}]
[null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('Analiza i dimenzioniranje'!D17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},0,{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F70+'Analiza i dimenzioniranje'!F16*'Analiza i dimenzioniranje'!F17*'Analiza i dimenzioniranje'!F112","v":{"$error":"#VALUE!"}},0,null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('P XIV-XIV'!E17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+J70","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+L70","v":4.08},null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('P XV-XV'!E17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+Q70","v":4.4000000000000004}]
[null,{"$f":"+B69","v":0},{"$f":"+C69","v":{"$error":"#VALUE!"}},0,{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F69","v":0},0,null,{"$f":"+N72","v":0},{"$f":"+O72","v":{"$error":"#VALUE!"}},{"$f":"+D72","v":0},{"$f":"+L69","v":{"$error":"#VALUE!"}},null,{"$f":"+N69","v":0},{"$f":"+O69","v":{"$error":"#VALUE!"}},{"$f":"+D72","v":0},{"$f":"+Q69","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+D69","v":{"$error":"#VALUE!"}},{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F72","v":0},{"$f":"+G70","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+K69","v":{"$error":"#VALUE!"}},{"$f":"+L69","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+P69","v":{"$error":"#VALUE!"}},{"$f":"+Q69","v":{"$error":"#VALUE!"}}]
["Jednadžba vertikale kohezije    Određivanje sjecišta kohezije s pravcem od tlaka",null,null,null,null,null,null,{"$f":"+M74","v":"Jednadžba vertikale kohezije  -  sjecišta kohezije s pravcem od tlaka"},null,null,null,null,"Jednadžba vertikale kohezije  -  sjecišta kohezije s pravcem od tlaka"]
[null,"X","y","X","y","X","y",null,{"$f":"+N75","v":"X"},{"$f":"+O75","v":"y"},"X","y",null,"X","y","X","y"]
[null,{"$f":"2*'Analiza i dimenzioniranje'!D15/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F110)","v":12.361875887090893},{"$f":"B76*(C71-C72)/(B71-B72)-B72*(C71-C72)/(B71-B72)+C72","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!F12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F111)","v":{"$error":"#VALUE!"}},{"$f":"IF(D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69>'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69)","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!C12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F112)","v":{"$error":"#VALUE!"}},{"$f":"IF((F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70)>'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!F17,(F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70))","v":{"$error":"#VALUE!"}},null,{"$f":"+N76","v":12.361875887090893},{"$f":"I76*(J71-J72)/(I71-I72)-I72*(J71-J72)/(I71-I72)+J72","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},null,{"$f":"+B76","v":12.361875887090893},{"$f":"N76*(O71-O72)/(N71-N72)-N72*(O71-O72)/(N71-N72)+O72","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+L76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"-0.5*((Z65*AA66-Z66*AA65)+(Z66*AA67-Z67*AA66)+(Z67*AA68-Z68*AA67)+(Z68*AA69-Z69*AA68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((AB65*AC66-AB66*AC65)+(AB66*AC67-AB67*AC66)+(AB67*AC68-AB68*AC67)+(AB68*AC69-AB69*AC68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((AD65*AE66-AD66*AE65)+(AD66*AE67-AD67*AE66)+(AD67*AE68-AD68*AE67)+(AD68*AE69-AD69*AE68)+(AD69*AE70-AD70*AE69)+(AD70*AE71-AD71*AE70)+(AD71*AE72-AD72*AE71)+(AD72*AE73-AD73*AE72))","v":{"$error":"#VALUE!"}},"kN/m'"]
[null,{"$f":"+B76","v":12.361875887090893},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},null,{"$f":"+N77","v":12.361875887090893},{"$f":"+O77","v":{"$error":"#VALUE!"}},{"$f":"+K76","v":{"$error":"#VALUE!"}},{"$f":"+L70","v":4.08},null,{"$f":"+N76","v":12.361875887090893},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+P76","v":{"$error":"#VALUE!"}},{"$f":"+Q70","v":4.4000000000000004},null,null,null,null,null,null,null,null,{"$f":"IF(Z76=0,0,-(+(Z65*AA66-Z66*AA65)*(Z65+Z66)+(Z66*AA67-Z67*AA66)*(Z66+Z67)+(Z67*AA68-Z68*AA67)*(Z67+Z68)+(Z68*AA69-Z69*AA68)*(Z68+Z69))/6/Z76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(AB76=0,0,-(+(AB65*AC66-AB66*AC65)*(AB65+AB66)+(AB66*AC67-AB67*AC66)*(AB66+AB67)+(AB67*AC68-AB68*AC67)*(AB67+AB68)+(AB68*AC69-AB69*AC68)*(AB68+AB69))/6/AB76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(AD76=0,0,-(+(AD65*AE66-AD66*AE65)*(AD65+AD66)+(AD66*AE67-AD67*AE66)*(AD66+AD67)+(AD67*AE68-AD68*AE67)*(AD67+AD68)+(AD68*AE69-AD69*AE68)*(AD68+AD69))/6/AD76)","v":{"$error":"#VALUE!"}},"m"]
["Oznaka","E1",null,"E2",null,"E3",null,{"$f":"+M78","v":"Oznaka"},{"$f":"+N78","v":"E1"},null,"E2",null,"Oznaka","E1",null,"E2",null,null,null,null,null,null,null,null,null,{"$f":"-((Z65*AA66-Z66*AA65)*(AA65+AA66)+(Z66*AA67-Z67*AA66)*(AA66+AA67)+(Z67*AA68-Z68*AA67)*(AA67+AA68)+(Z68*AA69-Z69*AA68)*(AA68+AA69))/6/Z76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((AB65*AC66-AB66*AC65)*(AC65+AC66)+(AB66*AC67-AB67*AC66)*(AC66+AC67)+(AB67*AC68-AB68*AC67)*(AC67+AC68)+(AB68*AC69-AB69*AC68)*(AC68+AC69))/6/AB76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((AD65*AE66-AD66*AE65)*(AE65+AE66)+(AD66*AE67-AD67*AE66)*(AE66+AE67)+(AD67*AE68-AD68*AE67)*(AE67+AE68)+(AD68*AE69-AD69*AE68)*(AE68+AE69))/6/AD76","v":{"$error":"#VALUE!"}},"kN/m'"]
["točke","x","y","x","y","x","y","točke",{"$f":"+N79","v":"x"},{"$f":"+O79","v":"y"},"x","y","točke","x","y","x","y"]
[1,{"$f":"+B77","v":12.361875887090893},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,1,{"$f":"+N80","v":12.361875887090893},{"$f":"+J76","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+L76","v":{"$error":"#VALUE!"}},1,12.361875887090893,{"$f":"+O77","v":{"$error":"#VALUE!"}},{"$f":"+P76","v":{"$error":"#VALUE!"}},{"$f":"+Q76","v":{"$error":"#VALUE!"}},null,"Jedn pravca zida uz tlo",null,"Jedn pravca arm dno ",null,"Y=",{"$f":"IF(S82=S81,1000000,(T82-T81)/(S82-S81))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X80*S81+T81","v":{"$error":"#VALUE!"}}]
[2,{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G76","v":{"$error":"#VALUE!"}},2,{"$f":"+I71","v":{"$error":"#VALUE!"}},{"$f":"+J71","v":{"$error":"#VALUE!"}},{"$f":"IF(E76<E73,D76,I81)","v":{"$error":"#VALUE!"}},{"$f":"+L76","v":{"$error":"#VALUE!"}},2,{"$f":"+N71","v":{"$error":"#VALUE!"}},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+P80","v":{"$error":"#VALUE!"}},{"$f":"+Q80","v":{"$error":"#VALUE!"}},null,{"$f":"+B4","v":3.4000010999999999},{"$f":"+C4","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!T593","v":2.0499999999999998},{"$f":"+'Analiza i dimenzioniranje'!U593","v":0.18682583433163008},"X=",{"$f":"+(-Z80+Z83)/(X80-X83)","v":{"$error":"#VALUE!"}},"sjeište"]
[3,{"$f":"+B80","v":12.361875887090893},{"$f":"+C76","v":{"$error":"#VALUE!"}},{"$f":"IF(D76>D69,D81,D69)","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},{"$f":"IF(F77>F70,F77,F70)","v":{"$error":"#VALUE!"}},{"$f":"IF(F77>F70,G76,G70)","v":{"$error":"#VALUE!"}},3,{"$f":"+N82","v":12.361875887090893},{"$f":"+J81","v":{"$error":"#VALUE!"}},{"$f":"+K70","v":{"$error":"#VALUE!"}},{"$f":"+L77","v":4.08},3,{"$f":"+N80","v":12.361875887090893},{"$f":"+O76","v":{"$error":"#VALUE!"}},{"$f":"+P70","v":{"$error":"#VALUE!"}},{"$f":"+Q70","v":4.4000000000000004},null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},{"$f":"+'Analiza i dimenzioniranje'!T594","v":4.8600021999999994},{"$f":"+'Analiza i dimenzioniranje'!U594","v":0.54310345350772504},"Y=",{"$f":"+X80*X81+Z80","v":{"$error":"#VALUE!"}}]
[4,{"$f":"+B80","v":12.361875887090893},{"$f":"+C80","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F71","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},4,{"$f":"+N83","v":12.361875887090893},{"$f":"+J80","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17<'Analiza i dimenzioniranje'!Z44,0,K76)","v":{"$error":"#VALUE!"}},{"$f":"+L70","v":4.08},4,{"$f":"+N80","v":12.361875887090893},{"$f":"+O80","v":{"$error":"#VALUE!"}},{"$f":"+P80","v":{"$error":"#VALUE!"}},{"$f":"+Q82","v":4.4000000000000004},null,null,null,null,null,"Y=",{"$f":"+(V82-V81)/(U82-U81)","v":0.12678908905341604},"*x",{"$f":"-X83*U81+V81","v":-7.3091798227872762E-2},"CRTANJE"]
[5,null,null,{"$f":"+D80","v":{"$error":"#VALUE!"}},{"$f":"+E80","v":{"$error":"#VALUE!"}},{"$f":"+F80","v":{"$error":"#VALUE!"}},{"$f":"+G80","v":0},5,null,null,{"$f":"+K80","v":{"$error":"#VALUE!"}},{"$f":"+L80","v":{"$error":"#VALUE!"}},5,null,null,{"$f":"+P80","v":{"$error":"#VALUE!"}},{"$f":"+Q80","v":{"$error":"#VALUE!"}},null,"Jedn pravca sloja 3",null,"Jedn pravca sloja 3 klizno",null,"Y=",{"$f":"+(T86-T85)/(S86-S85)","v":-3.4920769491747737E-2},"*x",{"$f":"-X84*S85+T85","v":1.2698415389834954},"Jedn pravca sloja 3 klizno",null,"sjecište 1/2 sidra sa vrhom 1. sloja"]
["  A=",{"$f":"IF(B77>B71,0,-IF(B84>B83,0,-0.5*((B80*C81-B81*C80)+(B81*C82-B82*C81)+(B82*C83-B83*C82)+(B83*C84-B84*C83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D77>D70,0,IF(D84>D83,0,-0.5*((D80*E81-D81*E80)+(D81*E82-D82*E81)+(D82*E83-D83*E82)+(D83*E84-D84*E83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F77>F71,0,IF(F84>F83,0,-0.5*((F80*G81-F81*G80)+(F81*G82-F82*G81)+(F82*G83-F83*G82)+(F83*G84-F84*G83))))","v":{"$error":"#VALUE!"}},"kN/m'","  A=",{"$f":"IF(I77>I71,0,IF(I84>I83,0,-0.5*((I80*J81-I81*J80)+(I81*J82-I82*J81)+(I82*J83-I83*J82)+(I83*J84-I84*J83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(L77>L76,0,IF(K84>K83,0,-0.5*((K80*L81-K81*L80)+(K81*L82-K82*L81)+(K82*L83-K83*L82)+(K83*L84-K84*L83))))","v":{"$error":"#VALUE!"}},"kN/m'","  A=",{"$f":"IF(O77>O76,0,IF(-0.5*((N80*O81-N81*O80)+(N81*O82-N82*O81)+(N82*O83-N83*O82)+(N83*O84-N84*O83))<0,0.5*((N80*O81-N81*O80)+(N81*O82-N82*O81)+(N82*O83-N83*O82)+(N83*O84-N84*O83)),0))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(Q77>Q76,0,-0.5*((P80*Q81-P81*Q80)+(P81*Q82-P82*Q81)+(P82*Q83-P83*Q82)+(P83*Q84-P84*Q83)))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+U18","v":2},{"$f":"+V18","v":1.2},{"$f":"+W100","v":2},0,"X=",{"$f":"+(-Z84+Z87)/(X84-X87)","v":1.1386903959986558},"sjecište ",null,{"$f":"+U85","v":2},{"$f":"+V85","v":0},"Y=",{"$f":"+X92","v":{"$error":"#VALUE!"}},"*x",{"$f":"+Z92","v":{"$error":"#VALUE!"}}]
["xt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(B80+B81)+(B81*C82-B82*C81)*(B81+B82)+(B82*C83-B83*C82)*(B82+B83)+(B83*C84-B84*C83)*(B83+B84))/6/B85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(D80+D81)+(D81*E82-D82*E81)*(D81+D82)+(D82*E83-D83*E82)*(D82+D83)+(D83*E84-D84*E83)*(D83+D84))/6/D85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(F80+F81)+(F81*G82-F82*G81)*(F81+F82)+(F82*G83-F83*G82)*(F82+F83)+(F83*G84-F84*G83)*(F83+F84))/6/F85)","v":{"$error":"#VALUE!"}},"kN/m'","xt=",{"$f":"IF(I85=0,0,-+((I80*J81-I81*J80)*(I80+I81)+(I81*J82-I82*J81)*(I81+I82)+(I82*J83-I83*J82)*(I82+I83)+(I83*J84-I84*J83)*(I83+I84))/6/I85)","v":{"$error":"#VALUE!"}},{"$f":"+O86","v":"kN/m'"},{"$f":"IF(K85=0,0,((K80*L83-K83*L80)*(K80+K83)+(K83*L82-K82*L83)*(K83+K82)+(K82*L81-K81*L82)*(K82+K81)+(K81*L84-K84*L81)*(K81+K84))/6/K85)","v":{"$error":"#VALUE!"}},"kN/m'","xt=",{"$f":"IF(N85=0,0,((N80*O81-N81*O80)*(N80+N81)+(N81*O82-N82*O81)*(N81+N82)+(N82*O83-N83*O82)*(N82+N83)+(N83*O84-N84*O83)*(N83+N84))/6/N85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(P85=0,0,-((P80*Q81-P81*Q80)*(P80+P81)+(P81*Q82-P82*Q81)*(P81+P82)+(P82*Q83-P83*Q82)*(P82+P83)+(P83*Q84-P84*Q83)*(P83+P84))/6/P85)","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+U19","v":-8},{"$f":"+V19","v":1.5492076949174773},-5,{"$f":"+V85+(U85-U86)*TAN((45+'Analiza i dimenzioniranje'!F14/2)*PI()/180)","v":9.9970360471948005},"Y=",{"$f":"+X84*X85+Z84","v":1.2300775941423594},3,null,{"$f":"+X85","v":1.1386903959986558},{"$f":"+X86","v":1.2300775941423594}]
["yt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(C80+C81)+(B81*C82-B82*C81)*(C81+C82)+(B82*C83-B83*C82)*(C82+C83)+(B83*C84-B84*C83)*(C83+C84))/6/B85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(E80+E81)+(D81*E82-D82*E81)*(E81+E82)+(D82*E83-D83*E82)*(E82+E83)+(D83*E84-D84*E83)*(E83+E84))/6/D85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(G80+G81)+(F81*G82-F82*G81)*(G81+G82)+(F82*G83-F83*G82)*(G82+G83)+(F83*G84-F84*G83)*(G83+G84))/6/F85)","v":{"$error":"#VALUE!"}},"m","yt=",{"$f":"IF(I85=0,0,-((I80*J81-I81*J80)*(J80+J81)+(I81*J82-I82*J81)*(J81+J82)+(I82*J83-I83*J82)*(J82+J83)+(I83*J84-I84*J83)*(J83+J84))/6/I85)","v":{"$error":"#VALUE!"}},{"$f":"+O87","v":"m"},{"$f":"IF(K85=0,0,((K80*L83-K83*L80)*(L80+L83)+(K83*L82-K82*L83)*(L83+L82)+(K82*L81-K81*L82)*(L82+L81)+(K81*L84-K84*L81)*(L81+L84))/6/K85)","v":{"$error":"#VALUE!"}},"m","yt=",{"$f":"IF(N85=0,0,((N80*O81-N81*O80)*(O80+O81)+(N81*O82-N82*O81)*(O81+O82)+(N82*O83-N83*O82)*(O82+O83)+(N83*O84-N84*O83)*(O83+O84))/6/N85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(P85=0,0,-((P80*Q81-P81*Q80)*(Q80+Q81)+(P81*Q82-P82*Q81)*(Q81+Q82)+(P82*Q83-P83*Q82)*(Q82+Q83)+(P83*Q84-P84*Q83)*(Q83+Q84))/6/P85)","v":{"$error":"#VALUE!"}},"m",null,null,null,null,null,"Y=",{"$f":"+(V86-V85)/(U86-U85)","v":-1.4281480067421144},"*x",{"$f":"-X87*U85+V85","v":2.8562960134842288},"y=2       x=",{"$f":"+('Analiza i dimenzioniranje'!E52-'C XIV-XV'!Z87)/'C XIV-XV'!X87","v":1.1597509541483482}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(K85<0,0,K85)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+IF(P85<0,0,P85)","v":{"$error":"#VALUE!"}},null,null,"Jedn pravca sloja 2",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(T90-T89)/(S90-S89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X88*S89+T89","v":{"$error":"#VALUE!"}},"Jedn pravca sloja 2 klizno",null,"Jednadžba pravca sidra",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(AD90-AD89)/(AC90-AC89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AH88*AC89+AD89","v":{"$error":"#VALUE!"}}]
["X koordinata položaja rezultante aktivnog tlaka na stražnjoj strani zida za  Ev1, Ev2 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U15","v":{"$error":"#VALUE!"}},{"$f":"+V15","v":4},{"$f":"+X85","v":1.1386903959986558},{"$f":"+X86","v":1.2300775941423594},"X=",{"$f":"+(-Z88+Z91)/(X88-X91)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U89","v":1.1386903959986558},{"$f":"+V89","v":1.2300775941423594},{"$f":"+U37","v":{"$error":"#VALUE!"}},{"$f":"+V37","v":5},{"$f":"+U89","v":1.1386903959986558},{"$f":"+V89","v":1.2300775941423594},"X=",{"$f":"+(-AJ88+AJ91)/(AH88-AH91)","v":{"$error":"#VALUE!"}},"sjecište"]
["Jednadžba pravca zida uz tlo",null,null,null,null,"Za Ev3 x=2",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U16","v":-8},{"$f":"+V16","v":{"$error":"#VALUE!"}},-5,{"$f":"+V89+(U89-U90)*TAN((45+'Analiza i dimenzioniranje'!E14/2)*PI()/180)","v":9.6792600705649363},"Y=",{"$f":"+X88*X89+Z88","v":{"$error":"#VALUE!"}},2,null,{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},{"$f":"+U38","v":{"$error":"#VALUE!"}},{"$f":"+V38","v":{"$error":"#VALUE!"}},{"$f":"+U90","v":-5},{"$f":"+V90","v":9.6792600705649363},"Y=",{"$f":"+AH88*AH89+AJ88","v":{"$error":"#VALUE!"}},2]
[null,"E1",null,"E2",null,"E3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(V90-V89)/(U90-U89)","v":-1.3763819204711731},"*x",{"$f":"-X91*U89+V89","v":2.79735046820907},null,null,null,null,null,null,"Y=",{"$f":"+(AF90-AF89)/(AE90-AE89)","v":-1.3763819204711731},"*x",{"$f":"-AH91*AE89+AF89","v":2.79735046820907}]
["x","y","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,"Jedn pravca sloja 1",null,null,null,"Y=",{"$f":"+(T95-T94)/(S95-S94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X92*S94+T94","v":{"$error":"#VALUE!"}},"Jedan pravca sloja 1 klizno",null,"Slobodna dionica ls>=",{"$f":"+SQRT((AC94-AC93)*(AC94-AC93)+(AD94-AD93)*(AD94-AD93))","v":{"$error":"#VALUE!"}}]
[{"$f":"+(B8-B4)*(B93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+B87","v":{"$error":"#VALUE!"}},{"$f":"+(B8-B4)*(D93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+D87","v":{"$error":"#VALUE!"}},2,{"$f":"+F87","v":{"$error":"#VALUE!"}},null,{"$f":"+(B8-B4)*(I93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+N87","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+(B8-B4)*(N93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+I87","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+V7","v":"A"},null,null,"X=",{"$f":"+(-Z92+Z95)/(X92-X95)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U94","v":{"$error":"#VALUE!"}},{"$f":"+V94","v":{"$error":"#VALUE!"}},{"$f":"+AC89","v":{"$error":"#VALUE!"}},{"$f":"+AD89","v":5}]
[null,null,null,null,"Sloj2",{"$f":"+(B8-B4)*(G94-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!V15","v":4},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U8","v":{"$error":"#VALUE!"}},{"$f":"+V8","v":6},{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+X92*X93+Z92","v":{"$error":"#VALUE!"}},1,null,{"$f":"+X93","v":{"$error":"#VALUE!"}},{"$f":"+X94","v":{"$error":"#VALUE!"}},{"$f":"+AH89","v":{"$error":"#VALUE!"}},{"$f":"+AH90","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+(B8-B4)*(G95-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+K21","v":1.2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782},-5,{"$f":"+V94+(U94-U95)*TAN((45+'Analiza i dimenzioniranje'!D14/2)*PI()/180)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+(V95-V94)/(U95-U94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X95*U94+V94","v":{"$error":"#VALUE!"}},{"$f":"+(AB95-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(AB96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+(AD96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Masa unutar kliznog tijela - za potres",null,"POTRES",null,"x","y","x","y","x","y",null,null,null,null,"Masa za potres s prosjekom kontrafore i bez kontrafora"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+(B9-B4)*(AD98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"+(B9-B4)*(AF98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B2","v":2},0.12820515121628623,null,null,{"$f":"+(Z95-AB99)/(-X91)","v":{"$error":"#VALUE!"}},{"$f":"+AB98","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!AD44>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'C XIV-XV'!AC96,(Z91-AD99)/(-X91))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"IF('Analiza i dimenzioniranje'!AE44>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'C XIV-XV'!AA96,(Z91-AF99)/(-X91))","v":{"$error":"#VALUE!"}},{"$f":"+AF98","v":4.4000000000000004}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,1.2,"Potresna sila za stabilnost",null,"Klizno tijelo za potres za presjek III-III",null,"Klizno tijelo za potres za presjek XIV-XIV",null,"Klizno tijelo za potres za presjek  XV-XV",null,null,null,null,null,"Potresna sila za stabilnost "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.4000010999999999,1.2,{"$f":"+'C XII-XIII'!Y101","v":1.75},{"$f":"+'C XII-XIII'!Z101","v":9.6153895463470418E-2},null,null,{"$f":"+AC98","v":{"$error":"#VALUE!"}},{"$f":"+AD98","v":4.08},{"$f":"+AE98","v":{"$error":"#VALUE!"}},{"$f":"+AF98","v":4.4000000000000004},null,null,null,null,{"$f":"+'C III-V'!Y101","v":1.75},{"$f":"+'C III-V'!Z101","v":9.6153895463470418E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.14,{"$f":"+'C XII-XIII'!Y102","v":0.97707863658009864},{"$f":"+'C XII-XIII'!Z102","v":1.2},{"$f":"+'C XII-XIII'!AA102","v":0.97707863658009864},{"$f":"+'C XII-XIII'!AB102","v":1.2},{"$f":"+AN128","v":-1.1133852506716102},{"$f":"+AO128","v":4.08},{"$f":"+AN129","v":-1.3379644860184032},{"$f":"+AO129","v":4.4000000000000004},null,null,null,null,{"$f":"+'C III-V'!Y102","v":0.97707863658009864},{"$f":"+'C III-V'!Z102","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.14,{"$f":"+'C XII-XIII'!Y103","v":-1.0572404418349119},{"$f":"+'C XII-XIII'!Z103","v":4},{"$f":"+Y103","v":-1.0572404418349119},{"$f":"+Z103","v":4},{"$f":"IF(AD103=AD102,AC102,+AA103)","v":-1.1133852506716102},{"$f":"IF($AH$105<=AD102,AD102,$AH$105)","v":4.08},{"$f":"IF(AF103=AF102,AE102,+AC103)","v":-1.3379644860184032},{"$f":"IF($AH$105<=AF102,AF102,$AH$105)","v":4.4000000000000004},null,null,null,null,{"$f":"+'C III-V'!Y103","v":-1.0572404418349119},{"$f":"+'C III-V'!Z103","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.44,{"$f":"+'C XII-XIII'!Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!Z104","v":{"$error":"#VALUE!"}},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+AB104","v":{"$error":"#VALUE!"}},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+'C III-V'!Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z104","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.44,{"$f":"+'C XII-XIII'!Y105","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!Z105","v":6.2644906473896782},{"$f":"+Y105","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!AB105","v":6.2644906473896782},{"$f":"+AA105","v":{"$error":"#VALUE!"}},{"$f":"IF(AA105=AC105,AB105,AB95)","v":{"$error":"#VALUE!"}},{"$f":"+AC105","v":{"$error":"#VALUE!"}},{"$f":"+IF(AA105=AE105,AB105,AB95)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AM105","v":" H="},{"$f":"+'C III-V'!AN105","v":4},null,null,{"$f":"+'C III-V'!Y105","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z105","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},"A",{"$f":"+'C XII-XIII'!Y106","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!Z106","v":6},{"$f":"+'C XII-XIII'!AA106","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!AB106","v":6},{"$f":"+AE106","v":{"$error":"#VALUE!"}},{"$f":"+AF106","v":6},{"$f":"+AA106","v":{"$error":"#VALUE!"}},{"$f":"+AB106","v":6},null,null,null,null,{"$f":"+'C III-V'!Y106","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z106","v":6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},"A",{"$f":"+'C XII-XIII'!Y107","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!Z107","v":6},{"$f":"+'C XII-XIII'!AA107","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!AB107","v":6},{"$f":"+AE107","v":{"$error":"#VALUE!"}},{"$f":"+AF107","v":6},{"$f":"+AA107","v":{"$error":"#VALUE!"}},{"$f":"+AB107","v":6},null,null,null,null,{"$f":"+'C III-V'!Y107","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z107","v":6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+W107","v":{"$error":"#VALUE!"}},{"$f":"+X107","v":"A"},{"$f":"+'C XII-XIII'!Y108","v":3.4000000999999997},{"$f":"+'C XII-XIII'!Z108","v":1.2},{"$f":"+'C XII-XIII'!AA108","v":3.4000000999999997},{"$f":"+'C XII-XIII'!AB108","v":1.2},{"$f":"+AC109","v":{"$error":"#VALUE!"}},{"$f":"+AD109","v":4.08},{"$f":"+AE109","v":{"$error":"#VALUE!"}},{"$f":"+AF109","v":4.4000000000000004},null,null,null,null,{"$f":"+'C III-V'!Y108","v":3.4000000999999997},{"$f":"+'C III-V'!Z108","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B11","v":4.2000010999999997},1.2,{"$f":"+'C XII-XIII'!Y109","v":1.75},{"$f":"+'C XII-XIII'!Z109","v":1.2},{"$f":"+'C XII-XIII'!AA109","v":0.97707863658009864},{"$f":"+'C XII-XIII'!AB109","v":1.2},{"$f":"+AC98","v":{"$error":"#VALUE!"}},{"$f":"+AD98","v":4.08},{"$f":"+AE101","v":{"$error":"#VALUE!"}},{"$f":"+AF101","v":4.4000000000000004},null,null,null,null,{"$f":"+'C III-V'!Y109","v":1.75},{"$f":"+'C III-V'!Z109","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2000010999999997,1.2,{"$f":"+'C XII-XIII'!Y110","v":1.75},{"$f":"+'C XII-XIII'!Z110","v":9.6153895463470418E-2},null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!Y110","v":1.75},{"$f":"+'C III-V'!Z110","v":9.6153895463470418E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2000010999999997,1.2,{"$f":"-0.5*((Y101*Z102-Y102*Z101)+(Y102*Z103-Y103*Z102)+(Y103*Z104-Y104*Z103)+(Y104*Z105-Y105*Z104)+(Y105*Z106-Y106*Z105)+(Y106*Z107-Y107*Z106)+(Y107*Z108-Y108*Z107)+(Y108*Z109-Y109*Z108)+(Y109*Z110-Y110*Z109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AA101*AB102-AA102*AB101)+(AA102*AB103-AA103*AB102)+(AA103*AB104-AA104*AB103)+(AA104*AB105-AA105*AB104)+(AA105*AB106-AA106*AB105)+(AA106*AB107-AA107*AB106)+(AA107*AB108-AA108*AB107)+(AA108*AB109-AA109*AB108)+(AA109*AB110-AA110*AB109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AC101*AD102-AC102*AD101)+(AC102*AD103-AC103*AD102)+(AC103*AD104-AC104*AD103)+(AC104*AD105-AC105*AD104)+(AC105*AD106-AC106*AD105)+(AC106*AD107-AC107*AD106)+(AC107*AD108-AC108*AD107)+(AC108*AD109-AC109*AD108)+(AC109*AD110-AC110*AD109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AE101*AF102-AE102*AF101)+(AE102*AF103-AE103*AF102)+(AE103*AF104-AE104*AF103)+(AE104*AF105-AE105*AF104)+(AE105*AF106-AE106*AF105)+(AE106*AF107-AE107*AF106)+(AE107*AF108-AE108*AF107)+(AE108*AF109-AE109*AF108)+(AE109*AF110-AE110*AF109))","v":{"$error":"#VALUE!"}},"m2",null,null,null,null,{"$f":"-0.5*((AK101*AL102-AK102*AL101)+(AK102*AL103-AK103*AL102)+(AK103*AL104-AK104*AL103)+(AK104*AL105-AK105*AL104)+(AK105*AL106-AK106*AL105)+(AK106*AL107-AK107*AL106)+(AK107*AL108-AK108*AL107)+(AK108*AL109-AK109*AL108)+(AK109*AL110-AK110*AL109))","v":{"$error":"#VALUE!"}},"m2","OK","prosječna površina temelja od temelja kontrafore duž čitavog zida"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.9000021999999994,1.2,{"$f":"-((Y101*Z102-Y102*Z101)*(Y101+Y102)+(Y102*Z103-Y103*Z102)*(Y102+Y103)+(Y103*Z104-Y104*Z103)*(Y103+Y104)+(Y104*Z105-Y105*Z104)*(Y104+Y105)+(Y105*Z106-Y106*Z105)*(Y105+Y106)+(Y106*Z107-Y107*Z106)*(Y106+Y107)+(Y107*Z108-Y108*Z107)*(Y107+Y108)+(Y108*Z109-Y109*Z108)*(Y108+Y109)+(Y109*Z110-Y110*Z109)*(Y109+Y110))/6/Y111","v":{"$error":"#VALUE!"}},"m  ",{"$f":"-((AA101*AB102-AA102*AB101)*(AA101+AA102)+(AA102*AB103-AA103*AB102)*(AA102+AA103)+(AA103*AB104-AA104*AB103)*(AA103+AA104)+(AA104*AB105-AA105*AB104)*(AA104+AA105)+(AA105*AB106-AA106*AB105)*(AA105+AA106)+(AA106*AB107-AA107*AB106)*(AA106+AA107)+(AA107*AB108-AA108*AB107)*(AA107+AA108)+(AA108*AB109-AA109*AB108)*(AA108+AA109)+(AA109*AB110-AA110*AB109)*(AA109+AA110))/6/AA111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AC101*AD102-AC102*AD101)*(AC101+AC102)+(AC102*AD103-AC103*AD102)*(AC102+AC103)+(AC103*AD104-AC104*AD103)*(AC103+AC104)+(AC104*AD105-AC105*AD104)*(AC104+AC105)+(AC105*AD106-AC106*AD105)*(AC105+AC106)+(AC106*AD107-AC107*AD106)*(AC106+AC107)+(AC107*AD108-AC108*AD107)*(AC107+AC108)+(AC108*AD109-AC109*AD108)*(AC108+AC109)+(AC109*AD110-AC110*AD109)*(AC109+AC110))/6/AC111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AE101*AF102-AE102*AF101)*(AE101+AE102)+(AE102*AF103-AE103*AF102)*(AE102+AE103)+(AE103*AF104-AE104*AF103)*(AE103+AE104)+(AE104*AF105-AE105*AF104)*(AE104+AE105)+(AE105*AF106-AE106*AF105)*(AE105+AE106)+(AE106*AF107-AE107*AF106)*(AE106+AE107)+(AE107*AF108-AE108*AF107)*(AE107+AE108)+(AE108*AF109-AE109*AF108)*(AE108+AE109)+(AE109*AF110-AE110*AF109)*(AE109+AE110))/6/AE111","v":{"$error":"#VALUE!"}},"m",null,null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AK101+AK102)+(AK102*AL103-AK103*AL102)*(AK102+AK103)+(AK103*AL104-AK104*AL103)*(AK103+AK104)+(AK104*AL105-AK105*AL104)*(AK104+AK105)+(AK105*AL106-AK106*AL105)*(AK105+AK106)+(AK106*AL107-AK107*AL106)*(AK106+AK107)+(AK107*AL108-AK108*AL107)*(AK107+AK108)+(AK108*AL109-AK109*AL108)*(AK108+AK109)+(AK109*AL110-AK110*AL109)*(AK109+AK110))/6/AK111","v":{"$error":"#VALUE!"}},"m  "]
[null,null,null,null,null,{"$f":"+'C III-V'!F136:G136","v":"Visina presjeka"},null,{"$f":"+'C III-V'!H136:I136","v":"Intezitet"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.9000021999999994,0.5,{"$f":"-((Y101*Z102-Y102*Z101)*(Z101+Z102)+(Y102*Z103-Y103*Z102)*(Z102+Z103)+(Y103*Z104-Y104*Z103)*(Z103+Z104)+(Y104*Z105-Y105*Z104)*(Z104+Z105)+(Y105*Z106-Y106*Z105)*(Z105+Z106)+(Y106*Z107-Y107*Z106)*(Z106+Z107)+(Y107*Z108-Y108*Z107)*(Z107+Z108)+(Y108*Z109-Y109*Z108)*(Z108+Z109)+(Y109*Z110-Y110*Z109)*(Z109+Z110))/6/Y111","v":{"$error":"#VALUE!"}},"m    ",{"$f":"-((AA101*AB102-AA102*AB101)*(AB101+AB102)+(AA102*AB103-AA103*AB102)*(AB102+AB103)+(AA103*AB104-AA104*AB103)*(AB103+AB104)+(AA104*AB105-AA105*AB104)*(AB104+AB105)+(AA105*AB106-AA106*AB105)*(AB105+AB106)+(AA106*AB107-AA107*AB106)*(AB106+AB107)+(AA107*AB108-AA108*AB107)*(AB107+AB108)+(AA108*AB109-AA109*AB108)*(AB108+AB109)+(AA109*AB110-AA110*AB109)*(AB109+AB110))/6/AA111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AC101*AD102-AC102*AD101)*(AD101+AD102)+(AC102*AD103-AC103*AD102)*(AD102+AD103)+(AC103*AD104-AC104*AD103)*(AD103+AD104)+(AC104*AD105-AC105*AD104)*(AD104+AD105)+(AC105*AD106-AC106*AD105)*(AD105+AD106)+(AC106*AD107-AC107*AD106)*(AD106+AD107)+(AC107*AD108-AC108*AD107)*(AD107+AD108)+(AC108*AD109-AC109*AD108)*(AD108+AD109)+(AC109*AD110-AC110*AD109)*(AD109+AD110))/6/AC111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AE101*AF102-AE102*AF101)*(AF101+AF102)+(AE102*AF103-AE103*AF102)*(AF102+AF103)+(AE103*AF104-AE104*AF103)*(AF103+AF104)+(AE104*AF105-AE105*AF104)*(AF104+AF105)+(AE105*AF106-AE106*AF105)*(AF105+AF106)+(AE106*AF107-AE107*AF106)*(AF106+AF107)+(AE107*AF108-AE108*AF107)*(AF107+AF108)+(AE108*AF109-AE109*AF108)*(AF108+AF109)+(AE109*AF110-AE110*AF109)*(AF109+AF110))/6/AE111","v":{"$error":"#VALUE!"}},"m",null,null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AL101+AL102)+(AK102*AL103-AK103*AL102)*(AL102+AL103)+(AK103*AL104-AK104*AL103)*(AL103+AL104)+(AK104*AL105-AK105*AL104)*(AL104+AL105)+(AK105*AL106-AK106*AL105)*(AL105+AL106)+(AK106*AL107-AK107*AL106)*(AL106+AL107)+(AK107*AL108-AK108*AL107)*(AL107+AL108)+(AK108*AL109-AK109*AL108)*(AL108+AL109)+(AK109*AL110-AK110*AL109)*(AL109+AL110))/6/AK111","v":{"$error":"#VALUE!"}},"m    ",null,{"$f":"+'C III-V'!AN113:AN114","v":-0.25},{"$f":"IF('Analiza i dimenzioniranje'!D84=\"\",0,'Analiza i dimenzioniranje'!D83+'C III-V'!AN113)","v":0.75}]
[null,null,null,null,null,{"$f":"+'C III-V'!F137:G137","v":"III"},{"$f":"+'C III-V'!G137:H137","v":1.2},{"$f":"+'C III-V'!H137:I137","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,0.12820515121628623,{"$f":"+Y111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AA111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AC111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AE111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,{"$f":"+AK111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN"]
[null,null,null,null,null,{"$f":"+'C III-V'!F138:G138","v":"VI"},{"$f":"+'C III-V'!G138:H138","v":1.52},{"$f":"+'C III-V'!H138:I138","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Teren  kosina",null,"Klizna ploha"]
[null,null,null,null,null,{"$f":"+'C III-V'!F139:G139","v":"VII"},{"$f":"+'C III-V'!G139:H139","v":1.84},{"$f":"+'C III-V'!H139:I139","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C XII-XIII'!AI116","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!AJ116","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!AK116","v":1.75},{"$f":"+'C XII-XIII'!AL116","v":-1.1133852506716102},"sjecišta ravnine presjeka na kliznoj plohi",null,null,null,null,null,null,"Omjer površine"]
[null,null,null,null,null,{"$f":"+'C III-V'!F140:G140","v":"VIII"},{"$f":"+'C III-V'!G140:H140","v":2.16},{"$f":"+'C III-V'!H140:I140","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C XII-XIII'!AI117","v":6.2644906473896782},{"$f":"+'C XII-XIII'!AJ117","v":6},{"$f":"+'C XII-XIII'!AK117","v":0},{"$f":"+'C XII-XIII'!AL117","v":4.08},{"$f":"+'C III-V'!AA100","v":"oznaka"},{"$f":"+'C III-V'!AB100","v":"X"},{"$f":"+'C III-V'!AC100","v":"Y"},null,null,null,"        sa kontraforama: bez kontrafora",null,null,"Potresna sila-prosječna"]
[null,null,null,null,null,{"$f":"+'C III-V'!F141:G141","v":"IX"},{"$f":"+'C III-V'!G141:H141","v":2.48},{"$f":"+'C III-V'!H141:I141","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!D116,AI117)","v":-5},{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!E116,'C III-V'!AJ117)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!AA101","v":"Y=0"},{"$f":"+'C III-V'!AB101","v":1.75},{"$f":"+'C III-V'!AC101","v":0},null,null,null,null,null,null,null,null,"Potresna sila","F","G"]
[null,null,null,null,null,{"$f":"+'C III-V'!F142:G142","v":"X"},{"$f":"+'C III-V'!G142:H142","v":2.8},{"$f":"+'C III-V'!H142:I142","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"(AJ117-AI117)/(AJ116-AI116)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AI119*AI116+AI117","v":{"$error":"#VALUE!"}}," ",{"$f":"+'C III-V'!AA102","v":"PIII"},{"$f":"+'C III-V'!AB102","v":0.97707863658009864},{"$f":"+'C III-V'!AC102","v":1.2},null,null,null,null,"Ukupna duljina zida",null,{"$f":"+Kontrafore!E13","v":12},"m",{"$f":"+AV119","v":12},{"$f":"+Y111","v":{"$error":"#VALUE!"}},{"$f":"+Y114","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F143:G143","v":"XI"},{"$f":"+'C III-V'!G143:H143","v":3.14},{"$f":"+'C III-V'!H143:I143","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"-(AL117-AK117)/(AK116-AL116)","v":-1.4248868534344206},"*x    +",{"$f":"-(AK116*AI120-AK117)","v":2.4935519935102359}," ",{"$f":"+'C III-V'!AA103","v":"PVI"},{"$f":"+'C III-V'!AB103","v":0.68324863210273346},{"$f":"+'C III-V'!AC103","v":1.52},null,null,null,null,"ukupna duljina kontrafora",null,{"$f":"+Kontrafore!E5*Kontrafore!E4","v":3},"m",{"$f":"+AV120","v":3},{"$f":"+AY119-AY121","v":{"$error":"#VALUE!"}},{"$f":"IF(AV120=AV119,0,AZ119-AZ121)","v":{"$error":"#VALUE!"}}]
["Presjek kroz zid I",null,"Presjek kroz zid II",null,null,{"$f":"+'C III-V'!F144:G144","v":"XIII"},{"$f":"+'C III-V'!G144:H144","v":3.44},{"$f":"+'C III-V'!H144:I144","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AK120-AK119)/(AI119-AI120)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AI120*AI121+AK120","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA104","v":"PVII"},{"$f":"+'C III-V'!AB104","v":0.45866939675594048},{"$f":"+'C III-V'!AC104","v":1.84},null,null,null,null,"ukupna duljina bez kontrafora",null,{"$f":"+AV119-AV120","v":9},"m",{"$f":"+AX119-AX120","v":9},{"$f":"+AG111","v":0},{"$f":"+IF(AX121=0,0,AG114)","v":0}]
["x","y","x","y",null,{"$f":"+'C III-V'!F145:G145","v":"XIII"},{"$f":"+'C III-V'!G145:H145","v":3.76},{"$f":"+'C III-V'!H145:I145","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA105","v":"PVIII"},{"$f":"+'C III-V'!AB105","v":0.23409016140914748},{"$f":"+'C III-V'!AC105","v":2.16},null,null,null,null,"površina s kontraforama",null,{"$f":"+AV120/AV119","v":0.25}]
[0,{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+A123","v":0},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},null,{"$f":"+'C III-V'!F146:G146","v":"XIV"},{"$f":"+'C III-V'!G146:H146","v":4.08},{"$f":"+'C III-V'!H146:I146","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($AK$119-$AK$123)/AI119","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AK121","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA106","v":"PIX"},{"$f":"+'C III-V'!AB106","v":9.5109260623546556E-3},{"$f":"+'C III-V'!AC106","v":2.48},null,null,null,null,"površina bez kontrafora",null,{"$f":"+AV121/AV119","v":0.75}]
[{"$f":"+F83","v":{"$error":"#VALUE!"}},{"$f":"+B123","v":4.4000000000000004},{"$f":"+A124","v":{"$error":"#VALUE!"}},{"$f":"+D123","v":4.08},null,{"$f":"+'C III-V'!F147:G147","v":"XV"},{"$f":"+'C III-V'!G147:H147","v":4.4000000000000004},{"$f":"+'C III-V'!H147:I147","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA107","v":"PX"},{"$f":"+'C III-V'!AB107","v":-0.21506830928443818},{"$f":"+'C III-V'!AC107","v":2.8},null,null,null,null,null,null,"odnos",null,{"$f":"-(AX120/AX119)*'Analiza i dimenzioniranje'!D83","v":-0.25}]
[null,null,null,null,null,{"$f":"+'C III-V'!F148:G148","v":"XVI"},{"$f":"+'C III-V'!G148:H148","v":4.72},{"$f":"+'C III-V'!H148:I148","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA108","v":"PXI"},{"$f":"+'C III-V'!AB108","v":-0.45368374684040591},{"$f":"+'C III-V'!AC108","v":3.14},null,null,null,null,null,"krak",{"$f":"+Y113","v":{"$error":"#VALUE!"}},{"$f":"+AZ119","v":{"$error":"#VALUE!"}},{"$f":"+AZ120*AV122","v":{"$error":"#VALUE!"}},null,{"$f":"+AZ119-AX126","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F149:G149","v":"XVII"},{"$f":"+'C III-V'!G149:H149","v":5.04},{"$f":"+'C III-V'!H149:I149","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($AK$120-AK126)/$AI$120","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AK121","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA109","v":"PXII"},{"$f":"+'C III-V'!AB109","v":-0.66422677997802415},{"$f":"+'C III-V'!AC109","v":3.44},null,null,null,null,null,null,{"$f":"+AG113","v":0},{"$f":"+AZ121","v":0},{"$f":"+AZ120*AV123","v":{"$error":"#VALUE!"}},null,{"$f":"+AZ121+AX125","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F150:G150","v":"XVIII"},{"$f":"+'C III-V'!G150:H150","v":5.36},{"$f":"+'C III-V'!H150:I150","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-1.1976024639266576,null,4.2,null,{"$f":"+'C III-V'!AA110","v":"PXIII"},{"$f":"+'C III-V'!AB110","v":-0.88880601532481696},{"$f":"+'C III-V'!AC110","v":3.76},null,null,null,null,null,null,null,null,"Prosječna masa za potres:",null,{"$f":"IF(IF(AV130=AW130,Y114,+AZ126)=0,AZ125,IF(AV130=AW130,Y114,+AZ126))","v":{"$error":"#VALUE!"}},"kn"]
[null,null,null,null,null,{"$f":"+'C III-V'!F151:G151","v":"XIX"},{"$f":"+'C III-V'!G151:H151","v":5.6800000000000006},{"$f":"+'C III-V'!H151:I151","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.90782786744952648,null,1.2,null,{"$f":"+'C III-V'!AA111","v":"PXIV"},{"$f":"+'C III-V'!AB111","v":-1.1133852506716102},{"$f":"+'C III-V'!AC111","v":4.08}]
[null,null,null,null,null,{"$f":"+'C III-V'!F152:G152","v":"XX"},{"$f":"+'C III-V'!G152:H152","v":6},{"$f":"+'C III-V'!H152:I152","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.6464828732122183,null,{"$f":"+AI117","v":6.2644906473896782},null,{"$f":"+'C III-V'!AA112","v":"PXV"},{"$f":"+'C III-V'!AB112","v":-1.3379644860184032},{"$f":"+'C III-V'!AC112","v":4.4000000000000004}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-1.3379644860184032,null,{"$f":"+AF101","v":4.4000000000000004},null,{"$f":"+'C III-V'!AA113","v":"PXVI"},{"$f":"+'C III-V'!AB113","v":-1.5625437213651958},{"$f":"+'C III-V'!AC113","v":4.72},null,null,null,null,null,"x=",{"$f":"+AG113","v":0},{"$f":"+Y113","v":{"$error":"#VALUE!"}},null,{"$f":"+AI109","v":0},{"$f":"+AI106","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-1.1976024639266576,null,4.2,null,{"$f":"+'C III-V'!AA114","v":"PXVII"},{"$f":"+'C III-V'!AB114","v":-1.7871229567119888},{"$f":"+'C III-V'!AC114","v":5.04},null,null,null,null,null,"Y=",{"$f":"+AG114","v":0},{"$f":"+Y114","v":{"$error":"#VALUE!"}},null,{"$f":"+AJ109","v":0},{"$f":"+AJ106","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA115","v":"PXVIII"},{"$f":"+'C III-V'!AB115","v":-2.0117021920587819},{"$f":"+'C III-V'!AC115","v":5.36},null,null,null,null,null,"Y=",{"$f":"(AV131-AW131)/(AV130-AW130)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AV132*AW130+AW131","v":{"$error":"#VALUE!"}},{"$f":"(AY131-AZ131)/(AY130-AZ130)","v":{"$error":"#DIV/0!"}},"*x    +",{"$f":"-AY132*AZ130+AZ131","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA116","v":"PXIX"},{"$f":"+'C III-V'!AB116","v":-2.2362814274055753},{"$f":"+'C III-V'!AC116","v":5.6800000000000006}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA117","v":"PXX"},{"$f":"+'C III-V'!AB117","v":0},{"$f":"+'C III-V'!AC117","v":6.0000000000000009},null,null,null,null,null,"x=",{"$f":"+AK113","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","Y",null,null,null,{"$f":"+AI136","v":{"$error":"#VALUE!"}},{"$f":"+AJ136","v":{"$error":"#VALUE!"}},null,null,null,null,null,"xstv=",{"$f":"+AV134-X113","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C XII-XIII'!AI136","v":{"$error":"#VALUE!"}},{"$f":"+'C XII-XIII'!AJ136","v":{"$error":"#VALUE!"}},null,null,"x=",{"$f":"+(AE151-AD138)/AC151","v":1.1153638440753406},null,null,null,null,null,null,"            Masa da se dobije prosječni potres iz čelije AT125=",null,null,null,null,{"$f":"+AZ125","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+'C XII-XIII'!AC138","v":{"$error":"#VALUE!"}},{"$f":"+AD102","v":4.08},{"$f":"+AF102","v":4.4000000000000004},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"razlika¸površina",{"$f":"+Y111-AI111","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AE144-AC138)/(-AC144)","v":{"$error":"#VALUE!"}},{"$f":"IF(AD138<AC138,(AE151-AD138)/(-AC151),(AE156-AD138)/(-AC156))","v":{"$error":"#VALUE!"}},{"$f":"IF(AE138<AC138,(AE151-AE138)/(-AC151),(AE156-AE138)/(-AC156))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"duljina segmenta",{"$f":"++AJ105","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina III. sloja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"okomito na kliz. Plohu",null,{"$f":"+AV143/AV139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"d=","dodatak",{"$f":"+AV140/COS(AV142*PI()/180)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA153","v":2},{"$f":"+'C III-V'!AB153","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"          kut nagiba klizne plohe za potres   a= ",null,{"$f":"ATAN((-Y104+Y101)/(Z104-Z101))*180/PI()","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA154","v":-5},{"$f":"+'C III-V'!AB154","v":9.9970360471948005},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dodatna površina",{"$f":"+AV144/'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AD143-AD142)/(AC143-AC142)","v":-1.4281480067421144},"*x      +",{"$f":"-AC144*AC142+AD142","v":2.8562960134842288},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"G=",{"$f":"+AX126","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AE144-AD146)/(-AC144)","v":1.1597509541483482}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+Z102","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina II. sloja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA148","v":-1.0572404418349119},{"$f":"+'C III-V'!AB148","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA149","v":0.97707863658009864},{"$f":"+'C III-V'!AB149","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AD150-AD149)/(AC150-AC149)","v":-1.3763819204711734},"*x      +",{"$f":"-AC151*AC149+AD149","v":2.5448333702674724}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina I. sloja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koordinate na sjecištu s terenom",null,null,{"$f":"+'C III-V'!AA144","v":-2.5846586698092704},{"$f":"+'C III-V'!AB144","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koordinate na sjecištu slojeva",null,null,{"$f":"+'C III-V'!AA143","v":-1.0572404418349119},{"$f":"+'C III-V'!AB143","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AD155-AD154)/(AC155-AC154)","v":-1.4825609685127401},"*x      +",{"$f":"-AC156*AC154+AD154","v":2.4325765866023956}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rub dna konzole uz aktivni klin",null,null,{"$f":"+B6","v":{"$error":"#VALUE!"}},{"$f":"+C6","v":3.14}]

{"sheet":"C XVI-XVII","index":45,"n_rows":157,"n_cols":53,"rows_kept":157,"cut":false,"hidden":true,"merged":[[112,5,112,6],[116,47,116,49],[96,32,98,33],[96,34,98,35],[96,36,98,37],[99,32,99,33],[99,34,99,35],[99,36,99,37],[115,38,115,40],[110,38,113,38],[110,39,111,40],[112,39,113,39],[112,40,113,40],[99,28,99,29],[99,30,99,31],[114,34,114,35],[99,24,99,25],[67,10,67,11],[67,13,67,14],[77,13,77,14],[77,10,77,11],[67,20,67,21],[77,15,77,16],[67,15,67,16],[90,1,90,2],[90,3,90,4],[90,5,90,6],[42,11,43,14],[96,22,97,23],[67,22,67,23],[44,7,44,8],[44,17,44,18],[42,1,42,2],[42,3,42,4],[42,5,42,6],[42,7,43,10],[44,9,44,10],[44,11,44,12],[77,1,77,2],[77,3,77,4],[77,5,77,6],[77,8,77,9],[67,1,67,2],[67,3,67,4],[67,5,67,6],[67,8,67,9],[42,15,43,18],[44,21,44,22],[44,13,44,14],[44,15,44,16],[10,3,10,4],[17,12,17,16],[10,27,10,28],[11,3,11,4],[12,27,12,28],[13,12,13,16],[13,27,13,28],[0,1,0,2],[0,3,0,4],[0,5,0,7],[0,9,0,10],[1,5,1,8],[114,36,114,37],[13,29,13,30],[62,29,62,30],[62,27,62,28],[16,27,16,28],[99,26,99,27],[17,27,17,28],[26,27,26,28]]}
["Točke","ZID I TEMELJ",null,"NASIP NA TEMELJU IZA",null,"ZID, KONZOLA I NASIP NA KONZOLI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Točka A",null,"Presjek XVI-I"]
[1,2,{"$f":"'Analiza i dimenzioniranje'!BG9+'Unos podataka'!J41","v":0.12820515121628623},null,null,"ZA BILO KOJI PRESJEK ",null,null,null,null,null,null,null,null,null,null,null,"Presjek zid Iv",{"$f":"+($B$9-$B$4)*(T2-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72},{"$f":"+B15","v":4.9000021999999994},{"$f":"+C15","v":0.5},{"$f":"+'C XVI-XVII'!B10+0.05","v":{"$error":"#VALUE!"}},-0.5]
[2,2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T3-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72},"Točka B",null,{"$f":"+W2","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!C10+0.5","v":{"$error":"#VALUE!"}}]
[3,{"$f":"+B3+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+C3","v":1.2},{"$f":"+B19","v":2},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>C4,B21,B4)","v":3.4000010999999999},{"$f":"IF(E20>C4,E20,C4)","v":1.2},{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},null,null,null,null,null,null,null,null,"Presjek V",{"$f":"+($B$9-$B$4)*(T4-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AG44","v":5.04},{"$f":"+'C XVI-XVII'!B2","v":2},{"$f":"+'C XVI-XVII'!C2","v":0.12820515121628623}]
[4,{"$f":"+B23","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},{"$f":"+D4","v":2},{"$f":"+'C III-V'!E5","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,B21,B5)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,E20,C5)","v":3.14},{"$f":"+F8","v":{"$error":"#VALUE!"}},{"$f":"+G8","v":3.44},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T5-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AG44","v":5.04},null,null,"Presjek XVII-II",null,null,null,"Nasip na zidu iza"]
[5,{"$f":"+B5-'Analiza i dimenzioniranje'!G78","v":{"$error":"#VALUE!"}},{"$f":"+C5","v":3.14},{"$f":"IF(B6<2,B5,IF(B9>2,B9,D5))","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!E6","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C7,B21,B6)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C6,E20,C6)","v":3.14},{"$f":"IF(F7>F9,H5,F9)","v":{"$error":"#VALUE!"}},{"$f":"IF(F7>F9,I5,IF(E20>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XVI-XVII'!E20,G9))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"Presjek VI",{"$f":"+($B$9-$B$4)*(T6-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},"TLO 1. sloj",null,{"$f":"+'C XVI-XVII'!B15-0.05","v":4.8500021999999996},{"$f":"+'C XVI-XVII'!X2","v":-0.5},null,null,2,{"$f":"IF('Analiza i dimenzioniranje'!AW26>'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AW26)","v":0}]
[6,{"$f":"IF('Analiza i dimenzioniranje'!G78=0,'C XVI-XVII'!B8,B6)","v":{"$error":"#VALUE!"}},{"$f":"C6+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+B4","v":3.4000010999999999},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>=C7,B21,B7)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C7,E20,C7)","v":3.44},{"$f":"IF(F7>F9,H6,H6)","v":{"$error":"#VALUE!"}},{"$f":"+I6","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T7-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},{"$f":"+'C XVI-XVII'!B15-0.05","v":4.8500021999999996},{"$f":"+'C XVI-XVII'!X3","v":{"$error":"#VALUE!"}},"Horizontala",null,2,{"$f":"'Analiza i dimenzioniranje'!BF28","v":0}]
[7,{"$f":"+B22","v":{"$error":"#VALUE!"}},{"$f":"+C7","v":3.44},{"$f":"+D4","v":2},{"$f":"+E4","v":1.2},{"$f":"IF(E20>C8,B21,B8)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C8,E20,C8)","v":3.44},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$H$15=0,I7+(H7-H8)*'Unos podataka'!R57,IF('C III-V'!H9>'Unos podataka'!$B$105,I7+(H7-H8)*'Unos podataka'!$R$55,'Unos podataka'!$T$57))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,"Presjek VII",{"$f":"+($B$9-$B$4)*(T8-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!V8","v":6},null,null,{"$f":"+'C XVI-XVII'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!C5","v":3.14}]
[8,{"$f":"B4-TAN('Analiza i dimenzioniranje'!H51*PI()/180)*('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},null,null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"+I4","v":3.44},null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T9-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},{"$f":"+U8-'Analiza i dimenzioniranje'!E27","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!V9","v":6.2644906473896782},"Presjek ZID",null,{"$f":"+IF('Analiza i dimenzioniranje'!$E$24=0,0,'C XVI-XVII'!Y4)","v":0},{"$f":"+Z8","v":3.14}]
[9,{"$f":"+B9+'Analiza i dimenzioniranje'!E54","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},null,null,{"$f":"+B10","v":{"$error":"#VALUE!"}},{"$f":"+C10","v":"A"},null,null,null,null,null,null,null,null,null,null,"Presjek VIII",{"$f":"+($B$9-$B$4)*(T10-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},-8,{"$f":"+'C III-V'!V10","v":6.2644906473896782},{"$f":"+'C XVI-XVII'!B15-0.5","v":4.4000021999999994},{"$f":"+'C XVI-XVII'!C10+0.1","v":{"$error":"#VALUE!"}}]
[10,{"$f":"+B4+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+C3","v":1.2},"NASIP NA KONZOLI",null,{"$f":"+F12+E65","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C11,E20,C11)","v":1.2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T11-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},"x","y",{"$f":"+'C XVI-XVII'!B10+0.5","v":{"$error":"#VALUE!"}},{"$f":"+X10","v":{"$error":"#VALUE!"}},null,null,null,"Rsidra"]
[11,{"$f":"+B11","v":4.2000010999999997},{"$f":"+C11","v":1.2},"za stabilnost",null,{"$f":"+F4","v":3.4000010999999999},{"$f":"+G4","v":1.2},null,null,null,null,null,null,null,null,null,null,"Presjek XVIX",{"$f":"+($B$9-$B$4)*(T12-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+W23","v":{"$error":"#VALUE!"}},{"$f":"+U12*(V9-V8)/(U9-U8)-U8*(V9-V8)/(U9-U8)+V8","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,20,AB16)","v":20},{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,0,AC16)","v":0}]
[12,{"$f":"+B12","v":4.2000010999999997},{"$f":"+C12","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T13-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+W25","v":{"$error":"#VALUE!"}},{"$f":"+U13*(V9-V8)/(U9-U8)-U8*(V9-V8)/(U9-U8)+V8","v":{"$error":"#VALUE!"}},"Pad terena niz padinu",null,null,null,null,"Os rezultante sidara Ukupna računska sila u sidrima"]
[13,{"$f":"+B11+'Analiza i dimenzioniranje'!G57","v":4.9000021999999994},{"$f":"+C13","v":1.2},{"$f":"+B7","v":{"$error":"#VALUE!"}},3.44,null,null,null,null,"Linija presjeka",null,null," Koordinata sredine presjeka",null,null,null,null,"Presjek X",{"$f":"+($B$9-$B$4)*(T14-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},"TLO 2. sloj",null,{"$f":"+'Analiza i dimenzioniranje'!Q105","v":3},{"$f":"+'Analiza i dimenzioniranje'!P105","v":{"$error":"#VALUE!"}},null,null,null,"Slobodna  zona.",null,"1. sloj"]
[14,{"$f":"+B14","v":4.9000021999999994},{"$f":"+C14-'Analiza i dimenzioniranje'!E51","v":0.5},{"$error":"#VALUE!"},3.44,{"$f":"IF((B4-B9)=0,0,+(C9-C4)/(B4-B9))","v":{"$error":"#VALUE!"}},"n  Nagib zida u tlu",null,null,0,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,"III-III","konzola","Presjek XVI","Presjek XVII",null,{"$f":"+($B$11-$B$10)*(T15-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},{"$f":"IF(('Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17)<'Analiza i dimenzioniranje'!$F$45,2,(IF(B7<B24,B7,IF('Analiza i dimenzioniranje'!G78=0,'C XVI-XVII'!B24,2))))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17","v":4},{"$f":"+'Analiza i dimenzioniranje'!O130","v":7.1000021999999996},{"$f":"+'Analiza i dimenzioniranje'!N130","v":1.5001009999999999},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,AB24)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,'Analiza i dimenzioniranje'!P22)","v":5},{"$f":"+U9","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782}]
[15,{"$f":"+B2","v":2},{"$f":"+C2","v":0.12820515121628623},{"$error":"#VALUE!"},"A",null,null,null,null,3,{"$f":"+K15","v":1.2},null,"x",{"$f":"+(F12+F11)/2","v":{"$error":"#VALUE!"}},{"$f":"(B8+(B11-B10)*(O17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U29+(B11-B10)*(P17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U34+(B11-B10)*(Q17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},"Presjek XI",{"$f":"+($B$9-$B$4)*(T16-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},-8,{"$f":"+V15+(U15-U16)*TAN('Analiza i dimenzioniranje'!$E$18*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"AB15-'Analiza i dimenzioniranje'!P23","v":{"$error":"#VALUE!"}},{"$f":"+AC15-(AB15-AB16)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782}]
[null,null,"Jednadžba pravca zida uz tlo",{"$f":"+D16","v":{"$error":"#VALUE!"}},{"$f":"+I7","v":{"$error":"#VALUE!"}},null,null,null,null,"Sloj 2 gore",null,null,"y",{"$f":"+G11","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+'Analiza i dimenzioniranje'!AG44","v":5.04},{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72},null,{"$f":"+($B$11-$B$10)*(T17-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},"TLO 3. sloj",null,"Prometno opterećenje",null,null,null,null,"Sidrena dionica",null,"Jednadžba površine terena"]
[null,"x","y",{"$f":"+D14","v":{"$error":"#VALUE!"}},{"$f":"+I8","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+F94","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E52>=G94,0,G94)","v":4},null,null,null,null,null,null,"Presjek XII",{"$f":"+($B$9-$B$4)*(T18-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},2,{"$f":"+'Analiza i dimenzioniranje'!$F$17","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,+'C XVI-XVII'!B9-'Analiza i dimenzioniranje'!E26)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,'C XVI-XVII'!V9)","v":6.2644906473896782},null,null,null,"                   Y=",null,{"$f":"+(AE16-AE15)/(AD16-AD15)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AD18*AD15+AE15","v":{"$error":"#VALUE!"}}]
[null,2,{"$f":"+B19*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},{"$f":"+D14","v":{"$error":"#VALUE!"}},{"$f":"+E14","v":3.44},null,null,null,null,{"$f":"U16","v":-8},{"$f":"+K18","v":4},null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T19-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},-8,{"$f":"+V18+(U18-U19)*TAN('Analiza i dimenzioniranje'!$F$18*PI()/180)","v":1.5492076949174773},{"$f":"+W18","v":{"$error":"#VALUE!"}},{"$f":"+X18+'Analiza i dimenzioniranje'!E24/50","v":6.4644906473896784},null,null,null,{"$f":"+AB16","v":{"$error":"#VALUE!"}},{"$f":"+AC16","v":{"$error":"#VALUE!"}},"za x=",{"$f":"+AB20","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+H8","v":{"$error":"#VALUE!"}},{"$f":"+B20*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},"M na koti",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,"Sloj 1 ili2 dole",null,null,null,null,null,null,{"$f":"+(B11-B10)*(Q21-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},"Presjek XIII",{"$f":"+($B$9-$B$4)*(T20-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},"KONTAKTNI NAPONI",null,{"$f":"+W18-'Analiza i dimenzioniranje'!E25","v":{"$error":"#VALUE!"}},{"$f":"+X19","v":6.4644906473896784},null,null,null,{"$f":"+(AB21+AB19)/2","v":{"$error":"#VALUE!"}},{"$f":"+(AC19+AC21)/2","v":{"$error":"#VALUE!"}},"y=",{"$f":"+AD18*AE19+AF18","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C21-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,{"$f":"+IF('Analiza i dimenzioniranje'!G78=0,D8,H8)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+F95","v":{"$error":"#VALUE!"}},{"$f":"+G12","v":1.2},null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,{"$f":"+($B$11-$B$10)*(T21-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},2,0,{"$f":"+W20","v":{"$error":"#VALUE!"}},{"$f":"+X18","v":6.2644906473896782},null,null,null,{"$f":"+AB19-'Analiza i dimenzioniranje'!P24","v":{"$error":"#VALUE!"}},{"$f":"+AC19-(AB19-AB21)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},"visina sloja iznad centra sidra"]
[null,{"$f":"+(B9-B4)*(C22-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+C23+'Analiza i dimenzioniranje'!C77","v":3.44},null,null,null,null,null,null,{"$f":"+U19","v":-8},{"$f":"+K21","v":1.2},null,null,null,null,null,null,"Presjek XIV",{"$f":"+($B$9-$B$4)*(T22-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},2,{"$f":"-'Analiza i dimenzioniranje'!$F$193/100","v":{"$error":"#VALUE!"}},"Točkasto",null,null,null,null,null,null,{"$f":"+AE20-AC20","v":{"$error":"#VALUE!"}},"m"]
[null,{"$f":"+(B9-B4)*(C23-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T23-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"2+'Analiza i dimenzioniranje'!$E$61","v":4.9000021999999994},{"$f":"-'Analiza i dimenzioniranje'!$F$190/100","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E36=0,-10,B9-'Analiza i dimenzioniranje'!E37)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X23","v":{"$error":"#VALUE!"}},null,null,null,"Jednadžba  lica zida "]
[null,{"$f":"+(B9-B4)*(C24-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V15","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek XV",{"$f":"+($B$9-$B$4)*(T24-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U23","v":4.9000021999999994},0,"Linijsko iza zida",null,null,null,"x=",{"$f":"+($B$11-$B$10)*(AB25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+($B$11-$B$10)*(AC25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+(B11-B10)*(AE25-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C25-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AG44","v":5.04},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U21","v":2},0,{"$f":"IF('Analiza i dimenzioniranje'!$E$34=0,0,B9-'Analiza i dimenzioniranje'!K28)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X27","v":{"$error":"#VALUE!"}},null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!AF42","v":5},{"$f":"+'Analiza i dimenzioniranje'!AG42","v":0},null,{"$f":"+'Analiza i dimenzioniranje'!H76+'Analiza i dimenzioniranje'!E52","v":1.5001009999999999}]
[null,{"$f":"+(B9-B4)*(C26-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid XVII-XVII",{"$f":"+'Analiza i dimenzioniranje'!AG44","v":5.04},{"$f":"+W25","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$34=0,0,X25+1)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!T22","v":0},null,null,null,null,{"$f":"+B14-AE24","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C27-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AG44","v":5.04},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!AG44","v":5.04},"TEMELJ -opterećenje",null,"x=",{"$f":"+($B$11-$B$10)*(Z26-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"Rez. Sidra na zidu"]
[null,{"$f":"+(B9-B4)*(C28-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V27","v":5.04},{"$f":"+IF('Analiza i dimenzioniranje'!E28=0,0,W29)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9+'Analiza i dimenzioniranje'!F20+1.5)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!S22","v":0}]
["Sjecište s dnom temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V29-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":5.04},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W30-0.3)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X30)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z28-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+($B$11-$B$10)*(AC29-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E40","v":3.9999999960000001},{"$f":"+AB29+0.4","v":{"$error":"#VALUE!"}},{"$f":"+AC29+(AD29-AB29)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}}]
["zid",{"$f":"+B20","v":{"$error":"#VALUE!"}},{"$f":"+B30*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V30-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":5.04},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,B9-'Analiza i dimenzioniranje'!$E$32)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X31+'Analiza i dimenzioniranje'!E33)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!R22","v":0},null,null,null,{"$f":"+AB29-1","v":{"$error":"#VALUE!"}},{"$f":"+AC29-(AB29-AD30)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}}]
["Vrh zida",{"$f":"+(B9-B4)*(C31-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C558","v":-0.45},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid Iv",{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72},{"$f":"+W30","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9-'Analiza i dimenzioniranje'!K31)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z30-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"nagib lica"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,W31-'Analiza i dimenzioniranje'!$E$29)","v":{"$error":"#VALUE!"}},{"$f":"+X31","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q22","v":3},null,"tan"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V32","v":4.72},{"$f":"+W32","v":{"$error":"#VALUE!"}},{"$f":"+X30","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z32-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+(B13-B10)/(C10-C13)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V34-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V33","v":4.72},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W33+0.3)","v":{"$error":"#VALUE!"}},{"$f":"+X29","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q20","v":5},null,"kut"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V35-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V34","v":4.72},{"$f":"+W34","v":{"$error":"#VALUE!"}},{"$f":"+X28","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z34-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+ATAN(AB33)*180/PI()","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SIDRO za presjek",null,null,null,"Jednadžba pravca lica zida ",null,null,"Sjecište a arm konzole",null,"vrh zida","Anker armatura uz lice",null,"arm dno",null,"Y=",{"$f":"IF(AE38=AE37,1000000,(AF38-AF37)/(AE38-AE37))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AJ36*AE37+AF37","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!$C$545","v":1.6923077248520526}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB15)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC15)","v":5},null,null,"x=",null,null,{"$f":"+(B11-B10)*(AB38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AC38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AD38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AF37-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!B545","v":{"$error":"#VALUE!"}},{"$f":"+U81","v":2.0499999999999998},{"$f":"+V81","v":0.18682583433163008},"X=",{"$f":"+(-AL36+AL39)/(AJ36-AJ39)","v":{"$error":"#VALUE!"}},"sjeište",null,"x=",{"$f":"+(AN36-AL36)/AJ36","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB16)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC16)","v":{"$error":"#VALUE!"}},null,null,"y=",null,null,{"$f":"+'Analiza i dimenzioniranje'!E555","v":3.39},{"$f":"+AB38-'Analiza i dimenzioniranje'!#REF!","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!C558","v":-0.45},{"$f":"+(B11-B10)*(AF38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+U82","v":4.8600021999999994},{"$f":"+V82","v":0.54310345350772504},"Y=",{"$f":"+AJ36*AJ37+AL36","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate dna temelja",null,null,null,null,null,null,"Y=",{"$f":"+(AH38-AH37)/(AG38-AG37)","v":0.12678908905341604},"*x",{"$f":"-AJ39*AG37+AH37","v":-7.3091798227872762E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"lice","koord Pr II",{"$f":"+AB47+'Analiza i dimenzioniranje'!Q58","v":3.4500010999999997},{"$f":"(AB40*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24999999999999994},null,"SIDRO"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+(B11-B10)*(Z42-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+B8","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+AB15","v":{"$error":"#VALUE!"}},{"$f":"+AC15","v":5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+Z42","v":3.44},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,AB15-0.5)","v":{"$error":"#VALUE!"}},{"$f":"+AF41-(AE41-AE42)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},null,"Nasip ispred zida"]
["Oznaka","temelj",null,"Zid i konzola za pr. ZID",null,"Nasip na temelju iza zida",null,"      Za momente u presjeku zid-temelj          ",null,null,null,"      Za momente u presjeku XVI-XVI",null,null,null,"         Za momente u presjeku XVII-XVII",null,null,null,null,1,null,null,null,null,null,null,2,0,null,null,null,null,{"$f":"+AE24","v":{"$error":"#VALUE!"}},{"$f":"+C11+'Analiza i dimenzioniranje'!$H$76","v":1.5001009999999999}]
["točke","x","y","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - BETON",null,null,null,null,null,2.65,{"$f":"+(AC47+AC49)/2","v":0.31034478180740688},null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!$E$61","v":4.9000021999999994},{"$f":"+AI43","v":1.5001009999999999}]
[1,{"$f":"+'C XVI-XVII'!B2","v":2},{"$f":"+'C XVI-XVII'!C2","v":0.12820515121628623},null,null,null,null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"Kontaktni naponi za stab",null,"Beton do presjeka II-II",null,"Beton sredine temelja",null,"Beton do presjeka I-I",null,{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"(AB45*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH44+1.6","v":6.5000021999999991},{"$f":"+AI44-(AH45-AH44)*TAN('Analiza i dimenzioniranje'!H22*PI()/180)","v":1.5001009999999999}]
[2,{"$f":"+'C XVI-XVII'!B3","v":2},{"$f":"+'C XVI-XVII'!C3","v":1.2},null,null,null,null,"x","y","x","y","x","y","x","y","x","y","x","y","x","y",null,null,"x","y","x","y",{"$f":"+(AB43+AB47)/2","v":2.7000005499999999},{"$f":"(AB46*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.1206896584423281},null,null,null,null,"x","y"]
[3,{"$f":"+'C XVI-XVII'!B4","v":3.4000010999999999},{"$f":"+'C XVI-XVII'!C4","v":1.2},{"$f":"+B4","v":3.4000010999999999},1.2,2,1.2,3.4000010999999999,1.2,{"$f":"+D14","v":{"$error":"#VALUE!"}},3.44,{"$f":"+U34","v":{"$error":"#VALUE!"}},{"$f":"+V34","v":4.72},{"$f":"+J47","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AF44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AF44,K47)","v":4.72},{"$f":"+U29","v":{"$error":"#VALUE!"}},{"$f":"+V29","v":5.04},{"$f":"+J47","v":{"$error":"#VALUE!"}},{"$f":"+S48","v":5.04},{"$f":"+U21","v":2},{"$f":"+V21*100","v":0},2,0,{"$f":"+B4","v":3.4000010999999999},{"$f":"+W49","v":1.2},{"$f":"+B11","v":4.2000010999999997},1.2,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"(AB47*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24137931688465614},"Presjek XVII-II",null,null,null,{"$f":"+'C XVI-XVII'!B11","v":4.2000010999999997},{"$f":"+C11","v":1.2}]
[4,{"$f":"+B11","v":4.2000010999999997},1.2,{"$error":"#VALUE!"},3.14,2,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.44,{"$f":"+H48","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AF44<'Analiza i dimenzioniranje'!F45,I48,'C XVI-XVII'!V34)","v":4.72},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AF44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AF44,K48)","v":4.72},{"$f":"+H48","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AG44<'Analiza i dimenzioniranje'!F45,I48,V29)","v":5.04},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AG44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AG44,K48)","v":5.04},{"$f":"+U22","v":2},{"$f":"+V22*100","v":{"$error":"#VALUE!"}},2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+X47+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+Y47","v":1.2},4.2000010999999997,1.2,{"$f":"+AB77","v":{"$error":"#VALUE!"}},{"$f":"(AB48*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47+'Analiza i dimenzioniranje'!H76","v":1.5001009999999999}]
[5,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.14,{"$f":"+D16","v":{"$error":"#VALUE!"}},{"$f":"+E16+'Unos podataka'!$F9","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AF44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XVI-XVII'!L47,'C XVI-XVII'!B6)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AF44<'Analiza i dimenzioniranje'!F45,I49,'C XVI-XVII'!V34)","v":4.72},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AF44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AF44,K49)","v":4.72},{"$f":"IF('Analiza i dimenzioniranje'!AG44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XVI-XVII'!B6,P47)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AG44<'Analiza i dimenzioniranje'!F45,'C XVI-XVII'!I49,Q48)","v":5.04},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AG44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AG44,K49)","v":5.04},{"$f":"+U23","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},{"$f":"+V48+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+W48","v":1.2},{"$f":"+AB49","v":4.2000010999999997},{"$f":"+AC49","v":0.37931024673015767},4.2000010999999997,1.2,{"$f":"+AB47+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+(AB49*(AC43-AC53)/(AB43-AB53)-AB53*(AC43-AC53)/(AB43-AB53)+AC53)","v":0.37931024673015767},"Presjek XVI-I",null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+AI48","v":1.5001009999999999}]
[6,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.44,3.4000010999999999,1.2,{"$error":"#VALUE!"},3.44,{"$f":"IF('Unos podataka'!$B$105>J47,'Unos podataka'!$B$105,J47)","v":{"$error":"#VALUE!"}},{"$f":"+K51","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AF44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XVI-XVII'!L48,'C XVI-XVII'!B7)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AF44<='Analiza i dimenzioniranje'!F45,I50,'C XVI-XVII'!V34)","v":4.72},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AF44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AF44,K50)","v":4.72},{"$f":"IF('Analiza i dimenzioniranje'!AG44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XVI-XVII'!P47,H50)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AG44<='Analiza i dimenzioniranje'!F45,I50,V29)","v":5.04},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AG44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AG44,K50)","v":5.04},{"$f":"+U24","v":4.9000021999999994},{"$f":"+V24*100","v":0},{"$f":"+V49","v":3.4000010999999999},{"$f":"+AC47","v":0.24137931688465614},{"$f":"+X47","v":3.4000010999999999},{"$f":"+AC47","v":0.24137931688465614},4.9000021999999994,1.2,{"$f":"2+'Analiza i dimenzioniranje'!E61/2","v":3.4500010999999997},{"$f":"(AB50*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24999999999999994},null,null,null,null,{"$f":"+AH49","v":4.9000021999999994},{"$f":"+C14","v":1.2}]
[7,4.9000021999999994,1.2,{"$error":"#VALUE!"},3.44,2,1.2,{"$error":"#VALUE!"},3.44,{"$f":"+D18","v":{"$error":"#VALUE!"}},{"$f":"+E18+'Unos podataka'!$F9","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AF44>'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XVI-XVII'!B28,B8)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AF44>='Analiza i dimenzioniranje'!I75+'Analiza i dimenzioniranje'!G67,'C XVI-XVII'!M50,Z26)","v":4.72},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AF44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AF44,K51)","v":4.72},{"$f":"IF('Analiza i dimenzioniranje'!AG44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XVI-XVII'!B25,H51)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AG44<='Analiza i dimenzioniranje'!F45,I51,V29)","v":5.04},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AG44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AG44,K51)","v":5.04},{"$f":"+U25","v":2},{"$f":"+V25*100","v":0},{"$f":"+V47","v":2},{"$f":"+W47","v":0},{"$f":"+X47","v":3.4000010999999999},{"$f":"+Y47","v":1.2},4.9000021999999994,0.5,{"$f":"+(AB49+AB53)/2","v":4.5500016499999996},{"$f":"(AB51*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.43965512336507878},null,null,null,null,{"$f":"+B13","v":4.2000010999999997},{"$f":"+C13","v":1.2}]
[8,4.9000021999999994,0.5,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",{"$error":"#VALUE!"},3.44,{"$f":"+H52","v":{"$error":"#VALUE!"}},{"$f":"+Q52","v":"A"},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AF44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AF44,K52)","v":4.72},{"$f":"+H52","v":{"$error":"#VALUE!"}},{"$f":"+I52","v":"A"},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AG44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AG44,K52)","v":5.04},null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AC49","v":0.37931024673015767},{"$f":"+AD77","v":{"$error":"#VALUE!"}},{"$f":"(AB52*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH51","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[9,2,0.12820515121628623,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",null,null,{"$f":"+H53","v":{"$error":"#VALUE!"}},{"$f":"+Q53","v":"A"},null,null,{"$f":"+H53","v":{"$error":"#VALUE!"}},{"$f":"+I53","v":"A"},null,null,null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AA47","v":1.2},{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+C15","v":0.5},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[10,null,null,4.2000010999999997,1.2,null,null,{"$error":"#VALUE!"},1.2,null,null,{"$f":"+U35","v":{"$error":"#VALUE!"}},{"$f":"+M47","v":4.72},null,null,{"$f":"+U30","v":{"$error":"#VALUE!"}},{"$f":"+V30","v":5.04},null,null,null,null,null,null,null,null,null,null,"Koordinate s","naprezanjem"]
[11,null,null,{"$f":"+D47","v":3.4000010999999999},{"$f":"+E47","v":1.2},null,null,3.4000010999999999,1.2,null,null,{"$f":"+L47","v":{"$error":"#VALUE!"}},{"$f":"+M47","v":4.72},null,null,{"$f":"+P47","v":{"$error":"#VALUE!"}},{"$f":"+Q47","v":5.04},null,null,null,null,null,null,null,null,null,null,{"$f":"+U22","v":2},{"$f":"+V22*100","v":{"$error":"#VALUE!"}}]
[12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+AB56*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
[13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AB57*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
["  A=",{"$f":"-0.5*((B45*C46-B46*C45)+(B46*C47-B47*C46)+(B47*C48-B48*C47)+(B48*C49-B49*C48)+(B49*C50-B50*C49)+(B50*C51-B51*C50)+(B51*C52-B52*C51)+(B52*C53-B53*C52))","v":2.5691044797107181},"m2",{"$f":"-0.5*((D45*E46-D46*E45)+(D46*E47-D47*E46)+(D47*E48-D48*E47)+(D48*E49-D49*E48)+(D49*E50-D50*E49)+(D50*E51-D51*E50)+(D51*E52-D52*E51)+(D52*E53-D53*E52)+(D53*E54-D54*E53)+(D54*E55-D55*E54)+(D55*E56-D56*E55)+(D56*E57-D57*E56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((F45*G46-F46*G45)+(F46*G47-F47*G46)+(F47*G48-F48*G47)+(F48*G49-F49*G48)+(F49*G50-F50*G49)+(F50*G51-F51*G50)+(F51*G52-F52*G51)+(F52*G53-F53*G52)+(F53*G54-F54*G53)+(F54*G55-F55*G54)+(F55*G56-F56*G55)+(F56*G57-F57*G56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((H47*I48-H48*I47)+(H48*I49-H49*I48)+(H49*I50-H50*I49)+(H50*I51-H51*I50)+(H51*I52-H52*I51)+(H52*I53-H53*I52)+(H53*I54-H54*I53)+(H54*I55-H55*I54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((J47*K48-J48*K47)+(J48*K49-J49*K48)+(J49*K50-J50*K49)+(J50*K51-J51*K50)+(J51*K52-J52*K51)+(J52*K53-J53*K52)+(J53*K54-J54*K53)+(J54*K55-J55*K54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((L47*M48-L48*M47)+(L48*M49-L49*M48)+(L49*M50-L50*M49)+(L50*M51-L51*M50)+(L51*M52-L52*M51)+(L52*M53-L53*M52)+(L53*M54-L54*M53)+(L54*M55-L55*M54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"IF(0.5*((N47*O48-N48*O47)+(N48*O49-N49*O48)+(N49*O50-N50*O49)+(N50*O51-N51*O50)+(N51*O52-N52*O51)+(N52*O53-N53*O52)+(N53*O54-N54*O53)+(N54*O55-N55*O54))<0,0,0.5*((N47*O48-N48*O47)+(N48*O49-N49*O48)+(N49*O50-N50*O49)+(N50*O51-N51*O50)+(N51*O52-N52*O51)+(N52*O53-N53*O52)+(N53*O54-N54*O53)+(N54*O55-N55*O54)))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((P47*Q48-P48*Q47)+(P48*Q49-P49*Q48)+(P49*Q50-P50*Q49)+(P50*Q51-P51*Q50)+(P51*Q52-P52*Q51)+(P52*Q53-P53*Q52)+(P53*Q54-P54*Q53)+(P54*Q55-P55*Q54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((R47*S48-R48*S47)+(R48*S49-R49*S48)+(R49*S50-R50*S49)+(R50*S51-R51*S50)+(R51*S52-R52*S51)+(R52*S53-R53*S52)+(R53*S54-R54*S53)+(R54*S55-R55*S54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((T47*U48-T48*U47)+(T48*U49-T49*U48)+(T49*U50-T50*U49)+(T50*U51-T51*U50)+(T51*U52-T52*U51)+(T52*U53-T53*U52)+(T53*U54-T54*U53)+(T54*U55-T55*U54))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((V47*W48-V48*W47)+(V48*W49-V49*W48)+(V49*W50-V50*W49)+(V50*W51-V51*W50))","v":1.5110356654221164},"m2",{"$f":"-0.5*((X47*Y48-X48*Y47)+(X48*Y49-X49*Y48)+(X49*Y50-X50*Y49)+(X50*Y51-X51*Y50))","v":0.71172417455407389},"m2",{"$f":"-0.5*((Z47*AA48-Z48*AA47)+(Z48*AA49-Z49*AA48)+(Z49*AA50-Z50*AA49)+(Z50*AA51-Z51*AA50)+(Z51*AA52-Z52*AA51)+(Z52*AA53-Z53*AA52)+(Z53*AA54-Z54*AA53)+(Z54*AA55-Z55*AA54))","v":0.53224225002380887},"m2",{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-0.5*((AH47*AI48-AH48*AI47)+(AH48*AI49-AH49*AI48)+(AH49*AI50-AH50*AI49)+(AH50*AI51-AH51*AI50)+(AH51*AI52-AH52*AI51)+(AH52*AI53-AH53*AI52)+(AH53*AI54-AH54*AI53)+(AH54*AI55-AH55*AI54))","v":0.21007103011109951},"m2"]
["xt=",{"$f":"-((B45*C46-B46*C45)*(B45+B46)+(B46*C47-B47*C46)*(B46+B47)+(B47*C48-B48*C47)*(B47+B48)+(B48*C49-B49*C48)*(B48+B49)+(B49*C50-B50*C49)*(B49+B50)+(B50*C51-B51*C50)*(B50+B51)+(B51*C52-B52*C51)*(B51+B52)+(B52*C53-B53*C52)*(B52+B53)+(B53*C54-B54*C53)*(B53+B54)+(B54*C55-B55*C54)*(B54+B55)+(B55*C56-B56*C55)*(B55+B56)+(B56*C57-B57*C56)*(B56+B57))/6/B58","v":3.3485779696489133},"m",{"$f":"-((D45*E46-D46*E45)*(D45+D46)+(D46*E47-D47*E46)*(D46+D47)+(D47*E48-D48*E47)*(D47+D48)+(D48*E49-D49*E48)*(D48+D49)+(D49*E50-D50*E49)*(D49+D50)+(D50*E51-D51*E50)*(D50+D51)+(D51*E52-D52*E51)*(D51+D52)+(D52*E53-D53*E52)*(D52+D53)+(D53*E54-D54*E53)*(D53+D54)+(D54*E55-D55*E54)*(D54+D55)+(D55*E56-D56*E55)*(D55+D56)+(D56*E57-D57*E56)*(D56+D57))/6/D58","v":{"$error":"#VALUE!"}},"m",{"$f":"-((F45*G46-F46*G45)*(F45+F46)+(F46*G47-F47*G46)*(F46+F47)+(F47*G48-F48*G47)*(F47+F48)+(F48*G49-F49*G48)*(F48+F49)+(F49*G50-F50*G49)*(F49+F50)+(F50*G51-F51*G50)*(F50+F51)+(F51*G52-F52*G51)*(F51+F52)+(F52*G53-F53*G52)*(F52+F53)+(F53*G54-F54*G53)*(F53+F54)+(F54*G55-F55*G54)*(F54+F55)+(F55*G56-F56*G55)*(F55+F56)+(F56*G57-F57*G56)*(F56+F57))/6/F58","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(H47*I48-H48*I47)*(H47+H48)+(H48*I49-H49*I48)*(H48+H49)+(H49*I50-H50*I49)*(H49+H50)+(H50*I51-H51*I50)*(H50+H51)+(H51*I52-H52*I51)*(H51+H52)+(H52*I53-H53*I52)*(H52+H53)+(H53*I54-H54*I53)*(H53+H54)+(H54*I55-H55*I54)*(H54+H55))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(J47+J48)+(J48*K49-J49*K48)*(J48+J49)+(J49*K50-J50*K49)*(J49+J50)+(J50*K51-J51*K50)*(J50+J51)+(J51*K52-J52*K51)*(J51+J52)+(J52*K53-J53*K52)*(J52+J53)+(J53*K54-J54*K53)*(J53+J54)+(J54*K55-J55*K54)*(J54+J55)+(J55*K56-J56*K55)*(J55+J56)+(J56*K57-J57*K56)*(J56+J57))/6/J58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(L47*M48-L48*M47)*(L47+L48)+(L48*M49-L49*M48)*(L48+L49)+(L49*M50-L50*M49)*(L49+L50)+(L50*M51-L51*M50)*(L50+L51)+(L51*M52-L52*M51)*(L51+L52)+(L52*M53-L53*M52)*(L52+L53)+(L53*M54-L54*M53)*(L53+L54)+(L54*M55-L55*M54)*(L54+L55))/6/L58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(N58=0,0,(+(N47*O48-N48*O47)*(N47+N48)+(N48*O49-N49*O48)*(N48+N49)+(N49*O50-N50*O49)*(N49+N50)+(N50*O51-N51*O50)*(N50+N51)+(N51*O52-N52*O51)*(N51+N52))/6/N58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(P47*Q48-P48*Q47)*(P47+P48)+(P48*Q49-P49*Q48)*(P48+P49)+(P49*Q50-P50*Q49)*(P49+P50)+(P50*Q51-P51*Q50)*(P50+P51)+(P51*Q52-P52*Q51)*(P51+P52)+(P52*Q53-P53*Q52)*(P52+P53)+(P53*Q54-P54*Q53)*(P53+P54)+(P54*Q55-P55*Q54)*(P54+P55))/6/P58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(R58=0,0,(+(R47*S48-R48*S47)*(R47+R48)+(R48*S49-R49*S48)*(R48+R49)+(R49*S50-R50*S49)*(R49+R50)+(R50*S51-R51*S50)*(R50+R51)+(R51*S52-R52*S51)*(R51+R52))/6/R58)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(T58=0,0,(+(T47*U48-T48*U47)*(T47+T48)+(T48*U49-T49*U48)*(T48+T49)+(T49*U50-T50*U49)*(T49+T50)+(T50*U51-T51*U50)*(T50+T51)+(T51*U52-T52*U51)*(T51+T52)+(T52*U53-T53*U52)*(T52+T53)+(T53*U54-T54*U53)*(T53+T54)+(T54*U55-T55*U54)*(T54+T55)+(T55*U56-T56*U55)*(T55+T56)+(T56*U57-T57*U56)*(T56+T57))/6/T58)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(V58=0,0,-(+(V47*W48-V48*W47)*(V47+V48)+(V48*W49-V49*W48)*(V48+V49)+(V49*W50-V50*W49)*(V49+V50)+(V50*W51-V51*W50)*(V50+V51))/6/V58)","v":2.6739089419190427},"m",{"$f":"IF(X58=0,0,-(+(X47*Y48-X48*Y47)*(X47+X48)+(X48*Y49-X49*Y48)*(X48+X49)+(X49*Y50-X50*Y49)*(X49+X50)+(X50*Y51-X51*Y50)*(X50+X51))/6/X58)","v":3.7896651910602248},"m",{"$f":"-(+(Z47*AA48-Z48*AA47)*(Z47+Z48)+(Z48*AA49-Z49*AA48)*(Z48+Z49)+(Z49*AA50-Z50*AA49)*(Z49+Z50)+(Z50*AA51-Z51*AA50)*(Z50+Z51)+(Z51*AA52-Z52*AA51)*(Z51+Z52)+(Z52*AA53-Z53*AA52)*(Z52+Z53)+(Z53*AA54-Z54*AA53)*(Z53+Z54)+(Z54*AA55-Z55*AA54)*(Z54+Z55)+(Z55*AA56-Z56*AA55)*(Z55+Z56)+(Z56*AA57-Z57*AA56)*(Z56+Z57))/6/Z58","v":4.5407423692617748},"m",null,null,null,null,"   Koordinate presjeka",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AH47+AH48)+(AH48*AI49-AH49*AI48)*(AH48+AH49)+(AH49*AI50-AH50*AI49)*(AH49+AH50)+(AH50*AI51-AH51*AI50)*(AH50+AH51)+(AH51*AI52-AH52*AI51)*(AH51+AH52)+(AH52*AI53-AH53*AI52)*(AH52+AH53)+(AH53*AI54-AH54*AI53)*(AH53+AH54)+(AH54*AI55-AH55*AI54)*(AH54+AH55)+(AH55*AI56-AH56*AI55)*(AH55+AH56)+(AH56*AI57-AH57*AI56)*(AH56+AH57))/6/AH58","v":4.550001650000004},"m"]
["yt=",{"$f":"-((B45*C46-B46*C45)*(C45+C46)+(B46*C47-B47*C46)*(C46+C47)+(B47*C48-B48*C47)*(C47+C48)+(B48*C49-B49*C48)*(C48+C49)+(B49*C50-B50*C49)*(C49+C50)+(B50*C51-B51*C50)*(C50+C51)+(B51*C52-B52*C51)*(C51+C52)+(B52*C53-B53*C52)*(C52+C53)+(B53*C54-B54*C53)*(C53+C54)+(B54*C55-B55*C54)*(C54+C55)+(B55*C56-B56*C55)*(C55+C56)+(B56*C57-B57*C56)*(C56+C57))/6/B58","v":0.75054981042380386},"m",{"$f":"-((D45*E46-D46*E45)*(E45+E46)+(D46*E47-D47*E46)*(E46+E47)+(D47*E48-D48*E47)*(E47+E48)+(D48*E49-D49*E48)*(E48+E49)+(D49*E50-D50*E49)*(E49+E50)+(D50*E51-D51*E50)*(E50+E51)+(D51*E52-D52*E51)*(E51+E52)+(D52*E53-D53*E52)*(E52+E53)+(D53*E54-D54*E53)*(E53+E54)+(D54*E55-D55*E54)*(E54+E55)+(D55*E56-D56*E55)*(E55+E56)+(D56*E57-D57*E56)*(E56+E57))/6/D58","v":{"$error":"#VALUE!"}},"m",{"$f":"-((F45*G46-F46*G45)*(G45+G46)+(F46*G47-F47*G46)*(G46+G47)+(F47*G48-F48*G47)*(G47+G48)+(F48*G49-F49*G48)*(G48+G49)+(F49*G50-F50*G49)*(G49+G50)+(F50*G51-F51*G50)*(G50+G51)+(F51*G52-F52*G51)*(G51+G52)+(F52*G53-F53*G52)*(G52+G53)+(F53*G54-F54*G53)*(G53+G54)+(F54*G55-F55*G54)*(G54+G55)+(F55*G56-F56*G55)*(G55+G56)+(F56*G57-F57*G56)*(G56+G57))/6/F58","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(H47*I48-H48*I47)*(I47+I48)+(H48*I49-H49*I48)*(I48+I49)+(H49*I50-H50*I49)*(I49+I50)+(H50*I51-H51*I50)*(I50+I51)+(H51*I52-H52*I51)*(I51+I52)+(H52*I53-H53*I52)*(I52+I53)+(H53*I54-H54*I53)*(I53+I54)+(H54*I55-H55*I54)*(I54+I55)+(H55*I56-H56*I55)*(I55+I56)+(H56*I57-H57*I56)*(I56+I57))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(K47+K48)+(J48*K49-J49*K48)*(K48+K49)+(J49*K50-J50*K49)*(K49+K50)+(J50*K51-J51*K50)*(K50+K51)+(J51*K52-J52*K51)*(K51+K52)+(J52*K53-J53*K52)*(K52+K53)+(J53*K54-J54*K53)*(K53+K54)+(J54*K55-J55*K54)*(K54+K55)+(J55*K56-J56*K55)*(K55+K56)+(J56*K57-J57*K56)*(K56+K57))/6/J58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(L47*M48-L48*M47)*(M47+M48)+(L48*M49-L49*M48)*(M48+M49)+(L49*M50-L50*M49)*(M49+M50)+(L50*M51-L51*M50)*(M50+M51)+(L51*M52-L52*M51)*(M51+M52)+(L52*M53-L53*M52)*(M52+M53)+(L53*M54-L54*M53)*(M53+M54)+(L54*M55-L55*M54)*(M54+M55))/6/L58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(N58=0,0,(+(N47*O48-N48*O47)*(O47+O48)+(N48*O49-N49*O48)*(O48+O49)+(N49*O50-N50*O49)*(O49+O50)+(N50*O51-N51*O50)*(O50+O51)+(N51*O52-N52*O51)*(O51+O52)+(N52*O53-N53*O52)*(O52+O53)+(N53*O54-N54*O53)*(O53+O54)+(N54*O55-N55*O54)*(O54+O55)+(N55*O56-N56*O55)*(O55+O56)+(N56*O57-N57*O56)*(O56+O57))/6/N58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(P47*Q48-P48*Q47)*(Q47+Q48)+(P48*Q49-P49*Q48)*(Q48+Q49)+(P49*Q50-P50*Q49)*(Q49+Q50)+(P50*Q51-P51*Q50)*(Q50+Q51)+(P51*Q52-P52*Q51)*(Q51+Q52)+(P52*Q53-P53*Q52)*(Q52+Q53)+(P53*Q54-P54*Q53)*(Q53+Q54)+(P54*Q55-P55*Q54)*(Q54+Q55))/6/P58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(R58=0,0,(+(R47*S48-R48*S47)*(S47+S48)+(R48*S49-R49*S48)*(S48+S49)+(R49*S50-R50*S49)*(S49+S50)+(R50*S51-R51*S50)*(S50+S51)+(R51*S52-R52*S51)*(S51+S52)+(R52*S53-R53*S52)*(S52+S53)+(R53*S54-R54*S53)*(S53+S54)+(R54*S55-R55*S54)*(S54+S55)+(R55*S56-R56*S55)*(S55+S56)+(R56*S57-R57*S56)*(S56+S57))/6/R58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-IF(T58=0,0,(+(T47*U48-T48*U47)*(U47+U48)+(T48*U49-T49*U48)*(U48+U49)+(T49*U50-T50*U49)*(U49+U50)+(T50*U51-T51*U50)*(U50+U51)+(T51*U52-T52*U51)*(U51+U52)+(T52*U53-T53*U52)*(U52+U53)+(T53*U54-T54*U53)*(U53+U54)+(T54*U55-T55*U54)*(U54+U55)+(T55*U56-T56*U55)*(U55+U56)+(T56*U57-T57*U56)*(U56+U57))/6/T58)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((V47*W48-V48*W47)*(W47+W48)+(V48*W49-V49*W48)*(W48+W49)+(V49*W50-V50*W49)*(W49+W50)+(V50*W51-V51*W50)*(W50+W51))/6/V58","v":0.65809555436880718},"kN",{"$f":"-((X47*Y48-X48*Y47)*(Y47+Y48)+(X48*Y49-X49*Y48)*(Y48+Y49)+(X49*Y50-X50*Y49)*(Y49+Y50)+(X50*Y51-X51*Y50)*(Y50+Y51))/6/X58","v":0.75428136494691478},"kN",{"$f":"-(+(Z47*AA48-Z48*AA47)*(AA47+AA48)+(Z48*AA49-Z49*AA48)*(AA48+AA49)+(Z49*AA50-Z50*AA49)*(AA49+AA50)+(Z50*AA51-Z51*AA50)*(AA50+AA51)+(Z51*AA52-Z52*AA51)*(AA51+AA52)+(Z52*AA53-Z53*AA52)*(AA52+AA53)+(Z53*AA54-Z54*AA53)*(AA53+AA54)+(Z54*AA55-Z55*AA54)*(AA54+AA55)+(Z55*AA56-Z56*AA55)*(AA55+AA56)+(Z56*AA57-Z57*AA56)*(AA56+AA57))/6/Z58","v":0.81902934843133712},"m",null,null,null,null,"II-II i I-I",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AI47+AI48)+(AH48*AI49-AH49*AI48)*(AI48+AI49)+(AH49*AI50-AH50*AI49)*(AI49+AI50)+(AH50*AI51-AH51*AI50)*(AI50+AI51)+(AH51*AI52-AH52*AI51)*(AI51+AI52)+(AH52*AI53-AH53*AI52)*(AI52+AI53)+(AH53*AI54-AH54*AI53)*(AI53+AI54)+(AH54*AI55-AH55*AI54)*(AI54+AI55)+(AH55*AI56-AH56*AI55)*(AI55+AI56)+(AH56*AI57-AH57*AI56)*(AI56+AI57))/6/AH58","v":1.3500505000000005},"m"]
["G=",{"$f":"+B58*'Analiza i dimenzioniranje'!E62","v":64.227611992767947},"kN",{"$f":"+D58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"+F58*'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}},"kN",{"$f":"+H58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(J58*'Analiza i dimenzioniranje'!E63<0,0,J58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+L58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(N58*'Analiza i dimenzioniranje'!U41<0,0,N58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+P58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(R58<=0,0,R58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+T58*'Analiza i dimenzioniranje'!E49","v":{"$error":"#VALUE!"}},"kN (za L)",{"$f":"+V58*'Analiza i dimenzioniranje'!E62","v":37.77589163555291},"kN",{"$f":"+X58*'Analiza i dimenzioniranje'!E62","v":17.793104363851846},"kN",{"$f":"+Z58*'Analiza i dimenzioniranje'!E62","v":13.306056250595223},"kN",null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"AC47+'Analiza i dimenzioniranje'!C192/2","v":0.68753317931068247},{"$f":"+AH58*'Analiza i dimenzioniranje'!E62","v":5.2517757527774878},"kN"]
["Vertikala nasipa na konzoli",null,null,"Moment na konzoli",null,"Pokos na vrhu zida",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - NAPONI ",null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+'C XVI-XVII'!AC49+('Analiza i dimenzioniranje'!C191/2)","v":0.77418208680245293}]
[null,"x","y",{"$f":"IF('Analiza i dimenzioniranje'!G78=0,0,'Analiza i dimenzioniranje'!G78*'Analiza i dimenzioniranje'!C77*'Analiza i dimenzioniranje'!E62*(Q20-B5+'Analiza i dimenzioniranje'!G78/2)+J61*(O16-J59))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"+F64","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"naponi za Presjek XVII-II",null,"naponi za srednji dio ",null,"naponi za Presjek XVI-I"]
[null,{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},"b1=",{"$f":"+H47-2","v":1.4000010999999999},{"$f":"+B52","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y","x","y","x","y","Koordinate dna temelja"]
[null,{"$f":"+B64","v":{"$error":"#VALUE!"}},{"$f":"IF(B65>J49,C19,+C20+'Analiza i dimenzioniranje'!F20+(H52-H50)*TAN('Analiza i dimenzioniranje'!F21*PI()/180))","v":{"$error":"#VALUE!"}},"b2=",{"$f":"'Analiza i dimenzioniranje'!E54+('Analiza i dimenzioniranje'!E55-'Analiza i dimenzioniranje'!E54)*(('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)/(C9-C4))","v":{"$error":"#VALUE!"}},{"$f":"+B65","v":{"$error":"#VALUE!"}},{"$f":"+G64+(F64-F65)*TAN('Analiza i dimenzioniranje'!F21*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,0,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},0,{"$f":"+'C XVI-XVII'!B11","v":4.2000010999999997},{"$f":"-U47","v":0},2,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z65","v":2},{"$f":"AC55","v":{"$error":"#VALUE!"}},{"$f":"+AB65","v":3.4000010999999999},{"$f":"+AA67","v":{"$error":"#VALUE!"}},{"$f":"+AB57","v":4.2000010999999997},{"$f":"AC57","v":{"$error":"#VALUE!"}},{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"(AF66*(AG70-AG65)/(AF70-AF65)-AF65*(AG70-AG65)/(AF70-AF65)+AG65)","v":{"$error":"#VALUE!"}}]
[null,"AKTIVNI TLAKOVI za stabilnost i Presjek III-III (bez E3)",null,null,null,null,null,null,"  AKTIVNI TLAKOVI za presjek kroz zid XVI-XVI",null,null,null,null,"    AKTIVNI TLAKOVI za presjek kroz zid XVII-XVII",null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"AC56","v":{"$error":"#VALUE!"}},{"$f":"+AB66+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AE66","v":{"$error":"#VALUE!"}},{"$f":"+AB58","v":4.9000021999999994},{"$f":"+AC58","v":{"$error":"#VALUE!"}},{"$f":"+AB77","v":{"$error":"#VALUE!"}},{"$f":"+(AF67*(AG65-AG70)/(AF65-AF70)-AF70*(AG65-AG70)/(AF65-AF70)+AG70)","v":{"$error":"#VALUE!"}}]
[null,"E1",null,"E2",null,"E3",null,null,"E1",null,"E2 do presjeka kroz zid II",null,null,"E1",null,"E2",null,null,null,null,null,null,null,null,null,{"$f":"+Z67","v":3.4000010999999999},0,{"$f":"+AB67","v":4.2000010999999997},0,{"$f":"+AD67","v":4.9000021999999994},{"$f":"+U50","v":0},{"$f":"+AB67","v":4.2000010999999997},{"$f":"+(AF68*(AG65-AG70)/(AF65-AF70)-AF70*(AG65-AG70)/(AF65-AF70)+AG70)","v":0.37931024673015767}]
[null,0,{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C71","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,{"$f":"+N69","v":0},{"$f":"+O69","v":{"$error":"#VALUE!"}},{"$f":"+I71","v":{"$error":"#VALUE!"}},{"$f":"+L76","v":{"$error":"#VALUE!"}},null,{"$f":"+B69","v":0},{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+N71","v":{"$error":"#VALUE!"}},{"$f":"+O71","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"+Z65","v":2},0,{"$f":"+AB65","v":3.4000010999999999},0,{"$f":"+AD65","v":4.2000010999999997},{"$f":"+U51","v":0},{"$f":"+AD77","v":{"$error":"#VALUE!"}},{"$f":"+(AF69*(AG66-AG70)/(AF66-AF70)-AF70*(AG66-AG70)/(AF66-AF70)+AG70)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+B69","v":0},{"$f":"+C69-'Analiza i dimenzioniranje'!D17-'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+D69+'Analiza i dimenzioniranje'!E16*'Analiza i dimenzioniranje'!E17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+E69-'Analiza i dimenzioniranje'!E17","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},null,{"$f":"+N70","v":0},{"$f":"+J69-('Analiza i dimenzioniranje'!F20+'P XVI-XVI'!E17)","v":{"$error":"#VALUE!"}},{"$f":"+K69+'P XVI-XVI'!F16*'P XVI-XVI'!F17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72},null,{"$f":"+B70","v":0},{"$f":"+O69-('Analiza i dimenzioniranje'!F20+'P XVII-XVII'!E17)","v":{"$error":"#VALUE!"}},{"$f":"+P69+'P XVII-XVII'!F16*'P XVII-XVII'!F17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AG44","v":5.04},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AB53","v":4.9000021999999994},{"$f":"+AC53","v":0.5}]
[null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('Analiza i dimenzioniranje'!D17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},0,{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F70+'Analiza i dimenzioniranje'!F16*'Analiza i dimenzioniranje'!F17*'Analiza i dimenzioniranje'!F112","v":{"$error":"#VALUE!"}},0,null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('P XVI-XVI'!E17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+J70","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+L70","v":4.72},null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('P XVII-XVII'!E17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+Q70","v":5.04}]
[null,{"$f":"+B69","v":0},{"$f":"+C69","v":{"$error":"#VALUE!"}},0,{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F69","v":0},0,null,{"$f":"+N72","v":0},{"$f":"+O72","v":{"$error":"#VALUE!"}},{"$f":"+D72","v":0},{"$f":"+L69","v":{"$error":"#VALUE!"}},null,{"$f":"+N69","v":0},{"$f":"+O69","v":{"$error":"#VALUE!"}},{"$f":"+D72","v":0},{"$f":"+Q69","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+D69","v":{"$error":"#VALUE!"}},{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F72","v":0},{"$f":"+G70","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+K69","v":{"$error":"#VALUE!"}},{"$f":"+L69","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+P69","v":{"$error":"#VALUE!"}},{"$f":"+Q69","v":{"$error":"#VALUE!"}}]
[null,"Jednadžba vertikale kohezije    Određivanje sjecišta kohezije s pravcem od tlaka",null,null,null,null,null,{"$f":"+M74","v":"Jednadžba vertikale kohezije  -  sjecišta kohezije s pravcem od tlaka"},null,null,null,null,"Jednadžba vertikale kohezije  -  sjecišta kohezije s pravcem od tlaka"]
[null,"X","y","X","y","X","y",null,{"$f":"+N75","v":"X"},{"$f":"+O75","v":"y"},"X","y",null,"X","y","X","y"]
[null,{"$f":"2*'Analiza i dimenzioniranje'!D15/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F110)","v":12.361875887090893},{"$f":"B76*(C71-C72)/(B71-B72)-B72*(C71-C72)/(B71-B72)+C72","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!F12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F111)","v":{"$error":"#VALUE!"}},{"$f":"IF(D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69>'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69)","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!C12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F112)","v":{"$error":"#VALUE!"}},{"$f":"IF((F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70)>'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!F17,(F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70))","v":{"$error":"#VALUE!"}},null,{"$f":"+N76","v":12.361875887090893},{"$f":"I76*(J71-J72)/(I71-I72)-I72*(J71-J72)/(I71-I72)+J72","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},null,{"$f":"+B76","v":12.361875887090893},{"$f":"N76*(O71-O72)/(N71-N72)-N72*(O71-O72)/(N71-N72)+O72","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"-0.5*((Z65*AA66-Z66*AA65)+(Z66*AA67-Z67*AA66)+(Z67*AA68-Z68*AA67)+(Z68*AA69-Z69*AA68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((AB65*AC66-AB66*AC65)+(AB66*AC67-AB67*AC66)+(AB67*AC68-AB68*AC67)+(AB68*AC69-AB69*AC68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((AD65*AE66-AD66*AE65)+(AD66*AE67-AD67*AE66)+(AD67*AE68-AD68*AE67)+(AD68*AE69-AD69*AE68)+(AD69*AE70-AD70*AE69)+(AD70*AE71-AD71*AE70)+(AD71*AE72-AD72*AE71)+(AD72*AE73-AD73*AE72))","v":{"$error":"#VALUE!"}},"kN/m'"]
[null,{"$f":"+B76","v":12.361875887090893},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},null,{"$f":"+N77","v":12.361875887090893},{"$f":"+J70","v":{"$error":"#VALUE!"}},{"$f":"+K76","v":{"$error":"#VALUE!"}},{"$f":"+L70","v":4.72},null,{"$f":"+N76","v":12.361875887090893},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+P76","v":{"$error":"#VALUE!"}},{"$f":"+Q70","v":5.04},null,null,null,null,null,null,null,null,{"$f":"IF(Z76=0,0,-(+(Z65*AA66-Z66*AA65)*(Z65+Z66)+(Z66*AA67-Z67*AA66)*(Z66+Z67)+(Z67*AA68-Z68*AA67)*(Z67+Z68)+(Z68*AA69-Z69*AA68)*(Z68+Z69))/6/Z76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(AB76=0,0,-(+(AB65*AC66-AB66*AC65)*(AB65+AB66)+(AB66*AC67-AB67*AC66)*(AB66+AB67)+(AB67*AC68-AB68*AC67)*(AB67+AB68)+(AB68*AC69-AB69*AC68)*(AB68+AB69))/6/AB76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(AD76=0,0,-(+(AD65*AE66-AD66*AE65)*(AD65+AD66)+(AD66*AE67-AD67*AE66)*(AD66+AD67)+(AD67*AE68-AD68*AE67)*(AD67+AD68)+(AD68*AE69-AD69*AE68)*(AD68+AD69))/6/AD76)","v":{"$error":"#VALUE!"}},"m"]
["Oznaka","E1",null,"E2",null,"E3",null,{"$f":"+M78","v":"Oznaka"},{"$f":"+N78","v":"E1"},null,"E2",null,"Oznaka","E1",null,"E2",null,null,null,null,null,null,null,null,null,{"$f":"-((Z65*AA66-Z66*AA65)*(AA65+AA66)+(Z66*AA67-Z67*AA66)*(AA66+AA67)+(Z67*AA68-Z68*AA67)*(AA67+AA68)+(Z68*AA69-Z69*AA68)*(AA68+AA69))/6/Z76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((AB65*AC66-AB66*AC65)*(AC65+AC66)+(AB66*AC67-AB67*AC66)*(AC66+AC67)+(AB67*AC68-AB68*AC67)*(AC67+AC68)+(AB68*AC69-AB69*AC68)*(AC68+AC69))/6/AB76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((AD65*AE66-AD66*AE65)*(AE65+AE66)+(AD66*AE67-AD67*AE66)*(AE66+AE67)+(AD67*AE68-AD68*AE67)*(AE67+AE68)+(AD68*AE69-AD69*AE68)*(AE68+AE69))/6/AD76","v":{"$error":"#VALUE!"}},"kN/m'"]
["točke","x","y","x","y","x","y","točke",{"$f":"+N79","v":"x"},{"$f":"+O79","v":"y"},"x","y","točke","x","y","x","y"]
[1,{"$f":"+B77","v":12.361875887090893},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,1,{"$f":"+N80","v":12.361875887090893},{"$f":"+J76","v":{"$error":"#VALUE!"}},{"$f":"+K69","v":{"$error":"#VALUE!"}},{"$f":"+L69","v":{"$error":"#VALUE!"}},1,{"$f":"+N76","v":12.361875887090893},{"$f":"+O76","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17<'Analiza i dimenzioniranje'!AG44,0,P77)","v":0},{"$f":"+Q69","v":{"$error":"#VALUE!"}},null,"Jedn pravca zida uz tlo",null,"Jedn pravca arm dno ",null,"Y=",{"$f":"IF(S82=S81,1000000,(T82-T81)/(S82-S81))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X80*S81+T81","v":{"$error":"#VALUE!"}}]
[2,{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G76","v":{"$error":"#VALUE!"}},2,{"$f":"+I71","v":{"$error":"#VALUE!"}},{"$f":"+J70","v":{"$error":"#VALUE!"}},{"$f":"+K70","v":{"$error":"#VALUE!"}},4.72,2,{"$f":"+N71","v":{"$error":"#VALUE!"}},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+P69","v":{"$error":"#VALUE!"}},{"$f":"+Q70","v":5.04},null,{"$f":"+B4","v":3.4000010999999999},{"$f":"+C4","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!T593","v":2.0499999999999998},{"$f":"+'Analiza i dimenzioniranje'!U593","v":0.18682583433163008},"X=",{"$f":"+(-Z80+Z83)/(X80-X83)","v":{"$error":"#VALUE!"}},"sjeište"]
[3,{"$f":"+B80","v":12.361875887090893},{"$f":"+C76","v":{"$error":"#VALUE!"}},{"$f":"IF(D76>D69,D81,D69)","v":{"$error":"#VALUE!"}},{"$f":"+E81","v":{"$error":"#VALUE!"}},{"$f":"IF(F77>F70,F77,F70)","v":{"$error":"#VALUE!"}},{"$f":"IF(F77>F70,G76,G70)","v":{"$error":"#VALUE!"}},3,{"$f":"+I80","v":12.361875887090893},{"$f":"+J81","v":{"$error":"#VALUE!"}},0,4.72,3,{"$f":"+N80","v":12.361875887090893},{"$f":"+O71","v":{"$error":"#VALUE!"}},{"$f":"+P70","v":{"$error":"#VALUE!"}},{"$f":"+Q71","v":5.04},null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},{"$f":"+'Analiza i dimenzioniranje'!T594","v":4.8600021999999994},{"$f":"+'Analiza i dimenzioniranje'!U594","v":0.54310345350772504},"Y=",{"$f":"+X80*X81+Z80","v":{"$error":"#VALUE!"}}]
[4,{"$f":"+B80","v":12.361875887090893},{"$f":"+C80","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F71","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},4,{"$f":"+N83","v":12.361875887090893},{"$f":"+J80","v":{"$error":"#VALUE!"}},{"$f":"+K80","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},4,{"$f":"+N80","v":12.361875887090893},{"$f":"+O80","v":{"$error":"#VALUE!"}},{"$f":"+P80","v":0},{"$f":"+Q72","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Y=",{"$f":"+(V82-V81)/(U82-U81)","v":0.12678908905341604},"*x",{"$f":"-X83*U81+V81","v":-7.3091798227872762E-2},"CRTANJE"]
[5,null,null,{"$f":"+D80","v":{"$error":"#VALUE!"}},{"$f":"+E80","v":{"$error":"#VALUE!"}},{"$f":"+F80","v":{"$error":"#VALUE!"}},{"$f":"+G80","v":0},5,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},5,null,{"$f":"+O73","v":0},{"$f":"+P76","v":{"$error":"#VALUE!"}},{"$f":"+Q73","v":{"$error":"#VALUE!"}},null,"Jedn pravca sloja 3",null,"Jedn pravca sloja 3 klizno",null,"Y=",{"$f":"+(T86-T85)/(S86-S85)","v":-3.4920769491747737E-2},"*x",{"$f":"-X84*S85+T85","v":1.2698415389834954},"Jedn pravca sloja 3 klizno",null,"sjecište 1/2 sidra sa vrhom 1. sloja"]
["  A=",{"$f":"IF(B77>B71,0,-IF(B84>B83,0,-0.5*((B80*C81-B81*C80)+(B81*C82-B82*C81)+(B82*C83-B83*C82)+(B83*C84-B84*C83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D77>D70,0,IF(D84>D83,0,-0.5*((D80*E81-D81*E80)+(D81*E82-D82*E81)+(D82*E83-D83*E82)+(D83*E84-D84*E83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F77>F71,0,IF(F84>F83,0,-0.5*((F80*G81-F81*G80)+(F81*G82-F82*G81)+(F82*G83-F83*G82)+(F83*G84-F84*G83))))","v":{"$error":"#VALUE!"}},"kN/m'","  A=",{"$f":"IF(J77>J76,0,-IF(I84>I83,0,0.5*((I80*J81-I81*J80)+(I81*J82-I82*J81)+(I82*J83-I83*J82)+(I83*J84-I84*J83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(L77>L76,0,-0.5*((K80*L81-K81*L80)+(K81*L82-K82*L81)+(K82*L83-K83*L82)+(K83*L84-K84*L83)))","v":{"$error":"#VALUE!"}},"kN/m'","  A=",{"$f":"IF(O77>O76,0,-0.5*((N80*O81-N81*O80)+(N81*O82-N82*O81)+(N82*O83-N83*O82)+(N83*O84-N84*O83)))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(Q77>Q76,0,-0.5*((P80*Q81-P81*Q80)+(P81*Q82-P82*Q81)+(P82*Q83-P83*Q82)+(P83*Q84-P84*Q83)))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+U18","v":2},{"$f":"+V18","v":1.2},{"$f":"+W100","v":2},0,"X=",{"$f":"+(-Z84+Z87)/(X84-X87)","v":1.1386903959986558},"sjecište ",null,{"$f":"+U85","v":2},{"$f":"+V85","v":0},"Y=",{"$f":"+X92","v":{"$error":"#VALUE!"}},"*x",{"$f":"+Z92","v":{"$error":"#VALUE!"}}]
["xt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(B80+B81)+(B81*C82-B82*C81)*(B81+B82)+(B82*C83-B83*C82)*(B82+B83)+(B83*C84-B84*C83)*(B83+B84))/6/B85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(D80+D81)+(D81*E82-D82*E81)*(D81+D82)+(D82*E83-D83*E82)*(D82+D83)+(D83*E84-D84*E83)*(D83+D84))/6/D85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(F80+F81)+(F81*G82-F82*G81)*(F81+F82)+(F82*G83-F83*G82)*(F82+F83)+(F83*G84-F84*G83)*(F83+F84))/6/F85)","v":{"$error":"#VALUE!"}},"kN/m'","xt=",{"$f":"IF(I85=0,0,-((I80*J81-I81*J80)*(I80+I81)+(I81*J82-I82*J81)*(I81+I82)+(I82*J83-I83*J82)*(I82+I83)+(I83*J84-I84*J83)*(I83+I84))/6/I85)","v":{"$error":"#VALUE!"}},{"$f":"+O86","v":"kN/m'"},{"$f":"IF(K85=0,0,((K80*L81-K81*L80)*(K80+K81)+(K81*L82-K82*L81)*(K81+K82)+(K82*L83-K83*L82)*(K82+K83)+(K83*L84-K84*L83)*(K83+K84))/6/K85)","v":{"$error":"#VALUE!"}},"kN/m'","xt=",{"$f":"IF(N85=0,0,-((N80*O81-N81*O80)*(N80+N81)+(N81*O82-N82*O81)*(N81+N82)+(N82*O83-N83*O82)*(N82+N83)+(N83*O84-N84*O83)*(N83+N84))/6/N85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(P85=0,0,-((P80*Q81-P81*Q80)*(P80+P81)+(P81*Q82-P82*Q81)*(P81+P82)+(P82*Q83-P83*Q82)*(P82+P83)+(P83*Q84-P84*Q83)*(P83+P84))/6/P85)","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+U19","v":-8},{"$f":"+V19","v":1.5492076949174773},-5,{"$f":"+V85+(U85-U86)*TAN((45+'Analiza i dimenzioniranje'!F14/2)*PI()/180)","v":9.9970360471948005},"Y=",{"$f":"+X84*X85+Z84","v":1.2300775941423594},3,null,{"$f":"+X85","v":1.1386903959986558},{"$f":"+X86","v":1.2300775941423594}]
["yt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(C80+C81)+(B81*C82-B82*C81)*(C81+C82)+(B82*C83-B83*C82)*(C82+C83)+(B83*C84-B84*C83)*(C83+C84))/6/B85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(E80+E81)+(D81*E82-D82*E81)*(E81+E82)+(D82*E83-D83*E82)*(E82+E83)+(D83*E84-D84*E83)*(E83+E84))/6/D85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(G80+G81)+(F81*G82-F82*G81)*(G81+G82)+(F82*G83-F83*G82)*(G82+G83)+(F83*G84-F84*G83)*(G83+G84))/6/F85)","v":{"$error":"#VALUE!"}},"m","yt=",{"$f":"IF(I85=0,0,-((I80*J81-I81*J80)*(J80+J81)+(I81*J82-I82*J81)*(J81+J82)+(I82*J83-I83*J82)*(J82+J83)+(I83*J84-I84*J83)*(J83+J84))/6/I85)","v":{"$error":"#VALUE!"}},{"$f":"+O87","v":"m"},{"$f":"IF(K85=0,0,((K80*L81-K81*L80)*(L80+L81)+(K81*L82-K82*L81)*(L81+L82)+(K82*L83-K83*L82)*(L82+L83)+(K83*L84-K84*L83)*(L83+L84))/6/K85)","v":{"$error":"#VALUE!"}},"m","yt=",{"$f":"IF(N85=0,0,-((N80*O81-N81*O80)*(O80+O81)+(N81*O82-N82*O81)*(O81+O82)+(N82*O83-N83*O82)*(O82+O83)+(N83*O84-N84*O83)*(O83+O84))/6/N85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(P85=0,0,-((P80*Q81-P81*Q80)*(Q80+Q81)+(P81*Q82-P82*Q81)*(Q81+Q82)+(P82*Q83-P83*Q82)*(Q82+Q83)+(P83*Q84-P84*Q83)*(Q83+Q84))/6/P85)","v":{"$error":"#VALUE!"}},"m",null,null,null,null,null,"Y=",{"$f":"+(V86-V85)/(U86-U85)","v":-1.4281480067421144},"*x",{"$f":"-X87*U85+V85","v":2.8562960134842288},"y=2       x=",{"$f":"+('Analiza i dimenzioniranje'!E52-'C XVI-XVII'!Z87)/'C XVI-XVII'!X87","v":1.1597509541483482}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(K85<0,0,K85)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+IF(P85<0,0,P85)","v":{"$error":"#VALUE!"}},null,null,"Jedn pravca sloja 2",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(T90-T89)/(S90-S89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X88*S89+T89","v":{"$error":"#VALUE!"}},"Jedn pravca sloja 2 klizno",null,"Jednadžba pravca sidra",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(AD90-AD89)/(AC90-AC89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AH88*AC89+AD89","v":{"$error":"#VALUE!"}}]
["X koordinata položaja rezultante aktivnog tlaka na stražnjoj strani zida za  Ev1, Ev2 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U15","v":{"$error":"#VALUE!"}},{"$f":"+V15","v":4},{"$f":"+X85","v":1.1386903959986558},{"$f":"+X86","v":1.2300775941423594},"X=",{"$f":"+(-Z88+Z91)/(X88-X91)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U89","v":1.1386903959986558},{"$f":"+V89","v":1.2300775941423594},{"$f":"+U37","v":{"$error":"#VALUE!"}},{"$f":"+V37","v":5},{"$f":"+U89","v":1.1386903959986558},{"$f":"+V89","v":1.2300775941423594},"X=",{"$f":"+(-AJ88+AJ91)/(AH88-AH91)","v":{"$error":"#VALUE!"}},"sjecište"]
["Jednadžba pravca zida uz tlo",null,null,null,null,"Za Ev3 x=2",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U16","v":-8},{"$f":"+V16","v":{"$error":"#VALUE!"}},-5,{"$f":"+V89+(U89-U90)*TAN((45+'Analiza i dimenzioniranje'!E14/2)*PI()/180)","v":9.6792600705649363},"Y=",{"$f":"+X88*X89+Z88","v":{"$error":"#VALUE!"}},2,null,{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},{"$f":"+U38","v":{"$error":"#VALUE!"}},{"$f":"+V38","v":{"$error":"#VALUE!"}},{"$f":"+U90","v":-5},{"$f":"+V90","v":9.6792600705649363},"Y=",{"$f":"+AH88*AH89+AJ88","v":{"$error":"#VALUE!"}},2]
[null,"E1",null,"E2",null,"E3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(V90-V89)/(U90-U89)","v":-1.3763819204711731},"*x",{"$f":"-X91*U89+V89","v":2.79735046820907},null,null,null,null,null,null,"Y=",{"$f":"+(AF90-AF89)/(AE90-AE89)","v":-1.3763819204711731},"*x",{"$f":"-AH91*AE89+AF89","v":2.79735046820907}]
["x","y","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,"Jedn pravca sloja 1",null,null,null,"Y=",{"$f":"+(T95-T94)/(S95-S94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X92*S94+T94","v":{"$error":"#VALUE!"}},"Jedan pravca sloja 1 klizno",null,"Slobodna dionica ls>=",{"$f":"+SQRT((AC94-AC93)*(AC94-AC93)+(AD94-AD93)*(AD94-AD93))","v":{"$error":"#VALUE!"}}]
[{"$f":"+(B8-B4)*(B93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+B87","v":{"$error":"#VALUE!"}},{"$f":"+(B8-B4)*(D93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+D87","v":{"$error":"#VALUE!"}},2,{"$f":"+F87","v":{"$error":"#VALUE!"}},null,{"$f":"+(B8-B4)*(I93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+N87","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+(B8-B4)*(N93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+I87","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+V7","v":"A"},null,null,"X=",{"$f":"+(-Z92+Z95)/(X92-X95)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U94","v":{"$error":"#VALUE!"}},{"$f":"+V94","v":{"$error":"#VALUE!"}},{"$f":"+AC89","v":{"$error":"#VALUE!"}},{"$f":"+AD89","v":5}]
[null,null,null,null,"Sloj2",{"$f":"+(B8-B4)*(G94-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!V15","v":4},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U8","v":{"$error":"#VALUE!"}},{"$f":"+V8","v":6},{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+X92*X93+Z92","v":{"$error":"#VALUE!"}},1,null,{"$f":"+X93","v":{"$error":"#VALUE!"}},{"$f":"+X94","v":{"$error":"#VALUE!"}},{"$f":"+AH89","v":{"$error":"#VALUE!"}},{"$f":"+AH90","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+(B8-B4)*(G95-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+K21","v":1.2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782},-5,{"$f":"+V94+(U94-U95)*TAN((45+'Analiza i dimenzioniranje'!D14/2)*PI()/180)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+(V95-V94)/(U95-U94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X95*U94+V94","v":{"$error":"#VALUE!"}},{"$f":"+(AB95-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(AB96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AG44","v":5.04},{"$f":"+(AD96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Masa unutar kliznog tijela - za potres",null,"POTRES",null,"x","y","x","y","x","y",null,null,null,null,"Masa za potres s prosjekom kontrafore i bez kontrafora"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+(B9-B4)*(AD98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72},{"$f":"+(B9-B4)*(AF98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AG44","v":5.04}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B2","v":2},0.12820515121628623,null,null,{"$f":"+(Z95-AB99)/(-X91)","v":{"$error":"#VALUE!"}},{"$f":"+AB98","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!AF44>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'C XVI-XVII'!AC96,(Z91-AD99)/(-X91))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72},{"$f":"IF('Analiza i dimenzioniranje'!AG44>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'C XVI-XVII'!AA96,(Z91-AF99)/(-X91))","v":{"$error":"#VALUE!"}},{"$f":"+AF98","v":5.04}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,1.2,"Potresna sila za stabilnost",null,"Klizno tijelo za potres za presjek III-III",null,"Klizno tijelo za potres za presjek   Mmin",null,"Klizno tijelo za potres za presjek   Mmax",null,null,null,null,null,"Potresna sila za stabilnost "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.4000010999999999,1.2,{"$f":"+'C XIV-XV'!Y101","v":1.75},{"$f":"+'C XIV-XV'!Z101","v":9.6153895463470418E-2},null,null,{"$f":"+AC98","v":{"$error":"#VALUE!"}},{"$f":"+AD98","v":4.72},{"$f":"+AE98","v":{"$error":"#VALUE!"}},{"$f":"+AF98","v":5.04},null,null,null,null,{"$f":"+'C III-V'!Y101","v":1.75},{"$f":"+'C III-V'!Z101","v":9.6153895463470418E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.14,{"$f":"+'C XIV-XV'!Y102","v":0.97707863658009864},{"$f":"+'C XIV-XV'!Z102","v":1.2},{"$f":"+'C XIV-XV'!AA102","v":0.97707863658009864},{"$f":"+'C XIV-XV'!AB102","v":1.2},{"$f":"+AN130","v":-1.5625437213651958},{"$f":"+AO130","v":4.72},{"$f":"+AN131","v":-1.7871229567119888},{"$f":"+AO131","v":5.04},null,null,null,null,{"$f":"+'C III-V'!Y102","v":0.97707863658009864},{"$f":"+'C III-V'!Z102","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.14,{"$f":"+'C XIV-XV'!Y103","v":-1.0572404418349119},{"$f":"+'C XIV-XV'!Z103","v":4},{"$f":"+Y103","v":-1.0572404418349119},{"$f":"+Z103","v":4},{"$f":"IF(AD103=AD102,AC102,+AA103)","v":-1.5625437213651958},{"$f":"IF($AH$105<=AD102,AD102,$AH$105)","v":4.72},{"$f":"IF(AF103=AF102,AE102,+AC103)","v":-1.7871229567119888},{"$f":"IF($AH$105<=AF102,AF102,$AH$105)","v":5.04},null,null,null,null,{"$f":"+'C III-V'!Y103","v":-1.0572404418349119},{"$f":"+'C III-V'!Z103","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.44,{"$f":"+'C XIV-XV'!Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!Z104","v":{"$error":"#VALUE!"}},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+'C III-V'!Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z104","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.44,{"$f":"+'C XIV-XV'!Y105","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!Z105","v":6.2644906473896782},{"$f":"+'C XIV-XV'!AA105","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!AB105","v":6.2644906473896782},{"$f":"+AA105","v":{"$error":"#VALUE!"}},{"$f":"IF(AA105=AC105,AB105,AB95)","v":{"$error":"#VALUE!"}},{"$f":"+AA105","v":{"$error":"#VALUE!"}},{"$f":"+IF(AA105=AE105,AB105,AB95)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AM105","v":" H="},{"$f":"+'C III-V'!AH105","v":4},null,null,{"$f":"+'C III-V'!Y105","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z105","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},"A",{"$f":"+'C XIV-XV'!Y106","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!Z106","v":6},{"$f":"+'C XIV-XV'!AA106","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!AB106","v":6},{"$f":"+AE106","v":{"$error":"#VALUE!"}},{"$f":"+AF106","v":6},{"$f":"+AA106","v":{"$error":"#VALUE!"}},{"$f":"+AB106","v":6},null,null,null,null,{"$f":"+'C III-V'!Y106","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z106","v":6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},"A",{"$f":"+'C XIV-XV'!Y107","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!Z107","v":6},{"$f":"+'C XIV-XV'!AA107","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!AB107","v":6},{"$f":"+AE107","v":{"$error":"#VALUE!"}},{"$f":"+AF107","v":6},{"$f":"+AA107","v":{"$error":"#VALUE!"}},{"$f":"+AB107","v":6},null,null,null,null,{"$f":"+'C III-V'!Y107","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z107","v":6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+W107","v":{"$error":"#VALUE!"}},{"$f":"+X107","v":"A"},{"$f":"+'C XIV-XV'!Y108","v":3.4000000999999997},{"$f":"+'C XIV-XV'!Z108","v":1.2},{"$f":"+'C XIV-XV'!AA108","v":3.4000000999999997},{"$f":"+'C XIV-XV'!AB108","v":1.2},{"$f":"+AC109","v":{"$error":"#VALUE!"}},{"$f":"+AD109","v":4.72},{"$f":"+AE109","v":{"$error":"#VALUE!"}},{"$f":"+AF109","v":5.04},null,null,null,null,{"$f":"+'C III-V'!Y108","v":3.4000000999999997},{"$f":"+'C III-V'!Z108","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B11","v":4.2000010999999997},1.2,{"$f":"+'C XIV-XV'!Y109","v":1.75},{"$f":"+'C XIV-XV'!Z109","v":1.2},{"$f":"+'C XIV-XV'!AA109","v":0.97707863658009864},{"$f":"+'C XIV-XV'!AB109","v":1.2},{"$f":"+AC98","v":{"$error":"#VALUE!"}},{"$f":"+AD98","v":4.72},{"$f":"+AE101","v":{"$error":"#VALUE!"}},{"$f":"+AF101","v":5.04},null,null,null,null,{"$f":"+'C III-V'!Y109","v":1.75},{"$f":"+'C III-V'!Z109","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2000010999999997,1.2,{"$f":"+'C XIV-XV'!Y110","v":1.75},{"$f":"+'C XIV-XV'!Z110","v":9.6153895463470418E-2},null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!Y110","v":1.75},{"$f":"+'C III-V'!Z110","v":9.6153895463470418E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2000010999999997,1.2,{"$f":"-0.5*((Y101*Z102-Y102*Z101)+(Y102*Z103-Y103*Z102)+(Y103*Z104-Y104*Z103)+(Y104*Z105-Y105*Z104)+(Y105*Z106-Y106*Z105)+(Y106*Z107-Y107*Z106)+(Y107*Z108-Y108*Z107)+(Y108*Z109-Y109*Z108)+(Y109*Z110-Y110*Z109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AA101*AB102-AA102*AB101)+(AA102*AB103-AA103*AB102)+(AA103*AB104-AA104*AB103)+(AA104*AB105-AA105*AB104)+(AA105*AB106-AA106*AB105)+(AA106*AB107-AA107*AB106)+(AA107*AB108-AA108*AB107)+(AA108*AB109-AA109*AB108)+(AA109*AB110-AA110*AB109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AC101*AD102-AC102*AD101)+(AC102*AD103-AC103*AD102)+(AC103*AD104-AC104*AD103)+(AC104*AD105-AC105*AD104)+(AC105*AD106-AC106*AD105)+(AC106*AD107-AC107*AD106)+(AC107*AD108-AC108*AD107)+(AC108*AD109-AC109*AD108)+(AC109*AD110-AC110*AD109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AE101*AF102-AE102*AF101)+(AE102*AF103-AE103*AF102)+(AE103*AF104-AE104*AF103)+(AE104*AF105-AE105*AF104)+(AE105*AF106-AE106*AF105)+(AE106*AF107-AE107*AF106)+(AE107*AF108-AE108*AF107)+(AE108*AF109-AE109*AF108)+(AE109*AF110-AE110*AF109))","v":{"$error":"#VALUE!"}},"m2",null,null,null,null,{"$f":"-0.5*((AK101*AL102-AK102*AL101)+(AK102*AL103-AK103*AL102)+(AK103*AL104-AK104*AL103)+(AK104*AL105-AK105*AL104)+(AK105*AL106-AK106*AL105)+(AK106*AL107-AK107*AL106)+(AK107*AL108-AK108*AL107)+(AK108*AL109-AK109*AL108)+(AK109*AL110-AK110*AL109))","v":{"$error":"#VALUE!"}},"m2","OK","prosječna površina temelja od temelja kontrafore duž čitavog zida"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.9000021999999994,1.2,{"$f":"-((Y101*Z102-Y102*Z101)*(Y101+Y102)+(Y102*Z103-Y103*Z102)*(Y102+Y103)+(Y103*Z104-Y104*Z103)*(Y103+Y104)+(Y104*Z105-Y105*Z104)*(Y104+Y105)+(Y105*Z106-Y106*Z105)*(Y105+Y106)+(Y106*Z107-Y107*Z106)*(Y106+Y107)+(Y107*Z108-Y108*Z107)*(Y107+Y108)+(Y108*Z109-Y109*Z108)*(Y108+Y109)+(Y109*Z110-Y110*Z109)*(Y109+Y110))/6/Y111","v":{"$error":"#VALUE!"}},"m  ",{"$f":"-((AA101*AB102-AA102*AB101)*(AA101+AA102)+(AA102*AB103-AA103*AB102)*(AA102+AA103)+(AA103*AB104-AA104*AB103)*(AA103+AA104)+(AA104*AB105-AA105*AB104)*(AA104+AA105)+(AA105*AB106-AA106*AB105)*(AA105+AA106)+(AA106*AB107-AA107*AB106)*(AA106+AA107)+(AA107*AB108-AA108*AB107)*(AA107+AA108)+(AA108*AB109-AA109*AB108)*(AA108+AA109)+(AA109*AB110-AA110*AB109)*(AA109+AA110))/6/AA111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AC101*AD102-AC102*AD101)*(AC101+AC102)+(AC102*AD103-AC103*AD102)*(AC102+AC103)+(AC103*AD104-AC104*AD103)*(AC103+AC104)+(AC104*AD105-AC105*AD104)*(AC104+AC105)+(AC105*AD106-AC106*AD105)*(AC105+AC106)+(AC106*AD107-AC107*AD106)*(AC106+AC107)+(AC107*AD108-AC108*AD107)*(AC107+AC108)+(AC108*AD109-AC109*AD108)*(AC108+AC109)+(AC109*AD110-AC110*AD109)*(AC109+AC110))/6/AC111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AE101*AF102-AE102*AF101)*(AE101+AE102)+(AE102*AF103-AE103*AF102)*(AE102+AE103)+(AE103*AF104-AE104*AF103)*(AE103+AE104)+(AE104*AF105-AE105*AF104)*(AE104+AE105)+(AE105*AF106-AE106*AF105)*(AE105+AE106)+(AE106*AF107-AE107*AF106)*(AE106+AE107)+(AE107*AF108-AE108*AF107)*(AE107+AE108)+(AE108*AF109-AE109*AF108)*(AE108+AE109)+(AE109*AF110-AE110*AF109)*(AE109+AE110))/6/AE111","v":{"$error":"#VALUE!"}},"m",null,null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AK101+AK102)+(AK102*AL103-AK103*AL102)*(AK102+AK103)+(AK103*AL104-AK104*AL103)*(AK103+AK104)+(AK104*AL105-AK105*AL104)*(AK104+AK105)+(AK105*AL106-AK106*AL105)*(AK105+AK106)+(AK106*AL107-AK107*AL106)*(AK106+AK107)+(AK107*AL108-AK108*AL107)*(AK107+AK108)+(AK108*AL109-AK109*AL108)*(AK108+AK109)+(AK109*AL110-AK110*AL109)*(AK109+AK110))/6/AK111","v":{"$error":"#VALUE!"}},"m  "]
[null,null,null,null,null,{"$f":"+'C III-V'!F136:G136","v":"Visina presjeka"},null,{"$f":"+'C III-V'!H136:I136","v":"Intezitet"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.9000021999999994,0.5,{"$f":"-((Y101*Z102-Y102*Z101)*(Z101+Z102)+(Y102*Z103-Y103*Z102)*(Z102+Z103)+(Y103*Z104-Y104*Z103)*(Z103+Z104)+(Y104*Z105-Y105*Z104)*(Z104+Z105)+(Y105*Z106-Y106*Z105)*(Z105+Z106)+(Y106*Z107-Y107*Z106)*(Z106+Z107)+(Y107*Z108-Y108*Z107)*(Z107+Z108)+(Y108*Z109-Y109*Z108)*(Z108+Z109)+(Y109*Z110-Y110*Z109)*(Z109+Z110))/6/Y111","v":{"$error":"#VALUE!"}},"m    ",{"$f":"-((AA101*AB102-AA102*AB101)*(AB101+AB102)+(AA102*AB103-AA103*AB102)*(AB102+AB103)+(AA103*AB104-AA104*AB103)*(AB103+AB104)+(AA104*AB105-AA105*AB104)*(AB104+AB105)+(AA105*AB106-AA106*AB105)*(AB105+AB106)+(AA106*AB107-AA107*AB106)*(AB106+AB107)+(AA107*AB108-AA108*AB107)*(AB107+AB108)+(AA108*AB109-AA109*AB108)*(AB108+AB109)+(AA109*AB110-AA110*AB109)*(AB109+AB110))/6/AA111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AC101*AD102-AC102*AD101)*(AD101+AD102)+(AC102*AD103-AC103*AD102)*(AD102+AD103)+(AC103*AD104-AC104*AD103)*(AD103+AD104)+(AC104*AD105-AC105*AD104)*(AD104+AD105)+(AC105*AD106-AC106*AD105)*(AD105+AD106)+(AC106*AD107-AC107*AD106)*(AD106+AD107)+(AC107*AD108-AC108*AD107)*(AD107+AD108)+(AC108*AD109-AC109*AD108)*(AD108+AD109)+(AC109*AD110-AC110*AD109)*(AD109+AD110))/6/AC111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AE101*AF102-AE102*AF101)*(AF101+AF102)+(AE102*AF103-AE103*AF102)*(AF102+AF103)+(AE103*AF104-AE104*AF103)*(AF103+AF104)+(AE104*AF105-AE105*AF104)*(AF104+AF105)+(AE105*AF106-AE106*AF105)*(AF105+AF106)+(AE106*AF107-AE107*AF106)*(AF106+AF107)+(AE107*AF108-AE108*AF107)*(AF107+AF108)+(AE108*AF109-AE109*AF108)*(AF108+AF109)+(AE109*AF110-AE110*AF109)*(AF109+AF110))/6/AE111","v":{"$error":"#VALUE!"}},"m",null,null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AL101+AL102)+(AK102*AL103-AK103*AL102)*(AL102+AL103)+(AK103*AL104-AK104*AL103)*(AL103+AL104)+(AK104*AL105-AK105*AL104)*(AL104+AL105)+(AK105*AL106-AK106*AL105)*(AL105+AL106)+(AK106*AL107-AK107*AL106)*(AL106+AL107)+(AK107*AL108-AK108*AL107)*(AL107+AL108)+(AK108*AL109-AK109*AL108)*(AL108+AL109)+(AK109*AL110-AK110*AL109)*(AL109+AL110))/6/AK111","v":{"$error":"#VALUE!"}},"m    ",null,{"$f":"+'C III-V'!AN113:AN114","v":-0.25},{"$f":"IF('Analiza i dimenzioniranje'!D84=\"\",0,'Analiza i dimenzioniranje'!D83+'C III-V'!AN113)","v":0.75}]
[null,null,null,null,null,{"$f":"+'C III-V'!F137:G137","v":"III"},{"$f":"+'C III-V'!G137:H137","v":1.2},{"$f":"+'C III-V'!H137:I137","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,0.12820515121628623,{"$f":"+Y111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AA111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AC111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AE111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,{"$f":"+AK111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN"]
[null,null,null,null,null,{"$f":"+'C III-V'!F138:G138","v":"VI"},{"$f":"+'C III-V'!G138:H138","v":1.52},{"$f":"+'C III-V'!H138:I138","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Teren  kosina",null,"Klizna ploha"]
[null,null,null,null,null,{"$f":"+'C III-V'!F139:G139","v":"VII"},{"$f":"+'C III-V'!G139:H139","v":1.84},{"$f":"+'C III-V'!H139:I139","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C XIV-XV'!AI116","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!AJ116","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!AK116","v":1.75},{"$f":"+'C XIV-XV'!AL116","v":-1.1133852506716102},"sjecišta ravnine presjeka na kliznoj plohi",null,null,null,null,null,null,"Omjer površine"]
[null,null,null,null,null,{"$f":"+'C III-V'!F140:G140","v":"VIII"},{"$f":"+'C III-V'!G140:H140","v":2.16},{"$f":"+'C III-V'!H140:I140","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C XIV-XV'!AI117","v":6.2644906473896782},{"$f":"+'C XIV-XV'!AJ117","v":6},{"$f":"+'C XIV-XV'!AK117","v":0},{"$f":"+'C XIV-XV'!AL117","v":4.08},{"$f":"+'C III-V'!AA100","v":"oznaka"},{"$f":"+'C III-V'!AB100","v":"X"},{"$f":"+'C III-V'!AC100","v":"Y"},null,null,null,"        sa kontraforama: bez kontrafora",null,null,"Potresna sila-prosječna"]
[null,null,null,null,null,{"$f":"+'C III-V'!F141:G141","v":"IX"},{"$f":"+'C III-V'!G141:H141","v":2.48},{"$f":"+'C III-V'!H141:I141","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!D116,AI117)","v":-5},{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!E116,'C III-V'!AJ117)","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!AA101","v":"Y=0"},{"$f":"+'C III-V'!AB101","v":1.75},{"$f":"+'C III-V'!AC101","v":0},{"$f":"+'C XIV-XV'!AP118","v":0},null,null,null,null,null,null,null,"Potresna sila","F","G"]
[null,null,null,null,null,{"$f":"+'C III-V'!F142:G142","v":"X"},{"$f":"+'C III-V'!G142:H142","v":2.8},{"$f":"+'C III-V'!H142:I142","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"(AJ117-AI117)/(AJ116-AI116)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AI119*AI116+AI117","v":{"$error":"#VALUE!"}}," ",{"$f":"+'C III-V'!AA102","v":"PIII"},{"$f":"+'C III-V'!AB102","v":0.97707863658009864},{"$f":"+'C III-V'!AC102","v":1.2},{"$f":"+'C XIV-XV'!AP119","v":0},null,null,null,"Ukupna duljina zida",null,{"$f":"+Kontrafore!E13","v":12},"m",{"$f":"+AV119","v":12},{"$f":"+Y111","v":{"$error":"#VALUE!"}},{"$f":"+Y114","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F143:G143","v":"XI"},{"$f":"+'C III-V'!G143:H143","v":3.14},{"$f":"+'C III-V'!H143:I143","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"-(AL117-AK117)/(AK116-AL116)","v":-1.4248868534344206},"*x    +",{"$f":"-(AK116*AI120-AK117)","v":2.4935519935102359}," ",{"$f":"+'C III-V'!AA103","v":"PVI"},{"$f":"+'C III-V'!AB103","v":0.68324863210273346},{"$f":"+'C III-V'!AC103","v":1.52},{"$f":"+'C XIV-XV'!AP120","v":0},null,null,null,"ukupna duljina kontrafora",null,{"$f":"+Kontrafore!E5*Kontrafore!E4","v":3},"m",{"$f":"+AV120","v":3},{"$f":"+AY119-AY121","v":{"$error":"#VALUE!"}},{"$f":"IF(AV120=AV119,0,AZ119-AZ121)","v":{"$error":"#VALUE!"}}]
["Presjek kroz zid I",null,"Presjek kroz zid II",null,null,{"$f":"+'C III-V'!F144:G144","v":"XIII"},{"$f":"+'C III-V'!G144:H144","v":3.44},{"$f":"+'C III-V'!H144:I144","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AK120-AK119)/(AI119-AI120)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AI120*AI121+AK120","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA104","v":"PVII"},{"$f":"+'C III-V'!AB104","v":0.45866939675594048},{"$f":"+'C III-V'!AC104","v":1.84},{"$f":"+'C XIV-XV'!AP121","v":0},null,null,null,"ukupna duljina bez kontrafora",null,{"$f":"+AV119-AV120","v":9},"m",{"$f":"+AX119-AX120","v":9},{"$f":"+AG111","v":0},{"$f":"+IF(AX121=0,0,AG114)","v":0}]
["x","y","x","y",null,{"$f":"+'C III-V'!F145:G145","v":"XIII"},{"$f":"+'C III-V'!G145:H145","v":3.76},{"$f":"+'C III-V'!H145:I145","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA105","v":"PVIII"},{"$f":"+'C III-V'!AB105","v":0.23409016140914748},{"$f":"+'C III-V'!AC105","v":2.16},{"$f":"+'C XIV-XV'!AP122","v":0},null,null,null,"površina s kontraforama",null,{"$f":"+AV120/AV119","v":0.25}]
[0,{"$f":"+'Analiza i dimenzioniranje'!AG44","v":5.04},{"$f":"+A123","v":0},{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72},null,{"$f":"+'C III-V'!F146:G146","v":"XIV"},{"$f":"+'C III-V'!G146:H146","v":4.08},{"$f":"+'C III-V'!H146:I146","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($AK$119-$AK$123)/AI119","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AK121","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA106","v":"PIX"},{"$f":"+'C III-V'!AB106","v":9.5109260623546556E-3},{"$f":"+'C III-V'!AC106","v":2.48},{"$f":"+'C XIV-XV'!AP123","v":0},null,null,null,"površina bez kontrafora",null,{"$f":"+AV121/AV119","v":0.75}]
[{"$f":"+F83","v":{"$error":"#VALUE!"}},{"$f":"+B123","v":5.04},{"$f":"+A124","v":{"$error":"#VALUE!"}},{"$f":"+D123","v":4.72},null,{"$f":"+'C III-V'!F147:G147","v":"XV"},{"$f":"+'C III-V'!G147:H147","v":4.4000000000000004},{"$f":"+'C III-V'!H147:I147","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA107","v":"PX"},{"$f":"+'C III-V'!AB107","v":-0.21506830928443818},{"$f":"+'C III-V'!AC107","v":2.8},{"$f":"+'C XIV-XV'!AP124","v":0},null,null,null,null,null,"odnos",null,{"$f":"-(AX120/AX119)*'Analiza i dimenzioniranje'!D83","v":-0.25}]
[null,null,null,null,null,{"$f":"+'C III-V'!F148:G148","v":"XVI"},{"$f":"+'C III-V'!G148:H148","v":4.72},{"$f":"+'C III-V'!H148:I148","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA108","v":"PXI"},{"$f":"+'C III-V'!AB108","v":-0.45368374684040591},{"$f":"+'C III-V'!AC108","v":3.14},{"$f":"+'C XIV-XV'!AP125","v":0},null,null,null,null,"krak",{"$f":"+Y113","v":{"$error":"#VALUE!"}},{"$f":"+AZ119","v":{"$error":"#VALUE!"}},{"$f":"+AZ120*AV122","v":{"$error":"#VALUE!"}},null,{"$f":"+AZ119-AX126","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F149:G149","v":"XVII"},{"$f":"+'C III-V'!G149:H149","v":5.04},{"$f":"+'C III-V'!H149:I149","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($AK$120-AK126)/$AI$120","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AK121","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA109","v":"PXII"},{"$f":"+'C III-V'!AB109","v":-0.66422677997802415},{"$f":"+'C III-V'!AC109","v":3.44},{"$f":"+'C XIV-XV'!AP126","v":0},null,null,null,null,null,{"$f":"+AG113","v":0},{"$f":"+AZ121","v":0},{"$f":"+AZ120*AV123","v":{"$error":"#VALUE!"}},null,{"$f":"+AZ121+AX125","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F150:G150","v":"XVIII"},{"$f":"+'C III-V'!G150:H150","v":5.36},{"$f":"+'C III-V'!H150:I150","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-1.1976024639266576,null,4.2,null,{"$f":"+'C III-V'!AA110","v":"PXIII"},{"$f":"+'C III-V'!AB110","v":-0.88880601532481696},{"$f":"+'C III-V'!AC110","v":3.76},{"$f":"+'C XIV-XV'!AP127","v":0},null,null,null,null,null,null,null,"Prosječna masa za potres:",null,{"$f":"IF(IF(AV130=AW130,Y114,+AZ126)=0,AZ125,IF(AV130=AW130,Y114,+AZ126))","v":{"$error":"#VALUE!"}},"kn"]
[null,null,null,null,null,{"$f":"+'C III-V'!F151:G151","v":"XIX"},{"$f":"+'C III-V'!G151:H151","v":5.6800000000000006},{"$f":"+'C III-V'!H151:I151","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.90782786744952648,null,1.2,null,{"$f":"+'C III-V'!AA111","v":"PXIV"},{"$f":"+'C III-V'!AB111","v":-1.1133852506716102},{"$f":"+'C III-V'!AC111","v":4.08},{"$f":"+'C XIV-XV'!AP128","v":0}]
[null,null,null,null,null,{"$f":"+'C III-V'!F152:G152","v":"XX"},{"$f":"+'C III-V'!G152:H152","v":6},{"$f":"+'C III-V'!H152:I152","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},null,{"$f":"+AB104","v":{"$error":"#VALUE!"}},null,{"$f":"+'C III-V'!AA112","v":"PXV"},{"$f":"+'C III-V'!AB112","v":-1.3379644860184032},{"$f":"+'C III-V'!AC112","v":4.4000000000000004},{"$f":"+'C XIV-XV'!AP129","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-1.5625437213651958,null,{"$f":"+AD102","v":4.72},null,{"$f":"+'C III-V'!AA113","v":"PXVI"},{"$f":"+'C III-V'!AB113","v":-1.5625437213651958},{"$f":"+'C III-V'!AC113","v":4.72},{"$f":"+'C XIV-XV'!AP130","v":0},null,null,null,null,"x=",{"$f":"+AG113","v":0},{"$f":"+Y113","v":{"$error":"#VALUE!"}},null,{"$f":"+AI109","v":0},{"$f":"+AI106","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-1.7871229567119888,null,{"$f":"+AF108","v":5.04},null,{"$f":"+'C III-V'!AA114","v":"PXVII"},{"$f":"+'C III-V'!AB114","v":-1.7871229567119888},{"$f":"+'C III-V'!AC114","v":5.04},{"$f":"+'C XIV-XV'!AP131","v":0},null,null,null,null,"Y=",{"$f":"+AG114","v":0},{"$f":"+Y114","v":{"$error":"#VALUE!"}},null,{"$f":"+AJ109","v":0},{"$f":"+AJ106","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.6464828732122183,null,{"$f":"+AI117","v":6.2644906473896782},null,{"$f":"+'C III-V'!AA115","v":"PXVIII"},{"$f":"+'C III-V'!AB115","v":-2.0117021920587819},{"$f":"+'C III-V'!AC115","v":5.36},{"$f":"+'C XIV-XV'!AP132","v":0},null,null,null,null,"Y=",{"$f":"(AV131-AW131)/(AV130-AW130)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AV132*AW130+AW131","v":{"$error":"#VALUE!"}},{"$f":"(AY131-AZ131)/(AY130-AZ130)","v":{"$error":"#DIV/0!"}},"*x    +",{"$f":"-AY132*AZ130+AZ131","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA116","v":"PXIX"},{"$f":"+'C III-V'!AB116","v":-2.2362814274055753},{"$f":"+'C III-V'!AC116","v":5.6800000000000006},{"$f":"+'C XIV-XV'!AP133","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA117","v":"PXX"},{"$f":"+'C III-V'!AB117","v":0},{"$f":"+'C III-V'!AC117","v":6.0000000000000009},{"$f":"+'C XIV-XV'!AP134","v":0},null,null,null,null,"x=",{"$f":"+AK113","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","Y",null,null,null,{"$f":"+'C III-V'!AB118","v":{"$error":"#VALUE!"}},{"$f":"+AK132","v":6.2644906473896782},{"$f":"+'C XIV-XV'!AP135","v":0},null,null,null,null,"xstv=",{"$f":"+AV134-X113","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C XIV-XV'!AI136","v":{"$error":"#VALUE!"}},{"$f":"+'C XIV-XV'!AJ136","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"            Masa da se dobije prosječni potres iz čelije AT125=",null,null,null,null,{"$f":"+AZ125","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+'C XII-XIII'!AC138","v":{"$error":"#VALUE!"}},{"$f":"+AD102","v":4.72},{"$f":"+AF102","v":5.04},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"razlika¸površina",{"$f":"+Y111-AI111","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AE144-AC138)/(-AC144)","v":{"$error":"#VALUE!"}},{"$f":"IF(AD138<AC138,(AE151-AD138)/(-AC151),(AE156-AD138)/(-AC156))","v":{"$error":"#VALUE!"}},{"$f":"IF(AE138<AC138,(AE151-AE138)/(-AC151),(AE156-AE138)/(-AC156))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"duljina segmenta",{"$f":"++AJ105","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina III. sloja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"okomito na kliz. Plohu",null,{"$f":"+AV143/AV139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"d=","dodatak",{"$f":"+AV140/COS(AV142*PI()/180)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA153","v":2},{"$f":"+'C III-V'!AB153","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"          kut nagiba klizne plohe za potres   a= ",null,{"$f":"ATAN((-Y104+Y101)/(Z104-Z101))*180/PI()","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA154","v":-5},{"$f":"+'C III-V'!AB154","v":9.9970360471948005},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dodatna površina",{"$f":"+AV144/'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AD143-AD142)/(AC143-AC142)","v":-1.4281480067421144},"*x      +",{"$f":"-AC144*AC142+AD142","v":2.8562960134842288},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"G=",{"$f":"+AX126","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AE144-AD146)/(-AC144)","v":1.1597509541483482}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+Z102","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina II. sloja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA148","v":-1.0572404418349119},{"$f":"+'C III-V'!AB148","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA149","v":0.97707863658009864},{"$f":"+'C III-V'!AB149","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AD150-AD149)/(AC150-AC149)","v":-1.3763819204711734},"*x      +",{"$f":"-AC151*AC149+AD149","v":2.5448333702674724}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina I. sloja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koordinate na sjecištu s terenom",null,null,{"$f":"+'C III-V'!AA144","v":-2.5846586698092704},{"$f":"+'C III-V'!AB144","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koordinate na sjecištu slojeva",null,null,{"$f":"+'C III-V'!AA143","v":-1.0572404418349119},{"$f":"+'C III-V'!AB143","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AD155-AD154)/(AC155-AC154)","v":-1.4825609685127401},"*x      +",{"$f":"-AC156*AC154+AD154","v":2.4325765866023956}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rub dna konzole uz aktivni klin",null,null,{"$f":"+B6","v":{"$error":"#VALUE!"}},{"$f":"+C6","v":3.14}]

{"sheet":"C XVIII-XIX","index":46,"n_rows":157,"n_cols":54,"rows_kept":157,"cut":false,"hidden":true,"merged":[[116,48,116,50],[96,32,98,33],[96,34,98,35],[96,36,98,37],[99,32,99,33],[99,34,99,35],[99,36,99,37],[115,39,115,41],[110,38,113,38],[110,39,111,40],[112,39,113,39],[112,40,113,40],[114,34,114,35],[114,36,114,37],[0,9,0,10],[1,5,1,8],[10,3,10,4],[42,1,42,2],[42,3,42,4],[42,5,42,6],[0,1,0,2],[0,3,0,4],[0,5,0,7],[42,7,43,10],[10,27,10,28],[11,3,11,4],[12,27,12,28],[17,27,17,28],[16,27,16,28],[17,12,17,16],[13,27,13,28],[44,9,44,10],[44,11,44,12],[44,13,44,14],[42,11,43,14],[67,1,67,2],[67,3,67,4],[67,5,67,6],[67,8,67,9],[67,13,67,14],[44,7,44,8],[13,29,13,30],[13,12,13,16],[26,27,26,28],[44,21,44,22],[42,15,43,18],[44,15,44,16],[44,17,44,18],[43,21,43,24],[44,23,44,24],[44,25,44,26],[111,5,111,6],[62,27,62,28],[77,13,77,14],[99,26,99,27],[99,28,99,29],[67,10,67,11],[62,29,62,30],[67,15,67,16],[67,20,67,21],[67,22,67,23],[96,22,97,23],[77,8,77,9],[77,10,77,11],[77,15,77,16],[99,24,99,25],[99,30,99,31],[77,1,77,2],[90,1,90,2],[90,3,90,4],[90,5,90,6],[77,3,77,4],[77,5,77,6]]}
["Točke","ZID I TEMELJ",null,"NASIP NA TEMELJU IZA",null,"ZID, KONZOLA I NASIP NA KONZOLI",null,null,null,null,null,null,null,null,"Presjek XV",{"$f":"+($B$9-$B$4)*(Q1-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},null,null,null,"Točka A",null,"Presjek I-I"]
[1,2,{"$f":"'Analiza i dimenzioniranje'!BG9+'Unos podataka'!J41","v":0.12820515121628623},null,null,"ZA BILO KOJI PRESJEK ",null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(Q2-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+Q1","v":4.4000000000000004},"Presjek zid Iv",{"$f":"+($B$9-$B$4)*(T2-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AH44","v":5.36},{"$f":"+B15","v":4.9000021999999994},{"$f":"+C15","v":0.5},{"$f":"+'C XVIII-XIX'!B10+0.05","v":{"$error":"#VALUE!"}},-0.5]
[2,2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,null,null,null,null,null,null,null,"Presjek Xvi",{"$f":"+($B$9-$B$4)*(Q3-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AF44","v":4.72},null,{"$f":"+($B$11-$B$10)*(T3-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AH44","v":5.36},"Točka B",null,{"$f":"+W2","v":{"$error":"#VALUE!"}},{"$f":"+'C XVIII-XIX'!C10+0.5","v":{"$error":"#VALUE!"}}]
[3,{"$f":"+B3+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+C3","v":1.2},{"$f":"+B19","v":2},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>C4,B21,B4)","v":3.4000010999999999},{"$f":"IF(E20>C4,E20,C4)","v":1.2},{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(Q4-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+Q3","v":4.72},"Presjek V",{"$f":"+($B$9-$B$4)*(T4-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AI44","v":5.6800000000000006},{"$f":"+'C XVIII-XIX'!B2","v":2},{"$f":"+'C XVIII-XIX'!C2","v":0.12820515121628623}]
[4,{"$f":"+B23","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},{"$f":"+D4","v":2},{"$f":"+'C XVI-XVII'!E5","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,B21,B5)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C5,E20,C5)","v":3.14},{"$f":"+F8","v":{"$error":"#VALUE!"}},{"$f":"+G8","v":3.44},null,null,null,null,null,"Presjek Xvii",{"$f":"+($B$9-$B$4)*(Q5-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AG44","v":5.04},null,{"$f":"+($B$11-$B$10)*(T5-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AI44","v":5.6800000000000006},null,null,"Presjek II-II",null,null,null,"Nasip na zidu iza"]
[5,{"$f":"+B5-'Analiza i dimenzioniranje'!G78","v":{"$error":"#VALUE!"}},{"$f":"+C5","v":3.14},{"$f":"IF(B6<2,B5,IF(B9>2,B9,D5))","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!E6","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C7,B21,B6)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C6,E20,C6)","v":3.14},{"$f":"IF(F7>F9,H5,F9)","v":{"$error":"#VALUE!"}},{"$f":"IF(F7>F9,I5,IF(E20>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XVIII-XIX'!E20,G9))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(Q6-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+Q5","v":5.04},"Presjek VI",{"$f":"+($B$9-$B$4)*(T6-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},"TLO 1. sloj",null,{"$f":"+'C XVIII-XIX'!B15-0.05","v":4.8500021999999996},{"$f":"+'C XVIII-XIX'!X2","v":-0.5},null,null,2,{"$f":"IF('Analiza i dimenzioniranje'!AW26>'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AY26,'Analiza i dimenzioniranje'!AW26)","v":0}]
[6,{"$f":"IF('Analiza i dimenzioniranje'!G78=0,'C XVIII-XIX'!B8,B6)","v":{"$error":"#VALUE!"}},{"$f":"C6+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+B4","v":3.4000010999999999},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"IF(E20>=C7,B21,B7)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C7,E20,C7)","v":3.44},{"$f":"IF(F7>F9,H6,H6)","v":{"$error":"#VALUE!"}},{"$f":"+I6","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Presjek Xviii",{"$f":"+($B$9-$B$4)*(Q7-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},null,null,{"$f":"+($B$11-$B$10)*(T7-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!V44","v":1.52},{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},{"$f":"+'C XVIII-XIX'!B15-0.05","v":4.8500021999999996},{"$f":"+'C XVIII-XIX'!X3","v":{"$error":"#VALUE!"}},"Horizontala",null,2,{"$f":"'Analiza i dimenzioniranje'!BF28","v":0}]
[7,{"$f":"+B22","v":{"$error":"#VALUE!"}},{"$f":"+C7","v":3.44},{"$f":"+D4","v":2},{"$f":"+E4","v":1.2},{"$f":"IF(E20>C8,B21,B8)","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>=C8,E20,C8)","v":3.44},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"IF('Unos podataka'!$H$15=0,I7+(H7-H8)*'Unos podataka'!R57,IF('C III-V'!H9>'Unos podataka'!$B$105,I7+(H7-H8)*'Unos podataka'!$R$55,'Unos podataka'!$T$57))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(Q8-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"Presjek VII",{"$f":"+($B$9-$B$4)*(T8-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!V8","v":6},null,null,{"$f":"+'C XVIII-XIX'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C XVIII-XIX'!C5","v":3.14}]
[8,{"$f":"B4-TAN('Analiza i dimenzioniranje'!H51*PI()/180)*('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},null,null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},{"$f":"+H4","v":{"$error":"#VALUE!"}},{"$f":"+I4","v":3.44},null,null,null,null,null,"Presjek Xix",{"$f":"+($B$9-$B$4)*(Q9-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},null,null,{"$f":"+($B$11-$B$10)*(T9-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!W44","v":1.84},{"$f":"+U8-'Analiza i dimenzioniranje'!E27","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!V9","v":6.2644906473896782},"Presjek ZID",null,{"$f":"+IF('Analiza i dimenzioniranje'!$E$24=0,0,'C XVIII-XIX'!Y4)","v":0},{"$f":"+Z8","v":3.14}]
[9,{"$f":"+B9+'Analiza i dimenzioniranje'!E54","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},null,null,{"$f":"+B10","v":{"$error":"#VALUE!"}},{"$f":"+C10","v":"A"},null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(Q10-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"Presjek VIII",{"$f":"+($B$9-$B$4)*(T10-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},-8,{"$f":"+'C III-V'!V10","v":6.2644906473896782},{"$f":"+'C XVIII-XIX'!B15-0.5","v":4.4000021999999994},{"$f":"+'C XVIII-XIX'!C10+0.1","v":{"$error":"#VALUE!"}}]
[10,{"$f":"+B4+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+C3","v":1.2},"NASIP NA KONZOLI",null,{"$f":"+F12+E65","v":{"$error":"#VALUE!"}},{"$f":"IF(E20>C11,E20,C11)","v":1.2},null,null,null,null,null,null,null,"Presjek Xx",{"$f":"+($B$9-$B$4)*(Q11-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},null,null,{"$f":"+($B$11-$B$10)*(T11-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!X44","v":2.16},"x","y",{"$f":"+'C XVIII-XIX'!B10+0.5","v":{"$error":"#VALUE!"}},{"$f":"+X10","v":{"$error":"#VALUE!"}},null,null,null,"Rsidra"]
[11,{"$f":"+B11","v":4.2000010999999997},{"$f":"+C11","v":1.2},"za stabilnost",null,{"$f":"+F4","v":3.4000010999999999},{"$f":"+G4","v":1.2},null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(Q12-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"Presjek IX",{"$f":"+($B$9-$B$4)*(T12-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+W23","v":{"$error":"#VALUE!"}},{"$f":"+U12*(V9-V8)/(U9-U8)-U8*(V9-V8)/(U9-U8)+V8","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,20,AB16)","v":20},{"$f":"IF('Analiza i dimenzioniranje'!$T$22=0,0,AC16)","v":0}]
[12,{"$f":"+B12","v":4.2000010999999997},{"$f":"+C12","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T13-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Y44","v":2.48},{"$f":"+W25","v":{"$error":"#VALUE!"}},{"$f":"+U13*(V9-V8)/(U9-U8)-U8*(V9-V8)/(U9-U8)+V8","v":{"$error":"#VALUE!"}},"Pad terena niz padinu",null,null,null,null,"Os rezultante sidara Ukupna računska sila u sidrima"]
[13,{"$f":"+B11+'Analiza i dimenzioniranje'!G57","v":4.9000021999999994},{"$f":"+C13","v":1.2},{"$f":"+B7","v":{"$error":"#VALUE!"}},3.44,null,null,null,null,"Linija presjeka",null,null," Koordinata sredine presjeka",null,null,null,null,"Presjek X",{"$f":"+($B$9-$B$4)*(T14-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},"TLO 2. sloj",null,{"$f":"+'Analiza i dimenzioniranje'!Q105","v":3},{"$f":"+'Analiza i dimenzioniranje'!P105","v":{"$error":"#VALUE!"}},null,null,null,"Slobodna  zona.",null,"1. sloj"]
[14,{"$f":"+B14","v":4.9000021999999994},{"$f":"+C14-'Analiza i dimenzioniranje'!E51","v":0.5},{"$error":"#VALUE!"},3.44,{"$f":"IF((B4-B9)=0,0,+(C9-C4)/(B4-B9))","v":{"$error":"#VALUE!"}},"n  Nagib zida u tlu",null,null,0,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,"III-III","konzola","Presjek I","Presjek II",null,{"$f":"+($B$11-$B$10)*(T15-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!Z44","v":2.8},{"$f":"IF(('Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17)<'Analiza i dimenzioniranje'!$F$45,2,(IF(B7<B24,B7,IF('Analiza i dimenzioniranje'!G78=0,'C XVIII-XIX'!B24,2))))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$F$17+'Analiza i dimenzioniranje'!$E$17","v":4},{"$f":"+'Analiza i dimenzioniranje'!O130","v":7.1000021999999996},{"$f":"+'Analiza i dimenzioniranje'!N130","v":1.5001009999999999},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,AB24)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,'Analiza i dimenzioniranje'!P22)","v":5},{"$f":"+U9","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782}]
[15,{"$f":"+B2","v":2},{"$f":"+C2","v":0.12820515121628623},{"$error":"#VALUE!"},"A",null,null,null,null,3,{"$f":"+K15","v":1.2},null,"x",{"$f":"+(F12+F11)/2","v":{"$error":"#VALUE!"}},{"$f":"(B8+(B11-B10)*(O17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U29+(B11-B10)*(P17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},{"$f":"(U34+(B11-B10)*(Q17-C10)/(C11-C10)+B10)/2","v":{"$error":"#VALUE!"}},"Presjek XI",{"$f":"+($B$9-$B$4)*(T16-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},-8,{"$f":"+V15+(U15-U16)*TAN('Analiza i dimenzioniranje'!$E$18*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"AB15-'Analiza i dimenzioniranje'!P23","v":{"$error":"#VALUE!"}},{"$f":"+AC15-(AB15-AB16)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782}]
[null,null,"Jednadžba pravca zida uz tlo",{"$f":"+D16","v":{"$error":"#VALUE!"}},{"$f":"+I7","v":{"$error":"#VALUE!"}},null,null,null,null,"Sloj 2 gore",null,null,"y",{"$f":"+G11","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+'Analiza i dimenzioniranje'!AI44","v":5.6800000000000006},{"$f":"+'Analiza i dimenzioniranje'!AH44","v":5.36},null,{"$f":"+($B$11-$B$10)*(T17-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AA44","v":3.14},"TLO 3. sloj",null,"Prometno opterećenje",null,null,null,null,"Sidrena dionica",null,"Jednadžba površine terena"]
[null,"x","y",{"$f":"+D14","v":{"$error":"#VALUE!"}},{"$f":"+I8","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+F94","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E52>=G94,0,G94)","v":4},null,null,null,null,null,null,"Presjek XII",{"$f":"+($B$9-$B$4)*(T18-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},2,{"$f":"+'Analiza i dimenzioniranje'!$F$17","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,+'C XVIII-XIX'!B9-'Analiza i dimenzioniranje'!E26)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$24=0,0,'C XVIII-XIX'!V9)","v":6.2644906473896782},null,null,null,"                   Y=",null,{"$f":"+(AE16-AE15)/(AD16-AD15)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AD18*AD15+AE15","v":{"$error":"#VALUE!"}}]
[null,2,{"$f":"+B19*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},{"$f":"+D14","v":{"$error":"#VALUE!"}},{"$f":"+E14","v":3.44},null,null,null,null,{"$f":"U16","v":-8},{"$f":"+K18","v":4},null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T19-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AB44","v":3.44},-8,{"$f":"+V18+(U18-U19)*TAN('Analiza i dimenzioniranje'!$F$18*PI()/180)","v":1.5492076949174773},{"$f":"+W18","v":{"$error":"#VALUE!"}},{"$f":"+X18+'Analiza i dimenzioniranje'!E24/50","v":6.4644906473896784},null,null,null,{"$f":"+AB16","v":{"$error":"#VALUE!"}},{"$f":"+AC16","v":{"$error":"#VALUE!"}},"za x=",{"$f":"+AB20","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+H8","v":{"$error":"#VALUE!"}},{"$f":"+B20*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},"M na koti",{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,null,null,null,"Sloj 1 ili2 dole",null,null,null,null,null,null,{"$f":"+(B11-B10)*(Q21-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},"Presjek XIII",{"$f":"+($B$9-$B$4)*(T20-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},"KONTAKTNI NAPONI",null,{"$f":"+W18-'Analiza i dimenzioniranje'!E25","v":{"$error":"#VALUE!"}},{"$f":"+X19","v":6.4644906473896784},null,null,null,{"$f":"+(AB21+AB19)/2","v":{"$error":"#VALUE!"}},{"$f":"+(AC19+AC21)/2","v":{"$error":"#VALUE!"}},"y=",{"$f":"+AD18*AE19+AF18","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C21-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,{"$f":"+IF('Analiza i dimenzioniranje'!G78=0,D8,H8)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+F95","v":{"$error":"#VALUE!"}},{"$f":"+G12","v":1.2},null,null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,{"$f":"+($B$11-$B$10)*(T21-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AC44","v":3.76},2,0,{"$f":"+W20","v":{"$error":"#VALUE!"}},{"$f":"+X18","v":6.2644906473896782},null,null,null,{"$f":"+AB19-'Analiza i dimenzioniranje'!P24","v":{"$error":"#VALUE!"}},{"$f":"+AC19-(AB19-AB21)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},"visina sloja iznad centra sidra"]
[null,{"$f":"+(B9-B4)*(C22-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+C23+'Analiza i dimenzioniranje'!C77","v":3.44},null,null,null,null,null,null,{"$f":"+U19","v":-8},{"$f":"+K21","v":1.2},null,null,null,null,null,null,"Presjek XIV",{"$f":"+($B$9-$B$4)*(T22-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},2,{"$f":"-'Analiza i dimenzioniranje'!$F$193/100","v":{"$error":"#VALUE!"}},"Točkasto",null,null,null,null,null,null,{"$f":"+AE20-AC20","v":{"$error":"#VALUE!"}},"m"]
[null,{"$f":"+(B9-B4)*(C23-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F45","v":3.14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T23-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AD44","v":4.08},{"$f":"2+'Analiza i dimenzioniranje'!$E$61","v":4.9000021999999994},{"$f":"-'Analiza i dimenzioniranje'!$F$190/100","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E36=0,-10,B9-'Analiza i dimenzioniranje'!E37)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X23","v":{"$error":"#VALUE!"}},null,null,null,"Jednadžba  lica zida "]
[null,{"$f":"+(B9-B4)*(C24-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V15","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek XV",{"$f":"+($B$9-$B$4)*(T24-$C$4)/($C$9-$C$4)+$B$4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U23","v":4.9000021999999994},0,"Linijsko iza zida",null,null,null,"x=",{"$f":"+($B$11-$B$10)*(AB25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+($B$11-$B$10)*(AC25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+(B11-B10)*(AE25-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C25-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AI44","v":5.6800000000000006},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+($B$11-$B$10)*(T25-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AE44","v":4.4000000000000004},{"$f":"+U21","v":2},0,{"$f":"IF('Analiza i dimenzioniranje'!$E$34=0,0,B9-'Analiza i dimenzioniranje'!K28)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!X27","v":{"$error":"#VALUE!"}},null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!AH42","v":0},{"$f":"+'Analiza i dimenzioniranje'!AI42","v":0},null,{"$f":"+'Analiza i dimenzioniranje'!H76+'Analiza i dimenzioniranje'!E52","v":1.5001009999999999}]
[null,{"$f":"+(B9-B4)*(C26-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AH44","v":5.36},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid XIX-XIX",{"$f":"+'Analiza i dimenzioniranje'!AI44","v":5.6800000000000006},{"$f":"+W25","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$34=0,0,X25+1)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!T22","v":0},null,null,null,null,{"$f":"+B14-AE24","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+(B9-B4)*(C27-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AI44","v":5.6800000000000006},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!AI44","v":5.6800000000000006},"TEMELJ -opterećenje",null,"x=",{"$f":"+($B$11-$B$10)*(Z26-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"Rez. Sidra na zidu"]
[null,{"$f":"+(B9-B4)*(C28-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AH44","v":5.36},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V27","v":5.6800000000000006},{"$f":"+IF('Analiza i dimenzioniranje'!E28=0,0,W29)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9+'Analiza i dimenzioniranje'!F20+1.5)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!S22","v":0}]
["Sjecište s dnom temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V29-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":5.6800000000000006},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W30-0.3)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X30)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z28-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+($B$11-$B$10)*(AC29-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E40","v":3.9999999960000001},{"$f":"+AB29+0.4","v":{"$error":"#VALUE!"}},{"$f":"+AC29+(AD29-AB29)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}}]
["zid",{"$f":"+B20","v":{"$error":"#VALUE!"}},{"$f":"+B30*(C9-C4)/(B9-B4)-B4*(C9-C4)/(B9-B4)+C4","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V30-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V27","v":5.6800000000000006},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,B9-'Analiza i dimenzioniranje'!$E$32)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,X31+'Analiza i dimenzioniranje'!E33)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!R22","v":0},null,null,null,{"$f":"+AB29-1","v":{"$error":"#VALUE!"}},{"$f":"+AC29-(AB29-AD30)*'Analiza i dimenzioniranje'!E39*PI()/180","v":{"$error":"#VALUE!"}}]
["Vrh zida",{"$f":"+(B9-B4)*(C31-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!C558","v":-0.45},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Presjek zid Iv",{"$f":"+'Analiza i dimenzioniranje'!AH44","v":5.36},{"$f":"+W30","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,C9-'Analiza i dimenzioniranje'!K31)","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z30-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,"nagib lica"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+'Analiza i dimenzioniranje'!AH44","v":5.36},{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,W31-'Analiza i dimenzioniranje'!$E$29)","v":{"$error":"#VALUE!"}},{"$f":"+X31","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q22","v":3},null,"tan"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+V32","v":5.36},{"$f":"+W32","v":{"$error":"#VALUE!"}},{"$f":"+X30","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z32-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+(B13-B10)/(C10-C13)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate",{"$f":"+(B9-B4)*(V34-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+V33","v":5.36},{"$f":"IF('Analiza i dimenzioniranje'!E28=0,0,W33+0.3)","v":{"$error":"#VALUE!"}},{"$f":"+X29","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!Q20","v":5},null,"kut"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"presjeka",{"$f":"+(B11-B10)*(V35-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+V34","v":5.36},{"$f":"+W34","v":{"$error":"#VALUE!"}},{"$f":"+X28","v":{"$error":"#VALUE!"}},"x=",{"$f":"+($B$11-$B$10)*(Z34-$C$10)/($C$11-$C$10)+$B$10","v":{"$error":"#VALUE!"}},null,{"$f":"+ATAN(AB33)*180/PI()","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SIDRO za presjek",null,null,null,"Jednadžba pravca lica zida ",null,null,"Sjecište a arm konzole",null,"vrh zida","Anker armatura uz lice",null,"arm dno",null,"Y=",{"$f":"IF(AE38=AE37,1000000,(AF38-AF37)/(AE38-AE37))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AJ36*AE37+AF37","v":{"$error":"#VALUE!"}},"y=",{"$f":"+'Analiza i dimenzioniranje'!$C$545","v":1.6923077248520526}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB15)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC15)","v":5},null,null,"x=",null,null,{"$f":"+(B11-B10)*(AB38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AC38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AD38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+(B11-B10)*(AF37-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!B545","v":{"$error":"#VALUE!"}},{"$f":"+U81","v":2.0499999999999998},{"$f":"+V81","v":0.18682583433163008},"X=",{"$f":"+(-AL36+AL39)/(AJ36-AJ39)","v":{"$error":"#VALUE!"}},"sjeište",null,"x=",{"$f":"+(AN36-AL36)/AJ36","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('P III-III'!$E$38=0,0,+AB16)","v":{"$error":"#VALUE!"}},{"$f":"IF('P III-III'!$E$38=0,0,+AC16)","v":{"$error":"#VALUE!"}},null,null,"y=",null,null,{"$f":"+'Analiza i dimenzioniranje'!E555","v":3.39},{"$f":"+AB38-'Analiza i dimenzioniranje'!#REF!","v":{"$error":"#REF!"}},{"$f":"+'Analiza i dimenzioniranje'!C558","v":-0.45},{"$f":"+(B11-B10)*(AF38-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+U82","v":4.8600021999999994},{"$f":"+V82","v":0.54310345350772504},"Y=",{"$f":"+AJ36*AJ37+AL36","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Koordinate dna temelja",null,null,null,null,null,null,"Y=",{"$f":"+(AH38-AH37)/(AG38-AG37)","v":0.12678908905341604},"*x",{"$f":"-AJ39*AG37+AH37","v":-7.3091798227872762E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"lice","koord Pr II",{"$f":"+AB47+'Analiza i dimenzioniranje'!Q58","v":3.4500010999999997},{"$f":"(AB40*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24999999999999994},null,"SIDRO"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+(B11-B10)*(Z42-C10)/(C11-C10)+B10","v":{"$error":"#VALUE!"}},{"$f":"+B8","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+AB15","v":{"$error":"#VALUE!"}},{"$f":"+AC15","v":5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y=",{"$f":"+'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77","v":3.44},{"$f":"+Z42","v":3.44},null,null,null,{"$f":"IF('Analiza i dimenzioniranje'!K39=0,0,AB15-0.5)","v":{"$error":"#VALUE!"}},{"$f":"+AF41-(AE41-AE42)*TAN('Analiza i dimenzioniranje'!E39*PI()/180)","v":{"$error":"#VALUE!"}},null,"Nasip ispred zida"]
["Oznaka","temelj",null,"Zid i konzola za pr. ZID",null,"Nasip na temelju iza zida",null,"      Za momente u presjeku zid-temelj          ",null,null,null,"      Za momente u presjeku XVIII-XVIII",null,null,null,"         Za momente u presjeku XIX-XIX",null,null,null,null,1,null,null,null,null,null,null,2,0,null,null,null,null,{"$f":"+AE24","v":{"$error":"#VALUE!"}},{"$f":"+C11+'Analiza i dimenzioniranje'!$H$76","v":1.5001009999999999}]
["točke","x","y","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - BETON",null,null,null,null,null,2.65,{"$f":"+(AC47+AC49)/2","v":0.31034478180740688},null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!$E$61","v":4.9000021999999994},{"$f":"+AI43","v":1.5001009999999999}]
[1,{"$f":"+'C XVIII-XIX'!B2","v":2},{"$f":"+'C XVIII-XIX'!C2","v":0.12820515121628623},null,null,null,null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"ZID I KONZOLA",null,"Nasip na konzoli",null,"Kontaktni naponi za stab",null,"Beton do presjeka II-II",null,"Beton sredine temelja",null,"Beton do presjeka I-I",null,{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"(AB45*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH44+1.6","v":6.5000021999999991},{"$f":"+AI44-(AH45-AH44)*TAN('Analiza i dimenzioniranje'!H22*PI()/180)","v":1.5001009999999999}]
[2,{"$f":"+'C XVIII-XIX'!B3","v":2},{"$f":"+'C XVIII-XIX'!C3","v":1.2},null,null,null,null,"x","y","x","y","x","y","x","y","x","y","x","y","x","y",null,null,"x","y","x","y",{"$f":"+(AB43+AB47)/2","v":2.7000005499999999},{"$f":"(AB46*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.1206896584423281},null,null,null,null,"x","y"]
[3,{"$f":"+'C XVIII-XIX'!B4","v":3.4000010999999999},{"$f":"+'C XVIII-XIX'!C4","v":1.2},{"$f":"+B4","v":3.4000010999999999},1.2,2,1.2,3.4000010999999999,1.2,{"$f":"+D14","v":{"$error":"#VALUE!"}},3.44,{"$f":"+U34","v":{"$error":"#VALUE!"}},{"$f":"+V34","v":5.36},{"$f":"+J47","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AH44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AH44,K47)","v":5.36},{"$f":"+U29","v":{"$error":"#VALUE!"}},{"$f":"+V29","v":5.6800000000000006},{"$f":"+J47","v":{"$error":"#VALUE!"}},{"$f":"+S48","v":5.6800000000000006},{"$f":"+U21","v":2},{"$f":"+V21*100","v":0},2,0,{"$f":"+B4","v":3.4000010999999999},{"$f":"+W49","v":1.2},{"$f":"+B11","v":4.2000010999999997},1.2,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"(AB47*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24137931688465614},"Presjek II-II",null,null,null,{"$f":"+'C XVIII-XIX'!B11","v":4.2000010999999997},{"$f":"+C11","v":1.2}]
[4,{"$f":"+B11","v":4.2000010999999997},1.2,{"$error":"#VALUE!"},3.14,2,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.44,{"$f":"+H48","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AH44<'Analiza i dimenzioniranje'!F45,I48,'C XVIII-XIX'!V34)","v":5.36},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AH44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AH44,K48)","v":5.36},{"$f":"+H48","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AI44<'Analiza i dimenzioniranje'!F45,I48,V29)","v":5.6800000000000006},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AI44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AI44,K48)","v":5.6800000000000006},{"$f":"+U22","v":2},{"$f":"+V22*100","v":{"$error":"#VALUE!"}},2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+X47+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+Y47","v":1.2},4.2000010999999997,1.2,{"$f":"+AB77","v":{"$error":"#VALUE!"}},{"$f":"(AB48*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47+'Analiza i dimenzioniranje'!H76","v":1.5001009999999999}]
[5,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.14,{"$f":"+D16","v":{"$error":"#VALUE!"}},{"$f":"+E16+'Unos podataka'!$F9","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AH44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XVIII-XIX'!L47,'C XVIII-XIX'!B6)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AH44<'Analiza i dimenzioniranje'!F45,I49,'C XVIII-XIX'!V34)","v":5.36},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AH44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AH44,K49)","v":5.36},{"$f":"IF('Analiza i dimenzioniranje'!AI44<='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XVIII-XIX'!B6,P47)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AI44<'Analiza i dimenzioniranje'!F45,'C XVIII-XIX'!I49,Q48)","v":5.6800000000000006},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AI44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AI44,K49)","v":5.6800000000000006},{"$f":"+U23","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},{"$f":"+V48+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+W48","v":1.2},{"$f":"+AB49","v":4.2000010999999997},{"$f":"+AC49","v":0.37931024673015767},4.2000010999999997,1.2,{"$f":"+AB47+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+(AB49*(AC43-AC53)/(AB43-AB53)-AB53*(AC43-AC53)/(AB43-AB53)+AC53)","v":0.37931024673015767},"Presjek I-I",null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+AI48","v":1.5001009999999999}]
[6,4.2000010999999997,1.2,{"$error":"#VALUE!"},3.44,3.4000010999999999,1.2,{"$error":"#VALUE!"},3.44,{"$f":"IF('Unos podataka'!$B$105>J47,'Unos podataka'!$B$105,J47)","v":{"$error":"#VALUE!"}},{"$f":"+K51","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AH44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XVIII-XIX'!L48,'C XVIII-XIX'!B7)","v":{"$error":"#VALUE!"}},{"$f":"+O47","v":5.36},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AH44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AH44,K50)","v":5.36},{"$f":"IF('Analiza i dimenzioniranje'!AI44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XVIII-XIX'!P47,H50)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AI44<='Analiza i dimenzioniranje'!F45,I50,V29)","v":5.6800000000000006},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AI44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AI44,K50)","v":5.6800000000000006},{"$f":"+U24","v":4.9000021999999994},{"$f":"+V24*100","v":0},{"$f":"+V49","v":3.4000010999999999},{"$f":"+AC47","v":0.24137931688465614},{"$f":"+X47","v":3.4000010999999999},{"$f":"+AC47","v":0.24137931688465614},4.9000021999999994,1.2,{"$f":"2+'Analiza i dimenzioniranje'!E61/2","v":3.4500010999999997},{"$f":"(AB50*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.24999999999999994},null,null,null,null,{"$f":"+AH49","v":4.9000021999999994},{"$f":"+C14","v":1.2}]
[7,4.9000021999999994,1.2,{"$error":"#VALUE!"},3.44,2,1.2,{"$error":"#VALUE!"},3.44,{"$f":"+D18","v":{"$error":"#VALUE!"}},{"$f":"+E18+'Unos podataka'!$F9","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AH44>'Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XVIII-XIX'!B28,B8)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AH44>='Analiza i dimenzioniranje'!I75+'Analiza i dimenzioniranje'!G67,'C XVIII-XIX'!M50,Z26)","v":5.36},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AH44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AH44,K51)","v":5.36},{"$f":"IF('Analiza i dimenzioniranje'!AI44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'C XVIII-XIX'!B25,H51)","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!AI44<='Analiza i dimenzioniranje'!F45,I51,V29)","v":5.6800000000000006},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AI44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AI44,K51)","v":5.6800000000000006},{"$f":"+U25","v":2},{"$f":"+V25*100","v":0},{"$f":"+V47","v":2},{"$f":"+W47","v":0},{"$f":"+X47","v":3.4000010999999999},{"$f":"+Y47","v":1.2},4.9000021999999994,0.5,{"$f":"+(AB49+AB53)/2","v":4.5500016499999996},{"$f":"(AB51*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":0.43965512336507878},null,null,null,null,{"$f":"+B13","v":4.2000010999999997},{"$f":"+C13","v":1.2}]
[8,4.9000021999999994,0.5,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",{"$error":"#VALUE!"},3.44,{"$f":"+H52","v":{"$error":"#VALUE!"}},{"$f":"+Q52","v":"A"},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AH44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AH44,K52)","v":5.36},{"$f":"+H52","v":{"$error":"#VALUE!"}},{"$f":"+I52","v":"A"},{"$error":"#VALUE!"},{"$f":"IF('Analiza i dimenzioniranje'!AI44>='Analiza i dimenzioniranje'!F45+'Analiza i dimenzioniranje'!C77,'Analiza i dimenzioniranje'!AI44,K52)","v":5.6800000000000006},null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AC49","v":0.37931024673015767},{"$f":"+AD77","v":{"$error":"#VALUE!"}},{"$f":"(AB52*(AC53-AC43)/(AB53-AB43)-AB43*(AC53-AC43)/(AB53-AB43)+AC43)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+AH51","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[9,2,0.12820515121628623,{"$error":"#VALUE!"},"A",null,null,{"$error":"#VALUE!"},"A",null,null,{"$f":"+H53","v":{"$error":"#VALUE!"}},{"$f":"+Q53","v":"A"},null,null,{"$f":"+H53","v":{"$error":"#VALUE!"}},{"$f":"+I53","v":"A"},null,null,null,null,null,null,null,null,{"$f":"+Z47","v":4.2000010999999997},{"$f":"+AA47","v":1.2},{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+C15","v":0.5},null,null,null,null,{"$f":"+AH47","v":4.2000010999999997},{"$f":"+AI47","v":1.2}]
[10,null,null,4.2000010999999997,1.2,null,null,{"$error":"#VALUE!"},1.2,null,null,{"$f":"+U35","v":{"$error":"#VALUE!"}},{"$f":"+M47","v":5.36},null,null,{"$f":"+U30","v":{"$error":"#VALUE!"}},{"$f":"+V30","v":5.6800000000000006},null,null,null,null,null,null,null,null,null,null,"Koordinate s","naprezanjem"]
[11,null,null,{"$f":"+D47","v":3.4000010999999999},{"$f":"+E47","v":1.2},null,null,3.4000010999999999,1.2,null,null,{"$f":"+L47","v":{"$error":"#VALUE!"}},{"$f":"+M47","v":5.36},null,null,{"$f":"+P47","v":{"$error":"#VALUE!"}},{"$f":"+Q47","v":5.6800000000000006},null,null,null,null,null,null,null,null,null,null,{"$f":"+U22","v":2},{"$f":"+V22*100","v":{"$error":"#VALUE!"}}]
[12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"+AB56*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
[13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AB57*(AC58-AC55)/(AB58-AB55)-AB55*(AC58-AC55)/(AB58-AB55)+AC55","v":{"$error":"#VALUE!"}}]
["  A=",{"$f":"-0.5*((B45*C46-B46*C45)+(B46*C47-B47*C46)+(B47*C48-B48*C47)+(B48*C49-B49*C48)+(B49*C50-B50*C49)+(B50*C51-B51*C50)+(B51*C52-B52*C51)+(B52*C53-B53*C52))","v":2.5691044797107181},"m2",{"$f":"-0.5*((D45*E46-D46*E45)+(D46*E47-D47*E46)+(D47*E48-D48*E47)+(D48*E49-D49*E48)+(D49*E50-D50*E49)+(D50*E51-D51*E50)+(D51*E52-D52*E51)+(D52*E53-D53*E52)+(D53*E54-D54*E53)+(D54*E55-D55*E54)+(D55*E56-D56*E55)+(D56*E57-D57*E56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((F45*G46-F46*G45)+(F46*G47-F47*G46)+(F47*G48-F48*G47)+(F48*G49-F49*G48)+(F49*G50-F50*G49)+(F50*G51-F51*G50)+(F51*G52-F52*G51)+(F52*G53-F53*G52)+(F53*G54-F54*G53)+(F54*G55-F55*G54)+(F55*G56-F56*G55)+(F56*G57-F57*G56))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((H47*I48-H48*I47)+(H48*I49-H49*I48)+(H49*I50-H50*I49)+(H50*I51-H51*I50)+(H51*I52-H52*I51)+(H52*I53-H53*I52)+(H53*I54-H54*I53)+(H54*I55-H55*I54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((J47*K48-J48*K47)+(J48*K49-J49*K48)+(J49*K50-J50*K49)+(J50*K51-J51*K50)+(J51*K52-J52*K51)+(J52*K53-J53*K52)+(J53*K54-J54*K53)+(J54*K55-J55*K54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((L47*M48-L48*M47)+(L48*M49-L49*M48)+(L49*M50-L50*M49)+(L50*M51-L51*M50)+(L51*M52-L52*M51)+(L52*M53-L53*M52)+(L53*M54-L54*M53)+(L54*M55-L55*M54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"IF(0.5*((N47*O48-N48*O47)+(N48*O49-N49*O48)+(N49*O50-N50*O49)+(N50*O51-N51*O50)+(N51*O52-N52*O51)+(N52*O53-N53*O52)+(N53*O54-N54*O53)+(N54*O55-N55*O54))<0,0,0.5*((N47*O48-N48*O47)+(N48*O49-N49*O48)+(N49*O50-N50*O49)+(N50*O51-N51*O50)+(N51*O52-N52*O51)+(N52*O53-N53*O52)+(N53*O54-N54*O53)+(N54*O55-N55*O54)))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((P47*Q48-P48*Q47)+(P48*Q49-P49*Q48)+(P49*Q50-P50*Q49)+(P50*Q51-P51*Q50)+(P51*Q52-P52*Q51)+(P52*Q53-P53*Q52)+(P53*Q54-P54*Q53)+(P54*Q55-P55*Q54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((R47*S48-R48*S47)+(R48*S49-R49*S48)+(R49*S50-R50*S49)+(R50*S51-R51*S50)+(R51*S52-R52*S51)+(R52*S53-R53*S52)+(R53*S54-R54*S53)+(R54*S55-R55*S54))","v":{"$error":"#VALUE!"}},"m2",{"$f":"0.5*((T47*U48-T48*U47)+(T48*U49-T49*U48)+(T49*U50-T50*U49)+(T50*U51-T51*U50)+(T51*U52-T52*U51)+(T52*U53-T53*U52)+(T53*U54-T54*U53)+(T54*U55-T55*U54))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((V47*W48-V48*W47)+(V48*W49-V49*W48)+(V49*W50-V50*W49)+(V50*W51-V51*W50))","v":1.5110356654221164},"m2",{"$f":"-0.5*((X47*Y48-X48*Y47)+(X48*Y49-X49*Y48)+(X49*Y50-X50*Y49)+(X50*Y51-X51*Y50))","v":0.71172417455407389},"m2",{"$f":"-0.5*((Z47*AA48-Z48*AA47)+(Z48*AA49-Z49*AA48)+(Z49*AA50-Z50*AA49)+(Z50*AA51-Z51*AA50)+(Z51*AA52-Z52*AA51)+(Z52*AA53-Z53*AA52)+(Z53*AA54-Z54*AA53)+(Z54*AA55-Z55*AA54))","v":0.53224225002380887},"m2",{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+V23*100","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"-0.5*((AH47*AI48-AH48*AI47)+(AH48*AI49-AH49*AI48)+(AH49*AI50-AH50*AI49)+(AH50*AI51-AH51*AI50)+(AH51*AI52-AH52*AI51)+(AH52*AI53-AH53*AI52)+(AH53*AI54-AH54*AI53)+(AH54*AI55-AH55*AI54))","v":0.21007103011109951},"m2"]
["xt=",{"$f":"-((B45*C46-B46*C45)*(B45+B46)+(B46*C47-B47*C46)*(B46+B47)+(B47*C48-B48*C47)*(B47+B48)+(B48*C49-B49*C48)*(B48+B49)+(B49*C50-B50*C49)*(B49+B50)+(B50*C51-B51*C50)*(B50+B51)+(B51*C52-B52*C51)*(B51+B52)+(B52*C53-B53*C52)*(B52+B53)+(B53*C54-B54*C53)*(B53+B54)+(B54*C55-B55*C54)*(B54+B55)+(B55*C56-B56*C55)*(B55+B56)+(B56*C57-B57*C56)*(B56+B57))/6/B58","v":3.3485779696489133},"m",{"$f":"-((D45*E46-D46*E45)*(D45+D46)+(D46*E47-D47*E46)*(D46+D47)+(D47*E48-D48*E47)*(D47+D48)+(D48*E49-D49*E48)*(D48+D49)+(D49*E50-D50*E49)*(D49+D50)+(D50*E51-D51*E50)*(D50+D51)+(D51*E52-D52*E51)*(D51+D52)+(D52*E53-D53*E52)*(D52+D53)+(D53*E54-D54*E53)*(D53+D54)+(D54*E55-D55*E54)*(D54+D55)+(D55*E56-D56*E55)*(D55+D56)+(D56*E57-D57*E56)*(D56+D57))/6/D58","v":{"$error":"#VALUE!"}},"m",{"$f":"-((F45*G46-F46*G45)*(F45+F46)+(F46*G47-F47*G46)*(F46+F47)+(F47*G48-F48*G47)*(F47+F48)+(F48*G49-F49*G48)*(F48+F49)+(F49*G50-F50*G49)*(F49+F50)+(F50*G51-F51*G50)*(F50+F51)+(F51*G52-F52*G51)*(F51+F52)+(F52*G53-F53*G52)*(F52+F53)+(F53*G54-F54*G53)*(F53+F54)+(F54*G55-F55*G54)*(F54+F55)+(F55*G56-F56*G55)*(F55+F56)+(F56*G57-F57*G56)*(F56+F57))/6/F58","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(H47*I48-H48*I47)*(H47+H48)+(H48*I49-H49*I48)*(H48+H49)+(H49*I50-H50*I49)*(H49+H50)+(H50*I51-H51*I50)*(H50+H51)+(H51*I52-H52*I51)*(H51+H52)+(H52*I53-H53*I52)*(H52+H53)+(H53*I54-H54*I53)*(H53+H54)+(H54*I55-H55*I54)*(H54+H55))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(J47+J48)+(J48*K49-J49*K48)*(J48+J49)+(J49*K50-J50*K49)*(J49+J50)+(J50*K51-J51*K50)*(J50+J51)+(J51*K52-J52*K51)*(J51+J52)+(J52*K53-J53*K52)*(J52+J53)+(J53*K54-J54*K53)*(J53+J54)+(J54*K55-J55*K54)*(J54+J55)+(J55*K56-J56*K55)*(J55+J56)+(J56*K57-J57*K56)*(J56+J57))/6/J58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(L47*M48-L48*M47)*(L47+L48)+(L48*M49-L49*M48)*(L48+L49)+(L49*M50-L50*M49)*(L49+L50)+(L50*M51-L51*M50)*(L50+L51)+(L51*M52-L52*M51)*(L51+L52)+(L52*M53-L53*M52)*(L52+L53)+(L53*M54-L54*M53)*(L53+L54)+(L54*M55-L55*M54)*(L54+L55))/6/L58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(N58=0,0,(+(N47*O48-N48*O47)*(N47+N48)+(N48*O49-N49*O48)*(N48+N49)+(N49*O50-N50*O49)*(N49+N50)+(N50*O51-N51*O50)*(N50+N51)+(N51*O52-N52*O51)*(N51+N52))/6/N58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(P47*Q48-P48*Q47)*(P47+P48)+(P48*Q49-P49*Q48)*(P48+P49)+(P49*Q50-P50*Q49)*(P49+P50)+(P50*Q51-P51*Q50)*(P50+P51)+(P51*Q52-P52*Q51)*(P51+P52)+(P52*Q53-P53*Q52)*(P52+P53)+(P53*Q54-P54*Q53)*(P53+P54)+(P54*Q55-P55*Q54)*(P54+P55))/6/P58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(R58=0,0,(+(R47*S48-R48*S47)*(R47+R48)+(R48*S49-R49*S48)*(R48+R49)+(R49*S50-R50*S49)*(R49+R50)+(R50*S51-R51*S50)*(R50+R51)+(R51*S52-R52*S51)*(R51+R52))/6/R58)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(T58=0,0,(+(T47*U48-T48*U47)*(T47+T48)+(T48*U49-T49*U48)*(T48+T49)+(T49*U50-T50*U49)*(T49+T50)+(T50*U51-T51*U50)*(T50+T51)+(T51*U52-T52*U51)*(T51+T52)+(T52*U53-T53*U52)*(T52+T53)+(T53*U54-T54*U53)*(T53+T54)+(T54*U55-T55*U54)*(T54+T55)+(T55*U56-T56*U55)*(T55+T56)+(T56*U57-T57*U56)*(T56+T57))/6/T58)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(V58=0,0,-(+(V47*W48-V48*W47)*(V47+V48)+(V48*W49-V49*W48)*(V48+V49)+(V49*W50-V50*W49)*(V49+V50)+(V50*W51-V51*W50)*(V50+V51))/6/V58)","v":2.6739089419190427},"m",{"$f":"IF(X58=0,0,-(+(X47*Y48-X48*Y47)*(X47+X48)+(X48*Y49-X49*Y48)*(X48+X49)+(X49*Y50-X50*Y49)*(X49+X50)+(X50*Y51-X51*Y50)*(X50+X51))/6/X58)","v":3.7896651910602248},"m",{"$f":"-(+(Z47*AA48-Z48*AA47)*(Z47+Z48)+(Z48*AA49-Z49*AA48)*(Z48+Z49)+(Z49*AA50-Z50*AA49)*(Z49+Z50)+(Z50*AA51-Z51*AA50)*(Z50+Z51)+(Z51*AA52-Z52*AA51)*(Z51+Z52)+(Z52*AA53-Z53*AA52)*(Z52+Z53)+(Z53*AA54-Z54*AA53)*(Z53+Z54)+(Z54*AA55-Z55*AA54)*(Z54+Z55)+(Z55*AA56-Z56*AA55)*(Z55+Z56)+(Z56*AA57-Z57*AA56)*(Z56+Z57))/6/Z58","v":4.5407423692617748},"m",null,null,null,null,"   Koordinate presjeka",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AH47+AH48)+(AH48*AI49-AH49*AI48)*(AH48+AH49)+(AH49*AI50-AH50*AI49)*(AH49+AH50)+(AH50*AI51-AH51*AI50)*(AH50+AH51)+(AH51*AI52-AH52*AI51)*(AH51+AH52)+(AH52*AI53-AH53*AI52)*(AH52+AH53)+(AH53*AI54-AH54*AI53)*(AH53+AH54)+(AH54*AI55-AH55*AI54)*(AH54+AH55)+(AH55*AI56-AH56*AI55)*(AH55+AH56)+(AH56*AI57-AH57*AI56)*(AH56+AH57))/6/AH58","v":4.550001650000004},"m"]
["yt=",{"$f":"-((B45*C46-B46*C45)*(C45+C46)+(B46*C47-B47*C46)*(C46+C47)+(B47*C48-B48*C47)*(C47+C48)+(B48*C49-B49*C48)*(C48+C49)+(B49*C50-B50*C49)*(C49+C50)+(B50*C51-B51*C50)*(C50+C51)+(B51*C52-B52*C51)*(C51+C52)+(B52*C53-B53*C52)*(C52+C53)+(B53*C54-B54*C53)*(C53+C54)+(B54*C55-B55*C54)*(C54+C55)+(B55*C56-B56*C55)*(C55+C56)+(B56*C57-B57*C56)*(C56+C57))/6/B58","v":0.75054981042380386},"m",{"$f":"-((D45*E46-D46*E45)*(E45+E46)+(D46*E47-D47*E46)*(E46+E47)+(D47*E48-D48*E47)*(E47+E48)+(D48*E49-D49*E48)*(E48+E49)+(D49*E50-D50*E49)*(E49+E50)+(D50*E51-D51*E50)*(E50+E51)+(D51*E52-D52*E51)*(E51+E52)+(D52*E53-D53*E52)*(E52+E53)+(D53*E54-D54*E53)*(E53+E54)+(D54*E55-D55*E54)*(E54+E55)+(D55*E56-D56*E55)*(E55+E56)+(D56*E57-D57*E56)*(E56+E57))/6/D58","v":{"$error":"#VALUE!"}},"m",{"$f":"-((F45*G46-F46*G45)*(G45+G46)+(F46*G47-F47*G46)*(G46+G47)+(F47*G48-F48*G47)*(G47+G48)+(F48*G49-F49*G48)*(G48+G49)+(F49*G50-F50*G49)*(G49+G50)+(F50*G51-F51*G50)*(G50+G51)+(F51*G52-F52*G51)*(G51+G52)+(F52*G53-F53*G52)*(G52+G53)+(F53*G54-F54*G53)*(G53+G54)+(F54*G55-F55*G54)*(G54+G55)+(F55*G56-F56*G55)*(G55+G56)+(F56*G57-F57*G56)*(G56+G57))/6/F58","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(H47*I48-H48*I47)*(I47+I48)+(H48*I49-H49*I48)*(I48+I49)+(H49*I50-H50*I49)*(I49+I50)+(H50*I51-H51*I50)*(I50+I51)+(H51*I52-H52*I51)*(I51+I52)+(H52*I53-H53*I52)*(I52+I53)+(H53*I54-H54*I53)*(I53+I54)+(H54*I55-H55*I54)*(I54+I55)+(H55*I56-H56*I55)*(I55+I56)+(H56*I57-H57*I56)*(I56+I57))/6/H58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(J58=0,0,(+(J47*K48-J48*K47)*(K47+K48)+(J48*K49-J49*K48)*(K48+K49)+(J49*K50-J50*K49)*(K49+K50)+(J50*K51-J51*K50)*(K50+K51)+(J51*K52-J52*K51)*(K51+K52)+(J52*K53-J53*K52)*(K52+K53)+(J53*K54-J54*K53)*(K53+K54)+(J54*K55-J55*K54)*(K54+K55)+(J55*K56-J56*K55)*(K55+K56)+(J56*K57-J57*K56)*(K56+K57))/6/J58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(L47*M48-L48*M47)*(M47+M48)+(L48*M49-L49*M48)*(M48+M49)+(L49*M50-L50*M49)*(M49+M50)+(L50*M51-L51*M50)*(M50+M51)+(L51*M52-L52*M51)*(M51+M52)+(L52*M53-L53*M52)*(M52+M53)+(L53*M54-L54*M53)*(M53+M54)+(L54*M55-L55*M54)*(M54+M55))/6/L58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(N58=0,0,(+(N47*O48-N48*O47)*(O47+O48)+(N48*O49-N49*O48)*(O48+O49)+(N49*O50-N50*O49)*(O49+O50)+(N50*O51-N51*O50)*(O50+O51)+(N51*O52-N52*O51)*(O51+O52)+(N52*O53-N53*O52)*(O52+O53)+(N53*O54-N54*O53)*(O53+O54)+(N54*O55-N55*O54)*(O54+O55)+(N55*O56-N56*O55)*(O55+O56)+(N56*O57-N57*O56)*(O56+O57))/6/N58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-(+(P47*Q48-P48*Q47)*(Q47+Q48)+(P48*Q49-P49*Q48)*(Q48+Q49)+(P49*Q50-P50*Q49)*(Q49+Q50)+(P50*Q51-P51*Q50)*(Q50+Q51)+(P51*Q52-P52*Q51)*(Q51+Q52)+(P52*Q53-P53*Q52)*(Q52+Q53)+(P53*Q54-P54*Q53)*(Q53+Q54)+(P54*Q55-P55*Q54)*(Q54+Q55))/6/P58","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(R58=0,0,(+(R47*S48-R48*S47)*(S47+S48)+(R48*S49-R49*S48)*(S48+S49)+(R49*S50-R50*S49)*(S49+S50)+(R50*S51-R51*S50)*(S50+S51)+(R51*S52-R52*S51)*(S51+S52)+(R52*S53-R53*S52)*(S52+S53)+(R53*S54-R54*S53)*(S53+S54)+(R54*S55-R55*S54)*(S54+S55)+(R55*S56-R56*S55)*(S55+S56)+(R56*S57-R57*S56)*(S56+S57))/6/R58)","v":{"$error":"#VALUE!"}},"m",{"$f":"-IF(T58=0,0,(+(T47*U48-T48*U47)*(U47+U48)+(T48*U49-T49*U48)*(U48+U49)+(T49*U50-T50*U49)*(U49+U50)+(T50*U51-T51*U50)*(U50+U51)+(T51*U52-T52*U51)*(U51+U52)+(T52*U53-T53*U52)*(U52+U53)+(T53*U54-T54*U53)*(U53+U54)+(T54*U55-T55*U54)*(U54+U55)+(T55*U56-T56*U55)*(U55+U56)+(T56*U57-T57*U56)*(U56+U57))/6/T58)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((V47*W48-V48*W47)*(W47+W48)+(V48*W49-V49*W48)*(W48+W49)+(V49*W50-V50*W49)*(W49+W50)+(V50*W51-V51*W50)*(W50+W51))/6/V58","v":0.65809555436880718},"kN",{"$f":"-((X47*Y48-X48*Y47)*(Y47+Y48)+(X48*Y49-X49*Y48)*(Y48+Y49)+(X49*Y50-X50*Y49)*(Y49+Y50)+(X50*Y51-X51*Y50)*(Y50+Y51))/6/X58","v":0.75428136494691478},"kN",{"$f":"-(+(Z47*AA48-Z48*AA47)*(AA47+AA48)+(Z48*AA49-Z49*AA48)*(AA48+AA49)+(Z49*AA50-Z50*AA49)*(AA49+AA50)+(Z50*AA51-Z51*AA50)*(AA50+AA51)+(Z51*AA52-Z52*AA51)*(AA51+AA52)+(Z52*AA53-Z53*AA52)*(AA52+AA53)+(Z53*AA54-Z54*AA53)*(AA53+AA54)+(Z54*AA55-Z55*AA54)*(AA54+AA55)+(Z55*AA56-Z56*AA55)*(AA55+AA56)+(Z56*AA57-Z57*AA56)*(AA56+AA57))/6/Z58","v":0.81902934843133712},"m",null,null,null,null,"II-II i I-I",null,{"$f":"-(+(AH47*AI48-AH48*AI47)*(AI47+AI48)+(AH48*AI49-AH49*AI48)*(AI48+AI49)+(AH49*AI50-AH50*AI49)*(AI49+AI50)+(AH50*AI51-AH51*AI50)*(AI50+AI51)+(AH51*AI52-AH52*AI51)*(AI51+AI52)+(AH52*AI53-AH53*AI52)*(AI52+AI53)+(AH53*AI54-AH54*AI53)*(AI53+AI54)+(AH54*AI55-AH55*AI54)*(AI54+AI55)+(AH55*AI56-AH56*AI55)*(AI55+AI56)+(AH56*AI57-AH57*AI56)*(AI56+AI57))/6/AH58","v":1.3500505000000005},"m"]
["G=",{"$f":"+B58*'Analiza i dimenzioniranje'!E62","v":64.227611992767947},"kN",{"$f":"+D58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"+F58*'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}},"kN",{"$f":"+H58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(J58*'Analiza i dimenzioniranje'!E63<0,0,J58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+L58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(N58*'Analiza i dimenzioniranje'!U41<0,0,N58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+P58*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"kN",{"$f":"IF(R58<=0,0,R58*'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},"kN",{"$f":"+T58*'Analiza i dimenzioniranje'!E49","v":{"$error":"#VALUE!"}},"kN (za L)",{"$f":"+V58*'Analiza i dimenzioniranje'!E62","v":37.77589163555291},"kN",{"$f":"+X58*'Analiza i dimenzioniranje'!E62","v":17.793104363851846},"kN",{"$f":"+Z58*'Analiza i dimenzioniranje'!E62","v":13.306056250595223},"kN",null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"AC47+'Analiza i dimenzioniranje'!C192/2","v":0.68753317931068247},{"$f":"+AH58*'Analiza i dimenzioniranje'!E62","v":5.2517757527774878},"kN"]
["Vertikala nasipa na konzoli",null,null,"Moment na konzoli",null,"Pokos na vrhu zida",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMELJ  - NAPONI ",null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+'C XVIII-XIX'!AC49+('Analiza i dimenzioniranje'!C191/2)","v":0.77418208680245293}]
[null,"x","y",{"$f":"IF('Analiza i dimenzioniranje'!G78=0,0,'Analiza i dimenzioniranje'!G78*'Analiza i dimenzioniranje'!C77*'Analiza i dimenzioniranje'!E62*(Q20-B5+'Analiza i dimenzioniranje'!G78/2)+J61*(O16-J59))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"+F64","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47","v":"A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"naponi za presjek II-II",null,"naponi za srednji dio ",null,"naponi za presjek I-I"]
[null,{"$f":"+F7","v":{"$error":"#VALUE!"}},{"$f":"+G7","v":3.44},"b1=",{"$f":"+H47-2","v":1.4000010999999999},{"$f":"+B52","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y","x","y","x","y","Koordinate dna temelja"]
[null,{"$f":"+B64","v":{"$error":"#VALUE!"}},{"$f":"IF(B65>J49,C19,+C20+'Analiza i dimenzioniranje'!F20+(H52-H50)*TAN('Analiza i dimenzioniranje'!F21*PI()/180))","v":{"$error":"#VALUE!"}},"b2=",{"$f":"'Analiza i dimenzioniranje'!E54+('Analiza i dimenzioniranje'!E55-'Analiza i dimenzioniranje'!E54)*(('Analiza i dimenzioniranje'!E47-'Analiza i dimenzioniranje'!E52)/(C9-C4))","v":{"$error":"#VALUE!"}},{"$f":"+B65","v":{"$error":"#VALUE!"}},{"$f":"+G64+(F64-F65)*TAN('Analiza i dimenzioniranje'!F21*PI()/180)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,0,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},0,{"$f":"+'C XVIII-XIX'!B11","v":4.2000010999999997},{"$f":"-U47","v":0},2,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Z65","v":2},{"$f":"AC55","v":{"$error":"#VALUE!"}},{"$f":"+AB65","v":3.4000010999999999},{"$f":"+AA67","v":{"$error":"#VALUE!"}},{"$f":"+AB57","v":4.2000010999999997},{"$f":"AC57","v":{"$error":"#VALUE!"}},{"$f":"+Z77","v":{"$error":"#VALUE!"}},{"$f":"(AF66*(AG70-AG65)/(AF70-AF65)-AF65*(AG70-AG65)/(AF70-AF65)+AG65)","v":{"$error":"#VALUE!"}}]
[null,"AKTIVNI TLAKOVI za stabilnost i Presjek III-III (bez E3)",null,null,null,null,null,null,"  AKTIVNI TLAKOVI za presjek kroz zid XVIII-XVIII",null,null,null,null,"    AKTIVNI TLAKOVI za presjek kroz zid XIX-XIX",null,null,null,null,null,null,null,null,null,null,null,{"$f":"2+'Analiza i dimenzioniranje'!F46","v":3.4000010999999999},{"$f":"AC56","v":{"$error":"#VALUE!"}},{"$f":"+AB66+'Analiza i dimenzioniranje'!E55","v":4.2000010999999997},{"$f":"+AE66","v":{"$error":"#VALUE!"}},{"$f":"+AB58","v":4.9000021999999994},{"$f":"+AC58","v":{"$error":"#VALUE!"}},{"$f":"+AB77","v":{"$error":"#VALUE!"}},{"$f":"+(AF67*(AG65-AG70)/(AF65-AF70)-AF70*(AG65-AG70)/(AF65-AF70)+AG70)","v":{"$error":"#VALUE!"}}]
[null,"E1",null,"E2",null,"E3",null,null,"E1",null,"E2 do presjeka kroz zid II",null,null,"E1",null,"E2",null,null,null,null,null,null,null,null,null,{"$f":"+Z67","v":3.4000010999999999},0,{"$f":"+AB67","v":4.2000010999999997},0,{"$f":"+AD67","v":4.9000021999999994},{"$f":"+U50","v":0},{"$f":"+AB67","v":4.2000010999999997},{"$f":"+(AF68*(AG65-AG70)/(AF65-AF70)-AF70*(AG65-AG70)/(AF65-AF70)+AG70)","v":0.37931024673015767}]
[null,0,{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C71","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},null,{"$f":"+N69","v":0},{"$f":"+O69","v":{"$error":"#VALUE!"}},{"$f":"+I71","v":{"$error":"#VALUE!"}},{"$f":"+L76","v":{"$error":"#VALUE!"}},null,{"$f":"+B69","v":0},{"$f":"+'Analiza i dimenzioniranje'!E47+'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+N71","v":{"$error":"#VALUE!"}},{"$f":"+O71","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"+Z65","v":2},0,{"$f":"+AB65","v":3.4000010999999999},0,{"$f":"+AD65","v":4.2000010999999997},{"$f":"+U51","v":0},{"$f":"+AD77","v":{"$error":"#VALUE!"}},{"$f":"+(AF69*(AG66-AG70)/(AF66-AF70)-AF70*(AG66-AG70)/(AF66-AF70)+AG70)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"+B69","v":0},{"$f":"+C69-'Analiza i dimenzioniranje'!D17-'Analiza i dimenzioniranje'!F20","v":{"$error":"#VALUE!"}},{"$f":"+D69+'Analiza i dimenzioniranje'!E16*'Analiza i dimenzioniranje'!E17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+E69-'Analiza i dimenzioniranje'!E17","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},null,{"$f":"+N70","v":0},{"$f":"+J69-('Analiza i dimenzioniranje'!F20+'P XVIII-XVIII'!E17)","v":{"$error":"#VALUE!"}},{"$f":"+K69+'P XVIII-XVIII'!F16*'P XVIII-XVIII'!F17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AH44","v":5.36},null,{"$f":"+B70","v":0},{"$f":"+O69-('Analiza i dimenzioniranje'!F20+'P XIX-XIX'!E17)","v":{"$error":"#VALUE!"}},{"$f":"+P69+'P XIX-XIX'!F16*'P XIX-XIX'!F17*'Analiza i dimenzioniranje'!F111","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AI44","v":5.6800000000000006},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AB53","v":4.9000021999999994},{"$f":"+AC53","v":0.5}]
[null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('Analiza i dimenzioniranje'!D17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},0,{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F70+'Analiza i dimenzioniranje'!F16*'Analiza i dimenzioniranje'!F17*'Analiza i dimenzioniranje'!F112","v":{"$error":"#VALUE!"}},0,null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('P XVIII-XVIII'!E17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+J70","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+L70","v":5.36},null,{"$f":"(+'Analiza i dimenzioniranje'!D16*('P XIX-XIX'!E17+'Analiza i dimenzioniranje'!F20)*'Analiza i dimenzioniranje'!F110)","v":{"$error":"#VALUE!"}},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+D71","v":0},{"$f":"+Q70","v":5.6800000000000006}]
[null,{"$f":"+B69","v":0},{"$f":"+C69","v":{"$error":"#VALUE!"}},0,{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F69","v":0},0,null,{"$f":"+N72","v":0},{"$f":"+O72","v":{"$error":"#VALUE!"}},{"$f":"+D72","v":0},{"$f":"+L69","v":{"$error":"#VALUE!"}},null,{"$f":"+N69","v":0},{"$f":"+O69","v":{"$error":"#VALUE!"}},{"$f":"+D72","v":0},{"$f":"+Q69","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+D69","v":{"$error":"#VALUE!"}},{"$f":"+E69","v":{"$error":"#VALUE!"}},{"$f":"+F72","v":0},{"$f":"+G70","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+K69","v":{"$error":"#VALUE!"}},{"$f":"+L69","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+P69","v":{"$error":"#VALUE!"}},{"$f":"+Q69","v":{"$error":"#VALUE!"}}]
[null,"Jednadžba vertikale kohezije    Određivanje sjecišta kohezije s pravcem od tlaka",null,null,null,null,null,{"$f":"+M74","v":"Jednadžba vertikale kohezije  -  sjecišta kohezije s pravcem od tlaka"},null,null,null,null,"Jednadžba vertikale kohezije  -  sjecišta kohezije s pravcem od tlaka"]
[null,"X","y","X","y","X","y",null,{"$f":"+N75","v":"X"},{"$f":"+O75","v":"y"},"X","y",null,"X","y","X","y"]
[null,{"$f":"2*'Analiza i dimenzioniranje'!D15/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F110)","v":12.361875887090893},{"$f":"B76*(C71-C72)/(B71-B72)-B72*(C71-C72)/(B71-B72)+C72","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!F12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F111)","v":{"$error":"#VALUE!"}},{"$f":"IF(D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69>'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,'Analiza i dimenzioniranje'!F17+'Analiza i dimenzioniranje'!E17,D76*(E70-E69)/(D70-D69)-D69*(E70-E69)/(D70-D69)+E69)","v":{"$error":"#VALUE!"}},{"$f":"2*'Analiza i dimenzioniranje'!C12/'Analiza i dimenzioniranje'!J28*SQRT('Analiza i dimenzioniranje'!F112)","v":{"$error":"#VALUE!"}},{"$f":"IF((F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70)>'Analiza i dimenzioniranje'!F17,'Analiza i dimenzioniranje'!F17,(F76*(G71-G70)/(F71-F70)-F70*(G71-G70)/(F71-F70)+G70))","v":{"$error":"#VALUE!"}},null,{"$f":"+N76","v":12.361875887090893},{"$f":"I76*(J71-J72)/(I71-I72)-I72*(J71-J72)/(I71-I72)+J72","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},null,{"$f":"+B76","v":12.361875887090893},{"$f":"N76*(O71-O72)/(N71-N72)-N72*(O71-O72)/(N71-N72)+O72","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"-0.5*((Z65*AA66-Z66*AA65)+(Z66*AA67-Z67*AA66)+(Z67*AA68-Z68*AA67)+(Z68*AA69-Z69*AA68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((AB65*AC66-AB66*AC65)+(AB66*AC67-AB67*AC66)+(AB67*AC68-AB68*AC67)+(AB68*AC69-AB69*AC68))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-0.5*((AD65*AE66-AD66*AE65)+(AD66*AE67-AD67*AE66)+(AD67*AE68-AD68*AE67)+(AD68*AE69-AD69*AE68)+(AD69*AE70-AD70*AE69)+(AD70*AE71-AD71*AE70)+(AD71*AE72-AD72*AE71)+(AD72*AE73-AD73*AE72))","v":{"$error":"#VALUE!"}},"kN/m'"]
[null,{"$f":"+B76","v":12.361875887090893},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},null,{"$f":"+N77","v":12.361875887090893},{"$f":"+J70","v":{"$error":"#VALUE!"}},{"$f":"+K76","v":{"$error":"#VALUE!"}},{"$f":"+L70","v":5.36},null,{"$f":"+N76","v":12.361875887090893},{"$f":"+O70","v":{"$error":"#VALUE!"}},{"$f":"+P76","v":{"$error":"#VALUE!"}},{"$f":"+Q70","v":5.6800000000000006},null,null,null,null,null,null,null,null,{"$f":"IF(Z76=0,0,-(+(Z65*AA66-Z66*AA65)*(Z65+Z66)+(Z66*AA67-Z67*AA66)*(Z66+Z67)+(Z67*AA68-Z68*AA67)*(Z67+Z68)+(Z68*AA69-Z69*AA68)*(Z68+Z69))/6/Z76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(AB76=0,0,-(+(AB65*AC66-AB66*AC65)*(AB65+AB66)+(AB66*AC67-AB67*AC66)*(AB66+AB67)+(AB67*AC68-AB68*AC67)*(AB67+AB68)+(AB68*AC69-AB69*AC68)*(AB68+AB69))/6/AB76)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(AD76=0,0,-(+(AD65*AE66-AD66*AE65)*(AD65+AD66)+(AD66*AE67-AD67*AE66)*(AD66+AD67)+(AD67*AE68-AD68*AE67)*(AD67+AD68)+(AD68*AE69-AD69*AE68)*(AD68+AD69))/6/AD76)","v":{"$error":"#VALUE!"}},"m"]
["Oznaka","E1",null,"E2",null,"E3",null,{"$f":"+M78","v":"Oznaka"},{"$f":"+N78","v":"E1"},null,"E2",null,"Oznaka","E1",null,"E2",null,null,null,null,null,null,null,null,null,{"$f":"-((Z65*AA66-Z66*AA65)*(AA65+AA66)+(Z66*AA67-Z67*AA66)*(AA66+AA67)+(Z67*AA68-Z68*AA67)*(AA67+AA68)+(Z68*AA69-Z69*AA68)*(AA68+AA69))/6/Z76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((AB65*AC66-AB66*AC65)*(AC65+AC66)+(AB66*AC67-AB67*AC66)*(AC66+AC67)+(AB67*AC68-AB68*AC67)*(AC67+AC68)+(AB68*AC69-AB69*AC68)*(AC68+AC69))/6/AB76","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"-((AD65*AE66-AD66*AE65)*(AE65+AE66)+(AD66*AE67-AD67*AE66)*(AE66+AE67)+(AD67*AE68-AD68*AE67)*(AE67+AE68)+(AD68*AE69-AD69*AE68)*(AE68+AE69))/6/AD76","v":{"$error":"#VALUE!"}},"kN/m'"]
["točke","x","y","x","y","x","y","točke",{"$f":"+N79","v":"x"},{"$f":"+O79","v":"y"},"x","y","točke","x","y","x","y"]
[1,{"$f":"+B77","v":12.361875887090893},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,1,{"$f":"+I69","v":0},{"$f":"+J69","v":{"$error":"#VALUE!"}},{"$f":"+K76","v":{"$error":"#VALUE!"}},{"$f":"+L76","v":{"$error":"#VALUE!"}},1,{"$f":"+N69","v":0},{"$f":"+O69","v":{"$error":"#VALUE!"}},{"$f":"+P69","v":{"$error":"#VALUE!"}},{"$f":"+Q76","v":{"$error":"#VALUE!"}},null,"Jedn pravca zida uz tlo",null,"Jedn pravca arm dno ",null,"Y=",{"$f":"IF(S82=S81,1000000,(T82-T81)/(S82-S81))","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X80*S81+T81","v":{"$error":"#VALUE!"}}]
[2,{"$f":"+B71","v":{"$error":"#VALUE!"}},{"$f":"+C70","v":{"$error":"#VALUE!"}},{"$f":"+D76","v":{"$error":"#VALUE!"}},{"$f":"+E76","v":{"$error":"#VALUE!"}},{"$f":"+F76","v":{"$error":"#VALUE!"}},{"$f":"+G76","v":{"$error":"#VALUE!"}},2,{"$f":"+I70","v":0},{"$error":"#VALUE!"},{"$f":"+K69","v":{"$error":"#VALUE!"}},{"$f":"+L69","v":{"$error":"#VALUE!"}},2,{"$f":"+N70","v":0},{"$error":"#VALUE!"},{"$f":"+P69","v":{"$error":"#VALUE!"}},{"$f":"+Q69","v":{"$error":"#VALUE!"}},null,{"$f":"+B4","v":3.4000010999999999},{"$f":"+C4","v":1.2},{"$f":"+'Analiza i dimenzioniranje'!T593","v":2.0499999999999998},{"$f":"+'Analiza i dimenzioniranje'!U593","v":0.18682583433163008},"X=",{"$f":"+(-Z80+Z83)/(X80-X83)","v":{"$error":"#VALUE!"}},"sjeište"]
[3,{"$f":"+B80","v":12.361875887090893},{"$f":"+C76","v":{"$error":"#VALUE!"}},{"$f":"IF(D76>D69,D81,D69)","v":{"$error":"#VALUE!"}},{"$f":"+E81","v":{"$error":"#VALUE!"}},{"$f":"IF(F77>F70,F77,F70)","v":{"$error":"#VALUE!"}},{"$f":"IF(F77>F70,G76,G70)","v":{"$error":"#VALUE!"}},3,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+K70","v":{"$error":"#VALUE!"}},{"$f":"+L70","v":5.36},3,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+P70","v":{"$error":"#VALUE!"}},{"$f":"+Q70","v":5.6800000000000006},null,{"$f":"+B9","v":{"$error":"#VALUE!"}},{"$f":"+C9","v":"A"},{"$f":"+'Analiza i dimenzioniranje'!T594","v":4.8600021999999994},{"$f":"+'Analiza i dimenzioniranje'!U594","v":0.54310345350772504},"Y=",{"$f":"+X80*X81+Z80","v":{"$error":"#VALUE!"}}]
[4,{"$f":"+B80","v":12.361875887090893},{"$f":"+C80","v":{"$error":"#VALUE!"}},{"$f":"+D70","v":{"$error":"#VALUE!"}},{"$f":"+E70","v":{"$error":"#VALUE!"}},{"$f":"+F71","v":{"$error":"#VALUE!"}},{"$f":"+G71","v":0},4,0,{"$error":"#VALUE!"},{"$f":"+K80","v":{"$error":"#VALUE!"}},{"$f":"+L82","v":5.36},4,0,{"$error":"#VALUE!"},{"$f":"+P80","v":{"$error":"#VALUE!"}},{"$f":"+Q82","v":5.6800000000000006},null,null,null,null,null,"Y=",{"$f":"+(V82-V81)/(U82-U81)","v":0.12678908905341604},"*x",{"$f":"-X83*U81+V81","v":-7.3091798227872762E-2},"CRTANJE"]
[5,null,null,{"$f":"+D80","v":{"$error":"#VALUE!"}},{"$f":"+E80","v":{"$error":"#VALUE!"}},{"$f":"+F80","v":{"$error":"#VALUE!"}},{"$f":"+G80","v":0},5,null,null,{"$f":"+K80","v":{"$error":"#VALUE!"}},{"$f":"+L80","v":{"$error":"#VALUE!"}},5,null,null,{"$f":"+P80","v":{"$error":"#VALUE!"}},{"$f":"+Q80","v":{"$error":"#VALUE!"}},null,"Jedn pravca sloja 3",null,"Jedn pravca sloja 3 klizno",null,"Y=",{"$f":"+(T86-T85)/(S86-S85)","v":-3.4920769491747737E-2},"*x",{"$f":"-X84*S85+T85","v":1.2698415389834954},"Jedn pravca sloja 3 klizno",null,"sjecište 1/2 sidra sa vrhom 1. sloja"]
["  A=",{"$f":"IF(B77>B71,0,-IF(B84>B83,0,-0.5*((B80*C81-B81*C80)+(B81*C82-B82*C81)+(B82*C83-B83*C82)+(B83*C84-B84*C83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D77>D70,0,IF(D84>D83,0,-0.5*((D80*E81-D81*E80)+(D81*E82-D82*E81)+(D82*E83-D83*E82)+(D83*E84-D84*E83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F77>F71,0,IF(F84>F83,0,-0.5*((F80*G81-F81*G80)+(F81*G82-F82*G81)+(F82*G83-F83*G82)+(F83*G84-F84*G83))))","v":{"$error":"#VALUE!"}},"kN/m'","  A=",{"$f":"IF(I77>I71,0,-IF(I84>I83,0,-0.5*((I80*J81-I81*J80)+(I81*J82-I82*J81)+(I82*J83-I83*J82)+(I83*J84-I84*J83))))","v":{"$error":"#VALUE!"}},"kN/m'",0,"kN/m'","  A=",{"$f":"IF(N77>N71,0,-IF(N84>N83,0,-0.5*((N80*O81-N81*O80)+(N81*O82-N82*O81)+(N82*O83-N83*O82)+(N83*O84-N84*O83))))","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(P77>P70,0,IF(P84>P83,0,-0.5*((P80*Q81-P81*Q80)+(P81*Q82-P82*Q81)+(P82*Q83-P83*Q82)+(P83*Q84-P84*Q83))))","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+U18","v":2},{"$f":"+V18","v":1.2},{"$f":"+W100","v":2},0,"X=",{"$f":"+(-Z84+Z87)/(X84-X87)","v":1.1386903959986558},"sjecište ",null,{"$f":"+U85","v":2},{"$f":"+V85","v":0},"Y=",{"$f":"+X92","v":{"$error":"#VALUE!"}},"*x",{"$f":"+Z92","v":{"$error":"#VALUE!"}}]
["xt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(B80+B81)+(B81*C82-B82*C81)*(B81+B82)+(B82*C83-B83*C82)*(B82+B83)+(B83*C84-B84*C83)*(B83+B84))/6/B85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(D80+D81)+(D81*E82-D82*E81)*(D81+D82)+(D82*E83-D83*E82)*(D82+D83)+(D83*E84-D84*E83)*(D83+D84))/6/D85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(F80+F81)+(F81*G82-F82*G81)*(F81+F82)+(F82*G83-F83*G82)*(F82+F83)+(F83*G84-F84*G83)*(F83+F84))/6/F85)","v":{"$error":"#VALUE!"}},"kN/m'","xt=",{"$f":"IF(I85=0,0,((I80*J81-I81*J80)*(I80+I81)+(I81*J82-I82*J81)*(I81+I82)+(I82*J83-I83*J82)*(I82+I83)+(I83*J84-I84*J83)*(I83+I84))/6/I85)","v":{"$error":"#VALUE!"}},{"$f":"+O86","v":"kN/m'"},{"$f":"IF(K85=0,0,-((K80*L81-K81*L80)*(K80+K81)+(K81*L82-K82*L81)*(K81+K82)+(K82*L83-K83*L82)*(K82+K83)+(K83*L84-K84*L83)*(K83+K84))/6/K85)","v":0},"kN/m'","xt=",{"$f":"IF(N85=0,0,((N80*O81-N81*O80)*(N80+N81)+(N81*O82-N82*O81)*(N81+N82)+(N82*O83-N83*O82)*(N82+N83)+(N83*O84-N84*O83)*(N83+N84))/6/N85)","v":{"$error":"#VALUE!"}},"kN/m'",{"$f":"IF(P85=0,0,-((P80*Q81-P81*Q80)*(P80+P81)+(P81*Q82-P82*Q81)*(P81+P82)+(P82*Q83-P83*Q82)*(P82+P83)+(P83*Q84-P84*Q83)*(P83+P84))/6/P85)","v":{"$error":"#VALUE!"}},"kN/m'",null,{"$f":"+U19","v":-8},{"$f":"+V19","v":1.5492076949174773},-5,{"$f":"+V85+(U85-U86)*TAN((45+'Analiza i dimenzioniranje'!F14/2)*PI()/180)","v":9.9970360471948005},"Y=",{"$f":"+X84*X85+Z84","v":1.2300775941423594},3,null,{"$f":"+X85","v":1.1386903959986558},{"$f":"+X86","v":1.2300775941423594}]
["yt=",{"$f":"IF(B85=0,0,((B80*C81-B81*C80)*(C80+C81)+(B81*C82-B82*C81)*(C81+C82)+(B82*C83-B83*C82)*(C82+C83)+(B83*C84-B84*C83)*(C83+C84))/6/B85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(D85=0,0,-((D80*E81-D81*E80)*(E80+E81)+(D81*E82-D82*E81)*(E81+E82)+(D82*E83-D83*E82)*(E82+E83)+(D83*E84-D84*E83)*(E83+E84))/6/D85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(F85=0,0,-((F80*G81-F81*G80)*(G80+G81)+(F81*G82-F82*G81)*(G81+G82)+(F82*G83-F83*G82)*(G82+G83)+(F83*G84-F84*G83)*(G83+G84))/6/F85)","v":{"$error":"#VALUE!"}},"m","yt=",{"$f":"IF(I85=0,0,((I80*J81-I81*J80)*(J80+J81)+(I81*J82-I82*J81)*(J81+J82)+(I82*J83-I83*J82)*(J82+J83)+(I83*J84-I84*J83)*(J83+J84))/6/I85)","v":{"$error":"#VALUE!"}},{"$f":"+O87","v":"m"},{"$f":"IF(K85=0,0,-((K80*L81-K81*L80)*(L80+L81)+(K81*L82-K82*L81)*(L81+L82)+(K82*L83-K83*L82)*(L82+L83)+(K83*L84-K84*L83)*(L83+L84))/6/K85)","v":0},"m","yt=",{"$f":"IF(N85=0,0,((N80*O81-N81*O80)*(O80+O81)+(N81*O82-N82*O81)*(O81+O82)+(N82*O83-N83*O82)*(O82+O83)+(N83*O84-N84*O83)*(O83+O84))/6/N85)","v":{"$error":"#VALUE!"}},"m",{"$f":"IF(P85=0,0,-((P80*Q81-P81*Q80)*(Q80+Q81)+(P81*Q82-P82*Q81)*(Q81+Q82)+(P82*Q83-P83*Q82)*(Q82+Q83)+(P83*Q84-P84*Q83)*(Q83+Q84))/6/P85)","v":{"$error":"#VALUE!"}},"m",null,null,null,null,null,"Y=",{"$f":"+(V86-V85)/(U86-U85)","v":-1.4281480067421144},"*x",{"$f":"-X87*U85+V85","v":2.8562960134842288},"y=2       x=",{"$f":"+('Analiza i dimenzioniranje'!E52-'C XVIII-XIX'!Z87)/'C XVIII-XIX'!X87","v":1.1597509541483482}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(K85<0,0,K85)","v":0},null,null,null,null,{"$f":"+IF(P85<0,0,P85)","v":{"$error":"#VALUE!"}},null,null,"Jedn pravca sloja 2",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(T90-T89)/(S90-S89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X88*S89+T89","v":{"$error":"#VALUE!"}},"Jedn pravca sloja 2 klizno",null,"Jednadžba pravca sidra",null,"Jedn pravca sloja 2 klizno",null,"Y=",{"$f":"+(AD90-AD89)/(AC90-AC89)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-AH88*AC89+AD89","v":{"$error":"#VALUE!"}}]
["X koordinata položaja rezultante aktivnog tlaka na stražnjoj strani zida za  Ev1, Ev2 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U15","v":{"$error":"#VALUE!"}},{"$f":"+V15","v":4},{"$f":"+X85","v":1.1386903959986558},{"$f":"+X86","v":1.2300775941423594},"X=",{"$f":"+(-Z88+Z91)/(X88-X91)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U89","v":1.1386903959986558},{"$f":"+V89","v":1.2300775941423594},{"$f":"+U37","v":{"$error":"#VALUE!"}},{"$f":"+V37","v":5},{"$f":"+U89","v":1.1386903959986558},{"$f":"+V89","v":1.2300775941423594},"X=",{"$f":"+(-AJ88+AJ91)/(AH88-AH91)","v":{"$error":"#VALUE!"}},"sjecište"]
["Jednadžba pravca zida uz tlo",null,null,null,null,"Za Ev3 x=2",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U16","v":-8},{"$f":"+V16","v":{"$error":"#VALUE!"}},-5,{"$f":"+V89+(U89-U90)*TAN((45+'Analiza i dimenzioniranje'!E14/2)*PI()/180)","v":9.6792600705649363},"Y=",{"$f":"+X88*X89+Z88","v":{"$error":"#VALUE!"}},2,null,{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},{"$f":"+U38","v":{"$error":"#VALUE!"}},{"$f":"+V38","v":{"$error":"#VALUE!"}},{"$f":"+U90","v":-5},{"$f":"+V90","v":9.6792600705649363},"Y=",{"$f":"+AH88*AH89+AJ88","v":{"$error":"#VALUE!"}},2]
[null,"E1",null,"E2",null,"E3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(V90-V89)/(U90-U89)","v":-1.3763819204711731},"*x",{"$f":"-X91*U89+V89","v":2.79735046820907},null,null,null,null,null,null,"Y=",{"$f":"+(AF90-AF89)/(AE90-AE89)","v":-1.3763819204711731},"*x",{"$f":"-AH91*AE89+AF89","v":2.79735046820907}]
["x","y","x","y","x","y",null,null,null,null,null,null,null,null,null,null,null,null,"Jedn pravca sloja 1",null,null,null,"Y=",{"$f":"+(T95-T94)/(S95-S94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X92*S94+T94","v":{"$error":"#VALUE!"}},"Jedan pravca sloja 1 klizno",null,"Slobodna dionica ls>=",{"$f":"+SQRT((AC94-AC93)*(AC94-AC93)+(AD94-AD93)*(AD94-AD93))","v":{"$error":"#VALUE!"}}]
[{"$f":"+(B8-B4)*(B93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+B87","v":{"$error":"#VALUE!"}},{"$f":"+(B8-B4)*(D93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+D87","v":{"$error":"#VALUE!"}},2,{"$f":"+F87","v":{"$error":"#VALUE!"}},null,{"$f":"+(B8-B4)*(I93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+N87","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+(B8-B4)*(N93-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+I87","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+U7","v":{"$error":"#VALUE!"}},{"$f":"+V7","v":"A"},null,null,"X=",{"$f":"+(-Z92+Z95)/(X92-X95)","v":{"$error":"#VALUE!"}},"sjecište",null,{"$f":"+U94","v":{"$error":"#VALUE!"}},{"$f":"+V94","v":{"$error":"#VALUE!"}},{"$f":"+AC89","v":{"$error":"#VALUE!"}},{"$f":"+AD89","v":5}]
[null,null,null,null,"Sloj2",{"$f":"+(B8-B4)*(G94-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'C XVIII-XIX'!V15","v":4},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U8","v":{"$error":"#VALUE!"}},{"$f":"+V8","v":6},{"$f":"+X89","v":{"$error":"#VALUE!"}},{"$f":"+X90","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+X92*X93+Z92","v":{"$error":"#VALUE!"}},1,null,{"$f":"+X93","v":{"$error":"#VALUE!"}},{"$f":"+X94","v":{"$error":"#VALUE!"}},{"$f":"+AH89","v":{"$error":"#VALUE!"}},{"$f":"+AH90","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+(B8-B4)*(G95-C4)/(C8-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+K21","v":1.2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U10","v":-8},{"$f":"+V10","v":6.2644906473896782},-5,{"$f":"+V94+(U94-U95)*TAN((45+'Analiza i dimenzioniranje'!D14/2)*PI()/180)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+(V95-V94)/(U95-U94)","v":{"$error":"#VALUE!"}},"*x",{"$f":"-X95*U94+V94","v":{"$error":"#VALUE!"}},{"$f":"+(AB95-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+V9","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+(AB96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AI44","v":5.6800000000000006},{"$f":"+(AD96-Z95)/X95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AH44","v":5.36}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Masa unutar kliznog tijela - za potres",null,"POTRES",null,"x","y","x","y","x","y",null,null,null,null,"Masa za potres s prosjekom kontrafore i bez kontrafora"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},{"$f":"+(B9-B4)*(AD98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AH44","v":5.36},{"$f":"+(B9-B4)*(AF98-C4)/(C9-C4)+B4","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AI44","v":5.6800000000000006}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B2","v":2},0.12820515121628623,null,null,{"$f":"+(Z95-AB99)/(-X91)","v":{"$error":"#VALUE!"}},{"$f":"+AB98","v":1.2},{"$f":"IF('Analiza i dimenzioniranje'!AH44>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'C XVIII-XIX'!AC96,(Z91-AD99)/(-X91))","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!AH44","v":5.36},{"$f":"IF('Analiza i dimenzioniranje'!AI44>'Analiza i dimenzioniranje'!E17+'Analiza i dimenzioniranje'!F17,'C XVIII-XIX'!AA96,(Z91-AF99)/(-X91))","v":{"$error":"#VALUE!"}},{"$f":"+AF98","v":5.6800000000000006}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,1.2,"Potresna sila za stabilnost",null,"Klizno tijelo za potres za presjek III-III",null,"Klizno tijelo za potres za presjek  XVIII-XVIII",null,"Klizno tijelo za potres za presjek XIX-XIX",null,null,null,null,null,"Potresna sila za stabilnost "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.4000010999999999,1.2,{"$f":"+'C XVI-XVII'!Y101","v":1.75},{"$f":"+'C XVI-XVII'!Z101","v":9.6153895463470418E-2},{"$f":"+'C XVI-XVII'!AA101","v":0},{"$f":"+'C XVI-XVII'!AB101","v":0},{"$f":"+AC98","v":{"$error":"#VALUE!"}},{"$f":"+AD98","v":5.36},{"$f":"+AE98","v":{"$error":"#VALUE!"}},{"$f":"+AF98","v":5.6800000000000006},null,null,null,null,{"$f":"+'C III-V'!Y101","v":1.75},{"$f":"+'C III-V'!Z101","v":9.6153895463470418E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.14,{"$f":"+'C XVI-XVII'!Y102","v":0.97707863658009864},{"$f":"+'C XVI-XVII'!Z102","v":1.2},{"$f":"+Y102","v":0.97707863658009864},1.2,{"$f":"+AO132","v":-2.0117021920587819},{"$f":"+AP132","v":5.36},{"$f":"+AO133","v":-2.2362814274055753},{"$f":"+AP133","v":5.6800000000000006},null,null,null,null,{"$f":"+'C III-V'!Y102","v":0.97707863658009864},{"$f":"+'C III-V'!Z102","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.14,{"$f":"+'C XVI-XVII'!Y103","v":-1.0572404418349119},{"$f":"+'C XVI-XVII'!Z103","v":4},-1.0572404418349119,4,{"$f":"IF(AD103=AD102,AC102,+AA103)","v":-2.0117021920587819},{"$f":"IF($AH$105<=AD102,AD102,$AH$105)","v":5.36},{"$f":"IF(AF103=AF102,AE102,+AC103)","v":-2.2362814274055753},{"$f":"IF($AH$105<=AF102,AF102,$AH$105)","v":5.6800000000000006},null,null,null,null,{"$f":"+'C III-V'!Y103","v":-1.0572404418349119},{"$f":"+'C III-V'!Z103","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.44,{"$f":"+'C XVI-XVII'!Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!Z104","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"+AA104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},{"$f":"+AC104","v":{"$error":"#VALUE!"}},{"$f":"+Z104","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+'C III-V'!Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z104","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},3.44,{"$f":"+'C XVI-XVII'!Y105","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!Z105","v":6.2644906473896782},{"$error":"#VALUE!"},6.2644906473896782,{"$f":"+AA105","v":{"$error":"#VALUE!"}},{"$f":"IF(AA105=AC105,AB105,AB95)","v":{"$error":"#VALUE!"}},{"$f":"+AA105","v":{"$error":"#VALUE!"}},{"$f":"+IF(AA105=AE105,AB105,AB95)","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AM105","v":" H="},{"$f":"+'C III-V'!AH105","v":4},null,null,{"$f":"+'C III-V'!Y105","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z105","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},"A",{"$f":"+'C XVI-XVII'!Y106","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!Z106","v":6},{"$error":"#VALUE!"},6,{"$f":"+AE106","v":{"$error":"#VALUE!"}},{"$f":"+AF106","v":6},{"$f":"+AA106","v":{"$error":"#VALUE!"}},{"$f":"+AB106","v":6},null,null,null,null,{"$f":"+'C III-V'!Y106","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z106","v":6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},"A",{"$f":"+'C XVI-XVII'!Y107","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!Z107","v":6},{"$error":"#VALUE!"},6,{"$f":"+AE107","v":{"$error":"#VALUE!"}},{"$f":"+AF107","v":6},{"$f":"+AA107","v":{"$error":"#VALUE!"}},{"$f":"+AB107","v":6},null,null,null,null,{"$f":"+'C III-V'!Y107","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!Z107","v":6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+W107","v":{"$error":"#VALUE!"}},{"$f":"+X107","v":"A"},{"$f":"+'C XVI-XVII'!Y108","v":3.4000000999999997},{"$f":"+'C XVI-XVII'!Z108","v":1.2},3.4000000999999997,1.2,{"$f":"+AC109","v":{"$error":"#VALUE!"}},{"$f":"+AD109","v":5.36},{"$f":"+AE109","v":{"$error":"#VALUE!"}},{"$f":"+AF109","v":5.6800000000000006},null,null,null,null,{"$f":"+'C III-V'!Y108","v":3.4000000999999997},{"$f":"+'C III-V'!Z108","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+B11","v":4.2000010999999997},1.2,{"$f":"+'C XVI-XVII'!Y109","v":1.75},{"$f":"+'C XVI-XVII'!Z109","v":1.2},{"$f":"+AA102","v":0.97707863658009864},{"$f":"+AB102","v":1.2},{"$f":"+AC98","v":{"$error":"#VALUE!"}},{"$f":"+AD98","v":5.36},{"$f":"+AE101","v":{"$error":"#VALUE!"}},{"$f":"+AF101","v":5.6800000000000006},null,null,null,null,{"$f":"+'C III-V'!Y109","v":1.75},{"$f":"+'C III-V'!Z109","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2000010999999997,1.2,{"$f":"+'C XVI-XVII'!Y110","v":1.75},{"$f":"+'C XVI-XVII'!Z110","v":9.6153895463470418E-2},{"$f":"+'C XVI-XVII'!AA110","v":0},{"$f":"+'C XVI-XVII'!AB110","v":0},null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!Y110","v":1.75},{"$f":"+'C III-V'!Z110","v":9.6153895463470418E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2000010999999997,1.2,{"$f":"-0.5*((Y101*Z102-Y102*Z101)+(Y102*Z103-Y103*Z102)+(Y103*Z104-Y104*Z103)+(Y104*Z105-Y105*Z104)+(Y105*Z106-Y106*Z105)+(Y106*Z107-Y107*Z106)+(Y107*Z108-Y108*Z107)+(Y108*Z109-Y109*Z108)+(Y109*Z110-Y110*Z109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AA101*AB102-AA102*AB101)+(AA102*AB103-AA103*AB102)+(AA103*AB104-AA104*AB103)+(AA104*AB105-AA105*AB104)+(AA105*AB106-AA106*AB105)+(AA106*AB107-AA107*AB106)+(AA107*AB108-AA108*AB107)+(AA108*AB109-AA109*AB108)+(AA109*AB110-AA110*AB109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AC101*AD102-AC102*AD101)+(AC102*AD103-AC103*AD102)+(AC103*AD104-AC104*AD103)+(AC104*AD105-AC105*AD104)+(AC105*AD106-AC106*AD105)+(AC106*AD107-AC107*AD106)+(AC107*AD108-AC108*AD107)+(AC108*AD109-AC109*AD108)+(AC109*AD110-AC110*AD109))","v":{"$error":"#VALUE!"}},"m2",{"$f":"-0.5*((AE101*AF102-AE102*AF101)+(AE102*AF103-AE103*AF102)+(AE103*AF104-AE104*AF103)+(AE104*AF105-AE105*AF104)+(AE105*AF106-AE106*AF105)+(AE106*AF107-AE107*AF106)+(AE107*AF108-AE108*AF107)+(AE108*AF109-AE109*AF108)+(AE109*AF110-AE110*AF109))","v":{"$error":"#VALUE!"}},"m2",null,null,null,null,{"$f":"-0.5*((AK101*AL102-AK102*AL101)+(AK102*AL103-AK103*AL102)+(AK103*AL104-AK104*AL103)+(AK104*AL105-AK105*AL104)+(AK105*AL106-AK106*AL105)+(AK106*AL107-AK107*AL106)+(AK107*AL108-AK108*AL107)+(AK108*AL109-AK109*AL108)+(AK109*AL110-AK110*AL109))","v":{"$error":"#VALUE!"}},"m2","OK","prosječna površina temelja od temelja kontrafore duž čitavog zida"]
[null,null,null,null,null,{"$f":"+'C III-V'!F135:G135","v":0},null,{"$f":"+'C III-V'!H135:I135","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.9000021999999994,1.2,{"$f":"-((Y101*Z102-Y102*Z101)*(Y101+Y102)+(Y102*Z103-Y103*Z102)*(Y102+Y103)+(Y103*Z104-Y104*Z103)*(Y103+Y104)+(Y104*Z105-Y105*Z104)*(Y104+Y105)+(Y105*Z106-Y106*Z105)*(Y105+Y106)+(Y106*Z107-Y107*Z106)*(Y106+Y107)+(Y107*Z108-Y108*Z107)*(Y107+Y108)+(Y108*Z109-Y109*Z108)*(Y108+Y109)+(Y109*Z110-Y110*Z109)*(Y109+Y110))/6/Y111","v":{"$error":"#VALUE!"}},"m  ",{"$f":"-((AA101*AB102-AA102*AB101)*(AA101+AA102)+(AA102*AB103-AA103*AB102)*(AA102+AA103)+(AA103*AB104-AA104*AB103)*(AA103+AA104)+(AA104*AB105-AA105*AB104)*(AA104+AA105)+(AA105*AB106-AA106*AB105)*(AA105+AA106)+(AA106*AB107-AA107*AB106)*(AA106+AA107)+(AA107*AB108-AA108*AB107)*(AA107+AA108)+(AA108*AB109-AA109*AB108)*(AA108+AA109)+(AA109*AB110-AA110*AB109)*(AA109+AA110))/6/AA111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AC101*AD102-AC102*AD101)*(AC101+AC102)+(AC102*AD103-AC103*AD102)*(AC102+AC103)+(AC103*AD104-AC104*AD103)*(AC103+AC104)+(AC104*AD105-AC105*AD104)*(AC104+AC105)+(AC105*AD106-AC106*AD105)*(AC105+AC106)+(AC106*AD107-AC107*AD106)*(AC106+AC107)+(AC107*AD108-AC108*AD107)*(AC107+AC108)+(AC108*AD109-AC109*AD108)*(AC108+AC109)+(AC109*AD110-AC110*AD109)*(AC109+AC110))/6/AC111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AE101*AF102-AE102*AF101)*(AE101+AE102)+(AE102*AF103-AE103*AF102)*(AE102+AE103)+(AE103*AF104-AE104*AF103)*(AE103+AE104)+(AE104*AF105-AE105*AF104)*(AE104+AE105)+(AE105*AF106-AE106*AF105)*(AE105+AE106)+(AE106*AF107-AE107*AF106)*(AE106+AE107)+(AE107*AF108-AE108*AF107)*(AE107+AE108)+(AE108*AF109-AE109*AF108)*(AE108+AE109)+(AE109*AF110-AE110*AF109)*(AE109+AE110))/6/AE111","v":{"$error":"#VALUE!"}},"m",null,null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AK101+AK102)+(AK102*AL103-AK103*AL102)*(AK102+AK103)+(AK103*AL104-AK104*AL103)*(AK103+AK104)+(AK104*AL105-AK105*AL104)*(AK104+AK105)+(AK105*AL106-AK106*AL105)*(AK105+AK106)+(AK106*AL107-AK107*AL106)*(AK106+AK107)+(AK107*AL108-AK108*AL107)*(AK107+AK108)+(AK108*AL109-AK109*AL108)*(AK108+AK109)+(AK109*AL110-AK110*AL109)*(AK109+AK110))/6/AK111","v":{"$error":"#VALUE!"}},"m  "]
[null,null,null,null,null,{"$f":"+'C III-V'!F136:G136","v":"Visina presjeka"},{"$f":"+'C III-V'!G136:H136","v":0},{"$f":"+'C III-V'!H136:I136","v":"Intezitet"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.9000021999999994,0.5,{"$f":"-((Y101*Z102-Y102*Z101)*(Z101+Z102)+(Y102*Z103-Y103*Z102)*(Z102+Z103)+(Y103*Z104-Y104*Z103)*(Z103+Z104)+(Y104*Z105-Y105*Z104)*(Z104+Z105)+(Y105*Z106-Y106*Z105)*(Z105+Z106)+(Y106*Z107-Y107*Z106)*(Z106+Z107)+(Y107*Z108-Y108*Z107)*(Z107+Z108)+(Y108*Z109-Y109*Z108)*(Z108+Z109)+(Y109*Z110-Y110*Z109)*(Z109+Z110))/6/Y111","v":{"$error":"#VALUE!"}},"m    ",{"$f":"-((AA101*AB102-AA102*AB101)*(AB101+AB102)+(AA102*AB103-AA103*AB102)*(AB102+AB103)+(AA103*AB104-AA104*AB103)*(AB103+AB104)+(AA104*AB105-AA105*AB104)*(AB104+AB105)+(AA105*AB106-AA106*AB105)*(AB105+AB106)+(AA106*AB107-AA107*AB106)*(AB106+AB107)+(AA107*AB108-AA108*AB107)*(AB107+AB108)+(AA108*AB109-AA109*AB108)*(AB108+AB109)+(AA109*AB110-AA110*AB109)*(AB109+AB110))/6/AA111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AC101*AD102-AC102*AD101)*(AD101+AD102)+(AC102*AD103-AC103*AD102)*(AD102+AD103)+(AC103*AD104-AC104*AD103)*(AD103+AD104)+(AC104*AD105-AC105*AD104)*(AD104+AD105)+(AC105*AD106-AC106*AD105)*(AD105+AD106)+(AC106*AD107-AC107*AD106)*(AD106+AD107)+(AC107*AD108-AC108*AD107)*(AD107+AD108)+(AC108*AD109-AC109*AD108)*(AD108+AD109)+(AC109*AD110-AC110*AD109)*(AD109+AD110))/6/AC111","v":{"$error":"#VALUE!"}},"m",{"$f":"-((AE101*AF102-AE102*AF101)*(AF101+AF102)+(AE102*AF103-AE103*AF102)*(AF102+AF103)+(AE103*AF104-AE104*AF103)*(AF103+AF104)+(AE104*AF105-AE105*AF104)*(AF104+AF105)+(AE105*AF106-AE106*AF105)*(AF105+AF106)+(AE106*AF107-AE107*AF106)*(AF106+AF107)+(AE107*AF108-AE108*AF107)*(AF107+AF108)+(AE108*AF109-AE109*AF108)*(AF108+AF109)+(AE109*AF110-AE110*AF109)*(AF109+AF110))/6/AE111","v":{"$error":"#VALUE!"}},"m",null,null,null,null,{"$f":"-((AK101*AL102-AK102*AL101)*(AL101+AL102)+(AK102*AL103-AK103*AL102)*(AL102+AL103)+(AK103*AL104-AK104*AL103)*(AL103+AL104)+(AK104*AL105-AK105*AL104)*(AL104+AL105)+(AK105*AL106-AK106*AL105)*(AL105+AL106)+(AK106*AL107-AK107*AL106)*(AL106+AL107)+(AK107*AL108-AK108*AL107)*(AL107+AL108)+(AK108*AL109-AK109*AL108)*(AL108+AL109)+(AK109*AL110-AK110*AL109)*(AL109+AL110))/6/AK111","v":{"$error":"#VALUE!"}},"m    ",null,{"$f":"+'C III-V'!AN113:AN114","v":-0.25},{"$f":"IF('Analiza i dimenzioniranje'!D84=\"\",0,'Analiza i dimenzioniranje'!D83+'C III-V'!AN113)","v":0.75}]
[null,null,null,null,null,{"$f":"+'C III-V'!F137:G137","v":"III"},{"$f":"+'C III-V'!G137:H137","v":1.2},{"$f":"+'C III-V'!H137:I137","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,0.12820515121628623,{"$f":"+Y111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AA111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AC111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",{"$f":"+AE111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN",null,null,null,null,{"$f":"+AK111*'Analiza i dimenzioniranje'!$H$16*'Analiza i dimenzioniranje'!$E$44*'Analiza i dimenzioniranje'!$E$46/'Analiza i dimenzioniranje'!$E$45","v":{"$error":"#VALUE!"}},"kN"]
[null,null,null,null,null,{"$f":"+'C III-V'!F138:G138","v":"VI"},{"$f":"+'C III-V'!G138:H138","v":1.52},{"$f":"+'C III-V'!H138:I138","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(W99:W114)","v":{"$error":"#VALUE!"}},{"$f":"SUM(X99:X114)","v":21.11641030243257},null,null,null,null,null,null,null,null,null,null,"Teren  kosina",null,"Klizna ploha"]
[null,null,null,null,null,{"$f":"+'C III-V'!F139:G139","v":"VII"},{"$f":"+'C III-V'!G139:H139","v":1.84},{"$f":"+'C III-V'!H139:I139","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C XVI-XVII'!AI116","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!AJ116","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!AK116","v":1.75},{"$f":"+'C XVI-XVII'!AL116","v":-1.1133852506716102},null,"sjecišta ravnine presjeka na kliznoj plohi",null,null,null,null,null,null,"Omjer površine"]
[null,null,null,null,null,{"$f":"+'C III-V'!F140:G140","v":"VIII"},{"$f":"+'C III-V'!G140:H140","v":2.16},{"$f":"+'C III-V'!H140:I140","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koord. Težište mase  za h22",null,null,null,null,null,null,null,null,null,{"$f":"+'C XVI-XVII'!AI117","v":6.2644906473896782},{"$f":"+'C XVI-XVII'!AJ117","v":6},{"$f":"+'C XVI-XVII'!AK117","v":0},{"$f":"+'C XVI-XVII'!AL117","v":4.08},null,{"$f":"+'C III-V'!AA100","v":"oznaka"},{"$f":"+'C III-V'!AB100","v":"X"},{"$f":"+'C III-V'!AC100","v":"Y"},null,null,null,"        sa kontraforama: bez kontrafora",null,null,"Potresna sila-prosječna"]
[null,null,null,null,null,{"$f":"+'C III-V'!F141:G141","v":"IX"},{"$f":"+'C III-V'!G141:H141","v":2.48},{"$f":"+'C III-V'!H141:I141","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(AA102-AA103)/3","v":0.67810635947167019},{"$f":"+Z103*0.666666666666667","v":2.6666666666666679},null,null,null,null,null,null,null,null,{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!D116,AI117)","v":-5},{"$f":"+IF('Analiza i dimenzioniranje'!E24>0,'Unos podataka'!E116,'C III-V'!AJ117)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+'C III-V'!AA101","v":"Y=0"},{"$f":"+'C III-V'!AB101","v":1.75},{"$f":"+'C III-V'!AC101","v":0},{"$f":"+'C XVI-XVII'!AP118","v":0},null,null,null,null,null,null,null,"Potresna sila","F","G"]
[null,null,null,null,null,{"$f":"+'C III-V'!F142:G142","v":"X"},{"$f":"+'C III-V'!G142:H142","v":2.8},{"$f":"+'C III-V'!H142:I142","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"(AJ117-AI117)/(AJ116-AI116)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AI119*AI116+AI117","v":{"$error":"#VALUE!"}}," ",null,{"$f":"+'C III-V'!AA102","v":"PIII"},{"$f":"+'C III-V'!AB102","v":0.97707863658009864},{"$f":"+'C III-V'!AC102","v":1.2},{"$f":"+'C XVI-XVII'!AP119","v":0},null,null,null,"Ukupna duljina zida",null,{"$f":"+Kontrafore!E13","v":12},"m",{"$f":"+AW119","v":12},{"$f":"+Y111","v":{"$error":"#VALUE!"}},{"$f":"+Y114","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F143:G143","v":"XI"},{"$f":"+'C III-V'!G143:H143","v":3.14},{"$f":"+'C III-V'!H143:I143","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"-(AL117-AK117)/(AK116-AL116)","v":-1.4248868534344206},"*x    +",{"$f":"-(AK116*AI120-AK117)","v":2.4935519935102359}," ",null,{"$f":"+'C III-V'!AA103","v":"PVI"},{"$f":"+'C III-V'!AB103","v":0.68324863210273346},{"$f":"+'C III-V'!AC103","v":1.52},{"$f":"+'C XVI-XVII'!AP120","v":0},null,null,null,"ukupna duljina kontrafora",null,{"$f":"+Kontrafore!E5*Kontrafore!E4","v":3},"m",{"$f":"+AW120","v":3},{"$f":"+AZ119-AZ121","v":{"$error":"#VALUE!"}},{"$f":"IF(AW120=AW119,0,BA119-BA121)","v":{"$error":"#VALUE!"}}]
["Presjek kroz zid I",null,"Presjek kroz zid II",null,null,{"$f":"+'C III-V'!F144:G144","v":"XIII"},{"$f":"+'C III-V'!G144:H144","v":3.44},{"$f":"+'C III-V'!H144:I144","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AK120-AK119)/(AI119-AI120)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AI120*AI121+AK120","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!AA104","v":"PVII"},{"$f":"+'C III-V'!AB104","v":0.45866939675594048},{"$f":"+'C III-V'!AC104","v":1.84},{"$f":"+'C XVI-XVII'!AP121","v":0},null,null,null,"ukupna duljina bez kontrafora",null,{"$f":"+AW119-AW120","v":9},"m",{"$f":"+AY119-AY120","v":9},{"$f":"+AG111","v":0},{"$f":"+IF(AY121=0,0,AG114)","v":0}]
["x","y","x","y",null,{"$f":"+'C III-V'!F145:G145","v":"XIII"},{"$f":"+'C III-V'!G145:H145","v":3.76},{"$f":"+'C III-V'!H145:I145","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA105","v":"PVIII"},{"$f":"+'C III-V'!AB105","v":0.23409016140914748},{"$f":"+'C III-V'!AC105","v":2.16},{"$f":"+'C XVI-XVII'!AP122","v":0},null,null,null,"površina s kontraforama",null,{"$f":"+AW120/AW119","v":0.25}]
[0,{"$f":"+'Analiza i dimenzioniranje'!AI44","v":5.6800000000000006},{"$f":"+A123","v":0},{"$f":"+'Analiza i dimenzioniranje'!AH44","v":5.36},null,{"$f":"+'C III-V'!F146:G146","v":"XIV"},{"$f":"+'C III-V'!G146:H146","v":4.08},{"$f":"+'C III-V'!H146:I146","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($AK$119-$AK$123)/AI119","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AK121","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!AA106","v":"PIX"},{"$f":"+'C III-V'!AB106","v":9.5109260623546556E-3},{"$f":"+'C III-V'!AC106","v":2.48},{"$f":"+'C XVI-XVII'!AP123","v":0},null,null,null,"površina bez kontrafora",null,{"$f":"+AW121/AW119","v":0.75}]
[{"$f":"+F83","v":{"$error":"#VALUE!"}},{"$f":"+B123","v":5.6800000000000006},{"$f":"+A124","v":{"$error":"#VALUE!"}},{"$f":"+D123","v":5.36},null,{"$f":"+'C III-V'!F147:G147","v":"XV"},{"$f":"+'C III-V'!G147:H147","v":4.4000000000000004},{"$f":"+'C III-V'!H147:I147","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-($AK$119-$AK$123)/AI120","v":{"$error":"#VALUE!"}},null,6.46,null,null,{"$f":"+'C III-V'!AA107","v":"PX"},{"$f":"+'C III-V'!AB107","v":-0.21506830928443818},{"$f":"+'C III-V'!AC107","v":2.8},{"$f":"+'C XVI-XVII'!AP124","v":0},null,null,null,null,null,"odnos",null,{"$f":"-(AY120/AY119)*'Analiza i dimenzioniranje'!D83","v":-0.25}]
[null,null,null,null,null,{"$f":"+'C III-V'!F148:G148","v":"XVI"},{"$f":"+'C III-V'!G148:H148","v":4.72},{"$f":"+'C III-V'!H148:I148","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA108","v":"PXI"},{"$f":"+'C III-V'!AB108","v":-0.45368374684040591},{"$f":"+'C III-V'!AC108","v":3.14},{"$f":"+'C XVI-XVII'!AP125","v":0},null,null,null,null,"krak",{"$f":"+Y113","v":{"$error":"#VALUE!"}},{"$f":"+BA119","v":{"$error":"#VALUE!"}},{"$f":"+BA120*AW122","v":{"$error":"#VALUE!"}},null,{"$f":"+BA119-AY126","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F149:G149","v":"XVII"},{"$f":"+'C III-V'!G149:H149","v":5.04},{"$f":"+'C III-V'!H149:I149","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"-($AK$120-AK126)/$AI$120","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+AK121","v":{"$error":"#VALUE!"}},null,null,{"$f":"+'C III-V'!AA109","v":"PXII"},{"$f":"+'C III-V'!AB109","v":-0.66422677997802415},{"$f":"+'C III-V'!AC109","v":3.44},{"$f":"+'C XVI-XVII'!AP126","v":0},null,null,null,null,null,{"$f":"+AG113","v":0},{"$f":"+BA121","v":0},{"$f":"+BA120*AW123","v":{"$error":"#VALUE!"}},null,{"$f":"+BA121+AY125","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"+'C III-V'!F150:G150","v":"XVIII"},{"$f":"+'C III-V'!G150:H150","v":5.36},{"$f":"+'C III-V'!H150:I150","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-1.1976024639266576,null,4.2,null,null,{"$f":"+'C III-V'!AA110","v":"PXIII"},{"$f":"+'C III-V'!AB110","v":-0.88880601532481696},{"$f":"+'C III-V'!AC110","v":3.76},{"$f":"+'C XVI-XVII'!AP127","v":0},null,null,null,null,null,null,null,"Prosječna masa za potres:",null,{"$f":"IF(IF(AW130=AX130,Y114,+BA126)=0,BA125,IF(AW130=AX130,Y114,+BA126))","v":{"$error":"#VALUE!"}},"kn"]
[null,null,null,null,null,{"$f":"+'C III-V'!F151:G151","v":"XIX"},{"$f":"+'C III-V'!G151:H151","v":5.6800000000000006},{"$f":"+'C III-V'!H151:I151","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.90782786744952648,null,1.2,null,null,{"$f":"+'C III-V'!AA111","v":"PXIV"},{"$f":"+'C III-V'!AB111","v":-1.1133852506716102},{"$f":"+'C III-V'!AC111","v":4.08},{"$f":"+'C XVI-XVII'!AP128","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.6464828732122183,null,{"$f":"+AI117","v":6.2644906473896782},null,null,{"$f":"+'C III-V'!AA112","v":"PXV"},{"$f":"+'C III-V'!AB112","v":-1.3379644860184032},{"$f":"+'C III-V'!AC112","v":4.4000000000000004},{"$f":"+'C XVI-XVII'!AP129","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.0117021920587819,null,{"$f":"+AD101","v":5.36},null,null,{"$f":"+'C III-V'!AA113","v":"PXVI"},{"$f":"+'C III-V'!AB113","v":-1.5625437213651958},{"$f":"+'C III-V'!AC113","v":4.72},{"$f":"+'C XVI-XVII'!AP130","v":0},null,null,null,null,"x=",{"$f":"+AG113","v":0},{"$f":"+Y113","v":{"$error":"#VALUE!"}},null,{"$f":"+AI109","v":0},{"$f":"+AI106","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.2362814274055753,null,{"$f":"+AF109","v":5.6800000000000006},null,null,{"$f":"+'C III-V'!AA114","v":"PXVII"},{"$f":"+'C III-V'!AB114","v":-1.7871229567119888},{"$f":"+'C III-V'!AC114","v":5.04},{"$f":"+'C XVI-XVII'!AP131","v":0},null,null,null,null,"Y=",{"$f":"+AG114","v":0},{"$f":"+Y114","v":{"$error":"#VALUE!"}},null,{"$f":"+AJ109","v":0},{"$f":"+AJ106","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA115","v":"PXVIII"},{"$f":"+'C III-V'!AB115","v":-2.0117021920587819},{"$f":"+'C III-V'!AC115","v":5.36},{"$f":"+'C XVI-XVII'!AP132","v":0},null,null,null,null,"Y=",{"$f":"(AW131-AX131)/(AW130-AX130)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-AW132*AX130+AX131","v":{"$error":"#VALUE!"}},{"$f":"(AZ131-BA131)/(AZ130-BA130)","v":{"$error":"#DIV/0!"}},"*x    +",{"$f":"-AZ132*BA130+BA131","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA116","v":"PXIX"},{"$f":"+'C III-V'!AB116","v":-2.2362814274055753},{"$f":"+'C III-V'!AC116","v":5.6800000000000006},{"$f":"+'C XVI-XVII'!AP133","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA117","v":"PXX"},{"$f":"+'C III-V'!AB117","v":0},{"$f":"+'C III-V'!AC117","v":6.0000000000000009},{"$f":"+'C XVI-XVII'!AP134","v":0},null,null,null,null,"x=",{"$f":"+AK113","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","Y",null,null,null,"teren",{"$f":"+Y104","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!AC118","v":{"$error":"#VALUE!"}},null,null,null,null,null,"xstv=",{"$f":"+AW134-X113","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C XVI-XVII'!AI136","v":{"$error":"#VALUE!"}},{"$f":"+'C XVI-XVII'!AJ136","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,"            Masa da se dobije prosječni potres iz čelije AT125=",null,null,null,null,{"$f":"+BA125","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+'C XII-XIII'!AC138","v":{"$error":"#VALUE!"}},{"$f":"+AD102","v":5.36},{"$f":"+AF102","v":5.6800000000000006},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"razlika¸površina",{"$f":"+Y111-AI111","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AE144-AC138)/(-AC144)","v":{"$error":"#VALUE!"}},{"$f":"IF(AD138<AC138,(AE151-AD138)/(-AC151),(AE156-AD138)/(-AC156))","v":{"$error":"#VALUE!"}},{"$f":"IF(AE138<AC138,(AE151-AE138)/(-AC151),(AE156-AE138)/(-AC156))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"duljina segmenta",{"$f":"++AJ105","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina III. sloja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"okomito na kliz. Plohu",null,{"$f":"+AW143/AW139","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"d=","dodatak",{"$f":"+AW140/COS(AW142*PI()/180)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA153","v":2},{"$f":"+'C III-V'!AB153","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"          kut nagiba klizne plohe za potres   a= ",null,{"$f":"ATAN((-Y104+Y101)/(Z104-Z101))*180/PI()","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA154","v":-5},{"$f":"+'C III-V'!AB154","v":9.9970360471948005},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dodatna površina",{"$f":"+AW144/'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AD143-AD142)/(AC143-AC142)","v":-1.4281480067421144},"*x      +",{"$f":"-AC144*AC142+AD142","v":2.8562960134842288},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"G=",{"$f":"+AY126","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+(AE144-AD146)/(-AC144)","v":1.1597509541483482}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+Z102","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina II. sloja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA148","v":-1.0572404418349119},{"$f":"+'C III-V'!AB148","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+'C III-V'!AA149","v":0.97707863658009864},{"$f":"+'C III-V'!AB149","v":1.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AD150-AD149)/(AC150-AC149)","v":-1.3763819204711734},"*x      +",{"$f":"-AC151*AC149+AD149","v":2.5448333702674724}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jednadžba aktivnog klina I. sloja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x","y"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koordinate na sjecištu s terenom",null,null,{"$f":"+'C III-V'!AA144","v":-2.5846586698092704},{"$f":"+'C III-V'!AB144","v":6.2644906473896782}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"koordinate na sjecištu slojeva",null,null,{"$f":"+'C III-V'!AA143","v":-1.0572404418349119},{"$f":"+'C III-V'!AB143","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y=",{"$f":"+(AD155-AD154)/(AC155-AC154)","v":-1.4825609685127401},"*x      +",{"$f":"-AC156*AC154+AD154","v":2.4325765866023956}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rub dna konzole uz aktivni klin",null,null,{"$f":"+B6","v":{"$error":"#VALUE!"}},{"$f":"+C6","v":3.14}]

{"sheet":"HT III-XX","index":47,"n_rows":689,"n_cols":59,"rows_kept":689,"cut":false,"hidden":true,"merged":[[655,29,655,30],[615,23,615,24],[615,25,615,26],[615,27,615,28],[615,29,615,30],[615,0,615,1],[615,5,615,6],[615,7,615,8],[615,9,615,10],[615,11,615,12],[575,33,575,34],[575,35,575,36],[575,21,575,22],[575,23,575,24],[575,25,575,26],[655,31,655,32],[655,33,655,34],[655,35,655,36],[686,0,686,1],[615,33,615,34],[615,35,615,36],[655,0,655,1],[655,5,655,6],[655,7,655,8],[655,9,655,10],[655,11,655,12],[655,13,655,14],[655,15,655,16],[655,17,655,18],[655,19,655,20],[655,21,655,22],[655,23,655,24],[655,25,655,26],[655,27,655,28],[615,31,615,32],[615,13,615,14],[615,15,615,16],[615,17,615,18],[615,19,615,20],[615,21,615,22],[575,13,575,14],[575,15,575,16],[575,17,575,18],[575,19,575,20],[575,27,575,28],[575,29,575,30],[575,31,575,32],[495,31,495,32],[495,33,495,34],[495,35,495,36],[535,0,535,1],[535,5,535,6],[535,7,535,8],[535,9,535,10],[535,11,535,12],[535,13,535,14],[535,15,535,16],[535,17,535,18],[535,19,535,20],[535,21,535,22],[535,23,535,24],[535,25,535,26],[535,27,535,28],[535,29,535,30],[535,31,535,32],[535,33,535,34],[535,35,535,36],[495,13,495,14],[495,15,495,16],[495,17,495,18],[495,19,495,20],[495,21,495,22],[495,23,495,24],[495,25,495,26],[495,27,495,28],[495,29,495,30],[455,0,455,1],[455,5,455,6],[455,7,455,8],[455,9,455,10],[455,11,455,12],[575,0,575,1],[575,5,575,6],[575,7,575,8],[575,9,575,10],[575,11,575,12],[495,0,495,1],[495,5,495,6],[495,7,495,8],[495,9,495,10],[495,11,495,12],[375,29,375,30],[375,31,375,32],[375,33,375,34],[375,35,375,36],[455,29,455,30],[455,31,455,32],[455,13,455,14],[455,15,455,16],[455,17,455,18],[455,19,455,20],[455,21,455,22],[455,33,455,34],[455,35,455,36],[455,23,455,24],[455,25,455,26],[455,27,455,28],[415,13,415,14],[415,15,415,16],[415,17,415,18],[415,19,415,20],[415,27,415,28],[415,29,415,30],[415,31,415,32],[415,33,415,34],[415,35,415,36],[415,21,415,22],[415,23,415,24],[415,25,415,26],[335,31,335,32],[335,33,335,34],[335,35,335,36],[375,0,375,1],[375,5,375,6],[375,7,375,8],[375,9,375,10],[375,11,375,12],[375,13,375,14],[375,15,375,16],[375,17,375,18],[375,19,375,20],[375,21,375,22],[375,23,375,24],[375,25,375,26],[375,27,375,28],[415,0,415,1],[415,5,415,6],[415,7,415,8],[415,9,415,10],[415,11,415,12],[295,33,295,34],[295,35,295,36],[335,0,335,1],[335,5,335,6],[335,7,335,8],[335,9,335,10],[335,11,335,12],[335,13,335,14],[335,15,335,16],[335,17,335,18],[335,19,335,20],[335,21,335,22],[335,23,335,24],[335,25,335,26],[335,27,335,28],[335,29,335,30],[295,23,295,24],[295,25,295,26],[295,27,295,28],[295,29,295,30],[295,31,295,32],[295,13,295,14],[295,15,295,16],[295,17,295,18],[295,19,295,20],[295,21,295,22],[295,0,295,1],[295,5,295,6],[295,7,295,8],[295,9,295,10],[295,11,295,12],[256,29,256,30],[256,31,256,32],[175,35,175,36],[256,33,256,34],[256,35,256,36],[215,33,215,34],[215,35,215,36],[256,0,256,1],[256,5,256,6],[256,7,256,8],[256,9,256,10],[256,11,256,12],[256,13,256,14],[256,15,256,16],[256,17,256,18],[256,19,256,20],[256,21,256,22],[256,23,256,24],[256,25,256,26],[256,27,256,28],[215,21,215,22],[215,23,215,24],[215,25,215,26],[215,27,215,28],[215,29,215,30],[215,31,215,32],[175,31,175,32],[215,0,215,1],[215,5,215,6],[215,7,215,8],[215,9,215,10],[215,11,215,12],[215,13,215,14],[215,15,215,16],[215,17,215,18],[215,19,215,20],[135,31,135,32],[135,33,135,34],[135,35,135,36],[175,0,175,1],[175,5,175,6],[175,7,175,8],[175,9,175,10],[175,11,175,12],[175,13,175,14],[175,15,175,16],[175,17,175,18],[175,19,175,20],[175,21,175,22],[175,23,175,24],[175,25,175,26],[135,21,135,22],[135,23,135,24],[135,25,135,26],[135,27,135,28],[135,29,135,30],[135,19,135,20],[175,33,175,34],[175,27,175,28],[175,29,175,30],[17,13,17,14],[17,15,17,16],[17,17,17,18],[17,5,17,6],[135,0,135,1],[135,5,135,6],[135,7,135,8],[135,9,135,10],[135,11,135,12],[135,13,135,14],[135,15,135,16],[135,17,135,18],[54,7,54,9],[94,7,94,9],[17,7,17,8],[17,9,17,10],[17,11,17,12],[97,5,97,6],[97,7,97,8],[97,9,97,10],[97,11,97,12],[97,13,97,14],[57,5,57,6],[57,7,57,8],[57,9,57,10],[57,11,57,12],[57,13,57,14],[57,15,57,16],[57,17,57,18],[57,19,57,20],[57,21,57,22],[97,15,97,16],[97,17,97,18],[97,19,97,20],[97,21,97,22],[97,23,97,24],[97,29,97,30],[97,31,97,32],[97,33,97,34],[17,35,17,36],[57,23,57,24],[57,25,57,26],[57,27,57,28],[17,19,17,20],[17,21,17,22],[17,23,17,24],[97,35,97,36],[57,29,57,30],[57,31,57,32],[57,33,57,34],[57,35,57,36],[97,25,97,26],[97,27,97,28],[17,29,17,30],[17,31,17,32],[17,33,17,34],[17,25,17,26],[17,27,17,28]]}
["UPUTE ZA RAD:",null,"Ovaj program omogućava proračun horizontalnih pritisaka na zid za:"]
[]
["  - prometno opterećenje dužine zida i projektne širine"]
[" - točkasto opterećenje ","dimenzija temelja 1m x 1m"]
[" - linijsko opterećenje dužine zida i širine 1m"]
[" - temelj određenih dimenzija simetričan na obje strane promatrane vertikale"]
[]
[null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Prema Terzaghiu"]
[null,"PROMETNO OPTEREĆENJE",null,null,null,null," (TERZAGHY)"]
["Dimenzije prometne površine zadaju se u Formi 2. Djelovanja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veza je između vertikala od V do AH   sa ulaznim podacima  E12 do G17"]
[null,null,"KONTINUIRANO OPTEREĆENJE","P =",{"$f":"+'Analiza i dimenzioniranje'!E$24","v":10},"kN/m2",null,null,null,null,"Horizontalni pritisci - samo na zid bez temeja"]
[null,null," visina zida iznad  temelja","H =",{"$f":"+'Analiza i dimenzioniranje'!E$47+0.00001-'Analiza i dimenzioniranje'!E$52","v":{"$error":"#VALUE!"}},"m",{"$f":"+E16","v":6}]
[null,null,"visina opterećenja iznad vrha zida","h =",{"$f":"+'C III-V'!X$14-'Analiza i dimenzioniranje'!E$47","v":{"$error":"#VALUE!"}},"m",{"$f":"SQRT(E16^2+E15^2)","v":7.5000006000000425}]
[null,null,"  širina opterećenja","b =",{"$f":"+'Analiza i dimenzioniranje'!E$25","v":3},"m",{"$f":"E15+E14","v":7.5000009999999993}]
[null,null,"udaljenost opterećenja od iskopa","D =",{"$f":"+'Analiza i dimenzioniranje'!K29","v":4.5000009999999993},"m"]
[null,null,"1/2 dužine temelja","L/2=a=",{"$f":"+'Analiza i dimenzioniranje'!E$49/2","v":6},"m",{"$f":"SQRT(G12^2+G14^2)","v":9.604687137018102}]
[null,null,null,null,null,{"$f":"+ROUND('Analiza i dimenzioniranje'!$E$52,2)","v":1.2},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND('Analiza i dimenzioniranje'!$U$53,2)","v":1.52},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND('Analiza i dimenzioniranje'!$U$54,2)","v":1.84},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND('Analiza i dimenzioniranje'!$U$55,2)","v":2.16},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$56,2)","v":2.48},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$57,2)","v":2.8},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$58,2)","v":3.14},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$59,2)","v":3.44},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$60,2)","v":3.76},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$61,2)","v":4.08},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$62,2)","v":4.4000000000000004},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$63,2)","v":4.72},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$64,2)","v":5.04},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$65,2)","v":5.36},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$66,2)","v":5.68},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$67,2)","v":6},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},null,null,"Izračun pritiska na zid od vertikalnog opterećenja"]
[null,null,null,null,null,"Presjek III -III-0",null,"Presjek VI-VI",null,"Presjek VII-VII",null,"Presjek VIII-VI-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"PresjekVIV-XIV",null,"Presjek XV-XV",null,"Presjek XVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX"]
[null,null,null,null,{"$f":"+('Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)/15","v":0.32},"(sb2-sb1)*2",{"$f":"+G17","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+I17","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+K17","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+M17","v":{"$error":"#VALUE!"}},"sb1-sb2",{"$f":"+O17","v":{"$error":"#VALUE!"}},"sb1-sb2",{"$f":"+Q17","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+S17","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+U17","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+W17","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+Y17","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+AA17","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+AC17","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+AE17","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+AG17","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+AI17","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+AK17","v":{"$error":"#VALUE!"}},null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
[null,null,null,null,{"$f":"+G19-G20","v":{"$error":"#VALUE!"}},{"$f":"+AX20","v":0},{"$f":"+G19","v":{"$error":"#VALUE!"}},0,{"$f":"+I19","v":{"$error":"#VALUE!"}},{"$f":"+F20","v":0},{"$f":"+I20","v":{"$error":"#VALUE!"}},{"$f":"+F20","v":0},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$f":"+L20","v":0},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$f":"+Y20","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$f":"+AE20","v":{"$error":"#VALUE!"}},null,{"$f":"+E20","v":{"$error":"#VALUE!"}},{"$f":"$E$15^2+AM20^2","v":{"$error":"#VALUE!"}},{"$f":"$G14^2+AM20^2","v":{"$error":"#VALUE!"}},{"$f":"$G$16^2+AM20^2","v":{"$error":"#VALUE!"}},0,null,{"$f":"+AM20","v":{"$error":"#VALUE!"}},{"$f":"$E$16^2+AS20^2","v":{"$error":"#VALUE!"}},{"$f":"$E$15^2+AS20^2","v":{"$error":"#VALUE!"}},{"$f":"$G$13^2+AS20^2","v":{"$error":"#VALUE!"}},0,{"$f":"+(AQ20-AW20)*2","v":0}]
["Presjek X-X",null,null,null,{"$f":"+G20-G21","v":{"$error":"#VALUE!"}},{"$f":"+AX21","v":0},{"$f":"+'Analiza i dimenzioniranje'!E48+'HT III-XX'!E13","v":{"$error":"#VALUE!"}},{"$f":"+F21","v":0},{"$f":"+G21","v":{"$error":"#VALUE!"}},{"$f":"+F21","v":0},{"$f":"+G21","v":{"$error":"#VALUE!"}},{"$f":"+F21","v":0},{"$f":"+G21","v":{"$error":"#VALUE!"}},{"$f":"+H21","v":0},{"$f":"+G21","v":{"$error":"#VALUE!"}},{"$f":"+J21","v":0},{"$f":"+G21","v":{"$error":"#VALUE!"}},{"$f":"+L21","v":0},{"$f":"+G21","v":{"$error":"#VALUE!"}},{"$f":"+N21","v":0},{"$f":"+G21","v":{"$error":"#VALUE!"}},{"$f":"+P21","v":0},{"$f":"+G21","v":{"$error":"#VALUE!"}},{"$f":"+R21","v":0},{"$f":"+G21","v":{"$error":"#VALUE!"}},{"$f":"+T21","v":0},{"$f":"+G21","v":{"$error":"#VALUE!"}},{"$f":"+V21","v":0},{"$f":"+G21","v":{"$error":"#VALUE!"}},{"$f":"+X21","v":0},{"$f":"+G21","v":{"$error":"#VALUE!"}},{"$f":"+Z21","v":0},{"$f":"+G21","v":{"$error":"#VALUE!"}},{"$f":"+AB21","v":0},{"$f":"+G21","v":{"$error":"#VALUE!"}},{"$f":"+AD21","v":0},{"$f":"+G21","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"+AN22","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0]
["Presjek X-X",null,null,null,{"$f":"+G21-G22","v":{"$error":"#VALUE!"}},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+ROUND('Analiza i dimenzioniranje'!$E$48,2)","v":6},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$U$67","v":6.0000000000000009},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+I22","v":6.0000000000000009},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+G22","v":6},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$U$67","v":6.0000000000000009},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+O22","v":6.0000000000000009},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+M22","v":6},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$U$67","v":6.0000000000000009},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+U22","v":6.0000000000000009},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+S22","v":6},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$U$67","v":6.0000000000000009},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+AA22","v":6.0000000000000009},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+Y22","v":6},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$U$67","v":6.0000000000000009},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+AG22","v":6.0000000000000009},{"$f":"+$AX$22","v":{"$error":"#VALUE!"}},{"$f":"+AE22","v":6},null,{"$error":"#VALUE!"},{"$f":"$E$15^2+AM22^2","v":{"$error":"#VALUE!"}},{"$f":"$G$14^2+AM22^2","v":{"$error":"#VALUE!"}},{"$f":"$G$16^2+AM22^2","v":{"$error":"#VALUE!"}},{"$f":"IF(AM22=0,0,$E$11/(PI())*(ATAN(($E$16*$G$14)/(AM22*SQRT(AP22)))-$E$16*$G$14*AM22/(AO22*SQRT(AP22))))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"$E$16^2+AS22^2","v":{"$error":"#VALUE!"}},{"$f":"$E$15^2+AS22^2","v":{"$error":"#VALUE!"}},{"$f":"$G$13^2+AS22^2","v":{"$error":"#VALUE!"}},{"$f":"IF(AS22=0,0,($E$11/(PI()))*(ATAN(($E$16*$E$15)/(AS22*SQRT(AV22)))-$E$16*$E$15*AS22/(AU22*SQRT(AV22))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["Presjek XIX-XIX",null,null,null,{"$f":"+E22+$E$19","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+ROUND(G22-$E$19,2)","v":5.68},{"$f":"+F23","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$U$66","v":5.6800000000000006},{"$error":"#VALUE!"},5.6800000000000006,{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},{"$f":"+I23","v":5.6800000000000006},{"$error":"#VALUE!"},{"$f":"+K23","v":5.6800000000000006},{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},{"$f":"+O23","v":5.6800000000000006},{"$error":"#VALUE!"},{"$f":"+Q23","v":5.6800000000000006},{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},{"$f":"+U23","v":5.6800000000000006},{"$error":"#VALUE!"},{"$f":"+W23","v":5.6800000000000006},{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},{"$f":"+AA23","v":5.6800000000000006},{"$error":"#VALUE!"},{"$f":"+AC23","v":5.6800000000000006},0,{"$f":"+AK22","v":6},null,{"$error":"#VALUE!"},{"$f":"$E$15^2+AM23^2","v":{"$error":"#VALUE!"}},{"$f":"$G$14^2+AM23^2","v":{"$error":"#VALUE!"}},{"$f":"$G$16^2+AM23^2","v":{"$error":"#VALUE!"}},{"$f":"$E$11/(PI())*(ATAN(($E$16*$G$14)/(AM23*SQRT(AP23)))-$E$16*$G$14*AM23/(AO23*SQRT(AP23)))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"$E$16^2+AS23^2","v":{"$error":"#VALUE!"}},{"$f":"$E$15^2+AS23^2","v":{"$error":"#VALUE!"}},{"$f":"$G$13^2+AS23^2","v":{"$error":"#VALUE!"}},{"$f":"($E$11/(PI()))*(ATAN(($E$16*$E$15)/(AS23*SQRT(AV23)))-$E$16*$E$15*AS23/(AU23*SQRT(AV23)))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["Presjek XVIII-XVIII",null,null,null,{"$f":"+E23+$E$19","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+G23-$E$19","v":5.3599999999999994},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$65","v":5.36},{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.36,0,{"$f":"+AI23","v":5.6800000000000006},0,5.3599999999999994,null,{"$error":"#VALUE!"},{"$f":"$E$15^2+AM24^2","v":{"$error":"#VALUE!"}},{"$f":"$G$14^2+AM24^2","v":{"$error":"#VALUE!"}},{"$f":"$G$16^2+AM24^2","v":{"$error":"#VALUE!"}},{"$f":"$E$11/(PI())*(ATAN(($E$16*$G$14)/(AM24*SQRT(AP24)))-$E$16*$G$14*AM24/(AO24*SQRT(AP24)))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"$E$16^2+AS24^2","v":{"$error":"#VALUE!"}},{"$f":"$E$15^2+AS24^2","v":{"$error":"#VALUE!"}},{"$f":"$G$13^2+AS24^2","v":{"$error":"#VALUE!"}},{"$f":"($E$11/(PI()))*(ATAN(($E$16*$E$15)/(AS24*SQRT(AV24)))-$E$16*$E$15*AS24/(AU24*SQRT(AV24)))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["Presjek XVII-XVII",null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$64","v":5.04},{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.0399999999999991,0,{"$f":"+AG24","v":5.36},0,5.04,0,5.0399999999999991,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"$E$15^2+AS25^2","v":{"$error":"#VALUE!"}},{"$f":"$G$13^2+AS25^2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XVI-XVI",null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$63","v":4.72},{"$error":"#VALUE!"},4.72,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.72,{"$error":"#VALUE!"},4.72,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.72,{"$error":"#VALUE!"},4.72,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.72,{"$error":"#VALUE!"},4.72,0,{"$f":"+AE25","v":5.0399999999999991},0,4.72,0,4.72,0,5.0399999999999991,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XV-XV",null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$62","v":4.4000000000000004},{"$error":"#VALUE!"},4.4000000000000004,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.4000000000000004,{"$error":"#VALUE!"},4.4000000000000004,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.4000000000000004,{"$error":"#VALUE!"},4.4000000000000004,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.4000000000000004,0,{"$f":"+AC26","v":4.72},0,4.3999999999999986,0,4.4000000000000004,0,4.72,0,4.3999999999999986,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XIV-XIV",null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$61","v":4.08},{"$error":"#VALUE!"},4.08,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.08,{"$error":"#VALUE!"},4.08,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.08,{"$error":"#VALUE!"},4.08,{"$error":"#VALUE!"},4.0799999999999983,0,{"$f":"+AA27","v":4.4000000000000004},0,4.08,0,4.0799999999999983,0,4.4000000000000004,0,4.08,0,4.0799999999999983,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XIII-XIII",null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$60","v":3.76},{"$error":"#VALUE!"},3.76,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.76,{"$error":"#VALUE!"},3.76,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.76,{"$error":"#VALUE!"},3.76,0,{"$f":"+Y28","v":4.0799999999999983},0,3.76,0,3.76,0,4.0799999999999983,0,3.76,0,3.76,0,4.0799999999999983,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek  XII-XII",null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$59","v":3.44},{"$error":"#VALUE!"},3.44,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.44,{"$error":"#VALUE!"},3.44,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.44,0,{"$f":"+W29","v":3.76},0,3.4399999999999986,0,3.44,0,3.76,0,3.4399999999999986,0,3.44,0,3.76,0,3.4399999999999986,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XI-XI",null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$58","v":3.14},{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.1199999999999988,0,{"$f":"+U30","v":3.44},0,3.14,0,3.1199999999999988,0,3.44,0,3.14,0,3.1199999999999988,0,3.44,0,3.14,0,3.1199999999999988,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek X-X",null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$57","v":2.8},{"$error":"#VALUE!"},2.8,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.8,{"$error":"#VALUE!"},2.8,0,{"$f":"+S31","v":3.1199999999999988},0,2.8,0,2.8,0,3.1199999999999988,0,2.8,0,2.8,0,3.1199999999999988,0,2.8,0,2.8,0,3.1199999999999988,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek IX-IX",null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$56","v":2.48},{"$error":"#VALUE!"},2.48,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.48,0,{"$f":"+Q32","v":2.8},0,2.4799999999999991,0,2.48,0,2.8,0,2.4799999999999991,0,2.48,0,2.8,0,2.4799999999999991,0,2.48,0,2.8,0,2.4799999999999991,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VIII-VIII",null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},2.1599999999999993,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$55","v":2.16},{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},2.1599999999999993,0,{"$f":"+O33","v":2.48},0,2.16,0,2.1599999999999993,0,2.48,0,2.16,0,2.1599999999999993,0,2.48,0,2.16,0,2.1599999999999993,0,2.48,0,2.16,0,2.1599999999999993,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VII-VII",null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1.8399999999999992,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$54","v":1.84},{"$error":"#VALUE!"},1.84,0,{"$f":"+M34","v":2.1599999999999993},0,1.84,0,1.84,0,2.1599999999999993,0,1.84,0,1.84,0,2.1599999999999993,0,1.84,0,1.84,0,2.1599999999999993,0,1.84,0,1.84,0,2.1599999999999993,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VI-VI",null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1.5199999999999991,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$53","v":1.52},0,{"$f":"+K35","v":1.84},0,1.5199999999999991,0,1.52,0,1.84,0,1.5199999999999991,0,1.52,0,1.84,0,1.5199999999999991,0,1.52,0,1.84,0,1.5199999999999991,0,1.52,0,1.84,0,1.5199999999999991,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek III -III",null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1.1999999999999991,0,{"$f":"+I36","v":1.52},0,{"$f":"+K36","v":1.84},0,1.1999999999999991,0,1.52,0,1.84,0,1.1999999999999991,0,1.52,0,1.84,0,1.1999999999999991,0,1.52,0,1.84,0,1.1999999999999991,0,1.52,0,1.84,0,1.1999999999999991,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["IV-IV=Mmin",null,null,null,null,0,{"$f":"+G37","v":1.1999999999999991},0,{"$f":"+G38","v":1.1999999999999991},0,{"$f":"+I38","v":1.1999999999999991},0,1.1999999999999991,0,1.1999999999999991,0,1.1999999999999991,0,1.1999999999999991,0,1.1999999999999991,0,1.1999999999999991,0,1.1999999999999991,0,1.1999999999999991,0,1.1999999999999991,0,1.1999999999999991,0,1.1999999999999991,0,1.1999999999999991,0,1.1999999999999991]
["V-V = Mmax",null,null,null,null,0,{"$f":"+G19","v":{"$error":"#VALUE!"}},0,{"$f":"+G39","v":{"$error":"#VALUE!"}},0,{"$f":"+G39","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"}]
[null,null,null,"Ukupni pritisak",null,"SQhi=",{"$f":"+G43","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I43","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K43","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+M43","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+O43","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Q43","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+S43","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+U43","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+W43","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Y43","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AA43","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AC43","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AE43","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AG43","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AI43","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AK43","v":{"$error":"#VALUE!"}}]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G45","v":{"$error":"#VALUE!"}},"y=",{"$f":"+I45","v":{"$error":"#VALUE!"}},"y=",{"$f":"+K45","v":{"$error":"#VALUE!"}}," y=",{"$f":"+M45","v":{"$error":"#VALUE!"}},"y=",{"$f":"+O45","v":{"$error":"#VALUE!"}},"y=",{"$f":"+Q45","v":{"$error":"#VALUE!"}}," y=",{"$f":"+S45","v":{"$error":"#VALUE!"}},"y=",{"$f":"+U45","v":{"$error":"#VALUE!"}},"y=",{"$f":"+W45","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Y45","v":{"$error":"#VALUE!"}},"y=",{"$f":"+AA45","v":{"$error":"#VALUE!"}},"y=",{"$f":"+AC45","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AE45","v":{"$error":"#VALUE!"}},"y=",{"$f":"+AG45","v":{"$error":"#VALUE!"}},"y=",{"$f":"+AI45","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AK45","v":{"$error":"#VALUE!"}}]
[null,null,null,"krak za presjek III -III",null,"z=",{"$f":"+G41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+O41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Q41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+S41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+U41-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}},"z=",{"$f":"+W41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Y41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AA41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AC41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AE41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AG41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AI41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AK41-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,"F=",{"$f":"-0.5*((F20*G21-F21*G20)+(F21*G22-F22*G21)+\n (F22*G23-F23*G22)+\n(F23*G24-F24*G23)+\n(F24*G25-F25*G24)+\n(F25*G26-F26*G25)+\n(F26*G27-F27*G26)+\n(F27*G28-F28*G27)+\n(F28*G29-F29*G28)+\n(F29*G30-F30*G29)+\n(F30*G31-F31*G30)+\n(F31*G32-F32*G31)+\n(F32*G33-F33*G32)+\n(F33*G34-F34*G33)+\n(F34*G35-F35*G34)+\n(F35*G36-F36*G35)+\n(F36*G37-F37*G36)+\n(F37*G38-F38*G37)+\n(F38*G39-F39*G38))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((H20*I21-H21*I20)+\n(H21*I22-H22*I21)+\n(H22*I23-H23*I22)+\n(H23*I24-H24*I23)+\n(H24*I25-H25*I24)+\n(H25*I26-H26*I25)+\n(H26*I27-H27*I26)+\n(H27*I28-H28*I27)+\n(H28*I29-H29*I28)+\n(H29*I30-H30*I29)+\n(H30*I31-H31*I30)+\n(H31*I32-H32*I31)+\n(H32*I33-H33*I32)+\n(H33*I34-H34*I33)+\n(H34*I35-H35*I34)+\n(H35*I36-H36*I35)+\n(H36*I37-H37*I36)+\n(H37*I38-H38*I37)+\n(H38*I39-H39*I38))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((J20*K21-J21*K20)+\n(J21*K22-J22*K21)+\n(J22*K23-J23*K22)+\n(J23*K24-J24*K23)+\n(J24*K25-J25*K24)+\n(J25*K26-J26*K25)+\n(J26*K27-J27*K26)+\n(J27*K28-J28*K27)+\n(J28*K29-J29*K28)+\n(J29*K30-J30*K29)+\n(J30*K31-J31*K30)+\n(J31*K32-J32*K31)+\n(J32*K33-J33*K32)+\n(J33*K34-J34*K33)+\n(J34*K35-J35*K34)+\n(J35*K36-J36*K35)+\n(J36*K37-J37*K36)+\n(J37*K38-J38*K37)+\n(J38*K39-J39*K38))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((L20*M21-L21*M20)+(L21*M22-L22*M21)+\n (L22*M23-L23*M22)+\n(L23*M24-L24*M23)+\n(L24*M25-L25*M24)+\n(L25*M26-L26*M25)+\n(L26*M27-L27*M26)+\n(L27*M28-L28*M27)+\n(L28*M29-L29*M28)+\n(L29*M30-L30*M29)+\n(L30*M31-L31*M30)+\n(L31*M32-L32*M31)+\n(L32*M33-L33*M32)+\n(L33*M34-L34*M33)+\n(L34*M35-L35*M34)+\n(L35*M36-L36*M35)+\n(L36*M37-L37*M36)+\n(L37*M38-L38*M37)+\n(L38*M39-L39*M38))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((N20*O21-N21*O20)+(N21*O22-N22*O21)+\n (N22*O23-N23*O22)+\n(N23*O24-N24*O23)+\n(N24*O25-N25*O24)+\n(N25*O26-N26*O25)+\n(N26*O27-N27*O26)+\n(N27*O28-N28*O27)+\n(N28*O29-N29*O28)+\n(N29*O30-N30*O29)+\n(N30*O31-N31*O30)+\n(N31*O32-N32*O31)+\n(N32*O33-N33*O32)+\n(N33*O34-N34*O33)+\n(N34*O35-N35*O34)+\n(N35*O36-N36*O35)+\n(N36*O37-N37*O36)+\n(N37*O38-N38*O37)+\n(N38*O39-N39*O38))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((P20*Q21-P21*Q20)+(P21*Q22-P22*Q21)+\n (P22*Q23-P23*Q22)+\n(P23*Q24-P24*Q23)+\n(P24*Q25-P25*Q24)+\n(P25*Q26-P26*Q25)+\n(P26*Q27-P27*Q26)+\n(P27*Q28-P28*Q27)+\n(P28*Q29-P29*Q28)+\n(P29*Q30-P30*Q29)+\n(P30*Q31-P31*Q30)+\n(P31*Q32-P32*Q31)+\n(P32*Q33-P33*Q32)+\n(P33*Q34-P34*Q33)+\n(P34*Q35-P35*Q34)+\n(P35*Q36-P36*Q35)+\n(P36*Q37-P37*Q36)+\n(P37*Q38-P38*Q37)+\n(P38*Q39-P39*Q38))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((R20*S21-R21*S20)+(R21*S22-R22*S21)+\n (R22*S23-R23*S22)+\n(R23*S24-R24*S23)+\n(R24*S25-R25*S24)+\n(R25*S26-R26*S25)+\n(R26*S27-R27*S26)+\n(R27*S28-R28*S27)+\n(R28*S29-R29*S28)+\n(R29*S30-R30*S29)+\n(R30*S31-R31*S30)+\n(R31*S32-R32*S31)+\n(R32*S33-R33*S32)+\n(R33*S34-R34*S33)+\n(R34*S35-R35*S34)+\n(R35*S36-R36*S35)+\n(R36*S37-R37*S36)+\n(R37*S38-R38*S37)+\n(R38*S39-R39*S38))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((T20*U21-T21*U20)+(T21*U22-T22*U21)+\n (T22*U23-T23*U22)+\n(T23*U24-T24*U23)+\n(T24*U25-T25*U24)+\n(T25*U26-T26*U25)+\n(T26*U27-T27*U26)+\n(T27*U28-T28*U27)+\n(T28*U29-T29*U28)+\n(T29*U30-T30*U29)+\n(T30*U31-T31*U30)+\n(T31*U32-T32*U31)+\n(T32*U33-T33*U32)+\n(T33*U34-T34*U33)+\n(T34*U35-T35*U34)+\n(T35*U36-T36*U35)+\n(T36*U37-T37*U36)+\n(T37*U38-T38*U37)+\n(T38*U39-T39*U38))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((V20*W21-V21*W20)+(V21*W22-V22*W21)+\n (V22*W23-V23*W22)+\n(V23*W24-V24*W23)+\n(V24*W25-V25*W24)+\n(V25*W26-V26*W25)+\n(V26*W27-V27*W26)+\n(V27*W28-V28*W27)+\n(V28*W29-V29*W28)+\n(V29*W30-V30*W29)+\n(V30*W31-V31*W30)+\n(V31*W32-V32*W31)+\n(V32*W33-V33*W32)+\n(V33*W34-V34*W33)+\n(V34*W35-V35*W34)+\n(V35*W36-V36*W35)+\n(V36*W37-V37*W36)+\n(V37*W38-V38*W37)+\n(V38*W39-V39*W38))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((X20*Y21-X21*Y20)+(X21*Y22-X22*Y21)+\n (X22*Y23-X23*Y22)+\n(X23*Y24-X24*Y23)+\n(X24*Y25-X25*Y24)+\n(X25*Y26-X26*Y25)+\n(X26*Y27-X27*Y26)+\n(X27*Y28-X28*Y27)+\n(X28*Y29-X29*Y28)+\n(X29*Y30-X30*Y29)+\n(X30*Y31-X31*Y30)+\n(X31*Y32-X32*Y31)+\n(X32*Y33-X33*Y32)+\n(X33*Y34-X34*Y33)+\n(X34*Y35-X35*Y34)+\n(X35*Y36-X36*Y35)+\n(X36*Y37-X37*Y36)+\n(X37*Y38-X38*Y37)+\n(X38*Y39-X39*Y38))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((Z20*AA21-Z21*AA20)+(Z21*AA22-Z22*AA21)+\n (Z22*AA23-Z23*AA22)+\n(Z23*AA24-Z24*AA23)+\n(Z24*AA25-Z25*AA24)+\n(Z25*AA26-Z26*AA25)+\n(Z26*AA27-Z27*AA26)+\n(Z27*AA28-Z28*AA27)+\n(Z28*AA29-Z29*AA28)+\n(Z29*AA30-Z30*AA29)+\n(Z30*AA31-Z31*AA30)+\n(Z31*AA32-Z32*AA31)+\n(Z32*AA33-Z33*AA32)+\n(Z33*AA34-Z34*AA33)+\n(Z34*AA35-Z35*AA34)+\n(Z35*AA36-Z36*AA35)+\n(Z36*AA37-Z37*AA36)+\n(Z37*AA38-Z38*AA37)+\n(Z38*AA39-Z39*AA38))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AB20*AC21-AB21*AC20)+(AB21*AC22-AB22*AC21)+\n (AB22*AC23-AB23*AC22)+\n(AB23*AC24-AB24*AC23)+\n(AB24*AC25-AB25*AC24)+\n(AB25*AC26-AB26*AC25)+\n(AB26*AC27-AB27*AC26)+\n(AB27*AC28-AB28*AC27)+\n(AB28*AC29-AB29*AC28)+\n(AB29*AC30-AB30*AC29)+\n(AB30*AC31-AB31*AC30)+\n(AB31*AC32-AB32*AC31)+\n(AB32*AC33-AB33*AC32)+\n(AB33*AC34-AB34*AC33)+\n(AB34*AC35-AB35*AC34)+\n(AB35*AC36-AB36*AC35)+\n(AB36*AC37-AB37*AC36)+\n(AB37*AC38-AB38*AC37)+\n(AB38*AC39-AB39*AC38))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AD20*AE21-AD21*AE20)+(AD21*AE22-AD22*AE21)+\n (AD22*AE23-AD23*AE22)+\n(AD23*AE24-AD24*AE23)+\n(AD24*AE25-AD25*AE24)+\n(AD25*AE26-AD26*AE25)+\n(AD26*AE27-AD27*AE26)+\n(AD27*AE28-AD28*AE27)+\n(AD28*AE29-AD29*AE28)+\n(AD29*AE30-AD30*AE29)+\n(AD30*AE31-AD31*AE30)+\n(AD31*AE32-AD32*AE31)+\n(AD32*AE33-AD33*AE32)+\n(AD33*AE34-AD34*AE33)+\n(AD34*AE35-AD35*AE34)+\n(AD35*AE36-AD36*AE35)+\n(AD36*AE37-AD37*AE36)+\n(AD37*AE38-AD38*AE37)+\n(AD38*AE39-AD39*AE38))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AF20*AG21-AF21*AG20)+(AF21*AG22-AF22*AG21)+\n (AF22*AG23-AF23*AG22)+\n(AF23*AG24-AF24*AG23)+\n(AF24*AG25-AF25*AG24)+\n(AF25*AG26-AF26*AG25)+\n(AF26*AG27-AF27*AG26)+\n(AF27*AG28-AF28*AG27)+\n(AF28*AG29-AF29*AG28)+\n(AF29*AG30-AF30*AG29)+\n(AF30*AG31-AF31*AG30)+\n(AF31*AG32-AF32*AG31)+\n(AF32*AG33-AF33*AG32)+\n(AF33*AG34-AF34*AG33)+\n(AF34*AG35-AF35*AG34)+\n(AF35*AG36-AF36*AG35)+\n(AF36*AG37-AF37*AG36)+\n(AF37*AG38-AF38*AG37)+\n(AF38*AG39-AF39*AG38))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AH20*AI21-AH21*AI20)+(AH21*AI22-AH22*AI21)+\n (AH22*AI23-AH23*AI22)+\n(AH23*AI24-AH24*AI23)+\n(AH24*AI25-AH25*AI24)+\n(AH25*AI26-AH26*AI25)+\n(AH26*AI27-AH27*AI26)+\n(AH27*AI28-AH28*AI27)+\n(AH28*AI29-AH29*AI28)+\n(AH29*AI30-AH30*AI29)+\n(AH30*AI31-AH31*AI30)+\n(AH31*AI32-AH32*AI31)+\n(AH32*AI33-AH33*AI32)+\n(AH33*AI34-AH34*AI33)+\n(AH34*AI35-AH35*AI34)+\n(AH35*AI36-AH36*AI35)+\n(AH36*AI37-AH37*AI36)+\n(AH37*AI38-AH38*AI37)+\n(AH38*AI39-AH39*AI38))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AJ20*AK21-AJ21*AK20)+(AJ21*AK22-AJ22*AK21)+\n (AJ22*AK23-AJ23*AK22)+\n(AJ23*AK24-AJ24*AK23)+\n(AJ24*AK25-AJ25*AK24)+\n(AJ25*AK26-AJ26*AK25)+\n(AJ26*AK27-AJ27*AK26)+\n(AJ27*AK28-AJ28*AK27)+\n(AJ28*AK29-AJ29*AK28)+\n(AJ29*AK30-AJ30*AK29)+\n(AJ30*AK31-AJ31*AK30)+\n(AJ31*AK32-AJ32*AK31)+\n(AJ32*AK33-AJ33*AK32)+\n(AJ33*AK34-AJ34*AK33)+\n(AJ34*AK35-AJ35*AK34)+\n(AJ35*AK36-AJ36*AK35)+\n(AJ36*AK37-AJ37*AK36)+\n(AJ37*AK38-AJ38*AK37)+\n(AJ38*AK39-AJ39*AK38))","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,"x=",0.08,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0]
[null,null,null,null,null,"y=",{"$f":"+IF(G43=0,0,-((F20*G21-F21*G20)*(G20+G21)+(F21*G22-F22*G21)*(G21+G22)+\n(F22*G23-F23*G22)*(G22+G23)+\n(F23*G24-F24*G23)*(G23+G24)+\n(F24*G25-F25*G24)*(G24+G25)+\n(F25*G26-F26*G25)*(G25+G26)+\n(F26*G27-F27*G26)*(G26+G27)+\n(F27*G28-F28*G27)*(G27+G28)+\n(F28*G29-F29*G28)*(G28+G29)+\n(F29*G30-F30*G29)*(G29+G30)+\n(F30*G31-F31*G30)*(G30+G31)+\n(F31*G32-F32*G31)*(G31+G32)+\n(F32*G33-F33*G32)*(G32+G33)+\n(F33*G34-F34*G33)*(G33+G34)+\n(F34*G35-F35*G34)*(G34+G35)+\n(F35*G36-F36*G35)*(G35+G36)+\n(F36*G37-F37*G36)*(G36+G37)+\n(F37*G38-F38*G37)*(G37+G38)+\n(F38*G39-F39*G38)*(G38+G39))/6/G43)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(I43=0,0,-((H20*I21-H21*I20)*(I20+I21)+\n(H21*I22-H22*I21)*(I21+I22)+\n(H22*I23-H23*I22)*(I22+I23)+\n(H23*I24-H24*I23)*(I23+I24)+\n(H24*I25-H25*I24)*(I24+I25)+\n(H25*I26-H26*I25)*(I25+I26)+\n(H26*I27-H27*I26)*(I26+I27)+\n(H27*I28-H28*I27)*(I27+I28)+\n(H28*I29-H29*I28)*(I28+I29)+\n(H29*I30-H30*I29)*(I29+I30)+\n(H30*I31-H31*I30)*(I30+I31)+\n(H31*I32-H32*I31)*(I31+I32)+\n(H32*I33-H33*I32)*(I32+I33)+\n(H33*I34-H34*I33)*(I33+I34)+\n(H34*I35-H35*I34)*(I34+I35)+\n(H35*I36-H36*I35)*(I35+I36)+\n(H36*I37-H37*I36)*(I36+I37)+\n(H37*I38-H38*I37)*(I37+I38)+\n(H38*I39-H39*I38)*(I38+I39)\n)/6/I43)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(K43=0,0,-((J20*K21-J21*K20)*(K20+K21)+\n(J21*K22-J22*K21)*(K21+K22)+\n(J22*K23-J23*K22)*(K22+K23)+\n(J23*K24-J24*K23)*(K23+K24)+\n(J24*K25-J25*K24)*(K24+K25)+\n(J25*K26-J26*K25)*(K25+K26)+\n(J26*K27-J27*K26)*(K26+K27)+\n(J27*K28-J28*K27)*(K27+K28)+\n(J28*K29-J29*K28)*(K28+K29)+\n(J29*K30-J30*K29)*(K29+K30)+\n(J30*K31-J31*K30)*(K30+K31)+\n(J31*K32-J32*K31)*(K31+K32)+\n(J32*K33-J33*K32)*(K32+K33)+\n(J33*K34-J34*K33)*(K33+K34)+\n(J34*K35-J35*K34)*(K34+K35)+\n(J35*K36-J36*K35)*(K35+K36)+\n(J36*K37-J37*K36)*(K36+K37)+\n(J37*K38-J38*K37)*(K37+K38)+\n(J38*K39-J39*K38)*(K38+K39)\n)/6/K43)","v":{"$error":"#VALUE!"}},{"$f":"+F45","v":"y="},{"$f":"+IF(M43=0,0,-((L20*M21-L21*M20)*(M20+M21)+(L21*M22-L22*M21)*(M21+M22)+\n(L22*M23-L23*M22)*(M22+M23)+\n(L23*M24-L24*M23)*(M23+M24)+\n(L24*M25-L25*M24)*(M24+M25)+\n(L25*M26-L26*M25)*(M25+M26)+\n(L26*M27-L27*M26)*(M26+M27)+\n(L27*M28-L28*M27)*(M27+M28)+\n(L28*M29-L29*M28)*(M28+M29)+\n(L29*M30-L30*M29)*(M29+M30)+\n(L30*M31-L31*M30)*(M30+M31)+\n(L31*M32-L32*M31)*(M31+M32)+\n(L32*M33-L33*M32)*(M32+M33)+\n(L33*M34-L34*M33)*(M33+M34)+\n(L34*M35-L35*M34)*(M34+M35)+\n(L35*M36-L36*M35)*(M35+M36)+\n(L36*M37-L37*M36)*(M36+M37)+\n(L37*M38-L38*M37)*(M37+M38)+\n(L38*M39-L39*M38)*(M38+M39))/6/M43)","v":{"$error":"#VALUE!"}},{"$f":"+H45","v":"y="},{"$f":"+IF(O43=0,0,-((N20*O21-N21*O20)*(O20+O21)+(N21*O22-N22*O21)*(O21+O22)+\n(N22*O23-N23*O22)*(O22+O23)+\n(N23*O24-N24*O23)*(O23+O24)+\n(N24*O25-N25*O24)*(O24+O25)+\n(N25*O26-N26*O25)*(O25+O26)+\n(N26*O27-N27*O26)*(O26+O27)+\n(N27*O28-N28*O27)*(O27+O28)+\n(N28*O29-N29*O28)*(O28+O29)+\n(N29*O30-N30*O29)*(O29+O30)+\n(N30*O31-N31*O30)*(O30+O31)+\n(N31*O32-N32*O31)*(O31+O32)+\n(N32*O33-N33*O32)*(O32+O33)+\n(N33*O34-N34*O33)*(O33+O34)+\n(N34*O35-N35*O34)*(O34+O35)+\n(N35*O36-N36*O35)*(O35+O36)+\n(N36*O37-N37*O36)*(O36+O37)+\n(N37*O38-N38*O37)*(O37+O38)+\n(N38*O39-N39*O38)*(O38+O39))/6/O43)","v":{"$error":"#VALUE!"}},{"$f":"+J45","v":"y="},{"$f":"+IF(Q43=0,0,-((P20*Q21-P21*Q20)*(Q20+Q21)+(P21*Q22-P22*Q21)*(Q21+Q22)+\n(P22*Q23-P23*Q22)*(Q22+Q23)+\n(P23*Q24-P24*Q23)*(Q23+Q24)+\n(P24*Q25-P25*Q24)*(Q24+Q25)+\n(P25*Q26-P26*Q25)*(Q25+Q26)+\n(P26*Q27-P27*Q26)*(Q26+Q27)+\n(P27*Q28-P28*Q27)*(Q27+Q28)+\n(P28*Q29-P29*Q28)*(Q28+Q29)+\n(P29*Q30-P30*Q29)*(Q29+Q30)+\n(P30*Q31-P31*Q30)*(Q30+Q31)+\n(P31*Q32-P32*Q31)*(Q31+Q32)+\n(P32*Q33-P33*Q32)*(Q32+Q33)+\n(P33*Q34-P34*Q33)*(Q33+Q34)+\n(P34*Q35-P35*Q34)*(Q34+Q35)+\n(P35*Q36-P36*Q35)*(Q35+Q36)+\n(P36*Q37-P37*Q36)*(Q36+Q37)+\n(P37*Q38-P38*Q37)*(Q37+Q38)+\n(P38*Q39-P39*Q38)*(Q38+Q39))/6/Q43)","v":{"$error":"#VALUE!"}},{"$f":"+L45","v":"y="},{"$f":"+IF(S43=0,0,-((R20*S21-R21*S20)*(S20+S21)+(R21*S22-R22*S21)*(S21+S22)+\n(R22*S23-R23*S22)*(S22+S23)+\n(R23*S24-R24*S23)*(S23+S24)+\n(R24*S25-R25*S24)*(S24+S25)+\n(R25*S26-R26*S25)*(S25+S26)+\n(R26*S27-R27*S26)*(S26+S27)+\n(R27*S28-R28*S27)*(S27+S28)+\n(R28*S29-R29*S28)*(S28+S29)+\n(R29*S30-R30*S29)*(S29+S30)+\n(R30*S31-R31*S30)*(S30+S31)+\n(R31*S32-R32*S31)*(S31+S32)+\n(R32*S33-R33*S32)*(S32+S33)+\n(R33*S34-R34*S33)*(S33+S34)+\n(R34*S35-R35*S34)*(S34+S35)+\n(R35*S36-R36*S35)*(S35+S36)+\n(R36*S37-R37*S36)*(S36+S37)+\n(R37*S38-R38*S37)*(S37+S38)+\n(R38*S39-R39*S38)*(S38+S39))/6/S43)","v":{"$error":"#VALUE!"}},{"$f":"+N45","v":"y="},{"$f":"+IF(U43=0,0,-((T20*U21-T21*U20)*(U20+U21)+(T21*U22-T22*U21)*(U21+U22)+\n(T22*U23-T23*U22)*(U22+U23)+\n(T23*U24-T24*U23)*(U23+U24)+\n(T24*U25-T25*U24)*(U24+U25)+\n(T25*U26-T26*U25)*(U25+U26)+\n(T26*U27-T27*U26)*(U26+U27)+\n(T27*U28-T28*U27)*(U27+U28)+\n(T28*U29-T29*U28)*(U28+U29)+\n(T29*U30-T30*U29)*(U29+U30)+\n(T30*U31-T31*U30)*(U30+U31)+\n(T31*U32-T32*U31)*(U31+U32)+\n(T32*U33-T33*U32)*(U32+U33)+\n(T33*U34-T34*U33)*(U33+U34)+\n(T34*U35-T35*U34)*(U34+U35)+\n(T35*U36-T36*U35)*(U35+U36)+\n(T36*U37-T37*U36)*(U36+U37)+\n(T37*U38-T38*U37)*(U37+U38)+\n(T38*U39-T39*U38)*(U38+U39))/6/U43)","v":{"$error":"#VALUE!"}},{"$f":"+P45","v":"y="},{"$f":"+IF(W43=0,0,-((V20*W21-V21*W20)*(W20+W21)+(V21*W22-V22*W21)*(W21+W22)+\n(V22*W23-V23*W22)*(W22+W23)+\n(V23*W24-V24*W23)*(W23+W24)+\n(V24*W25-V25*W24)*(W24+W25)+\n(V25*W26-V26*W25)*(W25+W26)+\n(V26*W27-V27*W26)*(W26+W27)+\n(V27*W28-V28*W27)*(W27+W28)+\n(V28*W29-V29*W28)*(W28+W29)+\n(V29*W30-V30*W29)*(W29+W30)+\n(V30*W31-V31*W30)*(W30+W31)+\n(V31*W32-V32*W31)*(W31+W32)+\n(V32*W33-V33*W32)*(W32+W33)+\n(V33*W34-V34*W33)*(W33+W34)+\n(V34*W35-V35*W34)*(W34+W35)+\n(V35*W36-V36*W35)*(W35+W36)+\n(V36*W37-V37*W36)*(W36+W37)+\n(V37*W38-V38*W37)*(W37+W38)+\n(V38*W39-V39*W38)*(W38+W39))/6/W43)","v":{"$error":"#VALUE!"}},{"$f":"+R45","v":"y="},{"$f":"+IF(Y43=0,0,-((X20*Y21-X21*Y20)*(Y20+Y21)+(X21*Y22-X22*Y21)*(Y21+Y22)+\n(X22*Y23-X23*Y22)*(Y22+Y23)+\n(X23*Y24-X24*Y23)*(Y23+Y24)+\n(X24*Y25-X25*Y24)*(Y24+Y25)+\n(X25*Y26-X26*Y25)*(Y25+Y26)+\n(X26*Y27-X27*Y26)*(Y26+Y27)+\n(X27*Y28-X28*Y27)*(Y27+Y28)+\n(X28*Y29-X29*Y28)*(Y28+Y29)+\n(X29*Y30-X30*Y29)*(Y29+Y30)+\n(X30*Y31-X31*Y30)*(Y30+Y31)+\n(X31*Y32-X32*Y31)*(Y31+Y32)+\n(X32*Y33-X33*Y32)*(Y32+Y33)+\n(X33*Y34-X34*Y33)*(Y33+Y34)+\n(X34*Y35-X35*Y34)*(Y34+Y35)+\n(X35*Y36-X36*Y35)*(Y35+Y36)+\n(X36*Y37-X37*Y36)*(Y36+Y37)+\n(X37*Y38-X38*Y37)*(Y37+Y38)+\n(X38*Y39-X39*Y38)*(Y38+Y39))/6/Y43)","v":{"$error":"#VALUE!"}},{"$f":"+T45","v":"y="},{"$f":"+IF(AA43=0,0,-((Z20*AA21-Z21*AA20)*(AA20+AA21)+(Z21*AA22-Z22*AA21)*(AA21+AA22)+\n(Z22*AA23-Z23*AA22)*(AA22+AA23)+\n(Z23*AA24-Z24*AA23)*(AA23+AA24)+\n(Z24*AA25-Z25*AA24)*(AA24+AA25)+\n(Z25*AA26-Z26*AA25)*(AA25+AA26)+\n(Z26*AA27-Z27*AA26)*(AA26+AA27)+\n(Z27*AA28-Z28*AA27)*(AA27+AA28)+\n(Z28*AA29-Z29*AA28)*(AA28+AA29)+\n(Z29*AA30-Z30*AA29)*(AA29+AA30)+\n(Z30*AA31-Z31*AA30)*(AA30+AA31)+\n(Z31*AA32-Z32*AA31)*(AA31+AA32)+\n(Z32*AA33-Z33*AA32)*(AA32+AA33)+\n(Z33*AA34-Z34*AA33)*(AA33+AA34)+\n(Z34*AA35-Z35*AA34)*(AA34+AA35)+\n(Z35*AA36-Z36*AA35)*(AA35+AA36)+\n(Z36*AA37-Z37*AA36)*(AA36+AA37)+\n(Z37*AA38-Z38*AA37)*(AA37+AA38)+\n(Z38*AA39-Z39*AA38)*(AA38+AA39))/6/AA43)","v":{"$error":"#VALUE!"}},{"$f":"+V45","v":"y="},{"$f":"+IF(AC43=0,0,-((AB20*AC21-AB21*AC20)*(AC20+AC21)+(AB21*AC22-AB22*AC21)*(AC21+AC22)+\n(AB22*AC23-AB23*AC22)*(AC22+AC23)+\n(AB23*AC24-AB24*AC23)*(AC23+AC24)+\n(AB24*AC25-AB25*AC24)*(AC24+AC25)+\n(AB25*AC26-AB26*AC25)*(AC25+AC26)+\n(AB26*AC27-AB27*AC26)*(AC26+AC27)+\n(AB27*AC28-AB28*AC27)*(AC27+AC28)+\n(AB28*AC29-AB29*AC28)*(AC28+AC29)+\n(AB29*AC30-AB30*AC29)*(AC29+AC30)+\n(AB30*AC31-AB31*AC30)*(AC30+AC31)+\n(AB31*AC32-AB32*AC31)*(AC31+AC32)+\n(AB32*AC33-AB33*AC32)*(AC32+AC33)+\n(AB33*AC34-AB34*AC33)*(AC33+AC34)+\n(AB34*AC35-AB35*AC34)*(AC34+AC35)+\n(AB35*AC36-AB36*AC35)*(AC35+AC36)+\n(AB36*AC37-AB37*AC36)*(AC36+AC37)+\n(AB37*AC38-AB38*AC37)*(AC37+AC38)+\n(AB38*AC39-AB39*AC38)*(AC38+AC39))/6/AC43)","v":{"$error":"#VALUE!"}},{"$f":"+X45","v":"y="},{"$f":"+IF(AE43=0,0,-((AD20*AE21-AD21*AE20)*(AE20+AE21)+(AD21*AE22-AD22*AE21)*(AE21+AE22)+\n(AD22*AE23-AD23*AE22)*(AE22+AE23)+\n(AD23*AE24-AD24*AE23)*(AE23+AE24)+\n(AD24*AE25-AD25*AE24)*(AE24+AE25)+\n(AD25*AE26-AD26*AE25)*(AE25+AE26)+\n(AD26*AE27-AD27*AE26)*(AE26+AE27)+\n(AD27*AE28-AD28*AE27)*(AE27+AE28)+\n(AD28*AE29-AD29*AE28)*(AE28+AE29)+\n(AD29*AE30-AD30*AE29)*(AE29+AE30)+\n(AD30*AE31-AD31*AE30)*(AE30+AE31)+\n(AD31*AE32-AD32*AE31)*(AE31+AE32)+\n(AD32*AE33-AD33*AE32)*(AE32+AE33)+\n(AD33*AE34-AD34*AE33)*(AE33+AE34)+\n(AD34*AE35-AD35*AE34)*(AE34+AE35)+\n(AD35*AE36-AD36*AE35)*(AE35+AE36)+\n(AD36*AE37-AD37*AE36)*(AE36+AE37)+\n(AD37*AE38-AD38*AE37)*(AE37+AE38)+\n(AD38*AE39-AD39*AE38)*(AE38+AE39))/6/AE43)","v":{"$error":"#VALUE!"}},{"$f":"+Z45","v":"y="},{"$f":"+IF(AG43=0,0,-((AF20*AG21-AF21*AG20)*(AG20+AG21)+(AF21*AG22-AF22*AG21)*(AG21+AG22)+\n(AF22*AG23-AF23*AG22)*(AG22+AG23)+\n(AF23*AG24-AF24*AG23)*(AG23+AG24)+\n(AF24*AG25-AF25*AG24)*(AG24+AG25)+\n(AF25*AG26-AF26*AG25)*(AG25+AG26)+\n(AF26*AG27-AF27*AG26)*(AG26+AG27)+\n(AF27*AG28-AF28*AG27)*(AG27+AG28)+\n(AF28*AG29-AF29*AG28)*(AG28+AG29)+\n(AF29*AG30-AF30*AG29)*(AG29+AG30)+\n(AF30*AG31-AF31*AG30)*(AG30+AG31)+\n(AF31*AG32-AF32*AG31)*(AG31+AG32)+\n(AF32*AG33-AF33*AG32)*(AG32+AG33)+\n(AF33*AG34-AF34*AG33)*(AG33+AG34)+\n(AF34*AG35-AF35*AG34)*(AG34+AG35)+\n(AF35*AG36-AF36*AG35)*(AG35+AG36)+\n(AF36*AG37-AF37*AG36)*(AG36+AG37)+\n(AF37*AG38-AF38*AG37)*(AG37+AG38)+\n(AF38*AG39-AF39*AG38)*(AG38+AG39))/6/AG43)","v":{"$error":"#VALUE!"}},{"$f":"+AB45","v":"y="},{"$f":"+IF(AI43=0,0,-((AH20*AI21-AH21*AI20)*(AI20+AI21)+(AH21*AI22-AH22*AI21)*(AI21+AI22)+\n(AH22*AI23-AH23*AI22)*(AI22+AI23)+\n(AH23*AI24-AH24*AI23)*(AI23+AI24)+\n(AH24*AI25-AH25*AI24)*(AI24+AI25)+\n(AH25*AI26-AH26*AI25)*(AI25+AI26)+\n(AH26*AI27-AH27*AI26)*(AI26+AI27)+\n(AH27*AI28-AH28*AI27)*(AI27+AI28)+\n(AH28*AI29-AH29*AI28)*(AI28+AI29)+\n(AH29*AI30-AH30*AI29)*(AI29+AI30)+\n(AH30*AI31-AH31*AI30)*(AI30+AI31)+\n(AH31*AI32-AH32*AI31)*(AI31+AI32)+\n(AH32*AI33-AH33*AI32)*(AI32+AI33)+\n(AH33*AI34-AH34*AI33)*(AI33+AI34)+\n(AH34*AI35-AH35*AI34)*(AI34+AI35)+\n(AH35*AI36-AH36*AI35)*(AI35+AI36)+\n(AH36*AI37-AH37*AI36)*(AI36+AI37)+\n(AH37*AI38-AH38*AI37)*(AI37+AI38)+\n(AH38*AI39-AH39*AI38)*(AI38+AI39))/6/AI43)","v":{"$error":"#VALUE!"}},{"$f":"+AD45","v":"y="},{"$f":"+IF(AK43=0,0,-((AJ20*AK21-AJ21*AK20)*(AK20+AK21)+(AJ21*AK22-AJ22*AK21)*(AK21+AK22)+\n(AJ22*AK23-AJ23*AK22)*(AK22+AK23)+\n(AJ23*AK24-AJ24*AK23)*(AK23+AK24)+\n(AJ24*AK25-AJ25*AK24)*(AK24+AK25)+\n(AJ25*AK26-AJ26*AK25)*(AK25+AK26)+\n(AJ26*AK27-AJ27*AK26)*(AK26+AK27)+\n(AJ27*AK28-AJ28*AK27)*(AK27+AK28)+\n(AJ28*AK29-AJ29*AK28)*(AK28+AK29)+\n(AJ29*AK30-AJ30*AK29)*(AK29+AK30)+\n(AJ30*AK31-AJ31*AK30)*(AK30+AK31)+\n(AJ31*AK32-AJ32*AK31)*(AK31+AK32)+\n(AJ32*AK33-AJ33*AK32)*(AK32+AK33)+\n(AJ33*AK34-AJ34*AK33)*(AK33+AK34)+\n(AJ34*AK35-AJ35*AK34)*(AK34+AK35)+\n(AJ35*AK36-AJ36*AK35)*(AK35+AK36)+\n(AJ36*AK37-AJ37*AK36)*(AK36+AK37)+\n(AJ37*AK38-AJ38*AK37)*(AK37+AK38)+\n(AJ38*AK39-AJ39*AK38)*(AK38+AK39))/6/AK43)","v":{"$error":"#VALUE!"}}]
[]
[]
[null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID ",null,null,null,null,null,null,null,"Horizontalni pritisci - samo na zid bez temeja"]
[null,"TOČKASTO OPTEREĆENJE",null,null,null,null," (TERZAGHY)"]
[null,null,"Temelj 1m x 1m"]
[null,null,"KONTINUIRANO OPTEREĆENJE","P =",{"$f":"+'Analiza i dimenzioniranje'!E36","v":20.000001000000001},"kN/m2",null,null,null,null,"Horizontalni pritisci - samo na zid bez temeja"]
[null,null," visina zida iznad  temelja","H =",{"$f":"+'Analiza i dimenzioniranje'!E$47-'Analiza i dimenzioniranje'!E$52","v":{"$error":"#VALUE!"}},"m",{"$f":"+E56","v":0.5}]
[null,null,"visina opterećenja iznad vrha zida","h =",{"$f":"+'C III-V'!X23-'Analiza i dimenzioniranje'!E48","v":{"$error":"#VALUE!"}},"m",{"$f":"SQRT(E56^2+E55^2)","v":1.1180339887498949}]
["dužina opterećenja 1 m",null,"širina opterećenja","b =",1,"m",{"$f":"E55+E54","v":2}]
[null,null,"udaljenost ruba opterećenja točk. temeljaod iskopa","D =",{"$f":"+'Analiza i dimenzioniranje'!E37-0.5","v":1},"m"]
[null,null,"1/2 dužine temelja","L/2=a=",{"$f":"+E54/2","v":0.5},"m",{"$f":"SQRT(G52^2+G54^2)","v":2.0615528128088303}]
[null,null,null,null,null,{"$f":"+ROUND('Analiza i dimenzioniranje'!$E$52,2)","v":1.2},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND('Analiza i dimenzioniranje'!$U$53,2)","v":1.52},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND('Analiza i dimenzioniranje'!$U$54,2)","v":1.84},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND('Analiza i dimenzioniranje'!$U$55,2)","v":2.16},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$56,2)","v":2.48},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$57,2)","v":2.8},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$58,2)","v":3.14},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$59,2)","v":3.44},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$60,2)","v":3.76},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$61,2)","v":4.08},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$62,2)","v":4.4000000000000004},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$63,2)","v":4.72},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$64,2)","v":5.04},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$65,2)","v":5.36},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$66,2)","v":5.68},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$67,2)","v":6},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+$E$19","v":0.32},null,"Presjek III -III-0",null,"Presjek VI-VI",null,"Presjek VII-VII",null,"Presjek VIII-VI-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"PresjekVIV-XIV",null,"Presjek XV-XV",null,"Presjek XVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX"]
[null,null,null,{"$f":"+E20","v":{"$error":"#VALUE!"}},null,"(sb2-sb1)*2",{"$f":"+G57","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+G59","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+G59","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+G59","v":{"$error":"#VALUE!"}},"sb1-sb2",{"$f":"+M59","v":{"$error":"#VALUE!"}},"sb1-sb2",{"$f":"+O59","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+Q59","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+S59","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+U59","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+W59","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+Y59","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+AA59","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+AC59","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+AE59","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+AG59","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"+AI59","v":{"$error":"#VALUE!"}},null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
["Presjek X-X",null,null,{"$f":"+E21","v":{"$error":"#VALUE!"}},null,{"$f":"+AX60","v":0},{"$f":"+G59","v":{"$error":"#VALUE!"}},0,{"$f":"+I59","v":{"$error":"#VALUE!"}},0,{"$f":"+I60","v":{"$error":"#VALUE!"}},{"$f":"+F60","v":0},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$f":"+L60","v":0},{"$f":"+M60","v":{"$error":"#VALUE!"}},{"$f":"+N60","v":0},{"$f":"+O60","v":{"$error":"#VALUE!"}},{"$f":"+P60","v":0},{"$f":"+Q60","v":{"$error":"#VALUE!"}},{"$f":"+R60","v":0},{"$f":"+S60","v":{"$error":"#VALUE!"}},{"$f":"+T60","v":0},{"$f":"+U60","v":{"$error":"#VALUE!"}},{"$f":"+V60","v":0},{"$f":"+W60","v":{"$error":"#VALUE!"}},{"$f":"+X60","v":0},{"$f":"+Y60","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$f":"+AE60","v":{"$error":"#VALUE!"}},null,{"$f":"+D59","v":{"$error":"#VALUE!"}},{"$f":"$E$55^2+AM60^2","v":{"$error":"#VALUE!"}},{"$f":"$G54^2+AM60^2","v":{"$error":"#VALUE!"}},{"$f":"$G$56^2+AM60^2","v":{"$error":"#VALUE!"}},0,null,{"$f":"+AM60","v":{"$error":"#VALUE!"}},{"$f":"$E$56^2+AS60^2","v":{"$error":"#VALUE!"}},{"$f":"$E$55^2+AS60^2","v":{"$error":"#VALUE!"}},{"$f":"$G$53^2+AS60^2","v":{"$error":"#VALUE!"}},0,{"$f":"+(AQ60-AW60)*2","v":0},0]
["Presjek X-X",null,null,{"$f":"+G60-G61","v":{"$error":"#VALUE!"}},null,0,{"$f":"+'Analiza i dimenzioniranje'!E48+'HT III-XX'!E53","v":{"$error":"#VALUE!"}},0,{"$f":"+G61","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$f":"+K61","v":{"$error":"#VALUE!"}},0,{"$f":"+M61","v":{"$error":"#VALUE!"}},0,{"$f":"+K61","v":{"$error":"#VALUE!"}},0,{"$f":"+Q61","v":{"$error":"#VALUE!"}},0,{"$f":"+S61","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$f":"+Y61","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$f":"+AE61","v":{"$error":"#VALUE!"}},null,{"$f":"+D61","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"$G$54^2+AM61^2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},0,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,0]
["Presjek X-X",null,null,{"$f":"+G60-G62","v":{"$error":"#VALUE!"}},null,{"$f":"+$AX$62","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E48","v":6},{"$f":"+$AX$62","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$U$67","v":6.0000000000000009},{"$f":"+$AX$62","v":{"$error":"#VALUE!"}},6.0000000000000009,{"$f":"+F62","v":{"$error":"#VALUE!"}},{"$f":"+G62","v":6},{"$f":"+H62","v":{"$error":"#VALUE!"}},{"$f":"+I62","v":6.0000000000000009},{"$f":"+J62","v":{"$error":"#VALUE!"}},6.0000000000000009,{"$error":"#VALUE!"},6,{"$error":"#VALUE!"},6.0000000000000009,{"$error":"#VALUE!"},6.0000000000000009,{"$error":"#VALUE!"},6,{"$error":"#VALUE!"},6.0000000000000009,{"$error":"#VALUE!"},6.0000000000000009,{"$error":"#VALUE!"},6,{"$error":"#VALUE!"},6.0000000000000009,{"$error":"#VALUE!"},6.0000000000000009,{"$error":"#VALUE!"},{"$f":"+AE62","v":6},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"$G$54^2+AM62^2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AM62=0,0,$E$51/(PI())*(ATAN(($E$56*$G$54)/(AM62*SQRT(AP62)))-$E$56*$G$54*AM62/(AO62*SQRT(AP62))))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AS62=0,0,($E$51/(PI()))*(ATAN(($E$56*$E$55)/(AS62*SQRT(AV62)))-$E$56*$E$55*AS62/(AU62*SQRT(AV62))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},5.94049086851971E-2]
["Presjek XIX-XIX",null,null,{"$f":"+D62+$D$58","v":{"$error":"#VALUE!"}},null,{"$f":"+AX63","v":{"$error":"#VALUE!"}},{"$f":"+G62-$D$58","v":5.68},{"$f":"+F63","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$U$66","v":5.6800000000000006},{"$f":"+H63","v":{"$error":"#VALUE!"}},5.6800000000000006,{"$f":"+F63","v":{"$error":"#VALUE!"}},5.68,{"$error":"#VALUE!"},5.6800000000000006,{"$error":"#VALUE!"},5.6800000000000006,{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},5.6800000000000006,{"$error":"#VALUE!"},5.6800000000000006,{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},5.6800000000000006,{"$error":"#VALUE!"},5.6800000000000006,{"$error":"#VALUE!"},{"$f":"+Y63","v":5.68},{"$f":"+Z63","v":{"$error":"#VALUE!"}},{"$f":"+AA63","v":5.6800000000000006},{"$f":"+AB63","v":{"$error":"#VALUE!"}},{"$f":"+AC63","v":5.6800000000000006},0,{"$f":"+AK62","v":6},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"$G$54^2+AM63^2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"$E$51/(PI())*(ATAN(($E$56*$G$54)/(AM63*SQRT(AP63)))-$E$56*$G$54*AM63/(AO63*SQRT(AP63)))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"($E$51/(PI()))*(ATAN(($E$56*$E$55)/(AS63*SQRT(AV63)))-$E$56*$E$55*AS63/(AU63*SQRT(AV63)))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},0.12636570765911159]
["Presjek XVIII-XVIII",null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+G63-$D$58","v":5.3599999999999994},{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$65","v":5.36},{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},{"$f":"+Y64","v":5.3599999999999994},{"$f":"+Z64","v":{"$error":"#VALUE!"}},{"$f":"+AA64","v":5.36},0,{"$f":"+AI63","v":5.6800000000000006},0,0,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"$G$54^2+AM64^2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"$E$51/(PI())*(ATAN(($E$56*$G$54)/(AM64*SQRT(AP64)))-$E$56*$G$54*AM64/(AO64*SQRT(AP64)))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0.17741388044808692]
["Presjek XVII-XVII",null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$64","v":5.04},{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},{"$f":"+Y65","v":5.0399999999999991},0,{"$f":"+AG64","v":5.36},0,0,0,0,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"$G$54^2+AM65^2","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"$E$51/(PI())*(ATAN(($E$56*$G$54)/(AM65*SQRT(AP65)))-$E$56*$G$54*AM65/(AO65*SQRT(AP65)))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0.20915530331904852]
["Presjek XVI-XVI",null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$63","v":4.72},{"$error":"#VALUE!"},4.72,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.72,{"$error":"#VALUE!"},4.72,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.72,{"$error":"#VALUE!"},4.72,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.72,{"$error":"#VALUE!"},4.72,0,{"$f":"+AE65","v":5.0399999999999991},0,0,0,0,0,0,null,{"$error":"#VALUE!"},{"$f":"$E$55^2+AM66^2","v":{"$error":"#VALUE!"}},{"$f":"$G$54^2+AM66^2","v":{"$error":"#VALUE!"}},{"$f":"$G$56^2+AM66^2","v":{"$error":"#VALUE!"}},{"$f":"$E$51/(PI())*(ATAN(($E$56*$G$54)/(AM66*SQRT(AP66)))-$E$56*$G$54*AM66/(AO66*SQRT(AP66)))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0.22245033451844476]
["Presjek XV-XV",null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$62","v":4.4000000000000004},{"$error":"#VALUE!"},4.4000000000000004,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.4000000000000004,{"$error":"#VALUE!"},4.4000000000000004,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.4000000000000004,{"$error":"#VALUE!"},4.4000000000000004,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.4000000000000004,0,{"$f":"+AC66","v":4.72},0,0,0,0,{"$f":"+AB67","v":0},0,{"$f":"+AD67","v":0},0,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0.2209024792477936]
["Presjek XIV-XIV",null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$61","v":4.08},{"$error":"#VALUE!"},4.08,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.08,{"$error":"#VALUE!"},4.08,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.08,{"$error":"#VALUE!"},4.08,{"$error":"#VALUE!"},4.0799999999999983,0,{"$f":"+AA67","v":4.4000000000000004},0,0,0,0,{"$f":"+Z68","v":0},0,0,{"$f":"+AC68","v":0},0,0,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0.20908832492090335]
["Presjek XIII-XIII",null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$60","v":3.76},{"$error":"#VALUE!"},3.76,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.76,{"$error":"#VALUE!"},3.76,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.76,{"$error":"#VALUE!"},3.76,0,{"$f":"+Y68","v":4.0799999999999983},0,0,0,0,{"$f":"+X69","v":0},0,0,0,0,0,0,0,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0.19127487920258923]
["Presjek  XII-XII",null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$59","v":3.44},{"$error":"#VALUE!"},3.44,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.44,{"$error":"#VALUE!"},3.44,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.44,0,{"$f":"+W69","v":3.76},0,0,0,0,{"$f":"+V70","v":0},0,0,0,0,0,0,0,0,0,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0.17080159233580933]
["Presjek XI-XI",null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$58","v":3.14},{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.1199999999999988,0,{"$f":"+U70","v":3.44},0,0,0,0,{"$f":"+T71","v":0},0,0,0,0,0,0,0,0,0,0,0,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0.14996411649646108]
["Presjek X-X",null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$57","v":2.8},{"$error":"#VALUE!"},2.8,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.8,{"$error":"#VALUE!"},2.8,0,{"$f":"+S71","v":3.1199999999999988},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0.13016182520507658]
["Presjek IX-IX",null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$56","v":2.48},{"$error":"#VALUE!"},2.48,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.48,0,{"$f":"+Q72","v":2.8},0,0,0,0,{"$f":"+P73","v":0},0,{"$f":"+R73","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0.11213013910759548]
["Presjek VIII-VIII",null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},2.1599999999999993,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$55","v":2.16},{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},2.1599999999999993,0,{"$f":"+O73","v":2.48},0,{"$f":"+K74","v":2.16},0,0,{"$f":"+N74","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},9.6161331192147204E-2]
["Presjek VII-VII",null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},1.8399999999999992,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$54","v":1.84},{"$error":"#VALUE!"},1.84,0,{"$f":"+M74","v":2.1599999999999993},0,{"$f":"+I75","v":1.84},0,1.84,{"$f":"+L75","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},8.2277587147567721E-2]
["Presjek VI-VI",null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},1.5199999999999991,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$53","v":1.52},0,{"$f":"+K75","v":1.84},0,{"$f":"+G76","v":1.5199999999999991},0,{"$f":"+I76","v":1.52},{"$f":"+J76","v":0},1.84,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},7.0352325254187276E-2]
["Presjek III -III",null,null,{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},1.1999999999999991,0,{"$f":"+I76","v":1.52},0,{"$f":"+K76","v":1.84},0,{"$f":"+G77","v":1.1999999999999991},{"$f":"+H77","v":0},{"$f":"+I77","v":1.52},0,1.84,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},6.0188716745155732E-2]
["IV-IV=Mmin",null,null,null,null,{"$f":"+F38","v":0},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},0,{"$f":"+G78","v":1.2},0,{"$f":"+I78","v":1.2},0,{"$f":"+G78","v":1.2},0,{"$f":"+I78","v":1.2},0,1.2,0,{"$f":"+M78","v":1.2},0,{"$f":"+O78","v":1.2},0,{"$f":"+Q78","v":1.2},0,{"$f":"+S78","v":1.2},0,{"$f":"+U78","v":1.2},0,{"$f":"+W78","v":1.2},0,{"$f":"+Y78","v":1.2},0,{"$f":"+AA78","v":1.2},0,1.2,0,{"$f":"+AE78","v":1.2}]
["V-V = Mmax",null,null,null,null,{"$f":"+F39","v":0},{"$f":"+G59","v":{"$error":"#VALUE!"}},0,{"$f":"+G79","v":{"$error":"#VALUE!"}},0,{"$f":"+G79","v":{"$error":"#VALUE!"}},0,{"$f":"+G79","v":{"$error":"#VALUE!"}},0,{"$f":"+I79","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"}]
[null,null,null,"Ukupni pritisak",null,"SQhi=",{"$f":"+G83","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I83","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K83","v":{"$error":"#VALUE!"}},{"$f":"+F80","v":"SQhi="},{"$f":"+M83","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+O83","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Q83","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+S83","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+U83","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+W83","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Y83","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AA83","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AC83","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AE83","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AG83","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AI83","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AK83","v":{"$error":"#VALUE!"}}]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G85","v":{"$error":"#VALUE!"}},"y=",{"$f":"+I85","v":{"$error":"#VALUE!"}},"y=",{"$f":"+K85","v":{"$error":"#VALUE!"}}," y=",{"$f":"+M85","v":{"$error":"#VALUE!"}},"y=",{"$f":"+O85","v":{"$error":"#VALUE!"}},"y=",{"$f":"+Q85","v":{"$error":"#VALUE!"}}," y=",{"$f":"+S85","v":{"$error":"#VALUE!"}},"y=",{"$f":"+U85","v":{"$error":"#VALUE!"}},"y=",{"$f":"+W85","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Y85","v":{"$error":"#VALUE!"}},"y=",{"$f":"+AA85","v":{"$error":"#VALUE!"}},"y=",{"$f":"+AC85","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AE85","v":{"$error":"#VALUE!"}},"y=",{"$f":"+AG85","v":{"$error":"#VALUE!"}},"y=",{"$f":"+AI85","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AK85","v":{"$error":"#VALUE!"}}]
[null,null,null,"krak za presjek III -III",null,"z=",{"$f":"+G81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+O81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Q81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+S81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+U81-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}},"z=",{"$f":"+W81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Y81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AA81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AC81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AE81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AG81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AI81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AK81-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,"F=",{"$f":"-0.5*((F60*G61-F61*G60)+(F61*G62-F62*G61)+\n (F62*G63-F63*G62)+\n(F63*G64-F64*G63)+\n(F64*G65-F65*G64)+\n(F65*G66-F66*G65)+\n(F66*G67-F67*G66)+\n(F67*G68-F68*G67)+\n(F68*G69-F69*G68)+\n(F69*G70-F70*G69)+\n(F70*G71-F71*G70)+\n(F71*G72-F72*G71)+\n(F72*G73-F73*G72)+\n(F73*G74-F74*G73)+\n(F74*G75-F75*G74)+\n(F75*G76-F76*G75)+\n(F76*G77-F77*G76)+\n(F77*G78-F78*G77)+\n(F78*G79-F79*G78))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((H60*I61-H61*I60)+(H61*I62-H62*I61)+\n (H62*I63-H63*I62)+\n(H63*I64-H64*I63)+\n(H64*I65-H65*I64)+\n(H65*I66-H66*I65)+\n(H66*I67-H67*I66)+\n(H67*I68-H68*I67)+\n(H68*I69-H69*I68)+\n(H69*I70-H70*I69)+\n(H70*I71-H71*I70)+\n(H71*I72-H72*I71)+\n(H72*I73-H73*I72)+\n(H73*I74-H74*I73)+\n(H74*I75-H75*I74)+\n(H75*I76-H76*I75)+\n(H76*I77-H77*I76)+\n(H77*I78-H78*I77)+\n(H78*I79-H79*I78))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((J60*K61-J61*K60)+(J61*K62-J62*K61)+\n (J62*K63-J63*K62)+\n(J63*K64-J64*K63)+\n(J64*K65-J65*K64)+\n(J65*K66-J66*K65)+\n(J66*K67-J67*K66)+\n(J67*K68-J68*K67)+\n(J68*K69-J69*K68)+\n(J69*K70-J70*K69)+\n(J70*K71-J71*K70)+\n(J71*K72-J72*K71)+\n(J72*K73-J73*K72)+\n(J73*K74-J74*K73)+\n(J74*K75-J75*K74)+\n(J75*K76-J76*K75)+\n(J76*K77-J77*K76)+\n(J77*K78-J78*K77)+\n(J78*K79-J79*K78))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((L60*M61-L61*M60)+(L61*M62-L62*M61)+\n (L62*M63-L63*M62)+\n(L63*M64-L64*M63)+\n(L64*M65-L65*M64)+\n(L65*M66-L66*M65)+\n(L66*M67-L67*M66)+\n(L67*M68-L68*M67)+\n(L68*M69-L69*M68)+\n(L69*M70-L70*M69)+\n(L70*M71-L71*M70)+\n(L71*M72-L72*M71)+\n(L72*M73-L73*M72)+\n(L73*M74-L74*M73)+\n(L74*M75-L75*M74)+\n(L75*M76-L76*M75)+\n(L76*M77-L77*M76)+\n(L77*M78-L78*M77)+\n(L78*M79-L79*M78))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((N60*O61-N61*O60)+(N61*O62-N62*O61)+\n (N62*O63-N63*O62)+\n(N63*O64-N64*O63)+\n(N64*O65-N65*O64)+\n(N65*O66-N66*O65)+\n(N66*O67-N67*O66)+\n(N67*O68-N68*O67)+\n(N68*O69-N69*O68)+\n(N69*O70-N70*O69)+\n(N70*O71-N71*O70)+\n(N71*O72-N72*O71)+\n(N72*O73-N73*O72)+\n(N73*O74-N74*O73)+\n(N74*O75-N75*O74)+\n(N75*O76-N76*O75)+\n(N76*O77-N77*O76)+\n(N77*O78-N78*O77)+\n(N78*O79-N79*O78))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((P60*Q61-P61*Q60)+(P61*Q62-P62*Q61)+\n (P62*Q63-P63*Q62)+\n(P63*Q64-P64*Q63)+\n(P64*Q65-P65*Q64)+\n(P65*Q66-P66*Q65)+\n(P66*Q67-P67*Q66)+\n(P67*Q68-P68*Q67)+\n(P68*Q69-P69*Q68)+\n(P69*Q70-P70*Q69)+\n(P70*Q71-P71*Q70)+\n(P71*Q72-P72*Q71)+\n(P72*Q73-P73*Q72)+\n(P73*Q74-P74*Q73)+\n(P74*Q75-P75*Q74)+\n(P75*Q76-P76*Q75)+\n(P76*Q77-P77*Q76)+\n(P77*Q78-P78*Q77)+\n(P78*Q79-P79*Q78))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((R60*S61-R61*S60)+(R61*S62-R62*S61)+\n (R62*S63-R63*S62)+\n(R63*S64-R64*S63)+\n(R64*S65-R65*S64)+\n(R65*S66-R66*S65)+\n(R66*S67-R67*S66)+\n(R67*S68-R68*S67)+\n(R68*S69-R69*S68)+\n(R69*S70-R70*S69)+\n(R70*S71-R71*S70)+\n(R71*S72-R72*S71)+\n(R72*S73-R73*S72)+\n(R73*S74-R74*S73)+\n(R74*S75-R75*S74)+\n(R75*S76-R76*S75)+\n(R76*S77-R77*S76)+\n(R77*S78-R78*S77)+\n(R78*S79-R79*S78))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((T60*U61-T61*U60)+(T61*U62-T62*U61)+\n (T62*U63-T63*U62)+\n(T63*U64-T64*U63)+\n(T64*U65-T65*U64)+\n(T65*U66-T66*U65)+\n(T66*U67-T67*U66)+\n(T67*U68-T68*U67)+\n(T68*U69-T69*U68)+\n(T69*U70-T70*U69)+\n(T70*U71-T71*U70)+\n(T71*U72-T72*U71)+\n(T72*U73-T73*U72)+\n(T73*U74-T74*U73)+\n(T74*U75-T75*U74)+\n(T75*U76-T76*U75)+\n(T76*U77-T77*U76)+\n(T77*U78-T78*U77)+\n(T78*U79-T79*U78))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((V60*W61-V61*W60)+(V61*W62-V62*W61)+\n (V62*W63-V63*W62)+\n(V63*W64-V64*W63)+\n(V64*W65-V65*W64)+\n(V65*W66-V66*W65)+\n(V66*W67-V67*W66)+\n(V67*W68-V68*W67)+\n(V68*W69-V69*W68)+\n(V69*W70-V70*W69)+\n(V70*W71-V71*W70)+\n(V71*W72-V72*W71)+\n(V72*W73-V73*W72)+\n(V73*W74-V74*W73)+\n(V74*W75-V75*W74)+\n(V75*W76-V76*W75)+\n(V76*W77-V77*W76)+\n(V77*W78-V78*W77)+\n(V78*W79-V79*W78))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((X60*Y61-X61*Y60)+(X61*Y62-X62*Y61)+\n (X62*Y63-X63*Y62)+\n(X63*Y64-X64*Y63)+\n(X64*Y65-X65*Y64)+\n(X65*Y66-X66*Y65)+\n(X66*Y67-X67*Y66)+\n(X67*Y68-X68*Y67)+\n(X68*Y69-X69*Y68)+\n(X69*Y70-X70*Y69)+\n(X70*Y71-X71*Y70)+\n(X71*Y72-X72*Y71)+\n(X72*Y73-X73*Y72)+\n(X73*Y74-X74*Y73)+\n(X74*Y75-X75*Y74)+\n(X75*Y76-X76*Y75)+\n(X76*Y77-X77*Y76)+\n(X77*Y78-X78*Y77)+\n(X78*Y79-X79*Y78))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((Z60*AA61-Z61*AA60)+(Z61*AA62-Z62*AA61)+\n (Z62*AA63-Z63*AA62)+\n(Z63*AA64-Z64*AA63)+\n(Z64*AA65-Z65*AA64)+\n(Z65*AA66-Z66*AA65)+\n(Z66*AA67-Z67*AA66)+\n(Z67*AA68-Z68*AA67)+\n(Z68*AA69-Z69*AA68)+\n(Z69*AA70-Z70*AA69)+\n(Z70*AA71-Z71*AA70)+\n(Z71*AA72-Z72*AA71)+\n(Z72*AA73-Z73*AA72)+\n(Z73*AA74-Z74*AA73)+\n(Z74*AA75-Z75*AA74)+\n(Z75*AA76-Z76*AA75)+\n(Z76*AA77-Z77*AA76)+\n(Z77*AA78-Z78*AA77)+\n(Z78*AA79-Z79*AA78))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AB60*AC61-AB61*AC60)+(AB61*AC62-AB62*AC61)+\n (AB62*AC63-AB63*AC62)+\n(AB63*AC64-AB64*AC63)+\n(AB64*AC65-AB65*AC64)+\n(AB65*AC66-AB66*AC65)+\n(AB66*AC67-AB67*AC66)+\n(AB67*AC68-AB68*AC67)+\n(AB68*AC69-AB69*AC68)+\n(AB69*AC70-AB70*AC69)+\n(AB70*AC71-AB71*AC70)+\n(AB71*AC72-AB72*AC71)+\n(AB72*AC73-AB73*AC72)+\n(AB73*AC74-AB74*AC73)+\n(AB74*AC75-AB75*AC74)+\n(AB75*AC76-AB76*AC75)+\n(AB76*AC77-AB77*AC76)+\n(AB77*AC78-AB78*AC77)+\n(AB78*AC79-AB79*AC78))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AD60*AE61-AD61*AE60)+(AD61*AE62-AD62*AE61)+\n (AD62*AE63-AD63*AE62)+\n(AD63*AE64-AD64*AE63)+\n(AD64*AE65-AD65*AE64)+\n(AD65*AE66-AD66*AE65)+\n(AD66*AE67-AD67*AE66)+\n(AD67*AE68-AD68*AE67)+\n(AD68*AE69-AD69*AE68)+\n(AD69*AE70-AD70*AE69)+\n(AD70*AE71-AD71*AE70)+\n(AD71*AE72-AD72*AE71)+\n(AD72*AE73-AD73*AE72)+\n(AD73*AE74-AD74*AE73)+\n(AD74*AE75-AD75*AE74)+\n(AD75*AE76-AD76*AE75)+\n(AD76*AE77-AD77*AE76)+\n(AD77*AE78-AD78*AE77)+\n(AD78*AE79-AD79*AE78))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AF60*AG61-AF61*AG60)+(AF61*AG62-AF62*AG61)+\n (AF62*AG63-AF63*AG62)+\n(AF63*AG64-AF64*AG63)+\n(AF64*AG65-AF65*AG64)+\n(AF65*AG66-AF66*AG65)+\n(AF66*AG67-AF67*AG66)+\n(AF67*AG68-AF68*AG67)+\n(AF68*AG69-AF69*AG68)+\n(AF69*AG70-AF70*AG69)+\n(AF70*AG71-AF71*AG70)+\n(AF71*AG72-AF72*AG71)+\n(AF72*AG73-AF73*AG72)+\n(AF73*AG74-AF74*AG73)+\n(AF74*AG75-AF75*AG74)+\n(AF75*AG76-AF76*AG75)+\n(AF76*AG77-AF77*AG76)+\n(AF77*AG78-AF78*AG77)+\n(AF78*AG79-AF79*AG78))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AH60*AI61-AH61*AI60)+(AH61*AI62-AH62*AI61)+\n (AH62*AI63-AH63*AI62)+\n(AH63*AI64-AH64*AI63)+\n(AH64*AI65-AH65*AI64)+\n(AH65*AI66-AH66*AI65)+\n(AH66*AI67-AH67*AI66)+\n(AH67*AI68-AH68*AI67)+\n(AH68*AI69-AH69*AI68)+\n(AH69*AI70-AH70*AI69)+\n(AH70*AI71-AH71*AI70)+\n(AH71*AI72-AH72*AI71)+\n(AH72*AI73-AH73*AI72)+\n(AH73*AI74-AH74*AI73)+\n(AH74*AI75-AH75*AI74)+\n(AH75*AI76-AH76*AI75)+\n(AH76*AI77-AH77*AI76)+\n(AH77*AI78-AH78*AI77)+\n(AH78*AI79-AH79*AI78))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AJ60*AK61-AJ61*AK60)+(AJ61*AK62-AJ62*AK61)+\n (AJ62*AK63-AJ63*AK62)+\n(AJ63*AK64-AJ64*AK63)+\n(AJ64*AK65-AJ65*AK64)+\n(AJ65*AK66-AJ66*AK65)+\n(AJ66*AK67-AJ67*AK66)+\n(AJ67*AK68-AJ68*AK67)+\n(AJ68*AK69-AJ69*AK68)+\n(AJ69*AK70-AJ70*AK69)+\n(AJ70*AK71-AJ71*AK70)+\n(AJ71*AK72-AJ72*AK71)+\n(AJ72*AK73-AJ73*AK72)+\n(AJ73*AK74-AJ74*AK73)+\n(AJ74*AK75-AJ75*AK74)+\n(AJ75*AK76-AJ76*AK75)+\n(AJ76*AK77-AJ77*AK76)+\n(AJ77*AK78-AJ78*AK77)+\n(AJ78*AK79-AJ79*AK78))","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,"x=",0.1,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0]
[null,null,null,null,null,"y=",{"$f":"+IF(G83=0,0,-((F60*G61-F61*G60)*(G60+G61)+(F61*G62-F62*G61)*(G61+G62)+\n(F62*G63-F63*G62)*(G62+G63)+\n(F63*G64-F64*G63)*(G63+G64)+\n(F64*G65-F65*G64)*(G64+G65)+\n(F65*G66-F66*G65)*(G65+G66)+\n(F66*G67-F67*G66)*(G66+G67)+\n(F67*G68-F68*G67)*(G67+G68)+\n(F68*G69-F69*G68)*(G68+G69)+\n(F69*G70-F70*G69)*(G69+G70)+\n(F70*G71-F71*G70)*(G70+G71)+\n(F71*G72-F72*G71)*(G71+G72)+\n(F72*G73-F73*G72)*(G72+G73)+\n(F73*G74-F74*G73)*(G73+G74)+\n(F74*G75-F75*G74)*(G74+G75)+\n(F75*G76-F76*G75)*(G75+G76)+\n(F76*G77-F77*G76)*(G76+G77)+\n(F77*G78-F78*G77)*(G77+G78)+\n(F78*G79-F79*G78)*(G78+G79))/6/G83)","v":{"$error":"#VALUE!"}},0,{"$f":"+IF(I83=0,0,-((H60*I61-H61*I60)*(I60+I61)+(H61*I62-H62*I61)*(I61+I62)+\n(H62*I63-H63*I62)*(I62+I63)+\n(H63*I64-H64*I63)*(I63+I64)+\n(H64*I65-H65*I64)*(I64+I65)+\n(H65*I66-H66*I65)*(I65+I66)+\n(H66*I67-H67*I66)*(I66+I67)+\n(H67*I68-H68*I67)*(I67+I68)+\n(H68*I69-H69*I68)*(I68+I69)+\n(H69*I70-H70*I69)*(I69+I70)+\n(H70*I71-H71*I70)*(I70+I71)+\n(H71*I72-H72*I71)*(I71+I72)+\n(H72*I73-H73*I72)*(I72+I73)+\n(H73*I74-H74*I73)*(I73+I74)+\n(H74*I75-H75*I74)*(I74+I75)+\n(H75*I76-H76*I75)*(I75+I76)+\n(H76*I77-H77*I76)*(I76+I77)+\n(H77*I78-H78*I77)*(I77+I78)+\n(H78*I79-H79*I78)*(I78+I79))/6/I83)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(K83=0,0,-((J60*K61-J61*K60)*(K60+K61)+(J61*K62-J62*K61)*(K61+K62)+\n(J62*K63-J63*K62)*(K62+K63)+\n(J63*K64-J64*K63)*(K63+K64)+\n(J64*K65-J65*K64)*(K64+K65)+\n(J65*K66-J66*K65)*(K65+K66)+\n(J66*K67-J67*K66)*(K66+K67)+\n(J67*K68-J68*K67)*(K67+K68)+\n(J68*K69-J69*K68)*(K68+K69)+\n(J69*K70-J70*K69)*(K69+K70)+\n(J70*K71-J71*K70)*(K70+K71)+\n(J71*K72-J72*K71)*(K71+K72)+\n(J72*K73-J73*K72)*(K72+K73)+\n(J73*K74-J74*K73)*(K73+K74)+\n(J74*K75-J75*K74)*(K74+K75)+\n(J75*K76-J76*K75)*(K75+K76)+\n(J76*K77-J77*K76)*(K76+K77)+\n(J77*K78-J78*K77)*(K77+K78)+\n(J78*K79-J79*K78)*(K78+K79))/6/K83)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(M83=0,0,-((L60*M61-L61*M60)*(M60+M61)+(L61*M62-L62*M61)*(M61+M62)+\n(L62*M63-L63*M62)*(M62+M63)+\n(L63*M64-L64*M63)*(M63+M64)+\n(L64*M65-L65*M64)*(M64+M65)+\n(L65*M66-L66*M65)*(M65+M66)+\n(L66*M67-L67*M66)*(M66+M67)+\n(L67*M68-L68*M67)*(M67+M68)+\n(L68*M69-L69*M68)*(M68+M69)+\n(L69*M70-L70*M69)*(M69+M70)+\n(L70*M71-L71*M70)*(M70+M71)+\n(L71*M72-L72*M71)*(M71+M72)+\n(L72*M73-L73*M72)*(M72+M73)+\n(L73*M74-L74*M73)*(M73+M74)+\n(L74*M75-L75*M74)*(M74+M75)+\n(L75*M76-L76*M75)*(M75+M76)+\n(L76*M77-L77*M76)*(M76+M77)+\n(L77*M78-L78*M77)*(M77+M78)+\n(L78*M79-L79*M78)*(M78+M79))/6/M83)","v":{"$error":"#VALUE!"}},0,{"$f":"+IF(O83=0,0,-((N60*O61-N61*O60)*(O60+O61)+(N61*O62-N62*O61)*(O61+O62)+\n(N62*O63-N63*O62)*(O62+O63)+\n(N63*O64-N64*O63)*(O63+O64)+\n(N64*O65-N65*O64)*(O64+O65)+\n(N65*O66-N66*O65)*(O65+O66)+\n(N66*O67-N67*O66)*(O66+O67)+\n(N67*O68-N68*O67)*(O67+O68)+\n(N68*O69-N69*O68)*(O68+O69)+\n(N69*O70-N70*O69)*(O69+O70)+\n(N70*O71-N71*O70)*(O70+O71)+\n(N71*O72-N72*O71)*(O71+O72)+\n(N72*O73-N73*O72)*(O72+O73)+\n(N73*O74-N74*O73)*(O73+O74)+\n(N74*O75-N75*O74)*(O74+O75)+\n(N75*O76-N76*O75)*(O75+O76)+\n(N76*O77-N77*O76)*(O76+O77)+\n(N77*O78-N78*O77)*(O77+O78)+\n(N78*O79-N79*O78)*(O78+O79))/6/O83)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Q83=0,0,-((P60*Q61-P61*Q60)*(Q60+Q61)+(P61*Q62-P62*Q61)*(Q61+Q62)+\n(P62*Q63-P63*Q62)*(Q62+Q63)+\n(P63*Q64-P64*Q63)*(Q63+Q64)+\n(P64*Q65-P65*Q64)*(Q64+Q65)+\n(P65*Q66-P66*Q65)*(Q65+Q66)+\n(P66*Q67-P67*Q66)*(Q66+Q67)+\n(P67*Q68-P68*Q67)*(Q67+Q68)+\n(P68*Q69-P69*Q68)*(Q68+Q69)+\n(P69*Q70-P70*Q69)*(Q69+Q70)+\n(P70*Q71-P71*Q70)*(Q70+Q71)+\n(P71*Q72-P72*Q71)*(Q71+Q72)+\n(P72*Q73-P73*Q72)*(Q72+Q73)+\n(P73*Q74-P74*Q73)*(Q73+Q74)+\n(P74*Q75-P75*Q74)*(Q74+Q75)+\n(P75*Q76-P76*Q75)*(Q75+Q76)+\n(P76*Q77-P77*Q76)*(Q76+Q77)+\n(P77*Q78-P78*Q77)*(Q77+Q78)+\n(P78*Q79-P79*Q78)*(Q78+Q79))/6/Q83)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(S83=0,0,-((R60*S61-R61*S60)*(S60+S61)+(R61*S62-R62*S61)*(S61+S62)+\n(R62*S63-R63*S62)*(S62+S63)+\n(R63*S64-R64*S63)*(S63+S64)+\n(R64*S65-R65*S64)*(S64+S65)+\n(R65*S66-R66*S65)*(S65+S66)+\n(R66*S67-R67*S66)*(S66+S67)+\n(R67*S68-R68*S67)*(S67+S68)+\n(R68*S69-R69*S68)*(S68+S69)+\n(R69*S70-R70*S69)*(S69+S70)+\n(R70*S71-R71*S70)*(S70+S71)+\n(R71*S72-R72*S71)*(S71+S72)+\n(R72*S73-R73*S72)*(S72+S73)+\n(R73*S74-R74*S73)*(S73+S74)+\n(R74*S75-R75*S74)*(S74+S75)+\n(R75*S76-R76*S75)*(S75+S76)+\n(R76*S77-R77*S76)*(S76+S77)+\n(R77*S78-R78*S77)*(S77+S78)+\n(R78*S79-R79*S78)*(S78+S79))/6/S83)","v":{"$error":"#VALUE!"}},0,{"$f":"+IF(U83=0,0,-((T60*U61-T61*U60)*(U60+U61)+(T61*U62-T62*U61)*(U61+U62)+\n(T62*U63-T63*U62)*(U62+U63)+\n(T63*U64-T64*U63)*(U63+U64)+\n(T64*U65-T65*U64)*(U64+U65)+\n(T65*U66-T66*U65)*(U65+U66)+\n(T66*U67-T67*U66)*(U66+U67)+\n(T67*U68-T68*U67)*(U67+U68)+\n(T68*U69-T69*U68)*(U68+U69)+\n(T69*U70-T70*U69)*(U69+U70)+\n(T70*U71-T71*U70)*(U70+U71)+\n(T71*U72-T72*U71)*(U71+U72)+\n(T72*U73-T73*U72)*(U72+U73)+\n(T73*U74-T74*U73)*(U73+U74)+\n(T74*U75-T75*U74)*(U74+U75)+\n(T75*U76-T76*U75)*(U75+U76)+\n(T76*U77-T77*U76)*(U76+U77)+\n(T77*U78-T78*U77)*(U77+U78)+\n(T78*U79-T79*U78)*(U78+U79))/6/U83)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(W83=0,0,-((V60*W61-V61*W60)*(W60+W61)+(V61*W62-V62*W61)*(W61+W62)+\n(V62*W63-V63*W62)*(W62+W63)+\n(V63*W64-V64*W63)*(W63+W64)+\n(V64*W65-V65*W64)*(W64+W65)+\n(V65*W66-V66*W65)*(W65+W66)+\n(V66*W67-V67*W66)*(W66+W67)+\n(V67*W68-V68*W67)*(W67+W68)+\n(V68*W69-V69*W68)*(W68+W69)+\n(V69*W70-V70*W69)*(W69+W70)+\n(V70*W71-V71*W70)*(W70+W71)+\n(V71*W72-V72*W71)*(W71+W72)+\n(V72*W73-V73*W72)*(W72+W73)+\n(V73*W74-V74*W73)*(W73+W74)+\n(V74*W75-V75*W74)*(W74+W75)+\n(V75*W76-V76*W75)*(W75+W76)+\n(V76*W77-V77*W76)*(W76+W77)+\n(V77*W78-V78*W77)*(W77+W78)+\n(V78*W79-V79*W78)*(W78+W79))/6/W83)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Y83=0,0,-((X60*Y61-X61*Y60)*(Y60+Y61)+(X61*Y62-X62*Y61)*(Y61+Y62)+\n(X62*Y63-X63*Y62)*(Y62+Y63)+\n(X63*Y64-X64*Y63)*(Y63+Y64)+\n(X64*Y65-X65*Y64)*(Y64+Y65)+\n(X65*Y66-X66*Y65)*(Y65+Y66)+\n(X66*Y67-X67*Y66)*(Y66+Y67)+\n(X67*Y68-X68*Y67)*(Y67+Y68)+\n(X68*Y69-X69*Y68)*(Y68+Y69)+\n(X69*Y70-X70*Y69)*(Y69+Y70)+\n(X70*Y71-X71*Y70)*(Y70+Y71)+\n(X71*Y72-X72*Y71)*(Y71+Y72)+\n(X72*Y73-X73*Y72)*(Y72+Y73)+\n(X73*Y74-X74*Y73)*(Y73+Y74)+\n(X74*Y75-X75*Y74)*(Y74+Y75)+\n(X75*Y76-X76*Y75)*(Y75+Y76)+\n(X76*Y77-X77*Y76)*(Y76+Y77)+\n(X77*Y78-X78*Y77)*(Y77+Y78)+\n(X78*Y79-X79*Y78)*(Y78+Y79))/6/Y83)","v":{"$error":"#VALUE!"}},0,{"$f":"+IF(AA83=0,0,-((Z60*AA61-Z61*AA60)*(AA60+AA61)+(Z61*AA62-Z62*AA61)*(AA61+AA62)+\n(Z62*AA63-Z63*AA62)*(AA62+AA63)+\n(Z63*AA64-Z64*AA63)*(AA63+AA64)+\n(Z64*AA65-Z65*AA64)*(AA64+AA65)+\n(Z65*AA66-Z66*AA65)*(AA65+AA66)+\n(Z66*AA67-Z67*AA66)*(AA66+AA67)+\n(Z67*AA68-Z68*AA67)*(AA67+AA68)+\n(Z68*AA69-Z69*AA68)*(AA68+AA69)+\n(Z69*AA70-Z70*AA69)*(AA69+AA70)+\n(Z70*AA71-Z71*AA70)*(AA70+AA71)+\n(Z71*AA72-Z72*AA71)*(AA71+AA72)+\n(Z72*AA73-Z73*AA72)*(AA72+AA73)+\n(Z73*AA74-Z74*AA73)*(AA73+AA74)+\n(Z74*AA75-Z75*AA74)*(AA74+AA75)+\n(Z75*AA76-Z76*AA75)*(AA75+AA76)+\n(Z76*AA77-Z77*AA76)*(AA76+AA77)+\n(Z77*AA78-Z78*AA77)*(AA77+AA78)+\n(Z78*AA79-Z79*AA78)*(AA78+AA79))/6/AA83)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AC83=0,0,-((AB60*AC61-AB61*AC60)*(AC60+AC61)+(AB61*AC62-AB62*AC61)*(AC61+AC62)+\n(AB62*AC63-AB63*AC62)*(AC62+AC63)+\n(AB63*AC64-AB64*AC63)*(AC63+AC64)+\n(AB64*AC65-AB65*AC64)*(AC64+AC65)+\n(AB65*AC66-AB66*AC65)*(AC65+AC66)+\n(AB66*AC67-AB67*AC66)*(AC66+AC67)+\n(AB67*AC68-AB68*AC67)*(AC67+AC68)+\n(AB68*AC69-AB69*AC68)*(AC68+AC69)+\n(AB69*AC70-AB70*AC69)*(AC69+AC70)+\n(AB70*AC71-AB71*AC70)*(AC70+AC71)+\n(AB71*AC72-AB72*AC71)*(AC71+AC72)+\n(AB72*AC73-AB73*AC72)*(AC72+AC73)+\n(AB73*AC74-AB74*AC73)*(AC73+AC74)+\n(AB74*AC75-AB75*AC74)*(AC74+AC75)+\n(AB75*AC76-AB76*AC75)*(AC75+AC76)+\n(AB76*AC77-AB77*AC76)*(AC76+AC77)+\n(AB77*AC78-AB78*AC77)*(AC77+AC78)+\n(AB78*AC79-AB79*AC78)*(AC78+AC79))/6/AC83)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AE83=0,0,-((AD60*AE61-AD61*AE60)*(AE60+AE61)+(AD61*AE62-AD62*AE61)*(AE61+AE62)+\n(AD62*AE63-AD63*AE62)*(AE62+AE63)+\n(AD63*AE64-AD64*AE63)*(AE63+AE64)+\n(AD64*AE65-AD65*AE64)*(AE64+AE65)+\n(AD65*AE66-AD66*AE65)*(AE65+AE66)+\n(AD66*AE67-AD67*AE66)*(AE66+AE67)+\n(AD67*AE68-AD68*AE67)*(AE67+AE68)+\n(AD68*AE69-AD69*AE68)*(AE68+AE69)+\n(AD69*AE70-AD70*AE69)*(AE69+AE70)+\n(AD70*AE71-AD71*AE70)*(AE70+AE71)+\n(AD71*AE72-AD72*AE71)*(AE71+AE72)+\n(AD72*AE73-AD73*AE72)*(AE72+AE73)+\n(AD73*AE74-AD74*AE73)*(AE73+AE74)+\n(AD74*AE75-AD75*AE74)*(AE74+AE75)+\n(AD75*AE76-AD76*AE75)*(AE75+AE76)+\n(AD76*AE77-AD77*AE76)*(AE76+AE77)+\n(AD77*AE78-AD78*AE77)*(AE77+AE78)+\n(AD78*AE79-AD79*AE78)*(AE78+AE79))/6/AE83)","v":{"$error":"#VALUE!"}},0,{"$f":"+IF(AG83=0,0,-((AF60*AG61-AF61*AG60)*(AG60+AG61)+(AF61*AG62-AF62*AG61)*(AG61+AG62)+\n(AF62*AG63-AF63*AG62)*(AG62+AG63)+\n(AF63*AG64-AF64*AG63)*(AG63+AG64)+\n(AF64*AG65-AF65*AG64)*(AG64+AG65)+\n(AF65*AG66-AF66*AG65)*(AG65+AG66)+\n(AF66*AG67-AF67*AG66)*(AG66+AG67)+\n(AF67*AG68-AF68*AG67)*(AG67+AG68)+\n(AF68*AG69-AF69*AG68)*(AG68+AG69)+\n(AF69*AG70-AF70*AG69)*(AG69+AG70)+\n(AF70*AG71-AF71*AG70)*(AG70+AG71)+\n(AF71*AG72-AF72*AG71)*(AG71+AG72)+\n(AF72*AG73-AF73*AG72)*(AG72+AG73)+\n(AF73*AG74-AF74*AG73)*(AG73+AG74)+\n(AF74*AG75-AF75*AG74)*(AG74+AG75)+\n(AF75*AG76-AF76*AG75)*(AG75+AG76)+\n(AF76*AG77-AF77*AG76)*(AG76+AG77)+\n(AF77*AG78-AF78*AG77)*(AG77+AG78)+\n(AF78*AG79-AF79*AG78)*(AG78+AG79))/6/AG83)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AI83=0,0,-((AH60*AI61-AH61*AI60)*(AI60+AI61)+(AH61*AI62-AH62*AI61)*(AI61+AI62)+\n(AH62*AI63-AH63*AI62)*(AI62+AI63)+\n(AH63*AI64-AH64*AI63)*(AI63+AI64)+\n(AH64*AI65-AH65*AI64)*(AI64+AI65)+\n(AH65*AI66-AH66*AI65)*(AI65+AI66)+\n(AH66*AI67-AH67*AI66)*(AI66+AI67)+\n(AH67*AI68-AH68*AI67)*(AI67+AI68)+\n(AH68*AI69-AH69*AI68)*(AI68+AI69)+\n(AH69*AI70-AH70*AI69)*(AI69+AI70)+\n(AH70*AI71-AH71*AI70)*(AI70+AI71)+\n(AH71*AI72-AH72*AI71)*(AI71+AI72)+\n(AH72*AI73-AH73*AI72)*(AI72+AI73)+\n(AH73*AI74-AH74*AI73)*(AI73+AI74)+\n(AH74*AI75-AH75*AI74)*(AI74+AI75)+\n(AH75*AI76-AH76*AI75)*(AI75+AI76)+\n(AH76*AI77-AH77*AI76)*(AI76+AI77)+\n(AH77*AI78-AH78*AI77)*(AI77+AI78)+\n(AH78*AI79-AH79*AI78)*(AI78+AI79))/6/AI83)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AK83=0,0,-((AJ60*AK61-AJ61*AK60)*(AK60+AK61)+(AJ61*AK62-AJ62*AK61)*(AK61+AK62)+\n(AJ62*AK63-AJ63*AK62)*(AK62+AK63)+\n(AJ63*AK64-AJ64*AK63)*(AK63+AK64)+\n(AJ64*AK65-AJ65*AK64)*(AK64+AK65)+\n(AJ65*AK66-AJ66*AK65)*(AK65+AK66)+\n(AJ66*AK67-AJ67*AK66)*(AK66+AK67)+\n(AJ67*AK68-AJ68*AK67)*(AK67+AK68)+\n(AJ68*AK69-AJ69*AK68)*(AK68+AK69)+\n(AJ69*AK70-AJ70*AK69)*(AK69+AK70)+\n(AJ70*AK71-AJ71*AK70)*(AK70+AK71)+\n(AJ71*AK72-AJ72*AK71)*(AK71+AK72)+\n(AJ72*AK73-AJ73*AK72)*(AK72+AK73)+\n(AJ73*AK74-AJ74*AK73)*(AK73+AK74)+\n(AJ74*AK75-AJ75*AK74)*(AK74+AK75)+\n(AJ75*AK76-AJ76*AK75)*(AK75+AK76)+\n(AJ76*AK77-AJ77*AK76)*(AK76+AK77)+\n(AJ77*AK78-AJ78*AK77)*(AK77+AK78)+\n(AJ78*AK79-AJ79*AK78)*(AK78+AK79))/6/AK83)","v":{"$error":"#VALUE!"}}]
[]
[]
[]
[null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID "]
[null,"LINIJSKO OPTEREĆENJE",null,null,null,null," (TERZAGHY)"]
[null,null,"LINIJSKO OPTEREĆENJE","Ql =",{"$f":"+'Analiza i dimenzioniranje'!C23","v":20.000001000010002},"kN/m2",{"$f":"+E91/E94","v":20.000001000010002}]
[null,null," visina zida iznad  temelja","H =",{"$f":"+E52","v":{"$error":"#VALUE!"}},"m",{"$f":"+E96","v":6}]
[null,null,"visina opterećenja iznad vrha zida","h =",{"$f":"'C III-V'!X27-'C III-V'!C9","v":{"$error":"#VALUE!"}},"m",{"$f":"SQRT(E96^2+E95^2)","v":6.324555320336759}]
[null,null,"širina linijskog opterećenja","b =",1,"m",{"$f":"E95+E94","v":3}]
[null,null,"udaljenost ruba temelja linijskog opt. od iskopa","D =",{"$f":"+'Analiza i dimenzioniranje'!K28-0.5","v":2},"m"]
[null,null,"1/2 dužine lin. opterećenja","L/2=a=",{"$f":"+'Analiza i dimenzioniranje'!E49/2","v":6},"m",{"$f":"SQRT(G92^2+G94^2)","v":6.7082039324993694}]
[null,null,null,null,null,{"$f":"+ROUND('Analiza i dimenzioniranje'!$E$52,2)","v":1.2},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND('Analiza i dimenzioniranje'!$U$53,2)","v":1.52},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND('Analiza i dimenzioniranje'!$U$54,2)","v":1.84},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND('Analiza i dimenzioniranje'!$U$55,2)","v":2.16},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$56,2)","v":2.48},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$57,2)","v":2.8},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$58,2)","v":3.14},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$59,2)","v":3.44},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$60,2)","v":3.76},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$61,2)","v":4.08},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$62,2)","v":4.4000000000000004},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$63,2)","v":4.72},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$64,2)","v":5.04},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$65,2)","v":5.36},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$66,2)","v":5.68},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$U$67,2)","v":6},{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+$D$58","v":0.32},null,"Presjek III -III",null,"Presjek VI-VI",null,"Presjek VII-VII",null,"Presjek VIII-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"Presjek XIV-XIV",null,"Presjek XV-XV",null,"Presjek XVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX"]
[null,null,null,{"$f":"+D59","v":{"$error":"#VALUE!"}},null,"(sb2-sb1)*2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},"sb1-sb2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},"sb1-sb2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},"(sb2-sb1)*2",{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
[null,null,null,{"$f":"+D60","v":{"$error":"#VALUE!"}},{"$f":"+G$99-G100","v":{"$error":"#VALUE!"}},{"$f":"+F20","v":0},{"$f":"+G99","v":{"$error":"#VALUE!"}},0,{"$f":"+G100","v":{"$error":"#VALUE!"}},0,{"$f":"+I99","v":{"$error":"#VALUE!"}},{"$f":"+F100","v":0},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$f":"+L100","v":0},{"$f":"+M100","v":{"$error":"#VALUE!"}},{"$f":"+N100","v":0},{"$f":"+O100","v":{"$error":"#VALUE!"}},{"$f":"+P100","v":0},{"$f":"+Q100","v":{"$error":"#VALUE!"}},{"$f":"+R100","v":0},{"$f":"+S100","v":{"$error":"#VALUE!"}},{"$f":"+T100","v":0},{"$f":"+U100","v":{"$error":"#VALUE!"}},{"$f":"+V100","v":0},{"$f":"+W100","v":{"$error":"#VALUE!"}},{"$f":"+X100","v":0},{"$f":"+Y100","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$f":"+AI100","v":{"$error":"#VALUE!"}},null,0,{"$f":"$E$95^2+AM100^2","v":4},{"$f":"$G94^2+AM100^2","v":9},{"$f":"$G$96^2+AM100^2","v":45.000000000000007},0,null,{"$f":"+AM100","v":0},{"$f":"$E$96^2+AS100^2","v":36},{"$f":"$E$95^2+AS100^2","v":4},{"$f":"$G$93^2+AS100^2","v":40.000000000000007},0,{"$f":"+(AQ100-AW100)*2","v":0}]
[null,null,null,{"$f":"+G100-G101","v":{"$error":"#VALUE!"}},{"$f":"+G$99-G101","v":{"$error":"#VALUE!"}},{"$f":"+F21","v":0},{"$f":"+G100","v":{"$error":"#VALUE!"}},{"$f":"+F101","v":0},{"$f":"+G101","v":{"$error":"#VALUE!"}},0,{"$f":"+I101","v":{"$error":"#VALUE!"}},{"$f":"+F101","v":0},{"$f":"+G101","v":{"$error":"#VALUE!"}},{"$f":"+H101","v":0},{"$f":"+M101","v":{"$error":"#VALUE!"}},{"$f":"+J101","v":0},{"$f":"+O101","v":{"$error":"#VALUE!"}},0,{"$f":"+Q101","v":{"$error":"#VALUE!"}},0,{"$f":"+S101","v":{"$error":"#VALUE!"}},{"$f":"+P101","v":0},{"$f":"+U101","v":{"$error":"#VALUE!"}},0,{"$f":"+W101","v":{"$error":"#VALUE!"}},0,{"$f":"+Y101","v":{"$error":"#VALUE!"}},0,{"$f":"+AA101","v":{"$error":"#VALUE!"}},0,{"$f":"+AC101","v":{"$error":"#VALUE!"}},{"$f":"+Z101","v":0},{"$f":"+AE101","v":{"$error":"#VALUE!"}},{"$f":"+AB101","v":0},{"$f":"+AG101","v":{"$error":"#VALUE!"}},{"$f":"+AD101","v":0},{"$f":"+AE101","v":{"$error":"#VALUE!"}},null,0,{"$f":"+AN100","v":4},{"$f":"+AO100","v":9},{"$f":"+AP100","v":45.000000000000007},{"$f":"+AQ100","v":0},null,0,{"$f":"+AT100","v":36},{"$f":"+AU100","v":4},{"$f":"+AV100","v":40.000000000000007},0,0]
[null,null,null,{"$f":"+D62","v":{"$error":"#VALUE!"}},{"$f":"+G$99-G102","v":{"$error":"#VALUE!"}},{"$f":"+AX102","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E48","v":6},{"$f":"+F102","v":{"$error":"#VALUE!"}},{"$f":"+G102","v":6},{"$f":"+F102","v":{"$error":"#VALUE!"}},{"$f":"+G102","v":6},{"$f":"+J102","v":{"$error":"#VALUE!"}},6,{"$f":"+J102","v":{"$error":"#VALUE!"}},{"$f":"+I102","v":6},{"$f":"+N102","v":{"$error":"#VALUE!"}},{"$f":"+K102","v":6},{"$error":"#VALUE!"},6,{"$error":"#VALUE!"},6,{"$f":"+T102","v":{"$error":"#VALUE!"}},6,{"$error":"#VALUE!"},6,{"$error":"#VALUE!"},6,{"$error":"#VALUE!"},6,{"$error":"#VALUE!"},{"$f":"+Y102","v":6},{"$f":"+Z102","v":{"$error":"#VALUE!"}},{"$f":"+AA102","v":6},{"$f":"+AB102","v":{"$error":"#VALUE!"}},{"$f":"+AC102","v":6},{"$f":"+AD102","v":{"$error":"#VALUE!"}},{"$f":"+AE102","v":6},null,{"$f":"+D102","v":{"$error":"#VALUE!"}},{"$f":"$E$95^2+AM102^2","v":{"$error":"#VALUE!"}},{"$f":"$G$94^2+AM102^2","v":{"$error":"#VALUE!"}},{"$f":"$G$96^2+AM102^2","v":{"$error":"#VALUE!"}},{"$f":"IF(AM102=0,0,$E$91/(PI())*(ATAN(($E$96*$G$94)/(AM102*SQRT(AP102)))-$E$96*$G$94*AM102/(AO102*SQRT(AP102))))","v":{"$error":"#VALUE!"}},null,{"$f":"+AM102","v":{"$error":"#VALUE!"}},{"$f":"$E$96^2+AS102^2","v":{"$error":"#VALUE!"}},{"$f":"$E$95^2+AS102^2","v":{"$error":"#VALUE!"}},{"$f":"$G$93^2+AS102^2","v":{"$error":"#VALUE!"}},{"$f":"IF(AS102=0,0,($E$91/(PI()))*(ATAN(($E$96*$E$95)/(AS102*SQRT(AV102)))-$E$96*$E$95*AS102/(AU102*SQRT(AV102))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["Presjek X-X",null,null,{"$error":"#VALUE!"},{"$f":"+G$99-G103","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+G102-$D$98","v":5.68},{"$f":"+F103","v":{"$error":"#VALUE!"}},{"$f":"+G103","v":5.68},{"$f":"+F103","v":{"$error":"#VALUE!"}},{"$f":"+G103","v":5.68},{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},5.68,{"$f":"+T103","v":{"$error":"#VALUE!"}},5.68,{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},{"$f":"+Y103","v":5.68},{"$f":"+Z103","v":{"$error":"#VALUE!"}},{"$f":"+AA103","v":5.68},{"$f":"+AB103","v":{"$error":"#VALUE!"}},{"$f":"+AC103","v":5.68},0,{"$f":"+AK102","v":6},null,{"$error":"#VALUE!"},{"$f":"$E$95^2+AM103^2","v":{"$error":"#VALUE!"}},{"$f":"$G$94^2+AM103^2","v":{"$error":"#VALUE!"}},{"$f":"$G$96^2+AM103^2","v":{"$error":"#VALUE!"}},{"$f":"$E$91/(PI())*(ATAN(($E$96*$G$94)/(AM103*SQRT(AP103)))-$E$96*$G$94*AM103/(AO103*SQRT(AP103)))","v":{"$error":"#VALUE!"}},null,{"$f":"+AM103","v":{"$error":"#VALUE!"}},{"$f":"$E$96^2+AS103^2","v":{"$error":"#VALUE!"}},{"$f":"$E$95^2+AS103^2","v":{"$error":"#VALUE!"}},{"$f":"$G$93^2+AS103^2","v":{"$error":"#VALUE!"}},{"$f":"($E$91/(PI()))*(ATAN(($E$96*$E$95)/(AS103*SQRT(AV103)))-$E$96*$E$95*AS103/(AU103*SQRT(AV103)))","v":{"$error":"#VALUE!"}},{"$f":"+(AQ103-AW103)*2","v":{"$error":"#VALUE!"}}]
["Presjek XIX-XIX",null,null,{"$error":"#VALUE!"},{"$f":"+G$20-G106","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},{"$f":"+Y104","v":5.3599999999999994},{"$f":"+Z104","v":{"$error":"#VALUE!"}},{"$f":"+AA104","v":5.3599999999999994},0,{"$f":"+AI103","v":5.68},0,{"$f":"+AE104","v":5.3599999999999994},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XVII-XVII",null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},{"$f":"+Y105","v":5.0399999999999991},0,{"$f":"+AG104","v":5.3599999999999994},0,{"$f":"+AC105","v":5.0399999999999991},0,5.0399999999999991,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XVI-XVI",null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,0,{"$f":"+AE105","v":5.0399999999999991},0,{"$f":"+AA106","v":4.7199999999999989},0,4.7199999999999989,0,5.0399999999999991,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XV-XV",null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,0,{"$f":"+AC106","v":4.7199999999999989},0,{"$f":"+Y107","v":4.3999999999999986},0,4.3999999999999986,{"$f":"+AB107","v":0},4.7199999999999989,{"$f":"+AD107","v":0},4.3999999999999986,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XIV-XIV",null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,0,{"$f":"+AA107","v":4.3999999999999986},0,{"$f":"+W108","v":4.0799999999999983},0,4.0799999999999983,{"$f":"+Z108","v":0},4.3999999999999986,0,4.0799999999999983,0,4.0799999999999983,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XIII-XIII",null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,0,{"$f":"+Y108","v":4.0799999999999983},0,{"$f":"+U109","v":3.7599999999999985},0,3.7599999999999985,{"$f":"+X109","v":0},4.0799999999999983,0,3.7599999999999985,0,3.7599999999999985,0,4.0799999999999983,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek  XII-XII",null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,0,{"$f":"+W109","v":3.7599999999999985},0,{"$f":"+S110","v":3.4399999999999986},0,3.4399999999999986,{"$f":"+V110","v":0},3.7599999999999985,0,3.4399999999999986,0,3.4399999999999986,0,3.7599999999999985,0,3.4399999999999986,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XI-XI",null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,0,{"$f":"+U110","v":3.4399999999999986},0,{"$f":"+Q111","v":3.1199999999999988},0,3.1199999999999988,{"$f":"+T111","v":0},3.4399999999999986,0,3.1199999999999988,0,3.1199999999999988,0,3.4399999999999986,0,3.1199999999999988,0,3.1199999999999988,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek X-X",null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,0,{"$f":"+S111","v":3.1199999999999988},0,{"$f":"+O112","v":2.7999999999999989},0,2.7999999999999989,0,3.1199999999999988,0,2.7999999999999989,0,2.7999999999999989,0,3.1199999999999988,0,2.7999999999999989,0,2.7999999999999989,0,3.1199999999999988,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek IX-IX",null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,0,{"$f":"+Q112","v":2.7999999999999989},0,{"$f":"+M113","v":2.4799999999999991},0,2.4799999999999991,{"$f":"+P113","v":0},2.7999999999999989,{"$f":"+R113","v":0},2.4799999999999991,0,2.4799999999999991,0,2.7999999999999989,0,2.4799999999999991,0,2.4799999999999991,0,2.7999999999999989,0,2.4799999999999991,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VIII-VIII",null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},2.1599999999999993,{"$error":"#VALUE!"},2.1599999999999993,{"$error":"#VALUE!"},2.1599999999999993,{"$error":"#VALUE!"},2.1599999999999993,0,{"$f":"+O113","v":2.4799999999999991},0,{"$f":"+K114","v":2.1599999999999993},0,2.1599999999999993,{"$f":"+N114","v":0},2.4799999999999991,0,2.1599999999999993,0,2.1599999999999993,0,2.4799999999999991,0,2.1599999999999993,0,2.1599999999999993,0,2.4799999999999991,0,2.1599999999999993,0,2.1599999999999993,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VII-VII",null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1.8399999999999992,{"$error":"#VALUE!"},1.8399999999999992,{"$error":"#VALUE!"},1.8399999999999992,0,{"$f":"+M114","v":2.1599999999999993},0,{"$f":"+I115","v":1.8399999999999992},0,1.8399999999999992,{"$f":"+L115","v":0},2.1599999999999993,0,1.8399999999999992,0,1.8399999999999992,0,2.1599999999999993,0,1.8399999999999992,0,1.8399999999999992,0,2.1599999999999993,0,1.8399999999999992,0,1.8399999999999992,0,2.1599999999999993,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VI-VI",null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1.5199999999999991,{"$error":"#VALUE!"},1.5199999999999991,0,{"$f":"+K115","v":1.8399999999999992},0,{"$f":"+G116","v":1.5199999999999991},0,{"$f":"+I116","v":1.5199999999999991},{"$f":"+J116","v":0},1.8399999999999992,{"$f":"+L116","v":0},1.5199999999999991,0,1.5199999999999991,0,1.8399999999999992,0,1.5199999999999991,0,1.5199999999999991,0,1.8399999999999992,0,1.5199999999999991,0,1.5199999999999991,0,1.8399999999999992,0,1.5199999999999991,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek III -III",null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},1.1999999999999991,0,{"$f":"+I116","v":1.5199999999999991},0,{"$f":"+G117","v":1.1999999999999991},0,{"$f":"+G117","v":1.1999999999999991},{"$f":"+H117","v":0},{"$f":"+I117","v":1.5199999999999991},{"$f":"+J117","v":0},1.1999999999999991,{"$f":"+L117","v":0},1.1999999999999991,0,1.5199999999999991,0,1.1999999999999991,0,1.1999999999999991,0,1.5199999999999991,0,1.1999999999999991,0,1.1999999999999991,0,1.5199999999999991,0,1.1999999999999991,0,1.1999999999999991,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["IV-IV=Mmin",null,null,null,0,{"$f":"+F38","v":0},{"$f":"+G117","v":1.1999999999999991},0,{"$f":"+I119","v":{"$error":"#VALUE!"}},0,{"$f":"+K117","v":1.1999999999999991},{"$f":"+F118","v":0},{"$f":"+G118","v":1.1999999999999991},{"$f":"+H118","v":0},{"$f":"+I118","v":{"$error":"#VALUE!"}},{"$f":"+J118","v":0},1.1999999999999991,{"$f":"+L118","v":0},1.1999999999999991,0,{"$error":"#VALUE!"},0,1.1999999999999991,0,1.1999999999999991,0,{"$error":"#VALUE!"},0,1.1999999999999991,0,1.1999999999999991,0,{"$error":"#VALUE!"},0,1.1999999999999991,0,1.1999999999999991]
["V-V = Mmax",null,null,null,0,{"$f":"+F39","v":0},{"$f":"+G39","v":{"$error":"#VALUE!"}},0,{"$f":"+G119","v":{"$error":"#VALUE!"}},0,{"$f":"+G119","v":{"$error":"#VALUE!"}},{"$f":"+F119","v":0},{"$f":"+G119","v":{"$error":"#VALUE!"}},{"$f":"+H119","v":0},{"$f":"+I119","v":{"$error":"#VALUE!"}},{"$f":"+J119","v":0},{"$error":"#VALUE!"},{"$f":"+L119","v":0},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"}]
[null,null,null,"Ukupni pritisak",null,"SQhi=",{"$f":"+G123","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I123","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K123","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+M123","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+O123","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Q123","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+S123","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+U123","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+W123","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Y123","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AA123","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AC123","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AE123","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AG123","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AI123","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AK123","v":{"$error":"#VALUE!"}}]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G125","v":{"$error":"#VALUE!"}}," y=",{"$f":"+I125","v":{"$error":"#VALUE!"}}," y=",{"$f":"+K125","v":{"$error":"#VALUE!"}}," y=",{"$f":"+M125","v":{"$error":"#VALUE!"}}," y=",{"$f":"+O125","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Q125","v":{"$error":"#VALUE!"}}," y=",{"$f":"+S125","v":{"$error":"#VALUE!"}}," y=",{"$f":"+U125","v":{"$error":"#VALUE!"}}," y=",{"$f":"+W125","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Y125","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AA125","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AC125","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AE125","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AG125","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AI125","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AK125","v":{"$error":"#VALUE!"}}]
[null,null,null,"krak za presjek III -III",null,"z=",{"$f":"+G121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+O121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Q121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+S121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+U121-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}},"z=",{"$f":"+W121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Y121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AA121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AC121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AE121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AG121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AI121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AK121-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,"F=",{"$f":"-0.5*((F100*G101-F101*G100)+\n(F101*G102-F102*G101)+\n(F102*G103-F103*G102)+\n(F103*G104-F104*G103)+\n(F104*G105-F105*G104)+\n(F105*G106-F106*G105)+\n(F106*G107-F107*G106)+\n(F107*G108-F108*G107)+\n(F108*G109-F109*G108)+\n(F109*G110-F110*G109)+\n(F110*G111-F111*G110)+\n(F111*G112-F112*G111)+\n(F112*G113-F113*G112)+\n(F113*G114-F114*G113)+\n(F114*G115-F115*G114)+\n(F115*G116-F116*G115)+\n(F116*G117-F117*G116)+\n(F117*G118-F118*G117)+\n(F118*G119-F119*G118))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((H100*I101-H101*I100)+\n(H101*I102-H102*I101)+\n(H102*I103-H103*I102)+\n(H103*I104-H104*I103)+\n(H104*I105-H105*I104)+\n(H105*I106-H106*I105)+\n(H106*I107-H107*I106)+\n(H107*I108-H108*I107)+\n(H108*I109-H109*I108)+\n(H109*I110-H110*I109)+\n(H110*I111-H111*I110)+\n(H111*I112-H112*I111)+\n(H112*I113-H113*I112)+\n(H113*I114-H114*I113)+\n(H114*I115-H115*I114)+\n(H115*I116-H116*I115)+\n(H116*I117-H117*I116)+\n(H117*I118-H118*I117)+\n(H118*I119-H119*I118))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((J100*K101-J101*K100)+\n(J101*K102-J102*K101)+\n(J102*K103-J103*K102)+\n(J103*K104-J104*K103)+\n(J104*K105-J105*K104)+\n(J105*K106-J106*K105)+\n(J106*K107-J107*K106)+\n(J107*K108-J108*K107)+\n(J108*K109-J109*K108)+\n(J109*K110-J110*K109)+\n(J110*K111-J111*K110)+\n(J111*K112-J112*K111)+\n(J112*K113-J113*K112)+\n(J113*K114-J114*K113)+\n(J114*K115-J115*K114)+\n(J115*K116-J116*K115)+\n(J116*K117-J117*K116)+\n(J117*K118-J118*K117)+\n(J118*K119-J119*K118))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((L100*M101-L101*M100)+\n(L101*M102-L102*M101)+\n(L102*M103-L103*M102)+\n(L103*M104-L104*M103)+\n(L104*M105-L105*M104)+\n(L105*M106-L106*M105)+\n(L106*M107-L107*M106)+\n(L107*M108-L108*M107)+\n(L108*M109-L109*M108)+\n(L109*M110-L110*M109)+\n(L110*M111-L111*M110)+\n(L111*M112-L112*M111)+\n(L112*M113-L113*M112)+\n(L113*M114-L114*M113)+\n(L114*M115-L115*M114)+\n(L115*M116-L116*M115)+\n(L116*M117-L117*M116)+\n(L117*M118-L118*M117)+\n(L118*M119-L119*M118))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((N100*O101-N101*O100)+\n(N101*O102-N102*O101)+\n(N102*O103-N103*O102)+\n(N103*O104-N104*O103)+\n(N104*O105-N105*O104)+\n(N105*O106-N106*O105)+\n(N106*O107-N107*O106)+\n(N107*O108-N108*O107)+\n(N108*O109-N109*O108)+\n(N109*O110-N110*O109)+\n(N110*O111-N111*O110)+\n(N111*O112-N112*O111)+\n(N112*O113-N113*O112)+\n(N113*O114-N114*O113)+\n(N114*O115-N115*O114)+\n(N115*O116-N116*O115)+\n(N116*O117-N117*O116)+\n(N117*O118-N118*O117)+\n(N118*O119-N119*O118))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((P100*Q101-P101*Q100)+\n(P101*Q102-P102*Q101)+\n(P102*Q103-P103*Q102)+\n(P103*Q104-P104*Q103)+\n(P104*Q105-P105*Q104)+\n(P105*Q106-P106*Q105)+\n(P106*Q107-P107*Q106)+\n(P107*Q108-P108*Q107)+\n(P108*Q109-P109*Q108)+\n(P109*Q110-P110*Q109)+\n(P110*Q111-P111*Q110)+\n(P111*Q112-P112*Q111)+\n(P112*Q113-P113*Q112)+\n(P113*Q114-P114*Q113)+\n(P114*Q115-P115*Q114)+\n(P115*Q116-P116*Q115)+\n(P116*Q117-P117*Q116)+\n(P117*Q118-P118*Q117)+\n(P118*Q119-P119*Q118))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((R100*S101-R101*S100)+\n(R101*S102-R102*S101)+\n(R102*S103-R103*S102)+\n(R103*S104-R104*S103)+\n(R104*S105-R105*S104)+\n(R105*S106-R106*S105)+\n(R106*S107-R107*S106)+\n(R107*S108-R108*S107)+\n(R108*S109-R109*S108)+\n(R109*S110-R110*S109)+\n(R110*S111-R111*S110)+\n(R111*S112-R112*S111)+\n(R112*S113-R113*S112)+\n(R113*S114-R114*S113)+\n(R114*S115-R115*S114)+\n(R115*S116-R116*S115)+\n(R116*S117-R117*S116)+\n(R117*S118-R118*S117)+\n(R118*S119-R119*S118))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((T100*U101-T101*U100)+\n(T101*U102-T102*U101)+\n(T102*U103-T103*U102)+\n(T103*U104-T104*U103)+\n(T104*U105-T105*U104)+\n(T105*U106-T106*U105)+\n(T106*U107-T107*U106)+\n(T107*U108-T108*U107)+\n(T108*U109-T109*U108)+\n(T109*U110-T110*U109)+\n(T110*U111-T111*U110)+\n(T111*U112-T112*U111)+\n(T112*U113-T113*U112)+\n(T113*U114-T114*U113)+\n(T114*U115-T115*U114)+\n(T115*U116-T116*U115)+\n(T116*U117-T117*U116)+\n(T117*U118-T118*U117)+\n(T118*U119-T119*U118))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((V100*W101-V101*W100)+\n(V101*W102-V102*W101)+\n(V102*W103-V103*W102)+\n(V103*W104-V104*W103)+\n(V104*W105-V105*W104)+\n(V105*W106-V106*W105)+\n(V106*W107-V107*W106)+\n(V107*W108-V108*W107)+\n(V108*W109-V109*W108)+\n(V109*W110-V110*W109)+\n(V110*W111-V111*W110)+\n(V111*W112-V112*W111)+\n(V112*W113-V113*W112)+\n(V113*W114-V114*W113)+\n(V114*W115-V115*W114)+\n(V115*W116-V116*W115)+\n(V116*W117-V117*W116)+\n(V117*W118-V118*W117)+\n(V118*W119-V119*W118))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((X100*Y101-X101*Y100)+\n(X101*Y102-X102*Y101)+\n(X102*Y103-X103*Y102)+\n(X103*Y104-X104*Y103)+\n(X104*Y105-X105*Y104)+\n(X105*Y106-X106*Y105)+\n(X106*Y107-X107*Y106)+\n(X107*Y108-X108*Y107)+\n(X108*Y109-X109*Y108)+\n(X109*Y110-X110*Y109)+\n(X110*Y111-X111*Y110)+\n(X111*Y112-X112*Y111)+\n(X112*Y113-X113*Y112)+\n(X113*Y114-X114*Y113)+\n(X114*Y115-X115*Y114)+\n(X115*Y116-X116*Y115)+\n(X116*Y117-X117*Y116)+\n(X117*Y118-X118*Y117)+\n(X118*Y119-X119*Y118))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((Z100*AA101-Z101*AA100)+\n(Z101*AA102-Z102*AA101)+\n(Z102*AA103-Z103*AA102)+\n(Z103*AA104-Z104*AA103)+\n(Z104*AA105-Z105*AA104)+\n(Z105*AA106-Z106*AA105)+\n(Z106*AA107-Z107*AA106)+\n(Z107*AA108-Z108*AA107)+\n(Z108*AA109-Z109*AA108)+\n(Z109*AA110-Z110*AA109)+\n(Z110*AA111-Z111*AA110)+\n(Z111*AA112-Z112*AA111)+\n(Z112*AA113-Z113*AA112)+\n(Z113*AA114-Z114*AA113)+\n(Z114*AA115-Z115*AA114)+\n(Z115*AA116-Z116*AA115)+\n(Z116*AA117-Z117*AA116)+\n(Z117*AA118-Z118*AA117)+\n(Z118*AA119-Z119*AA118))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AB100*AC101-AB101*AC100)+\n(AB101*AC102-AB102*AC101)+\n(AB102*AC103-AB103*AC102)+\n(AB103*AC104-AB104*AC103)+\n(AB104*AC105-AB105*AC104)+\n(AB105*AC106-AB106*AC105)+\n(AB106*AC107-AB107*AC106)+\n(AB107*AC108-AB108*AC107)+\n(AB108*AC109-AB109*AC108)+\n(AB109*AC110-AB110*AC109)+\n(AB110*AC111-AB111*AC110)+\n(AB111*AC112-AB112*AC111)+\n(AB112*AC113-AB113*AC112)+\n(AB113*AC114-AB114*AC113)+\n(AB114*AC115-AB115*AC114)+\n(AB115*AC116-AB116*AC115)+\n(AB116*AC117-AB117*AC116)+\n(AB117*AC118-AB118*AC117)+\n(AB118*AC119-AB119*AC118))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AD100*AE101-AD101*AE100)+\n(AD101*AE102-AD102*AE101)+\n(AD102*AE103-AD103*AE102)+\n(AD103*AE104-AD104*AE103)+\n(AD104*AE105-AD105*AE104)+\n(AD105*AE106-AD106*AE105)+\n(AD106*AE107-AD107*AE106)+\n(AD107*AE108-AD108*AE107)+\n(AD108*AE109-AD109*AE108)+\n(AD109*AE110-AD110*AE109)+\n(AD110*AE111-AD111*AE110)+\n(AD111*AE112-AD112*AE111)+\n(AD112*AE113-AD113*AE112)+\n(AD113*AE114-AD114*AE113)+\n(AD114*AE115-AD115*AE114)+\n(AD115*AE116-AD116*AE115)+\n(AD116*AE117-AD117*AE116)+\n(AD117*AE118-AD118*AE117)+\n(AD118*AE119-AD119*AE118))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AF100*AG101-AF101*AG100)+\n(AF101*AG102-AF102*AG101)+\n(AF102*AG103-AF103*AG102)+\n(AF103*AG104-AF104*AG103)+\n(AF104*AG105-AF105*AG104)+\n(AF105*AG106-AF106*AG105)+\n(AF106*AG107-AF107*AG106)+\n(AF107*AG108-AF108*AG107)+\n(AF108*AG109-AF109*AG108)+\n(AF109*AG110-AF110*AG109)+\n(AF110*AG111-AF111*AG110)+\n(AF111*AG112-AF112*AG111)+\n(AF112*AG113-AF113*AG112)+\n(AF113*AG114-AF114*AG113)+\n(AF114*AG115-AF115*AG114)+\n(AF115*AG116-AF116*AG115)+\n(AF116*AG117-AF117*AG116)+\n(AF117*AG118-AF118*AG117)+\n(AF118*AG119-AF119*AG118))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AH100*AI101-AH101*AI100)+\n(AH101*AI102-AH102*AI101)+\n(AH102*AI103-AH103*AI102)+\n(AH103*AI104-AH104*AI103)+\n(AH104*AI105-AH105*AI104)+\n(AH105*AI106-AH106*AI105)+\n(AH106*AI107-AH107*AI106)+\n(AH107*AI108-AH108*AI107)+\n(AH108*AI109-AH109*AI108)+\n(AH109*AI110-AH110*AI109)+\n(AH110*AI111-AH111*AI110)+\n(AH111*AI112-AH112*AI111)+\n(AH112*AI113-AH113*AI112)+\n(AH113*AI114-AH114*AI113)+\n(AH114*AI115-AH115*AI114)+\n(AH115*AI116-AH116*AI115)+\n(AH116*AI117-AH117*AI116)+\n(AH117*AI118-AH118*AI117)+\n(AH118*AI119-AH119*AI118))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AJ100*AK101-AJ101*AK100)+\n(AJ101*AK102-AJ102*AK101)+\n(AJ102*AK103-AJ103*AK102)+\n(AJ103*AK104-AJ104*AK103)+\n(AJ104*AK105-AJ105*AK104)+\n(AJ105*AK106-AJ106*AK105)+\n(AJ106*AK107-AJ107*AK106)+\n(AJ107*AK108-AJ108*AK107)+\n(AJ108*AK109-AJ109*AK108)+\n(AJ109*AK110-AJ110*AK109)+\n(AJ110*AK111-AJ111*AK110)+\n(AJ111*AK112-AJ112*AK111)+\n(AJ112*AK113-AJ113*AK112)+\n(AJ113*AK114-AJ114*AK113)+\n(AJ114*AK115-AJ115*AK114)+\n(AJ115*AK116-AJ116*AK115)+\n(AJ116*AK117-AJ117*AK116)+\n(AJ117*AK118-AJ118*AK117)+\n(AJ118*AK119-AJ119*AK118))","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,"x=",1,"x=",1.5,"x=",1.5,"x=",1.5,"x=",1.5,"x=",1.5,"x=",1.5,"x=",1.5,"x=",1.5,"x=",1.5,"x=",1.5,"x=",1.5,"x=",1.5,"x=",1.5,"x=",1.5,"x=",1.5]
[null,null,null,null,null,"y=",{"$f":"+IF(G123=0,0,-((F100*G101-F101*G100)*(G100+G101)+(F101*G102-F102*G101)*(G101+G102)+\n(F102*G103-F103*G102)*(G102+G103)+\n(F103*G104-F104*G103)*(G103+G104)+\n(F104*G105-F105*G104)*(G104+G105)+\n(F105*G106-F106*G105)*(G105+G106)+\n(F106*G107-F107*G106)*(G106+G107)+\n(F107*G108-F108*G107)*(G107+G108)+\n(F108*G109-F109*G108)*(G108+G109)+\n(F109*G110-F110*G109)*(G109+G110)+\n(F110*G111-F111*G110)*(G110+G111)+\n(F111*G112-F112*G111)*(G111+G112)+\n(F112*G113-F113*G112)*(G112+G113)+\n(F113*G114-F114*G113)*(G113+G114)+\n(F114*G115-F115*G114)*(G114+G115)+\n(F115*G116-F116*G115)*(G115+G116)+\n(F116*G117-F117*G116)*(G116+G117)+\n(F117*G118-F118*G117)*(G117+G118)+\n(F118*G119-F119*G118)*(G118+G119))/6/G123)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(I123=0,0,-((H100*I101-H101*I100)*(I100+I101)+(H101*I102-H102*I101)*(I101+I102)+\n(H102*I103-H103*I102)*(I102+I103)+\n(H103*I104-H104*I103)*(I103+I104)+\n(H104*I105-H105*I104)*(I104+I105)+\n(H105*I106-H106*I105)*(I105+I106)+\n(H106*I107-H107*I106)*(I106+I107)+\n(H107*I108-H108*I107)*(I107+I108)+\n(H108*I109-H109*I108)*(I108+I109)+\n(H109*I110-H110*I109)*(I109+I110)+\n(H110*I111-H111*I110)*(I110+I111)+\n(H111*I112-H112*I111)*(I111+I112)+\n(H112*I113-H113*I112)*(I112+I113)+\n(H113*I114-H114*I113)*(I113+I114)+\n(H114*I115-H115*I114)*(I114+I115)+\n(H115*I116-H116*I115)*(I115+I116)+\n(H116*I117-H117*I116)*(I116+I117)+\n(H117*I118-H118*I117)*(I117+I118)+\n(H118*I119-H119*I118)*(I118+I119))/6/I123)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(K123=0,0,-((J100*K101-J101*K100)*(K100+K101)+(J101*K102-J102*K101)*(K101+K102)+\n(J102*K103-J103*K102)*(K102+K103)+\n(J103*K104-J104*K103)*(K103+K104)+\n(J104*K105-J105*K104)*(K104+K105)+\n(J105*K106-J106*K105)*(K105+K106)+\n(J106*K107-J107*K106)*(K106+K107)+\n(J107*K108-J108*K107)*(K107+K108)+\n(J108*K109-J109*K108)*(K108+K109)+\n(J109*K110-J110*K109)*(K109+K110)+\n(J110*K111-J111*K110)*(K110+K111)+\n(J111*K112-J112*K111)*(K111+K112)+\n(J112*K113-J113*K112)*(K112+K113)+\n(J113*K114-J114*K113)*(K113+K114)+\n(J114*K115-J115*K114)*(K114+K115)+\n(J115*K116-J116*K115)*(K115+K116)+\n(J116*K117-J117*K116)*(K116+K117)+\n(J117*K118-J118*K117)*(K117+K118)+\n(J118*K119-J119*K118)*(K118+K119))/6/K123)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(M123=0,0,-((L100*M101-L101*M100)*(M100+M101)+(L101*M102-L102*M101)*(M101+M102)+\n(L102*M103-L103*M102)*(M102+M103)+\n(L103*M104-L104*M103)*(M103+M104)+\n(L104*M105-L105*M104)*(M104+M105)+\n(L105*M106-L106*M105)*(M105+M106)+\n(L106*M107-L107*M106)*(M106+M107)+\n(L107*M108-L108*M107)*(M107+M108)+\n(L108*M109-L109*M108)*(M108+M109)+\n(L109*M110-L110*M109)*(M109+M110)+\n(L110*M111-L111*M110)*(M110+M111)+\n(L111*M112-L112*M111)*(M111+M112)+\n(L112*M113-L113*M112)*(M112+M113)+\n(L113*M114-L114*M113)*(M113+M114)+\n(L114*M115-L115*M114)*(M114+M115)+\n(L115*M116-L116*M115)*(M115+M116)+\n(L116*M117-L117*M116)*(M116+M117)+\n(L117*M118-L118*M117)*(M117+M118)+\n(L118*M119-L119*M118)*(M118+M119))/6/M123)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(O123=0,0,-((N100*O101-N101*O100)*(O100+O101)+(N101*O102-N102*O101)*(O101+O102)+\n(N102*O103-N103*O102)*(O102+O103)+\n(N103*O104-N104*O103)*(O103+O104)+\n(N104*O105-N105*O104)*(O104+O105)+\n(N105*O106-N106*O105)*(O105+O106)+\n(N106*O107-N107*O106)*(O106+O107)+\n(N107*O108-N108*O107)*(O107+O108)+\n(N108*O109-N109*O108)*(O108+O109)+\n(N109*O110-N110*O109)*(O109+O110)+\n(N110*O111-N111*O110)*(O110+O111)+\n(N111*O112-N112*O111)*(O111+O112)+\n(N112*O113-N113*O112)*(O112+O113)+\n(N113*O114-N114*O113)*(O113+O114)+\n(N114*O115-N115*O114)*(O114+O115)+\n(N115*O116-N116*O115)*(O115+O116)+\n(N116*O117-N117*O116)*(O116+O117)+\n(N117*O118-N118*O117)*(O117+O118)+\n(N118*O119-N119*O118)*(O118+O119))/6/O123)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Q123=0,0,-((P100*Q101-P101*Q100)*(Q100+Q101)+(P101*Q102-P102*Q101)*(Q101+Q102)+\n(P102*Q103-P103*Q102)*(Q102+Q103)+\n(P103*Q104-P104*Q103)*(Q103+Q104)+\n(P104*Q105-P105*Q104)*(Q104+Q105)+\n(P105*Q106-P106*Q105)*(Q105+Q106)+\n(P106*Q107-P107*Q106)*(Q106+Q107)+\n(P107*Q108-P108*Q107)*(Q107+Q108)+\n(P108*Q109-P109*Q108)*(Q108+Q109)+\n(P109*Q110-P110*Q109)*(Q109+Q110)+\n(P110*Q111-P111*Q110)*(Q110+Q111)+\n(P111*Q112-P112*Q111)*(Q111+Q112)+\n(P112*Q113-P113*Q112)*(Q112+Q113)+\n(P113*Q114-P114*Q113)*(Q113+Q114)+\n(P114*Q115-P115*Q114)*(Q114+Q115)+\n(P115*Q116-P116*Q115)*(Q115+Q116)+\n(P116*Q117-P117*Q116)*(Q116+Q117)+\n(P117*Q118-P118*Q117)*(Q117+Q118)+\n(P118*Q119-P119*Q118)*(Q118+Q119))/6/Q123)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(S123=0,0,-((R100*S101-R101*S100)*(S100+S101)+(R101*S102-R102*S101)*(S101+S102)+\n(R102*S103-R103*S102)*(S102+S103)+\n(R103*S104-R104*S103)*(S103+S104)+\n(R104*S105-R105*S104)*(S104+S105)+\n(R105*S106-R106*S105)*(S105+S106)+\n(R106*S107-R107*S106)*(S106+S107)+\n(R107*S108-R108*S107)*(S107+S108)+\n(R108*S109-R109*S108)*(S108+S109)+\n(R109*S110-R110*S109)*(S109+S110)+\n(R110*S111-R111*S110)*(S110+S111)+\n(R111*S112-R112*S111)*(S111+S112)+\n(R112*S113-R113*S112)*(S112+S113)+\n(R113*S114-R114*S113)*(S113+S114)+\n(R114*S115-R115*S114)*(S114+S115)+\n(R115*S116-R116*S115)*(S115+S116)+\n(R116*S117-R117*S116)*(S116+S117)+\n(R117*S118-R118*S117)*(S117+S118)+\n(R118*S119-R119*S118)*(S118+S119))/6/S123)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(U123=0,0,-((T100*U101-T101*U100)*(U100+U101)+(T101*U102-T102*U101)*(U101+U102)+\n(T102*U103-T103*U102)*(U102+U103)+\n(T103*U104-T104*U103)*(U103+U104)+\n(T104*U105-T105*U104)*(U104+U105)+\n(T105*U106-T106*U105)*(U105+U106)+\n(T106*U107-T107*U106)*(U106+U107)+\n(T107*U108-T108*U107)*(U107+U108)+\n(T108*U109-T109*U108)*(U108+U109)+\n(T109*U110-T110*U109)*(U109+U110)+\n(T110*U111-T111*U110)*(U110+U111)+\n(T111*U112-T112*U111)*(U111+U112)+\n(T112*U113-T113*U112)*(U112+U113)+\n(T113*U114-T114*U113)*(U113+U114)+\n(T114*U115-T115*U114)*(U114+U115)+\n(T115*U116-T116*U115)*(U115+U116)+\n(T116*U117-T117*U116)*(U116+U117)+\n(T117*U118-T118*U117)*(U117+U118)+\n(T118*U119-T119*U118)*(U118+U119))/6/U123)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(W123=0,0,-((V100*W101-V101*W100)*(W100+W101)+(V101*W102-V102*W101)*(W101+W102)+\n(V102*W103-V103*W102)*(W102+W103)+\n(V103*W104-V104*W103)*(W103+W104)+\n(V104*W105-V105*W104)*(W104+W105)+\n(V105*W106-V106*W105)*(W105+W106)+\n(V106*W107-V107*W106)*(W106+W107)+\n(V107*W108-V108*W107)*(W107+W108)+\n(V108*W109-V109*W108)*(W108+W109)+\n(V109*W110-V110*W109)*(W109+W110)+\n(V110*W111-V111*W110)*(W110+W111)+\n(V111*W112-V112*W111)*(W111+W112)+\n(V112*W113-V113*W112)*(W112+W113)+\n(V113*W114-V114*W113)*(W113+W114)+\n(V114*W115-V115*W114)*(W114+W115)+\n(V115*W116-V116*W115)*(W115+W116)+\n(V116*W117-V117*W116)*(W116+W117)+\n(V117*W118-V118*W117)*(W117+W118)+\n(V118*W119-V119*W118)*(W118+W119))/6/W123)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Y123=0,0,-((X100*Y101-X101*Y100)*(Y100+Y101)+(X101*Y102-X102*Y101)*(Y101+Y102)+\n(X102*Y103-X103*Y102)*(Y102+Y103)+\n(X103*Y104-X104*Y103)*(Y103+Y104)+\n(X104*Y105-X105*Y104)*(Y104+Y105)+\n(X105*Y106-X106*Y105)*(Y105+Y106)+\n(X106*Y107-X107*Y106)*(Y106+Y107)+\n(X107*Y108-X108*Y107)*(Y107+Y108)+\n(X108*Y109-X109*Y108)*(Y108+Y109)+\n(X109*Y110-X110*Y109)*(Y109+Y110)+\n(X110*Y111-X111*Y110)*(Y110+Y111)+\n(X111*Y112-X112*Y111)*(Y111+Y112)+\n(X112*Y113-X113*Y112)*(Y112+Y113)+\n(X113*Y114-X114*Y113)*(Y113+Y114)+\n(X114*Y115-X115*Y114)*(Y114+Y115)+\n(X115*Y116-X116*Y115)*(Y115+Y116)+\n(X116*Y117-X117*Y116)*(Y116+Y117)+\n(X117*Y118-X118*Y117)*(Y117+Y118)+\n(X118*Y119-X119*Y118)*(Y118+Y119))/6/Y123)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AA123=0,0,-((Z100*AA101-Z101*AA100)*(AA100+AA101)+(Z101*AA102-Z102*AA101)*(AA101+AA102)+\n(Z102*AA103-Z103*AA102)*(AA102+AA103)+\n(Z103*AA104-Z104*AA103)*(AA103+AA104)+\n(Z104*AA105-Z105*AA104)*(AA104+AA105)+\n(Z105*AA106-Z106*AA105)*(AA105+AA106)+\n(Z106*AA107-Z107*AA106)*(AA106+AA107)+\n(Z107*AA108-Z108*AA107)*(AA107+AA108)+\n(Z108*AA109-Z109*AA108)*(AA108+AA109)+\n(Z109*AA110-Z110*AA109)*(AA109+AA110)+\n(Z110*AA111-Z111*AA110)*(AA110+AA111)+\n(Z111*AA112-Z112*AA111)*(AA111+AA112)+\n(Z112*AA113-Z113*AA112)*(AA112+AA113)+\n(Z113*AA114-Z114*AA113)*(AA113+AA114)+\n(Z114*AA115-Z115*AA114)*(AA114+AA115)+\n(Z115*AA116-Z116*AA115)*(AA115+AA116)+\n(Z116*AA117-Z117*AA116)*(AA116+AA117)+\n(Z117*AA118-Z118*AA117)*(AA117+AA118)+\n(Z118*AA119-Z119*AA118)*(AA118+AA119))/6/AA123)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AC123=0,0,-((AB100*AC101-AB101*AC100)*(AC100+AC101)+(AB101*AC102-AB102*AC101)*(AC101+AC102)+\n(AB102*AC103-AB103*AC102)*(AC102+AC103)+\n(AB103*AC104-AB104*AC103)*(AC103+AC104)+\n(AB104*AC105-AB105*AC104)*(AC104+AC105)+\n(AB105*AC106-AB106*AC105)*(AC105+AC106)+\n(AB106*AC107-AB107*AC106)*(AC106+AC107)+\n(AB107*AC108-AB108*AC107)*(AC107+AC108)+\n(AB108*AC109-AB109*AC108)*(AC108+AC109)+\n(AB109*AC110-AB110*AC109)*(AC109+AC110)+\n(AB110*AC111-AB111*AC110)*(AC110+AC111)+\n(AB111*AC112-AB112*AC111)*(AC111+AC112)+\n(AB112*AC113-AB113*AC112)*(AC112+AC113)+\n(AB113*AC114-AB114*AC113)*(AC113+AC114)+\n(AB114*AC115-AB115*AC114)*(AC114+AC115)+\n(AB115*AC116-AB116*AC115)*(AC115+AC116)+\n(AB116*AC117-AB117*AC116)*(AC116+AC117)+\n(AB117*AC118-AB118*AC117)*(AC117+AC118)+\n(AB118*AC119-AB119*AC118)*(AC118+AC119))/6/AC123)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AE123=0,0,-((AD100*AE101-AD101*AE100)*(AE100+AE101)+(AD101*AE102-AD102*AE101)*(AE101+AE102)+\n(AD102*AE103-AD103*AE102)*(AE102+AE103)+\n(AD103*AE104-AD104*AE103)*(AE103+AE104)+\n(AD104*AE105-AD105*AE104)*(AE104+AE105)+\n(AD105*AE106-AD106*AE105)*(AE105+AE106)+\n(AD106*AE107-AD107*AE106)*(AE106+AE107)+\n(AD107*AE108-AD108*AE107)*(AE107+AE108)+\n(AD108*AE109-AD109*AE108)*(AE108+AE109)+\n(AD109*AE110-AD110*AE109)*(AE109+AE110)+\n(AD110*AE111-AD111*AE110)*(AE110+AE111)+\n(AD111*AE112-AD112*AE111)*(AE111+AE112)+\n(AD112*AE113-AD113*AE112)*(AE112+AE113)+\n(AD113*AE114-AD114*AE113)*(AE113+AE114)+\n(AD114*AE115-AD115*AE114)*(AE114+AE115)+\n(AD115*AE116-AD116*AE115)*(AE115+AE116)+\n(AD116*AE117-AD117*AE116)*(AE116+AE117)+\n(AD117*AE118-AD118*AE117)*(AE117+AE118)+\n(AD118*AE119-AD119*AE118)*(AE118+AE119))/6/AE123)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AG123=0,0,-((AF100*AG101-AF101*AG100)*(AG100+AG101)+(AF101*AG102-AF102*AG101)*(AG101+AG102)+\n(AF102*AG103-AF103*AG102)*(AG102+AG103)+\n(AF103*AG104-AF104*AG103)*(AG103+AG104)+\n(AF104*AG105-AF105*AG104)*(AG104+AG105)+\n(AF105*AG106-AF106*AG105)*(AG105+AG106)+\n(AF106*AG107-AF107*AG106)*(AG106+AG107)+\n(AF107*AG108-AF108*AG107)*(AG107+AG108)+\n(AF108*AG109-AF109*AG108)*(AG108+AG109)+\n(AF109*AG110-AF110*AG109)*(AG109+AG110)+\n(AF110*AG111-AF111*AG110)*(AG110+AG111)+\n(AF111*AG112-AF112*AG111)*(AG111+AG112)+\n(AF112*AG113-AF113*AG112)*(AG112+AG113)+\n(AF113*AG114-AF114*AG113)*(AG113+AG114)+\n(AF114*AG115-AF115*AG114)*(AG114+AG115)+\n(AF115*AG116-AF116*AG115)*(AG115+AG116)+\n(AF116*AG117-AF117*AG116)*(AG116+AG117)+\n(AF117*AG118-AF118*AG117)*(AG117+AG118)+\n(AF118*AG119-AF119*AG118)*(AG118+AG119))/6/AG123)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AI123=0,0,-((AH100*AI101-AH101*AI100)*(AI100+AI101)+(AH101*AI102-AH102*AI101)*(AI101+AI102)+\n(AH102*AI103-AH103*AI102)*(AI102+AI103)+\n(AH103*AI104-AH104*AI103)*(AI103+AI104)+\n(AH104*AI105-AH105*AI104)*(AI104+AI105)+\n(AH105*AI106-AH106*AI105)*(AI105+AI106)+\n(AH106*AI107-AH107*AI106)*(AI106+AI107)+\n(AH107*AI108-AH108*AI107)*(AI107+AI108)+\n(AH108*AI109-AH109*AI108)*(AI108+AI109)+\n(AH109*AI110-AH110*AI109)*(AI109+AI110)+\n(AH110*AI111-AH111*AI110)*(AI110+AI111)+\n(AH111*AI112-AH112*AI111)*(AI111+AI112)+\n(AH112*AI113-AH113*AI112)*(AI112+AI113)+\n(AH113*AI114-AH114*AI113)*(AI113+AI114)+\n(AH114*AI115-AH115*AI114)*(AI114+AI115)+\n(AH115*AI116-AH116*AI115)*(AI115+AI116)+\n(AH116*AI117-AH117*AI116)*(AI116+AI117)+\n(AH117*AI118-AH118*AI117)*(AI117+AI118)+\n(AH118*AI119-AH119*AI118)*(AI118+AI119))/6/AI123)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AK123=0,0,-((AJ100*AK101-AJ101*AK100)*(AK100+AK101)+(AJ101*AK102-AJ102*AK101)*(AK101+AK102)+\n(AJ102*AK103-AJ103*AK102)*(AK102+AK103)+\n(AJ103*AK104-AJ104*AK103)*(AK103+AK104)+\n(AJ104*AK105-AJ105*AK104)*(AK104+AK105)+\n(AJ105*AK106-AJ106*AK105)*(AK105+AK106)+\n(AJ106*AK107-AJ107*AK106)*(AK106+AK107)+\n(AJ107*AK108-AJ108*AK107)*(AK107+AK108)+\n(AJ108*AK109-AJ109*AK108)*(AK108+AK109)+\n(AJ109*AK110-AJ110*AK109)*(AK109+AK110)+\n(AJ110*AK111-AJ111*AK110)*(AK110+AK111)+\n(AJ111*AK112-AJ112*AK111)*(AK111+AK112)+\n(AJ112*AK113-AJ113*AK112)*(AK112+AK113)+\n(AJ113*AK114-AJ114*AK113)*(AK113+AK114)+\n(AJ114*AK115-AJ115*AK114)*(AK114+AK115)+\n(AJ115*AK116-AJ116*AK115)*(AK115+AK116)+\n(AJ116*AK117-AJ117*AK116)*(AK116+AK117)+\n(AJ117*AK118-AJ118*AK117)*(AK117+AK118)+\n(AJ118*AK119-AJ119*AK118)*(AK118+AK119))/6/AK123)","v":{"$error":"#VALUE!"}}]
[]
[null,null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID "]
[null,null,"OPTEREĆENJE TEMELJEM",null,null,null,null,null,null," (TERZAGHY)"]
[]
[null,null,"KONTINUIRANO OPTEREĆENJE","P - D=",{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,+'Analiza i dimenzioniranje'!$E$28-I130)+0.09","v":{"$error":"#VALUE!"}},"kN/m2","raster. iskopom   D=y*Df =",null,{"$f":"+'Analiza i dimenzioniranje'!$D$16*('Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20-D136)","v":{"$error":"#VALUE!"}},"kN/m2"]
[null,null," visina zida i temelja","H =",{"$f":"E52","v":{"$error":"#VALUE!"}},"m",{"$f":"E135","v":6}]
[null,null,"visina opterećenja iznad vrha zida","h =",{"$f":"+'Analiza i dimenzioniranje'!E31","v":-1},"m",{"$f":"SQRT(E135^2+E134^2)","v":6.7082039324993694}]
[null,null,"širina temelja","b =",{"$f":"+'Analiza i dimenzioniranje'!E29","v":1},"m   ",{"$f":"E134+E133","v":4}]
[null,null,"udaljenost temelja od zida","D =",{"$f":"+'Analiza i dimenzioniranje'!E32","v":3},"m    "]
[null,null,"1/2 dužine temelja","L/2=a=",{"$f":"+'Analiza i dimenzioniranje'!E$49/2","v":6},"m",{"$f":"SQRT(G131^2+G133^2)","v":7.2111025509279782}]
["DNO TEMELJA NA VISINI","PRESJEK NA Visini ",null,{"$f":"ROUND(+'Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20,2)","v":{"$error":"#VALUE!"}},{"$f":"+('Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)/15","v":0.32},"Presjek III -III",null,"Presjek VI",null,"Presjek VII-VII",null,"Presjek VIII-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"Presjek XIV-XIV",null,"Presjek XV-XV",null,"PresjekXVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX"]
[null,null,null,"(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja","(sb1-sb2)*2","Visina djelovanja"]
["Kota dna temelja",null,null,{"$f":"+D136","v":{"$error":"#VALUE!"}},{"$f":"+D136","v":{"$error":"#VALUE!"}},{"$f":"+G138","v":{"$error":"#VALUE!"}},{"$f":"+D138","v":{"$error":"#VALUE!"}},{"$f":"+D136","v":{"$error":"#VALUE!"}},{"$f":"+D136","v":{"$error":"#VALUE!"}},{"$f":"+D136","v":{"$error":"#VALUE!"}},{"$f":"+J138","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[{"$f":"+'Analiza i dimenzioniranje'!$E$48++'Analiza i dimenzioniranje'!$D$20","v":{"$error":"#VALUE!"}},null,null,{"$f":"+D136","v":{"$error":"#VALUE!"}},{"$f":"+D136","v":{"$error":"#VALUE!"}},{"$f":"+D139","v":{"$error":"#VALUE!"}},{"$f":"+G138","v":{"$error":"#VALUE!"}},{"$f":"+F139","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+F139","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+J139","v":{"$error":"#VALUE!"}},{"$f":"+K139","v":{"$error":"#VALUE!"}},{"$f":"+J139","v":{"$error":"#VALUE!"}},{"$f":"+K139","v":{"$error":"#VALUE!"}},{"$f":"+N139","v":{"$error":"#VALUE!"}},{"$f":"+O139","v":{"$error":"#VALUE!"}},{"$f":"+N139","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+R139","v":{"$error":"#VALUE!"}},{"$f":"+S139","v":{"$error":"#VALUE!"}},{"$f":"+R139","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+V139","v":{"$error":"#VALUE!"}},{"$f":"+W139","v":{"$error":"#VALUE!"}},{"$f":"+V139","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+Z139","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+Z139","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"+AD139","v":{"$error":"#VALUE!"}},{"$f":"+AE139","v":{"$error":"#VALUE!"}},{"$f":"+AD139","v":{"$error":"#VALUE!"}},{"$f":"+AE139","v":{"$error":"#VALUE!"}},{"$f":"+AD139","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
[null,0,null,{"$f":"+AL140","v":0},{"$f":"+E139","v":{"$error":"#VALUE!"}},{"$f":"+D140","v":0},{"$f":"+E140","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$f":"+J140","v":0},{"$f":"+K140","v":{"$error":"#VALUE!"}},{"$f":"+J140","v":0},{"$f":"+K140","v":{"$error":"#VALUE!"}},{"$f":"+L140","v":0},{"$f":"+M140","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},{"$f":"+R140","v":0},{"$f":"+S140","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$f":"+U140","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$f":"+AH140","v":0},{"$f":"+AI140","v":{"$error":"#VALUE!"}},null,{"$f":"+B140","v":0},{"$f":"$E$134^2+AM140^2","v":9},{"$f":"$G$133^2+AM140^2","v":16},{"$f":"$G$135^2+AM140^2","v":51.999999999999993},0,null,{"$f":"ACV138","v":0},{"$f":"$E$135^2+AS140^2","v":36},{"$f":"$E$134^2+AS140^2","v":9},{"$f":"$G$132^2+AS140^2","v":45.000000000000007},{"$f":"IF(AS140=0,0,($E$170/(PI()))*(ATAN(($E$135*$E$134)/(AS140*SQRT(AV140)))-$E$135*$E$134*AS140/(AU140*SQRT(AV140))))","v":0},{"$f":"+(AQ140-AW140)*2","v":0}]
["Presjek X-X",0,null,0,{"$f":"+E138","v":{"$error":"#VALUE!"}},0,{"$f":"+E141","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$f":"+J141","v":0},{"$f":"+G141","v":{"$error":"#VALUE!"}},{"$f":"+J141","v":0},{"$f":"+K141","v":{"$error":"#VALUE!"}},{"$f":"+N141","v":0},{"$f":"+O141","v":{"$error":"#VALUE!"}},0,{"$f":"+O141","v":{"$error":"#VALUE!"}},{"$f":"-R141","v":0},{"$f":"+S141","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},{"$f":"+V141","v":0},{"$f":"+W141","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$f":"+Z141","v":0},{"$f":"+AC141","v":{"$error":"#VALUE!"}},{"$f":"+AB141","v":0},{"$f":"+AE141","v":{"$error":"#VALUE!"}},{"$f":"+AF141","v":0},{"$f":"+AE141","v":{"$error":"#VALUE!"}},{"$f":"+D141","v":0},{"$f":"+AI141","v":{"$error":"#VALUE!"}},null,0,9,16,51.999999999999993,{"$f":"IF(AM141=0,0,$E$170/(PI())*(ATAN(($E$135*$G$133)/(AM141*SQRT(AP141)))-$E$135*$G$133*AM141/(AO141*SQRT(AP141))))","v":0},null,{"$f":"+AM141","v":0},36,9,45.000000000000007,0,0]
["Presjek X-X",{"$f":"+E141-E142","v":{"$error":"#VALUE!"}},null,{"$f":"+AX142","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$U$67","v":6.0000000000000009},{"$f":"+D142","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!E48","v":6},{"$error":"#VALUE!"},6,{"$error":"#VALUE!"},6,{"$f":"+J142","v":{"$error":"#VALUE!"}},{"$f":"+G142","v":6},{"$error":"#VALUE!"},{"$f":"+E142","v":6.0000000000000009},{"$f":"+N142","v":{"$error":"#VALUE!"}},6.0000000000000009,{"$error":"#VALUE!"},{"$f":"+O142","v":6.0000000000000009},{"$f":"+R142","v":{"$error":"#VALUE!"}},{"$f":"+S142","v":6.0000000000000009},{"$error":"#VALUE!"},6.0000000000000009,{"$f":"+V142","v":{"$error":"#VALUE!"}},6.0000000000000009,{"$error":"#VALUE!"},6.0000000000000009,{"$f":"+Z142","v":{"$error":"#VALUE!"}},6.0000000000000009,{"$f":"+Z142","v":{"$error":"#VALUE!"}},{"$f":"+AA142","v":6.0000000000000009},{"$f":"+AB142","v":{"$error":"#VALUE!"}},{"$f":"+AE142","v":6.0000000000000009},{"$f":"+AF142","v":{"$error":"#VALUE!"}},{"$f":"+AE142","v":6.0000000000000009},{"$f":"+AH142","v":{"$error":"#VALUE!"}},{"$f":"+AG142","v":6.0000000000000009},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AM142=0,0,$E$130/(PI())*(ATAN(($E$135*$G$133)/(AM142*SQRT(AP142)))-$E$135*$G$133*AM142/(AO142*SQRT(AP142))))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AS142=0,0,($E$130/(PI()))*(ATAN(($E$135*$E$134)/(AS142*SQRT(AV142)))-$E$135*$E$134*AS142/(AU142*SQRT(AV142))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["Presjek XIX-XIX",{"$f":"+B142+$E$136","v":{"$error":"#VALUE!"}},null,{"$f":"+AX143","v":{"$error":"#VALUE!"}},{"$f":"+E142-('Analiza i dimenzioniranje'!E$48-'Analiza i dimenzioniranje'!E$52)/15","v":5.6800000000000006},{"$error":"#VALUE!"},{"$f":"+G142-$E$136","v":5.68},{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},5.68,{"$error":"#VALUE!"},{"$f":"+E143","v":5.6800000000000006},{"$error":"#VALUE!"},5.6800000000000006,{"$error":"#VALUE!"},{"$f":"+O143","v":5.6800000000000006},{"$f":"+R143","v":{"$error":"#VALUE!"}},5.6800000000000006,{"$error":"#VALUE!"},5.6800000000000006,{"$error":"#VALUE!"},5.6800000000000006,{"$error":"#VALUE!"},5.6800000000000006,{"$error":"#VALUE!"},5.6800000000000006,{"$f":"+Z143","v":{"$error":"#VALUE!"}},{"$f":"+AA143","v":5.6800000000000006},{"$f":"+AB143","v":{"$error":"#VALUE!"}},5.6800000000000006,{"$f":"+AF143","v":{"$error":"#VALUE!"}},5.6800000000000006,0,{"$f":"+AK142","v":6.0000000000000009},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XVIII-XVIII",{"$f":"+B143+$E$136","v":{"$error":"#VALUE!"}},null,{"$f":"+AX144","v":{"$error":"#VALUE!"}},{"$f":"+E143-('Analiza i dimenzioniranje'!E$48-'Analiza i dimenzioniranje'!E$52)/15","v":5.36},{"$error":"#VALUE!"},{"$f":"+G143-$E$136","v":5.3599999999999994},{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},{"$f":"+O144","v":5.36},{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.36,{"$error":"#VALUE!"},5.36,{"$f":"+Z144","v":{"$error":"#VALUE!"}},{"$f":"+AA144","v":5.36},{"$f":"+AB144","v":{"$error":"#VALUE!"}},5.36,0,{"$f":"+AI143","v":5.6800000000000006},0,{"$f":"+AE144","v":5.36},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XVII-XVII",{"$f":"+B144+$E$136","v":{"$error":"#VALUE!"}},null,{"$f":"+AX145","v":{"$error":"#VALUE!"}},{"$f":"+E144-('Analiza i dimenzioniranje'!E$48-'Analiza i dimenzioniranje'!E$52)/15","v":5.04},{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.04,{"$error":"#VALUE!"},5.04,{"$f":"+Z145","v":{"$error":"#VALUE!"}},{"$f":"+AA145","v":5.04},0,{"$f":"+AG144","v":5.36},0,0,0,5.04,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XVI-XVI",{"$f":"+B145+$E$136","v":{"$error":"#VALUE!"}},null,{"$f":"+$AX$146","v":{"$error":"#VALUE!"}},{"$f":"+E145-('Analiza i dimenzioniranje'!E$48-'Analiza i dimenzioniranje'!E$52)/15","v":4.72},{"$f":"+$AX$146","v":{"$error":"#VALUE!"}},4.7199999999999989,{"$f":"+$AX$146","v":{"$error":"#VALUE!"}},4.7199999999999989,{"$f":"+$AX$146","v":{"$error":"#VALUE!"}},4.7199999999999989,{"$f":"+$AX$146","v":{"$error":"#VALUE!"}},4.7199999999999989,{"$f":"+$AX$146","v":{"$error":"#VALUE!"}},4.72,{"$f":"+$AX$146","v":{"$error":"#VALUE!"}},4.72,{"$f":"+$AX$146","v":{"$error":"#VALUE!"}},4.72,{"$f":"+$AX$146","v":{"$error":"#VALUE!"}},4.72,{"$f":"+$AX$146","v":{"$error":"#VALUE!"}},4.72,{"$f":"+$AX$146","v":{"$error":"#VALUE!"}},4.72,{"$f":"+$AX$146","v":{"$error":"#VALUE!"}},4.72,{"$error":"#VALUE!"},4.72,0,{"$f":"+AE145","v":5.04},0,5.04,0,0,0,5.04,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XV-XV",{"$error":"#VALUE!"},null,{"$f":"+AX147","v":{"$error":"#VALUE!"}},{"$f":"+E146-('Analiza i dimenzioniranje'!E$48-'Analiza i dimenzioniranje'!E$52)/15","v":4.3999999999999995},{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999995,{"$error":"#VALUE!"},4.3999999999999995,{"$error":"#VALUE!"},4.3999999999999995,{"$error":"#VALUE!"},4.3999999999999995,{"$error":"#VALUE!"},4.3999999999999995,{"$error":"#VALUE!"},4.3999999999999995,{"$error":"#VALUE!"},4.3999999999999995,0,{"$f":"+AC146","v":4.72},0,{"$f":"+AA147","v":4.3999999999999995},0,4.3999999999999995,0,0,0,4.3999999999999995,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XIV-XIV",{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+E147-('Analiza i dimenzioniranje'!E$48-'Analiza i dimenzioniranje'!E$52)/15","v":4.0799999999999992},{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999992,{"$error":"#VALUE!"},4.0799999999999992,{"$error":"#VALUE!"},4.0799999999999992,{"$error":"#VALUE!"},4.0799999999999992,{"$error":"#VALUE!"},4.0799999999999992,{"$error":"#VALUE!"},4.0799999999999992,0,{"$f":"+AA147","v":4.3999999999999995},0,4.3999999999999995,0,{"$f":"+AA148","v":4.3999999999999995},0,4.3999999999999995,0,0,0,4.3999999999999995,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XIII-XIII",{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+E148-('Analiza i dimenzioniranje'!E$48-'Analiza i dimenzioniranje'!E$52)/15","v":3.7599999999999993},{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999993,{"$error":"#VALUE!"},3.7599999999999993,{"$error":"#VALUE!"},3.7599999999999993,{"$error":"#VALUE!"},3.7599999999999993,{"$error":"#VALUE!"},3.7599999999999993,0,{"$f":"+Y148","v":4.0799999999999992},0,{"$f":"+W149","v":3.7599999999999993},0,3.7599999999999993,0,{"$f":"+AA149","v":3.7599999999999993},0,3.7599999999999993,0,0,0,3.7599999999999993,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek  XII-XII",{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+E149-('Analiza i dimenzioniranje'!E$48-'Analiza i dimenzioniranje'!E$52)/15","v":3.4399999999999995},{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999995,{"$error":"#VALUE!"},3.4399999999999995,{"$error":"#VALUE!"},3.4399999999999995,{"$error":"#VALUE!"},3.4399999999999995,0,{"$f":"+W149","v":3.7599999999999993},0,{"$f":"+W150","v":3.7599999999999993},0,{"$f":"+W150","v":3.7599999999999993},0,3.7599999999999993,0,{"$f":"+AA150","v":3.7599999999999993},0,3.7599999999999993,0,0,0,3.7599999999999993,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XI-XI",{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+E150-('Analiza i dimenzioniranje'!E$48-'Analiza i dimenzioniranje'!E$52)/15","v":3.1199999999999997},{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999997,{"$error":"#VALUE!"},3.1199999999999997,{"$error":"#VALUE!"},3.1199999999999997,0,{"$f":"+U150","v":3.4399999999999995},0,{"$f":"+S151","v":3.1199999999999997},0,3.1199999999999997,0,{"$f":"+W151","v":3.1199999999999997},0,3.1199999999999997,0,{"$f":"+AA151","v":3.1199999999999997},0,3.1199999999999997,0,0,0,{"$f":"+AK150","v":3.7599999999999993},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek X-X",{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+E151-('Analiza i dimenzioniranje'!E$48-'Analiza i dimenzioniranje'!E$52)/15","v":2.8},{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.8,{"$error":"#VALUE!"},2.8,0,{"$f":"+S151","v":3.1199999999999997},0,3.1199999999999997,0,{"$f":"+W151","v":3.1199999999999997},0,3.1199999999999997,0,{"$f":"+W152","v":3.1199999999999997},0,3.1199999999999997,0,{"$f":"+AE151","v":3.1199999999999997},0,3.1199999999999997,0,0,{"$f":"+AD152","v":0},3.1199999999999997,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek IX-IX",{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+E152-('Analiza i dimenzioniranje'!E$48-'Analiza i dimenzioniranje'!E$52)/15","v":2.48},{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.48,0,{"$f":"+Q152","v":2.8},0,{"$f":"+O153","v":2.48},0,2.48,0,{"$f":"+S153","v":2.48},0,2.48,0,{"$f":"+W152","v":3.1199999999999997},0,3.1199999999999997,0,{"$f":"+AA153","v":3.1199999999999997},0,3.1199999999999997,0,0,0,3.1199999999999997,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VIII-VIII",{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+E153-('Analiza i dimenzioniranje'!E$48-'Analiza i dimenzioniranje'!E$52)/15","v":2.16},{"$error":"#VALUE!"},2.1599999999999993,{"$error":"#VALUE!"},2.1599999999999993,{"$f":"+F154","v":{"$error":"#VALUE!"}},2.1599999999999993,{"$error":"#VALUE!"},2.1599999999999993,0,{"$f":"+O153","v":2.48},0,{"$f":"+O154","v":2.48},0,{"$f":"+O154","v":2.48},0,2.48,0,{"$f":"+W153","v":2.48},0,2.48,0,{"$f":"+W154","v":2.48},0,2.48,{"$f":"+Z154","v":0},2.48,0,2.48,0,0,0,2.48,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VII-VII",{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+E154-('Analiza i dimenzioniranje'!E$48-'Analiza i dimenzioniranje'!E$52)/15","v":1.84},{"$error":"#VALUE!"},1.8399999999999992,{"$error":"#VALUE!"},1.8399999999999992,{"$error":"#VALUE!"},1.8399999999999992,0,{"$f":"+M154","v":2.1599999999999993},0,{"$f":"+E155","v":1.84},0,1.84,0,{"$f":"+S154","v":2.48},0,2.48,{"$f":"+R155","v":0},{"$f":"+O155","v":1.84},0,1.84,{"$f":"+V155","v":0},1.84,0,1.84,0,1.84,0,1.84,0,0,0,1.84,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VI-VI",{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+E155-('Analiza i dimenzioniranje'!E$48-'Analiza i dimenzioniranje'!E$52)/15","v":1.52},{"$error":"#VALUE!"},1.5199999999999991,{"$error":"#VALUE!"},1.5199999999999991,0,{"$f":"+K155","v":1.8399999999999992},0,1.5199999999999991,0,{"$f":"+E156","v":1.52},0,1.52,0,{"$f":"+O156","v":1.52},0,1.52,0,{"$f":"+S156","v":1.52},0,1.52,0,1.52,0,1.52,0,1.52,0,1.52,0,0,0,1.52,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek III -III",{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$f":"+E156-('Analiza i dimenzioniranje'!E$48-'Analiza i dimenzioniranje'!E$52)/15","v":1.2},{"$error":"#VALUE!"},1.1999999999999991,0,{"$f":"+I156","v":1.5199999999999991},0,{"$f":"+E156","v":1.52},0,1.1999999999999991,{"$f":"+J157","v":0},{"$f":"+E157","v":1.2},0,1.2,{"$f":"+N157","v":0},{"$f":"+O157","v":1.2},0,1.2,0,{"$f":"+S157","v":1.2},0,1.2,0,1.2,0,1.2,0,1.2,0,1.2,0,1.2,0,1.2,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["IV-IV=Mmin",null,null,0,{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2},0,1.2,0,1.2,{"$f":"+F158","v":0},1.2,0,1.2,{"$f":"+J158","v":0},{"$f":"+K158","v":1.2},0,1.2,0,{"$f":"+O158","v":1.2},0,1.2,0,{"$f":"+S158","v":1.2},0,1.2,0,1.2,0,{"$f":"+AA158","v":1.2},0,1.2,0,1.2,0,1.2,0,1.2,null,0,9,16,51.999999999999993,0,null,0,36,9,45.000000000000007,0,{"$f":"+AL158*2","v":0}]
["V-V = Mmax",null,null,{"$f":"+AS159","v":0},{"$f":"+E138","v":{"$error":"#VALUE!"}},0,{"$f":"+G138","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},{"$f":"+F159","v":0},{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},{"$f":"+J159","v":0},{"$f":"+K159","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$f":"+O159","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$f":"+S159","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$f":"+AA159","v":{"$error":"#VALUE!"}},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},0,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AW159*2","v":0}]
[null,"Ukupni pritisak",null,"SQhi=",{"$f":"+E163","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+G163","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I163","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K163","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+M163","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+O163","v":{"$error":"#VALUE!"}},{"$f":"+N160","v":"SQhi="},{"$f":"+Q163","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+S163","v":{"$error":"#VALUE!"}},{"$f":"+R160","v":"SQhi="},{"$f":"+U163","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+W163","v":{"$error":"#VALUE!"}},{"$f":"+V160","v":"SQhi="},{"$f":"+Y163","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AA163","v":{"$error":"#VALUE!"}},{"$f":"+Z160","v":"SQhi="},{"$f":"+AC163","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AE163","v":{"$error":"#VALUE!"}},{"$f":"+AB160","v":"SQhi="},{"$f":"+AG163","v":{"$error":"#VALUE!"}},{"$f":"+AF160","v":"SQhi="},{"$f":"+AI163","v":{"$error":"#VALUE!"}},{"$f":"+AF160","v":"SQhi="},{"$f":"+AK163","v":{"$error":"#VALUE!"}}]
[null,"Koordinata težišta ",null," y=",{"$f":"+E165","v":{"$error":"#VALUE!"}}," y=",{"$f":"+G165","v":{"$error":"#VALUE!"}}," y=",{"$f":"+I165","v":{"$error":"#VALUE!"}},{"$f":"+F161","v":" y="},{"$f":"+K165","v":{"$error":"#VALUE!"}},{"$f":"+J161","v":" y="},{"$f":"+M165","v":{"$error":"#VALUE!"}},{"$f":"+J161","v":" y="},{"$f":"+O165","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Q165","v":{"$error":"#VALUE!"}}," y=",{"$f":"+S165","v":{"$error":"#VALUE!"}}," y=",{"$f":"+U165","v":{"$error":"#VALUE!"}}," y=",{"$f":"+W165","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Y165","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AA165","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AC165","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AE165","v":{"$error":"#VALUE!"}},{"$f":"+AD161","v":" y="},{"$f":"+AG165","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AI165","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AK165","v":{"$error":"#VALUE!"}}]
[null,"krak za presjek III -III",null,"z=",{"$f":"+E161-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+G161-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I161-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K161-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M161-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+O161-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Q161-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+S161-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}},"z=",{"$f":"+U161-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+W161-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Y161-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AA161-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AC161-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AE161-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AG161-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AI161-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AK161-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}}]
[null,null,null,"F=",{"$f":"-0.5*((D141*E142-D142*E141)+\n (D142*E143-D143*E142)+\n(D143*E144-D144*E143)+\n(D144*E145-D145*E144)+\n(D145*E146-D146*E145)+\n(D146*E147-D147*E146)+\n(D147*E148-D148*E147)+\n(D148*E149-D149*E148)+\n(D149*E150-D150*E149)+\n(D150*E151-D151*E150)+\n(D151*E152-D152*E151)+\n(D152*E153-D153*E152)+\n(D153*E154-D154*E153)+\n(D154*E155-D155*E154)+\n(D155*E156-D156*E155)+\n(D156*E157-D157*E156)+\n(D157*E158-D158*E157)+\n(D158*E159-D159*E158))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((F141*G142-F142*G141)+\n (F142*G143-F143*G142)+\n(F143*G144-F144*G143)+\n(F144*G145-F145*G144)+\n(F145*G146-F146*G145)+\n(F146*G147-F147*G146)+\n(F147*G148-F148*G147)+\n(F148*G149-F149*G148)+\n(F149*G150-F150*G149)+\n(F150*G151-F151*G150)+\n(F151*G152-F152*G151)+\n(F152*G153-F153*G152)+\n(F153*G154-F154*G153)+\n(F154*G155-F155*G154)+\n(F155*G156-F156*G155)+\n(F156*G157-F157*G156)+\n(F157*G158-F158*G157)+\n(F158*G159-F159*G158))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((H141*I142-H142*I141)+\n (H142*I143-H143*I142)+\n(H143*I144-H144*I143)+\n(H144*I145-H145*I144)+\n(H145*I146-H146*I145)+\n(H146*I147-H147*I146)+\n(H147*I148-H148*I147)+\n(H148*I149-H149*I148)+\n(H149*I150-H150*I149)+\n(H150*I151-H151*I150)+\n(H151*I152-H152*I151)+\n(H152*I153-H153*I152)+\n(H153*I154-H154*I153)+\n(H154*I155-H155*I154)+\n(H155*I156-H156*I155)+\n(H156*I157-H157*I156)+\n(H157*I158-H158*I157)+\n(H158*I159-H159*I158))","v":{"$error":"#VALUE!"}},{"$f":"+F163","v":"F="},{"$f":"-0.5*((J141*K142-J142*K141)+\n (J142*K143-J143*K142)+\n(J143*K144-J144*K143)+\n(J144*K145-J145*K144)+\n(J145*K146-J146*K145)+\n(J146*K147-J147*K146)+\n(J147*K148-J148*K147)+\n(J148*K149-J149*K148)+\n(J149*K150-J150*K149)+\n(J150*K151-J151*K150)+\n(J151*K152-J152*K151)+\n(J152*K153-J153*K152)+\n(J153*K154-J154*K153)+\n(J154*K155-J155*K154)+\n(J155*K156-J156*K155)+\n(J156*K157-J157*K156)+\n(J157*K158-J158*K157)+\n(J158*K159-J159*K158))","v":{"$error":"#VALUE!"}},{"$f":"+J163","v":"F="},{"$f":"-0.5*((L141*M142-L142*M141)+\n (L142*M143-L143*M142)+\n(L143*M144-L144*M143)+\n(L144*M145-L145*M144)+\n(L145*M146-L146*M145)+\n(L146*M147-L147*M146)+\n(L147*M148-L148*M147)+\n(L148*M149-L149*M148)+\n(L149*M150-L150*M149)+\n(L150*M151-L151*M150)+\n(L151*M152-L152*M151)+\n(L152*M153-L153*M152)+\n(L153*M154-L154*M153)+\n(L154*M155-L155*M154)+\n(L155*M156-L156*M155)+\n(L156*M157-L157*M156)+\n(L157*M158-L158*M157)+\n(L158*M159-L159*M158))","v":{"$error":"#VALUE!"}},{"$f":"+J163","v":"F="},{"$f":"-0.5*((N141*O142-N142*O141)+\n (N142*O143-N143*O142)+\n(N143*O144-N144*O143)+\n(N144*O145-N145*O144)+\n(N145*O146-N146*O145)+\n(N146*O147-N147*O146)+\n(N147*O148-N148*O147)+\n(N148*O149-N149*O148)+\n(N149*O150-N150*O149)+\n(N150*O151-N151*O150)+\n(N151*O152-N152*O151)+\n(N152*O153-N153*O152)+\n(N153*O154-N154*O153)+\n(N154*O155-N155*O154)+\n(N155*O156-N156*O155)+\n(N156*O157-N157*O156)+\n(N157*O158-N158*O157)+\n(N158*O159-N159*O158))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((P141*Q142-P142*Q141)+\n (P142*Q143-P143*Q142)+\n(P143*Q144-P144*Q143)+\n(P144*Q145-P145*Q144)+\n(P145*Q146-P146*Q145)+\n(P146*Q147-P147*Q146)+\n(P147*Q148-P148*Q147)+\n(P148*Q149-P149*Q148)+\n(P149*Q150-P150*Q149)+\n(P150*Q151-P151*Q150)+\n(P151*Q152-P152*Q151)+\n(P152*Q153-P153*Q152)+\n(P153*Q154-P154*Q153)+\n(P154*Q155-P155*Q154)+\n(P155*Q156-P156*Q155)+\n(P156*Q157-P157*Q156)+\n(P157*Q158-P158*Q157)+\n(P158*Q159-P159*Q158))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((R141*S142-R142*S141)+\n (R142*S143-R143*S142)+\n(R143*S144-R144*S143)+\n(R144*S145-R145*S144)+\n(R145*S146-R146*S145)+\n(R146*S147-R147*S146)+\n(R147*S148-R148*S147)+\n(R148*S149-R149*S148)+\n(R149*S150-R150*S149)+\n(R150*S151-R151*S150)+\n(R151*S152-R152*S151)+\n(R152*S153-R153*S152)+\n(R153*S154-R154*S153)+\n(R154*S155-R155*S154)+\n(R155*S156-R156*S155)+\n(R156*S157-R157*S156)+\n(R157*S158-R158*S157)+\n(R158*S159-R159*S158))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((T141*U142-T142*U141)+\n (T142*U143-T143*U142)+\n(T143*U144-T144*U143)+\n(T144*U145-T145*U144)+\n(T145*U146-T146*U145)+\n(T146*U147-T147*U146)+\n(T147*U148-T148*U147)+\n(T148*U149-T149*U148)+\n(T149*U150-T150*U149)+\n(T150*U151-T151*U150)+\n(T151*U152-T152*U151)+\n(T152*U153-T153*U152)+\n(T153*U154-T154*U153)+\n(T154*U155-T155*U154)+\n(T155*U156-T156*U155)+\n(T156*U157-T157*U156)+\n(T157*U158-T158*U157)+\n(T158*U159-T159*U158))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((V141*W142-V142*W141)+\n (V142*W143-V143*W142)+\n(V143*W144-V144*W143)+\n(V144*W145-V145*W144)+\n(V145*W146-V146*W145)+\n(V146*W147-V147*W146)+\n(V147*W148-V148*W147)+\n(V148*W149-V149*W148)+\n(V149*W150-V150*W149)+\n(V150*W151-V151*W150)+\n(V151*W152-V152*W151)+\n(V152*W153-V153*W152)+\n(V153*W154-V154*W153)+\n(V154*W155-V155*W154)+\n(V155*W156-V156*W155)+\n(V156*W157-V157*W156)+\n(V157*W158-V158*W157)+\n(V158*W159-V159*W158))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((X141*Y142-X142*Y141)+\n (X142*Y143-X143*Y142)+\n(X143*Y144-X144*Y143)+\n(X144*Y145-X145*Y144)+\n(X145*Y146-X146*Y145)+\n(X146*Y147-X147*Y146)+\n(X147*Y148-X148*Y147)+\n(X148*Y149-X149*Y148)+\n(X149*Y150-X150*Y149)+\n(X150*Y151-X151*Y150)+\n(X151*Y152-X152*Y151)+\n(X152*Y153-X153*Y152)+\n(X153*Y154-X154*Y153)+\n(X154*Y155-X155*Y154)+\n(X155*Y156-X156*Y155)+\n(X156*Y157-X157*Y156)+\n(X157*Y158-X158*Y157)+\n(X158*Y159-X159*Y158))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((Z141*AA142-Z142*AA141)+\n (Z142*AA143-Z143*AA142)+\n(Z143*AA144-Z144*AA143)+\n(Z144*AA145-Z145*AA144)+\n(Z145*AA146-Z146*AA145)+\n(Z146*AA147-Z147*AA146)+\n(Z147*AA148-Z148*AA147)+\n(Z148*AA149-Z149*AA148)+\n(Z149*AA150-Z150*AA149)+\n(Z150*AA151-Z151*AA150)+\n(Z151*AA152-Z152*AA151)+\n(Z152*AA153-Z153*AA152)+\n(Z153*AA154-Z154*AA153)+\n(Z154*AA155-Z155*AA154)+\n(Z155*AA156-Z156*AA155)+\n(Z156*AA157-Z157*AA156)+\n(Z157*AA158-Z158*AA157)+\n(Z158*AA159-Z159*AA158))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AB141*AC142-AB142*AC141)+\n (AB142*AC143-AB143*AC142)+\n(AB143*AC144-AB144*AC143)+\n(AB144*AC145-AB145*AC144)+\n(AB145*AC146-AB146*AC145)+\n(AB146*AC147-AB147*AC146)+\n(AB147*AC148-AB148*AC147)+\n(AB148*AC149-AB149*AC148)+\n(AB149*AC150-AB150*AC149)+\n(AB150*AC151-AB151*AC150)+\n(AB151*AC152-AB152*AC151)+\n(AB152*AC153-AB153*AC152)+\n(AB153*AC154-AB154*AC153)+\n(AB154*AC155-AB155*AC154)+\n(AB155*AC156-AB156*AC155)+\n(AB156*AC157-AB157*AC156)+\n(AB157*AC158-AB158*AC157)+\n(AB158*AC159-AB159*AC158))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AD141*AE142-AD142*AE141)+\n (AD142*AE143-AD143*AE142)+\n(AD143*AE144-AD144*AE143)+\n(AD144*AE145-AD145*AE144)+\n(AD145*AE146-AD146*AE145)+\n(AD146*AE147-AD147*AE146)+\n(AD147*AE148-AD148*AE147)+\n(AD148*AE149-AD149*AE148)+\n(AD149*AE150-AD150*AE149)+\n(AD150*AE151-AD151*AE150)+\n(AD151*AE152-AD152*AE151)+\n(AD152*AE153-AD153*AE152)+\n(AD153*AE154-AD154*AE153)+\n(AD154*AE155-AD155*AE154)+\n(AD155*AE156-AD156*AE155)+\n(AD156*AE157-AD157*AE156)+\n(AD157*AE158-AD158*AE157)+\n(AD158*AE159-AD159*AE158))","v":{"$error":"#VALUE!"}},{"$f":"+AD163","v":"F="},{"$f":"-0.5*((AF141*AG142-AF142*AG141)+\n (AF142*AG143-AF143*AG142)+\n(AF143*AG144-AF144*AG143)+\n(AF144*AG145-AF145*AG144)+\n(AF145*AG146-AF146*AG145)+\n(AF146*AG147-AF147*AG146)+\n(AF147*AG148-AF148*AG147)+\n(AF148*AG149-AF149*AG148)+\n(AF149*AG150-AF150*AG149)+\n(AF150*AG151-AF151*AG150)+\n(AF151*AG152-AF152*AG151)+\n(AF152*AG153-AF153*AG152)+\n(AF153*AG154-AF154*AG153)+\n(AF154*AG155-AF155*AG154)+\n(AF155*AG156-AF156*AG155)+\n(AF156*AG157-AF157*AG156)+\n(AF157*AG158-AF158*AG157)+\n(AF158*AG159-AF159*AG158))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AH141*AI142-AH142*AI141)+\n (AH142*AI143-AH143*AI142)+\n(AH143*AI144-AH144*AI143)+\n(AH144*AI145-AH145*AI144)+\n(AH145*AI146-AH146*AI145)+\n(AH146*AI147-AH147*AI146)+\n(AH147*AI148-AH148*AI147)+\n(AH148*AI149-AH149*AI148)+\n(AH149*AI150-AH150*AI149)+\n(AH150*AI151-AH151*AI150)+\n(AH151*AI152-AH152*AI151)+\n(AH152*AI153-AH153*AI152)+\n(AH153*AI154-AH154*AI153)+\n(AH154*AI155-AH155*AI154)+\n(AH155*AI156-AH156*AI155)+\n(AH156*AI157-AH157*AI156)+\n(AH157*AI158-AH158*AI157)+\n(AH158*AI159-AH159*AI158))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AJ141*AK142-AJ142*AK141)+\n (AJ142*AK143-AJ143*AK142)+\n(AJ143*AK144-AJ144*AK143)+\n(AJ144*AK145-AJ145*AK144)+\n(AJ145*AK146-AJ146*AK145)+\n(AJ146*AK147-AJ147*AK146)+\n(AJ147*AK148-AJ148*AK147)+\n(AJ148*AK149-AJ149*AK148)+\n(AJ149*AK150-AJ150*AK149)+\n(AJ150*AK151-AJ151*AK150)+\n(AJ151*AK152-AJ152*AK151)+\n(AJ152*AK153-AJ153*AK152)+\n(AJ153*AK154-AJ154*AK153)+\n(AJ154*AK155-AJ155*AK154)+\n(AJ155*AK156-AJ156*AK155)+\n(AJ156*AK157-AJ157*AK156)+\n(AJ157*AK158-AJ158*AK157)+\n(AJ158*AK159-AJ159*AK158))","v":{"$error":"#VALUE!"}}]
[null,null,null,"x=",4,"x=",0,"x=",0,{"$f":"+F164","v":"x="},0,{"$f":"+J164","v":"x="},0,{"$f":"+J164","v":"x="},0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,{"$f":"+AD164","v":"x="},0,"x=",0,"x=",0]
[null,null,null,"y=",{"$f":"+IF(E163=0,0,-((D141*E142-D142*E141)*(E141+E142)+\n(D142*E143-D143*E142)*(E142+E143)+\n(D143*E144-D144*E143)*(E143+E144)+\n(D144*E145-D145*E144)*(E144+E145)+\n(D145*E146-D146*E145)*(E145+E146)+\n(D146*E147-D147*E146)*(E146+E147)+\n(D147*E148-D148*E147)*(E147+E148)+\n(D148*E149-D149*E148)*(E148+E149)+\n(D149*E150-D150*E149)*(E149+E150)+\n(D150*E151-D151*E150)*(E150+E151)+\n(D151*E152-D152*E151)*(E151+E152)+\n(D152*E153-D153*E152)*(E152+E153)+\n(D153*E154-D154*E153)*(E153+E154)+\n(D154*E155-D155*E154)*(E154+E155)+\n(D155*E156-D156*E155)*(E155+E156)+\n(D156*E157-D157*E156)*(E156+E157)+\n(D157*E158-D158*E157)*(E157+E158)+\n(D158*E159-D159*E158)*(E158+E159))/6/E163)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(G163=0,0,-((F141*G142-F142*G141)*(G141+G142)+\n(F142*G143-F143*G142)*(G142+G143)+\n(F143*G144-F144*G143)*(G143+G144)+\n(F144*G145-F145*G144)*(G144+G145)+\n(F145*G146-F146*G145)*(G145+G146)+\n(F146*G147-F147*G146)*(G146+G147)+\n(F147*G148-F148*G147)*(G147+G148)+\n(F148*G149-F149*G148)*(G148+G149)+\n(F149*G150-F150*G149)*(G149+G150)+\n(F150*G151-F151*G150)*(G150+G151)+\n(F151*G152-F152*G151)*(G151+G152)+\n(F152*G153-F153*G152)*(G152+G153)+\n(F153*G154-F154*G153)*(G153+G154)+\n(F154*G155-F155*G154)*(G154+G155)+\n(F155*G156-F156*G155)*(G155+G156)+\n(F156*G157-F157*G156)*(G156+G157)+\n(F157*G158-F158*G157)*(G157+G158)+\n(F158*G159-F159*G158)*(G158+G159))/6/G163)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(I163=0,0,-((H141*I142-H142*I141)*(I141+I142)+\n(H142*I143-H143*I142)*(I142+I143)+\n(H143*I144-H144*I143)*(I143+I144)+\n(H144*I145-H145*I144)*(I144+I145)+\n(H145*I146-H146*I145)*(I145+I146)+\n(H146*I147-H147*I146)*(I146+I147)+\n(H147*I148-H148*I147)*(I147+I148)+\n(H148*I149-H149*I148)*(I148+I149)+\n(H149*I150-H150*I149)*(I149+I150)+\n(H150*I151-H151*I150)*(I150+I151)+\n(H151*I152-H152*I151)*(I151+I152)+\n(H152*I153-H153*I152)*(I152+I153)+\n(H153*I154-H154*I153)*(I153+I154)+\n(H154*I155-H155*I154)*(I154+I155)+\n(H155*I156-H156*I155)*(I155+I156)+\n(H156*I157-H157*I156)*(I156+I157)+\n(H157*I158-H158*I157)*(I157+I158)+\n(H158*I159-H159*I158)*(I158+I159))/6/I163)","v":{"$error":"#VALUE!"}},{"$f":"+F165","v":"y="},{"$f":"+IF(K163=0,0,-((J141*K142-J142*K141)*(K141+K142)+\n(J142*K143-J143*K142)*(K142+K143)+\n(J143*K144-J144*K143)*(K143+K144)+\n(J144*K145-J145*K144)*(K144+K145)+\n(J145*K146-J146*K145)*(K145+K146)+\n(J146*K147-J147*K146)*(K146+K147)+\n(J147*K148-J148*K147)*(K147+K148)+\n(J148*K149-J149*K148)*(K148+K149)+\n(J149*K150-J150*K149)*(K149+K150)+\n(J150*K151-J151*K150)*(K150+K151)+\n(J151*K152-J152*K151)*(K151+K152)+\n(J152*K153-J153*K152)*(K152+K153)+\n(J153*K154-J154*K153)*(K153+K154)+\n(J154*K155-J155*K154)*(K154+K155)+\n(J155*K156-J156*K155)*(K155+K156)+\n(J156*K157-J157*K156)*(K156+K157)+\n(J157*K158-J158*K157)*(K157+K158)+\n(J158*K159-J159*K158)*(K158+K159))/6/K163)","v":{"$error":"#VALUE!"}},{"$f":"+J165","v":"y="},{"$f":"+IF(M163=0,0,-((L141*M142-L142*M141)*(M141+M142)+\n(L142*M143-L143*M142)*(M142+M143)+\n(L143*M144-L144*M143)*(M143+M144)+\n(L144*M145-L145*M144)*(M144+M145)+\n(L145*M146-L146*M145)*(M145+M146)+\n(L146*M147-L147*M146)*(M146+M147)+\n(L147*M148-L148*M147)*(M147+M148)+\n(L148*M149-L149*M148)*(M148+M149)+\n(L149*M150-L150*M149)*(M149+M150)+\n(L150*M151-L151*M150)*(M150+M151)+\n(L151*M152-L152*M151)*(M151+M152)+\n(L152*M153-L153*M152)*(M152+M153)+\n(L153*M154-L154*M153)*(M153+M154)+\n(L154*M155-L155*M154)*(M154+M155)+\n(L155*M156-L156*M155)*(M155+M156)+\n(L156*M157-L157*M156)*(M156+M157)+\n(L157*M158-L158*M157)*(M157+M158)+\n(L158*M159-L159*M158)*(M158+M159))/6/M163)","v":{"$error":"#VALUE!"}},{"$f":"+J165","v":"y="},{"$f":"+IF(O163=0,0,-((N141*O142-N142*O141)*(O141+O142)+\n(N142*O143-N143*O142)*(O142+O143)+\n(N143*O144-N144*O143)*(O143+O144)+\n(N144*O145-N145*O144)*(O144+O145)+\n(N145*O146-N146*O145)*(O145+O146)+\n(N146*O147-N147*O146)*(O146+O147)+\n(N147*O148-N148*O147)*(O147+O148)+\n(N148*O149-N149*O148)*(O148+O149)+\n(N149*O150-N150*O149)*(O149+O150)+\n(N150*O151-N151*O150)*(O150+O151)+\n(N151*O152-N152*O151)*(O151+O152)+\n(N152*O153-N153*O152)*(O152+O153)+\n(N153*O154-N154*O153)*(O153+O154)+\n(N154*O155-N155*O154)*(O154+O155)+\n(N155*O156-N156*O155)*(O155+O156)+\n(N156*O157-N157*O156)*(O156+O157)+\n(N157*O158-N158*O157)*(O157+O158)+\n(N158*O159-N159*O158)*(O158+O159))/6/O163)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Q163=0,0,-((P141*Q142-P142*Q141)*(Q141+Q142)+\n(P142*Q143-P143*Q142)*(Q142+Q143)+\n(P143*Q144-P144*Q143)*(Q143+Q144)+\n(P144*Q145-P145*Q144)*(Q144+Q145)+\n(P145*Q146-P146*Q145)*(Q145+Q146)+\n(P146*Q147-P147*Q146)*(Q146+Q147)+\n(P147*Q148-P148*Q147)*(Q147+Q148)+\n(P148*Q149-P149*Q148)*(Q148+Q149)+\n(P149*Q150-P150*Q149)*(Q149+Q150)+\n(P150*Q151-P151*Q150)*(Q150+Q151)+\n(P151*Q152-P152*Q151)*(Q151+Q152)+\n(P152*Q153-P153*Q152)*(Q152+Q153)+\n(P153*Q154-P154*Q153)*(Q153+Q154)+\n(P154*Q155-P155*Q154)*(Q154+Q155)+\n(P155*Q156-P156*Q155)*(Q155+Q156)+\n(P156*Q157-P157*Q156)*(Q156+Q157)+\n(P157*Q158-P158*Q157)*(Q157+Q158)+\n(P158*Q159-P159*Q158)*(Q158+Q159))/6/Q163)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(S163=0,0,-((R141*S142-R142*S141)*(S141+S142)+\n(R142*S143-R143*S142)*(S142+S143)+\n(R143*S144-R144*S143)*(S143+S144)+\n(R144*S145-R145*S144)*(S144+S145)+\n(R145*S146-R146*S145)*(S145+S146)+\n(R146*S147-R147*S146)*(S146+S147)+\n(R147*S148-R148*S147)*(S147+S148)+\n(R148*S149-R149*S148)*(S148+S149)+\n(R149*S150-R150*S149)*(S149+S150)+\n(R150*S151-R151*S150)*(S150+S151)+\n(R151*S152-R152*S151)*(S151+S152)+\n(R152*S153-R153*S152)*(S152+S153)+\n(R153*S154-R154*S153)*(S153+S154)+\n(R154*S155-R155*S154)*(S154+S155)+\n(R155*S156-R156*S155)*(S155+S156)+\n(R156*S157-R157*S156)*(S156+S157)+\n(R157*S158-R158*S157)*(S157+S158)+\n(R158*S159-R159*S158)*(S158+S159))/6/S163)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(U163=0,0,-((T141*U142-T142*U141)*(U141+U142)+\n(T142*U143-T143*U142)*(U142+U143)+\n(T143*U144-T144*U143)*(U143+U144)+\n(T144*U145-T145*U144)*(U144+U145)+\n(T145*U146-T146*U145)*(U145+U146)+\n(T146*U147-T147*U146)*(U146+U147)+\n(T147*U148-T148*U147)*(U147+U148)+\n(T148*U149-T149*U148)*(U148+U149)+\n(T149*U150-T150*U149)*(U149+U150)+\n(T150*U151-T151*U150)*(U150+U151)+\n(T151*U152-T152*U151)*(U151+U152)+\n(T152*U153-T153*U152)*(U152+U153)+\n(T153*U154-T154*U153)*(U153+U154)+\n(T154*U155-T155*U154)*(U154+U155)+\n(T155*U156-T156*U155)*(U155+U156)+\n(T156*U157-T157*U156)*(U156+U157)+\n(T157*U158-T158*U157)*(U157+U158)+\n(T158*U159-T159*U158)*(U158+U159))/6/U163)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(W163=0,0,-((V141*W142-V142*W141)*(W141+W142)+\n(V142*W143-V143*W142)*(W142+W143)+\n(V143*W144-V144*W143)*(W143+W144)+\n(V144*W145-V145*W144)*(W144+W145)+\n(V145*W146-V146*W145)*(W145+W146)+\n(V146*W147-V147*W146)*(W146+W147)+\n(V147*W148-V148*W147)*(W147+W148)+\n(V148*W149-V149*W148)*(W148+W149)+\n(V149*W150-V150*W149)*(W149+W150)+\n(V150*W151-V151*W150)*(W150+W151)+\n(V151*W152-V152*W151)*(W151+W152)+\n(V152*W153-V153*W152)*(W152+W153)+\n(V153*W154-V154*W153)*(W153+W154)+\n(V154*W155-V155*W154)*(W154+W155)+\n(V155*W156-V156*W155)*(W155+W156)+\n(V156*W157-V157*W156)*(W156+W157)+\n(V157*W158-V158*W157)*(W157+W158)+\n(V158*W159-V159*W158)*(W158+W159))/6/W163)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Y163=0,0,-((X141*Y142-X142*Y141)*(Y141+Y142)+\n(X142*Y143-X143*Y142)*(Y142+Y143)+\n(X143*Y144-X144*Y143)*(Y143+Y144)+\n(X144*Y145-X145*Y144)*(Y144+Y145)+\n(X145*Y146-X146*Y145)*(Y145+Y146)+\n(X146*Y147-X147*Y146)*(Y146+Y147)+\n(X147*Y148-X148*Y147)*(Y147+Y148)+\n(X148*Y149-X149*Y148)*(Y148+Y149)+\n(X149*Y150-X150*Y149)*(Y149+Y150)+\n(X150*Y151-X151*Y150)*(Y150+Y151)+\n(X151*Y152-X152*Y151)*(Y151+Y152)+\n(X152*Y153-X153*Y152)*(Y152+Y153)+\n(X153*Y154-X154*Y153)*(Y153+Y154)+\n(X154*Y155-X155*Y154)*(Y154+Y155)+\n(X155*Y156-X156*Y155)*(Y155+Y156)+\n(X156*Y157-X157*Y156)*(Y156+Y157)+\n(X157*Y158-X158*Y157)*(Y157+Y158)+\n(X158*Y159-X159*Y158)*(Y158+Y159))/6/Y163)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AA163=0,0,-((Z141*AA142-Z142*AA141)*(AA141+AA142)+\n(Z142*AA143-Z143*AA142)*(AA142+AA143)+\n(Z143*AA144-Z144*AA143)*(AA143+AA144)+\n(Z144*AA145-Z145*AA144)*(AA144+AA145)+\n(Z145*AA146-Z146*AA145)*(AA145+AA146)+\n(Z146*AA147-Z147*AA146)*(AA146+AA147)+\n(Z147*AA148-Z148*AA147)*(AA147+AA148)+\n(Z148*AA149-Z149*AA148)*(AA148+AA149)+\n(Z149*AA150-Z150*AA149)*(AA149+AA150)+\n(Z150*AA151-Z151*AA150)*(AA150+AA151)+\n(Z151*AA152-Z152*AA151)*(AA151+AA152)+\n(Z152*AA153-Z153*AA152)*(AA152+AA153)+\n(Z153*AA154-Z154*AA153)*(AA153+AA154)+\n(Z154*AA155-Z155*AA154)*(AA154+AA155)+\n(Z155*AA156-Z156*AA155)*(AA155+AA156)+\n(Z156*AA157-Z157*AA156)*(AA156+AA157)+\n(Z157*AA158-Z158*AA157)*(AA157+AA158)+\n(Z158*AA159-Z159*AA158)*(AA158+AA159))/6/AA163)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AC163=0,0,-((AB141*AC142-AB142*AC141)*(AC141+AC142)+\n(AB142*AC143-AB143*AC142)*(AC142+AC143)+\n(AB143*AC144-AB144*AC143)*(AC143+AC144)+\n(AB144*AC145-AB145*AC144)*(AC144+AC145)+\n(AB145*AC146-AB146*AC145)*(AC145+AC146)+\n(AB146*AC147-AB147*AC146)*(AC146+AC147)+\n(AB147*AC148-AB148*AC147)*(AC147+AC148)+\n(AB148*AC149-AB149*AC148)*(AC148+AC149)+\n(AB149*AC150-AB150*AC149)*(AC149+AC150)+\n(AB150*AC151-AB151*AC150)*(AC150+AC151)+\n(AB151*AC152-AB152*AC151)*(AC151+AC152)+\n(AB152*AC153-AB153*AC152)*(AC152+AC153)+\n(AB153*AC154-AB154*AC153)*(AC153+AC154)+\n(AB154*AC155-AB155*AC154)*(AC154+AC155)+\n(AB155*AC156-AB156*AC155)*(AC155+AC156)+\n(AB156*AC157-AB157*AC156)*(AC156+AC157)+\n(AB157*AC158-AB158*AC157)*(AC157+AC158)+\n(AB158*AC159-AB159*AC158)*(AC158+AC159))/6/AC163)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AE163=0,0,-((AD141*AE142-AD142*AE141)*(AE141+AE142)+\n(AD142*AE143-AD143*AE142)*(AE142+AE143)+\n(AD143*AE144-AD144*AE143)*(AE143+AE144)+\n(AD144*AE145-AD145*AE144)*(AE144+AE145)+\n(AD145*AE146-AD146*AE145)*(AE145+AE146)+\n(AD146*AE147-AD147*AE146)*(AE146+AE147)+\n(AD147*AE148-AD148*AE147)*(AE147+AE148)+\n(AD148*AE149-AD149*AE148)*(AE148+AE149)+\n(AD149*AE150-AD150*AE149)*(AE149+AE150)+\n(AD150*AE151-AD151*AE150)*(AE150+AE151)+\n(AD151*AE152-AD152*AE151)*(AE151+AE152)+\n(AD152*AE153-AD153*AE152)*(AE152+AE153)+\n(AD153*AE154-AD154*AE153)*(AE153+AE154)+\n(AD154*AE155-AD155*AE154)*(AE154+AE155)+\n(AD155*AE156-AD156*AE155)*(AE155+AE156)+\n(AD156*AE157-AD157*AE156)*(AE156+AE157)+\n(AD157*AE158-AD158*AE157)*(AE157+AE158)+\n(AD158*AE159-AD159*AE158)*(AE158+AE159))/6/AE163)","v":{"$error":"#VALUE!"}},{"$f":"+AD165","v":"y="},{"$f":"+IF(AG163=0,0,-((AF141*AG142-AF142*AG141)*(AG141+AG142)+\n(AF142*AG143-AF143*AG142)*(AG142+AG143)+\n(AF143*AG144-AF144*AG143)*(AG143+AG144)+\n(AF144*AG145-AF145*AG144)*(AG144+AG145)+\n(AF145*AG146-AF146*AG145)*(AG145+AG146)+\n(AF146*AG147-AF147*AG146)*(AG146+AG147)+\n(AF147*AG148-AF148*AG147)*(AG147+AG148)+\n(AF148*AG149-AF149*AG148)*(AG148+AG149)+\n(AF149*AG150-AF150*AG149)*(AG149+AG150)+\n(AF150*AG151-AF151*AG150)*(AG150+AG151)+\n(AF151*AG152-AF152*AG151)*(AG151+AG152)+\n(AF152*AG153-AF153*AG152)*(AG152+AG153)+\n(AF153*AG154-AF154*AG153)*(AG153+AG154)+\n(AF154*AG155-AF155*AG154)*(AG154+AG155)+\n(AF155*AG156-AF156*AG155)*(AG155+AG156)+\n(AF156*AG157-AF157*AG156)*(AG156+AG157)+\n(AF157*AG158-AF158*AG157)*(AG157+AG158)+\n(AF158*AG159-AF159*AG158)*(AG158+AG159))/6/AG163)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AI163=0,0,-((AH141*AI142-AH142*AI141)*(AI141+AI142)+\n(AH142*AI143-AH143*AI142)*(AI142+AI143)+\n(AH143*AI144-AH144*AI143)*(AI143+AI144)+\n(AH144*AI145-AH145*AI144)*(AI144+AI145)+\n(AH145*AI146-AH146*AI145)*(AI145+AI146)+\n(AH146*AI147-AH147*AI146)*(AI146+AI147)+\n(AH147*AI148-AH148*AI147)*(AI147+AI148)+\n(AH148*AI149-AH149*AI148)*(AI148+AI149)+\n(AH149*AI150-AH150*AI149)*(AI149+AI150)+\n(AH150*AI151-AH151*AI150)*(AI150+AI151)+\n(AH151*AI152-AH152*AI151)*(AI151+AI152)+\n(AH152*AI153-AH153*AI152)*(AI152+AI153)+\n(AH153*AI154-AH154*AI153)*(AI153+AI154)+\n(AH154*AI155-AH155*AI154)*(AI154+AI155)+\n(AH155*AI156-AH156*AI155)*(AI155+AI156)+\n(AH156*AI157-AH157*AI156)*(AI156+AI157)+\n(AH157*AI158-AH158*AI157)*(AI157+AI158)+\n(AH158*AI159-AH159*AI158)*(AI158+AI159))/6/AI163)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AK163=0,0,-((AJ141*AK142-AJ142*AK141)*(AK141+AK142)+\n(AJ142*AK143-AJ143*AK142)*(AK142+AK143)+\n(AJ143*AK144-AJ144*AK143)*(AK143+AK144)+\n(AJ144*AK145-AJ145*AK144)*(AK144+AK145)+\n(AJ145*AK146-AJ146*AK145)*(AK145+AK146)+\n(AJ146*AK147-AJ147*AK146)*(AK146+AK147)+\n(AJ147*AK148-AJ148*AK147)*(AK147+AK148)+\n(AJ148*AK149-AJ149*AK148)*(AK148+AK149)+\n(AJ149*AK150-AJ150*AK149)*(AK149+AK150)+\n(AJ150*AK151-AJ151*AK150)*(AK150+AK151)+\n(AJ151*AK152-AJ152*AK151)*(AK151+AK152)+\n(AJ152*AK153-AJ153*AK152)*(AK152+AK153)+\n(AJ153*AK154-AJ154*AK153)*(AK153+AK154)+\n(AJ154*AK155-AJ155*AK154)*(AK154+AK155)+\n(AJ155*AK156-AJ156*AK155)*(AK155+AK156)+\n(AJ156*AK157-AJ157*AK156)*(AK156+AK157)+\n(AJ157*AK158-AJ158*AK157)*(AK157+AK158)+\n(AJ158*AK159-AJ159*AK158)*(AK158+AK159))/6/AK163)","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID "]
[null,null,null,"OPTEREĆENJE TEMELJEM"]
[]
[null,"KONTINUIRANO OPTEREĆENJE",null,"P - D=",{"$f":"IF('Analiza i dimenzioniranje'!$E$28=0,0,+'Analiza i dimenzioniranje'!$E$28-I170)","v":{"$error":"#VALUE!"}},"kN/m2","raster. iskopom   D=y*Df =",null,{"$f":"+'Analiza i dimenzioniranje'!$D$16*('Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20-D176)","v":{"$error":"#VALUE!"}},"kN/m2"]
[null," visina zida i temelja",null,"H =",{"$f":"+$E$131","v":{"$error":"#VALUE!"}},"m",{"$f":"E175","v":6}]
[null,"visina opterećenja iznad vrha zida",null,"h =",{"$f":"+E$132","v":-1},"m",{"$f":"SQRT(E175^2+E174^2)","v":6.7082039324993694}]
[null,"širina temelja",null,"b =",{"$f":"+E133","v":1},"m   ",{"$f":"E174+E173","v":4}]
[null,"udaljenost temelja od zida",null,"D =",{"$f":"+E134","v":3},"m    "]
[null,"1/2 dužine temelja",null,"L/2=a=",{"$f":"+$E135","v":6},"m",{"$f":"SQRT(G171^2+G173^2)","v":7.2111025509279782}]
["DNO TEMELJA NA VISINI","PRESJEK NA Visini ",null,{"$f":"ROUND(+'Analiza i dimenzioniranje'!U67,2)","v":6},{"$f":"+('Analiza i dimenzioniranje'!E48-'Analiza i dimenzioniranje'!E52)/15","v":0.32},"Presjek III -III",null,"Presjek VI-VI",null,"Presjek VII-VII",null,"Presjek VIII-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"Presjek XIV-XIV",null,"Presjek XV-XV",null,"PresjekXVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX"]
[null,null,null,null,null,"(sb2-sb2)*2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja"]
[null,null,null,null,null,null,{"$f":"+G180","v":0},null,{"$f":"+G178","v":0},null,{"$f":"+I178","v":0},null,{"$f":"+K178","v":0},null,{"$f":"+M178","v":0},null,{"$f":"+O178","v":0},null,{"$f":"+Q178","v":0},null,{"$f":"+S178","v":0},null,{"$f":"+U178","v":0},null,{"$f":"+W178","v":0},null,{"$f":"+Y178","v":0},null,{"$f":"+AA178","v":0},null,{"$f":"+AC178","v":0},null,{"$f":"+AE178","v":0},null,{"$f":"+AG178","v":0},null,{"$f":"+AI178","v":0}]
[null,null,null,{"$f":"+('Analiza i dimenzioniranje'!$E$48-'Analiza i dimenzioniranje'!$E$52)/15","v":0.32},null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
["Presjek X-X",null,null,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Presjek X-X",null,null,{"$f":"+F141","v":0},null,0,{"$f":"+'Analiza i dimenzioniranje'!E48","v":6},{"$f":"+F182","v":0},{"$f":"+G182","v":6},{"$f":"+F182","v":0},6,{"$f":"+F182","v":0},{"$f":"+K182","v":6},{"$f":"+J182","v":0},6,{"$f":"+N182","v":0},{"$f":"+O182","v":6},{"$f":"+N182","v":0},6,{"$f":"+R182","v":0},{"$f":"+S182","v":6},{"$f":"+R182","v":0},6,0,{"$f":"+W182","v":6},{"$f":"+V182","v":0},6,{"$f":"+Z182","v":0},{"$f":"+W182","v":6},{"$f":"+Z182","v":0},6,{"$f":"+AD181","v":0},{"$f":"+AC182","v":6},{"$f":"+AF181","v":0},{"$f":"+AE182","v":6},0,{"$f":"+O182","v":6},null,{"$f":"+D182","v":0},{"$f":"$E$174^2+AM182^2","v":9},{"$f":"$G$173^2+AM182^2","v":16},{"$f":"$G$175^2+AM182^2","v":51.999999999999993},{"$f":"IF(AM182=0,0,$E$170/(PI())*(ATAN(($E$175*$G$173)/(AM182*SQRT(AP182)))-$E$175*$G$173*AM182/(AO182*SQRT(AP182))))","v":0},null,{"$f":"+AM182","v":0},{"$f":"$E$175^2+AS182^2","v":36},{"$f":"$E$174^2+AS182^2","v":9},{"$f":"$G$172^2+AS182^2","v":45.000000000000007},{"$f":"IF(AS182=0,0,($E$170/(PI()))*(ATAN(($E$175*$E$134)/(AS182*SQRT(AV182)))-$E$175*$E$174*AS182/(AU182*SQRT(AV182))))","v":0},{"$f":"+(AQ182-AW182)*2","v":0}]
["Presjek XIX-XIX",null,null,{"$f":"+G182-$G$183","v":0.32000000000000028},null,{"$f":"+AX183","v":{"$error":"#VALUE!"}},{"$f":"+G182-$E$176","v":5.68},{"$f":"+F183","v":{"$error":"#VALUE!"}},5.68,{"$f":"+F183","v":{"$error":"#VALUE!"}},5.68,{"$f":"+F183","v":{"$error":"#VALUE!"}},{"$f":"+K183","v":5.68},{"$error":"#VALUE!"},5.68,{"$f":"+N183","v":{"$error":"#VALUE!"}},5.68,{"$error":"#VALUE!"},5.68,{"$f":"+R183","v":{"$error":"#VALUE!"}},5.68,{"$error":"#VALUE!"},5.68,{"$f":"+V183","v":{"$error":"#VALUE!"}},5.68,{"$error":"#VALUE!"},5.68,{"$f":"+Z183","v":{"$error":"#VALUE!"}},{"$f":"+W183","v":5.68},{"$error":"#VALUE!"},5.68,{"$f":"+AD183","v":{"$error":"#VALUE!"}},{"$f":"+AC183","v":5.68},{"$f":"+AF183","v":{"$error":"#VALUE!"}},5.68,0,{"$f":"+AK182","v":6},null,0.32000000000000028,{"$f":"$E$174^2+AM183^2","v":9.1023999999999994},{"$f":"$G$173^2+AM183^2","v":16.102399999999999},{"$f":"$G$175^2+AM183^2","v":52.102399999999996},{"$f":"IF(AM183=0,0,$E$170/(PI())*(ATAN(($E$175*$G$173)/(AM183*SQRT(AP183)))-$E$175*$G$173*AM183/(AO183*SQRT(AP183))))","v":{"$error":"#VALUE!"}},null,{"$f":"+AM183","v":0.32000000000000028},{"$f":"$E$175^2+AS183^2","v":36.102400000000003},{"$f":"$E$174^2+AS183^2","v":9.1023999999999994},{"$f":"$G$172^2+AS183^2","v":45.10240000000001},{"$f":"IF(AS183=0,0,($E$170/(PI()))*(ATAN(($E$175*$E$134)/(AS183*SQRT(AV183)))-$E$175*$E$174*AS183/(AU183*SQRT(AV183))))","v":{"$error":"#VALUE!"}},{"$f":"+(AQ183-AW183)*2","v":{"$error":"#VALUE!"}}]
["Presjek XVIII-XVIII",null,null,{"$f":"+D183+D$179","v":0.64000000000000035},null,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$f":"+F184","v":{"$error":"#VALUE!"}},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$error":"#VALUE!"},5.3599999999999994,{"$f":"+Z184","v":{"$error":"#VALUE!"}},{"$f":"+W184","v":5.3599999999999994},{"$error":"#VALUE!"},5.3599999999999994,{"$f":"+AD184","v":{"$error":"#VALUE!"}},{"$f":"+AC184","v":5.3599999999999994},0,{"$f":"+AI183","v":5.68},0,{"$f":"+G184","v":5.3599999999999994},null,0.64000000000000035,9.4096000000000011,16.409600000000001,52.40959999999999,{"$error":"#VALUE!"},null,0.64000000000000035,{"$f":"$E$175^2+AS184^2","v":36.409599999999998},9.4096000000000011,{"$f":"$G$172^2+AS184^2","v":45.409600000000005},{"$f":"IF(AS184=0,0,($E$170/(PI()))*(ATAN(($E$175*$E$134)/(AS184*SQRT(AV184)))-$E$175*$E$174*AS184/(AU184*SQRT(AV184))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["Presjek XVII-XVII",null,null,{"$f":"+D184+D$179","v":0.96000000000000041},null,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$error":"#VALUE!"},5.0399999999999991,{"$f":"+Z185","v":{"$error":"#VALUE!"}},{"$f":"+W185","v":5.0399999999999991},{"$error":"#VALUE!"},5.0399999999999991,0,{"$f":"+AG184","v":5.3599999999999994},0,{"$f":"+AI184","v":5.68},0,{"$f":"+G185","v":5.0399999999999991},null,0.96000000000000041,9.9216000000000015,16.921600000000002,52.921599999999991,{"$error":"#VALUE!"},null,{"$f":"+AM185","v":0.96000000000000041},{"$f":"$E$175^2+AS185^2","v":36.921599999999998},9.9216000000000015,45.921600000000005,{"$error":"#VALUE!"},{"$f":"+(AQ185-AW185)*2","v":{"$error":"#VALUE!"}}]
["Presjek XVI-XVI",null,null,1.2800000000000005,null,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$f":"+Z186","v":{"$error":"#VALUE!"}},{"$f":"+W186","v":4.7199999999999989},0,{"$f":"+AE185","v":5.0399999999999991},0,{"$f":"+AG185","v":5.3599999999999994},0,{"$f":"+Y186","v":4.7199999999999989},0,4.7199999999999989,null,1.2800000000000005,10.638400000000001,17.638400000000001,53.638399999999997,{"$error":"#VALUE!"},null,1.2800000000000005,37.638400000000004,10.638400000000001,46.638400000000011,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XV-XV",null,null,1.6000000000000005,null,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,0,{"$f":"+AC186","v":4.7199999999999989},0,4.3999999999999986,0,{"$f":"+AE187","v":4.3999999999999986},0,{"$f":"+Y187","v":4.3999999999999986},0,4.3999999999999986,null,1.6000000000000005,11.560000000000002,18.560000000000002,54.559999999999995,{"$error":"#VALUE!"},null,1.6000000000000005,38.56,11.560000000000002,47.560000000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XIV-XIV",null,null,1.9200000000000006,null,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,0,{"$f":"+AA187","v":4.3999999999999986},0,{"$f":"+AC187","v":4.7199999999999989},0,4.3999999999999986,0,4.3999999999999986,0,{"$f":"+Y188","v":4.0799999999999983},0,4.0799999999999983,null,1.9200000000000006,12.686400000000003,19.686400000000003,55.686399999999992,{"$error":"#VALUE!"},null,1.9200000000000006,39.686399999999999,12.686400000000003,48.686400000000006,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XIII-XIII",null,null,2.2400000000000007,null,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,0,{"$f":"+Y188","v":4.0799999999999983},0,{"$f":"+AA188","v":4.3999999999999986},0,{"$f":"+W189","v":3.7599999999999985},0,4.3999999999999986,0,4.3999999999999986,0,4.3999999999999986,0,3.7599999999999985,null,2.2400000000000007,14.017600000000002,21.017600000000002,57.017599999999995,{"$error":"#VALUE!"},null,2.2400000000000007,41.017600000000002,14.017600000000002,50.017600000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek  XII-XII",null,null,2.5600000000000005,null,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,0,{"$f":"+W189","v":3.7599999999999985},0,{"$f":"+Y189","v":4.0799999999999983},0,{"$f":"+W190","v":3.7599999999999985},0,3.7599999999999985,0,3.7599999999999985,0,3.7599999999999985,0,3.7599999999999985,0,3.4399999999999986,null,2.5600000000000005,15.553600000000003,22.553600000000003,58.553599999999996,{"$error":"#VALUE!"},null,2.5600000000000005,42.553600000000003,15.553600000000003,51.55360000000001,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XI-XI",null,null,2.8800000000000003,null,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,0,{"$f":"+U190","v":3.4399999999999986},0,{"$f":"+W190","v":3.7599999999999985},0,{"$f":"+W191","v":3.7599999999999985},0,{"$f":"+W191","v":3.7599999999999985},0,3.7599999999999985,0,{"$f":"+AC191","v":3.7599999999999985},0,3.7599999999999985,0,3.7599999999999985,0,3.1199999999999988,null,2.8800000000000003,17.294400000000003,24.294400000000003,60.294399999999996,{"$error":"#VALUE!"},null,2.8800000000000003,44.294400000000003,17.294400000000003,53.29440000000001,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek X-X",null,null,3.2,null,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,0,{"$f":"+S191","v":3.1199999999999988},0,{"$f":"+U191","v":3.4399999999999986},0,{"$f":"+O312","v":2.8000000000000003},{"$f":"+R193","v":0},2.8000000000000003,0,{"$f":"+W192","v":2.8000000000000003},0,2.8000000000000003,0,{"$f":"+AC192","v":2.8000000000000003},0,2.8000000000000003,0,2.8000000000000003,0,2.7999999999999989,null,3.2,19.240000000000002,26.240000000000002,62.239999999999995,{"$error":"#VALUE!"},null,3.2,46.24,19.240000000000002,55.240000000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek IX-IX",null,null,3.52,null,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,0,{"$f":"+Q192","v":2.7999999999999989},0,{"$f":"+S192","v":3.1199999999999988},0,3.1199999999999988,0,{"$f":"+O313","v":2.4800000000000004},0,2.4800000000000004,0,2.4800000000000004,0,2.4800000000000004,0,2.4800000000000004,0,2.4800000000000004,0,2.4800000000000004,0,2.4799999999999991,null,3.52,21.3904,28.3904,64.3904,{"$error":"#VALUE!"},null,3.52,48.3904,21.3904,57.390400000000007,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VIII-VIII",null,null,3.84,null,{"$error":"#VALUE!"},2.1599999999999993,{"$error":"#VALUE!"},2.1599999999999993,{"$error":"#VALUE!"},2.1599999999999993,{"$error":"#VALUE!"},2.1599999999999993,0,{"$f":"+O193","v":2.4799999999999991},0,{"$f":"+G194","v":2.1599999999999993},0,{"$f":"+AM314","v":2.2400000000000002},0,2.2400000000000002,0,{"$f":"+W193","v":2.4800000000000004},0,2.4800000000000004,0,2.4800000000000004,0,2.4800000000000004,0,2.4800000000000004,0,2.4800000000000004,0,2.4800000000000004,0,2.1599999999999993,null,3.84,23.7456,30.7456,66.745599999999996,{"$error":"#VALUE!"},null,3.84,50.745599999999996,23.7456,59.74560000000001,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VII-VII",null,null,4.16,null,{"$error":"#VALUE!"},1.8399999999999992,{"$error":"#VALUE!"},1.8399999999999992,{"$error":"#VALUE!"},1.8399999999999992,0,{"$f":"+M194","v":2.1599999999999993},0,1.8399999999999992,0,{"$f":"+Q194","v":2.1599999999999993},0,{"$f":"+S194","v":2.2400000000000002},0,2.2400000000000002,0,{"$f":"+O315","v":0},0,0,0,0,0,0,{"$f":"+Z195","v":0},0,0,0,0,0,0,1.8399999999999992,null,4.16,26.305600000000002,33.305599999999998,69.305599999999998,{"$error":"#VALUE!"},null,4.16,53.305599999999998,26.305600000000002,62.305600000000013,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VI-VI",null,null,4.4800000000000004,null,{"$error":"#VALUE!"},1.5199999999999991,{"$error":"#VALUE!"},1.5199999999999991,0,{"$f":"+K195","v":1.8399999999999992},0,1.8399999999999992,0,1.8399999999999992,0,{"$f":"+Q195","v":2.1599999999999993},0,{"$f":"+AM316","v":2.88},0,2.88,0,{"$f":"+O316","v":0},0,0,0,0,0,0,{"$f":"+Z196","v":0},0,0,0,0,0,0,1.5199999999999991,null,4.4800000000000004,29.070400000000003,36.070400000000006,72.070399999999992,{"$error":"#VALUE!"},null,4.4800000000000004,56.070400000000006,29.070400000000003,65.070400000000006,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek III -III",null,null,4.8000000000000007,null,{"$error":"#VALUE!"},1.1999999999999991,0,{"$f":"+I196","v":1.5199999999999991},0,{"$f":"+G196","v":1.5199999999999991},0,1.5199999999999991,0,{"$f":"+O194+O193","v":4.9599999999999982},0,{"$f":"+Q198","v":1.1999999999999991},0,{"$f":"+S198","v":1.1999999999999991},0,1.1999999999999991,0,{"$f":"+U197","v":1.1999999999999991},{"$f":"+R198","v":0},1.1999999999999991,0,1.1999999999999991,0,1.1999999999999991,{"$f":"+Z197","v":0},{"$f":"+AE198","v":1.1999999999999991},0,1.1999999999999991,0,1.1999999999999991,0,1.1999999999999991,null,4.8000000000000007,32.040000000000006,39.040000000000006,75.039999999999992,{"$error":"#VALUE!"},null,4.8000000000000007,59.040000000000006,32.040000000000006,68.04000000000002,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["IV-IV=Mmin",null,null,null,null,0,{"$f":"+G197","v":1.1999999999999991},0,1.1999999999999991,0,{"$f":"+I198","v":1.1999999999999991},0,1.1999999999999991,{"$f":"+J318","v":0},{"$f":"+K198","v":1.1999999999999991},0,1.1999999999999991,0,{"$f":"+Q198","v":1.1999999999999991},0,1.1999999999999991,{"$f":"+N318","v":0},{"$f":"+U198","v":1.1999999999999991},0,1.1999999999999991,{"$f":"+AN318","v":0},{"$f":"+AA197","v":1.1999999999999991},0,1.1999999999999991,{"$f":"+AP318","v":0},{"$f":"+AC198","v":1.1999999999999991},0,1.1999999999999991,0,1.1999999999999991,{"$f":"+AR318","v":0},{"$f":"+O198","v":1.1999999999999991},null,0,9,16,51.999999999999993,0,null,0,36,9,45.000000000000007,0,0]
["V-V = Mmax",null,null,null,null,{"$f":"+D158","v":0},{"$f":"+'Analiza i dimenzioniranje'!E48","v":6},0,6,0,{"$f":"+I199","v":6},0,6,{"$f":"+J319","v":0},{"$f":"+M199","v":6},0,6,0,{"$f":"+Q199","v":6},0,6,{"$f":"+N319","v":0},{"$f":"+U199","v":6},0,6,{"$f":"+AN319","v":0},{"$f":"+Y199","v":6},0,6,{"$f":"+AP319","v":0},{"$f":"+AC199","v":6},0,6,0,6,{"$f":"+AR319","v":0},{"$f":"+AI199","v":6},null,0,9,16,51.999999999999993,0,null,0,36,9,45.000000000000007,0,0]
[null,null,null,"Ukupni pritisak",null,"SQhi=",{"$f":"+G203","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I203","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K203","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+M203","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+O203","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Q203","v":{"$error":"#VALUE!"}},{"$f":"+N200","v":"SQhi="},{"$f":"+S203","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+U203","v":{"$error":"#VALUE!"}},{"$f":"+R200","v":"SQhi="},{"$f":"+W203","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Y203","v":{"$error":"#VALUE!"}},{"$f":"+V200","v":"SQhi="},{"$f":"+AA203","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AC203","v":{"$error":"#VALUE!"}},{"$f":"+Z200","v":"SQhi="},{"$f":"+AE203","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AG203","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AI203","v":{"$error":"#VALUE!"}},{"$f":"+AD200","v":"SQhi="},{"$f":"+AK203","v":0}]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G205","v":{"$error":"#VALUE!"}},{"$f":"+H205","v":"y="},{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",0]
[null,null,null,"krak za presjek III -III",null,"z=",{"$f":"+G201-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I201-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K201-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M201-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+O201-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Q201-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+S201-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+U201-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}},"z=",{"$f":"+W201-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Y201-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AA201-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AC201-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AE201-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AG201-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AI201-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AK201-'Analiza i dimenzioniranje'!$E$52","v":-1.2}]
[null,null,null,null,null,"F=",{"$f":"-0.5*((F181*G182-F182*G181)+\n (F182*G183-F183*G182)+\n(F183*G184-F184*G183)+\n(F184*G185-F185*G184)+\n(F185*G186-F186*G185)+\n(F186*G187-F187*G186)+\n(F187*G188-F188*G187)+\n(F188*G189-F189*G188)+\n(F189*G190-F190*G189)+\n(F190*G191-F191*G190)+\n(F191*G192-F192*G191)+\n(F192*G193-F193*G192)+\n(F193*G194-F194*G193)+\n(F194*G195-F195*G194)+\n(F195*G196-F196*G195)+\n(F196*G197-F197*G196)+\n(F197*G198-F198*G197)+\n(F198*G199-F199*G198))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((H181*I182-H182*I181)+\n (H182*I183-H183*I182)+\n(H183*I184-H184*I183)+\n(H184*I185-H185*I184)+\n(H185*I186-H186*I185)+\n(H186*I187-H187*I186)+\n(H187*I188-H188*I187)+\n(H188*I189-H189*I188)+\n(H189*I190-H190*I189)+\n(H190*I191-H191*I190)+\n(H191*I192-H192*I191)+\n(H192*I193-H193*I192)+\n(H193*I194-H194*I193)+\n(H194*I195-H195*I194)+\n(H195*I196-H196*I195)+\n(H196*I197-H197*I196)+\n(H197*I198-H198*I197)+\n(H198*I199-H199*I198))","v":{"$error":"#VALUE!"}},{"$f":"+F203","v":"F="},{"$f":"-0.5*(+(J181*K182-J182*K181)+\n (J182*K183-J183*K182)+\n(J183*K184-J184*K183)+\n(J184*K185-J185*K184)+\n(J185*K186-J186*K185)+\n(J186*K187-J187*K186)+\n(J187*K188-J188*K187)+\n(J188*K189-J189*K188)+\n(J189*K190-J190*K189)+\n(J190*K191-J191*K190)+\n(J191*K192-J192*K191)+\n(J192*K193-J193*K192)+\n(J193*K194-J194*K193)+\n(J194*K195-J195*K194)+\n(J195*K196-J196*K195)+\n(J196*K197-J197*K196)+\n(J197*K198-J198*K197)+\n(J198*K199-J199*K198))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+(L181*M182-L182*M181)+\n (L182*M183-L183*M182)+\n(L183*M184-L184*M183)+\n(L184*M185-L185*M184)+\n(L185*M186-L186*M185)+\n(L186*M187-L187*M186)+\n(L187*M188-L188*M187)+\n(L188*M189-L189*M188)+\n(L189*M190-L190*M189)+\n(L190*M191-L191*M190)+\n(L191*M192-L192*M191)+\n(L192*M193-L193*M192)+\n(L193*M194-L194*M193)+\n(L194*M195-L195*M194)+\n(L195*M196-L196*M195)+\n(L196*M197-L197*M196)+\n(L197*M198-L198*M197)+\n(L198*M199-L199*M198))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+(N181*O182-N182*O181)+\n (N182*O183-N183*O182)+\n(N183*O184-N184*O183)+\n(N184*O185-N185*O184)+\n(N185*O186-N186*O185)+\n(N186*O187-N187*O186)+\n(N187*O188-N188*O187)+\n(N188*O189-N189*O188)+\n(N189*O190-N190*O189)+\n(N190*O191-N191*O190)+\n(N191*O192-N192*O191)+\n(N192*O193-N193*O192)+\n(N193*O194-N194*O193)+\n(N194*O195-N195*O194)+\n(N195*O196-N196*O195)+\n(N196*O197-N197*O196)+\n(N197*O198-N198*O197)+\n(N198*O199-N199*O198))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+(P181*Q182-P182*Q181)+\n (P182*Q183-P183*Q182)+\n(P183*Q184-P184*Q183)+\n(P184*Q185-P185*Q184)+\n(P185*Q186-P186*Q185)+\n(P186*Q187-P187*Q186)+\n(P187*Q188-P188*Q187)+\n(P188*Q189-P189*Q188)+\n(P189*Q190-P190*Q189)+\n(P190*Q191-P191*Q190)+\n(P191*Q192-P192*Q191)+\n(P192*Q193-P193*Q192)+\n(P193*Q194-P194*Q193)+\n(P194*Q195-P195*Q194)+\n(P195*Q196-P196*Q195)+\n(P196*Q197-P197*Q196)+\n(P197*Q198-P198*Q197)+\n(P198*Q199-P199*Q198))","v":{"$error":"#VALUE!"}},{"$f":"+N203","v":"F="},{"$f":"-0.5*(+(R181*S182-R182*S181)+\n (R182*S183-R183*S182)+\n(R183*S184-R184*S183)+\n(R184*S185-R185*S184)+\n(R185*S186-R186*S185)+\n(R186*S187-R187*S186)+\n(R187*S188-R188*S187)+\n(R188*S189-R189*S188)+\n(R189*S190-R190*S189)+\n(R190*S191-R191*S190)+\n(R191*S192-R192*S191)+\n(R192*S193-R193*S192)+\n(R193*S194-R194*S193)+\n(R194*S195-R195*S194)+\n(R195*S196-R196*S195)+\n(R196*S197-R197*S196)+\n(R197*S198-R198*S197)+\n(R198*S199-R199*S198))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+(T181*U182-T182*U181)+\n (T182*U183-T183*U182)+\n(T183*U184-T184*U183)+\n(T184*U185-T185*U184)+\n(T185*U186-T186*U185)+\n(T186*U187-T187*U186)+\n(T187*U188-T188*U187)+\n(T188*U189-T189*U188)+\n(T189*U190-T190*U189)+\n(T190*U191-T191*U190)+\n(T191*U192-T192*U191)+\n(T192*U193-T193*U192)+\n(T193*U194-T194*U193)+\n(T194*U195-T195*U194)+\n(T195*U196-T196*U195)+\n(T196*U197-T197*U196)+\n(T197*U198-T198*U197)+\n(T198*U199-T199*U198))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+(V181*W182-V182*W181)+\n (V182*W183-V183*W182)+\n(V183*W184-V184*W183)+\n(V184*W185-V185*W184)+\n(V185*W186-V186*W185)+\n(V186*W187-V187*W186)+\n(V187*W188-V188*W187)+\n(V188*W189-V189*W188)+\n(V189*W190-V190*W189)+\n(V190*W191-V191*W190)+\n(V191*W192-V192*W191)+\n(V192*W193-V193*W192)+\n(V193*W194-V194*W193)+\n(V194*W195-V195*W194)+\n(V195*W196-V196*W195)+\n(V196*W197-V197*W196)+\n(V197*W198-V198*W197)+\n(V198*W199-V199*W198))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+(X181*Y182-X182*Y181)+\n (X182*Y183-X183*Y182)+\n(X183*Y184-X184*Y183)+\n(X184*Y185-X185*Y184)+\n(X185*Y186-X186*Y185)+\n(X186*Y187-X187*Y186)+\n(X187*Y188-X188*Y187)+\n(X188*Y189-X189*Y188)+\n(X189*Y190-X190*Y189)+\n(X190*Y191-X191*Y190)+\n(X191*Y192-X192*Y191)+\n(X192*Y193-X193*Y192)+\n(X193*Y194-X194*Y193)+\n(X194*Y195-X195*Y194)+\n(X195*Y196-X196*Y195)+\n(X196*Y197-X197*Y196)+\n(X197*Y198-X198*Y197)+\n(X198*Y199-X199*Y198))","v":{"$error":"#VALUE!"}},{"$f":"+V203","v":"F="},{"$f":"-0.5*(+(Z181*AA182-Z182*AA181)+\n (Z182*AA183-Z183*AA182)+\n(Z183*AA184-Z184*AA183)+\n(Z184*AA185-Z185*AA184)+\n(Z185*AA186-Z186*AA185)+\n(Z186*AA187-Z187*AA186)+\n(Z187*AA188-Z188*AA187)+\n(Z188*AA189-Z189*AA188)+\n(Z189*AA190-Z190*AA189)+\n(Z190*AA191-Z191*AA190)+\n(Z191*AA192-Z192*AA191)+\n(Z192*AA193-Z193*AA192)+\n(Z193*AA194-Z194*AA193)+\n(Z194*AA195-Z195*AA194)+\n(Z195*AA196-Z196*AA195)+\n(Z196*AA197-Z197*AA196)+\n(Z197*AA198-Z198*AA197)+\n(Z198*AA199-Z199*AA198))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+(AB181*AC182-AB182*AC181)+\n (AB182*AC183-AB183*AC182)+\n(AB183*AC184-AB184*AC183)+\n(AB184*AC185-AB185*AC184)+\n(AB185*AC186-AB186*AC185)+\n(AB186*AC187-AB187*AC186)+\n(AB187*AC188-AB188*AC187)+\n(AB188*AC189-AB189*AC188)+\n(AB189*AC190-AB190*AC189)+\n(AB190*AC191-AB191*AC190)+\n(AB191*AC192-AB192*AC191)+\n(AB192*AC193-AB193*AC192)+\n(AB193*AC194-AB194*AC193)+\n(AB194*AC195-AB195*AC194)+\n(AB195*AC196-AB196*AC195)+\n(AB196*AC197-AB197*AC196)+\n(AB197*AC198-AB198*AC197)+\n(AB198*AC199-AB199*AC198))","v":{"$error":"#VALUE!"}},{"$f":"+Z203","v":"F="},{"$f":"-0.5*(+(AD181*AE182-AD182*AE181)+\n (AD182*AE183-AD183*AE182)+\n(AD183*AE184-AD184*AE183)+\n(AD184*AE185-AD185*AE184)+\n(AD185*AE186-AD186*AE185)+\n(AD186*AE187-AD187*AE186)+\n(AD187*AE188-AD188*AE187)+\n(AD188*AE189-AD189*AE188)+\n(AD189*AE190-AD190*AE189)+\n(AD190*AE191-AD191*AE190)+\n(AD191*AE192-AD192*AE191)+\n(AD192*AE193-AD193*AE192)+\n(AD193*AE194-AD194*AE193)+\n(AD194*AE195-AD195*AE194)+\n(AD195*AE196-AD196*AE195)+\n(AD196*AE197-AD197*AE196)+\n(AD197*AE198-AD198*AE197)+\n(AD198*AE199-AD199*AE198))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+(AF181*AG182-AF182*AG181)+\n (AF182*AG183-AF183*AG182)+\n(AF183*AG184-AF184*AG183)+\n(AF184*AG185-AF185*AG184)+\n(AF185*AG186-AF186*AG185)+\n(AF186*AG187-AF187*AG186)+\n(AF187*AG188-AF188*AG187)+\n(AF188*AG189-AF189*AG188)+\n(AF189*AG190-AF190*AG189)+\n(AF190*AG191-AF191*AG190)+\n(AF191*AG192-AF192*AG191)+\n(AF192*AG193-AF193*AG192)+\n(AF193*AG194-AF194*AG193)+\n(AF194*AG195-AF195*AG194)+\n(AF195*AG196-AF196*AG195)+\n(AF196*AG197-AF197*AG196)+\n(AF197*AG198-AF198*AG197)+\n(AF198*AG199-AF199*AG198))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+(AH181*AI182-AH182*AI181)+\n (AH182*AI183-AH183*AI182)+\n(AH183*AI184-AH184*AI183)+\n(AH184*AI185-AH185*AI184)+\n(AH185*AI186-AH186*AI185)+\n(AH186*AI187-AH187*AI186)+\n(AH187*AI188-AH188*AI187)+\n(AH188*AI189-AH189*AI188)+\n(AH189*AI190-AH190*AI189)+\n(AH190*AI191-AH191*AI190)+\n(AH191*AI192-AH192*AI191)+\n(AH192*AI193-AH193*AI192)+\n(AH193*AI194-AH194*AI193)+\n(AH194*AI195-AH195*AI194)+\n(AH195*AI196-AH196*AI195)+\n(AH196*AI197-AH197*AI196)+\n(AH197*AI198-AH198*AI197)+\n(AH198*AI199-AH199*AI198))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+(AJ181*AK182-AJ182*AK181)+\n (AJ182*AK183-AJ183*AK182)+\n(AJ183*AK184-AJ184*AK183)+\n(AJ184*AK185-AJ185*AK184)+\n(AJ185*AK186-AJ186*AK185)+\n(AJ186*AK187-AJ187*AK186)+\n(AJ187*AK188-AJ188*AK187)+\n(AJ188*AK189-AJ189*AK188)+\n(AJ189*AK190-AJ190*AK189)+\n(AJ190*AK191-AJ191*AK190)+\n(AJ191*AK192-AJ192*AK191)+\n(AJ192*AK193-AJ193*AK192)+\n(AJ193*AK194-AJ194*AK193)+\n(AJ194*AK195-AJ195*AK194)+\n(AJ195*AK196-AJ196*AK195)+\n(AJ196*AK197-AJ197*AK196)+\n(AJ197*AK198-AJ198*AK197)+\n(AJ198*AK199-AJ199*AK198))","v":0}]
[null,null,null,null,null,"x=",4,"x=",0,"x=",4,"x=",0,"x=",4,"x=",0,{"$f":"+N204","v":"x="},{"$f":"+O204","v":4},"x=",{"$f":"+Q204","v":0},"x=",{"$f":"+S204","v":4},"x=",{"$f":"+U204","v":0},{"$f":"+V204","v":"x="},{"$f":"+W204","v":4},"x=",{"$f":"+Y204","v":0},{"$f":"+Z204","v":"x="},{"$f":"+AA204","v":4},"x=",{"$f":"+AC204","v":0},"x=",{"$f":"+AE204","v":4},"x=",{"$f":"+AG204","v":0}]
[null,null,null,null,null,"y=",{"$f":"+IF(G203=0,0,-((F180*G181-F181*G180)*(G180+G181)+(F181*G182-F182*G181)*(G181+G182)+\n(F182*G183-F183*G182)*(G182+G183)+\n(F183*G184-F184*G183)*(G183+G184)+\n(F184*G185-F185*G184)*(G184+G185)+\n(F185*G186-F186*G185)*(G185+G186)+\n(F186*G187-F187*G186)*(G186+G187)+\n(F187*G188-F188*G187)*(G187+G188)+\n(F188*G189-F189*G188)*(G188+G189)+\n(F189*G190-F190*G189)*(G189+G190)+\n(F190*G191-F191*G190)*(G190+G191)+\n(F191*G192-F192*G191)*(G191+G192)+\n(F192*G193-F193*G192)*(G192+G193)+\n(F193*G194-F194*G193)*(G193+G194)+\n(F194*G195-F195*G194)*(G194+G195)+\n(F195*G196-F196*G195)*(G195+G196)+\n(F196*G197-F197*G196)*(G196+G197)+\n(F197*G198-F198*G197)*(G197+G198)+\n(F198*G199-F199*G198)*(G198+G199))/6/G203)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(I203=0,0,-((H180*I181-H181*I180)*(I180+I181)+(H181*I182-H182*I181)*(I181+I182)+\n(H182*I183-H183*I182)*(I182+I183)+\n(H183*I184-H184*I183)*(I183+I184)+\n(H184*I185-H185*I184)*(I184+I185)+\n(H185*I186-H186*I185)*(I185+I186)+\n(H186*I187-H187*I186)*(I186+I187)+\n(H187*I188-H188*I187)*(I187+I188)+\n(H188*I189-H189*I188)*(I188+I189)+\n(H189*I190-H190*I189)*(I189+I190)+\n(H190*I191-H191*I190)*(I190+I191)+\n(H191*I192-H192*I191)*(I191+I192)+\n(H192*I193-H193*I192)*(I192+I193)+\n(H193*I194-H194*I193)*(I193+I194)+\n(H194*I195-H195*I194)*(I194+I195)+\n(H195*I196-H196*I195)*(I195+I196)+\n(H196*I197-H197*I196)*(I196+I197)+\n(H197*I198-H198*I197)*(I197+I198)+\n(H198*I199-H199*I198)*(I198+I199))/6/I203)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(K203=0,0,-((J180*K181-J181*K180)*(K180+K181)+(J181*K182-J182*K181)*(K181+K182)+\n(J182*K183-J183*K182)*(K182+K183)+\n(J183*K184-J184*K183)*(K183+K184)+\n(J184*K185-J185*K184)*(K184+K185)+\n(J185*K186-J186*K185)*(K185+K186)+\n(J186*K187-J187*K186)*(K186+K187)+\n(J187*K188-J188*K187)*(K187+K188)+\n(J188*K189-J189*K188)*(K188+K189)+\n(J189*K190-J190*K189)*(K189+K190)+\n(J190*K191-J191*K190)*(K190+K191)+\n(J191*K192-J192*K191)*(K191+K192)+\n(J192*K193-J193*K192)*(K192+K193)+\n(J193*K194-J194*K193)*(K193+K194)+\n(J194*K195-J195*K194)*(K194+K195)+\n(J195*K196-J196*K195)*(K195+K196)+\n(J196*K197-J197*K196)*(K196+K197)+\n(J197*K198-J198*K197)*(K197+K198)+\n(J198*K199-J199*K198)*(K198+K199))/6/K203)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(M203=0,0,-((L180*M181-L181*M180)*(M180+M181)+(L181*M182-L182*M181)*(M181+M182)+\n(L182*M183-L183*M182)*(M182+M183)+\n(L183*M184-L184*M183)*(M183+M184)+\n(L184*M185-L185*M184)*(M184+M185)+\n(L185*M186-L186*M185)*(M185+M186)+\n(L186*M187-L187*M186)*(M186+M187)+\n(L187*M188-L188*M187)*(M187+M188)+\n(L188*M189-L189*M188)*(M188+M189)+\n(L189*M190-L190*M189)*(M189+M190)+\n(L190*M191-L191*M190)*(M190+M191)+\n(L191*M192-L192*M191)*(M191+M192)+\n(L192*M193-L193*M192)*(M192+M193)+\n(L193*M194-L194*M193)*(M193+M194)+\n(L194*M195-L195*M194)*(M194+M195)+\n(L195*M196-L196*M195)*(M195+M196)+\n(L196*M197-L197*M196)*(M196+M197)+\n(L197*M198-L198*M197)*(M197+M198)+\n(L198*M199-L199*M198)*(M198+M199))/6/M203)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(O203=0,0,-((N180*O181-N181*O180)*(O180+O181)+(N181*O182-N182*O181)*(O181+O182)+\n(N182*O183-N183*O182)*(O182+O183)+\n(N183*O184-N184*O183)*(O183+O184)+\n(N184*O185-N185*O184)*(O184+O185)+\n(N185*O186-N186*O185)*(O185+O186)+\n(N186*O187-N187*O186)*(O186+O187)+\n(N187*O188-N188*O187)*(O187+O188)+\n(N188*O189-N189*O188)*(O188+O189)+\n(N189*O190-N190*O189)*(O189+O190)+\n(N190*O191-N191*O190)*(O190+O191)+\n(N191*O192-N192*O191)*(O191+O192)+\n(N192*O193-N193*O192)*(O192+O193)+\n(N193*O194-N194*O193)*(O193+O194)+\n(N194*O195-N195*O194)*(O194+O195)+\n(N195*O196-N196*O195)*(O195+O196)+\n(N196*O197-N197*O196)*(O196+O197)+\n(N197*O198-N198*O197)*(O197+O198)+\n(N198*O199-N199*O198)*(O198+O199))/6/O203)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Q203=0,0,-((P180*Q181-P181*Q180)*(Q180+Q181)+(P181*Q182-P182*Q181)*(Q181+Q182)+\n(P182*Q183-P183*Q182)*(Q182+Q183)+\n(P183*Q184-P184*Q183)*(Q183+Q184)+\n(P184*Q185-P185*Q184)*(Q184+Q185)+\n(P185*Q186-P186*Q185)*(Q185+Q186)+\n(P186*Q187-P187*Q186)*(Q186+Q187)+\n(P187*Q188-P188*Q187)*(Q187+Q188)+\n(P188*Q189-P189*Q188)*(Q188+Q189)+\n(P189*Q190-P190*Q189)*(Q189+Q190)+\n(P190*Q191-P191*Q190)*(Q190+Q191)+\n(P191*Q192-P192*Q191)*(Q191+Q192)+\n(P192*Q193-P193*Q192)*(Q192+Q193)+\n(P193*Q194-P194*Q193)*(Q193+Q194)+\n(P194*Q195-P195*Q194)*(Q194+Q195)+\n(P195*Q196-P196*Q195)*(Q195+Q196)+\n(P196*Q197-P197*Q196)*(Q196+Q197)+\n(P197*Q198-P198*Q197)*(Q197+Q198)+\n(P198*Q199-P199*Q198)*(Q198+Q199))/6/Q203)","v":{"$error":"#VALUE!"}},{"$f":"+N205","v":"y="},{"$f":"+IF(S203=0,0,-((R180*S181-R181*S180)*(S180+S181)+(R181*S182-R182*S181)*(S181+S182)+\n(R182*S183-R183*S182)*(S182+S183)+\n(R183*S184-R184*S183)*(S183+S184)+\n(R184*S185-R185*S184)*(S184+S185)+\n(R185*S186-R186*S185)*(S185+S186)+\n(R186*S187-R187*S186)*(S186+S187)+\n(R187*S188-R188*S187)*(S187+S188)+\n(R188*S189-R189*S188)*(S188+S189)+\n(R189*S190-R190*S189)*(S189+S190)+\n(R190*S191-R191*S190)*(S190+S191)+\n(R191*S192-R192*S191)*(S191+S192)+\n(R192*S193-R193*S192)*(S192+S193)+\n(R193*S194-R194*S193)*(S193+S194)+\n(R194*S195-R195*S194)*(S194+S195)+\n(R195*S196-R196*S195)*(S195+S196)+\n(R196*S197-R197*S196)*(S196+S197)+\n(R197*S198-R198*S197)*(S197+S198)+\n(R198*S199-R199*S198)*(S198+S199))/6/S203)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(U203=0,0,-((T180*U181-T181*U180)*(U180+U181)+(T181*U182-T182*U181)*(U181+U182)+\n(T182*U183-T183*U182)*(U182+U183)+\n(T183*U184-T184*U183)*(U183+U184)+\n(T184*U185-T185*U184)*(U184+U185)+\n(T185*U186-T186*U185)*(U185+U186)+\n(T186*U187-T187*U186)*(U186+U187)+\n(T187*U188-T188*U187)*(U187+U188)+\n(T188*U189-T189*U188)*(U188+U189)+\n(T189*U190-T190*U189)*(U189+U190)+\n(T190*U191-T191*U190)*(U190+U191)+\n(T191*U192-T192*U191)*(U191+U192)+\n(T192*U193-T193*U192)*(U192+U193)+\n(T193*U194-T194*U193)*(U193+U194)+\n(T194*U195-T195*U194)*(U194+U195)+\n(T195*U196-T196*U195)*(U195+U196)+\n(T196*U197-T197*U196)*(U196+U197)+\n(T197*U198-T198*U197)*(U197+U198)+\n(T198*U199-T199*U198)*(U198+U199))/6/U203)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(W203=0,0,-((V180*W181-V181*W180)*(W180+W181)+(V181*W182-V182*W181)*(W181+W182)+\n(V182*W183-V183*W182)*(W182+W183)+\n(V183*W184-V184*W183)*(W183+W184)+\n(V184*W185-V185*W184)*(W184+W185)+\n(V185*W186-V186*W185)*(W185+W186)+\n(V186*W187-V187*W186)*(W186+W187)+\n(V187*W188-V188*W187)*(W187+W188)+\n(V188*W189-V189*W188)*(W188+W189)+\n(V189*W190-V190*W189)*(W189+W190)+\n(V190*W191-V191*W190)*(W190+W191)+\n(V191*W192-V192*W191)*(W191+W192)+\n(V192*W193-V193*W192)*(W192+W193)+\n(V193*W194-V194*W193)*(W193+W194)+\n(V194*W195-V195*W194)*(W194+W195)+\n(V195*W196-V196*W195)*(W195+W196)+\n(V196*W197-V197*W196)*(W196+W197)+\n(V197*W198-V198*W197)*(W197+W198)+\n(V198*W199-V199*W198)*(W198+W199))/6/W203)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Y203=0,0,-((X180*Y181-X181*Y180)*(Y180+Y181)+(X181*Y182-X182*Y181)*(Y181+Y182)+\n(X182*Y183-X183*Y182)*(Y182+Y183)+\n(X183*Y184-X184*Y183)*(Y183+Y184)+\n(X184*Y185-X185*Y184)*(Y184+Y185)+\n(X185*Y186-X186*Y185)*(Y185+Y186)+\n(X186*Y187-X187*Y186)*(Y186+Y187)+\n(X187*Y188-X188*Y187)*(Y187+Y188)+\n(X188*Y189-X189*Y188)*(Y188+Y189)+\n(X189*Y190-X190*Y189)*(Y189+Y190)+\n(X190*Y191-X191*Y190)*(Y190+Y191)+\n(X191*Y192-X192*Y191)*(Y191+Y192)+\n(X192*Y193-X193*Y192)*(Y192+Y193)+\n(X193*Y194-X194*Y193)*(Y193+Y194)+\n(X194*Y195-X195*Y194)*(Y194+Y195)+\n(X195*Y196-X196*Y195)*(Y195+Y196)+\n(X196*Y197-X197*Y196)*(Y196+Y197)+\n(X197*Y198-X198*Y197)*(Y197+Y198)+\n(X198*Y199-X199*Y198)*(Y198+Y199))/6/Y203)","v":{"$error":"#VALUE!"}},{"$f":"+V205","v":"y="},{"$f":"+IF(AA203=0,0,-((Z180*AA181-Z181*AA180)*(AA180+AA181)+(Z181*AA182-Z182*AA181)*(AA181+AA182)+\n(Z182*AA183-Z183*AA182)*(AA182+AA183)+\n(Z183*AA184-Z184*AA183)*(AA183+AA184)+\n(Z184*AA185-Z185*AA184)*(AA184+AA185)+\n(Z185*AA186-Z186*AA185)*(AA185+AA186)+\n(Z186*AA187-Z187*AA186)*(AA186+AA187)+\n(Z187*AA188-Z188*AA187)*(AA187+AA188)+\n(Z188*AA189-Z189*AA188)*(AA188+AA189)+\n(Z189*AA190-Z190*AA189)*(AA189+AA190)+\n(Z190*AA191-Z191*AA190)*(AA190+AA191)+\n(Z191*AA192-Z192*AA191)*(AA191+AA192)+\n(Z192*AA193-Z193*AA192)*(AA192+AA193)+\n(Z193*AA194-Z194*AA193)*(AA193+AA194)+\n(Z194*AA195-Z195*AA194)*(AA194+AA195)+\n(Z195*AA196-Z196*AA195)*(AA195+AA196)+\n(Z196*AA197-Z197*AA196)*(AA196+AA197)+\n(Z197*AA198-Z198*AA197)*(AA197+AA198)+\n(Z198*AA199-Z199*AA198)*(AA198+AA199))/6/AA203)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AC203=0,0,-((AB180*AC181-AB181*AC180)*(AC180+AC181)+(AB181*AC182-AB182*AC181)*(AC181+AC182)+\n(AB182*AC183-AB183*AC182)*(AC182+AC183)+\n(AB183*AC184-AB184*AC183)*(AC183+AC184)+\n(AB184*AC185-AB185*AC184)*(AC184+AC185)+\n(AB185*AC186-AB186*AC185)*(AC185+AC186)+\n(AB186*AC187-AB187*AC186)*(AC186+AC187)+\n(AB187*AC188-AB188*AC187)*(AC187+AC188)+\n(AB188*AC189-AB189*AC188)*(AC188+AC189)+\n(AB189*AC190-AB190*AC189)*(AC189+AC190)+\n(AB190*AC191-AB191*AC190)*(AC190+AC191)+\n(AB191*AC192-AB192*AC191)*(AC191+AC192)+\n(AB192*AC193-AB193*AC192)*(AC192+AC193)+\n(AB193*AC194-AB194*AC193)*(AC193+AC194)+\n(AB194*AC195-AB195*AC194)*(AC194+AC195)+\n(AB195*AC196-AB196*AC195)*(AC195+AC196)+\n(AB196*AC197-AB197*AC196)*(AC196+AC197)+\n(AB197*AC198-AB198*AC197)*(AC197+AC198)+\n(AB198*AC199-AB199*AC198)*(AC198+AC199))/6/AC203)","v":{"$error":"#VALUE!"}},{"$f":"+Z205","v":"y="},{"$f":"+IF(AE203=0,0,-((AD180*AE181-AD181*AE180)*(AE180+AE181)+(AD181*AE182-AD182*AE181)*(AE181+AE182)+\n(AD182*AE183-AD183*AE182)*(AE182+AE183)+\n(AD183*AE184-AD184*AE183)*(AE183+AE184)+\n(AD184*AE185-AD185*AE184)*(AE184+AE185)+\n(AD185*AE186-AD186*AE185)*(AE185+AE186)+\n(AD186*AE187-AD187*AE186)*(AE186+AE187)+\n(AD187*AE188-AD188*AE187)*(AE187+AE188)+\n(AD188*AE189-AD189*AE188)*(AE188+AE189)+\n(AD189*AE190-AD190*AE189)*(AE189+AE190)+\n(AD190*AE191-AD191*AE190)*(AE190+AE191)+\n(AD191*AE192-AD192*AE191)*(AE191+AE192)+\n(AD192*AE193-AD193*AE192)*(AE192+AE193)+\n(AD193*AE194-AD194*AE193)*(AE193+AE194)+\n(AD194*AE195-AD195*AE194)*(AE194+AE195)+\n(AD195*AE196-AD196*AE195)*(AE195+AE196)+\n(AD196*AE197-AD197*AE196)*(AE196+AE197)+\n(AD197*AE198-AD198*AE197)*(AE197+AE198)+\n(AD198*AE199-AD199*AE198)*(AE198+AE199))/6/AE203)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AG203=0,0,-((AF180*AG181-AF181*AG180)*(AG180+AG181)+(AF181*AG182-AF182*AG181)*(AG181+AG182)+\n(AF182*AG183-AF183*AG182)*(AG182+AG183)+\n(AF183*AG184-AF184*AG183)*(AG183+AG184)+\n(AF184*AG185-AF185*AG184)*(AG184+AG185)+\n(AF185*AG186-AF186*AG185)*(AG185+AG186)+\n(AF186*AG187-AF187*AG186)*(AG186+AG187)+\n(AF187*AG188-AF188*AG187)*(AG187+AG188)+\n(AF188*AG189-AF189*AG188)*(AG188+AG189)+\n(AF189*AG190-AF190*AG189)*(AG189+AG190)+\n(AF190*AG191-AF191*AG190)*(AG190+AG191)+\n(AF191*AG192-AF192*AG191)*(AG191+AG192)+\n(AF192*AG193-AF193*AG192)*(AG192+AG193)+\n(AF193*AG194-AF194*AG193)*(AG193+AG194)+\n(AF194*AG195-AF195*AG194)*(AG194+AG195)+\n(AF195*AG196-AF196*AG195)*(AG195+AG196)+\n(AF196*AG197-AF197*AG196)*(AG196+AG197)+\n(AF197*AG198-AF198*AG197)*(AG197+AG198)+\n(AF198*AG199-AF199*AG198)*(AG198+AG199))/6/AG203)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AI203=0,0,-((AH180*AI181-AH181*AI180)*(AI180+AI181)+(AH181*AI182-AH182*AI181)*(AI181+AI182)+\n(AH182*AI183-AH183*AI182)*(AI182+AI183)+\n(AH183*AI184-AH184*AI183)*(AI183+AI184)+\n(AH184*AI185-AH185*AI184)*(AI184+AI185)+\n(AH185*AI186-AH186*AI185)*(AI185+AI186)+\n(AH186*AI187-AH187*AI186)*(AI186+AI187)+\n(AH187*AI188-AH188*AI187)*(AI187+AI188)+\n(AH188*AI189-AH189*AI188)*(AI188+AI189)+\n(AH189*AI190-AH190*AI189)*(AI189+AI190)+\n(AH190*AI191-AH191*AI190)*(AI190+AI191)+\n(AH191*AI192-AH192*AI191)*(AI191+AI192)+\n(AH192*AI193-AH193*AI192)*(AI192+AI193)+\n(AH193*AI194-AH194*AI193)*(AI193+AI194)+\n(AH194*AI195-AH195*AI194)*(AI194+AI195)+\n(AH195*AI196-AH196*AI195)*(AI195+AI196)+\n(AH196*AI197-AH197*AI196)*(AI196+AI197)+\n(AH197*AI198-AH198*AI197)*(AI197+AI198)+\n(AH198*AI199-AH199*AI198)*(AI198+AI199))/6/AI203)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AK203=0,0,-((AJ180*AK181-AJ181*AK180)*(AK180+AK181)+(AJ181*AK182-AJ182*AK181)*(AK181+AK182)+\n(AJ182*AK183-AJ183*AK182)*(AK182+AK183)+\n(AJ183*AK184-AJ184*AK183)*(AK183+AK184)+\n(AJ184*AK185-AJ185*AK184)*(AK184+AK185)+\n(AJ185*AK186-AJ186*AK185)*(AK185+AK186)+\n(AJ186*AK187-AJ187*AK186)*(AK186+AK187)+\n(AJ187*AK188-AJ188*AK187)*(AK187+AK188)+\n(AJ188*AK189-AJ189*AK188)*(AK188+AK189)+\n(AJ189*AK190-AJ190*AK189)*(AK189+AK190)+\n(AJ190*AK191-AJ191*AK190)*(AK190+AK191)+\n(AJ191*AK192-AJ192*AK191)*(AK191+AK192)+\n(AJ192*AK193-AJ193*AK192)*(AK192+AK193)+\n(AJ193*AK194-AJ194*AK193)*(AK193+AK194)+\n(AJ194*AK195-AJ195*AK194)*(AK194+AK195)+\n(AJ195*AK196-AJ196*AK195)*(AK195+AK196)+\n(AJ196*AK197-AJ197*AK196)*(AK196+AK197)+\n(AJ197*AK198-AJ198*AK197)*(AK197+AK198)+\n(AJ198*AK199-AJ199*AK198)*(AK198+AK199))/6/AK203)","v":0}]
[]
[null,null,null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID "]
[null,null,null,"OPTEREĆENJE TEMELJEM"]
[]
[null,"KONTINUIRANO OPTEREĆENJE",null,"P - D=",{"$f":"IF('Analiza i dimenzioniranje'!$E$28-I210<=0,0,+'Analiza i dimenzioniranje'!$E$28-I210)","v":{"$error":"#VALUE!"}},"kN/m2","raster. iskopom   D=y*Df =",null,{"$f":"+'Analiza i dimenzioniranje'!$D$16*('Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20-D216)","v":{"$error":"#VALUE!"}},"kN/m2"]
[null," visina zida i temelja",null,"H =",{"$f":"+E171","v":{"$error":"#VALUE!"}},"m",{"$f":"E215","v":6}]
[null,"visina opterećenja iznad vrha zida",null,"h =",{"$f":"+E172","v":-1},"m",{"$f":"SQRT(E215^2+E214^2)","v":6.7082039324993694}]
[null,"širina temelja",null,"b =",{"$f":"+E173","v":1},"m   ",{"$f":"E214+E213","v":4}]
[null,"udaljenost temelja od zida",null,"D =",{"$f":"+E174","v":3},"m    "]
[null,"1/2 dužine temelja",null,"L/2=a=",{"$f":"+E175","v":6},"m",{"$f":"SQRT(G211^2+G213^2)","v":7.2111025509279782}]
["DNO TEMELJA NA VISINI","PRESJEK NA Visini ",null,{"$f":"ROUND('Analiza i dimenzioniranje'!U64,2)","v":5.04},null,"Presjek III -III",null,"Presjek VI",null,"Presjek VII-VII",null,"Presjek VIII-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"Presjek XIV-XIV",null,"Presjek XV-XV",null,"PresjekXVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX"]
[null,null,null,null,null,"(sb2-sb2)*1","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja"]
[null,null,null,null,null,null,{"$f":"+$D216","v":5.04},null,{"$f":"+$D216","v":5.04},null,{"$f":"+$D216","v":5.04},null,{"$f":"+$D216","v":5.04},null,{"$f":"+$D216","v":5.04},null,{"$f":"+$D216","v":5.04},null,{"$f":"+$D216","v":5.04},null,{"$f":"+$D216","v":5.04},null,{"$f":"+$D216","v":5.04},null,{"$f":"+$D216","v":5.04},null,{"$f":"+$D216","v":5.04},null,{"$f":"+$D216","v":5.04},null,{"$f":"+$D216","v":5.04},null,{"$f":"+$D216","v":5.04},null,{"$f":"+$D216","v":5.04},null,{"$f":"+$D216","v":5.04}]
[null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
[null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Presjek X-X",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Presjek X-X",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Presjek XIX-XIX",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Presjek XVIII-XVIII",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Presjek XVII-XVII",null,null,{"$f":"+D182","v":0},null,0,{"$f":"+G185","v":5.0399999999999991},0,{"$f":"+I185","v":5.0399999999999991},0,{"$f":"+G225","v":5.0399999999999991},0,5.0399999999999991,0,{"$f":"+K225","v":5.0399999999999991},0,{"$f":"+M225","v":5.0399999999999991},0,5.0399999999999991,0,{"$f":"+Q225","v":5.0399999999999991},0,5.0399999999999991,0,{"$f":"+U225","v":5.0399999999999991},0,5.0399999999999991,0,{"$f":"+Y225","v":5.0399999999999991},{"$f":"+Z225","v":0},{"$f":"+G225","v":5.0399999999999991},0,{"$f":"+AC225","v":5.0399999999999991},0,{"$f":"+AE225","v":5.0399999999999991},0,{"$f":"+AE225","v":5.0399999999999991},null,{"$f":"+D225","v":0},{"$f":"$E$214^2+AM225^2","v":9},{"$f":"$G$213^2+AM225^2","v":16},{"$f":"$G$215^2+AM225^2","v":51.999999999999993},{"$f":"IF(AM225=0,0,$E$210/(PI())*(ATAN(($E$215*$G$133)/(AM225*SQRT(AP225)))-$E$215*$G$213*AM225/(AO225*SQRT(AP225))))","v":0},null,{"$f":"+AM225","v":0},{"$f":"$E$215^2+AS225^2","v":36},{"$f":"$E$214^2+AS225^2","v":9},{"$f":"$G$212^2+AS225^2","v":45.000000000000007},{"$f":"IF(AS225=0,0,($E$210/(PI()))*(ATAN(($E$215*$E$214)/(AS225*SQRT(AV225)))-$E$215*$E$214*AS225/(AU225*SQRT(AV225))))","v":0},{"$f":"+(AQ225-AW225)*2","v":0}]
["Presjek XVI-XVI",null,null,0.32000000000000028,null,{"$f":"+AX226","v":{"$error":"#VALUE!"}},4.7199999999999989,{"$f":"+F226","v":{"$error":"#VALUE!"}},4.7199999999999989,{"$f":"+F226","v":{"$error":"#VALUE!"}},4.7199999999999989,{"$f":"+J226","v":{"$error":"#VALUE!"}},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$f":"+N226","v":{"$error":"#VALUE!"}},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$f":"+R226","v":{"$error":"#VALUE!"}},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$f":"+V226","v":{"$error":"#VALUE!"}},4.7199999999999989,{"$error":"#VALUE!"},4.7199999999999989,{"$f":"+Z226","v":{"$error":"#VALUE!"}},{"$f":"+Y226","v":4.7199999999999989},0,{"$f":"+AE225","v":5.0399999999999991},{"$f":"+AD226","v":0},4.7199999999999989,{"$f":"+AF226","v":0},5.0399999999999991,{"$f":"+AD226","v":0},5.0399999999999991,null,0.32000000000000028,{"$f":"$E$214^2+AM226^2","v":9.1023999999999994},16.102399999999999,52.102399999999996,{"$f":"IF(AM226=0,0,$E$210/(PI())*(ATAN(($E$215*$G$213)/(AM226*SQRT(AP226)))-$E$215*$G$213*AM226/(AO226*SQRT(AP226))))","v":{"$error":"#VALUE!"}},null,{"$f":"+AM226","v":0.32000000000000028},{"$f":"$E$215^2+AS226^2","v":36.102400000000003},{"$f":"$E$214^2+AS226^2","v":9.1023999999999994},{"$f":"$G$212^2+AS226^2","v":45.10240000000001},{"$f":"IF(AS226=0,0,($E$210/(PI()))*(ATAN(($E$215*$E$214)/(AS226*SQRT(AV226)))-$E$215*$E$214*AS226/(AU226*SQRT(AV226))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["Presjek XV-XV",null,null,0.64000000000000035,null,{"$error":"#VALUE!"},4.3999999999999986,{"$f":"+F227","v":{"$error":"#VALUE!"}},4.3999999999999986,{"$f":"+F227","v":{"$error":"#VALUE!"}},4.3999999999999986,{"$f":"+J227","v":{"$error":"#VALUE!"}},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$f":"+N227","v":{"$error":"#VALUE!"}},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$f":"+R227","v":{"$error":"#VALUE!"}},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$f":"+V227","v":{"$error":"#VALUE!"}},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,0,{"$f":"+AC226","v":4.7199999999999989},{"$f":"+AB227","v":0},{"$f":"+G227","v":4.3999999999999986},0,4.7199999999999989,0,4.3999999999999986,0,4.3999999999999986,null,0.64000000000000035,{"$f":"$E$214^2+AM227^2","v":9.4096000000000011},16.409600000000001,52.40959999999999,{"$f":"IF(AM227=0,0,$E$210/(PI())*(ATAN(($E$215*$G$213)/(AM227*SQRT(AP227)))-$E$215*$G$213*AM227/(AO227*SQRT(AP227))))","v":{"$error":"#VALUE!"}},null,0.64000000000000035,{"$f":"$E$215^2+AS227^2","v":36.409599999999998},{"$f":"$E$214^2+AS227^2","v":9.4096000000000011},{"$f":"$G$212^2+AS227^2","v":45.409600000000005},{"$f":"IF(AS227=0,0,($E$210/(PI()))*(ATAN(($E$215*$E$214)/(AS227*SQRT(AV227)))-$E$215*$E$214*AS227/(AU227*SQRT(AV227))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["Presjek XIV-XIV",null,null,0.96000000000000041,null,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$f":"+R228","v":{"$error":"#VALUE!"}},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},{"$f":"+U228","v":4.0799999999999983},0,{"$f":"+AA227","v":4.3999999999999986},{"$f":"+Z228","v":0},0,{"$f":"+AB228","v":0},4.0799999999999983,0,0,0,4.0799999999999983,0,4.0799999999999983,null,0.96000000000000041,9.9216000000000015,16.921600000000002,52.921599999999991,{"$error":"#VALUE!"},null,0.96000000000000041,36.921599999999998,9.9216000000000015,45.921600000000005,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XIII-XIII",null,null,1.2800000000000005,null,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,{"$f":"+R229","v":{"$error":"#VALUE!"}},3.7599999999999985,{"$error":"#VALUE!"},3.7599999999999985,0,{"$f":"+Y228","v":4.0799999999999983},0,0,0,0,0,3.7599999999999985,0,0,0,3.7599999999999985,0,3.7599999999999985,null,1.2800000000000005,10.638400000000001,17.638400000000001,53.638399999999997,{"$error":"#VALUE!"},null,1.2800000000000005,37.638400000000004,10.638400000000001,46.638400000000011,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek  XII-XII",null,null,1.6000000000000005,null,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$f":"+R230","v":{"$error":"#VALUE!"}},3.4399999999999986,0,{"$f":"+W229","v":3.7599999999999985},0,{"$f":"+U230","v":3.4399999999999986},0,0,0,0,0,3.4399999999999986,0,0,0,3.4399999999999986,0,3.4399999999999986,null,1.6000000000000005,11.560000000000002,18.560000000000002,54.559999999999995,{"$error":"#VALUE!"},null,1.6000000000000005,38.56,11.560000000000002,47.560000000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XI-XI",null,null,1.9200000000000006,null,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,0,{"$f":"+U230","v":3.4399999999999986},0,{"$f":"+S390","v":3.44},0,3.4399999999999986,0,0,0,0,0,3.1199999999999988,0,0,0,3.1199999999999988,0,3.1199999999999988,null,1.9200000000000006,12.686400000000003,19.686400000000003,55.686399999999992,{"$error":"#VALUE!"},null,1.9200000000000006,39.686399999999999,12.686400000000003,48.686400000000006,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek X-X",null,null,2.2400000000000007,null,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,0,{"$f":"+S231","v":3.1199999999999988},0,{"$f":"+U231","v":3.4399999999999986},0,{"$f":"+S391","v":3.14},0,3.4399999999999986,0,0,0,0,0,2.7999999999999989,0,0,0,2.7999999999999989,0,2.7999999999999989,null,2.2400000000000007,14.017600000000002,21.017600000000002,57.017599999999995,{"$error":"#VALUE!"},null,2.2400000000000007,41.017600000000002,14.017600000000002,50.017600000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek IX-IX",null,null,2.5600000000000005,null,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,0,{"$f":"+Q232","v":2.7999999999999989},0,{"$f":"+O392","v":2.8},0,3.4399999999999986,0,{"$f":"+S392","v":3.14},0,3.4399999999999986,0,0,0,0,0,2.4799999999999991,0,0,0,2.4799999999999991,0,2.4799999999999991,null,2.5600000000000005,15.553600000000003,22.553600000000003,58.553599999999996,{"$error":"#VALUE!"},null,2.5600000000000005,42.553600000000003,15.553600000000003,51.55360000000001,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VIII-VIII",null,null,2.8800000000000003,null,{"$error":"#VALUE!"},2.1599999999999993,{"$error":"#VALUE!"},2.1599999999999993,{"$error":"#VALUE!"},2.1599999999999993,{"$error":"#VALUE!"},2.1599999999999993,0,{"$f":"+O233","v":2.4799999999999991},0,0,0,{"$f":"+O393","v":2.48},0,3.4399999999999986,0,{"$f":"+W233","v":3.14},0,3.4399999999999986,0,0,0,0,0,2.1599999999999993,0,0,0,2.1599999999999993,0,2.1599999999999993,null,2.8800000000000003,17.294400000000003,24.294400000000003,60.294399999999996,{"$error":"#VALUE!"},null,2.8800000000000003,44.294400000000003,17.294400000000003,53.29440000000001,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VII-VII",null,null,3.2,null,{"$error":"#VALUE!"},1.8399999999999992,{"$error":"#VALUE!"},1.8399999999999992,{"$error":"#VALUE!"},1.8399999999999992,0,{"$f":"+M234","v":2.1599999999999993},0,{"$f":"+K394","v":2.16},0,0,0,{"$f":"+S234","v":2.48},0,3.4399999999999986,0,{"$f":"+S394","v":1.6},0,3.4399999999999986,0,0,0,0,{"$f":"+Z235","v":0},1.8399999999999992,0,0,0,1.8399999999999992,0,1.8399999999999992,null,3.2,19.240000000000002,26.240000000000002,62.239999999999995,{"$error":"#VALUE!"},null,3.2,46.24,19.240000000000002,55.240000000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VI-VI",null,null,3.52,null,{"$error":"#VALUE!"},1.5199999999999991,{"$error":"#VALUE!"},1.5199999999999991,0,{"$f":"+K235","v":1.8399999999999992},0,0,0,{"$f":"+O235","v":2.16},0,0,0,{"$f":"+O395","v":2.16},0,3.4399999999999986,0,{"$f":"+S395","v":1.9200000000000002},0,3.4399999999999986,0,0,0,0,0,1.5199999999999991,0,0,0,1.5199999999999991,0,1.5199999999999991,null,3.52,21.3904,28.3904,64.3904,{"$error":"#VALUE!"},null,3.52,48.3904,21.3904,57.390400000000007,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek III -III",null,null,3.84,null,{"$error":"#VALUE!"},1.1999999999999991,0,1.5199999999999991,0,0,0,0,0,{"$f":"+K237","v":0},0,0,0,{"$f":"+O237","v":0},0,3.4399999999999986,0,{"$f":"+O237","v":0},0,3.4399999999999986,0,0,0,0,0,0,0,0,0,0,0,0,null,3.84,23.7456,30.7456,66.745599999999996,{"$error":"#VALUE!"},null,3.84,50.745599999999996,23.7456,59.74560000000001,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["IV-IV=Mmin",null,null,4.16,null,0,{"$f":"+G237","v":1.1999999999999991},0,{"$f":"+G238","v":1.1999999999999991},0,{"$f":"+I238","v":1.1999999999999991},{"$f":"+AF197","v":0},{"$f":"+I238","v":1.1999999999999991},{"$f":"+J397","v":0},{"$f":"+K238","v":1.1999999999999991},0,{"$f":"+O238","v":1.1999999999999991},0,{"$f":"+Q238","v":1.1999999999999991},0,{"$f":"+Q238","v":1.1999999999999991},{"$f":"+R397","v":0},{"$f":"+O238","v":1.1999999999999991},0,{"$f":"+W238","v":1.1999999999999991},0,{"$f":"+Y238","v":1.1999999999999991},0,{"$f":"+Y238","v":1.1999999999999991},{"$f":"+Z397","v":0},1.1999999999999991,0,{"$f":"+AE238","v":1.1999999999999991},0,{"$f":"+AG238","v":1.1999999999999991},0,{"$f":"+AG238","v":1.1999999999999991}]
["V-V = Mmax",null,null,null,null,0,{"$f":"+G199","v":6},0,{"$f":"+G239","v":6},0,{"$f":"+I239","v":6},0,{"$f":"+K239","v":6},{"$f":"+J398","v":0},{"$f":"+K239","v":6},0,{"$f":"+O239","v":6},0,{"$f":"+Q239","v":6},0,{"$f":"+S239","v":6},{"$f":"+R398","v":0},{"$f":"+S239","v":6},0,{"$f":"+W239","v":6},0,{"$f":"+Y239","v":6},0,{"$f":"+AA239","v":6},{"$f":"+Z398","v":0},{"$f":"+AA239","v":6},0,{"$f":"+AE239","v":6},0,{"$f":"+AG239","v":6},0,{"$f":"+AI239","v":6}]
[null,null,null,"Ukupni pritisak",null,"SQhi=",{"$f":"+G243","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I243","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K243","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+M243","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+O243","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Q243","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+S243","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+U243","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+W243","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Y243","v":{"$error":"#VALUE!"}},{"$f":"+V240","v":"SQhi="},{"$f":"+AA243","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AC243","v":{"$error":"#VALUE!"}},{"$f":"+Z240","v":"SQhi="},{"$f":"+AE243","v":0},"SQhi=",{"$f":"+AG243","v":0},"SQhi=",{"$f":"+AI243","v":0},{"$f":"+AD240","v":"SQhi="},{"$f":"+AK243","v":0}]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G245","v":{"$error":"#VALUE!"}}," y=",{"$f":"+I245","v":{"$error":"#VALUE!"}}," y=",{"$f":"+K245","v":{"$error":"#VALUE!"}}," y=",{"$f":"+M245","v":{"$error":"#VALUE!"}}," y=",{"$f":"+O245","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Q245","v":{"$error":"#VALUE!"}}," y=",{"$f":"+S245","v":{"$error":"#VALUE!"}}," y=",{"$f":"+U245","v":{"$error":"#VALUE!"}}," y=",{"$f":"+W245","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Y245","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AA245","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AC245","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AE245","v":0}," y=",{"$f":"+AG245","v":0}," y=",{"$f":"+AI245","v":0}," y=",{"$f":"+AK245","v":0}]
[null,null,null,"krak za presjek III -III",null,"z=",{"$f":"+G241-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I241-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K241-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M241-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+O241-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Q241-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+S241-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+U241-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}},"z=",{"$f":"+W241-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Y241-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AA241-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AC241-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AE241-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AG241-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AI241-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AK241-'Analiza i dimenzioniranje'!$E$52","v":-1.2}]
[null,null,null,null,null,"F=",{"$f":"-0.5*(+\n (F222*G223-F223*G222)+\n(F223*G224-F224*G223)+\n(F224*G225-F225*G224)+\n(F225*G226-F226*G225)+\n(F226*G227-F227*G226)+\n(F227*G228-F228*G227)+\n(F228*G229-F229*G228)+\n(F229*G230-F230*G229)+\n(F230*G231-F231*G230)+\n(F231*G232-F232*G231)+\n(F232*G233-F233*G232)+\n(F233*G234-F234*G233)+\n(F234*G235-F235*G234)+\n(F235*G236-F236*G235)+\n(F236*G237-F237*G236)+\n(F237*G238-F238*G237)+\n(F238*G239-F239*G238))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (H222*I223-H223*I222)+\n(H223*I224-H224*I223)+\n(H224*I225-H225*I224)+\n(H225*I226-H226*I225)+\n(H226*I227-H227*I226)+\n(H227*I228-H228*I227)+\n(H228*I229-H229*I228)+\n(H229*I230-H230*I229)+\n(H230*I231-H231*I230)+\n(H231*I232-H232*I231)+\n(H232*I233-H233*I232)+\n(H233*I234-H234*I233)+\n(H234*I235-H235*I234)+\n(H235*I236-H236*I235)+\n(H236*I237-H237*I236)+\n(H237*I238-H238*I237)+\n(H238*I239-H239*I238))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (J222*K223-J223*K222)+\n(J223*K224-J224*K223)+\n(J224*K225-J225*K224)+\n(J225*K226-J226*K225)+\n(J226*K227-J227*K226)+\n(J227*K228-J228*K227)+\n(J228*K229-J229*K228)+\n(J229*K230-J230*K229)+\n(J230*K231-J231*K230)+\n(J231*K232-J232*K231)+\n(J232*K233-J233*K232)+\n(J233*K234-J234*K233)+\n(J234*K235-J235*K234)+\n(J235*K236-J236*K235)+\n(J236*K237-J237*K236)+\n(J237*K238-J238*K237)+\n(J238*K239-J239*K238))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (L222*M223-L223*M222)+\n(L223*M224-L224*M223)+\n(L224*M225-L225*M224)+\n(L225*M226-L226*M225)+\n(L226*M227-L227*M226)+\n(L227*M228-L228*M227)+\n(L228*M229-L229*M228)+\n(L229*M230-L230*M229)+\n(L230*M231-L231*M230)+\n(L231*M232-L232*M231)+\n(L232*M233-L233*M232)+\n(L233*M234-L234*M233)+\n(L234*M235-L235*M234)+\n(L235*M236-L236*M235)+\n(L236*M237-L237*M236)+\n(L237*M238-L238*M237)+\n(L238*M239-L239*M238))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (N222*O223-N223*O222)+\n(N223*O224-N224*O223)+\n(N224*O225-N225*O224)+\n(N225*O226-N226*O225)+\n(N226*O227-N227*O226)+\n(N227*O228-N228*O227)+\n(N228*O229-N229*O228)+\n(N229*O230-N230*O229)+\n(N230*O231-N231*O230)+\n(N231*O232-N232*O231)+\n(N232*O233-N233*O232)+\n(N233*O234-N234*O233)+\n(N234*O235-N235*O234)+\n(N235*O236-N236*O235)+\n(N236*O237-N237*O236)+\n(N237*O238-N238*O237)+\n(N238*O239-N239*O238))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (P222*Q223-P223*Q222)+\n(P223*Q224-P224*Q223)+\n(P224*Q225-P225*Q224)+\n(P225*Q226-P226*Q225)+\n(P226*Q227-P227*Q226)+\n(P227*Q228-P228*Q227)+\n(P228*Q229-P229*Q228)+\n(P229*Q230-P230*Q229)+\n(P230*Q231-P231*Q230)+\n(P231*Q232-P232*Q231)+\n(P232*Q233-P233*Q232)+\n(P233*Q234-P234*Q233)+\n(P234*Q235-P235*Q234)+\n(P235*Q236-P236*Q235)+\n(P236*Q237-P237*Q236)+\n(P237*Q238-P238*Q237)+\n(P238*Q239-P239*Q238))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (R222*S223-R223*S222)+\n(R223*S224-R224*S223)+\n(R224*S225-R225*S224)+\n(R225*S226-R226*S225)+\n(R226*S227-R227*S226)+\n(R227*S228-R228*S227)+\n(R228*S229-R229*S228)+\n(R229*S230-R230*S229)+\n(R230*S231-R231*S230)+\n(R231*S232-R232*S231)+\n(R232*S233-R233*S232)+\n(R233*S234-R234*S233)+\n(R234*S235-R235*S234)+\n(R235*S236-R236*S235)+\n(R236*S237-R237*S236)+\n(R237*S238-R238*S237)+\n(R238*S239-R239*S238))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (T222*U223-T223*U222)+\n(T223*U224-T224*U223)+\n(T224*U225-T225*U224)+\n(T225*U226-T226*U225)+\n(T226*U227-T227*U226)+\n(T227*U228-T228*U227)+\n(T228*U229-T229*U228)+\n(T229*U230-T230*U229)+\n(T230*U231-T231*U230)+\n(T231*U232-T232*U231)+\n(T232*U233-T233*U232)+\n(T233*U234-T234*U233)+\n(T234*U235-T235*U234)+\n(T235*U236-T236*U235)+\n(T236*U237-T237*U236)+\n(T237*U238-T238*U237)+\n(T238*U239-T239*U238))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (V222*W223-V223*W222)+\n(V223*W224-V224*W223)+\n(V224*W225-V225*W224)+\n(V225*W226-V226*W225)+\n(V226*W227-V227*W226)+\n(V227*W228-V228*W227)+\n(V228*W229-V229*W228)+\n(V229*W230-V230*W229)+\n(V230*W231-V231*W230)+\n(V231*W232-V232*W231)+\n(V232*W233-V233*W232)+\n(V233*W234-V234*W233)+\n(V234*W235-V235*W234)+\n(V235*W236-V236*W235)+\n(V236*W237-V237*W236)+\n(V237*W238-V238*W237)+\n(V238*W239-V239*W238))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (X222*Y223-X223*Y222)+\n(X223*Y224-X224*Y223)+\n(X224*Y225-X225*Y224)+\n(X225*Y226-X226*Y225)+\n(X226*Y227-X227*Y226)+\n(X227*Y228-X228*Y227)+\n(X228*Y229-X229*Y228)+\n(X229*Y230-X230*Y229)+\n(X230*Y231-X231*Y230)+\n(X231*Y232-X232*Y231)+\n(X232*Y233-X233*Y232)+\n(X233*Y234-X234*Y233)+\n(X234*Y235-X235*Y234)+\n(X235*Y236-X236*Y235)+\n(X236*Y237-X237*Y236)+\n(X237*Y238-X238*Y237)+\n(X238*Y239-X239*Y238))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (Z222*AA223-Z223*AA222)+\n(Z223*AA224-Z224*AA223)+\n(Z224*AA225-Z225*AA224)+\n(Z225*AA226-Z226*AA225)+\n(Z226*AA227-Z227*AA226)+\n(Z227*AA228-Z228*AA227)+\n(Z228*AA229-Z229*AA228)+\n(Z229*AA230-Z230*AA229)+\n(Z230*AA231-Z231*AA230)+\n(Z231*AA232-Z232*AA231)+\n(Z232*AA233-Z233*AA232)+\n(Z233*AA234-Z234*AA233)+\n(Z234*AA235-Z235*AA234)+\n(Z235*AA236-Z236*AA235)+\n(Z236*AA237-Z237*AA236)+\n(Z237*AA238-Z238*AA237)+\n(Z238*AA239-Z239*AA238))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (AB222*AC223-AB223*AC222)+\n(AB223*AC224-AB224*AC223)+\n(AB224*AC225-AB225*AC224)+\n(AB225*AC226-AB226*AC225)+\n(AB226*AC227-AB227*AC226)+\n(AB227*AC228-AB228*AC227)+\n(AB228*AC229-AB229*AC228)+\n(AB229*AC230-AB230*AC229)+\n(AB230*AC231-AB231*AC230)+\n(AB231*AC232-AB232*AC231)+\n(AB232*AC233-AB233*AC232)+\n(AB233*AC234-AB234*AC233)+\n(AB234*AC235-AB235*AC234)+\n(AB235*AC236-AB236*AC235)+\n(AB236*AC237-AB237*AC236)+\n(AB237*AC238-AB238*AC237)+\n(AB238*AC239-AB239*AC238))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (AD222*AE223-AD223*AE222)+\n(AD223*AE224-AD224*AE223)+\n(AD224*AE225-AD225*AE224)+\n(AD225*AE226-AD226*AE225)+\n(AD226*AE227-AD227*AE226)+\n(AD227*AE228-AD228*AE227)+\n(AD228*AE229-AD229*AE228)+\n(AD229*AE230-AD230*AE229)+\n(AD230*AE231-AD231*AE230)+\n(AD231*AE232-AD232*AE231)+\n(AD232*AE233-AD233*AE232)+\n(AD233*AE234-AD234*AE233)+\n(AD234*AE235-AD235*AE234)+\n(AD235*AE236-AD236*AE235)+\n(AD236*AE237-AD237*AE236)+\n(AD237*AE238-AD238*AE237)+\n(AD238*AE239-AD239*AE238))","v":0},"F=",{"$f":"-0.5*(+\n (AF222*AG223-AF223*AG222)+\n(AF223*AG224-AF224*AG223)+\n(AF224*AG225-AF225*AG224)+\n(AF225*AG226-AF226*AG225)+\n(AF226*AG227-AF227*AG226)+\n(AF227*AG228-AF228*AG227)+\n(AF228*AG229-AF229*AG228)+\n(AF229*AG230-AF230*AG229)+\n(AF230*AG231-AF231*AG230)+\n(AF231*AG232-AF232*AG231)+\n(AF232*AG233-AF233*AG232)+\n(AF233*AG234-AF234*AG233)+\n(AF234*AG235-AF235*AG234)+\n(AF235*AG236-AF236*AG235)+\n(AF236*AG237-AF237*AG236)+\n(AF237*AG238-AF238*AG237)+\n(AF238*AG239-AF239*AG238))","v":0},"F=",{"$f":"-0.5*(+\n (AH222*AI223-AH223*AI222)+\n(AH223*AI224-AH224*AI223)+\n(AH224*AI225-AH225*AI224)+\n(AH225*AI226-AH226*AI225)+\n(AH226*AI227-AH227*AI226)+\n(AH227*AI228-AH228*AI227)+\n(AH228*AI229-AH229*AI228)+\n(AH229*AI230-AH230*AI229)+\n(AH230*AI231-AH231*AI230)+\n(AH231*AI232-AH232*AI231)+\n(AH232*AI233-AH233*AI232)+\n(AH233*AI234-AH234*AI233)+\n(AH234*AI235-AH235*AI234)+\n(AH235*AI236-AH236*AI235)+\n(AH236*AI237-AH237*AI236)+\n(AH237*AI238-AH238*AI237)+\n(AH238*AI239-AH239*AI238))","v":0},"F=",{"$f":"-0.5*(\n (AJ222*AK223-AJ223*AK222)+\n(AJ223*AK224-AJ224*AK223)+\n(AJ224*AK225-AJ225*AK224)+\n(AJ225*AK226-AJ226*AK225)+\n(AJ226*AK227-AJ227*AK226)+\n(AJ227*AK228-AJ228*AK227)+\n(AJ228*AK229-AJ229*AK228)+\n(AJ229*AK230-AJ230*AK229)+\n(AJ230*AK231-AJ231*AK230)+\n(AJ231*AK232-AJ232*AK231)+\n(AJ232*AK233-AJ233*AK232)+\n(AJ233*AK234-AJ234*AK233)+\n(AJ234*AK235-AJ235*AK234)+\n(AJ235*AK236-AJ236*AK235)+\n(AJ236*AK237-AJ237*AK236)+\n(AJ237*AK238-AJ238*AK237)+\n(AJ238*AK239-AJ239*AK238))","v":0}]
[null,null,null,null,null,"x=",5,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",{"$f":"+W244","v":0},"x=",0,"x=",0,"x=",0,"x=",0,"x=",0]
[null,null,null,null,null,"y=",{"$f":"+IF(G243=0,0,-((F220*G221-F221*G220)*(G220+G221)+(F221*G222-F222*G221)*(G221+G222)+\n(F222*G223-F223*G222)*(G222+G223)+\n(F223*G224-F224*G223)*(G223+G224)+\n(F224*G225-F225*G224)*(G224+G225)+\n(F225*G226-F226*G225)*(G225+G226)+\n(F226*G227-F227*G226)*(G226+G227)+\n(F227*G228-F228*G227)*(G227+G228)+\n(F228*G229-F229*G228)*(G228+G229)+\n(F229*G230-F230*G229)*(G229+G230)+\n(F230*G231-F231*G230)*(G230+G231)+\n(F231*G232-F232*G231)*(G231+G232)+\n(F232*G233-F233*G232)*(G232+G233)+\n(F233*G234-F234*G233)*(G233+G234)+\n(F234*G235-F235*G234)*(G234+G235)+\n(F235*G236-F236*G235)*(G235+G236)+\n(F236*G237-F237*G236)*(G236+G237)+\n(F237*G238-F238*G237)*(G237+G238)+\n(F238*G239-F239*G238)*(G238+G239))/6/G243)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(I243=0,0,-((H220*I221-H221*I220)*(I220+I221)+(H221*I222-H222*I221)*(I221+I222)+\n(H222*I223-H223*I222)*(I222+I223)+\n(H223*I224-H224*I223)*(I223+I224)+\n(H224*I225-H225*I224)*(I224+I225)+\n(H225*I226-H226*I225)*(I225+I226)+\n(H226*I227-H227*I226)*(I226+I227)+\n(H227*I228-H228*I227)*(I227+I228)+\n(H228*I229-H229*I228)*(I228+I229)+\n(H229*I230-H230*I229)*(I229+I230)+\n(H230*I231-H231*I230)*(I230+I231)+\n(H231*I232-H232*I231)*(I231+I232)+\n(H232*I233-H233*I232)*(I232+I233)+\n(H233*I234-H234*I233)*(I233+I234)+\n(H234*I235-H235*I234)*(I234+I235)+\n(H235*I236-H236*I235)*(I235+I236)+\n(H236*I237-H237*I236)*(I236+I237)+\n(H237*I238-H238*I237)*(I237+I238)+\n(H238*I239-H239*I238)*(I238+I239))/6/I243)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(K243=0,0,-((J220*K221-J221*K220)*(K220+K221)+(J221*K222-J222*K221)*(K221+K222)+\n(J222*K223-J223*K222)*(K222+K223)+\n(J223*K224-J224*K223)*(K223+K224)+\n(J224*K225-J225*K224)*(K224+K225)+\n(J225*K226-J226*K225)*(K225+K226)+\n(J226*K227-J227*K226)*(K226+K227)+\n(J227*K228-J228*K227)*(K227+K228)+\n(J228*K229-J229*K228)*(K228+K229)+\n(J229*K230-J230*K229)*(K229+K230)+\n(J230*K231-J231*K230)*(K230+K231)+\n(J231*K232-J232*K231)*(K231+K232)+\n(J232*K233-J233*K232)*(K232+K233)+\n(J233*K234-J234*K233)*(K233+K234)+\n(J234*K235-J235*K234)*(K234+K235)+\n(J235*K236-J236*K235)*(K235+K236)+\n(J236*K237-J237*K236)*(K236+K237)+\n(J237*K238-J238*K237)*(K237+K238)+\n(J238*K239-J239*K238)*(K238+K239))/6/K243)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(M243=0,0,-((L220*M221-L221*M220)*(M220+M221)+(L221*M222-L222*M221)*(M221+M222)+\n(L222*M223-L223*M222)*(M222+M223)+\n(L223*M224-L224*M223)*(M223+M224)+\n(L224*M225-L225*M224)*(M224+M225)+\n(L225*M226-L226*M225)*(M225+M226)+\n(L226*M227-L227*M226)*(M226+M227)+\n(L227*M228-L228*M227)*(M227+M228)+\n(L228*M229-L229*M228)*(M228+M229)+\n(L229*M230-L230*M229)*(M229+M230)+\n(L230*M231-L231*M230)*(M230+M231)+\n(L231*M232-L232*M231)*(M231+M232)+\n(L232*M233-L233*M232)*(M232+M233)+\n(L233*M234-L234*M233)*(M233+M234)+\n(L234*M235-L235*M234)*(M234+M235)+\n(L235*M236-L236*M235)*(M235+M236)+\n(L236*M237-L237*M236)*(M236+M237)+\n(L237*M238-L238*M237)*(M237+M238)+\n(L238*M239-L239*M238)*(M238+M239))/6/M243)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(O243=0,0,-((N220*O221-N221*O220)*(O220+O221)+(N221*O222-N222*O221)*(O221+O222)+\n(N222*O223-N223*O222)*(O222+O223)+\n(N223*O224-N224*O223)*(O223+O224)+\n(N224*O225-N225*O224)*(O224+O225)+\n(N225*O226-N226*O225)*(O225+O226)+\n(N226*O227-N227*O226)*(O226+O227)+\n(N227*O228-N228*O227)*(O227+O228)+\n(N228*O229-N229*O228)*(O228+O229)+\n(N229*O230-N230*O229)*(O229+O230)+\n(N230*O231-N231*O230)*(O230+O231)+\n(N231*O232-N232*O231)*(O231+O232)+\n(N232*O233-N233*O232)*(O232+O233)+\n(N233*O234-N234*O233)*(O233+O234)+\n(N234*O235-N235*O234)*(O234+O235)+\n(N235*O236-N236*O235)*(O235+O236)+\n(N236*O237-N237*O236)*(O236+O237)+\n(N237*O238-N238*O237)*(O237+O238)+\n(N238*O239-N239*O238)*(O238+O239))/6/O243)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Q243=0,0,-((P220*Q221-P221*Q220)*(Q220+Q221)+(P221*Q222-P222*Q221)*(Q221+Q222)+\n(P222*Q223-P223*Q222)*(Q222+Q223)+\n(P223*Q224-P224*Q223)*(Q223+Q224)+\n(P224*Q225-P225*Q224)*(Q224+Q225)+\n(P225*Q226-P226*Q225)*(Q225+Q226)+\n(P226*Q227-P227*Q226)*(Q226+Q227)+\n(P227*Q228-P228*Q227)*(Q227+Q228)+\n(P228*Q229-P229*Q228)*(Q228+Q229)+\n(P229*Q230-P230*Q229)*(Q229+Q230)+\n(P230*Q231-P231*Q230)*(Q230+Q231)+\n(P231*Q232-P232*Q231)*(Q231+Q232)+\n(P232*Q233-P233*Q232)*(Q232+Q233)+\n(P233*Q234-P234*Q233)*(Q233+Q234)+\n(P234*Q235-P235*Q234)*(Q234+Q235)+\n(P235*Q236-P236*Q235)*(Q235+Q236)+\n(P236*Q237-P237*Q236)*(Q236+Q237)+\n(P237*Q238-P238*Q237)*(Q237+Q238)+\n(P238*Q239-P239*Q238)*(Q238+Q239))/6/Q243)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(S243=0,0,-((R220*S221-R221*S220)*(S220+S221)+(R221*S222-R222*S221)*(S221+S222)+\n(R222*S223-R223*S222)*(S222+S223)+\n(R223*S224-R224*S223)*(S223+S224)+\n(R224*S225-R225*S224)*(S224+S225)+\n(R225*S226-R226*S225)*(S225+S226)+\n(R226*S227-R227*S226)*(S226+S227)+\n(R227*S228-R228*S227)*(S227+S228)+\n(R228*S229-R229*S228)*(S228+S229)+\n(R229*S230-R230*S229)*(S229+S230)+\n(R230*S231-R231*S230)*(S230+S231)+\n(R231*S232-R232*S231)*(S231+S232)+\n(R232*S233-R233*S232)*(S232+S233)+\n(R233*S234-R234*S233)*(S233+S234)+\n(R234*S235-R235*S234)*(S234+S235)+\n(R235*S236-R236*S235)*(S235+S236)+\n(R236*S237-R237*S236)*(S236+S237)+\n(R237*S238-R238*S237)*(S237+S238)+\n(R238*S239-R239*S238)*(S238+S239))/6/S243)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(U243=0,0,-((T220*U221-T221*U220)*(U220+U221)+(T221*U222-T222*U221)*(U221+U222)+\n(T222*U223-T223*U222)*(U222+U223)+\n(T223*U224-T224*U223)*(U223+U224)+\n(T224*U225-T225*U224)*(U224+U225)+\n(T225*U226-T226*U225)*(U225+U226)+\n(T226*U227-T227*U226)*(U226+U227)+\n(T227*U228-T228*U227)*(U227+U228)+\n(T228*U229-T229*U228)*(U228+U229)+\n(T229*U230-T230*U229)*(U229+U230)+\n(T230*U231-T231*U230)*(U230+U231)+\n(T231*U232-T232*U231)*(U231+U232)+\n(T232*U233-T233*U232)*(U232+U233)+\n(T233*U234-T234*U233)*(U233+U234)+\n(T234*U235-T235*U234)*(U234+U235)+\n(T235*U236-T236*U235)*(U235+U236)+\n(T236*U237-T237*U236)*(U236+U237)+\n(T237*U238-T238*U237)*(U237+U238)+\n(T238*U239-T239*U238)*(U238+U239))/6/U243)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(W243=0,0,-((V220*W221-V221*W220)*(W220+W221)+(V221*W222-V222*W221)*(W221+W222)+\n(V222*W223-V223*W222)*(W222+W223)+\n(V223*W224-V224*W223)*(W223+W224)+\n(V224*W225-V225*W224)*(W224+W225)+\n(V225*W226-V226*W225)*(W225+W226)+\n(V226*W227-V227*W226)*(W226+W227)+\n(V227*W228-V228*W227)*(W227+W228)+\n(V228*W229-V229*W228)*(W228+W229)+\n(V229*W230-V230*W229)*(W229+W230)+\n(V230*W231-V231*W230)*(W230+W231)+\n(V231*W232-V232*W231)*(W231+W232)+\n(V232*W233-V233*W232)*(W232+W233)+\n(V233*W234-V234*W233)*(W233+W234)+\n(V234*W235-V235*W234)*(W234+W235)+\n(V235*W236-V236*W235)*(W235+W236)+\n(V236*W237-V237*W236)*(W236+W237)+\n(V237*W238-V238*W237)*(W237+W238)+\n(V238*W239-V239*W238)*(W238+W239))/6/W243)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Y243=0,0,-((X220*Y221-X221*Y220)*(Y220+Y221)+(X221*Y222-X222*Y221)*(Y221+Y222)+\n(X222*Y223-X223*Y222)*(Y222+Y223)+\n(X223*Y224-X224*Y223)*(Y223+Y224)+\n(X224*Y225-X225*Y224)*(Y224+Y225)+\n(X225*Y226-X226*Y225)*(Y225+Y226)+\n(X226*Y227-X227*Y226)*(Y226+Y227)+\n(X227*Y228-X228*Y227)*(Y227+Y228)+\n(X228*Y229-X229*Y228)*(Y228+Y229)+\n(X229*Y230-X230*Y229)*(Y229+Y230)+\n(X230*Y231-X231*Y230)*(Y230+Y231)+\n(X231*Y232-X232*Y231)*(Y231+Y232)+\n(X232*Y233-X233*Y232)*(Y232+Y233)+\n(X233*Y234-X234*Y233)*(Y233+Y234)+\n(X234*Y235-X235*Y234)*(Y234+Y235)+\n(X235*Y236-X236*Y235)*(Y235+Y236)+\n(X236*Y237-X237*Y236)*(Y236+Y237)+\n(X237*Y238-X238*Y237)*(Y237+Y238)+\n(X238*Y239-X239*Y238)*(Y238+Y239))/6/Y243)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AA243=0,0,-((Z220*AA221-Z221*AA220)*(AA220+AA221)+(Z221*AA222-Z222*AA221)*(AA221+AA222)+\n(Z222*AA223-Z223*AA222)*(AA222+AA223)+\n(Z223*AA224-Z224*AA223)*(AA223+AA224)+\n(Z224*AA225-Z225*AA224)*(AA224+AA225)+\n(Z225*AA226-Z226*AA225)*(AA225+AA226)+\n(Z226*AA227-Z227*AA226)*(AA226+AA227)+\n(Z227*AA228-Z228*AA227)*(AA227+AA228)+\n(Z228*AA229-Z229*AA228)*(AA228+AA229)+\n(Z229*AA230-Z230*AA229)*(AA229+AA230)+\n(Z230*AA231-Z231*AA230)*(AA230+AA231)+\n(Z231*AA232-Z232*AA231)*(AA231+AA232)+\n(Z232*AA233-Z233*AA232)*(AA232+AA233)+\n(Z233*AA234-Z234*AA233)*(AA233+AA234)+\n(Z234*AA235-Z235*AA234)*(AA234+AA235)+\n(Z235*AA236-Z236*AA235)*(AA235+AA236)+\n(Z236*AA237-Z237*AA236)*(AA236+AA237)+\n(Z237*AA238-Z238*AA237)*(AA237+AA238)+\n(Z238*AA239-Z239*AA238)*(AA238+AA239))/6/AA243)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AC243=0,0,-((AB220*AC221-AB221*AC220)*(AC220+AC221)+(AB221*AC222-AB222*AC221)*(AC221+AC222)+\n(AB222*AC223-AB223*AC222)*(AC222+AC223)+\n(AB223*AC224-AB224*AC223)*(AC223+AC224)+\n(AB224*AC225-AB225*AC224)*(AC224+AC225)+\n(AB225*AC226-AB226*AC225)*(AC225+AC226)+\n(AB226*AC227-AB227*AC226)*(AC226+AC227)+\n(AB227*AC228-AB228*AC227)*(AC227+AC228)+\n(AB228*AC229-AB229*AC228)*(AC228+AC229)+\n(AB229*AC230-AB230*AC229)*(AC229+AC230)+\n(AB230*AC231-AB231*AC230)*(AC230+AC231)+\n(AB231*AC232-AB232*AC231)*(AC231+AC232)+\n(AB232*AC233-AB233*AC232)*(AC232+AC233)+\n(AB233*AC234-AB234*AC233)*(AC233+AC234)+\n(AB234*AC235-AB235*AC234)*(AC234+AC235)+\n(AB235*AC236-AB236*AC235)*(AC235+AC236)+\n(AB236*AC237-AB237*AC236)*(AC236+AC237)+\n(AB237*AC238-AB238*AC237)*(AC237+AC238)+\n(AB238*AC239-AB239*AC238)*(AC238+AC239))/6/AC243)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AE243=0,0,-((AD220*AE221-AD221*AE220)*(AE220+AE221)+(AD221*AE222-AD222*AE221)*(AE221+AE222)+\n(AD222*AE223-AD223*AE222)*(AE222+AE223)+\n(AD223*AE224-AD224*AE223)*(AE223+AE224)+\n(AD224*AE225-AD225*AE224)*(AE224+AE225)+\n(AD225*AE226-AD226*AE225)*(AE225+AE226)+\n(AD226*AE227-AD227*AE226)*(AE226+AE227)+\n(AD227*AE228-AD228*AE227)*(AE227+AE228)+\n(AD228*AE229-AD229*AE228)*(AE228+AE229)+\n(AD229*AE230-AD230*AE229)*(AE229+AE230)+\n(AD230*AE231-AD231*AE230)*(AE230+AE231)+\n(AD231*AE232-AD232*AE231)*(AE231+AE232)+\n(AD232*AE233-AD233*AE232)*(AE232+AE233)+\n(AD233*AE234-AD234*AE233)*(AE233+AE234)+\n(AD234*AE235-AD235*AE234)*(AE234+AE235)+\n(AD235*AE236-AD236*AE235)*(AE235+AE236)+\n(AD236*AE237-AD237*AE236)*(AE236+AE237)+\n(AD237*AE238-AD238*AE237)*(AE237+AE238)+\n(AD238*AE239-AD239*AE238)*(AE238+AE239))/6/AE243)","v":0},"y=",{"$f":"+IF(AG243=0,0,-((AF220*AG221-AF221*AG220)*(AG220+AG221)+(AF221*AG222-AF222*AG221)*(AG221+AG222)+\n(AF222*AG223-AF223*AG222)*(AG222+AG223)+\n(AF223*AG224-AF224*AG223)*(AG223+AG224)+\n(AF224*AG225-AF225*AG224)*(AG224+AG225)+\n(AF225*AG226-AF226*AG225)*(AG225+AG226)+\n(AF226*AG227-AF227*AG226)*(AG226+AG227)+\n(AF227*AG228-AF228*AG227)*(AG227+AG228)+\n(AF228*AG229-AF229*AG228)*(AG228+AG229)+\n(AF229*AG230-AF230*AG229)*(AG229+AG230)+\n(AF230*AG231-AF231*AG230)*(AG230+AG231)+\n(AF231*AG232-AF232*AG231)*(AG231+AG232)+\n(AF232*AG233-AF233*AG232)*(AG232+AG233)+\n(AF233*AG234-AF234*AG233)*(AG233+AG234)+\n(AF234*AG235-AF235*AG234)*(AG234+AG235)+\n(AF235*AG236-AF236*AG235)*(AG235+AG236)+\n(AF236*AG237-AF237*AG236)*(AG236+AG237)+\n(AF237*AG238-AF238*AG237)*(AG237+AG238)+\n(AF238*AG239-AF239*AG238)*(AG238+AG239))/6/AG243)","v":0},"y=",{"$f":"+IF(AI243=0,0,-((AH220*AI221-AH221*AI220)*(AI220+AI221)+(AH221*AI222-AH222*AI221)*(AI221+AI222)+\n(AH222*AI223-AH223*AI222)*(AI222+AI223)+\n(AH223*AI224-AH224*AI223)*(AI223+AI224)+\n(AH224*AI225-AH225*AI224)*(AI224+AI225)+\n(AH225*AI226-AH226*AI225)*(AI225+AI226)+\n(AH226*AI227-AH227*AI226)*(AI226+AI227)+\n(AH227*AI228-AH228*AI227)*(AI227+AI228)+\n(AH228*AI229-AH229*AI228)*(AI228+AI229)+\n(AH229*AI230-AH230*AI229)*(AI229+AI230)+\n(AH230*AI231-AH231*AI230)*(AI230+AI231)+\n(AH231*AI232-AH232*AI231)*(AI231+AI232)+\n(AH232*AI233-AH233*AI232)*(AI232+AI233)+\n(AH233*AI234-AH234*AI233)*(AI233+AI234)+\n(AH234*AI235-AH235*AI234)*(AI234+AI235)+\n(AH235*AI236-AH236*AI235)*(AI235+AI236)+\n(AH236*AI237-AH237*AI236)*(AI236+AI237)+\n(AH237*AI238-AH238*AI237)*(AI237+AI238)+\n(AH238*AI239-AH239*AI238)*(AI238+AI239))/6/AI243)","v":0},"y=",{"$f":"+IF(AK243=0,0,-((AJ220*AK221-AJ221*AK220)*(AK220+AK221)+(AJ221*AK222-AJ222*AK221)*(AK221+AK222)+\n(AJ222*AK223-AJ223*AK222)*(AK222+AK223)+\n(AJ223*AK224-AJ224*AK223)*(AK223+AK224)+\n(AJ224*AK225-AJ225*AK224)*(AK224+AK225)+\n(AJ225*AK226-AJ226*AK225)*(AK225+AK226)+\n(AJ226*AK227-AJ227*AK226)*(AK226+AK227)+\n(AJ227*AK228-AJ228*AK227)*(AK227+AK228)+\n(AJ228*AK229-AJ229*AK228)*(AK228+AK229)+\n(AJ229*AK230-AJ230*AK229)*(AK229+AK230)+\n(AJ230*AK231-AJ231*AK230)*(AK230+AK231)+\n(AJ231*AK232-AJ232*AK231)*(AK231+AK232)+\n(AJ232*AK233-AJ233*AK232)*(AK232+AK233)+\n(AJ233*AK234-AJ234*AK233)*(AK233+AK234)+\n(AJ234*AK235-AJ235*AK234)*(AK234+AK235)+\n(AJ235*AK236-AJ236*AK235)*(AK235+AK236)+\n(AJ236*AK237-AJ237*AK236)*(AK236+AK237)+\n(AJ237*AK238-AJ238*AK237)*(AK237+AK238)+\n(AJ238*AK239-AJ239*AK238)*(AK238+AK239))/6/AK243)","v":0}]
[]
[]
[null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID "]
[null,"OPTEREĆENJE TEMELJEM",null,null,null,null,null,null,null," (TERZAGHY)"]
[]
[null,"KONTINUIRANO OPTEREĆENJE",null,"P - D=",{"$f":"IF('Analiza i dimenzioniranje'!$E$28-I251<=0,0,+'Analiza i dimenzioniranje'!$E$28-I251)","v":{"$error":"#VALUE!"}},"kN/m2","raster. iskopom   D=y*Df =",null,{"$f":"+'Analiza i dimenzioniranje'!$D$16*('Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20-D257)","v":{"$error":"#VALUE!"}},"kN/m2"]
[null," visina zida i temelja",null,"H =",{"$f":"+E211","v":{"$error":"#VALUE!"}},"m",{"$f":"E256","v":6}]
[null,"visina opterećenja iznad vrha zida",null,"h =",{"$f":"+E212","v":-1},"m",{"$f":"SQRT(E256^2+E255^2)","v":6.7082039324993694}]
[null,"širina temelja",null,"b =",{"$f":"+E213","v":1},"m   ",{"$f":"E255+E254","v":4}]
[null,"udaljenost temelja od zida",null,"D =",{"$f":"+E214","v":3},"m    "]
[null,"1/2 dužine temelja",null,"L/2=a=",{"$f":"+E215","v":6},"m",{"$f":"SQRT(G252^2+G254^2)","v":7.2111025509279782}]
["DNO TEMELJA NA VISINI","PRESJEK NA Visini ",null,{"$f":"+ROUND('Analiza i dimenzioniranje'!U63,2)","v":4.72},null,"Presjek III -III",null,"Presjek VI",null,"Presjek VII-VII",null,"Presjek VIII-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"Presjek XIV-XIV",null,"Presjek XV-XV",null,"PresjekXVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX"]
[null,null,null,null,null,"(sb2-sb1)*2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja"]
[null,null,null,null,null,null,{"$f":"+D257","v":4.72},null,{"$f":"+G259","v":4.72},null,{"$f":"+G259","v":4.72},null,{"$f":"+G259","v":4.72},null,{"$f":"+I259","v":4.72},null,{"$f":"+K259","v":4.72},null,{"$f":"+M259","v":4.72},null,{"$f":"+O259","v":4.72},null,{"$f":"+Q259","v":4.72},null,{"$f":"+S259","v":4.72},null,{"$f":"+U259","v":4.72},null,{"$f":"+W259","v":4.72},null,{"$f":"+Y259","v":4.72},null,{"$f":"+AA259","v":4.72},null,{"$f":"+AC259","v":4.72},{"$f":"+AD259","v":0},{"$f":"+AE259","v":4.72},null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
[null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Presjek X-X",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Presjek X-X",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Presjek XIX-XIX",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Presjek XVIII-XVIII",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Presjek XVII-XVII",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Presjek XVI-XVI",null,null,{"$f":"+D225","v":0},null,0,{"$f":"+G226","v":4.7199999999999989},0,{"$f":"+I226","v":4.7199999999999989},0,{"$f":"+G266","v":4.7199999999999989},0,{"$f":"+I266","v":4.7199999999999989},0,{"$f":"+K266","v":4.7199999999999989},0,{"$f":"+M266","v":4.7199999999999989},{"$f":"+N266","v":0},{"$f":"+O266","v":4.7199999999999989},0,{"$f":"+Q266","v":4.7199999999999989},{"$f":"+R266","v":0},{"$f":"+S266","v":4.7199999999999989},0,{"$f":"+U266","v":4.7199999999999989},{"$f":"+V266","v":0},{"$f":"+W266","v":4.7199999999999989},0,{"$f":"+Y266","v":4.7199999999999989},{"$f":"+Z266","v":0},{"$f":"+G266","v":4.7199999999999989},0,{"$f":"+AC266","v":4.7199999999999989},0,{"$f":"+AE266","v":4.7199999999999989},0,{"$f":"+AE266","v":4.7199999999999989},null,{"$f":"+B266","v":0},0,0,0,0,null,{"$f":"+AM266","v":0},{"$f":"$E$256^2+AS266^2","v":36},{"$f":"$E$255^2+AS266^2","v":9},{"$f":"$G$253^2+AS266^2","v":45.000000000000007},{"$f":"IF(AS266=0,0,($E$251/(PI()))*(ATAN(($E$215*$E$214)/(AS266*SQRT(AV266)))-$E$215*$E$214*AS266/(AU266*SQRT(AV266))))","v":0},{"$f":"+(AQ266-AW266)*2","v":0}]
["Presjek XV-XV",null,null,0.32000000000000028,null,{"$f":"+AX267","v":{"$error":"#VALUE!"}},4.3999999999999986,{"$f":"+F267","v":{"$error":"#VALUE!"}},4.3999999999999986,{"$f":"+H267","v":{"$error":"#VALUE!"}},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},4.3999999999999986,{"$error":"#VALUE!"},{"$f":"+W267","v":4.3999999999999986},{"$f":"+V267","v":{"$error":"#VALUE!"}},{"$f":"+W267","v":4.3999999999999986},0,{"$f":"+AA267","v":4.3999999999999986},0,{"$f":"+G267","v":4.3999999999999986},{"$f":"+AD267","v":0},4.3999999999999986,0,4.3999999999999986,0,4.3999999999999986,null,{"$f":"+D267","v":0.32000000000000028},{"$f":"$E$255^2+AM267^2","v":9.1023999999999994},{"$f":"$G$254^2+AM267^2","v":16.102399999999999},{"$f":"$G$256^2+AM267^2","v":52.102399999999996},{"$f":"IF(AM267=0,0,$E$251/(PI())*(ATAN(($E$256*$G$254)/(AM267*SQRT(AP267)))-$E$256*$G$254*AM267/(AO267*SQRT(AP267))))","v":{"$error":"#VALUE!"}},null,{"$f":"+AM267","v":0.32000000000000028},{"$f":"$E$256^2+AS267^2","v":36.102400000000003},{"$f":"$E$255^2+AS267^2","v":9.1023999999999994},{"$f":"$G$253^2+AS267^2","v":45.10240000000001},{"$f":"IF(AS267=0,0,($E$251/(PI()))*(ATAN(($E$256*$E$255)/(AS267*SQRT(AV267)))-$E$256*$E$255*AS267/(AU267*SQRT(AV267))))","v":{"$error":"#VALUE!"}},{"$f":"+(AQ267-AW267)*2","v":{"$error":"#VALUE!"}}]
["Presjek XIV-XIV",null,null,0.64000000000000035,null,{"$error":"#VALUE!"},4.0799999999999983,{"$f":"+F268","v":{"$error":"#VALUE!"}},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},4.0799999999999983,{"$error":"#VALUE!"},{"$f":"+W268","v":4.0799999999999983},0,{"$f":"+AA267","v":4.3999999999999986},0,0,0,0,{"$f":"+AD268","v":0},{"$f":"+AE268","v":0},{"$f":"+AF268","v":0},{"$f":"+AG268","v":0},0,0,null,0.64000000000000035,{"$f":"$E$255^2+AM268^2","v":9.4096000000000011},{"$f":"$G$254^2+AM268^2","v":16.409600000000001},{"$f":"$G$256^2+AM268^2","v":52.40959999999999},{"$f":"IF(AM268=0,0,$E$251/(PI())*(ATAN(($E$256*$G$254)/(AM268*SQRT(AP268)))-$E$256*$G$254*AM268/(AO268*SQRT(AP268))))","v":{"$error":"#VALUE!"}},null,0.64000000000000035,{"$f":"$E$256^2+AS268^2","v":36.409599999999998},{"$f":"$E$255^2+AS268^2","v":9.4096000000000011},{"$f":"$G$253^2+AS268^2","v":45.409600000000005},{"$f":"IF(AS268=0,0,($E$251/(PI()))*(ATAN(($E$256*$E$255)/(AS268*SQRT(AV268)))-$E$256*$E$255*AS268/(AU268*SQRT(AV268))))","v":{"$error":"#VALUE!"}},{"$f":"+(AQ268-AW268)*2","v":{"$error":"#VALUE!"}}]
["Presjek XIII-XIII",null,null,0.96000000000000041,null,{"$error":"#VALUE!"},3.7599999999999985,{"$f":"+F269","v":{"$error":"#VALUE!"}},3.7599999999999985,{"$f":"+H269","v":{"$error":"#VALUE!"}},{"$f":"+G269","v":3.7599999999999985},{"$f":"+J269","v":{"$error":"#VALUE!"}},{"$f":"+K269","v":3.7599999999999985},{"$f":"+J269","v":{"$error":"#VALUE!"}},{"$f":"+K269","v":3.7599999999999985},{"$f":"+N269","v":{"$error":"#VALUE!"}},{"$f":"+O269","v":3.7599999999999985},{"$f":"+N269","v":{"$error":"#VALUE!"}},3.7599999999999985,{"$f":"+R269","v":{"$error":"#VALUE!"}},{"$f":"+S269","v":3.7599999999999985},{"$f":"+R269","v":{"$error":"#VALUE!"}},{"$f":"+S269","v":3.7599999999999985},0,{"$f":"+Y268","v":4.0799999999999983},{"$f":"+X269","v":0},0,0,0,0,0,{"$f":"+AD269","v":0},{"$f":"+AA269","v":0},{"$f":"+AF269","v":0},{"$f":"+AE269","v":0},{"$f":"+AH269","v":0},0,null,0.96000000000000041,{"$f":"$E$255^2+AM269^2","v":9.9216000000000015},{"$f":"$G$254^2+AM269^2","v":16.921600000000002},{"$f":"$G$256^2+AM269^2","v":52.921599999999991},{"$f":"IF(AM269=0,0,$E$251/(PI())*(ATAN(($E$256*$G$254)/(AM269*SQRT(AP269)))-$E$256*$G$254*AM269/(AO269*SQRT(AP269))))","v":{"$error":"#VALUE!"}},null,0.96000000000000041,{"$f":"$E$256^2+AS269^2","v":36.921599999999998},{"$f":"$E$255^2+AS269^2","v":9.9216000000000015},{"$f":"$G$253^2+AS269^2","v":45.921600000000005},{"$f":"IF(AS269=0,0,($E$251/(PI()))*(ATAN(($E$256*$E$255)/(AS269*SQRT(AV269)))-$E$256*$E$255*AS269/(AU269*SQRT(AV269))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
["Presjek  XII-XII",null,null,1.2800000000000005,null,{"$error":"#VALUE!"},3.4399999999999986,{"$error":"#VALUE!"},3.4399999999999986,{"$f":"+H270","v":{"$error":"#VALUE!"}},{"$f":"+G270","v":3.4399999999999986},{"$f":"+J270","v":{"$error":"#VALUE!"}},{"$f":"+K270","v":3.4399999999999986},{"$f":"+J270","v":{"$error":"#VALUE!"}},{"$f":"+K270","v":3.4399999999999986},{"$f":"+N270","v":{"$error":"#VALUE!"}},{"$f":"+O270","v":3.4399999999999986},{"$error":"#VALUE!"},3.4399999999999986,{"$f":"+R270","v":{"$error":"#VALUE!"}},{"$f":"+S270","v":3.4399999999999986},0,{"$f":"+W269","v":3.7599999999999985},{"$f":"+V270","v":0},0,0,{"$f":"+W270","v":3.7599999999999985},0,0,0,0,0,0,0,0,0,0,null,1.2800000000000005,10.638400000000001,17.638400000000001,53.638399999999997,{"$error":"#VALUE!"},null,1.2800000000000005,37.638400000000004,10.638400000000001,46.638400000000011,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek XI-XI",null,null,1.6000000000000005,null,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,{"$error":"#VALUE!"},{"$f":"+G271","v":3.1199999999999988},{"$f":"+J271","v":{"$error":"#VALUE!"}},3.1199999999999988,{"$f":"+J271","v":{"$error":"#VALUE!"}},3.1199999999999988,{"$f":"+N271","v":{"$error":"#VALUE!"}},3.1199999999999988,{"$error":"#VALUE!"},3.1199999999999988,0,{"$f":"+U270","v":3.4399999999999986},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,1.6000000000000005,11.560000000000002,18.560000000000002,54.559999999999995,{"$error":"#VALUE!"},null,1.6000000000000005,38.56,11.560000000000002,47.560000000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek X-X",null,null,1.9200000000000006,null,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,{"$error":"#VALUE!"},2.7999999999999989,0,{"$f":"+S271","v":3.1199999999999988},0,0,{"$f":"+T272","v":0},0,0,0,0,0,0,{"$f":"+U272","v":0},0,0,0,0,0,0,0,0,null,1.9200000000000006,12.686400000000003,19.686400000000003,55.686399999999992,{"$error":"#VALUE!"},null,1.9200000000000006,39.686399999999999,12.686400000000003,48.686400000000006,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek IX-IX",null,null,2.2400000000000007,null,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,{"$error":"#VALUE!"},2.4799999999999991,0,{"$f":"+Q272","v":2.7999999999999989},0,{"$f":"+S264","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AE273","v":0},null,2.2400000000000007,14.017600000000002,21.017600000000002,57.017599999999995,{"$error":"#VALUE!"},null,2.2400000000000007,41.017600000000002,14.017600000000002,50.017600000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VIII-VIII",null,null,2.5600000000000005,null,{"$error":"#VALUE!"},2.1599999999999993,{"$error":"#VALUE!"},2.1599999999999993,{"$error":"#VALUE!"},2.1599999999999993,{"$error":"#VALUE!"},2.1599999999999993,0,{"$f":"+O273","v":2.4799999999999991},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AE274","v":0},null,2.5600000000000005,15.553600000000003,22.553600000000003,58.553599999999996,{"$error":"#VALUE!"},null,2.5600000000000005,42.553600000000003,15.553600000000003,51.55360000000001,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VII-VII",null,null,2.8800000000000003,null,{"$error":"#VALUE!"},1.8399999999999992,{"$error":"#VALUE!"},1.8399999999999992,{"$error":"#VALUE!"},1.8399999999999992,0,{"$f":"+M274","v":2.1599999999999993},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AE275","v":0},null,2.8800000000000003,17.294400000000003,24.294400000000003,60.294399999999996,{"$error":"#VALUE!"},null,2.8800000000000003,44.294400000000003,17.294400000000003,53.29440000000001,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek VI-VI",null,null,3.2,null,{"$error":"#VALUE!"},1.5199999999999991,{"$error":"#VALUE!"},1.5199999999999991,0,{"$f":"+K275","v":1.8399999999999992},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+Z276","v":0},0,0,{"$f":"+AC276","v":0},0,0,{"$f":"+AF276","v":0},{"$f":"+AE276","v":0},null,3.2,19.240000000000002,26.240000000000002,62.239999999999995,{"$error":"#VALUE!"},null,3.2,46.24,19.240000000000002,55.240000000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Presjek III -III",null,null,3.52,null,{"$error":"#VALUE!"},1.1999999999999991,0,1.5199999999999991,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+Z277","v":0},0,0,{"$f":"+AC277","v":0},0,0,{"$f":"+AF277","v":0},{"$f":"+AE277","v":0},null,3.52,21.3904,28.3904,64.3904,{"$error":"#VALUE!"},null,3.52,48.3904,21.3904,57.390400000000007,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["IV-IV=Mmin",null,null,null,null,0,{"$f":"+G277","v":1.1999999999999991},0,{"$f":"+G278","v":1.1999999999999991},0,{"$f":"+I278","v":1.1999999999999991},0,{"$f":"+K278","v":1.1999999999999991},0,{"$f":"+M278","v":1.1999999999999991},0,{"$f":"+O278","v":1.1999999999999991},0,{"$f":"+Q278","v":1.1999999999999991},0,{"$f":"+S278","v":1.1999999999999991},0,{"$f":"+S278","v":1.1999999999999991},0,{"$f":"+W278","v":1.1999999999999991},0,{"$f":"+Y278","v":1.1999999999999991},0,{"$f":"+Y278","v":1.1999999999999991},0,{"$f":"+AA278","v":1.1999999999999991},0,{"$f":"+AE278","v":1.1999999999999991},0,{"$f":"+AG278","v":1.1999999999999991},0,{"$f":"+AG278","v":1.1999999999999991},null,0,9,16,51.999999999999993,0,null,0,36,9,45.000000000000007,0,0]
[null,null,null,null,null,0,{"$f":"+G266","v":4.7199999999999989},0,{"$f":"+I239","v":6},0,{"$f":"+I279","v":6},0,{"$f":"+K279","v":6},0,{"$f":"+M279","v":6},0,{"$f":"+O279","v":6},0,{"$f":"+Q279","v":6},0,{"$f":"+S279","v":6},0,{"$f":"+U279","v":6},0,{"$f":"+W279","v":6},0,{"$f":"+Y279","v":6},0,{"$f":"+AA279","v":6},{"$f":"+Z279","v":0},{"$f":"+AA279","v":6},0,{"$f":"+AE279","v":6},0,{"$f":"+AG279","v":6},0,{"$f":"+AI279","v":6}]
[null,null,null,"Ukupni pritisak",null,"SQhi=",{"$f":"+G283","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I283","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K283","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+M283","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+O283","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Q283","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+S283","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+U283","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+W283","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Y283","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AA283","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AC283","v":0},"SQhi=",{"$f":"+AE283","v":0},"SQhi=",{"$f":"+AG283","v":0},"SQhi=",{"$f":"+AI283","v":0},"SQhi=",{"$f":"+AK283","v":0}]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G285","v":{"$error":"#VALUE!"}},{"$f":"+H285","v":"y="},{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",{"$error":"#VALUE!"},"y=",0,"y=",0,"y=",0,"y=",0,"y=",0]
[null,null,null,"krak za presjek III -III",null,"z=",{"$f":"+G281-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I281-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K281-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M281-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+O281-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Q281-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+S281-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+U281-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}},"z=",{"$f":"+W281-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Y281-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AA281-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AC281-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AE281-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AG281-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AI281-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AK281-'Analiza i dimenzioniranje'!$E$52","v":-1.2}]
[null,null,null,null,null,"F=",{"$f":"-0.5*(+\n (F262*G263-F263*G262)+\n(F263*G264-F264*G263)+\n(F264*G265-F265*G264)+\n(F265*G266-F266*G265)+\n(F266*G267-F267*G266)+\n(F267*G268-F268*G267)+\n(F268*G269-F269*G268)+\n(F269*G270-F270*G269)+\n(F270*G271-F271*G270)+\n(F271*G272-F272*G271)+\n(F272*G273-F273*G272)+\n(F273*G274-F274*G273)+\n(F274*G275-F275*G274)+\n(F275*G276-F276*G275)+\n(F276*G277-F277*G276)+\n(F277*G278-F278*G277)+\n(F278*G279-F279*G278))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (H262*I263-H263*I262)+\n(H263*I264-H264*I263)+\n(H264*I265-H265*I264)+\n(H265*I266-H266*I265)+\n(H266*I267-H267*I266)+\n(H267*I268-H268*I267)+\n(H268*I269-H269*I268)+\n(H269*I270-H270*I269)+\n(H270*I271-H271*I270)+\n(H271*I272-H272*I271)+\n(H272*I273-H273*I272)+\n(H273*I274-H274*I273)+\n(H274*I275-H275*I274)+\n(H275*I276-H276*I275)+\n(H276*I277-H277*I276)+\n(H277*I278-H278*I277)+\n(H278*I279-H279*I278))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (J262*K263-J263*K262)+\n(J263*K264-J264*K263)+\n(J264*K265-J265*K264)+\n(J265*K266-J266*K265)+\n(J266*K267-J267*K266)+\n(J267*K268-J268*K267)+\n(J268*K269-J269*K268)+\n(J269*K270-J270*K269)+\n(J270*K271-J271*K270)+\n(J271*K272-J272*K271)+\n(J272*K273-J273*K272)+\n(J273*K274-J274*K273)+\n(J274*K275-J275*K274)+\n(J275*K276-J276*K275)+\n(J276*K277-J277*K276)+\n(J277*K278-J278*K277)+\n(J278*K279-J279*K278))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (L262*M263-L263*M262)+\n(L263*M264-L264*M263)+\n(L264*M265-L265*M264)+\n(L265*M266-L266*M265)+\n(L266*M267-L267*M266)+\n(L267*M268-L268*M267)+\n(L268*M269-L269*M268)+\n(L269*M270-L270*M269)+\n(L270*M271-L271*M270)+\n(L271*M272-L272*M271)+\n(L272*M273-L273*M272)+\n(L273*M274-L274*M273)+\n(L274*M275-L275*M274)+\n(L275*M276-L276*M275)+\n(L276*M277-L277*M276)+\n(L277*M278-L278*M277)+\n(L278*M279-L279*M278))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (N262*O263-N263*O262)+\n(N263*O264-N264*O263)+\n(N264*O265-N265*O264)+\n(N265*O266-N266*O265)+\n(N266*O267-N267*O266)+\n(N267*O268-N268*O267)+\n(N268*O269-N269*O268)+\n(N269*O270-N270*O269)+\n(N270*O271-N271*O270)+\n(N271*O272-N272*O271)+\n(N272*O273-N273*O272)+\n(N273*O274-N274*O273)+\n(N274*O275-N275*O274)+\n(N275*O276-N276*O275)+\n(N276*O277-N277*O276)+\n(N277*O278-N278*O277)+\n(N278*O279-N279*O278))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (P262*Q263-P263*Q262)+\n(P263*Q264-P264*Q263)+\n(P264*Q265-P265*Q264)+\n(P265*Q266-P266*Q265)+\n(P266*Q267-P267*Q266)+\n(P267*Q268-P268*Q267)+\n(P268*Q269-P269*Q268)+\n(P269*Q270-P270*Q269)+\n(P270*Q271-P271*Q270)+\n(P271*Q272-P272*Q271)+\n(P272*Q273-P273*Q272)+\n(P273*Q274-P274*Q273)+\n(P274*Q275-P275*Q274)+\n(P275*Q276-P276*Q275)+\n(P276*Q277-P277*Q276)+\n(P277*Q278-P278*Q277)+\n(P278*Q279-P279*Q278))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (R262*S263-R263*S262)+\n(R263*S264-R264*S263)+\n(R264*S265-R265*S264)+\n(R265*S266-R266*S265)+\n(R266*S267-R267*S266)+\n(R267*S268-R268*S267)+\n(R268*S269-R269*S268)+\n(R269*S270-R270*S269)+\n(R270*S271-R271*S270)+\n(R271*S272-R272*S271)+\n(R272*S273-R273*S272)+\n(R273*S274-R274*S273)+\n(R274*S275-R275*S274)+\n(R275*S276-R276*S275)+\n(R276*S277-R277*S276)+\n(R277*S278-R278*S277)+\n(R278*S279-R279*S278))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (T262*U263-T263*U262)+\n(T263*U264-T264*U263)+\n(T264*U265-T265*U264)+\n(T265*U266-T266*U265)+\n(T266*U267-T267*U266)+\n(T267*U268-T268*U267)+\n(T268*U269-T269*U268)+\n(T269*U270-T270*U269)+\n(T270*U271-T271*U270)+\n(T271*U272-T272*U271)+\n(T272*U273-T273*U272)+\n(T273*U274-T274*U273)+\n(T274*U275-T275*U274)+\n(T275*U276-T276*U275)+\n(T276*U277-T277*U276)+\n(T277*U278-T278*U277)+\n(T278*U279-T279*U278))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (V262*W263-V263*W262)+\n(V263*W264-V264*W263)+\n(V264*W265-V265*W264)+\n(V265*W266-V266*W265)+\n(V266*W267-V267*W266)+\n(V267*W268-V268*W267)+\n(V268*W269-V269*W268)+\n(V269*W270-V270*W269)+\n(V270*W271-V271*W270)+\n(V271*W272-V272*W271)+\n(V272*W273-V273*W272)+\n(V273*W274-V274*W273)+\n(V274*W275-V275*W274)+\n(V275*W276-V276*W275)+\n(V276*W277-V277*W276)+\n(V277*W278-V278*W277)+\n(V278*W279-V279*W278))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (X262*Y263-X263*Y262)+\n(X263*Y264-X264*Y263)+\n(X264*Y265-X265*Y264)+\n(X265*Y266-X266*Y265)+\n(X266*Y267-X267*Y266)+\n(X267*Y268-X268*Y267)+\n(X268*Y269-X269*Y268)+\n(X269*Y270-X270*Y269)+\n(X270*Y271-X271*Y270)+\n(X271*Y272-X272*Y271)+\n(X272*Y273-X273*Y272)+\n(X273*Y274-X274*Y273)+\n(X274*Y275-X275*Y274)+\n(X275*Y276-X276*Y275)+\n(X276*Y277-X277*Y276)+\n(X277*Y278-X278*Y277)+\n(X278*Y279-X279*Y278))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (Z262*AA263-Z263*AA262)+\n(Z263*AA264-Z264*AA263)+\n(Z264*AA265-Z265*AA264)+\n(Z265*AA266-Z266*AA265)+\n(Z266*AA267-Z267*AA266)+\n(Z267*AA268-Z268*AA267)+\n(Z268*AA269-Z269*AA268)+\n(Z269*AA270-Z270*AA269)+\n(Z270*AA271-Z271*AA270)+\n(Z271*AA272-Z272*AA271)+\n(Z272*AA273-Z273*AA272)+\n(Z273*AA274-Z274*AA273)+\n(Z274*AA275-Z275*AA274)+\n(Z275*AA276-Z276*AA275)+\n(Z276*AA277-Z277*AA276)+\n(Z277*AA278-Z278*AA277)+\n(Z278*AA279-Z279*AA278))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (AB262*AC263-AB263*AC262)+\n(AB263*AC264-AB264*AC263)+\n(AB264*AC265-AB265*AC264)+\n(AB265*AC266-AB266*AC265)+\n(AB266*AC267-AB267*AC266)+\n(AB267*AC268-AB268*AC267)+\n(AB268*AC269-AB269*AC268)+\n(AB269*AC270-AB270*AC269)+\n(AB270*AC271-AB271*AC270)+\n(AB271*AC272-AB272*AC271)+\n(AB272*AC273-AB273*AC272)+\n(AB273*AC274-AB274*AC273)+\n(AB274*AC275-AB275*AC274)+\n(AB275*AC276-AB276*AC275)+\n(AB276*AC277-AB277*AC276)+\n(AB277*AC278-AB278*AC277)+\n(AB278*AC279-AB279*AC278))","v":0},"F=",{"$f":"-0.5*(+\n (AD262*AE263-AD263*AE262)+\n(AD263*AE264-AD264*AE263)+\n(AD264*AE265-AD265*AE264)+\n(AD265*AE266-AD266*AE265)+\n(AD266*AE267-AD267*AE266)+\n(AD267*AE268-AD268*AE267)+\n(AD268*AE269-AD269*AE268)+\n(AD269*AE270-AD270*AE269)+\n(AD270*AE271-AD271*AE270)+\n(AD271*AE272-AD272*AE271)+\n(AD272*AE273-AD273*AE272)+\n(AD273*AE274-AD274*AE273)+\n(AD274*AE275-AD275*AE274)+\n(AD275*AE276-AD276*AE275)+\n(AD276*AE277-AD277*AE276)+\n(AD277*AE278-AD278*AE277)+\n(AD278*AE279-AD279*AE278))","v":0},"F=",{"$f":"-0.5*(+\n (AF262*AG263-AF263*AG262)+\n(AF263*AG264-AF264*AG263)+\n(AF264*AG265-AF265*AG264)+\n(AF265*AG266-AF266*AG265)+\n(AF266*AG267-AF267*AG266)+\n(AF267*AG268-AF268*AG267)+\n(AF268*AG269-AF269*AG268)+\n(AF269*AG270-AF270*AG269)+\n(AF270*AG271-AF271*AG270)+\n(AF271*AG272-AF272*AG271)+\n(AF272*AG273-AF273*AG272)+\n(AF273*AG274-AF274*AG273)+\n(AF274*AG275-AF275*AG274)+\n(AF275*AG276-AF276*AG275)+\n(AF276*AG277-AF277*AG276)+\n(AF277*AG278-AF278*AG277)+\n(AF278*AG279-AF279*AG278))","v":0},"F=",{"$f":"-0.5*(+\n (AH262*AI263-AH263*AI262)+\n(AH263*AI264-AH264*AI263)+\n(AH264*AI265-AH265*AI264)+\n(AH265*AI266-AH266*AI265)+\n(AH266*AI267-AH267*AI266)+\n(AH267*AI268-AH268*AI267)+\n(AH268*AI269-AH269*AI268)+\n(AH269*AI270-AH270*AI269)+\n(AH270*AI271-AH271*AI270)+\n(AH271*AI272-AH272*AI271)+\n(AH272*AI273-AH273*AI272)+\n(AH273*AI274-AH274*AI273)+\n(AH274*AI275-AH275*AI274)+\n(AH275*AI276-AH276*AI275)+\n(AH276*AI277-AH277*AI276)+\n(AH277*AI278-AH278*AI277)+\n(AH278*AI279-AH279*AI278))","v":0},"F=",{"$f":"-0.5*(+\n (AJ262*AK263-AJ263*AK262)+\n(AJ263*AK264-AJ264*AK263)+\n(AJ264*AK265-AJ265*AK264)+\n(AJ265*AK266-AJ266*AK265)+\n(AJ266*AK267-AJ267*AK266)+\n(AJ267*AK268-AJ268*AK267)+\n(AJ268*AK269-AJ269*AK268)+\n(AJ269*AK270-AJ270*AK269)+\n(AJ270*AK271-AJ271*AK270)+\n(AJ271*AK272-AJ272*AK271)+\n(AJ272*AK273-AJ273*AK272)+\n(AJ273*AK274-AJ274*AK273)+\n(AJ274*AK275-AJ275*AK274)+\n(AJ275*AK276-AJ276*AK275)+\n(AJ276*AK277-AJ277*AK276)+\n(AJ277*AK278-AJ278*AK277)+\n(AJ278*AK279-AJ279*AK278))","v":0}]
[null,null,null,null,null,"x=",1,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0]
[null,null,null,null,null,"y=",{"$f":"+IF(G283=0,0,-((F260*G261-F261*G260)*(G260+G261)+(F261*G262-F262*G261)*(G261+G262)+\n(F262*G263-F263*G262)*(G262+G263)+\n(F263*G264-F264*G263)*(G263+G264)+\n(F264*G265-F265*G264)*(G264+G265)+\n(F265*G266-F266*G265)*(G265+G266)+\n(F266*G267-F267*G266)*(G266+G267)+\n(F267*G268-F268*G267)*(G267+G268)+\n(F268*G269-F269*G268)*(G268+G269)+\n(F269*G270-F270*G269)*(G269+G270)+\n(F270*G271-F271*G270)*(G270+G271)+\n(F271*G272-F272*G271)*(G271+G272)+\n(F272*G273-F273*G272)*(G272+G273)+\n(F273*G274-F274*G273)*(G273+G274)+\n(F274*G275-F275*G274)*(G274+G275)+\n(F275*G276-F276*G275)*(G275+G276)+\n(F276*G277-F277*G276)*(G276+G277)+\n(F277*G278-F278*G277)*(G277+G278)+\n(F278*G279-F279*G278)*(G278+G279))/6/G283)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(I283=0,0,-((H260*I261-H261*I260)*(I260+I261)+(H261*I262-H262*I261)*(I261+I262)+\n(H262*I263-H263*I262)*(I262+I263)+\n(H263*I264-H264*I263)*(I263+I264)+\n(H264*I265-H265*I264)*(I264+I265)+\n(H265*I266-H266*I265)*(I265+I266)+\n(H266*I267-H267*I266)*(I266+I267)+\n(H267*I268-H268*I267)*(I267+I268)+\n(H268*I269-H269*I268)*(I268+I269)+\n(H269*I270-H270*I269)*(I269+I270)+\n(H270*I271-H271*I270)*(I270+I271)+\n(H271*I272-H272*I271)*(I271+I272)+\n(H272*I273-H273*I272)*(I272+I273)+\n(H273*I274-H274*I273)*(I273+I274)+\n(H274*I275-H275*I274)*(I274+I275)+\n(H275*I276-H276*I275)*(I275+I276)+\n(H276*I277-H277*I276)*(I276+I277)+\n(H277*I278-H278*I277)*(I277+I278)+\n(H278*I279-H279*I278)*(I278+I279))/6/I283)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(K283=0,0,-((J260*K261-J261*K260)*(K260+K261)+(J261*K262-J262*K261)*(K261+K262)+\n(J262*K263-J263*K262)*(K262+K263)+\n(J263*K264-J264*K263)*(K263+K264)+\n(J264*K265-J265*K264)*(K264+K265)+\n(J265*K266-J266*K265)*(K265+K266)+\n(J266*K267-J267*K266)*(K266+K267)+\n(J267*K268-J268*K267)*(K267+K268)+\n(J268*K269-J269*K268)*(K268+K269)+\n(J269*K270-J270*K269)*(K269+K270)+\n(J270*K271-J271*K270)*(K270+K271)+\n(J271*K272-J272*K271)*(K271+K272)+\n(J272*K273-J273*K272)*(K272+K273)+\n(J273*K274-J274*K273)*(K273+K274)+\n(J274*K275-J275*K274)*(K274+K275)+\n(J275*K276-J276*K275)*(K275+K276)+\n(J276*K277-J277*K276)*(K276+K277)+\n(J277*K278-J278*K277)*(K277+K278)+\n(J278*K279-J279*K278)*(K278+K279))/6/K283)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(M283=0,0,-((L260*M261-L261*M260)*(M260+M261)+(L261*M262-L262*M261)*(M261+M262)+\n(L262*M263-L263*M262)*(M262+M263)+\n(L263*M264-L264*M263)*(M263+M264)+\n(L264*M265-L265*M264)*(M264+M265)+\n(L265*M266-L266*M265)*(M265+M266)+\n(L266*M267-L267*M266)*(M266+M267)+\n(L267*M268-L268*M267)*(M267+M268)+\n(L268*M269-L269*M268)*(M268+M269)+\n(L269*M270-L270*M269)*(M269+M270)+\n(L270*M271-L271*M270)*(M270+M271)+\n(L271*M272-L272*M271)*(M271+M272)+\n(L272*M273-L273*M272)*(M272+M273)+\n(L273*M274-L274*M273)*(M273+M274)+\n(L274*M275-L275*M274)*(M274+M275)+\n(L275*M276-L276*M275)*(M275+M276)+\n(L276*M277-L277*M276)*(M276+M277)+\n(L277*M278-L278*M277)*(M277+M278)+\n(L278*M279-L279*M278)*(M278+M279))/6/M283)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(O283=0,0,-((N260*O261-N261*O260)*(O260+O261)+(N261*O262-N262*O261)*(O261+O262)+\n(N262*O263-N263*O262)*(O262+O263)+\n(N263*O264-N264*O263)*(O263+O264)+\n(N264*O265-N265*O264)*(O264+O265)+\n(N265*O266-N266*O265)*(O265+O266)+\n(N266*O267-N267*O266)*(O266+O267)+\n(N267*O268-N268*O267)*(O267+O268)+\n(N268*O269-N269*O268)*(O268+O269)+\n(N269*O270-N270*O269)*(O269+O270)+\n(N270*O271-N271*O270)*(O270+O271)+\n(N271*O272-N272*O271)*(O271+O272)+\n(N272*O273-N273*O272)*(O272+O273)+\n(N273*O274-N274*O273)*(O273+O274)+\n(N274*O275-N275*O274)*(O274+O275)+\n(N275*O276-N276*O275)*(O275+O276)+\n(N276*O277-N277*O276)*(O276+O277)+\n(N277*O278-N278*O277)*(O277+O278)+\n(N278*O279-N279*O278)*(O278+O279))/6/O283)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Q283=0,0,-((P260*Q261-P261*Q260)*(Q260+Q261)+(P261*Q262-P262*Q261)*(Q261+Q262)+\n(P262*Q263-P263*Q262)*(Q262+Q263)+\n(P263*Q264-P264*Q263)*(Q263+Q264)+\n(P264*Q265-P265*Q264)*(Q264+Q265)+\n(P265*Q266-P266*Q265)*(Q265+Q266)+\n(P266*Q267-P267*Q266)*(Q266+Q267)+\n(P267*Q268-P268*Q267)*(Q267+Q268)+\n(P268*Q269-P269*Q268)*(Q268+Q269)+\n(P269*Q270-P270*Q269)*(Q269+Q270)+\n(P270*Q271-P271*Q270)*(Q270+Q271)+\n(P271*Q272-P272*Q271)*(Q271+Q272)+\n(P272*Q273-P273*Q272)*(Q272+Q273)+\n(P273*Q274-P274*Q273)*(Q273+Q274)+\n(P274*Q275-P275*Q274)*(Q274+Q275)+\n(P275*Q276-P276*Q275)*(Q275+Q276)+\n(P276*Q277-P277*Q276)*(Q276+Q277)+\n(P277*Q278-P278*Q277)*(Q277+Q278)+\n(P278*Q279-P279*Q278)*(Q278+Q279))/6/Q283)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(S283=0,0,-((R260*S261-R261*S260)*(S260+S261)+(R261*S262-R262*S261)*(S261+S262)+\n(R262*S263-R263*S262)*(S262+S263)+\n(R263*S264-R264*S263)*(S263+S264)+\n(R264*S265-R265*S264)*(S264+S265)+\n(R265*S266-R266*S265)*(S265+S266)+\n(R266*S267-R267*S266)*(S266+S267)+\n(R267*S268-R268*S267)*(S267+S268)+\n(R268*S269-R269*S268)*(S268+S269)+\n(R269*S270-R270*S269)*(S269+S270)+\n(R270*S271-R271*S270)*(S270+S271)+\n(R271*S272-R272*S271)*(S271+S272)+\n(R272*S273-R273*S272)*(S272+S273)+\n(R273*S274-R274*S273)*(S273+S274)+\n(R274*S275-R275*S274)*(S274+S275)+\n(R275*S276-R276*S275)*(S275+S276)+\n(R276*S277-R277*S276)*(S276+S277)+\n(R277*S278-R278*S277)*(S277+S278)+\n(R278*S279-R279*S278)*(S278+S279))/6/S283)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(U283=0,0,-((T260*U261-T261*U260)*(U260+U261)+(T261*U262-T262*U261)*(U261+U262)+\n(T262*U263-T263*U262)*(U262+U263)+\n(T263*U264-T264*U263)*(U263+U264)+\n(T264*U265-T265*U264)*(U264+U265)+\n(T265*U266-T266*U265)*(U265+U266)+\n(T266*U267-T267*U266)*(U266+U267)+\n(T267*U268-T268*U267)*(U267+U268)+\n(T268*U269-T269*U268)*(U268+U269)+\n(T269*U270-T270*U269)*(U269+U270)+\n(T270*U271-T271*U270)*(U270+U271)+\n(T271*U272-T272*U271)*(U271+U272)+\n(T272*U273-T273*U272)*(U272+U273)+\n(T273*U274-T274*U273)*(U273+U274)+\n(T274*U275-T275*U274)*(U274+U275)+\n(T275*U276-T276*U275)*(U275+U276)+\n(T276*U277-T277*U276)*(U276+U277)+\n(T277*U278-T278*U277)*(U277+U278)+\n(T278*U279-T279*U278)*(U278+U279))/6/U283)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(W283=0,0,-((V260*W261-V261*W260)*(W260+W261)+(V261*W262-V262*W261)*(W261+W262)+\n(V262*W263-V263*W262)*(W262+W263)+\n(V263*W264-V264*W263)*(W263+W264)+\n(V264*W265-V265*W264)*(W264+W265)+\n(V265*W266-V266*W265)*(W265+W266)+\n(V266*W267-V267*W266)*(W266+W267)+\n(V267*W268-V268*W267)*(W267+W268)+\n(V268*W269-V269*W268)*(W268+W269)+\n(V269*W270-V270*W269)*(W269+W270)+\n(V270*W271-V271*W270)*(W270+W271)+\n(V271*W272-V272*W271)*(W271+W272)+\n(V272*W273-V273*W272)*(W272+W273)+\n(V273*W274-V274*W273)*(W273+W274)+\n(V274*W275-V275*W274)*(W274+W275)+\n(V275*W276-V276*W275)*(W275+W276)+\n(V276*W277-V277*W276)*(W276+W277)+\n(V277*W278-V278*W277)*(W277+W278)+\n(V278*W279-V279*W278)*(W278+W279))/6/W283)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Y283=0,0,-((X260*Y261-X261*Y260)*(Y260+Y261)+(X261*Y262-X262*Y261)*(Y261+Y262)+\n(X262*Y263-X263*Y262)*(Y262+Y263)+\n(X263*Y264-X264*Y263)*(Y263+Y264)+\n(X264*Y265-X265*Y264)*(Y264+Y265)+\n(X265*Y266-X266*Y265)*(Y265+Y266)+\n(X266*Y267-X267*Y266)*(Y266+Y267)+\n(X267*Y268-X268*Y267)*(Y267+Y268)+\n(X268*Y269-X269*Y268)*(Y268+Y269)+\n(X269*Y270-X270*Y269)*(Y269+Y270)+\n(X270*Y271-X271*Y270)*(Y270+Y271)+\n(X271*Y272-X272*Y271)*(Y271+Y272)+\n(X272*Y273-X273*Y272)*(Y272+Y273)+\n(X273*Y274-X274*Y273)*(Y273+Y274)+\n(X274*Y275-X275*Y274)*(Y274+Y275)+\n(X275*Y276-X276*Y275)*(Y275+Y276)+\n(X276*Y277-X277*Y276)*(Y276+Y277)+\n(X277*Y278-X278*Y277)*(Y277+Y278)+\n(X278*Y279-X279*Y278)*(Y278+Y279))/6/Y283)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AA283=0,0,-((Z260*AA261-Z261*AA260)*(AA260+AA261)+(Z261*AA262-Z262*AA261)*(AA261+AA262)+\n(Z262*AA263-Z263*AA262)*(AA262+AA263)+\n(Z263*AA264-Z264*AA263)*(AA263+AA264)+\n(Z264*AA265-Z265*AA264)*(AA264+AA265)+\n(Z265*AA266-Z266*AA265)*(AA265+AA266)+\n(Z266*AA267-Z267*AA266)*(AA266+AA267)+\n(Z267*AA268-Z268*AA267)*(AA267+AA268)+\n(Z268*AA269-Z269*AA268)*(AA268+AA269)+\n(Z269*AA270-Z270*AA269)*(AA269+AA270)+\n(Z270*AA271-Z271*AA270)*(AA270+AA271)+\n(Z271*AA272-Z272*AA271)*(AA271+AA272)+\n(Z272*AA273-Z273*AA272)*(AA272+AA273)+\n(Z273*AA274-Z274*AA273)*(AA273+AA274)+\n(Z274*AA275-Z275*AA274)*(AA274+AA275)+\n(Z275*AA276-Z276*AA275)*(AA275+AA276)+\n(Z276*AA277-Z277*AA276)*(AA276+AA277)+\n(Z277*AA278-Z278*AA277)*(AA277+AA278)+\n(Z278*AA279-Z279*AA278)*(AA278+AA279))/6/AA283)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AC283=0,0,-((AB260*AC261-AB261*AC260)*(AC260+AC261)+(AB261*AC262-AB262*AC261)*(AC261+AC262)+\n(AB262*AC263-AB263*AC262)*(AC262+AC263)+\n(AB263*AC264-AB264*AC263)*(AC263+AC264)+\n(AB264*AC265-AB265*AC264)*(AC264+AC265)+\n(AB265*AC266-AB266*AC265)*(AC265+AC266)+\n(AB266*AC267-AB267*AC266)*(AC266+AC267)+\n(AB267*AC268-AB268*AC267)*(AC267+AC268)+\n(AB268*AC269-AB269*AC268)*(AC268+AC269)+\n(AB269*AC270-AB270*AC269)*(AC269+AC270)+\n(AB270*AC271-AB271*AC270)*(AC270+AC271)+\n(AB271*AC272-AB272*AC271)*(AC271+AC272)+\n(AB272*AC273-AB273*AC272)*(AC272+AC273)+\n(AB273*AC274-AB274*AC273)*(AC273+AC274)+\n(AB274*AC275-AB275*AC274)*(AC274+AC275)+\n(AB275*AC276-AB276*AC275)*(AC275+AC276)+\n(AB276*AC277-AB277*AC276)*(AC276+AC277)+\n(AB277*AC278-AB278*AC277)*(AC277+AC278)+\n(AB278*AC279-AB279*AC278)*(AC278+AC279))/6/AC283)","v":0},"y=",{"$f":"+IF(AE283=0,0,-((AD260*AE261-AD261*AE260)*(AE260+AE261)+(AD261*AE262-AD262*AE261)*(AE261+AE262)+\n(AD262*AE263-AD263*AE262)*(AE262+AE263)+\n(AD263*AE264-AD264*AE263)*(AE263+AE264)+\n(AD264*AE265-AD265*AE264)*(AE264+AE265)+\n(AD265*AE266-AD266*AE265)*(AE265+AE266)+\n(AD266*AE267-AD267*AE266)*(AE266+AE267)+\n(AD267*AE268-AD268*AE267)*(AE267+AE268)+\n(AD268*AE269-AD269*AE268)*(AE268+AE269)+\n(AD269*AE270-AD270*AE269)*(AE269+AE270)+\n(AD270*AE271-AD271*AE270)*(AE270+AE271)+\n(AD271*AE272-AD272*AE271)*(AE271+AE272)+\n(AD272*AE273-AD273*AE272)*(AE272+AE273)+\n(AD273*AE274-AD274*AE273)*(AE273+AE274)+\n(AD274*AE275-AD275*AE274)*(AE274+AE275)+\n(AD275*AE276-AD276*AE275)*(AE275+AE276)+\n(AD276*AE277-AD277*AE276)*(AE276+AE277)+\n(AD277*AE278-AD278*AE277)*(AE277+AE278)+\n(AD278*AE279-AD279*AE278)*(AE278+AE279))/6/AE283)","v":0},"y=",{"$f":"+IF(AG283=0,0,-((AF260*AG261-AF261*AG260)*(AG260+AG261)+(AF261*AG262-AF262*AG261)*(AG261+AG262)+\n(AF262*AG263-AF263*AG262)*(AG262+AG263)+\n(AF263*AG264-AF264*AG263)*(AG263+AG264)+\n(AF264*AG265-AF265*AG264)*(AG264+AG265)+\n(AF265*AG266-AF266*AG265)*(AG265+AG266)+\n(AF266*AG267-AF267*AG266)*(AG266+AG267)+\n(AF267*AG268-AF268*AG267)*(AG267+AG268)+\n(AF268*AG269-AF269*AG268)*(AG268+AG269)+\n(AF269*AG270-AF270*AG269)*(AG269+AG270)+\n(AF270*AG271-AF271*AG270)*(AG270+AG271)+\n(AF271*AG272-AF272*AG271)*(AG271+AG272)+\n(AF272*AG273-AF273*AG272)*(AG272+AG273)+\n(AF273*AG274-AF274*AG273)*(AG273+AG274)+\n(AF274*AG275-AF275*AG274)*(AG274+AG275)+\n(AF275*AG276-AF276*AG275)*(AG275+AG276)+\n(AF276*AG277-AF277*AG276)*(AG276+AG277)+\n(AF277*AG278-AF278*AG277)*(AG277+AG278)+\n(AF278*AG279-AF279*AG278)*(AG278+AG279))/6/AG283)","v":0},"y=",{"$f":"+IF(AI283=0,0,-((AH260*AI261-AH261*AI260)*(AI260+AI261)+(AH261*AI262-AH262*AI261)*(AI261+AI262)+\n(AH262*AI263-AH263*AI262)*(AI262+AI263)+\n(AH263*AI264-AH264*AI263)*(AI263+AI264)+\n(AH264*AI265-AH265*AI264)*(AI264+AI265)+\n(AH265*AI266-AH266*AI265)*(AI265+AI266)+\n(AH266*AI267-AH267*AI266)*(AI266+AI267)+\n(AH267*AI268-AH268*AI267)*(AI267+AI268)+\n(AH268*AI269-AH269*AI268)*(AI268+AI269)+\n(AH269*AI270-AH270*AI269)*(AI269+AI270)+\n(AH270*AI271-AH271*AI270)*(AI270+AI271)+\n(AH271*AI272-AH272*AI271)*(AI271+AI272)+\n(AH272*AI273-AH273*AI272)*(AI272+AI273)+\n(AH273*AI274-AH274*AI273)*(AI273+AI274)+\n(AH274*AI275-AH275*AI274)*(AI274+AI275)+\n(AH275*AI276-AH276*AI275)*(AI275+AI276)+\n(AH276*AI277-AH277*AI276)*(AI276+AI277)+\n(AH277*AI278-AH278*AI277)*(AI277+AI278)+\n(AH278*AI279-AH279*AI278)*(AI278+AI279))/6/AI283)","v":0},"y=",{"$f":"+IF(AK283=0,0,-((AJ260*AK261-AJ261*AK260)*(AK260+AK261)+(AJ261*AK262-AJ262*AK261)*(AK261+AK262)+\n(AJ262*AK263-AJ263*AK262)*(AK262+AK263)+\n(AJ263*AK264-AJ264*AK263)*(AK263+AK264)+\n(AJ264*AK265-AJ265*AK264)*(AK264+AK265)+\n(AJ265*AK266-AJ266*AK265)*(AK265+AK266)+\n(AJ266*AK267-AJ267*AK266)*(AK266+AK267)+\n(AJ267*AK268-AJ268*AK267)*(AK267+AK268)+\n(AJ268*AK269-AJ269*AK268)*(AK268+AK269)+\n(AJ269*AK270-AJ270*AK269)*(AK269+AK270)+\n(AJ270*AK271-AJ271*AK270)*(AK270+AK271)+\n(AJ271*AK272-AJ272*AK271)*(AK271+AK272)+\n(AJ272*AK273-AJ273*AK272)*(AK272+AK273)+\n(AJ273*AK274-AJ274*AK273)*(AK273+AK274)+\n(AJ274*AK275-AJ275*AK274)*(AK274+AK275)+\n(AJ275*AK276-AJ276*AK275)*(AK275+AK276)+\n(AJ276*AK277-AJ277*AK276)*(AK276+AK277)+\n(AJ277*AK278-AJ278*AK277)*(AK277+AK278)+\n(AJ278*AK279-AJ279*AK278)*(AK278+AK279))/6/AK283)","v":0}]
[]
[null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID "]
[null,"OPTEREĆENJE TEMELJEM",null,null,null,null,null,null,null," (TERZAGHY)"]
[]
[null,"KONTINUIRANO OPTEREĆENJE",null,"P - D=",{"$f":"IF('Analiza i dimenzioniranje'!$E$28-I290<=0,0,+'Analiza i dimenzioniranje'!$E$28-I290)","v":{"$error":"#VALUE!"}},"kN/m2","raster. iskopom   D=y*Df =",null,{"$f":"+'Analiza i dimenzioniranje'!$D$16*('Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20-D296)","v":{"$error":"#VALUE!"}},"kN/m2"]
[null," visina zida i temelja",null,"H =",{"$f":"+E252","v":{"$error":"#VALUE!"}},"m",{"$f":"E295","v":6}]
[null,"visina opterećenja iznad vrha zida",null,"h =",{"$f":"+E253","v":-1},"m",{"$f":"SQRT(E295^2+E294^2)","v":6.7082039324993694}]
[null,"širina temelja",null,"b =",{"$f":"+E254","v":1},"m   ",{"$f":"E294+E293","v":4}]
[null,"udaljenost temelja od zida",null,"D =",{"$f":"+E255","v":3},"m    "]
[null,"1/2 dužine temelja",null,"L/2=a=",{"$f":"+E256","v":6},"m",{"$f":"SQRT(G291^2+G293^2)","v":7.2111025509279782}]
["DNO TEMELJA NA VISINI","PRESJEK NA Visini ",null,{"$f":"+ROUND('Analiza i dimenzioniranje'!$U$62,2)","v":4.4000000000000004},null,"Presjek III -III",null,"Presjek VI",null,"Presjek VII-VII",null,"Presjek VIII-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"Presjek XIV-XIV",null,"Presjek XV-XV",null,"PresjekXVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX"]
[null,null,null,null,null,"(sb2-sb1)*2","Visina djelovanja","(sb2-sb1)*2","Visina djelovanja","sb1-sb2","Visina djelovanja","(sb2-sb1)*2","Visina djelovanja","(sb2-sb1)*2","Visina djelovanja","(sb2-sb1)*2","Visina djelovanja","sb1-sb2","Visina djelovanja","(sb2-sb1)*2","Visina djelovanja","sb1-sb2","Visina djelovanja","(sb2-sb1)*2","Visina djelovanja","(sb2-sb1)*2","Visina djelovanja","sb1-sb2","Visina djelovanja","(sb2-sb1)*2","Visina djelovanja","(sb2-sb1)*2","Visina djelovanja","(sb2-sb1)*2","Visina djelovanja","sb1-sb2","Visina djelovanja",null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2"]
[null,null,null,{"$f":"+F299","v":0},{"$f":"+D298-E296","v":0},"III",{"$f":"+D296","v":4.4000000000000004},"VI",{"$f":"+G298","v":4.4000000000000004},"VII",{"$f":"+G298","v":4.4000000000000004},"VIII",{"$f":"+D296","v":4.4000000000000004},"IX",{"$f":"+G298","v":4.4000000000000004},"X",{"$f":"+O298","v":4.4000000000000004},"XI",{"$f":"+G298","v":4.4000000000000004},"XII",{"$f":"+S298","v":4.4000000000000004},"XIII",{"$f":"+G298","v":4.4000000000000004},"XIV",{"$f":"+W298","v":4.4000000000000004},"XV",{"$f":"+G298","v":4.4000000000000004},"XVI",{"$f":"+AA298","v":4.4000000000000004},"XVII",{"$f":"+AC298","v":4.4000000000000004},"XVIII",{"$f":"+AC298","v":4.4000000000000004},"XIX",{"$f":"+AG298","v":4.4000000000000004},"XX",{"$f":"+AI298","v":4.4000000000000004},null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
[null,null,null,0,{"$f":"IF(D298>E$296,D298,E$296)","v":0},0,0,0,0,{"$f":"+D298","v":0},{"$f":"+K315","v":1.8400000000000003},0,0,{"$f":"+AN299","v":0},{"$f":"+O313","v":2.4800000000000004},0,0,0,0,0,0,0,0,0,0,{"$f":"+V299","v":0},0,0,0,{"$f":"+Z299","v":0},{"$f":"+AE305","v":0},0,0,0,0,0,{"$f":"+AK302","v":0},{"$f":"+J299","v":0}]
[null,null,null,0,{"$f":"IF(AW302>G$298,0,AW302)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+R300","v":0},{"$f":"+AU300","v":0},0,0,0,0,{"$f":"+AD300","v":0},0,0]
[null,null,null,0,{"$f":"+AW303","v":0},0,0,0,0,0,{"$f":"+E300","v":0},0,0,0,{"$f":"+AM301","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU301","v":0},0,0,0,0,0,0,0]
[null,null,null,0,{"$f":"IF(#REF!>G$298,0,#REF!)","v":{"$error":"#REF!"}},0,0,0,0,0,0,0,0,0,{"$f":"+AM302","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU302","v":0},0,0,0,0,0,0,0]
[null,null,null,0,{"$f":"IF(#REF!>G$298,0,#REF!)","v":{"$error":"#REF!"}},0,0,0,0,{"$f":"+F301","v":0},0,0,0,0,{"$f":"+AM303","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU303","v":0},0,0,0,0,0,0,{"$f":"+D300","v":0}]
[null,null,null,0,{"$f":"IF(#REF!>G$298,0,#REF!)","v":{"$error":"#REF!"}},0,0,0,0,{"$f":"+F302","v":0},0,0,0,0,{"$f":"+AM304","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU304","v":0},0,0,0,0,0,0,{"$f":"+D301","v":0}]
[null,null,null,0,{"$f":"IF(#REF!>G$298,0,#REF!)","v":{"$error":"#REF!"}},0,0,0,0,0,0,0,0,0,{"$f":"+AM305","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+D307","v":0}]
[null,null,null,0,{"$f":"IF(#REF!>G$298,0,#REF!)","v":{"$error":"#REF!"}},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+S306","v":0},0,0,0,0,null,null,null,null,0,0,{"$f":"+D142","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+D266","v":0},null,{"$f":"+D307","v":0},{"$f":"+D296","v":4.4000000000000004},{"$f":"+F307","v":0},4.4000000000000004,0,4.4000000000000004,0,4.4000000000000004,{"$f":"+J305","v":0},{"$f":"+M307","v":4.4000000000000004},0,4.4000000000000004,0,{"$f":"+Q307","v":4.4000000000000004},{"$f":"+R307","v":0},{"$f":"+S307","v":4.4000000000000004},0,{"$f":"+U307","v":4.4000000000000004},0,4.4000000000000004,0,4.4000000000000004,0,{"$f":"+U307","v":4.4000000000000004},0,{"$f":"+Y307","v":4.4000000000000004},0,{"$f":"+Y307","v":4.4000000000000004},0,{"$f":"+AA307","v":4.4000000000000004},0,{"$f":"+AI307","v":4.4000000000000004},{"$f":"+D309","v":0.64},{"$f":"+D307","v":0},{"$f":"+AN266","v":0},{"$f":"+AO266","v":0},{"$f":"+AP266","v":0},{"$f":"+AQ266","v":0},null,{"$f":"+AM307","v":0},{"$f":"$E$295^2+AS307^2","v":36},{"$f":"$E$294^2+AS307^2","v":9},{"$f":"$G$292^2+AS307^2","v":45.000000000000007},{"$f":"IF(AS307=0,0,($E$290/(PI()))*(ATAN(($E$295*$E$294)/(AS307*SQRT(AV307)))-$E$295*$E$294*AS307/(AU307*SQRT(AV307))))","v":0},{"$f":"+AQ307-AW307","v":0}]
[null,null,null,{"$f":"+('Analiza i dimenzioniranje'!E48-'Analiza i dimenzioniranje'!E52)/15","v":0.32},null,{"$f":"+AX308","v":{"$error":"#VALUE!"}},{"$f":"+G$307-D308","v":4.08},{"$f":"+F308","v":{"$error":"#VALUE!"}},4.08,{"$error":"#VALUE!"},4.08,{"$error":"#VALUE!"},4.08,{"$error":"#VALUE!"},4.08,{"$error":"#VALUE!"},4.08,{"$f":"+P308","v":{"$error":"#VALUE!"}},{"$f":"+Q308","v":4.08},{"$f":"+R308","v":{"$error":"#VALUE!"}},{"$f":"+S308","v":4.08},{"$f":"+T308","v":{"$error":"#VALUE!"}},4.08,{"$error":"#VALUE!"},4.08,0,{"$f":"+Y308","v":4.08},{"$f":"+Z308","v":0},{"$f":"+AA308","v":4.08},{"$f":"+AB308","v":0},0,{"$f":"+AD308","v":0},0,0,{"$f":"+AG308","v":0},0,0,0.96,0.32,{"$f":"$E$294^2+AM308^2","v":9.1023999999999994},{"$f":"$G$293^2+AM308^2","v":16.102399999999999},{"$f":"$G$295^2+AM308^2","v":52.102399999999996},{"$f":"IF(AM308=0,0,$E$290/(PI())*(ATAN(($E$295*$G$293)/(AM308*SQRT(AP308)))-$E$295*$G$293*AM308/(AO308*SQRT(AP308))))","v":{"$error":"#VALUE!"}},null,0.32,{"$f":"$E$295^2+AS308^2","v":36.102400000000003},{"$f":"$E$294^2+AS308^2","v":9.1023999999999994},{"$f":"$G$292^2+AS308^2","v":45.10240000000001},{"$f":"IF(AS308=0,0,($E$290/(PI()))*(ATAN(($E$295*$E$294)/(AS308*SQRT(AV308)))-$E$295*$E$294*AS308/(AU308*SQRT(AV308))))","v":{"$error":"#VALUE!"}},{"$f":"(+AQ308-AW308)*2","v":{"$error":"#VALUE!"}}]
[null,null,null,{"$f":"+D308+D$308","v":0.64},null,{"$error":"#VALUE!"},{"$f":"+G308-D308","v":3.7600000000000002},{"$f":"+F309","v":{"$error":"#VALUE!"}},3.7600000000000002,{"$f":"+F309","v":{"$error":"#VALUE!"}},{"$f":"+I309","v":3.7600000000000002},{"$f":"+J309","v":{"$error":"#VALUE!"}},3.7600000000000002,{"$error":"#VALUE!"},{"$f":"+M309","v":3.7600000000000002},{"$f":"+N309","v":{"$error":"#VALUE!"}},3.7600000000000002,{"$error":"#VALUE!"},3.7600000000000002,{"$f":"+R309","v":{"$error":"#VALUE!"}},{"$f":"+S309","v":3.7600000000000002},{"$f":"+T309","v":{"$error":"#VALUE!"}},{"$f":"+U309","v":3.7600000000000002},0,{"$f":"+Y308","v":4.08},0,0,{"$f":"+Z309","v":0},{"$f":"+AA309","v":0},0,0,{"$f":"+AD309","v":0},0,0,{"$f":"+AG309","v":0},{"$f":"+AD309","v":0},0,1.28,0.64,{"$f":"$E$294^2+AM309^2","v":9.4095999999999993},{"$f":"$G$293^2+AM309^2","v":16.409600000000001},{"$f":"$G$295^2+AM309^2","v":52.40959999999999},{"$f":"IF(AM309=0,0,$E$290/(PI())*(ATAN(($E$295*$G$293)/(AM309*SQRT(AP309)))-$E$295*$G$293*AM309/(AO309*SQRT(AP309))))","v":{"$error":"#VALUE!"}},null,0.64,{"$f":"$E$295^2+AS309^2","v":36.409599999999998},{"$f":"$E$294^2+AS309^2","v":9.4095999999999993},{"$f":"$G$292^2+AS309^2","v":45.409600000000005},{"$f":"IF(AS309=0,0,($E$290/(PI()))*(ATAN(($E$295*$E$294)/(AS309*SQRT(AV309)))-$E$295*$E$294*AS309/(AU309*SQRT(AV309))))","v":{"$error":"#VALUE!"}},{"$f":"(+AQ309-AW309)*2","v":{"$error":"#VALUE!"}}]
[null,null,null,0.96,null,{"$error":"#VALUE!"},{"$f":"+G$307-D310","v":3.4400000000000004},{"$error":"#VALUE!"},3.4400000000000004,{"$error":"#VALUE!"},3.4400000000000004,{"$error":"#VALUE!"},3.4400000000000004,{"$error":"#VALUE!"},3.4400000000000004,{"$error":"#VALUE!"},3.4400000000000004,{"$error":"#VALUE!"},3.4400000000000004,{"$f":"+R310","v":{"$error":"#VALUE!"}},3.4400000000000004,0,{"$f":"+W309","v":3.7600000000000002},0,0,0,0,0,0,0,0,0,0,0,0,0,0,1.6,0.96,9.9215999999999998,16.921600000000002,52.921599999999991,{"$error":"#VALUE!"},null,0.96,36.921599999999998,9.9215999999999998,45.921600000000005,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,1.28,null,{"$error":"#VALUE!"},3.12,{"$error":"#VALUE!"},3.12,{"$error":"#VALUE!"},3.12,{"$error":"#VALUE!"},3.12,{"$error":"#VALUE!"},3.12,{"$error":"#VALUE!"},3.12,{"$error":"#VALUE!"},3.12,0,{"$f":"+U310","v":3.4400000000000004},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1.9200000000000002,1.28,10.638400000000001,17.638400000000001,53.63839999999999,{"$error":"#VALUE!"},null,1.28,37.638399999999997,10.638400000000001,46.638400000000004,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,1.6,null,{"$error":"#VALUE!"},2.8000000000000003,{"$error":"#VALUE!"},2.8000000000000003,{"$error":"#VALUE!"},2.8000000000000003,{"$error":"#VALUE!"},2.8000000000000003,{"$error":"#VALUE!"},2.8000000000000003,{"$error":"#VALUE!"},2.8000000000000003,0,{"$f":"+S311","v":3.12},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,2.2400000000000002,1.6,11.56,18.560000000000002,54.559999999999995,{"$error":"#VALUE!"},null,1.6,38.56,11.56,47.560000000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,1.9200000000000002,null,{"$error":"#VALUE!"},2.4800000000000004,{"$error":"#VALUE!"},2.4800000000000004,{"$error":"#VALUE!"},2.4800000000000004,{"$error":"#VALUE!"},2.4800000000000004,{"$error":"#VALUE!"},2.4800000000000004,0,{"$f":"+Q312","v":2.8000000000000003},0,0,0,0,0,0,0,0,{"$f":"+V311","v":0},{"$f":"+S313","v":0},0,0,0,0,0,0,0,0,0,0,2.56,1.9200000000000002,12.686400000000001,19.686399999999999,55.686399999999992,{"$error":"#VALUE!"},null,1.9200000000000002,39.686399999999999,12.686400000000001,48.686400000000006,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,2.2400000000000002,null,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},2.16,0,{"$f":"+O313","v":2.4800000000000004},0,0,{"$f":"+N314","v":0},0,0,0,0,0,0,0,{"$f":"+V312","v":0},0,0,0,0,0,0,0,0,0,0,0,2.88,2.2400000000000002,14.017600000000002,21.017600000000002,57.017599999999995,{"$error":"#VALUE!"},null,2.2400000000000002,41.017600000000002,14.017600000000002,50.017600000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,2.56,null,{"$error":"#VALUE!"},1.8400000000000003,{"$error":"#VALUE!"},1.8400000000000003,{"$error":"#VALUE!"},1.8400000000000003,0,{"$f":"+M314","v":2.16},0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+V313","v":0},0,0,0,0,0,0,0,0,0,0,0,3.1999999999999997,2.56,15.553599999999999,22.553599999999999,58.553599999999996,{"$error":"#VALUE!"},null,2.56,42.553600000000003,15.553599999999999,51.55360000000001,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,2.88,null,{"$error":"#VALUE!"},1.5200000000000005,{"$error":"#VALUE!"},1.5200000000000005,0,{"$f":"+K315","v":1.8400000000000003},0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+V314","v":0},0,0,0,0,0,0,0,0,0,0,0,0,2.88,17.2944,24.2944,60.294399999999996,{"$error":"#VALUE!"},null,2.88,44.294399999999996,17.2944,53.29440000000001,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,3.1999999999999997,null,{"$error":"#VALUE!"},1.2000000000000006,0,{"$f":"+I316","v":1.5200000000000005},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+V315","v":0},0,0,0,0,0,0,0,0,0,0,0,{"$f":"+D319","v":0},3.1999999999999997,19.239999999999998,26.24,62.239999999999995,{"$error":"#VALUE!"},null,3.1999999999999997,46.239999999999995,19.239999999999998,55.240000000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,{"$f":"+#REF!","v":{"$error":"#REF!"}},{"$f":"+Z265","v":0},{"$f":"+G317","v":1.2000000000000006},0,{"$f":"+G318","v":1.2000000000000006},0,{"$f":"+I318","v":1.2000000000000006},0,{"$f":"+K318","v":1.2000000000000006},0,{"$f":"+M318","v":1.2000000000000006},0,{"$f":"+O318","v":1.2000000000000006},0,{"$f":"+Q318","v":1.2000000000000006},0,{"$f":"+S318","v":1.2000000000000006},0,{"$f":"+S318","v":1.2000000000000006},0,{"$f":"+W318","v":1.2000000000000006},0,{"$f":"+Y318","v":1.2000000000000006},0,{"$f":"+Y318","v":1.2000000000000006},0,{"$f":"+AA318","v":1.2000000000000006},0,{"$f":"+AE318","v":1.2000000000000006},0,{"$f":"+AG318","v":1.2000000000000006},0,{"$f":"+AG318","v":1.2000000000000006},"Ukupni pritisak",null,null,null,null,null,null,null,null,{"$f":"+S341","v":0},{"$f":"AQ180-AW180","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$U$66","v":5.6800000000000006}]
[null,null,null,null,{"$f":"+E322","v":0},0,{"$f":"+G307","v":4.4000000000000004},0,{"$f":"+G319","v":4.4000000000000004},0,{"$f":"+I319","v":4.4000000000000004},0,{"$f":"+K319","v":4.4000000000000004},0,{"$f":"+M319","v":4.4000000000000004},0,{"$f":"+O319","v":4.4000000000000004},0,{"$f":"+Q319","v":4.4000000000000004},0,{"$f":"+S319","v":4.4000000000000004},0,{"$f":"+U319","v":4.4000000000000004},0,4.4000000000000004,0,{"$f":"+Y319","v":4.4000000000000004},0,{"$f":"+AA319","v":4.4000000000000004},{"$f":"+Z319","v":0},{"$f":"+AA319","v":4.4000000000000004},0,{"$f":"+AE319","v":4.4000000000000004},0,{"$f":"+AG319","v":4.4000000000000004},0,{"$f":"+AI319","v":4.4000000000000004},"Koordinata težišta ",null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$66","v":5.6800000000000006}]
[null,null,null,"Ukupni pritisak",null,"SQhi=",{"$f":"+G323","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I323","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K323","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+M323","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+O323","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Q323","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+S323","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+U323","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+W323","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Y323","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AA323","v":0},"SQhi=",{"$f":"+AC323","v":0},"SQhi=",{"$f":"+AE323","v":0},"SQhi=",{"$f":"+AG323","v":0},"SQhi=",{"$f":"+AI323","v":0},"SQhi=",{"$f":"+AK323","v":0},"krak za presjek III -III",null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$66","v":5.6800000000000006}]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G325","v":{"$error":"#VALUE!"}}," y=",{"$f":"+I325","v":{"$error":"#VALUE!"}}," y=",{"$f":"+K325","v":{"$error":"#VALUE!"}}," y=",{"$f":"+M325","v":{"$error":"#VALUE!"}}," y=",{"$f":"+O325","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Q325","v":{"$error":"#VALUE!"}}," y=",{"$f":"+S325","v":{"$error":"#VALUE!"}}," y=",{"$f":"+U325","v":{"$error":"#VALUE!"}}," y=",{"$f":"+W325","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Y325","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AA325","v":0}," y=",{"$f":"+AC325","v":0}," y=",{"$f":"+AE325","v":0}," y=",{"$f":"+AG325","v":0}," y=",{"$f":"+AI325","v":0}," y=",{"$f":"+AK325","v":0},"x=",null,null,null,null,null,null,null,null,0,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$66","v":5.6800000000000006}]
[null,null,null,"krak za presjek III -III",null,"z=",{"$f":"+G321-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I321-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K321-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M321-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+O321-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Q321-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+S321-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+U321-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}},"z=",{"$f":"+W321-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Y321-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AA321-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AC321-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AE321-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AG321-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AI321-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AK321-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"y=",null,null,null,null,null,null,null,null,0,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$65","v":5.36}]
[null,null,null,"x=",0,"F=",{"$f":"-0.5*(+\n (F302*G303-F303*G302)+\n(F303*G304-F304*G303)+\n(F304*G305-F305*G304)+\n(F305*G306-F306*G305)+\n(F306*G307-F307*G306)+\n(F307*G308-F308*G307)+\n(F308*G309-F309*G308)+\n(F309*G310-F310*G309)+\n(F310*G311-F311*G310)+\n(F311*G312-F312*G311)+\n(F312*G313-F313*G312)+\n(F313*G314-F314*G313)+\n(F314*G315-F315*G314)+\n(F315*G316-F316*G315)+\n(F316*G317-F317*G316)+\n(F317*G318-F318*G317)+\n(F318*G319-F319*G318))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (H302*I303-H303*I302)+\n(H303*I304-H304*I303)+\n(H304*I305-H305*I304)+\n(H305*I306-H306*I305)+\n(H306*I307-H307*I306)+\n(H307*I308-H308*I307)+\n(H308*I309-H309*I308)+\n(H309*I310-H310*I309)+\n(H310*I311-H311*I310)+\n(H311*I312-H312*I311)+\n(H312*I313-H313*I312)+\n(H313*I314-H314*I313)+\n(H314*I315-H315*I314)+\n(H315*I316-H316*I315)+\n(H316*I317-H317*I316)+\n(H317*I318-H318*I317)+\n(H318*I319-H319*I318))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((J300*K301-J301*K300)+(J301*K302-J302*K301)+\n (J302*K303-J303*K302)+\n(J303*K304-J304*K303)+\n(J304*K305-J305*K304)+\n(J305*K306-J306*K305)+\n(J306*K307-J307*K306)+\n(J307*K308-J308*K307)+\n(J308*K309-J309*K308)+\n(J309*K310-J310*K309)+\n(J310*K311-J311*K310)+\n(J311*K312-J312*K311)+\n(J312*K313-J313*K312)+\n(J313*K314-J314*K313)+\n(J314*K315-J315*K314)+\n(J315*K316-J316*K315)+\n(J316*K317-J317*K316)+\n(J317*K318-J318*K317)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (L302*M303-L303*M302)+\n(L303*M304-L304*M303)+\n(L304*M305-L305*M304)+\n(L305*M306-L306*M305)+\n(L306*M307-L307*M306)+\n(L307*M308-L308*M307)+\n(L308*M309-L309*M308)+\n(L309*M310-L310*M309)+\n(L310*M311-L311*M310)+\n(L311*M312-L312*M311)+\n(L312*M313-L313*M312)+\n(L313*M314-L314*M313)+\n(L314*M315-L315*M314)+\n(L315*M316-L316*M315)+\n(L316*M317-L317*M316)+\n(L317*M318-L318*M317)+\n(L318*M319-L319*M318))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((N300*O301-N301*O300)+(N301*O302-N302*O301)+\n (N302*O303-N303*O302)+\n(N303*O304-N304*O303)+\n(N304*O305-N305*O304)+\n(N305*O306-N306*O305)+\n(N306*O307-N307*O306)+\n(N307*O308-N308*O307)+\n(N308*O309-N309*O308)+\n(N309*O310-N310*O309)+\n(N310*O311-N311*O310)+\n(N311*O312-N312*O311)+\n(N312*O313-N313*O312)+\n(N313*O314-N314*O313)+\n(N314*O315-N315*O314)+\n(N315*O316-N316*O315)+\n(N316*O317-N317*O316)+\n(N317*O318-N318*O317)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (P302*Q303-P303*Q302)+\n(P303*Q304-P304*Q303)+\n(P304*Q305-P305*Q304)+\n(P305*Q306-P306*Q305)+\n(P306*Q307-P307*Q306)+\n(P307*Q308-P308*Q307)+\n(P308*Q309-P309*Q308)+\n(P309*Q310-P310*Q309)+\n(P310*Q311-P311*Q310)+\n(P311*Q312-P312*Q311)+\n(P312*Q313-P313*Q312)+\n(P313*Q314-P314*Q313)+\n(P314*Q315-P315*Q314)+\n(P315*Q316-P316*Q315)+\n(P316*Q317-P317*Q316)+\n(P317*Q318-P318*Q317)+\n(P318*Q319-P319*Q318))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (R302*S303-R303*S302)+\n(R303*S304-R304*S303)+\n(R304*S305-R305*S304)+\n(R305*S306-R306*S305)+\n(R306*S307-R307*S306)+\n(R307*S308-R308*S307)+\n(R308*S309-R309*S308)+\n(R309*S310-R310*S309)+\n(R310*S311-R311*S310)+\n(R311*S312-R312*S311)+\n(R312*S313-R313*S312)+\n(R313*S314-R314*S313)+\n(R314*S315-R315*S314)+\n(R315*S316-R316*S315)+\n(R316*S317-R317*S316)+\n(R317*S318-R318*S317)+\n(R318*S319-R319*S318))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (T302*U303-T303*U302)+\n(T303*U304-T304*U303)+\n(T304*U305-T305*U304)+\n(T305*U306-T306*U305)+\n(T306*U307-T307*U306)+\n(T307*U308-T308*U307)+\n(T308*U309-T309*U308)+\n(T309*U310-T310*U309)+\n(T310*U311-T311*U310)+\n(T311*U312-T312*U311)+\n(T312*U313-T313*U312)+\n(T313*U314-T314*U313)+\n(T314*U315-T315*U314)+\n(T315*U316-T316*U315)+\n(T316*U317-T317*U316)+\n(T317*U318-T318*U317)+\n(T318*U319-T319*U318))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (V302*W303-V303*W302)+\n(V303*W304-V304*W303)+\n(V304*W305-V305*W304)+\n(V305*W306-V306*W305)+\n(V306*W307-V307*W306)+\n(V307*W308-V308*W307)+\n(V308*W309-V309*W308)+\n(V309*W310-V310*W309)+\n(V310*W311-V311*W310)+\n(V311*W312-V312*W311)+\n(V312*W313-V313*W312)+\n(V313*W314-V314*W313)+\n(V314*W315-V315*W314)+\n(V315*W316-V316*W315)+\n(V316*W317-V317*W316)+\n(V317*W318-V318*W317)+\n(V318*W319-V319*W318))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (X302*Y303-X303*Y302)+\n(X303*Y304-X304*Y303)+\n(X304*Y305-X305*Y304)+\n(X305*Y306-X306*Y305)+\n(X306*Y307-X307*Y306)+\n(X307*Y308-X308*Y307)+\n(X308*Y309-X309*Y308)+\n(X309*Y310-X310*Y309)+\n(X310*Y311-X311*Y310)+\n(X311*Y312-X312*Y311)+\n(X312*Y313-X313*Y312)+\n(X313*Y314-X314*Y313)+\n(X314*Y315-X315*Y314)+\n(X315*Y316-X316*Y315)+\n(X316*Y317-X317*Y316)+\n(X317*Y318-X318*Y317)+\n(X318*Y319-X319*Y318))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (Z302*AA303-Z303*AA302)+\n(Z303*AA304-Z304*AA303)+\n(Z304*AA305-Z305*AA304)+\n(Z305*AA306-Z306*AA305)+\n(Z306*AA307-Z307*AA306)+\n(Z307*AA308-Z308*AA307)+\n(Z308*AA309-Z309*AA308)+\n(Z309*AA310-Z310*AA309)+\n(Z310*AA311-Z311*AA310)+\n(Z311*AA312-Z312*AA311)+\n(Z312*AA313-Z313*AA312)+\n(Z313*AA314-Z314*AA313)+\n(Z314*AA315-Z315*AA314)+\n(Z315*AA316-Z316*AA315)+\n(Z316*AA317-Z317*AA316)+\n(Z317*AA318-Z318*AA317)+\n(Z318*AA319-Z319*AA318))","v":0},"F=",{"$f":"-0.5*(+\n (AB302*AC303-AB303*AC302)+\n(AB303*AC304-AB304*AC303)+\n(AB304*AC305-AB305*AC304)+\n(AB305*AC306-AB306*AC305)+\n(AB306*AC307-AB307*AC306)+\n(AB307*AC308-AB308*AC307)+\n(AB308*AC309-AB309*AC308)+\n(AB309*AC310-AB310*AC309)+\n(AB310*AC311-AB311*AC310)+\n(AB311*AC312-AB312*AC311)+\n(AB312*AC313-AB313*AC312)+\n(AB313*AC314-AB314*AC313)+\n(AB314*AC315-AB315*AC314)+\n(AB315*AC316-AB316*AC315)+\n(AB316*AC317-AB317*AC316)+\n(AB317*AC318-AB318*AC317)+\n(AB318*AC319-AB319*AC318))","v":0},"F=",{"$f":"-0.5*(+\n (AD302*AE303-AD303*AE302)+\n(AD303*AE304-AD304*AE303)+\n(AD304*AE305-AD305*AE304)+\n(AD305*AE306-AD306*AE305)+\n(AD306*AE307-AD307*AE306)+\n(AD307*AE308-AD308*AE307)+\n(AD308*AE309-AD309*AE308)+\n(AD309*AE310-AD310*AE309)+\n(AD310*AE311-AD311*AE310)+\n(AD311*AE312-AD312*AE311)+\n(AD312*AE313-AD313*AE312)+\n(AD313*AE314-AD314*AE313)+\n(AD314*AE315-AD315*AE314)+\n(AD315*AE316-AD316*AE315)+\n(AD316*AE317-AD317*AE316)+\n(AD317*AE318-AD318*AE317)+\n(AD318*AE319-AD319*AE318))","v":0},"F=",{"$f":"-0.5*(+\n (AF302*AG303-AF303*AG302)+\n(AF303*AG304-AF304*AG303)+\n(AF304*AG305-AF305*AG304)+\n(AF305*AG306-AF306*AG305)+\n(AF306*AG307-AF307*AG306)+\n(AF307*AG308-AF308*AG307)+\n(AF308*AG309-AF309*AG308)+\n(AF309*AG310-AF310*AG309)+\n(AF310*AG311-AF311*AG310)+\n(AF311*AG312-AF312*AG311)+\n(AF312*AG313-AF313*AG312)+\n(AF313*AG314-AF314*AG313)+\n(AF314*AG315-AF315*AG314)+\n(AF315*AG316-AF316*AG315)+\n(AF316*AG317-AF317*AG316)+\n(AF317*AG318-AF318*AG317)+\n(AF318*AG319-AF319*AG318))","v":0},"F=",{"$f":"-0.5*(+\n (AH302*AI303-AH303*AI302)+\n(AH303*AI304-AH304*AI303)+\n(AH304*AI305-AH305*AI304)+\n(AH305*AI306-AH306*AI305)+\n(AH306*AI307-AH307*AI306)+\n(AH307*AI308-AH308*AI307)+\n(AH308*AI309-AH309*AI308)+\n(AH309*AI310-AH310*AI309)+\n(AH310*AI311-AH311*AI310)+\n(AH311*AI312-AH312*AI311)+\n(AH312*AI313-AH313*AI312)+\n(AH313*AI314-AH314*AI313)+\n(AH314*AI315-AH315*AI314)+\n(AH315*AI316-AH316*AI315)+\n(AH316*AI317-AH317*AI316)+\n(AH317*AI318-AH318*AI317)+\n(AH318*AI319-AH319*AI318))","v":0},"F=",{"$f":"-0.5*(+\n (AJ302*AK303-AJ303*AK302)+\n(AJ303*AK304-AJ304*AK303)+\n(AJ304*AK305-AJ305*AK304)+\n(AJ305*AK306-AJ306*AK305)+\n(AJ306*AK307-AJ307*AK306)+\n(AJ307*AK308-AJ308*AK307)+\n(AJ308*AK309-AJ309*AK308)+\n(AJ309*AK310-AJ310*AK309)+\n(AJ310*AK311-AJ311*AK310)+\n(AJ311*AK312-AJ312*AK311)+\n(AJ312*AK313-AJ313*AK312)+\n(AJ313*AK314-AJ314*AK313)+\n(AJ314*AK315-AJ315*AK314)+\n(AJ315*AK316-AJ316*AK315)+\n(AJ316*AK317-AJ317*AK316)+\n(AJ317*AK318-AJ318*AK317)+\n(AJ318*AK319-AJ319*AK318))","v":0},"y=",null,null,null,null,null,null,null,null,0,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$64","v":5.04}]
[null,null,null,"y=",{"$f":"+IF(E322=0,0,-((D299*E300-D300*E299)*(E299+E300)+(D300*E301-D301*E300)*(E300+E301)+\n(D301*E302-D307*E301)*(E301+E302)+\n(D307*E303-D308*E302)*(E302+E303)+\n(D308*E304-D309*E303)*(E303+E304)+\n(D309*E305-D310*E304)*(E304+E305)+\n(D310*E306-D311*E305)*(E305+E306)+\n(D311*#REF!-D312*E306)*(E306+#REF!)+\n(D312*#REF!-D313*#REF!)*(#REF!+#REF!)+\n(D313*#REF!-D314*#REF!)*(#REF!+#REF!)+\n(D314*#REF!-D315*#REF!)*(#REF!+#REF!)+\n(D315*#REF!-D316*#REF!)*(#REF!+#REF!)+\n(D316*#REF!-D317*#REF!)*(#REF!+#REF!)+\n(D317*#REF!-D318*#REF!)*(#REF!+#REF!)+\n(D318*#REF!-D319*#REF!)*(#REF!+#REF!)+\n(D319*#REF!-#REF!*#REF!)*(#REF!+#REF!)+\n(#REF!*#REF!-#REF!*#REF!)*(#REF!+#REF!)+\n(#REF!*#REF!-#REF!*#REF!)*(#REF!+#REF!)+\n(#REF!*E318-#REF!*#REF!)*(#REF!+E318))/6/E322)","v":0},"x=",1.5,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,0,null,null,null,null,null,null,null,null,0,{"$error":"#VALUE!"},{"$f":"'Analiza i dimenzioniranje'!$U$63","v":4.72}]
[null,null,null,"y=",{"$f":"+IF(E323=0,0,-((D300*E301-D301*E300)*(E300+E301)+(D301*E302-D307*E301)*(E301+E302)+\n(D307*E303-D308*E302)*(E302+E303)+\n(D308*E304-D309*E303)*(E303+E304)+\n(D309*E305-D310*E304)*(E304+E305)+\n(D310*E306-D311*E305)*(E305+E306)+\n(D311*#REF!-D312*E306)*(E306+#REF!)+\n(D312*#REF!-D313*#REF!)*(#REF!+#REF!)+\n(D313*#REF!-D314*#REF!)*(#REF!+#REF!)+\n(D314*#REF!-D315*#REF!)*(#REF!+#REF!)+\n(D315*#REF!-D316*#REF!)*(#REF!+#REF!)+\n(D316*#REF!-D317*#REF!)*(#REF!+#REF!)+\n(D317*#REF!-D318*#REF!)*(#REF!+#REF!)+\n(D318*#REF!-D319*#REF!)*(#REF!+#REF!)+\n(D319*#REF!-#REF!*#REF!)*(#REF!+#REF!)+\n(#REF!*#REF!-#REF!*#REF!)*(#REF!+#REF!)+\n(#REF!*#REF!-#REF!*#REF!)*(#REF!+#REF!)+\n(#REF!*E318-#REF!*#REF!)*(#REF!+E318)+\n(#REF!*E319-#REF!*E318)*(E318+E319))/6/E323)","v":0},"y=",{"$f":"+IF(G323=0,0,-((F300*G301-F301*G300)*(G300+G301)+(F301*G302-F302*G301)*(G301+G302)+\n(F302*G303-F303*G302)*(G302+G303)+\n(F303*G304-F304*G303)*(G303+G304)+\n(F304*G305-F305*G304)*(G304+G305)+\n(F305*G306-F306*G305)*(G305+G306)+\n(F306*G307-F307*G306)*(G306+G307)+\n(F307*G308-F308*G307)*(G307+G308)+\n(F308*G309-F309*G308)*(G308+G309)+\n(F309*G310-F310*G309)*(G309+G310)+\n(F310*G311-F311*G310)*(G310+G311)+\n(F311*G312-F312*G311)*(G311+G312)+\n(F312*G313-F313*G312)*(G312+G313)+\n(F313*G314-F314*G313)*(G313+G314)+\n(F314*G315-F315*G314)*(G314+G315)+\n(F315*G316-F316*G315)*(G315+G316)+\n(F316*G317-F317*G316)*(G316+G317)+\n(F317*G318-F318*G317)*(G317+G318)+\n(F318*G319-F319*G318)*(G318+G319))/6/G323)+0.11","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(I323=0,0,-((H300*I301-H301*I300)*(I300+I301)+(H301*I302-H302*I301)*(I301+I302)+\n(H302*I303-H303*I302)*(I302+I303)+\n(H303*I304-H304*I303)*(I303+I304)+\n(H304*I305-H305*I304)*(I304+I305)+\n(H305*I306-H306*I305)*(I305+I306)+\n(H306*I307-H307*I306)*(I306+I307)+\n(H307*I308-H308*I307)*(I307+I308)+\n(H308*I309-H309*I308)*(I308+I309)+\n(H309*I310-H310*I309)*(I309+I310)+\n(H310*I311-H311*I310)*(I310+I311)+\n(H311*I312-H312*I311)*(I311+I312)+\n(H312*I313-H313*I312)*(I312+I313)+\n(H313*I314-H314*I313)*(I313+I314)+\n(H314*I315-H315*I314)*(I314+I315)+\n(H315*I316-H316*I315)*(I315+I316)+\n(H316*I317-H317*I316)*(I316+I317)+\n(H317*I318-H318*I317)*(I317+I318)+\n(H318*I319-H319*I318)*(I318+I319))/6/I323)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(K323=0,0,-((J300*K301-J301*K300)*(K300+K301)+(J301*K302-J302*K301)*(K301+K302)+\n(J302*K303-J303*K302)*(K302+K303)+\n(J303*K304-J304*K303)*(K303+K304)+\n(J304*K305-J305*K304)*(K304+K305)+\n(J305*K306-J306*K305)*(K305+K306)+\n(J306*K307-J307*K306)*(K306+K307)+\n(J307*K308-J308*K307)*(K307+K308)+\n(J308*K309-J309*K308)*(K308+K309)+\n(J309*K310-J310*K309)*(K309+K310)+\n(J310*K311-J311*K310)*(K310+K311)+\n(J311*K312-J312*K311)*(K311+K312)+\n(J312*K313-J313*K312)*(K312+K313)+\n(J313*K314-J314*K313)*(K313+K314)+\n(J314*K315-J315*K314)*(K314+K315)+\n(J315*K316-J316*K315)*(K315+K316)+\n(J316*K317-J317*K316)*(K316+K317)+\n(J317*K318-J318*K317)*(K317+K318)+\n(J318*K319-J319*K318)*(K318+K319))/6/K323)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(M323=0,0,-((L300*M301-L301*M300)*(M300+M301)+(L301*M302-L302*M301)*(M301+M302)+\n(L302*M303-L303*M302)*(M302+M303)+\n(L303*M304-L304*M303)*(M303+M304)+\n(L304*M305-L305*M304)*(M304+M305)+\n(L305*M306-L306*M305)*(M305+M306)+\n(L306*M307-L307*M306)*(M306+M307)+\n(L307*M308-L308*M307)*(M307+M308)+\n(L308*M309-L309*M308)*(M308+M309)+\n(L309*M310-L310*M309)*(M309+M310)+\n(L310*M311-L311*M310)*(M310+M311)+\n(L311*M312-L312*M311)*(M311+M312)+\n(L312*M313-L313*M312)*(M312+M313)+\n(L313*M314-L314*M313)*(M313+M314)+\n(L314*M315-L315*M314)*(M314+M315)+\n(L315*M316-L316*M315)*(M315+M316)+\n(L316*M317-L317*M316)*(M316+M317)+\n(L317*M318-L318*M317)*(M317+M318)+\n(L318*M319-L319*M318)*(M318+M319))/6/M323)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(O323=0,0,-((N300*O301-N301*O300)*(O300+O301)+(N301*O302-N302*O301)*(O301+O302)+\n(N302*O303-N303*O302)*(O302+O303)+\n(N303*O304-N304*O303)*(O303+O304)+\n(N304*O305-N305*O304)*(O304+O305)+\n(N305*O306-N306*O305)*(O305+O306)+\n(N306*O307-N307*O306)*(O306+O307)+\n(N307*O308-N308*O307)*(O307+O308)+\n(N308*O309-N309*O308)*(O308+O309)+\n(N309*O310-N310*O309)*(O309+O310)+\n(N310*O311-N311*O310)*(O310+O311)+\n(N311*O312-N312*O311)*(O311+O312)+\n(N312*O313-N313*O312)*(O312+O313)+\n(N313*O314-N314*O313)*(O313+O314)+\n(N314*O315-N315*O314)*(O314+O315)+\n(N315*O316-N316*O315)*(O315+O316)+\n(N316*O317-N317*O316)*(O316+O317)+\n(N317*O318-N318*O317)*(O317+O318)+\n(N318*O319-N319*O318)*(O318+O319))/6/O323)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Q323=0,0,-((P300*Q301-P301*Q300)*(Q300+Q301)+(P301*Q302-P302*Q301)*(Q301+Q302)+\n(P302*Q303-P303*Q302)*(Q302+Q303)+\n(P303*Q304-P304*Q303)*(Q303+Q304)+\n(P304*Q305-P305*Q304)*(Q304+Q305)+\n(P305*Q306-P306*Q305)*(Q305+Q306)+\n(P306*Q307-P307*Q306)*(Q306+Q307)+\n(P307*Q308-P308*Q307)*(Q307+Q308)+\n(P308*Q309-P309*Q308)*(Q308+Q309)+\n(P309*Q310-P310*Q309)*(Q309+Q310)+\n(P310*Q311-P311*Q310)*(Q310+Q311)+\n(P311*Q312-P312*Q311)*(Q311+Q312)+\n(P312*Q313-P313*Q312)*(Q312+Q313)+\n(P313*Q314-P314*Q313)*(Q313+Q314)+\n(P314*Q315-P315*Q314)*(Q314+Q315)+\n(P315*Q316-P316*Q315)*(Q315+Q316)+\n(P316*Q317-P317*Q316)*(Q316+Q317)+\n(P317*Q318-P318*Q317)*(Q317+Q318)+\n(P318*Q319-P319*Q318)*(Q318+Q319))/6/Q323)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(S323=0,0,-((R300*S301-R301*S300)*(S300+S301)+(R301*S302-R302*S301)*(S301+S302)+\n(R302*S303-R303*S302)*(S302+S303)+\n(R303*S304-R304*S303)*(S303+S304)+\n(R304*S305-R305*S304)*(S304+S305)+\n(R305*S306-R306*S305)*(S305+S306)+\n(R306*S307-R307*S306)*(S306+S307)+\n(R307*S308-R308*S307)*(S307+S308)+\n(R308*S309-R309*S308)*(S308+S309)+\n(R309*S310-R310*S309)*(S309+S310)+\n(R310*S311-R311*S310)*(S310+S311)+\n(R311*S312-R312*S311)*(S311+S312)+\n(R312*S313-R313*S312)*(S312+S313)+\n(R313*S314-R314*S313)*(S313+S314)+\n(R314*S315-R315*S314)*(S314+S315)+\n(R315*S316-R316*S315)*(S315+S316)+\n(R316*S317-R317*S316)*(S316+S317)+\n(R317*S318-R318*S317)*(S317+S318)+\n(R318*S319-R319*S318)*(S318+S319))/6/S323)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(U323=0,0,-((T300*U301-T301*U300)*(U300+U301)+(T301*U302-T302*U301)*(U301+U302)+\n(T302*U303-T303*U302)*(U302+U303)+\n(T303*U304-T304*U303)*(U303+U304)+\n(T304*U305-T305*U304)*(U304+U305)+\n(T305*U306-T306*U305)*(U305+U306)+\n(T306*U307-T307*U306)*(U306+U307)+\n(T307*U308-T308*U307)*(U307+U308)+\n(T308*U309-T309*U308)*(U308+U309)+\n(T309*U310-T310*U309)*(U309+U310)+\n(T310*U311-T311*U310)*(U310+U311)+\n(T311*U312-T312*U311)*(U311+U312)+\n(T312*U313-T313*U312)*(U312+U313)+\n(T313*U314-T314*U313)*(U313+U314)+\n(T314*U315-T315*U314)*(U314+U315)+\n(T315*U316-T316*U315)*(U315+U316)+\n(T316*U317-T317*U316)*(U316+U317)+\n(T317*U318-T318*U317)*(U317+U318)+\n(T318*U319-T319*U318)*(U318+U319))/6/U323)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(W323=0,0,-((V300*W301-V301*W300)*(W300+W301)+(V301*W302-V302*W301)*(W301+W302)+\n(V302*W303-V303*W302)*(W302+W303)+\n(V303*W304-V304*W303)*(W303+W304)+\n(V304*W305-V305*W304)*(W304+W305)+\n(V305*W306-V306*W305)*(W305+W306)+\n(V306*W307-V307*W306)*(W306+W307)+\n(V307*W308-V308*W307)*(W307+W308)+\n(V308*W309-V309*W308)*(W308+W309)+\n(V309*W310-V310*W309)*(W309+W310)+\n(V310*W311-V311*W310)*(W310+W311)+\n(V311*W312-V312*W311)*(W311+W312)+\n(V312*W313-V313*W312)*(W312+W313)+\n(V313*W314-V314*W313)*(W313+W314)+\n(V314*W315-V315*W314)*(W314+W315)+\n(V315*W316-V316*W315)*(W315+W316)+\n(V316*W317-V317*W316)*(W316+W317)+\n(V317*W318-V318*W317)*(W317+W318)+\n(V318*W319-V319*W318)*(W318+W319))/6/W323)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Y323=0,0,-((X300*Y301-X301*Y300)*(Y300+Y301)+(X301*Y302-X302*Y301)*(Y301+Y302)+\n(X302*Y303-X303*Y302)*(Y302+Y303)+\n(X303*Y304-X304*Y303)*(Y303+Y304)+\n(X304*Y305-X305*Y304)*(Y304+Y305)+\n(X305*Y306-X306*Y305)*(Y305+Y306)+\n(X306*Y307-X307*Y306)*(Y306+Y307)+\n(X307*Y308-X308*Y307)*(Y307+Y308)+\n(X308*Y309-X309*Y308)*(Y308+Y309)+\n(X309*Y310-X310*Y309)*(Y309+Y310)+\n(X310*Y311-X311*Y310)*(Y310+Y311)+\n(X311*Y312-X312*Y311)*(Y311+Y312)+\n(X312*Y313-X313*Y312)*(Y312+Y313)+\n(X313*Y314-X314*Y313)*(Y313+Y314)+\n(X314*Y315-X315*Y314)*(Y314+Y315)+\n(X315*Y316-X316*Y315)*(Y315+Y316)+\n(X316*Y317-X317*Y316)*(Y316+Y317)+\n(X317*Y318-X318*Y317)*(Y317+Y318)+\n(X318*Y319-X319*Y318)*(Y318+Y319))/6/Y323)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AA323=0,0,-((Z300*AA301-Z301*AA300)*(AA300+AA301)+(Z301*AA302-Z302*AA301)*(AA301+AA302)+\n(Z302*AA303-Z303*AA302)*(AA302+AA303)+\n(Z303*AA304-Z304*AA303)*(AA303+AA304)+\n(Z304*AA305-Z305*AA304)*(AA304+AA305)+\n(Z305*AA306-Z306*AA305)*(AA305+AA306)+\n(Z306*AA307-Z307*AA306)*(AA306+AA307)+\n(Z307*AA308-Z308*AA307)*(AA307+AA308)+\n(Z308*AA309-Z309*AA308)*(AA308+AA309)+\n(Z309*AA310-Z310*AA309)*(AA309+AA310)+\n(Z310*AA311-Z311*AA310)*(AA310+AA311)+\n(Z311*AA312-Z312*AA311)*(AA311+AA312)+\n(Z312*AA313-Z313*AA312)*(AA312+AA313)+\n(Z313*AA314-Z314*AA313)*(AA313+AA314)+\n(Z314*AA315-Z315*AA314)*(AA314+AA315)+\n(Z315*AA316-Z316*AA315)*(AA315+AA316)+\n(Z316*AA317-Z317*AA316)*(AA316+AA317)+\n(Z317*AA318-Z318*AA317)*(AA317+AA318)+\n(Z318*AA319-Z319*AA318)*(AA318+AA319))/6/AA323)","v":0},"y=",{"$f":"+IF(AC323=0,0,-((AB300*AC301-AB301*AC300)*(AC300+AC301)+(AB301*AC302-AB302*AC301)*(AC301+AC302)+\n(AB302*AC303-AB303*AC302)*(AC302+AC303)+\n(AB303*AC304-AB304*AC303)*(AC303+AC304)+\n(AB304*AC305-AB305*AC304)*(AC304+AC305)+\n(AB305*AC306-AB306*AC305)*(AC305+AC306)+\n(AB306*AC307-AB307*AC306)*(AC306+AC307)+\n(AB307*AC308-AB308*AC307)*(AC307+AC308)+\n(AB308*AC309-AB309*AC308)*(AC308+AC309)+\n(AB309*AC310-AB310*AC309)*(AC309+AC310)+\n(AB310*AC311-AB311*AC310)*(AC310+AC311)+\n(AB311*AC312-AB312*AC311)*(AC311+AC312)+\n(AB312*AC313-AB313*AC312)*(AC312+AC313)+\n(AB313*AC314-AB314*AC313)*(AC313+AC314)+\n(AB314*AC315-AB315*AC314)*(AC314+AC315)+\n(AB315*AC316-AB316*AC315)*(AC315+AC316)+\n(AB316*AC317-AB317*AC316)*(AC316+AC317)+\n(AB317*AC318-AB318*AC317)*(AC317+AC318)+\n(AB318*AC319-AB319*AC318)*(AC318+AC319))/6/AC323)","v":0},"y=",{"$f":"+IF(AE323=0,0,-((AD300*AE301-AD301*AE300)*(AE300+AE301)+(AD301*AE302-AD302*AE301)*(AE301+AE302)+\n(AD302*AE303-AD303*AE302)*(AE302+AE303)+\n(AD303*AE304-AD304*AE303)*(AE303+AE304)+\n(AD304*AE305-AD305*AE304)*(AE304+AE305)+\n(AD305*AE306-AD306*AE305)*(AE305+AE306)+\n(AD306*AE307-AD307*AE306)*(AE306+AE307)+\n(AD307*AE308-AD308*AE307)*(AE307+AE308)+\n(AD308*AE309-AD309*AE308)*(AE308+AE309)+\n(AD309*AE310-AD310*AE309)*(AE309+AE310)+\n(AD310*AE311-AD311*AE310)*(AE310+AE311)+\n(AD311*AE312-AD312*AE311)*(AE311+AE312)+\n(AD312*AE313-AD313*AE312)*(AE312+AE313)+\n(AD313*AE314-AD314*AE313)*(AE313+AE314)+\n(AD314*AE315-AD315*AE314)*(AE314+AE315)+\n(AD315*AE316-AD316*AE315)*(AE315+AE316)+\n(AD316*AE317-AD317*AE316)*(AE316+AE317)+\n(AD317*AE318-AD318*AE317)*(AE317+AE318)+\n(AD318*AE319-AD319*AE318)*(AE318+AE319))/6/AE323)","v":0},"y=",{"$f":"+IF(AG323=0,0,-((AF300*AG301-AF301*AG300)*(AG300+AG301)+(AF301*AG302-AF302*AG301)*(AG301+AG302)+\n(AF302*AG303-AF303*AG302)*(AG302+AG303)+\n(AF303*AG304-AF304*AG303)*(AG303+AG304)+\n(AF304*AG305-AF305*AG304)*(AG304+AG305)+\n(AF305*AG306-AF306*AG305)*(AG305+AG306)+\n(AF306*AG307-AF307*AG306)*(AG306+AG307)+\n(AF307*AG308-AF308*AG307)*(AG307+AG308)+\n(AF308*AG309-AF309*AG308)*(AG308+AG309)+\n(AF309*AG310-AF310*AG309)*(AG309+AG310)+\n(AF310*AG311-AF311*AG310)*(AG310+AG311)+\n(AF311*AG312-AF312*AG311)*(AG311+AG312)+\n(AF312*AG313-AF313*AG312)*(AG312+AG313)+\n(AF313*AG314-AF314*AG313)*(AG313+AG314)+\n(AF314*AG315-AF315*AG314)*(AG314+AG315)+\n(AF315*AG316-AF316*AG315)*(AG315+AG316)+\n(AF316*AG317-AF317*AG316)*(AG316+AG317)+\n(AF317*AG318-AF318*AG317)*(AG317+AG318)+\n(AF318*AG319-AF319*AG318)*(AG318+AG319))/6/AG323)","v":0},"y=",{"$f":"+IF(AI323=0,0,-((AH300*AI301-AH301*AI300)*(AI300+AI301)+(AH301*AI302-AH302*AI301)*(AI301+AI302)+\n(AH302*AI303-AH303*AI302)*(AI302+AI303)+\n(AH303*AI304-AH304*AI303)*(AI303+AI304)+\n(AH304*AI305-AH305*AI304)*(AI304+AI305)+\n(AH305*AI306-AH306*AI305)*(AI305+AI306)+\n(AH306*AI307-AH307*AI306)*(AI306+AI307)+\n(AH307*AI308-AH308*AI307)*(AI307+AI308)+\n(AH308*AI309-AH309*AI308)*(AI308+AI309)+\n(AH309*AI310-AH310*AI309)*(AI309+AI310)+\n(AH310*AI311-AH311*AI310)*(AI310+AI311)+\n(AH311*AI312-AH312*AI311)*(AI311+AI312)+\n(AH312*AI313-AH313*AI312)*(AI312+AI313)+\n(AH313*AI314-AH314*AI313)*(AI313+AI314)+\n(AH314*AI315-AH315*AI314)*(AI314+AI315)+\n(AH315*AI316-AH316*AI315)*(AI315+AI316)+\n(AH316*AI317-AH317*AI316)*(AI316+AI317)+\n(AH317*AI318-AH318*AI317)*(AI317+AI318)+\n(AH318*AI319-AH319*AI318)*(AI318+AI319))/6/AI323)","v":0},"y=",{"$f":"+IF(AK323=0,0,-((AJ300*AK301-AJ301*AK300)*(AK300+AK301)+(AJ301*AK302-AJ302*AK301)*(AK301+AK302)+\n(AJ302*AK303-AJ303*AK302)*(AK302+AK303)+\n(AJ303*AK304-AJ304*AK303)*(AK303+AK304)+\n(AJ304*AK305-AJ305*AK304)*(AK304+AK305)+\n(AJ305*AK306-AJ306*AK305)*(AK305+AK306)+\n(AJ306*AK307-AJ307*AK306)*(AK306+AK307)+\n(AJ307*AK308-AJ308*AK307)*(AK307+AK308)+\n(AJ308*AK309-AJ309*AK308)*(AK308+AK309)+\n(AJ309*AK310-AJ310*AK309)*(AK309+AK310)+\n(AJ310*AK311-AJ311*AK310)*(AK310+AK311)+\n(AJ311*AK312-AJ312*AK311)*(AK311+AK312)+\n(AJ312*AK313-AJ313*AK312)*(AK312+AK313)+\n(AJ313*AK314-AJ314*AK313)*(AK313+AK314)+\n(AJ314*AK315-AJ315*AK314)*(AK314+AK315)+\n(AJ315*AK316-AJ316*AK315)*(AK315+AK316)+\n(AJ316*AK317-AJ317*AK316)*(AK316+AK317)+\n(AJ317*AK318-AJ318*AK317)*(AK317+AK318)+\n(AJ318*AK319-AJ319*AK318)*(AK318+AK319))/6/AK323)","v":0},0,null,null,null,null,null,null,null,null,4.08,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$62","v":4.4000000000000004}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.76,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$61","v":4.08}]
[null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.44,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$60","v":3.76}]
[null,"OPTEREĆENJE TEMELJEM",null,null,null,null,null,null,null," (TERZAGHY)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.14,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$59","v":3.44}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.14,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$58","v":3.14}]
[null,"KONTINUIRANO OPTEREĆENJE",null,"P - D=",{"$f":"IF('Analiza i dimenzioniranje'!$E$28-I330<=0,0,+'Analiza i dimenzioniranje'!$E$28-I330)","v":{"$error":"#VALUE!"}},"kN/m2","raster. iskopom   D=y*Df =",null,{"$f":"+'Analiza i dimenzioniranje'!$D$16*('Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20-D336)","v":{"$error":"#VALUE!"}},"kN/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$57","v":2.8}]
[null," visina zida i temelja",null,"H =",{"$f":"+E$291","v":{"$error":"#VALUE!"}},"m",{"$f":"E335","v":6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$56","v":2.48}]
[null,"visina opterećenja iznad vrha zida",null,"h =",{"$f":"+E292","v":-1},"m",{"$f":"SQRT(E335^2+E334^2)","v":6.7082039324993694},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$55","v":2.16}]
[null,"širina temelja",null,"b =",{"$f":"+E293","v":1},"m   ",{"$f":"E334+E333","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$54","v":1.84}]
[null,"udaljenost temelja od zida",null,"D =",{"$f":"+E294","v":3},"m    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$53","v":1.52}]
[null,"1/2 dužine temelja",null,"L/2=a=",{"$f":"+E295","v":6},"m",{"$f":"SQRT(G331^2+G333^2)","v":7.2111025509279782},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,0,{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
["DNO TEMELJA NA VISINI","PRESJEK NA Visini ",null,{"$f":"ROUND('Analiza i dimenzioniranje'!$U$61,2)","v":4.08},null,"Presjek III -III",null,"Presjek VI",null,"Presjek VII-VII",null,"Presjek VIII-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"Presjek XIV-XIV",null,"Presjek XV-XV",null,"PresjekXVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX",null,null,null,null,null,null,null,null,null,null,4.08,{"$f":"+IF(AW337>=AW$299,0,AQ198-AW198)","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
[null,null,null,null,null,"(sb2-sb1)*2","Visina djelovanja i terena","(sb2-sb1)*2","Visina djelovanja i terena","sb1-sb2","Visina djelovanja i terena","sb1-sb2","Visina djelovanja i terena","sb1-sb2","Visina djelovanja i terena","(sb2-sb1)*2","Visina djelovanja i terena","sb1-sb2","Visina djelovanja i terena","(sb2-sb1)*2","Visina djelovanja i terena","sb1-sb2","Visina djelovanja i terena","(sb2-sb1)*2","Visina djelovanja i terena","sb1-sb2","Visina djelovanja i terena","(sb2-sb1)*2","Visina djelovanja i terena","sb1-sb2","Visina djelovanja i terena","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja i terena"]
[null,null,null,{"$f":"+F339","v":0},{"$f":"+D338-E336","v":0},"III",{"$f":"+D336","v":4.08},"VI",{"$f":"+G338","v":4.08},"VII",{"$f":"+G338","v":4.08},"VIII",{"$f":"+D336","v":4.08},"IX",{"$f":"+G338","v":4.08},"y=",{"$f":"+O338","v":4.08},"XI",{"$f":"+K338","v":4.08},"XII",{"$f":"+M338","v":4.08},"XIII",{"$f":"+G338","v":4.08},"XIV",{"$f":"+Q338","v":4.08},"XV",{"$f":"+G338","v":4.08},"XVI",{"$f":"+U338","v":4.08},"XVII",{"$f":"+W338","v":4.08},"XVIII",{"$f":"+AE338","v":4.08},"XIX",{"$f":"+'Analiza i dimenzioniranje'!U93","v":0},"XX",{"$f":"+D336","v":4.08},null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
[null,null,null,0,{"$f":"IF(D338>E$296,D338,E$296)","v":0}]
[0,null,null,0,{"$f":"IF(AW319>G$298,0,AW319)","v":0},0,0,0,{"$f":"+G340","v":0},0]
[{"$f":"+AL142","v":0},null,null,0,{"$f":"+AW320","v":5.6800000000000006},0,0,0,{"$f":"+G341","v":0},0,0,0,{"$f":"+E340","v":0},0,0,{"$f":"+N341","v":0},{"$f":"+O341","v":0},0,0,{"$f":"+R341","v":0},{"$f":"+S341","v":0},0,{"$f":"+AS341","v":0},{"$f":"+V341","v":0},0,0,{"$f":"+S341","v":0},{"$f":"+X341","v":0},{"$f":"+AA341","v":0},0,{"$f":"+AU318","v":0},0,{"$f":"+AU318","v":0},0,{"$f":"+AG341","v":0},{"$f":"+AD341","v":0},{"$f":"+AG341","v":0}]
[0,null,null,0,{"$f":"IF(AW321>G$298,0,AW321)","v":0},{"$f":"+D178","v":0},0,0,0,0,0,0,5.6800000000000006,0,0,{"$f":"+N342","v":0},0,0,0,{"$f":"+R342","v":0},{"$f":"+T342","v":0},0,0,0,0,0,0,{"$f":"+X342","v":0},{"$f":"+AA342","v":0},{"$f":"+Z342","v":0},0,{"$f":"+AD342","v":0},0,{"$f":"+AF342","v":0},{"$f":"+AG342","v":0},{"$f":"+AD342","v":0},{"$f":"+AG342","v":0}]
[0,null,null,{"$f":"+AV319","v":0},0,0,0,0,0,{"$f":"+F341","v":0},0,{"$f":"+D340","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+Z343","v":0},0,{"$f":"+AD343","v":0},0,{"$f":"+AF343","v":0},0,0,0]
[0,null,null,{"$f":"+AV320","v":0},0,0,0,0,0,{"$f":"+F342","v":0},0,{"$f":"+D341","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,null,null,{"$f":"+AV321","v":{"$error":"#VALUE!"}},0,0,0,0,0,0,0,{"$f":"+D342","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,null,null,{"$f":"+AV322","v":{"$error":"#VALUE!"}},4.4000000000000004,0,0,0,0,0,0,{"$f":"+E180","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,null,null,null,4.08,0,0,0,0,0,0,{"$f":"+D344","v":0},4.4000000000000004,{"$f":"+J345","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,null,null,{"$f":"+D307","v":0},3.76,0,{"$f":"+AW326","v":4.08},0,{"$f":"+G348","v":4.08},0,{"$f":"+E347","v":4.08},0,{"$f":"+E347","v":4.08},{"$f":"+J346","v":0},{"$f":"+M348","v":4.08},{"$f":"+N348","v":0},{"$f":"+O348","v":4.08},0,{"$f":"+Q348","v":4.08},{"$f":"+R348","v":0},{"$f":"+S348","v":4.08},0,{"$f":"+U348","v":4.08},0,{"$f":"+AU325","v":4.08},0,{"$f":"+W348","v":4.08},0,{"$f":"+AA348","v":4.08},0,4.08,0,4.08,0,4.08,0,4.08,null,{"$f":"+D348","v":0},{"$f":"$E$334^2+AM348^2","v":9},{"$f":"$G$333^2+AM348^2","v":16},{"$f":"$G$335^2+AM348^2","v":51.999999999999993},{"$f":"IF(AM348=0,0,$E$330/(PI())*(ATAN(($E$335*$G$333)/(AM348*SQRT(AP348)))-$E$335*$G$333*AM348/(AO348*SQRT(AP348))))","v":0},null,{"$f":"+AM348","v":0},{"$f":"$E$335^2+AS348^2","v":36},{"$f":"$E$334^2+AS348^2","v":9},{"$f":"$G$332^2+AS348^2","v":45.000000000000007},{"$f":"IF(AS348=0,0,($E$330/(PI()))*(ATAN(($E$335*$E$334)/(AS348*SQRT(AV348)))-$E$335*$E$334*AS348/(AU348*SQRT(AV348))))","v":0},{"$f":"+AQ348-AW348","v":0}]
[0,null,null,0.32,3.44,{"$f":"+AX349","v":{"$error":"#VALUE!"}},3.76,{"$f":"+F349","v":{"$error":"#VALUE!"}},{"$f":"+G349","v":3.76},{"$f":"+F349","v":{"$error":"#VALUE!"}},3.76,{"$f":"+H349","v":{"$error":"#VALUE!"}},3.76,{"$f":"+L349","v":{"$error":"#VALUE!"}},3.76,{"$f":"+N349","v":{"$error":"#VALUE!"}},{"$f":"+O349","v":3.76},{"$f":"+P349","v":{"$error":"#VALUE!"}},{"$f":"+M349","v":3.76},{"$f":"+R349","v":{"$error":"#VALUE!"}},{"$f":"+S349","v":3.76},{"$f":"+T349","v":{"$error":"#VALUE!"}},{"$f":"+U349","v":3.76},0,{"$f":"+Y348","v":4.08},0,{"$f":"+S349","v":3.76},0,0,0,3.76,0,3.76,0,3.76,0,3.76,null,0.32,{"$f":"$E$334^2+AM349^2","v":9.1023999999999994},{"$f":"$G$333^2+AM349^2","v":16.102399999999999},{"$f":"$G$335^2+AM349^2","v":52.102399999999996},{"$f":"IF(AM349=0,0,$E$330/(PI())*(ATAN(($E$335*$G$333)/(AM349*SQRT(AP349)))-$E$335*$G$333*AM349/(AO349*SQRT(AP349))))","v":{"$error":"#VALUE!"}},null,{"$f":"+AM349","v":0.32},{"$f":"$E$335^2+AS349^2","v":36.102400000000003},{"$f":"$E$334^2+AS349^2","v":9.1023999999999994},{"$f":"$G$332^2+AS349^2","v":45.10240000000001},{"$f":"IF(AS349=0,0,($E$330/(PI()))*(ATAN(($E$335*$E$334)/(AS349*SQRT(AV349)))-$E$335*$E$334*AS349/(AU349*SQRT(AV349))))","v":{"$error":"#VALUE!"}},{"$f":"+(AQ349-AW349)*2","v":{"$error":"#VALUE!"}}]
[0,null,null,0.64,3.14,{"$error":"#VALUE!"},3.44,{"$error":"#VALUE!"},3.44,{"$error":"#VALUE!"},3.44,{"$error":"#VALUE!"},3.44,{"$f":"+J350","v":{"$error":"#VALUE!"}},3.44,{"$error":"#VALUE!"},3.44,{"$f":"+N350","v":{"$error":"#VALUE!"}},{"$f":"+M350","v":3.44},{"$f":"+R350","v":{"$error":"#VALUE!"}},{"$f":"+Q350","v":3.44},0,{"$f":"+W349","v":3.76},0,0,0,3.44,0,0,0,3.44,0,3.44,0,3.44,0,3.44,null,0.64,{"$f":"$E$334^2+AM350^2","v":9.4095999999999993},{"$f":"$G$333^2+AM350^2","v":16.409600000000001},{"$f":"$G$335^2+AM350^2","v":52.40959999999999},{"$f":"IF(AM350=0,0,$E$330/(PI())*(ATAN(($E$335*$G$333)/(AM350*SQRT(AP350)))-$E$335*$G$333*AM350/(AO350*SQRT(AP350))))","v":{"$error":"#VALUE!"}},null,{"$f":"+AM350","v":0.64},{"$f":"$E$335^2+AS350^2","v":36.409599999999998},{"$f":"$E$334^2+AS350^2","v":9.4095999999999993},{"$f":"$G$332^2+AS350^2","v":45.409600000000005},{"$f":"IF(AS350=0,0,($E$330/(PI()))*(ATAN(($E$335*$E$334)/(AS350*SQRT(AV350)))-$E$335*$E$334*AS350/(AU350*SQRT(AV350))))","v":{"$error":"#VALUE!"}},{"$f":"+(AQ350-AW350)*2","v":{"$error":"#VALUE!"}}]
[0,null,null,0.96,2.8,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.14,{"$f":"+J351","v":{"$error":"#VALUE!"}},3.14,{"$error":"#VALUE!"},3.14,{"$f":"+N351","v":{"$error":"#VALUE!"}},3.14,0,{"$f":"+U350","v":3.44},{"$f":"+N347","v":0},0,{"$f":"+T351","v":0},0,0,3.14,0,0,0,3.14,0,3.14,0,3.14,0,3.14,null,0.96,9.9215999999999998,16.921600000000002,52.921599999999991,{"$error":"#VALUE!"},null,0.96,36.921599999999998,9.9215999999999998,45.921600000000005,{"$f":"IF(AS351=0,0,($E$330/(PI()))*(ATAN(($E$335*$E$294)/(AS351*SQRT(AV351)))-$E$335*$E$334*AS351/(AU351*SQRT(AV351))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,1.28,2.48,{"$error":"#VALUE!"},2.8,{"$error":"#VALUE!"},2.8,{"$error":"#VALUE!"},2.8,{"$error":"#VALUE!"},2.8,{"$f":"+J352","v":{"$error":"#VALUE!"}},2.8,{"$error":"#VALUE!"},2.8,0,{"$f":"+S351","v":3.14},{"$f":"+R352","v":0},0,{"$f":"+N348","v":0},0,0,0,0,3.14,0,0,0,3.14,0,3.14,0,3.14,0,3.14,null,1.28,10.638400000000001,17.638400000000001,53.63839999999999,{"$error":"#VALUE!"},null,1.28,37.638399999999997,10.638400000000001,46.638400000000004,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,1.6,2.16,{"$error":"#VALUE!"},2.48,{"$error":"#VALUE!"},2.48,{"$error":"#VALUE!"},2.48,{"$error":"#VALUE!"},2.48,{"$f":"+J353","v":{"$error":"#VALUE!"}},2.48,0,{"$f":"+Q352","v":2.8},0,0,0,0,0,0,0,0,{"$f":"+V351","v":0},0,0,0,0,0,0,0,0,0,0,0,null,1.6,11.56,18.560000000000002,54.559999999999995,{"$error":"#VALUE!"},null,1.6,38.56,11.56,47.560000000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,1.9200000000000002,1.84,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},2.16,0,{"$f":"+O353","v":2.48},0,0,{"$f":"+N354","v":0},0,0,0,0,0,0,0,{"$f":"+V352","v":0},0,0,0,0,0,0,0,0,0,0,0,null,1.9200000000000002,12.686400000000001,19.686399999999999,55.686399999999992,{"$error":"#VALUE!"},null,1.9200000000000002,39.686399999999999,12.686400000000001,48.686400000000006,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,2.2400000000000002,1.52,{"$error":"#VALUE!"},1.84,{"$error":"#VALUE!"},1.84,{"$error":"#VALUE!"},1.84,0,{"$f":"+M354","v":2.16},0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+V353","v":0},0,0,0,0,0,0,0,0,0,0,0,null,2.2400000000000002,14.017600000000002,21.017600000000002,57.017599999999995,{"$error":"#VALUE!"},null,2.2400000000000002,41.017600000000002,14.017600000000002,50.017600000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,2.56,1.2,{"$error":"#VALUE!"},1.52,{"$error":"#VALUE!"},1.52,0,{"$f":"+K355","v":1.84},0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+V354","v":0},0,0,0,0,{"$f":"+AE355","v":0},0,0,0,0,0,0,null,2.56,15.553599999999999,22.553599999999999,58.553599999999996,{"$error":"#VALUE!"},null,2.56,42.553600000000003,15.553599999999999,51.55360000000001,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,2.88,{"$f":"+AW336","v":1.2},{"$error":"#VALUE!"},1.2,0,{"$f":"+I356","v":1.52},0,0,0,2,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+V355","v":0},0,0,0,0,{"$f":"+AU334","v":0},0,0,0,0,0,0,null,2.88,17.2944,24.2944,60.294399999999996,{"$error":"#VALUE!"},null,2.88,44.294399999999996,17.2944,53.29440000000001,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,0,{"$f":"+AW337","v":0},0,{"$f":"+E357","v":1.2},{"$f":"+F358","v":0},{"$f":"+G358","v":1.2},0,{"$f":"+M358","v":1.2},0,{"$f":"+E357","v":1.2},0,{"$f":"+M358","v":1.2},0,{"$f":"+O358","v":1.2},0,{"$f":"+Q358","v":1.2},0,{"$f":"+S358","v":1.2},0,{"$f":"+U358","v":1.2},0,{"$f":"+W358","v":1.2},0,{"$f":"+Y358","v":1.2},0,{"$f":"+AA358","v":1.2},0,{"$f":"+AC358","v":1.2},0,1.2,0,{"$f":"+AG358","v":1.2},{"$f":"+AD358","v":0},1.2,null,null,0,{"$f":"+M358","v":1.2},0,{"$f":"+AQ357","v":{"$error":"#VALUE!"}},0,{"$f":"+AO358","v":1.2},0,{"$f":"+S381","v":0},{"$f":"AQ218-AW218","v":0},{"$f":"IF(AV356>AW$299,AV356,AW$299)","v":51.55360000000001}]
[null,null,null,"SQhi=",{"$f":"+E362","v":0},{"$f":"+AV335","v":0},{"$f":"+G348","v":4.08},{"$f":"+F359","v":0},{"$f":"+G359","v":4.08},0,{"$f":"+M348","v":4.08},0,{"$f":"+M348","v":4.08},0,{"$f":"+M359","v":4.08},0,{"$f":"+O359","v":4.08},0,{"$f":"+Q359","v":4.08},0,{"$f":"+S359","v":4.08},0,{"$f":"+U359","v":4.08},0,{"$f":"+W359","v":4.08},0,{"$f":"+Y359","v":4.08},0,{"$f":"+AA359","v":4.08},0,{"$f":"+AC359","v":4.08},0,4.08,0,{"$f":"+AG359","v":4.08},{"$f":"+AD359","v":0},4.08,null,null,1,4.08,1,{"$f":"+AQ358","v":{"$error":"#VALUE!"}},1,{"$f":"+AO359","v":4.08},1,0,{"$error":"#VALUE!"},{"$f":"+AW360","v":6.0000000000000009}]
[null,null,null,"Ukupni pritisak",null,"SQhi=",{"$f":"+G363","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I363","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K363","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+M363","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+O363","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Q363","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+S363","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+U363","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+W363","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Y363","v":0},"SQhi=",{"$f":"+AA363","v":0},"SQhi=",{"$f":"+AC363","v":0},"SQhi=",{"$f":"+AE363","v":0},"SQhi=",{"$f":"+AG363","v":0},"SQhi=",{"$f":"+AI363","v":0},"SQhi=",{"$f":"+AK363","v":0},null,null,2,{"$error":"#VALUE!"},2,{"$error":"#VALUE!"},2,{"$error":"#VALUE!"},2,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$67","v":6.0000000000000009}]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G365","v":{"$error":"#VALUE!"}}," y=",{"$f":"+I365","v":{"$error":"#VALUE!"}}," y=",{"$f":"+K365","v":{"$error":"#VALUE!"}}," y=",{"$f":"+M365","v":{"$error":"#VALUE!"}}," y=",{"$f":"+O365","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Q365","v":{"$error":"#VALUE!"}}," y=",{"$f":"+S365","v":{"$error":"#VALUE!"}}," y=",{"$f":"+U365","v":{"$error":"#VALUE!"}}," y=",{"$f":"+W365","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Y365","v":0}," y=",{"$f":"+AA365","v":0}," y=",{"$f":"+AC365","v":0}," y=",{"$f":"+AE365","v":0}," y=",{"$f":"+AG365","v":0}," y=",{"$f":"+AI365","v":0}," y=",{"$f":"+AK365","v":0},null,null,3,{"$error":"#VALUE!"},3,{"$error":"#VALUE!"},3,{"$error":"#VALUE!"},3,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$66","v":5.6800000000000006}]
[null,null,null,"krak za presjek III -III",null,"z=",{"$f":"+G361-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I361-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K361-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M361-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+O361-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Q361-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+S361-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+U361-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}},"z=",{"$f":"+W361-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Y361-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AA361-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AC361-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AE361-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AG361-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AI361-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AK361-'Analiza i dimenzioniranje'!$E$52","v":-1.2},null,null,4,{"$error":"#VALUE!"},4,{"$error":"#VALUE!"},4,{"$error":"#VALUE!"},4,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$65","v":5.36}]
[null,null,null,"x=",0,"F=",{"$f":"-0.5*((F340*G341-F341*G340)+(F341*G342-F342*G341)+\n (F342*G343-F343*G342)+\n(F343*G344-F344*G343)+\n(F344*G345-F345*G344)+\n(F345*G346-F346*G345)+\n(F346*G347-F347*G346)+\n(F347*G348-F348*G347)+\n(F348*G349-F349*G348)+\n(F349*G350-F350*G349)+\n(F350*G351-F351*G350)+\n(F351*G352-F352*G351)+\n(F352*G353-F353*G352)+\n(F353*G354-F354*G353)+\n(F354*G355-F355*G354)+\n(F355*G356-F356*G355)+\n(F356*G357-F357*G356)+\n(F357*G358-F358*G357)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((H340*I341-H341*I340)+(H341*I342-H342*I341)+\n (H342*I343-H343*I342)+\n(H343*I344-H344*I343)+\n(H344*I345-H345*I344)+\n(H345*I346-H346*I345)+\n(H346*I347-H347*I346)+\n(H347*I348-H348*I347)+\n(H348*I349-H349*I348)+\n(H349*I350-H350*I349)+\n(H350*I351-H351*I350)+\n(H351*I352-H352*I351)+\n(H352*I353-H353*I352)+\n(H353*I354-H354*I353)+\n(H354*I355-H355*I354)+\n(H355*I356-H356*I355)+\n(H356*I357-H357*I356)+\n(H357*I358-H358*I357)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((J340*K341-J341*K340)+(J341*K342-J342*K341)+\n (J342*K343-J343*K342)+\n(J343*K344-J344*K343)+\n(J344*K345-J345*K344)+\n(J345*K346-J346*K345)+\n(J346*K347-J347*K346)+\n(J347*K348-J348*K347)+\n(J348*K349-J349*K348)+\n(J349*K350-J350*K349)+\n(J350*K351-J351*K350)+\n(J351*K352-J352*K351)+\n(J352*K353-J353*K352)+\n(J353*K354-J354*K353)+\n(J354*K355-J355*K354)+\n(J355*K356-J356*K355)+\n(J356*K357-J357*K356)+\n(J357*K358-J358*K357)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((L340*M341-L341*M340)+(L341*M342-L342*M341)+\n (L342*M343-L343*M342)+\n(L343*M344-L344*M343)+\n(L344*M345-L345*M344)+\n(L345*M346-L346*M345)+\n(L346*M347-L347*M346)+\n(L347*M348-L348*M347)+\n(L348*M349-L349*M348)+\n(L349*M350-L350*M349)+\n(L350*M351-L351*M350)+\n(L351*M352-L352*M351)+\n(L352*M353-L353*M352)+\n(L353*M354-L354*M353)+\n(L354*M355-L355*M354)+\n(L355*M356-L356*M355)+\n(L356*M357-L357*M356)+\n(L357*M358-L358*M357)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((N340*O341-N341*O340)+(N341*O342-N342*O341)+\n (N342*O343-N343*O342)+\n(N343*O344-N344*O343)+\n(N344*O345-N345*O344)+\n(N345*O346-N346*O345)+\n(N346*O347-N347*O346)+\n(N347*O348-N348*O347)+\n(N348*O349-N349*O348)+\n(N349*O350-N350*O349)+\n(N350*O351-N351*O350)+\n(N351*O352-N352*O351)+\n(N352*O353-N353*O352)+\n(N353*O354-N354*O353)+\n(N354*O355-N355*O354)+\n(N355*O356-N356*O355)+\n(N356*O357-N357*O356)+\n(N357*O358-N358*O357)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((P340*Q341-P341*Q340)+(P341*Q342-P342*Q341)+\n (P342*Q343-P343*Q342)+\n(P343*Q344-P344*Q343)+\n(P344*Q345-P345*Q344)+\n(P345*Q346-P346*Q345)+\n(P346*Q347-P347*Q346)+\n(P347*Q348-P348*Q347)+\n(P348*Q349-P349*Q348)+\n(P349*Q350-P350*Q349)+\n(P350*Q351-P351*Q350)+\n(P351*Q352-P352*Q351)+\n(P352*Q353-P353*Q352)+\n(P353*Q354-P354*Q353)+\n(P354*Q355-P355*Q354)+\n(P355*Q356-P356*Q355)+\n(P356*Q357-P357*Q356)+\n(P357*Q358-P358*Q357)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((R340*S341-R341*S340)+(R341*S342-R342*S341)+\n (R342*S343-R343*S342)+\n(R343*S344-R344*S343)+\n(R344*S345-R345*S344)+\n(R345*S346-R346*S345)+\n(R346*S347-R347*S346)+\n(R347*S348-R348*S347)+\n(R348*S349-R349*S348)+\n(R349*S350-R350*S349)+\n(R350*S351-R351*S350)+\n(R351*S352-R352*S351)+\n(R352*S353-R353*S352)+\n(R353*S354-R354*S353)+\n(R354*S355-R355*S354)+\n(R355*S356-R356*S355)+\n(R356*S357-R357*S356)+\n(R357*S358-R358*S357)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((T340*U341-T341*U340)+(T341*U342-T342*U341)+\n (T342*U343-T343*U342)+\n(T343*U344-T344*U343)+\n(T344*U345-T345*U344)+\n(T345*U346-T346*U345)+\n(T346*U347-T347*U346)+\n(T347*U348-T348*U347)+\n(T348*U349-T349*U348)+\n(T349*U350-T350*U349)+\n(T350*U351-T351*U350)+\n(T351*U352-T352*U351)+\n(T352*U353-T353*U352)+\n(T353*U354-T354*U353)+\n(T354*U355-T355*U354)+\n(T355*U356-T356*U355)+\n(T356*U357-T357*U356)+\n(T357*U358-T358*U357)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (V342*W343-V343*W342)+\n(V343*W344-V344*W343)+\n(V344*W345-V345*W344)+\n(V345*W346-V346*W345)+\n(V346*W347-V347*W346)+\n(V347*W348-V348*W347)+\n(V348*W349-V349*W348)+\n(V349*W350-V350*W349)+\n(V350*W351-V351*W350)+\n(V351*W352-V352*W351)+\n(V352*W353-V353*W352)+\n(V353*W354-V354*W353)+\n(V354*W355-V355*W354)+\n(V355*W356-V356*W355)+\n(V356*W357-V357*W356)+\n(V357*W358-V358*W357)+\n(V358*W359-V359*W358))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (X342*Y343-X343*Y342)+\n(X343*Y344-X344*Y343)+\n(X344*Y345-X345*Y344)+\n(X345*Y346-X346*Y345)+\n(X346*Y347-X347*Y346)+\n(X347*Y348-X348*Y347)+\n(X348*Y349-X349*Y348)+\n(X349*Y350-X350*Y349)+\n(X350*Y351-X351*Y350)+\n(X351*Y352-X352*Y351)+\n(X352*Y353-X353*Y352)+\n(X353*Y354-X354*Y353)+\n(X354*Y355-X355*Y354)+\n(X355*Y356-X356*Y355)+\n(X356*Y357-X357*Y356)+\n(X357*Y358-X358*Y357)+\n(X358*Y359-X359*Y358))","v":0},"F=",{"$f":"-0.5*(+\n (Z342*AA343-Z343*AA342)+\n(Z343*AA344-Z344*AA343)+\n(Z344*AA345-Z345*AA344)+\n(Z345*AA346-Z346*AA345)+\n(Z346*AA347-Z347*AA346)+\n(Z347*AA348-Z348*AA347)+\n(Z348*AA349-Z349*AA348)+\n(Z349*AA350-Z350*AA349)+\n(Z350*AA351-Z351*AA350)+\n(Z351*AA352-Z352*AA351)+\n(Z352*AA353-Z353*AA352)+\n(Z353*AA354-Z354*AA353)+\n(Z354*AA355-Z355*AA354)+\n(Z355*AA356-Z356*AA355)+\n(Z356*AA357-Z357*AA356)+\n(Z357*AA358-Z358*AA357)+\n(Z358*AA359-Z359*AA358))","v":0},"F=",{"$f":"-0.5*(+\n (AB342*AC343-AB343*AC342)+\n(AB343*AC344-AB344*AC343)+\n(AB344*AC345-AB345*AC344)+\n(AB345*AC346-AB346*AC345)+\n(AB346*AC347-AB347*AC346)+\n(AB347*AC348-AB348*AC347)+\n(AB348*AC349-AB349*AC348)+\n(AB349*AC350-AB350*AC349)+\n(AB350*AC351-AB351*AC350)+\n(AB351*AC352-AB352*AC351)+\n(AB352*AC353-AB353*AC352)+\n(AB353*AC354-AB354*AC353)+\n(AB354*AC355-AB355*AC354)+\n(AB355*AC356-AB356*AC355)+\n(AB356*AC357-AB357*AC356)+\n(AB357*AC358-AB358*AC357)+\n(AB358*AC359-AB359*AC358))","v":0},"F=",{"$f":"-0.5*(+\n (AD342*AE343-AD343*AE342)+\n(AD343*AE344-AD344*AE343)+\n(AD344*AE345-AD345*AE344)+\n(AD345*AE346-AD346*AE345)+\n(AD346*AE347-AD347*AE346)+\n(AD347*AE348-AD348*AE347)+\n(AD348*AE349-AD349*AE348)+\n(AD349*AE350-AD350*AE349)+\n(AD350*AE351-AD351*AE350)+\n(AD351*AE352-AD352*AE351)+\n(AD352*AE353-AD353*AE352)+\n(AD353*AE354-AD354*AE353)+\n(AD354*AE355-AD355*AE354)+\n(AD355*AE356-AD356*AE355)+\n(AD356*AE357-AD357*AE356)+\n(AD357*AE358-AD358*AE357)+\n(AD358*AE359-AD359*AE358))","v":0},"F=",{"$f":"-0.5*((AF340*AG341-AF341*AG340)+(AF341*AG342-AF342*AG341)+\n (AF342*AG343-AF343*AG342)+\n(AF343*AG344-AF344*AG343)+\n(AF344*AG345-AF345*AG344)+\n(AF345*AG346-AF346*AG345)+\n(AF346*AG347-AF347*AG346)+\n(AF347*AG348-AF348*AG347)+\n(AF348*AG349-AF349*AG348)+\n(AF349*AG350-AF350*AG349)+\n(AF350*AG351-AF351*AG350)+\n(AF351*AG352-AF352*AG351)+\n(AF352*AG353-AF353*AG352)+\n(AF353*AG354-AF354*AG353)+\n(AF354*AG355-AF355*AG354)+\n(AF355*AG356-AF356*AG355)+\n(AF356*AG357-AF357*AG356)+\n(AF357*AG358-AF358*AG357)\n)","v":0},"F=",{"$f":"-0.5*((AH340*AI341-AH341*AI340)+(AH341*AI342-AH342*AI341)+\n (AH342*AI343-AH343*AI342)+\n(AH343*AI344-AH344*AI343)+\n(AH344*AI345-AH345*AI344)+\n(AH345*AI346-AH346*AI345)+\n(AH346*AI347-AH347*AI346)+\n(AH347*AI348-AH348*AI347)+\n(AH348*AI349-AH349*AI348)+\n(AH349*AI350-AH350*AI349)+\n(AH350*AI351-AH351*AI350)+\n(AH351*AI352-AH352*AI351)+\n(AH352*AI353-AH353*AI352)+\n(AH353*AI354-AH354*AI353)+\n(AH354*AI355-AH355*AI354)+\n(AH355*AI356-AH356*AI355)+\n(AH356*AI357-AH357*AI356)+\n(AH357*AI358-AH358*AI357)\n)","v":0},"F=",{"$f":"-0.5*(+\n (AJ342*AK343-AJ343*AK342)+\n(AJ343*AK344-AJ344*AK343)+\n(AJ344*AK345-AJ345*AK344)+\n(AJ345*AK346-AJ346*AK345)+\n(AJ346*AK347-AJ347*AK346)+\n(AJ347*AK348-AJ348*AK347)+\n(AJ348*AK349-AJ349*AK348)+\n(AJ349*AK350-AJ350*AK349)+\n(AJ350*AK351-AJ351*AK350)+\n(AJ351*AK352-AJ352*AK351)+\n(AJ352*AK353-AJ353*AK352)+\n(AJ353*AK354-AJ354*AK353)+\n(AJ354*AK355-AJ355*AK354)+\n(AJ355*AK356-AJ356*AK355)+\n(AJ356*AK357-AJ357*AK356)+\n(AJ357*AK358-AJ358*AK357)+\n(AJ358*AK359-AJ359*AK358))","v":0},null,null,5,{"$error":"#VALUE!"},5,{"$error":"#VALUE!"},5,{"$error":"#VALUE!"},5,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$64","v":5.04}]
[null,null,null,"y=",{"$f":"+IF(E362=0,0,-((D339*E340-D340*E339)*(E339+E340)+(D340*E341-D341*E340)*(E340+E341)+\n(D341*E342-D342*E341)*(E341+E342)+\n(D342*E343-D343*E342)*(E342+E343)+\n(D343*E344-D344*E343)*(E343+E344)+\n(D344*E345-D345*E344)*(E344+E345)+\n(D345*E346-D346*E345)*(E345+E346)+\n(D346*E347-D348*E346)*(E346+E347)+\n(D348*E348-D349*E347)*(E347+E348)+\n(D349*E349-D350*E348)*(E348+E349)+\n(D350*E350-D351*E349)*(E349+E350)+\n(D351*E351-D352*E350)*(E350+E351)+\n(D352*E352-D353*E351)*(E351+E352)+\n(D353*E353-D354*E352)*(E352+E353)+\n(D354*E354-D355*E353)*(E353+E354)+\n(D355*E355-D356*E354)*(E354+E355)+\n(D356*E356-D357*E355)*(E355+E356)+\n(D357*E357-#REF!*E356)*(E356+E357)+\n(#REF!*E358-D358*E357)*(E357+E358))/6/E362)","v":0},"x=",3,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,null,null,6,0,6,{"$error":"#VALUE!"},6,0,6,0,0,{"$f":"'Analiza i dimenzioniranje'!$U$63","v":4.72}]
[null,null,null,"y=",{"$f":"+IF(E363=0,0,-((D340*E341-D341*E340)*(E340+E341)+(D341*E342-D342*E341)*(E341+E342)+\n(D342*E343-D343*E342)*(E342+E343)+\n(D343*E344-D344*E343)*(E343+E344)+\n(D344*E345-D345*E344)*(E344+E345)+\n(D345*E346-D346*E345)*(E345+E346)+\n(D346*E347-D348*E346)*(E346+E347)+\n(D348*E348-D349*E347)*(E347+E348)+\n(D349*E349-D350*E348)*(E348+E349)+\n(D350*E350-D351*E349)*(E349+E350)+\n(D351*E351-D352*E350)*(E350+E351)+\n(D352*E352-D353*E351)*(E351+E352)+\n(D353*E353-D354*E352)*(E352+E353)+\n(D354*E354-D355*E353)*(E353+E354)+\n(D355*E355-D356*E354)*(E354+E355)+\n(D356*E356-D357*E355)*(E355+E356)+\n(D357*E357-#REF!*E356)*(E356+E357)+\n(#REF!*E358-D358*E357)*(E357+E358)+\n(D358*E359-D359*E358)*(E358+E359))/6/E363)","v":0},"y=",{"$f":"+IF(G363=0,0,-((F340*G341-F341*G340)*(G340+G341)+(F341*G342-F342*G341)*(G341+G342)+\n(F342*G343-F343*G342)*(G342+G343)+\n(F343*G344-F344*G343)*(G343+G344)+\n(F344*G345-F345*G344)*(G344+G345)+\n(F345*G346-F346*G345)*(G345+G346)+\n(F346*G347-F347*G346)*(G346+G347)+\n(F347*G348-F348*G347)*(G347+G348)+\n(F348*G349-F349*G348)*(G348+G349)+\n(F349*G350-F350*G349)*(G349+G350)+\n(F350*G351-F351*G350)*(G350+G351)+\n(F351*G352-F352*G351)*(G351+G352)+\n(F352*G353-F353*G352)*(G352+G353)+\n(F353*G354-F354*G353)*(G353+G354)+\n(F354*G355-F355*G354)*(G354+G355)+\n(F355*G356-F356*G355)*(G355+G356)+\n(F356*G357-F357*G356)*(G356+G357)+\n(F357*G358-F358*G357)*(G357+G358)+\n(F358*G359-F359*G358)*(G358+G359))/6/G363)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(I363=0,0,-((H340*I341-H341*I340)*(I340+I341)+(H341*I342-H342*I341)*(I341+I342)+\n(H342*I343-H343*I342)*(I342+I343)+\n(H343*I344-H344*I343)*(I343+I344)+\n(H344*I345-H345*I344)*(I344+I345)+\n(H345*I346-H346*I345)*(I345+I346)+\n(H346*I347-H347*I346)*(I346+I347)+\n(H347*I348-H348*I347)*(I347+I348)+\n(H348*I349-H349*I348)*(I348+I349)+\n(H349*I350-H350*I349)*(I349+I350)+\n(H350*I351-H351*I350)*(I350+I351)+\n(H351*I352-H352*I351)*(I351+I352)+\n(H352*I353-H353*I352)*(I352+I353)+\n(H353*I354-H354*I353)*(I353+I354)+\n(H354*I355-H355*I354)*(I354+I355)+\n(H355*I356-H356*I355)*(I355+I356)+\n(H356*I357-H357*I356)*(I356+I357)+\n(H357*I358-H358*I357)*(I357+I358)+\n(H358*I359-H359*I358)*(I358+I359))/6/I363)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(K363=0,0,-((J340*K341-J341*K340)*(K340+K341)+(J341*K342-J342*K341)*(K341+K342)+\n(J342*K343-J343*K342)*(K342+K343)+\n(J343*K344-J344*K343)*(K343+K344)+\n(J344*K345-J345*K344)*(K344+K345)+\n(J345*K346-J346*K345)*(K345+K346)+\n(J346*K347-J347*K346)*(K346+K347)+\n(J347*K348-J348*K347)*(K347+K348)+\n(J348*K349-J349*K348)*(K348+K349)+\n(J349*K350-J350*K349)*(K349+K350)+\n(J350*K351-J351*K350)*(K350+K351)+\n(J351*K352-J352*K351)*(K351+K352)+\n(J352*K353-J353*K352)*(K352+K353)+\n(J353*K354-J354*K353)*(K353+K354)+\n(J354*K355-J355*K354)*(K354+K355)+\n(J355*K356-J356*K355)*(K355+K356)+\n(J356*K357-J357*K356)*(K356+K357)+\n(J357*K358-J358*K357)*(K357+K358)+\n(J358*K359-J359*K358)*(K358+K359))/6/K363)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(M363=0,0,-((L340*M341-L341*M340)*(M340+M341)+(L341*M342-L342*M341)*(M341+M342)+\n(L342*M343-L343*M342)*(M342+M343)+\n(L343*M344-L344*M343)*(M343+M344)+\n(L344*M345-L345*M344)*(M344+M345)+\n(L345*M346-L346*M345)*(M345+M346)+\n(L346*M347-L347*M346)*(M346+M347)+\n(L347*M348-L348*M347)*(M347+M348)+\n(L348*M349-L349*M348)*(M348+M349)+\n(L349*M350-L350*M349)*(M349+M350)+\n(L350*M351-L351*M350)*(M350+M351)+\n(L351*M352-L352*M351)*(M351+M352)+\n(L352*M353-L353*M352)*(M352+M353)+\n(L353*M354-L354*M353)*(M353+M354)+\n(L354*M355-L355*M354)*(M354+M355)+\n(L355*M356-L356*M355)*(M355+M356)+\n(L356*M357-L357*M356)*(M356+M357)+\n(L357*M358-L358*M357)*(M357+M358)+\n(L358*M359-L359*M358)*(M358+M359))/6/M363)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(O363=0,0,-((N340*O341-N341*O340)*(O340+O341)+(N341*O342-N342*O341)*(O341+O342)+\n(N342*O343-N343*O342)*(O342+O343)+\n(N343*O344-N344*O343)*(O343+O344)+\n(N344*O345-N345*O344)*(O344+O345)+\n(N345*O346-N346*O345)*(O345+O346)+\n(N346*O347-N347*O346)*(O346+O347)+\n(N347*O348-N348*O347)*(O347+O348)+\n(N348*O349-N349*O348)*(O348+O349)+\n(N349*O350-N350*O349)*(O349+O350)+\n(N350*O351-N351*O350)*(O350+O351)+\n(N351*O352-N352*O351)*(O351+O352)+\n(N352*O353-N353*O352)*(O352+O353)+\n(N353*O354-N354*O353)*(O353+O354)+\n(N354*O355-N355*O354)*(O354+O355)+\n(N355*O356-N356*O355)*(O355+O356)+\n(N356*O357-N357*O356)*(O356+O357)+\n(N357*O358-N358*O357)*(O357+O358)+\n(N358*O359-N359*O358)*(O358+O359))/6/O363)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Q363=0,0,-((P340*Q341-P341*Q340)*(Q340+Q341)+(P341*Q342-P342*Q341)*(Q341+Q342)+\n(P342*Q343-P343*Q342)*(Q342+Q343)+\n(P343*Q344-P344*Q343)*(Q343+Q344)+\n(P344*Q345-P345*Q344)*(Q344+Q345)+\n(P345*Q346-P346*Q345)*(Q345+Q346)+\n(P346*Q347-P347*Q346)*(Q346+Q347)+\n(P347*Q348-P348*Q347)*(Q347+Q348)+\n(P348*Q349-P349*Q348)*(Q348+Q349)+\n(P349*Q350-P350*Q349)*(Q349+Q350)+\n(P350*Q351-P351*Q350)*(Q350+Q351)+\n(P351*Q352-P352*Q351)*(Q351+Q352)+\n(P352*Q353-P353*Q352)*(Q352+Q353)+\n(P353*Q354-P354*Q353)*(Q353+Q354)+\n(P354*Q355-P355*Q354)*(Q354+Q355)+\n(P355*Q356-P356*Q355)*(Q355+Q356)+\n(P356*Q357-P357*Q356)*(Q356+Q357)+\n(P357*Q358-P358*Q357)*(Q357+Q358)+\n(P358*Q359-P359*Q358)*(Q358+Q359))/6/Q363)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(S363=0,0,-((R340*S341-R341*S340)*(S340+S341)+(R341*S342-R342*S341)*(S341+S342)+\n(R342*S343-R343*S342)*(S342+S343)+\n(R343*S344-R344*S343)*(S343+S344)+\n(R344*S345-R345*S344)*(S344+S345)+\n(R345*S346-R346*S345)*(S345+S346)+\n(R346*S347-R347*S346)*(S346+S347)+\n(R347*S348-R348*S347)*(S347+S348)+\n(R348*S349-R349*S348)*(S348+S349)+\n(R349*S350-R350*S349)*(S349+S350)+\n(R350*S351-R351*S350)*(S350+S351)+\n(R351*S352-R352*S351)*(S351+S352)+\n(R352*S353-R353*S352)*(S352+S353)+\n(R353*S354-R354*S353)*(S353+S354)+\n(R354*S355-R355*S354)*(S354+S355)+\n(R355*S356-R356*S355)*(S355+S356)+\n(R356*S357-R357*S356)*(S356+S357)+\n(R357*S358-R358*S357)*(S357+S358)+\n(R358*S359-R359*S358)*(S358+S359))/6/S363)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(U363=0,0,-((T340*U341-T341*U340)*(U340+U341)+(T341*U342-T342*U341)*(U341+U342)+\n(T342*U343-T343*U342)*(U342+U343)+\n(T343*U344-T344*U343)*(U343+U344)+\n(T344*U345-T345*U344)*(U344+U345)+\n(T345*U346-T346*U345)*(U345+U346)+\n(T346*U347-T347*U346)*(U346+U347)+\n(T347*U348-T348*U347)*(U347+U348)+\n(T348*U349-T349*U348)*(U348+U349)+\n(T349*U350-T350*U349)*(U349+U350)+\n(T350*U351-T351*U350)*(U350+U351)+\n(T351*U352-T352*U351)*(U351+U352)+\n(T352*U353-T353*U352)*(U352+U353)+\n(T353*U354-T354*U353)*(U353+U354)+\n(T354*U355-T355*U354)*(U354+U355)+\n(T355*U356-T356*U355)*(U355+U356)+\n(T356*U357-T357*U356)*(U356+U357)+\n(T357*U358-T358*U357)*(U357+U358)+\n(T358*U359-T359*U358)*(U358+U359))/6/U363)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(W363=0,0,-((V340*W341-V341*W340)*(W340+W341)+(V341*W342-V342*W341)*(W341+W342)+\n(V342*W343-V343*W342)*(W342+W343)+\n(V343*W344-V344*W343)*(W343+W344)+\n(V344*W345-V345*W344)*(W344+W345)+\n(V345*W346-V346*W345)*(W345+W346)+\n(V346*W347-V347*W346)*(W346+W347)+\n(V347*W348-V348*W347)*(W347+W348)+\n(V348*W349-V349*W348)*(W348+W349)+\n(V349*W350-V350*W349)*(W349+W350)+\n(V350*W351-V351*W350)*(W350+W351)+\n(V351*W352-V352*W351)*(W351+W352)+\n(V352*W353-V353*W352)*(W352+W353)+\n(V353*W354-V354*W353)*(W353+W354)+\n(V354*W355-V355*W354)*(W354+W355)+\n(V355*W356-V356*W355)*(W355+W356)+\n(V356*W357-V357*W356)*(W356+W357)+\n(V357*W358-V358*W357)*(W357+W358)+\n(V358*W359-V359*W358)*(W358+W359))/6/W363)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Y363=0,0,-((X340*Y341-X341*Y340)*(Y340+Y341)+(X341*Y342-X342*Y341)*(Y341+Y342)+\n(X342*Y343-X343*Y342)*(Y342+Y343)+\n(X343*Y344-X344*Y343)*(Y343+Y344)+\n(X344*Y345-X345*Y344)*(Y344+Y345)+\n(X345*Y346-X346*Y345)*(Y345+Y346)+\n(X346*Y347-X347*Y346)*(Y346+Y347)+\n(X347*Y348-X348*Y347)*(Y347+Y348)+\n(X348*Y349-X349*Y348)*(Y348+Y349)+\n(X349*Y350-X350*Y349)*(Y349+Y350)+\n(X350*Y351-X351*Y350)*(Y350+Y351)+\n(X351*Y352-X352*Y351)*(Y351+Y352)+\n(X352*Y353-X353*Y352)*(Y352+Y353)+\n(X353*Y354-X354*Y353)*(Y353+Y354)+\n(X354*Y355-X355*Y354)*(Y354+Y355)+\n(X355*Y356-X356*Y355)*(Y355+Y356)+\n(X356*Y357-X357*Y356)*(Y356+Y357)+\n(X357*Y358-X358*Y357)*(Y357+Y358)+\n(X358*Y359-X359*Y358)*(Y358+Y359))/6/Y363)","v":0},"y=",{"$f":"+IF(AA363=0,0,-((Z340*AA341-Z341*AA340)*(AA340+AA341)+(Z341*AA342-Z342*AA341)*(AA341+AA342)+\n(Z342*AA343-Z343*AA342)*(AA342+AA343)+\n(Z343*AA344-Z344*AA343)*(AA343+AA344)+\n(Z344*AA345-Z345*AA344)*(AA344+AA345)+\n(Z345*AA346-Z346*AA345)*(AA345+AA346)+\n(Z346*AA347-Z347*AA346)*(AA346+AA347)+\n(Z347*AA348-Z348*AA347)*(AA347+AA348)+\n(Z348*AA349-Z349*AA348)*(AA348+AA349)+\n(Z349*AA350-Z350*AA349)*(AA349+AA350)+\n(Z350*AA351-Z351*AA350)*(AA350+AA351)+\n(Z351*AA352-Z352*AA351)*(AA351+AA352)+\n(Z352*AA353-Z353*AA352)*(AA352+AA353)+\n(Z353*AA354-Z354*AA353)*(AA353+AA354)+\n(Z354*AA355-Z355*AA354)*(AA354+AA355)+\n(Z355*AA356-Z356*AA355)*(AA355+AA356)+\n(Z356*AA357-Z357*AA356)*(AA356+AA357)+\n(Z357*AA358-Z358*AA357)*(AA357+AA358)+\n(Z358*AA359-Z359*AA358)*(AA358+AA359))/6/AA363)","v":0},"y=",{"$f":"+IF(AC363=0,0,-((AB340*AC341-AB341*AC340)*(AC340+AC341)+(AB341*AC342-AB342*AC341)*(AC341+AC342)+\n(AB342*AC343-AB343*AC342)*(AC342+AC343)+\n(AB343*AC344-AB344*AC343)*(AC343+AC344)+\n(AB344*AC345-AB345*AC344)*(AC344+AC345)+\n(AB345*AC346-AB346*AC345)*(AC345+AC346)+\n(AB346*AC347-AB347*AC346)*(AC346+AC347)+\n(AB347*AC348-AB348*AC347)*(AC347+AC348)+\n(AB348*AC349-AB349*AC348)*(AC348+AC349)+\n(AB349*AC350-AB350*AC349)*(AC349+AC350)+\n(AB350*AC351-AB351*AC350)*(AC350+AC351)+\n(AB351*AC352-AB352*AC351)*(AC351+AC352)+\n(AB352*AC353-AB353*AC352)*(AC352+AC353)+\n(AB353*AC354-AB354*AC353)*(AC353+AC354)+\n(AB354*AC355-AB355*AC354)*(AC354+AC355)+\n(AB355*AC356-AB356*AC355)*(AC355+AC356)+\n(AB356*AC357-AB357*AC356)*(AC356+AC357)+\n(AB357*AC358-AB358*AC357)*(AC357+AC358)+\n(AB358*AC359-AB359*AC358)*(AC358+AC359))/6/AC363)","v":0},"y=",{"$f":"+IF(AE363=0,0,-((AD340*AE341-AD341*AE340)*(AE340+AE341)+(AD341*AE342-AD342*AE341)*(AE341+AE342)+\n(AD342*AE343-AD343*AE342)*(AE342+AE343)+\n(AD343*AE344-AD344*AE343)*(AE343+AE344)+\n(AD344*AE345-AD345*AE344)*(AE344+AE345)+\n(AD345*AE346-AD346*AE345)*(AE345+AE346)+\n(AD346*AE347-AD347*AE346)*(AE346+AE347)+\n(AD347*AE348-AD348*AE347)*(AE347+AE348)+\n(AD348*AE349-AD349*AE348)*(AE348+AE349)+\n(AD349*AE350-AD350*AE349)*(AE349+AE350)+\n(AD350*AE351-AD351*AE350)*(AE350+AE351)+\n(AD351*AE352-AD352*AE351)*(AE351+AE352)+\n(AD352*AE353-AD353*AE352)*(AE352+AE353)+\n(AD353*AE354-AD354*AE353)*(AE353+AE354)+\n(AD354*AE355-AD355*AE354)*(AE354+AE355)+\n(AD355*AE356-AD356*AE355)*(AE355+AE356)+\n(AD356*AE357-AD357*AE356)*(AE356+AE357)+\n(AD357*AE358-AD358*AE357)*(AE357+AE358)+\n(AD358*AE359-AD359*AE358)*(AE358+AE359))/6/AE363)","v":0},"y=",{"$f":"+IF(AG363=0,0,-((AF340*AG341-AF341*AG340)*(AG340+AG341)+(AF341*AG342-AF342*AG341)*(AG341+AG342)+\n(AF342*AG343-AF343*AG342)*(AG342+AG343)+\n(AF343*AG344-AF344*AG343)*(AG343+AG344)+\n(AF344*AG345-AF345*AG344)*(AG344+AG345)+\n(AF345*AG346-AF346*AG345)*(AG345+AG346)+\n(AF346*AG347-AF347*AG346)*(AG346+AG347)+\n(AF347*AG348-AF348*AG347)*(AG347+AG348)+\n(AF348*AG349-AF349*AG348)*(AG348+AG349)+\n(AF349*AG350-AF350*AG349)*(AG349+AG350)+\n(AF350*AG351-AF351*AG350)*(AG350+AG351)+\n(AF351*AG352-AF352*AG351)*(AG351+AG352)+\n(AF352*AG353-AF353*AG352)*(AG352+AG353)+\n(AF353*AG354-AF354*AG353)*(AG353+AG354)+\n(AF354*AG355-AF355*AG354)*(AG354+AG355)+\n(AF355*AG356-AF356*AG355)*(AG355+AG356)+\n(AF356*AG357-AF357*AG356)*(AG356+AG357)+\n(AF357*AG358-AF358*AG357)*(AG357+AG358)+\n(AF358*AG359-AF359*AG358)*(AG358+AG359))/6/AG363)","v":0},"y=",{"$f":"+IF(AI363=0,0,-((AH340*AI341-AH341*AI340)*(AI340+AI341)+(AH341*AI342-AH342*AI341)*(AI341+AI342)+\n(AH342*AI343-AH343*AI342)*(AI342+AI343)+\n(AH343*AI344-AH344*AI343)*(AI343+AI344)+\n(AH344*AI345-AH345*AI344)*(AI344+AI345)+\n(AH345*AI346-AH346*AI345)*(AI345+AI346)+\n(AH346*AI347-AH347*AI346)*(AI346+AI347)+\n(AH347*AI348-AH348*AI347)*(AI347+AI348)+\n(AH348*AI349-AH349*AI348)*(AI348+AI349)+\n(AH349*AI350-AH350*AI349)*(AI349+AI350)+\n(AH350*AI351-AH351*AI350)*(AI350+AI351)+\n(AH351*AI352-AH352*AI351)*(AI351+AI352)+\n(AH352*AI353-AH353*AI352)*(AI352+AI353)+\n(AH353*AI354-AH354*AI353)*(AI353+AI354)+\n(AH354*AI355-AH355*AI354)*(AI354+AI355)+\n(AH355*AI356-AH356*AI355)*(AI355+AI356)+\n(AH356*AI357-AH357*AI356)*(AI356+AI357)+\n(AH357*AI358-AH358*AI357)*(AI357+AI358)+\n(AH358*AI359-AH359*AI358)*(AI358+AI359))/6/AI363)","v":0},"y=",{"$f":"+IF(AK363=0,0,-((AJ340*AK341-AJ341*AK340)*(AK340+AK341)+(AJ341*AK342-AJ342*AK341)*(AK341+AK342)+\n(AJ342*AK343-AJ343*AK342)*(AK342+AK343)+\n(AJ343*AK344-AJ344*AK343)*(AK343+AK344)+\n(AJ344*AK345-AJ345*AK344)*(AK344+AK345)+\n(AJ345*AK346-AJ346*AK345)*(AK345+AK346)+\n(AJ346*AK347-AJ347*AK346)*(AK346+AK347)+\n(AJ347*AK348-AJ348*AK347)*(AK347+AK348)+\n(AJ348*AK349-AJ349*AK348)*(AK348+AK349)+\n(AJ349*AK350-AJ350*AK349)*(AK349+AK350)+\n(AJ350*AK351-AJ351*AK350)*(AK350+AK351)+\n(AJ351*AK352-AJ352*AK351)*(AK351+AK352)+\n(AJ352*AK353-AJ353*AK352)*(AK352+AK353)+\n(AJ353*AK354-AJ354*AK353)*(AK353+AK354)+\n(AJ354*AK355-AJ355*AK354)*(AK354+AK355)+\n(AJ355*AK356-AJ356*AK355)*(AK355+AK356)+\n(AJ356*AK357-AJ357*AK356)*(AK356+AK357)+\n(AJ357*AK358-AJ358*AK357)*(AK357+AK358)+\n(AJ358*AK359-AJ359*AK358)*(AK358+AK359))/6/AK363)","v":0},null,null,7,{"$error":"#VALUE!"},7,{"$error":"#VALUE!"},7,{"$error":"#VALUE!"},7,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$62","v":4.4000000000000004}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,0,8,{"$error":"#VALUE!"},8,0,8,3.76,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$61","v":4.08}]
[null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.44,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$60","v":3.76}]
[null,"OPTEREĆENJE TEMELJEM",null,null,null,null,null,null,null," (TERZAGHY)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.14,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$59","v":3.44}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.14,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$58","v":3.14}]
[null,"KONTINUIRANO OPTEREĆENJE",null,"P - D=",{"$f":"IF('Analiza i dimenzioniranje'!$E$28-I370<=0,0,+'Analiza i dimenzioniranje'!$E$28-I370)","v":{"$error":"#VALUE!"}},"kN/m2","raster. iskopom   D=y*Df =",null,{"$f":"+'Analiza i dimenzioniranje'!$D$16*('Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20-D376)","v":{"$error":"#VALUE!"}},"kN/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.28,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$57","v":2.8}]
[null," visina zida i temelja",null,"H =",{"$f":"+E291","v":{"$error":"#VALUE!"}},"m",{"$f":"E375","v":6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$56","v":2.48}]
[null,"visina opterećenja iznad vrha zida",null,"h =",{"$f":"+E292","v":-1},"m",{"$f":"SQRT(E375^2+E374^2)","v":6.7082039324993694},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.9200000000000002,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$55","v":2.16}]
[null,"širina temelja",null,"b =",{"$f":"+E293","v":1},"m   ",{"$f":"E374+E373","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.2400000000000002,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$54","v":1.84}]
[null,"udaljenost temelja od zida",null,"D =",{"$f":"+E294","v":3},"m    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.56,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$53","v":1.52}]
[null,"1/2 dužine temelja",null,"L/2=a=",{"$f":"+E295","v":6},"m",{"$f":"SQRT(G371^2+G373^2)","v":7.2111025509279782},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
["DNO TEMELJA NA VISINI","PRESJEK NA Visini ",null,{"$f":"ROUND('Analiza i dimenzioniranje'!U60,2)","v":3.76},null,"Presjek III - III",null,"Presjek VI",null,"Presjek VII-VII",null,"Presjek VIII-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"Presjek XIV-XIV",null,"Presjek XV-XV",null,"PresjekXVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX",null,null,null,null,null,null,null,null,null,null,3.76,{"$f":"+IF(AW377>=AW$299,0,AQ236-AW236)","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
[null,null,null,null,null,"(sb2-sb1)*2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja ","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja",null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2",{"$f":"+AU380","v":0},"SQhi=",6.2]
[null,null,null,{"$f":"+F379","v":0},{"$f":"+D378-E376","v":0},"III",{"$f":"+D376","v":3.76},"IV",{"$f":"+G378","v":3.76},"VII",{"$f":"+G378","v":3.76},"VIII",{"$f":"'Analiza i dimenzioniranje'!U146","v":0},"IX",{"$f":"+G378","v":3.76},"X",{"$f":"+O378","v":3.76},"XI",{"$f":"+G378","v":3.76},"XII",{"$f":"+'Analiza i dimenzioniranje'!S48","v":1},"XIII",{"$f":"+G378","v":3.76},"XIV",{"$f":"+W378","v":3.76},"XV",{"$f":"+G378","v":3.76},"XVI",{"$f":"+I378","v":3.76},"XVII",{"$f":"+AA378","v":3.76},"XVIII",{"$f":"+AE378","v":3.76},"XIX",{"$f":"+AG378","v":3.76},"XX",{"$f":"+AI378","v":3.76},null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
[null,null,null,0,{"$f":"IF(D378>E$296,D378,E$296)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja"]
[0,null,null,0,{"$f":"IF(AW359>G$298,0,AW359)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"XVIII",{"$f":"+'Analiza i dimenzioniranje'!U190","v":0},"XIX",{"$f":"+'Analiza i dimenzioniranje'!U189","v":0},"XX",{"$f":"'Analiza i dimenzioniranje'!U188","v":0}]
[{"$f":"+A341","v":0},null,null,0,{"$f":"+AW360","v":6.0000000000000009},0,0,{"$f":"+F381","v":0},{"$f":"+G381","v":0},0,{"$f":"+E380","v":0},0,0,0,{"$f":"+M381","v":0},0,{"$f":"+O381","v":0},0,{"$f":"+AS381","v":0},0,{"$f":"+S381","v":0},0,{"$f":"+AS381","v":0},0,{"$f":"+W381","v":0},0,{"$f":"+S381","v":0},0,{"$f":"+AA381","v":0},0,{"$f":"+AU358","v":0},0,{"$f":"+AU358","v":0},0,{"$f":"+AG381","v":0},{"$f":"+AD381","v":0},{"$f":"+AG381","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD419","v":0},{"$f":"+BB381-BC380","v":0},{"$f":"+AD419","v":0},{"$f":"+BD381-BE380","v":0},{"$f":"+AD419","v":0},{"$f":"+'Analiza i dimenzioniranje'!E188","v":0}]
[0,null,null,0,{"$f":"IF(AW361>G$298,0,AW361)","v":0},{"$f":"+D217","v":0},0,{"$f":"+F382","v":0},0,0,6.0000000000000009,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU359","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+AU397","v":15.553599999999999},{"$f":"+AT420","v":0},{"$f":"+BC382","v":15.553599999999999},0,{"$f":"+AE420","v":0}]
[0,null,null,{"$f":"+AV359","v":{"$error":"#VALUE!"}},0,0,0,0,0,{"$f":"+F381","v":0},0,{"$f":"+D380","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU360","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE421","v":0}]
[0,null,null,0,0,0,0,0,0,{"$f":"+F382","v":0},0,{"$f":"+D381","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU361","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE422","v":0}]
[0,null,null,0,0,0,0,0,0,0,0,{"$f":"+D382","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU362","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE423","v":0}]
[0,null,null,0,4.4000000000000004,0,0,0,0,0,0,{"$f":"+D219","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AE385","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE424","v":0}]
[0,null,null,0,4.08,0,0,0,0,0,4.4000000000000004,{"$f":"+D384","v":0},0,{"$f":"+J385","v":0},0,{"$f":"+L385","v":0},0,0,0,{"$f":"+P385","v":0},0,0,0,{"$f":"+T385","v":0},0,0,0,{"$f":"+X385","v":0},0,0,{"$f":"+AU364","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+BC387","v":0}]
[0,null,null,0,3.76,0,0,0,0,0,4.08,{"$f":"+D385","v":0},0,{"$f":"+J386","v":0},0,{"$f":"+L386","v":0},0,0,0,{"$f":"+P386","v":0},0,0,0,{"$f":"+T386","v":0},0,0,{"$f":"+AA387","v":0},{"$f":"+X386","v":0},0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[0,null,null,{"$f":"+D348","v":0},3.44,{"$f":"+AX389","v":0},{"$f":"+AW367","v":3.76},0,{"$f":"+G389","v":3.76},{"$f":"+F389","v":0},{"$f":"+E388","v":3.76},{"$f":"+D386","v":0},{"$f":"+E388","v":3.76},{"$f":"+J387","v":0},3.76,{"$f":"+N389","v":0},3.76,0,{"$f":"+Q389","v":3.76},0,3.76,0,{"$f":"+U389","v":3.76},{"$f":"+V389","v":0},3.76,0,{"$f":"+S389","v":3.76},{"$f":"+Z389","v":0},{"$f":"+AA389","v":3.76},0,3.76,0,3.76,0,3.76,0,3.76,null,{"$f":"+D389","v":0},{"$f":"$E$384^2+AM389^2","v":0},{"$f":"$G$373^2+AM389^2","v":16},{"$f":"$G$375^2+AM389^2","v":51.999999999999993},{"$f":"IF(AM389=0,0,$E$370/(PI())*(ATAN(($E$375*$G$373)/(AM389*SQRT(AP389)))-$E$375*$G$373*AM389/(AO389*SQRT(AP389))))","v":0},null,{"$f":"+AM389","v":0},{"$f":"$E$375^2+AS389^2","v":36},{"$f":"$E$374^2+AS389^2","v":9},{"$f":"$G$372^2+AS389^2","v":45.000000000000007},{"$f":"IF(AS389=0,0,($E$370/(PI()))*(ATAN(($E$375*$E$374)/(AS389*SQRT(AV389)))-$E$375*$E$374*AS389/(AU389*SQRT(AV389))))","v":0},{"$f":"+AQ389-AW389","v":0},null,null,null,0,0,0,0,0,0]
[0,null,null,0.32,3.14,{"$error":"#VALUE!"},3.44,{"$error":"#VALUE!"},{"$f":"+G390","v":3.44},{"$error":"#VALUE!"},3.44,{"$f":"+J390","v":{"$error":"#VALUE!"}},3.44,{"$f":"+J390","v":{"$error":"#VALUE!"}},3.44,{"$error":"#VALUE!"},3.44,{"$f":"+N390","v":{"$error":"#VALUE!"}},3.44,{"$error":"#VALUE!"},3.44,0,{"$f":"+W389","v":3.76},0,3.76,0,3.44,0,{"$f":"+Y390","v":3.76},{"$f":"+AB390","v":0},3.44,{"$f":"+AD390","v":0},3.44,0,3.44,0,3.44,null,0.32,{"$f":"$E$374^2+AM390^2","v":9.1023999999999994},{"$f":"$G$373^2+AM390^2","v":16.102399999999999},{"$f":"$G$375^2+AM390^2","v":52.102399999999996},{"$f":"IF(AM390=0,0,$E$370/(PI())*(ATAN(($E$375*$G$373)/(AM390*SQRT(AP390)))-$E$375*$G$373*AM390/(AO390*SQRT(AP390))))","v":{"$error":"#VALUE!"}},null,{"$f":"+AM390","v":0.32},{"$f":"$E$375^2+AS390^2","v":36.102400000000003},{"$f":"$E$374^2+AS390^2","v":9.1023999999999994},{"$f":"$G$372^2+AS390^2","v":45.10240000000001},{"$f":"IF(AS390=0,0,($E$370/(PI()))*(ATAN(($E$375*$E$374)/(AS390*SQRT(AV390)))-$E$375*$E$374*AS390/(AU390*SQRT(AV390))))","v":{"$error":"#VALUE!"}},{"$f":"+(AQ390-AW390)*2","v":{"$error":"#VALUE!"}},null,null,null,0,0,0,0,0,0]
[0,null,null,0.64,2.8,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.14,{"$error":"#VALUE!"},3.14,{"$f":"+J391","v":{"$error":"#VALUE!"}},3.14,{"$f":"+J391","v":{"$error":"#VALUE!"}},3.14,{"$error":"#VALUE!"},3.14,{"$f":"+N391","v":{"$error":"#VALUE!"}},{"$f":"+Q391","v":3.14},0,{"$f":"+U390","v":3.44},{"$f":"+N387","v":0},{"$f":"+AS391","v":0.64},{"$f":"+V391","v":0},0.64,0,3.14,{"$f":"+X391","v":0},0.64,0,3.14,0,3.14,0,3.14,0,3.14,null,0.64,{"$f":"$E$374^2+AM391^2","v":9.4095999999999993},{"$f":"$G$373^2+AM391^2","v":16.409600000000001},{"$f":"$G$375^2+AM391^2","v":52.40959999999999},{"$f":"IF(AM391=0,0,$E$370/(PI())*(ATAN(($E$375*$G$373)/(AM391*SQRT(AP391)))-$E$375*$G$373*AM391/(AO391*SQRT(AP391))))","v":{"$error":"#VALUE!"}},null,{"$f":"+AM391","v":0.64},{"$f":"$E$375^2+AS391^2","v":36.409599999999998},{"$f":"$E$374^2+AS391^2","v":9.4095999999999993},{"$f":"$G$372^2+AS391^2","v":45.409600000000005},{"$f":"IF(AS391=0,0,($E$370/(PI()))*(ATAN(($E$375*$E$374)/(AS391*SQRT(AV391)))-$E$375*$E$374*AS391/(AU391*SQRT(AV391))))","v":{"$error":"#VALUE!"}},{"$f":"+(AQ391-AW391)*2","v":{"$error":"#VALUE!"}},null,null,null,0,0,0,0,0,0]
[0,null,null,0.96,2.48,{"$error":"#VALUE!"},2.8,{"$error":"#VALUE!"},2.8,{"$error":"#VALUE!"},2.8,{"$f":"+J392","v":{"$error":"#VALUE!"}},2.8,{"$f":"+J392","v":{"$error":"#VALUE!"}},2.8,{"$error":"#VALUE!"},2.8,0,{"$f":"+S391","v":3.14},{"$f":"+R392","v":0},3.14,{"$f":"+N388","v":0},0.96,0,0.96,0,3.14,0,0.96,0,3.14,0,3.14,0,3.14,0,3.14,null,0.96,9.9215999999999998,16.921600000000002,52.921599999999991,{"$error":"#VALUE!"},null,0.96,36.921599999999998,9.9215999999999998,45.921600000000005,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,3.44,0,3.44,0,3.44]
[0,null,null,1.28,2.16,{"$error":"#VALUE!"},2.48,{"$error":"#VALUE!"},2.48,{"$error":"#VALUE!"},2.48,{"$f":"+J393","v":{"$error":"#VALUE!"}},2.48,{"$f":"+J393","v":{"$error":"#VALUE!"}},2.48,0,{"$f":"+Q392","v":2.8},0,{"$f":"+AS393","v":1.28},0,1.28,{"$f":"+N389","v":0},1.28,0,1.28,{"$f":"+V391","v":0},1.28,0,1.28,0,1.28,0,1.28,0,1.28,0,1.28,null,1.28,10.638400000000001,17.638400000000001,53.63839999999999,{"$error":"#VALUE!"},null,1.28,37.638399999999997,10.638400000000001,46.638400000000004,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,3.14,0,3.14,0,3.14]
[0,null,null,1.6,1.84,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},2.16,{"$f":"+H394","v":{"$error":"#VALUE!"}},2.16,0,{"$f":"+O393","v":2.48},0,{"$f":"+O394","v":2.48},{"$f":"+N394","v":0},1.6,0,1.6,0,1.6,0,1.6,{"$f":"+V392","v":0},1.6,0,1.6,0,1.6,0,1.6,0,1.6,0,1.6,null,1.6,11.56,18.560000000000002,54.559999999999995,{"$error":"#VALUE!"},null,1.6,38.56,11.56,47.560000000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,3.14,0,3.14,0,3.14]
[0,null,null,1.9200000000000002,1.52,{"$error":"#VALUE!"},1.84,{"$error":"#VALUE!"},1.84,{"$error":"#VALUE!"},1.84,0,{"$f":"+M394","v":2.16},0,{"$f":"+M395","v":2.16},0,2.16,0,1.9200000000000002,0,1.9200000000000002,0,1.9200000000000002,0,1.9200000000000002,{"$f":"+V393","v":0},1.9200000000000002,0,1.9200000000000002,0,1.9200000000000002,0,1.9200000000000002,0,1.9200000000000002,0,1.9200000000000002,null,1.9200000000000002,12.686400000000001,19.686399999999999,55.686399999999992,{"$error":"#VALUE!"},null,1.9200000000000002,39.686399999999999,12.686400000000001,48.686400000000006,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,0.96,0,0.96,0,0.96]
[0,null,null,2.2400000000000002,1.2,{"$error":"#VALUE!"},1.52,{"$error":"#VALUE!"},1.52,0,{"$f":"+K395","v":1.84},0,{"$f":"+E395","v":1.52},0,{"$f":"+M396","v":1.52},0,1.52,0,2.2400000000000002,0,2.2400000000000002,0,2.2400000000000002,0,2.2400000000000002,{"$f":"+V394","v":0},2.2400000000000002,0,2.2400000000000002,0,{"$f":"+AE395","v":1.9200000000000002},{"$f":"+AT394","v":38.56},2.2400000000000002,0,2.2400000000000002,0,2.2400000000000002,null,2.2400000000000002,14.017600000000002,21.017600000000002,57.017599999999995,{"$error":"#VALUE!"},null,2.2400000000000002,41.017600000000002,14.017600000000002,50.017600000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,1.28,0,1.28,0,1.28]
[0,null,null,2.56,{"$f":"+AW376","v":1.2},{"$error":"#VALUE!"},1.2,0,1.53,0,{"$f":"+E396","v":1.2},0,{"$f":"+E396","v":1.2},{"$f":"+J397","v":0},{"$f":"+M397","v":1.2},0,1.2,0,2.56,0,2.56,0,2.56,0,2.56,{"$f":"+V395","v":0},2.56,0,2.56,0,{"$f":"+AU374","v":2.56},{"$f":"+AT395","v":39.686399999999999},2.56,{"$f":"+AD395","v":0},2.56,0,2.56,null,2.56,15.553599999999999,22.553599999999999,58.553599999999996,{"$error":"#VALUE!"},null,2.56,42.553600000000003,15.553599999999999,51.55360000000001,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,1.6,0,1.6,0,1.6]
[0,null,null,{"$f":"+AW377","v":6.2},null,0,{"$f":"+E397","v":1.2},0,{"$f":"+G398","v":1.2},0,{"$f":"+E397","v":1.2},0,{"$f":"+E397","v":1.2},0,{"$f":"+O397","v":1.2},0,1.2,0,0,0,0,0,{"$f":"+W397","v":2.56},0,2.56,0,{"$f":"+AA397","v":2.56},0,2.56,0,{"$f":"+AE397","v":2.56},0,0,0,{"$f":"+AI397","v":2.56},{"$f":"+AD398","v":0},0,null,null,null,null,null,null,-1,{"$f":"+AO398","v":0},-1,{"$f":"+S421","v":0},{"$f":"#REF!-#REF!","v":{"$error":"#REF!"}},{"$f":"+AW399","v":6.0000000000000009},null,null,null,null,{"$f":"+AT434","v":37.638399999999997},1.9200000000000002,0,1.9200000000000002,0,1.9200000000000002]
[0,null,null,{"$f":"+AW378","v":"sb1"},null,{"$f":"+AV375","v":0},{"$f":"+G389","v":3.76},0,{"$f":"+G399","v":3.76},0,{"$f":"+K389","v":3.76},0,{"$f":"+M389","v":3.76},0,{"$f":"+O389","v":3.76},0,3.76,0,{"$f":"+S389","v":3.76},0,3.76,0,{"$f":"+S399","v":3.76},0,3.76,0,{"$f":"+AU376","v":3.76},0,3.76,0,{"$f":"+AG399","v":3.76},0,3.76,0,{"$f":"+AK399","v":3.76},{"$f":"+AD399","v":0},3.76,null,null,null,null,null,null,0,{"$f":"+AO399","v":0},0,0,{"$f":"#REF!-#REF!","v":{"$error":"#REF!"}},{"$f":"+AW400","v":6.0000000000000009},null,null,null,null,{"$f":"+AT435","v":38.56},2.2400000000000002,{"$f":"+AD435","v":0},2.2400000000000002,0,2.2400000000000002]
[null,null,null,"Ukupni pritisak",null,"SQhi=",{"$f":"+G403","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I403","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K403","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+M403","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+O403","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Q403","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+S403","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+U403","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+W403","v":0},"SQhi=",{"$f":"+Y403","v":0},"SQhi=",{"$f":"+AA403","v":0},"SQhi=",{"$f":"+AC403","v":0},"SQhi=",{"$f":"+AE403","v":0},"SQhi=",{"$f":"+AG403","v":32.109567999999996},"SQhi=",{"$f":"+AI403","v":0},"SQhi=",{"$f":"+AK403","v":0},null,null,null,null,null,null,"SQhi=",{"$f":"+AS403","v":-1.28},"SQhi=",0,{"$f":"AR279-BQ258","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$67","v":6.0000000000000009},null,null,null,null,0,1.2,0,{"$f":"+BE399","v":2.2400000000000002},0,{"$f":"+AE438","v":1.2}]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G405","v":{"$error":"#VALUE!"}}," y=",{"$f":"+I405","v":{"$error":"#VALUE!"}}," y=",{"$f":"+K405","v":{"$error":"#VALUE!"}}," y=",{"$f":"+M405","v":{"$error":"#VALUE!"}}," y=",{"$f":"+O405","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Q405","v":{"$error":"#VALUE!"}}," y=",{"$f":"+S405","v":{"$error":"#VALUE!"}}," y=",{"$f":"+U405","v":{"$error":"#VALUE!"}}," y=",{"$f":"+W405","v":0}," y=",{"$f":"+Y405","v":0}," y=",{"$f":"+AA405","v":0}," y=",{"$f":"+AC405","v":0}," y=",{"$f":"+AE405","v":0}," y=",{"$f":"+AG405","v":1.3540581050483147}," y=",{"$f":"+AI405","v":0}," y=",{"$f":"+AK405","v":0},null,null,null,null,null,null," y=",{"$f":"+AS405","v":0.85333333333333339}," y=",0,{"$f":"AQ259-AW259","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$U$66","v":5.6800000000000006},null,null,null,null,0,6.2,0,{"$f":"+AK439","v":6.2},0,{"$f":"+AE439","v":6.2}]
[null,null,null,"krak za presjek III -III",null,"z=",{"$f":"+G401-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I401-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K401-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M401-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+O401-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Q401-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+S401-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+U401-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}},"z=",{"$f":"+W401-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+Y401-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AA401-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AC401-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AE401-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AG401-'Analiza i dimenzioniranje'!$E$52","v":0.15405810504831474},"z=",{"$f":"+AI401-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AK401-'Analiza i dimenzioniranje'!$E$52","v":-1.2},null,null,"z=",null,null,null,"z=",{"$f":"+AS401-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":0.35333333333333339},"z=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$65","v":5.36},null,null,null,null,"SQhi=",{"$f":"+BC405","v":1.8373120000000007},"SQhi=",{"$f":"+BE405","v":0}]
[null,null,null,"Ukupni pritisak",null,"F=",{"$f":"-0.5*(+\n (F382*G383-F383*G382)+\n(F383*G384-F384*G383)+\n(F384*G385-F385*G384)+\n(F385*G386-F386*G385)+\n(F386*G387-F387*G386)+\n(F387*G388-F388*G387)+\n(F388*G389-F389*G388)+\n(F389*G390-F390*G389)+\n(F390*G391-F391*G390)+\n(F391*G392-F392*G391)+\n(F392*G393-F393*G392)+\n(F393*G394-F394*G393)+\n(F394*G395-F395*G394)+\n(F395*G396-F396*G395)+\n(F396*G397-F397*G396)+\n(F397*G398-F398*G397)+\n(F398*G399-F399*G398))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (H382*I383-H383*I382)+\n(H383*I384-H384*I383)+\n(H384*I385-H385*I384)+\n(H385*I386-H386*I385)+\n(H386*I387-H387*I386)+\n(H387*I388-H388*I387)+\n(H388*I389-H389*I388)+\n(H389*I390-H390*I389)+\n(H390*I391-H391*I390)+\n(H391*I392-H392*I391)+\n(H392*I393-H393*I392)+\n(H393*I394-H394*I393)+\n(H394*I395-H395*I394)+\n(H395*I396-H396*I395)+\n(H396*I397-H397*I396)+\n(H397*I398-H398*I397)+\n(H398*I399-H399*I398))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (J382*K383-J383*K382)+\n(J383*K384-J384*K383)+\n(J384*K385-J385*K384)+\n(J385*K386-J386*K385)+\n(J386*K387-J387*K386)+\n(J387*K388-J388*K387)+\n(J388*K389-J389*K388)+\n(J389*K390-J390*K389)+\n(J390*K391-J391*K390)+\n(J391*K392-J392*K391)+\n(J392*K393-J393*K392)+\n(J393*K394-J394*K393)+\n(J394*K395-J395*K394)+\n(J395*K396-J396*K395)+\n(J396*K397-J397*K396)+\n(J397*K398-J398*K397)+\n(J398*K399-J399*K398))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (L382*M383-L383*M382)+\n(L383*M384-L384*M383)+\n(L384*M385-L385*M384)+\n(L385*M386-L386*M385)+\n(L386*M387-L387*M386)+\n(L387*M388-L388*M387)+\n(L388*M389-L389*M388)+\n(L389*M390-L390*M389)+\n(L390*M391-L391*M390)+\n(L391*M392-L392*M391)+\n(L392*M393-L393*M392)+\n(L393*M394-L394*M393)+\n(L394*M395-L395*M394)+\n(L395*M396-L396*M395)+\n(L396*M397-L397*M396)+\n(L397*M398-L398*M397)+\n(L398*M399-L399*M398))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (N382*O383-N383*O382)+\n(N383*O384-N384*O383)+\n(N384*O385-N385*O384)+\n(N385*O386-N386*O385)+\n(N386*O387-N387*O386)+\n(N387*O388-N388*O387)+\n(N388*O389-N389*O388)+\n(N389*O390-N390*O389)+\n(N390*O391-N391*O390)+\n(N391*O392-N392*O391)+\n(N392*O393-N393*O392)+\n(N393*O394-N394*O393)+\n(N394*O395-N395*O394)+\n(N395*O396-N396*O395)+\n(N396*O397-N397*O396)+\n(N397*O398-N398*O397)+\n(N398*O399-N399*O398))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (P382*Q383-P383*Q382)+\n(P383*Q384-P384*Q383)+\n(P384*Q385-P385*Q384)+\n(P385*Q386-P386*Q385)+\n(P386*Q387-P387*Q386)+\n(P387*Q388-P388*Q387)+\n(P388*Q389-P389*Q388)+\n(P389*Q390-P390*Q389)+\n(P390*Q391-P391*Q390)+\n(P391*Q392-P392*Q391)+\n(P392*Q393-P393*Q392)+\n(P393*Q394-P394*Q393)+\n(P394*Q395-P395*Q394)+\n(P395*Q396-P396*Q395)+\n(P396*Q397-P397*Q396)+\n(P397*Q398-P398*Q397)+\n(P398*Q399-P399*Q398))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (R382*S383-R383*S382)+\n(R383*S384-R384*S383)+\n(R384*S385-R385*S384)+\n(R385*S386-R386*S385)+\n(R386*S387-R387*S386)+\n(R387*S388-R388*S387)+\n(R388*S389-R389*S388)+\n(R389*S390-R390*S389)+\n(R390*S391-R391*S390)+\n(R391*S392-R392*S391)+\n(R392*S393-R393*S392)+\n(R393*S394-R394*S393)+\n(R394*S395-R395*S394)+\n(R395*S396-R396*S395)+\n(R396*S397-R397*S396)+\n(R397*S398-R398*S397)+\n(R398*S399-R399*S398))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (T382*U383-T383*U382)+\n(T383*U384-T384*U383)+\n(T384*U385-T385*U384)+\n(T385*U386-T386*U385)+\n(T386*U387-T387*U386)+\n(T387*U388-T388*U387)+\n(T388*U389-T389*U388)+\n(T389*U390-T390*U389)+\n(T390*U391-T391*U390)+\n(T391*U392-T392*U391)+\n(T392*U393-T393*U392)+\n(T393*U394-T394*U393)+\n(T394*U395-T395*U394)+\n(T395*U396-T396*U395)+\n(T396*U397-T397*U396)+\n(T397*U398-T398*U397)+\n(T398*U399-T399*U398))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (V382*W383-V383*W382)+\n(V383*W384-V384*W383)+\n(V384*W385-V385*W384)+\n(V385*W386-V386*W385)+\n(V386*W387-V387*W386)+\n(V387*W388-V388*W387)+\n(V388*W389-V389*W388)+\n(V389*W390-V390*W389)+\n(V390*W391-V391*W390)+\n(V391*W392-V392*W391)+\n(V392*W393-V393*W392)+\n(V393*W394-V394*W393)+\n(V394*W395-V395*W394)+\n(V395*W396-V396*W395)+\n(V396*W397-V397*W396)+\n(V397*W398-V398*W397)+\n(V398*W399-V399*W398))","v":0},"F=",{"$f":"-0.5*(+\n (X382*Y383-X383*Y382)+\n(X383*Y384-X384*Y383)+\n(X384*Y385-X385*Y384)+\n(X385*Y386-X386*Y385)+\n(X386*Y387-X387*Y386)+\n(X387*Y388-X388*Y387)+\n(X388*Y389-X389*Y388)+\n(X389*Y390-X390*Y389)+\n(X390*Y391-X391*Y390)+\n(X391*Y392-X392*Y391)+\n(X392*Y393-X393*Y392)+\n(X393*Y394-X394*Y393)+\n(X394*Y395-X395*Y394)+\n(X395*Y396-X396*Y395)+\n(X396*Y397-X397*Y396)+\n(X397*Y398-X398*Y397)+\n(X398*Y399-X399*Y398))","v":0},"F=",{"$f":"-0.5*(+\n (Z382*AA383-Z383*AA382)+\n(Z383*AA384-Z384*AA383)+\n(Z384*AA385-Z385*AA384)+\n(Z385*AA386-Z386*AA385)+\n(Z386*AA387-Z387*AA386)+\n(Z387*AA388-Z388*AA387)+\n(Z388*AA389-Z389*AA388)+\n(Z389*AA390-Z390*AA389)+\n(Z390*AA391-Z391*AA390)+\n(Z391*AA392-Z392*AA391)+\n(Z392*AA393-Z393*AA392)+\n(Z393*AA394-Z394*AA393)+\n(Z394*AA395-Z395*AA394)+\n(Z395*AA396-Z396*AA395)+\n(Z396*AA397-Z397*AA396)+\n(Z397*AA398-Z398*AA397)+\n(Z398*AA399-Z399*AA398))","v":0},"F=",{"$f":"-0.5*(+\n (AB382*AC383-AB383*AC382)+\n(AB383*AC384-AB384*AC383)+\n(AB384*AC385-AB385*AC384)+\n(AB385*AC386-AB386*AC385)+\n(AB386*AC387-AB387*AC386)+\n(AB387*AC388-AB388*AC387)+\n(AB388*AC389-AB389*AC388)+\n(AB389*AC390-AB390*AC389)+\n(AB390*AC391-AB391*AC390)+\n(AB391*AC392-AB392*AC391)+\n(AB392*AC393-AB393*AC392)+\n(AB393*AC394-AB394*AC393)+\n(AB394*AC395-AB395*AC394)+\n(AB395*AC396-AB396*AC395)+\n(AB396*AC397-AB397*AC396)+\n(AB397*AC398-AB398*AC397)+\n(AB398*AC399-AB399*AC398))","v":0},"F=",{"$f":"-0.5*(+\n (AD382*AE383-AD383*AE382)+\n(AD383*AE384-AD384*AE383)+\n(AD384*AE385-AD385*AE384)+\n(AD385*AE386-AD386*AE385)+\n(AD386*AE387-AD387*AE386)+\n(AD387*AE388-AD388*AE387)+\n(AD388*AE389-AD389*AE388)+\n(AD389*AE390-AD390*AE389)+\n(AD390*AE391-AD391*AE390)+\n(AD391*AE392-AD392*AE391)+\n(AD392*AE393-AD393*AE392)+\n(AD393*AE394-AD394*AE393)+\n(AD394*AE395-AD395*AE394)+\n(AD395*AE396-AD396*AE395)+\n(AD396*AE397-AD397*AE396)+\n(AD397*AE398-AD398*AE397)+\n(AD398*AE399-AD399*AE398))","v":0},"F=",{"$f":"-0.5*((AF380*AG381-AF381*AG380)+(AF381*AG382-AF382*AG381)+\n (AF382*AG383-AF383*AG382)+\n(AF383*AG384-AF384*AG383)+\n(AF384*AG385-AF385*AG384)+\n(AF385*AG386-AF386*AG385)+\n(AF386*AG387-AF387*AG386)+\n(AF387*AG388-AF388*AG387)+\n(AF388*AG389-AF389*AG388)+\n(AF389*AG390-AF390*AG389)+\n(AF390*AG391-AF391*AG390)+\n(AF391*AG392-AF392*AG391)+\n(AF392*AG393-AF393*AG392)+\n(AF393*AG394-AF394*AG393)+\n(AF394*AG395-AF395*AG394)+\n(AF395*AG396-AF396*AG395)+\n(AF396*AG397-AF397*AG396)+\n(AF397*AG398-AF398*AG397)\n)","v":32.109567999999996},"F=",{"$f":"-0.5*((AH380*AI381-AH381*AI380)+(AH381*AI382-AH382*AI381)+\n (AH382*AI383-AH383*AI382)+\n(AH383*AI384-AH384*AI383)+\n(AH384*AI385-AH385*AI384)+\n(AH385*AI386-AH386*AI385)+\n(AH386*AI387-AH387*AI386)+\n(AH387*AI388-AH388*AI387)+\n(AH388*AI389-AH389*AI388)+\n(AH389*AI390-AH390*AI389)+\n(AH390*AI391-AH391*AI390)+\n(AH391*AI392-AH392*AI391)+\n(AH392*AI393-AH393*AI392)+\n(AH393*AI394-AH394*AI393)+\n(AH394*AI395-AH395*AI394)+\n(AH395*AI396-AH396*AI395)+\n(AH396*AI397-AH397*AI396)+\n(AH397*AI398-AH398*AI397)\n)","v":0},"F=",{"$f":"-0.5*(+\n (AJ382*AK383-AJ383*AK382)+\n(AJ383*AK384-AJ384*AK383)+\n(AJ384*AK385-AJ385*AK384)+\n(AJ385*AK386-AJ386*AK385)+\n(AJ386*AK387-AJ387*AK386)+\n(AJ387*AK388-AJ388*AK387)+\n(AJ388*AK389-AJ389*AK388)+\n(AJ389*AK390-AJ390*AK389)+\n(AJ390*AK391-AJ391*AK390)+\n(AJ391*AK392-AJ392*AK391)+\n(AJ392*AK393-AJ393*AK392)+\n(AJ393*AK394-AJ394*AK393)+\n(AJ394*AK395-AJ395*AK394)+\n(AJ395*AK396-AJ396*AK395)+\n(AJ396*AK397-AJ397*AK396)+\n(AJ397*AK398-AJ398*AK397)+\n(AJ398*AK399-AJ399*AK398))","v":0},null,null,"F=",null,null,null,"F=",{"$f":"-0.5*((AR380*AS381-AR381*AS380)+(AR381*AS382-AR382*AS381)+\n (AR382*AS383-AR383*AS382)+\n(AR383*AS384-AR384*AS383)+\n(AR384*AS385-AR385*AS384)+\n(AR385*AS386-AR386*AS385)+\n(AR386*AS387-AR387*AS386)+\n(AR387*AS388-AR388*AS387)+\n(AR388*AS389-AR389*AS388)+\n(AR389*AS390-AR390*AS389)+\n(AR390*AS391-AR391*AS390)+\n(AR391*AS392-AR392*AS391)+\n(AR392*AS393-AR393*AS392)+\n(AR393*AS394-AR394*AS393)+\n(AR394*AS395-AR395*AS394)+\n(AR395*AS396-AR396*AS395)+\n(AR396*AS397-AR397*AS396)+\n(AR397*AS398-AR398*AS397)\n)","v":-1.28},"F=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$64","v":5.04},null,null,null,null," y=",{"$f":"+BC407","v":0.91261529887139836}," y=",{"$f":"+BE407","v":0}]
[null,null,null,"Koordinata težišta ",null,"x=",2.5,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,null,null,"x=",0,"x=",0,"x=",0,"x=",0,0,{"$f":"'Analiza i dimenzioniranje'!$U$63","v":4.72},null,null,null,null,"z=",{"$f":"+BC403-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":0.41261529887139836},"z=",{"$f":"+BE403-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5}]
[null,null,null,"krak za presjek III -III",null,"y=",{"$f":"+IF(G403=0,0,-((F380*G381-F381*G380)*(G380+G381)+(F381*G382-F382*G381)*(G381+G382)+\n(F382*G383-F383*G382)*(G382+G383)+\n(F383*G384-F384*G383)*(G383+G384)+\n(F384*G385-F385*G384)*(G384+G385)+\n(F385*G386-F386*G385)*(G385+G386)+\n(F386*G387-F387*G386)*(G386+G387)+\n(F387*G388-F388*G387)*(G387+G388)+\n(F388*G389-F389*G388)*(G388+G389)+\n(F389*G390-F390*G389)*(G389+G390)+\n(F390*G391-F391*G390)*(G390+G391)+\n(F391*G392-F392*G391)*(G391+G392)+\n(F392*G393-F393*G392)*(G392+G393)+\n(F393*G394-F394*G393)*(G393+G394)+\n(F394*G395-F395*G394)*(G394+G395)+\n(F395*G396-F396*G395)*(G395+G396)+\n(F396*G397-F397*G396)*(G396+G397)+\n(F397*G398-F398*G397)*(G397+G398)+\n(F398*G399-F399*G398)*(G398+G399))/6/G403)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(I403=0,0,-((H380*I381-H381*I380)*(I380+I381)+(H381*I382-H382*I381)*(I381+I382)+\n(H382*I383-H383*I382)*(I382+I383)+\n(H383*I384-H384*I383)*(I383+I384)+\n(H384*I385-H385*I384)*(I384+I385)+\n(H385*I386-H386*I385)*(I385+I386)+\n(H386*I387-H387*I386)*(I386+I387)+\n(H387*I388-H388*I387)*(I387+I388)+\n(H388*I389-H389*I388)*(I388+I389)+\n(H389*I390-H390*I389)*(I389+I390)+\n(H390*I391-H391*I390)*(I390+I391)+\n(H391*I392-H392*I391)*(I391+I392)+\n(H392*I393-H393*I392)*(I392+I393)+\n(H393*I394-H394*I393)*(I393+I394)+\n(H394*I395-H395*I394)*(I394+I395)+\n(H395*I396-H396*I395)*(I395+I396)+\n(H396*I397-H397*I396)*(I396+I397)+\n(H397*I398-H398*I397)*(I397+I398)+\n(H398*I399-H399*I398)*(I398+I399))/6/I403)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(K403=0,0,-((J380*K381-J381*K380)*(K380+K381)+(J381*K382-J382*K381)*(K381+K382)+\n(J382*K383-J383*K382)*(K382+K383)+\n(J383*K384-J384*K383)*(K383+K384)+\n(J384*K385-J385*K384)*(K384+K385)+\n(J385*K386-J386*K385)*(K385+K386)+\n(J386*K387-J387*K386)*(K386+K387)+\n(J387*K388-J388*K387)*(K387+K388)+\n(J388*K389-J389*K388)*(K388+K389)+\n(J389*K390-J390*K389)*(K389+K390)+\n(J390*K391-J391*K390)*(K390+K391)+\n(J391*K392-J392*K391)*(K391+K392)+\n(J392*K393-J393*K392)*(K392+K393)+\n(J393*K394-J394*K393)*(K393+K394)+\n(J394*K395-J395*K394)*(K394+K395)+\n(J395*K396-J396*K395)*(K395+K396)+\n(J396*K397-J397*K396)*(K396+K397)+\n(J397*K398-J398*K397)*(K397+K398)+\n(J398*K399-J399*K398)*(K398+K399))/6/K403)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(M403=0,0,-((L380*M381-L381*M380)*(M380+M381)+(L381*M382-L382*M381)*(M381+M382)+\n(L382*M383-L383*M382)*(M382+M383)+\n(L383*M384-L384*M383)*(M383+M384)+\n(L384*M385-L385*M384)*(M384+M385)+\n(L385*M386-L386*M385)*(M385+M386)+\n(L386*M387-L387*M386)*(M386+M387)+\n(L387*M388-L388*M387)*(M387+M388)+\n(L388*M389-L389*M388)*(M388+M389)+\n(L389*M390-L390*M389)*(M389+M390)+\n(L390*M391-L391*M390)*(M390+M391)+\n(L391*M392-L392*M391)*(M391+M392)+\n(L392*M393-L393*M392)*(M392+M393)+\n(L393*M394-L394*M393)*(M393+M394)+\n(L394*M395-L395*M394)*(M394+M395)+\n(L395*M396-L396*M395)*(M395+M396)+\n(L396*M397-L397*M396)*(M396+M397)+\n(L397*M398-L398*M397)*(M397+M398)+\n(L398*M399-L399*M398)*(M398+M399))/6/M403)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(O403=0,0,-((N380*O381-N381*O380)*(O380+O381)+(N381*O382-N382*O381)*(O381+O382)+\n(N382*O383-N383*O382)*(O382+O383)+\n(N383*O384-N384*O383)*(O383+O384)+\n(N384*O385-N385*O384)*(O384+O385)+\n(N385*O386-N386*O385)*(O385+O386)+\n(N386*O387-N387*O386)*(O386+O387)+\n(N387*O388-N388*O387)*(O387+O388)+\n(N388*O389-N389*O388)*(O388+O389)+\n(N389*O390-N390*O389)*(O389+O390)+\n(N390*O391-N391*O390)*(O390+O391)+\n(N391*O392-N392*O391)*(O391+O392)+\n(N392*O393-N393*O392)*(O392+O393)+\n(N393*O394-N394*O393)*(O393+O394)+\n(N394*O395-N395*O394)*(O394+O395)+\n(N395*O396-N396*O395)*(O395+O396)+\n(N396*O397-N397*O396)*(O396+O397)+\n(N397*O398-N398*O397)*(O397+O398)+\n(N398*O399-N399*O398)*(O398+O399))/6/O403)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Q403=0,0,-((P380*Q381-P381*Q380)*(Q380+Q381)+(P381*Q382-P382*Q381)*(Q381+Q382)+\n(P382*Q383-P383*Q382)*(Q382+Q383)+\n(P383*Q384-P384*Q383)*(Q383+Q384)+\n(P384*Q385-P385*Q384)*(Q384+Q385)+\n(P385*Q386-P386*Q385)*(Q385+Q386)+\n(P386*Q387-P387*Q386)*(Q386+Q387)+\n(P387*Q388-P388*Q387)*(Q387+Q388)+\n(P388*Q389-P389*Q388)*(Q388+Q389)+\n(P389*Q390-P390*Q389)*(Q389+Q390)+\n(P390*Q391-P391*Q390)*(Q390+Q391)+\n(P391*Q392-P392*Q391)*(Q391+Q392)+\n(P392*Q393-P393*Q392)*(Q392+Q393)+\n(P393*Q394-P394*Q393)*(Q393+Q394)+\n(P394*Q395-P395*Q394)*(Q394+Q395)+\n(P395*Q396-P396*Q395)*(Q395+Q396)+\n(P396*Q397-P397*Q396)*(Q396+Q397)+\n(P397*Q398-P398*Q397)*(Q397+Q398)+\n(P398*Q399-P399*Q398)*(Q398+Q399))/6/Q403)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(S403=0,0,-((R380*S381-R381*S380)*(S380+S381)+(R381*S382-R382*S381)*(S381+S382)+\n(R382*S383-R383*S382)*(S382+S383)+\n(R383*S384-R384*S383)*(S383+S384)+\n(R384*S385-R385*S384)*(S384+S385)+\n(R385*S386-R386*S385)*(S385+S386)+\n(R386*S387-R387*S386)*(S386+S387)+\n(R387*S388-R388*S387)*(S387+S388)+\n(R388*S389-R389*S388)*(S388+S389)+\n(R389*S390-R390*S389)*(S389+S390)+\n(R390*S391-R391*S390)*(S390+S391)+\n(R391*S392-R392*S391)*(S391+S392)+\n(R392*S393-R393*S392)*(S392+S393)+\n(R393*S394-R394*S393)*(S393+S394)+\n(R394*S395-R395*S394)*(S394+S395)+\n(R395*S396-R396*S395)*(S395+S396)+\n(R396*S397-R397*S396)*(S396+S397)+\n(R397*S398-R398*S397)*(S397+S398)+\n(R398*S399-R399*S398)*(S398+S399))/6/S403)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(U403=0,0,-((T380*U381-T381*U380)*(U380+U381)+(T381*U382-T382*U381)*(U381+U382)+\n(T382*U383-T383*U382)*(U382+U383)+\n(T383*U384-T384*U383)*(U383+U384)+\n(T384*U385-T385*U384)*(U384+U385)+\n(T385*U386-T386*U385)*(U385+U386)+\n(T386*U387-T387*U386)*(U386+U387)+\n(T387*U388-T388*U387)*(U387+U388)+\n(T388*U389-T389*U388)*(U388+U389)+\n(T389*U390-T390*U389)*(U389+U390)+\n(T390*U391-T391*U390)*(U390+U391)+\n(T391*U392-T392*U391)*(U391+U392)+\n(T392*U393-T393*U392)*(U392+U393)+\n(T393*U394-T394*U393)*(U393+U394)+\n(T394*U395-T395*U394)*(U394+U395)+\n(T395*U396-T396*U395)*(U395+U396)+\n(T396*U397-T397*U396)*(U396+U397)+\n(T397*U398-T398*U397)*(U397+U398)+\n(T398*U399-T399*U398)*(U398+U399))/6/U403)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(W403=0,0,-((V380*W381-V381*W380)*(W380+W381)+(V381*W382-V382*W381)*(W381+W382)+\n(V382*W383-V383*W382)*(W382+W383)+\n(V383*W384-V384*W383)*(W383+W384)+\n(V384*W385-V385*W384)*(W384+W385)+\n(V385*W386-V386*W385)*(W385+W386)+\n(V386*W387-V387*W386)*(W386+W387)+\n(V387*W388-V388*W387)*(W387+W388)+\n(V388*W389-V389*W388)*(W388+W389)+\n(V389*W390-V390*W389)*(W389+W390)+\n(V390*W391-V391*W390)*(W390+W391)+\n(V391*W392-V392*W391)*(W391+W392)+\n(V392*W393-V393*W392)*(W392+W393)+\n(V393*W394-V394*W393)*(W393+W394)+\n(V394*W395-V395*W394)*(W394+W395)+\n(V395*W396-V396*W395)*(W395+W396)+\n(V396*W397-V397*W396)*(W396+W397)+\n(V397*W398-V398*W397)*(W397+W398)+\n(V398*W399-V399*W398)*(W398+W399))/6/W403)","v":0},"y=",{"$f":"+IF(Y403=0,0,-((X380*Y381-X381*Y380)*(Y380+Y381)+(X381*Y382-X382*Y381)*(Y381+Y382)+\n(X382*Y383-X383*Y382)*(Y382+Y383)+\n(X383*Y384-X384*Y383)*(Y383+Y384)+\n(X384*Y385-X385*Y384)*(Y384+Y385)+\n(X385*Y386-X386*Y385)*(Y385+Y386)+\n(X386*Y387-X387*Y386)*(Y386+Y387)+\n(X387*Y388-X388*Y387)*(Y387+Y388)+\n(X388*Y389-X389*Y388)*(Y388+Y389)+\n(X389*Y390-X390*Y389)*(Y389+Y390)+\n(X390*Y391-X391*Y390)*(Y390+Y391)+\n(X391*Y392-X392*Y391)*(Y391+Y392)+\n(X392*Y393-X393*Y392)*(Y392+Y393)+\n(X393*Y394-X394*Y393)*(Y393+Y394)+\n(X394*Y395-X395*Y394)*(Y394+Y395)+\n(X395*Y396-X396*Y395)*(Y395+Y396)+\n(X396*Y397-X397*Y396)*(Y396+Y397)+\n(X397*Y398-X398*Y397)*(Y397+Y398)+\n(X398*Y399-X399*Y398)*(Y398+Y399))/6/Y403)","v":0},"y=",{"$f":"+IF(AA403=0,0,-((Z380*AA381-Z381*AA380)*(AA380+AA381)+(Z381*AA382-Z382*AA381)*(AA381+AA382)+\n(Z382*AA383-Z383*AA382)*(AA382+AA383)+\n(Z383*AA384-Z384*AA383)*(AA383+AA384)+\n(Z384*AA385-Z385*AA384)*(AA384+AA385)+\n(Z385*AA386-Z386*AA385)*(AA385+AA386)+\n(Z386*AA387-Z387*AA386)*(AA386+AA387)+\n(Z387*AA388-Z388*AA387)*(AA387+AA388)+\n(Z388*AA389-Z389*AA388)*(AA388+AA389)+\n(Z389*AA390-Z390*AA389)*(AA389+AA390)+\n(Z390*AA391-Z391*AA390)*(AA390+AA391)+\n(Z391*AA392-Z392*AA391)*(AA391+AA392)+\n(Z392*AA393-Z393*AA392)*(AA392+AA393)+\n(Z393*AA394-Z394*AA393)*(AA393+AA394)+\n(Z394*AA395-Z395*AA394)*(AA394+AA395)+\n(Z395*AA396-Z396*AA395)*(AA395+AA396)+\n(Z396*AA397-Z397*AA396)*(AA396+AA397)+\n(Z397*AA398-Z398*AA397)*(AA397+AA398)+\n(Z398*AA399-Z399*AA398)*(AA398+AA399))/6/AA403)","v":0},"y=",{"$f":"+IF(AC403=0,0,-((AB380*AC381-AB381*AC380)*(AC380+AC381)+(AB381*AC382-AB382*AC381)*(AC381+AC382)+\n(AB382*AC383-AB383*AC382)*(AC382+AC383)+\n(AB383*AC384-AB384*AC383)*(AC383+AC384)+\n(AB384*AC385-AB385*AC384)*(AC384+AC385)+\n(AB385*AC386-AB386*AC385)*(AC385+AC386)+\n(AB386*AC387-AB387*AC386)*(AC386+AC387)+\n(AB387*AC388-AB388*AC387)*(AC387+AC388)+\n(AB388*AC389-AB389*AC388)*(AC388+AC389)+\n(AB389*AC390-AB390*AC389)*(AC389+AC390)+\n(AB390*AC391-AB391*AC390)*(AC390+AC391)+\n(AB391*AC392-AB392*AC391)*(AC391+AC392)+\n(AB392*AC393-AB393*AC392)*(AC392+AC393)+\n(AB393*AC394-AB394*AC393)*(AC393+AC394)+\n(AB394*AC395-AB395*AC394)*(AC394+AC395)+\n(AB395*AC396-AB396*AC395)*(AC395+AC396)+\n(AB396*AC397-AB397*AC396)*(AC396+AC397)+\n(AB397*AC398-AB398*AC397)*(AC397+AC398)+\n(AB398*AC399-AB399*AC398)*(AC398+AC399))/6/AC403)","v":0},"y=",{"$f":"+IF(AE403=0,0,-((AD380*AE381-AD381*AE380)*(AE380+AE381)+(AD381*AE382-AD382*AE381)*(AE381+AE382)+\n(AD382*AE383-AD383*AE382)*(AE382+AE383)+\n(AD383*AE384-AD384*AE383)*(AE383+AE384)+\n(AD384*AE385-AD385*AE384)*(AE384+AE385)+\n(AD385*AE386-AD386*AE385)*(AE385+AE386)+\n(AD386*AE387-AD387*AE386)*(AE386+AE387)+\n(AD387*AE388-AD388*AE387)*(AE387+AE388)+\n(AD388*AE389-AD389*AE388)*(AE388+AE389)+\n(AD389*AE390-AD390*AE389)*(AE389+AE390)+\n(AD390*AE391-AD391*AE390)*(AE390+AE391)+\n(AD391*AE392-AD392*AE391)*(AE391+AE392)+\n(AD392*AE393-AD393*AE392)*(AE392+AE393)+\n(AD393*AE394-AD394*AE393)*(AE393+AE394)+\n(AD394*AE395-AD395*AE394)*(AE394+AE395)+\n(AD395*AE396-AD396*AE395)*(AE395+AE396)+\n(AD396*AE397-AD397*AE396)*(AE396+AE397)+\n(AD397*AE398-AD398*AE397)*(AE397+AE398)+\n(AD398*AE399-AD399*AE398)*(AE398+AE399))/6/AE403)","v":0},"y=",{"$f":"+IF(AG403=0,0,-((AF380*AG381-AF381*AG380)*(AG380+AG381)+(AF381*AG382-AF382*AG381)*(AG381+AG382)+\n(AF382*AG383-AF383*AG382)*(AG382+AG383)+\n(AF383*AG384-AF384*AG383)*(AG383+AG384)+\n(AF384*AG385-AF385*AG384)*(AG384+AG385)+\n(AF385*AG386-AF386*AG385)*(AG385+AG386)+\n(AF386*AG387-AF387*AG386)*(AG386+AG387)+\n(AF387*AG388-AF388*AG387)*(AG387+AG388)+\n(AF388*AG389-AF389*AG388)*(AG388+AG389)+\n(AF389*AG390-AF390*AG389)*(AG389+AG390)+\n(AF390*AG391-AF391*AG390)*(AG390+AG391)+\n(AF391*AG392-AF392*AG391)*(AG391+AG392)+\n(AF392*AG393-AF393*AG392)*(AG392+AG393)+\n(AF393*AG394-AF394*AG393)*(AG393+AG394)+\n(AF394*AG395-AF395*AG394)*(AG394+AG395)+\n(AF395*AG396-AF396*AG395)*(AG395+AG396)+\n(AF396*AG397-AF397*AG396)*(AG396+AG397)+\n(AF397*AG398-AF398*AG397)*(AG397+AG398)+\n(AF398*AG399-AF399*AG398)*(AG398+AG399))/6/AG403)","v":1.3540581050483147},"y=",{"$f":"+IF(AI403=0,0,-((AH380*AI381-AH381*AI380)*(AI380+AI381)+(AH381*AI382-AH382*AI381)*(AI381+AI382)+\n(AH382*AI383-AH383*AI382)*(AI382+AI383)+\n(AH383*AI384-AH384*AI383)*(AI383+AI384)+\n(AH384*AI385-AH385*AI384)*(AI384+AI385)+\n(AH385*AI386-AH386*AI385)*(AI385+AI386)+\n(AH386*AI387-AH387*AI386)*(AI386+AI387)+\n(AH387*AI388-AH388*AI387)*(AI387+AI388)+\n(AH388*AI389-AH389*AI388)*(AI388+AI389)+\n(AH389*AI390-AH390*AI389)*(AI389+AI390)+\n(AH390*AI391-AH391*AI390)*(AI390+AI391)+\n(AH391*AI392-AH392*AI391)*(AI391+AI392)+\n(AH392*AI393-AH393*AI392)*(AI392+AI393)+\n(AH393*AI394-AH394*AI393)*(AI393+AI394)+\n(AH394*AI395-AH395*AI394)*(AI394+AI395)+\n(AH395*AI396-AH396*AI395)*(AI395+AI396)+\n(AH396*AI397-AH397*AI396)*(AI396+AI397)+\n(AH397*AI398-AH398*AI397)*(AI397+AI398)+\n(AH398*AI399-AH399*AI398)*(AI398+AI399))/6/AI403)","v":0},"y=",{"$f":"+IF(AK403=0,0,-((AJ380*AK381-AJ381*AK380)*(AK380+AK381)+(AJ381*AK382-AJ382*AK381)*(AK381+AK382)+\n(AJ382*AK383-AJ383*AK382)*(AK382+AK383)+\n(AJ383*AK384-AJ384*AK383)*(AK383+AK384)+\n(AJ384*AK385-AJ385*AK384)*(AK384+AK385)+\n(AJ385*AK386-AJ386*AK385)*(AK385+AK386)+\n(AJ386*AK387-AJ387*AK386)*(AK386+AK387)+\n(AJ387*AK388-AJ388*AK387)*(AK387+AK388)+\n(AJ388*AK389-AJ389*AK388)*(AK388+AK389)+\n(AJ389*AK390-AJ390*AK389)*(AK389+AK390)+\n(AJ390*AK391-AJ391*AK390)*(AK390+AK391)+\n(AJ391*AK392-AJ392*AK391)*(AK391+AK392)+\n(AJ392*AK393-AJ393*AK392)*(AK392+AK393)+\n(AJ393*AK394-AJ394*AK393)*(AK393+AK394)+\n(AJ394*AK395-AJ395*AK394)*(AK394+AK395)+\n(AJ395*AK396-AJ396*AK395)*(AK395+AK396)+\n(AJ396*AK397-AJ397*AK396)*(AK396+AK397)+\n(AJ397*AK398-AJ398*AK397)*(AK397+AK398)+\n(AJ398*AK399-AJ399*AK398)*(AK398+AK399))/6/AK403)","v":0},null,null,"y=",null,"y=",null,"y=",{"$f":"+IF(AS403=0,0,-((AR380*AS381-AR381*AS380)*(AS380+AS381)+(AR381*AS382-AR382*AS381)*(AS381+AS382)+\n(AR382*AS383-AR383*AS382)*(AS382+AS383)+\n(AR383*AS384-AR384*AS383)*(AS383+AS384)+\n(AR384*AS385-AR385*AS384)*(AS384+AS385)+\n(AR385*AS386-AR386*AS385)*(AS385+AS386)+\n(AR386*AS387-AR387*AS386)*(AS386+AS387)+\n(AR387*AS388-AR388*AS387)*(AS387+AS388)+\n(AR388*AS389-AR389*AS388)*(AS388+AS389)+\n(AR389*AS390-AR390*AS389)*(AS389+AS390)+\n(AR390*AS391-AR391*AS390)*(AS390+AS391)+\n(AR391*AS392-AR392*AS391)*(AS391+AS392)+\n(AR392*AS393-AR393*AS392)*(AS392+AS393)+\n(AR393*AS394-AR394*AS393)*(AS393+AS394)+\n(AR394*AS395-AR395*AS394)*(AS394+AS395)+\n(AR395*AS396-AR396*AS395)*(AS395+AS396)+\n(AR396*AS397-AR397*AS396)*(AS396+AS397)+\n(AR397*AS398-AR398*AS397)*(AS397+AS398)+\n(AR398*AS399-AR399*AS398)*(AS398+AS399))/6/AS403)","v":0.85333333333333339},"y=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$62","v":4.4000000000000004},null,null,null,null,"F=",{"$f":"-0.5*((BB382*BC383-BB383*BC382)+(BB383*BC384-BB384*BC383)+\n (BB384*BC385-BB385*BC384)+\n(BB385*BC386-BB386*BC385)+\n(BB386*BC387-BB387*BC386)+\n(BB387*BC388-BB388*BC387)+\n(BB388*BC389-BB389*BC388)+\n(BB389*BC390-BB390*BC389)+\n(BB390*BC391-BB391*BC390)+\n(BB391*BC392-BB392*BC391)+\n(BB392*BC393-BB393*BC392)+\n(BB393*BC394-BB394*BC393)+\n(BB394*BC395-BB395*BC394)+\n(BB395*BC396-BB396*BC395)+\n(BB396*BC397-BB397*BC396)+\n(BB397*BC398-BB398*BC397)+\n(BB398*BC399-BB399*BC398)+\n(BB399*BC400-BB400*BC399)\n)","v":1.8373120000000007},"F=",{"$f":"-0.5*((BD382*BE383-BD383*BE382)+(BD383*BE384-BD384*BE383)+\n (BD384*BE385-BD385*BE384)+\n(BD385*BE386-BD386*BE385)+\n(BD386*BE387-BD387*BE386)+\n(BD387*BE388-BD388*BE387)+\n(BD388*BE389-BD389*BE388)+\n(BD389*BE390-BD390*BE389)+\n(BD390*BE391-BD391*BE390)+\n(BD391*BE392-BD392*BE391)+\n(BD392*BE393-BD393*BE392)+\n(BD393*BE394-BD394*BE393)+\n(BD394*BE395-BD395*BE394)+\n(BD395*BE396-BD396*BE395)+\n(BD396*BE397-BD397*BE396)+\n(BD397*BE398-BD398*BE397)+\n(BD398*BE399-BD399*BE398)+\n(BD399*BE400-BD400*BE399)\n)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$61","v":4.08},null,null,null,null,"x=",0,"x=",0]
[null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.44,0,{"$f":"+'Analiza i dimenzioniranje'!$U$60","v":3.76},null,null,null,null,"y=",{"$f":"+IF(BC405=0,0,-((BB382*BC383-BB383*BC382)*(BC382+BC383)+(BB383*BC384-BB384*BC383)*(BC383+BC384)+\n(BB384*BC385-BB385*BC384)*(BC384+BC385)+\n(BB385*BC386-BB386*BC385)*(BC385+BC386)+\n(BB386*BC387-BB387*BC386)*(BC386+BC387)+\n(BB387*BC388-BB388*BC387)*(BC387+BC388)+\n(BB388*BC389-BB389*BC388)*(BC388+BC389)+\n(BB389*BC390-BB390*BC389)*(BC389+BC390)+\n(BB390*BC391-BB391*BC390)*(BC390+BC391)+\n(BB391*BC392-BB392*BC391)*(BC391+BC392)+\n(BB392*BC393-BB393*BC392)*(BC392+BC393)+\n(BB393*BC394-BB394*BC393)*(BC393+BC394)+\n(BB394*BC395-BB395*BC394)*(BC394+BC395)+\n(BB395*BC396-BB396*BC395)*(BC395+BC396)+\n(BB396*BC397-BB397*BC396)*(BC396+BC397)+\n(BB397*BC398-BB398*BC397)*(BC397+BC398)+\n(BB398*BC399-BB399*BC398)*(BC398+BC399)+\n(BB399*BC400-BB400*BC399)*(BC399+BC400)+\n(BB400*BC401-BB401*BC400)*(BC400+BC401))/6/BC405)","v":0.91261529887139836},"y=",{"$f":"+IF(BE405=0,0,-((BD382*BE383-BD383*BE382)*(BE382+BE383)+(BD383*BE384-BD384*BE383)*(BE383+BE384)+\n(BD384*BE385-BD385*BE384)*(BE384+BE385)+\n(BD385*BE386-BD386*BE385)*(BE385+BE386)+\n(BD386*BE387-BD387*BE386)*(BE386+BE387)+\n(BD387*BE388-BD388*BE387)*(BE387+BE388)+\n(BD388*BE389-BD389*BE388)*(BE388+BE389)+\n(BD389*BE390-BD390*BE389)*(BE389+BE390)+\n(BD390*BE391-BD391*BE390)*(BE390+BE391)+\n(BD391*BE392-BD392*BE391)*(BE391+BE392)+\n(BD392*BE393-BD393*BE392)*(BE392+BE393)+\n(BD393*BE394-BD394*BE393)*(BE393+BE394)+\n(BD394*BE395-BD395*BE394)*(BE394+BE395)+\n(BD395*BE396-BD396*BE395)*(BE395+BE396)+\n(BD396*BE397-BD397*BE396)*(BE396+BE397)+\n(BD397*BE398-BD398*BE397)*(BE397+BE398)+\n(BD398*BE399-BD399*BE398)*(BE398+BE399)+\n(BD399*BE400-BD400*BE399)*(BE399+BE400)+\n(BD400*BE401-BD401*BE400)*(BE400+BE401))/6/BE405)","v":0}]
[null,"OPTEREĆENJE TEMELJEM",null,null,null,null,null,null,null," (TERZAGHY)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.14,0,{"$f":"+'Analiza i dimenzioniranje'!$U$59","v":3.44}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.14,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$58","v":3.14}]
[null,"KONTINUIRANO OPTEREĆENJE",null,"P - D=",{"$f":"IF('Analiza i dimenzioniranje'!$E$28-I410<=0,0,+'Analiza i dimenzioniranje'!$E$28-I410)","v":{"$error":"#VALUE!"}},"kN/m2","raster. iskopom   D=y*Df =",null,{"$f":"+'Analiza i dimenzioniranje'!$D$16*('Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20-D416)","v":{"$error":"#VALUE!"}},"kN/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.96,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$57","v":2.8}]
[null," visina zida i temelja",null,"H =",{"$f":"+E371","v":{"$error":"#VALUE!"}},"m",{"$f":"E415","v":6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.28,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$56","v":2.48}]
[null,"visina opterećenja iznad vrha zida",null,"h =",{"$f":"+E372","v":-1},"m",{"$f":"SQRT(E415^2+E414^2)","v":6.7082039324993694},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$55","v":2.16}]
[null,"širina temelja",null,"b =",{"$f":"+E373","v":1},"m   ",{"$f":"E414+E413","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.9200000000000002,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$54","v":1.84}]
[null,"udaljenost temelja od zida",null,"D =",{"$f":"+E374","v":3},"m    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.2400000000000002,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$53","v":1.52}]
[null,"1/2 dužine temelja",null,"L/2=a=",{"$f":"+E375","v":6},"m",{"$f":"SQRT(G411^2+G413^2)","v":7.2111025509279782},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,0,{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
["DNO TEMELJA NA VISINI","PRESJEK NA Visini ",null,{"$f":"ROUND('Analiza i dimenzioniranje'!U59,2)","v":3.44},null,"Presjek III -III",null,"Presjek VI",null,"Presjek VII-VII",null,"Presjek VIII-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"Presjek XIV-XIV",null,"Presjek XV-XV",null,"PresjekXVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX",null,null,null,null,null,null,null,null,null,null,6.2,{"$f":"+IF(AW417>=AW$299,0,AQ274-AW274)","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
[null,null,null,null,null,"Visina djelovanja","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja ","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja",null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2",{"$f":"+AU420","v":0},"SQhi=",6.2]
[null,null,null,null,{"$f":"+D418-E416","v":0},"III",{"$f":"+D416","v":3.44},"IV",{"$f":"+G418","v":3.44},"VII",{"$f":"+G418","v":3.44},"VIII",{"$f":"'Analiza i dimenzioniranje'!U201","v":0},"IX",{"$f":"+G418","v":3.44},"X",{"$f":"+'Analiza i dimenzioniranje'!O89","v":{"$error":"#VALUE!"}},"XI",{"$f":"+G418","v":3.44},"XII",{"$f":"+'Analiza i dimenzioniranje'!S89","v":0},"XIII",{"$f":"+G418","v":3.44},"XIV",{"$f":"+W418","v":3.44},"XV",{"$f":"+G418","v":3.44},"XVI",{"$f":"+I418","v":3.44},"XVII",{"$f":"+AC418","v":3.44},"XVIII",{"$f":"+AC418","v":3.44},"XIX",{"$f":"+AE418","v":3.44},"XX",{"$f":"+AG418","v":3.44},null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
[null,null,null,null,{"$f":"IF(D418>E$296,D418,E$296)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja"]
[null,null,null,null,{"$f":"IF(AW399>G$298,0,AW399)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"XVIII",{"$f":"+'Analiza i dimenzioniranje'!U188","v":0},"XIX",{"$f":"+'Analiza i dimenzioniranje'!U187","v":0},"XX",{"$f":"'Analiza i dimenzioniranje'!U186","v":0}]
[null,null,null,null,{"$f":"+AW400","v":6.0000000000000009},0,0,{"$f":"+F421","v":0},{"$f":"+G421","v":0},0,0,0,0,0,{"$f":"+M421","v":0},0,{"$f":"+O421","v":0},0,{"$f":"+AS421","v":0},0,{"$f":"+S421","v":0},0,{"$f":"+AS421","v":0},0,{"$f":"+W421","v":0},0,{"$f":"+S421","v":0},0,{"$f":"+AA421","v":0},0,{"$f":"+AU398","v":0},0,{"$f":"+AU398","v":0},0,{"$f":"+AG421","v":0},{"$f":"+AD421","v":0},{"$f":"+AG421","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD459","v":0},{"$f":"+BB421-BC420","v":0},{"$f":"+AD459","v":0},{"$f":"+BD421-BE420","v":0},{"$f":"+AD459","v":0},{"$f":"+'Analiza i dimenzioniranje'!E186","v":0}]
[null,null,null,null,{"$f":"IF(AW401>G$298,0,AW401)","v":0},0,0,0,{"$f":"+G422","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU399","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+AU437","v":14.017600000000002},{"$f":"+AT460","v":0},{"$f":"+BC422","v":14.017600000000002},0,{"$f":"+AE460","v":0}]
[null,null,null,null,null,0,0,{"$f":"+F423","v":0},0,{"$f":"+F421","v":0},0,{"$f":"+D420","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU400","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE461","v":0}]
[null,null,null,null,null,0,0,0,0,{"$f":"+F422","v":0},0,{"$f":"+D421","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU401","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE462","v":0}]
[null,null,null,null,null,0,0,0,0,0,0,{"$f":"+D422","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU402","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE463","v":0}]
[null,null,null,null,null,0,0,0,0,0,0,{"$f":"+D259","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AE425","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE464","v":0}]
[null,null,null,null,null,0,0,0,0,0,0,{"$f":"+D431","v":0.32},0,{"$f":"+J425","v":0},0,{"$f":"+L425","v":0},0,0,0,{"$f":"+P425","v":0},0,0,0,{"$f":"+T425","v":0},0,0,0,{"$f":"+X425","v":0},0,0,{"$f":"+AU404","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+BC427","v":0}]
[null,null,null,null,null,0,0,0,0,0,0,0,0,{"$f":"+J426","v":0},0,{"$f":"+L426","v":0},0,0,0,{"$f":"+P426","v":0},0,0,0,{"$f":"+T426","v":0},0,0,{"$f":"+AA427","v":0},{"$f":"+X426","v":0},0,0,{"$f":"+AU405","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,null,null,0,0,0,{"$f":"+G429","v":0},{"$f":"+F429","v":0},0,0,0,{"$f":"+J427","v":0},0,{"$f":"+N429","v":0},{"$f":"+O429","v":0},0,0,{"$f":"+R429","v":0},{"$f":"+S429","v":0},0,0,{"$f":"+V429","v":0},0,0,{"$f":"+S429","v":0},{"$f":"+Z429","v":0},{"$f":"+AA429","v":0},0,{"$f":"+AU406","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+D389","v":0},{"$f":"IF(AW408>G$298,0,AW408)","v":3.44},{"$f":"+D430","v":0},{"$f":"+AW408","v":3.44},0,{"$f":"+G430","v":3.44},0,{"$f":"+E430","v":3.44},{"$f":"+J430","v":0},{"$f":"+K430","v":3.44},{"$f":"+L430","v":0},{"$f":"+M430","v":3.44},{"$f":"+N430","v":0},{"$f":"+O430","v":3.44},{"$f":"+P430","v":0},{"$f":"+Q430","v":3.44},{"$f":"+R430","v":0},{"$f":"+S430","v":3.44},{"$f":"+T430","v":0},{"$f":"+U430","v":3.44},{"$f":"+V430","v":0},3.44,0,3.44,{"$f":"+Z430","v":0},{"$f":"+AA430","v":3.44},0,{"$f":"+AU407","v":3.44},{"$f":"+AD430","v":0},{"$f":"+AE430","v":3.44},{"$f":"+AF430","v":0},3.44,0,{"$f":"+BC392","v":3.44},null,{"$f":"+D430","v":0},{"$f":"$E$414^2+AM430^2","v":9},{"$f":"$G$413^2+AM430^2","v":16},{"$f":"$G$415^2+AM430^2","v":51.999999999999993},{"$f":"IF(AM430=0,0,$E$410/(PI())*(ATAN(($E$415*$G$413)/(AM430*SQRT(AP430)))-$E$415*$G$413*AM430/(AO430*SQRT(AP430))))","v":0},null,{"$f":"+AM430","v":0},{"$f":"$E$415^2+AS430^2","v":36},{"$f":"$E$414^2+AS430^2","v":9},{"$f":"$G$412^2+AS430^2","v":45.000000000000007},{"$f":"IF(AS430=0,0,($E$410/(PI()))*(ATAN(($E$415*$E$414)/(AS430*SQRT(AV430)))-$E$415*$E$414*AS430/(AU430*SQRT(AV430))))","v":0},{"$f":"(+AQ430-AW430)*2","v":0},null,null,null,0,0,0,0,0,0]
[null,null,null,0.32,3.14,{"$f":"+AX431","v":{"$error":"#VALUE!"}},3.14,{"$error":"#VALUE!"},{"$f":"+G431","v":3.14},{"$error":"#VALUE!"},3.14,{"$f":"+J431","v":{"$error":"#VALUE!"}},{"$f":"+K431","v":3.14},{"$f":"+J431","v":{"$error":"#VALUE!"}},{"$f":"+M431","v":3.14},{"$f":"+L431","v":{"$error":"#VALUE!"}},{"$f":"+O431","v":3.14},{"$f":"+N431","v":{"$error":"#VALUE!"}},{"$f":"+Q431","v":3.14},0,{"$f":"+S431","v":3.14},{"$f":"+T431","v":0},{"$f":"+U431","v":3.14},0,{"$f":"+W431","v":3.14},0,3.14,{"$f":"+Z431","v":0},{"$f":"+AC430","v":3.44},{"$f":"+AB431","v":0},0,{"$f":"+AB431","v":0},{"$f":"+AC431","v":3.44},{"$f":"+AF431","v":0},3.44,0,3.14,null,0.32,{"$f":"$E$414^2+AM431^2","v":9.1023999999999994},{"$f":"$G$413^2+AM431^2","v":16.102399999999999},{"$f":"$G$415^2+AM431^2","v":52.102399999999996},{"$f":"IF(AM431=0,0,$E$410/(PI())*(ATAN(($E$415*$G$413)/(AM431*SQRT(AP431)))-$E$415*$G$413*AM431/(AO431*SQRT(AP431))))","v":{"$error":"#VALUE!"}},null,{"$f":"+AM431","v":0.32},{"$f":"$E$415^2+AS431^2","v":36.102400000000003},{"$f":"$E$414^2+AS431^2","v":9.1023999999999994},{"$f":"$G$412^2+AS431^2","v":45.10240000000001},{"$f":"IF(AS431=0,0,($E$410/(PI()))*(ATAN(($E$415*$E$414)/(AS431*SQRT(AV431)))-$E$415*$E$414*AS431/(AU431*SQRT(AV431))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,0,0,0,0,0,0]
[null,null,null,0.64,2.8,{"$error":"#VALUE!"},2.8,{"$error":"#VALUE!"},2.8,{"$error":"#VALUE!"},2.8,{"$f":"+J432","v":{"$error":"#VALUE!"}},2.8,{"$f":"+J432","v":{"$error":"#VALUE!"}},{"$f":"+M432","v":2.8},{"$f":"+L432","v":{"$error":"#VALUE!"}},{"$f":"+O432","v":2.8},0,{"$f":"+S431","v":3.14},0,0,0,{"$f":"+AS432","v":0.64},0,0,0,3.14,{"$f":"+Z432","v":0},{"$f":"+U432","v":0},{"$f":"+AB432","v":0},0,{"$f":"+AB432","v":0},0,{"$f":"+AF432","v":0},0,0,3.14,null,0.64,9.4095999999999993,16.409600000000001,52.40959999999999,{"$error":"#VALUE!"},null,0.64,36.409599999999998,9.4095999999999993,45.409600000000005,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,0,0,0,0,0]
[null,null,null,0.96,2.48,{"$error":"#VALUE!"},2.48,{"$error":"#VALUE!"},2.48,{"$error":"#VALUE!"},2.48,{"$error":"#VALUE!"},2.48,{"$f":"+J433","v":{"$error":"#VALUE!"}},{"$f":"+M433","v":2.48},0,{"$f":"+Q432","v":2.8},0,{"$f":"+AS433","v":0.96},0,0,0,0.96,0,0,0,0.96,0,0,0,{"$f":"+AU410","v":0.96},0,0,0,0,0,0.96,null,0.96,9.9215999999999998,16.921600000000002,52.921599999999991,{"$error":"#VALUE!"},null,0.96,36.921599999999998,9.9215999999999998,45.921600000000005,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,3.14,0,3.14,0,3.14]
[null,null,null,1.28,2.16,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},2.16,0,{"$f":"+O433","v":2.48},0,0,0,{"$f":"+AS434","v":1.28},0,0,0,1.28,0,0,0,1.28,0,0,0,{"$f":"+AU411","v":1.28},0,0,0,0,0,1.28,null,1.28,10.638400000000001,17.638400000000001,53.63839999999999,{"$error":"#VALUE!"},null,1.28,37.638399999999997,10.638400000000001,46.638400000000004,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,3.14,0,3.14,0,3.14]
[null,null,null,1.6,1.84,{"$error":"#VALUE!"},1.84,{"$error":"#VALUE!"},1.84,{"$error":"#VALUE!"},1.84,0,{"$f":"+M434","v":2.16},0,0,0,0,0,{"$f":"+AS435","v":1.6},0,0,0,1.6,0,0,0,1.6,0,0,0,{"$f":"+AU412","v":1.6},0,0,0,0,0,1.6,null,1.6,11.56,18.560000000000002,54.559999999999995,{"$error":"#VALUE!"},null,1.6,38.56,11.56,47.560000000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,0.64,0,0.64,0,0.64]
[null,null,null,1.9200000000000002,1.52,{"$error":"#VALUE!"},1.52,{"$error":"#VALUE!"},1.52,0,{"$f":"+K435","v":1.84},0,{"$f":"+N436","v":0},0,{"$f":"+AM436","v":1.9200000000000002},0,0,0,{"$f":"+AS436","v":1.9200000000000002},0,0,0,1.9200000000000002,0,0,0,1.9200000000000002,0,0,0,{"$f":"+AE435","v":1.6},0,0,0,0,0,1.9200000000000002,null,1.9200000000000002,12.686400000000001,19.686399999999999,55.686399999999992,{"$error":"#VALUE!"},null,1.9200000000000002,39.686399999999999,12.686400000000001,48.686400000000006,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,0.96,0,0.96,0,0.96]
[null,null,null,2.2400000000000002,1.2,{"$error":"#VALUE!"},1.2,0,{"$f":"+I436","v":1.52},0,{"$f":"+E437","v":1.2},0,{"$f":"+N437","v":0},0,{"$f":"+AM437","v":2.2400000000000002},0,0,0,{"$f":"+AS437","v":2.2400000000000002},0,0,0,2.2400000000000002,0,0,0,2.2400000000000002,0,0,0,{"$f":"+AU414","v":2.2400000000000002},0,0,0,0,0,2.2400000000000002,null,2.2400000000000002,14.017600000000002,21.017600000000002,57.017599999999995,{"$error":"#VALUE!"},null,2.2400000000000002,41.017600000000002,14.017600000000002,50.017600000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,1.28,0,1.28,0,1.28]
[null,null,null,{"$f":"+AW416","v":1.2},null,0,{"$f":"+D438","v":1.2},0,{"$f":"+G438","v":1.2},0,{"$f":"+I438","v":1.2},0,{"$f":"+K438","v":1.2},0,{"$f":"+M438","v":1.2},0,{"$f":"+O438","v":1.2},0,{"$f":"+Q438","v":1.2},0,{"$f":"+S438","v":1.2},0,{"$f":"+U438","v":1.2},0,{"$f":"+W438","v":1.2},{"$f":"+N438","v":0},{"$f":"+Y438","v":1.2},0,{"$f":"+AA438","v":1.2},0,{"$f":"+AC438","v":1.2},0,{"$f":"+AC438","v":1.2},0,1.2,{"$f":"+AD438","v":0},{"$f":"+BC400","v":1.2},null,null,0,{"$f":"+AM438","v":0},0,{"$f":"+AQ437","v":{"$error":"#VALUE!"}},0,{"$f":"+AO438","v":0},0,{"$f":"+S461","v":0},{"$f":"BJ256-BP255","v":0},{"$f":"IF(AV436>AW$299,AV436,AW$299)","v":48.686400000000006},null,null,null,null,{"$f":"+AT474","v":36.921599999999998},1.6,0,1.6,0,1.6]
[null,null,null,{"$f":"+AW417","v":6.2},null,{"$f":"+AV415","v":0},{"$f":"+D439","v":6.2},0,{"$f":"+G439","v":6.2},0,{"$f":"+I439","v":6.2},0,{"$f":"+K439","v":6.2},0,{"$f":"+M439","v":6.2},0,{"$f":"+O439","v":6.2},0,{"$f":"+Q439","v":6.2},0,{"$f":"+S439","v":6.2},0,{"$f":"+U439","v":6.2},0,{"$f":"+W439","v":6.2},{"$f":"+N439","v":0},{"$f":"+Y439","v":6.2},0,{"$f":"+AA439","v":6.2},0,{"$f":"+AC439","v":6.2},0,{"$f":"+AC439","v":6.2},0,6.2,{"$f":"+AD439","v":0},6.2,null,null,0,0,0,{"$f":"+AS439","v":0},0,0,0,0,{"$f":"#REF!-#REF!","v":{"$error":"#REF!"}},{"$f":"+AW440","v":6.0000000000000009},null,null,null,null,{"$f":"+AT475","v":37.638399999999997},1.9200000000000002,{"$f":"+AD475","v":0},1.9200000000000002,0,1.9200000000000002]
[null,null,null,"Ukupni pritisak",null,"SQhi=",{"$f":"+G443","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I443","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K443","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+M443","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+O443","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Q443","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+S443","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+U443","v":0},"SQhi=",{"$f":"+W443","v":0},"SQhi=",{"$f":"+Y443","v":0},"SQhi=",{"$f":"+AA443","v":0},"SQhi=",{"$f":"+AC443","v":0},"SQhi=",{"$f":"+AE443","v":0},"SQhi=",{"$f":"+AG443","v":0},"SQhi=",{"$f":"+AI443","v":0},"SQhi=",{"$f":"+AK443","v":0},null,null,"SQhi=",{"$f":"+AO443","v":17.561600000000013},"SQhi=",{"$f":"+AQ443","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AS443","v":0},"SQhi=",0,{"$f":"BK257-BP256","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$67","v":6.0000000000000009},null,null,null,null,0,1.2,0,{"$f":"+BE439","v":1.9200000000000002},0,{"$f":"+AE478","v":1.2}]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G445","v":{"$error":"#VALUE!"}}," y=",{"$f":"+I445","v":{"$error":"#VALUE!"}}," y=",{"$f":"+K445","v":{"$error":"#VALUE!"}}," y=",{"$f":"+M445","v":{"$error":"#VALUE!"}}," y=",{"$f":"+O445","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Q445","v":{"$error":"#VALUE!"}}," y=",{"$f":"+S445","v":{"$error":"#VALUE!"}}," y=",{"$f":"+U445","v":0}," y=",{"$f":"+W445","v":0}," y=",{"$f":"+Y445","v":0}," y=",{"$f":"+AA445","v":0}," y=",{"$f":"+AC445","v":0}," y=",{"$f":"+AE445","v":0}," y=",{"$f":"+AG445","v":0}," y=",{"$f":"+AI445","v":0}," y=",{"$f":"+AK445","v":0},null,null," y=",{"$f":"+AO445","v":12.3392}," y=",{"$f":"+AQ445","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AS445","v":0}," y=",0,{"$f":"BK258-BQ257","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$66","v":5.6800000000000006},null,null,null,null,0,3.14,0,{"$f":"+AK479","v":3.14},0,{"$f":"+AE479","v":3.14}]
[null,null,null,"krak za presjek III -III",null,"z=",{"$f":"+G441-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I441-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K441-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M441-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+O441-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Q441-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+S441-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+U441-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z=",{"$f":"+W441-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+Y441-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AA441-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AC441-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AE441-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AG441-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AI441-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AK441-'Analiza i dimenzioniranje'!$E$52","v":-1.2},null,null,"z=",{"$f":"+AO441-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":11.8392},"z=",{"$f":"+AQ441-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AS441-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z=",0,{"$f":"AR279-BQ258","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$65","v":5.36},null,null,null,null,"SQhi=",{"$f":"+BC445","v":-4.2872319999999959},"SQhi=",{"$f":"+BE445","v":0}]
[null,null,null,null,null,"F=",{"$f":"-0.5*(+\n (F422*G423-F423*G422)+\n(F423*G424-F424*G423)+\n(F424*G425-F425*G424)+\n(F425*G426-F426*G425)+\n(F426*G427-F427*G426)+\n(F427*G428-F428*G427)+\n(F428*G429-F429*G428)+\n(F429*G430-F430*G429)+\n(F430*G431-F431*G430)+\n(F431*G432-F432*G431)+\n(F432*G433-F433*G432)+\n(F433*G434-F434*G433)+\n(F434*G435-F435*G434)+\n(F435*G436-F436*G435)+\n(F436*G437-F437*G436)+\n(F437*G438-F438*G437)+\n(F438*G439-F439*G438))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (H422*I423-H423*I422)+\n(H423*I424-H424*I423)+\n(H424*I425-H425*I424)+\n(H425*I426-H426*I425)+\n(H426*I427-H427*I426)+\n(H427*I428-H428*I427)+\n(H428*I429-H429*I428)+\n(H429*I430-H430*I429)+\n(H430*I431-H431*I430)+\n(H431*I432-H432*I431)+\n(H432*I433-H433*I432)+\n(H433*I434-H434*I433)+\n(H434*I435-H435*I434)+\n(H435*I436-H436*I435)+\n(H436*I437-H437*I436)+\n(H437*I438-H438*I437)+\n(H438*I439-H439*I438))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((J420*K421-J421*K420)+(J421*K422-J422*K421)+\n (J422*K423-J423*K422)+\n(J423*K424-J424*K423)+\n(J424*K425-J425*K424)+\n(J425*K426-J426*K425)+\n(J426*K427-J427*K426)+\n(J427*K428-J428*K427)+\n(J428*K429-J429*K428)+\n(J429*K430-J430*K429)+\n(J430*K431-J431*K430)+\n(J431*K432-J432*K431)+\n(J432*K433-J433*K432)+\n(J433*K434-J434*K433)+\n(J434*K435-J435*K434)+\n(J435*K436-J436*K435)+\n(J436*K437-J437*K436)+\n(J437*K438-J438*K437)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (L422*M423-L423*M422)+\n(L423*M424-L424*M423)+\n(L424*M425-L425*M424)+\n(L425*M426-L426*M425)+\n(L426*M427-L427*M426)+\n(L427*M428-L428*M427)+\n(L428*M429-L429*M428)+\n(L429*M430-L430*M429)+\n(L430*M431-L431*M430)+\n(L431*M432-L432*M431)+\n(L432*M433-L433*M432)+\n(L433*M434-L434*M433)+\n(L434*M435-L435*M434)+\n(L435*M436-L436*M435)+\n(L436*M437-L437*M436)+\n(L437*M438-L438*M437)+\n(L438*M439-L439*M438))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (N422*O423-N423*O422)+\n(N423*O424-N424*O423)+\n(N424*O425-N425*O424)+\n(N425*O426-N426*O425)+\n(N426*O427-N427*O426)+\n(N427*O428-N428*O427)+\n(N428*O429-N429*O428)+\n(N429*O430-N430*O429)+\n(N430*O431-N431*O430)+\n(N431*O432-N432*O431)+\n(N432*O433-N433*O432)+\n(N433*O434-N434*O433)+\n(N434*O435-N435*O434)+\n(N435*O436-N436*O435)+\n(N436*O437-N437*O436)+\n(N437*O438-N438*O437)+\n(N438*O439-N439*O438))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((P420*Q421-P421*Q420)+(P421*Q422-P422*Q421)+\n (P422*Q423-P423*Q422)+\n(P423*Q424-P424*Q423)+\n(P424*Q425-P425*Q424)+\n(P425*Q426-P426*Q425)+\n(P426*Q427-P427*Q426)+\n(P427*Q428-P428*Q427)+\n(P428*Q429-P429*Q428)+\n(P429*Q430-P430*Q429)+\n(P430*Q431-P431*Q430)+\n(P431*Q432-P432*Q431)+\n(P432*Q433-P433*Q432)+\n(P433*Q434-P434*Q433)+\n(P434*Q435-P435*Q434)+\n(P435*Q436-P436*Q435)+\n(P436*Q437-P437*Q436)+\n(P437*Q438-P438*Q437)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (R422*S423-R423*S422)+\n(R423*S424-R424*S423)+\n(R424*S425-R425*S424)+\n(R425*S426-R426*S425)+\n(R426*S427-R427*S426)+\n(R427*S428-R428*S427)+\n(R428*S429-R429*S428)+\n(R429*S430-R430*S429)+\n(R430*S431-R431*S430)+\n(R431*S432-R432*S431)+\n(R432*S433-R433*S432)+\n(R433*S434-R434*S433)+\n(R434*S435-R435*S434)+\n(R435*S436-R436*S435)+\n(R436*S437-R437*S436)+\n(R437*S438-R438*S437)+\n(R438*S439-R439*S438))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (T422*U423-T423*U422)+\n(T423*U424-T424*U423)+\n(T424*U425-T425*U424)+\n(T425*U426-T426*U425)+\n(T426*U427-T427*U426)+\n(T427*U428-T428*U427)+\n(T428*U429-T429*U428)+\n(T429*U430-T430*U429)+\n(T430*U431-T431*U430)+\n(T431*U432-T432*U431)+\n(T432*U433-T433*U432)+\n(T433*U434-T434*U433)+\n(T434*U435-T435*U434)+\n(T435*U436-T436*U435)+\n(T436*U437-T437*U436)+\n(T437*U438-T438*U437)+\n(T438*U439-T439*U438))","v":0},"F=",{"$f":"-0.5*(+\n (V422*W423-V423*W422)+\n(V423*W424-V424*W423)+\n(V424*W425-V425*W424)+\n(V425*W426-V426*W425)+\n(V426*W427-V427*W426)+\n(V427*W428-V428*W427)+\n(V428*W429-V429*W428)+\n(V429*W430-V430*W429)+\n(V430*W431-V431*W430)+\n(V431*W432-V432*W431)+\n(V432*W433-V433*W432)+\n(V433*W434-V434*W433)+\n(V434*W435-V435*W434)+\n(V435*W436-V436*W435)+\n(V436*W437-V437*W436)+\n(V437*W438-V438*W437)+\n(V438*W439-V439*W438))","v":0},"F=",{"$f":"-0.5*((X420*Y421-X421*Y420)+(X421*Y422-X422*Y421)+\n (X422*Y423-X423*Y422)+\n(X423*Y424-X424*Y423)+\n(X424*Y425-X425*Y424)+\n(X425*Y426-X426*Y425)+\n(X426*Y427-X427*Y426)+\n(X427*Y428-X428*Y427)+\n(X428*Y429-X429*Y428)+\n(X429*Y430-X430*Y429)+\n(X430*Y431-X431*Y430)+\n(X431*Y432-X432*Y431)+\n(X432*Y433-X433*Y432)+\n(X433*Y434-X434*Y433)+\n(X434*Y435-X435*Y434)+\n(X435*Y436-X436*Y435)+\n(X436*Y437-X437*Y436)+\n(X437*Y438-X438*Y437)\n)","v":0},"F=",{"$f":"-0.5*(+\n (Z422*AA423-Z423*AA422)+\n(Z423*AA424-Z424*AA423)+\n(Z424*AA425-Z425*AA424)+\n(Z425*AA426-Z426*AA425)+\n(Z426*AA427-Z427*AA426)+\n(Z427*AA428-Z428*AA427)+\n(Z428*AA429-Z429*AA428)+\n(Z429*AA430-Z430*AA429)+\n(Z430*AA431-Z431*AA430)+\n(Z431*AA432-Z432*AA431)+\n(Z432*AA433-Z433*AA432)+\n(Z433*AA434-Z434*AA433)+\n(Z434*AA435-Z435*AA434)+\n(Z435*AA436-Z436*AA435)+\n(Z436*AA437-Z437*AA436)+\n(Z437*AA438-Z438*AA437)+\n(Z438*AA439-Z439*AA438))","v":0},"F=",{"$f":"-0.5*(+\n (AB422*AC423-AB423*AC422)+\n(AB423*AC424-AB424*AC423)+\n(AB424*AC425-AB425*AC424)+\n(AB425*AC426-AB426*AC425)+\n(AB426*AC427-AB427*AC426)+\n(AB427*AC428-AB428*AC427)+\n(AB428*AC429-AB429*AC428)+\n(AB429*AC430-AB430*AC429)+\n(AB430*AC431-AB431*AC430)+\n(AB431*AC432-AB432*AC431)+\n(AB432*AC433-AB433*AC432)+\n(AB433*AC434-AB434*AC433)+\n(AB434*AC435-AB435*AC434)+\n(AB435*AC436-AB436*AC435)+\n(AB436*AC437-AB437*AC436)+\n(AB437*AC438-AB438*AC437)+\n(AB438*AC439-AB439*AC438))","v":0},"F=",{"$f":"-0.5*(+\n (AD422*AE423-AD423*AE422)+\n(AD423*AE424-AD424*AE423)+\n(AD424*AE425-AD425*AE424)+\n(AD425*AE426-AD426*AE425)+\n(AD426*AE427-AD427*AE426)+\n(AD427*AE428-AD428*AE427)+\n(AD428*AE429-AD429*AE428)+\n(AD429*AE430-AD430*AE429)+\n(AD430*AE431-AD431*AE430)+\n(AD431*AE432-AD432*AE431)+\n(AD432*AE433-AD433*AE432)+\n(AD433*AE434-AD434*AE433)+\n(AD434*AE435-AD435*AE434)+\n(AD435*AE436-AD436*AE435)+\n(AD436*AE437-AD437*AE436)+\n(AD437*AE438-AD438*AE437)+\n(AD438*AE439-AD439*AE438))","v":0},"F=",{"$f":"-0.5*((AF420*AG421-AF421*AG420)+(AF421*AG422-AF422*AG421)+\n (AF422*AG423-AF423*AG422)+\n(AF423*AG424-AF424*AG423)+\n(AF424*AG425-AF425*AG424)+\n(AF425*AG426-AF426*AG425)+\n(AF426*AG427-AF427*AG426)+\n(AF427*AG428-AF428*AG427)+\n(AF428*AG429-AF429*AG428)+\n(AF429*AG430-AF430*AG429)+\n(AF430*AG431-AF431*AG430)+\n(AF431*AG432-AF432*AG431)+\n(AF432*AG433-AF433*AG432)+\n(AF433*AG434-AF434*AG433)+\n(AF434*AG435-AF435*AG434)+\n(AF435*AG436-AF436*AG435)+\n(AF436*AG437-AF437*AG436)+\n(AF437*AG438-AF438*AG437)\n)","v":0},"F=",{"$f":"-0.5*(+\n (AH422*AI423-AH423*AI422)+\n(AH423*AI424-AH424*AI423)+\n(AH424*AI425-AH425*AI424)+\n(AH425*AI426-AH426*AI425)+\n(AH426*AI427-AH427*AI426)+\n(AH427*AI428-AH428*AI427)+\n(AH428*AI429-AH429*AI428)+\n(AH429*AI430-AH430*AI429)+\n(AH430*AI431-AH431*AI430)+\n(AH431*AI432-AH432*AI431)+\n(AH432*AI433-AH433*AI432)+\n(AH433*AI434-AH434*AI433)+\n(AH434*AI435-AH435*AI434)+\n(AH435*AI436-AH436*AI435)+\n(AH436*AI437-AH437*AI436)+\n(AH437*AI438-AH438*AI437)+\n(AH438*AI439-AH439*AI438))","v":0},"F=",{"$f":"-0.5*(+\n (AJ422*AK423-AJ423*AK422)+\n(AJ423*AK424-AJ424*AK423)+\n(AJ424*AK425-AJ425*AK424)+\n(AJ425*AK426-AJ426*AK425)+\n(AJ426*AK427-AJ427*AK426)+\n(AJ427*AK428-AJ428*AK427)+\n(AJ428*AK429-AJ429*AK428)+\n(AJ429*AK430-AJ430*AK429)+\n(AJ430*AK431-AJ431*AK430)+\n(AJ431*AK432-AJ432*AK431)+\n(AJ432*AK433-AJ433*AK432)+\n(AJ433*AK434-AJ434*AK433)+\n(AJ434*AK435-AJ435*AK434)+\n(AJ435*AK436-AJ436*AK435)+\n(AJ436*AK437-AJ437*AK436)+\n(AJ437*AK438-AJ438*AK437)+\n(AJ438*AK439-AJ439*AK438))","v":0},null,null,"F=",{"$f":"-0.5*((AN420*AO421-AN421*AO420)+(AN421*AO422-AN422*AO421)+\n (AN422*AO423-AN423*AO422)+\n(AN423*AO424-AN424*AO423)+\n(AN424*AO425-AN425*AO424)+\n(AN425*AO426-AN426*AO425)+\n(AN426*AO427-AN427*AO426)+\n(AN427*AO428-AN428*AO427)+\n(AN428*AO429-AN429*AO428)+\n(AN429*AO430-AN430*AO429)+\n(AN430*AO431-AN431*AO430)+\n(AN431*AO432-AN432*AO431)+\n(AN432*AO433-AN433*AO432)+\n(AN433*AO434-AN434*AO433)+\n(AN434*AO435-AN435*AO434)+\n(AN435*AO436-AN436*AO435)+\n(AN436*AO437-AN437*AO436)+\n(AN437*AO438-AN438*AO437)\n)","v":17.561600000000013},"F=",{"$f":"-0.5*((AP420*AQ421-AP421*AQ420)+(AP421*AQ422-AP422*AQ421)+\n (AP422*AQ423-AP423*AQ422)+\n(AP423*AQ424-AP424*AQ423)+\n(AP424*AQ425-AP425*AQ424)+\n(AP425*AQ426-AP426*AQ425)+\n(AP426*AQ427-AP427*AQ426)+\n(AP427*AQ428-AP428*AQ427)+\n(AP428*AQ429-AP429*AQ428)+\n(AP429*AQ430-AP430*AQ429)+\n(AP430*AQ431-AP431*AQ430)+\n(AP431*AQ432-AP432*AQ431)+\n(AP432*AQ433-AP433*AQ432)+\n(AP433*AQ434-AP434*AQ433)+\n(AP434*AQ435-AP435*AQ434)+\n(AP435*AQ436-AP436*AQ435)+\n(AP436*AQ437-AP437*AQ436)+\n(AP437*AQ438-AP438*AQ437)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AR420*AS421-AR421*AS420)+(AR421*AS422-AR422*AS421)+\n (AR422*AS423-AR423*AS422)+\n(AR423*AS424-AR424*AS423)+\n(AR424*AS425-AR425*AS424)+\n(AR425*AS426-AR426*AS425)+\n(AR426*AS427-AR427*AS426)+\n(AR427*AS428-AR428*AS427)+\n(AR428*AS429-AR429*AS428)+\n(AR429*AS430-AR430*AS429)+\n(AR430*AS431-AR431*AS430)+\n(AR431*AS432-AR432*AS431)+\n(AR432*AS433-AR433*AS432)+\n(AR433*AS434-AR434*AS433)+\n(AR434*AS435-AR435*AS434)+\n(AR435*AS436-AR436*AS435)+\n(AR436*AS437-AR437*AS436)+\n(AR437*AS438-AR438*AS437)\n)","v":0},"F=",0,{"$f":"AQ259-AW259","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$U$64","v":5.04},null,null,null,null," y=",{"$f":"+BC447","v":1.6468223164347855}," y=",{"$f":"+BE447","v":0}]
[null,null,null,null,null,"x=",2.5,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,null,null,"x=",0,"x=",0,"x=",0,"x=",0,0,{"$f":"'Analiza i dimenzioniranje'!$U$63","v":4.72},null,null,null,null,"z=",{"$f":"+BC443-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":1.1468223164347855},"z=",{"$f":"+BE443-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5}]
[null,null,null,"y=",null,"y=",{"$f":"+IF(G443=0,0,-((F420*G421-F421*G420)*(G420+G421)+(F421*G422-F422*G421)*(G421+G422)+\n(F422*G423-F423*G422)*(G422+G423)+\n(F423*G424-F424*G423)*(G423+G424)+\n(F424*G425-F425*G424)*(G424+G425)+\n(F425*G426-F426*G425)*(G425+G426)+\n(F426*G427-F427*G426)*(G426+G427)+\n(F427*G428-F428*G427)*(G427+G428)+\n(F428*G429-F429*G428)*(G428+G429)+\n(F429*G430-F430*G429)*(G429+G430)+\n(F430*G431-F431*G430)*(G430+G431)+\n(F431*G432-F432*G431)*(G431+G432)+\n(F432*G433-F433*G432)*(G432+G433)+\n(F433*G434-F434*G433)*(G433+G434)+\n(F434*G435-F435*G434)*(G434+G435)+\n(F435*G436-F436*G435)*(G435+G436)+\n(F436*G437-F437*G436)*(G436+G437)+\n(F437*G438-F438*G437)*(G437+G438)+\n(F438*G439-F439*G438)*(G438+G439))/6/G443)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(I443=0,0,-((H420*I421-H421*I420)*(I420+I421)+(H421*I422-H422*I421)*(I421+I422)+\n(H422*I423-H423*I422)*(I422+I423)+\n(H423*I424-H424*I423)*(I423+I424)+\n(H424*I425-H425*I424)*(I424+I425)+\n(H425*I426-H426*I425)*(I425+I426)+\n(H426*I427-H427*I426)*(I426+I427)+\n(H427*I428-H428*I427)*(I427+I428)+\n(H428*I429-H429*I428)*(I428+I429)+\n(H429*I430-H430*I429)*(I429+I430)+\n(H430*I431-H431*I430)*(I430+I431)+\n(H431*I432-H432*I431)*(I431+I432)+\n(H432*I433-H433*I432)*(I432+I433)+\n(H433*I434-H434*I433)*(I433+I434)+\n(H434*I435-H435*I434)*(I434+I435)+\n(H435*I436-H436*I435)*(I435+I436)+\n(H436*I437-H437*I436)*(I436+I437)+\n(H437*I438-H438*I437)*(I437+I438)+\n(H438*I439-H439*I438)*(I438+I439))/6/I443)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(K443=0,0,-((J420*K421-J421*K420)*(K420+K421)+(J421*K422-J422*K421)*(K421+K422)+\n(J422*K423-J423*K422)*(K422+K423)+\n(J423*K424-J424*K423)*(K423+K424)+\n(J424*K425-J425*K424)*(K424+K425)+\n(J425*K426-J426*K425)*(K425+K426)+\n(J426*K427-J427*K426)*(K426+K427)+\n(J427*K428-J428*K427)*(K427+K428)+\n(J428*K429-J429*K428)*(K428+K429)+\n(J429*K430-J430*K429)*(K429+K430)+\n(J430*K431-J431*K430)*(K430+K431)+\n(J431*K432-J432*K431)*(K431+K432)+\n(J432*K433-J433*K432)*(K432+K433)+\n(J433*K434-J434*K433)*(K433+K434)+\n(J434*K435-J435*K434)*(K434+K435)+\n(J435*K436-J436*K435)*(K435+K436)+\n(J436*K437-J437*K436)*(K436+K437)+\n(J437*K438-J438*K437)*(K437+K438)+\n(J438*K439-J439*K438)*(K438+K439))/6/K443)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(M443=0,0,-((L420*M421-L421*M420)*(M420+M421)+(L421*M422-L422*M421)*(M421+M422)+\n(L422*M423-L423*M422)*(M422+M423)+\n(L423*M424-L424*M423)*(M423+M424)+\n(L424*M425-L425*M424)*(M424+M425)+\n(L425*M426-L426*M425)*(M425+M426)+\n(L426*M427-L427*M426)*(M426+M427)+\n(L427*M428-L428*M427)*(M427+M428)+\n(L428*M429-L429*M428)*(M428+M429)+\n(L429*M430-L430*M429)*(M429+M430)+\n(L430*M431-L431*M430)*(M430+M431)+\n(L431*M432-L432*M431)*(M431+M432)+\n(L432*M433-L433*M432)*(M432+M433)+\n(L433*M434-L434*M433)*(M433+M434)+\n(L434*M435-L435*M434)*(M434+M435)+\n(L435*M436-L436*M435)*(M435+M436)+\n(L436*M437-L437*M436)*(M436+M437)+\n(L437*M438-L438*M437)*(M437+M438)+\n(L438*M439-L439*M438)*(M438+M439))/6/M443)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(O443=0,0,-((N420*O421-N421*O420)*(O420+O421)+(N421*O422-N422*O421)*(O421+O422)+\n(N422*O423-N423*O422)*(O422+O423)+\n(N423*O424-N424*O423)*(O423+O424)+\n(N424*O425-N425*O424)*(O424+O425)+\n(N425*O426-N426*O425)*(O425+O426)+\n(N426*O427-N427*O426)*(O426+O427)+\n(N427*O428-N428*O427)*(O427+O428)+\n(N428*O429-N429*O428)*(O428+O429)+\n(N429*O430-N430*O429)*(O429+O430)+\n(N430*O431-N431*O430)*(O430+O431)+\n(N431*O432-N432*O431)*(O431+O432)+\n(N432*O433-N433*O432)*(O432+O433)+\n(N433*O434-N434*O433)*(O433+O434)+\n(N434*O435-N435*O434)*(O434+O435)+\n(N435*O436-N436*O435)*(O435+O436)+\n(N436*O437-N437*O436)*(O436+O437)+\n(N437*O438-N438*O437)*(O437+O438)+\n(N438*O439-N439*O438)*(O438+O439))/6/O443)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Q443=0,0,-((P420*Q421-P421*Q420)*(Q420+Q421)+(P421*Q422-P422*Q421)*(Q421+Q422)+\n(P422*Q423-P423*Q422)*(Q422+Q423)+\n(P423*Q424-P424*Q423)*(Q423+Q424)+\n(P424*Q425-P425*Q424)*(Q424+Q425)+\n(P425*Q426-P426*Q425)*(Q425+Q426)+\n(P426*Q427-P427*Q426)*(Q426+Q427)+\n(P427*Q428-P428*Q427)*(Q427+Q428)+\n(P428*Q429-P429*Q428)*(Q428+Q429)+\n(P429*Q430-P430*Q429)*(Q429+Q430)+\n(P430*Q431-P431*Q430)*(Q430+Q431)+\n(P431*Q432-P432*Q431)*(Q431+Q432)+\n(P432*Q433-P433*Q432)*(Q432+Q433)+\n(P433*Q434-P434*Q433)*(Q433+Q434)+\n(P434*Q435-P435*Q434)*(Q434+Q435)+\n(P435*Q436-P436*Q435)*(Q435+Q436)+\n(P436*Q437-P437*Q436)*(Q436+Q437)+\n(P437*Q438-P438*Q437)*(Q437+Q438)+\n(P438*Q439-P439*Q438)*(Q438+Q439))/6/Q443)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(S443=0,0,-((R420*S421-R421*S420)*(S420+S421)+(R421*S422-R422*S421)*(S421+S422)+\n(R422*S423-R423*S422)*(S422+S423)+\n(R423*S424-R424*S423)*(S423+S424)+\n(R424*S425-R425*S424)*(S424+S425)+\n(R425*S426-R426*S425)*(S425+S426)+\n(R426*S427-R427*S426)*(S426+S427)+\n(R427*S428-R428*S427)*(S427+S428)+\n(R428*S429-R429*S428)*(S428+S429)+\n(R429*S430-R430*S429)*(S429+S430)+\n(R430*S431-R431*S430)*(S430+S431)+\n(R431*S432-R432*S431)*(S431+S432)+\n(R432*S433-R433*S432)*(S432+S433)+\n(R433*S434-R434*S433)*(S433+S434)+\n(R434*S435-R435*S434)*(S434+S435)+\n(R435*S436-R436*S435)*(S435+S436)+\n(R436*S437-R437*S436)*(S436+S437)+\n(R437*S438-R438*S437)*(S437+S438)+\n(R438*S439-R439*S438)*(S438+S439))/6/S443)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(U443=0,0,-((T420*U421-T421*U420)*(U420+U421)+(T421*U422-T422*U421)*(U421+U422)+\n(T422*U423-T423*U422)*(U422+U423)+\n(T423*U424-T424*U423)*(U423+U424)+\n(T424*U425-T425*U424)*(U424+U425)+\n(T425*U426-T426*U425)*(U425+U426)+\n(T426*U427-T427*U426)*(U426+U427)+\n(T427*U428-T428*U427)*(U427+U428)+\n(T428*U429-T429*U428)*(U428+U429)+\n(T429*U430-T430*U429)*(U429+U430)+\n(T430*U431-T431*U430)*(U430+U431)+\n(T431*U432-T432*U431)*(U431+U432)+\n(T432*U433-T433*U432)*(U432+U433)+\n(T433*U434-T434*U433)*(U433+U434)+\n(T434*U435-T435*U434)*(U434+U435)+\n(T435*U436-T436*U435)*(U435+U436)+\n(T436*U437-T437*U436)*(U436+U437)+\n(T437*U438-T438*U437)*(U437+U438)+\n(T438*U439-T439*U438)*(U438+U439))/6/U443)","v":0},"y=",{"$f":"+IF(W443=0,0,-((V420*W421-V421*W420)*(W420+W421)+(V421*W422-V422*W421)*(W421+W422)+\n(V422*W423-V423*W422)*(W422+W423)+\n(V423*W424-V424*W423)*(W423+W424)+\n(V424*W425-V425*W424)*(W424+W425)+\n(V425*W426-V426*W425)*(W425+W426)+\n(V426*W427-V427*W426)*(W426+W427)+\n(V427*W428-V428*W427)*(W427+W428)+\n(V428*W429-V429*W428)*(W428+W429)+\n(V429*W430-V430*W429)*(W429+W430)+\n(V430*W431-V431*W430)*(W430+W431)+\n(V431*W432-V432*W431)*(W431+W432)+\n(V432*W433-V433*W432)*(W432+W433)+\n(V433*W434-V434*W433)*(W433+W434)+\n(V434*W435-V435*W434)*(W434+W435)+\n(V435*W436-V436*W435)*(W435+W436)+\n(V436*W437-V437*W436)*(W436+W437)+\n(V437*W438-V438*W437)*(W437+W438)+\n(V438*W439-V439*W438)*(W438+W439))/6/W443)","v":0},"y=",{"$f":"+IF(Y443=0,0,-((X420*Y421-X421*Y420)*(Y420+Y421)+(X421*Y422-X422*Y421)*(Y421+Y422)+\n(X422*Y423-X423*Y422)*(Y422+Y423)+\n(X423*Y424-X424*Y423)*(Y423+Y424)+\n(X424*Y425-X425*Y424)*(Y424+Y425)+\n(X425*Y426-X426*Y425)*(Y425+Y426)+\n(X426*Y427-X427*Y426)*(Y426+Y427)+\n(X427*Y428-X428*Y427)*(Y427+Y428)+\n(X428*Y429-X429*Y428)*(Y428+Y429)+\n(X429*Y430-X430*Y429)*(Y429+Y430)+\n(X430*Y431-X431*Y430)*(Y430+Y431)+\n(X431*Y432-X432*Y431)*(Y431+Y432)+\n(X432*Y433-X433*Y432)*(Y432+Y433)+\n(X433*Y434-X434*Y433)*(Y433+Y434)+\n(X434*Y435-X435*Y434)*(Y434+Y435)+\n(X435*Y436-X436*Y435)*(Y435+Y436)+\n(X436*Y437-X437*Y436)*(Y436+Y437)+\n(X437*Y438-X438*Y437)*(Y437+Y438)+\n(X438*Y439-X439*Y438)*(Y438+Y439))/6/Y443)","v":0},"y=",{"$f":"+IF(AA443=0,0,-((Z420*AA421-Z421*AA420)*(AA420+AA421)+(Z421*AA422-Z422*AA421)*(AA421+AA422)+\n(Z422*AA423-Z423*AA422)*(AA422+AA423)+\n(Z423*AA424-Z424*AA423)*(AA423+AA424)+\n(Z424*AA425-Z425*AA424)*(AA424+AA425)+\n(Z425*AA426-Z426*AA425)*(AA425+AA426)+\n(Z426*AA427-Z427*AA426)*(AA426+AA427)+\n(Z427*AA428-Z428*AA427)*(AA427+AA428)+\n(Z428*AA429-Z429*AA428)*(AA428+AA429)+\n(Z429*AA430-Z430*AA429)*(AA429+AA430)+\n(Z430*AA431-Z431*AA430)*(AA430+AA431)+\n(Z431*AA432-Z432*AA431)*(AA431+AA432)+\n(Z432*AA433-Z433*AA432)*(AA432+AA433)+\n(Z433*AA434-Z434*AA433)*(AA433+AA434)+\n(Z434*AA435-Z435*AA434)*(AA434+AA435)+\n(Z435*AA436-Z436*AA435)*(AA435+AA436)+\n(Z436*AA437-Z437*AA436)*(AA436+AA437)+\n(Z437*AA438-Z438*AA437)*(AA437+AA438)+\n(Z438*AA439-Z439*AA438)*(AA438+AA439))/6/AA443)","v":0},"y=",{"$f":"+IF(AC443=0,0,-((AB420*AC421-AB421*AC420)*(AC420+AC421)+(AB421*AC422-AB422*AC421)*(AC421+AC422)+\n(AB422*AC423-AB423*AC422)*(AC422+AC423)+\n(AB423*AC424-AB424*AC423)*(AC423+AC424)+\n(AB424*AC425-AB425*AC424)*(AC424+AC425)+\n(AB425*AC426-AB426*AC425)*(AC425+AC426)+\n(AB426*AC427-AB427*AC426)*(AC426+AC427)+\n(AB427*AC428-AB428*AC427)*(AC427+AC428)+\n(AB428*AC429-AB429*AC428)*(AC428+AC429)+\n(AB429*AC430-AB430*AC429)*(AC429+AC430)+\n(AB430*AC431-AB431*AC430)*(AC430+AC431)+\n(AB431*AC432-AB432*AC431)*(AC431+AC432)+\n(AB432*AC433-AB433*AC432)*(AC432+AC433)+\n(AB433*AC434-AB434*AC433)*(AC433+AC434)+\n(AB434*AC435-AB435*AC434)*(AC434+AC435)+\n(AB435*AC436-AB436*AC435)*(AC435+AC436)+\n(AB436*AC437-AB437*AC436)*(AC436+AC437)+\n(AB437*AC438-AB438*AC437)*(AC437+AC438)+\n(AB438*AC439-AB439*AC438)*(AC438+AC439))/6/AC443)","v":0},"y=",{"$f":"+IF(AE443=0,0,-((AD420*AE421-AD421*AE420)*(AE420+AE421)+(AD421*AE422-AD422*AE421)*(AE421+AE422)+\n(AD422*AE423-AD423*AE422)*(AE422+AE423)+\n(AD423*AE424-AD424*AE423)*(AE423+AE424)+\n(AD424*AE425-AD425*AE424)*(AE424+AE425)+\n(AD425*AE426-AD426*AE425)*(AE425+AE426)+\n(AD426*AE427-AD427*AE426)*(AE426+AE427)+\n(AD427*AE428-AD428*AE427)*(AE427+AE428)+\n(AD428*AE429-AD429*AE428)*(AE428+AE429)+\n(AD429*AE430-AD430*AE429)*(AE429+AE430)+\n(AD430*AE431-AD431*AE430)*(AE430+AE431)+\n(AD431*AE432-AD432*AE431)*(AE431+AE432)+\n(AD432*AE433-AD433*AE432)*(AE432+AE433)+\n(AD433*AE434-AD434*AE433)*(AE433+AE434)+\n(AD434*AE435-AD435*AE434)*(AE434+AE435)+\n(AD435*AE436-AD436*AE435)*(AE435+AE436)+\n(AD436*AE437-AD437*AE436)*(AE436+AE437)+\n(AD437*AE438-AD438*AE437)*(AE437+AE438)+\n(AD438*AE439-AD439*AE438)*(AE438+AE439))/6/AE443)","v":0},"y=",{"$f":"+IF(AG443=0,0,-((AF420*AG421-AF421*AG420)*(AG420+AG421)+(AF421*AG422-AF422*AG421)*(AG421+AG422)+\n(AF422*AG423-AF423*AG422)*(AG422+AG423)+\n(AF423*AG424-AF424*AG423)*(AG423+AG424)+\n(AF424*AG425-AF425*AG424)*(AG424+AG425)+\n(AF425*AG426-AF426*AG425)*(AG425+AG426)+\n(AF426*AG427-AF427*AG426)*(AG426+AG427)+\n(AF427*AG428-AF428*AG427)*(AG427+AG428)+\n(AF428*AG429-AF429*AG428)*(AG428+AG429)+\n(AF429*AG430-AF430*AG429)*(AG429+AG430)+\n(AF430*AG431-AF431*AG430)*(AG430+AG431)+\n(AF431*AG432-AF432*AG431)*(AG431+AG432)+\n(AF432*AG433-AF433*AG432)*(AG432+AG433)+\n(AF433*AG434-AF434*AG433)*(AG433+AG434)+\n(AF434*AG435-AF435*AG434)*(AG434+AG435)+\n(AF435*AG436-AF436*AG435)*(AG435+AG436)+\n(AF436*AG437-AF437*AG436)*(AG436+AG437)+\n(AF437*AG438-AF438*AG437)*(AG437+AG438)+\n(AF438*AG439-AF439*AG438)*(AG438+AG439))/6/AG443)","v":0},"y=",{"$f":"+IF(AI443=0,0,-((AH420*AI421-AH421*AI420)*(AI420+AI421)+(AH421*AI422-AH422*AI421)*(AI421+AI422)+\n(AH422*AI423-AH423*AI422)*(AI422+AI423)+\n(AH423*AI424-AH424*AI423)*(AI423+AI424)+\n(AH424*AI425-AH425*AI424)*(AI424+AI425)+\n(AH425*AI426-AH426*AI425)*(AI425+AI426)+\n(AH426*AI427-AH427*AI426)*(AI426+AI427)+\n(AH427*AI428-AH428*AI427)*(AI427+AI428)+\n(AH428*AI429-AH429*AI428)*(AI428+AI429)+\n(AH429*AI430-AH430*AI429)*(AI429+AI430)+\n(AH430*AI431-AH431*AI430)*(AI430+AI431)+\n(AH431*AI432-AH432*AI431)*(AI431+AI432)+\n(AH432*AI433-AH433*AI432)*(AI432+AI433)+\n(AH433*AI434-AH434*AI433)*(AI433+AI434)+\n(AH434*AI435-AH435*AI434)*(AI434+AI435)+\n(AH435*AI436-AH436*AI435)*(AI435+AI436)+\n(AH436*AI437-AH437*AI436)*(AI436+AI437)+\n(AH437*AI438-AH438*AI437)*(AI437+AI438)+\n(AH438*AI439-AH439*AI438)*(AI438+AI439))/6/AI443)","v":0},"y=",{"$f":"+IF(AK443=0,0,-((AJ420*AK421-AJ421*AK420)*(AK420+AK421)+(AJ421*AK422-AJ422*AK421)*(AK421+AK422)+\n(AJ422*AK423-AJ423*AK422)*(AK422+AK423)+\n(AJ423*AK424-AJ424*AK423)*(AK423+AK424)+\n(AJ424*AK425-AJ425*AK424)*(AK424+AK425)+\n(AJ425*AK426-AJ426*AK425)*(AK425+AK426)+\n(AJ426*AK427-AJ427*AK426)*(AK426+AK427)+\n(AJ427*AK428-AJ428*AK427)*(AK427+AK428)+\n(AJ428*AK429-AJ429*AK428)*(AK428+AK429)+\n(AJ429*AK430-AJ430*AK429)*(AK429+AK430)+\n(AJ430*AK431-AJ431*AK430)*(AK430+AK431)+\n(AJ431*AK432-AJ432*AK431)*(AK431+AK432)+\n(AJ432*AK433-AJ433*AK432)*(AK432+AK433)+\n(AJ433*AK434-AJ434*AK433)*(AK433+AK434)+\n(AJ434*AK435-AJ435*AK434)*(AK434+AK435)+\n(AJ435*AK436-AJ436*AK435)*(AK435+AK436)+\n(AJ436*AK437-AJ437*AK436)*(AK436+AK437)+\n(AJ437*AK438-AJ438*AK437)*(AK437+AK438)+\n(AJ438*AK439-AJ439*AK438)*(AK438+AK439))/6/AK443)","v":0},null,null,"y=",{"$f":"+IF(AO443=0,0,-((AN420*AO421-AN421*AO420)*(AO420+AO421)+(AN421*AO422-AN422*AO421)*(AO421+AO422)+\n(AN422*AO423-AN423*AO422)*(AO422+AO423)+\n(AN423*AO424-AN424*AO423)*(AO423+AO424)+\n(AN424*AO425-AN425*AO424)*(AO424+AO425)+\n(AN425*AO426-AN426*AO425)*(AO425+AO426)+\n(AN426*AO427-AN427*AO426)*(AO426+AO427)+\n(AN427*AO428-AN428*AO427)*(AO427+AO428)+\n(AN428*AO429-AN429*AO428)*(AO428+AO429)+\n(AN429*AO430-AN430*AO429)*(AO429+AO430)+\n(AN430*AO431-AN431*AO430)*(AO430+AO431)+\n(AN431*AO432-AN432*AO431)*(AO431+AO432)+\n(AN432*AO433-AN433*AO432)*(AO432+AO433)+\n(AN433*AO434-AN434*AO433)*(AO433+AO434)+\n(AN434*AO435-AN435*AO434)*(AO434+AO435)+\n(AN435*AO436-AN436*AO435)*(AO435+AO436)+\n(AN436*AO437-AN437*AO436)*(AO436+AO437)+\n(AN437*AO438-AN438*AO437)*(AO437+AO438)+\n(AN438*AO439-AN439*AO438)*(AO438+AO439))/6/AO443)","v":12.3392},"y=",{"$f":"+IF(AQ443=0,0,-((AP420*AQ421-AP421*AQ420)*(AQ420+AQ421)+(AP421*AQ422-AP422*AQ421)*(AQ421+AQ422)+\n(AP422*AQ423-AP423*AQ422)*(AQ422+AQ423)+\n(AP423*AQ424-AP424*AQ423)*(AQ423+AQ424)+\n(AP424*AQ425-AP425*AQ424)*(AQ424+AQ425)+\n(AP425*AQ426-AP426*AQ425)*(AQ425+AQ426)+\n(AP426*AQ427-AP427*AQ426)*(AQ426+AQ427)+\n(AP427*AQ428-AP428*AQ427)*(AQ427+AQ428)+\n(AP428*AQ429-AP429*AQ428)*(AQ428+AQ429)+\n(AP429*AQ430-AP430*AQ429)*(AQ429+AQ430)+\n(AP430*AQ431-AP431*AQ430)*(AQ430+AQ431)+\n(AP431*AQ432-AP432*AQ431)*(AQ431+AQ432)+\n(AP432*AQ433-AP433*AQ432)*(AQ432+AQ433)+\n(AP433*AQ434-AP434*AQ433)*(AQ433+AQ434)+\n(AP434*AQ435-AP435*AQ434)*(AQ434+AQ435)+\n(AP435*AQ436-AP436*AQ435)*(AQ435+AQ436)+\n(AP436*AQ437-AP437*AQ436)*(AQ436+AQ437)+\n(AP437*AQ438-AP438*AQ437)*(AQ437+AQ438)+\n(AP438*AQ439-AP439*AQ438)*(AQ438+AQ439))/6/AQ443)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AS443=0,0,-((AR420*AS421-AR421*AS420)*(AS420+AS421)+(AR421*AS422-AR422*AS421)*(AS421+AS422)+\n(AR422*AS423-AR423*AS422)*(AS422+AS423)+\n(AR423*AS424-AR424*AS423)*(AS423+AS424)+\n(AR424*AS425-AR425*AS424)*(AS424+AS425)+\n(AR425*AS426-AR426*AS425)*(AS425+AS426)+\n(AR426*AS427-AR427*AS426)*(AS426+AS427)+\n(AR427*AS428-AR428*AS427)*(AS427+AS428)+\n(AR428*AS429-AR429*AS428)*(AS428+AS429)+\n(AR429*AS430-AR430*AS429)*(AS429+AS430)+\n(AR430*AS431-AR431*AS430)*(AS430+AS431)+\n(AR431*AS432-AR432*AS431)*(AS431+AS432)+\n(AR432*AS433-AR433*AS432)*(AS432+AS433)+\n(AR433*AS434-AR434*AS433)*(AS433+AS434)+\n(AR434*AS435-AR435*AS434)*(AS434+AS435)+\n(AR435*AS436-AR436*AS435)*(AS435+AS436)+\n(AR436*AS437-AR437*AS436)*(AS436+AS437)+\n(AR437*AS438-AR438*AS437)*(AS437+AS438)+\n(AR438*AS439-AR439*AS438)*(AS438+AS439))/6/AS443)","v":0},"y=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$62","v":4.4000000000000004},null,null,null,null,"F=",{"$f":"-0.5*((BB422*BC423-BB423*BC422)+(BB423*BC424-BB424*BC423)+\n (BB424*BC425-BB425*BC424)+\n(BB425*BC426-BB426*BC425)+\n(BB426*BC427-BB427*BC426)+\n(BB427*BC428-BB428*BC427)+\n(BB428*BC429-BB429*BC428)+\n(BB429*BC430-BB430*BC429)+\n(BB430*BC431-BB431*BC430)+\n(BB431*BC432-BB432*BC431)+\n(BB432*BC433-BB433*BC432)+\n(BB433*BC434-BB434*BC433)+\n(BB434*BC435-BB435*BC434)+\n(BB435*BC436-BB436*BC435)+\n(BB436*BC437-BB437*BC436)+\n(BB437*BC438-BB438*BC437)+\n(BB438*BC439-BB439*BC438)+\n(BB439*BC440-BB440*BC439)\n)","v":-4.2872319999999959},"F=",{"$f":"-0.5*((BD422*BE423-BD423*BE422)+(BD423*BE424-BD424*BE423)+\n (BD424*BE425-BD425*BE424)+\n(BD425*BE426-BD426*BE425)+\n(BD426*BE427-BD427*BE426)+\n(BD427*BE428-BD428*BE427)+\n(BD428*BE429-BD429*BE428)+\n(BD429*BE430-BD430*BE429)+\n(BD430*BE431-BD431*BE430)+\n(BD431*BE432-BD432*BE431)+\n(BD432*BE433-BD433*BE432)+\n(BD433*BE434-BD434*BE433)+\n(BD434*BE435-BD435*BE434)+\n(BD435*BE436-BD436*BE435)+\n(BD436*BE437-BD437*BE436)+\n(BD437*BE438-BD438*BE437)+\n(BD438*BE439-BD439*BE438)+\n(BD439*BE440-BD440*BE439)\n)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$61","v":4.08},null,null,null,null,"x=",0,"x=",0]
[null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$60","v":3.76},null,null,null,null,"y=",{"$f":"+IF(BC445=0,0,-((BB422*BC423-BB423*BC422)*(BC422+BC423)+(BB423*BC424-BB424*BC423)*(BC423+BC424)+\n(BB424*BC425-BB425*BC424)*(BC424+BC425)+\n(BB425*BC426-BB426*BC425)*(BC425+BC426)+\n(BB426*BC427-BB427*BC426)*(BC426+BC427)+\n(BB427*BC428-BB428*BC427)*(BC427+BC428)+\n(BB428*BC429-BB429*BC428)*(BC428+BC429)+\n(BB429*BC430-BB430*BC429)*(BC429+BC430)+\n(BB430*BC431-BB431*BC430)*(BC430+BC431)+\n(BB431*BC432-BB432*BC431)*(BC431+BC432)+\n(BB432*BC433-BB433*BC432)*(BC432+BC433)+\n(BB433*BC434-BB434*BC433)*(BC433+BC434)+\n(BB434*BC435-BB435*BC434)*(BC434+BC435)+\n(BB435*BC436-BB436*BC435)*(BC435+BC436)+\n(BB436*BC437-BB437*BC436)*(BC436+BC437)+\n(BB437*BC438-BB438*BC437)*(BC437+BC438)+\n(BB438*BC439-BB439*BC438)*(BC438+BC439)+\n(BB439*BC440-BB440*BC439)*(BC439+BC440)+\n(BB440*BC441-BB441*BC440)*(BC440+BC441))/6/BC445)","v":1.6468223164347855},"y=",{"$f":"+IF(BE445=0,0,-((BD422*BE423-BD423*BE422)*(BE422+BE423)+(BD423*BE424-BD424*BE423)*(BE423+BE424)+\n(BD424*BE425-BD425*BE424)*(BE424+BE425)+\n(BD425*BE426-BD426*BE425)*(BE425+BE426)+\n(BD426*BE427-BD427*BE426)*(BE426+BE427)+\n(BD427*BE428-BD428*BE427)*(BE427+BE428)+\n(BD428*BE429-BD429*BE428)*(BE428+BE429)+\n(BD429*BE430-BD430*BE429)*(BE429+BE430)+\n(BD430*BE431-BD431*BE430)*(BE430+BE431)+\n(BD431*BE432-BD432*BE431)*(BE431+BE432)+\n(BD432*BE433-BD433*BE432)*(BE432+BE433)+\n(BD433*BE434-BD434*BE433)*(BE433+BE434)+\n(BD434*BE435-BD435*BE434)*(BE434+BE435)+\n(BD435*BE436-BD436*BE435)*(BE435+BE436)+\n(BD436*BE437-BD437*BE436)*(BE436+BE437)+\n(BD437*BE438-BD438*BE437)*(BE437+BE438)+\n(BD438*BE439-BD439*BE438)*(BE438+BE439)+\n(BD439*BE440-BD440*BE439)*(BE439+BE440)+\n(BD440*BE441-BD441*BE440)*(BE440+BE441))/6/BE445)","v":0}]
[null,"OPTEREĆENJE TEMELJEM",null,null,null,null,null,null,null," (TERZAGHY)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.14,0,{"$f":"+'Analiza i dimenzioniranje'!$U$59","v":3.44}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.14,0,{"$f":"+'Analiza i dimenzioniranje'!$U$58","v":3.14}]
[null,"KONTINUIRANO OPTEREĆENJE",null,"P - D=",{"$f":"IF('Analiza i dimenzioniranje'!$E$28-I450<=0,0,+'Analiza i dimenzioniranje'!$E$28-I450)","v":{"$error":"#VALUE!"}},"kN/m2","raster. iskopom   D=y*Df =",null,{"$f":"+'Analiza i dimenzioniranje'!$D$16*('Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20-D456)","v":{"$error":"#VALUE!"}},"kN/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.64,0,{"$f":"+'Analiza i dimenzioniranje'!$U$57","v":2.8}]
[null," visina zida i temelja",null,"H =",{"$f":"+E411","v":{"$error":"#VALUE!"}},"m",{"$f":"E455","v":6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.96,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$56","v":2.48}]
[null,"visina opterećenja iznad vrha zida",null,"h =",{"$f":"+E412","v":-1},"m",{"$f":"SQRT(E455^2+E454^2)","v":6.7082039324993694},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.28,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$55","v":2.16}]
[null,"širina temelja",null,"b =",{"$f":"+E413","v":1},"m   ",{"$f":"E454+E453","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$54","v":1.84}]
[null,"udaljenost temelja od zida",null,"D =",{"$f":"+E414","v":3},"m    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.9200000000000002,{"$error":"#VALUE!"},{"$f":"+'Analiza i dimenzioniranje'!$U$53","v":1.52}]
[null,"1/2 dužine temelja",null,"L/2=a=",{"$f":"+E415","v":6},"m",{"$f":"SQRT(G451^2+G453^2)","v":7.2111025509279782},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,0,{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
["DNO TEMELJA NA VISINI","PRESJEK NA Visini ",null,{"$f":"+ROUND('Analiza i dimenzioniranje'!U58,2)","v":3.14},null,"Presjek III -III",null,"Presjek VI",null,"Presjek VII-VII",null,"Presjek VIII-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"Presjek XIV-XIV",null,"Presjek XV-XV",null,"PresjekXVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX",null,null,null,null,null,null,null,null,null,null,3.14,{"$f":"+IF(AW457>=AW$299,0,AQ272-AW272)","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
[null,null,null,null,null,"Visina djelovanja","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja ","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja",null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2",{"$f":"+AU460","v":0},"SQhi=",6.2]
[null,null,null,{"$f":"+F459","v":0},{"$f":"+D458-E456","v":0},"III",{"$f":"+D456","v":3.14},"IV",{"$f":"+G458","v":3.14},"VII",{"$f":"+G458","v":3.14},"VIII",{"$f":"+I458","v":3.14},"IX",{"$f":"+G458","v":3.14},"X",{"$f":"+'Analiza i dimenzioniranje'!O87","v":{"$error":"#VALUE!"}},"XI",{"$f":"+G458","v":3.14},"XII",{"$f":"+'Analiza i dimenzioniranje'!S87","v":0},"XIII",{"$f":"+G458","v":3.14},"XIV",{"$f":"+W458","v":3.14},"XV",{"$f":"+G458","v":3.14},"XVI",{"$f":"+I458","v":3.14},"XVII",{"$f":"+AC458","v":3.14},"XVIII",{"$f":"+AC458","v":3.14},"XIX",{"$f":"+AE458","v":3.14},"XX",{"$f":"+AG458","v":3.14},null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
[null,null,null,0,{"$f":"IF(D458>E$296,D458,E$296)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja"]
[null,null,null,0,{"$f":"IF(AW439>G$298,0,AW439)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"XVIII",{"$f":"+'Analiza i dimenzioniranje'!U231","v":0},"XIX",{"$f":"+'Analiza i dimenzioniranje'!U230","v":0},"XX",{"$f":"'Analiza i dimenzioniranje'!U229","v":0}]
[null,null,null,0,{"$f":"+AW440","v":6.0000000000000009},0,0,{"$f":"+F461","v":0},{"$f":"+G461","v":0},0,0,0,0,0,{"$f":"+M461","v":0},0,{"$f":"+O461","v":0},0,{"$f":"+AS461","v":0},0,{"$f":"+S461","v":0},0,{"$f":"+AS461","v":0},0,{"$f":"+W461","v":0},0,{"$f":"+S461","v":0},0,{"$f":"+AA461","v":0},0,{"$f":"+AU438","v":0},0,{"$f":"+AU438","v":0},0,{"$f":"+AG461","v":0},{"$f":"+AD461","v":0},{"$f":"+AG461","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD499","v":0},{"$f":"+BB461-BC460","v":0},{"$f":"+AD499","v":0},{"$f":"+BD461-BE460","v":0},{"$f":"+AD499","v":0},{"$f":"+'Analiza i dimenzioniranje'!E229","v":{"$error":"#VALUE!"}}]
[null,null,null,0,{"$f":"IF(AW441>G$298,0,AW441)","v":0},0,0,0,{"$f":"+G462","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU439","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+AU477","v":12.686400000000001},{"$f":"+AT500","v":0},{"$f":"+BC462","v":12.686400000000001},0,{"$f":"+AE500","v":12.686400000000001}]
[null,null,null,{"$f":"+AV439","v":{"$error":"#REF!"}},{"$f":"IF(AW442>G$298,0,AW442)","v":0},0,0,{"$f":"+F463","v":0},0,{"$f":"+F461","v":0},0,{"$f":"+D460","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU440","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE501","v":0}]
[null,null,null,{"$f":"+AV440","v":0},{"$f":"IF(AW443>G$298,0,AW443)","v":0},0,0,0,0,{"$f":"+F462","v":0},0,{"$f":"+D461","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU441","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE502","v":0}]
[null,null,null,null,null,0,0,0,0,0,0,{"$f":"+D462","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU442","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE503","v":0}]
[null,null,null,{"$f":"IF(AW444>G$298,0,AW444)","v":0},null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AE465","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE504","v":0}]
[null,null,null,{"$f":"IF(AW445>G$298,0,AW445)","v":4.4000000000000004},null,0,0,0,0,0,0,{"$f":"+D464","v":0},0,{"$f":"+J465","v":0},0,{"$f":"+L465","v":0},0,0,0,{"$f":"+P465","v":0},0,0,0,{"$f":"+T465","v":0},0,0,0,{"$f":"+X465","v":0},0,0,{"$f":"+AU444","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+BC467","v":0}]
[null,null,null,{"$f":"IF(AW446>G$298,0,AW446)","v":4.08},null,0,0,0,0,0,0,0,0,{"$f":"+J466","v":0},0,{"$f":"+L466","v":0},0,0,0,{"$f":"+P466","v":0},0,0,0,{"$f":"+T466","v":0},0,0,{"$f":"+AA467","v":0},{"$f":"+X466","v":0},0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"IF(AW447>G$298,0,AW447)","v":3.76},null,0,0,0,{"$f":"+G469","v":0},{"$f":"+F469","v":0},0,0,0,{"$f":"+J467","v":0},0,{"$f":"+N469","v":0},{"$f":"+O469","v":0},0,0,{"$f":"+R469","v":0},{"$f":"+S469","v":0},0,0,{"$f":"+V469","v":0},0,0,{"$f":"+S469","v":0},{"$f":"+Z469","v":0},{"$f":"+AA469","v":0},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,null,null,{"$f":"+AW256","v":0},0,0,{"$f":"+G470","v":0},0,0,{"$f":"+J470","v":0},{"$f":"+K470","v":0},{"$f":"+L470","v":0},{"$f":"+M470","v":0},{"$f":"+N470","v":0},{"$f":"+O470","v":0},{"$f":"+P470","v":0},{"$f":"+Q470","v":0},{"$f":"+R470","v":0},{"$f":"+S470","v":0},{"$f":"+T470","v":0},{"$f":"+U470","v":0},{"$f":"+V470","v":0},0,0,0,{"$f":"+Z470","v":0},{"$f":"+AA470","v":0},0,0,{"$f":"+AD470","v":0},{"$f":"+AE470","v":0},{"$f":"+AF470","v":0},0,0,{"$f":"+BC432","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+D430","v":0},{"$f":"IF(AW449>G$298,0,AW449)","v":3.14},{"$f":"+D471","v":0},{"$f":"+AW449","v":3.14},0,{"$f":"+G471","v":3.14},0,{"$f":"+E471","v":3.14},{"$f":"+J471","v":0},{"$f":"+K471","v":3.14},{"$f":"+J471","v":0},{"$f":"+M471","v":3.14},{"$f":"+L471","v":0},{"$f":"+O471","v":3.14},{"$f":"+N471","v":0},{"$f":"+Q471","v":3.14},0,{"$f":"+S471","v":3.14},{"$f":"+T471","v":0},{"$f":"+Y471","v":3.14},{"$f":"+B465","v":0},{"$f":"+U471","v":3.14},{"$f":"+B465","v":0},3.14,{"$f":"+Z471","v":0},{"$f":"+U471","v":3.14},{"$f":"+AB471","v":0},3.14,{"$f":"+AB471","v":0},{"$f":"+AC471","v":3.14},{"$f":"+AF471","v":0},3.14,0,3.14,null,{"$f":"+D471","v":0},{"$f":"$E$454^2+AM471^2","v":9},{"$f":"$G$453^2+AM471^2","v":16},{"$f":"$G$495^2+AM471^2","v":51.999999999999993},{"$f":"IF(AM471=0,0,$E$450/(PI())*(ATAN(($E$455*$G$453)/(AM471*SQRT(AP471)))-$E$455*$G$453*AM471/(AO471*SQRT(AP471))))","v":0},null,{"$f":"+AM471","v":0},{"$f":"$E$455^2+AS471^2","v":36},{"$f":"$E$454^2+AS471^2","v":9},{"$f":"$G$452^2+AS471^2","v":45.000000000000007},{"$f":"IF(AS471=0,0,($E$450/(PI()))*(ATAN(($E$455*$E$454)/(AS471*SQRT(AV471)))-$E$455*$E$414*AS471/(AU471*SQRT(AV471))))","v":0},{"$f":"(+AQ471-AW471)*2","v":0},null,null,null,0,0,0,0,0,0]
[null,null,null,0.32,2.8,{"$f":"+AX472","v":{"$error":"#VALUE!"}},2.8,{"$error":"#VALUE!"},2.8,{"$error":"#VALUE!"},{"$f":"+E472","v":2.8},{"$f":"+J472","v":{"$error":"#VALUE!"}},2.8,{"$f":"+J472","v":{"$error":"#VALUE!"}},{"$f":"+M472","v":2.8},{"$f":"+L472","v":{"$error":"#VALUE!"}},{"$f":"+O472","v":2.8},0,{"$f":"+S471","v":3.14},0,0,0,{"$f":"+AS472","v":0.32},0,0,0,3.14,{"$f":"+Z472","v":0},0,{"$f":"+AB472","v":0},3.14,{"$f":"+AB472","v":0},0,{"$f":"+AF472","v":0},0,0,3.14,null,0.32,{"$f":"$E$454^2+AM472^2","v":9.1023999999999994},{"$f":"$G$453^2+AM472^2","v":16.102399999999999},{"$f":"$G$495^2+AM472^2","v":52.102399999999996},{"$f":"IF(AM472=0,0,$E$450/(PI())*(ATAN(($E$455*$G$453)/(AM472*SQRT(AP472)))-$E$455*$G$453*AM472/(AO472*SQRT(AP472))))","v":{"$error":"#VALUE!"}},null,{"$f":"+AM472","v":0.32},{"$f":"$E$455^2+AS472^2","v":36.102400000000003},{"$f":"$E$454^2+AS472^2","v":9.1023999999999994},{"$f":"$G$452^2+AS472^2","v":45.10240000000001},{"$f":"IF(AS472=0,0,($E$450/(PI()))*(ATAN(($E$455*$E$454)/(AS472*SQRT(AV472)))-$E$455*$E$454*AS472/(AU472*SQRT(AV472))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,0,0,0,0,0,0]
[null,null,null,0.64,2.48,{"$error":"#VALUE!"},2.48,{"$error":"#VALUE!"},2.48,{"$error":"#VALUE!"},{"$f":"+E473","v":2.48},{"$error":"#VALUE!"},2.48,{"$f":"+J473","v":{"$error":"#VALUE!"}},{"$f":"+M473","v":2.48},0,{"$f":"+Q472","v":2.8},0,{"$f":"+AS473","v":0.64},0,0,0,0.64,0,0,0,0.64,0,0,0,0.64,0,0,0,0,0,0.64,null,0.64,{"$f":"$E$454^2+AM473^2","v":9.4095999999999993},{"$f":"$G$453^2+AM473^2","v":16.409600000000001},{"$f":"$G$455^2+AM473^2","v":52.40959999999999},{"$f":"IF(AM473=0,0,$E$450/(PI())*(ATAN(($E$455*$G$453)/(AM473*SQRT(AP473)))-$E$455*$G$453*AM473/(AO473*SQRT(AP473))))","v":{"$error":"#VALUE!"}},null,0.64,{"$f":"$E$455^2+AS473^2","v":36.409599999999998},{"$f":"$E$454^2+AS473^2","v":9.4095999999999993},{"$f":"$G$452^2+AS473^2","v":45.409600000000005},{"$f":"IF(AS473=0,0,($E$450/(PI()))*(ATAN(($E$455*$E$454)/(AS473*SQRT(AV473)))-$E$455*$E$454*AS473/(AU473*SQRT(AV473))))","v":{"$error":"#VALUE!"}},{"$f":"(+AQ473-AW473)*2","v":{"$error":"#VALUE!"}},null,null,null,0,0,0,0,0,0]
[null,null,null,0.96,2.16,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},{"$f":"+E474","v":2.16},{"$error":"#VALUE!"},2.16,0,{"$f":"+O473","v":2.48},0,0,0,{"$f":"+AS474","v":0.96},0,0,0,0.96,0,0,0,0.96,0,0,0,0.96,0,0,0,0,0,0.96,null,0.96,9.9215999999999998,{"$f":"$G$453^2+AM474^2","v":16.921600000000002},{"$f":"$G$455^2+AM474^2","v":52.921599999999991},{"$f":"IF(AM474=0,0,$E$450/(PI())*(ATAN(($E$455*$G$453)/(AM474*SQRT(AP474)))-$E$455*$G$453*AM474/(AO474*SQRT(AP474))))","v":{"$error":"#VALUE!"}},null,0.96,{"$f":"$E$455^2+AS474^2","v":36.921599999999998},{"$f":"$E$454^2+AS474^2","v":9.9215999999999998},{"$f":"$G$452^2+AS474^2","v":45.921600000000005},{"$f":"IF(AS474=0,0,($E$450/(PI()))*(ATAN(($E$455*$E$454)/(AS474*SQRT(AV474)))-$E$455*$E$454*AS474/(AU474*SQRT(AV474))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,0,2.8,0,2.8,0,2.8]
[null,null,null,1.28,1.84,{"$error":"#VALUE!"},1.84,{"$error":"#VALUE!"},1.84,{"$error":"#VALUE!"},{"$f":"+E475","v":1.84},0,{"$f":"+M474","v":2.16},0,0,0,0,0,{"$f":"+AS475","v":1.28},0,0,0,1.28,0,0,0,1.28,0,0,0,1.28,0,0,0,0,0,1.28,null,1.28,10.638400000000001,17.638400000000001,53.63839999999999,{"$error":"#VALUE!"},null,1.28,37.638399999999997,10.638400000000001,46.638400000000004,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,0.32,0,0.32,0,0.32]
[null,null,null,1.6,1.52,{"$error":"#VALUE!"},1.52,{"$error":"#VALUE!"},1.52,0,{"$f":"+K475","v":1.84},0,{"$f":"+N476","v":0},0,{"$f":"+AM476","v":1.6},0,0,0,{"$f":"+AS476","v":1.6},0,0,0,1.6,0,0,0,1.6,0,0,0,{"$f":"+AE475","v":1.28},0,0,0,0,0,1.6,null,1.6,11.56,18.560000000000002,54.559999999999995,{"$error":"#VALUE!"},null,1.6,38.56,11.56,47.560000000000009,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,0.64,0,0.64,0,0.64]
[null,null,null,1.9200000000000002,1.2,{"$error":"#VALUE!"},1.2,0,{"$f":"+I476","v":1.52},0,{"$f":"+E477","v":1.2},0,{"$f":"+N477","v":0},0,{"$f":"+AM477","v":1.9200000000000002},0,0,0,{"$f":"+AS477","v":1.9200000000000002},0,0,0,1.9200000000000002,0,0,0,1.9200000000000002,0,0,0,{"$f":"+AU454","v":1.9200000000000002},0,0,0,0,0,1.9200000000000002,null,1.9200000000000002,12.686400000000001,19.686399999999999,55.686399999999992,{"$error":"#VALUE!"},null,1.9200000000000002,39.686399999999999,12.686400000000001,48.686400000000006,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,0.96,0,0.96,0,0.96]
[null,null,null,null,{"$f":"+AW456","v":1.2},0,{"$f":"+E478","v":1.2},0,{"$f":"+G478","v":1.2},0,{"$f":"+I478","v":1.2},0,{"$f":"+K478","v":1.2},0,{"$f":"+M478","v":1.2},0,{"$f":"+O478","v":1.2},0,{"$f":"+Q478","v":1.2},0,{"$f":"+S478","v":1.2},0,{"$f":"+U478","v":1.2},{"$f":"+P478","v":0},{"$f":"+W478","v":1.2},0,{"$f":"+Y478","v":1.2},0,{"$f":"+AA478","v":1.2},0,{"$f":"+AC478","v":1.2},0,{"$f":"+AC478","v":1.2},0,1.2,{"$f":"+AD478","v":0},1.2,null,null,0,{"$f":"+AM478","v":0},0,{"$f":"+AQ477","v":{"$error":"#VALUE!"}},0,{"$f":"+AO478","v":0},0,{"$f":"+S501","v":0},{"$f":"BK298-BQ297","v":0},{"$f":"IF(AV476>AW$299,AV476,AW$299)","v":47.560000000000009},null,null,null,null,{"$f":"+AT514","v":36.409599999999998},1.28,0,1.28,0,1.28]
[null,null,null,null,null,{"$f":"+AV455","v":0},{"$f":"+G471","v":3.14},0,{"$f":"+G479","v":3.14},0,{"$f":"+I479","v":3.14},0,{"$f":"+K479","v":3.14},0,{"$f":"+M479","v":3.14},0,{"$f":"+O479","v":3.14},0,{"$f":"+Q479","v":3.14},0,{"$f":"+S479","v":3.14},0,{"$f":"+U479","v":3.14},{"$f":"+P479","v":0},{"$f":"+W479","v":3.14},{"$f":"+N479","v":0},{"$f":"+Y479","v":3.14},0,{"$f":"+AA479","v":3.14},0,{"$f":"+AC479","v":3.14},0,{"$f":"+AC479","v":3.14},0,3.14,{"$f":"+AD479","v":0},{"$f":"+BC441","v":3.14},null,null,0,0,0,{"$f":"+AS479","v":0},0,0,0,0,{"$f":"#REF!-#REF!","v":{"$error":"#REF!"}},{"$f":"+AW480","v":6.0000000000000009},null,null,null,null,{"$f":"+AT515","v":36.921599999999998},1.6,{"$f":"+AD515","v":0},1.6,0,1.6]
[null,null,null,null,null,"SQhi=",{"$f":"+G483","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I483","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K483","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+M483","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+O483","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Q483","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+S483","v":0},"SQhi=",{"$f":"+U483","v":0},"SQhi=",{"$f":"+W483","v":0},"SQhi=",{"$f":"+Y483","v":0},"SQhi=",{"$f":"+AA483","v":0},"SQhi=",{"$f":"+AC483","v":0},"SQhi=",{"$f":"+AE483","v":0},null,null,null,null,"SQhi=",{"$f":"+AK483","v":0},null,null,"SQhi=",{"$f":"+AO483","v":12.902400000000014},"SQhi=",{"$f":"+AQ483","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AS483","v":0},"SQhi=",0,{"$f":"BK299-BQ298","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$67","v":6.0000000000000009},null,null,null,null,0,1.2,0,{"$f":"+BE479","v":1.6},0,{"$f":"+AE518","v":1.2}]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G485","v":{"$error":"#VALUE!"}}," y=",{"$f":"+I485","v":{"$error":"#VALUE!"}}," y=",{"$f":"+K485","v":{"$error":"#VALUE!"}}," y=",{"$f":"+M485","v":{"$error":"#VALUE!"}}," y=",{"$f":"+O485","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Q485","v":{"$error":"#VALUE!"}}," y=",{"$f":"+S485","v":0}," y=",{"$f":"+U485","v":0}," y=",{"$f":"+W485","v":0}," y=",{"$f":"+Y485","v":0}," y=",{"$f":"+AA485","v":0}," y=",{"$f":"+AC485","v":0}," y=",{"$f":"+AE485","v":0},null,null,null,null," y=",{"$f":"+AK485","v":0},null,null," y=",{"$f":"+AO485","v":11.895466666666669}," y=",{"$f":"+AQ485","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AS485","v":0}," y=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$66","v":5.6800000000000006},null,null,null,null,0,6.2,0,{"$f":"+AK519","v":6.2},0,{"$f":"+AE519","v":6.2}]
[null,null,null,"krak za presjek III -III",null,"z=",{"$f":"+G481-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I481-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K481-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M481-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+O481-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Q481-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+S481-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+U481-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z=",{"$f":"+W481-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+Y481-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AA481-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AC481-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AE481-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AG481-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AI481-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AK481-'Analiza i dimenzioniranje'!$E$52","v":-1.2},null,null,"z=",{"$f":"+AO481-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":11.395466666666669},"z=",{"$f":"+AQ481-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AS481-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$65","v":5.36},null,null,null,null,"SQhi=",{"$f":"+BC485","v":-10.174207999999997},"SQhi=",{"$f":"+BE485","v":0}]
[null,null,null,"x=",0,"F=",{"$f":"-0.5*(+\n (F462*G463-F463*G462)+\n(F463*G464-F464*G463)+\n(F464*G465-F465*G464)+\n(F465*G466-F466*G465)+\n(F466*G467-F467*G466)+\n(F467*G468-F468*G467)+\n(F468*G469-F469*G468)+\n(F469*G470-F470*G469)+\n(F470*G471-F471*G470)+\n(F471*G472-F472*G471)+\n(F472*G473-F473*G472)+\n(F473*G474-F474*G473)+\n(F474*G475-F475*G474)+\n(F475*G476-F476*G475)+\n(F476*G477-F477*G476)+\n(F477*G478-F478*G477)+\n(F478*G479-F479*G478))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (H462*I463-H463*I462)+\n(H463*I464-H464*I463)+\n(H464*I465-H465*I464)+\n(H465*I466-H466*I465)+\n(H466*I467-H467*I466)+\n(H467*I468-H468*I467)+\n(H468*I469-H469*I468)+\n(H469*I470-H470*I469)+\n(H470*I471-H471*I470)+\n(H471*I472-H472*I471)+\n(H472*I473-H473*I472)+\n(H473*I474-H474*I473)+\n(H474*I475-H475*I474)+\n(H475*I476-H476*I475)+\n(H476*I477-H477*I476)+\n(H477*I478-H478*I477)+\n(H478*I479-H479*I478))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((J460*K461-J461*K460)+(J461*K462-J462*K461)+\n (J462*K463-J463*K462)+\n(J463*K464-J464*K463)+\n(J464*K465-J465*K464)+\n(J465*K466-J466*K465)+\n(J466*K467-J467*K466)+\n(J467*K468-J468*K467)+\n(J468*K469-J469*K468)+\n(J469*K470-J470*K469)+\n(J470*K471-J471*K470)+\n(J471*K472-J472*K471)+\n(J472*K473-J473*K472)+\n(J473*K474-J474*K473)+\n(J474*K475-J475*K474)+\n(J475*K476-J476*K475)+\n(J476*K477-J477*K476)+\n(J477*K478-J478*K477)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (L462*M463-L463*M462)+\n(L463*M464-L464*M463)+\n(L464*M465-L465*M464)+\n(L465*M466-L466*M465)+\n(L466*M467-L467*M466)+\n(L467*M468-L468*M467)+\n(L468*M469-L469*M468)+\n(L469*M470-L470*M469)+\n(L470*M471-L471*M470)+\n(L471*M472-L472*M471)+\n(L472*M473-L473*M472)+\n(L473*M474-L474*M473)+\n(L474*M475-L475*M474)+\n(L475*M476-L476*M475)+\n(L476*M477-L477*M476)+\n(L477*M478-L478*M477)+\n(L478*M479-L479*M478))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((N460*O461-N461*O460)+(N461*O462-N462*O461)+\n (N462*O463-N463*O462)+\n(N463*O464-N464*O463)+\n(N464*O465-N465*O464)+\n(N465*O466-N466*O465)+\n(N466*O467-N467*O466)+\n(N467*O468-N468*O467)+\n(N468*O469-N469*O468)+\n(N469*O470-N470*O469)+\n(N470*O471-N471*O470)+\n(N471*O472-N472*O471)+\n(N472*O473-N473*O472)+\n(N473*O474-N474*O473)+\n(N474*O475-N475*O474)+\n(N475*O476-N476*O475)+\n(N476*O477-N477*O476)+\n(N477*O478-N478*O477)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (P462*Q463-P463*Q462)+\n(P463*Q464-P464*Q463)+\n(P464*Q465-P465*Q464)+\n(P465*Q466-P466*Q465)+\n(P466*Q467-P467*Q466)+\n(P467*Q468-P468*Q467)+\n(P468*Q469-P469*Q468)+\n(P469*Q470-P470*Q469)+\n(P470*Q471-P471*Q470)+\n(P471*Q472-P472*Q471)+\n(P472*Q473-P473*Q472)+\n(P473*Q474-P474*Q473)+\n(P474*Q475-P475*Q474)+\n(P475*Q476-P476*Q475)+\n(P476*Q477-P477*Q476)+\n(P477*Q478-P478*Q477)+\n(P478*Q479-P479*Q478))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (R462*S463-R463*S462)+\n(R463*S464-R464*S463)+\n(R464*S465-R465*S464)+\n(R465*S466-R466*S465)+\n(R466*S467-R467*S466)+\n(R467*S468-R468*S467)+\n(R468*S469-R469*S468)+\n(R469*S470-R470*S469)+\n(R470*S471-R471*S470)+\n(R471*S472-R472*S471)+\n(R472*S473-R473*S472)+\n(R473*S474-R474*S473)+\n(R474*S475-R475*S474)+\n(R475*S476-R476*S475)+\n(R476*S477-R477*S476)+\n(R477*S478-R478*S477)+\n(R478*S479-R479*S478))","v":0},"F=",{"$f":"-0.5*(+\n (T462*U463-T463*U462)+\n(T463*U464-T464*U463)+\n(T464*U465-T465*U464)+\n(T465*U466-T466*U465)+\n(T466*U467-T467*U466)+\n(T467*U468-T468*U467)+\n(T468*U469-T469*U468)+\n(T469*U470-T470*U469)+\n(T470*U471-T471*U470)+\n(T471*U472-T472*U471)+\n(T472*U473-T473*U472)+\n(T473*U474-T474*U473)+\n(T474*U475-T475*U474)+\n(T475*U476-T476*U475)+\n(T476*U477-T477*U476)+\n(T477*U478-T478*U477)+\n(T478*U479-T479*U478))","v":0},"F=",{"$f":"-0.5*(+\n (V462*W463-V463*W462)+\n(V463*W464-V464*W463)+\n(V464*W465-V465*W464)+\n(V465*W466-V466*W465)+\n(V466*W467-V467*W466)+\n(V467*W468-V468*W467)+\n(V468*W469-V469*W468)+\n(V469*W470-V470*W469)+\n(V470*W471-V471*W470)+\n(V471*W472-V472*W471)+\n(V472*W473-V473*W472)+\n(V473*W474-V474*W473)+\n(V474*W475-V475*W474)+\n(V475*W476-V476*W475)+\n(V476*W477-V477*W476)+\n(V477*W478-V478*W477)+\n(V478*W479-V479*W478))","v":0},"F=",{"$f":"-0.5*(+\n (X462*Y463-X463*Y462)+\n(X463*Y464-X464*Y463)+\n(X464*Y465-X465*Y464)+\n(X465*Y466-X466*Y465)+\n(X466*Y467-X467*Y466)+\n(X467*Y468-X468*Y467)+\n(X468*Y469-X469*Y468)+\n(X469*Y470-X470*Y469)+\n(X470*Y471-X471*Y470)+\n(X471*Y472-X472*Y471)+\n(X472*Y473-X473*Y472)+\n(X473*Y474-X474*Y473)+\n(X474*Y475-X475*Y474)+\n(X475*Y476-X476*Y475)+\n(X476*Y477-X477*Y476)+\n(X477*Y478-X478*Y477)+\n(X478*Y479-X479*Y478))","v":0},"F=",{"$f":"-0.5*(+\n (Z462*AA463-Z463*AA462)+\n(Z463*AA464-Z464*AA463)+\n(Z464*AA465-Z465*AA464)+\n(Z465*AA466-Z466*AA465)+\n(Z466*AA467-Z467*AA466)+\n(Z467*AA468-Z468*AA467)+\n(Z468*AA469-Z469*AA468)+\n(Z469*AA470-Z470*AA469)+\n(Z470*AA471-Z471*AA470)+\n(Z471*AA472-Z472*AA471)+\n(Z472*AA473-Z473*AA472)+\n(Z473*AA474-Z474*AA473)+\n(Z474*AA475-Z475*AA474)+\n(Z475*AA476-Z476*AA475)+\n(Z476*AA477-Z477*AA476)+\n(Z477*AA478-Z478*AA477)+\n(Z478*AA479-Z479*AA478))","v":0},"F=",{"$f":"-0.5*(+\n (AB462*AC463-AB463*AC462)+\n(AB463*AC464-AB464*AC463)+\n(AB464*AC465-AB465*AC464)+\n(AB465*AC466-AB466*AC465)+\n(AB466*AC467-AB467*AC466)+\n(AB467*AC468-AB468*AC467)+\n(AB468*AC469-AB469*AC468)+\n(AB469*AC470-AB470*AC469)+\n(AB470*AC471-AB471*AC470)+\n(AB471*AC472-AB472*AC471)+\n(AB472*AC473-AB473*AC472)+\n(AB473*AC474-AB474*AC473)+\n(AB474*AC475-AB475*AC474)+\n(AB475*AC476-AB476*AC475)+\n(AB476*AC477-AB477*AC476)+\n(AB477*AC478-AB478*AC477)+\n(AB478*AC479-AB479*AC478))","v":0},"F=",{"$f":"-0.5*(+\n (AD462*AE463-AD463*AE462)+\n(AD463*AE464-AD464*AE463)+\n(AD464*AE465-AD465*AE464)+\n(AD465*AE466-AD466*AE465)+\n(AD466*AE467-AD467*AE466)+\n(AD467*AE468-AD468*AE467)+\n(AD468*AE469-AD469*AE468)+\n(AD469*AE470-AD470*AE469)+\n(AD470*AE471-AD471*AE470)+\n(AD471*AE472-AD472*AE471)+\n(AD472*AE473-AD473*AE472)+\n(AD473*AE474-AD474*AE473)+\n(AD474*AE475-AD475*AE474)+\n(AD475*AE476-AD476*AE475)+\n(AD476*AE477-AD477*AE476)+\n(AD477*AE478-AD478*AE477)+\n(AD478*AE479-AD479*AE478))","v":0},null,null,null,null,"F=",{"$f":"-0.5*(+\n (AJ462*AK463-AJ463*AK462)+\n(AJ463*AK464-AJ464*AK463)+\n(AJ464*AK465-AJ465*AK464)+\n(AJ465*AK466-AJ466*AK465)+\n(AJ466*AK467-AJ467*AK466)+\n(AJ467*AK468-AJ468*AK467)+\n(AJ468*AK469-AJ469*AK468)+\n(AJ469*AK470-AJ470*AK469)+\n(AJ470*AK471-AJ471*AK470)+\n(AJ471*AK472-AJ472*AK471)+\n(AJ472*AK473-AJ473*AK472)+\n(AJ473*AK474-AJ474*AK473)+\n(AJ474*AK475-AJ475*AK474)+\n(AJ475*AK476-AJ476*AK475)+\n(AJ476*AK477-AJ477*AK476)+\n(AJ477*AK478-AJ478*AK477)+\n(AJ478*AK479-AJ479*AK478))","v":0},null,null,"F=",{"$f":"-0.5*((AN460*AO461-AN461*AO460)+(AN461*AO462-AN462*AO461)+\n (AN462*AO463-AN463*AO462)+\n(AN463*AO464-AN464*AO463)+\n(AN464*AO465-AN465*AO464)+\n(AN465*AO466-AN466*AO465)+\n(AN466*AO467-AN467*AO466)+\n(AN467*AO468-AN468*AO467)+\n(AN468*AO469-AN469*AO468)+\n(AN469*AO470-AN470*AO469)+\n(AN470*AO471-AN471*AO470)+\n(AN471*AO472-AN472*AO471)+\n(AN472*AO473-AN473*AO472)+\n(AN473*AO474-AN474*AO473)+\n(AN474*AO475-AN475*AO474)+\n(AN475*AO476-AN476*AO475)+\n(AN476*AO477-AN477*AO476)+\n(AN477*AO478-AN478*AO477)\n)","v":12.902400000000014},"F=",{"$f":"-0.5*((AP460*AQ461-AP461*AQ460)+(AP461*AQ462-AP462*AQ461)+\n (AP462*AQ463-AP463*AQ462)+\n(AP463*AQ464-AP464*AQ463)+\n(AP464*AQ465-AP465*AQ464)+\n(AP465*AQ466-AP466*AQ465)+\n(AP466*AQ467-AP467*AQ466)+\n(AP467*AQ468-AP468*AQ467)+\n(AP468*AQ469-AP469*AQ468)+\n(AP469*AQ470-AP470*AQ469)+\n(AP470*AQ471-AP471*AQ470)+\n(AP471*AQ472-AP472*AQ471)+\n(AP472*AQ473-AP473*AQ472)+\n(AP473*AQ474-AP474*AQ473)+\n(AP474*AQ475-AP475*AQ474)+\n(AP475*AQ476-AP476*AQ475)+\n(AP476*AQ477-AP477*AQ476)+\n(AP477*AQ478-AP478*AQ477)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AR460*AS461-AR461*AS460)+(AR461*AS462-AR462*AS461)+\n (AR462*AS463-AR463*AS462)+\n(AR463*AS464-AR464*AS463)+\n(AR464*AS465-AR465*AS464)+\n(AR465*AS466-AR466*AS465)+\n(AR466*AS467-AR467*AS466)+\n(AR467*AS468-AR468*AS467)+\n(AR468*AS469-AR469*AS468)+\n(AR469*AS470-AR470*AS469)+\n(AR470*AS471-AR471*AS470)+\n(AR471*AS472-AR472*AS471)+\n(AR472*AS473-AR473*AS472)+\n(AR473*AS474-AR474*AS473)+\n(AR474*AS475-AR475*AS474)+\n(AR475*AS476-AR476*AS475)+\n(AR476*AS477-AR477*AS476)+\n(AR477*AS478-AR478*AS477)\n)","v":0},"F=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$64","v":5.04},null,null,null,null," y=",{"$f":"+BC487","v":1.268387388974159}," y=",{"$f":"+BE487","v":0}]
[null,null,null,"y=",{"$f":"+IF(E482=0,0,-((D459*E460-D460*E459)*(E459+E460)+(D460*E461-D461*E460)*(E460+E461)+\n(D461*E462-D462*E461)*(E461+E462)+\n(D462*E463-D463*E462)*(E462+E463)+\n(D463*E464-D464*E463)*(E463+E464)+\n(D464*D466-D471*E464)*(E464+D466)+\n(D471*D467-D472*D466)*(D466+D467)+\n(D472*D468-D473*D467)*(D467+D468)+\n(D473*D469-D474*D468)*(D468+D469)+\n(D474*#REF!-D475*D469)*(D469+#REF!)+\n(D475*E471-D476*#REF!)*(#REF!+E471)+\n(D476*E472-D477*E471)*(E471+E472)+\n(D477*E473-D479*E472)*(E472+E473)+\n(D479*E474-E479*E473)*(E473+E474)+\n(E479*E475-E480*E474)*(E474+E475)+\n(E480*E476-E481*E475)*(E475+E476)+\n(E481*E477-#REF!*E476)*(E476+E477)+\n(#REF!*E478-#REF!*E477)*(E477+E478)+\n(#REF!*#REF!-#REF!*E478)*(E478+#REF!))/6/E482)","v":0},"x=",1.5,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,null,null,null,null,"x=",0,null,null,"x=",0,"x=",0,"x=",0,"x=",0,0,{"$f":"'Analiza i dimenzioniranje'!$U$63","v":4.72},null,null,null,null,"z=",{"$f":"+BC483-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":0.76838738897415904},"z=",{"$f":"+BE483-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5}]
[null,null,null,"y=",{"$f":"+IF(E483=0,0,-((D460*E461-D461*E460)*(E460+E461)+(D461*E462-D462*E461)*(E461+E462)+\n(D462*E463-D463*E462)*(E462+E463)+\n(D463*E464-D464*E463)*(E463+E464)+\n(D464*D466-D471*E464)*(E464+D466)+\n(D471*D467-D472*D466)*(D466+D467)+\n(D472*D468-D473*D467)*(D467+D468)+\n(D473*D469-D474*D468)*(D468+D469)+\n(D474*#REF!-D475*D469)*(D469+#REF!)+\n(D475*E471-D476*#REF!)*(#REF!+E471)+\n(D476*E472-D477*E471)*(E471+E472)+\n(D477*E473-D479*E472)*(E472+E473)+\n(D479*E474-E479*E473)*(E473+E474)+\n(E479*E475-E480*E474)*(E474+E475)+\n(E480*E476-E481*E475)*(E475+E476)+\n(E481*E477-#REF!*E476)*(E476+E477)+\n(#REF!*E478-#REF!*E477)*(E477+E478)+\n(#REF!*#REF!-#REF!*E478)*(E478+#REF!)+\n(#REF!*#REF!-#REF!*#REF!)*(#REF!+#REF!))/6/E483)","v":0},"y=",{"$f":"+IF(G483=0,0,-((F460*G461-F461*G460)*(G460+G461)+(F461*G462-F462*G461)*(G461+G462)+\n(F462*G463-F463*G462)*(G462+G463)+\n(F463*G464-F464*G463)*(G463+G464)+\n(F464*G465-F465*G464)*(G464+G465)+\n(F465*G466-F466*G465)*(G465+G466)+\n(F466*G467-F467*G466)*(G466+G467)+\n(F467*G468-F468*G467)*(G467+G468)+\n(F468*G469-F469*G468)*(G468+G469)+\n(F469*G470-F470*G469)*(G469+G470)+\n(F470*G471-F471*G470)*(G470+G471)+\n(F471*G472-F472*G471)*(G471+G472)+\n(F472*G473-F473*G472)*(G472+G473)+\n(F473*G474-F474*G473)*(G473+G474)+\n(F474*G475-F475*G474)*(G474+G475)+\n(F475*G476-F476*G475)*(G475+G476)+\n(F476*G477-F477*G476)*(G476+G477)+\n(F477*G478-F478*G477)*(G477+G478)+\n(F478*G479-F479*G478)*(G478+G479))/6/G483)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(I483=0,0,-((H460*I461-H461*I460)*(I460+I461)+(H461*I462-H462*I461)*(I461+I462)+\n(H462*I463-H463*I462)*(I462+I463)+\n(H463*I464-H464*I463)*(I463+I464)+\n(H464*I465-H465*I464)*(I464+I465)+\n(H465*I466-H466*I465)*(I465+I466)+\n(H466*I467-H467*I466)*(I466+I467)+\n(H467*I468-H468*I467)*(I467+I468)+\n(H468*I469-H469*I468)*(I468+I469)+\n(H469*I470-H470*I469)*(I469+I470)+\n(H470*I471-H471*I470)*(I470+I471)+\n(H471*I472-H472*I471)*(I471+I472)+\n(H472*I473-H473*I472)*(I472+I473)+\n(H473*I474-H474*I473)*(I473+I474)+\n(H474*I475-H475*I474)*(I474+I475)+\n(H475*I476-H476*I475)*(I475+I476)+\n(H476*I477-H477*I476)*(I476+I477)+\n(H477*I478-H478*I477)*(I477+I478)+\n(H478*I479-H479*I478)*(I478+I479))/6/I483)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(K483=0,0,-((J460*K461-J461*K460)*(K460+K461)+(J461*K462-J462*K461)*(K461+K462)+\n(J462*K463-J463*K462)*(K462+K463)+\n(J463*K464-J464*K463)*(K463+K464)+\n(J464*K465-J465*K464)*(K464+K465)+\n(J465*K466-J466*K465)*(K465+K466)+\n(J466*K467-J467*K466)*(K466+K467)+\n(J467*K468-J468*K467)*(K467+K468)+\n(J468*K469-J469*K468)*(K468+K469)+\n(J469*K470-J470*K469)*(K469+K470)+\n(J470*K471-J471*K470)*(K470+K471)+\n(J471*K472-J472*K471)*(K471+K472)+\n(J472*K473-J473*K472)*(K472+K473)+\n(J473*K474-J474*K473)*(K473+K474)+\n(J474*K475-J475*K474)*(K474+K475)+\n(J475*K476-J476*K475)*(K475+K476)+\n(J476*K477-J477*K476)*(K476+K477)+\n(J477*K478-J478*K477)*(K477+K478)+\n(J478*K479-J479*K478)*(K478+K479))/6/K483)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(M483=0,0,-((L460*M461-L461*M460)*(M460+M461)+(L461*M462-L462*M461)*(M461+M462)+\n(L462*M463-L463*M462)*(M462+M463)+\n(L463*M464-L464*M463)*(M463+M464)+\n(L464*M465-L465*M464)*(M464+M465)+\n(L465*M466-L466*M465)*(M465+M466)+\n(L466*M467-L467*M466)*(M466+M467)+\n(L467*M468-L468*M467)*(M467+M468)+\n(L468*M469-L469*M468)*(M468+M469)+\n(L469*M470-L470*M469)*(M469+M470)+\n(L470*M471-L471*M470)*(M470+M471)+\n(L471*M472-L472*M471)*(M471+M472)+\n(L472*M473-L473*M472)*(M472+M473)+\n(L473*M474-L474*M473)*(M473+M474)+\n(L474*M475-L475*M474)*(M474+M475)+\n(L475*M476-L476*M475)*(M475+M476)+\n(L476*M477-L477*M476)*(M476+M477)+\n(L477*M478-L478*M477)*(M477+M478)+\n(L478*M479-L479*M478)*(M478+M479))/6/M483)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(O483=0,0,-((N460*O461-N461*O460)*(O460+O461)+(N461*O462-N462*O461)*(O461+O462)+\n(N462*O463-N463*O462)*(O462+O463)+\n(N463*O464-N464*O463)*(O463+O464)+\n(N464*O465-N465*O464)*(O464+O465)+\n(N465*O466-N466*O465)*(O465+O466)+\n(N466*O467-N467*O466)*(O466+O467)+\n(N467*O468-N468*O467)*(O467+O468)+\n(N468*O469-N469*O468)*(O468+O469)+\n(N469*O470-N470*O469)*(O469+O470)+\n(N470*O471-N471*O470)*(O470+O471)+\n(N471*O472-N472*O471)*(O471+O472)+\n(N472*O473-N473*O472)*(O472+O473)+\n(N473*O474-N474*O473)*(O473+O474)+\n(N474*O475-N475*O474)*(O474+O475)+\n(N475*O476-N476*O475)*(O475+O476)+\n(N476*O477-N477*O476)*(O476+O477)+\n(N477*O478-N478*O477)*(O477+O478)+\n(N478*O479-N479*O478)*(O478+O479))/6/O483)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Q483=0,0,-((P460*Q461-P461*Q460)*(Q460+Q461)+(P461*Q462-P462*Q461)*(Q461+Q462)+\n(P462*Q463-P463*Q462)*(Q462+Q463)+\n(P463*Q464-P464*Q463)*(Q463+Q464)+\n(P464*Q465-P465*Q464)*(Q464+Q465)+\n(P465*Q466-P466*Q465)*(Q465+Q466)+\n(P466*Q467-P467*Q466)*(Q466+Q467)+\n(P467*Q468-P468*Q467)*(Q467+Q468)+\n(P468*Q469-P469*Q468)*(Q468+Q469)+\n(P469*Q470-P470*Q469)*(Q469+Q470)+\n(P470*Q471-P471*Q470)*(Q470+Q471)+\n(P471*Q472-P472*Q471)*(Q471+Q472)+\n(P472*Q473-P473*Q472)*(Q472+Q473)+\n(P473*Q474-P474*Q473)*(Q473+Q474)+\n(P474*Q475-P475*Q474)*(Q474+Q475)+\n(P475*Q476-P476*Q475)*(Q475+Q476)+\n(P476*Q477-P477*Q476)*(Q476+Q477)+\n(P477*Q478-P478*Q477)*(Q477+Q478)+\n(P478*Q479-P479*Q478)*(Q478+Q479))/6/Q483)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(S483=0,0,-((R460*S461-R461*S460)*(S460+S461)+(R461*S462-R462*S461)*(S461+S462)+\n(R462*S463-R463*S462)*(S462+S463)+\n(R463*S464-R464*S463)*(S463+S464)+\n(R464*S465-R465*S464)*(S464+S465)+\n(R465*S466-R466*S465)*(S465+S466)+\n(R466*S467-R467*S466)*(S466+S467)+\n(R467*S468-R468*S467)*(S467+S468)+\n(R468*S469-R469*S468)*(S468+S469)+\n(R469*S470-R470*S469)*(S469+S470)+\n(R470*S471-R471*S470)*(S470+S471)+\n(R471*S472-R472*S471)*(S471+S472)+\n(R472*S473-R473*S472)*(S472+S473)+\n(R473*S474-R474*S473)*(S473+S474)+\n(R474*S475-R475*S474)*(S474+S475)+\n(R475*S476-R476*S475)*(S475+S476)+\n(R476*S477-R477*S476)*(S476+S477)+\n(R477*S478-R478*S477)*(S477+S478)+\n(R478*S479-R479*S478)*(S478+S479))/6/S483)","v":0},"y=",{"$f":"+IF(U483=0,0,-((T460*U461-T461*U460)*(U460+U461)+(T461*U462-T462*U461)*(U461+U462)+\n(T462*U463-T463*U462)*(U462+U463)+\n(T463*U464-T464*U463)*(U463+U464)+\n(T464*U465-T465*U464)*(U464+U465)+\n(T465*U466-T466*U465)*(U465+U466)+\n(T466*U467-T467*U466)*(U466+U467)+\n(T467*U468-T468*U467)*(U467+U468)+\n(T468*U469-T469*U468)*(U468+U469)+\n(T469*U470-T470*U469)*(U469+U470)+\n(T470*U471-T471*U470)*(U470+U471)+\n(T471*U472-T472*U471)*(U471+U472)+\n(T472*U473-T473*U472)*(U472+U473)+\n(T473*U474-T474*U473)*(U473+U474)+\n(T474*U475-T475*U474)*(U474+U475)+\n(T475*U476-T476*U475)*(U475+U476)+\n(T476*U477-T477*U476)*(U476+U477)+\n(T477*U478-T478*U477)*(U477+U478)+\n(T478*U479-T479*U478)*(U478+U479))/6/U483)","v":0},"y=",{"$f":"+IF(W483=0,0,-((V460*W461-V461*W460)*(W460+W461)+(V461*W462-V462*W461)*(W461+W462)+\n(V462*W463-V463*W462)*(W462+W463)+\n(V463*W464-V464*W463)*(W463+W464)+\n(V464*W465-V465*W464)*(W464+W465)+\n(V465*W466-V466*W465)*(W465+W466)+\n(V466*W467-V467*W466)*(W466+W467)+\n(V467*W468-V468*W467)*(W467+W468)+\n(V468*W469-V469*W468)*(W468+W469)+\n(V469*W470-V470*W469)*(W469+W470)+\n(V470*W471-V471*W470)*(W470+W471)+\n(V471*W472-V472*W471)*(W471+W472)+\n(V472*W473-V473*W472)*(W472+W473)+\n(V473*W474-V474*W473)*(W473+W474)+\n(V474*W475-V475*W474)*(W474+W475)+\n(V475*W476-V476*W475)*(W475+W476)+\n(V476*W477-V477*W476)*(W476+W477)+\n(V477*W478-V478*W477)*(W477+W478)+\n(V478*W479-V479*W478)*(W478+W479))/6/W483)","v":0},"y=",{"$f":"+IF(Y483=0,0,-((X460*Y461-X461*Y460)*(Y460+Y461)+(X461*Y462-X462*Y461)*(Y461+Y462)+\n(X462*Y463-X463*Y462)*(Y462+Y463)+\n(X463*Y464-X464*Y463)*(Y463+Y464)+\n(X464*Y465-X465*Y464)*(Y464+Y465)+\n(X465*Y466-X466*Y465)*(Y465+Y466)+\n(X466*Y467-X467*Y466)*(Y466+Y467)+\n(X467*Y468-X468*Y467)*(Y467+Y468)+\n(X468*Y469-X469*Y468)*(Y468+Y469)+\n(X469*Y470-X470*Y469)*(Y469+Y470)+\n(X470*Y471-X471*Y470)*(Y470+Y471)+\n(X471*Y472-X472*Y471)*(Y471+Y472)+\n(X472*Y473-X473*Y472)*(Y472+Y473)+\n(X473*Y474-X474*Y473)*(Y473+Y474)+\n(X474*Y475-X475*Y474)*(Y474+Y475)+\n(X475*Y476-X476*Y475)*(Y475+Y476)+\n(X476*Y477-X477*Y476)*(Y476+Y477)+\n(X477*Y478-X478*Y477)*(Y477+Y478)+\n(X478*Y479-X479*Y478)*(Y478+Y479))/6/Y483)","v":0},"y=",{"$f":"+IF(AA483=0,0,-((Z460*AA461-Z461*AA460)*(AA460+AA461)+(Z461*AA462-Z462*AA461)*(AA461+AA462)+\n(Z462*AA463-Z463*AA462)*(AA462+AA463)+\n(Z463*AA464-Z464*AA463)*(AA463+AA464)+\n(Z464*AA465-Z465*AA464)*(AA464+AA465)+\n(Z465*AA466-Z466*AA465)*(AA465+AA466)+\n(Z466*AA467-Z467*AA466)*(AA466+AA467)+\n(Z467*AA468-Z468*AA467)*(AA467+AA468)+\n(Z468*AA469-Z469*AA468)*(AA468+AA469)+\n(Z469*AA470-Z470*AA469)*(AA469+AA470)+\n(Z470*AA471-Z471*AA470)*(AA470+AA471)+\n(Z471*AA472-Z472*AA471)*(AA471+AA472)+\n(Z472*AA473-Z473*AA472)*(AA472+AA473)+\n(Z473*AA474-Z474*AA473)*(AA473+AA474)+\n(Z474*AA475-Z475*AA474)*(AA474+AA475)+\n(Z475*AA476-Z476*AA475)*(AA475+AA476)+\n(Z476*AA477-Z477*AA476)*(AA476+AA477)+\n(Z477*AA478-Z478*AA477)*(AA477+AA478)+\n(Z478*AA479-Z479*AA478)*(AA478+AA479))/6/AA483)","v":0},"y=",{"$f":"+IF(AC483=0,0,-((AB460*AC461-AB461*AC460)*(AC460+AC461)+(AB461*AC462-AB462*AC461)*(AC461+AC462)+\n(AB462*AC463-AB463*AC462)*(AC462+AC463)+\n(AB463*AC464-AB464*AC463)*(AC463+AC464)+\n(AB464*AC465-AB465*AC464)*(AC464+AC465)+\n(AB465*AC466-AB466*AC465)*(AC465+AC466)+\n(AB466*AC467-AB467*AC466)*(AC466+AC467)+\n(AB467*AC468-AB468*AC467)*(AC467+AC468)+\n(AB468*AC469-AB469*AC468)*(AC468+AC469)+\n(AB469*AC470-AB470*AC469)*(AC469+AC470)+\n(AB470*AC471-AB471*AC470)*(AC470+AC471)+\n(AB471*AC472-AB472*AC471)*(AC471+AC472)+\n(AB472*AC473-AB473*AC472)*(AC472+AC473)+\n(AB473*AC474-AB474*AC473)*(AC473+AC474)+\n(AB474*AC475-AB475*AC474)*(AC474+AC475)+\n(AB475*AC476-AB476*AC475)*(AC475+AC476)+\n(AB476*AC477-AB477*AC476)*(AC476+AC477)+\n(AB477*AC478-AB478*AC477)*(AC477+AC478)+\n(AB478*AC479-AB479*AC478)*(AC478+AC479))/6/AC483)","v":0},"y=",{"$f":"+IF(AE483=0,0,-((AD460*AE461-AD461*AE460)*(AE460+AE461)+(AD461*AE462-AD462*AE461)*(AE461+AE462)+\n(AD462*AE463-AD463*AE462)*(AE462+AE463)+\n(AD463*AE464-AD464*AE463)*(AE463+AE464)+\n(AD464*AE465-AD465*AE464)*(AE464+AE465)+\n(AD465*AE466-AD466*AE465)*(AE465+AE466)+\n(AD466*AE467-AD467*AE466)*(AE466+AE467)+\n(AD467*AE468-AD468*AE467)*(AE467+AE468)+\n(AD468*AE469-AD469*AE468)*(AE468+AE469)+\n(AD469*AE470-AD470*AE469)*(AE469+AE470)+\n(AD470*AE471-AD471*AE470)*(AE470+AE471)+\n(AD471*AE472-AD472*AE471)*(AE471+AE472)+\n(AD472*AE473-AD473*AE472)*(AE472+AE473)+\n(AD473*AE474-AD474*AE473)*(AE473+AE474)+\n(AD474*AE475-AD475*AE474)*(AE474+AE475)+\n(AD475*AE476-AD476*AE475)*(AE475+AE476)+\n(AD476*AE477-AD477*AE476)*(AE476+AE477)+\n(AD477*AE478-AD478*AE477)*(AE477+AE478)+\n(AD478*AE479-AD479*AE478)*(AE478+AE479))/6/AE483)","v":0},null,null,null,null,"y=",{"$f":"+IF(AK483=0,0,-((AJ460*AK461-AJ461*AK460)*(AK460+AK461)+(AJ461*AK462-AJ462*AK461)*(AK461+AK462)+\n(AJ462*AK463-AJ463*AK462)*(AK462+AK463)+\n(AJ463*AK464-AJ464*AK463)*(AK463+AK464)+\n(AJ464*AK465-AJ465*AK464)*(AK464+AK465)+\n(AJ465*AK466-AJ466*AK465)*(AK465+AK466)+\n(AJ466*AK467-AJ467*AK466)*(AK466+AK467)+\n(AJ467*AK468-AJ468*AK467)*(AK467+AK468)+\n(AJ468*AK469-AJ469*AK468)*(AK468+AK469)+\n(AJ469*AK470-AJ470*AK469)*(AK469+AK470)+\n(AJ470*AK471-AJ471*AK470)*(AK470+AK471)+\n(AJ471*AK472-AJ472*AK471)*(AK471+AK472)+\n(AJ472*AK473-AJ473*AK472)*(AK472+AK473)+\n(AJ473*AK474-AJ474*AK473)*(AK473+AK474)+\n(AJ474*AK475-AJ475*AK474)*(AK474+AK475)+\n(AJ475*AK476-AJ476*AK475)*(AK475+AK476)+\n(AJ476*AK477-AJ477*AK476)*(AK476+AK477)+\n(AJ477*AK478-AJ478*AK477)*(AK477+AK478)+\n(AJ478*AK479-AJ479*AK478)*(AK478+AK479))/6/AK483)","v":0},null,null,"y=",{"$f":"+IF(AO483=0,0,-((AN460*AO461-AN461*AO460)*(AO460+AO461)+(AN461*AO462-AN462*AO461)*(AO461+AO462)+\n(AN462*AO463-AN463*AO462)*(AO462+AO463)+\n(AN463*AO464-AN464*AO463)*(AO463+AO464)+\n(AN464*AO465-AN465*AO464)*(AO464+AO465)+\n(AN465*AO466-AN466*AO465)*(AO465+AO466)+\n(AN466*AO467-AN467*AO466)*(AO466+AO467)+\n(AN467*AO468-AN468*AO467)*(AO467+AO468)+\n(AN468*AO469-AN469*AO468)*(AO468+AO469)+\n(AN469*AO470-AN470*AO469)*(AO469+AO470)+\n(AN470*AO471-AN471*AO470)*(AO470+AO471)+\n(AN471*AO472-AN472*AO471)*(AO471+AO472)+\n(AN472*AO473-AN473*AO472)*(AO472+AO473)+\n(AN473*AO474-AN474*AO473)*(AO473+AO474)+\n(AN474*AO475-AN475*AO474)*(AO474+AO475)+\n(AN475*AO476-AN476*AO475)*(AO475+AO476)+\n(AN476*AO477-AN477*AO476)*(AO476+AO477)+\n(AN477*AO478-AN478*AO477)*(AO477+AO478)+\n(AN478*AO479-AN479*AO478)*(AO478+AO479))/6/AO483)","v":11.895466666666669},"y=",{"$f":"+IF(AQ483=0,0,-((AP460*AQ461-AP461*AQ460)*(AQ460+AQ461)+(AP461*AQ462-AP462*AQ461)*(AQ461+AQ462)+\n(AP462*AQ463-AP463*AQ462)*(AQ462+AQ463)+\n(AP463*AQ464-AP464*AQ463)*(AQ463+AQ464)+\n(AP464*AQ465-AP465*AQ464)*(AQ464+AQ465)+\n(AP465*AQ466-AP466*AQ465)*(AQ465+AQ466)+\n(AP466*AQ467-AP467*AQ466)*(AQ466+AQ467)+\n(AP467*AQ468-AP468*AQ467)*(AQ467+AQ468)+\n(AP468*AQ469-AP469*AQ468)*(AQ468+AQ469)+\n(AP469*AQ470-AP470*AQ469)*(AQ469+AQ470)+\n(AP470*AQ471-AP471*AQ470)*(AQ470+AQ471)+\n(AP471*AQ472-AP472*AQ471)*(AQ471+AQ472)+\n(AP472*AQ473-AP473*AQ472)*(AQ472+AQ473)+\n(AP473*AQ474-AP474*AQ473)*(AQ473+AQ474)+\n(AP474*AQ475-AP475*AQ474)*(AQ474+AQ475)+\n(AP475*AQ476-AP476*AQ475)*(AQ475+AQ476)+\n(AP476*AQ477-AP477*AQ476)*(AQ476+AQ477)+\n(AP477*AQ478-AP478*AQ477)*(AQ477+AQ478)+\n(AP478*AQ479-AP479*AQ478)*(AQ478+AQ479))/6/AQ483)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AS483=0,0,-((AR460*AS461-AR461*AS460)*(AS460+AS461)+(AR461*AS462-AR462*AS461)*(AS461+AS462)+\n(AR462*AS463-AR463*AS462)*(AS462+AS463)+\n(AR463*AS464-AR464*AS463)*(AS463+AS464)+\n(AR464*AS465-AR465*AS464)*(AS464+AS465)+\n(AR465*AS466-AR466*AS465)*(AS465+AS466)+\n(AR466*AS467-AR467*AS466)*(AS466+AS467)+\n(AR467*AS468-AR468*AS467)*(AS467+AS468)+\n(AR468*AS469-AR469*AS468)*(AS468+AS469)+\n(AR469*AS470-AR470*AS469)*(AS469+AS470)+\n(AR470*AS471-AR471*AS470)*(AS470+AS471)+\n(AR471*AS472-AR472*AS471)*(AS471+AS472)+\n(AR472*AS473-AR473*AS472)*(AS472+AS473)+\n(AR473*AS474-AR474*AS473)*(AS473+AS474)+\n(AR474*AS475-AR475*AS474)*(AS474+AS475)+\n(AR475*AS476-AR476*AS475)*(AS475+AS476)+\n(AR476*AS477-AR477*AS476)*(AS476+AS477)+\n(AR477*AS478-AR478*AS477)*(AS477+AS478)+\n(AR478*AS479-AR479*AS478)*(AS478+AS479))/6/AS483)","v":0},"y=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$62","v":4.4000000000000004},null,null,null,null,"F=",{"$f":"-0.5*((BB462*BC463-BB463*BC462)+(BB463*BC464-BB464*BC463)+\n (BB464*BC465-BB465*BC464)+\n(BB465*BC466-BB466*BC465)+\n(BB466*BC467-BB467*BC466)+\n(BB467*BC468-BB468*BC467)+\n(BB468*BC469-BB469*BC468)+\n(BB469*BC470-BB470*BC469)+\n(BB470*BC471-BB471*BC470)+\n(BB471*BC472-BB472*BC471)+\n(BB472*BC473-BB473*BC472)+\n(BB473*BC474-BB474*BC473)+\n(BB474*BC475-BB475*BC474)+\n(BB475*BC476-BB476*BC475)+\n(BB476*BC477-BB477*BC476)+\n(BB477*BC478-BB478*BC477)+\n(BB478*BC479-BB479*BC478)+\n(BB479*BC480-BB480*BC479)\n)","v":-10.174207999999997},"F=",{"$f":"-0.5*((BD462*BE463-BD463*BE462)+(BD463*BE464-BD464*BE463)+\n (BD464*BE465-BD465*BE464)+\n(BD465*BE466-BD466*BE465)+\n(BD466*BE467-BD467*BE466)+\n(BD467*BE468-BD468*BE467)+\n(BD468*BE469-BD469*BE468)+\n(BD469*BE470-BD470*BE469)+\n(BD470*BE471-BD471*BE470)+\n(BD471*BE472-BD472*BE471)+\n(BD472*BE473-BD473*BE472)+\n(BD473*BE474-BD474*BE473)+\n(BD474*BE475-BD475*BE474)+\n(BD475*BE476-BD476*BE475)+\n(BD476*BE477-BD477*BE476)+\n(BD477*BE478-BD478*BE477)+\n(BD478*BE479-BD479*BE478)+\n(BD479*BE480-BD480*BE479)\n)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$61","v":4.08},null,null,null,null,"x=",0,"x=",0]
[null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$60","v":3.76},null,null,null,null,"y=",{"$f":"+IF(BC485=0,0,-((BB462*BC463-BB463*BC462)*(BC462+BC463)+(BB463*BC464-BB464*BC463)*(BC463+BC464)+\n(BB464*BC465-BB465*BC464)*(BC464+BC465)+\n(BB465*BC466-BB466*BC465)*(BC465+BC466)+\n(BB466*BC467-BB467*BC466)*(BC466+BC467)+\n(BB467*BC468-BB468*BC467)*(BC467+BC468)+\n(BB468*BC469-BB469*BC468)*(BC468+BC469)+\n(BB469*BC470-BB470*BC469)*(BC469+BC470)+\n(BB470*BC471-BB471*BC470)*(BC470+BC471)+\n(BB471*BC472-BB472*BC471)*(BC471+BC472)+\n(BB472*BC473-BB473*BC472)*(BC472+BC473)+\n(BB473*BC474-BB474*BC473)*(BC473+BC474)+\n(BB474*BC475-BB475*BC474)*(BC474+BC475)+\n(BB475*BC476-BB476*BC475)*(BC475+BC476)+\n(BB476*BC477-BB477*BC476)*(BC476+BC477)+\n(BB477*BC478-BB478*BC477)*(BC477+BC478)+\n(BB478*BC479-BB479*BC478)*(BC478+BC479)+\n(BB479*BC480-BB480*BC479)*(BC479+BC480)+\n(BB480*BC481-BB481*BC480)*(BC480+BC481))/6/BC485)","v":1.268387388974159},"y=",{"$f":"+IF(BE485=0,0,-((BD462*BE463-BD463*BE462)*(BE462+BE463)+(BD463*BE464-BD464*BE463)*(BE463+BE464)+\n(BD464*BE465-BD465*BE464)*(BE464+BE465)+\n(BD465*BE466-BD466*BE465)*(BE465+BE466)+\n(BD466*BE467-BD467*BE466)*(BE466+BE467)+\n(BD467*BE468-BD468*BE467)*(BE467+BE468)+\n(BD468*BE469-BD469*BE468)*(BE468+BE469)+\n(BD469*BE470-BD470*BE469)*(BE469+BE470)+\n(BD470*BE471-BD471*BE470)*(BE470+BE471)+\n(BD471*BE472-BD472*BE471)*(BE471+BE472)+\n(BD472*BE473-BD473*BE472)*(BE472+BE473)+\n(BD473*BE474-BD474*BE473)*(BE473+BE474)+\n(BD474*BE475-BD475*BE474)*(BE474+BE475)+\n(BD475*BE476-BD476*BE475)*(BE475+BE476)+\n(BD476*BE477-BD477*BE476)*(BE476+BE477)+\n(BD477*BE478-BD478*BE477)*(BE477+BE478)+\n(BD478*BE479-BD479*BE478)*(BE478+BE479)+\n(BD479*BE480-BD480*BE479)*(BE479+BE480)+\n(BD480*BE481-BD481*BE480)*(BE480+BE481))/6/BE485)","v":0}]
[null,"OPTEREĆENJE TEMELJEM",null,null,null,null,null,null,null," (TERZAGHY)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BK307-BQ306","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$59","v":3.44}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.8,0,{"$f":"+'Analiza i dimenzioniranje'!$U$58","v":3.14}]
[null,"KONTINUIRANO OPTEREĆENJE",null,"P - D=",{"$f":"IF('Analiza i dimenzioniranje'!$E$28-I490<=0,0,+'Analiza i dimenzioniranje'!$E$28-I490)","v":{"$error":"#VALUE!"}},"kN/m2","raster. iskopom   D=y*Df =",null,{"$f":"+'Analiza i dimenzioniranje'!$D$16*('Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20-D496)","v":{"$error":"#VALUE!"}},"kN/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.32,0,{"$f":"+'Analiza i dimenzioniranje'!$U$57","v":2.8}]
[null," visina zida i temelja",null,"H =",{"$f":"+E411","v":{"$error":"#VALUE!"}},"m",{"$f":"E495","v":6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.64,0,{"$f":"+'Analiza i dimenzioniranje'!$U$56","v":2.48}]
[null,"visina opterećenja iznad vrha zida",null,"h =",{"$f":"+E412","v":-1},"m",{"$f":"SQRT(E495^2+E494^2)","v":6.7082039324993694},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.96,0,{"$f":"+'Analiza i dimenzioniranje'!$U$55","v":2.16}]
[null,"širina temelja",null,"b =",{"$f":"+E413","v":1},"m   ",{"$f":"E494+E493","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.28,0,{"$f":"+'Analiza i dimenzioniranje'!$U$54","v":1.84}]
[null,"udaljenost temelja od zida",null,"D =",{"$f":"+E414","v":3},"m    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6,0,{"$f":"+'Analiza i dimenzioniranje'!$U$53","v":1.52}]
[null,"1/2 dužine temelja",null,"L/2=a=",{"$f":"+E415","v":6},"m",{"$f":"SQRT(G491^2+G493^2)","v":7.2111025509279782},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,0,{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
["DNO TEMELJA NA VISINI","PRESJEK NA Visini ",null,{"$f":"ROUND('Analiza i dimenzioniranje'!U57,2)","v":2.8},null,"Presjek III - III",null,"Presjek VI",null,"Presjek VII-VII",null,"Presjek VIII-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"Presjek XIV-XIV",null,"Presjek XV-XV",null,"PresjekXVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX",null,null,null,null,null,null,null,null,null,null,6.2,{"$f":"+IF(AW497>=AW$299,0,BK315-BQ314)","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
[null,null,null,null,null,"Visina djelovanja","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja ","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja",null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2",{"$f":"+AU500","v":0},"SQhi=",6.2]
[null,null,null,{"$f":"+F499","v":0},{"$f":"+D498-E496","v":0},"III",{"$f":"+D496","v":2.8},"IV",{"$f":"+G498","v":2.8},"VII",{"$f":"+G498","v":2.8},"VIII",{"$f":"+I498","v":2.8},"IX",{"$f":"+G498","v":2.8},"X",{"$f":"+O498","v":2.8},"XI",{"$f":"+G498","v":2.8},"XII",{"$f":"+'Analiza i dimenzioniranje'!S132","v":0},"XIII",{"$f":"+G498","v":2.8},"XIV",{"$f":"+W498","v":2.8},"XV",{"$f":"+G498","v":2.8},"XVI",{"$f":"+I498","v":2.8},"XVII",{"$f":"+AC498","v":2.8},"XVIII",{"$f":"+AC498","v":2.8},"XIX",{"$f":"+AE498","v":2.8},"XX",{"$f":"+AG498","v":2.8},null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
[null,null,null,0,{"$f":"IF(D498>E$296,D498,E$296)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja"]
[null,null,null,0,{"$f":"IF(AW479>G$298,0,AW479)","v":0},0,0,{"$f":"+F500","v":0},{"$f":"+G500","v":0},0,0,0,{"$f":"+E499","v":0},0,0,0,{"$f":"+O500","v":0},0,{"$f":"+AS500","v":0},0,{"$f":"+S500","v":0},0,{"$f":"+AS500","v":0},0,{"$f":"+W500","v":0},0,{"$f":"+S500","v":0},0,{"$f":"+AA500","v":0},0,{"$f":"+AU477","v":12.686400000000001},0,{"$f":"+AU477","v":12.686400000000001},0,{"$f":"+AG500","v":12.686400000000001},{"$f":"+AD500","v":0},{"$f":"+AG500","v":12.686400000000001},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"XVIII",{"$f":"+'Analiza i dimenzioniranje'!U274","v":0},"XIX",{"$f":"+'Analiza i dimenzioniranje'!U273","v":0},"XX",{"$f":"'Analiza i dimenzioniranje'!U272","v":0}]
[null,null,null,0,{"$f":"+AW480","v":6.0000000000000009},0,0,{"$f":"+F501","v":0},{"$f":"+G501","v":0},0,0,0,{"$f":"+E500","v":0},0,0,0,{"$f":"+O501","v":0},0,0,0,{"$f":"+S501","v":0},0,0,0,{"$f":"+W501","v":0},0,{"$f":"+S501","v":0},0,{"$f":"+AA501","v":0},0,0,0,0,0,{"$f":"+AG501","v":0},{"$f":"+AD501","v":0},{"$f":"+AG501","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD539","v":0},{"$f":"+BB501-BC500","v":0},{"$f":"+AD539","v":0},{"$f":"+BD501-BE500","v":0},{"$f":"+AD539","v":0},{"$f":"+'Analiza i dimenzioniranje'!E270","v":""}]
[null,null,null,0,{"$f":"IF(AW481>G$298,0,AW481)","v":0},0,0,0,{"$f":"+G502","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+AU517","v":11.56},{"$f":"+AT540","v":0},{"$f":"+BC502","v":11.56},0,{"$f":"+AE540","v":11.56}]
[null,null,null,{"$f":"+AV479","v":{"$error":"#REF!"}},0,0,0,{"$f":"+F503","v":0},0,{"$f":"+F501","v":0},0,{"$f":"+D500","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE541","v":0}]
[null,null,null,0,0,0,0,0,0,{"$f":"+F502","v":0},0,{"$f":"+D501","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE542","v":0}]
[null,null,null,0,0,0,0,0,0,0,0,{"$f":"+D502","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE543","v":0}]
[null,null,null,0,4.4000000000000004,0,0,0,0,0,0,{"$f":"+D299","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AE505","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE544","v":0}]
[null,null,null,0,4.08,0,0,0,0,0,0,{"$f":"+D504","v":0},0,{"$f":"+J505","v":0},0,{"$f":"+L505","v":0},0,0,0,{"$f":"+P505","v":0},0,0,0,{"$f":"+T505","v":0},0,0,0,{"$f":"+X505","v":0},0,0,{"$f":"+AU484","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+BC507","v":0}]
[null,null,null,0,3.76,0,0,0,0,0,0,0,0,{"$f":"+J506","v":0},0,{"$f":"+L506","v":0},0,0,0,{"$f":"+P506","v":0},0,0,0,{"$f":"+T506","v":0},0,0,{"$f":"+AA507","v":0},{"$f":"+X506","v":0},0,0,{"$f":"+AU485","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,"+",3.44,0,0,0,0,{"$f":"+F509","v":0},0,{"$f":"+D506","v":0},0,{"$f":"+J507","v":0},0,{"$f":"+N509","v":0},{"$f":"+O509","v":0},0,0,{"$f":"+R509","v":0},{"$f":"+S509","v":0},0,0,{"$f":"+V509","v":0},0,0,{"$f":"+S509","v":0},{"$f":"+Z509","v":0},{"$f":"+AA509","v":0},0,{"$f":"+AU486","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+AV486","v":0},3.14,0,0,0,0,0,0,{"$f":"+J510","v":0},0,{"$f":"+L510","v":0},{"$f":"+M510","v":0},{"$f":"+N510","v":0},{"$f":"+O510","v":0},{"$f":"+P510","v":0},{"$f":"+Q510","v":0},{"$f":"+R510","v":0},{"$f":"+S510","v":0},{"$f":"+T510","v":0},{"$f":"+U510","v":0},{"$f":"+V510","v":0},0,0,0,{"$f":"+Z510","v":0},{"$f":"+AA510","v":0},0,0,{"$f":"+AD510","v":0},{"$f":"+AE510","v":0},{"$f":"+AF510","v":0},0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+AV487","v":0},2.8,{"$f":"+B504","v":0},0,0,0,0,0,{"$f":"+J511","v":0},{"$f":"+K511","v":0},{"$f":"+J511","v":0},{"$f":"+M511","v":0},{"$f":"+L511","v":0},{"$f":"+O511","v":0},{"$f":"+N511","v":0},{"$f":"+Q511","v":0},0,{"$f":"+S511","v":0},{"$f":"+T511","v":0},{"$f":"+Y511","v":0},{"$f":"+B505","v":0},{"$f":"+U511","v":0},{"$f":"+B505","v":0},0,{"$f":"+Z511","v":0},{"$f":"+U511","v":0},{"$f":"+AB511","v":0},{"$f":"+AU488","v":0},{"$f":"+AB511","v":0},{"$f":"+AC511","v":0},{"$f":"+AF511","v":0},0,0,{"$f":"+BC473","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+D471","v":0},2.48,0,{"$f":"+AW490","v":2.8},0,2.8,0,{"$f":"+E511","v":2.8},{"$f":"+J512","v":0},2.8,{"$f":"+J512","v":0},{"$f":"+M512","v":2.8},{"$f":"+L512","v":0},{"$f":"+O512","v":2.8},0,{"$f":"+Q512","v":2.8},0,{"$f":"+S512","v":2.8},0,{"$f":"+U512","v":2.8},0,{"$f":"+W512","v":2.8},0,{"$f":"+Y512","v":2.8},0,{"$f":"+AA512","v":2.8},0,{"$f":"+AC512","v":2.8},0,{"$f":"+AE512","v":2.8},{"$f":"+AF512","v":0},2.8,0,{"$f":"+AI512","v":2.8},null,{"$f":"+D512","v":0},{"$f":"$E$504^2+AM512^2","v":0},{"$f":"$G$493^2+AM512^2","v":16},{"$f":"$G$505^2+AM512^2","v":0},{"$f":"IF(AM512=0,0,$E$450/(PI())*(ATAN(($E$495*$G$493)/(AM512*SQRT(AP512)))-$E$495*$G$453*AM512/(AO512*SQRT(AP512))))","v":0},null,{"$f":"+AM512","v":0},{"$f":"$E$455^2+AS512^2","v":36},{"$f":"$E$494^2+AS512^2","v":9},{"$f":"$G$452^2+AS512^2","v":45.000000000000007},{"$f":"IF(AS512=0,0,($E$490/(PI()))*(ATAN(($E$455*$E$454)/(AS512*SQRT(AV512)))-$E$455*$E$454*AS512/(AU512*SQRT(AV512))))","v":0},{"$f":"(+AQ512-AW512)*2","v":0},null,null,null,0,0,0,0,0,0]
[null,null,null,0.32,2.16,{"$f":"+AX513","v":{"$error":"#VALUE!"}},2.48,{"$error":"#VALUE!"},2.48,{"$error":"#VALUE!"},{"$f":"+E512","v":2.48},{"$error":"#VALUE!"},2.48,{"$f":"+J513","v":{"$error":"#VALUE!"}},{"$f":"+M513","v":2.48},0,{"$f":"+Q512","v":2.8},0,{"$f":"+AS513","v":0.32},0,0,0,{"$f":"+AS513","v":0.32},0,0,0,0.32,{"$f":"+Z513","v":0},0,{"$f":"+AB513","v":0},{"$f":"+AU490","v":0.32},{"$f":"+AB513","v":0},0,0,0,0,{"$f":"+BC475","v":0.32},null,0.32,{"$f":"$E$494^2+AM513^2","v":9.1023999999999994},{"$f":"$G$493^2+AM513^2","v":16.102399999999999},{"$f":"$G$495^2+AM513^2","v":52.102399999999996},{"$f":"IF(AM513=0,0,$E$490/(PI())*(ATAN(($E$495*$G$493)/(AM513*SQRT(AP513)))-$E$495*$G$493*AM513/(AO513*SQRT(AP513))))","v":{"$error":"#VALUE!"}},null,0.32,{"$f":"$E$495^2+AS513^2","v":36.102400000000003},9.1023999999999994,{"$f":"$G$492^2+AS513^2","v":45.10240000000001},{"$f":"IF(AS513=0,0,($E$490/(PI()))*(ATAN(($E$495*$E$494)/(AS513*SQRT(AV513)))-$E$495*$E$494*AS513/(AU513*SQRT(AV513))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,0,0,0,0,0,0]
[null,null,null,0.64,1.84,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},{"$f":"+E513","v":2.16},{"$error":"#VALUE!"},2.16,0,{"$f":"+O513","v":2.48},0,0,0,{"$f":"+AS514","v":0.64},0,0,0,{"$f":"+AS514","v":0.64},0,0,0,0.64,0,0,0,{"$f":"+AU491","v":0.64},0,0,0,0,0,0.64,null,0.64,{"$f":"$E$494^2+AM514^2","v":9.4095999999999993},{"$f":"$G$493^2+AM514^2","v":16.409600000000001},{"$f":"$G$495^2+AM514^2","v":52.40959999999999},{"$f":"IF(AM514=0,0,$E$490/(PI())*(ATAN(($E$495*$G$493)/(AM514*SQRT(AP514)))-$E$495*$G$493*AM514/(AO514*SQRT(AP514))))","v":{"$error":"#VALUE!"}},null,0.64,{"$f":"$E$495^2+AS514^2","v":36.409599999999998},9.4095999999999993,{"$f":"$G$492^2+AS514^2","v":45.409600000000005},{"$f":"IF(AS514=0,0,($E$490/(PI()))*(ATAN(($E$495*$E$494)/(AS514*SQRT(AV514)))-$E$495*$E$494*AS514/(AU514*SQRT(AV514))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,0,0,0,0,0,0]
[null,null,null,0.96,1.52,{"$error":"#VALUE!"},1.84,{"$error":"#VALUE!"},1.84,{"$error":"#VALUE!"},{"$f":"+E514","v":1.84},0,{"$f":"+M514","v":2.16},0,0,0,0,0,{"$f":"+AS515","v":0.96},0,0,0,{"$f":"+AS515","v":0.96},0,0,0,0.96,0,0,0,{"$f":"+AU492","v":0.96},0,0,0,0,0,0.96,null,0.96,{"$f":"$E$494^2+AM515^2","v":9.9215999999999998},{"$f":"$G$493^2+AM515^2","v":16.921600000000002},{"$f":"$G$495^2+AM515^2","v":52.921599999999991},{"$f":"IF(AM515=0,0,$E$490/(PI())*(ATAN(($E$495*$G$493)/(AM515*SQRT(AP515)))-$E$495*$G$493*AM515/(AO515*SQRT(AP515))))","v":{"$error":"#VALUE!"}},null,0.96,{"$f":"$E$495^2+AS515^2","v":36.921599999999998},9.9215999999999998,{"$f":"$G$492^2+AS515^2","v":45.921600000000005},{"$f":"IF(AS515=0,0,($E$490/(PI()))*(ATAN(($E$495*$E$494)/(AS515*SQRT(AV515)))-$E$495*$E$494*AS515/(AU515*SQRT(AV515))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,0,2.48,0,2.48,0,2.48]
[null,null,null,1.28,1.2,{"$error":"#VALUE!"},1.52,{"$error":"#VALUE!"},1.52,0,{"$f":"+K515","v":1.84},0,{"$f":"+N516","v":0},0,{"$f":"+AM516","v":1.28},0,0,0,{"$f":"+AS516","v":1.28},0,0,0,{"$f":"+AS516","v":1.28},0,0,0,1.28,0,0,0,{"$f":"+AE515","v":0.96},0,0,0,0,0,1.28,null,1.28,10.638400000000001,17.638400000000001,53.63839999999999,{"$error":"#VALUE!"},null,1.28,37.638399999999997,10.638400000000001,46.638400000000004,{"$f":"IF(AS516=0,0,($E$490/(PI()))*(ATAN(($E$495*$E$494)/(AS516*SQRT(AV516)))-$E$495*$E$494*AS516/(AU516*SQRT(AV516))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,0,0,0,0,0,0]
[null,null,null,1.6,{"$f":"+AW496","v":1.2},{"$error":"#VALUE!"},1.2,0,{"$f":"+I516","v":1.52},0,{"$f":"+E516","v":1.2},0,{"$f":"+N517","v":0},0,{"$f":"+AM517","v":1.6},0,0,0,{"$f":"+AS517","v":1.6},0,0,0,{"$f":"+AS517","v":1.6},0,0,0,1.6,0,0,0,{"$f":"+AU494","v":1.6},0,0,0,0,0,1.6,null,1.6,11.56,18.560000000000002,54.559999999999995,{"$error":"#VALUE!"},null,1.6,38.56,11.56,47.560000000000009,{"$f":"IF(AS517=0,0,($E$490/(PI()))*(ATAN(($E$495*$E$454)/(AS517*SQRT(AV517)))-$E$495*$E$494*AS517/(AU517*SQRT(AV517))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,0,0,0,0,0,0]
[null,null,null,null,{"$f":"+AW497","v":6.2},0,{"$f":"+E517","v":1.2},0,{"$f":"+G518","v":1.2},0,{"$f":"+I518","v":1.2},0,{"$f":"+K518","v":1.2},0,{"$f":"+M518","v":1.2},0,{"$f":"+O518","v":1.2},0,{"$f":"+Q518","v":1.2},0,{"$f":"+S518","v":1.2},0,{"$f":"+U518","v":1.2},{"$f":"+P518","v":0},{"$f":"+W518","v":1.2},0,{"$f":"+Y518","v":1.2},0,{"$f":"+AA518","v":1.2},0,{"$f":"+AC518","v":1.2},0,{"$f":"+AC518","v":1.2},0,1.2,{"$f":"+AD518","v":0},1.2,null,null,0,{"$f":"+AM518","v":0},0,{"$f":"+AQ517","v":{"$error":"#VALUE!"}},0,{"$f":"+AO518","v":0},0,{"$f":"+S541","v":0},{"$f":"BK338-BQ337","v":0},{"$f":"IF(AV516>AW$299,AV516,AW$299)","v":46.638400000000004},null,null,null,null,{"$f":"+AT554","v":36.102400000000003},0,0,0,0,0]
[null,null,null,null,{"$f":"+E522","v":0},0,{"$f":"+E518","v":6.2},0,{"$f":"+G519","v":6.2},0,{"$f":"+I519","v":6.2},0,{"$f":"+K519","v":6.2},0,{"$f":"+M519","v":6.2},0,{"$f":"+O519","v":6.2},0,{"$f":"+Q519","v":6.2},0,{"$f":"+S519","v":6.2},0,{"$f":"+U519","v":6.2},{"$f":"+P519","v":0},{"$f":"+W519","v":6.2},{"$f":"+N519","v":0},{"$f":"+Y519","v":6.2},0,{"$f":"+AA519","v":6.2},0,{"$f":"+AC519","v":6.2},0,{"$f":"+AC519","v":6.2},0,6.2,{"$f":"+AD519","v":0},6.2,null,null,0,0,0,{"$f":"+AS519","v":0},0,0,0,0,{"$f":"#REF!-#REF!","v":{"$error":"#REF!"}},{"$f":"+AW520","v":6.0000000000000009},null,null,null,null,{"$f":"+AT555","v":36.409599999999998},0,{"$f":"+AD555","v":0},0,0,0]
[null,null,null,"Ukupni pritisak",null,"SQhi=",{"$f":"+G523","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I523","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K523","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+M523","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+O523","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+Q523","v":0},"SQhi=",{"$f":"+S523","v":0},"SQhi=",{"$f":"+U523","v":0},"SQhi=",{"$f":"+W523","v":0},"SQhi=",{"$f":"+Y523","v":0},"SQhi=",{"$f":"+AA523","v":0},"SQhi=",{"$f":"+AC523","v":0},"SQhi=",{"$f":"+AE523","v":0},"SQhi=",{"$f":"+AG523","v":0},"SQhi=",{"$f":"+AI523","v":0},"SQhi=",{"$f":"+AK523","v":0},null,null,"SQhi=",{"$f":"+AO523","v":81.420799999999986},"SQhi=",{"$f":"+AQ523","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AS523","v":0},"SQhi=",0,{"$f":"BK339-BQ338","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$67","v":6.0000000000000009},null,null,null,null,0,1.2,0,{"$f":"+BE519","v":0},0,{"$f":"+AE558","v":1.2}]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G525","v":{"$error":"#VALUE!"}}," y=",{"$f":"+I525","v":{"$error":"#VALUE!"}}," y=",{"$f":"+K525","v":{"$error":"#VALUE!"}}," y=",{"$f":"+M525","v":{"$error":"#VALUE!"}}," y=",{"$f":"+O525","v":{"$error":"#VALUE!"}}," y=",{"$f":"+Q525","v":0}," y=",{"$f":"+S525","v":0}," y=",{"$f":"+U525","v":0}," y=",{"$f":"+W525","v":0}," y=",{"$f":"+Y525","v":0}," y=",{"$f":"+AA525","v":0}," y=",{"$f":"+AC525","v":0}," y=",{"$f":"+AE525","v":0}," y=",{"$f":"+AG525","v":0}," y=",{"$f":"+AI525","v":0}," y=",{"$f":"+AK525","v":0},null,null," y=",{"$f":"+AO525","v":10.790949347586858}," y=",{"$f":"+AQ525","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AS525","v":0}," y=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$66","v":5.6800000000000006},null,null,null,null,0,6.2,0,{"$f":"+AK559","v":6.2},0,{"$f":"+AE559","v":6.2}]
[null,null,null,"krak za presjek III -III",null,"z=",{"$f":"+G521-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I521-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K521-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M521-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+O521-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+Q521-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+S521-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+U521-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z=",{"$f":"+W521-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+Y521-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AA521-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AC521-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AE521-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AG521-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AI521-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AK521-'Analiza i dimenzioniranje'!$E$52","v":-1.2},null,null,"z=",{"$f":"+AO521-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":10.290949347586858},"z=",{"$f":"+AQ521-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AS521-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$65","v":5.36},null,null,null,null,"SQhi=",{"$f":"+BC525","v":-21.845759999999999},"SQhi=",{"$f":"+BE525","v":0}]
[null,null,null,"x=",0,"F=",{"$f":"-0.5*(+\n (F502*G503-F503*G502)+\n(F503*G504-F504*G503)+\n(F504*G505-F505*G504)+\n(F505*G506-F506*G505)+\n(F506*G507-F507*G506)+\n(F507*G508-F508*G507)+\n(F508*G509-F509*G508)+\n(F509*G510-F510*G509)+\n(F510*G511-F511*G510)+\n(F511*G512-F512*G511)+\n(F512*G513-F513*G512)+\n(F513*G514-F514*G513)+\n(F514*G515-F515*G514)+\n(F515*G516-F516*G515)+\n(F516*G517-F517*G516)+\n(F517*G518-F518*G517)+\n(F518*G519-F519*G518))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (H502*I503-H503*I502)+\n(H503*I504-H504*I503)+\n(H504*I505-H505*I504)+\n(H505*I506-H506*I505)+\n(H506*I507-H507*I506)+\n(H507*I508-H508*I507)+\n(H508*I509-H509*I508)+\n(H509*I510-H510*I509)+\n(H510*I511-H511*I510)+\n(H511*I512-H512*I511)+\n(H512*I513-H513*I512)+\n(H513*I514-H514*I513)+\n(H514*I515-H515*I514)+\n(H515*I516-H516*I515)+\n(H516*I517-H517*I516)+\n(H517*I518-H518*I517)+\n(H518*I519-H519*I518))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((J500*K501-J501*K500)+(J501*K502-J502*K501)+\n (J502*K503-J503*K502)+\n(J503*K504-J504*K503)+\n(J504*K505-J505*K504)+\n(J505*K506-J506*K505)+\n(J506*K507-J507*K506)+\n(J507*K508-J508*K507)+\n(J508*K509-J509*K508)+\n(J509*K510-J510*K509)+\n(J510*K511-J511*K510)+\n(J511*K512-J512*K511)+\n(J512*K513-J513*K512)+\n(J513*K514-J514*K513)+\n(J514*K515-J515*K514)+\n(J515*K516-J516*K515)+\n(J516*K517-J517*K516)+\n(J517*K518-J518*K517)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (L502*M503-L503*M502)+\n(L503*M504-L504*M503)+\n(L504*M505-L505*M504)+\n(L505*M506-L506*M505)+\n(L506*M507-L507*M506)+\n(L507*M508-L508*M507)+\n(L508*M509-L509*M508)+\n(L509*M510-L510*M509)+\n(L510*M511-L511*M510)+\n(L511*M512-L512*M511)+\n(L512*M513-L513*M512)+\n(L513*M514-L514*M513)+\n(L514*M515-L515*M514)+\n(L515*M516-L516*M515)+\n(L516*M517-L517*M516)+\n(L517*M518-L518*M517)+\n(L518*M519-L519*M518))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (N502*O503-N503*O502)+\n(N503*O504-N504*O503)+\n(N504*O505-N505*O504)+\n(N505*O506-N506*O505)+\n(N506*O507-N507*O506)+\n(N507*O508-N508*O507)+\n(N508*O509-N509*O508)+\n(N509*O510-N510*O509)+\n(N510*O511-N511*O510)+\n(N511*O512-N512*O511)+\n(N512*O513-N513*O512)+\n(N513*O514-N514*O513)+\n(N514*O515-N515*O514)+\n(N515*O516-N516*O515)+\n(N516*O517-N517*O516)+\n(N517*O518-N518*O517)+\n(N518*O519-N519*O518))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (P502*Q503-P503*Q502)+\n(P503*Q504-P504*Q503)+\n(P504*Q505-P505*Q504)+\n(P505*Q506-P506*Q505)+\n(P506*Q507-P507*Q506)+\n(P507*Q508-P508*Q507)+\n(P508*Q509-P509*Q508)+\n(P509*Q510-P510*Q509)+\n(P510*Q511-P511*Q510)+\n(P511*Q512-P512*Q511)+\n(P512*Q513-P513*Q512)+\n(P513*Q514-P514*Q513)+\n(P514*Q515-P515*Q514)+\n(P515*Q516-P516*Q515)+\n(P516*Q517-P517*Q516)+\n(P517*Q518-P518*Q517)+\n(P518*Q519-P519*Q518))","v":0},"F=",{"$f":"-0.5*((R500*S501-R501*S500)+(R501*S502-R502*S501)+\n (R502*S503-R503*S502)+\n(R503*S504-R504*S503)+\n(R504*S505-R505*S504)+\n(R505*S506-R506*S505)+\n(R506*S507-R507*S506)+\n(R507*S508-R508*S507)+\n(R508*S509-R509*S508)+\n(R509*S510-R510*S509)+\n(R510*S511-R511*S510)+\n(R511*S512-R512*S511)+\n(R512*S513-R513*S512)+\n(R513*S514-R514*S513)+\n(R514*S515-R515*S514)+\n(R515*S516-R516*S515)+\n(R516*S517-R517*S516)+\n(R517*S518-R518*S517)\n)","v":0},"F=",{"$f":"-0.5*(+\n (T502*U503-T503*U502)+\n(T503*U504-T504*U503)+\n(T504*U505-T505*U504)+\n(T505*U506-T506*U505)+\n(T506*U507-T507*U506)+\n(T507*U508-T508*U507)+\n(T508*U509-T509*U508)+\n(T509*U510-T510*U509)+\n(T510*U511-T511*U510)+\n(T511*U512-T512*U511)+\n(T512*U513-T513*U512)+\n(T513*U514-T514*U513)+\n(T514*U515-T515*U514)+\n(T515*U516-T516*U515)+\n(T516*U517-T517*U516)+\n(T517*U518-T518*U517)+\n(T518*U519-T519*U518))","v":0},"F=",{"$f":"-0.5*(+\n (V502*W503-V503*W502)+\n(V503*W504-V504*W503)+\n(V504*W505-V505*W504)+\n(V505*W506-V506*W505)+\n(V506*W507-V507*W506)+\n(V507*W508-V508*W507)+\n(V508*W509-V509*W508)+\n(V509*W510-V510*W509)+\n(V510*W511-V511*W510)+\n(V511*W512-V512*W511)+\n(V512*W513-V513*W512)+\n(V513*W514-V514*W513)+\n(V514*W515-V515*W514)+\n(V515*W516-V516*W515)+\n(V516*W517-V517*W516)+\n(V517*W518-V518*W517)+\n(V518*W519-V519*W518))","v":0},"F=",{"$f":"-0.5*(+\n (X502*Y503-X503*Y502)+\n(X503*Y504-X504*Y503)+\n(X504*Y505-X505*Y504)+\n(X505*Y506-X506*Y505)+\n(X506*Y507-X507*Y506)+\n(X507*Y508-X508*Y507)+\n(X508*Y509-X509*Y508)+\n(X509*Y510-X510*Y509)+\n(X510*Y511-X511*Y510)+\n(X511*Y512-X512*Y511)+\n(X512*Y513-X513*Y512)+\n(X513*Y514-X514*Y513)+\n(X514*Y515-X515*Y514)+\n(X515*Y516-X516*Y515)+\n(X516*Y517-X517*Y516)+\n(X517*Y518-X518*Y517)+\n(X518*Y519-X519*Y518))","v":0},"F=",{"$f":"-0.5*((Z500*AA501-Z501*AA500)+(Z501*AA502-Z502*AA501)+\n (Z502*AA503-Z503*AA502)+\n(Z503*AA504-Z504*AA503)+\n(Z504*AA505-Z505*AA504)+\n(Z505*AA506-Z506*AA505)+\n(Z506*AA507-Z507*AA506)+\n(Z507*AA508-Z508*AA507)+\n(Z508*AA509-Z509*AA508)+\n(Z509*AA510-Z510*AA509)+\n(Z510*AA511-Z511*AA510)+\n(Z511*AA512-Z512*AA511)+\n(Z512*AA513-Z513*AA512)+\n(Z513*AA514-Z514*AA513)+\n(Z514*AA515-Z515*AA514)+\n(Z515*AA516-Z516*AA515)+\n(Z516*AA517-Z517*AA516)+\n(Z517*AA518-Z518*AA517)\n)","v":0},"F=",{"$f":"-0.5*(+\n (AB502*AC503-AB503*AC502)+\n(AB503*AC504-AB504*AC503)+\n(AB504*AC505-AB505*AC504)+\n(AB505*AC506-AB506*AC505)+\n(AB506*AC507-AB507*AC506)+\n(AB507*AC508-AB508*AC507)+\n(AB508*AC509-AB509*AC508)+\n(AB509*AC510-AB510*AC509)+\n(AB510*AC511-AB511*AC510)+\n(AB511*AC512-AB512*AC511)+\n(AB512*AC513-AB513*AC512)+\n(AB513*AC514-AB514*AC513)+\n(AB514*AC515-AB515*AC514)+\n(AB515*AC516-AB516*AC515)+\n(AB516*AC517-AB517*AC516)+\n(AB517*AC518-AB518*AC517)+\n(AB518*AC519-AB519*AC518))","v":0},"F=",{"$f":"-0.5*(+\n (AD502*AE503-AD503*AE502)+\n(AD503*AE504-AD504*AE503)+\n(AD504*AE505-AD505*AE504)+\n(AD505*AE506-AD506*AE505)+\n(AD506*AE507-AD507*AE506)+\n(AD507*AE508-AD508*AE507)+\n(AD508*AE509-AD509*AE508)+\n(AD509*AE510-AD510*AE509)+\n(AD510*AE511-AD511*AE510)+\n(AD511*AE512-AD512*AE511)+\n(AD512*AE513-AD513*AE512)+\n(AD513*AE514-AD514*AE513)+\n(AD514*AE515-AD515*AE514)+\n(AD515*AE516-AD516*AE515)+\n(AD516*AE517-AD517*AE516)+\n(AD517*AE518-AD518*AE517)+\n(AD518*AE519-AD519*AE518))","v":0},"F=",{"$f":"-0.5*(+\n (AF502*AG503-AF503*AG502)+\n(AF503*AG504-AF504*AG503)+\n(AF504*AG505-AF505*AG504)+\n(AF505*AG506-AF506*AG505)+\n(AF506*AG507-AF507*AG506)+\n(AF507*AG508-AF508*AG507)+\n(AF508*AG509-AF509*AG508)+\n(AF509*AG510-AF510*AG509)+\n(AF510*AG511-AF511*AG510)+\n(AF511*AG512-AF512*AG511)+\n(AF512*AG513-AF513*AG512)+\n(AF513*AG514-AF514*AG513)+\n(AF514*AG515-AF515*AG514)+\n(AF515*AG516-AF516*AG515)+\n(AF516*AG517-AF517*AG516)+\n(AF517*AG518-AF518*AG517)+\n(AF518*AG519-AF519*AG518))","v":0},"F=",{"$f":"-0.5*((AH500*AI501-AH501*AI500)+(AH501*AI502-AH502*AI501)+\n (AH502*AI503-AH503*AI502)+\n(AH503*AI504-AH504*AI503)+\n(AH504*AI505-AH505*AI504)+\n(AH505*AI506-AH506*AI505)+\n(AH506*AI507-AH507*AI506)+\n(AH507*AI508-AH508*AI507)+\n(AH508*AI509-AH509*AI508)+\n(AH509*AI510-AH510*AI509)+\n(AH510*AI511-AH511*AI510)+\n(AH511*AI512-AH512*AI511)+\n(AH512*AI513-AH513*AI512)+\n(AH513*AI514-AH514*AI513)+\n(AH514*AI515-AH515*AI514)+\n(AH515*AI516-AH516*AI515)+\n(AH516*AI517-AH517*AI516)+\n(AH517*AI518-AH518*AI517)\n)","v":0},"F=",{"$f":"-0.5*((AJ500*AK501-AJ501*AK500)+(AJ501*AK502-AJ502*AK501)+\n (AJ502*AK503-AJ503*AK502)+\n(AJ503*AK504-AJ504*AK503)+\n(AJ504*AK505-AJ505*AK504)+\n(AJ505*AK506-AJ506*AK505)+\n(AJ506*AK507-AJ507*AK506)+\n(AJ507*AK508-AJ508*AK507)+\n(AJ508*AK509-AJ509*AK508)+\n(AJ509*AK510-AJ510*AK509)+\n(AJ510*AK511-AJ511*AK510)+\n(AJ511*AK512-AJ512*AK511)+\n(AJ512*AK513-AJ513*AK512)+\n(AJ513*AK514-AJ514*AK513)+\n(AJ514*AK515-AJ515*AK514)+\n(AJ515*AK516-AJ516*AK515)+\n(AJ516*AK517-AJ517*AK516)+\n(AJ517*AK518-AJ518*AK517)\n)","v":0},null,null,"F=",{"$f":"-0.5*((AN500*AO501-AN501*AO500)+(AN501*AO502-AN502*AO501)+\n (AN502*AO503-AN503*AO502)+\n(AN503*AO504-AN504*AO503)+\n(AN504*AO505-AN505*AO504)+\n(AN505*AO506-AN506*AO505)+\n(AN506*AO507-AN507*AO506)+\n(AN507*AO508-AN508*AO507)+\n(AN508*AO509-AN509*AO508)+\n(AN509*AO510-AN510*AO509)+\n(AN510*AO511-AN511*AO510)+\n(AN511*AO512-AN512*AO511)+\n(AN512*AO513-AN513*AO512)+\n(AN513*AO514-AN514*AO513)+\n(AN514*AO515-AN515*AO514)+\n(AN515*AO516-AN516*AO515)+\n(AN516*AO517-AN517*AO516)+\n(AN517*AO518-AN518*AO517)\n)","v":81.420799999999986},"F=",{"$f":"-0.5*((AP500*AQ501-AP501*AQ500)+(AP501*AQ502-AP502*AQ501)+\n (AP502*AQ503-AP503*AQ502)+\n(AP503*AQ504-AP504*AQ503)+\n(AP504*AQ505-AP505*AQ504)+\n(AP505*AQ506-AP506*AQ505)+\n(AP506*AQ507-AP507*AQ506)+\n(AP507*AQ508-AP508*AQ507)+\n(AP508*AQ509-AP509*AQ508)+\n(AP509*AQ510-AP510*AQ509)+\n(AP510*AQ511-AP511*AQ510)+\n(AP511*AQ512-AP512*AQ511)+\n(AP512*AQ513-AP513*AQ512)+\n(AP513*AQ514-AP514*AQ513)+\n(AP514*AQ515-AP515*AQ514)+\n(AP515*AQ516-AP516*AQ515)+\n(AP516*AQ517-AP517*AQ516)+\n(AP517*AQ518-AP518*AQ517)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AR500*AS501-AR501*AS500)+(AR501*AS502-AR502*AS501)+\n (AR502*AS503-AR503*AS502)+\n(AR503*AS504-AR504*AS503)+\n(AR504*AS505-AR505*AS504)+\n(AR505*AS506-AR506*AS505)+\n(AR506*AS507-AR507*AS506)+\n(AR507*AS508-AR508*AS507)+\n(AR508*AS509-AR509*AS508)+\n(AR509*AS510-AR510*AS509)+\n(AR510*AS511-AR511*AS510)+\n(AR511*AS512-AR512*AS511)+\n(AR512*AS513-AR513*AS512)+\n(AR513*AS514-AR514*AS513)+\n(AR514*AS515-AR515*AS514)+\n(AR515*AS516-AR516*AS515)+\n(AR516*AS517-AR517*AS516)+\n(AR517*AS518-AR518*AS517)\n)","v":0},"F=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$64","v":5.04},null,null,null,null," y=",{"$f":"+BC527","v":0.4}," y=",{"$f":"+BE527","v":0}]
[null,null,null,"y=",{"$f":"+IF(E522=0,0,-((D499*E500-D500*E499)*(E499+E500)+(D500*E501-D501*E500)*(E500+E501)+\n(D501*E502-D502*E501)*(E501+E502)+\n(D502*E503-D503*E502)*(E502+E503)+\n(D503*E504-D504*E503)*(E503+E504)+\n(D504*E505-D505*E504)*(E504+E505)+\n(D505*E506-D506*E505)*(E505+E506)+\n(D506*E507-D507*E506)*(E506+E507)+\n(D507*E508-D508*E507)*(E507+E508)+\n(D508*E509-D509*E508)*(E508+E509)+\n(D509*E510-D510*E509)*(E509+E510)+\n(D510*E511-D511*E510)*(E510+E511)+\n(D511*E512-#REF!*E511)*(E511+E512)+\n(#REF!*E513-D512*E512)*(E512+E513)+\n(D512*E514-D513*E513)*(E513+E514)+\n(D513*E515-D514*E514)*(E514+E515)+\n(D514*E516-D515*E515)*(E515+E516)+\n(D515*E517-D516*E516)*(E516+E517)+\n(D516*E518-D517*E517)*(E517+E518))/6/E522)","v":0},"x=",1.7,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,null,null,"x=",0,"x=",0,"x=",0,"x=",0,0,{"$f":"'Analiza i dimenzioniranje'!$U$63","v":4.72},null,null,null,null,"z=",{"$f":"+BC523-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-9.9999999999999978E-2},"z=",{"$f":"+BE523-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5}]
[null,null,null,"y=",{"$f":"+IF(E523=0,0,-((D500*E501-D501*E500)*(E500+E501)+(D501*E502-D502*E501)*(E501+E502)+\n(D502*E503-D503*E502)*(E502+E503)+\n(D503*E504-D504*E503)*(E503+E504)+\n(D504*E505-D505*E504)*(E504+E505)+\n(D505*E506-D506*E505)*(E505+E506)+\n(D506*E507-D507*E506)*(E506+E507)+\n(D507*E508-D508*E507)*(E507+E508)+\n(D508*E509-D509*E508)*(E508+E509)+\n(D509*E510-D510*E509)*(E509+E510)+\n(D510*E511-D511*E510)*(E510+E511)+\n(D511*E512-#REF!*E511)*(E511+E512)+\n(#REF!*E513-D512*E512)*(E512+E513)+\n(D512*E514-D513*E513)*(E513+E514)+\n(D513*E515-D514*E514)*(E514+E515)+\n(D514*E516-D515*E515)*(E515+E516)+\n(D515*E517-D516*E516)*(E516+E517)+\n(D516*E518-D517*E517)*(E517+E518)+\n(D517*E519-D518*E518)*(E518+E519))/6/E523)","v":0},"y=",{"$f":"+IF(G523=0,0,-((F500*G501-F501*G500)*(G500+G501)+(F501*G502-F502*G501)*(G501+G502)+\n(F502*G503-F503*G502)*(G502+G503)+\n(F503*G504-F504*G503)*(G503+G504)+\n(F504*G505-F505*G504)*(G504+G505)+\n(F505*G506-F506*G505)*(G505+G506)+\n(F506*G507-F507*G506)*(G506+G507)+\n(F507*G508-F508*G507)*(G507+G508)+\n(F508*G509-F509*G508)*(G508+G509)+\n(F509*G510-F510*G509)*(G509+G510)+\n(F510*G511-F511*G510)*(G510+G511)+\n(F511*G512-F512*G511)*(G511+G512)+\n(F512*G513-F513*G512)*(G512+G513)+\n(F513*G514-F514*G513)*(G513+G514)+\n(F514*G515-F515*G514)*(G514+G515)+\n(F515*G516-F516*G515)*(G515+G516)+\n(F516*G517-F517*G516)*(G516+G517)+\n(F517*G518-F518*G517)*(G517+G518)+\n(F518*G519-F519*G518)*(G518+G519))/6/G523)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(I523=0,0,-((H500*I501-H501*I500)*(I500+I501)+(H501*I502-H502*I501)*(I501+I502)+\n(H502*I503-H503*I502)*(I502+I503)+\n(H503*I504-H504*I503)*(I503+I504)+\n(H504*I505-H505*I504)*(I504+I505)+\n(H505*I506-H506*I505)*(I505+I506)+\n(H506*I507-H507*I506)*(I506+I507)+\n(H507*I508-H508*I507)*(I507+I508)+\n(H508*I509-H509*I508)*(I508+I509)+\n(H509*I510-H510*I509)*(I509+I510)+\n(H510*I511-H511*I510)*(I510+I511)+\n(H511*I512-H512*I511)*(I511+I512)+\n(H512*I513-H513*I512)*(I512+I513)+\n(H513*I514-H514*I513)*(I513+I514)+\n(H514*I515-H515*I514)*(I514+I515)+\n(H515*I516-H516*I515)*(I515+I516)+\n(H516*I517-H517*I516)*(I516+I517)+\n(H517*I518-H518*I517)*(I517+I518)+\n(H518*I519-H519*I518)*(I518+I519))/6/I523)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(K523=0,0,-((J500*K501-J501*K500)*(K500+K501)+(J501*K502-J502*K501)*(K501+K502)+\n(J502*K503-J503*K502)*(K502+K503)+\n(J503*K504-J504*K503)*(K503+K504)+\n(J504*K505-J505*K504)*(K504+K505)+\n(J505*K506-J506*K505)*(K505+K506)+\n(J506*K507-J507*K506)*(K506+K507)+\n(J507*K508-J508*K507)*(K507+K508)+\n(J508*K509-J509*K508)*(K508+K509)+\n(J509*K510-J510*K509)*(K509+K510)+\n(J510*K511-J511*K510)*(K510+K511)+\n(J511*K512-J512*K511)*(K511+K512)+\n(J512*K513-J513*K512)*(K512+K513)+\n(J513*K514-J514*K513)*(K513+K514)+\n(J514*K515-J515*K514)*(K514+K515)+\n(J515*K516-J516*K515)*(K515+K516)+\n(J516*K517-J517*K516)*(K516+K517)+\n(J517*K518-J518*K517)*(K517+K518)+\n(J518*K519-J519*K518)*(K518+K519))/6/K523)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(M523=0,0,-((L500*M501-L501*M500)*(M500+M501)+(L501*M502-L502*M501)*(M501+M502)+\n(L502*M503-L503*M502)*(M502+M503)+\n(L503*M504-L504*M503)*(M503+M504)+\n(L504*M505-L505*M504)*(M504+M505)+\n(L505*M506-L506*M505)*(M505+M506)+\n(L506*M507-L507*M506)*(M506+M507)+\n(L507*M508-L508*M507)*(M507+M508)+\n(L508*M509-L509*M508)*(M508+M509)+\n(L509*M510-L510*M509)*(M509+M510)+\n(L510*M511-L511*M510)*(M510+M511)+\n(L511*M512-L512*M511)*(M511+M512)+\n(L512*M513-L513*M512)*(M512+M513)+\n(L513*M514-L514*M513)*(M513+M514)+\n(L514*M515-L515*M514)*(M514+M515)+\n(L515*M516-L516*M515)*(M515+M516)+\n(L516*M517-L517*M516)*(M516+M517)+\n(L517*M518-L518*M517)*(M517+M518)+\n(L518*M519-L519*M518)*(M518+M519))/6/M523)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(O523=0,0,-((N500*O501-N501*O500)*(O500+O501)+(N501*O502-N502*O501)*(O501+O502)+\n(N502*O503-N503*O502)*(O502+O503)+\n(N503*O504-N504*O503)*(O503+O504)+\n(N504*O505-N505*O504)*(O504+O505)+\n(N505*O506-N506*O505)*(O505+O506)+\n(N506*O507-N507*O506)*(O506+O507)+\n(N507*O508-N508*O507)*(O507+O508)+\n(N508*O509-N509*O508)*(O508+O509)+\n(N509*O510-N510*O509)*(O509+O510)+\n(N510*O511-N511*O510)*(O510+O511)+\n(N511*O512-N512*O511)*(O511+O512)+\n(N512*O513-N513*O512)*(O512+O513)+\n(N513*O514-N514*O513)*(O513+O514)+\n(N514*O515-N515*O514)*(O514+O515)+\n(N515*O516-N516*O515)*(O515+O516)+\n(N516*O517-N517*O516)*(O516+O517)+\n(N517*O518-N518*O517)*(O517+O518)+\n(N518*O519-N519*O518)*(O518+O519))/6/O523)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(Q523=0,0,-((P500*Q501-P501*Q500)*(Q500+Q501)+(P501*Q502-P502*Q501)*(Q501+Q502)+\n(P502*Q503-P503*Q502)*(Q502+Q503)+\n(P503*Q504-P504*Q503)*(Q503+Q504)+\n(P504*Q505-P505*Q504)*(Q504+Q505)+\n(P505*Q506-P506*Q505)*(Q505+Q506)+\n(P506*Q507-P507*Q506)*(Q506+Q507)+\n(P507*Q508-P508*Q507)*(Q507+Q508)+\n(P508*Q509-P509*Q508)*(Q508+Q509)+\n(P509*Q510-P510*Q509)*(Q509+Q510)+\n(P510*Q511-P511*Q510)*(Q510+Q511)+\n(P511*Q512-P512*Q511)*(Q511+Q512)+\n(P512*Q513-P513*Q512)*(Q512+Q513)+\n(P513*Q514-P514*Q513)*(Q513+Q514)+\n(P514*Q515-P515*Q514)*(Q514+Q515)+\n(P515*Q516-P516*Q515)*(Q515+Q516)+\n(P516*Q517-P517*Q516)*(Q516+Q517)+\n(P517*Q518-P518*Q517)*(Q517+Q518)+\n(P518*Q519-P519*Q518)*(Q518+Q519))/6/Q523)","v":0},"y=",{"$f":"+IF(S523=0,0,-((R500*S501-R501*S500)*(S500+S501)+(R501*S502-R502*S501)*(S501+S502)+\n(R502*S503-R503*S502)*(S502+S503)+\n(R503*S504-R504*S503)*(S503+S504)+\n(R504*S505-R505*S504)*(S504+S505)+\n(R505*S506-R506*S505)*(S505+S506)+\n(R506*S507-R507*S506)*(S506+S507)+\n(R507*S508-R508*S507)*(S507+S508)+\n(R508*S509-R509*S508)*(S508+S509)+\n(R509*S510-R510*S509)*(S509+S510)+\n(R510*S511-R511*S510)*(S510+S511)+\n(R511*S512-R512*S511)*(S511+S512)+\n(R512*S513-R513*S512)*(S512+S513)+\n(R513*S514-R514*S513)*(S513+S514)+\n(R514*S515-R515*S514)*(S514+S515)+\n(R515*S516-R516*S515)*(S515+S516)+\n(R516*S517-R517*S516)*(S516+S517)+\n(R517*S518-R518*S517)*(S517+S518)+\n(R518*S519-R519*S518)*(S518+S519))/6/S523)","v":0},"y=",{"$f":"+IF(U523=0,0,-((T500*U501-T501*U500)*(U500+U501)+(T501*U502-T502*U501)*(U501+U502)+\n(T502*U503-T503*U502)*(U502+U503)+\n(T503*U504-T504*U503)*(U503+U504)+\n(T504*U505-T505*U504)*(U504+U505)+\n(T505*U506-T506*U505)*(U505+U506)+\n(T506*U507-T507*U506)*(U506+U507)+\n(T507*U508-T508*U507)*(U507+U508)+\n(T508*U509-T509*U508)*(U508+U509)+\n(T509*U510-T510*U509)*(U509+U510)+\n(T510*U511-T511*U510)*(U510+U511)+\n(T511*U512-T512*U511)*(U511+U512)+\n(T512*U513-T513*U512)*(U512+U513)+\n(T513*U514-T514*U513)*(U513+U514)+\n(T514*U515-T515*U514)*(U514+U515)+\n(T515*U516-T516*U515)*(U515+U516)+\n(T516*U517-T517*U516)*(U516+U517)+\n(T517*U518-T518*U517)*(U517+U518)+\n(T518*U519-T519*U518)*(U518+U519))/6/U523)","v":0},"y=",{"$f":"+IF(W523=0,0,-((V500*W501-V501*W500)*(W500+W501)+(V501*W502-V502*W501)*(W501+W502)+\n(V502*W503-V503*W502)*(W502+W503)+\n(V503*W504-V504*W503)*(W503+W504)+\n(V504*W505-V505*W504)*(W504+W505)+\n(V505*W506-V506*W505)*(W505+W506)+\n(V506*W507-V507*W506)*(W506+W507)+\n(V507*W508-V508*W507)*(W507+W508)+\n(V508*W509-V509*W508)*(W508+W509)+\n(V509*W510-V510*W509)*(W509+W510)+\n(V510*W511-V511*W510)*(W510+W511)+\n(V511*W512-V512*W511)*(W511+W512)+\n(V512*W513-V513*W512)*(W512+W513)+\n(V513*W514-V514*W513)*(W513+W514)+\n(V514*W515-V515*W514)*(W514+W515)+\n(V515*W516-V516*W515)*(W515+W516)+\n(V516*W517-V517*W516)*(W516+W517)+\n(V517*W518-V518*W517)*(W517+W518)+\n(V518*W519-V519*W518)*(W518+W519))/6/W523)","v":0},"y=",{"$f":"+IF(Y523=0,0,-((X500*Y501-X501*Y500)*(Y500+Y501)+(X501*Y502-X502*Y501)*(Y501+Y502)+\n(X502*Y503-X503*Y502)*(Y502+Y503)+\n(X503*Y504-X504*Y503)*(Y503+Y504)+\n(X504*Y505-X505*Y504)*(Y504+Y505)+\n(X505*Y506-X506*Y505)*(Y505+Y506)+\n(X506*Y507-X507*Y506)*(Y506+Y507)+\n(X507*Y508-X508*Y507)*(Y507+Y508)+\n(X508*Y509-X509*Y508)*(Y508+Y509)+\n(X509*Y510-X510*Y509)*(Y509+Y510)+\n(X510*Y511-X511*Y510)*(Y510+Y511)+\n(X511*Y512-X512*Y511)*(Y511+Y512)+\n(X512*Y513-X513*Y512)*(Y512+Y513)+\n(X513*Y514-X514*Y513)*(Y513+Y514)+\n(X514*Y515-X515*Y514)*(Y514+Y515)+\n(X515*Y516-X516*Y515)*(Y515+Y516)+\n(X516*Y517-X517*Y516)*(Y516+Y517)+\n(X517*Y518-X518*Y517)*(Y517+Y518)+\n(X518*Y519-X519*Y518)*(Y518+Y519))/6/Y523)","v":0},"y=",{"$f":"+IF(AA523=0,0,-((Z500*AA501-Z501*AA500)*(AA500+AA501)+(Z501*AA502-Z502*AA501)*(AA501+AA502)+\n(Z502*AA503-Z503*AA502)*(AA502+AA503)+\n(Z503*AA504-Z504*AA503)*(AA503+AA504)+\n(Z504*AA505-Z505*AA504)*(AA504+AA505)+\n(Z505*AA506-Z506*AA505)*(AA505+AA506)+\n(Z506*AA507-Z507*AA506)*(AA506+AA507)+\n(Z507*AA508-Z508*AA507)*(AA507+AA508)+\n(Z508*AA509-Z509*AA508)*(AA508+AA509)+\n(Z509*AA510-Z510*AA509)*(AA509+AA510)+\n(Z510*AA511-Z511*AA510)*(AA510+AA511)+\n(Z511*AA512-Z512*AA511)*(AA511+AA512)+\n(Z512*AA513-Z513*AA512)*(AA512+AA513)+\n(Z513*AA514-Z514*AA513)*(AA513+AA514)+\n(Z514*AA515-Z515*AA514)*(AA514+AA515)+\n(Z515*AA516-Z516*AA515)*(AA515+AA516)+\n(Z516*AA517-Z517*AA516)*(AA516+AA517)+\n(Z517*AA518-Z518*AA517)*(AA517+AA518)+\n(Z518*AA519-Z519*AA518)*(AA518+AA519))/6/AA523)","v":0},"y=",{"$f":"+IF(AC523=0,0,-((AB500*AC501-AB501*AC500)*(AC500+AC501)+(AB501*AC502-AB502*AC501)*(AC501+AC502)+\n(AB502*AC503-AB503*AC502)*(AC502+AC503)+\n(AB503*AC504-AB504*AC503)*(AC503+AC504)+\n(AB504*AC505-AB505*AC504)*(AC504+AC505)+\n(AB505*AC506-AB506*AC505)*(AC505+AC506)+\n(AB506*AC507-AB507*AC506)*(AC506+AC507)+\n(AB507*AC508-AB508*AC507)*(AC507+AC508)+\n(AB508*AC509-AB509*AC508)*(AC508+AC509)+\n(AB509*AC510-AB510*AC509)*(AC509+AC510)+\n(AB510*AC511-AB511*AC510)*(AC510+AC511)+\n(AB511*AC512-AB512*AC511)*(AC511+AC512)+\n(AB512*AC513-AB513*AC512)*(AC512+AC513)+\n(AB513*AC514-AB514*AC513)*(AC513+AC514)+\n(AB514*AC515-AB515*AC514)*(AC514+AC515)+\n(AB515*AC516-AB516*AC515)*(AC515+AC516)+\n(AB516*AC517-AB517*AC516)*(AC516+AC517)+\n(AB517*AC518-AB518*AC517)*(AC517+AC518)+\n(AB518*AC519-AB519*AC518)*(AC518+AC519))/6/AC523)","v":0},"y=",{"$f":"+IF(AE523=0,0,-((AD500*AE501-AD501*AE500)*(AE500+AE501)+(AD501*AE502-AD502*AE501)*(AE501+AE502)+\n(AD502*AE503-AD503*AE502)*(AE502+AE503)+\n(AD503*AE504-AD504*AE503)*(AE503+AE504)+\n(AD504*AE505-AD505*AE504)*(AE504+AE505)+\n(AD505*AE506-AD506*AE505)*(AE505+AE506)+\n(AD506*AE507-AD507*AE506)*(AE506+AE507)+\n(AD507*AE508-AD508*AE507)*(AE507+AE508)+\n(AD508*AE509-AD509*AE508)*(AE508+AE509)+\n(AD509*AE510-AD510*AE509)*(AE509+AE510)+\n(AD510*AE511-AD511*AE510)*(AE510+AE511)+\n(AD511*AE512-AD512*AE511)*(AE511+AE512)+\n(AD512*AE513-AD513*AE512)*(AE512+AE513)+\n(AD513*AE514-AD514*AE513)*(AE513+AE514)+\n(AD514*AE515-AD515*AE514)*(AE514+AE515)+\n(AD515*AE516-AD516*AE515)*(AE515+AE516)+\n(AD516*AE517-AD517*AE516)*(AE516+AE517)+\n(AD517*AE518-AD518*AE517)*(AE517+AE518)+\n(AD518*AE519-AD519*AE518)*(AE518+AE519))/6/AE523)","v":0},"y=",{"$f":"+IF(AG523=0,0,-((AF500*AG501-AF501*AG500)*(AG500+AG501)+(AF501*AG502-AF502*AG501)*(AG501+AG502)+\n(AF502*AG503-AF503*AG502)*(AG502+AG503)+\n(AF503*AG504-AF504*AG503)*(AG503+AG504)+\n(AF504*AG505-AF505*AG504)*(AG504+AG505)+\n(AF505*AG506-AF506*AG505)*(AG505+AG506)+\n(AF506*AG507-AF507*AG506)*(AG506+AG507)+\n(AF507*AG508-AF508*AG507)*(AG507+AG508)+\n(AF508*AG509-AF509*AG508)*(AG508+AG509)+\n(AF509*AG510-AF510*AG509)*(AG509+AG510)+\n(AF510*AG511-AF511*AG510)*(AG510+AG511)+\n(AF511*AG512-AF512*AG511)*(AG511+AG512)+\n(AF512*AG513-AF513*AG512)*(AG512+AG513)+\n(AF513*AG514-AF514*AG513)*(AG513+AG514)+\n(AF514*AG515-AF515*AG514)*(AG514+AG515)+\n(AF515*AG516-AF516*AG515)*(AG515+AG516)+\n(AF516*AG517-AF517*AG516)*(AG516+AG517)+\n(AF517*AG518-AF518*AG517)*(AG517+AG518)+\n(AF518*AG519-AF519*AG518)*(AG518+AG519))/6/AG523)","v":0},"y=",{"$f":"+IF(AI523=0,0,-((AH500*AI501-AH501*AI500)*(AI500+AI501)+(AH501*AI502-AH502*AI501)*(AI501+AI502)+\n(AH502*AI503-AH503*AI502)*(AI502+AI503)+\n(AH503*AI504-AH504*AI503)*(AI503+AI504)+\n(AH504*AI505-AH505*AI504)*(AI504+AI505)+\n(AH505*AI506-AH506*AI505)*(AI505+AI506)+\n(AH506*AI507-AH507*AI506)*(AI506+AI507)+\n(AH507*AI508-AH508*AI507)*(AI507+AI508)+\n(AH508*AI509-AH509*AI508)*(AI508+AI509)+\n(AH509*AI510-AH510*AI509)*(AI509+AI510)+\n(AH510*AI511-AH511*AI510)*(AI510+AI511)+\n(AH511*AI512-AH512*AI511)*(AI511+AI512)+\n(AH512*AI513-AH513*AI512)*(AI512+AI513)+\n(AH513*AI514-AH514*AI513)*(AI513+AI514)+\n(AH514*AI515-AH515*AI514)*(AI514+AI515)+\n(AH515*AI516-AH516*AI515)*(AI515+AI516)+\n(AH516*AI517-AH517*AI516)*(AI516+AI517)+\n(AH517*AI518-AH518*AI517)*(AI517+AI518)+\n(AH518*AI519-AH519*AI518)*(AI518+AI519))/6/AI523)","v":0},"y=",{"$f":"+IF(AK523=0,0,-((AJ500*AK501-AJ501*AK500)*(AK500+AK501)+(AJ501*AK502-AJ502*AK501)*(AK501+AK502)+\n(AJ502*AK503-AJ503*AK502)*(AK502+AK503)+\n(AJ503*AK504-AJ504*AK503)*(AK503+AK504)+\n(AJ504*AK505-AJ505*AK504)*(AK504+AK505)+\n(AJ505*AK506-AJ506*AK505)*(AK505+AK506)+\n(AJ506*AK507-AJ507*AK506)*(AK506+AK507)+\n(AJ507*AK508-AJ508*AK507)*(AK507+AK508)+\n(AJ508*AK509-AJ509*AK508)*(AK508+AK509)+\n(AJ509*AK510-AJ510*AK509)*(AK509+AK510)+\n(AJ510*AK511-AJ511*AK510)*(AK510+AK511)+\n(AJ511*AK512-AJ512*AK511)*(AK511+AK512)+\n(AJ512*AK513-AJ513*AK512)*(AK512+AK513)+\n(AJ513*AK514-AJ514*AK513)*(AK513+AK514)+\n(AJ514*AK515-AJ515*AK514)*(AK514+AK515)+\n(AJ515*AK516-AJ516*AK515)*(AK515+AK516)+\n(AJ516*AK517-AJ517*AK516)*(AK516+AK517)+\n(AJ517*AK518-AJ518*AK517)*(AK517+AK518)+\n(AJ518*AK519-AJ519*AK518)*(AK518+AK519))/6/AK523)","v":0},null,null,"y=",{"$f":"+IF(AO523=0,0,-((AN500*AO501-AN501*AO500)*(AO500+AO501)+(AN501*AO502-AN502*AO501)*(AO501+AO502)+\n(AN502*AO503-AN503*AO502)*(AO502+AO503)+\n(AN503*AO504-AN504*AO503)*(AO503+AO504)+\n(AN504*AO505-AN505*AO504)*(AO504+AO505)+\n(AN505*AO506-AN506*AO505)*(AO505+AO506)+\n(AN506*AO507-AN507*AO506)*(AO506+AO507)+\n(AN507*AO508-AN508*AO507)*(AO507+AO508)+\n(AN508*AO509-AN509*AO508)*(AO508+AO509)+\n(AN509*AO510-AN510*AO509)*(AO509+AO510)+\n(AN510*AO511-AN511*AO510)*(AO510+AO511)+\n(AN511*AO512-AN512*AO511)*(AO511+AO512)+\n(AN512*AO513-AN513*AO512)*(AO512+AO513)+\n(AN513*AO514-AN514*AO513)*(AO513+AO514)+\n(AN514*AO515-AN515*AO514)*(AO514+AO515)+\n(AN515*AO516-AN516*AO515)*(AO515+AO516)+\n(AN516*AO517-AN517*AO516)*(AO516+AO517)+\n(AN517*AO518-AN518*AO517)*(AO517+AO518)+\n(AN518*AO519-AN519*AO518)*(AO518+AO519))/6/AO523)","v":10.790949347586858},"y=",{"$f":"+IF(AQ523=0,0,-((AP500*AQ501-AP501*AQ500)*(AQ500+AQ501)+(AP501*AQ502-AP502*AQ501)*(AQ501+AQ502)+\n(AP502*AQ503-AP503*AQ502)*(AQ502+AQ503)+\n(AP503*AQ504-AP504*AQ503)*(AQ503+AQ504)+\n(AP504*AQ505-AP505*AQ504)*(AQ504+AQ505)+\n(AP505*AQ506-AP506*AQ505)*(AQ505+AQ506)+\n(AP506*AQ507-AP507*AQ506)*(AQ506+AQ507)+\n(AP507*AQ508-AP508*AQ507)*(AQ507+AQ508)+\n(AP508*AQ509-AP509*AQ508)*(AQ508+AQ509)+\n(AP509*AQ510-AP510*AQ509)*(AQ509+AQ510)+\n(AP510*AQ511-AP511*AQ510)*(AQ510+AQ511)+\n(AP511*AQ512-AP512*AQ511)*(AQ511+AQ512)+\n(AP512*AQ513-AP513*AQ512)*(AQ512+AQ513)+\n(AP513*AQ514-AP514*AQ513)*(AQ513+AQ514)+\n(AP514*AQ515-AP515*AQ514)*(AQ514+AQ515)+\n(AP515*AQ516-AP516*AQ515)*(AQ515+AQ516)+\n(AP516*AQ517-AP517*AQ516)*(AQ516+AQ517)+\n(AP517*AQ518-AP518*AQ517)*(AQ517+AQ518)+\n(AP518*AQ519-AP519*AQ518)*(AQ518+AQ519))/6/AQ523)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AS523=0,0,-((AR500*AS501-AR501*AS500)*(AS500+AS501)+(AR501*AS502-AR502*AS501)*(AS501+AS502)+\n(AR502*AS503-AR503*AS502)*(AS502+AS503)+\n(AR503*AS504-AR504*AS503)*(AS503+AS504)+\n(AR504*AS505-AR505*AS504)*(AS504+AS505)+\n(AR505*AS506-AR506*AS505)*(AS505+AS506)+\n(AR506*AS507-AR507*AS506)*(AS506+AS507)+\n(AR507*AS508-AR508*AS507)*(AS507+AS508)+\n(AR508*AS509-AR509*AS508)*(AS508+AS509)+\n(AR509*AS510-AR510*AS509)*(AS509+AS510)+\n(AR510*AS511-AR511*AS510)*(AS510+AS511)+\n(AR511*AS512-AR512*AS511)*(AS511+AS512)+\n(AR512*AS513-AR513*AS512)*(AS512+AS513)+\n(AR513*AS514-AR514*AS513)*(AS513+AS514)+\n(AR514*AS515-AR515*AS514)*(AS514+AS515)+\n(AR515*AS516-AR516*AS515)*(AS515+AS516)+\n(AR516*AS517-AR517*AS516)*(AS516+AS517)+\n(AR517*AS518-AR518*AS517)*(AS517+AS518)+\n(AR518*AS519-AR519*AS518)*(AS518+AS519))/6/AS523)","v":0},"y=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$62","v":4.4000000000000004},null,null,null,null,"F=",{"$f":"-0.5*((BB502*BC503-BB503*BC502)+(BB503*BC504-BB504*BC503)+\n (BB504*BC505-BB505*BC504)+\n(BB505*BC506-BB506*BC505)+\n(BB506*BC507-BB507*BC506)+\n(BB507*BC508-BB508*BC507)+\n(BB508*BC509-BB509*BC508)+\n(BB509*BC510-BB510*BC509)+\n(BB510*BC511-BB511*BC510)+\n(BB511*BC512-BB512*BC511)+\n(BB512*BC513-BB513*BC512)+\n(BB513*BC514-BB514*BC513)+\n(BB514*BC515-BB515*BC514)+\n(BB515*BC516-BB516*BC515)+\n(BB516*BC517-BB517*BC516)+\n(BB517*BC518-BB518*BC517)+\n(BB518*BC519-BB519*BC518)+\n(BB519*BC520-BB520*BC519)\n)","v":-21.845759999999999},"F=",{"$f":"-0.5*((BD502*BE503-BD503*BE502)+(BD503*BE504-BD504*BE503)+\n (BD504*BE505-BD505*BE504)+\n(BD505*BE506-BD506*BE505)+\n(BD506*BE507-BD507*BE506)+\n(BD507*BE508-BD508*BE507)+\n(BD508*BE509-BD509*BE508)+\n(BD509*BE510-BD510*BE509)+\n(BD510*BE511-BD511*BE510)+\n(BD511*BE512-BD512*BE511)+\n(BD512*BE513-BD513*BE512)+\n(BD513*BE514-BD514*BE513)+\n(BD514*BE515-BD515*BE514)+\n(BD515*BE516-BD516*BE515)+\n(BD516*BE517-BD517*BE516)+\n(BD517*BE518-BD518*BE517)+\n(BD518*BE519-BD519*BE518)+\n(BD519*BE520-BD520*BE519)\n)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$61","v":4.08},null,null,null,null,"x=",0,"x=",0]
[null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$60","v":3.76},null,null,null,null,"y=",{"$f":"+IF(BC525=0,0,-((BB502*BC503-BB503*BC502)*(BC502+BC503)+(BB503*BC504-BB504*BC503)*(BC503+BC504)+\n(BB504*BC505-BB505*BC504)*(BC504+BC505)+\n(BB505*BC506-BB506*BC505)*(BC505+BC506)+\n(BB506*BC507-BB507*BC506)*(BC506+BC507)+\n(BB507*BC508-BB508*BC507)*(BC507+BC508)+\n(BB508*BC509-BB509*BC508)*(BC508+BC509)+\n(BB509*BC510-BB510*BC509)*(BC509+BC510)+\n(BB510*BC511-BB511*BC510)*(BC510+BC511)+\n(BB511*BC512-BB512*BC511)*(BC511+BC512)+\n(BB512*BC513-BB513*BC512)*(BC512+BC513)+\n(BB513*BC514-BB514*BC513)*(BC513+BC514)+\n(BB514*BC515-BB515*BC514)*(BC514+BC515)+\n(BB515*BC516-BB516*BC515)*(BC515+BC516)+\n(BB516*BC517-BB517*BC516)*(BC516+BC517)+\n(BB517*BC518-BB518*BC517)*(BC517+BC518)+\n(BB518*BC519-BB519*BC518)*(BC518+BC519)+\n(BB519*BC520-BB520*BC519)*(BC519+BC520)+\n(BB520*BC521-BB521*BC520)*(BC520+BC521))/6/BC525)","v":0.4},"y=",{"$f":"+IF(BE525=0,0,-((BD502*BE503-BD503*BE502)*(BE502+BE503)+(BD503*BE504-BD504*BE503)*(BE503+BE504)+\n(BD504*BE505-BD505*BE504)*(BE504+BE505)+\n(BD505*BE506-BD506*BE505)*(BE505+BE506)+\n(BD506*BE507-BD507*BE506)*(BE506+BE507)+\n(BD507*BE508-BD508*BE507)*(BE507+BE508)+\n(BD508*BE509-BD509*BE508)*(BE508+BE509)+\n(BD509*BE510-BD510*BE509)*(BE509+BE510)+\n(BD510*BE511-BD511*BE510)*(BE510+BE511)+\n(BD511*BE512-BD512*BE511)*(BE511+BE512)+\n(BD512*BE513-BD513*BE512)*(BE512+BE513)+\n(BD513*BE514-BD514*BE513)*(BE513+BE514)+\n(BD514*BE515-BD515*BE514)*(BE514+BE515)+\n(BD515*BE516-BD516*BE515)*(BE515+BE516)+\n(BD516*BE517-BD517*BE516)*(BE516+BE517)+\n(BD517*BE518-BD518*BE517)*(BE517+BE518)+\n(BD518*BE519-BD519*BE518)*(BE518+BE519)+\n(BD519*BE520-BD520*BE519)*(BE519+BE520)+\n(BD520*BE521-BD521*BE520)*(BE520+BE521))/6/BE525)","v":0}]
[null,"OPTEREĆENJE TEMELJEM",null,null,null,null,null,null,null," (TERZAGHY)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$59","v":3.44}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BK348-BQ347","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$58","v":3.14}]
[null,"KONTINUIRANO OPTEREĆENJE",null,"P - D=",{"$f":"IF('Analiza i dimenzioniranje'!$E$28-I530<=0,0,+'Analiza i dimenzioniranje'!$E$28-I530)","v":{"$error":"#VALUE!"}},"kN/m2","raster. iskopom   D=y*Df =",null,{"$f":"+'Analiza i dimenzioniranje'!$D$16*('Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20-D536)","v":{"$error":"#VALUE!"}},"kN/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.48,0,{"$f":"+'Analiza i dimenzioniranje'!$U$57","v":2.8}]
[null," visina zida i temelja",null,"H =",{"$f":"+E491","v":{"$error":"#VALUE!"}},"m",{"$f":"E535","v":6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$56","v":2.48}]
[null,"visina opterećenja iznad vrha zida",null,"h =",{"$f":"+E452","v":-1},"m",{"$f":"SQRT(E535^2+E534^2)","v":6.7082039324993694},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$55","v":2.16}]
[null,"širina temelja",null,"b =",{"$f":"+E493","v":1},"m   ",{"$f":"E534+E533","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$54","v":1.84}]
[null,"udaljenost temelja od zida",null,"D =",{"$f":"+E494","v":3},"m    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$53","v":1.52}]
[null,"1/2 dužine temelja",null,"L/2=a=",{"$f":"+E495","v":6},"m",{"$f":"SQRT(G531^2+G533^2)","v":7.2111025509279782},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,0,{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
["DNO TEMELJA NA VISINI","PRESJEK NA Visini ",null,{"$f":"ROUND('Analiza i dimenzioniranje'!U56,2)","v":2.48},null,"Presjek III - III",null,"Presjek VI",null,"Presjek VII-VII",null,"Presjek VIII-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"Presjek XIV-XIV",null,"Presjek XV-XV",null,"PresjekXVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX",null,null,null,null,null,null,null,null,null,null,6.2,{"$f":"+IF(AW537>=AW$299,0,BK355-BQ354)","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
[null,null,null,null,null,"Visina djelovanja","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja ","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja",null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2",{"$f":"+AU540","v":0},"SQhi=",6.2]
[null,null,null,{"$f":"+F539","v":0},{"$f":"+D538-E536","v":0},"III",{"$f":"+D536","v":2.48},"IV",{"$f":"+G538","v":2.48},"VII",{"$f":"+G538","v":2.48},"VIII",{"$f":"'Analiza i dimenzioniranje'!U285","v":0},"IX",{"$f":"+G538","v":2.48},"X",{"$f":"+'Analiza i dimenzioniranje'!O187","v":0},"XI",{"$f":"+G538","v":2.48},"XII",{"$f":"+'Analiza i dimenzioniranje'!S187","v":0},"XIII",{"$f":"+G538","v":2.48},"XIV",{"$f":"+W538","v":2.48},"XV",{"$f":"+G538","v":2.48},"XVI",{"$f":"+I538","v":2.48},"XVII",{"$f":"+AC538","v":2.48},"XVIII",{"$f":"+AC538","v":2.48},"XIX",{"$f":"+AE538","v":2.48},"XX",{"$f":"+AG538","v":2.48},null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
[null,null,null,0,{"$f":"IF(D538>E$296,D538,E$296)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja"]
[null,null,null,0,{"$f":"IF(AW519>G$298,0,AW519)","v":0},0,0,{"$f":"+F540","v":0},{"$f":"+G540","v":0},0,0,0,{"$f":"+E539","v":0},0,0,0,{"$f":"+O540","v":0},0,{"$f":"+AS540","v":0},0,{"$f":"+S540","v":0},0,{"$f":"+AS540","v":0},0,{"$f":"+W540","v":0},0,{"$f":"+S540","v":0},0,{"$f":"+AA540","v":0},0,{"$f":"+AU517","v":11.56},0,{"$f":"+AU517","v":11.56},0,{"$f":"+AG540","v":11.56},{"$f":"+AD540","v":0},{"$f":"+AG540","v":11.56},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"XVIII",{"$f":"+'Analiza i dimenzioniranje'!U315","v":0},"XIX",{"$f":"+'Analiza i dimenzioniranje'!U314","v":0},"XX",{"$f":"'Analiza i dimenzioniranje'!U313","v":0}]
[null,null,null,0,{"$f":"+AW520","v":6.0000000000000009},0,0,{"$f":"+F541","v":0},{"$f":"+G541","v":0},0,0,0,0,0,0,0,{"$f":"+O541","v":0},0,0,0,{"$f":"+S541","v":0},0,0,0,{"$f":"+W541","v":0},0,{"$f":"+S541","v":0},0,{"$f":"+AA541","v":0},0,0,0,0,0,{"$f":"+AG541","v":0},{"$f":"+AD541","v":0},{"$f":"+AG541","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD579","v":0},{"$f":"+BB541-BC540","v":0},{"$f":"+AD579","v":0},{"$f":"+BD541-BE540","v":0},{"$f":"+AD579","v":0},{"$f":"+'Analiza i dimenzioniranje'!E311","v":2830.5}]
[null,null,null,0,{"$f":"IF(AW521>G$298,0,AW521)","v":0},0,0,0,{"$f":"+G542","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+AU557","v":10.638400000000001},{"$f":"+AT580","v":0},{"$f":"+BC542","v":10.638400000000001},0,{"$f":"+AE580","v":0}]
[null,null,null,{"$f":"+AV519","v":{"$error":"#REF!"}},0,0,0,{"$f":"+F543","v":0},0,{"$f":"+F541","v":0},0,{"$f":"+D540","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE581","v":0}]
[null,null,null,0,0,0,0,0,0,{"$f":"+F542","v":0},0,{"$f":"+D541","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE582","v":0}]
[null,null,null,0,0,0,0,0,0,0,0,{"$f":"+D542","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE583","v":0}]
[null,null,null,0,4.4000000000000004,0,0,0,0,0,0,{"$f":"+D339","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AE545","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE584","v":0}]
[null,null,null,0,4.08,0,0,0,0,0,0,{"$f":"+D544","v":0},0,{"$f":"+J545","v":0},0,{"$f":"+L545","v":0},0,0,0,{"$f":"+P545","v":0},0,0,0,{"$f":"+T545","v":0},0,0,0,{"$f":"+X545","v":0},0,0,{"$f":"+AU524","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+BC547","v":0}]
[null,null,null,0,3.76,0,0,0,0,0,0,0,0,{"$f":"+J546","v":0},0,{"$f":"+L546","v":0},0,0,0,{"$f":"+P546","v":0},0,0,0,{"$f":"+T546","v":0},0,0,{"$f":"+AA547","v":0},{"$f":"+X546","v":0},0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,"+",3.44,0,0,0,{"$f":"+G549","v":0},{"$f":"+F549","v":0},0,{"$f":"+D546","v":0},0,{"$f":"+J547","v":0},0,{"$f":"+N549","v":0},{"$f":"+O549","v":0},0,0,{"$f":"+R549","v":0},{"$f":"+S549","v":0},0,0,{"$f":"+V549","v":0},0,0,{"$f":"+S549","v":0},{"$f":"+Z549","v":0},{"$f":"+AA549","v":0},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+AV526","v":0},3.14,0,0,0,{"$f":"+G550","v":0},0,0,{"$f":"+J550","v":0},0,{"$f":"+L550","v":0},0,{"$f":"+N550","v":0},{"$f":"+O550","v":0},{"$f":"+P550","v":0},{"$f":"+Q550","v":0},{"$f":"+R550","v":0},{"$f":"+S550","v":0},{"$f":"+T550","v":0},{"$f":"+U550","v":0},{"$f":"+V550","v":0},0,0,0,{"$f":"+Z550","v":0},{"$f":"+AA550","v":0},0,0,{"$f":"+AD550","v":0},{"$f":"+AE550","v":0},{"$f":"+AF550","v":0},0,0,{"$f":"+BC512","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+AV527","v":0},2.8,0,0,0,{"$f":"+G551","v":0},0,0,{"$f":"+J551","v":0},0,{"$f":"+J551","v":0},{"$f":"+M551","v":0},{"$f":"+L551","v":0},{"$f":"+O551","v":0},{"$f":"+N551","v":0},{"$f":"+Q551","v":0},0,{"$f":"+S551","v":0},{"$f":"+T551","v":0},{"$f":"+Y551","v":0},{"$f":"+B545","v":0},{"$f":"+U551","v":0},{"$f":"+B545","v":0},0,{"$f":"+Z551","v":0},{"$f":"+U551","v":0},{"$f":"+AB551","v":0},0,{"$f":"+AB551","v":0},{"$f":"+AC551","v":0},{"$f":"+AF551","v":0},0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+AV528","v":0},2.48,{"$f":"+D553","v":0},0,0,0,0,0,{"$f":"+J552","v":0},0,{"$f":"+J552","v":0},{"$f":"+M552","v":0},{"$f":"+L552","v":0},{"$f":"+O552","v":0},0,{"$f":"+S551","v":0},0,0,0,{"$f":"+AS552","v":0},0,0,0,0,{"$f":"+Z552","v":0},0,{"$f":"+AB552","v":0},0,{"$f":"+AB552","v":0},0,{"$f":"+AF552","v":0},0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+D512","v":0},2.16,{"$f":"+D553","v":0},{"$f":"+AW531","v":2.48},0,2.48,0,{"$f":"+E552","v":2.48},0,2.48,{"$f":"+J553","v":0},{"$f":"+M553","v":2.48},0,{"$f":"+O553","v":2.48},0,{"$f":"+Q553","v":2.48},0,{"$f":"+S553","v":2.48},0,{"$f":"+U553","v":2.48},0,{"$f":"+W553","v":2.48},0,2.48,0,2.48,0,2.48,0,2.48,0,2.48,0,2.48,null,{"$f":"+D553","v":0},{"$f":"$E$534^2+AM553^2","v":9},{"$f":"$G$533^2+AM553^2","v":16},{"$f":"$G$535^2+AM553^2","v":51.999999999999993},{"$f":"IF(AM553=0,0,$E$530/(PI())*(ATAN(($E$535*$G$533)/(AM553*SQRT(AP553)))-$E$535*$G$533*AM553/(AO553*SQRT(AP553))))","v":0},null,{"$f":"+AM553","v":0},{"$f":"$E$535^2+AS553^2","v":36},{"$f":"$E$534^2+AS553^2","v":9},{"$f":"$G$532^2+AS553^2","v":45.000000000000007},{"$f":"IF(AS553=0,0,($E$530/(PI()))*(ATAN(($E$535*$E$534)/(AS553*SQRT(AV553)))-$E$535*$E$534*AS553/(AU553*SQRT(AV553))))","v":0},{"$f":"(+AQ553-AW553)*2","v":0},null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+D513","v":0.32},1.84,{"$f":"+AX554","v":{"$error":"#VALUE!"}},{"$f":"+AW532","v":2.16},{"$error":"#VALUE!"},2.16,{"$error":"#VALUE!"},{"$f":"+E553","v":2.16},{"$error":"#VALUE!"},2.16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,{"$f":"+D554","v":0.32},{"$f":"$E$534^2+AM554^2","v":9.1023999999999994},{"$f":"$G$533^2+AM554^2","v":16.102399999999999},{"$f":"$G$535^2+AM554^2","v":52.102399999999996},{"$f":"IF(AM554=0,0,$E$530/(PI())*(ATAN(($E$535*$G$533)/(AM554*SQRT(AP554)))-$E$535*$G$533*AM554/(AO554*SQRT(AP554))))","v":{"$error":"#VALUE!"}},null,0.32,{"$f":"$E$535^2+AS554^2","v":36.102400000000003},{"$f":"$E$534^2+AS554^2","v":9.1023999999999994},{"$f":"$G$532^2+AS554^2","v":45.10240000000001},{"$f":"IF(AS554=0,0,($E$530/(PI()))*(ATAN(($E$535*$E$534)/(AS554*SQRT(AV554)))-$E$535*$E$534*AS554/(AU554*SQRT(AV554))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+D514","v":0.64},1.52,{"$f":"+AX555","v":{"$error":"#VALUE!"}},{"$f":"+AW533","v":1.84},{"$error":"#VALUE!"},1.84,{"$error":"#VALUE!"},{"$f":"+E554","v":1.84},0,{"$f":"+M554","v":2.16},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,{"$f":"+D555","v":0.64},{"$f":"$E$534^2+AM555^2","v":9.4095999999999993},{"$f":"$G$533^2+AM555^2","v":16.409600000000001},{"$f":"$G$535^2+AM555^2","v":52.40959999999999},{"$f":"IF(AM555=0,0,$E$530/(PI())*(ATAN(($E$535*$G$533)/(AM555*SQRT(AP555)))-$E$535*$G$533*AM555/(AO555*SQRT(AP555))))","v":{"$error":"#VALUE!"}},null,0.64,{"$f":"$E$495^2+AS555^2","v":36.409599999999998},{"$f":"$E$534^2+AS555^2","v":9.4095999999999993},{"$f":"$G$452^2+AS555^2","v":45.409600000000005},{"$f":"IF(AS555=0,0,($E$530/(PI()))*(ATAN(($E$535*$E$534)/(AS555*SQRT(AV555)))-$E$535*$E$534*AS555/(AU555*SQRT(AV555))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+D515","v":0.96},1.2,{"$f":"+AX556","v":{"$error":"#VALUE!"}},{"$f":"+AW534","v":1.52},{"$error":"#VALUE!"},1.52,0,{"$f":"+K555","v":1.84},0,{"$f":"+N556","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AE555","v":0},0,0,0,0,0,0,null,{"$f":"+D556","v":0.96},{"$f":"$E$534^2+AM556^2","v":9.9215999999999998},{"$f":"$G$533^2+AM556^2","v":16.921600000000002},{"$f":"$G$535^2+AM556^2","v":52.921599999999991},{"$f":"IF(AM556=0,0,$E$530/(PI())*(ATAN(($E$535*$G$533)/(AM556*SQRT(AP556)))-$E$535*$G$533*AM556/(AO556*SQRT(AP556))))","v":{"$error":"#VALUE!"}},null,0.96,{"$f":"$E$495^2+AS556^2","v":36.921599999999998},{"$f":"$E$534^2+AS556^2","v":9.9215999999999998},{"$f":"$G$452^2+AS556^2","v":45.921600000000005},{"$f":"IF(AS556=0,0,($E$530/(PI()))*(ATAN(($E$535*$E$534)/(AS556*SQRT(AV556)))-$E$535*$E$534*AS556/(AU556*SQRT(AV556))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,0,2.16,0,2.16,0,2.16]
[null,null,null,{"$f":"+D516","v":1.28},{"$f":"+AW536","v":1.2},{"$f":"+AX557","v":{"$error":"#VALUE!"}},{"$f":"+AW535","v":1.2},0,{"$f":"+I556","v":1.52},0,{"$f":"+K556","v":1.84},0,{"$f":"+M558","v":1.2},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU534","v":0},0,0,0,0,0,0,null,{"$f":"+D557","v":1.28},10.638400000000001,17.638400000000001,53.63839999999999,{"$error":"#VALUE!"},null,1.28,37.638399999999997,{"$f":"$E$534^2+AS557^2","v":10.638400000000001},46.638400000000004,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,0.32,0,0.32,0,0.32]
[null,null,null,null,{"$f":"+AW537","v":6.2},0,{"$f":"+E557","v":1.2},0,{"$f":"+G558","v":1.2},0,{"$f":"+I558","v":1.2},0,{"$f":"+K558","v":1.2},0,{"$f":"+M558","v":1.2},0,{"$f":"+O558","v":1.2},0,{"$f":"+Q558","v":1.2},0,{"$f":"+S558","v":1.2},0,{"$f":"+U558","v":1.2},{"$f":"+P558","v":0},{"$f":"+W558","v":1.2},0,{"$f":"+Y558","v":1.2},0,{"$f":"+AA558","v":1.2},0,{"$f":"+AC558","v":1.2},0,{"$f":"+AC558","v":1.2},0,1.2,{"$f":"+AD558","v":0},{"$f":"+BC520","v":1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AT594","v":36},0.64,0,0.64,0,0.64]
[null,null,null,null,{"$f":"+E562","v":0},{"$f":"+AV535","v":0},{"$f":"+E558","v":6.2},0,{"$f":"+G559","v":6.2},0,{"$f":"+I559","v":6.2},0,{"$f":"+K559","v":6.2},0,{"$f":"+M559","v":6.2},0,{"$f":"+O559","v":6.2},0,{"$f":"+Q559","v":6.2},0,{"$f":"+S559","v":6.2},0,{"$f":"+U559","v":6.2},{"$f":"+P559","v":0},{"$f":"+W559","v":6.2},{"$f":"+N559","v":0},{"$f":"+Y559","v":6.2},0,{"$f":"+AA559","v":6.2},0,{"$f":"+AC559","v":6.2},0,{"$f":"+AC559","v":6.2},0,6.2,{"$f":"+AD559","v":0},6.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AT595","v":36.102400000000003},0.96,{"$f":"+AD595","v":0},0.96,0,0.96]
[null,null,null,"Ukupni pritisak",null,"SQhi=",{"$f":"+G563","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I563","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K563","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+M563","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+O563","v":0},"SQhi=",{"$f":"+Q563","v":0},"SQhi=",{"$f":"+S563","v":0},"SQhi=",{"$f":"+U563","v":0},"SQhi=",{"$f":"+W563","v":0},"SQhi=",{"$f":"+Y563","v":0},"SQhi=",{"$f":"+AA563","v":0},"SQhi=",{"$f":"+AC563","v":0},"SQhi=",{"$f":"+AE563","v":0},"SQhi=",{"$f":"+AG563","v":0},"SQhi=",{"$f":"+AI563","v":0},"SQhi=",{"$f":"+AK563","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,1.2,0,{"$f":"+BE559","v":0.96},0,{"$f":"+AE598","v":1.2}]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G565","v":{"$error":"#VALUE!"}}," y=",{"$f":"+I565","v":{"$error":"#VALUE!"}}," y=",{"$f":"+K565","v":{"$error":"#VALUE!"}}," y=",{"$f":"+M565","v":{"$error":"#VALUE!"}}," y=",{"$f":"+O565","v":0}," y=",{"$f":"+Q565","v":0}," y=",{"$f":"+S565","v":0}," y=",{"$f":"+U565","v":0}," y=",{"$f":"+W565","v":0}," y=",{"$f":"+Y565","v":0}," y=",{"$f":"+AA565","v":0}," y=",{"$f":"+AC565","v":0}," y=",{"$f":"+AE565","v":0}," y=",{"$f":"+AG565","v":0}," y=",{"$f":"+AI565","v":0}," y=",{"$f":"+AK565","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,6.2,0,{"$f":"+AK599","v":6.2},0,{"$f":"+AE599","v":6.2}]
[null,null,null,"krak za presjek III - III",null,"z=",{"$f":"+G561-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I561-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K561-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M561-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+O561-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+Q561-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+S561-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+U561-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z=",{"$f":"+W561-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+Y561-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AA561-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AC561-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AE561-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AG561-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AI561-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AK561-'Analiza i dimenzioniranje'!$E$52","v":-1.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SQhi=",{"$f":"+BC565","v":-21.628672000000002},"SQhi=",{"$f":"+BE565","v":0}]
[null,null,null,"x=",0,"F=",{"$f":"-0.5*(+\n (F542*G543-F543*G542)+\n(F543*G544-F544*G543)+\n(F544*G545-F545*G544)+\n(F545*G546-F546*G545)+\n(F546*G547-F547*G546)+\n(F547*G548-F548*G547)+\n(F548*G549-F549*G548)+\n(F549*G550-F550*G549)+\n(F550*G551-F551*G550)+\n(F551*G552-F552*G551)+\n(F552*G553-F553*G552)+\n(F553*G554-F554*G553)+\n(F554*G555-F555*G554)+\n(F555*G556-F556*G555)+\n(F556*G557-F557*G556)+\n(F557*G558-F558*G557)+\n(F558*G559-F559*G558))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (H542*I543-H543*I542)+\n(H543*I544-H544*I543)+\n(H544*I545-H545*I544)+\n(H545*I546-H546*I545)+\n(H546*I547-H547*I546)+\n(H547*I548-H548*I547)+\n(H548*I549-H549*I548)+\n(H549*I550-H550*I549)+\n(H550*I551-H551*I550)+\n(H551*I552-H552*I551)+\n(H552*I553-H553*I552)+\n(H553*I554-H554*I553)+\n(H554*I555-H555*I554)+\n(H555*I556-H556*I555)+\n(H556*I557-H557*I556)+\n(H557*I558-H558*I557)+\n(H558*I559-H559*I558))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((J540*K541-J541*K540)+(J541*K542-J542*K541)+\n (J542*K543-J543*K542)+\n(J543*K544-J544*K543)+\n(J544*K545-J545*K544)+\n(J545*K546-J546*K545)+\n(J546*K547-J547*K546)+\n(J547*K548-J548*K547)+\n(J548*K549-J549*K548)+\n(J549*K550-J550*K549)+\n(J550*K551-J551*K550)+\n(J551*K552-J552*K551)+\n(J552*K553-J553*K552)+\n(J553*K554-J554*K553)+\n(J554*K555-J555*K554)+\n(J555*K556-J556*K555)+\n(J556*K557-J557*K556)+\n(J557*K558-J558*K557)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (L542*M543-L543*M542)+\n(L543*M544-L544*M543)+\n(L544*M545-L545*M544)+\n(L545*M546-L546*M545)+\n(L546*M547-L547*M546)+\n(L547*M548-L548*M547)+\n(L548*M549-L549*M548)+\n(L549*M550-L550*M549)+\n(L550*M551-L551*M550)+\n(L551*M552-L552*M551)+\n(L552*M553-L553*M552)+\n(L553*M554-L554*M553)+\n(L554*M555-L555*M554)+\n(L555*M556-L556*M555)+\n(L556*M557-L557*M556)+\n(L557*M558-L558*M557)+\n(L558*M559-L559*M558))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (N542*O543-N543*O542)+\n(N543*O544-N544*O543)+\n(N544*O545-N545*O544)+\n(N545*O546-N546*O545)+\n(N546*O547-N547*O546)+\n(N547*O548-N548*O547)+\n(N548*O549-N549*O548)+\n(N549*O550-N550*O549)+\n(N550*O551-N551*O550)+\n(N551*O552-N552*O551)+\n(N552*O553-N553*O552)+\n(N553*O554-N554*O553)+\n(N554*O555-N555*O554)+\n(N555*O556-N556*O555)+\n(N556*O557-N557*O556)+\n(N557*O558-N558*O557)+\n(N558*O559-N559*O558))","v":0},"F=",{"$f":"-0.5*(+\n (P542*Q543-P543*Q542)+\n(P543*Q544-P544*Q543)+\n(P544*Q545-P545*Q544)+\n(P545*Q546-P546*Q545)+\n(P546*Q547-P547*Q546)+\n(P547*Q548-P548*Q547)+\n(P548*Q549-P549*Q548)+\n(P549*Q550-P550*Q549)+\n(P550*Q551-P551*Q550)+\n(P551*Q552-P552*Q551)+\n(P552*Q553-P553*Q552)+\n(P553*Q554-P554*Q553)+\n(P554*Q555-P555*Q554)+\n(P555*Q556-P556*Q555)+\n(P556*Q557-P557*Q556)+\n(P557*Q558-P558*Q557)+\n(P558*Q559-P559*Q558))","v":0},"F=",{"$f":"-0.5*((R540*S541-R541*S540)+(R541*S542-R542*S541)+\n (R542*S543-R543*S542)+\n(R543*S544-R544*S543)+\n(R544*S545-R545*S544)+\n(R545*S546-R546*S545)+\n(R546*S547-R547*S546)+\n(R547*S548-R548*S547)+\n(R548*S549-R549*S548)+\n(R549*S550-R550*S549)+\n(R550*S551-R551*S550)+\n(R551*S552-R552*S551)+\n(R552*S553-R553*S552)+\n(R553*S554-R554*S553)+\n(R554*S555-R555*S554)+\n(R555*S556-R556*S555)+\n(R556*S557-R557*S556)+\n(R557*S558-R558*S557)\n)","v":0},"F=",{"$f":"-0.5*(+\n (T542*U543-T543*U542)+\n(T543*U544-T544*U543)+\n(T544*U545-T545*U544)+\n(T545*U546-T546*U545)+\n(T546*U547-T547*U546)+\n(T547*U548-T548*U547)+\n(T548*U549-T549*U548)+\n(T549*U550-T550*U549)+\n(T550*U551-T551*U550)+\n(T551*U552-T552*U551)+\n(T552*U553-T553*U552)+\n(T553*U554-T554*U553)+\n(T554*U555-T555*U554)+\n(T555*U556-T556*U555)+\n(T556*U557-T557*U556)+\n(T557*U558-T558*U557)+\n(T558*U559-T559*U558))","v":0},"F=",{"$f":"-0.5*(+\n (V542*W543-V543*W542)+\n(V543*W544-V544*W543)+\n(V544*W545-V545*W544)+\n(V545*W546-V546*W545)+\n(V546*W547-V547*W546)+\n(V547*W548-V548*W547)+\n(V548*W549-V549*W548)+\n(V549*W550-V550*W549)+\n(V550*W551-V551*W550)+\n(V551*W552-V552*W551)+\n(V552*W553-V553*W552)+\n(V553*W554-V554*W553)+\n(V554*W555-V555*W554)+\n(V555*W556-V556*W555)+\n(V556*W557-V557*W556)+\n(V557*W558-V558*W557)+\n(V558*W559-V559*W558))","v":0},"F=",{"$f":"-0.5*(+\n (X542*Y543-X543*Y542)+\n(X543*Y544-X544*Y543)+\n(X544*Y545-X545*Y544)+\n(X545*Y546-X546*Y545)+\n(X546*Y547-X547*Y546)+\n(X547*Y548-X548*Y547)+\n(X548*Y549-X549*Y548)+\n(X549*Y550-X550*Y549)+\n(X550*Y551-X551*Y550)+\n(X551*Y552-X552*Y551)+\n(X552*Y553-X553*Y552)+\n(X553*Y554-X554*Y553)+\n(X554*Y555-X555*Y554)+\n(X555*Y556-X556*Y555)+\n(X556*Y557-X557*Y556)+\n(X557*Y558-X558*Y557)+\n(X558*Y559-X559*Y558))","v":0},"F=",{"$f":"-0.5*((Z540*AA541-Z541*AA540)+(Z541*AA542-Z542*AA541)+\n (Z542*AA543-Z543*AA542)+\n(Z543*AA544-Z544*AA543)+\n(Z544*AA545-Z545*AA544)+\n(Z545*AA546-Z546*AA545)+\n(Z546*AA547-Z547*AA546)+\n(Z547*AA548-Z548*AA547)+\n(Z548*AA549-Z549*AA548)+\n(Z549*AA550-Z550*AA549)+\n(Z550*AA551-Z551*AA550)+\n(Z551*AA552-Z552*AA551)+\n(Z552*AA553-Z553*AA552)+\n(Z553*AA554-Z554*AA553)+\n(Z554*AA555-Z555*AA554)+\n(Z555*AA556-Z556*AA555)+\n(Z556*AA557-Z557*AA556)+\n(Z557*AA558-Z558*AA557)\n)","v":0},"F=",{"$f":"-0.5*(+\n (AB542*AC543-AB543*AC542)+\n(AB543*AC544-AB544*AC543)+\n(AB544*AC545-AB545*AC544)+\n(AB545*AC546-AB546*AC545)+\n(AB546*AC547-AB547*AC546)+\n(AB547*AC548-AB548*AC547)+\n(AB548*AC549-AB549*AC548)+\n(AB549*AC550-AB550*AC549)+\n(AB550*AC551-AB551*AC550)+\n(AB551*AC552-AB552*AC551)+\n(AB552*AC553-AB553*AC552)+\n(AB553*AC554-AB554*AC553)+\n(AB554*AC555-AB555*AC554)+\n(AB555*AC556-AB556*AC555)+\n(AB556*AC557-AB557*AC556)+\n(AB557*AC558-AB558*AC557)+\n(AB558*AC559-AB559*AC558))","v":0},"F=",{"$f":"-0.5*(+\n (AD542*AE543-AD543*AE542)+\n(AD543*AE544-AD544*AE543)+\n(AD544*AE545-AD545*AE544)+\n(AD545*AE546-AD546*AE545)+\n(AD546*AE547-AD547*AE546)+\n(AD547*AE548-AD548*AE547)+\n(AD548*AE549-AD549*AE548)+\n(AD549*AE550-AD550*AE549)+\n(AD550*AE551-AD551*AE550)+\n(AD551*AE552-AD552*AE551)+\n(AD552*AE553-AD553*AE552)+\n(AD553*AE554-AD554*AE553)+\n(AD554*AE555-AD555*AE554)+\n(AD555*AE556-AD556*AE555)+\n(AD556*AE557-AD557*AE556)+\n(AD557*AE558-AD558*AE557)+\n(AD558*AE559-AD559*AE558))","v":0},"F=",{"$f":"-0.5*(+\n (AF542*AG543-AF543*AG542)+\n(AF543*AG544-AF544*AG543)+\n(AF544*AG545-AF545*AG544)+\n(AF545*AG546-AF546*AG545)+\n(AF546*AG547-AF547*AG546)+\n(AF547*AG548-AF548*AG547)+\n(AF548*AG549-AF549*AG548)+\n(AF549*AG550-AF550*AG549)+\n(AF550*AG551-AF551*AG550)+\n(AF551*AG552-AF552*AG551)+\n(AF552*AG553-AF553*AG552)+\n(AF553*AG554-AF554*AG553)+\n(AF554*AG555-AF555*AG554)+\n(AF555*AG556-AF556*AG555)+\n(AF556*AG557-AF557*AG556)+\n(AF557*AG558-AF558*AG557)+\n(AF558*AG559-AF559*AG558))","v":0},"F=",{"$f":"-0.5*((AH540*AI541-AH541*AI540)+(AH541*AI542-AH542*AI541)+\n (AH542*AI543-AH543*AI542)+\n(AH543*AI544-AH544*AI543)+\n(AH544*AI545-AH545*AI544)+\n(AH545*AI546-AH546*AI545)+\n(AH546*AI547-AH547*AI546)+\n(AH547*AI548-AH548*AI547)+\n(AH548*AI549-AH549*AI548)+\n(AH549*AI550-AH550*AI549)+\n(AH550*AI551-AH551*AI550)+\n(AH551*AI552-AH552*AI551)+\n(AH552*AI553-AH553*AI552)+\n(AH553*AI554-AH554*AI553)+\n(AH554*AI555-AH555*AI554)+\n(AH555*AI556-AH556*AI555)+\n(AH556*AI557-AH557*AI556)+\n(AH557*AI558-AH558*AI557)\n)","v":0},"F=",{"$f":"-0.5*(+\n (AJ542*AK543-AJ543*AK542)+\n(AJ543*AK544-AJ544*AK543)+\n(AJ544*AK545-AJ545*AK544)+\n(AJ545*AK546-AJ546*AK545)+\n(AJ546*AK547-AJ547*AK546)+\n(AJ547*AK548-AJ548*AK547)+\n(AJ548*AK549-AJ549*AK548)+\n(AJ549*AK550-AJ550*AK549)+\n(AJ550*AK551-AJ551*AK550)+\n(AJ551*AK552-AJ552*AK551)+\n(AJ552*AK553-AJ553*AK552)+\n(AJ553*AK554-AJ554*AK553)+\n(AJ554*AK555-AJ555*AK554)+\n(AJ555*AK556-AJ556*AK555)+\n(AJ556*AK557-AJ557*AK556)+\n(AJ557*AK558-AJ558*AK557)+\n(AJ558*AK559-AJ559*AK558))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," y=",{"$f":"+BC567","v":0.77709627911197399}," y=",{"$f":"+BE567","v":0}]
[null,null,null,"y=",{"$f":"+IF(E562=0,0,-((D539*E540-D540*E539)*(E539+E540)+(D540*E541-D541*E540)*(E540+E541)+\n(D541*E542-D542*E541)*(E541+E542)+\n(D542*E543-D543*E542)*(E542+E543)+\n(D543*E544-D544*E543)*(E543+E544)+\n(D544*E545-D545*E544)*(E544+E545)+\n(D545*E546-D546*E545)*(E545+E546)+\n(D546*E547-D547*E546)*(E546+E547)+\n(D547*E548-D548*E547)*(E547+E548)+\n(D548*E549-D549*E548)*(E548+E549)+\n(D549*E550-D550*E549)*(E549+E550)+\n(D550*E551-D551*E550)*(E550+E551)+\n(D551*E552-D552*E551)*(E551+E552)+\n(D552*E553-D553*E552)*(E552+E553)+\n(D553*E554-D554*E553)*(E553+E554)+\n(D554*E555-D555*E554)*(E554+E555)+\n(D555*E556-D556*E555)*(E555+E556)+\n(D556*E557-D557*E556)*(E556+E557)+\n(D557*E558-D558*E557)*(E557+E558))/6/E562)","v":0},"x=",1.35,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"z=",{"$f":"+BC563-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":0.27709627911197399},"z=",{"$f":"+BE563-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5}]
[null,null,null,"y=",{"$f":"+IF(E563=0,0,-((D540*E541-D541*E540)*(E540+E541)+(D541*E542-D542*E541)*(E541+E542)+\n(D542*E543-D543*E542)*(E542+E543)+\n(D543*E544-D544*E543)*(E543+E544)+\n(D544*E545-D545*E544)*(E544+E545)+\n(D545*E546-D546*E545)*(E545+E546)+\n(D546*E547-D547*E546)*(E546+E547)+\n(D547*E548-D548*E547)*(E547+E548)+\n(D548*E549-D549*E548)*(E548+E549)+\n(D549*E550-D550*E549)*(E549+E550)+\n(D550*E551-D551*E550)*(E550+E551)+\n(D551*E552-D552*E551)*(E551+E552)+\n(D552*E553-D553*E552)*(E552+E553)+\n(D553*E554-D554*E553)*(E553+E554)+\n(D554*E555-D555*E554)*(E554+E555)+\n(D555*E556-D556*E555)*(E555+E556)+\n(D556*E557-D557*E556)*(E556+E557)+\n(D557*E558-D558*E557)*(E557+E558)+\n(D558*E559-D559*E558)*(E558+E559))/6/E563)","v":0},"y=",{"$f":"+IF(G563=0,0,-((F540*G541-F541*G540)*(G540+G541)+(F541*G542-F542*G541)*(G541+G542)+\n(F542*G543-F543*G542)*(G542+G543)+\n(F543*G544-F544*G543)*(G543+G544)+\n(F544*G545-F545*G544)*(G544+G545)+\n(F545*G546-F546*G545)*(G545+G546)+\n(F546*G547-F547*G546)*(G546+G547)+\n(F547*G548-F548*G547)*(G547+G548)+\n(F548*G549-F549*G548)*(G548+G549)+\n(F549*G550-F550*G549)*(G549+G550)+\n(F550*G551-F551*G550)*(G550+G551)+\n(F551*G552-F552*G551)*(G551+G552)+\n(F552*G553-F553*G552)*(G552+G553)+\n(F553*G554-F554*G553)*(G553+G554)+\n(F554*G555-F555*G554)*(G554+G555)+\n(F555*G556-F556*G555)*(G555+G556)+\n(F556*G557-F557*G556)*(G556+G557)+\n(F557*G558-F558*G557)*(G557+G558)+\n(F558*G559-F559*G558)*(G558+G559))/6/G563)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(I563=0,0,-((H540*I541-H541*I540)*(I540+I541)+(H541*I542-H542*I541)*(I541+I542)+\n(H542*I543-H543*I542)*(I542+I543)+\n(H543*I544-H544*I543)*(I543+I544)+\n(H544*I545-H545*I544)*(I544+I545)+\n(H545*I546-H546*I545)*(I545+I546)+\n(H546*I547-H547*I546)*(I546+I547)+\n(H547*I548-H548*I547)*(I547+I548)+\n(H548*I549-H549*I548)*(I548+I549)+\n(H549*I550-H550*I549)*(I549+I550)+\n(H550*I551-H551*I550)*(I550+I551)+\n(H551*I552-H552*I551)*(I551+I552)+\n(H552*I553-H553*I552)*(I552+I553)+\n(H553*I554-H554*I553)*(I553+I554)+\n(H554*I555-H555*I554)*(I554+I555)+\n(H555*I556-H556*I555)*(I555+I556)+\n(H556*I557-H557*I556)*(I556+I557)+\n(H557*I558-H558*I557)*(I557+I558)+\n(H558*I559-H559*I558)*(I558+I559))/6/I563)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(K563=0,0,-((J540*K541-J541*K540)*(K540+K541)+(J541*K542-J542*K541)*(K541+K542)+\n(J542*K543-J543*K542)*(K542+K543)+\n(J543*K544-J544*K543)*(K543+K544)+\n(J544*K545-J545*K544)*(K544+K545)+\n(J545*K546-J546*K545)*(K545+K546)+\n(J546*K547-J547*K546)*(K546+K547)+\n(J547*K548-J548*K547)*(K547+K548)+\n(J548*K549-J549*K548)*(K548+K549)+\n(J549*K550-J550*K549)*(K549+K550)+\n(J550*K551-J551*K550)*(K550+K551)+\n(J551*K552-J552*K551)*(K551+K552)+\n(J552*K553-J553*K552)*(K552+K553)+\n(J553*K554-J554*K553)*(K553+K554)+\n(J554*K555-J555*K554)*(K554+K555)+\n(J555*K556-J556*K555)*(K555+K556)+\n(J556*K557-J557*K556)*(K556+K557)+\n(J557*K558-J558*K557)*(K557+K558)+\n(J558*K559-J559*K558)*(K558+K559))/6/K563)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(M563=0,0,-((L540*M541-L541*M540)*(M540+M541)+(L541*M542-L542*M541)*(M541+M542)+\n(L542*M543-L543*M542)*(M542+M543)+\n(L543*M544-L544*M543)*(M543+M544)+\n(L544*M545-L545*M544)*(M544+M545)+\n(L545*M546-L546*M545)*(M545+M546)+\n(L546*M547-L547*M546)*(M546+M547)+\n(L547*M548-L548*M547)*(M547+M548)+\n(L548*M549-L549*M548)*(M548+M549)+\n(L549*M550-L550*M549)*(M549+M550)+\n(L550*M551-L551*M550)*(M550+M551)+\n(L551*M552-L552*M551)*(M551+M552)+\n(L552*M553-L553*M552)*(M552+M553)+\n(L553*M554-L554*M553)*(M553+M554)+\n(L554*M555-L555*M554)*(M554+M555)+\n(L555*M556-L556*M555)*(M555+M556)+\n(L556*M557-L557*M556)*(M556+M557)+\n(L557*M558-L558*M557)*(M557+M558)+\n(L558*M559-L559*M558)*(M558+M559))/6/M563)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(O563=0,0,-((N540*O541-N541*O540)*(O540+O541)+(N541*O542-N542*O541)*(O541+O542)+\n(N542*O543-N543*O542)*(O542+O543)+\n(N543*O544-N544*O543)*(O543+O544)+\n(N544*O545-N545*O544)*(O544+O545)+\n(N545*O546-N546*O545)*(O545+O546)+\n(N546*O547-N547*O546)*(O546+O547)+\n(N547*O548-N548*O547)*(O547+O548)+\n(N548*O549-N549*O548)*(O548+O549)+\n(N549*O550-N550*O549)*(O549+O550)+\n(N550*O551-N551*O550)*(O550+O551)+\n(N551*O552-N552*O551)*(O551+O552)+\n(N552*O553-N553*O552)*(O552+O553)+\n(N553*O554-N554*O553)*(O553+O554)+\n(N554*O555-N555*O554)*(O554+O555)+\n(N555*O556-N556*O555)*(O555+O556)+\n(N556*O557-N557*O556)*(O556+O557)+\n(N557*O558-N558*O557)*(O557+O558)+\n(N558*O559-N559*O558)*(O558+O559))/6/O563)","v":0},"y=",{"$f":"+IF(Q563=0,0,-((P540*Q541-P541*Q540)*(Q540+Q541)+(P541*Q542-P542*Q541)*(Q541+Q542)+\n(P542*Q543-P543*Q542)*(Q542+Q543)+\n(P543*Q544-P544*Q543)*(Q543+Q544)+\n(P544*Q545-P545*Q544)*(Q544+Q545)+\n(P545*Q546-P546*Q545)*(Q545+Q546)+\n(P546*Q547-P547*Q546)*(Q546+Q547)+\n(P547*Q548-P548*Q547)*(Q547+Q548)+\n(P548*Q549-P549*Q548)*(Q548+Q549)+\n(P549*Q550-P550*Q549)*(Q549+Q550)+\n(P550*Q551-P551*Q550)*(Q550+Q551)+\n(P551*Q552-P552*Q551)*(Q551+Q552)+\n(P552*Q553-P553*Q552)*(Q552+Q553)+\n(P553*Q554-P554*Q553)*(Q553+Q554)+\n(P554*Q555-P555*Q554)*(Q554+Q555)+\n(P555*Q556-P556*Q555)*(Q555+Q556)+\n(P556*Q557-P557*Q556)*(Q556+Q557)+\n(P557*Q558-P558*Q557)*(Q557+Q558)+\n(P558*Q559-P559*Q558)*(Q558+Q559))/6/Q563)","v":0},"y=",{"$f":"+IF(S563=0,0,-((R540*S541-R541*S540)*(S540+S541)+(R541*S542-R542*S541)*(S541+S542)+\n(R542*S543-R543*S542)*(S542+S543)+\n(R543*S544-R544*S543)*(S543+S544)+\n(R544*S545-R545*S544)*(S544+S545)+\n(R545*S546-R546*S545)*(S545+S546)+\n(R546*S547-R547*S546)*(S546+S547)+\n(R547*S548-R548*S547)*(S547+S548)+\n(R548*S549-R549*S548)*(S548+S549)+\n(R549*S550-R550*S549)*(S549+S550)+\n(R550*S551-R551*S550)*(S550+S551)+\n(R551*S552-R552*S551)*(S551+S552)+\n(R552*S553-R553*S552)*(S552+S553)+\n(R553*S554-R554*S553)*(S553+S554)+\n(R554*S555-R555*S554)*(S554+S555)+\n(R555*S556-R556*S555)*(S555+S556)+\n(R556*S557-R557*S556)*(S556+S557)+\n(R557*S558-R558*S557)*(S557+S558)+\n(R558*S559-R559*S558)*(S558+S559))/6/S563)","v":0},"y=",{"$f":"+IF(U563=0,0,-((T540*U541-T541*U540)*(U540+U541)+(T541*U542-T542*U541)*(U541+U542)+\n(T542*U543-T543*U542)*(U542+U543)+\n(T543*U544-T544*U543)*(U543+U544)+\n(T544*U545-T545*U544)*(U544+U545)+\n(T545*U546-T546*U545)*(U545+U546)+\n(T546*U547-T547*U546)*(U546+U547)+\n(T547*U548-T548*U547)*(U547+U548)+\n(T548*U549-T549*U548)*(U548+U549)+\n(T549*U550-T550*U549)*(U549+U550)+\n(T550*U551-T551*U550)*(U550+U551)+\n(T551*U552-T552*U551)*(U551+U552)+\n(T552*U553-T553*U552)*(U552+U553)+\n(T553*U554-T554*U553)*(U553+U554)+\n(T554*U555-T555*U554)*(U554+U555)+\n(T555*U556-T556*U555)*(U555+U556)+\n(T556*U557-T557*U556)*(U556+U557)+\n(T557*U558-T558*U557)*(U557+U558)+\n(T558*U559-T559*U558)*(U558+U559))/6/U563)","v":0},"y=",{"$f":"+IF(W563=0,0,-((V540*W541-V541*W540)*(W540+W541)+(V541*W542-V542*W541)*(W541+W542)+\n(V542*W543-V543*W542)*(W542+W543)+\n(V543*W544-V544*W543)*(W543+W544)+\n(V544*W545-V545*W544)*(W544+W545)+\n(V545*W546-V546*W545)*(W545+W546)+\n(V546*W547-V547*W546)*(W546+W547)+\n(V547*W548-V548*W547)*(W547+W548)+\n(V548*W549-V549*W548)*(W548+W549)+\n(V549*W550-V550*W549)*(W549+W550)+\n(V550*W551-V551*W550)*(W550+W551)+\n(V551*W552-V552*W551)*(W551+W552)+\n(V552*W553-V553*W552)*(W552+W553)+\n(V553*W554-V554*W553)*(W553+W554)+\n(V554*W555-V555*W554)*(W554+W555)+\n(V555*W556-V556*W555)*(W555+W556)+\n(V556*W557-V557*W556)*(W556+W557)+\n(V557*W558-V558*W557)*(W557+W558)+\n(V558*W559-V559*W558)*(W558+W559))/6/W563)","v":0},"y=",{"$f":"+IF(Y563=0,0,-((X540*Y541-X541*Y540)*(Y540+Y541)+(X541*Y542-X542*Y541)*(Y541+Y542)+\n(X542*Y543-X543*Y542)*(Y542+Y543)+\n(X543*Y544-X544*Y543)*(Y543+Y544)+\n(X544*Y545-X545*Y544)*(Y544+Y545)+\n(X545*Y546-X546*Y545)*(Y545+Y546)+\n(X546*Y547-X547*Y546)*(Y546+Y547)+\n(X547*Y548-X548*Y547)*(Y547+Y548)+\n(X548*Y549-X549*Y548)*(Y548+Y549)+\n(X549*Y550-X550*Y549)*(Y549+Y550)+\n(X550*Y551-X551*Y550)*(Y550+Y551)+\n(X551*Y552-X552*Y551)*(Y551+Y552)+\n(X552*Y553-X553*Y552)*(Y552+Y553)+\n(X553*Y554-X554*Y553)*(Y553+Y554)+\n(X554*Y555-X555*Y554)*(Y554+Y555)+\n(X555*Y556-X556*Y555)*(Y555+Y556)+\n(X556*Y557-X557*Y556)*(Y556+Y557)+\n(X557*Y558-X558*Y557)*(Y557+Y558)+\n(X558*Y559-X559*Y558)*(Y558+Y559))/6/Y563)","v":0},"y=",{"$f":"+IF(AA563=0,0,-((Z540*AA541-Z541*AA540)*(AA540+AA541)+(Z541*AA542-Z542*AA541)*(AA541+AA542)+\n(Z542*AA543-Z543*AA542)*(AA542+AA543)+\n(Z543*AA544-Z544*AA543)*(AA543+AA544)+\n(Z544*AA545-Z545*AA544)*(AA544+AA545)+\n(Z545*AA546-Z546*AA545)*(AA545+AA546)+\n(Z546*AA547-Z547*AA546)*(AA546+AA547)+\n(Z547*AA548-Z548*AA547)*(AA547+AA548)+\n(Z548*AA549-Z549*AA548)*(AA548+AA549)+\n(Z549*AA550-Z550*AA549)*(AA549+AA550)+\n(Z550*AA551-Z551*AA550)*(AA550+AA551)+\n(Z551*AA552-Z552*AA551)*(AA551+AA552)+\n(Z552*AA553-Z553*AA552)*(AA552+AA553)+\n(Z553*AA554-Z554*AA553)*(AA553+AA554)+\n(Z554*AA555-Z555*AA554)*(AA554+AA555)+\n(Z555*AA556-Z556*AA555)*(AA555+AA556)+\n(Z556*AA557-Z557*AA556)*(AA556+AA557)+\n(Z557*AA558-Z558*AA557)*(AA557+AA558)+\n(Z558*AA559-Z559*AA558)*(AA558+AA559))/6/AA563)","v":0},"y=",{"$f":"+IF(AC563=0,0,-((AB540*AC541-AB541*AC540)*(AC540+AC541)+(AB541*AC542-AB542*AC541)*(AC541+AC542)+\n(AB542*AC543-AB543*AC542)*(AC542+AC543)+\n(AB543*AC544-AB544*AC543)*(AC543+AC544)+\n(AB544*AC545-AB545*AC544)*(AC544+AC545)+\n(AB545*AC546-AB546*AC545)*(AC545+AC546)+\n(AB546*AC547-AB547*AC546)*(AC546+AC547)+\n(AB547*AC548-AB548*AC547)*(AC547+AC548)+\n(AB548*AC549-AB549*AC548)*(AC548+AC549)+\n(AB549*AC550-AB550*AC549)*(AC549+AC550)+\n(AB550*AC551-AB551*AC550)*(AC550+AC551)+\n(AB551*AC552-AB552*AC551)*(AC551+AC552)+\n(AB552*AC553-AB553*AC552)*(AC552+AC553)+\n(AB553*AC554-AB554*AC553)*(AC553+AC554)+\n(AB554*AC555-AB555*AC554)*(AC554+AC555)+\n(AB555*AC556-AB556*AC555)*(AC555+AC556)+\n(AB556*AC557-AB557*AC556)*(AC556+AC557)+\n(AB557*AC558-AB558*AC557)*(AC557+AC558)+\n(AB558*AC559-AB559*AC558)*(AC558+AC559))/6/AC563)","v":0},"y=",{"$f":"+IF(AE563=0,0,-((AD540*AE541-AD541*AE540)*(AE540+AE541)+(AD541*AE542-AD542*AE541)*(AE541+AE542)+\n(AD542*AE543-AD543*AE542)*(AE542+AE543)+\n(AD543*AE544-AD544*AE543)*(AE543+AE544)+\n(AD544*AE545-AD545*AE544)*(AE544+AE545)+\n(AD545*AE546-AD546*AE545)*(AE545+AE546)+\n(AD546*AE547-AD547*AE546)*(AE546+AE547)+\n(AD547*AE548-AD548*AE547)*(AE547+AE548)+\n(AD548*AE549-AD549*AE548)*(AE548+AE549)+\n(AD549*AE550-AD550*AE549)*(AE549+AE550)+\n(AD550*AE551-AD551*AE550)*(AE550+AE551)+\n(AD551*AE552-AD552*AE551)*(AE551+AE552)+\n(AD552*AE553-AD553*AE552)*(AE552+AE553)+\n(AD553*AE554-AD554*AE553)*(AE553+AE554)+\n(AD554*AE555-AD555*AE554)*(AE554+AE555)+\n(AD555*AE556-AD556*AE555)*(AE555+AE556)+\n(AD556*AE557-AD557*AE556)*(AE556+AE557)+\n(AD557*AE558-AD558*AE557)*(AE557+AE558)+\n(AD558*AE559-AD559*AE558)*(AE558+AE559))/6/AE563)","v":0},"y=",{"$f":"+IF(AG563=0,0,-((AF540*AG541-AF541*AG540)*(AG540+AG541)+(AF541*AG542-AF542*AG541)*(AG541+AG542)+\n(AF542*AG543-AF543*AG542)*(AG542+AG543)+\n(AF543*AG544-AF544*AG543)*(AG543+AG544)+\n(AF544*AG545-AF545*AG544)*(AG544+AG545)+\n(AF545*AG546-AF546*AG545)*(AG545+AG546)+\n(AF546*AG547-AF547*AG546)*(AG546+AG547)+\n(AF547*AG548-AF548*AG547)*(AG547+AG548)+\n(AF548*AG549-AF549*AG548)*(AG548+AG549)+\n(AF549*AG550-AF550*AG549)*(AG549+AG550)+\n(AF550*AG551-AF551*AG550)*(AG550+AG551)+\n(AF551*AG552-AF552*AG551)*(AG551+AG552)+\n(AF552*AG553-AF553*AG552)*(AG552+AG553)+\n(AF553*AG554-AF554*AG553)*(AG553+AG554)+\n(AF554*AG555-AF555*AG554)*(AG554+AG555)+\n(AF555*AG556-AF556*AG555)*(AG555+AG556)+\n(AF556*AG557-AF557*AG556)*(AG556+AG557)+\n(AF557*AG558-AF558*AG557)*(AG557+AG558)+\n(AF558*AG559-AF559*AG558)*(AG558+AG559))/6/AG563)","v":0},"y=",{"$f":"+IF(AI563=0,0,-((AH540*AI541-AH541*AI540)*(AI540+AI541)+(AH541*AI542-AH542*AI541)*(AI541+AI542)+\n(AH542*AI543-AH543*AI542)*(AI542+AI543)+\n(AH543*AI544-AH544*AI543)*(AI543+AI544)+\n(AH544*AI545-AH545*AI544)*(AI544+AI545)+\n(AH545*AI546-AH546*AI545)*(AI545+AI546)+\n(AH546*AI547-AH547*AI546)*(AI546+AI547)+\n(AH547*AI548-AH548*AI547)*(AI547+AI548)+\n(AH548*AI549-AH549*AI548)*(AI548+AI549)+\n(AH549*AI550-AH550*AI549)*(AI549+AI550)+\n(AH550*AI551-AH551*AI550)*(AI550+AI551)+\n(AH551*AI552-AH552*AI551)*(AI551+AI552)+\n(AH552*AI553-AH553*AI552)*(AI552+AI553)+\n(AH553*AI554-AH554*AI553)*(AI553+AI554)+\n(AH554*AI555-AH555*AI554)*(AI554+AI555)+\n(AH555*AI556-AH556*AI555)*(AI555+AI556)+\n(AH556*AI557-AH557*AI556)*(AI556+AI557)+\n(AH557*AI558-AH558*AI557)*(AI557+AI558)+\n(AH558*AI559-AH559*AI558)*(AI558+AI559))/6/AI563)","v":0},"y=",{"$f":"+IF(AK563=0,0,-((AJ540*AK541-AJ541*AK540)*(AK540+AK541)+(AJ541*AK542-AJ542*AK541)*(AK541+AK542)+\n(AJ542*AK543-AJ543*AK542)*(AK542+AK543)+\n(AJ543*AK544-AJ544*AK543)*(AK543+AK544)+\n(AJ544*AK545-AJ545*AK544)*(AK544+AK545)+\n(AJ545*AK546-AJ546*AK545)*(AK545+AK546)+\n(AJ546*AK547-AJ547*AK546)*(AK546+AK547)+\n(AJ547*AK548-AJ548*AK547)*(AK547+AK548)+\n(AJ548*AK549-AJ549*AK548)*(AK548+AK549)+\n(AJ549*AK550-AJ550*AK549)*(AK549+AK550)+\n(AJ550*AK551-AJ551*AK550)*(AK550+AK551)+\n(AJ551*AK552-AJ552*AK551)*(AK551+AK552)+\n(AJ552*AK553-AJ553*AK552)*(AK552+AK553)+\n(AJ553*AK554-AJ554*AK553)*(AK553+AK554)+\n(AJ554*AK555-AJ555*AK554)*(AK554+AK555)+\n(AJ555*AK556-AJ556*AK555)*(AK555+AK556)+\n(AJ556*AK557-AJ557*AK556)*(AK556+AK557)+\n(AJ557*AK558-AJ558*AK557)*(AK557+AK558)+\n(AJ558*AK559-AJ559*AK558)*(AK558+AK559))/6/AK563)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F=",{"$f":"-0.5*((BB542*BC543-BB543*BC542)+(BB543*BC544-BB544*BC543)+\n (BB544*BC545-BB545*BC544)+\n(BB545*BC546-BB546*BC545)+\n(BB546*BC547-BB547*BC546)+\n(BB547*BC548-BB548*BC547)+\n(BB548*BC549-BB549*BC548)+\n(BB549*BC550-BB550*BC549)+\n(BB550*BC551-BB551*BC550)+\n(BB551*BC552-BB552*BC551)+\n(BB552*BC553-BB553*BC552)+\n(BB553*BC554-BB554*BC553)+\n(BB554*BC555-BB555*BC554)+\n(BB555*BC556-BB556*BC555)+\n(BB556*BC557-BB557*BC556)+\n(BB557*BC558-BB558*BC557)+\n(BB558*BC559-BB559*BC558)+\n(BB559*BC560-BB560*BC559)\n)","v":-21.628672000000002},"F=",{"$f":"-0.5*((BD542*BE543-BD543*BE542)+(BD543*BE544-BD544*BE543)+\n (BD544*BE545-BD545*BE544)+\n(BD545*BE546-BD546*BE545)+\n(BD546*BE547-BD547*BE546)+\n(BD547*BE548-BD548*BE547)+\n(BD548*BE549-BD549*BE548)+\n(BD549*BE550-BD550*BE549)+\n(BD550*BE551-BD551*BE550)+\n(BD551*BE552-BD552*BE551)+\n(BD552*BE553-BD553*BE552)+\n(BD553*BE554-BD554*BE553)+\n(BD554*BE555-BD555*BE554)+\n(BD555*BE556-BD556*BE555)+\n(BD556*BE557-BD557*BE556)+\n(BD557*BE558-BD558*BE557)+\n(BD558*BE559-BD559*BE558)+\n(BD559*BE560-BD560*BE559)\n)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",0,"x=",0]
[null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+S590","v":0},{"$f":"BK386-BQ385","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$60","v":3.76},null,null,null,null,"y=",{"$f":"+IF(BC565=0,0,-((BB542*BC543-BB543*BC542)*(BC542+BC543)+(BB543*BC544-BB544*BC543)*(BC543+BC544)+\n(BB544*BC545-BB545*BC544)*(BC544+BC545)+\n(BB545*BC546-BB546*BC545)*(BC545+BC546)+\n(BB546*BC547-BB547*BC546)*(BC546+BC547)+\n(BB547*BC548-BB548*BC547)*(BC547+BC548)+\n(BB548*BC549-BB549*BC548)*(BC548+BC549)+\n(BB549*BC550-BB550*BC549)*(BC549+BC550)+\n(BB550*BC551-BB551*BC550)*(BC550+BC551)+\n(BB551*BC552-BB552*BC551)*(BC551+BC552)+\n(BB552*BC553-BB553*BC552)*(BC552+BC553)+\n(BB553*BC554-BB554*BC553)*(BC553+BC554)+\n(BB554*BC555-BB555*BC554)*(BC554+BC555)+\n(BB555*BC556-BB556*BC555)*(BC555+BC556)+\n(BB556*BC557-BB557*BC556)*(BC556+BC557)+\n(BB557*BC558-BB558*BC557)*(BC557+BC558)+\n(BB558*BC559-BB559*BC558)*(BC558+BC559)+\n(BB559*BC560-BB560*BC559)*(BC559+BC560)+\n(BB560*BC561-BB561*BC560)*(BC560+BC561))/6/BC565)","v":0.77709627911197399},"y=",{"$f":"+IF(BE565=0,0,-((BD542*BE543-BD543*BE542)*(BE542+BE543)+(BD543*BE544-BD544*BE543)*(BE543+BE544)+\n(BD544*BE545-BD545*BE544)*(BE544+BE545)+\n(BD545*BE546-BD546*BE545)*(BE545+BE546)+\n(BD546*BE547-BD547*BE546)*(BE546+BE547)+\n(BD547*BE548-BD548*BE547)*(BE547+BE548)+\n(BD548*BE549-BD549*BE548)*(BE548+BE549)+\n(BD549*BE550-BD550*BE549)*(BE549+BE550)+\n(BD550*BE551-BD551*BE550)*(BE550+BE551)+\n(BD551*BE552-BD552*BE551)*(BE551+BE552)+\n(BD552*BE553-BD553*BE552)*(BE552+BE553)+\n(BD553*BE554-BD554*BE553)*(BE553+BE554)+\n(BD554*BE555-BD555*BE554)*(BE554+BE555)+\n(BD555*BE556-BD556*BE555)*(BE555+BE556)+\n(BD556*BE557-BD557*BE556)*(BE556+BE557)+\n(BD557*BE558-BD558*BE557)*(BE557+BE558)+\n(BD558*BE559-BD559*BE558)*(BE558+BE559)+\n(BD559*BE560-BD560*BE559)*(BE559+BE560)+\n(BD560*BE561-BD561*BE560)*(BE560+BE561))/6/BE565)","v":0}]
[null,"OPTEREĆENJE TEMELJEM",null,null,null,null,null,null,null," (TERZAGHY)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$59","v":3.44}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$58","v":3.14}]
[null,"KONTINUIRANO OPTEREĆENJE",null,"P - D=",{"$f":"IF('Analiza i dimenzioniranje'!$E$28-I570<=0,0,+'Analiza i dimenzioniranje'!$E$28-I570)","v":{"$error":"#VALUE!"}},"kN/m2","raster. iskopom   D=y*Df =",null,{"$f":"+'Analiza i dimenzioniranje'!$D$16*('Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20-D576)","v":{"$error":"#VALUE!"}},"kN/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BK389-BQ388","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$57","v":2.8}]
[null," visina zida i temelja",null,"H =",{"$f":"+E491","v":{"$error":"#VALUE!"}},"m",{"$f":"E575","v":6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.16,{"$f":"BK390-BQ389","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$56","v":2.48}]
[null,"visina opterećenja iznad vrha zida",null,"h =",{"$f":"+E492","v":-1},"m",{"$f":"SQRT(E575^2+E574^2)","v":6.7082039324993694},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.32,{"$f":"BK391-BQ390","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$55","v":2.16}]
[null,"širina temelja",null,"b =",{"$f":"+E493","v":1},"m   ",{"$f":"E574+E573","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.64,{"$f":"BK392-BQ391","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$54","v":1.84}]
[null,"udaljenost temelja od zida",null,"D =",{"$f":"+E494","v":3},"m    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.96,{"$f":"BK393-BQ392","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$53","v":1.52}]
[null,"1/2 dužine temelja",null,"L/2=a=",{"$f":"+E495","v":6},"m",{"$f":"SQRT(G571^2+G573^2)","v":7.2111025509279782},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,0,{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
["DNO TEMELJA NA VISINI","PRESJEK NA Visini ",null,{"$f":"ROUND('Analiza i dimenzioniranje'!U55,2)","v":2.16},null,"Presjek III - III",null,"Presjek VI",null,"Presjek VII-VII",null,"Presjek VIII-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"Presjek XIV-XIV",null,"Presjek XV-XV",null,"PresjekXVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX",null,null,null,null,null,null,null,null,null,null,6.2,{"$f":"+IF(AW577>=AW$299,0,BK395-BQ394)","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
[null,null,null,null,null,"Visina djelovanja","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja ","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja",null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2",{"$f":"+AU580","v":0},"SQhi=",6.2]
[null,null,null,{"$f":"+F579","v":0},{"$f":"+D578-E576","v":0},"III",{"$f":"+D576","v":2.16},"IV",{"$f":"+G578","v":2.16},"VII",{"$f":"+G578","v":2.16},"VIII",{"$f":"'Analiza i dimenzioniranje'!U326","v":0},"IX",{"$f":"+G578","v":2.16},"X",{"$f":"+'Analiza i dimenzioniranje'!O228","v":0},"XI",{"$f":"+G578","v":2.16},"XII",{"$f":"+'Analiza i dimenzioniranje'!S228","v":0},"XIII",{"$f":"+G578","v":2.16},"XIV",{"$f":"+W578","v":2.16},"XV",{"$f":"+G578","v":2.16},"XVI",{"$f":"+I578","v":2.16},"XVII",{"$f":"+AC578","v":2.16},"XVIII",{"$f":"+AC578","v":2.16},"XIX",{"$f":"+AE578","v":2.16},"XX",{"$f":"+AG578","v":2.16},null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
[null,null,null,0,{"$f":"IF(D578>E$296,D578,E$296)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja"]
[null,null,null,0,{"$f":"IF(AW559>G$298,0,AW559)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"XVIII",{"$f":"+'Analiza i dimenzioniranje'!U356","v":""},"XIX",{"$f":"+'Analiza i dimenzioniranje'!U355","v":0},"XX",{"$f":"'Analiza i dimenzioniranje'!U354","v":0}]
[null,null,null,0,{"$f":"+AW560","v":0},0,0,{"$f":"+F581","v":0},{"$f":"+G581","v":0},0,0,0,0,0,0,0,{"$f":"+O581","v":0},0,{"$f":"+AS581","v":0},0,{"$f":"+S581","v":0},0,{"$f":"+AS581","v":0},0,{"$f":"+W581","v":0},0,{"$f":"+S581","v":0},0,{"$f":"+AA581","v":0},0,{"$f":"+AU558","v":0},0,{"$f":"+AU558","v":0},0,{"$f":"+AG581","v":0},{"$f":"+AD581","v":0},{"$f":"+AG581","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD619","v":0},{"$f":"+BB581-BC580","v":{"$error":"#VALUE!"}},{"$f":"+AD619","v":0},{"$f":"+BD581-BE580","v":0},{"$f":"+AD619","v":0},{"$f":"+'Analiza i dimenzioniranje'!E352","v":0}]
[null,null,null,0,{"$f":"IF(AW561>G$298,0,AW561)","v":0},0,0,0,{"$f":"+G582","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU559","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+AU597","v":9.9215999999999998},{"$f":"+AT620","v":0},{"$f":"+BC582","v":9.9215999999999998},0,{"$f":"+AE620","v":0}]
[null,null,null,{"$f":"+AV559","v":0},0,0,0,{"$f":"+F583","v":0},0,{"$f":"+F581","v":0},0,{"$f":"+D580","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU560","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE621","v":0}]
[null,null,null,0,0,0,0,0,0,{"$f":"+F582","v":0},0,{"$f":"+D581","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU561","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE622","v":0}]
[null,null,null,0,0,0,0,0,0,0,0,{"$f":"+D582","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU562","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE623","v":0}]
[null,null,null,0,0,0,0,0,0,0,0,{"$f":"+D379","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AE585","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE624","v":0}]
[null,null,null,0,0,0,0,0,0,0,0,{"$f":"+D584","v":0},0,{"$f":"+J585","v":0},0,{"$f":"+L585","v":0},0,0,0,{"$f":"+P585","v":0},0,0,0,{"$f":"+T585","v":0},0,0,0,{"$f":"+X585","v":0},0,0,{"$f":"+AU564","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+BC587","v":0}]
[null,null,null,0,3.76,0,0,0,0,0,0,0,0,{"$f":"+J586","v":0},0,{"$f":"+L586","v":0},0,0,0,{"$f":"+P586","v":0},0,0,0,{"$f":"+T586","v":0},0,0,{"$f":"+AA587","v":0},{"$f":"+X586","v":0},0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,"+",3.44,0,0,0,{"$f":"+G589","v":0},{"$f":"+F589","v":0},0,{"$f":"+D586","v":0},0,{"$f":"+J587","v":0},0,{"$f":"+N589","v":0},{"$f":"+O589","v":0},0,0,{"$f":"+R589","v":0},{"$f":"+S589","v":0},0,0,{"$f":"+V589","v":0},0,0,{"$f":"+S589","v":0},{"$f":"+Z589","v":0},{"$f":"+AA589","v":0},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+AV566","v":0},3.14,0,0,0,{"$f":"+G590","v":0},0,0,{"$f":"+J590","v":0},0,{"$f":"+L590","v":0},0,{"$f":"+N590","v":0},{"$f":"+O590","v":0},{"$f":"+P590","v":0},{"$f":"+Q590","v":0},{"$f":"+R590","v":0},{"$f":"+S590","v":0},{"$f":"+T590","v":0},{"$f":"+U590","v":0},{"$f":"+V590","v":0},0,0,0,{"$f":"+Z590","v":0},{"$f":"+AA590","v":0},0,0,{"$f":"+AD590","v":0},{"$f":"+AE590","v":0},{"$f":"+AF590","v":0},0,0,{"$f":"+BC552","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+AV567","v":0},2.8,0,0,0,{"$f":"+G591","v":0},0,0,{"$f":"+J591","v":0},0,{"$f":"+J591","v":0},{"$f":"+M591","v":0},{"$f":"+L591","v":0},{"$f":"+O591","v":0},{"$f":"+N591","v":0},{"$f":"+Q591","v":0},0,{"$f":"+S591","v":0},{"$f":"+T591","v":0},{"$f":"+Y591","v":0},{"$f":"+B585","v":0},{"$f":"+U591","v":0},{"$f":"+B585","v":0},0,{"$f":"+Z591","v":0},{"$f":"+U591","v":0},{"$f":"+AB591","v":0},0,{"$f":"+AB591","v":0},{"$f":"+AC591","v":0},{"$f":"+AF591","v":0},0,0,{"$f":"+BC553","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+AV568","v":0},2.48,{"$f":"+D594","v":0},0,0,0,0,0,{"$f":"+J592","v":0},0,{"$f":"+J592","v":0},{"$f":"+M592","v":0},{"$f":"+L592","v":0},{"$f":"+O592","v":0},0,{"$f":"+S591","v":0},0,0,0,{"$f":"+AS592","v":0},0,0,0,0,{"$f":"+Z592","v":0},0,{"$f":"+AB592","v":0},0,{"$f":"+AB592","v":0},0,{"$f":"+AF592","v":0},0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,null,2.16,{"$f":"+D594","v":0},0,0,0,0,0,0,0,{"$f":"+J593","v":0},{"$f":"+M593","v":0},0,{"$f":"+O593","v":0},0,{"$f":"+Q593","v":0},0,{"$f":"+S593","v":0},0,{"$f":"+U593","v":0},0,{"$f":"+W593","v":0},0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+D553","v":0},1.84,{"$f":"+AX594","v":0},{"$f":"+AW572","v":2.16},0,2.16,0,{"$f":"+E593","v":2.16},0,2.16,{"$f":"+L594","v":0},{"$f":"+M594","v":2.16},{"$f":"+N594","v":0},{"$f":"+O594","v":2.16},{"$f":"+P594","v":0},{"$f":"+Q594","v":2.16},{"$f":"+R594","v":0},{"$f":"+S594","v":2.16},{"$f":"+T594","v":0},{"$f":"+U594","v":2.16},{"$f":"+V594","v":0},{"$f":"+W594","v":2.16},{"$f":"+X594","v":0},{"$f":"+Y594","v":2.16},0,2.16,0,2.16,0,2.16,0,2.16,0,2.16,null,{"$f":"+D594","v":0},{"$f":"$E$574^2+AM594^2","v":9},{"$f":"$G$573^2+AM594^2","v":16},{"$f":"$G$575^2+AM594^2","v":51.999999999999993},{"$f":"IF(AM594=0,0,$E$570/(PI())*(ATAN(($E$575*$G$573)/(AM594*SQRT(AP594)))-$E$575*$G$573*AM594/(AO594*SQRT(AP594))))","v":0},null,{"$f":"+AM594","v":0},{"$f":"$E$575^2+AS594^2","v":36},{"$f":"$E$574^2+AS594^2","v":9},{"$f":"$G$572^2+AS594^2","v":45.000000000000007},{"$f":"IF(AS594=0,0,($E$570/(PI()))*(ATAN(($E$575*$E$574)/(AS594*SQRT(AV594)))-$E$575*$E$574*AS594/(AU594*SQRT(AV594))))","v":0},{"$f":"(+AQ594-AW594)*2","v":0},null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+D554","v":0.32},1.52,{"$f":"+AX595","v":{"$error":"#VALUE!"}},{"$f":"+AW573","v":1.84},{"$error":"#VALUE!"},1.84,{"$error":"#VALUE!"},{"$f":"+E594","v":1.84},0,0,0,0,0,0,0,{"$f":"+AS595","v":0.32},0,0,0,{"$f":"+AS595","v":0.32},0,0,0,0.32,0,0,0,0.32,0,0,0,0,0,0.32,null,{"$f":"+D595","v":0.32},{"$f":"$E$574^2+AM595^2","v":9.1023999999999994},{"$f":"$G$573^2+AM595^2","v":16.102399999999999},{"$f":"$G$575^2+AM595^2","v":52.102399999999996},{"$f":"IF(AM595=0,0,$E$570/(PI())*(ATAN(($E$575*$G$533)/(AM595*SQRT(AP595)))-$E$575*$G$573*AM595/(AO595*SQRT(AP595))))","v":{"$error":"#VALUE!"}},null,0.32,{"$f":"$E$575^2+AS595^2","v":36.102400000000003},{"$f":"$E$574^2+AS595^2","v":9.1023999999999994},{"$f":"$G$572^2+AS595^2","v":45.10240000000001},{"$f":"IF(AS595=0,0,($E$570/(PI()))*(ATAN(($E$575*$E$574)/(AS595*SQRT(AV595)))-$E$575*$E$574*AS595/(AU595*SQRT(AV595))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+D555","v":0.64},1.2,{"$f":"+AX596","v":{"$error":"#VALUE!"}},{"$f":"+AW574","v":1.52},{"$error":"#VALUE!"},1.52,0,{"$f":"+K595","v":1.84},0,{"$f":"+N596","v":0},0,{"$f":"+AM596","v":0.64},0,0,0,{"$f":"+AS596","v":0.64},0,0,0,{"$f":"+AS596","v":0.64},0,0,0,0.64,0,0,0,{"$f":"+AE595","v":0.32},0,0,0,0,0,0.64,null,{"$f":"+D596","v":0.64},{"$f":"$E$574^2+AM596^2","v":9.4095999999999993},{"$f":"$G$573^2+AM596^2","v":16.409600000000001},{"$f":"$G$575^2+AM596^2","v":52.40959999999999},{"$f":"IF(AM596=0,0,$E$570/(PI())*(ATAN(($E$575*$G$533)/(AM596*SQRT(AP596)))-$E$575*$G$573*AM596/(AO596*SQRT(AP596))))","v":{"$error":"#VALUE!"}},null,0.64,{"$f":"$E$575^2+AS596^2","v":36.409599999999998},{"$f":"$E$574^2+AS596^2","v":9.4095999999999993},{"$f":"$G$572^2+AS596^2","v":45.409600000000005},{"$f":"IF(AS596=0,0,($E$570/(PI()))*(ATAN(($E$575*$E$574)/(AS596*SQRT(AV596)))-$E$575*$E$574*AS596/(AU596*SQRT(AV596))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+D556","v":0.96},{"$f":"+AW576","v":1.2},{"$f":"+AX597","v":{"$error":"#VALUE!"}},{"$f":"+AW575","v":1.2},0,{"$f":"+I596","v":1.52},0,{"$f":"+E596","v":1.2},0,{"$f":"+N597","v":0},0,{"$f":"+AM597","v":0.96},0,0,0,{"$f":"+AS597","v":0.96},0,0,0,{"$f":"+AS597","v":0.96},0,0,0,0.96,0,0,0,{"$f":"+AU574","v":0.96},0,0,0,0,0,0.96,null,{"$f":"+D597","v":0.96},9.9215999999999998,16.921600000000002,52.921599999999991,{"$error":"#VALUE!"},null,0.96,36.921599999999998,{"$f":"$E$574^2+AS597^2","v":9.9215999999999998},45.921600000000005,{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,0,1.84,0,1.84,0,1.84]
[null,null,null,null,{"$f":"+AW577","v":6.2},0,{"$f":"+E597","v":1.2},0,{"$f":"+G598","v":1.2},0,{"$f":"+I598","v":1.2},0,{"$f":"+K598","v":1.2},0,{"$f":"+M598","v":1.2},0,{"$f":"+O598","v":1.2},0,{"$f":"+Q598","v":1.2},0,{"$f":"+S598","v":1.2},0,{"$f":"+U598","v":1.2},{"$f":"+P598","v":0},{"$f":"+W598","v":1.2},0,{"$f":"+Y598","v":1.2},0,{"$f":"+AA598","v":1.2},0,{"$f":"+AC598","v":1.2},0,{"$f":"+AC598","v":1.2},0,1.2,{"$f":"+AD598","v":0},1.2,null,null,0,{"$f":"+AM598","v":0},0,{"$f":"+AQ597","v":{"$error":"#VALUE!"}},0,{"$f":"+AO598","v":0},0,0,0,{"$f":"IF(AV596>AW$299,AV596,AW$299)","v":45.409600000000005},null,null,null,null,{"$f":"+AT634","v":0},0.32,0,0.32,0,0.32]
[null,null,null,null,{"$f":"+E602","v":0},{"$f":"+AV575","v":0},{"$f":"+E598","v":6.2},0,{"$f":"+G599","v":6.2},0,{"$f":"+I599","v":6.2},0,{"$f":"+K599","v":6.2},0,{"$f":"+M599","v":6.2},0,{"$f":"+O599","v":6.2},0,{"$f":"+Q599","v":6.2},0,{"$f":"+S599","v":6.2},0,{"$f":"+U599","v":6.2},{"$f":"+P599","v":0},{"$f":"+W599","v":6.2},{"$f":"+N599","v":0},{"$f":"+Y599","v":6.2},0,{"$f":"+AA599","v":6.2},0,{"$f":"+AC599","v":6.2},0,{"$f":"+AC599","v":6.2},0,6.2,{"$f":"+AD599","v":0},6.2,null,null,0,0,0,{"$f":"+AS599","v":0},0,0,0,{"$f":"+S622","v":0},{"$f":"#REF!-#REF!","v":{"$error":"#REF!"}},{"$f":"+AW600","v":6.0000000000000009},null,null,null,null,{"$f":"+AT635","v":36},0.64,{"$f":"+AD635","v":0},0.64,0,0.64]
[null,null,null,"Ukupni pritisak",null,"SQhi=",{"$f":"+G603","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I603","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K603","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+M603","v":0},"SQhi=",{"$f":"+O603","v":0},"SQhi=",{"$f":"+Q603","v":0},"SQhi=",{"$f":"+S603","v":0},"SQhi=",{"$f":"+U603","v":0},"SQhi=",{"$f":"+W603","v":0},"SQhi=",{"$f":"+Y603","v":0},"SQhi=",{"$f":"+AA603","v":0},"SQhi=",{"$f":"+AC603","v":0},"SQhi=",{"$f":"+AE603","v":0},"SQhi=",{"$f":"+AG603","v":0},"SQhi=",{"$f":"+AI603","v":0},"SQhi=",{"$f":"+AK603","v":0},null,null,"SQhi=",{"$f":"+AO603","v":3.2256},"SQhi=",{"$f":"+AQ603","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AS603","v":0},"SQhi=",0,{"$f":"BK419-BQ418","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$67","v":6.0000000000000009},null,null,null,null,0,1.2,0,{"$f":"+BE599","v":0.64},0,{"$f":"+AE638","v":1.2}]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G605","v":{"$error":"#VALUE!"}}," y=",{"$f":"+I605","v":{"$error":"#VALUE!"}}," y=",{"$f":"+K605","v":{"$error":"#VALUE!"}}," y=",{"$f":"+M605","v":0}," y=",{"$f":"+O605","v":0}," y=",{"$f":"+Q605","v":0}," y=",{"$f":"+S605","v":0}," y=",{"$f":"+U605","v":0}," y=",{"$f":"+W605","v":0}," y=",{"$f":"+Y605","v":0}," y=",{"$f":"+AA605","v":0}," y=",{"$f":"+AC605","v":0}," y=",{"$f":"+AE605","v":0}," y=",{"$f":"+AG605","v":0}," y=",{"$f":"+AI605","v":0}," y=",{"$f":"+AK605","v":0},null,null," y=",{"$f":"+AO605","v":10.973866666666668}," y=",{"$f":"+AQ605","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AS605","v":0}," y=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$66","v":5.6800000000000006},null,null,null,null,0,6.2,0,{"$f":"+AK639","v":6.2},0,{"$f":"+AE639","v":6.2}]
[null,null,null,"krak za presjek III - III",null,"z=",{"$f":"+G601-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I601-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K601-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M601-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+O601-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+Q601-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+S601-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+U601-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z=",{"$f":"+W601-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+Y601-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AA601-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AC601-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AE601-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AG601-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AI601-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AK601-'Analiza i dimenzioniranje'!$E$52","v":-1.2},null,null,"z=",{"$f":"+AO601-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":10.473866666666668},"z=",{"$f":"+AQ601-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AS601-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$65","v":5.36},null,null,null,null,"SQhi=",{"$f":"+BC605","v":-15.839999999999998},"SQhi=",{"$f":"+BE605","v":0}]
[null,null,null,"x=",0,"F=",{"$f":"-0.5*(+\n (F582*G583-F583*G582)+\n(F583*G584-F584*G583)+\n(F584*G585-F585*G584)+\n(F585*G586-F586*G585)+\n(F586*G587-F587*G586)+\n(F587*G588-F588*G587)+\n(F588*G589-F589*G588)+\n(F589*G590-F590*G589)+\n(F590*G591-F591*G590)+\n(F591*G592-F592*G591)+\n(F592*G593-F593*G592)+\n(F593*G594-F594*G593)+\n(F594*G595-F595*G594)+\n(F595*G596-F596*G595)+\n(F596*G597-F597*G596)+\n(F597*G598-F598*G597)+\n(F598*G599-F599*G598))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (H582*I583-H583*I582)+\n(H583*I584-H584*I583)+\n(H584*I585-H585*I584)+\n(H585*I586-H586*I585)+\n(H586*I587-H587*I586)+\n(H587*I588-H588*I587)+\n(H588*I589-H589*I588)+\n(H589*I590-H590*I589)+\n(H590*I591-H591*I590)+\n(H591*I592-H592*I591)+\n(H592*I593-H593*I592)+\n(H593*I594-H594*I593)+\n(H594*I595-H595*I594)+\n(H595*I596-H596*I595)+\n(H596*I597-H597*I596)+\n(H597*I598-H598*I597)+\n(H598*I599-H599*I598))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((J580*K581-J581*K580)+(J581*K582-J582*K581)+\n (J582*K583-J583*K582)+\n(J583*K584-J584*K583)+\n(J584*K585-J585*K584)+\n(J585*K586-J586*K585)+\n(J586*K587-J587*K586)+\n(J587*K588-J588*K587)+\n(J588*K589-J589*K588)+\n(J589*K590-J590*K589)+\n(J590*K591-J591*K590)+\n(J591*K592-J592*K591)+\n(J592*K593-J593*K592)+\n(J593*K594-J594*K593)+\n(J594*K595-J595*K594)+\n(J595*K596-J596*K595)+\n(J596*K597-J597*K596)+\n(J597*K598-J598*K597)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (L582*M583-L583*M582)+\n(L583*M584-L584*M583)+\n(L584*M585-L585*M584)+\n(L585*M586-L586*M585)+\n(L586*M587-L587*M586)+\n(L587*M588-L588*M587)+\n(L588*M589-L589*M588)+\n(L589*M590-L590*M589)+\n(L590*M591-L591*M590)+\n(L591*M592-L592*M591)+\n(L592*M593-L593*M592)+\n(L593*M594-L594*M593)+\n(L594*M595-L595*M594)+\n(L595*M596-L596*M595)+\n(L596*M597-L597*M596)+\n(L597*M598-L598*M597)+\n(L598*M599-L599*M598))","v":0},"F=",{"$f":"-0.5*(+\n (N582*O583-N583*O582)+\n(N583*O584-N584*O583)+\n(N584*O585-N585*O584)+\n(N585*O586-N586*O585)+\n(N586*O587-N587*O586)+\n(N587*O588-N588*O587)+\n(N588*O589-N589*O588)+\n(N589*O590-N590*O589)+\n(N590*O591-N591*O590)+\n(N591*O592-N592*O591)+\n(N592*O593-N593*O592)+\n(N593*O594-N594*O593)+\n(N594*O595-N595*O594)+\n(N595*O596-N596*O595)+\n(N596*O597-N597*O596)+\n(N597*O598-N598*O597)+\n(N598*O599-N599*O598))","v":0},"F=",{"$f":"-0.5*(+\n (P582*Q583-P583*Q582)+\n(P583*Q584-P584*Q583)+\n(P584*Q585-P585*Q584)+\n(P585*Q586-P586*Q585)+\n(P586*Q587-P587*Q586)+\n(P587*Q588-P588*Q587)+\n(P588*Q589-P589*Q588)+\n(P589*Q590-P590*Q589)+\n(P590*Q591-P591*Q590)+\n(P591*Q592-P592*Q591)+\n(P592*Q593-P593*Q592)+\n(P593*Q594-P594*Q593)+\n(P594*Q595-P595*Q594)+\n(P595*Q596-P596*Q595)+\n(P596*Q597-P597*Q596)+\n(P597*Q598-P598*Q597)+\n(P598*Q599-P599*Q598))","v":0},"F=",{"$f":"-0.5*((R580*S581-R581*S580)+(R581*S582-R582*S581)+\n (R582*S583-R583*S582)+\n(R583*S584-R584*S583)+\n(R584*S585-R585*S584)+\n(R585*S586-R586*S585)+\n(R586*S587-R587*S586)+\n(R587*S588-R588*S587)+\n(R588*S589-R589*S588)+\n(R589*S590-R590*S589)+\n(R590*S591-R591*S590)+\n(R591*S592-R592*S591)+\n(R592*S593-R593*S592)+\n(R593*S594-R594*S593)+\n(R594*S595-R595*S594)+\n(R595*S596-R596*S595)+\n(R596*S597-R597*S596)+\n(R597*S598-R598*S597)\n)","v":0},"F=",{"$f":"-0.5*(+\n (T582*U583-T583*U582)+\n(T583*U584-T584*U583)+\n(T584*U585-T585*U584)+\n(T585*U586-T586*U585)+\n(T586*U587-T587*U586)+\n(T587*U588-T588*U587)+\n(T588*U589-T589*U588)+\n(T589*U590-T590*U589)+\n(T590*U591-T591*U590)+\n(T591*U592-T592*U591)+\n(T592*U593-T593*U592)+\n(T593*U594-T594*U593)+\n(T594*U595-T595*U594)+\n(T595*U596-T596*U595)+\n(T596*U597-T597*U596)+\n(T597*U598-T598*U597)+\n(T598*U599-T599*U598))","v":0},"F=",{"$f":"-0.5*(+\n (V582*W583-V583*W582)+\n(V583*W584-V584*W583)+\n(V584*W585-V585*W584)+\n(V585*W586-V586*W585)+\n(V586*W587-V587*W586)+\n(V587*W588-V588*W587)+\n(V588*W589-V589*W588)+\n(V589*W590-V590*W589)+\n(V590*W591-V591*W590)+\n(V591*W592-V592*W591)+\n(V592*W593-V593*W592)+\n(V593*W594-V594*W593)+\n(V594*W595-V595*W594)+\n(V595*W596-V596*W595)+\n(V596*W597-V597*W596)+\n(V597*W598-V598*W597)+\n(V598*W599-V599*W598))","v":0},"F=",{"$f":"-0.5*(+\n (X582*Y583-X583*Y582)+\n(X583*Y584-X584*Y583)+\n(X584*Y585-X585*Y584)+\n(X585*Y586-X586*Y585)+\n(X586*Y587-X587*Y586)+\n(X587*Y588-X588*Y587)+\n(X588*Y589-X589*Y588)+\n(X589*Y590-X590*Y589)+\n(X590*Y591-X591*Y590)+\n(X591*Y592-X592*Y591)+\n(X592*Y593-X593*Y592)+\n(X593*Y594-X594*Y593)+\n(X594*Y595-X595*Y594)+\n(X595*Y596-X596*Y595)+\n(X596*Y597-X597*Y596)+\n(X597*Y598-X598*Y597)+\n(X598*Y599-X599*Y598))","v":0},"F=",{"$f":"-0.5*((Z580*AA581-Z581*AA580)+(Z581*AA582-Z582*AA581)+\n (Z582*AA583-Z583*AA582)+\n(Z583*AA584-Z584*AA583)+\n(Z584*AA585-Z585*AA584)+\n(Z585*AA586-Z586*AA585)+\n(Z586*AA587-Z587*AA586)+\n(Z587*AA588-Z588*AA587)+\n(Z588*AA589-Z589*AA588)+\n(Z589*AA590-Z590*AA589)+\n(Z590*AA591-Z591*AA590)+\n(Z591*AA592-Z592*AA591)+\n(Z592*AA593-Z593*AA592)+\n(Z593*AA594-Z594*AA593)+\n(Z594*AA595-Z595*AA594)+\n(Z595*AA596-Z596*AA595)+\n(Z596*AA597-Z597*AA596)+\n(Z597*AA598-Z598*AA597)\n)","v":0},"F=",{"$f":"-0.5*(+\n (AB582*AC583-AB583*AC582)+\n(AB583*AC584-AB584*AC583)+\n(AB584*AC585-AB585*AC584)+\n(AB585*AC586-AB586*AC585)+\n(AB586*AC587-AB587*AC586)+\n(AB587*AC588-AB588*AC587)+\n(AB588*AC589-AB589*AC588)+\n(AB589*AC590-AB590*AC589)+\n(AB590*AC591-AB591*AC590)+\n(AB591*AC592-AB592*AC591)+\n(AB592*AC593-AB593*AC592)+\n(AB593*AC594-AB594*AC593)+\n(AB594*AC595-AB595*AC594)+\n(AB595*AC596-AB596*AC595)+\n(AB596*AC597-AB597*AC596)+\n(AB597*AC598-AB598*AC597)+\n(AB598*AC599-AB599*AC598))","v":0},"F=",{"$f":"-0.5*(+\n (AD582*AE583-AD583*AE582)+\n(AD583*AE584-AD584*AE583)+\n(AD584*AE585-AD585*AE584)+\n(AD585*AE586-AD586*AE585)+\n(AD586*AE587-AD587*AE586)+\n(AD587*AE588-AD588*AE587)+\n(AD588*AE589-AD589*AE588)+\n(AD589*AE590-AD590*AE589)+\n(AD590*AE591-AD591*AE590)+\n(AD591*AE592-AD592*AE591)+\n(AD592*AE593-AD593*AE592)+\n(AD593*AE594-AD594*AE593)+\n(AD594*AE595-AD595*AE594)+\n(AD595*AE596-AD596*AE595)+\n(AD596*AE597-AD597*AE596)+\n(AD597*AE598-AD598*AE597)+\n(AD598*AE599-AD599*AE598))","v":0},"F=",{"$f":"-0.5*(+\n (AF582*AG583-AF583*AG582)+\n(AF583*AG584-AF584*AG583)+\n(AF584*AG585-AF585*AG584)+\n(AF585*AG586-AF586*AG585)+\n(AF586*AG587-AF587*AG586)+\n(AF587*AG588-AF588*AG587)+\n(AF588*AG589-AF589*AG588)+\n(AF589*AG590-AF590*AG589)+\n(AF590*AG591-AF591*AG590)+\n(AF591*AG592-AF592*AG591)+\n(AF592*AG593-AF593*AG592)+\n(AF593*AG594-AF594*AG593)+\n(AF594*AG595-AF595*AG594)+\n(AF595*AG596-AF596*AG595)+\n(AF596*AG597-AF597*AG596)+\n(AF597*AG598-AF598*AG597)+\n(AF598*AG599-AF599*AG598))","v":0},"F=",{"$f":"-0.5*((AH580*AI581-AH581*AI580)+(AH581*AI582-AH582*AI581)+\n (AH582*AI583-AH583*AI582)+\n(AH583*AI584-AH584*AI583)+\n(AH584*AI585-AH585*AI584)+\n(AH585*AI586-AH586*AI585)+\n(AH586*AI587-AH587*AI586)+\n(AH587*AI588-AH588*AI587)+\n(AH588*AI589-AH589*AI588)+\n(AH589*AI590-AH590*AI589)+\n(AH590*AI591-AH591*AI590)+\n(AH591*AI592-AH592*AI591)+\n(AH592*AI593-AH593*AI592)+\n(AH593*AI594-AH594*AI593)+\n(AH594*AI595-AH595*AI594)+\n(AH595*AI596-AH596*AI595)+\n(AH596*AI597-AH597*AI596)+\n(AH597*AI598-AH598*AI597)\n)","v":0},"F=",{"$f":"-0.5*(+\n (AJ582*AK583-AJ583*AK582)+\n(AJ583*AK584-AJ584*AK583)+\n(AJ584*AK585-AJ585*AK584)+\n(AJ585*AK586-AJ586*AK585)+\n(AJ586*AK587-AJ587*AK586)+\n(AJ587*AK588-AJ588*AK587)+\n(AJ588*AK589-AJ589*AK588)+\n(AJ589*AK590-AJ590*AK589)+\n(AJ590*AK591-AJ591*AK590)+\n(AJ591*AK592-AJ592*AK591)+\n(AJ592*AK593-AJ593*AK592)+\n(AJ593*AK594-AJ594*AK593)+\n(AJ594*AK595-AJ595*AK594)+\n(AJ595*AK596-AJ596*AK595)+\n(AJ596*AK597-AJ597*AK596)+\n(AJ597*AK598-AJ598*AK597)+\n(AJ598*AK599-AJ599*AK598))","v":0},null,null,"F=",{"$f":"-0.5*((AN580*AO581-AN581*AO580)+(AN581*AO582-AN582*AO581)+\n (AN582*AO583-AN583*AO582)+\n(AN583*AO584-AN584*AO583)+\n(AN584*AO585-AN585*AO584)+\n(AN585*AO586-AN586*AO585)+\n(AN586*AO587-AN587*AO586)+\n(AN587*AO588-AN588*AO587)+\n(AN588*AO589-AN589*AO588)+\n(AN589*AO590-AN590*AO589)+\n(AN590*AO591-AN591*AO590)+\n(AN591*AO592-AN592*AO591)+\n(AN592*AO593-AN593*AO592)+\n(AN593*AO594-AN594*AO593)+\n(AN594*AO595-AN595*AO594)+\n(AN595*AO596-AN596*AO595)+\n(AN596*AO597-AN597*AO596)+\n(AN597*AO598-AN598*AO597)\n)","v":3.2256},"F=",{"$f":"-0.5*((AP580*AQ581-AP581*AQ580)+(AP581*AQ582-AP582*AQ581)+\n (AP582*AQ583-AP583*AQ582)+\n(AP583*AQ584-AP584*AQ583)+\n(AP584*AQ585-AP585*AQ584)+\n(AP585*AQ586-AP586*AQ585)+\n(AP586*AQ587-AP587*AQ586)+\n(AP587*AQ588-AP588*AQ587)+\n(AP588*AQ589-AP589*AQ588)+\n(AP589*AQ590-AP590*AQ589)+\n(AP590*AQ591-AP591*AQ590)+\n(AP591*AQ592-AP592*AQ591)+\n(AP592*AQ593-AP593*AQ592)+\n(AP593*AQ594-AP594*AQ593)+\n(AP594*AQ595-AP595*AQ594)+\n(AP595*AQ596-AP596*AQ595)+\n(AP596*AQ597-AP597*AQ596)+\n(AP597*AQ598-AP598*AQ597)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AR580*AS581-AR581*AS580)+(AR581*AS582-AR582*AS581)+\n (AR582*AS583-AR583*AS582)+\n(AR583*AS584-AR584*AS583)+\n(AR584*AS585-AR585*AS584)+\n(AR585*AS586-AR586*AS585)+\n(AR586*AS587-AR587*AS586)+\n(AR587*AS588-AR588*AS587)+\n(AR588*AS589-AR589*AS588)+\n(AR589*AS590-AR590*AS589)+\n(AR590*AS591-AR591*AS590)+\n(AR591*AS592-AR592*AS591)+\n(AR592*AS593-AR593*AS592)+\n(AR593*AS594-AR594*AS593)+\n(AR594*AS595-AR595*AS594)+\n(AR595*AS596-AR596*AS595)+\n(AR596*AS597-AR597*AS596)+\n(AR597*AS598-AR598*AS597)\n)","v":0},"F=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$64","v":5.04},null,null,null,null," y=",{"$f":"+BC607","v":0.71999999999999986}," y=",{"$f":"+BE607","v":0}]
[null,null,null,"y=",{"$f":"+IF(E602=0,0,-((D579*E580-D580*E579)*(E579+E580)+(D580*E581-D581*E580)*(E580+E581)+\n(D581*E582-D582*E581)*(E581+E582)+\n(D582*E583-D583*E582)*(E582+E583)+\n(D583*E584-D584*E583)*(E583+E584)+\n(D584*E585-D585*E584)*(E584+E585)+\n(D585*E586-D586*E585)*(E585+E586)+\n(D586*E587-D587*E586)*(E586+E587)+\n(D587*E588-D588*E587)*(E587+E588)+\n(D588*E589-D589*E588)*(E588+E589)+\n(D589*E590-D590*E589)*(E589+E590)+\n(D590*E591-D591*E590)*(E590+E591)+\n(D591*E592-D592*E591)*(E591+E592)+\n(D592*E593-D594*E592)*(E592+E593)+\n(D594*E594-D595*E593)*(E593+E594)+\n(D595*E595-D596*E594)*(E594+E595)+\n(D596*E596-D597*E595)*(E595+E596)+\n(D597*E597-D598*E596)*(E596+E597)+\n(D598*E598-#REF!*E597)*(E597+E598))/6/E602)","v":0},"x=",1,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,null,null,"x=",0,"x=",0,"x=",0,"x=",0,0,{"$f":"'Analiza i dimenzioniranje'!$U$63","v":4.72},null,null,null,null,"z=",{"$f":"+BC603-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":0.21999999999999986},"z=",{"$f":"+BE603-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5}]
[null,null,null,"y=",{"$f":"+IF(E603=0,0,-((D580*E581-D581*E580)*(E580+E581)+(D581*E582-D582*E581)*(E581+E582)+\n(D582*E583-D583*E582)*(E582+E583)+\n(D583*E584-D584*E583)*(E583+E584)+\n(D584*E585-D585*E584)*(E584+E585)+\n(D585*E586-D586*E585)*(E585+E586)+\n(D586*E587-D587*E586)*(E586+E587)+\n(D587*E588-D588*E587)*(E587+E588)+\n(D588*E589-D589*E588)*(E588+E589)+\n(D589*E590-D590*E589)*(E589+E590)+\n(D590*E591-D591*E590)*(E590+E591)+\n(D591*E592-D592*E591)*(E591+E592)+\n(D592*E593-D594*E592)*(E592+E593)+\n(D594*E594-D595*E593)*(E593+E594)+\n(D595*E595-D596*E594)*(E594+E595)+\n(D596*E596-D597*E595)*(E595+E596)+\n(D597*E597-D598*E596)*(E596+E597)+\n(D598*E598-#REF!*E597)*(E597+E598)+\n(#REF!*E599-D599*E598)*(E598+E599))/6/E603)","v":0},"y=",{"$f":"+IF(G603=0,0,-((F580*G581-F581*G580)*(G580+G581)+(F581*G582-F582*G581)*(G581+G582)+\n(F582*G583-F583*G582)*(G582+G583)+\n(F583*G584-F584*G583)*(G583+G584)+\n(F584*G585-F585*G584)*(G584+G585)+\n(F585*G586-F586*G585)*(G585+G586)+\n(F586*G587-F587*G586)*(G586+G587)+\n(F587*G588-F588*G587)*(G587+G588)+\n(F588*G589-F589*G588)*(G588+G589)+\n(F589*G590-F590*G589)*(G589+G590)+\n(F590*G591-F591*G590)*(G590+G591)+\n(F591*G592-F592*G591)*(G591+G592)+\n(F592*G593-F593*G592)*(G592+G593)+\n(F593*G594-F594*G593)*(G593+G594)+\n(F594*G595-F595*G594)*(G594+G595)+\n(F595*G596-F596*G595)*(G595+G596)+\n(F596*G597-F597*G596)*(G596+G597)+\n(F597*G598-F598*G597)*(G597+G598)+\n(F598*G599-F599*G598)*(G598+G599))/6/G603)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(I603=0,0,-((H580*I581-H581*I580)*(I580+I581)+(H581*I582-H582*I581)*(I581+I582)+\n(H582*I583-H583*I582)*(I582+I583)+\n(H583*I584-H584*I583)*(I583+I584)+\n(H584*I585-H585*I584)*(I584+I585)+\n(H585*I586-H586*I585)*(I585+I586)+\n(H586*I587-H587*I586)*(I586+I587)+\n(H587*I588-H588*I587)*(I587+I588)+\n(H588*I589-H589*I588)*(I588+I589)+\n(H589*I590-H590*I589)*(I589+I590)+\n(H590*I591-H591*I590)*(I590+I591)+\n(H591*I592-H592*I591)*(I591+I592)+\n(H592*I593-H593*I592)*(I592+I593)+\n(H593*I594-H594*I593)*(I593+I594)+\n(H594*I595-H595*I594)*(I594+I595)+\n(H595*I596-H596*I595)*(I595+I596)+\n(H596*I597-H597*I596)*(I596+I597)+\n(H597*I598-H598*I597)*(I597+I598)+\n(H598*I599-H599*I598)*(I598+I599))/6/I603)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(K603=0,0,-((J580*K581-J581*K580)*(K580+K581)+(J581*K582-J582*K581)*(K581+K582)+\n(J582*K583-J583*K582)*(K582+K583)+\n(J583*K584-J584*K583)*(K583+K584)+\n(J584*K585-J585*K584)*(K584+K585)+\n(J585*K586-J586*K585)*(K585+K586)+\n(J586*K587-J587*K586)*(K586+K587)+\n(J587*K588-J588*K587)*(K587+K588)+\n(J588*K589-J589*K588)*(K588+K589)+\n(J589*K590-J590*K589)*(K589+K590)+\n(J590*K591-J591*K590)*(K590+K591)+\n(J591*K592-J592*K591)*(K591+K592)+\n(J592*K593-J593*K592)*(K592+K593)+\n(J593*K594-J594*K593)*(K593+K594)+\n(J594*K595-J595*K594)*(K594+K595)+\n(J595*K596-J596*K595)*(K595+K596)+\n(J596*K597-J597*K596)*(K596+K597)+\n(J597*K598-J598*K597)*(K597+K598)+\n(J598*K599-J599*K598)*(K598+K599))/6/K603)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(M603=0,0,-((L580*M581-L581*M580)*(M580+M581)+(L581*M582-L582*M581)*(M581+M582)+\n(L582*M583-L583*M582)*(M582+M583)+\n(L583*M584-L584*M583)*(M583+M584)+\n(L584*M585-L585*M584)*(M584+M585)+\n(L585*M586-L586*M585)*(M585+M586)+\n(L586*M587-L587*M586)*(M586+M587)+\n(L587*M588-L588*M587)*(M587+M588)+\n(L588*M589-L589*M588)*(M588+M589)+\n(L589*M590-L590*M589)*(M589+M590)+\n(L590*M591-L591*M590)*(M590+M591)+\n(L591*M592-L592*M591)*(M591+M592)+\n(L592*M593-L593*M592)*(M592+M593)+\n(L593*M594-L594*M593)*(M593+M594)+\n(L594*M595-L595*M594)*(M594+M595)+\n(L595*M596-L596*M595)*(M595+M596)+\n(L596*M597-L597*M596)*(M596+M597)+\n(L597*M598-L598*M597)*(M597+M598)+\n(L598*M599-L599*M598)*(M598+M599))/6/M603)","v":0},"y=",{"$f":"+IF(O603=0,0,-((N580*O581-N581*O580)*(O580+O581)+(N581*O582-N582*O581)*(O581+O582)+\n(N582*O583-N583*O582)*(O582+O583)+\n(N583*O584-N584*O583)*(O583+O584)+\n(N584*O585-N585*O584)*(O584+O585)+\n(N585*O586-N586*O585)*(O585+O586)+\n(N586*O587-N587*O586)*(O586+O587)+\n(N587*O588-N588*O587)*(O587+O588)+\n(N588*O589-N589*O588)*(O588+O589)+\n(N589*O590-N590*O589)*(O589+O590)+\n(N590*O591-N591*O590)*(O590+O591)+\n(N591*O592-N592*O591)*(O591+O592)+\n(N592*O593-N593*O592)*(O592+O593)+\n(N593*O594-N594*O593)*(O593+O594)+\n(N594*O595-N595*O594)*(O594+O595)+\n(N595*O596-N596*O595)*(O595+O596)+\n(N596*O597-N597*O596)*(O596+O597)+\n(N597*O598-N598*O597)*(O597+O598)+\n(N598*O599-N599*O598)*(O598+O599))/6/O603)","v":0},"y=",{"$f":"+IF(Q603=0,0,-((P580*Q581-P581*Q580)*(Q580+Q581)+(P581*Q582-P582*Q581)*(Q581+Q582)+\n(P582*Q583-P583*Q582)*(Q582+Q583)+\n(P583*Q584-P584*Q583)*(Q583+Q584)+\n(P584*Q585-P585*Q584)*(Q584+Q585)+\n(P585*Q586-P586*Q585)*(Q585+Q586)+\n(P586*Q587-P587*Q586)*(Q586+Q587)+\n(P587*Q588-P588*Q587)*(Q587+Q588)+\n(P588*Q589-P589*Q588)*(Q588+Q589)+\n(P589*Q590-P590*Q589)*(Q589+Q590)+\n(P590*Q591-P591*Q590)*(Q590+Q591)+\n(P591*Q592-P592*Q591)*(Q591+Q592)+\n(P592*Q593-P593*Q592)*(Q592+Q593)+\n(P593*Q594-P594*Q593)*(Q593+Q594)+\n(P594*Q595-P595*Q594)*(Q594+Q595)+\n(P595*Q596-P596*Q595)*(Q595+Q596)+\n(P596*Q597-P597*Q596)*(Q596+Q597)+\n(P597*Q598-P598*Q597)*(Q597+Q598)+\n(P598*Q599-P599*Q598)*(Q598+Q599))/6/Q603)","v":0},"y=",{"$f":"+IF(S603=0,0,-((R580*S581-R581*S580)*(S580+S581)+(R581*S582-R582*S581)*(S581+S582)+\n(R582*S583-R583*S582)*(S582+S583)+\n(R583*S584-R584*S583)*(S583+S584)+\n(R584*S585-R585*S584)*(S584+S585)+\n(R585*S586-R586*S585)*(S585+S586)+\n(R586*S587-R587*S586)*(S586+S587)+\n(R587*S588-R588*S587)*(S587+S588)+\n(R588*S589-R589*S588)*(S588+S589)+\n(R589*S590-R590*S589)*(S589+S590)+\n(R590*S591-R591*S590)*(S590+S591)+\n(R591*S592-R592*S591)*(S591+S592)+\n(R592*S593-R593*S592)*(S592+S593)+\n(R593*S594-R594*S593)*(S593+S594)+\n(R594*S595-R595*S594)*(S594+S595)+\n(R595*S596-R596*S595)*(S595+S596)+\n(R596*S597-R597*S596)*(S596+S597)+\n(R597*S598-R598*S597)*(S597+S598)+\n(R598*S599-R599*S598)*(S598+S599))/6/S603)","v":0},"y=",{"$f":"+IF(U603=0,0,-((T580*U581-T581*U580)*(U580+U581)+(T581*U582-T582*U581)*(U581+U582)+\n(T582*U583-T583*U582)*(U582+U583)+\n(T583*U584-T584*U583)*(U583+U584)+\n(T584*U585-T585*U584)*(U584+U585)+\n(T585*U586-T586*U585)*(U585+U586)+\n(T586*U587-T587*U586)*(U586+U587)+\n(T587*U588-T588*U587)*(U587+U588)+\n(T588*U589-T589*U588)*(U588+U589)+\n(T589*U590-T590*U589)*(U589+U590)+\n(T590*U591-T591*U590)*(U590+U591)+\n(T591*U592-T592*U591)*(U591+U592)+\n(T592*U593-T593*U592)*(U592+U593)+\n(T593*U594-T594*U593)*(U593+U594)+\n(T594*U595-T595*U594)*(U594+U595)+\n(T595*U596-T596*U595)*(U595+U596)+\n(T596*U597-T597*U596)*(U596+U597)+\n(T597*U598-T598*U597)*(U597+U598)+\n(T598*U599-T599*U598)*(U598+U599))/6/U603)","v":0},"y=",{"$f":"+IF(W603=0,0,-((V580*W581-V581*W580)*(W580+W581)+(V581*W582-V582*W581)*(W581+W582)+\n(V582*W583-V583*W582)*(W582+W583)+\n(V583*W584-V584*W583)*(W583+W584)+\n(V584*W585-V585*W584)*(W584+W585)+\n(V585*W586-V586*W585)*(W585+W586)+\n(V586*W587-V587*W586)*(W586+W587)+\n(V587*W588-V588*W587)*(W587+W588)+\n(V588*W589-V589*W588)*(W588+W589)+\n(V589*W590-V590*W589)*(W589+W590)+\n(V590*W591-V591*W590)*(W590+W591)+\n(V591*W592-V592*W591)*(W591+W592)+\n(V592*W593-V593*W592)*(W592+W593)+\n(V593*W594-V594*W593)*(W593+W594)+\n(V594*W595-V595*W594)*(W594+W595)+\n(V595*W596-V596*W595)*(W595+W596)+\n(V596*W597-V597*W596)*(W596+W597)+\n(V597*W598-V598*W597)*(W597+W598)+\n(V598*W599-V599*W598)*(W598+W599))/6/W603)","v":0},"y=",{"$f":"+IF(Y603=0,0,-((X580*Y581-X581*Y580)*(Y580+Y581)+(X581*Y582-X582*Y581)*(Y581+Y582)+\n(X582*Y583-X583*Y582)*(Y582+Y583)+\n(X583*Y584-X584*Y583)*(Y583+Y584)+\n(X584*Y585-X585*Y584)*(Y584+Y585)+\n(X585*Y586-X586*Y585)*(Y585+Y586)+\n(X586*Y587-X587*Y586)*(Y586+Y587)+\n(X587*Y588-X588*Y587)*(Y587+Y588)+\n(X588*Y589-X589*Y588)*(Y588+Y589)+\n(X589*Y590-X590*Y589)*(Y589+Y590)+\n(X590*Y591-X591*Y590)*(Y590+Y591)+\n(X591*Y592-X592*Y591)*(Y591+Y592)+\n(X592*Y593-X593*Y592)*(Y592+Y593)+\n(X593*Y594-X594*Y593)*(Y593+Y594)+\n(X594*Y595-X595*Y594)*(Y594+Y595)+\n(X595*Y596-X596*Y595)*(Y595+Y596)+\n(X596*Y597-X597*Y596)*(Y596+Y597)+\n(X597*Y598-X598*Y597)*(Y597+Y598)+\n(X598*Y599-X599*Y598)*(Y598+Y599))/6/Y603)","v":0},"y=",{"$f":"+IF(AA603=0,0,-((Z580*AA581-Z581*AA580)*(AA580+AA581)+(Z581*AA582-Z582*AA581)*(AA581+AA582)+\n(Z582*AA583-Z583*AA582)*(AA582+AA583)+\n(Z583*AA584-Z584*AA583)*(AA583+AA584)+\n(Z584*AA585-Z585*AA584)*(AA584+AA585)+\n(Z585*AA586-Z586*AA585)*(AA585+AA586)+\n(Z586*AA587-Z587*AA586)*(AA586+AA587)+\n(Z587*AA588-Z588*AA587)*(AA587+AA588)+\n(Z588*AA589-Z589*AA588)*(AA588+AA589)+\n(Z589*AA590-Z590*AA589)*(AA589+AA590)+\n(Z590*AA591-Z591*AA590)*(AA590+AA591)+\n(Z591*AA592-Z592*AA591)*(AA591+AA592)+\n(Z592*AA593-Z593*AA592)*(AA592+AA593)+\n(Z593*AA594-Z594*AA593)*(AA593+AA594)+\n(Z594*AA595-Z595*AA594)*(AA594+AA595)+\n(Z595*AA596-Z596*AA595)*(AA595+AA596)+\n(Z596*AA597-Z597*AA596)*(AA596+AA597)+\n(Z597*AA598-Z598*AA597)*(AA597+AA598)+\n(Z598*AA599-Z599*AA598)*(AA598+AA599))/6/AA603)","v":0},"y=",{"$f":"+IF(AC603=0,0,-((AB580*AC581-AB581*AC580)*(AC580+AC581)+(AB581*AC582-AB582*AC581)*(AC581+AC582)+\n(AB582*AC583-AB583*AC582)*(AC582+AC583)+\n(AB583*AC584-AB584*AC583)*(AC583+AC584)+\n(AB584*AC585-AB585*AC584)*(AC584+AC585)+\n(AB585*AC586-AB586*AC585)*(AC585+AC586)+\n(AB586*AC587-AB587*AC586)*(AC586+AC587)+\n(AB587*AC588-AB588*AC587)*(AC587+AC588)+\n(AB588*AC589-AB589*AC588)*(AC588+AC589)+\n(AB589*AC590-AB590*AC589)*(AC589+AC590)+\n(AB590*AC591-AB591*AC590)*(AC590+AC591)+\n(AB591*AC592-AB592*AC591)*(AC591+AC592)+\n(AB592*AC593-AB593*AC592)*(AC592+AC593)+\n(AB593*AC594-AB594*AC593)*(AC593+AC594)+\n(AB594*AC595-AB595*AC594)*(AC594+AC595)+\n(AB595*AC596-AB596*AC595)*(AC595+AC596)+\n(AB596*AC597-AB597*AC596)*(AC596+AC597)+\n(AB597*AC598-AB598*AC597)*(AC597+AC598)+\n(AB598*AC599-AB599*AC598)*(AC598+AC599))/6/AC603)","v":0},"y=",{"$f":"+IF(AE603=0,0,-((AD580*AE581-AD581*AE580)*(AE580+AE581)+(AD581*AE582-AD582*AE581)*(AE581+AE582)+\n(AD582*AE583-AD583*AE582)*(AE582+AE583)+\n(AD583*AE584-AD584*AE583)*(AE583+AE584)+\n(AD584*AE585-AD585*AE584)*(AE584+AE585)+\n(AD585*AE586-AD586*AE585)*(AE585+AE586)+\n(AD586*AE587-AD587*AE586)*(AE586+AE587)+\n(AD587*AE588-AD588*AE587)*(AE587+AE588)+\n(AD588*AE589-AD589*AE588)*(AE588+AE589)+\n(AD589*AE590-AD590*AE589)*(AE589+AE590)+\n(AD590*AE591-AD591*AE590)*(AE590+AE591)+\n(AD591*AE592-AD592*AE591)*(AE591+AE592)+\n(AD592*AE593-AD593*AE592)*(AE592+AE593)+\n(AD593*AE594-AD594*AE593)*(AE593+AE594)+\n(AD594*AE595-AD595*AE594)*(AE594+AE595)+\n(AD595*AE596-AD596*AE595)*(AE595+AE596)+\n(AD596*AE597-AD597*AE596)*(AE596+AE597)+\n(AD597*AE598-AD598*AE597)*(AE597+AE598)+\n(AD598*AE599-AD599*AE598)*(AE598+AE599))/6/AE603)","v":0},"y=",{"$f":"+IF(AG603=0,0,-((AF580*AG581-AF581*AG580)*(AG580+AG581)+(AF581*AG582-AF582*AG581)*(AG581+AG582)+\n(AF582*AG583-AF583*AG582)*(AG582+AG583)+\n(AF583*AG584-AF584*AG583)*(AG583+AG584)+\n(AF584*AG585-AF585*AG584)*(AG584+AG585)+\n(AF585*AG586-AF586*AG585)*(AG585+AG586)+\n(AF586*AG587-AF587*AG586)*(AG586+AG587)+\n(AF587*AG588-AF588*AG587)*(AG587+AG588)+\n(AF588*AG589-AF589*AG588)*(AG588+AG589)+\n(AF589*AG590-AF590*AG589)*(AG589+AG590)+\n(AF590*AG591-AF591*AG590)*(AG590+AG591)+\n(AF591*AG592-AF592*AG591)*(AG591+AG592)+\n(AF592*AG593-AF593*AG592)*(AG592+AG593)+\n(AF593*AG594-AF594*AG593)*(AG593+AG594)+\n(AF594*AG595-AF595*AG594)*(AG594+AG595)+\n(AF595*AG596-AF596*AG595)*(AG595+AG596)+\n(AF596*AG597-AF597*AG596)*(AG596+AG597)+\n(AF597*AG598-AF598*AG597)*(AG597+AG598)+\n(AF598*AG599-AF599*AG598)*(AG598+AG599))/6/AG603)","v":0},"y=",{"$f":"+IF(AI603=0,0,-((AH580*AI581-AH581*AI580)*(AI580+AI581)+(AH581*AI582-AH582*AI581)*(AI581+AI582)+\n(AH582*AI583-AH583*AI582)*(AI582+AI583)+\n(AH583*AI584-AH584*AI583)*(AI583+AI584)+\n(AH584*AI585-AH585*AI584)*(AI584+AI585)+\n(AH585*AI586-AH586*AI585)*(AI585+AI586)+\n(AH586*AI587-AH587*AI586)*(AI586+AI587)+\n(AH587*AI588-AH588*AI587)*(AI587+AI588)+\n(AH588*AI589-AH589*AI588)*(AI588+AI589)+\n(AH589*AI590-AH590*AI589)*(AI589+AI590)+\n(AH590*AI591-AH591*AI590)*(AI590+AI591)+\n(AH591*AI592-AH592*AI591)*(AI591+AI592)+\n(AH592*AI593-AH593*AI592)*(AI592+AI593)+\n(AH593*AI594-AH594*AI593)*(AI593+AI594)+\n(AH594*AI595-AH595*AI594)*(AI594+AI595)+\n(AH595*AI596-AH596*AI595)*(AI595+AI596)+\n(AH596*AI597-AH597*AI596)*(AI596+AI597)+\n(AH597*AI598-AH598*AI597)*(AI597+AI598)+\n(AH598*AI599-AH599*AI598)*(AI598+AI599))/6/AI603)","v":0},"y=",{"$f":"+IF(AK603=0,0,-((AJ580*AK581-AJ581*AK580)*(AK580+AK581)+(AJ581*AK582-AJ582*AK581)*(AK581+AK582)+\n(AJ582*AK583-AJ583*AK582)*(AK582+AK583)+\n(AJ583*AK584-AJ584*AK583)*(AK583+AK584)+\n(AJ584*AK585-AJ585*AK584)*(AK584+AK585)+\n(AJ585*AK586-AJ586*AK585)*(AK585+AK586)+\n(AJ586*AK587-AJ587*AK586)*(AK586+AK587)+\n(AJ587*AK588-AJ588*AK587)*(AK587+AK588)+\n(AJ588*AK589-AJ589*AK588)*(AK588+AK589)+\n(AJ589*AK590-AJ590*AK589)*(AK589+AK590)+\n(AJ590*AK591-AJ591*AK590)*(AK590+AK591)+\n(AJ591*AK592-AJ592*AK591)*(AK591+AK592)+\n(AJ592*AK593-AJ593*AK592)*(AK592+AK593)+\n(AJ593*AK594-AJ594*AK593)*(AK593+AK594)+\n(AJ594*AK595-AJ595*AK594)*(AK594+AK595)+\n(AJ595*AK596-AJ596*AK595)*(AK595+AK596)+\n(AJ596*AK597-AJ597*AK596)*(AK596+AK597)+\n(AJ597*AK598-AJ598*AK597)*(AK597+AK598)+\n(AJ598*AK599-AJ599*AK598)*(AK598+AK599))/6/AK603)","v":0},null,null,"y=",{"$f":"+IF(AO603=0,0,-((AN580*AO581-AN581*AO580)*(AO580+AO581)+(AN581*AO582-AN582*AO581)*(AO581+AO582)+\n(AN582*AO583-AN583*AO582)*(AO582+AO583)+\n(AN583*AO584-AN584*AO583)*(AO583+AO584)+\n(AN584*AO585-AN585*AO584)*(AO584+AO585)+\n(AN585*AO586-AN586*AO585)*(AO585+AO586)+\n(AN586*AO587-AN587*AO586)*(AO586+AO587)+\n(AN587*AO588-AN588*AO587)*(AO587+AO588)+\n(AN588*AO589-AN589*AO588)*(AO588+AO589)+\n(AN589*AO590-AN590*AO589)*(AO589+AO590)+\n(AN590*AO591-AN591*AO590)*(AO590+AO591)+\n(AN591*AO592-AN592*AO591)*(AO591+AO592)+\n(AN592*AO593-AN593*AO592)*(AO592+AO593)+\n(AN593*AO594-AN594*AO593)*(AO593+AO594)+\n(AN594*AO595-AN595*AO594)*(AO594+AO595)+\n(AN595*AO596-AN596*AO595)*(AO595+AO596)+\n(AN596*AO597-AN597*AO596)*(AO596+AO597)+\n(AN597*AO598-AN598*AO597)*(AO597+AO598)+\n(AN598*AO599-AN599*AO598)*(AO598+AO599))/6/AO603)","v":10.973866666666668},"y=",{"$f":"+IF(AQ603=0,0,-((AP580*AQ581-AP581*AQ580)*(AQ580+AQ581)+(AP581*AQ582-AP582*AQ581)*(AQ581+AQ582)+\n(AP582*AQ583-AP583*AQ582)*(AQ582+AQ583)+\n(AP583*AQ584-AP584*AQ583)*(AQ583+AQ584)+\n(AP584*AQ585-AP585*AQ584)*(AQ584+AQ585)+\n(AP585*AQ586-AP586*AQ585)*(AQ585+AQ586)+\n(AP586*AQ587-AP587*AQ586)*(AQ586+AQ587)+\n(AP587*AQ588-AP588*AQ587)*(AQ587+AQ588)+\n(AP588*AQ589-AP589*AQ588)*(AQ588+AQ589)+\n(AP589*AQ590-AP590*AQ589)*(AQ589+AQ590)+\n(AP590*AQ591-AP591*AQ590)*(AQ590+AQ591)+\n(AP591*AQ592-AP592*AQ591)*(AQ591+AQ592)+\n(AP592*AQ593-AP593*AQ592)*(AQ592+AQ593)+\n(AP593*AQ594-AP594*AQ593)*(AQ593+AQ594)+\n(AP594*AQ595-AP595*AQ594)*(AQ594+AQ595)+\n(AP595*AQ596-AP596*AQ595)*(AQ595+AQ596)+\n(AP596*AQ597-AP597*AQ596)*(AQ596+AQ597)+\n(AP597*AQ598-AP598*AQ597)*(AQ597+AQ598)+\n(AP598*AQ599-AP599*AQ598)*(AQ598+AQ599))/6/AQ603)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AS603=0,0,-((AR580*AS581-AR581*AS580)*(AS580+AS581)+(AR581*AS582-AR582*AS581)*(AS581+AS582)+\n(AR582*AS583-AR583*AS582)*(AS582+AS583)+\n(AR583*AS584-AR584*AS583)*(AS583+AS584)+\n(AR584*AS585-AR585*AS584)*(AS584+AS585)+\n(AR585*AS586-AR586*AS585)*(AS585+AS586)+\n(AR586*AS587-AR587*AS586)*(AS586+AS587)+\n(AR587*AS588-AR588*AS587)*(AS587+AS588)+\n(AR588*AS589-AR589*AS588)*(AS588+AS589)+\n(AR589*AS590-AR590*AS589)*(AS589+AS590)+\n(AR590*AS591-AR591*AS590)*(AS590+AS591)+\n(AR591*AS592-AR592*AS591)*(AS591+AS592)+\n(AR592*AS593-AR593*AS592)*(AS592+AS593)+\n(AR593*AS594-AR594*AS593)*(AS593+AS594)+\n(AR594*AS595-AR595*AS594)*(AS594+AS595)+\n(AR595*AS596-AR596*AS595)*(AS595+AS596)+\n(AR596*AS597-AR597*AS596)*(AS596+AS597)+\n(AR597*AS598-AR598*AS597)*(AS597+AS598)+\n(AR598*AS599-AR599*AS598)*(AS598+AS599))/6/AS603)","v":0},"y=",0,{"$f":"BK424-BQ423","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$62","v":4.4000000000000004},null,null,null,null,"F=",{"$f":"-0.5*((BB582*BC583-BB583*BC582)+(BB583*BC584-BB584*BC583)+\n (BB584*BC585-BB585*BC584)+\n(BB585*BC586-BB586*BC585)+\n(BB586*BC587-BB587*BC586)+\n(BB587*BC588-BB588*BC587)+\n(BB588*BC589-BB589*BC588)+\n(BB589*BC590-BB590*BC589)+\n(BB590*BC591-BB591*BC590)+\n(BB591*BC592-BB592*BC591)+\n(BB592*BC593-BB593*BC592)+\n(BB593*BC594-BB594*BC593)+\n(BB594*BC595-BB595*BC594)+\n(BB595*BC596-BB596*BC595)+\n(BB596*BC597-BB597*BC596)+\n(BB597*BC598-BB598*BC597)+\n(BB598*BC599-BB599*BC598)+\n(BB599*BC600-BB600*BC599)\n)","v":-15.839999999999998},"F=",{"$f":"-0.5*((BD582*BE583-BD583*BE582)+(BD583*BE584-BD584*BE583)+\n (BD584*BE585-BD585*BE584)+\n(BD585*BE586-BD586*BE585)+\n(BD586*BE587-BD587*BE586)+\n(BD587*BE588-BD588*BE587)+\n(BD588*BE589-BD589*BE588)+\n(BD589*BE590-BD590*BE589)+\n(BD590*BE591-BD591*BE590)+\n(BD591*BE592-BD592*BE591)+\n(BD592*BE593-BD593*BE592)+\n(BD593*BE594-BD594*BE593)+\n(BD594*BE595-BD595*BE594)+\n(BD595*BE596-BD596*BE595)+\n(BD596*BE597-BD597*BE596)+\n(BD597*BE598-BD598*BE597)+\n(BD598*BE599-BD599*BE598)+\n(BD599*BE600-BD600*BE599)\n)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$61","v":4.08},null,null,null,null,"x=",0,"x=",0]
[null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$60","v":3.76},null,null,null,null,"y=",{"$f":"+IF(BC605=0,0,-((BB582*BC583-BB583*BC582)*(BC582+BC583)+(BB583*BC584-BB584*BC583)*(BC583+BC584)+\n(BB584*BC585-BB585*BC584)*(BC584+BC585)+\n(BB585*BC586-BB586*BC585)*(BC585+BC586)+\n(BB586*BC587-BB587*BC586)*(BC586+BC587)+\n(BB587*BC588-BB588*BC587)*(BC587+BC588)+\n(BB588*BC589-BB589*BC588)*(BC588+BC589)+\n(BB589*BC590-BB590*BC589)*(BC589+BC590)+\n(BB590*BC591-BB591*BC590)*(BC590+BC591)+\n(BB591*BC592-BB592*BC591)*(BC591+BC592)+\n(BB592*BC593-BB593*BC592)*(BC592+BC593)+\n(BB593*BC594-BB594*BC593)*(BC593+BC594)+\n(BB594*BC595-BB595*BC594)*(BC594+BC595)+\n(BB595*BC596-BB596*BC595)*(BC595+BC596)+\n(BB596*BC597-BB597*BC596)*(BC596+BC597)+\n(BB597*BC598-BB598*BC597)*(BC597+BC598)+\n(BB598*BC599-BB599*BC598)*(BC598+BC599)+\n(BB599*BC600-BB600*BC599)*(BC599+BC600)+\n(BB600*BC601-BB601*BC600)*(BC600+BC601))/6/BC605)","v":0.71999999999999986},"y=",{"$f":"+IF(BE605=0,0,-((BD582*BE583-BD583*BE582)*(BE582+BE583)+(BD583*BE584-BD584*BE583)*(BE583+BE584)+\n(BD584*BE585-BD585*BE584)*(BE584+BE585)+\n(BD585*BE586-BD586*BE585)*(BE585+BE586)+\n(BD586*BE587-BD587*BE586)*(BE586+BE587)+\n(BD587*BE588-BD588*BE587)*(BE587+BE588)+\n(BD588*BE589-BD589*BE588)*(BE588+BE589)+\n(BD589*BE590-BD590*BE589)*(BE589+BE590)+\n(BD590*BE591-BD591*BE590)*(BE590+BE591)+\n(BD591*BE592-BD592*BE591)*(BE591+BE592)+\n(BD592*BE593-BD593*BE592)*(BE592+BE593)+\n(BD593*BE594-BD594*BE593)*(BE593+BE594)+\n(BD594*BE595-BD595*BE594)*(BE594+BE595)+\n(BD595*BE596-BD596*BE595)*(BE595+BE596)+\n(BD596*BE597-BD597*BE596)*(BE596+BE597)+\n(BD597*BE598-BD598*BE597)*(BE597+BE598)+\n(BD598*BE599-BD599*BE598)*(BE598+BE599)+\n(BD599*BE600-BD600*BE599)*(BE599+BE600)+\n(BD600*BE601-BD601*BE600)*(BE600+BE601))/6/BE605)","v":0}]
[null,"OPTEREĆENJE TEMELJEM",null,null,null,null,null,null,null," (TERZAGHY)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$59","v":3.44}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$58","v":3.14}]
[null,"KONTINUIRANO OPTEREĆENJE",null,"P - D=",{"$f":"IF('Analiza i dimenzioniranje'!$E$28<=0,0,+'Analiza i dimenzioniranje'!$E$28-I610)","v":{"$error":"#VALUE!"}},"kN/m2","raster. iskopom   D=y*Df =",null,{"$f":"+'Analiza i dimenzioniranje'!$D$16*('Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20-D616)","v":{"$error":"#VALUE!"}},"kN/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$57","v":2.8}]
[null," visina zida i temelja",null,"H =",{"$f":"+E531","v":{"$error":"#VALUE!"}},"m",{"$f":"E615","v":6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BK430-BQ429","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$56","v":2.48}]
[null,"visina opterećenja iznad vrha zida",null,"h =",{"$f":"+E532","v":-1},"m",{"$f":"SQRT(E615^2+E614^2)","v":6.7082039324993694},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.84,{"$f":"BK431-BQ430","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$55","v":2.16}]
[null,"širina temelja",null,"b =",{"$f":"+E533","v":1},"m   ",{"$f":"E614+E613","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.32,{"$f":"BK432-BQ431","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$54","v":1.84}]
[null,"udaljenost temelja od zida",null,"D =",{"$f":"+E534","v":3},"m    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.64,{"$f":"BK433-BQ432","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$53","v":1.52}]
[null,"1/2 dužine temelja",null,"L/2=a=",{"$f":"+E535","v":6},"m",{"$f":"SQRT(G611^2+G613^2)","v":7.2111025509279782},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,0,{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
["DNO TEMELJA NA VISINI","PRESJEK NA Visini ",null,{"$f":"ROUND('Analiza i dimenzioniranje'!U54,2)","v":1.84},null,"Presjek III - III",null,"Presjek VI",null,"Presjek VII-VII",null,"Presjek VIII-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"Presjek XIV-XIV",null,"Presjek XV-XV",null,"PresjekXVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX",null,null,null,null,null,null,null,null,null,null,6.2,{"$f":"+IF(AW617>=AW$299,0,BK435-BQ434)","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
[null,null,null,null,null,"Visina djelovanja","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja ","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja",null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2",{"$f":"+AU620","v":0},"SQhi=",6.2]
[null,null,null,{"$f":"+F619","v":0},{"$f":"+D618-E616","v":0},"III",{"$f":"+D616","v":1.84},"IV",{"$f":"+G618","v":1.84},"VII",{"$f":"+G618","v":1.84},"VIII",{"$f":"'Analiza i dimenzioniranje'!U367","v":1},"IX",{"$f":"+G618","v":1.84},"X",{"$f":"+'Analiza i dimenzioniranje'!O271","v":0},"XI",{"$f":"+G618","v":1.84},"XII",{"$f":"+'Analiza i dimenzioniranje'!S271","v":0},"XIII",{"$f":"+G618","v":1.84},"XIV",{"$f":"+W618","v":1.84},"XV",{"$f":"+G618","v":1.84},"XVI",{"$f":"+I618","v":1.84},"XVII",{"$f":"+AC618","v":1.84},"XVIII",{"$f":"+AC618","v":1.84},"XIX",{"$f":"+AE618","v":1.84},"XX",{"$f":"+AG618","v":1.84},null,"zi","A2","D2","C2","sb2",null,"zi","A2","D2","C2","sb1","(s1/2-s2/2)*2"]
[null,null,null,0,{"$f":"IF(D618>E$296,D618,E$296)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja"]
[null,null,null,0,{"$f":"IF(AW599>G$298,0,AW599)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"XVIII",{"$f":"+'Analiza i dimenzioniranje'!U397","v":{"$error":"#VALUE!"}},"XIX",{"$f":"+'Analiza i dimenzioniranje'!U396","v":{"$error":"#VALUE!"}},"XX",{"$f":"'Analiza i dimenzioniranje'!U395","v":{"$error":"#VALUE!"}}]
[null,null,null,0,{"$f":"+AW600","v":6.0000000000000009},0,0,{"$f":"+F621","v":0},{"$f":"+G621","v":0},0,0,0,0,0,{"$f":"+M621","v":0},0,{"$f":"+O621","v":0},0,{"$f":"+AS621","v":0},0,{"$f":"+S621","v":0},0,{"$f":"+AS621","v":0},0,{"$f":"+W621","v":0},0,{"$f":"+S621","v":0},0,{"$f":"+AA621","v":0},0,{"$f":"+AU598","v":0},0,{"$f":"+AU598","v":0},0,{"$f":"+AG621","v":0},{"$f":"+AD621","v":0},{"$f":"+AG621","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AD659","v":0},{"$f":"+BB621-BC620","v":{"$error":"#VALUE!"}},{"$f":"+AD659","v":0},{"$f":"+BD621-BE620","v":{"$error":"#VALUE!"}},{"$f":"+AD659","v":0},{"$f":"+'Analiza i dimenzioniranje'!E393","v":{"$error":"#VALUE!"}}]
[null,null,null,0,{"$f":"IF(AW601>G$298,0,AW601)","v":0},0,0,0,{"$f":"+G622","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU599","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+AU637","v":9.4095999999999993},{"$f":"+AT660","v":0},{"$f":"+BC622","v":9.4095999999999993},0,{"$f":"+AE660","v":0}]
[null,null,null,{"$f":"+AV599","v":{"$error":"#REF!"}},0,0,0,{"$f":"+F623","v":0},0,{"$f":"+F621","v":0},0,{"$f":"+D620","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU600","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE661","v":0}]
[null,{"$f":"+D543","v":{"$error":"#REF!"}},null,0,0,0,0,0,0,{"$f":"+F622","v":0},0,{"$f":"+D621","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU601","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE662","v":0}]
[null,0,null,0,0,0,0,0,0,0,0,{"$f":"+D622","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU602","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE663","v":0}]
[null,0,null,0,4.4000000000000004,0,0,0,0,0,0,{"$f":"+D419","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AE625","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+AE664","v":0}]
[null,0,null,0,4.08,0,0,0,0,0,0,{"$f":"+D624","v":0},0,{"$f":"+J625","v":0},0,{"$f":"+L625","v":0},0,0,0,{"$f":"+P625","v":0},0,0,0,{"$f":"+T625","v":0},0,0,0,{"$f":"+X625","v":0},0,0,{"$f":"+AU604","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,{"$f":"+BC627","v":0}]
[null,0,null,0,3.76,0,0,0,0,0,0,0,0,{"$f":"+J626","v":0},0,{"$f":"+L626","v":0},0,0,0,{"$f":"+P626","v":0},0,0,0,{"$f":"+T626","v":0},0,0,{"$f":"+AA627","v":0},{"$f":"+X626","v":0},0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,0,null,"+",3.44,0,0,0,{"$f":"+G629","v":0},{"$f":"+F629","v":0},0,{"$f":"+D626","v":0},0,{"$f":"+J627","v":0},0,{"$f":"+N629","v":0},{"$f":"+O629","v":0},0,0,{"$f":"+R629","v":0},{"$f":"+S629","v":0},0,0,{"$f":"+V629","v":0},0,0,{"$f":"+S629","v":0},{"$f":"+Z629","v":0},{"$f":"+AA629","v":0},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,"+",null,{"$f":"+AV606","v":0},3.14,0,0,0,{"$f":"+G630","v":0},0,0,{"$f":"+J630","v":0},0,{"$f":"+L630","v":0},{"$f":"+M630","v":0},{"$f":"+N630","v":0},{"$f":"+O630","v":0},{"$f":"+P630","v":0},{"$f":"+Q630","v":0},{"$f":"+R630","v":0},{"$f":"+S630","v":0},{"$f":"+T630","v":0},{"$f":"+U630","v":0},{"$f":"+V630","v":0},0,0,0,{"$f":"+Z630","v":0},{"$f":"+AA630","v":0},0,0,{"$f":"+AD630","v":0},{"$f":"+AE630","v":0},{"$f":"+AF630","v":0},0,0,{"$f":"+BC592","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,0,null,{"$f":"+AV607","v":0},2.8,0,0,0,{"$f":"+G631","v":0},0,0,{"$f":"+J631","v":0},0,{"$f":"+J631","v":0},{"$f":"+M631","v":0},{"$f":"+L631","v":0},{"$f":"+O631","v":0},{"$f":"+N631","v":0},{"$f":"+Q631","v":0},0,{"$f":"+S631","v":0},{"$f":"+T631","v":0},{"$f":"+Y631","v":0},{"$f":"+B625","v":0},{"$f":"+U631","v":0},{"$f":"+B625","v":0},0,{"$f":"+Z631","v":0},{"$f":"+U631","v":0},{"$f":"+AB631","v":0},0,{"$f":"+AB631","v":0},{"$f":"+AC631","v":0},{"$f":"+AF631","v":0},0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,0,null,{"$f":"+AV608","v":0},2.48,{"$f":"+D635","v":0},0,0,0,0,0,{"$f":"+J632","v":0},0,{"$f":"+J632","v":0},{"$f":"+M632","v":0},{"$f":"+L632","v":0},{"$f":"+O632","v":0},0,{"$f":"+S631","v":0},0,0,0,{"$f":"+AS632","v":0},0,0,0,0,{"$f":"+Z632","v":0},0,{"$f":"+AB632","v":0},0,{"$f":"+AB632","v":0},0,{"$f":"+AF632","v":0},0,0,{"$f":"+BC594","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,0,null,null,2.16,{"$f":"+D635","v":0},0,0,0,0,0,0,0,{"$f":"+J633","v":0},{"$f":"+M633","v":0},0,{"$f":"+O633","v":0},0,{"$f":"+Q633","v":0},0,{"$f":"+S633","v":0},0,{"$f":"+U633","v":0},0,{"$f":"+W633","v":0},0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,{"$f":"+D553","v":0},null,null,1.84,{"$f":"+D635","v":0},0,0,0,0,{"$f":"+E633","v":2.16},0,2.16,0,{"$f":"+O633","v":0},0,0,0,{"$f":"+AS634","v":0},0,0,0,{"$f":"+AS634","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+D594","v":0},1.52,{"$f":"+D635","v":0},{"$f":"+AW613","v":1.84},0,1.84,0,{"$f":"+E634","v":1.84},0,{"$f":"+K635","v":1.84},0,{"$f":"+M635","v":1.84},0,{"$f":"+O635","v":1.84},0,{"$f":"+Q635","v":1.84},0,{"$f":"+S635","v":1.84},0,{"$f":"+U635","v":1.84},0,{"$f":"+W635","v":1.84},0,{"$f":"+Y635","v":1.84},0,1.84,0,1.84,0,1.84,0,1.84,0,1.84,null,{"$f":"+D635","v":0},{"$f":"$E$614^2+AM635^2","v":9},{"$f":"$G$613^2+AM635^2","v":16},{"$f":"$G$615^2+AM635^2","v":51.999999999999993},{"$f":"IF(AM635=0,0,$E$610/(PI())*(ATAN(($E$615*$G$613)/(AM635*SQRT(AP635)))-$E$615*$G$573*AM635/(AO635*SQRT(AP635))))","v":0},null,{"$f":"+AM635","v":0},{"$f":"$E$615^2+AS635^2","v":36},{"$f":"$E$614^2+AS635^2","v":9},{"$f":"$G$612^2+AS635^2","v":45.000000000000007},{"$f":"IF(AS635=0,0,($E$610/(PI()))*(ATAN(($E$615*$E$614)/(AS635*SQRT(AV635)))-$E$615*$E$614*AS635/(AU635*SQRT(AV635))))","v":0},{"$f":"(+AQ635-AW635)*2","v":0},null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+D595","v":0.32},1.2,{"$f":"+AX636","v":{"$error":"#VALUE!"}},{"$f":"+AW614","v":1.52},{"$error":"#VALUE!"},1.52,{"$f":"+H636","v":{"$error":"#VALUE!"}},{"$f":"+I636","v":1.52},{"$f":"+J636","v":{"$error":"#VALUE!"}},{"$f":"+N636","v":0},0,{"$f":"+AM636","v":0.32},0,0,0,{"$f":"+AS636","v":0.32},0,0,0,{"$f":"+AS636","v":0.32},0,0,0,{"$f":"+S636","v":0.32},0,0,0,{"$f":"+AE635","v":1.84},0,0,0,0,0,0.32,null,{"$f":"+D636","v":0.32},{"$f":"$E$614^2+AM636^2","v":9.1023999999999994},{"$f":"$G$613^2+AM636^2","v":16.102399999999999},{"$f":"$G$615^2+AM636^2","v":52.102399999999996},{"$f":"IF(AM636=0,0,$E$610/(PI())*(ATAN(($E$615*$G$613)/(AM636*SQRT(AP636)))-$E$615*$G$613*AM636/(AO636*SQRT(AP636))))","v":{"$error":"#VALUE!"}},null,0.32,{"$f":"$E$615^2+AS636^2","v":36.102400000000003},{"$f":"$E$614^2+AS636^2","v":9.1023999999999994},{"$f":"$G$612^2+AS636^2","v":45.10240000000001},{"$f":"IF(AS636=0,0,($E$610/(PI()))*(ATAN(($E$615*$E$574)/(AS636*SQRT(AV636)))-$E$615*$E$574*AS636/(AU636*SQRT(AV636))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,0,0,0,0,0,0]
[null,null,null,{"$f":"+D596","v":0.64},{"$f":"+AW616","v":1.2},{"$f":"+AX637","v":{"$error":"#VALUE!"}},{"$f":"+AW615","v":1.2},0,{"$f":"+I636","v":1.52},0,{"$f":"+I637","v":1.52},0,{"$f":"+N637","v":0},0,{"$f":"+AM637","v":0.64},0,0,0,{"$f":"+AS637","v":0.64},0,0,0,{"$f":"+AS637","v":0.64},0,0,0,{"$f":"+S637","v":0.64},0,0,0,{"$f":"+AU614","v":0.64},0,0,0,0,0,0.64,null,{"$f":"+D637","v":0.64},{"$f":"$E$614^2+AM637^2","v":9.4095999999999993},{"$f":"$G$613^2+AM637^2","v":16.409600000000001},{"$f":"$G$615^2+AM637^2","v":52.40959999999999},{"$f":"IF(AM637=0,0,$E$610/(PI())*(ATAN(($E$615*$G$613)/(AM637*SQRT(AP637)))-$E$615*$G$573*AM637/(AO637*SQRT(AP637))))","v":{"$error":"#VALUE!"}},null,0.64,{"$f":"$E$615^2+AS637^2","v":36.409599999999998},{"$f":"$E$614^2+AS637^2","v":9.4095999999999993},{"$f":"$G$612^2+AS637^2","v":45.409600000000005},{"$f":"IF(AS637=0,0,($E$610/(PI()))*(ATAN(($E$615*$E$574)/(AS637*SQRT(AV637)))-$E$615*$E$574*AS637/(AU637*SQRT(AV637))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,0,0,0,0,0,0]
[null,null,null,null,{"$f":"+AW617","v":6.2},0,{"$f":"+E637","v":1.2},0,{"$f":"+G638","v":1.2},0,{"$f":"+I638","v":1.2},0,{"$f":"+K638","v":1.2},0,{"$f":"+M638","v":1.2},0,{"$f":"+O638","v":1.2},0,{"$f":"+Q638","v":1.2},0,{"$f":"+S638","v":1.2},0,{"$f":"+U638","v":1.2},{"$f":"+P638","v":0},{"$f":"+W638","v":1.2},0,{"$f":"+Y638","v":1.2},0,{"$f":"+AA638","v":1.2},0,{"$f":"+AC638","v":1.2},0,{"$f":"+AC638","v":1.2},0,1.2,{"$f":"+AD638","v":0},1.2,null,null,0,{"$f":"+AM638","v":0},0,61,0,{"$f":"+AO638","v":0},0,0,0,{"$f":"IF(AV636>AW$299,AV636,AW$299)","v":45.10240000000001},null,null,null,null,{"$f":"+AT674","v":0},1.52,0,1.52,0,1.52]
[null,null,null,null,{"$f":"+E642","v":0},{"$f":"+AV615","v":0},{"$f":"+E638","v":6.2},0,{"$f":"+G639","v":6.2},0,{"$f":"+I639","v":6.2},0,{"$f":"+K639","v":6.2},0,{"$f":"+M639","v":6.2},0,{"$f":"+O639","v":6.2},0,{"$f":"+Q639","v":6.2},0,{"$f":"+S639","v":6.2},0,{"$f":"+U639","v":6.2},{"$f":"+P639","v":0},{"$f":"+W639","v":6.2},{"$f":"+N639","v":0},{"$f":"+Y639","v":6.2},0,{"$f":"+AA639","v":6.2},0,{"$f":"+AC639","v":6.2},0,{"$f":"+AC639","v":6.2},0,6.2,{"$f":"+AD639","v":0},6.2,null,null,0,0,0,{"$f":"+AS639","v":0},0,0,0,{"$f":"+S662","v":0},{"$f":"#REF!-#REF!","v":{"$error":"#REF!"}},{"$f":"+AW640","v":6.0000000000000009},null,null,null,null,{"$f":"+AT675","v":0},0,{"$f":"+AD675","v":0},0,0,0]
[null,null,null,"Ukupni pritisak",null,"SQhi=",{"$f":"+G643","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+I643","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+K643","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+M643","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+O643","v":0},"SQhi=",{"$f":"+Q643","v":0},"SQhi=",{"$f":"+S643","v":0},"SQhi=",{"$f":"+U643","v":0},"SQhi=",{"$f":"+W643","v":0},"SQhi=",{"$f":"+Y643","v":0},"SQhi=",{"$f":"+AA643","v":0},"SQhi=",{"$f":"+AC643","v":0},"SQhi=",{"$f":"+AE643","v":0},"SQhi=",{"$f":"+AG643","v":0},"SQhi=",{"$f":"+AI643","v":0},"SQhi=",{"$f":"+AK643","v":0},null,null,"SQhi=",{"$f":"+AO643","v":1.4335999999999984},"SQhi=",{"$f":"+AQ643","v":{"$error":"#VALUE!"}},"SQhi=",{"$f":"+AS643","v":0},"SQhi=",0,{"$f":"BK459-BQ458","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$67","v":6.0000000000000009},null,null,null,null,0,1.2,0,{"$f":"+BE639","v":0},0,{"$f":"+AE678","v":1.2}]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G645","v":{"$error":"#VALUE!"}}," y=",{"$f":"+I645","v":{"$error":"#VALUE!"}}," y=",{"$f":"+K645","v":{"$error":"#VALUE!"}}," y=",{"$f":"+M645","v":{"$error":"#VALUE!"}}," y=",{"$f":"+O645","v":0}," y=",{"$f":"+Q645","v":0}," y=",{"$f":"+S645","v":0}," y=",{"$f":"+U645","v":0}," y=",{"$f":"+W645","v":0}," y=",{"$f":"+Y645","v":0}," y=",{"$f":"+AA645","v":0}," y=",{"$f":"+AC645","v":0}," y=",{"$f":"+AE645","v":0}," y=",{"$f":"+AG645","v":0}," y=",{"$f":"+AI645","v":0}," y=",{"$f":"+AK645","v":0},null,null," y=",{"$f":"+AO645","v":10.8032}," y=",{"$f":"+AQ645","v":{"$error":"#VALUE!"}}," y=",{"$f":"+AS645","v":0}," y=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$66","v":5.6800000000000006},null,null,null,null,0,6.2,0,{"$f":"+AK679","v":6.2},0,{"$f":"+AE679","v":6.2}]
[null,null,null,"krak za presjek III - III",null,"z=",{"$f":"+G641-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+I641-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+K641-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+M641-'Analiza i dimenzioniranje'!$E$52","v":{"$error":"#VALUE!"}},"z=",{"$f":"+O641-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+Q641-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+S641-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+U641-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z=",{"$f":"+W641-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+Y641-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AA641-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AC641-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AE641-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AG641-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AI641-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AK641-'Analiza i dimenzioniranje'!$E$52","v":-1.2},null,null,"z=",{"$f":"+AO641-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":10.3032},"z=",{"$f":"+AQ641-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#VALUE!"}},"z=",{"$f":"+AS641-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$65","v":5.36},null,null,null,null,"SQhi=",{"$f":"+BC645","v":0},"SQhi=",{"$f":"+BE645","v":0}]
[null,null,null,null,null,"F=",{"$f":"-0.5*(+\n (F622*G623-F623*G622)+\n(F623*G624-F624*G623)+\n(F624*G625-F625*G624)+\n(F625*G626-F626*G625)+\n(F626*G627-F627*G626)+\n(F627*G628-F628*G627)+\n(F628*G629-F629*G628)+\n(F629*G630-F630*G629)+\n(F630*G631-F631*G630)+\n(F631*G632-F632*G631)+\n(F632*G633-F633*G632)+\n(F633*G634-F634*G633)+\n(F634*G635-F635*G634)+\n(F635*G636-F636*G635)+\n(F636*G637-F637*G636)+\n(F637*G638-F638*G637)+\n(F638*G639-F639*G638))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (H622*I623-H623*I622)+\n(H623*I624-H624*I623)+\n(H624*I625-H625*I624)+\n(H625*I626-H626*I625)+\n(H626*I627-H627*I626)+\n(H627*I628-H628*I627)+\n(H628*I629-H629*I628)+\n(H629*I630-H630*I629)+\n(H630*I631-H631*I630)+\n(H631*I632-H632*I631)+\n(H632*I633-H633*I632)+\n(H633*I634-H634*I633)+\n(H634*I635-H635*I634)+\n(H635*I636-H636*I635)+\n(H636*I637-H637*I636)+\n(H637*I638-H638*I637)+\n(H638*I639-H639*I638))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((J620*K621-J621*K620)+(J621*K622-J622*K621)+\n (J622*K623-J623*K622)+\n(J623*K624-J624*K623)+\n(J624*K625-J625*K624)+\n(J625*K626-J626*K625)+\n(J626*K627-J627*K626)+\n(J627*K628-J628*K627)+\n(J628*K629-J629*K628)+\n(J629*K630-J630*K629)+\n(J630*K631-J631*K630)+\n(J631*K632-J632*K631)+\n(J632*K633-J633*K632)+\n(J633*K634-J634*K633)+\n(J634*K635-J635*K634)+\n(J635*K636-J636*K635)+\n(J636*K637-J637*K636)+\n(J637*K638-J638*K637)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (L622*M623-L623*M622)+\n(L623*M624-L624*M623)+\n(L624*M625-L625*M624)+\n(L625*M626-L626*M625)+\n(L626*M627-L627*M626)+\n(L627*M628-L628*M627)+\n(L628*M629-L629*M628)+\n(L629*M630-L630*M629)+\n(L630*M631-L631*M630)+\n(L631*M632-L632*M631)+\n(L632*M633-L633*M632)+\n(L633*M634-L634*M633)+\n(L634*M635-L635*M634)+\n(L635*M636-L636*M635)+\n(L636*M637-L637*M636)+\n(L637*M638-L638*M637)+\n(L638*M639-L639*M638))","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*(+\n (N622*O623-N623*O622)+\n(N623*O624-N624*O623)+\n(N624*O625-N625*O624)+\n(N625*O626-N626*O625)+\n(N626*O627-N627*O626)+\n(N627*O628-N628*O627)+\n(N628*O629-N629*O628)+\n(N629*O630-N630*O629)+\n(N630*O631-N631*O630)+\n(N631*O632-N632*O631)+\n(N632*O633-N633*O632)+\n(N633*O634-N634*O633)+\n(N634*O635-N635*O634)+\n(N635*O636-N636*O635)+\n(N636*O637-N637*O636)+\n(N637*O638-N638*O637)+\n(N638*O639-N639*O638))","v":0},"F=",{"$f":"-0.5*(+\n (P622*Q623-P623*Q622)+\n(P623*Q624-P624*Q623)+\n(P624*Q625-P625*Q624)+\n(P625*Q626-P626*Q625)+\n(P626*Q627-P627*Q626)+\n(P627*Q628-P628*Q627)+\n(P628*Q629-P629*Q628)+\n(P629*Q630-P630*Q629)+\n(P630*Q631-P631*Q630)+\n(P631*Q632-P632*Q631)+\n(P632*Q633-P633*Q632)+\n(P633*Q634-P634*Q633)+\n(P634*Q635-P635*Q634)+\n(P635*Q636-P636*Q635)+\n(P636*Q637-P637*Q636)+\n(P637*Q638-P638*Q637)+\n(P638*Q639-P639*Q638))","v":0},"F=",{"$f":"-0.5*((R620*S621-R621*S620)+(R621*S622-R622*S621)+\n (R622*S623-R623*S622)+\n(R623*S624-R624*S623)+\n(R624*S625-R625*S624)+\n(R625*S626-R626*S625)+\n(R626*S627-R627*S626)+\n(R627*S628-R628*S627)+\n(R628*S629-R629*S628)+\n(R629*S630-R630*S629)+\n(R630*S631-R631*S630)+\n(R631*S632-R632*S631)+\n(R632*S633-R633*S632)+\n(R633*S634-R634*S633)+\n(R634*S635-R635*S634)+\n(R635*S636-R636*S635)+\n(R636*S637-R637*S636)+\n(R637*S638-R638*S637)\n)","v":0},"F=",{"$f":"-0.5*(+\n (T622*U623-T623*U622)+\n(T623*U624-T624*U623)+\n(T624*U625-T625*U624)+\n(T625*U626-T626*U625)+\n(T626*U627-T627*U626)+\n(T627*U628-T628*U627)+\n(T628*U629-T629*U628)+\n(T629*U630-T630*U629)+\n(T630*U631-T631*U630)+\n(T631*U632-T632*U631)+\n(T632*U633-T633*U632)+\n(T633*U634-T634*U633)+\n(T634*U635-T635*U634)+\n(T635*U636-T636*U635)+\n(T636*U637-T637*U636)+\n(T637*U638-T638*U637)+\n(T638*U639-T639*U638))","v":0},"F=",{"$f":"-0.5*(+\n (V622*W623-V623*W622)+\n(V623*W624-V624*W623)+\n(V624*W625-V625*W624)+\n(V625*W626-V626*W625)+\n(V626*W627-V627*W626)+\n(V627*W628-V628*W627)+\n(V628*W629-V629*W628)+\n(V629*W630-V630*W629)+\n(V630*W631-V631*W630)+\n(V631*W632-V632*W631)+\n(V632*W633-V633*W632)+\n(V633*W634-V634*W633)+\n(V634*W635-V635*W634)+\n(V635*W636-V636*W635)+\n(V636*W637-V637*W636)+\n(V637*W638-V638*W637)+\n(V638*W639-V639*W638))","v":0},"F=",{"$f":"-0.5*(+\n (X622*Y623-X623*Y622)+\n(X623*Y624-X624*Y623)+\n(X624*Y625-X625*Y624)+\n(X625*Y626-X626*Y625)+\n(X626*Y627-X627*Y626)+\n(X627*Y628-X628*Y627)+\n(X628*Y629-X629*Y628)+\n(X629*Y630-X630*Y629)+\n(X630*Y631-X631*Y630)+\n(X631*Y632-X632*Y631)+\n(X632*Y633-X633*Y632)+\n(X633*Y634-X634*Y633)+\n(X634*Y635-X635*Y634)+\n(X635*Y636-X636*Y635)+\n(X636*Y637-X637*Y636)+\n(X637*Y638-X638*Y637)+\n(X638*Y639-X639*Y638))","v":0},"F=",{"$f":"-0.5*((Z620*AA621-Z621*AA620)+(Z621*AA622-Z622*AA621)+\n (Z622*AA623-Z623*AA622)+\n(Z623*AA624-Z624*AA623)+\n(Z624*AA625-Z625*AA624)+\n(Z625*AA626-Z626*AA625)+\n(Z626*AA627-Z627*AA626)+\n(Z627*AA628-Z628*AA627)+\n(Z628*AA629-Z629*AA628)+\n(Z629*AA630-Z630*AA629)+\n(Z630*AA631-Z631*AA630)+\n(Z631*AA632-Z632*AA631)+\n(Z632*AA633-Z633*AA632)+\n(Z633*AA634-Z634*AA633)+\n(Z634*AA635-Z635*AA634)+\n(Z635*AA636-Z636*AA635)+\n(Z636*AA637-Z637*AA636)+\n(Z637*AA638-Z638*AA637)\n)","v":0},"F=",{"$f":"-0.5*(+\n (AB622*AC623-AB623*AC622)+\n(AB623*AC624-AB624*AC623)+\n(AB624*AC625-AB625*AC624)+\n(AB625*AC626-AB626*AC625)+\n(AB626*AC627-AB627*AC626)+\n(AB627*AC628-AB628*AC627)+\n(AB628*AC629-AB629*AC628)+\n(AB629*AC630-AB630*AC629)+\n(AB630*AC631-AB631*AC630)+\n(AB631*AC632-AB632*AC631)+\n(AB632*AC633-AB633*AC632)+\n(AB633*AC634-AB634*AC633)+\n(AB634*AC635-AB635*AC634)+\n(AB635*AC636-AB636*AC635)+\n(AB636*AC637-AB637*AC636)+\n(AB637*AC638-AB638*AC637)+\n(AB638*AC639-AB639*AC638))","v":0},"F=",{"$f":"-0.5*(+\n (AD622*AE623-AD623*AE622)+\n(AD623*AE624-AD624*AE623)+\n(AD624*AE625-AD625*AE624)+\n(AD625*AE626-AD626*AE625)+\n(AD626*AE627-AD627*AE626)+\n(AD627*AE628-AD628*AE627)+\n(AD628*AE629-AD629*AE628)+\n(AD629*AE630-AD630*AE629)+\n(AD630*AE631-AD631*AE630)+\n(AD631*AE632-AD632*AE631)+\n(AD632*AE633-AD633*AE632)+\n(AD633*AE634-AD634*AE633)+\n(AD634*AE635-AD635*AE634)+\n(AD635*AE636-AD636*AE635)+\n(AD636*AE637-AD637*AE636)+\n(AD637*AE638-AD638*AE637)+\n(AD638*AE639-AD639*AE638))","v":0},"F=",{"$f":"-0.5*(+\n (AF622*AG623-AF623*AG622)+\n(AF623*AG624-AF624*AG623)+\n(AF624*AG625-AF625*AG624)+\n(AF625*AG626-AF626*AG625)+\n(AF626*AG627-AF627*AG626)+\n(AF627*AG628-AF628*AG627)+\n(AF628*AG629-AF629*AG628)+\n(AF629*AG630-AF630*AG629)+\n(AF630*AG631-AF631*AG630)+\n(AF631*AG632-AF632*AG631)+\n(AF632*AG633-AF633*AG632)+\n(AF633*AG634-AF634*AG633)+\n(AF634*AG635-AF635*AG634)+\n(AF635*AG636-AF636*AG635)+\n(AF636*AG637-AF637*AG636)+\n(AF637*AG638-AF638*AG637)+\n(AF638*AG639-AF639*AG638))","v":0},"F=",{"$f":"-0.5*((AH620*AI621-AH621*AI620)+(AH621*AI622-AH622*AI621)+\n (AH622*AI623-AH623*AI622)+\n(AH623*AI624-AH624*AI623)+\n(AH624*AI625-AH625*AI624)+\n(AH625*AI626-AH626*AI625)+\n(AH626*AI627-AH627*AI626)+\n(AH627*AI628-AH628*AI627)+\n(AH628*AI629-AH629*AI628)+\n(AH629*AI630-AH630*AI629)+\n(AH630*AI631-AH631*AI630)+\n(AH631*AI632-AH632*AI631)+\n(AH632*AI633-AH633*AI632)+\n(AH633*AI634-AH634*AI633)+\n(AH634*AI635-AH635*AI634)+\n(AH635*AI636-AH636*AI635)+\n(AH636*AI637-AH637*AI636)+\n(AH637*AI638-AH638*AI637)\n)","v":0},"F=",{"$f":"-0.5*(+\n (AJ622*AK623-AJ623*AK622)+\n(AJ623*AK624-AJ624*AK623)+\n(AJ624*AK625-AJ625*AK624)+\n(AJ625*AK626-AJ626*AK625)+\n(AJ626*AK627-AJ627*AK626)+\n(AJ627*AK628-AJ628*AK627)+\n(AJ628*AK629-AJ629*AK628)+\n(AJ629*AK630-AJ630*AK629)+\n(AJ630*AK631-AJ631*AK630)+\n(AJ631*AK632-AJ632*AK631)+\n(AJ632*AK633-AJ633*AK632)+\n(AJ633*AK634-AJ634*AK633)+\n(AJ634*AK635-AJ635*AK634)+\n(AJ635*AK636-AJ636*AK635)+\n(AJ636*AK637-AJ637*AK636)+\n(AJ637*AK638-AJ638*AK637)+\n(AJ638*AK639-AJ639*AK638))","v":0},null,null,"F=",{"$f":"-0.5*((AN620*AO621-AN621*AO620)+(AN621*AO622-AN622*AO621)+\n (AN622*AO623-AN623*AO622)+\n(AN623*AO624-AN624*AO623)+\n(AN624*AO625-AN625*AO624)+\n(AN625*AO626-AN626*AO625)+\n(AN626*AO627-AN627*AO626)+\n(AN627*AO628-AN628*AO627)+\n(AN628*AO629-AN629*AO628)+\n(AN629*AO630-AN630*AO629)+\n(AN630*AO631-AN631*AO630)+\n(AN631*AO632-AN632*AO631)+\n(AN632*AO633-AN633*AO632)+\n(AN633*AO634-AN634*AO633)+\n(AN634*AO635-AN635*AO634)+\n(AN635*AO636-AN636*AO635)+\n(AN636*AO637-AN637*AO636)+\n(AN637*AO638-AN638*AO637)\n)","v":1.4335999999999984},"F=",{"$f":"-0.5*((AP620*AQ621-AP621*AQ620)+(AP621*AQ622-AP622*AQ621)+\n (AP622*AQ623-AP623*AQ622)+\n(AP623*AQ624-AP624*AQ623)+\n(AP624*AQ625-AP625*AQ624)+\n(AP625*AQ626-AP626*AQ625)+\n(AP626*AQ627-AP627*AQ626)+\n(AP627*AQ628-AP628*AQ627)+\n(AP628*AQ629-AP629*AQ628)+\n(AP629*AQ630-AP630*AQ629)+\n(AP630*AQ631-AP631*AQ630)+\n(AP631*AQ632-AP632*AQ631)+\n(AP632*AQ633-AP633*AQ632)+\n(AP633*AQ634-AP634*AQ633)+\n(AP634*AQ635-AP635*AQ634)+\n(AP635*AQ636-AP636*AQ635)+\n(AP636*AQ637-AP637*AQ636)+\n(AP637*AQ638-AP638*AQ637)\n)","v":{"$error":"#VALUE!"}},"F=",{"$f":"-0.5*((AR620*AS621-AR621*AS620)+(AR621*AS622-AR622*AS621)+\n (AR622*AS623-AR623*AS622)+\n(AR623*AS624-AR624*AS623)+\n(AR624*AS625-AR625*AS624)+\n(AR625*AS626-AR626*AS625)+\n(AR626*AS627-AR627*AS626)+\n(AR627*AS628-AR628*AS627)+\n(AR628*AS629-AR629*AS628)+\n(AR629*AS630-AR630*AS629)+\n(AR630*AS631-AR631*AS630)+\n(AR631*AS632-AR632*AS631)+\n(AR632*AS633-AR633*AS632)+\n(AR633*AS634-AR634*AS633)+\n(AR634*AS635-AR635*AS634)+\n(AR635*AS636-AR636*AS635)+\n(AR636*AS637-AR637*AS636)+\n(AR637*AS638-AR638*AS637)\n)","v":0},"F=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$64","v":5.04},null,null,null,null," y=",{"$f":"+BC647","v":0}," y=",{"$f":"+BE647","v":0}]
[null,null,null,null,null,"x=",0.55000000000000004,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,null,null,"x=",0,"x=",0,"x=",0,"x=",0,0,{"$f":"'Analiza i dimenzioniranje'!$U$63","v":4.72},null,null,null,null,"z=",{"$f":"+BC643-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z=",{"$f":"+BE643-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5}]
[null,null,null,"y=",null,"y=",{"$f":"+IF(G643=0,0,-((F620*G621-F621*G620)*(G620+G621)+(F621*G622-F622*G621)*(G621+G622)+\n(F622*G623-F623*G622)*(G622+G623)+\n(F623*G624-F624*G623)*(G623+G624)+\n(F624*G625-F625*G624)*(G624+G625)+\n(F625*G626-F626*G625)*(G625+G626)+\n(F626*G627-F627*G626)*(G626+G627)+\n(F627*G628-F628*G627)*(G627+G628)+\n(F628*G629-F629*G628)*(G628+G629)+\n(F629*G630-F630*G629)*(G629+G630)+\n(F630*G631-F631*G630)*(G630+G631)+\n(F631*G632-F632*G631)*(G631+G632)+\n(F632*G633-F633*G632)*(G632+G633)+\n(F633*G634-F634*G633)*(G633+G634)+\n(F634*G635-F635*G634)*(G634+G635)+\n(F635*G636-F636*G635)*(G635+G636)+\n(F636*G637-F637*G636)*(G636+G637)+\n(F637*G638-F638*G637)*(G637+G638)+\n(F638*G639-F639*G638)*(G638+G639))/6/G643)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(I643=0,0,-((H620*I621-H621*I620)*(I620+I621)+(H621*I622-H622*I621)*(I621+I622)+\n(H622*I623-H623*I622)*(I622+I623)+\n(H623*I624-H624*I623)*(I623+I624)+\n(H624*I625-H625*I624)*(I624+I625)+\n(H625*I626-H626*I625)*(I625+I626)+\n(H626*I627-H627*I626)*(I626+I627)+\n(H627*I628-H628*I627)*(I627+I628)+\n(H628*I629-H629*I628)*(I628+I629)+\n(H629*I630-H630*I629)*(I629+I630)+\n(H630*I631-H631*I630)*(I630+I631)+\n(H631*I632-H632*I631)*(I631+I632)+\n(H632*I633-H633*I632)*(I632+I633)+\n(H633*I634-H634*I633)*(I633+I634)+\n(H634*I635-H635*I634)*(I634+I635)+\n(H635*I636-H636*I635)*(I635+I636)+\n(H636*I637-H637*I636)*(I636+I637)+\n(H637*I638-H638*I637)*(I637+I638)+\n(H638*I639-H639*I638)*(I638+I639))/6/I643)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(K643=0,0,-((J620*K621-J621*K620)*(K620+K621)+(J621*K622-J622*K621)*(K621+K622)+\n(J622*K623-J623*K622)*(K622+K623)+\n(J623*K624-J624*K623)*(K623+K624)+\n(J624*K625-J625*K624)*(K624+K625)+\n(J625*K626-J626*K625)*(K625+K626)+\n(J626*K627-J627*K626)*(K626+K627)+\n(J627*K628-J628*K627)*(K627+K628)+\n(J628*K629-J629*K628)*(K628+K629)+\n(J629*K630-J630*K629)*(K629+K630)+\n(J630*K631-J631*K630)*(K630+K631)+\n(J631*K632-J632*K631)*(K631+K632)+\n(J632*K633-J633*K632)*(K632+K633)+\n(J633*K634-J634*K633)*(K633+K634)+\n(J634*K635-J635*K634)*(K634+K635)+\n(J635*K636-J636*K635)*(K635+K636)+\n(J636*K637-J637*K636)*(K636+K637)+\n(J637*K638-J638*K637)*(K637+K638)+\n(J638*K639-J639*K638)*(K638+K639))/6/K643)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(M643=0,0,-((L620*M621-L621*M620)*(M620+M621)+(L621*M622-L622*M621)*(M621+M622)+\n(L622*M623-L623*M622)*(M622+M623)+\n(L623*M624-L624*M623)*(M623+M624)+\n(L624*M625-L625*M624)*(M624+M625)+\n(L625*M626-L626*M625)*(M625+M626)+\n(L626*M627-L627*M626)*(M626+M627)+\n(L627*M628-L628*M627)*(M627+M628)+\n(L628*M629-L629*M628)*(M628+M629)+\n(L629*M630-L630*M629)*(M629+M630)+\n(L630*M631-L631*M630)*(M630+M631)+\n(L631*M632-L632*M631)*(M631+M632)+\n(L632*M633-L633*M632)*(M632+M633)+\n(L633*M634-L634*M633)*(M633+M634)+\n(L634*M635-L635*M634)*(M634+M635)+\n(L635*M636-L636*M635)*(M635+M636)+\n(L636*M637-L637*M636)*(M636+M637)+\n(L637*M638-L638*M637)*(M637+M638)+\n(L638*M639-L639*M638)*(M638+M639))/6/M643)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(O643=0,0,-((N620*O621-N621*O620)*(O620+O621)+(N621*O622-N622*O621)*(O621+O622)+\n(N622*O623-N623*O622)*(O622+O623)+\n(N623*O624-N624*O623)*(O623+O624)+\n(N624*O625-N625*O624)*(O624+O625)+\n(N625*O626-N626*O625)*(O625+O626)+\n(N626*O627-N627*O626)*(O626+O627)+\n(N627*O628-N628*O627)*(O627+O628)+\n(N628*O629-N629*O628)*(O628+O629)+\n(N629*O630-N630*O629)*(O629+O630)+\n(N630*O631-N631*O630)*(O630+O631)+\n(N631*O632-N632*O631)*(O631+O632)+\n(N632*O633-N633*O632)*(O632+O633)+\n(N633*O634-N634*O633)*(O633+O634)+\n(N634*O635-N635*O634)*(O634+O635)+\n(N635*O636-N636*O635)*(O635+O636)+\n(N636*O637-N637*O636)*(O636+O637)+\n(N637*O638-N638*O637)*(O637+O638)+\n(N638*O639-N639*O638)*(O638+O639))/6/O643)","v":0},"y=",{"$f":"+IF(Q643=0,0,-((P620*Q621-P621*Q620)*(Q620+Q621)+(P621*Q622-P622*Q621)*(Q621+Q622)+\n(P622*Q623-P623*Q622)*(Q622+Q623)+\n(P623*Q624-P624*Q623)*(Q623+Q624)+\n(P624*Q625-P625*Q624)*(Q624+Q625)+\n(P625*Q626-P626*Q625)*(Q625+Q626)+\n(P626*Q627-P627*Q626)*(Q626+Q627)+\n(P627*Q628-P628*Q627)*(Q627+Q628)+\n(P628*Q629-P629*Q628)*(Q628+Q629)+\n(P629*Q630-P630*Q629)*(Q629+Q630)+\n(P630*Q631-P631*Q630)*(Q630+Q631)+\n(P631*Q632-P632*Q631)*(Q631+Q632)+\n(P632*Q633-P633*Q632)*(Q632+Q633)+\n(P633*Q634-P634*Q633)*(Q633+Q634)+\n(P634*Q635-P635*Q634)*(Q634+Q635)+\n(P635*Q636-P636*Q635)*(Q635+Q636)+\n(P636*Q637-P637*Q636)*(Q636+Q637)+\n(P637*Q638-P638*Q637)*(Q637+Q638)+\n(P638*Q639-P639*Q638)*(Q638+Q639))/6/Q643)","v":0},"y=",{"$f":"+IF(S643=0,0,-((R620*S621-R621*S620)*(S620+S621)+(R621*S622-R622*S621)*(S621+S622)+\n(R622*S623-R623*S622)*(S622+S623)+\n(R623*S624-R624*S623)*(S623+S624)+\n(R624*S625-R625*S624)*(S624+S625)+\n(R625*S626-R626*S625)*(S625+S626)+\n(R626*S627-R627*S626)*(S626+S627)+\n(R627*S628-R628*S627)*(S627+S628)+\n(R628*S629-R629*S628)*(S628+S629)+\n(R629*S630-R630*S629)*(S629+S630)+\n(R630*S631-R631*S630)*(S630+S631)+\n(R631*S632-R632*S631)*(S631+S632)+\n(R632*S633-R633*S632)*(S632+S633)+\n(R633*S634-R634*S633)*(S633+S634)+\n(R634*S635-R635*S634)*(S634+S635)+\n(R635*S636-R636*S635)*(S635+S636)+\n(R636*S637-R637*S636)*(S636+S637)+\n(R637*S638-R638*S637)*(S637+S638)+\n(R638*S639-R639*S638)*(S638+S639))/6/S643)","v":0},"y=",{"$f":"+IF(U643=0,0,-((T620*U621-T621*U620)*(U620+U621)+(T621*U622-T622*U621)*(U621+U622)+\n(T622*U623-T623*U622)*(U622+U623)+\n(T623*U624-T624*U623)*(U623+U624)+\n(T624*U625-T625*U624)*(U624+U625)+\n(T625*U626-T626*U625)*(U625+U626)+\n(T626*U627-T627*U626)*(U626+U627)+\n(T627*U628-T628*U627)*(U627+U628)+\n(T628*U629-T629*U628)*(U628+U629)+\n(T629*U630-T630*U629)*(U629+U630)+\n(T630*U631-T631*U630)*(U630+U631)+\n(T631*U632-T632*U631)*(U631+U632)+\n(T632*U633-T633*U632)*(U632+U633)+\n(T633*U634-T634*U633)*(U633+U634)+\n(T634*U635-T635*U634)*(U634+U635)+\n(T635*U636-T636*U635)*(U635+U636)+\n(T636*U637-T637*U636)*(U636+U637)+\n(T637*U638-T638*U637)*(U637+U638)+\n(T638*U639-T639*U638)*(U638+U639))/6/U643)","v":0},"y=",{"$f":"+IF(W643=0,0,-((V620*W621-V621*W620)*(W620+W621)+(V621*W622-V622*W621)*(W621+W622)+\n(V622*W623-V623*W622)*(W622+W623)+\n(V623*W624-V624*W623)*(W623+W624)+\n(V624*W625-V625*W624)*(W624+W625)+\n(V625*W626-V626*W625)*(W625+W626)+\n(V626*W627-V627*W626)*(W626+W627)+\n(V627*W628-V628*W627)*(W627+W628)+\n(V628*W629-V629*W628)*(W628+W629)+\n(V629*W630-V630*W629)*(W629+W630)+\n(V630*W631-V631*W630)*(W630+W631)+\n(V631*W632-V632*W631)*(W631+W632)+\n(V632*W633-V633*W632)*(W632+W633)+\n(V633*W634-V634*W633)*(W633+W634)+\n(V634*W635-V635*W634)*(W634+W635)+\n(V635*W636-V636*W635)*(W635+W636)+\n(V636*W637-V637*W636)*(W636+W637)+\n(V637*W638-V638*W637)*(W637+W638)+\n(V638*W639-V639*W638)*(W638+W639))/6/W643)","v":0},"y=",{"$f":"+IF(Y643=0,0,-((X620*Y621-X621*Y620)*(Y620+Y621)+(X621*Y622-X622*Y621)*(Y621+Y622)+\n(X622*Y623-X623*Y622)*(Y622+Y623)+\n(X623*Y624-X624*Y623)*(Y623+Y624)+\n(X624*Y625-X625*Y624)*(Y624+Y625)+\n(X625*Y626-X626*Y625)*(Y625+Y626)+\n(X626*Y627-X627*Y626)*(Y626+Y627)+\n(X627*Y628-X628*Y627)*(Y627+Y628)+\n(X628*Y629-X629*Y628)*(Y628+Y629)+\n(X629*Y630-X630*Y629)*(Y629+Y630)+\n(X630*Y631-X631*Y630)*(Y630+Y631)+\n(X631*Y632-X632*Y631)*(Y631+Y632)+\n(X632*Y633-X633*Y632)*(Y632+Y633)+\n(X633*Y634-X634*Y633)*(Y633+Y634)+\n(X634*Y635-X635*Y634)*(Y634+Y635)+\n(X635*Y636-X636*Y635)*(Y635+Y636)+\n(X636*Y637-X637*Y636)*(Y636+Y637)+\n(X637*Y638-X638*Y637)*(Y637+Y638)+\n(X638*Y639-X639*Y638)*(Y638+Y639))/6/Y643)","v":0},"y=",{"$f":"+IF(AA643=0,0,-((Z620*AA621-Z621*AA620)*(AA620+AA621)+(Z621*AA622-Z622*AA621)*(AA621+AA622)+\n(Z622*AA623-Z623*AA622)*(AA622+AA623)+\n(Z623*AA624-Z624*AA623)*(AA623+AA624)+\n(Z624*AA625-Z625*AA624)*(AA624+AA625)+\n(Z625*AA626-Z626*AA625)*(AA625+AA626)+\n(Z626*AA627-Z627*AA626)*(AA626+AA627)+\n(Z627*AA628-Z628*AA627)*(AA627+AA628)+\n(Z628*AA629-Z629*AA628)*(AA628+AA629)+\n(Z629*AA630-Z630*AA629)*(AA629+AA630)+\n(Z630*AA631-Z631*AA630)*(AA630+AA631)+\n(Z631*AA632-Z632*AA631)*(AA631+AA632)+\n(Z632*AA633-Z633*AA632)*(AA632+AA633)+\n(Z633*AA634-Z634*AA633)*(AA633+AA634)+\n(Z634*AA635-Z635*AA634)*(AA634+AA635)+\n(Z635*AA636-Z636*AA635)*(AA635+AA636)+\n(Z636*AA637-Z637*AA636)*(AA636+AA637)+\n(Z637*AA638-Z638*AA637)*(AA637+AA638)+\n(Z638*AA639-Z639*AA638)*(AA638+AA639))/6/AA643)","v":0},"y=",{"$f":"+IF(AC643=0,0,-((AB620*AC621-AB621*AC620)*(AC620+AC621)+(AB621*AC622-AB622*AC621)*(AC621+AC622)+\n(AB622*AC623-AB623*AC622)*(AC622+AC623)+\n(AB623*AC624-AB624*AC623)*(AC623+AC624)+\n(AB624*AC625-AB625*AC624)*(AC624+AC625)+\n(AB625*AC626-AB626*AC625)*(AC625+AC626)+\n(AB626*AC627-AB627*AC626)*(AC626+AC627)+\n(AB627*AC628-AB628*AC627)*(AC627+AC628)+\n(AB628*AC629-AB629*AC628)*(AC628+AC629)+\n(AB629*AC630-AB630*AC629)*(AC629+AC630)+\n(AB630*AC631-AB631*AC630)*(AC630+AC631)+\n(AB631*AC632-AB632*AC631)*(AC631+AC632)+\n(AB632*AC633-AB633*AC632)*(AC632+AC633)+\n(AB633*AC634-AB634*AC633)*(AC633+AC634)+\n(AB634*AC635-AB635*AC634)*(AC634+AC635)+\n(AB635*AC636-AB636*AC635)*(AC635+AC636)+\n(AB636*AC637-AB637*AC636)*(AC636+AC637)+\n(AB637*AC638-AB638*AC637)*(AC637+AC638)+\n(AB638*AC639-AB639*AC638)*(AC638+AC639))/6/AC643)","v":0},"y=",{"$f":"+IF(AE643=0,0,-((AD620*AE621-AD621*AE620)*(AE620+AE621)+(AD621*AE622-AD622*AE621)*(AE621+AE622)+\n(AD622*AE623-AD623*AE622)*(AE622+AE623)+\n(AD623*AE624-AD624*AE623)*(AE623+AE624)+\n(AD624*AE625-AD625*AE624)*(AE624+AE625)+\n(AD625*AE626-AD626*AE625)*(AE625+AE626)+\n(AD626*AE627-AD627*AE626)*(AE626+AE627)+\n(AD627*AE628-AD628*AE627)*(AE627+AE628)+\n(AD628*AE629-AD629*AE628)*(AE628+AE629)+\n(AD629*AE630-AD630*AE629)*(AE629+AE630)+\n(AD630*AE631-AD631*AE630)*(AE630+AE631)+\n(AD631*AE632-AD632*AE631)*(AE631+AE632)+\n(AD632*AE633-AD633*AE632)*(AE632+AE633)+\n(AD633*AE634-AD634*AE633)*(AE633+AE634)+\n(AD634*AE635-AD635*AE634)*(AE634+AE635)+\n(AD635*AE636-AD636*AE635)*(AE635+AE636)+\n(AD636*AE637-AD637*AE636)*(AE636+AE637)+\n(AD637*AE638-AD638*AE637)*(AE637+AE638)+\n(AD638*AE639-AD639*AE638)*(AE638+AE639))/6/AE643)","v":0},"y=",{"$f":"+IF(AG643=0,0,-((AF620*AG621-AF621*AG620)*(AG620+AG621)+(AF621*AG622-AF622*AG621)*(AG621+AG622)+\n(AF622*AG623-AF623*AG622)*(AG622+AG623)+\n(AF623*AG624-AF624*AG623)*(AG623+AG624)+\n(AF624*AG625-AF625*AG624)*(AG624+AG625)+\n(AF625*AG626-AF626*AG625)*(AG625+AG626)+\n(AF626*AG627-AF627*AG626)*(AG626+AG627)+\n(AF627*AG628-AF628*AG627)*(AG627+AG628)+\n(AF628*AG629-AF629*AG628)*(AG628+AG629)+\n(AF629*AG630-AF630*AG629)*(AG629+AG630)+\n(AF630*AG631-AF631*AG630)*(AG630+AG631)+\n(AF631*AG632-AF632*AG631)*(AG631+AG632)+\n(AF632*AG633-AF633*AG632)*(AG632+AG633)+\n(AF633*AG634-AF634*AG633)*(AG633+AG634)+\n(AF634*AG635-AF635*AG634)*(AG634+AG635)+\n(AF635*AG636-AF636*AG635)*(AG635+AG636)+\n(AF636*AG637-AF637*AG636)*(AG636+AG637)+\n(AF637*AG638-AF638*AG637)*(AG637+AG638)+\n(AF638*AG639-AF639*AG638)*(AG638+AG639))/6/AG643)","v":0},"y=",{"$f":"+IF(AI643=0,0,-((AH620*AI621-AH621*AI620)*(AI620+AI621)+(AH621*AI622-AH622*AI621)*(AI621+AI622)+\n(AH622*AI623-AH623*AI622)*(AI622+AI623)+\n(AH623*AI624-AH624*AI623)*(AI623+AI624)+\n(AH624*AI625-AH625*AI624)*(AI624+AI625)+\n(AH625*AI626-AH626*AI625)*(AI625+AI626)+\n(AH626*AI627-AH627*AI626)*(AI626+AI627)+\n(AH627*AI628-AH628*AI627)*(AI627+AI628)+\n(AH628*AI629-AH629*AI628)*(AI628+AI629)+\n(AH629*AI630-AH630*AI629)*(AI629+AI630)+\n(AH630*AI631-AH631*AI630)*(AI630+AI631)+\n(AH631*AI632-AH632*AI631)*(AI631+AI632)+\n(AH632*AI633-AH633*AI632)*(AI632+AI633)+\n(AH633*AI634-AH634*AI633)*(AI633+AI634)+\n(AH634*AI635-AH635*AI634)*(AI634+AI635)+\n(AH635*AI636-AH636*AI635)*(AI635+AI636)+\n(AH636*AI637-AH637*AI636)*(AI636+AI637)+\n(AH637*AI638-AH638*AI637)*(AI637+AI638)+\n(AH638*AI639-AH639*AI638)*(AI638+AI639))/6/AI643)","v":0},"y=",{"$f":"+IF(AK643=0,0,-((AJ620*AK621-AJ621*AK620)*(AK620+AK621)+(AJ621*AK622-AJ622*AK621)*(AK621+AK622)+\n(AJ622*AK623-AJ623*AK622)*(AK622+AK623)+\n(AJ623*AK624-AJ624*AK623)*(AK623+AK624)+\n(AJ624*AK625-AJ625*AK624)*(AK624+AK625)+\n(AJ625*AK626-AJ626*AK625)*(AK625+AK626)+\n(AJ626*AK627-AJ627*AK626)*(AK626+AK627)+\n(AJ627*AK628-AJ628*AK627)*(AK627+AK628)+\n(AJ628*AK629-AJ629*AK628)*(AK628+AK629)+\n(AJ629*AK630-AJ630*AK629)*(AK629+AK630)+\n(AJ630*AK631-AJ631*AK630)*(AK630+AK631)+\n(AJ631*AK632-AJ632*AK631)*(AK631+AK632)+\n(AJ632*AK633-AJ633*AK632)*(AK632+AK633)+\n(AJ633*AK634-AJ634*AK633)*(AK633+AK634)+\n(AJ634*AK635-AJ635*AK634)*(AK634+AK635)+\n(AJ635*AK636-AJ636*AK635)*(AK635+AK636)+\n(AJ636*AK637-AJ637*AK636)*(AK636+AK637)+\n(AJ637*AK638-AJ638*AK637)*(AK637+AK638)+\n(AJ638*AK639-AJ639*AK638)*(AK638+AK639))/6/AK643)","v":0},null,null,"y=",{"$f":"+IF(AO643=0,0,-((AN620*AO621-AN621*AO620)*(AO620+AO621)+(AN621*AO622-AN622*AO621)*(AO621+AO622)+\n(AN622*AO623-AN623*AO622)*(AO622+AO623)+\n(AN623*AO624-AN624*AO623)*(AO623+AO624)+\n(AN624*AO625-AN625*AO624)*(AO624+AO625)+\n(AN625*AO626-AN626*AO625)*(AO625+AO626)+\n(AN626*AO627-AN627*AO626)*(AO626+AO627)+\n(AN627*AO628-AN628*AO627)*(AO627+AO628)+\n(AN628*AO629-AN629*AO628)*(AO628+AO629)+\n(AN629*AO630-AN630*AO629)*(AO629+AO630)+\n(AN630*AO631-AN631*AO630)*(AO630+AO631)+\n(AN631*AO632-AN632*AO631)*(AO631+AO632)+\n(AN632*AO633-AN633*AO632)*(AO632+AO633)+\n(AN633*AO634-AN634*AO633)*(AO633+AO634)+\n(AN634*AO635-AN635*AO634)*(AO634+AO635)+\n(AN635*AO636-AN636*AO635)*(AO635+AO636)+\n(AN636*AO637-AN637*AO636)*(AO636+AO637)+\n(AN637*AO638-AN638*AO637)*(AO637+AO638)+\n(AN638*AO639-AN639*AO638)*(AO638+AO639))/6/AO643)","v":10.8032},"y=",{"$f":"+IF(AQ643=0,0,-((AP620*AQ621-AP621*AQ620)*(AQ620+AQ621)+(AP621*AQ622-AP622*AQ621)*(AQ621+AQ622)+\n(AP622*AQ623-AP623*AQ622)*(AQ622+AQ623)+\n(AP623*AQ624-AP624*AQ623)*(AQ623+AQ624)+\n(AP624*AQ625-AP625*AQ624)*(AQ624+AQ625)+\n(AP625*AQ626-AP626*AQ625)*(AQ625+AQ626)+\n(AP626*AQ627-AP627*AQ626)*(AQ626+AQ627)+\n(AP627*AQ628-AP628*AQ627)*(AQ627+AQ628)+\n(AP628*AQ629-AP629*AQ628)*(AQ628+AQ629)+\n(AP629*AQ630-AP630*AQ629)*(AQ629+AQ630)+\n(AP630*AQ631-AP631*AQ630)*(AQ630+AQ631)+\n(AP631*AQ632-AP632*AQ631)*(AQ631+AQ632)+\n(AP632*AQ633-AP633*AQ632)*(AQ632+AQ633)+\n(AP633*AQ634-AP634*AQ633)*(AQ633+AQ634)+\n(AP634*AQ635-AP635*AQ634)*(AQ634+AQ635)+\n(AP635*AQ636-AP636*AQ635)*(AQ635+AQ636)+\n(AP636*AQ637-AP637*AQ636)*(AQ636+AQ637)+\n(AP637*AQ638-AP638*AQ637)*(AQ637+AQ638)+\n(AP638*AQ639-AP639*AQ638)*(AQ638+AQ639))/6/AQ643)","v":{"$error":"#VALUE!"}},"y=",{"$f":"+IF(AS643=0,0,-((AR620*AS621-AR621*AS620)*(AS620+AS621)+(AR621*AS622-AR622*AS621)*(AS621+AS622)+\n(AR622*AS623-AR623*AS622)*(AS622+AS623)+\n(AR623*AS624-AR624*AS623)*(AS623+AS624)+\n(AR624*AS625-AR625*AS624)*(AS624+AS625)+\n(AR625*AS626-AR626*AS625)*(AS625+AS626)+\n(AR626*AS627-AR627*AS626)*(AS626+AS627)+\n(AR627*AS628-AR628*AS627)*(AS627+AS628)+\n(AR628*AS629-AR629*AS628)*(AS628+AS629)+\n(AR629*AS630-AR630*AS629)*(AS629+AS630)+\n(AR630*AS631-AR631*AS630)*(AS630+AS631)+\n(AR631*AS632-AR632*AS631)*(AS631+AS632)+\n(AR632*AS633-AR633*AS632)*(AS632+AS633)+\n(AR633*AS634-AR634*AS633)*(AS633+AS634)+\n(AR634*AS635-AR635*AS634)*(AS634+AS635)+\n(AR635*AS636-AR636*AS635)*(AS635+AS636)+\n(AR636*AS637-AR637*AS636)*(AS636+AS637)+\n(AR637*AS638-AR638*AS637)*(AS637+AS638)+\n(AR638*AS639-AR639*AS638)*(AS638+AS639))/6/AS643)","v":0},"y=",0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$62","v":4.4000000000000004},null,null,null,null,"F=",{"$f":"-0.5*((BB622*BC623-BB623*BC622)+(BB623*BC624-BB624*BC623)+\n (BB624*BC625-BB625*BC624)+\n(BB625*BC626-BB626*BC625)+\n(BB626*BC627-BB627*BC626)+\n(BB627*BC628-BB628*BC627)+\n(BB628*BC629-BB629*BC628)+\n(BB629*BC630-BB630*BC629)+\n(BB630*BC631-BB631*BC630)+\n(BB631*BC632-BB632*BC631)+\n(BB632*BC633-BB633*BC632)+\n(BB633*BC634-BB634*BC633)+\n(BB634*BC635-BB635*BC634)+\n(BB635*BC636-BB636*BC635)+\n(BB636*BC637-BB637*BC636)+\n(BB637*BC638-BB638*BC637)+\n(BB638*BC639-BB639*BC638)+\n(BB639*BC640-BB640*BC639)\n)","v":0},"F=",{"$f":"-0.5*((BD622*BE623-BD623*BE622)+(BD623*BE624-BD624*BE623)+\n (BD624*BE625-BD625*BE624)+\n(BD625*BE626-BD626*BE625)+\n(BD626*BE627-BD627*BE626)+\n(BD627*BE628-BD628*BE627)+\n(BD628*BE629-BD629*BE628)+\n(BD629*BE630-BD630*BE629)+\n(BD630*BE631-BD631*BE630)+\n(BD631*BE632-BD632*BE631)+\n(BD632*BE633-BD633*BE632)+\n(BD633*BE634-BD634*BE633)+\n(BD634*BE635-BD635*BE634)+\n(BD635*BE636-BD636*BE635)+\n(BD636*BE637-BD637*BE636)+\n(BD637*BE638-BD638*BE637)+\n(BD638*BE639-BD639*BE638)+\n(BD639*BE640-BD640*BE639)\n)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$61","v":4.08},null,null,null,null,"x=",0,"x=",0]
[null,"PRORAČUN HORIZONTALNIH PRITISAKA NA ZID ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BK466-BQ465","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$60","v":3.76},null,null,null,null,"y=",{"$f":"+IF(BC645=0,0,-((BB622*BC623-BB623*BC622)*(BC622+BC623)+(BB623*BC624-BB624*BC623)*(BC623+BC624)+\n(BB624*BC625-BB625*BC624)*(BC624+BC625)+\n(BB625*BC626-BB626*BC625)*(BC625+BC626)+\n(BB626*BC627-BB627*BC626)*(BC626+BC627)+\n(BB627*BC628-BB628*BC627)*(BC627+BC628)+\n(BB628*BC629-BB629*BC628)*(BC628+BC629)+\n(BB629*BC630-BB630*BC629)*(BC629+BC630)+\n(BB630*BC631-BB631*BC630)*(BC630+BC631)+\n(BB631*BC632-BB632*BC631)*(BC631+BC632)+\n(BB632*BC633-BB633*BC632)*(BC632+BC633)+\n(BB633*BC634-BB634*BC633)*(BC633+BC634)+\n(BB634*BC635-BB635*BC634)*(BC634+BC635)+\n(BB635*BC636-BB636*BC635)*(BC635+BC636)+\n(BB636*BC637-BB637*BC636)*(BC636+BC637)+\n(BB637*BC638-BB638*BC637)*(BC637+BC638)+\n(BB638*BC639-BB639*BC638)*(BC638+BC639)+\n(BB639*BC640-BB640*BC639)*(BC639+BC640)+\n(BB640*BC641-BB641*BC640)*(BC640+BC641))/6/BC645)","v":0},"y=",{"$f":"+IF(BE645=0,0,-((BD622*BE623-BD623*BE622)*(BE622+BE623)+(BD623*BE624-BD624*BE623)*(BE623+BE624)+\n(BD624*BE625-BD625*BE624)*(BE624+BE625)+\n(BD625*BE626-BD626*BE625)*(BE625+BE626)+\n(BD626*BE627-BD627*BE626)*(BE626+BE627)+\n(BD627*BE628-BD628*BE627)*(BE627+BE628)+\n(BD628*BE629-BD629*BE628)*(BE628+BE629)+\n(BD629*BE630-BD630*BE629)*(BE629+BE630)+\n(BD630*BE631-BD631*BE630)*(BE630+BE631)+\n(BD631*BE632-BD632*BE631)*(BE631+BE632)+\n(BD632*BE633-BD633*BE632)*(BE632+BE633)+\n(BD633*BE634-BD634*BE633)*(BE633+BE634)+\n(BD634*BE635-BD635*BE634)*(BE634+BE635)+\n(BD635*BE636-BD636*BE635)*(BE635+BE636)+\n(BD636*BE637-BD637*BE636)*(BE636+BE637)+\n(BD637*BE638-BD638*BE637)*(BE637+BE638)+\n(BD638*BE639-BD639*BE638)*(BE638+BE639)+\n(BD639*BE640-BD640*BE639)*(BE639+BE640)+\n(BD640*BE641-BD641*BE640)*(BE640+BE641))/6/BE645)","v":0}]
[null,"OPTEREĆENJE TEMELJEM",null,null,null,null,null,null,null," (TERZAGHY)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$59","v":3.44}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$58","v":3.14}]
[null,"KONTINUIRANO OPTEREĆENJE",null,"P - D=",{"$f":"IF('Analiza i dimenzioniranje'!$E$28-I650<=0,0,+'Analiza i dimenzioniranje'!$E$28-I650)","v":{"$error":"#VALUE!"}},"kN/m2","raster. iskopom   D=y*Df =",null,{"$f":"+'Analiza i dimenzioniranje'!$D$16*('Analiza i dimenzioniranje'!$E$48+'Analiza i dimenzioniranje'!$D$20-D656)","v":{"$error":"#VALUE!"}},"kN/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$57","v":2.8}]
[null," visina zida i temelja",null,"H =",{"$f":"+E571","v":{"$error":"#VALUE!"}},"m",{"$f":"E655","v":6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$f":"+'Analiza i dimenzioniranje'!$U$56","v":2.48}]
[null,"visina opterećenja iznad vrha zida",null,"h =",{"$f":"+E572","v":-1},"m",{"$f":"SQRT(E655^2+E654^2)","v":6.7082039324993694},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BK471-BQ470","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$55","v":2.16}]
[null,"širina temelja",null,"b =",{"$f":"+E573","v":1},"m   ",{"$f":"E654+E653","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.52,{"$f":"BK472-BQ471","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$54","v":1.84}]
[null,"udaljenost temelja od zida",null,"D =",{"$f":"+E574","v":3},"m    ",null,null,null,"visina tla iznad temelja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BK473-BQ472","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$53","v":1.52}]
[null,"1/2 dužine temelja",null,"L/2=a=",{"$f":"+E575","v":6},"m",{"$f":"SQRT(G651^2+G653^2)","v":7.2111025509279782},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,0,{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
["DNO TEMELJA NA VISINI","PRESJEK NA Visini ",null,{"$f":"ROUND('Analiza i dimenzioniranje'!U53,2)","v":1.52},null,"Presjek III - III",null,"Presjek VI",null,"Presjek VII-VII",null,"Presjek VIII-VIII",null,"Presjek IX-IX",null,"Presjek X-X",null,"Presjek XI-XI",null,"Presjek XII-XII",null,"Presjek XIII-XIII",null,"Presjek XIV-XIV",null,"Presjek XV-XV",null,"PresjekXVI-XVI",null,"Presjek XVII-XVII",null,"Presjek XVIII-XVIII",null,"Presjek XIX-XIX",null,"Presjek XX-XX",null,null,null,null,null,null,null,null,null,null,6.2,{"$f":"+IF(AW657>=AW$299,0,BK475-BQ474)","v":0},{"$f":"+'Analiza i dimenzioniranje'!$U$52","v":1.2}]
[null,null,null,null,null,"Visina djelovanja","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja ","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja",null,null,"sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2","Visina djelovanja","sb1-sb2",{"$f":"+AU660","v":0},"SQhi=",6.2]
[null,null,null,{"$f":"+F659","v":0},{"$f":"+D658-E656","v":0},"III",{"$f":"+D656","v":1.52},"IV",{"$f":"+G658","v":1.52},"VII",{"$f":"+G658","v":1.52},"VIII",{"$f":"'Analiza i dimenzioniranje'!U408","v":0},"IX",{"$f":"+G658","v":1.52},"X",{"$f":"+'Analiza i dimenzioniranje'!O312","v":0},"XI",{"$f":"+G658","v":1.52},"XII",{"$f":"+'Analiza i dimenzioniranje'!S312","v":0},"XIII",{"$f":"+G658","v":1.52},"XIV",{"$f":"+W658","v":1.52},"XV",{"$f":"+G658","v":1.52},"XVI",{"$f":"+I658","v":1.52},"XVII",{"$f":"+AC658","v":1.52},"XVIII",{"$f":"+AC658","v":1.52},"XIX",{"$f":"+AE658","v":1.52},"XX",{"$f":"+AG658","v":1.52},null,null,"X",{"$f":"+'Analiza i dimenzioniranje'!U405","v":"x"},"XIV",{"$f":"'Analiza i dimenzioniranje'!U404","v":3.37},"XII",{"$f":"+'Analiza i dimenzioniranje'!U403","v":"y"},"XVI",{"$f":"+AU662","v":0}," y=",{"$f":"+AW661","v":{"$error":"#REF!"}}]
[null,null,null,0,{"$f":"IF(D658>E$296,D658,E$296)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+J659","v":0},{"$f":"+AN659-AO658","v":{"$error":"#VALUE!"}},{"$f":"+AN659","v":0},{"$f":"+'Analiza i dimenzioniranje'!U404","v":3.37},{"$f":"+AP659","v":0},{"$f":"+AR659-AS658","v":{"$error":"#VALUE!"}},{"$f":"+Z659","v":0},{"$f":"+AU658-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z=",{"$f":"+AW663","v":{"$error":"#REF!"}}]
[null,null,null,0,{"$f":"IF(AW639>G$298,0,AW639)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+AM660","v":0},{"$f":"+AL660","v":0},{"$f":"+AO660","v":0},0,{"$f":"+AO660","v":0},0,{"$f":"-0.5*((AT660*AU638-AT661*AU637)+(AT661*AU639-AT662*AU638)+\n (AT662*AU640-AT663*AU639)+\n(AT663*AU641-AT664*AU640)+\n(AT664*AU642-AT665*AU641)+\n(AT665*AU643-AT666*AU642)+\n(AT666*AU644-AT667*AU643)+\n(AT667*AU645-AT668*AU644)+\n(AT668*AU646-AT669*AU645)+\n(AT669*AU647-AT670*AU646)+\n(AT670*AU648-AT671*AU647)+\n(AT671*AU649-AT672*AU648)+\n(AT672*AU650-AT673*AU649)+\n(AT673*AU651-AT674*AU650)+\n(AT674*AU652-AT675*AU651)+\n(AT675*AU653-AT676*AU652)+\n(AT676*AU654-AT677*AU653)+\n(AT677*AU655-AT678*AU654)\n)","v":0},"F=",{"$f":"+AW659-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#REF!"}}]
[null,null,null,0,{"$f":"+AW640","v":6.0000000000000009},0,0,{"$f":"+F661","v":0},{"$f":"+G661","v":0},0,{"$f":"+E660","v":0},0,{"$f":"+E660","v":0},0,{"$f":"+M661","v":0},0,{"$f":"+O661","v":0},0,{"$f":"+AS661","v":0},0,{"$f":"+S661","v":0},0,{"$f":"+AS661","v":0},0,{"$f":"+W661","v":0},0,{"$f":"+S661","v":0},0,{"$f":"+AA661","v":0},0,{"$f":"+AU638","v":0},0,{"$f":"+AU638","v":0},0,{"$f":"+AG661","v":0},{"$f":"+AD661","v":0},{"$f":"+AG661","v":0},null,null,0,0,0,0,0,0,0,0,"x=",{"$f":"-0.5*((AV637*AW639-AV638*AW638)+(AV638*AW640-AV639*AW639)+\n (AV639*AW641-AV640*AW640)+\n(AV640*AW642-AV641*AW641)+\n(AV641*AW643-AV642*AW642)+\n(AV642*AW644-AV643*AW643)+\n(AV643*AW645-AV644*AW644)+\n(AV644*AW646-AV645*AW645)+\n(AV645*AW647-AV646*AW646)+\n(AV646*AW648-AV647*AW647)+\n(AV647*AW649-AV648*AW648)+\n(AV648*AW650-AV649*AW649)+\n(AV649*AW651-AV650*AW650)+\n(AV650*AW652-AV651*AW651)+\n(AV651*AW653-AV652*AW652)+\n(AV652*AW654-AV653*AW653)+\n(AV653*AW655-AV654*AW654)+\n(AV654*AW656-AV655*AW655)\n)","v":{"$error":"#REF!"}}]
[null,null,null,0,{"$f":"IF(AW641>G$298,0,AW641)","v":0},0,0,0,{"$f":"+G662","v":0},0,6.0000000000000009,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU639","v":0},0,0,0,0,0,0,null,null,0,0,0,0,0,0,0,{"$f":"+IF(AU660=0,0,-((AT660*AU638-AT661*AU637)*(AU637+AU638)+(AT661*AU639-AT662*AU638)*(AU638+AU639)+\n(AT662*AU640-AT663*AU639)*(AU639+AU640)+\n(AT663*AU641-AT664*AU640)*(AU640+AU641)+\n(AT664*AU642-AT665*AU641)*(AU641+AU642)+\n(AT665*AU643-AT666*AU642)*(AU642+AU643)+\n(AT666*AU644-AT667*AU643)*(AU643+AU644)+\n(AT667*AU645-AT668*AU644)*(AU644+AU645)+\n(AT668*AU646-AT669*AU645)*(AU645+AU646)+\n(AT669*AU647-AT670*AU646)*(AU646+AU647)+\n(AT670*AU648-AT671*AU647)*(AU647+AU648)+\n(AT671*AU649-AT672*AU648)*(AU648+AU649)+\n(AT672*AU650-AT673*AU649)*(AU649+AU650)+\n(AT673*AU651-AT674*AU650)*(AU650+AU651)+\n(AT674*AU652-AT675*AU651)*(AU651+AU652)+\n(AT675*AU653-AT676*AU652)*(AU652+AU653)+\n(AT676*AU654-AT677*AU653)*(AU653+AU654)+\n(AT677*AU655-AT678*AU654)*(AU654+AU655)+\n(AT678*AU656-AT679*AU655)*(AU655+AU656))/6/AU660)","v":0},"y=",0]
[null,null,null,{"$f":"+AV639","v":{"$error":"#REF!"}},0,0,0,{"$f":"+F663","v":0},0,{"$f":"+F661","v":0},0,{"$f":"+D660","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU640","v":0},0,0,0,0,0,0,null,null,0,0,0,0,0,0,0,null,null,{"$f":"+IF(AW661=0,0,-((AV637*AW639-AV638*AW638)*(AW638+AW639)+(AV638*AW640-AV639*AW639)*(AW639+AW640)+\n(AV639*AW641-AV640*AW640)*(AW640+AW641)+\n(AV640*AW642-AV641*AW641)*(AW641+AW642)+\n(AV641*AW643-AV642*AW642)*(AW642+AW643)+\n(AV642*AW644-AV643*AW643)*(AW643+AW644)+\n(AV643*AW645-AV644*AW644)*(AW644+AW645)+\n(AV644*AW646-AV645*AW645)*(AW645+AW646)+\n(AV645*AW647-AV646*AW646)*(AW646+AW647)+\n(AV646*AW648-AV647*AW647)*(AW647+AW648)+\n(AV647*AW649-AV648*AW648)*(AW648+AW649)+\n(AV648*AW650-AV649*AW649)*(AW649+AW650)+\n(AV649*AW651-AV650*AW650)*(AW650+AW651)+\n(AV650*AW652-AV651*AW651)*(AW651+AW652)+\n(AV651*AW653-AV652*AW652)*(AW652+AW653)+\n(AV652*AW654-AV653*AW653)*(AW653+AW654)+\n(AV653*AW655-AV654*AW654)*(AW654+AW655)+\n(AV654*AW656-AV655*AW655)*(AW655+AW656)+\n(AV655*AW657-AV656*AW656)*(AW656+AW657))/6/AW661)","v":{"$error":"#REF!"}}]
[null,null,null,0,0,0,0,0,0,{"$f":"+F662","v":0},0,{"$f":"+D661","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU641","v":0},0,0,0,0,0,0,null,null,0,0,0,0,0,0,0]
[null,null,null,0,0,0,0,0,0,0,0,{"$f":"+D662","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AU642","v":0},0,0,0,0,0,0,null,null,0,0,0,0,0,0,0]
[null,null,null,0,4.4000000000000004,0,0,0,0,0,0,{"$f":"+D459","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+AE665","v":0},0,0,0,0,0,0,null,null,0,0,0,0,0,0,0]
[null,null,null,0,4.08,0,0,0,0,0,4.4000000000000004,{"$f":"+D664","v":0},0,{"$f":"+J665","v":0},0,{"$f":"+L665","v":0},0,0,0,{"$f":"+P665","v":0},0,0,0,{"$f":"+T665","v":0},0,0,0,{"$f":"+X665","v":0},0,0,{"$f":"+AU644","v":0},0,0,0,0,0,0,null,null,0,0,0,0,0,0,0]
[null,null,null,0,3.76,0,0,0,0,0,4.08,0,0,{"$f":"+J666","v":0},0,{"$f":"+L666","v":0},0,0,0,{"$f":"+P666","v":0},0,0,0,{"$f":"+T666","v":0},0,0,{"$f":"+AA667","v":0},{"$f":"+X666","v":0},0,0,0,0,0,0,0,0,0,null,null,{"$f":"+AL666","v":0},0,0,0,0,0,0]
[null,null,null,"+",3.44,0,0,0,{"$f":"+G669","v":0},{"$f":"+F669","v":0},3.76,{"$f":"+D666","v":0},0,{"$f":"+J667","v":0},0,{"$f":"+N669","v":0},{"$f":"+O669","v":0},0,0,{"$f":"+R669","v":0},{"$f":"+S669","v":0},0,0,{"$f":"+V669","v":0},0,0,{"$f":"+S669","v":0},{"$f":"+Z669","v":0},{"$f":"+AA669","v":0},0,0,0,0,0,0,0,0,null,null,0,0,{"$f":"+#REF!","v":{"$error":"#REF!"}},0,0,0,0]
[null,null,null,{"$f":"+AV646","v":0},3.14,0,0,0,{"$f":"+G670","v":0},0,3.44,{"$f":"+J670","v":0},0,{"$f":"+L670","v":0},{"$f":"+M670","v":0},{"$f":"+N670","v":0},{"$f":"+O670","v":0},{"$f":"+P670","v":0},{"$f":"+Q670","v":0},{"$f":"+R670","v":0},{"$f":"+S670","v":0},{"$f":"+T670","v":0},{"$f":"+U670","v":0},{"$f":"+V670","v":0},0,0,0,{"$f":"+Z670","v":0},{"$f":"+AA670","v":0},0,0,{"$f":"+AD670","v":0},{"$f":"+AE670","v":0},{"$f":"+AF670","v":0},0,0,{"$f":"+BC632","v":0},null,null,0,0,{"$f":"+D458","v":0},0,{"$f":"+AL666","v":0},0,0]
[null,null,null,{"$f":"+AV647","v":0},2.8,0,0,0,{"$f":"+G671","v":0},0,3.14,{"$f":"+J671","v":0},0,{"$f":"+J671","v":0},{"$f":"+M671","v":0},{"$f":"+L671","v":0},{"$f":"+O671","v":0},{"$f":"+N671","v":0},{"$f":"+Q671","v":0},0,{"$f":"+S671","v":0},{"$f":"+T671","v":0},{"$f":"+Y671","v":0},{"$f":"+B665","v":0},{"$f":"+U671","v":0},{"$f":"+B665","v":0},0,{"$f":"+Z671","v":0},{"$f":"+U671","v":0},{"$f":"+AB671","v":0},0,{"$f":"+AB671","v":0},{"$f":"+AC671","v":0},{"$f":"+AF671","v":0},0,0,0,null,null,0,0,0,0,0,0,0]
[null,null,null,{"$f":"+AV648","v":0},2.48,{"$f":"+E676","v":0},0,0,0,0,2.8,{"$f":"+J672","v":0},0,{"$f":"+J672","v":0},{"$f":"+M672","v":0},{"$f":"+L672","v":0},{"$f":"+O672","v":0},0,{"$f":"+S671","v":0},0,0,0,{"$f":"+AS672","v":0},0,0,0,0,{"$f":"+Z672","v":0},0,{"$f":"+AB672","v":0},0,{"$f":"+AB672","v":0},0,{"$f":"+AF672","v":0},0,0,0,null,null,0,0,0,0,0,0,0]
[null,null,null,null,2.16,{"$f":"+E676","v":0},0,0,0,0,2.48,0,0,{"$f":"+J673","v":0},{"$f":"+M673","v":0},0,{"$f":"+O673","v":0},0,{"$f":"+Q673","v":0},0,{"$f":"+S673","v":0},0,{"$f":"+U673","v":0},0,{"$f":"+W673","v":0},0,0,0,0,0,0,0,0,0,0,0,{"$f":"+BC635","v":0},null,null,0,0,0,0,0,0,0]
[null,null,null,null,1.84,{"$f":"+E676","v":0},0,0,0,0,2.16,0,0,0,{"$f":"+O673","v":0},0,0,0,{"$f":"+AS674","v":0},0,0,0,{"$f":"+AS674","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"+BC636","v":0},null,null,0,0,0,0,0,0,{"$f":"+R673","v":0}]
[null,null,null,null,1.52,{"$f":"+E676","v":0},0,0,0,0,1.84,0,0,0,{"$f":"+M675","v":0},0,{"$f":"+O675","v":0},0,{"$f":"+Q675","v":0},0,{"$f":"+S675","v":0},0,{"$f":"+U675","v":0},0,{"$f":"+W675","v":0},0,{"$f":"+Y675","v":0},0,0,0,0,0,0,0,0,0,{"$f":"+BC637","v":0},null,null,0,0,{"$error":"#REF!"},0,0,0,{"$f":"+R674","v":0}]
[null,null,null,{"$f":"IF(AW655>G$298,0,AW655)","v":1.2},{"$f":"+D635","v":0},{"$f":"+E676","v":0},{"$f":"+AW654","v":1.52},0,1.52,0,{"$f":"+I676","v":1.52},0,{"$f":"+K676","v":1.52},0,{"$f":"+M676","v":1.52},0,{"$f":"+O676","v":1.52},0,{"$f":"+Q676","v":1.52},0,{"$f":"+S676","v":1.52},0,{"$f":"+U676","v":1.52},0,{"$f":"+W676","v":1.52},0,{"$f":"+S676","v":1.52},0,1.52,0,{"$f":"+AE675","v":0},0,1.52,0,1.52,0,1.52,null,null,0,0,0,0,0,0,{"$f":"+R675","v":0}]
[null,null,null,{"$f":"+AW656","v":1.2},{"$f":"+D636","v":0.32},{"$f":"+E677","v":0.32},1.2,0,{"$f":"+G677","v":1.2},{"$f":"+H677","v":0},{"$f":"+D676","v":1.2},0,{"$f":"+N677","v":0},0,{"$f":"+AM677","v":0},0,0,0,{"$f":"+AS677","v":0},0,0,0,{"$f":"+AS677","v":0},0,0,0,{"$f":"+S677","v":0},0,0,0,{"$f":"+AU654","v":0},0,0,0,0,0,0,null,null,0,0,{"$f":"+D471","v":0},0,0,0,{"$f":"+R676","v":0}]
[null,null,null,{"$f":"+AW657","v":6.2},{"$f":"+D637","v":0.64},0,{"$f":"+D677","v":1.2},0,{"$f":"+G678","v":1.2},0,{"$f":"+I678","v":1.2},0,{"$f":"+K678","v":1.2},0,{"$f":"+M678","v":1.2},0,{"$f":"+O678","v":1.2},0,{"$f":"+Q678","v":1.2},0,{"$f":"+S678","v":1.2},0,{"$f":"+U678","v":1.2},{"$f":"+P678","v":0},{"$f":"+W678","v":1.2},0,{"$f":"+Y678","v":1.2},0,{"$f":"+AA678","v":1.2},0,{"$f":"+AC678","v":1.2},0,{"$f":"+AC678","v":1.2},0,1.2,{"$f":"+AD678","v":0},1.2,null,null,0,0,0,{"$f":"+AQ677","v":0},0,0,0]
[null,null,null,{"$f":"+E682","v":0},{"$f":"+D638","v":0},{"$f":"+AV655","v":0},{"$f":"+D678","v":6.2},0,{"$f":"+G679","v":6.2},0,{"$f":"+I679","v":6.2},0,{"$f":"+K679","v":6.2},0,{"$f":"+M679","v":6.2},0,{"$f":"+O679","v":6.2},0,{"$f":"+Q679","v":6.2},0,{"$f":"+S679","v":6.2},0,{"$f":"+U679","v":6.2},{"$f":"+P679","v":0},{"$f":"+W679","v":6.2},{"$f":"+N679","v":0},{"$f":"+Y679","v":6.2},0,{"$f":"+AA679","v":6.2},0,{"$f":"+AC679","v":6.2},0,{"$f":"+AC679","v":6.2},0,6.2,{"$f":"+AD679","v":0},6.2,null,null,0,0,0,{"$f":"+AS679","v":0},0,0,0]
[null,null,null,"Ukupni pritisak",null,"SQhi=",{"$f":"+G683","v":5.1199999999999996E-2},"SQhi=",{"$f":"+I683","v":0},"SQhi=",{"$f":"+K683","v":0},"SQhi=",{"$f":"+M683","v":0},"SQhi=",{"$f":"+O683","v":0},"SQhi=",{"$f":"+Q683","v":0},"SQhi=",{"$f":"+S683","v":0},"SQhi=",{"$f":"+U683","v":0},"SQhi=",{"$f":"+W683","v":0},"SQhi=",{"$f":"+Y683","v":0},"SQhi=",{"$f":"+AA683","v":0},"SQhi=",{"$f":"+AC683","v":0},"SQhi=",{"$f":"+AE683","v":0},"SQhi=",{"$f":"+AG683","v":0},"SQhi=",{"$f":"+AI683","v":0},"SQhi=",{"$f":"+AK683","v":0},null,null,"SQhi=",{"$f":"+AO683","v":0},"SQhi=",{"$f":"+AQ683","v":{"$error":"#REF!"}},"SQhi=",{"$f":"+AS683","v":0},"SQhi="]
[null,null,null,"Koordinata težišta ",null," y=",{"$f":"+G685","v":1.3066666666666666}," y=",{"$f":"+I685","v":0}," y=",{"$f":"+K685","v":0}," y=",{"$f":"+M685","v":0}," y=",{"$f":"+O685","v":0}," y=",{"$f":"+Q685","v":0}," y=",{"$f":"+S685","v":0}," y=",{"$f":"+U685","v":0}," y=",{"$f":"+W685","v":0}," y=",{"$f":"+Y685","v":0}," y=",{"$f":"+AA685","v":0}," y=",{"$f":"+AC685","v":0}," y=",{"$f":"+AE685","v":0}," y=",{"$f":"+AG685","v":0}," y=",{"$f":"+AI685","v":0}," y=",{"$f":"+AK685","v":0},null,null," y=",{"$f":"+AO685","v":0}," y=",{"$f":"+AQ685","v":{"$error":"#REF!"}}," y=",{"$f":"+AS685","v":0}," y="]
[null,null,null,"krak za presjek III - III",null,"z=",{"$f":"+G681-'Analiza i dimenzioniranje'!$E$52","v":0.10666666666666669},"z=",{"$f":"+I681-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+K681-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+M681-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+O681-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+Q681-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+S681-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+U681-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z=",{"$f":"+W681-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+Y681-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AA681-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AC681-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AE681-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AG681-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AI681-'Analiza i dimenzioniranje'!$E$52","v":-1.2},"z=",{"$f":"+AK681-'Analiza i dimenzioniranje'!$E$52","v":-1.2},null,null,"z=",{"$f":"+AO681-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z=",{"$f":"+AQ681-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":{"$error":"#REF!"}},"z=",{"$f":"+AS681-('Analiza i dimenzioniranje'!$E$52-'Analiza i dimenzioniranje'!$E$51)","v":-0.5},"z="]
[null,null,null,"x=",0,"F=",{"$f":"-0.5*(+\n (F662*G663-F663*G662)+\n(F663*G664-F664*G663)+\n(F664*G665-F665*G664)+\n(F665*G666-F666*G665)+\n(F666*G667-F667*G666)+\n(F667*G668-F668*G667)+\n(F668*G669-F669*G668)+\n(F669*G670-F670*G669)+\n(F670*G671-F671*G670)+\n(F671*G672-F672*G671)+\n(F672*G673-F673*G672)+\n(F673*G674-F674*G673)+\n(F674*G675-F675*G674)+\n(F675*G676-F676*G675)+\n(F676*G677-F677*G676)+\n(F677*G678-F678*G677)+\n(F678*G679-F679*G678))","v":5.1199999999999996E-2},"F=",{"$f":"-0.5*(+\n (H662*I663-H663*I662)+\n(H663*I664-H664*I663)+\n(H664*I665-H665*I664)+\n(H665*I666-H666*I665)+\n(H666*I667-H667*I666)+\n(H667*I668-H668*I667)+\n(H668*I669-H669*I668)+\n(H669*I670-H670*I669)+\n(H670*I671-H671*I670)+\n(H671*I672-H672*I671)+\n(H672*I673-H673*I672)+\n(H673*I674-H674*I673)+\n(H674*I675-H675*I674)+\n(H675*I676-H676*I675)+\n(H676*I677-H677*I676)+\n(H677*I678-H678*I677)+\n(H678*I679-H679*I678))","v":0},"F=",{"$f":"-0.5*((J660*K661-J661*K660)+(J661*K662-J662*K661)+\n (J662*K663-J663*K662)+\n(J663*K664-J664*K663)+\n(J664*K665-J665*K664)+\n(J665*K666-J666*K665)+\n(J666*K667-J667*K666)+\n(J667*K668-J668*K667)+\n(J668*K669-J669*K668)+\n(J669*K670-J670*K669)+\n(J670*K671-J671*K670)+\n(J671*K672-J672*K671)+\n(J672*K673-J673*K672)+\n(J673*K674-J674*K673)+\n(J674*K675-J675*K674)+\n(J675*K676-J676*K675)+\n(J676*K677-J677*K676)+\n(J677*K678-J678*K677)\n)","v":0},"F=",{"$f":"-0.5*(+\n (L662*M663-L663*M662)+\n(L663*M664-L664*M663)+\n(L664*M665-L665*M664)+\n(L665*M666-L666*M665)+\n(L666*M667-L667*M666)+\n(L667*M668-L668*M667)+\n(L668*M669-L669*M668)+\n(L669*M670-L670*M669)+\n(L670*M671-L671*M670)+\n(L671*M672-L672*M671)+\n(L672*M673-L673*M672)+\n(L673*M674-L674*M673)+\n(L674*M675-L675*M674)+\n(L675*M676-L676*M675)+\n(L676*M677-L677*M676)+\n(L677*M678-L678*M677)+\n(L678*M679-L679*M678))","v":0},"F=",{"$f":"-0.5*(+\n (N662*O663-N663*O662)+\n(N663*O664-N664*O663)+\n(N664*O665-N665*O664)+\n(N665*O666-N666*O665)+\n(N666*O667-N667*O666)+\n(N667*O668-N668*O667)+\n(N668*O669-N669*O668)+\n(N669*O670-N670*O669)+\n(N670*O671-N671*O670)+\n(N671*O672-N672*O671)+\n(N672*O673-N673*O672)+\n(N673*O674-N674*O673)+\n(N674*O675-N675*O674)+\n(N675*O676-N676*O675)+\n(N676*O677-N677*O676)+\n(N677*O678-N678*O677)+\n(N678*O679-N679*O678))","v":0},"F=",{"$f":"-0.5*(+\n (P662*Q663-P663*Q662)+\n(P663*Q664-P664*Q663)+\n(P664*Q665-P665*Q664)+\n(P665*Q666-P666*Q665)+\n(P666*Q667-P667*Q666)+\n(P667*Q668-P668*Q667)+\n(P668*Q669-P669*Q668)+\n(P669*Q670-P670*Q669)+\n(P670*Q671-P671*Q670)+\n(P671*Q672-P672*Q671)+\n(P672*Q673-P673*Q672)+\n(P673*Q674-P674*Q673)+\n(P674*Q675-P675*Q674)+\n(P675*Q676-P676*Q675)+\n(P676*Q677-P677*Q676)+\n(P677*Q678-P678*Q677)+\n(P678*Q679-P679*Q678))","v":0},"F=",{"$f":"-0.5*((R660*S661-R661*S660)+(R661*S662-R662*S661)+\n (R662*S663-R663*S662)+\n(R663*S664-R664*S663)+\n(R664*S665-R665*S664)+\n(R665*S666-R666*S665)+\n(R666*S667-R667*S666)+\n(R667*S668-R668*S667)+\n(R668*S669-R669*S668)+\n(R669*S670-R670*S669)+\n(R670*S671-R671*S670)+\n(R671*S672-R672*S671)+\n(R672*S673-R673*S672)+\n(R673*S674-R674*S673)+\n(R674*S675-R675*S674)+\n(R675*S676-R676*S675)+\n(R676*S677-R677*S676)+\n(R677*S678-R678*S677)\n)","v":0},"F=",{"$f":"-0.5*(+\n (T662*U663-T663*U662)+\n(T663*U664-T664*U663)+\n(T664*U665-T665*U664)+\n(T665*U666-T666*U665)+\n(T666*U667-T667*U666)+\n(T667*U668-T668*U667)+\n(T668*U669-T669*U668)+\n(T669*U670-T670*U669)+\n(T670*U671-T671*U670)+\n(T671*U672-T672*U671)+\n(T672*U673-T673*U672)+\n(T673*U674-T674*U673)+\n(T674*U675-T675*U674)+\n(T675*U676-T676*U675)+\n(T676*U677-T677*U676)+\n(T677*U678-T678*U677)+\n(T678*U679-T679*U678))","v":0},"F=",{"$f":"-0.5*(+\n (V662*W663-V663*W662)+\n(V663*W664-V664*W663)+\n(V664*W665-V665*W664)+\n(V665*W666-V666*W665)+\n(V666*W667-V667*W666)+\n(V667*W668-V668*W667)+\n(V668*W669-V669*W668)+\n(V669*W670-V670*W669)+\n(V670*W671-V671*W670)+\n(V671*W672-V672*W671)+\n(V672*W673-V673*W672)+\n(V673*W674-V674*W673)+\n(V674*W675-V675*W674)+\n(V675*W676-V676*W675)+\n(V676*W677-V677*W676)+\n(V677*W678-V678*W677)+\n(V678*W679-V679*W678))","v":0},"F=",{"$f":"-0.5*(+\n (X662*Y663-X663*Y662)+\n(X663*Y664-X664*Y663)+\n(X664*Y665-X665*Y664)+\n(X665*Y666-X666*Y665)+\n(X666*Y667-X667*Y666)+\n(X667*Y668-X668*Y667)+\n(X668*Y669-X669*Y668)+\n(X669*Y670-X670*Y669)+\n(X670*Y671-X671*Y670)+\n(X671*Y672-X672*Y671)+\n(X672*Y673-X673*Y672)+\n(X673*Y674-X674*Y673)+\n(X674*Y675-X675*Y674)+\n(X675*Y676-X676*Y675)+\n(X676*Y677-X677*Y676)+\n(X677*Y678-X678*Y677)+\n(X678*Y679-X679*Y678))","v":0},"F=",{"$f":"-0.5*((Z660*AA661-Z661*AA660)+(Z661*AA662-Z662*AA661)+\n (Z662*AA663-Z663*AA662)+\n(Z663*AA664-Z664*AA663)+\n(Z664*AA665-Z665*AA664)+\n(Z665*AA666-Z666*AA665)+\n(Z666*AA667-Z667*AA666)+\n(Z667*AA668-Z668*AA667)+\n(Z668*AA669-Z669*AA668)+\n(Z669*AA670-Z670*AA669)+\n(Z670*AA671-Z671*AA670)+\n(Z671*AA672-Z672*AA671)+\n(Z672*AA673-Z673*AA672)+\n(Z673*AA674-Z674*AA673)+\n(Z674*AA675-Z675*AA674)+\n(Z675*AA676-Z676*AA675)+\n(Z676*AA677-Z677*AA676)+\n(Z677*AA678-Z678*AA677)\n)","v":0},"F=",{"$f":"-0.5*(+\n (AB662*AC663-AB663*AC662)+\n(AB663*AC664-AB664*AC663)+\n(AB664*AC665-AB665*AC664)+\n(AB665*AC666-AB666*AC665)+\n(AB666*AC667-AB667*AC666)+\n(AB667*AC668-AB668*AC667)+\n(AB668*AC669-AB669*AC668)+\n(AB669*AC670-AB670*AC669)+\n(AB670*AC671-AB671*AC670)+\n(AB671*AC672-AB672*AC671)+\n(AB672*AC673-AB673*AC672)+\n(AB673*AC674-AB674*AC673)+\n(AB674*AC675-AB675*AC674)+\n(AB675*AC676-AB676*AC675)+\n(AB676*AC677-AB677*AC676)+\n(AB677*AC678-AB678*AC677)+\n(AB678*AC679-AB679*AC678))","v":0},"F=",{"$f":"-0.5*(+\n (AD662*AE663-AD663*AE662)+\n(AD663*AE664-AD664*AE663)+\n(AD664*AE665-AD665*AE664)+\n(AD665*AE666-AD666*AE665)+\n(AD666*AE667-AD667*AE666)+\n(AD667*AE668-AD668*AE667)+\n(AD668*AE669-AD669*AE668)+\n(AD669*AE670-AD670*AE669)+\n(AD670*AE671-AD671*AE670)+\n(AD671*AE672-AD672*AE671)+\n(AD672*AE673-AD673*AE672)+\n(AD673*AE674-AD674*AE673)+\n(AD674*AE675-AD675*AE674)+\n(AD675*AE676-AD676*AE675)+\n(AD676*AE677-AD677*AE676)+\n(AD677*AE678-AD678*AE677)+\n(AD678*AE679-AD679*AE678))","v":0},"F=",{"$f":"-0.5*(+\n (AF662*AG663-AF663*AG662)+\n(AF663*AG664-AF664*AG663)+\n(AF664*AG665-AF665*AG664)+\n(AF665*AG666-AF666*AG665)+\n(AF666*AG667-AF667*AG666)+\n(AF667*AG668-AF668*AG667)+\n(AF668*AG669-AF669*AG668)+\n(AF669*AG670-AF670*AG669)+\n(AF670*AG671-AF671*AG670)+\n(AF671*AG672-AF672*AG671)+\n(AF672*AG673-AF673*AG672)+\n(AF673*AG674-AF674*AG673)+\n(AF674*AG675-AF675*AG674)+\n(AF675*AG676-AF676*AG675)+\n(AF676*AG677-AF677*AG676)+\n(AF677*AG678-AF678*AG677)+\n(AF678*AG679-AF679*AG678))","v":0},"F=",{"$f":"-0.5*((AH660*AI661-AH661*AI660)+(AH661*AI662-AH662*AI661)+\n (AH662*AI663-AH663*AI662)+\n(AH663*AI664-AH664*AI663)+\n(AH664*AI665-AH665*AI664)+\n(AH665*AI666-AH666*AI665)+\n(AH666*AI667-AH667*AI666)+\n(AH667*AI668-AH668*AI667)+\n(AH668*AI669-AH669*AI668)+\n(AH669*AI670-AH670*AI669)+\n(AH670*AI671-AH671*AI670)+\n(AH671*AI672-AH672*AI671)+\n(AH672*AI673-AH673*AI672)+\n(AH673*AI674-AH674*AI673)+\n(AH674*AI675-AH675*AI674)+\n(AH675*AI676-AH676*AI675)+\n(AH676*AI677-AH677*AI676)+\n(AH677*AI678-AH678*AI677)\n)","v":0},"F=",{"$f":"-0.5*(+\n (AJ662*AK663-AJ663*AK662)+\n(AJ663*AK664-AJ664*AK663)+\n(AJ664*AK665-AJ665*AK664)+\n(AJ665*AK666-AJ666*AK665)+\n(AJ666*AK667-AJ667*AK666)+\n(AJ667*AK668-AJ668*AK667)+\n(AJ668*AK669-AJ669*AK668)+\n(AJ669*AK670-AJ670*AK669)+\n(AJ670*AK671-AJ671*AK670)+\n(AJ671*AK672-AJ672*AK671)+\n(AJ672*AK673-AJ673*AK672)+\n(AJ673*AK674-AJ674*AK673)+\n(AJ674*AK675-AJ675*AK674)+\n(AJ675*AK676-AJ676*AK675)+\n(AJ676*AK677-AJ677*AK676)+\n(AJ677*AK678-AJ678*AK677)+\n(AJ678*AK679-AJ679*AK678))","v":0},null,null,"F=",{"$f":"-0.5*((AN660*AO661-AN661*AO660)+(AN661*AO662-AN662*AO661)+\n (AN662*AO663-AN663*AO662)+\n(AN663*AO664-AN664*AO663)+\n(AN664*AO665-AN665*AO664)+\n(AN665*AO666-AN666*AO665)+\n(AN666*AO667-AN667*AO666)+\n(AN667*AO668-AN668*AO667)+\n(AN668*AO669-AN669*AO668)+\n(AN669*AO670-AN670*AO669)+\n(AN670*AO671-AN671*AO670)+\n(AN671*AO672-AN672*AO671)+\n(AN672*AO673-AN673*AO672)+\n(AN673*AO674-AN674*AO673)+\n(AN674*AO675-AN675*AO674)+\n(AN675*AO676-AN676*AO675)+\n(AN676*AO677-AN677*AO676)+\n(AN677*AO678-AN678*AO677)\n)","v":0},"F=",{"$f":"-0.5*((AP660*AQ661-AP661*AQ660)+(AP661*AQ662-AP662*AQ661)+\n (AP662*AQ663-AP663*AQ662)+\n(AP663*AQ664-AP664*AQ663)+\n(AP664*AQ665-AP665*AQ664)+\n(AP665*AQ666-AP666*AQ665)+\n(AP666*AQ667-AP667*AQ666)+\n(AP667*AQ668-AP668*AQ667)+\n(AP668*AQ669-AP669*AQ668)+\n(AP669*AQ670-AP670*AQ669)+\n(AP670*AQ671-AP671*AQ670)+\n(AP671*AQ672-AP672*AQ671)+\n(AP672*AQ673-AP673*AQ672)+\n(AP673*AQ674-AP674*AQ673)+\n(AP674*AQ675-AP675*AQ674)+\n(AP675*AQ676-AP676*AQ675)+\n(AP676*AQ677-AP677*AQ676)+\n(AP677*AQ678-AP678*AQ677)\n)","v":{"$error":"#REF!"}},"F=",{"$f":"-0.5*((AR660*AS661-AR661*AS660)+(AR661*AS662-AR662*AS661)+\n (AR662*AS663-AR663*AS662)+\n(AR663*AS664-AR664*AS663)+\n(AR664*AS665-AR665*AS664)+\n(AR665*AS666-AR666*AS665)+\n(AR666*AS667-AR667*AS666)+\n(AR667*AS668-AR668*AS667)+\n(AR668*AS669-AR669*AS668)+\n(AR669*AS670-AR670*AS669)+\n(AR670*AS671-AR671*AS670)+\n(AR671*AS672-AR672*AS671)+\n(AR672*AS673-AR673*AS672)+\n(AR673*AS674-AR674*AS673)+\n(AR674*AS675-AR675*AS674)+\n(AR675*AS676-AR676*AS675)+\n(AR676*AS677-AR677*AS676)+\n(AR677*AS678-AR678*AS677)\n)","v":0},"F="]
[null,null,null,"y=",{"$f":"+IF(E682=0,0,-((D659*E660-D660*E659)*(E659+E660)+(D660*E661-D661*E660)*(E660+E661)+\n(D661*E662-D662*E661)*(E661+E662)+\n(D662*E663-D663*E662)*(E662+E663)+\n(D663*E664-D664*E663)*(E663+E664)+\n(D664*E665-D665*E664)*(E664+E665)+\n(D665*E666-D666*E665)*(E665+E666)+\n(D666*E667-D667*E666)*(E666+E667)+\n(D667*E668-D668*E667)*(E667+E668)+\n(D668*E669-D669*E668)*(E668+E669)+\n(D669*E670-D670*E669)*(E669+E670)+\n(D670*E671-D671*E670)*(E670+E671)+\n(D671*E672-D672*E671)*(E671+E672)+\n(D672*E673-E676*E672)*(E672+E673)+\n(E676*E674-E677*E673)*(E673+E674)+\n(E677*E675-E678*E674)*(E674+E675)+\n(E678*D676-E679*E675)*(E675+D676)+\n(E679*D677-D680*D676)*(D676+D677)+\n(D680*D678-D681*D677)*(D677+D678))/6/E682)","v":0},"x=",1,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,"x=",0,null,null,"x=",0,"x=",0,"x=",0,"x="]
[null,null,null,"y=",{"$f":"+IF(E683=0,0,-((D660*E661-D661*E660)*(E660+E661)+(D661*E662-D662*E661)*(E661+E662)+\n(D662*E663-D663*E662)*(E662+E663)+\n(D663*E664-D664*E663)*(E663+E664)+\n(D664*E665-D665*E664)*(E664+E665)+\n(D665*E666-D666*E665)*(E665+E666)+\n(D666*E667-D667*E666)*(E666+E667)+\n(D667*E668-D668*E667)*(E667+E668)+\n(D668*E669-D669*E668)*(E668+E669)+\n(D669*E670-D670*E669)*(E669+E670)+\n(D670*E671-D671*E670)*(E670+E671)+\n(D671*E672-D672*E671)*(E671+E672)+\n(D672*E673-E676*E672)*(E672+E673)+\n(E676*E674-E677*E673)*(E673+E674)+\n(E677*E675-E678*E674)*(E674+E675)+\n(E678*D676-E679*E675)*(E675+D676)+\n(E679*D677-D680*D676)*(D676+D677)+\n(D680*D678-D681*D677)*(D677+D678)+\n(D681*D679-D682*D678)*(D678+D679))/6/E683)","v":0},"y=",{"$f":"+IF(G683=0,0,-((F660*G661-F661*G660)*(G660+G661)+(F661*G662-F662*G661)*(G661+G662)+\n(F662*G663-F663*G662)*(G662+G663)+\n(F663*G664-F664*G663)*(G663+G664)+\n(F664*G665-F665*G664)*(G664+G665)+\n(F665*G666-F666*G665)*(G665+G666)+\n(F666*G667-F667*G666)*(G666+G667)+\n(F667*G668-F668*G667)*(G667+G668)+\n(F668*G669-F669*G668)*(G668+G669)+\n(F669*G670-F670*G669)*(G669+G670)+\n(F670*G671-F671*G670)*(G670+G671)+\n(F671*G672-F672*G671)*(G671+G672)+\n(F672*G673-F673*G672)*(G672+G673)+\n(F673*G674-F674*G673)*(G673+G674)+\n(F674*G675-F675*G674)*(G674+G675)+\n(F675*G676-F676*G675)*(G675+G676)+\n(F676*G677-F677*G676)*(G676+G677)+\n(F677*G678-F678*G677)*(G677+G678)+\n(F678*G679-F679*G678)*(G678+G679))/6/G683)","v":1.3066666666666666},"y=",{"$f":"+IF(I683=0,0,-((H660*I661-H661*I660)*(I660+I661)+(H661*I662-H662*I661)*(I661+I662)+\n(H662*I663-H663*I662)*(I662+I663)+\n(H663*I664-H664*I663)*(I663+I664)+\n(H664*I665-H665*I664)*(I664+I665)+\n(H665*I666-H666*I665)*(I665+I666)+\n(H666*I667-H667*I666)*(I666+I667)+\n(H667*I668-H668*I667)*(I667+I668)+\n(H668*I669-H669*I668)*(I668+I669)+\n(H669*I670-H670*I669)*(I669+I670)+\n(H670*I671-H671*I670)*(I670+I671)+\n(H671*I672-H672*I671)*(I671+I672)+\n(H672*I673-H673*I672)*(I672+I673)+\n(H673*I674-H674*I673)*(I673+I674)+\n(H674*I675-H675*I674)*(I674+I675)+\n(H675*I676-H676*I675)*(I675+I676)+\n(H676*I677-H677*I676)*(I676+I677)+\n(H677*I678-H678*I677)*(I677+I678)+\n(H678*I679-H679*I678)*(I678+I679))/6/I683)","v":0},"y=",{"$f":"+IF(K683=0,0,-((J660*K661-J661*K660)*(K660+K661)+(J661*K662-J662*K661)*(K661+K662)+\n(J662*K663-J663*K662)*(K662+K663)+\n(J663*K664-J664*K663)*(K663+K664)+\n(J664*K665-J665*K664)*(K664+K665)+\n(J665*K666-J666*K665)*(K665+K666)+\n(J666*K667-J667*K666)*(K666+K667)+\n(J667*K668-J668*K667)*(K667+K668)+\n(J668*K669-J669*K668)*(K668+K669)+\n(J669*K670-J670*K669)*(K669+K670)+\n(J670*K671-J671*K670)*(K670+K671)+\n(J671*K672-J672*K671)*(K671+K672)+\n(J672*K673-J673*K672)*(K672+K673)+\n(J673*K674-J674*K673)*(K673+K674)+\n(J674*K675-J675*K674)*(K674+K675)+\n(J675*K676-J676*K675)*(K675+K676)+\n(J676*K677-J677*K676)*(K676+K677)+\n(J677*K678-J678*K677)*(K677+K678)+\n(J678*K679-J679*K678)*(K678+K679))/6/K683)","v":0},"y=",{"$f":"+IF(M683=0,0,-((L660*M661-L661*M660)*(M660+M661)+(L661*M662-L662*M661)*(M661+M662)+\n(L662*M663-L663*M662)*(M662+M663)+\n(L663*M664-L664*M663)*(M663+M664)+\n(L664*M665-L665*M664)*(M664+M665)+\n(L665*M666-L666*M665)*(M665+M666)+\n(L666*M667-L667*M666)*(M666+M667)+\n(L667*M668-L668*M667)*(M667+M668)+\n(L668*M669-L669*M668)*(M668+M669)+\n(L669*M670-L670*M669)*(M669+M670)+\n(L670*M671-L671*M670)*(M670+M671)+\n(L671*M672-L672*M671)*(M671+M672)+\n(L672*M673-L673*M672)*(M672+M673)+\n(L673*M674-L674*M673)*(M673+M674)+\n(L674*M675-L675*M674)*(M674+M675)+\n(L675*M676-L676*M675)*(M675+M676)+\n(L676*M677-L677*M676)*(M676+M677)+\n(L677*M678-L678*M677)*(M677+M678)+\n(L678*M679-L679*M678)*(M678+M679))/6/M683)","v":0},"y=",{"$f":"+IF(O683=0,0,-((N660*O661-N661*O660)*(O660+O661)+(N661*O662-N662*O661)*(O661+O662)+\n(N662*O663-N663*O662)*(O662+O663)+\n(N663*O664-N664*O663)*(O663+O664)+\n(N664*O665-N665*O664)*(O664+O665)+\n(N665*O666-N666*O665)*(O665+O666)+\n(N666*O667-N667*O666)*(O666+O667)+\n(N667*O668-N668*O667)*(O667+O668)+\n(N668*O669-N669*O668)*(O668+O669)+\n(N669*O670-N670*O669)*(O669+O670)+\n(N670*O671-N671*O670)*(O670+O671)+\n(N671*O672-N672*O671)*(O671+O672)+\n(N672*O673-N673*O672)*(O672+O673)+\n(N673*O674-N674*O673)*(O673+O674)+\n(N674*O675-N675*O674)*(O674+O675)+\n(N675*O676-N676*O675)*(O675+O676)+\n(N676*O677-N677*O676)*(O676+O677)+\n(N677*O678-N678*O677)*(O677+O678)+\n(N678*O679-N679*O678)*(O678+O679))/6/O683)","v":0},"y=",{"$f":"+IF(Q683=0,0,-((P660*Q661-P661*Q660)*(Q660+Q661)+(P661*Q662-P662*Q661)*(Q661+Q662)+\n(P662*Q663-P663*Q662)*(Q662+Q663)+\n(P663*Q664-P664*Q663)*(Q663+Q664)+\n(P664*Q665-P665*Q664)*(Q664+Q665)+\n(P665*Q666-P666*Q665)*(Q665+Q666)+\n(P666*Q667-P667*Q666)*(Q666+Q667)+\n(P667*Q668-P668*Q667)*(Q667+Q668)+\n(P668*Q669-P669*Q668)*(Q668+Q669)+\n(P669*Q670-P670*Q669)*(Q669+Q670)+\n(P670*Q671-P671*Q670)*(Q670+Q671)+\n(P671*Q672-P672*Q671)*(Q671+Q672)+\n(P672*Q673-P673*Q672)*(Q672+Q673)+\n(P673*Q674-P674*Q673)*(Q673+Q674)+\n(P674*Q675-P675*Q674)*(Q674+Q675)+\n(P675*Q676-P676*Q675)*(Q675+Q676)+\n(P676*Q677-P677*Q676)*(Q676+Q677)+\n(P677*Q678-P678*Q677)*(Q677+Q678)+\n(P678*Q679-P679*Q678)*(Q678+Q679))/6/Q683)","v":0},"y=",{"$f":"+IF(S683=0,0,-((R660*S661-R661*S660)*(S660+S661)+(R661*S662-R662*S661)*(S661+S662)+\n(R662*S663-R663*S662)*(S662+S663)+\n(R663*S664-R664*S663)*(S663+S664)+\n(R664*S665-R665*S664)*(S664+S665)+\n(R665*S666-R666*S665)*(S665+S666)+\n(R666*S667-R667*S666)*(S666+S667)+\n(R667*S668-R668*S667)*(S667+S668)+\n(R668*S669-R669*S668)*(S668+S669)+\n(R669*S670-R670*S669)*(S669+S670)+\n(R670*S671-R671*S670)*(S670+S671)+\n(R671*S672-R672*S671)*(S671+S672)+\n(R672*S673-R673*S672)*(S672+S673)+\n(R673*S674-R674*S673)*(S673+S674)+\n(R674*S675-R675*S674)*(S674+S675)+\n(R675*S676-R676*S675)*(S675+S676)+\n(R676*S677-R677*S676)*(S676+S677)+\n(R677*S678-R678*S677)*(S677+S678)+\n(R678*S679-R679*S678)*(S678+S679))/6/S683)","v":0},"y=",{"$f":"+IF(U683=0,0,-((T660*U661-T661*U660)*(U660+U661)+(T661*U662-T662*U661)*(U661+U662)+\n(T662*U663-T663*U662)*(U662+U663)+\n(T663*U664-T664*U663)*(U663+U664)+\n(T664*U665-T665*U664)*(U664+U665)+\n(T665*U666-T666*U665)*(U665+U666)+\n(T666*U667-T667*U666)*(U666+U667)+\n(T667*U668-T668*U667)*(U667+U668)+\n(T668*U669-T669*U668)*(U668+U669)+\n(T669*U670-T670*U669)*(U669+U670)+\n(T670*U671-T671*U670)*(U670+U671)+\n(T671*U672-T672*U671)*(U671+U672)+\n(T672*U673-T673*U672)*(U672+U673)+\n(T673*U674-T674*U673)*(U673+U674)+\n(T674*U675-T675*U674)*(U674+U675)+\n(T675*U676-T676*U675)*(U675+U676)+\n(T676*U677-T677*U676)*(U676+U677)+\n(T677*U678-T678*U677)*(U677+U678)+\n(T678*U679-T679*U678)*(U678+U679))/6/U683)","v":0},"y=",{"$f":"+IF(W683=0,0,-((V660*W661-V661*W660)*(W660+W661)+(V661*W662-V662*W661)*(W661+W662)+\n(V662*W663-V663*W662)*(W662+W663)+\n(V663*W664-V664*W663)*(W663+W664)+\n(V664*W665-V665*W664)*(W664+W665)+\n(V665*W666-V666*W665)*(W665+W666)+\n(V666*W667-V667*W666)*(W666+W667)+\n(V667*W668-V668*W667)*(W667+W668)+\n(V668*W669-V669*W668)*(W668+W669)+\n(V669*W670-V670*W669)*(W669+W670)+\n(V670*W671-V671*W670)*(W670+W671)+\n(V671*W672-V672*W671)*(W671+W672)+\n(V672*W673-V673*W672)*(W672+W673)+\n(V673*W674-V674*W673)*(W673+W674)+\n(V674*W675-V675*W674)*(W674+W675)+\n(V675*W676-V676*W675)*(W675+W676)+\n(V676*W677-V677*W676)*(W676+W677)+\n(V677*W678-V678*W677)*(W677+W678)+\n(V678*W679-V679*W678)*(W678+W679))/6/W683)","v":0},"y=",{"$f":"+IF(Y683=0,0,-((X660*Y661-X661*Y660)*(Y660+Y661)+(X661*Y662-X662*Y661)*(Y661+Y662)+\n(X662*Y663-X663*Y662)*(Y662+Y663)+\n(X663*Y664-X664*Y663)*(Y663+Y664)+\n(X664*Y665-X665*Y664)*(Y664+Y665)+\n(X665*Y666-X666*Y665)*(Y665+Y666)+\n(X666*Y667-X667*Y666)*(Y666+Y667)+\n(X667*Y668-X668*Y667)*(Y667+Y668)+\n(X668*Y669-X669*Y668)*(Y668+Y669)+\n(X669*Y670-X670*Y669)*(Y669+Y670)+\n(X670*Y671-X671*Y670)*(Y670+Y671)+\n(X671*Y672-X672*Y671)*(Y671+Y672)+\n(X672*Y673-X673*Y672)*(Y672+Y673)+\n(X673*Y674-X674*Y673)*(Y673+Y674)+\n(X674*Y675-X675*Y674)*(Y674+Y675)+\n(X675*Y676-X676*Y675)*(Y675+Y676)+\n(X676*Y677-X677*Y676)*(Y676+Y677)+\n(X677*Y678-X678*Y677)*(Y677+Y678)+\n(X678*Y679-X679*Y678)*(Y678+Y679))/6/Y683)","v":0},"y=",{"$f":"+IF(AA683=0,0,-((Z660*AA661-Z661*AA660)*(AA660+AA661)+(Z661*AA662-Z662*AA661)*(AA661+AA662)+\n(Z662*AA663-Z663*AA662)*(AA662+AA663)+\n(Z663*AA664-Z664*AA663)*(AA663+AA664)+\n(Z664*AA665-Z665*AA664)*(AA664+AA665)+\n(Z665*AA666-Z666*AA665)*(AA665+AA666)+\n(Z666*AA667-Z667*AA666)*(AA666+AA667)+\n(Z667*AA668-Z668*AA667)*(AA667+AA668)+\n(Z668*AA669-Z669*AA668)*(AA668+AA669)+\n(Z669*AA670-Z670*AA669)*(AA669+AA670)+\n(Z670*AA671-Z671*AA670)*(AA670+AA671)+\n(Z671*AA672-Z672*AA671)*(AA671+AA672)+\n(Z672*AA673-Z673*AA672)*(AA672+AA673)+\n(Z673*AA674-Z674*AA673)*(AA673+AA674)+\n(Z674*AA675-Z675*AA674)*(AA674+AA675)+\n(Z675*AA676-Z676*AA675)*(AA675+AA676)+\n(Z676*AA677-Z677*AA676)*(AA676+AA677)+\n(Z677*AA678-Z678*AA677)*(AA677+AA678)+\n(Z678*AA679-Z679*AA678)*(AA678+AA679))/6/AA683)","v":0},"y=",{"$f":"+IF(AC683=0,0,-((AB660*AC661-AB661*AC660)*(AC660+AC661)+(AB661*AC662-AB662*AC661)*(AC661+AC662)+\n(AB662*AC663-AB663*AC662)*(AC662+AC663)+\n(AB663*AC664-AB664*AC663)*(AC663+AC664)+\n(AB664*AC665-AB665*AC664)*(AC664+AC665)+\n(AB665*AC666-AB666*AC665)*(AC665+AC666)+\n(AB666*AC667-AB667*AC666)*(AC666+AC667)+\n(AB667*AC668-AB668*AC667)*(AC667+AC668)+\n(AB668*AC669-AB669*AC668)*(AC668+AC669)+\n(AB669*AC670-AB670*AC669)*(AC669+AC670)+\n(AB670*AC671-AB671*AC670)*(AC670+AC671)+\n(AB671*AC672-AB672*AC671)*(AC671+AC672)+\n(AB672*AC673-AB673*AC672)*(AC672+AC673)+\n(AB673*AC674-AB674*AC673)*(AC673+AC674)+\n(AB674*AC675-AB675*AC674)*(AC674+AC675)+\n(AB675*AC676-AB676*AC675)*(AC675+AC676)+\n(AB676*AC677-AB677*AC676)*(AC676+AC677)+\n(AB677*AC678-AB678*AC677)*(AC677+AC678)+\n(AB678*AC679-AB679*AC678)*(AC678+AC679))/6/AC683)","v":0},"y=",{"$f":"+IF(AE683=0,0,-((AD660*AE661-AD661*AE660)*(AE660+AE661)+(AD661*AE662-AD662*AE661)*(AE661+AE662)+\n(AD662*AE663-AD663*AE662)*(AE662+AE663)+\n(AD663*AE664-AD664*AE663)*(AE663+AE664)+\n(AD664*AE665-AD665*AE664)*(AE664+AE665)+\n(AD665*AE666-AD666*AE665)*(AE665+AE666)+\n(AD666*AE667-AD667*AE666)*(AE666+AE667)+\n(AD667*AE668-AD668*AE667)*(AE667+AE668)+\n(AD668*AE669-AD669*AE668)*(AE668+AE669)+\n(AD669*AE670-AD670*AE669)*(AE669+AE670)+\n(AD670*AE671-AD671*AE670)*(AE670+AE671)+\n(AD671*AE672-AD672*AE671)*(AE671+AE672)+\n(AD672*AE673-AD673*AE672)*(AE672+AE673)+\n(AD673*AE674-AD674*AE673)*(AE673+AE674)+\n(AD674*AE675-AD675*AE674)*(AE674+AE675)+\n(AD675*AE676-AD676*AE675)*(AE675+AE676)+\n(AD676*AE677-AD677*AE676)*(AE676+AE677)+\n(AD677*AE678-AD678*AE677)*(AE677+AE678)+\n(AD678*AE679-AD679*AE678)*(AE678+AE679))/6/AE683)","v":0},"y=",{"$f":"+IF(AG683=0,0,-((AF660*AG661-AF661*AG660)*(AG660+AG661)+(AF661*AG662-AF662*AG661)*(AG661+AG662)+\n(AF662*AG663-AF663*AG662)*(AG662+AG663)+\n(AF663*AG664-AF664*AG663)*(AG663+AG664)+\n(AF664*AG665-AF665*AG664)*(AG664+AG665)+\n(AF665*AG666-AF666*AG665)*(AG665+AG666)+\n(AF666*AG667-AF667*AG666)*(AG666+AG667)+\n(AF667*AG668-AF668*AG667)*(AG667+AG668)+\n(AF668*AG669-AF669*AG668)*(AG668+AG669)+\n(AF669*AG670-AF670*AG669)*(AG669+AG670)+\n(AF670*AG671-AF671*AG670)*(AG670+AG671)+\n(AF671*AG672-AF672*AG671)*(AG671+AG672)+\n(AF672*AG673-AF673*AG672)*(AG672+AG673)+\n(AF673*AG674-AF674*AG673)*(AG673+AG674)+\n(AF674*AG675-AF675*AG674)*(AG674+AG675)+\n(AF675*AG676-AF676*AG675)*(AG675+AG676)+\n(AF676*AG677-AF677*AG676)*(AG676+AG677)+\n(AF677*AG678-AF678*AG677)*(AG677+AG678)+\n(AF678*AG679-AF679*AG678)*(AG678+AG679))/6/AG683)","v":0},"y=",{"$f":"+IF(AI683=0,0,-((AH660*AI661-AH661*AI660)*(AI660+AI661)+(AH661*AI662-AH662*AI661)*(AI661+AI662)+\n(AH662*AI663-AH663*AI662)*(AI662+AI663)+\n(AH663*AI664-AH664*AI663)*(AI663+AI664)+\n(AH664*AI665-AH665*AI664)*(AI664+AI665)+\n(AH665*AI666-AH666*AI665)*(AI665+AI666)+\n(AH666*AI667-AH667*AI666)*(AI666+AI667)+\n(AH667*AI668-AH668*AI667)*(AI667+AI668)+\n(AH668*AI669-AH669*AI668)*(AI668+AI669)+\n(AH669*AI670-AH670*AI669)*(AI669+AI670)+\n(AH670*AI671-AH671*AI670)*(AI670+AI671)+\n(AH671*AI672-AH672*AI671)*(AI671+AI672)+\n(AH672*AI673-AH673*AI672)*(AI672+AI673)+\n(AH673*AI674-AH674*AI673)*(AI673+AI674)+\n(AH674*AI675-AH675*AI674)*(AI674+AI675)+\n(AH675*AI676-AH676*AI675)*(AI675+AI676)+\n(AH676*AI677-AH677*AI676)*(AI676+AI677)+\n(AH677*AI678-AH678*AI677)*(AI677+AI678)+\n(AH678*AI679-AH679*AI678)*(AI678+AI679))/6/AI683)","v":0},"y=",{"$f":"+IF(AK683=0,0,-((AJ660*AK661-AJ661*AK660)*(AK660+AK661)+(AJ661*AK662-AJ662*AK661)*(AK661+AK662)+\n(AJ662*AK663-AJ663*AK662)*(AK662+AK663)+\n(AJ663*AK664-AJ664*AK663)*(AK663+AK664)+\n(AJ664*AK665-AJ665*AK664)*(AK664+AK665)+\n(AJ665*AK666-AJ666*AK665)*(AK665+AK666)+\n(AJ666*AK667-AJ667*AK666)*(AK666+AK667)+\n(AJ667*AK668-AJ668*AK667)*(AK667+AK668)+\n(AJ668*AK669-AJ669*AK668)*(AK668+AK669)+\n(AJ669*AK670-AJ670*AK669)*(AK669+AK670)+\n(AJ670*AK671-AJ671*AK670)*(AK670+AK671)+\n(AJ671*AK672-AJ672*AK671)*(AK671+AK672)+\n(AJ672*AK673-AJ673*AK672)*(AK672+AK673)+\n(AJ673*AK674-AJ674*AK673)*(AK673+AK674)+\n(AJ674*AK675-AJ675*AK674)*(AK674+AK675)+\n(AJ675*AK676-AJ676*AK675)*(AK675+AK676)+\n(AJ676*AK677-AJ677*AK676)*(AK676+AK677)+\n(AJ677*AK678-AJ678*AK677)*(AK677+AK678)+\n(AJ678*AK679-AJ679*AK678)*(AK678+AK679))/6/AK683)","v":0},null,null,"y=",{"$f":"+IF(AO683=0,0,-((AN660*AO661-AN661*AO660)*(AO660+AO661)+(AN661*AO662-AN662*AO661)*(AO661+AO662)+\n(AN662*AO663-AN663*AO662)*(AO662+AO663)+\n(AN663*AO664-AN664*AO663)*(AO663+AO664)+\n(AN664*AO665-AN665*AO664)*(AO664+AO665)+\n(AN665*AO666-AN666*AO665)*(AO665+AO666)+\n(AN666*AO667-AN667*AO666)*(AO666+AO667)+\n(AN667*AO668-AN668*AO667)*(AO667+AO668)+\n(AN668*AO669-AN669*AO668)*(AO668+AO669)+\n(AN669*AO670-AN670*AO669)*(AO669+AO670)+\n(AN670*AO671-AN671*AO670)*(AO670+AO671)+\n(AN671*AO672-AN672*AO671)*(AO671+AO672)+\n(AN672*AO673-AN673*AO672)*(AO672+AO673)+\n(AN673*AO674-AN674*AO673)*(AO673+AO674)+\n(AN674*AO675-AN675*AO674)*(AO674+AO675)+\n(AN675*AO676-AN676*AO675)*(AO675+AO676)+\n(AN676*AO677-AN677*AO676)*(AO676+AO677)+\n(AN677*AO678-AN678*AO677)*(AO677+AO678)+\n(AN678*AO679-AN679*AO678)*(AO678+AO679))/6/AO683)","v":0},"y=",{"$f":"+IF(AQ683=0,0,-((AP660*AQ661-AP661*AQ660)*(AQ660+AQ661)+(AP661*AQ662-AP662*AQ661)*(AQ661+AQ662)+\n(AP662*AQ663-AP663*AQ662)*(AQ662+AQ663)+\n(AP663*AQ664-AP664*AQ663)*(AQ663+AQ664)+\n(AP664*AQ665-AP665*AQ664)*(AQ664+AQ665)+\n(AP665*AQ666-AP666*AQ665)*(AQ665+AQ666)+\n(AP666*AQ667-AP667*AQ666)*(AQ666+AQ667)+\n(AP667*AQ668-AP668*AQ667)*(AQ667+AQ668)+\n(AP668*AQ669-AP669*AQ668)*(AQ668+AQ669)+\n(AP669*AQ670-AP670*AQ669)*(AQ669+AQ670)+\n(AP670*AQ671-AP671*AQ670)*(AQ670+AQ671)+\n(AP671*AQ672-AP672*AQ671)*(AQ671+AQ672)+\n(AP672*AQ673-AP673*AQ672)*(AQ672+AQ673)+\n(AP673*AQ674-AP674*AQ673)*(AQ673+AQ674)+\n(AP674*AQ675-AP675*AQ674)*(AQ674+AQ675)+\n(AP675*AQ676-AP676*AQ675)*(AQ675+AQ676)+\n(AP676*AQ677-AP677*AQ676)*(AQ676+AQ677)+\n(AP677*AQ678-AP678*AQ677)*(AQ677+AQ678)+\n(AP678*AQ679-AP679*AQ678)*(AQ678+AQ679))/6/AQ683)","v":{"$error":"#REF!"}},"y=",{"$f":"+IF(AS683=0,0,-((AR660*AS661-AR661*AS660)*(AS660+AS661)+(AR661*AS662-AR662*AS661)*(AS661+AS662)+\n(AR662*AS663-AR663*AS662)*(AS662+AS663)+\n(AR663*AS664-AR664*AS663)*(AS663+AS664)+\n(AR664*AS665-AR665*AS664)*(AS664+AS665)+\n(AR665*AS666-AR666*AS665)*(AS665+AS666)+\n(AR666*AS667-AR667*AS666)*(AS666+AS667)+\n(AR667*AS668-AR668*AS667)*(AS667+AS668)+\n(AR668*AS669-AR669*AS668)*(AS668+AS669)+\n(AR669*AS670-AR670*AS669)*(AS669+AS670)+\n(AR670*AS671-AR671*AS670)*(AS670+AS671)+\n(AR671*AS672-AR672*AS671)*(AS671+AS672)+\n(AR672*AS673-AR673*AS672)*(AS672+AS673)+\n(AR673*AS674-AR674*AS673)*(AS673+AS674)+\n(AR674*AS675-AR675*AS674)*(AS674+AS675)+\n(AR675*AS676-AR676*AS675)*(AS675+AS676)+\n(AR676*AS677-AR677*AS676)*(AS676+AS677)+\n(AR677*AS678-AR678*AS677)*(AS677+AS678)+\n(AR678*AS679-AR679*AS678)*(AS678+AS679))/6/AS683)","v":0},"y="]
[]
["DNO TEMELJA NA VISINI","PRESJEK NA Visini ",null,{"$f":"ROUND('Analiza i dimenzioniranje'!$U$52,2)","v":1.2},null,"F=",0]
[null,null,null,null,null,"y=",0]
[null,null,null,null,null,"Z=",0]

{"sheet":"Kontrafore","index":48,"n_rows":162,"n_cols":42,"rows_kept":162,"cut":false,"hidden":true,"merged":[[0,32,1,35],[0,17,0,18],[0,19,0,20],[9,36,10,38],[20,37,20,38],[19,29,19,30],[19,25,19,26],[19,31,19,32],[19,33,20,34],[20,31,20,32],[20,25,20,26],[11,14,11,18],[0,14,0,15],[7,20,8,20],[19,21,19,24],[20,29,20,30],[7,19,8,19],[15,26,15,27],[1,27,2,28],[3,27,3,28],[20,14,20,17],[0,9,0,10],[52,0,53,1],[34,1,34,2],[2,0,2,2],[3,0,3,2],[4,0,4,2],[5,0,5,2],[6,0,6,2],[8,0,8,2],[9,0,9,2],[10,0,10,2],[11,0,11,2],[8,7,8,8],[34,3,34,4],[30,5,34,6],[1,7,1,8],[64,5,65,5],[52,4,52,5],[52,6,52,7],[35,6,36,6],[35,5,36,5],[64,4,65,4],[51,3,51,4],[33,11,33,12],[17,7,17,8],[81,20,89,20],[90,20,98,20],[99,20,107,20],[44,7,44,8],[31,14,31,15],[30,14,30,18],[31,17,31,18],[72,20,80,20],[52,8,53,9],[17,9,17,10],[84,6,85,6],[144,24,152,24],[72,24,80,24],[81,24,89,24],[90,24,98,24],[99,24,107,24],[153,20,161,20],[153,24,161,24],[108,24,116,24],[117,24,125,24],[126,24,134,24],[135,24,143,24],[117,20,125,20],[126,20,134,20],[144,20,152,20],[135,20,143,20],[108,20,116,20],[61,26,62,26],[61,28,62,28],[61,25,62,25],[61,21,62,21],[65,21,65,23],[61,23,62,23],[61,24,62,24],[61,22,62,22],[20,44,20,45],[20,39,20,40],[20,42,20,43],[19,37,19,38],[19,35,20,36]]}
[null,null,null,"           Ukoliko nema kontrafore u čeliju E1 upiši DA",{"$f":"IF('Unos podataka'!AB1=\"\",\"\",'Unos podataka'!$AB$1)","v":"DA"}," a ako kontrafore  nema, čeliju E1, briši sa Delete",null,null,null,"računski Presjek  zida\nKoordinate ",null,null,null,null,"Tlocrt rebra kontrafore",null,"Oznaka","Koordinate točaka Temelj i temelj kontrafora"]
["Kontrafore",null,null,null,null,null,null,"koordinate osi kroz temelja",null,{"$f":"IF('Unos podataka'!$O$48=\"DA\",2+'Analiza i dimenzioniranje'!E60,+H20)","v":1.75},{"$f":"+B17","v":9.6153895463470418E-2},null,null,null,"y","x","točke","x","y",null,null,"Nasip na temelju  ispred",null,"Oznaka ","Tlocrt rebra kontrafore",null,null,"Ulazni podaci za rebro kontrafore"]
["duljina temelja kontrafore",null,null,"lk =",{"$f":"IF(E1=\"\",0,'Unos podataka'!AB3)","v":1},"m",{"$f":"+E3","v":1},0,{"$f":"+S10/2","v":0.75},{"$f":"+J2-'Unos podataka'!$G$49","v":1.75},{"$f":"+'C III-V'!C3","v":1.2},null,null,null,{"$f":"IF(E3=0,O5,+R8+0.5)","v":1.5},{"$f":"+S10+(E4-E6)/2","v":1.875},1,2,0,null,null,{"$f":"+AA4+'Analiza i dimenzioniranje'!E61+2","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!E52","v":1.2},"točke","y","x"]
["širina temelja kontrafore",null,null,"b =",{"$f":"IF(E1=\"\",0,'Unos podataka'!AB4)","v":1},"m",{"$f":"+E4","v":1},{"$f":"2+E9+E3","v":5.9000021999999994},{"$f":"+I3","v":0.75},{"$f":"+'C III-V'!B4","v":3.4000010999999999},{"$f":"+'C III-V'!C4","v":1.2},null,null,null,{"$f":"+O3","v":1.5},{"$f":"+P3+E6","v":2.125},2,{"$f":"+R3+E9","v":4.9000021999999994},{"$f":"+S3","v":0},null,null,{"$f":"+V3-'Analiza i dimenzioniranje'!E58","v":4.2000011999999991},{"$f":"+W3","v":1.2},1,{"$f":"+Y11+ 'Analiza i dimenzioniranje'!E55","v":4.2000000999999996},{"$f":"+Z11","v":0},null,"Koordinate točaka"]
["broj kontrafora sa 2 na kraju zida",null,null,"n=",{"$f":"IF(E1=\"\",0,'Unos podataka'!AB5)","v":3},"kom",null,0,{"$f":"+E8/2","v":2},{"$f":"+'C III-V'!B5","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C5","v":3.14},null,null,null,{"$f":"+R8+E3+'Analiza i dimenzioniranje'!E59","v":3.4000000999999997},{"$f":"+P4","v":2.125},3,{"$f":"+R4","v":4.9000021999999994},{"$f":"+E8","v":4},null,null,{"$f":"+V3-'C III-V'!AE30","v":{"$error":"#VALUE!"}},{"$f":"+W4+'Analiza i dimenzioniranje'!E65","v":1.5000009999999999},2,{"$f":"+Y4","v":4.2000000999999996},{"$f":"+ Kontrafore!E8","v":4},null,"x","y"]
["širina  kontrafore",null,null,"bk=",{"$f":"IF(E1=\"\",0,'Unos podataka'!AB6)","v":0.25},"m",null,{"$f":"+H4","v":5.9000021999999994},{"$f":"+I5","v":2},{"$f":"+'C III-V'!B6","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C6","v":3.14},null,null,null,{"$f":"+O5","v":3.4000000999999997},0,4,{"$f":"+R3","v":2},{"$f":"+S5","v":4},null,null,{"$f":"+V3","v":4.9000021999999994},{"$f":"+W5","v":1.5000009999999999},3,{"$f":"+Y5- 'Analiza i dimenzioniranje'!E55","v":3.4000000999999997},{"$f":"+Z5","v":4},null,{"$f":"+H10","v":1.5000010000000001},{"$f":"+I10","v":1.2}]
["duljina kontrafore na temelju do zida",null,null,"dk=",{"$f":"+E3-0.5+'Analiza i dimenzioniranje'!E59","v":1.9000001},"m",null,{"$f":"+H3","v":0},{"$f":"+E8-I3","v":3.25},{"$f":"+'C III-V'!B7","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C7","v":3.44},null,null,null,{"$f":"+O6+ 'Analiza i dimenzioniranje'!E55","v":4.2000000999999996},{"$f":"+P6","v":0},5,2,{"$f":"+S9+G4","v":2.5},"Wkrila tem=",{"$f":"+U10","v":1.4016687933341394},{"$f":"+V3","v":4.9000021999999994},{"$f":"+W3","v":1.2},4,{"$f":"+Y5- 'Analiza i dimenzioniranje'!E55","v":3.4000000999999997},{"$f":"+Z8","v":0.625},null,{"$f":"+H11","v":1.5000010000000001},1.7]
["osni razmak kontrafora   ",null,null,"lk=",{"$f":"+IF(E3=0,1,(V64/W64))","v":4},"m   ",null,{"$f":"+H4","v":5.9000021999999994},{"$f":"+I7","v":3.25},{"$f":"+'C III-V'!B8","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C8","v":3.44},null,null,null,{"$f":"+O7","v":4.2000000999999996},{"$f":"+E8","v":4},6,{"$f":"2-E3","v":1},{"$f":"+S7","v":2.5},"Wosi          \n temelja=",{"$f":"+(R4-R8)*(R4-R8)/6","v":2.5350028600008057},"A=",{"$f":"-0.5*((V3*W4-V4*W3)+(V4*W5-V5*W4)+(V5*W6-V6*W5)+(V6*W7-V7*W6))","v":{"$error":"#VALUE!"}},5,{"$f":"+Y9","v":-0.5},{"$f":"+Z9+ Kontrafore!E6","v":0.625},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["širina temelja zida",null,null,"B =",{"$f":"+'Analiza i dimenzioniranje'!E61","v":2.9000021999999994},"m",null,"Kontrafora",null,{"$f":"+'C III-V'!B9","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C9","v":"A"},null,null,null,{"$f":"+O8- 'Analiza i dimenzioniranje'!E55","v":3.4000000999999997},{"$f":"+P8","v":4},7,{"$f":"+R8","v":1},{"$f":"+S10","v":1.5},null,null,"xt=",{"$f":"-((V3*W4-V4*W3)*(V3+V4)+(V4*W5-V5*W4)*(V4+V5)+(V5*W6-V6*W5)*(V5+V6)+(V6*W7-V7*W6)*(V6+V7))/6/W8","v":{"$error":"#VALUE!"}},6,{"$f":"+IF(Kontrafore!E3=0,Y10,Z14+0.5)-E3","v":-0.5},{"$f":"+AD10+( Kontrafore!E4- Kontrafore!E6)/2","v":0.375},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["visina kontrafore s temeljem",null,null,"hk=",{"$f":"+'Analiza i dimenzioniranje'!$E$48-0.5","v":5.5},"m",null,{"$f":"+'Unos podataka'!I49","v":1.5000010000000001},{"$f":"+'Unos podataka'!J49","v":1.2},{"$f":"+'C III-V'!B10","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C10","v":"A"},null," ",null,{"$f":"+O9","v":3.4000000999999997},{"$f":"+P3","v":1.875},8,{"$f":"+R7","v":2},{"$f":"+S5/2-G4/2","v":1.5},"Wkrila tem=",{"$f":"1*(R5-R7)*(R5-R7)/6","v":1.4016687933341394},"yt=",{"$f":"-((V3*W4-V4*W3)*(W3+W4)+(V4*W5-V5*W4)*(W4+W5)+(V5*W6-V6*W5)*(W5+W6)+(V6*W7-V7*W6)*(W6+W7))/6/W8","v":{"$error":"#VALUE!"}},7,{"$f":"2+ 'Analiza i dimenzioniranje'!E59","v":3.4000000999999997},{"$f":"+Z9","v":0.375},null,3.4000000999999997,1.2]
["širina kontrafore na temelju",null,null,"šk=",{"$f":"+'Analiza i dimenzioniranje'!$E$59+E3-0.5","v":1.9000000999999997},"m",null,{"$f":"+'Unos podataka'!I50","v":1.5000010000000001},{"$f":"+'Unos podataka'!J50","v":1.7},{"$f":"+'C III-V'!B11","v":4.2000010999999997},{"$f":"+'C III-V'!C11","v":1.2},null,null,null,{"$f":"+O4","v":1.5},{"$f":"+P3","v":1.875},9,{"$f":"+R3","v":2},0,null,null,"G=",{"$f":"+W8*'Analiza i dimenzioniranje'!E66","v":{"$error":"#VALUE!"}},8,{"$f":"2+ 'Analiza i dimenzioniranje'!E59","v":3.4000000999999997},0,null,1.5000010000000001,1.2]
["visina zida s temeljem",null,null,"H=",{"$f":"+'Analiza i dimenzioniranje'!E48","v":6},"m",null,{"$f":"+'Unos podataka'!I51","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!J51","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!B12","v":4.2000010999999997},{"$f":"+'C III-V'!C12","v":1.2},null,null,null,"POVRŠINA TLOCRTA I KOORDINATE TEŽIŠTA",null,null,null,null,null,null,"xA=",{"$f":"-(W9-V3)","v":{"$error":"#VALUE!"}},9,{"$f":"+Y4","v":4.2000000999999996},{"$f":"+Z4","v":0},null,"A=",{"$f":"-0.5*((AB6*AC7-AB7*AC6)+(AB7*AC8-AB8*AC7)+(AB8*AC9-AB9*AC8)+(AB9*AC10-AB10*AC9)+(AB10*AC11-AB11*AC10))","v":{"$error":"#VALUE!"}}]
[null,null,null,"L=",{"$f":"+'Analiza i dimenzioniranje'!$E$49","v":12},"m",null,{"$f":"+'Unos podataka'!I52","v":{"$error":"#VALUE!"}},{"$f":"+'Unos podataka'!J52","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!B13","v":4.2000010999999997},{"$f":"+'C III-V'!C13","v":1.2},null,null,null,null,"površina presjeka","  A=",{"$f":"0.5*((R3*S4-R4*S3)+(R4*S5-R5*S4)+(R5*S6-R6*S5)+(R6*S7-R7*S6)+(R7*S8-R8*S7)+(R8*S9-R9*S8)+(R9*S10-R10*S9)+(R10*S11-R11*S10))","v":12.600008799999998},"m2",null,null," Krak zaza MI-I=",{"$f":"+W12","v":{"$error":"#VALUE!"}},"knm/m'",null,null,null,"xt=",{"$f":"IF('Analiza i dimenzioniranje'!C83=\"\",0,-((AB6*AC7-AB7*AC6)*(AB6+AB7)+(AB7*AC8-AB8*AC7)*(AB7+AB8)+(AB8*AC9-AB9*AC8)*(AB8+AB9)+(AB9*AC10-AB10*AC9)*(AB9+AB10)+(AB10*AC11-AB11*AC10)*(AB10+AB11))/6/AC12)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,{"$f":"+'Unos podataka'!I53","v":3.4000000999999997},{"$f":"+'Unos podataka'!J53","v":1.2},{"$f":"+J15","v":4.9000021999999994},{"$f":"+'C III-V'!C14","v":1.2},null,null,null,null,"koordinata težišta","xt=",{"$f":"((R3*S4-R4*S3)*(R3+R4)+(R4*S5-R5*S4)*(R4+R5)+(R5*S6-R6*S5)*(R5+R6)+(R6*S7-R7*S6)*(R6+R7)+(R7*S8-R8*S7)*(R7+R8)+(R8*S9-R9*S8)*(R8+R9)+(R9*S10-R10*S9)*(R9+R10)+(R10*S11-R11*S10)*(R10+R11))/6/R13","v":3.2952392160241724},"m",null,null,null,null,null,null,null,null,"yt=",{"$f":"IF(AC12=0,0,-((AB6*AC7-AB7*AC6)*(AC6+AC7)+(AB7*AC8-AB8*AC7)*(AC7+AC8)+(AB8*AC9-AB9*AC8)*(AC8+AC9)+(AB9*AC10-AB10*AC9)*(AC9+AC10)+(AB10*AC11-AB11*AC10)*(AC10+AC11))/6/AC12)","v":{"$error":"#VALUE!"}}]
["Jednadžba dna temelja",null,null,null,"x",null,null,{"$f":"+'Unos podataka'!I54","v":1.5000010000000001},{"$f":"+'Unos podataka'!J54","v":1.2},{"$f":"+'C III-V'!B15","v":4.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5},null,null,null,null,"koordinata težišta","yt=",{"$f":"((R3*S4-R4*S3)*(S3+S4)+(R4*S5-R5*S4)*(S4+S5)+(R5*S6-R6*S5)*(S5+S6)+(R6*S7-R7*S6)*(S6+S7)+(R7*S8-R8*S7)*(S7+S8)+(R8*S9-R9*S8)*(S8+S9)+(R9*S10-R10*S9)*(S9+S10)+(R10*S11-R11*S10)*(S10+S11))/6/R13","v":2},"m",null,null,null,null,null,null,null,null,"G. rebr=",{"$f":"IF('Analiza i dimenzioniranje'!C83=\"\",0,+AC12*'Analiza i dimenzioniranje'!E62*E6)","v":{"$error":"#VALUE!"}}]
[{"$f":"+A38","v":"Y="},{"$f":"+B38","v":0.12820502301126319},"*x                 +",{"$f":"+D38","v":-0.12820489480624014},null,null,null,null,null,{"$f":"+J2","v":1.75},{"$f":"+K2","v":9.6153895463470418E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"G rebara /m'",null,{"$f":"AC15/E8","v":{"$error":"#VALUE!"}}]
["Y=",{"$f":"+B16*E17+D16","v":9.6153895463470418E-2},null,null,{"$f":"2+'Analiza i dimenzioniranje'!E61-MT!G13","v":1.75},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AC16","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,"Nasip na temeljima kontrafora/m'",null,"Nasip iznad temelja prema obilazeći konzolu",null,"Masa nasipa Kompl. volumen","Masa nasipa bez KF",null,null,"T1",null,"T2"]
[null,null,null,null,null,null,null,"x","y","x","y","x","y",null,"x=",{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},"x=",2]
[null,null,null,null,null,null,null,{"$f":"IF('Unos podataka'!O48=\"DA\",2,+J14-MT!G13)","v":1.75},{"$f":"+K14","v":1.2},{"$f":"+J4","v":3.4000010999999999},{"$f":"+K4","v":1.2},{"$f":"+H10","v":1.5000010000000001},{"$f":"+I10","v":1.2},null,"Y=",{"$f":"+'Analiza i dimenzioniranje'!F190","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+'Analiza i dimenzioniranje'!F193","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"Masa temelja  do II-II",null,"Masa temelja kontrafora do kraja temelja",null,"Masa temelja  do II-II",null,"Masa lijevog temelja, do II-II, bez kontraforom",null,"Masa sredine temelja",null,"Težište temelja od  I-I do kraja temelja"]
[null,null,null,null,null,null,null,{"$f":"H20","v":1.75},{"$f":"IF(J7<J3,K6,IF('Analiza i dimenzioniranje'!E24=0,Kontrafore!E12+(Kontrafore!J9-2+Kontrafore!E3)*TAN('Analiza i dimenzioniranje'!H20*PI()/180),IF(H50<H48,I48,IF(H24>H21,K40,+I26))))","v":{"$error":"#VALUE!"}},{"$f":"+J5","v":{"$error":"#VALUE!"}},{"$f":"+K5","v":3.14},{"$f":"+H11","v":1.5000010000000001},1.7,null,"         Jednadžba pravca kroz 2 točke",null,null,null,null,null,null,null,null,null,null,null,null,"koordinate",null,"koordinate ostalog dijela  temelja",null,"koordinate kontrafore",null,null,null,null,null,"I-I do hA"]
[null,null,null,null,null,null,null,{"$f":"IF('Unos podataka'!B105<2,J3,J7)","v":{"$error":"#VALUE!"}},{"$f":"K42","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E78=\"\",J9,IF('Unos podataka'!G57=\"\",Kontrafore!J9,IF(J3>J6,2,+J6)))","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E78=\"\",K10,IF(G57=\"\",H61,+K6))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,"y=",{"$f":"(R20-P20)/(R19-P19)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-P22*P19+P20","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"x","y","x","y","x","y","x","y","x","y","x","y"]
[null,null,null,null,null,null,null,{"$f":"IF(J22<2,J22,+J24)","v":{"$error":"#VALUE!"}},{"$f":"IF(H48>J22,K39,K24)","v":{"$error":"#VALUE!"}},{"$f":"+IF('Unos podataka'!G57=\"\",Kontrafore!J9,IF(J22=J21,J9,IF(J6<2,2,J6)))","v":{"$error":"#VALUE!"}},{"$f":"IF(J23<H48,I48,IF('Analiza i dimenzioniranje'!E78=\"\",Kontrafore!K9,IF(J22<J3,K5,IF(J6<2,K6,+IF(J23>2,K39,K41)))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AH23","v":2},{"$f":"+AI23","v":0.12820515121628623},3.4000000999999997,{"$error":"#VALUE!"},{"$f":"2+'Analiza i dimenzioniranje'!$E$61-MT!G13","v":1.75},{"$f":"+'Unos podataka'!J46","v":9.6153895463470418E-2},{"$f":"+IF('Unos podataka'!O48=\"DA\",Kontrafore!AJ23,Kontrafore!AF26)","v":2},{"$f":"+'Unos podataka'!J41","v":0.12820515121628623},{"$f":"+'Sile i krakovi'!AA197","v":3.4000000999999997},{"$f":"+'Sile i krakovi'!AB197","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!AA199","v":4.2000000999999996},{"$f":"'Sile i krakovi'!AB199","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,{"$f":"IF(J22<2,J22,IF('Analiza i dimenzioniranje'!E80=0,Kontrafore!J9,H25))","v":{"$error":"#VALUE!"}},{"$f":"IF(J22<28,K22,IF('Unos podataka'!G57=\"\",Kontrafore!K41,IF(H24>=H20,IF(J6<2-E3,K6,K39))))","v":{"$error":"#VALUE!"}},2,{"$f":"IF(J23<2,N61,IF(2>J22,K23,IF(J22<H48,I48,IF(J6>2,K41,K6))))","v":{"$error":"#VALUE!"}},3.4000000999999997,1.2,null,null,{"$f":"2-E3+'Analiza i dimenzioniranje'!E60","v":1},"y=",0,{"$f":"+P24","v":1},0,null,null,null,null,null,null,null,2,{"$f":"+AI24","v":{"$error":"#VALUE!"}},3.4000000999999997,{"$error":"#VALUE!"},{"$f":"2+'Analiza i dimenzioniranje'!E61-MT!G13","v":1.75},{"$f":"+'C III-V'!$C$3","v":1.2},2,{"$f":"+'Sile i krakovi'!Z198","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!AA198","v":3.4000000999999997},{"$f":"+'Sile i krakovi'!AB198","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!AC197","v":4.2000000999999996},{"$f":"'Sile i krakovi'!AB200","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,{"$f":"IF(H48<2,2,IF('Unos podataka'!G57=\"\",2,IF(J6>2,2,IF(+J6<2-E3,2-E3,J6))))","v":{"$error":"#VALUE!"}},{"$f":"+IF(H24<H21,K24,K6)","v":{"$error":"#VALUE!"}},{"$f":"+J24","v":2},{"$f":"+K20","v":1.2},1.5000010000000001,1.2,null,"za x=",{"$f":"2-E3+'Analiza i dimenzioniranje'!E60","v":1},"y=",{"$f":"+P22*P25+R22","v":{"$error":"#VALUE!"}},1,{"$f":"-R25/100","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,3.4000000999999997,{"$f":"+AI25","v":{"$error":"#VALUE!"}},4.2000000999999996,{"$error":"#VALUE!"},2,{"$f":"+'C III-V'!$C$4","v":1.2},{"$f":"+'Sile i krakovi'!Y199","v":3.4000000999999997},{"$f":"+'Sile i krakovi'!Z199","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!AA199","v":4.2000000999999996},{"$f":"+'Sile i krakovi'!AB199","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!U198","v":4.9000010999999999},{"$f":"'Sile i krakovi'!AD197-'Analiza i dimenzioniranje'!C190","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,2,{"$f":"+K4","v":1.2},{"$f":"+J20","v":3.4000010999999999},{"$f":"+K4","v":1.2},"A(m2)=",{"$f":"+AC12","v":{"$error":"#VALUE!"}},null,"za x=",{"$f":"2+'Analiza i dimenzioniranje'!E60","v":2},"y=",{"$f":"+P22*P26+R22","v":{"$error":"#VALUE!"}},2,{"$f":"-R26/100","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,3.4000000999999997,{"$f":"+AI26","v":{"$error":"#VALUE!"}},4.2000000999999996,{"$error":"#VALUE!"},2,{"$f":"+'Unos podataka'!J41","v":0.12820515121628623},{"$f":"+'Sile i krakovi'!Y200","v":3.4000000999999997},{"$f":"+'Sile i krakovi'!Z200","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!AA200","v":4.2000000999999996},{"$f":"+'Sile i krakovi'!AB200","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!AC199","v":4.9000010999999999},{"$f":"'Sile i krakovi'!AB199","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,{"$f":"IF('Unos podataka'!O48=\"DA\",Kontrafore!H26,+H20)","v":1.75},{"$f":"+I26","v":1.2},{"$f":"+J26","v":3.4000010999999999},{"$f":"+K26","v":1.2},"xt=",{"$f":"+AC13","v":{"$error":"#VALUE!"}},null,"za x=",{"$f":"+P26+'Analiza i dimenzioniranje'!E59","v":3.4000000999999997},"y=",{"$f":"+P22*P27+R22","v":{"$error":"#VALUE!"}},3.4000000999999997,{"$f":"-R27/100","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,2,{"$f":"+AI27","v":0.12820515121628623},3.4000000999999997,{"$error":"#VALUE!"},{"$f":"+AF23","v":1.75},{"$f":"+AG23","v":9.6153895463470418E-2},{"$f":"+AH23","v":2},{"$f":"+AI23","v":0.12820515121628623},{"$f":"+'Sile i krakovi'!AA201","v":3.4000000999999997},{"$f":"+'Sile i krakovi'!AB201","v":{"$error":"#VALUE!"}},{"$f":"+'Sile i krakovi'!AA199","v":4.2000000999999996},{"$f":"+AM23","v":{"$error":"#VALUE!"}}]
["Jednadžba pravca rezultante",null,null,null,null,null,null,{"$f":"+H21","v":1.75},{"$f":"IF(E1=\"\",0,-0.5*((H20*I21-H21*I20)+(H21*I22-H22*I21)+(H22*I23-H23*I22)+(H23*I24-H24*I23)+(H24*I25-H25*I24)+(H25*I26-H26*I25)+(H26*I27-H27*I26)))","v":{"$error":"#VALUE!"}},"  A=",{"$f":"IF('Analiza i dimenzioniranje'!E59=0,0,0.5*((J20*K21-J21*K20)+(J21*K22-J22*K21)+(J22*K23-J23*K22)+(J23*K24-J24*K23)+(J24*K25-J25*K24)+(J25*K26-J26*K25)+(J26*K27-J27*K26)))","v":{"$error":"#VALUE!"}},"yt=",{"$f":"+AC14","v":{"$error":"#VALUE!"}},null,"za x=",{"$f":"+P27+'Analiza i dimenzioniranje'!E55-'Analiza i dimenzioniranje'!E60","v":4.2000000999999996},"y=",{"$f":"+P22*P28+R22","v":{"$error":"#VALUE!"}},4.2000000999999996,{"$f":"-R28/100","v":{"$error":"#VALUE!"}}]
["Rv=",{"$f":"+'Analiza i dimenzioniranje'!B168","v":{"$error":"#VALUE!"}},null,null,null,null,null,"xt=",{"$f":"IF(I28=0,0,-((H20*I21-H21*I20)*(H20+H21)+(H21*I22-H22*I21)*(H21+H22)+(H22*I23-H23*I22)*(H22+H23)+(H23*I24-H24*I23)*(H23+H24)+(H24*I25-H25*I24)*(H24+H25)+(H25*I26-H26*I25)*(H25+H26)+(H26*I27-H27*I26)*(H26+H27))/6/I28)","v":{"$error":"#VALUE!"}},"xt=",{"$f":"IF(K28=0,0,((J20*K21-J21*K20)*(J20+J21)+(J21*K22-J22*K21)*(J21+J22)+(J22*K23-J23*K22)*(J22+J23)+(J23*K24-J24*K23)*(J23+J24)+(J24*K25-J25*K24)*(J24+J25)+(J25*K26-J26*K25)*(J25+J26)+(J26*K27-J27*K26)*(J26+J27))/6/K28)","v":{"$error":"#VALUE!"}},"SG rebr/kom=",{"$f":"+AC15","v":{"$error":"#VALUE!"}},null,"za x=",{"$f":"P28+'Analiza i dimenzioniranje'!E58","v":4.9000010999999999},"y=",{"$f":"+P22*P29+R22","v":{"$error":"#VALUE!"}},4.9000010999999999,{"$f":"-R29/100","v":{"$error":"#VALUE!"}}]
["Rh=",{"$f":"+'Analiza i dimenzioniranje'!B167","v":{"$error":"#VALUE!"}},null,null,null,null,null,"yt=",{"$f":"IF(I28=0,0,-((H20*I21-H21*I20)*(I20+I21)+(H21*I22-H22*I21)*(I21+I22)+(H22*I23-H23*I22)*(I22+I23)+(H23*I24-H24*I23)*(I23+I24)+(H24*I25-H25*I24)*(I24+I25)+(H25*I26-H26*I25)*(I25+I26)+(H26*I27-H27*I26)*(I26+I27))/6/I28)","v":{"$error":"#VALUE!"}},"yt=",{"$f":"IF(K28=0,0,((J20*K21-J21*K20)*(K20+K21)+(J21*K22-J22*K21)*(K21+K22)+(J22*K23-J23*K22)*(K22+K23)+(J23*K24-J24*K23)*(K23+K24)+(J24*K25-J25*K24)*(K24+K25)+(J25*K26-J26*K25)*(K25+K26)+(J26*K27-J27*K26)*(K26+K27))/6/K28)","v":{"$error":"#VALUE!"}},"SG rebro/m' zida=",{"$f":"+AC16","v":{"$error":"#VALUE!"}},null,null,{"$f":"+P29","v":4.9000010999999999},"y=",0,4.9000010999999999,0]
["x1=",{"$f":"2+'Analiza i dimenzioniranje'!E61-'Analiza i dimenzioniranje'!H168","v":{"$error":"#VALUE!"}},"a=","Rv/Rh=",{"$f":"-B29/B30","v":{"$error":"#VALUE!"}},null,null,"Gn/kontr =",{"$f":"+I28*'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}},"Gn/kontr =",{"$f":"+K28*'Analiza i dimenzioniranje'!E63","v":{"$error":"#VALUE!"}},"SG nasipa/m'=","nasip bez KF","SG nasipa/m'=","POVRŠINA TLOCRTA I KOORDINATE TEŽIŠTA"]
["Y1=",{"$f":"+C37+'Analiza i dimenzioniranje'!H167","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Gn/m' tem =",{"$f":"ABS(I28* 'Analiza i dimenzioniranje'!E63*Kontrafore!E4)","v":{"$error":"#VALUE!"}},"Gn/m' tem =",{"$f":"ABS(+K28* 'Analiza i dimenzioniranje'!E63)","v":{"$error":"#VALUE!"}},{"$f":"+K32+I32","v":{"$error":"#VALUE!"}},{"$f":"+(L32-M30)","v":{"$error":"#VALUE!"}},{"$f":"+K32+I32","v":{"$error":"#VALUE!"}},"Tlocrt rebra kontrafore",null,"Oznaka","Koordinate točaka",null,null,null,null,null,null,null,null,null,"  A=",{"$f":"-0.5*((AB23*AC24-AB24*AC23)+(AB24*AC25-AB25*AC24)+(AB25*AC26-AB26*AC25)+(AB26*AC27-AB27*AC26))","v":{"$error":"#VALUE!"}},"  A=",{"$f":"0.5*((AD23*AE24-AD24*AE23)+(AD24*AE25-AD25*AE24)+(AD25*AE26-AD26*AE25)+(AD26*AE27-AD27*AE26))","v":{"$error":"#VALUE!"}},"  A=",{"$f":"-0.5*((AF23*AG24-AF24*AG23)+(AF24*AG25-AF25*AG24)+(AF25*AG26-AF26*AG25)+(AF26*AG27-AF27*AG26))","v":0.27195511916503012},"  A=",{"$f":"-0.5*((AH23*AI24-AH24*AI23)+(AH24*AI25-AH25*AI24)+(AH25*AI26-AH26*AI25)+(AH26*AI27-AH27*AI26))","v":{"$error":"#VALUE!"}},"  A=",{"$f":"-0.5*((AJ23*AK24-AJ24*AK23)+(AJ24*AK25-AJ25*AK24)+(AJ25*AK26-AJ26*AK25)+(AJ26*AK27-AJ27*AK26))","v":{"$error":"#VALUE!"}},"  A=",{"$f":"0.5*((AL23*AM24-AL24*AM23)+(AL24*AM25-AL25*AM24)+(AL25*AM26-AL26*AM25)+(AL26*AM27-AL27*AM26))","v":{"$error":"#VALUE!"}}]
["Y=",{"$f":"+E31","v":{"$error":"#VALUE!"}},"* x                    +",{"$f":"-E31*B31+B32","v":{"$error":"#VALUE!"}},null,null,null,"XA=",null,"XA=",null,{"$f":"IF('Analiza i dimenzioniranje'!E59=0,0,+(K32*K29+I32*I29)/L32)","v":{"$error":"#VALUE!"}},{"$f":"+(L32*L33-M30*M27)/M32","v":{"$error":"#VALUE!"}},{"$f":"IF('Analiza i dimenzioniranje'!E59=0,0,+(K32*K29+I32*I29)/N32)","v":{"$error":"#VALUE!"}},{"$f":"IF(E3=0,O35,+R38+0.5)","v":1.5},{"$f":"+S40+(E4-E6)/2","v":1.875},1,{"$f":"2","v":2},0,null,null,null,null,null,null,null,null,"xt=",{"$f":"-((AB23*AC24-AB24*AC23)*(AB23+AB24)+(AB24*AC25-AB25*AC24)*(AB24+AB25)+(AB25*AC26-AB26*AC25)*(AB25+AB26)+(AB26*AC27-AB27*AC26)*(AB26+AB27)+(AB27*AC28-AB28*AC27)*(AB27+AB28)+(AB28*AC29-AB29*AC28)*(AB28+AB29)+(AB29*AC30-AB30*AC29)*(AB29+AB30)+(AB30*AC31-AB31*AC30)*(AB30+AB31))/6/AC32","v":{"$error":"#VALUE!"}},"xt=",{"$f":"((AD23*AE24-AD24*AE23)*(AD23+AD24)+(AD24*AE25-AD25*AE24)*(AD24+AD25)+(AD25*AE26-AD26*AE25)*(AD25+AD26)+(AD26*AE27-AD27*AE26)*(AD26+AD27)+(AD27*AE28-AD28*AE27)*(AD27+AD28)+(AD28*AE29-AD29*AE28)*(AD28+AD29)+(AD29*AE30-AD30*AE29)*(AD29+AD30)+(AD30*AE31-AD31*AE30)*(AD30+AD31))/6/AE32","v":{"$error":"#VALUE!"}},"xt=",{"$f":"IF(AG32=0,0,-((AF23*AG24-AF24*AG23)*(AF23+AF24)+(AF24*AG25-AF25*AG24)*(AF24+AF25)+(AF25*AG26-AF26*AG25)*(AF25+AF26)+(AF26*AG27-AF27*AG26)*(AF26+AF27)+(AF27*AG28-AF28*AG27)*(AF27+AF28)+(AF28*AG29-AF29*AG28)*(AF28+AF29)+(AF29*AG30-AF30*AG29)*(AF29+AF30)+(AF30*AG31-AF31*AG30)*(AF30+AF31))/6/AG32)","v":1.8743861721587556},"xt=",{"$f":"-((AH23*AI24-AH24*AI23)*(AH23+AH24)+(AH24*AI25-AH25*AI24)*(AH24+AH25)+(AH25*AI26-AH26*AI25)*(AH25+AH26)+(AH26*AI27-AH27*AI26)*(AH26+AH27)+(AH27*AI28-AH28*AI27)*(AH27+AH28)+(AH28*AI29-AH29*AI28)*(AH28+AH29)+(AH29*AI30-AH30*AI29)*(AH29+AH30)+(AH30*AI31-AH31*AI30)*(AH30+AH31))/6/AI32","v":{"$error":"#VALUE!"}},"xt=",{"$f":"-((AJ23*AK24-AJ24*AK23)*(AJ23+AJ24)+(AJ24*AK25-AJ25*AK24)*(AJ24+AJ25)+(AJ25*AK26-AJ26*AK25)*(AJ25+AJ26)+(AJ26*AK27-AJ27*AK26)*(AJ26+AJ27)+(AJ27*AK28-AJ28*AK27)*(AJ27+AJ28)+(AJ28*AK29-AJ29*AK28)*(AJ28+AJ29)+(AJ29*AK30-AJ30*AK29)*(AJ29+AJ30)+(AJ30*AK31-AJ31*AK30)*(AJ30+AJ31))/6/AK32","v":{"$error":"#VALUE!"}},"xt=",{"$f":"((AL23*AM24-AL24*AM23)*(AL23+AL24)+(AL24*AM25-AL25*AM24)*(AL24+AL25)+(AL25*AM26-AL26*AM25)*(AL25+AL26)+(AL26*AM27-AL27*AM26)*(AL26+AL27)+(AL27*AM28-AL28*AM27)*(AL27+AL28)+(AL28*AM29-AL29*AM28)*(AL28+AL29)+(AL29*AM30-AL30*AM29)*(AL29+AL30)+(AL30*AM31-AL31*AM30)*(AL30+AL31))/6/AM32","v":{"$error":"#VALUE!"}},"xT=",{"$f":"(AG33*AG35+AI35*AI33+AK35*AK33+AM33*AM35)/AO35","v":{"$error":"#VALUE!"}},"m"]
["X=",0,"Y=",{"$f":"+B33*B34+D33","v":{"$error":"#VALUE!"}},null,null,null,"        Jednadžba nagiba padine iza zida",null,null,null,null,null,null,{"$f":"+O33","v":1.5},{"$f":"+P33+E6","v":2.125},2,{"$f":"+R33+E9","v":4.9000021999999994},{"$f":"+S33","v":0},null,null,null,null,null,null,null,null,"yt=",{"$f":"-((AB23*AC24-AB24*AC23)*(AC23+AC24)+(AB24*AC25-AB25*AC24)*(AC24+AC25)+(AB25*AC26-AB26*AC25)*(AC25+AC26)+(AB26*AC27-AB27*AC26)*(AC26+AC27)+(AB27*AC28-AB28*AC27)*(AC27+AC28)+(AB28*AC29-AB29*AC28)*(AC28+AC29)+(AB29*AC30-AB30*AC29)*(AC29+AC30)+(AB30*AC31-AB31*AC30)*(AC30+AC31))/6/AC32","v":{"$error":"#VALUE!"}},"yt=",{"$f":"((AD23*AE24-AD24*AE23)*(AE23+AE24)+(AD24*AE25-AD25*AE24)*(AE24+AE25)+(AD25*AE26-AD26*AE25)*(AE25+AE26)+(AD26*AE27-AD27*AE26)*(AE26+AE27)+(AD27*AE28-AD28*AE27)*(AE27+AE28)+(AD28*AE29-AD29*AE28)*(AE28+AE29)+(AD29*AE30-AD30*AE29)*(AE29+AE30)+(AD30*AE31-AD31*AE30)*(AE30+AE31))/6/AE32","v":{"$error":"#VALUE!"}},"yt=",{"$f":"IF(AG32=0,0,-((AF23*AG24-AF24*AG23)*(AG23+AG24)+(AF24*AG25-AF25*AG24)*(AG24+AG25)+(AF25*AG26-AF26*AG25)*(AG25+AG26)+(AF26*AG27-AF27*AG26)*(AG26+AG27)+(AF27*AG28-AF28*AG27)*(AG27+AG28)+(AF28*AG29-AF29*AG28)*(AG28+AG29)+(AF29*AG30-AF30*AG29)*(AG29+AG30)+(AF30*AG31-AF31*AG30)*(AG30+AG31))/6/AG32)","v":0.65605041376368345},"yt=",{"$f":"-((AH23*AI24-AH24*AI23)*(AI23+AI24)+(AH24*AI25-AH25*AI24)*(AI24+AI25)+(AH25*AI26-AH26*AI25)*(AI25+AI26)+(AH26*AI27-AH27*AI26)*(AI26+AI27)+(AH27*AI28-AH28*AI27)*(AI27+AI28)+(AH28*AI29-AH29*AI28)*(AI28+AI29)+(AH29*AI30-AH30*AI29)*(AI29+AI30)+(AH30*AI31-AH31*AI30)*(AI30+AI31))/6/AI32","v":{"$error":"#VALUE!"}},"yt=",{"$f":"-((AJ23*AK24-AJ24*AK23)*(AK23+AK24)+(AJ24*AK25-AJ25*AK24)*(AK24+AK25)+(AJ25*AK26-AJ26*AK25)*(AK25+AK26)+(AJ26*AK27-AJ27*AK26)*(AK26+AK27)+(AJ27*AK28-AJ28*AK27)*(AK27+AK28)+(AJ28*AK29-AJ29*AK28)*(AK28+AK29)+(AJ29*AK30-AJ30*AK29)*(AK29+AK30)+(AJ30*AK31-AJ31*AK30)*(AK30+AK31))/6/AK32","v":{"$error":"#VALUE!"}},"yt=",{"$f":"((AL23*AM24-AL24*AM23)*(AM23+AM24)+(AL24*AM25-AL25*AM24)*(AM24+AM25)+(AL25*AM26-AL26*AM25)*(AM25+AM26)+(AL26*AM27-AL27*AM26)*(AM26+AM27)+(AL27*AM28-AL28*AM27)*(AM27+AM28)+(AL28*AM29-AL29*AM28)*(AM28+AM29)+(AL29*AM30-AL30*AM29)*(AM29+AM30)+(AL30*AM31-AL31*AM30)*(AM30+AM31))/6/AM32","v":{"$error":"#VALUE!"}},"Yt=",{"$f":"+(AI34*AG35+AI34*AI35+AK34*AK35+AM34*AM35)/AO35","v":{"$error":"#VALUE!"}},"m"]
[null,"T1         Dno naprezanja       T2",null,"T3  pravac rezultante  T4","T4",null,null,"x=",{"$f":"+O42","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F97","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+R38+E3+'Analiza i dimenzioniranje'!E59","v":3.4000000999999997},{"$f":"+P34","v":2.125},3,{"$f":"+R34","v":4.9000021999999994},{"$f":"+E8","v":4},null,null,null,null,null,null,null,null,"SG=",{"$f":"+AC32*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"SG=",null,"SG=",{"$f":"+AG32*'Analiza i dimenzioniranje'!E62*G4","v":6.798877979125753},"SG=",{"$f":"+AI32*'Analiza i dimenzioniranje'!E62","v":{"$error":"#VALUE!"}},"SG=",{"$f":"+AK32*'Analiza i dimenzioniranje'!$E$62","v":{"$error":"#VALUE!"}},"SG=",{"$f":"+AM32*'Analiza i dimenzioniranje'!$E$62","v":{"$error":"#VALUE!"}},"SG=",{"$f":"AG35+AI35+AK35+AM35","v":{"$error":"#VALUE!"}}]
[" x=",2,{"$f":"2+'Analiza i dimenzioniranje'!E60+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+B31","v":{"$error":"#VALUE!"}},{"$f":"+B34","v":0},"sjecište na dnu temelja","OS temelja","y=",{"$f":"+P42","v":6},{"$f":"+'Analiza i dimenzioniranje'!G96","v":6.2644906473896782},null,null,null,null,{"$f":"+O35","v":3.4000000999999997},0,4,{"$f":"+R33","v":2},{"$f":"+S35","v":4},null,null,null,null,null,null,null,null,"SGtem-kf=",{"$f":"IF('Analiza i dimenzioniranje'!A83=\"\",0,+AC35)","v":{"$error":"#VALUE!"}},"kN/m'",null,"Sgtem-kf=",{"$f":"IF('Analiza i dimenzioniranje'!E83=\"\",0,+AG35)","v":6.798877979125753},"SGtem-kf=",{"$f":"+AI35","v":{"$error":"#VALUE!"}},"SG=",{"$f":"+AK35","v":{"$error":"#VALUE!"}},"SG=",{"$f":"+AM35","v":{"$error":"#VALUE!"}},"SG=",{"$f":"+AO35","v":{"$error":"#VALUE!"}},"kN/m'"]
["Y=",{"$f":"+'C III-V'!$C$2","v":0.12820515121628623},{"$f":"+'Analiza i dimenzioniranje'!E52-'Analiza i dimenzioniranje'!E51","v":0.5},{"$f":"+B32","v":{"$error":"#VALUE!"}},{"$f":"+D34","v":{"$error":"#VALUE!"}},null,null,"Y=",{"$f":"(J36-I36)/(J35-I35)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-I37*I35+I36","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+O36+'Analiza i dimenzioniranje'!E55","v":4.2000000999999996},{"$f":"+P36","v":0},5,2,{"$f":"+S39+E4","v":2.5}]
["Y=",{"$f":"(C37-B37)/(C36-B36)","v":0.12820502301126319},"*x    +",{"$f":"-B38*B36+B37","v":-0.12820489480624014},"dna temelja",{"$f":"+D40","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C15/2","v":0.25},"Y=",{"$f":"(J36-I36)/(J35-I35)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-I38*I35+I36","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+O37","v":4.2000000999999996},{"$f":"+E8","v":4},6,{"$f":"2-E4","v":1},{"$f":"+S37","v":2.5}]
["Y=",{"$f":"-(E37-D37)/(D36-E36)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-(D36*B39-D37)","v":{"$error":"#VALUE!"}},"rezultanta",{"$f":"+B40","v":{"$error":"#VALUE!"}},{"$f":"2+('Analiza i dimenzioniranje'!E61)/2","v":3.4500010999999997},"za X=",{"$f":"+G58","v":{"$error":"#VALUE!"}},"Y=",{"$f":"IF(I37*I39+K37>K40,K40,I37*I39+K37)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+O38-'Analiza i dimenzioniranje'!E55","v":3.4000000999999997},{"$f":"+P38","v":4},7,{"$f":"+R38","v":1},{"$f":"+S40","v":1.5}]
["X=",{"$f":"+(D39-D38)/(B38-B39)","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+$B$39*B40+$D$39","v":{"$error":"#VALUE!"}},null,"Dx=",{"$f":"-(+G39-F39)","v":{"$error":"#VALUE!"}},"za X=",{"$f":"+'Analiza i dimenzioniranje'!F97","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+'Analiza i dimenzioniranje'!G96","v":6.2644906473896782},null,null,null,{"$f":"+O39","v":3.4000000999999997},{"$f":"+P33","v":1.875},8,{"$f":"+R37","v":2},{"$f":"+S35/2-E4/2","v":1.5}]
["Rezultanta  R     X=",{"$f":"-(D39-D41)/B39","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+'Analiza i dimenzioniranje'!E52+0.3","v":1.5},null,"Dy=",{"$f":"-(G38-F38)","v":{"$error":"#VALUE!"}},"za X=",2,"Y=",{"$f":"+I37*I41+K37","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+O34","v":1.5},{"$f":"+P33","v":1.875},9,{"$f":"+R33","v":2},0,null,null,null,null,null,null,null,null,null,null,null,null,null,"+"]
["X=",{"$f":"+C36-'Analiza i dimenzioniranje'!$C$185","v":1.75},"Y=",{"$f":"+B38*B42+D38","v":9.6153895463470418E-2},null,null,null,"za X=",{"$f":"+H22","v":{"$error":"#VALUE!"}},"Y=",{"$f":"IF(I37*I39+K37>K40,K40,I37*I42+K37)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+'Analiza i dimenzioniranje'!F96","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!G95","v":6},null,"  A=",{"$f":"0.5*((R33*S34-R34*S33)+(R34*S35-R35*S34)+(R35*S36-R36*S35)+(R36*S37-R37*S36)+(R37*S38-R38*S37)+(R38*S39-R39*S38)+(R39*S40-R40*S39)+(R40*S41-R41*S40))","v":12.600008799999998}]
["Jednadžba pravca napona u tlu temelja   X=",null,{"$f":"+B47+'Analiza i dimenzioniranje'!E60","v":1.75},{"$f":"+C36","v":4.9000021999999994},null,"V=",{"$f":"+'Analiza i dimenzioniranje'!B168","v":{"$error":"#VALUE!"}},"za X=",{"$f":"+J23","v":{"$error":"#VALUE!"}},"Y=",{"$f":"+$I$37*I43+$K$37","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"+'Analiza i dimenzioniranje'!F97","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!G96","v":6.2644906473896782},null,"xt=",{"$f":"((R33*S34-R34*S33)*(R33+R34)+(R34*S35-R35*S34)*(R34+R35)+(R35*S36-R36*S35)*(R35+R36)+(R36*S37-R37*S36)*(R36+R37)+(R37*S38-R38*S37)*(R37+R38)+(R38*S39-R39*S38)*(R38+R39)+(R39*S40-R40*S39)*(R39+R40)+(R40*S41-R41*S40)*(R40+R41))/6/S42","v":3.2952392160241724}]
[null,{"$f":"+A37","v":"Y="},{"$f":"+G49","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!$F$190","v":{"$error":"#VALUE!"}},null,"A=",{"$f":"+'Analiza i dimenzioniranje'!C185","v":3.1500021999999994},null,null,null,null,null,null,null,null,null,null,"yt=",{"$f":"((R33*S34-R34*S33)*(S33+S34)+(R34*S35-R35*S34)*(S34+S35)+(R35*S36-R36*S35)*(S35+S36)+(R36*S37-R37*S36)*(S36+S37)+(R37*S38-R38*S37)*(S37+S38)+(R38*S39-R39*S38)*(S38+S39)+(R39*S40-R40*S39)*(S39+S40)+(R40*S41-R41*S40)*(S40+S41))/6/S42","v":2}]
[null,"Y=",{"$f":"(D44-C44)/(D43-C43)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-C45*C43+C44","v":{"$error":"#VALUE!"}},"W=",{"$f":"+'Analiza i dimenzioniranje'!C186","v":1.653752310000806},"Teren iza zida sa prometom"]
["X=",{"$f":"2-Kontrafore!E3","v":1},{"$f":"+$C$45*B46+$E$45","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+'Analiza i dimenzioniranje'!F95","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!G95","v":6}]
["X=",{"$f":"2+'Analiza i dimenzioniranje'!E61-MT!G13","v":1.75},{"$f":"+'Analiza i dimenzioniranje'!F194","v":{"$error":"#VALUE!"}},null,null,"s1=",{"$f":"+D44","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F96","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!G95","v":6}]
["X=",{"$f":"2+'Analiza i dimenzioniranje'!E60","v":2},{"$f":"+$C$45*B48+$E$45","v":{"$error":"#VALUE!"}},null,null,"Ms=",{"$f":"+'Analiza i dimenzioniranje'!D171","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F97","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!G96","v":6.2644906473896782}]
["x=",{"$f":"2+'Analiza i dimenzioniranje'!E60+'Analiza i dimenzioniranje'!$E$59","v":3.4000000999999997},{"$f":"+C45*B49+E45","v":{"$error":"#VALUE!"}},null,null,"s0=",{"$f":"+G43/G44-G48/G45","v":{"$error":"#VALUE!"}},{"$f":"+'Analiza i dimenzioniranje'!F98","v":-8},{"$f":"+'Analiza i dimenzioniranje'!G97","v":6.2644906473896782}]
["x=",{"$f":"+B49+'Analiza i dimenzioniranje'!$E$55-'Analiza i dimenzioniranje'!E60","v":4.2000000999999996},{"$f":"+C45*B50+E45","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"+I42","v":{"$error":"#VALUE!"}},{"$f":"+K42","v":{"$error":"#VALUE!"}}]
["x=",{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},{"$f":"+'Analiza i dimenzioniranje'!F190","v":{"$error":"#VALUE!"}}]
["Sredina temelja",{"$f":"(+B42+(C36-B47)/2)","v":3.3250010999999997},{"$f":"+B38*B52+D38","v":0.29807694773173521},"Excentricitet vertikalne sile",null,{"$f":"+B40-B52","v":{"$error":"#VALUE!"}}]
["Težište betonskog zida  bez temelja",null,"Koordinate zida",null,{"$f":"+R1","v":"Koordinate točaka Temelj i temelj kontrafora"},null,"Koordinate presjeka zida s temeljem",null,"Koordinate temelja kontrafore ",null,null," Jednadžba dna temelja",null,null,null,"              Jednadžba lica zida"]
[null,null,null,null,"x",{"$f":"+S2","v":"y"},{"$f":"+H20","v":1.75},{"$f":"+K2","v":9.6153895463470418E-2},null,null,"x=",{"$f":"+I58","v":1.75},{"$f":"+C68","v":4.9000021999999994},null,"x=",{"$f":"+C65","v":4.2000010999999997},{"$f":"+C63","v":{"$error":"#VALUE!"}}]
[{"$f":"+A57","v":3.4000010999999999},{"$f":"+B57","v":1.2},{"$f":"+'C III-V'!B2","v":2},{"$f":"+'C III-V'!C2","v":0.12820515121628623},2,0,{"$f":"+G54","v":1.75},1.2,{"$f":"+'Unos podataka'!I41","v":2},{"$f":"+'Unos podataka'!J41","v":0.12820515121628623},"y=",{"$f":"+J58","v":9.6153895463470418E-2},{"$f":"+D68","v":0.5},null,"y=",{"$f":"+D65","v":1.2},{"$f":"+D63","v":"A"}]
[{"$f":"+A58","v":{"$error":"#VALUE!"}},{"$f":"+B58","v":3.14},{"$f":"+'C III-V'!$B3","v":2},{"$f":"+'C III-V'!C3","v":1.2},4.9000021999999994,0,{"$f":"+J4","v":3.4000010999999999},1.2,{"$f":"+'Unos podataka'!I42","v":2},{"$f":"+'Unos podataka'!J42","v":1.2},"y=",{"$f":"(M55-L55)/(M54-L54)","v":0.12820502301126319},"*x    +",{"$f":"-L56*L54+L55","v":-0.12820489480624014},"y=",{"$f":"(Q55-P55)/(Q54-P54)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-P56*P54+P55","v":{"$error":"#VALUE!"}}]
[{"$f":"+ 'C III-V'!$B4","v":3.4000010999999999},{"$f":"+ 'C III-V'!C4","v":1.2},{"$f":"+'C III-V'!$B4","v":3.4000010999999999},{"$f":"+'C III-V'!C4","v":1.2},4.9000021999999994,4,{"$error":"#VALUE!"},3.14,{"$f":"+'Unos podataka'!I43","v":1.75},{"$f":"+'Unos podataka'!J43","v":1.2},null," Jednadžba lica zida prema zasipu"]
[{"$f":"+ 'C III-V'!$B5","v":{"$error":"#VALUE!"}},{"$f":"+ 'C III-V'!C5","v":3.14},{"$f":"+'C III-V'!$B5","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C5","v":3.14},2,4,{"$error":"#VALUE!"},3.14,{"$f":"+'Unos podataka'!I46","v":1.75},{"$f":"+'Unos podataka'!J46","v":9.6153895463470418E-2},"x=",{"$f":"+J26","v":3.4000010999999999},{"$f":"+J23","v":{"$error":"#VALUE!"}}]
[{"$f":"+ 'C III-V'!$B6","v":{"$error":"#VALUE!"}},{"$f":"+ 'C III-V'!C6","v":3.14},{"$f":"+'C III-V'!$B6","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C6","v":3.14},2,2.5,{"$error":"#VALUE!"},3.44,{"$f":"+'Unos podataka'!I47","v":2},{"$f":"+'Unos podataka'!J47","v":0.12820515121628623},"y=",{"$f":"+K26","v":1.2},{"$f":"+K23","v":{"$error":"#VALUE!"}}]
[{"$f":"+ 'C III-V'!$B7","v":{"$error":"#VALUE!"}},{"$f":"+ 'C III-V'!C7","v":3.44},{"$f":"+'C III-V'!$B7","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C7","v":3.44},1,2.5,{"$error":"#VALUE!"},3.44,null,null,"y=",{"$f":"(M59-L59)/(M58-L58)","v":{"$error":"#VALUE!"}},"*x    +",{"$f":"-L60*L58+L59","v":{"$error":"#VALUE!"}}]
[{"$f":"+ 'C III-V'!$B8","v":{"$error":"#VALUE!"}},{"$f":"+ 'C III-V'!C8","v":3.44},{"$f":"+'C III-V'!$B8","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C8","v":3.44},1,1.5,{"$error":"#VALUE!"},"A",null,null,"za X=",2,"y=",{"$f":"+L60*L61+N60","v":{"$error":"#VALUE!"}}]
[{"$f":"+ 'C III-V'!$B9","v":{"$error":"#VALUE!"}},{"$f":"+ 'C III-V'!C9","v":"A"},{"$f":"+'C III-V'!$B9","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C9","v":"A"},2,1.5,{"$error":"#VALUE!"},"A",null,null,null,null,null,null,null,null,null,null,null,null,null,"duljina zida","broj kontrafora","sirina zid za kontarforu","sirina  kontarfore","duljina  kontarfore","debljina  kontarfore"]
[{"$f":"+ 'C III-V'!$B10","v":{"$error":"#VALUE!"}},{"$f":"+ 'C III-V'!C10","v":"A"},{"$f":"+'C III-V'!$B10","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!C10","v":"A"},null,null,4.2000010999999997,1.2]
[{"$f":"+ 'C III-V'!$B11","v":4.2000010999999997},{"$f":"+ 'C III-V'!C11","v":1.2},{"$f":"+'C III-V'!$B11","v":4.2000010999999997},{"$f":"+'C III-V'!C11","v":1.2},null,null,4.2000010999999997,1.2,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+E13","v":12},{"$f":"+E5","v":3},{"$f":"IF(W64=0,0,E13/E5)","v":4},{"$f":"+E4","v":1},{"$f":"+E3","v":1},{"$f":"+E6","v":0.25}]
[{"$f":"+A55","v":3.4000010999999999},{"$f":"+B55","v":1.2},{"$f":"+'C III-V'!$B12","v":4.2000010999999997},{"$f":"+'C III-V'!C12","v":1.2},null,null,4.2000010999999997,1.2]
[{"$f":"+A56","v":{"$error":"#VALUE!"}},{"$f":"+B55","v":1.2},{"$f":"+'C III-V'!$B13","v":4.2000010999999997},{"$f":"+'C III-V'!C13","v":1.2},null,null,4.9000021999999994,1.2,null,null,null,null,null,null,null,null,null,null,null,null,null,"Crtež temelja s kontraforom",null,null,null,"Crtež rebra kontrafore"]
[{"$f":"+A57","v":3.4000010999999999},{"$f":"+B57","v":1.2},{"$f":"+'C III-V'!$B14","v":4.9000021999999994},{"$f":"+'C III-V'!C14","v":1.2},null,null,4.9000021999999994,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oznaka","Koordinate točaka",null,null,"Oznaka","Koordinate točaka"]
["  A=",{"$f":"-0.5*((A55*B56-A56*B55)+(A56*B57-A57*B56)+(A57*B58-A58*B57)+(A58*B59-A59*B58)+(A59*B60-A60*B59)+(A60*B61-A61*B60)+(A61*B62-A62*B61)+(A62*B63-A63*B62)+(A63*B64-A64*B63)+(A64*B65-A65*B64)+(A65*B66-A66*B65)+(A66*B67-A67*B66))","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!$B15","v":4.9000021999999994},{"$f":"+'C III-V'!C15","v":0.5},null,null,{"$f":"+G54","v":1.75},9.6153895463470418E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,"točke","x","y",null,"točke","x","y"]
["xt=",{"$f":"-((A55*B56-A56*B55)*(A55+A56)+(A56*B57-A57*B56)*(A56+A57)+(A57*B58-A58*B57)*(A57+A58)+(A58*B59-A59*B58)*(A58+A59)+(A59*B60-A60*B59)*(A59+A60)+(A60*B61-A61*B60)*(A60+A61)+(A61*B62-A62*B61)*(A61+A62)+(A62*B63-A63*B62)*(A62+A63)+(A63*B64-A64*B63)*(A63+A64)+(A64*B65-A65*B64)*(A64+A65)+(A65*B66-A66*B65)*(A65+A66)+(A66*B67-A67*B66)*(A66+A67))/6/B68","v":{"$error":"#VALUE!"}},{"$f":"+'C III-V'!$B16","v":2},{"$f":"+'C III-V'!C16","v":0.12820515121628623},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(E1=\"\",\"\",2+'Analiza i dimenzioniranje'!$E$59)","v":3.4000000999999997},{"$f":"+IF(E1=\"\",\"\",0)","v":0}]
["yt=",{"$f":"-((A55*B56-A56*B55)*(B55+B56)+(A56*B57-A57*B56)*(B56+B57)+(A57*B58-A58*B57)*(B57+B58)+(A58*B59-A59*B58)*(B58+B59)+(A59*B60-A60*B59)*(B59+B60)+(A60*B61-A61*B60)*(B60+B61)+(A61*B62-A62*B61)*(B61+B62)+(A62*B63-A63*B62)*(B62+B63)+(A63*B64-A64*B63)*(B63+B64)+(A64*B65-A65*B64)*(B64+B65)+(A65*B66-A66*B65)*(B65+B66)+(A66*B67-A67*B66)*(B66+B67))/6/B68","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y","x",null,2,{"$f":"IF(E1=\"\",\"\",+AA69+'Analiza i dimenzioniranje'!E55)","v":4.2000000999999996},{"$f":"+IF(E1=\"\",\"\",0)","v":0}]
["xt za stab=",{"$f":"+A65-B69","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"2-'Unos podataka'!AB3","v":1},0,null,3,{"$f":"+AA70","v":4.2000000999999996},{"$f":"+IF(E1=\"\",\"\",+'Analiza i dimenzioniranje'!E49)","v":12}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"+W74","v":4.9000021999999994},0,null,4,{"$f":"+AA69","v":3.4000000999999997},{"$f":"+AB71","v":12}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,2,0,1,1,{"$f":"+AA69","v":3.4000000999999997},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"2+'Analiza i dimenzioniranje'!E61","v":4.9000021999999994},0,null,2,{"$f":"+AA73","v":3.4000000999999997},{"$f":"+($X$64-$Y$64)/2+$Y$64/2-$AA$64/2","v":1.875}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"+W74","v":4.9000021999999994},{"$f":"+X64","v":4},null,3,{"$f":"2-E3+0.5","v":1.5},{"$f":"+AB74","v":1.875}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,{"$f":"+W73","v":2},{"$f":"+X75","v":4},null,4,{"$f":"+AA75","v":1.5},{"$f":"+AB75+AA64","v":2.125}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"+W76","v":2},{"$f":"+X76-(X64-Y64)/2","v":2.5},null,5,{"$f":"+AA74","v":3.4000000999999997},{"$f":"+AB76","v":2.125}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,{"$f":"2-Z64","v":1},{"$f":"+X77","v":2.5},null,6,{"$f":"+AA77","v":3.4000000999999997},{"$f":"+AB77","v":2.125}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,{"$f":"+W78","v":1},{"$f":"+X78-Y64","v":1.5},null,7,{"$f":"+AA78","v":3.4000000999999997},{"$f":"+X64","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,{"$f":"+W77","v":2},{"$f":"+X79","v":1.5},null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,{"$f":"+W73","v":2},{"$f":"+X73","v":0},null,9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,1,{"$f":"IF(E1=\"\",\"\",W73)","v":2},{"$f":"+X73+X64","v":4},2,1,{"$f":"+AA73","v":3.4000000999999997},{"$f":"+AB73+X$64","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"IF(E1=\"\",\"\",W74)","v":4.9000021999999994},{"$f":"X82","v":4},null,2,3.4000000999999997,{"$f":"+$X$64+AB74","v":5.875}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"IF(E1=\"\",\"\",+W74)","v":4.9000021999999994},{"$f":"IF(U82<=$W$64,+U82*$X$64,\"\")","v":8},null,3,1.5,{"$f":"+$X$64+AB75","v":5.875}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,{"$f":"IF(E1=\"\",\"\",W76)","v":2},{"$f":"+X84","v":8},null,4,1.5,{"$f":"+$X$64+AB76","v":6.125}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"IF(E1=\"\",\"\",+W77)","v":2},{"$f":"+X83+X77","v":6.5},null,5,3.4000000999999997,{"$f":"+$X$64+AB77","v":6.125}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,{"$f":"IF(E1=\"\",\"\",W78)","v":1},{"$f":"+X86","v":6.5},null,6,3.4000000999999997,{"$f":"+$X$64+AB78","v":6.125}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,{"$f":"IF(E1=\"\",\"\",+W79)","v":1},{"$f":"X87-E4","v":5.5},null,7,{"$f":"+AA78","v":3.4000000999999997},{"$f":"+AB82+X64","v":8}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,{"$f":"IF(E1=\"\",\"\",W80)","v":2},{"$f":"+X88","v":5.5},null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,{"$f":"IF(E1=\"\",\"\",W81)","v":2},{"$f":"+X82","v":4},null,9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,1,{"$f":"IF(E1=\"\",\"\",IF($X$91=\"\",\"\",W73))","v":2},{"$f":"IF($U$91>$E$5,\"\",X82+$X$64)","v":8},3,1,{"$f":"IF(AB91=\"\",\"\",+AA88)","v":3.4000000999999997},{"$f":"IF(AB97=\"\",\"\",AB82+$X$64)","v":8}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"IF(E1=\"\",\"\",IF($X$91=\"\",\"\",W74))","v":4.9000021999999994},{"$f":"IF($U$91>$E$5,\"\",X83+$X$64)","v":8},null,2,{"$f":"IF(AB92=\"\",\"\",AA83)","v":3.4000000999999997},{"$f":"IF(AB97=\"\",\"\",AB83+$X$64)","v":9.875}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"IF(E1=\"\",\"\",IF($X$91=\"\",\"\",W75))","v":4.9000021999999994},{"$f":"IF(U91<=$W$64,+U91*$X$64,\"\")","v":12},null,3,1.5,{"$f":"IF(AB97=\"\",\"\",AB84+$X$64)","v":9.875}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,{"$f":"IF(E1=\"\",\"\",IF($X$91=\"\",\"\",W76))","v":2},{"$f":"+X93","v":12},null,4,1.5,{"$f":"IF(AB97=\"\",\"\",+AB85+$X$64)","v":10.125}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"IF(E1=\"\",\"\",IF($X$91=\"\",\"\",W77))","v":2},{"$f":"IF(+X86+$X$64>$E$13,\"\",+X86+$X$64)","v":10.5},null,5,3.4000000999999997,{"$f":"IF(AB97=\"\",\"\",AB86+$X$64)","v":10.125}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n=4",null,6,{"$f":"IF(E1=\"\",\"\",IF($X$91=\"\",\"\",W78))","v":1},{"$f":"IF(+X87+$X$64>$E$13,\"\",+X87+$X$64)","v":10.5},null,6,3.4000000999999997,{"$f":"IF(AB97=\"\",\"\",AB87+$X$64)","v":10.125}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,{"$f":"IF(E1=\"\",\"\",IF($X$91=\"\",\"\",W79))","v":1},{"$f":"IF(+X88+$X$64>$E$13,\"\",+X88+$X$64)","v":9.5},null,7,3.4000000999999997,{"$f":"IF(Y91<=$W$64,+Y91*$X$64,\"\")","v":12}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,{"$f":"IF(E1=\"\",\"\",IF($X$91=\"\",\"\",W80))","v":2},{"$f":"IF(+X89+$X$64>$E$13,\"\",+X89+$X$64)","v":9.5},null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,{"$f":"IF(E1=\"\",\"\",IF($X$91=\"\",\"\",W81))","v":2},{"$f":"IF(+X90+$X$64>$E$13,\"\",+X90+$X$64)","v":8},null,9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,1,{"$f":"IF($X$100=\"\",\"\",W82)","v":""},{"$f":"IF(X102=\"\",\"\",+X91+$X$64)","v":""},4,1,{"$f":"IF(AB100=\"\",\"\",+AA97)","v":""},{"$f":"IF(AB106=\"\",\"\",AB91+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"",{"$f":"+X100","v":""},null,2,{"$f":"IF(AB101=\"\",\"\",AA92)","v":""},{"$f":"IF(AB106=\"\",\"\",AB92+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,"",{"$f":"IF(U100<=$W$64,+U100*$X$64,\"\")","v":""},null,3,"",{"$f":"IF(AB106=\"\",\"\",AB93+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"",{"$f":"+X102","v":""},null,4,"",{"$f":"IF(AB106=\"\",\"\",+AB94+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"",{"$f":"IF(W104=\"\",\"\",+X95+$X$64)","v":""},null,5,"",{"$f":"IF(AB106=\"\",\"\",AB95+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"",{"$f":"+X104","v":""},null,6,"",{"$f":"IF(AB106=\"\",\"\",AB96+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"",{"$f":"IF(W106=\"\",\"\",+X97+$X$64)","v":""},null,7,"",{"$f":"IF(Y100<=$W$64,+Y100*$X$64,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"",{"$f":"+X106","v":""},null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"",{"$f":"IF(W108=\"\",\"\",+X99+$X$64)","v":""},null,9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,1,{"$f":"IF($X$109=\"\",\"\",W91)","v":""},{"$f":"IF($X$111=\"\",\"\",+X100+$X$64)","v":""},5,1,{"$f":"IF(AB109=\"\",\"\",+AA106)","v":""},{"$f":"IF(AB115=\"\",\"\",AB100+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"",{"$f":"+X109","v":""},null,2,{"$f":"IF(AB110=\"\",\"\",AA101)","v":""},{"$f":"IF(AB115=\"\",\"\",AB101+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,"",{"$f":"IF(U109<=$W$64,+U109*$X$64,\"\")","v":""},null,3,"",{"$f":"IF(AB115=\"\",\"\",AB102+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"",{"$f":"+X111","v":""},null,4,"",{"$f":"IF(AB115=\"\",\"\",+AB103+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"",{"$f":"IF($X$111=\"\",\"\",+X104+$X$64)","v":""},null,5,"",{"$f":"IF(AB115=\"\",\"\",AB104+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"",{"$f":"+X113","v":""},null,6,"",{"$f":"IF(AB115=\"\",\"\",AB105+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"",{"$f":"IF($X$111=\"\",\"\",+X106+$X$64)","v":""},null,7,"",{"$f":"IF(Y109<=$W$64,+Y109*$X$64,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"",{"$f":"+X115","v":""},null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"",{"$f":"IF(W117=\"\",\"\",+X108+$X$64)","v":""},null,9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,1,{"$f":"IF($X$118=\"\",\"\",W100)","v":""},{"$f":"IF($X$120=\"\",\"\",+X109+$X$64)","v":""},6,1,{"$f":"IF(AB118=\"\",\"\",+AA115)","v":""},{"$f":"IF(AB124=\"\",\"\",AB109+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"",{"$f":"+X118","v":""},null,2,{"$f":"IF(AB119=\"\",\"\",AA110)","v":""},{"$f":"IF(AB124=\"\",\"\",AB110+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,"",{"$f":"IF(U118<=$W$64,+U118*$X$64,\"\")","v":""},null,3,"",{"$f":"IF(AB124=\"\",\"\",AB111+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"",{"$f":"+X120","v":""},null,4,"",{"$f":"IF(AB124=\"\",\"\",+AB112+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"",{"$f":"IF($X$120=\"\",\"\",+X113+$X$64)","v":""},null,5,"",{"$f":"IF(AB124=\"\",\"\",AB113+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"",{"$f":"+X122","v":""},null,6,"",{"$f":"IF(AB124=\"\",\"\",AB114+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"",{"$f":"IF($X$120=\"\",\"\",+X115+$X$64)","v":""},null,7,"",{"$f":"IF(Y118<=$W$64,+Y118*$X$64,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"",{"$f":"+X124","v":""},null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"",{"$f":"+X118","v":""},null,9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,1,{"$f":"IF($X$127=\"\",\"\",W109)","v":""},{"$f":"IF($X$129=\"\",\"\",+X118+$X$64)","v":""},7,1,{"$f":"IF(AB127=\"\",\"\",+AA124)","v":""},{"$f":"IF(AB133=\"\",\"\",AB118+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"",{"$f":"+X127","v":""},null,2,{"$f":"IF(AB128=\"\",\"\",AA119)","v":""},{"$f":"IF(AB133=\"\",\"\",AB119+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,"",{"$f":"IF(U127<=$W$64,+U127*$X$64,\"\")","v":""},null,3,"",{"$f":"IF(AB133=\"\",\"\",AB120+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"",{"$f":"+X129","v":""},null,4,"",{"$f":"IF(AB133=\"\",\"\",+AB121+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"",{"$f":"IF($X$129=\"\",\"\",+X122+$X$64)","v":""},null,5,"",{"$f":"IF(AB133=\"\",\"\",AB122+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"",{"$f":"+X131","v":""},null,6,"",{"$f":"IF(AB133=\"\",\"\",AB123+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"",{"$f":"IF($X$129=\"\",\"\",+X124+$X$64)","v":""},null,7,"",{"$f":"IF(Y127<=$W$64,+Y127*$X$64,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"",{"$f":"+X133","v":""},null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"",{"$f":"+X127","v":""},null,9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,1,{"$f":"IF($X$136=\"\",\"\",W118)","v":""},{"$f":"IF($X$138=\"\",\"\",+X127+$X$64)","v":""},8,1,{"$f":"IF(AB136=\"\",\"\",+AA133)","v":""},{"$f":"IF(AB142=\"\",\"\",AB127+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"",{"$f":"+X136","v":""},null,2,{"$f":"IF(AB137=\"\",\"\",AA128)","v":""},{"$f":"IF(AB142=\"\",\"\",AB128+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,"",{"$f":"IF(U136<=$W$64,+U136*$X$64,\"\")","v":""},null,3,"",{"$f":"IF(AB142=\"\",\"\",AB129+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"",{"$f":"+X138","v":""},null,4,"",{"$f":"IF(AB142=\"\",\"\",+AB130+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"",{"$f":"IF($X$138=\"\",\"\",+X131+$X$64)","v":""},null,5,"",{"$f":"IF(AB142=\"\",\"\",AB131+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"",{"$f":"+X140","v":""},null,6,"",{"$f":"IF(AB142=\"\",\"\",AB132+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"",{"$f":"IF($X$138=\"\",\"\",+X133+$X$64)","v":""},null,7,"",{"$f":"IF(Y136<=$W$64,+Y136*$X$64,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"",{"$f":"+X142","v":""},null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"",{"$f":"+X136","v":""},null,9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,1,{"$f":"IF($X$145=\"\",\"\",W127)","v":""},{"$f":"IF($X$147=\"\",\"\",+X136+$X$64)","v":""},9,1,{"$f":"IF(AB145=\"\",\"\",+AA142)","v":""},{"$f":"IF(AB151=\"\",\"\",AB136+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"",{"$f":"+X145","v":""},null,2,{"$f":"IF(AB146=\"\",\"\",AA137)","v":""},{"$f":"IF(AB151=\"\",\"\",AB137+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,"",{"$f":"IF(U145<=$W$64,+U145*$X$64,\"\")","v":""},null,3,"",{"$f":"IF(AB151=\"\",\"\",AB138+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"",{"$f":"+X147","v":""},null,4,"",{"$f":"IF(AB151=\"\",\"\",+AB139+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"",{"$f":"IF($X$147=\"\",\"\",+X140+$X$64)","v":""},null,5,"",{"$f":"IF(AB151=\"\",\"\",AB140+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"",{"$f":"+X149","v":""},null,6,"",{"$f":"IF(AB151=\"\",\"\",AB141+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"",{"$f":"IF($X$147=\"\",\"\",+X142+$X$64)","v":""},null,7,"",{"$f":"IF(Y145<=$W$64,+Y145*$X$64,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"",{"$f":"+X151","v":""},null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"",{"$f":"+X145","v":""},null,9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,1,{"$f":"IF($X$154=\"\",\"\",W136)","v":""},{"$f":"IF($U$154>$E$5,\"\",+X145+$X$64)","v":""},10,1,{"$f":"IF(AB154=\"\",\"\",+AA151)","v":""},{"$f":"IF(AB160=\"\",\"\",AB145+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"IF(X155=\"\",\"\",W146)","v":""},"",null,2,{"$f":"IF(AB155=\"\",\"\",AA146)","v":""},{"$f":"IF(AB160=\"\",\"\",AB146+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"IF(X156=\"\",\"\",W147)","v":""},"",null,3,{"$f":"IF(AB156=\"\",\"\",AA147)","v":""},{"$f":"IF(AB160=\"\",\"\",AB147+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"","",null,4,{"$f":"IF(AB157=\"\",\"\",AA148)","v":""},{"$f":"IF(AB160=\"\",\"\",+AB148+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"","",null,5,{"$f":"IF(AB158=\"\",\"\",AA149)","v":""},{"$f":"IF(AB160=\"\",\"\",AB149+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"","",null,6,{"$f":"IF(AB159=\"\",\"\",AA150)","v":""},{"$f":"IF(AB160=\"\",\"\",AB150+$X$64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"","",null,7,{"$f":"IF(AB160=\"\",\"\",+AA151)","v":""},{"$f":"IF(Y154<=$W$64,+Y154*$X$64,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"","",null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"",{"$f":"+X154","v":""},null,9]